3GPP TS 22.088 V16.0.0 (2020-07)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Services and System Aspects;

Call Barring (CB) supplementary services;  
Stage 1

(Release 16)

** 

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.  
The present document has not been subject to any approval process by the 3GPPOrganisational Partners and shall not be implemented.  
This Specification is provided for future development work within 3GPPonly. The Organisational Partners accept no liability for any use of this Specification.  
Specifications and reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organisational Partners' Publications Offices.

Keywords

LTE, GSM, UMTS, call barring, supplementary service, stage 1

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword [5](#__RefHeading___Toc367451514)

0 Scope [6](#__RefHeading___Toc367451515)

0.1 References [6](#__RefHeading___Toc367451516)

0.2 Abbreviations [7](#__RefHeading___Toc367451517)

1 Barring of outgoing calls [7](#__RefHeading___Toc367451518)

1.1 Definition [7](#__RefHeading___Toc367451519)

1.2 General description [7](#__RefHeading___Toc367451520)

1.2.1 Description [7](#__RefHeading___Toc367451521)

1.2.2 Applicability to telecommunication services [8](#__RefHeading___Toc367451522)

1.2.3 Terminology [8](#__RefHeading___Toc367451523)

1.3 Normal procedures with successful outcome [8](#__RefHeading___Toc367451524)

1.3.1 Provision [8](#__RefHeading___Toc367451525)

1.3.2 Withdrawal [9](#__RefHeading___Toc367451526)

1.3.3 Registration [9](#__RefHeading___Toc367451527)

1.3.4 Erasure [9](#__RefHeading___Toc367451528)

1.3.5 Activation [9](#__RefHeading___Toc367451529)

1.3.6 Deactivation [10](#__RefHeading___Toc367451530)

1.3.7 Invocation [10](#__RefHeading___Toc367451531)

1.3.8 Normal operation with successful outcome [10](#__RefHeading___Toc367451532)

1.3.11 Interrogation [10](#__RefHeading___Toc367451533)

1.4 Exceptional procedures or unsuccessful outcome [11](#__RefHeading___Toc367451534)

1.4.1 Provision [11](#__RefHeading___Toc367451535)

1.4.2 Registration [11](#__RefHeading___Toc367451536)

1.4.4 Activation [11](#__RefHeading___Toc367451537)

1.4.5 Deactivation [11](#__RefHeading___Toc367451538)

1.5 Alternate procedures [11](#__RefHeading___Toc367451539)

1.6 Interactions with other supplementary services [12](#__RefHeading___Toc367451540)

1.6.82.1 Call forwarding unconditional [12](#__RefHeading___Toc367451541)

1.6.82.2 Call forwarding on mobile subscriber busy [12](#__RefHeading___Toc367451542)

1.6.82.3 Call forwarding on no reply [12](#__RefHeading___Toc367451543)

1.6.82.4 Call forwarding on mobile subscriber not reachable [12](#__RefHeading___Toc367451544)

1.6.83.1 Call waiting [12](#__RefHeading___Toc367451545)

1.6.83.2 Call hold [12](#__RefHeading___Toc367451546)

1.6.84 MultiParty service [12](#__RefHeading___Toc367451547)

1.6.85.1 Closed user group [12](#__RefHeading___Toc367451548)

1.7 Interworking considerations [12](#__RefHeading___Toc367451549)

2 Barring of incoming calls [12](#__RefHeading___Toc367451550)

2.1 Definition [12](#__RefHeading___Toc367451551)

2.2 General description [13](#__RefHeading___Toc367451552)

2.2.1 Description [13](#__RefHeading___Toc367451553)

2.2.2 Applicability to telecommunication services [13](#__RefHeading___Toc367451554)

2.2.3 Terminology [13](#__RefHeading___Toc367451555)

2.3 Normal procedures with successful outcome [13](#__RefHeading___Toc367451556)

2.3.1 Provision [13](#__RefHeading___Toc367451557)

2.3.2 Withdrawal [14](#__RefHeading___Toc367451558)

2.3.3 Registration [14](#__RefHeading___Toc367451559)

2.3.4 Erasure [14](#__RefHeading___Toc367451560)

2.3.5 Activation [14](#__RefHeading___Toc367451561)

2.3.6 Deactivation [15](#__RefHeading___Toc367451562)

2.3.7 Invocation [15](#__RefHeading___Toc367451563)

2.3.8 Normal operation with successful outcome [15](#__RefHeading___Toc367451564)

2.3.11 Interrogation [15](#__RefHeading___Toc367451565)

2.4 Exceptional procedures or unsuccessful outcome [15](#__RefHeading___Toc367451566)

2.4.2 Registration [15](#__RefHeading___Toc367451567)

2.4.4 Activation [16](#__RefHeading___Toc367451568)

2.4.5 Deactivation [16](#__RefHeading___Toc367451569)

2.5 Alternate procedures [16](#__RefHeading___Toc367451570)

2.6 Interactions with other supplementary services [16](#__RefHeading___Toc367451571)

2.6.82.1 Call forwarding unconditional [16](#__RefHeading___Toc367451572)

2.6.82.2 Call forwarding on mobile subscriber busy [16](#__RefHeading___Toc367451573)

2.6.82.3 Call forwarding on no reply [17](#__RefHeading___Toc367451574)

2.6.82.4 Call forwarding on mobile subscriber not reachable [17](#__RefHeading___Toc367451575)

2.6.83.2 Call hold [17](#__RefHeading___Toc367451576)

2.6.81.1 Calling Line Identification [17](#__RefHeading___Toc367451577)

2.6.84 MultiParty service [17](#__RefHeading___Toc367451578)

2.6.85.1 Closed user group [17](#__RefHeading___Toc367451579)

2.7 Interworking considerations [17](#__RefHeading___Toc367451580)

Annex A (informative): Change history [18](#__RefHeading___Toc367451581)

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# 0 Scope

The present document describes the supplementary services belonging to the group Call Restriction Supplementary Services.

The general aspects - including definitions and recommended provision - of the description of the supplementary services are given in 3GPP TS 22.004 [2].

The Call Restriction supplementary services allow the possibility for a mobile subscriber to have barring of certain categories of outgoing or incoming calls at the mobile subscribers access.

The group of Call Restriction Services includes two supplementary services:

- barring of outgoing calls;

- barring of incoming calls.

By use of subscription options, the mobile subscriber can at provision time select a set of one or more barring programs to determine the categories of calls to be barred. The following categories are defined:

- all outgoing calls;

- outgoing international calls;

- outgoing international calls except those directed to the home PLMN country;

- all incoming calls;

- incoming calls when roaming outside the home PLMN country.

NOTE 1: Each category (barring program) is handled as a single supplementary service.

NOTE 2: The call barring program "incoming calls when roaming outside the home PLMN country" is only relevant if as a general rule the called mobile subscriber pays the charges for the forwarded part of the call from his home PLMN country to any other country.

The barring services can be offered to a mobile subscriber with a password option allowing the activation and deactivation by the subscriber. One password per mobile subscriber is supported by the network for all barring services. For the definition of the password, the description of its use and its management, see 3GPP TS 22.004 [2].

## 0.1 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

* References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.
* For a specific reference, subsequent revisions do not apply.
* For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TS 22.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 22.004: "General on supplementary services".

[3] 3GPP TS 22.030: "Man‑Machine Interface (MMI) of the Mobile Station (MS)".

[4] 3GPP TS 22.082: "Call Forwarding (CF) supplementary services ‑ Stage 1".

[5] 3GPP TS 22.084: "MultiParty (MPTY) supplementary services ‑ Stage 1".

[6] 3GPP TS 22.081: "Line Identification supplementary services - Stage 1".

## 0.2 Abbreviations

Abbreviations used in the present document are listed in 3GPP TS 21.905 [1].

# 1 Barring of outgoing calls

## 1.1 Definition

This service makes it possible for a mobile subscriber to have barring of certain categories of outgoing calls according to a barring program which is selected from a set of one or more barring programs chosen at provision time and is valid for all outgoing calls, or just those associated with a specific basic service group.

The ability of the served mobile subscriber to receive calls and to set-up emergency calls remains unaffected.

## 1.2 General description

### 1.2.1 Description

The mobile subscriber may determine by subscription of a set of one or more unique barring programs what kind of outgoing calls shall be barred.

The following barring programs are defined:

1) Barring of all outgoing calls;

2) Barring of outgoing international calls;

3) Barring of outgoing international calls except those directed to the home PLMN country.

The PLMN will ensure that only one of the barring programs is active per basic service group. The activation of one specific barring program will override an already active one (i.e. the old one will be permanently deactivated).

Description of contents of barring programs:

**Barring of all outgoing calls:**

With this barring program there are no outgoing set-up possibilities, except emergency calls.

**Barring of outgoing international calls:**

Outgoing call set-up possibilities exist only to subscribers of the PLMN(s) and the fixed network(s) of the country where the mobile subscriber is presently located. So the present PLMN may be the home PLMN or a visited PLMN, respectively the fixed network may be that of the home PLMN country or that of a visited PLMN country.

NOTE 1: This definition implies that mobile subscribers, subscribed to a PLMN in the country in which the served mobile subscriber roams, can be called irrespective where they roam. On the other hand, mobile subscribers, subscribed to any PLMN in another country than the one in which the served mobile subscriber roams, cannot be called even if they roam in the same PLMN area as the served mobile subscriber.

**Barring of all outgoing international calls except those directed to the home PLMN country:**

Outgoing call set-up possibilities exist only to subscribers of the PLMN(s) and the fixed network(s) of the country where the mobile subscriber is presently located or to mobile subscribers of the home PLMN country of the served mobile subscriber and to subscribers of the fixed network(s) in the home PLMN country. So the present PLMN may be the home PLMN or a visited PLMN, respectively the fixed network may be that of the home PLMN country or that of a visited PLMN country.

NOTE 2: This definition implies that mobile subscribers, subscribed to a PLMN in the country in which the served mobile subscriber roams or mobile subscribers subscribed to any PLMN in the same country as the served mobile subscriber home PLMN can be called irrespective where they roam. On the other hand, mobile subscribers, subscribed to any PLMN in another country than the one in which the served mobile subscriber roams and not belonging to the same country as the served mobile subscriber, cannot be called even if they roam in the same PLMN area as the served mobile subscriber or if they roam in the home PLMN country of the served mobile subscriber.

In the case of SMS, this barring program shall prevent the subscriber from sending Short Messages using a Service Centre Address that is not part of the subscriber's home PLMN country numbering plan.

### 1.2.2 Applicability to telecommunication services

The applicability of this supplementary service is defined in 3GPP TS 22.004 [2].

### 1.2.3 Terminology

A barring program defines the subscribed barring condition and will determine the categories of calls to be barred.

## 1.3 Normal procedures with successful outcome

### 1.3.1 Provision

The supplementary service will be provided after pre-arrangement with the service provider. At provision, subscription options should be selected by the served mobile subscriber.

The service can be offered with two subscription options.

The first subscription option is the definition of the barring condition by a set of one or more barring programs. This subscription option applies to all basic services subscribed. Only one value can be selected for the barring condition.

The second subscription option relates to the control of the call barring supplementary service(s). The subscriber may choose to have the control of the service(s) by use of a password, or may leave the control to the service provider. The value of this subscription option is valid collectively for all basic services and all call barring supplementary services to which the subscriber subscribes to.

Subscription options are summarized below:

|  |  |
| --- | --- |
| Subscription option | Value |
|  |  |
| Barring condition | - barring program 1 |
|  |  |
|  | - barring program 2 |
|  |  |
|  | - barring program 3 |
|  |  |
|  | - barring program 1 and |
|  | barring program 2 |
|  |  |
|  | - barring program 1 and |
|  | barring program 3 |
|  |  |
|  | - barring program 2 and |
|  | barring program 3 |
|  |  |
|  | - barring program 1 and |
|  | barring program 2 and |
|  | barring program 3 |
|  |  |
| Control of barring services | - by subscriber using password |
|  | - by the service provider |

NOTE: A service provider needs not offer the option "control of barring services" to his subscribers. However, the support of the password facility is mandatory in the network for visiting subscribers.

### 1.3.2 Withdrawal

The service will be withdrawn at the subscriber’s request or for administrative reasons.

### 1.3.3 Registration

If the served mobile subscriber at provision time has selected the subscription option "control of barring services by subscriber using password", the service provider has to register a password at provision time. Furthermore the served mobile subscriber can change the password at any time by an appropriate control procedure which is described in 3GPP TS 22.004 [2].

### 1.3.4 Erasure

If the served mobile subscriber at provision time has selected the subscription option "control of barring services by subscriber using password", a password can be erased as described in 3GPP TS 22.004.

### 1.3.5 Activation

Activation takes place with an appropriate control procedure by the subscriber or by the service provider. The activation of barring of outgoing calls does not affect any current communication. Only one barring program may be activated at a time for one basic service group.. The activation of a barring program will deactivate an already active one.

If the served mobile subscriber at provision time has selected the subscription option "control of barring services by subscriber using password", the supplementary service is activated if the subscriber provides the following information to the network:

- password;

- information as to whether all calls or calls of a specific basic service group should be barred.

NOTE: If no Basic Service code is inserted by the user this is interpreted as the group "All Basic Services".

- selected barring program.

If the served mobile subscriber at provision time has selected the subscription option "control of barring services by service provider", the supplementary service cannot be activated by the subscriber. The activation has to be performed by the service provider.

The activation status attached to different basic service groups can be modified separately.

### 1.3.6 Deactivation

Deactivation takes place by means of an appropriate control procedure by the subscriber, or by the service provider, or finally by activation of a new barring program for the same basic service group.

If the served mobile subscriber at provision time has selected the subscription option "control of barring services by subscriber using password", the supplementary service is deactivated if the subscriber provides the following information to the network:

- password;

- information as to whether barring of all calls or calls of a specific basic service group should be deactivated.

NOTE: If no Basic Service code is inserted by the user this is interpreted as the group "All Basic Services".

- selected barring program (i.e. the code for one specific Outgoing Barring program given in 3GPP TS 22.030) or selected barring supplementary service (i.e. the code for Outgoing Barring Service or the code for All Barring Services given in 3GPP TS 22.030).

If the served mobile subscriber at provision time has selected the subscription option "control of barring services by service provider", the supplementary service cannot be deactivated by the subscriber. The deactivation has to be performed by the service provider.

### 1.3.7 Invocation

The supplementary service is automatically invoked by the network upon a request for an outgoing call for a basic service not allowed by an active barring program for the corresponding basic service group. In the case of Short Message, only the Service Centre Address is relevant for the Call Barring service.

### 1.3.8 Normal operation with successful outcome

When barring of outgoing calls is active for a basic service group, each outgoing call set-up to a number not allowed by the barring program related to that basic service group will be refused by the network. In this case the served mobile subscriber will receive an indication that the call is not permitted and has been barred.

When barring of outgoing calls is active, the ability of the served mobile subscriber to receive calls is not affected.

When barring of outgoing calls is active, the ability of the served mobile subscriber to set-up emergency calls is not affected.

### 1.3.11 Interrogation

The subscriber shall by an appropriate control procedure be given the possibility to get a list of all basic service groups for which the given barring program is active (irrespective of whether it is operative or quiescent).

In the situation when a subscriber has activated BOIC-exHC and is roaming in a PLMN not supporting this supplementary service, the local PLMN will return - as an answer to interrogation - the status "not supported".

This information may be translated by the mobile station to inform the user about the replacement of BOIC-exHC with BOIC.

If the served mobile subscriber wants to retrieve information from the local PLMN about the status of BOIC, she has to repeat the interrogation procedure with the supplementary service code for BOIC.

## 1.4 Exceptional procedures or unsuccessful outcome

### 1.4.1 Provision

A PLMN which does not support the barring program "Barring of Outgoing International Calls Except Those Directed to the Home PLMN Country", shall replace this program with "Barring of Outgoing International Calls".

### 1.4.2 Registration

If the served mobile subscriber at provision time has selected the subscription option "control of barring services by service provider", an attempt to register a password will be denied and the served mobile subscriber should receive a notification.

When the served mobile subscriber at provision time has selected the subscription option "control of barring services by the subscriber using password", the handling of incorrect password entry is described in 3GPP TS 22.004 [2].

### 1.4.4 Activation

If the served mobile subscriber at provision time has selected the subscription option "control of barring services by the service provider", an attempt to activate the barring services will be denied and the served mobile subscriber should receive a notification.

When the served mobile subscriber at provision time has selected the subscription option "control of barring services by subscriber using a password", the handling of incorrect password entry is described in 3GPP TS 22.0004.

The barring of outgoing calls activation request must specify the basic service group and the selected barring program. If the subscriber does not completely specify for which basic service group (individual basic service group or all basic service groups) barring of outgoing calls is to be activated and the selected barring program, the network will reject the activation request with appropriate cause.

NOTE 1: If no basic service group code is inserted by the user this is interpreted as the group "All Basic Services".

NOTE 2: The group "all basic services" in the context of barring of outgoing calls means all except emergency calls.

### 1.4.5 Deactivation

If the served mobile subscriber, at provision time, has selected the subscription option "control of barring services by the service provider", an attempt to deactivate will be denied and the served mobile subscriber should receive a notification.

If the served mobile subscriber, at provision time, has selected the subscription option "control of the barring services by the subscriber using password", the handling of incorrect password entry is described in 3GPP TS 22.004 [2].

The barring of outgoing calls deactivation request must specify the basic service group and the selected barring program (i.e. the code for one specific Outgoing Barring program given in 3GPP TS 22.030) or the selected barring supplementary service (i.e. the code for Outgoing Barring Service or the code for All Barring Services given in 3GPP TS 22.030). If the subscriber does not completely specify for which basic service group (individual basic service group or all basic service groups) barring of outgoing calls is to be deactivated and the selected barring program or supplementary service, the network will reject the deactivation request with appropriate cause.

NOTE: If no basic service group code is inserted by the user this is interpreted as the group "All Basic Services".

## 1.5 Alternate procedures

None identified.

## 1.6 Interactions with other supplementary services

#### 1.6.82.1 Call forwarding unconditional

See 3GPP TS 22.082 [4].

#### 1.6.82.2 Call forwarding on mobile subscriber busy

See 3GPP TS 22.082 [4].

#### 1.6.82.3 Call forwarding on no reply

See 3GPP TS 22.082 [4].

#### 1.6.82.4 Call forwarding on mobile subscriber not reachable

See 3GPP TS 22.082 [4].

#### 1.6.83.1 Call waiting

The activation of barring of outgoing calls at the calling mobile subscriber's side does not affect any currently waiting calls originated by the calling mobile subscriber.

#### 1.6.83.2 Call hold

If barring of outgoing calls is activated after a call hold is invoked on an outgoing call, the held call can be retrieved. Any new outgoing call to a number not allowed by the barring program is barred.

### 1.6.84 MultiParty service

See 3GPP TS 22.084 [5].

#### 1.6.85.1 Closed user group

Barring of outgoing calls takes precedence over the CUG restrictions. The activation of barring of outgoing calls during an outgoing call does not affect any current CUG call.

## 1.7 Interworking considerations

None identified.

# 2 Barring of incoming calls

## 2.1 Definition

This service makes it possible for a mobile subscriber to have barring of certain categories of incoming calls according to a barring program which is selected from a set of one or more barring programs chosen at provision time and is valid for all incoming calls, or just those associated with a specific basic service group.

The ability of the served mobile subscriber to set-up outgoing calls remains unaffected.

## 2.2 General description

### 2.2.1 Description

The mobile subscriber may determine by subscription of a set of one or more barring programs what kind of incoming calls shall be barred.

The following barring programs are defined:

1) Barring of all incoming calls;

2) Barring of incoming calls when roaming outside the home PLMN country;

3) Anonymous Call Rejection.

The barring programs 2) and 3) may be active simultaneously per basic service group, but can not be active simultaneously with the barring program 1) per basic service group. The PLMN will ensure that exclusive barring programs are not active simultaneously per basic service group. The activation of one specific barring program will override an already active exclusive one (i.e. the old one will be permanently deactivated).

If barring programs 2) and 3) are active simultaneously for a specific basic service group, the barring program 2) shall apply when the called subscriber is roaming outside the home PLMN country.

Description of contents of barring programs:

**Barring of all incoming calls:**

With this barring program there will be no set-up of incoming calls to the served subscriber.

**Barring of incoming calls when roaming outside the home PLMN country:**

With this barring program, calls which are terminated for the served subscriber will be barred if the subscriber is roaming outside the home PLMN country (i.e. the program is active and operative). The ability to receive calls in the home PLMN country remains unaffected (i.e. the program is active and quiescent).

**Anonymous Call Rejection:**

With this barring program, calls which are terminated for the served subscriber will be barred when the CLI presentation is restricted according to CLIR. The calls are barred regardless of the current state (e.g. free or busy) of the served subscriber’s access. The calling user will be given an appropriate indication that the call has been rejected due to the application of the ACR supplementary service. Calls which are terminated for the served subscriber without a CLI or when CLI presentation is not available, is allowed, or is restricted by the network shall be allowed.

### 2.2.2 Applicability to telecommunication services

The applicability of this supplementary service is defined in 3GPP TS 22.004 [2].

### 2.2.3 Terminology

A barring program defines the subscribed barring condition and will determine the categories of calls to be barred.

## 2.3 Normal procedures with successful outcome

### 2.3.1 Provision

The supplementary service will be provided after pre-arrangement with the service provider. At provision, subscription options should be selected by the served mobile subscriber.

The service can be offered with two subscription options.

The first subscription option is the definition of the barring condition by a set of one or more barring programs. This subscription option applies to all basic services subscribed to. Only one value can be selected for the barring condition.

The second subscription option relates to the control of the call barring supplementary service(s). The subscriber may choose to have the control of the service(s) by use of a password, or may leave the control to the service provider. The value of this subscription option is valid collectively for all basic services and all call barring supplementary services to which the subscriber subscribes to.

Subscription options are summarized below:

|  |  |
| --- | --- |
| Subscription option | Value |
|  |  |
| Barring condition | - barring program 1 |
|  |  |
|  | - barring program 2 |
|  |  |
|  | - barring program 1 and |
|  | barring program 2 |
|  |  |
| Control of barring services | - by subscriber using password |
|  |  |
|  | - by the service provider |
|  |  |

NOTE: A service provider needs not offer the option "control of barring services" to his subscribers. However, the support of the password facility is mandatory in the network for visiting subscribers.

### 2.3.2 Withdrawal

The service will be withdrawn at the subscriber’s request or for administrative reasons.

### 2.3.3 Registration

If the served mobile subscriber at provision time has selected the subscription option "control of barring services by subscriber using password", the service provider has to register a password at provision time. Furthermore, the served mobile subscriber can change the password at any time by an appropriate control procedure which is described in 3GPP TS 22.004 [2].

### 2.3.4 Erasure

If the served mobile subscriber at provision time has selected the subscription option "control of barring services by subscriber using password", a password can be erased as described in 3GPP TS 22.004 [2].

### 2.3.5 Activation

Activation takes place with an appropriate control procedure by the subscriber or by the service provider. The activation of barring of incoming calls does not affect any current communication. Only one barring program may be activated at a time for one basic service group. The activation of the barring program will deactivate an already active one.

If the served mobile subscriber, at provision time, has selected the subscription option "control of barring services by subscriber using password", the supplementary service is activated if the subscriber provides the following information to the network:

- password;

- information as to whether all calls or calls of a specific basic service group should be barred.

NOTE: If no Basic Service code is inserted by the user this is interpreted as the group "All Basic Services".

- selected barring program.

If the served mobile subscriber at provision time has selected the subscription option "control of barring services by service provider", the supplementary service cannot be activated by the subscriber. The activation has to be performed by the service provider.

The activation status attached to different basic service groups can be modified separately.

### 2.3.6 Deactivation

Deactivation takes place by means of an appropriate control procedure by the subscriber, or by the service provider, or finally by activation of a new barring program for the same basic service group.

If the served mobile subscriber at provision time has selected the subscription option "control of barring services by subscriber using password", the supplementary service is deactivated if the subscriber provides the following information to the network:

- password;

- information as to whether barring of all calls or calls of a specific basic service group should be deactivated.

NOTE: If no Basic Service code is inserted by the user this is interpreted as the group "All Basic Services".

- selected barring program (i.e. the code for one specific Incoming Barring program given in 3GPP TS 22.030) or selected barring supplementary service (i.e. the code for Incoming Barring Service or the code for All Barring Services given in 3GPP TS 22.030).

If the served mobile subscriber, at provision time, has selected the subscription option "control of barring services by service provider", the supplementary service cannot be deactivated by the subscriber. The deactivation has to be performed by the service provider.

### 2.3.7 Invocation

The supplementary service is automatically invoked by the network upon a request for an incoming call for a basic service not allowed by an active and operative barring program for the corresponding basic service group.

### 2.3.8 Normal operation with successful outcome

When barring of incoming calls is active for a basic service group, each incoming call set-up not allowed by the barring program related to that basic service group will be refused by the network. In this case the calling mobile subscriber will receive an indication that the call is not permitted and has been barred.

When barring of incoming calls is active, the ability of the served mobile subscriber to originate calls is not affected.

### 2.3.11 Interrogation

The subscriber shall by an appropriate control procedure be given the possibility to get a list of all basic service groups for which the given barring program is active (irrespective of whether it is operative or quiescent).

## 2.4 Exceptional procedures or unsuccessful outcome

### 2.4.2 Registration

If the served mobile subscriber, at provision time, has selected the subscription option "control of barring services by service provider", an attempt to register a password will be denied and the served mobile subscriber should receive a notification.

When the served mobile subscriber, at provision time, has selected the subscription option "control of barring services by subscriber using password", the handling of incorrect password entry is as described in 3GPP TS 22.004 [2].

### 2.4.4 Activation

If the served mobile subscriber, at provision time, has selected the subscription option "control of barring services by the service provider", an attempt to activate the barring services will be denied and the served mobile subscriber should receive a notification.

If the served mobile subscriber, at provision time, has selected the subscription option "control of barring services by the subscriber using password", the handling of incorrect password entry is as described in 3GPP TS 22.004 [2].

The barring of incoming calls activation request must specify the basic service group and the selected barring program. If the subscriber does not completely specify for which basic service (individual basic service group or all basic service groups) barring of incoming calls is to be activated and the selected barring program, the network will reject the activation request with appropriate cause.

NOTE: If no Basic Service group code is inserted by the user this is interpreted as the group "All Basic Services".

### 2.4.5 Deactivation

If the served mobile subscriber, at provision time, has selected the subscription option "control of barring services by the service provider", an attempt to deactivate will be denied and the served mobile subscriber should receive a notification.

If the served mobile subscriber, at provision time, has selected the subscription option "control of barring services by the subscriber using password", the handling of incorrect password entry is as described in 3GPP TS 22.004 [2].

The barring of incoming calls deactivation request must specify the basic service group and the selected barring program (i.e. the code for one specific Incoming Barring program given in 3GPP TS 22.030) or the selected barring supplementary service (i.e. the code for Incoming Barring Service or the code for All Barring Services given in 3GPP TS 22.030). If the subscriber does not completely specify for which basic service group (individual basic service group or all basic service groups) barring of incoming calls is to be deactivated and the selected barring program or supplementary service, the network will reject the deactivation request with appropriate cause.

NOTE: If no Basic Service group code is inserted by the user this is interpreted as the group "All Basic Services".

## 2.5 Alternate procedures

None identified.

## 2.6 Interactions with other supplementary services

#### 2.6.82.1 Call forwarding unconditional

Except for ACR, see 3GPP TS 22.082 [4].

For ACR, if the served (forwarding) user has activated the ACR supplementary service, then the ACR supplementary service shall take precedence over the Call forwarding unconditional supplementary service, i.e. , a call which is terminated for the served subscriber when CLI presentation is restricted shall be rejected according to the ACR supplementary service.

#### 2.6.82.2 Call forwarding on mobile subscriber busy

Except for ACR, see 3GPP TS 22.082 [4].

For ACR, i f the served (forwarding) user has activated the ACR supplementary service, then the ACR supplementary service shall take precedence over the Call forwarding on mobile subscriber busy supplementary service i.e. , a call which is terminated for the served subscriber when CLI is restricted shall be rejected according to the ACR supplementary service.

#### 2.6.82.3 Call forwarding on no reply

Except for ACR , see 3GPP TS 22.082 [4].

For ACR, if the served (forwarding) user has activated the ACR supplementary service, then the ACR supplementary service shall take precedence over the Call forwarding on no reply supplementary service, i.e., a call which is terminated for the served subscriber when CLI is restricted shall be rejected according to the ACR supplementary service.

#### 2.6.82.4 Call forwarding on mobile subscriber not reachable

Except for ACR, see 3GPP TS 22.082 [4].

For ACR, if the served (forwarding) user has activated the ACR supplementary service, then the ACR supplementary service shall take precedence over the Call forwarding on mobile subscriber not reachable supplementary service i.e., a call which is terminated for the served subscriber when CLI is restricted shall be rejected according to the ACR supplementary service.

#### 2.6.83.2 Call hold

If barring of incoming calls is activated after a call hold is invoked on an incoming call, the held call can be retrieved. Any new incoming call not allowed by the barring program is barred.

#### 2.6.81.1 Calling Line Identification

If the called user has subscribed to the override category according to the CLIP supplementary service [6], then the CLIP supplementary service shall take precedence over the ACR supplementary service, i.e., a call which is terminated for the served subscriber when CLI is restricted shall be offered to the served subscriber.

### 2.6.84 MultiParty service

See 3GPP TS 22.084 [5].

#### 2.6.85.1 Closed user group

Except for ACR, barring of incoming calls takes precedence over the CUG restrictions. The activation of barring of incoming calls during an incoming call does not affect any current CUG call.

If the called user has activated the ACR supplementary service, then if a closed user group call is offered to a called user belonging to the same closed user group, the closed user group call shall take precedence over the ACR supplementary service. If the called user also has the incoming access capability within the closed user group supplementary service, and if the offered call to the called user is also a non-closed user group call or a closed user group call to which the called party does not belong, the ACR supplementary service shall take precedence over the closed user group supplementary service.

## 2.7 Interworking considerations

None identified.

Annex A (informative):  
Change history

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | | | | | |
| **TSG SA#** | **SA Doc.** | **SA1 Doc** | **Spec** | **CR** | **Rev** | **Rel** | **Cat** | **Subject/Comment** | **Old** | **New** | **WI** |
| Jun 1999 |  |  | GSM  02.88 |  |  |  |  | Transferred to 3GPP SA1 | 7.0.0 |  |  |
| SA#04 |  |  | 22.088 |  |  | R99 |  | Transferred to 3GPP SA1 |  | 3.0.0 |  |
| SP-05 | SP-99479 | S1-99635 | 22.088 | 001 |  | R99 | D | Editorial changes for alignment | 3.0.0 | 3.0.1 | Editorial changes |
| 22/05/00 |  |  | 22.088 | None |  | R99 |  | Correction of wrong implementation of CR | 3.0.1 | 3.0.2 |  |
| SP-11 | SP-010065 | S1-010258 | 22.088 |  |  | Rel-4 |  | Transferred to 3GPP Release 4 | 3.0.2 | 4.0.0 |  |
| SP-15 | SP-020045 | S1-020457 | 22.088 | 002 | - | Rel-4 | F | Editorial CR to correct terms and references | 4.0.0 | 4.1.0 | CORRECT |
| SP-16 | SP-020267 | S1-021043 | 22.088 |  |  | Rel-5 |  | Updated from Rel-4 to Rel5 | 4.1.0 | 5.0.0 |  |
| SP-26 | SP-040744 | S1-040997 | 22.088 |  |  | Rel-6 |  | Updated from Rel-5 to Rel-6 | 5.0.0 | 6.0.0 |  |
| SP-36 |  |  | 22.088 |  |  | Rel-7 |  | Updated from Rel-6 to Rel-7 | 6.0.0 | 7.0.0 |  |
| SP-42 | - | - |  |  |  | Rel-8 |  | Updated from Rel-7 to Rel-8 | 7.0.0 | 8.0.0 |  |
| SP-46 | - | - | - | - | - | - | - | Updated to Rel-9 by MCC | 8.0.0 | 9.0.0 |  |
| 2011-03 | - | - | - | - | - | - | - | Update to Rel-10 version (MCC) | 9.0.0 | 10.0.0 |  |
| SP-52 | SP-110376 | S1-111434 | 22.088 | 0003 | 4 | Rel-11 | B | Addition of Anonymous Call Rejection as a SS | 10.0.0 | 11.0.0 | ACR\_CS |
| SP-61 | SP-130456 | S1-134178 | 22.088 | 0006 | 4 | Rel-11 | F | SMSC Usage Restriction in Roaming | 11.0.0 | 11.1.0 | TEI11 |
| 2014-10 | - | - | - | - | - | - | - | Update to Rel-12 version (MCC) | 11.1.0 | 12.0.0 |  |
| 2015-12 | - | - | - | - | - | - | - | Updated to Rel-13 by MCC | 12.0.0 | 13.0.0 |  |
| 2017-03 | - | - | - | - | - | - | - | Updated to Rel-14 by MCC | 13.0.0 | 14.0.0 |  |
| 2018-06 | - | - | - | - | - | - | - | Updated to Rel-15 by MCC | 14.0.0 | 15.0.0 |  |
| SA#88e | - | - | - | - | - | - | - | Updated to Rel-16 by MCC | 15.0.0 | 16.0.0 |  |