3GPP TS 23.135 V16.0.0 (2020-07)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Core Network and Terminals;

Multicall supplementary service;   
Stage 2

(Release 16)

** 

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.   
The present document has not been subject to any approval process by the 3GPPOrganisational Partners and shall not be implemented.   
This Specification is provided for future development work within 3GPPonly. The Organisational Partners accept no liability for any use of this Specification.  
Specifications and reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organisational Partners' Publications Offices.

Keywords

UMTS, network, supplementary service, multicall, stage 2

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword [5](#__RefHeading___Toc517463936)

1 Scope [5](#__RefHeading___Toc517463937)

2 References [5](#__RefHeading___Toc517463938)

3 Definitions and abbreviations [6](#__RefHeading___Toc517463939)

3.1 Definitions [6](#__RefHeading___Toc517463940)

3.2 Abbreviations [6](#__RefHeading___Toc517463941)

4 Descriptions [6](#__RefHeading___Toc517463942)

4.1 Handling of Multicall [6](#__RefHeading___Toc517463943)

4.1.1 Provision [6](#__RefHeading___Toc517463944)

4.1.2 Withdrawal [6](#__RefHeading___Toc517463945)

4.1.3 Registration [6](#__RefHeading___Toc517463946)

4.1.4 Erasure [7](#__RefHeading___Toc517463947)

4.1.5 Activation [8](#__RefHeading___Toc517463948)

4.1.6 Deactivation [8](#__RefHeading___Toc517463949)

4.1.7 Interrogation [8](#__RefHeading___Toc517463950)

4.2 Call related procedures [10](#__RefHeading___Toc517463951)

4.2.1 MO call [10](#__RefHeading___Toc517463952)

4.2.2 MT call [10](#__RefHeading___Toc517463953)

4.3 Messages and their contents [12](#__RefHeading___Toc517463954)

4.3.1 Messages between MS and MSC [12](#__RefHeading___Toc517463955)

4.3.2 Messages on B interface (MSC-VLR) [13](#__RefHeading___Toc517463956)

4.3.2.1 Send Info For Outgoing Call [13](#__RefHeading___Toc517463957)

4.3.2.2 Send Info For Outgoing Call negative response [13](#__RefHeading___Toc517463958)

4.3.2.3 Send Info For Incoming Call [13](#__RefHeading___Toc517463959)

4.3.2.4 Send Info For Incoming Call ack [13](#__RefHeading___Toc517463960)

4.3.2.5 Send Info For Incoming Call negative response [13](#__RefHeading___Toc517463961)

4.3.2.6 Complete Call [13](#__RefHeading___Toc517463962)

4.3.2.7 Complete Call ack [13](#__RefHeading___Toc517463963)

4.3.2.8 Page MS [13](#__RefHeading___Toc517463964)

4.3.2.9 Page MS negative response [14](#__RefHeading___Toc517463965)

4.3.2.10 Process Access Request [14](#__RefHeading___Toc517463966)

4.3.2.11 Process Access Request ack [14](#__RefHeading___Toc517463967)

4.3.2.12 Process Access Request negative response [14](#__RefHeading___Toc517463968)

4.3.2.13 Search For MS [14](#__RefHeading___Toc517463969)

4.3.2.14 Search For MS ack [14](#__RefHeading___Toc517463970)

4.3.2.15 Search For MS negative response [14](#__RefHeading___Toc517463971)

5 Network entity functions [15](#__RefHeading___Toc517463972)

5.1 General [15](#__RefHeading___Toc517463973)

5.2 MO call [15](#__RefHeading___Toc517463974)

5.2.1 Functional requirements of serving MSC [15](#__RefHeading___Toc517463975)

5.2.2 Functional requirements of VLR [16](#__RefHeading___Toc517463976)

5.3 MT call [18](#__RefHeading___Toc517463977)

5.3.1 Functional requirements of serving MSC [18](#__RefHeading___Toc517463978)

5.3.2 Functional requirements of VLR [22](#__RefHeading___Toc517463979)

6 Interaction with telecommunication services [24](#__RefHeading___Toc517463980)

6.1 Speech [24](#__RefHeading___Toc517463981)

6.2 Short message service [24](#__RefHeading___Toc517463982)

6.3 Facsimile service [24](#__RefHeading___Toc517463983)

6.4 Data circuit asynchronous [24](#__RefHeading___Toc517463984)

6.5 Data circuit synchronous [24](#__RefHeading___Toc517463985)

6.6 Void [24](#__RefHeading___Toc517463986)

6.7 GPRS [24](#__RefHeading___Toc517463987)

7 Interaction with other supplementary services [24](#__RefHeading___Toc517463988)

7.1 Line Identification services [24](#__RefHeading___Toc517463989)

7.2 Call forwarding unconditional (CFU) [24](#__RefHeading___Toc517463990)

7.3 Call forward on busy (CFB) [25](#__RefHeading___Toc517463991)

7.4 Call forwarding on no reply (CFNRy) [25](#__RefHeading___Toc517463992)

7.5 Call forwarding on MS not reachable (CFNRc) [25](#__RefHeading___Toc517463993)

7.6 Call Hold (CH) [25](#__RefHeading___Toc517463994)

7.7 Call Waiting (CW) [25](#__RefHeading___Toc517463995)

7.8 Multiparty service (MPTY) [25](#__RefHeading___Toc517463996)

7.9 Closed user group (CUG) [25](#__RefHeading___Toc517463997)

7.10 Advice Of Charge (AoC) [25](#__RefHeading___Toc517463998)

7.11 Call Barring services [25](#__RefHeading___Toc517463999)

7.12 Explicit call transfer (ECT) [25](#__RefHeading___Toc517464000)

7.13 Call Deflection (CD) [25](#__RefHeading___Toc517464001)

7.14 Completion of calls to busy subscriber (CCBS) [25](#__RefHeading___Toc517464002)

8 Interaction with network features [26](#__RefHeading___Toc517464003)

8.1 Customised Applications for Mobile network Enhanced Logic (CAMEL) [26](#__RefHeading___Toc517464004)

8.2 Support of Optimal Routeing (SOR) [26](#__RefHeading___Toc517464005)

8.3 Operator Determined Barring (ODB) [26](#__RefHeading___Toc517464006)

9 Information stored in the HLR [26](#__RefHeading___Toc517464007)

10 State transition model [26](#__RefHeading___Toc517464008)

11 Transfer of information from HLR to VLR [27](#__RefHeading___Toc517464009)

12 Information stored in VLR [27](#__RefHeading___Toc517464010)

13 Handover [27](#__RefHeading___Toc517464011)

Annex A (informative): Examples [28](#__RefHeading___Toc517464012)

Annex B (informative): Change history [32](#__RefHeading___Toc517464013)

# Foreword

This Technical Specification (TS) has been produced by the 3rd Generation Partnership Project (3GPP).

The present document gives the stage 2 description of the Multicall service within the 3GPP system.

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# 1 Scope

The present document gives the stage 2 description of the Multicall supplementary service.

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies.

[1] 3GPP TR 21.905: "3GPP Vocabulary".

[2] 3GPP TS 22.100: "UMTS Phase 1".

[3] 3GPP TS 22.105: "Services & Service capabilities".

[4] 3GPP TS 22.135: "Multicall Stage 1".

[5] 3GPP TS 23.009: "Handover procedures".

[6] 3GPP TS 23.011: "Technical realisation of supplementary services".

[7] 3GPP TS 23.018: "Basic call handling; Technical realization".

[8] 3GPP TS 23.083: "Call Waiting (CW) and Call Hold (HOLD) Supplementary Service - Stage 2".

[9] 3GPP TS 24.008: "Mobile radio interface layer 3 specification Core Network Protocol – Stage 3".

# 3 Definitions and abbreviations

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in TS 22.135 and the following apply.

**Speech Call:** speech call means one of TS11 (Telephony), TS12 (Emergency call), TS61 (Alternate speech and facsimile group 3).

## 3.2 Abbreviations

Abbreviations used in the present document are listed in TR 21.905.

# 4 Descriptions

## 4.1 Handling of Multicall

### 4.1.1 Provision

No special signalling procedures apply.

### 4.1.2 Withdrawal

No special signalling procedures apply.

### 4.1.3 Registration

The information flow for registration is shown in figure 1. The registration process is shown in figure 2.



Figure 1: Registration of Multicall



Figure 2: Process Register\_Multicall\_HLR

### 4.1.4 Erasure

No special signalling procedures apply.

### 4.1.5 Activation

The service provider shall provide an initial value for N**br\_**User when activating the service. No special signalling procedures apply.

### 4.1.6 Deactivation

No special signalling procedures apply.

### 4.1.7 Interrogation

The information flow for interrogation is shown in figure 3. The interrogation process is shown in figure 4.



Figure 3: Interrogation of Multicall



Figure 4: Process Interrogate\_Multicall\_VLR

## 4.2 Call related procedures

The procedures for basic call handling are specified in 3GPP TS 23.018. These shall also be used for Multicall.

### 4.2.1 MO call

Figure 5 shows the flow of information between network elements for an MO call:



Figure 5: Information flow for mobile originating call

### 4.2.2 MT call

Figure 6 and Figure 7 show the flow of information between network elements for an MT call:

- Case 1: When the MS requests a new bearer in call confirmed. (Figure 6).

- Case 2: When the MS requests a new bearer in Connect. (Figure 7).



Figure 6: Information flow for mobile terminating call (Case1)



Figure 7: Information flow for mobile terminating call (Case2)

## 4.3 Messages and their contents

This clause contains the detailed description of the information flows used by Multicall.

Each Information Element, IE, is marked as (M) Mandatory, (C) Conditional or (O) Optional. A mandatory information element shall always be present. A conditional information shall be present if certain conditions are fulfilled; if those conditions are not fulfilled it shall be absent. An optional information element may be present or absent, at the discretion of the application at the sending entity. This categorisation is a functional classification, i.e., stage 2 information and not a stage 3 classification to be used for the protocol.

The stage 2 and stage 3 message and information element names are not necessarily identical.

### 4.3.1 Messages between MS and MSC

Table 1 indicates messages between the MS and the MSC for mobile originating calls and mobile terminating calls. (Refer to TS 24.008).

The MS shall indicate the maximum number of bearers supported by the MS in the CC capabilities IE. The MS shall also indicate the maximum number of simultaneous speech bearers supported by the MS for future compatibility. For Release 99, the maximum number of simultaneous speech bearers is 1. If the MS does not indicate the maximum number of bearers the network shall assume it does not support Multicall.

The network supporting Multicall shall indicate the capability in the NW CC capabilities IE. If the NW CC capabilities IE is not sent from the network, the MS supporting Multicall shall assume that the network doesn't support Multicall. If an MS initiating an emergency call is located in a network that does not support Multicall, the MS shall release one or more existing call to ensure that the emergency call can be established.

Table 1: Messages between MS and MSC

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Message** | **Message sender** | Information element name | **Information element Required** | **Information element description** |
| Setup (MO) | MS | Stream Identifier | M | This information element indicates which bearer (new or existing) shall be used for the call. |
| CC Capabilities | C | For the first call, this information element shall be included to indicate the maximum number of bearers supported by the MS. |
| Emergency Setup | MS | Stream Identifier | M | This information element indicates which bearer (new or existing) shall be used for the call. |
| Call Confirmed | MS | Stream Identifier | M | This information element indicates whether a new bearer is requested, i.e. SI=value which is not used by any of the existing bearers , or no bearer is requested at that point in time, i.e. SI="no bearer". |
| CC Capabilities | C | For the first call, this information element shall be included to indicate the maximum number of bearers supported by the MS. |
| Connect (MT) | MS | Stream Identifier | C | This IE shall be present in the Connect message if the SI contained "No bearer" in the Call Confirmed message, otherwise shall be absent. |
| Setup (MT) | NW | NW CC Capabilities | C | This information element shall be present for the first call. |
| Call Proceeding | NW | NW CC Capabilities | C |

### 4.3.2 Messages on B interface (MSC-VLR)

#### 4.3.2.1 Send Info For Outgoing Call

This message is specified in 3GPP TS 23.018. The following additional information element is required:

|  |  |  |
| --- | --- | --- |
| Information element name | Required | Description |
| Total number of bearers in use | M | Total number includes the new bearer if requested for the call. |

#### 4.3.2.2 Send Info For Outgoing Call negative response

This message is specified in 3GPP TS 23.018. The following additional information element is required:

|  |  |  |
| --- | --- | --- |
| Information element name | Required | Description |
| Negative response information element | M | If the VLR detects that the OG call can not be permitted because Multicall limit set by the user is exceeded, it shall indicate " N**br**\_User is exceeded" as the negative response information element value.  If the VLR detects that the OG call can not be permitted because the user is not provisioned with Multicall, it shall indicate "Multicall not provisioned" as the negative response information element value. |

#### 4.3.2.3 Send Info For Incoming Call

This message is specified in TS 23.018.

#### 4.3.2.4 Send Info For Incoming Call ack

This message is specified in TS 23.018.

#### 4.3.2.5 Send Info For Incoming Call negative response

This message is specified in TS 23.018.

#### 4.3.2.6 Complete Call

This message is specified in TS 23.018.

#### 4.3.2.7 Complete Call ack

This message is specified in TS 23.018.

#### 4.3.2.8 Page MS

This message is specified in 3GPP TS 23.018. The following additional information element is required:

|  |  |  |
| --- | --- | --- |
| Information element name | Required | Description |
| N**br**\_User | M | Shall be present if the subscriber is provisioned with Multicall. |

#### 4.3.2.9 Page MS negative response

This message is specified in 3GPP TS 23.018. The following additional information element is required:

|  |  |  |
| --- | --- | --- |
| Information element name | Required | Description |
| Basic service list | C | If the MSC detects subscriber busy (More Calls Possible), the Basic service list shall be included, see Table 2. |

Table 2: Basic Service List setting

|  |  |  |
| --- | --- | --- |
| **Condition** | | **Setting** |
| The terminating call type is speech | There exists an active or held speech call | Basic service of active call via the same bearer as the existing speech call. If an active call does not exist via the same bearer as the existing speech call "speech" shall be indicated. |
| There exists no speech call | All basic services of ongoing calls |
| The terminating call type is not speech | | All basic services of ongoing calls |

#### 4.3.2.10 Process Access Request

This message is specified in TS 23.018.

#### 4.3.2.11 Process Access Request ack

This message is specified in TS 23.018.

#### 4.3.2.12 Process Access Request negative response

This message is specified in TS 23.018.

#### 4.3.2.13 Search For MS

This message is specified in 3GPP TS 23.018. The following additional information element is required:

|  |  |  |
| --- | --- | --- |
| Information element name | Required | Description |
| N**br**\_User | M | Shall be present if the subscriber is provisioned with Multicall. |

#### 4.3.2.14 Search For MS ack

This message is specified in 3GPP TS 23.018.

#### 4.3.2.15 Search For MS negative response

This message is specified in 3GPP TS 23.018. The following additional information element is required:

|  |  |  |
| --- | --- | --- |
| Information element name | Required | Description |
| Basic service list | C | If the MSC detects subscriber busy (More Calls Possible), the Basic service list shall be included, see Table 2. |

# 5 Network entity functions

The following SDL diagrams describe the procedures within individual network entities for handling Multicall.

## 5.1 General

The MSC shall check whether the maximum number of bearers has been reached for both MO and MT call. In counting of the current number of bearers for the target subscriber, the following situations are counted as an active bearer.

- Call in set-up.

- Established call.

- Call on hold.

- Call on hold and established call on the same bearer.

- Call on hold and MO call in Setup on the same bearer.

## 5.2 MO call

### 5.2.1 Functional requirements of serving MSC

Figure 8: Procedure Check\_OG\_Multicall\_MSC.

This procedure is called when the MSC receives a Setup message from the MS. After handover procedure completion to another MSC, N**br**\_SN as defined for the target MSC shall overwrite the previous N**br**\_SN.



Figure 8: Procedure Check\_OG\_Multicall\_MSC

### 5.2.2 Functional requirements of VLR

Figure 9: Procedure Check\_OG\_Multicall\_VLR.

This procedure is called when the VLR receives a Send Info For Outgoing Call message from the MSC.



Figure 9: Procedure Check\_OG\_Multicall\_VLR

## 5.3 MT call

### 5.3.1 Functional requirements of serving MSC

Figure 10: Procedure Check\_MT\_Multicall\_MSC.

This procedure is called when the MSC receives a Page MS message or a Search For MS message from the VLR. The maximum number of bearers (N**br**) indicates the minimum value of N**br**\_User, N**br**\_SN and N**br**\_UE. After handover to another MSC is completed, N**br**\_SN, as defined for the target MSC, shall overwrite the previous N**br**\_SN.

"Call in Setup" means that the MS is engaged in at least one call that has not reached the established phase (called party answer).

The test "Call waiting" takes the "Yes" exit if a waiting call has been offered to the subscriber but the outcome of offering the call has not been determined.

Figure 11: Procedure Establish\_Terminating\_TCH\_Multicall.

This procedure is called when the MSC receives a Call Confirmed or a Connect message from the MS. If the MS indicates "No bearer" as the value of the Stream Identifier in the Call Confirmed message the test "Bearer allocation pending" takes the "Yes" exit.

Figure 12: Procedure MC\_TCH\_Check

This procedure is called when the MSC needs to establish a terminating TCH.



Figure 10: Procedure Check\_MT\_Multicall\_MSC



Figure 11: Procedure Establish\_Terminating\_TCH\_Multicall



Figure 12: Procedure MC\_TCH\_Check

### 5.3.2 Functional requirements of VLR

Figure 13: Procedure Get\_CW\_Subscription\_Info\_Multicall\_VLR.

This procedure is called when the VLR receives a Page MS negative response message or a Search For MS negative response message with the negative response IE set to "Busy (More Calls Possible)".



Figure 13: Procedure Get\_CW\_Subscription\_Info\_Multicall\_VLR

# 6 Interaction with telecommunication services

## 6.1 Speech

The Multicall supplementary service does not provide multiple traffic channels for speech calls. Refer to Procedure Check\_OG\_Multicall\_MSC and Procedure Check\_MT\_Multicall\_MSC.

If N**br**\_UE is greater than N**br**\_SN, the mobile station may initiate an Emergency call even if N**br**\_SN has been reached. When the network receives an Emergency call Setup message from the mobile station:

- if N**br**\_SN has not been reached, the network shall accept it regardless of N**br**\_SB or N**br**\_User;

- if N**br**\_SN has been reached, the network shall reject the emergency call setup attempt. The MS shall release one or more existing calls and it shall re-initiate an Emergency call.

The MS shall ensure that an emergency call Setup request is acceptable to a serving network which does not support multicall, if necessary by releasing one or more existing calls.

## 6.2 Short message service

No impact.

## 6.3 Facsimile service

The Multicall supplementary service provides multiple traffic channels for facsimile service except for alternate speech and facsimile group 3.

## 6.4 Data circuit asynchronous

The Multicall supplementary service provides multiple traffic channels for data circuit asynchronous.

## 6.5 Data circuit synchronous

The Multicall supplementary service provides multiple traffic channels for data circuit synchronous.

## 6.6 Void

## 6.7 GPRS

No impact.

# 7 Interaction with other supplementary services

## 7.1 Line Identification services

No impact.

## 7.2 Call forwarding unconditional (CFU)

No impact.

## 7.3 Call forward on busy (CFB)

The condition NDUB occurs in accordance with the definition for multicall. (See TS 22.135).

## 7.4 Call forwarding on no reply (CFNRy)

No impact.

## 7.5 Call forwarding on MS not reachable (CFNRc)

No impact.

## 7.6 Call Hold (CH)

No impact.

## 7.7 Call Waiting (CW)

Call Waiting SS will be invoked under the conditions described in TS 22.135.

## 7.8 Multiparty service (MPTY)

No impact.

## 7.9 Closed user group (CUG)

No impact.

## 7.10 Advice Of Charge (AoC)

No impact.

## 7.11 Call Barring services

No impact.

## 7.12 Explicit call transfer (ECT)

No impact.

## 7.13 Call Deflection (CD)

No impact.

## 7.14 Completion of calls to busy subscriber (CCBS)

The NDUB condition occurs in accordance with the definition for multicall. (See 3GPP TS 22.135).

A subscriber provisioned with multicall is in the idle state when the subscriber has no ongoing (active or held) calls. CCBS requests in the destination B CCBS queue shall be processed if destination B is idle.

# 8 Interaction with network features

## 8.1 Customised Applications for Mobile network Enhanced Logic (CAMEL)

No impact.

## 8.2 Support of Optimal Routeing (SOR)

No impact.

## 8.3 Operator Determined Barring (ODB)

No impact.

# 9 Information stored in the HLR

The following logical states are applicable for Multicall (refer to TS 23.011 for an explanation of the notation):

|  |  |  |  |
| --- | --- | --- | --- |
| **Provisioning State** | **Registration State** | **Activation State** | **HLR Induction State** |
| (Not Provisioned, | Not Applicable, | Not Active, | Not Induced) |
| (Provisioned, | Registered, | Active and Operative, | Not Induced) |

The HLR shall store:

- The state of Multicall (which shall be one of the valid states listed above) per subscriber.

- The subscription option "maximum number of bearers N**br**\_SB" per subscriber:

- This subscription option takes a value in the range (2 – 7).

- The subscription option "maximum number of bearers N**br**\_User" per subscriber:

- This subscription option takes a value in the range (1 – N**br**\_SB).

# 10 State transition model

Figure 14 shows the successful cases of transition between the applicable logical states of Multicall. The state changes are caused by actions of the service provider.

Note that error cases are not shown in the diagram, as they normally do not cause a state change. Additionally, some successful requests may not cause a state change. Hence they are not shown in the diagram.



Figure 14: State transition model for Multicall

# 11 Transfer of information from HLR to VLR

If the provisioning state for Multicall is "Provisioned" then when the subscriber registers on a VLR the HLR shall send that VLR information about the logical state of Multicall, N**br\_**Userand N**br**\_SB.

If the logical state of Multicall, the subscription options N**br**\_SB or N**br\_**Userare changed while a subscriber is registered on a VLR then the HLR shall inform the VLR of the new logical state of Multicall, the new N**br\_**User or the new N**br**\_SB.

# 12 Information stored in VLR

The VLR shall store the service state information, N**br**\_SB and N**br\_**Useras received from the HLR.

# 13 Handover

In the case that the network supports Multicall, it shall be possible to handover multiple bearers (See TS 23.009).

Annex A (informative):  
Examples

The following table shows some examples:

**1 Mobile Originating Call (MO call).**

As an example: Nbr=2.

| **Current Status** | | | | **Additional MO call** | |
| --- | --- | --- | --- | --- | --- |
| **No** | **Status** | **Number of bearers** | **Number of calls** | **Speech** | **Data** |
| 1 | None | 0 | 0 | Acceptable | Acceptable |
| 2 | 1 Speech call(active) | 1 | 1 | Rejected | Acceptable |
| 3 | 1 Speech call(on hold) | 1 | 1 | Acceptable  (with same SI)  Rejected  (with another SI) | Acceptable |
| 4 | 1 Data call(active) | 1 | 1 | Acceptable | Acceptable |
| 5 | 1 Speech call(on hold)  1 Speech call(active) | 1 | 2 | Rejected | Acceptable |
| 6 | 1 Speech call(on hold)  1 Data call(active) | 1 | 2 | Rejected | Acceptable |
| 7 | Multiparty  (2-5 remote parties: active) | 1 | 2 - 5 | Rejected | Acceptable |
| 8 | Multiparty  (2-5 remote parties: on hold) | 1 | 2 - 5 | Acceptable  (with same SI)  Rejected  (with another SI) | Acceptable |
| 9 | 1 Speech call(active)  1 Data call(active) | 2 | 2 | Rejected | Rejected |
| 10 | 1 Speech call(on hold)  1 Data call(active) | 2 | 2 | Acceptable  (with same SI as speech call)  Rejected  (with another SI) | Acceptable  (with same SI as speech call)  Rejected  (with another SI) |
| 11 | 1 Speech call(on hold)  1 Speech call(active)  1 Data call(active) | 2 | 3 | Rejected | Rejected |
| 12 | 2 Data call(active) | 2 | 2 | Rejected | Rejected |
| 13 | 1 Speech call(on hold)  2 Data call(active) | 2 | 3 | Rejected | Rejected |
| 14 | Multiparty  (2-5 remote parties: active)  1 Data call(active) | 2 | 3 - 6 | Rejected | Rejected |
| 15 | Multiparty  (2-5 remote parties: on hold)  1 Data call(active) | 2 | 3 - 6 | Acceptable  (with same SI as speech call)  Rejected  (with another SI) | Acceptable  (with same SI as speech call)  Rejected  (with another SI) |

**2 Mobile Terminated Call (MT call).**

As an example: Nbr=2 (CW is not active).

| **Current Status** | | | | **Additional MT call** | |
| --- | --- | --- | --- | --- | --- |
| **No** | **Status** | **Number of bearers** | **Number of calls** | **Speech** | **Data** |
| 1 | None | 0 | 0 | Offered | Offered |
| 2 | 1 Speech call(active) | 1 | 1 | Busy | Offered |
| 3 | 1 Speech call(on hold) | 1 | 1 | Busy | Offered |
| 4 | 1 Data call(active) | 1 | 1 | Offered | Offered |
| 5 | 1 Speech call(on hold)  1 Speech call(active) | 1 | 2 | Busy | Offered |
| 6 | 1 Speech call(on hold)  1 Data call(active) | 1 | 2 | Busy | Offered |
| 7 | Multiparty  (2-5 remote parties: active) | 1 | 2 - 5 | Busy | Offered |
| 8 | Multiparty  (2-5 remote parties: on hold) | 1 | 2 - 5 | Busy | Offered |
| 9 | 1 Speech call(active)  1 Data call(active) | 2 | 2 | Busy | Busy |
| 10 | 1 Speech call(on hold)  1 Data call(active) | 2 | 2 | Busy | Busy |
| 11 | 1 Speech call(on hold)  1 Speech call(active)  1 Data call(active) | 2 | 3 | Busy | Busy |
| 12 | 2 Data call(active) | 2 | 2 | Busy | Busy |
| 13 | 1 Speech call(on hold)  2 Data call(active) | 2 | 3 | Busy | Busy |
| 14 | Multiparty  (2-5 remote parties: active)  1 Data call(active) | 2 | 3 - 6 | Busy | Busy |
| 15 | Multiparty  (2-5 remote parties: on hold)  1 Data call(active) | 2 | 3 - 6 | Busy | Busy |

**3 Call Waiting (CW).**

As an example: Nbr=2 (CW is provisioned).

| **Current Status** | | | | **Additional MT call** | |
| --- | --- | --- | --- | --- | --- |
| **No** | **Status** | **CW status for speech** | **CW status for data** | **Speech** | **Data** |
| 1 | None | - | - | - | - |
| 2 | 1 Speech call(active) | active | - | CW offered | MT offered |
| Not active | - | busy | MT offered |
| 3 | 1 Speech call(on hold) | active | - | CW offered | MT offered |
| Not active |  | busy | MT offered |
| 4 | 1 Data call(active) | - | active | MT offered | MT offered |
| Not active | MT offered | MT offered |
| 5 | 1 Speech call(on hold) via bearer A  1 Speech call(active) via bearer A | active | active | CW offered | MT offered |
| active | Not active | CW offered | MT offered |
| Not active | active | busy | MT offered |
| Not active | Not active | busy | MT offered |
| 6 | 1 Speech call(on hold) via bearer A  1 Data call(active) via bearer A | active | active | CW offered | MT offered |
| active | Not active | busy | MT offered |
| Not active | active | CW offered | MT offered |
| Not active | Not active | busy | MT offered |
| 7 | Multiparty via bearer A  (2-5 remote parties: active) | active | - | CW offered | MT offered |
| Not active | - | Busy | MT offered |
| 8 | Multiparty via bearer A  (2-5 remote parties: on hold) | active | - | CW offered | MT offered |
| Not active | - | busy | MT offered |
| 9 | 1 Speech call(active) via bearer A  1 Data call(active) via bearer B | active | active | CW offered | CW offered |
| active | Not active | CW offered | CW offered |
| Not active | active | busy | CW offered |
| Not active | Not active | busy | busy |
| 10 | 1 Speech call(on hold) via bearer A  1 Data call(active) via bearer B | active | active | CW offered | CW offered |
| active | Not active | CW offered | CW offered |
| Not active | active | busy | CW offered |
| Not active | Not active | busy | busy |
| 11 | 1 Speech call(on hold) via bearer A  1 Speech call(active) via bearer A  1 Data call(active) via bearer B | active | active | CW offered | CW offered |
| active | Not active | CW offered | CW offered |
| Not active | active | busy | CW offered |
| Not active | Not active | busy | busy |
| 12 | 2 Data call(active) | - | active | CW offered | CW offered |
| - | Not active | busy | busy |
| 13 | 1 Speech call(on hold) via bearer A  2 Data call(active) via bearer A and B | - | active | CW offered | CW offered |
| - | Not active | Busy | Busy |
| 14 | Multiparty via bearer A  (2-5 remote parties: active)  1 Data call(active) via bearer B | active | active | CW offered | CW offered |
| active | Not active | CW offered | CW offered |
| Not active | active | busy | CW offered |
| Not active | Not active | busy | busy |
| 15 | Multiparty via bearer A  (2-5 remote parties: on hold)  1 Data call(active) via bearer B | active | active | CW offered | CW offered |
| active | Not active | CW offered | CW offered |
| Not active | active | busy | CW offered |
| Not active | Not active | busy | busy |

Annex B (informative):  
Change history

| TSG CN# | Spec | CR | <Phase> | New Version | Subject/Comment |
| --- | --- | --- | --- | --- | --- |
| CN#07 | 23.135 |  | R99 | 3.0.0 | Approved at TSGN#07 |
| CN#08 | 23.135 | 001r1 | R99 | 3.1.0 | Clean-up and corrections for Multicall Stage 2 |
| CN#09 | 23.135 | 002r4 | R99 | 3.2.0 | Requirement on Network to Tear Down Calls to Accept EC in Multicall |
| CN#09 | 23.135 | 004r1 | R99 | 3.2.0 | Correction to MT\_Multicall SDL |
| CN#09 | 23.135 | 003r1 | Rel-4 | 4.0.0 | Inclusion of call hold in basic call handling |
| CN#16 | 23.135 |  | Rel-5 | 5.0.0 | Release 5 after CN#16 |
| CN#26 | 23.135 |  | Rel-6 | 6.0.0 | Release 6 after CN#26 |
| CT#36 | 23.135 |  | Rel-7 | 7.0.0 | Upgraded unchanged from Rel-6 |
| CT#42 | 23.135 |  | Rel-8 | 8.0.0 | Upgraded unchanged from Rel-7 |
| CT#46 | 23.135 | - | Rel-9 | 9.0.0 | Update to Rel-9 version (MCC) |
| 2011-03 | 23.135 | - | Rel-10 | 10.0.0 | Update to Rel-10 version (MCC) |
| 2012-09 | 23.135 | - | Rel-11 | 11.0.0 | Update to Rel-11 version (MCC) |
| 2014-09 | 23.135 | - | Rel-12 | 12.0.0 | Update to Rel-12 version (MCC) |
| 2015-12 | 23.135 |  | Rel-13 | 13.0.0 | Update to Rel-13 version (MCC) |
| 2017-03 | 23.135 | - | Rel-14 | 14.0.0 | Update to Rel-14 version (MCC) |
| 2018-06 | 23.135 | - | Rel-15 | 15.0.0 | Update to Rel-15 version (MCC) |
| 2020-07 | 23.135 | - | Rel-16 | 16.0.0 | Update to Rel-16 version (MCC) |