3GPP TS 24.285 V16.0.0 (2020-07)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Core Network and Terminals;

Allowed Closed Subscriber Group (CSG) list;

Management Object (MO)

(Release 16)

* *

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP..  
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.  
This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

Keywords

UMTS, LTE, Supplementary Service, Management

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword [4](#__RefHeading___Toc280546707)

1 Scope [5](#__RefHeading___Toc280546708)

2 References [5](#__RefHeading___Toc280546709)

3 Definitions and abbreviations [5](#__RefHeading___Toc280546710)

3.1 Definitions [5](#__RefHeading___Toc280546711)

3.2 Abbreviations [5](#__RefHeading___Toc280546712)

4 Allowed CSG List Management Object [6](#__RefHeading___Toc280546713)

5 Management Object parameters [6](#__RefHeading___Toc280546714)

5.1 General [6](#__RefHeading___Toc280546715)

5.2 Node: *<X>* [6](#__RefHeading___Toc280546716)

5.3 /*<X>*/AllowedCSGEntries [7](#__RefHeading___Toc280546717)

5.4 /*<X>*/AllowedCSGEntries/<X> [7](#__RefHeading___Toc280546718)

5.5 /<X>/AllowedCSGEntries/<X>/PLMN\_ID [7](#__RefHeading___Toc280546719)

5.6 /*<X>*/AllowedCSGEntries/<X>/CSG-entries [7](#__RefHeading___Toc280546720)

5.7 /*<X>*/AllowedCSGEntries/<X>/CSG-entries/<X> [7](#__RefHeading___Toc280546721)

5.8 /<X>/AllowedCSGEntries/<X>/CSG-entries/<X>/CSG\_ID [8](#__RefHeading___Toc280546722)

5.9 /*<X>*/AllowedCSGEntries/<X>/CSG-entries/<X>/HNB\_Name [8](#__RefHeading___Toc280546723)

5.10 /<X>/AllowedCSGEntries/<X>/CSG-entries/<X>/CSG\_Type [8](#__RefHeading___Toc280546724)

5.11 /*<X>*/OperatorCSGEntries [8](#__RefHeading___Toc280546725)

5.12 /*<X>*/OperatorCSGEntries/<X> [9](#__RefHeading___Toc280546726)

5.13 /<X>/OperatorCSGEntries/<X>/PLMN\_ID [9](#__RefHeading___Toc280546727)

5.14 /*<X>*/OperatorCSGEntries/<X>/CSG-entries [9](#__RefHeading___Toc280546728)

5.15 /*<X>*/OperatorCSGEntries/<X>/CSG-entries/<X> [9](#__RefHeading___Toc280546729)

5.16 /<X>/OperatorCSGEntries/<X>/CSG-entries/<X>/CSG\_ID [9](#__RefHeading___Toc280546730)

5.17 /*<X>*/OperatorCSGEntries/<X>/CSG-entries/<X>/HNB\_Name [10](#__RefHeading___Toc280546731)

5.18 /<X>/ OperatorCSGEntries /<X>/CSG-entries/<X>/CSG\_Type [10](#__RefHeading___Toc280546732)

5.19 /*<X>*/Ext/ [10](#__RefHeading___Toc280546733)

5.20 /<X>/OperatorCSGEntries/<X>/OperatorCSGEntries\_Only\_thisPLMN [10](#__RefHeading___Toc280546734)

5.21 /<X>/OperatorCSGEntries/OperatorCSGEntries\_Only [11](#__RefHeading___Toc280546735)

Annex A (informative): Management Object DDF [12](#__RefHeading___Toc280546736)

Annex B (informative): Change history [16](#__RefHeading___Toc280546737)

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# 1 Scope

The present document specifies an Allowed Closed Subscriber Group (CSG) List Management Object (MO).

The Allowed CSG List MO is compatible with the OMA Device Management (DM) protocol specifications, version 1.2 and upwards, and is defined using the OMA DM Device Description Framework (DDF) as described in the Enabler Release Definition OMA-ERELD-DM-V1\_2 [5].

The Allowed CSG List MO consists of relevant parameters for that can be used by the UE to select the appropriate CSG cell based on its subscription.

The Allowed CSG List MO defines the relevant parameters related to the Allowed CSG List and to the Operator CSG List.

The usage of the Allowed CSG List for in the idle mode process and the mobility management procedure is defined in 3GPP TS 23.122 [2], 3GPP TS 24.008 [3] and 3GPP TS 24.301 [4].

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[1A] 3GPP TS 23.003: "Numbering, addressing and identification".

[2] 3GPP TS 23.122: "Non-Access-Stratum functions related to Mobile Station (MS) in idle mode".

[3] 3GPP TS 24.008: "Mobile Radio Interface Layer 3 specification; Core Network Protocols; Stage 3"

[4] 3GPP TS 24.301: " Non-Access-Stratum (NAS) protocol for Evolved Packet System (EPS); Stage 3"

[5] OMA-ERELD-DM-V1\_2: "Enabler Release Definition for OMA Device Management".

# 3 Definitions and abbreviations

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in 3GPP TR 21.905 [1] apply.

## 3.2 Abbreviations

For the purposes of the present document, the following abbreviations apply:

CSG Closed Subscriber Group

DM Device Management

HNB Home NodeB/eNodeB

MO Management Object

OMA Open Mobile Alliance

PLMN Public Land Mobile Network

UE User Equipment

# 4 Allowed CSG List Management Object

The Allowed CSG List Management Object (MO) is used to manage the list of allowed CSG IDs, the Operator CSG IDs and the related restricted access information at UE.

The Management Object Identifier is: urn:oma:mo:ext-3gpp-csg:1.0.

The OMA DM Access Control List (ACL) property mechanism (see OMA-ERELD-DM-V1\_2 [5]) may be used to grant or deny access rights to OMA DM servers in order to modify nodes and leaf objects of the Allowed CSG list MO.

The following nodes and leaf objects are possible under the Allowed CSG List node as described in figure 4-1:



Figure 4-1: The Allowed CSG List Management Object

When a UE receives an Allowed CSG List Management Object (MO) containing the Allowed CSG List, it shall update its Allowed CSG list stored in a USIM or in a non-volatile memory in the ME.

When a UE receives an Allowed CSG List Management Object (MO) containing the Operator CSG List, it shall update the Operator CSG List stored in a non-volatile memory in the ME.

# 5 Management Object parameters

## 5.1 General

This clause describes the parameters for the Allowed CSG List Management Object (MO).

## 5.2 Node: *<X>*

This interior node acts as a placeholder for zero or one accounts for a fixed node.

- Occurrence: ZeroOrOne

- Format: node

- Access Types: Get

- Values: N/A

## 5.3 /*<X>*/AllowedCSGEntries

The AllowedCSGEntries interior node is used to allow a reference to a list of allowed CSG entries.

- Occurrence: One

- Format: node

- Access Types: Get

- Values: N/A

## 5.4 /*<X>*/AllowedCSGEntries/<X>

This run-time node acts as a placeholder for one or more allowed CSG entries.

- Occurrence: OneOrMore

- Format: node

- Access Types: Get

- Values: N/A

## 5.5 /<X>/AllowedCSGEntries/<X>/PLMN\_ID

The PLMN\_ID leaf represents a PLMN Identifier

- Occurrence: One

- Format: chr

- Access Types: Get, Replace

- Values: <PLMN Identifier>

The value of the PLMN Identifier shall be a PLMN-Id as specified in 3GPP TS 23.003 [1A].

## 5.6 /*<X>*/AllowedCSGEntries/<X>/CSG-entries

The CSG-entries interior node is used to allow a reference to a list of allowed CSG entries in a PLMN.

- Occurrence: One

- Format: node

- Access Types: Get

- Values: N/A

## 5.7 /*<X>*/AllowedCSGEntries/<X>/CSG-entries/<X>

This run-time node acts as a placeholder for one or more CSG entries (the CSG Identity, its related HNB Name and CSG Type) in a PLMN.

- Occurrence: OneOrMore

- Format: node

- Access Types: Get

- Values: N/A

## 5.8 /<X>/AllowedCSGEntries/<X>/CSG-entries/<X>/CSG\_ID

The CSG\_ID leaf represents a CSG Identifier.

- Occurrence: One

- Format: bin

- Access Types: Get, Replace

- Values: <CSG Identifier>

The value of the CSG Identifier shall be coded as a CSG-ID as specified in 3GPP TS 23.003 [1A].

## 5.9 /*<X>*/AllowedCSGEntries/<X>/CSG-entries/<X>/HNB\_Name

The HNB\_name leaf represents a HNB Name.

- Occurrence: ZeroOrOne

- Format: chr

- Access Types: Get, Replace

- Values: <HNB Name>

The value of the HNB Name shall be coded as specified in 3GPP TS 23.003 [1A].

## 5.10 /<X>/AllowedCSGEntries/<X>/CSG-entries/<X>/CSG\_Type

The CSG Type leaf represents a CSG type.

- Occurrence: ZeroOrOne

- Format: chr

- Access Types: Get, Replace

- Values: <CSG Type>

The value of the CSG Type shall be coded as specified in 3GPP TS 23.003 [1A].

## 5.11 /*<X>*/OperatorCSGEntries

The OperatorCSGEntries interior node is used to allow a reference to a list of operator CSG entries.

- Occurrence: ZeroOrOne

- Format: node

- Access Types: Get

- Values: N/A

## 5.12 /*<X>*/OperatorCSGEntries/<X>

This run-time node acts as a placeholder for one or more operator CSG entries.

- Occurrence: OneOrMore

- Format: node

- Access Types: Get

- Values: N/A

## 5.13 /<X>/OperatorCSGEntries/<X>/PLMN\_ID

The PLMN\_ID leaf represents a PLMN Identifier.

- Occurrence: One

- Format: chr

- Access Types: Get, Replace

- Values: <PLMN Identifier>

The value of the PLMN Identifier shall be a PLMN-Id as specified in 3GPP TS 23.003 [1A].

## 5.14 /*<X>*/OperatorCSGEntries/<X>/CSG-entries

The CSG-entries interior node is used to allow a reference to a list of operator CSG entries in a PLMN.

- Occurrence: One

- Format: node

- Access Types: Get

- Values: N/A

## 5.15 /*<X>*/OperatorCSGEntries/<X>/CSG-entries/<X>

This run-time node acts as a placeholder for one or more CSG entries (the CSG Identity, its related HNB Name and CSG Type) in a PLMN.

- Occurrence: OneOrMore

- Format: node

- Access Types: Get

- Values: N/A

## 5.16 /<X>/OperatorCSGEntries/<X>/CSG-entries/<X>/CSG\_ID

The CSG\_ID leaf represents a CSG Identifier.

- Occurrence: One

- Format: bin

- Access Types: Get, Replace

- Values: <CSG Identifier>

The value of the CSG Identifier shall be coded as a CSG-ID as specified in 3GPP TS 23.003 [1A].

## 5.17 /*<X>*/OperatorCSGEntries/<X>/CSG-entries/<X>/HNB\_Name

The HNB\_name leaf represents a HNB Name.

- Occurrence: ZeroOrOne

- Format: chr

- Access Types: Get, Replace

- Values: <HNB Name>

The value of the HNB Name shall be coded as specified in 3GPP TS 23.003 [1A].

## 5.18 /<X>/ OperatorCSGEntries /<X>/CSG-entries/<X>/CSG\_Type

The CSG Type leaf represents a CSG type.

- Occurrence: ZeroOrOne

- Format: chr

- Access Types: Get, Replace

- Values: <CSG Type>

The value of the CSG Type shall be coded as specified in 3GPP TS 23.003 [1A].

## 5.19 /*<X>*/Ext/

The Ext is an interior node for where the vendor specific information about the Allowed CSG List MO is being placed (vendor meaning application vendor, device vendor etc.). Usually the vendor extension is identified by vendor specific name under the ext node. The tree structure under the vendor identified is not defined and can therefore include one or more un-standardized sub-trees.

- Occurrence: ZeroOrOne

- Format: node

- Access Types: Get, Replace

- Values: N/A

## 5.20 /<X>/OperatorCSGEntries/<X>/OperatorCSGEntries\_Only\_thisPLMN

The OperatorCSGEntries\_Only\_thisPLMN leaf is used to indicate which CSGs the UE is configured to present to the user for a certain PLMN ID during manual CSG selection.

- Occurrence: ZeroOrOne

- Format: bool

- Access Types: Get, Replace

- Values: "false", "true"

"false" – Indicates that HPLMN has configured the UE to present to the user CSGs for the PLMN indicated in PLMN\_ID leaf without any restriction.

"true" – Indicates that HPLMN has configured the UE to present to the user only the CSGs in the Operator CSG List for the PLMN indicated in PLMN\_ID leaf.

NOTE: For the value "true", if the HPLMN has not included any CSG entry for the PLMN indicated in PLMN\_ID leaf, the UE is implicitly configured to not display any CSG for this PLMN during manual CSG selection.

If the OperatorCSGEntries\_Only\_thisPLMN leaf is not included, then its value is equal to the value of OperatorCSGEntries\_Only leaf.

## 5.21 /<X>/OperatorCSGEntries/OperatorCSGEntries\_Only

The OperatorCSGEntries\_Only leaf is used to indicate which CSGs the UE is configured to present to the user during manual CSG selection for every PLMN not included in the OperatorCSGEntries leaf and for every PLMN for which an OperatorCSGEntries\_Only\_thisPLMN leaf was not included.

- Occurrence: ZeroOrOne

- Format: bool

- Access Types: Get, Replace

- Values: "false", "true"

"false" – Indicates that the HPLMN has configured the UE, for every PLMN not included in any PLMN\_ID leaf in the OperatorCSGEntries leaf or for which an OperatorCSGEntries\_Only\_thisPLMN leaf was not included, to present to the user CSGs without any restriction.

"true" – Indicates that the HPLMN has configured the UE, for every PLMN not included in any PLMN\_ID leaf in the OperatorCSGEntries leaf or any PLMN for which an OperatorCSGEntries\_Only\_thisPLMN leaf was not included, to present to the user only the CSGs in the Operator CSG List.

NOTE: For the value "true", if the HPLMN has not included any CSG entry in the OperatorCSGList for a certain PLMN, the UE is implicitly configured to not display any CSG for that PLMN during manual CSG selection.

If the OperatorCSGEntries\_Only leaf is not included, the default OperatorCSGEntries\_Only value is "false".

Annex A (informative):  
Management Object DDF

This DDF is the standardized minimal set. A vendor can define its own DDF for the complete device. This DDF can include more features than this minimal standardized version.

<?xml version="1.0" encoding="UTF-8"?>

<!DOCTYPE MgmtTree PUBLIC "-//OMA//DTD-DM-DDF 1.2//EN"

"http://www.openmobilealliance.org/tech/DTD/dm\_ddf-v1\_2.dtd">

<MgmtTree>

<VerDTD>1.2</VerDTD>

<Node>

<NodeName/>

<DFProperties>

<AccessType> <Get/> </AccessType>

<DFFormat> <node/> </DFFormat>

<Occurrence> <ZeroOrOne/> </Occurrence>

<DFTitle>Root Node of the UE Allowed CSG List</DFTitle>

<DFType>

<DDFName>urn:oma:ext-3gpp-csg:1.0</DDFName>

</DFType>

</DFProperties>

<Node>

<NodeName>AllowedCSGEntries</NodeName>

<DFProperties>

<AccessType> <Get/> </AccessType>

<DFFormat> <node/> </DFFormat>

<Occurrence> <One/> </Occurrence>

<DFTitle>This node specifies the parent node for allowed CSG entries</DFTitle>

<DFType> <MIME>text/plain</MIME> </DFType>

</DFProperties>

<Node>

<NodeName/>

<DFProperties>

<AccessType> <Get/> </AccessType>

<DFFormat> <node/> </DFFormat>

<Occurrence> <OneOrMore/> </Occurrence>

<DFTitle>This node specifies the parent node for PLMN entries</DFTitle>

<DFType> <MIME>text/plain</MIME> </DFType>

</DFProperties>

<Node>

<NodeName>PLMN\_ID</NodeName>

<DFProperties>

<AccessType> <Get/> <Replace/></AccessType>

<DFFormat> <chr/> </DFFormat>

<Occurrence> <One/> </Occurrence>

<DFTitle>This leaf specifies the PLMN ID</DFTitle>

<DFType> <MIME>text/plain</MIME> </DFType>

</DFProperties>

</Node>

<Node>

<NodeName>CSG-entries</NodeName>

<DFProperties>

<AccessType> <Get/> </AccessType>

<DFFormat> <node/> </DFFormat>

<Occurrence> <One/> </Occurrence>

<DFTitle>This node specifies the parent node for CSG entries</DFTitle>

<DFType> <MIME>text/plain</MIME> </DFType>

</DFProperties>

<Node>

<NodeName/>

<DFProperties>

<AccessType> <Get/> </AccessType>

<DFFormat> <node/> </DFFormat>

<Occurrence> <OneOrMore/> </Occurrence>

<DFTitle>This node specifies CSG entries for specific PLMN</DFTitle>

<DFType> <MIME>text/plain</MIME> </DFType>

</DFProperties>

<Node>

<NodeName>CSG\_ID</NodeName>

<DFProperties>

<AccessType> <Get/> <Replace/></AccessType>

<DFFormat> <bin/> </DFFormat>

<Occurrence> <One/> </Occurrence>

<DFTitle>This leaf specifies the CSG identifier</DFTitle>

<DFType> <MIME>text/plain</MIME> </DFType>

</DFProperties>

</Node>

<Node>

<NodeName> HNB\_Name </NodeName>

<DFProperties>

<AccessType> <Get /> <Replace/></AccessType>

<DFFormat> <chr/> </DFFormat>

<Occurrence> <ZeroOrOne/> </Occurrence>

<DFTitle>This leaf node specifies the HNB Name</DFTitle>

<DFType> <MIME>text/plain</MIME> </DFType>

</DFProperties>

</Node>

<Node>

<NodeName> CSG Type </NodeName>

<DFProperties>

<AccessType> <Get /> <Replace/></AccessType>

<DFFormat> <chr/> </DFFormat>

<Occurrence> <ZeroOrOne/> </Occurrence>

<DFTitle>This leaf node specifies the CSG Type</DFTitle>

<DFType> <MIME>text/plain</MIME> </DFType>

</DFProperties>

</Node>

</Node>

</Node>

</Node>

</Node>

<Node>

<NodeName>OperatorCSGEntries</NodeName>

<DFProperties>

<AccessType> <Get/> </AccessType>

<DFFormat> <node/> </DFFormat>

<Occurrence> <ZeroOrOne/> </Occurrence>

<DFTitle>This node specifies the parent node for operator CSG entries</DFTitle>

<DFType> <MIME>text/plain</MIME> </DFType>

</DFProperties>

<Node>

**<NodeName>OperatorCSGEntries\_Only</NodeName>**

<DFProperties>

<AccessType> <Get/> <Replace/></AccessType>

<DFFormat> <bool/> </DFFormat>

<Occurrence> <ZeroOrOne /> </Occurrence>

<DFTitle>This leaf specifies which CSGs to display to the user</DFTitle>

<DFType> <MIME>text/plain</MIME> </DFType>

</DFProperties>

</Node>

<Node>

<NodeName/>

<DFProperties>

<AccessType> <Get/> </AccessType>

<DFFormat> <node/> </DFFormat>

<Occurrence> <OneOrMore/> </Occurrence>

<DFTitle>This node specifies the parent node for PLMN entries</DFTitle>

<DFType> <MIME>text/plain</MIME> </DFType>

</DFProperties>

<Node>

<NodeName>PLMN\_ID</NodeName>

<DFProperties>

<AccessType> <Get/> <Replace/></AccessType>

<DFFormat> <chr/> </DFFormat>

<Occurrence> <One/> </Occurrence>

<DFTitle>This leaf specifies the PLMN ID</DFTitle>

<DFType> <MIME>text/plain</MIME> </DFType>

</DFProperties>

</Node>

<Node>

<NodeName>OperatorCSGEntries\_Only\_thisPLMN</NodeName>

<DFProperties>

<AccessType> <Get/> <Replace/></AccessType>

<DFFormat> <bool/> </DFFormat>

<Occurrence> <ZeroOrOne /> </Occurrence>

<DFTitle>This leaf specifies which CSGs to display to the user</DFTitle>

<DFType> <MIME>text/plain</MIME> </DFType>

</DFProperties>

</Node>

<Node>

<NodeName>CSG-entries</NodeName>

<DFProperties>

<AccessType> <Get/> </AccessType>

<DFFormat> <node/> </DFFormat>

<Occurrence> <One/> </Occurrence>

<DFTitle>This node specifies the parent node for CSG entries</DFTitle>

<DFType> <MIME>text/plain</MIME> </DFType>

</DFProperties>

<Node>

<NodeName/>

<DFProperties>

<AccessType> <Get/> </AccessType>

<DFFormat> <node/> </DFFormat>

<Occurrence> <OneOrMore/> </Occurrence>

<DFTitle>This node specifies CSG entries for specific PLMN</DFTitle>

<DFType> <MIME>text/plain</MIME> </DFType>

</DFProperties>

<Node>

<NodeName>CSG\_ID</NodeName>

<DFProperties>

<AccessType> <Get/> <Replace/></AccessType>

<DFFormat> <bin/> </DFFormat>

<Occurrence> <One/> </Occurrence>

<DFTitle>This leaf specifies the CSG identifier</DFTitle>

<DFType> <MIME>text/plain</MIME> </DFType>

</DFProperties>

</Node>

<Node>

<NodeName> HNB\_Name </NodeName>

<DFProperties>

<AccessType> <Get /> <Replace/></AccessType>

<DFFormat> <chr/> </DFFormat>

<Occurrence> <ZeroOrOne/> </Occurrence>

<DFTitle>This leaf node specifies the HNB Name</DFTitle>

<DFType> <MIME>text/plain</MIME> </DFType>

</DFProperties>

</Node>

<Node>

<NodeName> CSG Type </NodeName>

<DFProperties>

<AccessType> <Get /> <Replace/></AccessType>

<DFFormat> <chr/> </DFFormat>

<Occurrence> <ZeroOrOne/> </Occurrence>

<DFTitle>This leaf node specifies the CSG Type</DFTitle>

<DFType> <MIME>text/plain</MIME> </DFType>

</DFProperties>

</Node>

</Node>

</Node>

</Node>

</Node>

<Node>

<NodeName>Ext</NodeName>

<DFProperties>

<AccessType>

<Get/>

</AccessType>

<DFFormat>

<node/>

</DFFormat>

<Occurrence>

<ZeroOrOne/>

</Occurrence>

<Scope>

<Permanent/>

</Scope>

<DFTitle>A collection of all extension objects</DFTitle>

<DFType>

<DDFName/>

</DFType>

</DFProperties>

</Node>

</Node>

</MgmtTree>

Annex B (informative):  
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **TSG #** | **TSG Doc.** | **CR** | **Rev** | **Subject/Comment** | **Old** | **New** |
| 2008-09 |  |  |  |  | Version 0.0.1: Preliminary proposal |  | 0.0.1 |
| 2008-10 |  |  |  |  | Version 0.0.2: TS number is added | 0.0.1 | 0.0.2 |
| 2008-11 |  |  |  |  | C1-085374 | 0.0.2 | 0.1.0 |
| 2008-11 |  |  |  |  | Editorial corrections | 0.1.0 | 0.1.1 |
| 2008-11 |  |  |  |  | Version 1.0.0 created for presentation to CT#42 for information | 0.1.1 | 1.0.0 |
| 2009-02 |  |  |  |  | C1-090705 | 1.0.0 | 1.1.0 |
| 2009-02 | CT-43 |  |  |  | Version 2.0.0 created for presentation to CT#43 for approval | 1.1.0 | 2.0.0 |
| 2009-03 | CT-43 |  |  |  | Version 8.0.0 created after approval at CT#43 | 2.0.0 | 8.0.0 |
| 2009-06 | CT-44 | CP-090423 | 0001 |  | urn for the CSG MO registered by OMNA and minor corrections and cleanups | 8.0.0 | 8.1.0 |
| 2009-06 | CT-44 | CP-090423 | 0002 | 1 | Updating the allowed CSG list on receiving OMA DM message | 8.0.0 | 8.1.0 |
| 2009-06 | CT-44 |  |  |  | Cover sheet template fixed by MCC | 8.0.0 | 8.1.0 |
| 2009-06 |  |  |  |  | Correct version shown on cover | 8.1.0 | 8.1.1 |
| 2009-09 | CT-45 | CP-090677 | 0003 | 1 | Support of CSG Type in Allowed CSG MO | 8.1.1 | 8.2.0 |
| 2009-09 | CT-45 | CP-090633 | 0004 | 2 | Introduction of Operator CSG List in the MO | 82.0 | 9.0.0 |
| 2009-12 | CT-46 | CP-090918 | 0006 |  | Correction of the OMA DM object for the Allowed CSG list | 9.0.0 | 9.1.0 |
| 2009-12 | CT-46 | CP-090935 | 0007 |  | Support of CSG Type for Operator CSG List | 9.0.0 | 9.1.0 |
| 2010-06 | CT-48 | CP-100350 | 0011 |  | Occurrence of HNB\_Name and CSG\_Type | 9.1.0 | 9.2.0 |
| 2010-06 | CT-48 | CP-100370 | 0010 | 1 | Updating Operator CSG List | 9.2.0 | 10.0.0 |
| 2010-09 | CT-49 | CP-100606 | 0021 |  | Correcting DDF of allowed CSG list MO | 10.0.0 | 10.1.0 |
| 2010-12 | CT-50 | CP-100748 | 0023 | 3 | Support for displaying only CSGs in the Operator CSG List | 10.1.0 | 10.2.0 |
| 2012-09 | CT-57 |  |  |  | Upgrade to Rel-11 | 10.2.0 | 11.0.0 |
| 2014-09 | CT-65 |  |  |  | Upgrade to Rel-12 | 11.0.0 | 12.0.0 |
| 2015-12 | CT-70 |  |  |  | Upgrade to Rel-13 | 12.0.0 | 13.0.0 |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2017-03 | CT-75 |  |  |  |  | Upgrade to Rel-14 | 14.0.0 |
| 2018-06 | SA-80 | - | - | - |  | Update to Rel-15 version (MCC) | 15.0.0 |
| 2020-07 | SA-88e | - | - | - |  | Update to Rel-16 version (MCC) | **16.0.0** |