3GPP TS 24.483 V16.8.0 (2022-06)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Core Network and Terminals;

Mission Critical Services (MCS) Management Object (MO)

(Release 16)

** 

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP..  
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.  
This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

Keywords

LTE, MCPTT, management

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword [33](#__RefHeading___Toc106437716)

1 Scope [34](#__RefHeading___Toc106437717)

2 References [35](#__RefHeading___Toc106437718)

3 Definitions and abbreviations [36](#__RefHeading___Toc106437719)

3.1 Definitions [36](#__RefHeading___Toc106437720)

3.2 Abbreviations [36](#__RefHeading___Toc106437721)

4 MCPTT UE configuration MO [36](#__RefHeading___Toc106437722)

4.1 General [36](#__RefHeading___Toc106437723)

4.2 MCPTT UE configuration MO parameters [37](#__RefHeading___Toc106437724)

4.2.1 General [37](#__RefHeading___Toc106437725)

4.2.2 Node: *<x>* [37](#__RefHeading___Toc106437726)

4.2.3 /*<x>*/Name [37](#__RefHeading___Toc106437727)

4.2.4 /*<x>*/Ext/ [38](#__RefHeading___Toc106437728)

4.2.5 /*<x>*/Common [38](#__RefHeading___Toc106437729)

4.2.6 /*<x>*/Common/PrivateCall [38](#__RefHeading___Toc106437730)

4.2.7 /*<x>*/Common/PrivateCall/MaxCallN10 [38](#__RefHeading___Toc106437731)

4.2.8 /*<x>*/Common/MCPTTGroupCall [39](#__RefHeading___Toc106437732)

4.2.9 /*<x>*/Common/MCPTTGroupCall/MaxCallN4 [39](#__RefHeading___Toc106437733)

4.2.10 /*<x>*/Common/MCPTTGroupCall/MaxTransmissionN5 [39](#__RefHeading___Toc106437734)

4.2.11 /*<x>*/Common/MCPTTGroupCall/PrioritizedMCPTTGroup [39](#__RefHeading___Toc106437735)

4.2.12 /*<x>*/Common/MCPTTGroupCall/PrioritizedMCPTTGroup/<x> [39](#__RefHeading___Toc106437736)

4.2.13 /*<x>*/Common/MCPTTGroupCall/PrioritizedMCPTTGroup/<x>/ MCPTTGroupID [40](#__RefHeading___Toc106437737)

4.2.14 /*<x>*/Common/MCPTTGroupCall/PrioritizedMCPTTGroup/<x>/ MCPTTGroupPriorityHierarchy [40](#__RefHeading___Toc106437738)

4.2.15 /*<x>*/OnNetwork [40](#__RefHeading___Toc106437739)

4.2.16 /*<x>*/OnNetwork/RelayService [40](#__RefHeading___Toc106437740)

4.2.17 /*<x>*/OnNetwork/IPv6Preferred [41](#__RefHeading___Toc106437741)

4.2.18 /*<x>*/OnNetwork/RelayedMCPTTGroup [41](#__RefHeading___Toc106437742)

4.2.19 /*<x>*/OnNetwork/RelayedMCPTTGroup/<x> [41](#__RefHeading___Toc106437743)

4.2.20 /*<x>*/OnNetwork/RelayedMCPTTGroup/<x>/MCPTTGroupID [41](#__RefHeading___Toc106437744)

4.2.21 /*<x>*/OnNetwork/RelayedMCPTTGroup/<x>/RelayServiceCode [42](#__RefHeading___Toc106437745)

5 MCPTT user profile MO [42](#__RefHeading___Toc106437746)

5.1 General [42](#__RefHeading___Toc106437747)

5.2 MCPTT user profile MO parameters [45](#__RefHeading___Toc106437748)

5.2.1 General [45](#__RefHeading___Toc106437749)

5.2.2 Node: *<x>* [46](#__RefHeading___Toc106437750)

5.2.3 /*<x>*/Name [46](#__RefHeading___Toc106437751)

5.2.4 /*<x>*/Ext/ [46](#__RefHeading___Toc106437752)

5.2.5 /*<x>*/<x> [46](#__RefHeading___Toc106437753)

5.2.6 /*<x>*/<x>/Common [47](#__RefHeading___Toc106437754)

5.2.7 /*<x>*/*<x>*/Common/MCPTTUserID [47](#__RefHeading___Toc106437755)

5.2.7A /*<x>*/*<x>*/Common/MCPTTUserProfileIndex [47](#__RefHeading___Toc106437756)

5.2.7B /*<x>*/*<x>*/Common/MCPTTUserProfileName [47](#__RefHeading___Toc106437757)

5.2.7C /*<x>*/*<x>*/Common/PreSelectedIndication [47](#__RefHeading___Toc106437758)

5.2.8 /*<x>*/*<x>*/Common/UserAliases [48](#__RefHeading___Toc106437759)

5.2.8A /*<x>*/*<x>*/Common/UserAliases/<x> [48](#__RefHeading___Toc106437760)

5.2.8B /*<x>*/*<x>*/Common/UserAliases/<x>/UserAlias [48](#__RefHeading___Toc106437761)

5.2.9 /*<x>*/*<x>*/Common/AuthorisedAlias [48](#__RefHeading___Toc106437762)

5.2.10 /*<x>*/<x>/Common/ParticipantType [49](#__RefHeading___Toc106437763)

5.2.11 /*<x>*/<x>/Common/Organization [49](#__RefHeading___Toc106437764)

5.2.12 /*<x>*/*<x>*/Common/PrivateCall [49](#__RefHeading___Toc106437765)

5.2.13 /*<x>*/*<x>*/Common/PrivateCall/Authorised [49](#__RefHeading___Toc106437766)

5.2.14 /*<x>*/*<x>*/Common/PrivateCall/AuthorisedAny [50](#__RefHeading___Toc106437767)

5.2.15 /*<x>*/<x>/Common/PrivateCall/UserList [50](#__RefHeading___Toc106437768)

5.2.16 /*<x>*/<x>/Common/PrivateCall/UserList/<x> [50](#__RefHeading___Toc106437769)

5.2.16A /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry [50](#__RefHeading___Toc106437770)

5.2.17 /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry/MCPTTID [51](#__RefHeading___Toc106437771)

5.2.18 /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry/ DiscoveryGroupID [51](#__RefHeading___Toc106437772)

5.2.19 /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry/ UserInfoID [51](#__RefHeading___Toc106437773)

5.2.19A /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry/ DisplayName [51](#__RefHeading___Toc106437774)

5.2.19B /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry/ PrivateCallKMSURI [52](#__RefHeading___Toc106437775)

5.2.20 /*<x>*/*<x>*/Common/PrivateCall/ManualCommence [52](#__RefHeading___Toc106437776)

5.2.21 /*<x>*/*<x>*/Common/PrivateCall/AutoCommence [52](#__RefHeading___Toc106437777)

5.2.22 /*<x>*/*<x>*/Common/PrivateCall/AutoAnswer [52](#__RefHeading___Toc106437778)

5.2.23 /*<x>*/*<x>*/Common/PrivateCall/FailRestrict [53](#__RefHeading___Toc106437779)

5.2.24 /*<x>*/*<x>*/Common/PrivateCall/AllowedMediaProtection [53](#__RefHeading___Toc106437780)

5.2.25 /*<x>*/*<x>*/Common/PrivateCall/AllowedFloorControlProtection [53](#__RefHeading___Toc106437781)

5.2.26 /*<x>*/*<x>*/Common/PrivateCall/EmergencyCall [54](#__RefHeading___Toc106437782)

5.2.27 /*<x>*/*<x>*/Common/PrivateCall/EmergencyCall/Authorised [54](#__RefHeading___Toc106437783)

5.2.28 /*<x>*/*<x>*/Common/PrivateCall/EmergencyCall/CancelPriority [54](#__RefHeading___Toc106437784)

5.2.29 /*<x>*/*<x>*/Common/PrivateCall/EmergencyCall/ MCPTTPrivateRecipient [54](#__RefHeading___Toc106437785)

5.2.29A /*<x>*/<x>/Common/PrivateCall/EmergencyCall/ MCPTTPrivateRecipient/Entry [55](#__RefHeading___Toc106437786)

5.2.29B /*<x>*/*<x>*/Common/PrivateCall/EmergencyCall/ MCPTTPrivateRecipient/Entry/ID [55](#__RefHeading___Toc106437787)

5.2.29C /*<x>*/<x>/Common/PrivateCall/EmergencyCall/ MCPTTPrivateRecipient/Entry/DiscoveryGroupID [55](#__RefHeading___Toc106437788)

5.2.29D /*<x>*/<x>/Common/PrivateCall/EmergencyCall/ MCPTTPrivateRecipient/Entry/UserInfoID [55](#__RefHeading___Toc106437789)

5.2.29E /*<x>*/*<x>*/Common/PrivateCall/EmergencyCall/ MCPTTPrivateRecipient/Entry/DisplayName [56](#__RefHeading___Toc106437790)

5.2.29F /*<x>*/*<x>*/Common/PrivateCall/EmergencyCall/ MCPTTPrivateRecipient/Entry/Usage [56](#__RefHeading___Toc106437791)

5.2.30 /*<x>*/*<x>*/Common/MCPTTGroupCall [56](#__RefHeading___Toc106437792)

5.2.31 /*<x>*/*<x>*/Common/MCPTTGroupCall/ MaxSimultaneousCallsN6 [57](#__RefHeading___Toc106437793)

5.2.32 /*<x>*/*<x>*/Common/MCPTTGroupCall/EmergencyCall [57](#__RefHeading___Toc106437794)

5.2.33 /*<x>*/*<x>*/Common/MCPTTGroupCall/EmergencyCall/Enabled [57](#__RefHeading___Toc106437795)

5.2.34 /*<x>*/*<x>*/Common/MCPTTGroupCall/EmergencyCall/ MCPTTGroupInitiation [57](#__RefHeading___Toc106437796)

5.2.34A /*<x>*/<x>/Common/MCPTTGroupCall/EmergencyCall/ MCPTTGroupInitiation/Entry [58](#__RefHeading___Toc106437797)

5.2.34B /*<x>*/*<x>*/Common/MCPTTGroupCall/EmergencyCall/ MCPTTGroupInitiation/Entry/GroupID [58](#__RefHeading___Toc106437798)

5.2.34C /*<x>*/*<x>*/Common/MCPTTGroupCall/EmergencyCall/ MCPTTGroupInitiation/Entry/DisplayName [58](#__RefHeading___Toc106437799)

5.2.34D /*<x>*/*<x>*/Common/MCPTTGroupCall/EmergencyCall/ MCPTTGroupInitiation/Entry/Usage [58](#__RefHeading___Toc106437800)

5.2.35 /*<x>*/*<x>*/Common/MCPTTGroupCall/EmergencyCall/ CancelMCPTTGroup [59](#__RefHeading___Toc106437801)

5.2.36 /*<x>*/*<x>*/Common/MCPTTGroupCall/ImminentPerilCall [59](#__RefHeading___Toc106437802)

5.2.37 /*<x>*/*<x>*/Common/MCPTTGroupCall/ImminentPerilCall/ Authorised [59](#__RefHeading___Toc106437803)

5.2.38 /*<x>*/*<x>*/Common/MCPTTGroupCall/ImminentPerilCall/ Cancel [59](#__RefHeading___Toc106437804)

5.2.39 /*<x>*/*<x>*/Common/MCPTTGroupCall/ImminentPerilCall/ MCPTTGroupInitiation [60](#__RefHeading___Toc106437805)

5.2.39A /*<x>*/<x>/Common/MCPTTGroupCall/ImminentPerilCall/ MCPTTGroupInitiation/Entry [60](#__RefHeading___Toc106437806)

5.2.39B /*<x>*/*<x>*/Common/MCPTTGroupCall/ImminentPerilCall/ MCPTTGroupInitiation/Entry/GroupID [60](#__RefHeading___Toc106437807)

5.2.39C /*<x>*/*<x>*/Common/MCPTTGroupCall/ImminentPerilCall/ MCPTTGroupInitiation/DisplayName [60](#__RefHeading___Toc106437808)

5.2.39D /*<x>*/*<x>*/Common/MCPTTGroupCall/ImminentPerilCall/ MCPTTGroupInitiation/Entry/Usage [61](#__RefHeading___Toc106437809)

5.2.40 /*<x>*/*<x>*/Common/MCPTTGroupCall/EmergencyAlert [61](#__RefHeading___Toc106437810)

5.2.41 /*<x>*/*<x>*/Common/MCPTTGroupCall/EmergencyAlert/ Authorised [61](#__RefHeading___Toc106437811)

5.2.42 /*<x>*/*<x>*/Common/MCPTTGroupCall/EmergencyAlert/ Cancel [62](#__RefHeading___Toc106437812)

5.2.43 Void [62](#__RefHeading___Toc106437813)

5.2.43A /*<x>*/<x>/Common/MCPTTGroupCall/EmergencyAlert/Entry [62](#__RefHeading___Toc106437814)

5.2.43B /*<x>*/*<x>*/Common/MCPTTGroupCall/EmergencyAlert/Entry/ID [62](#__RefHeading___Toc106437815)

5.2.43C Void [62](#__RefHeading___Toc106437816)

5.2.43D /*<x>*/*<x>*/Common/MCPTTGroupCall/EmergencyAlert/Entry/ DisplayName [62](#__RefHeading___Toc106437817)

5.2.43E /*<x>*/*<x>*/Common/MCPTTGroupCall/EmergencyAlert/Entry/Usage [63](#__RefHeading___Toc106437818)

5.2.43F /*<x>*/*<x>*/Common/MCPTTGroupCall/Priority [63](#__RefHeading___Toc106437819)

5.2.44 Void [63](#__RefHeading___Toc106437820)

5.2.45 /*<x>*/*<x>*/Common/MCPTTGroupBroadcast [63](#__RefHeading___Toc106437821)

5.2.46 /*<x>*/*<x>*/Common/MCPTTGroupBroadcast/Authorised [64](#__RefHeading___Toc106437822)

5.2.47 /*<x>*/*<x>*/Common/UserBroadcast [64](#__RefHeading___Toc106437823)

5.2.48 /*<x>*/*<x>*/Common/UserBroadcast/Authorised [64](#__RefHeading___Toc106437824)

5.2.48A /*<x>*/*<x>*/OnNetwork [64](#__RefHeading___Toc106437825)

5.2.48B1 /*<x>*/*<x>*/OnNetwork/MCPTTGroupList [64](#__RefHeading___Toc106437826)

5.2.48B2 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x> [65](#__RefHeading___Toc106437827)

5.2.48B3 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry [65](#__RefHeading___Toc106437828)

5.2.48B4 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ MCPTTGroupID [65](#__RefHeading___Toc106437829)

5.2.48B4A /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation [65](#__RefHeading___Toc106437830)

5.2.48B4A0 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x> [66](#__RefHeading___Toc106437831)

5.2.48B4A1 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/ [66](#__RefHeading___Toc106437832)

5.2.48B4A2 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x> [66](#__RefHeading___Toc106437833)

5.2.48B4A3 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry [66](#__RefHeading___Toc106437834)

5.2.48B4A4 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea [67](#__RefHeading___Toc106437835)

5.2.48B4A5 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea [67](#__RefHeading___Toc106437836)

5.2.48B4A6 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea/<x> [67](#__RefHeading___Toc106437837)

5.2.48B4A7 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea/<x>/PointCoordinateType [68](#__RefHeading___Toc106437838)

5.2.48B4A8 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/ Longitude [68](#__RefHeading___Toc106437839)

5.2.48B4A9 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude [68](#__RefHeading___Toc106437840)

5.2.48B4A10 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea [69](#__RefHeading___Toc106437841)

5.2.48B4A11 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Center [69](#__RefHeading___Toc106437842)

5.2.48B4A12 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType [69](#__RefHeading___Toc106437843)

5.2.48B4A13 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Longitude [70](#__RefHeading___Toc106437844)

5.2.48B4A14 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Latitude [70](#__RefHeading___Toc106437845)

5.2.48B4A15 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Radius [70](#__RefHeading___Toc106437846)

5.2.48B4A16 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/OffsetAngle [71](#__RefHeading___Toc106437847)

5.2.48B4A17 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/IncludedAngle [71](#__RefHeading___Toc106437848)

5.2.48B4A18 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Speed [71](#__RefHeading___Toc106437849)

5.2.48B4A19 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Speed/MinimumSpeed [72](#__RefHeading___Toc106437850)

5.2.48B4A20 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Speed/MaximumSpeed [72](#__RefHeading___Toc106437851)

5.2.48B4A21 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Heading [72](#__RefHeading___Toc106437852)

5.2.48B4A22 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Heading/MinimumHeading [73](#__RefHeading___Toc106437853)

5.2.48B4A23 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Heading/MaximumHeading [73](#__RefHeading___Toc106437854)

5.2.48B4A24 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea [73](#__RefHeading___Toc106437855)

5.2.48B4A25 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea [74](#__RefHeading___Toc106437856)

5.2.48B4A26 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea/<x> [74](#__RefHeading___Toc106437857)

5.2.48B4A27 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea/<x>/PointCoordinateType [74](#__RefHeading___Toc106437858)

5.2.48B4A28 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude [75](#__RefHeading___Toc106437859)

5.2.48B4A29 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude [75](#__RefHeading___Toc106437860)

5.2.48B4A30 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea [75](#__RefHeading___Toc106437861)

5.2.48B4A31 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Center [76](#__RefHeading___Toc106437862)

5.2.48B4A32 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType [76](#__RefHeading___Toc106437863)

5.2.48B4A33 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Longitude [76](#__RefHeading___Toc106437864)

5.2.48B4A34 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Latitude [77](#__RefHeading___Toc106437865)

5.2.48B4A35 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Radius [77](#__RefHeading___Toc106437866)

5.2.48B4A36 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/OffsetAngle [77](#__RefHeading___Toc106437867)

5.2.48B4A37 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/IncludedAngle [78](#__RefHeading___Toc106437868)

5.2.48B4A38 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Speed [78](#__RefHeading___Toc106437869)

5.2.48B4A39 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Speed/MinimumSpeed [78](#__RefHeading___Toc106437870)

5.2.48B4A40 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Speed/MaximumSpeed [79](#__RefHeading___Toc106437871)

5.2.48B4A41 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Heading [79](#__RefHeading___Toc106437872)

5.2.48B4A42 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Heading/MinimumHeading [79](#__RefHeading___Toc106437873)

5.2.48B4A43 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Heading/MaximumHeading [80](#__RefHeading___Toc106437874)

5.2.48B4A44 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfActiveFunctionalAliases [80](#__RefHeading___Toc106437875)

5.2.48B4A45 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfActiveFunctionalAliases/<x> [80](#__RefHeading___Toc106437876)

5.2.48B4A46 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfActiveFunctionalAliases/<x>/Entry [80](#__RefHeading___Toc106437877)

5.2.48B4A47 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfActiveFunctionalAliases/<x>/Entry/ FunctionalAlias [81](#__RefHeading___Toc106437878)

5.2.48B4B /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation [81](#__RefHeading___Toc106437879)

5.2.48B4B0 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x> [81](#__RefHeading___Toc106437880)

5.2.48B4B1 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/ [81](#__RefHeading___Toc106437881)

5.2.48B4B2 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x> [82](#__RefHeading___Toc106437882)

5.2.48B4B3 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry [82](#__RefHeading___Toc106437883)

5.2.48B4B4 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea [82](#__RefHeading___Toc106437884)

5.2.48B4B5 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea [82](#__RefHeading___Toc106437885)

5.2.48B4B6 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea/<x> [83](#__RefHeading___Toc106437886)

5.2.48B4B7 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea/<x>/PointCoordinateType [83](#__RefHeading___Toc106437887)

5.2.48B4B8 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/ Longitude [83](#__RefHeading___Toc106437888)

5.2.48B4B9 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude [84](#__RefHeading___Toc106437889)

5.2.48B4B10 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea [84](#__RefHeading___Toc106437890)

5.2.48B4A11 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Center [84](#__RefHeading___Toc106437891)

5.2.48B4B12 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType [85](#__RefHeading___Toc106437892)

5.2.48B4B13 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Longitude [85](#__RefHeading___Toc106437893)

5.2.48B4B14 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Latitude [85](#__RefHeading___Toc106437894)

5.2.48B4B15 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Radius [86](#__RefHeading___Toc106437895)

5.2.48B4B16 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/OffsetAngle [86](#__RefHeading___Toc106437896)

5.2.48B4B17 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/IncludedAngle [86](#__RefHeading___Toc106437897)

5.2.48B4B18 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Speed [87](#__RefHeading___Toc106437898)

5.2.48B4B19 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Speed/MinimumSpeed [87](#__RefHeading___Toc106437899)

5.2.48B4B20 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Speed/MaximumSpeed [87](#__RefHeading___Toc106437900)

5.2.48B4B21 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Heading [88](#__RefHeading___Toc106437901)

5.2.48B4B22 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Heading/MinimumHeading [88](#__RefHeading___Toc106437902)

5.2.48B4B23 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Heading/MaximumHeading [88](#__RefHeading___Toc106437903)

5.2.48B4B24 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea [89](#__RefHeading___Toc106437904)

5.2.48B4B25 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea [89](#__RefHeading___Toc106437905)

5.2.48B4B26 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea/<x> [89](#__RefHeading___Toc106437906)

5.2.48B4B27 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea/<x>/PointCoordinateType [90](#__RefHeading___Toc106437907)

5.2.48B4B28 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude [90](#__RefHeading___Toc106437908)

5.2.48B4B29 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude [90](#__RefHeading___Toc106437909)

5.2.48B4B30 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea [91](#__RefHeading___Toc106437910)

5.2.48B4B31 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Center [91](#__RefHeading___Toc106437911)

5.2.48B4B32 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType [91](#__RefHeading___Toc106437912)

5.2.48B4B33 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Longitude [92](#__RefHeading___Toc106437913)

5.2.48B4B34 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Latitude [92](#__RefHeading___Toc106437914)

5.2.48B4B35 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Radius [92](#__RefHeading___Toc106437915)

5.2.48B4B36 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/OffsetAngle [93](#__RefHeading___Toc106437916)

5.2.48B4B37 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/IncludedAngle [93](#__RefHeading___Toc106437917)

5.2.48B4B38 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Speed [93](#__RefHeading___Toc106437918)

5.2.48B4B39 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Speed/MinimumSpeed [94](#__RefHeading___Toc106437919)

5.2.48B4B40 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Speed/MaximumSpeed [94](#__RefHeading___Toc106437920)

5.2.48B4B41 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Heading [94](#__RefHeading___Toc106437921)

5.2.48B4B42 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Heading/MinimumHeading [95](#__RefHeading___Toc106437922)

5.2.48B4B43 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Heading/MaximumHeading [95](#__RefHeading___Toc106437923)

5.2.48B4B44 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfActiveFunctionalAliases [95](#__RefHeading___Toc106437924)

5.2.48B4B45 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfActiveFunctionalAliases/<x> [96](#__RefHeading___Toc106437925)

5.2.48B4B46 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfActiveFunctionalAliases/<x>/Entry [96](#__RefHeading___Toc106437926)

5.2.48B4B47 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfActiveFunctionalAliases/<x>/Entry/ FunctionalAlias [96](#__RefHeading___Toc106437927)

5.2.48B5 /*<x>*/*<x>*/OnNetwork/MCPTTGroupList/<x>/Entry/DisplayName [96](#__RefHeading___Toc106437928)

5.2.48B6 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ ManualDeaffiliationNotAllowedIfAffiliationRulesAreMet [97](#__RefHeading___Toc106437929)

5.2.48B7 /<x>/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RelativePresentationPriority [97](#__RefHeading___Toc106437930)

5.2.48B8 /<x>/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/GMSServID [97](#__RefHeading___Toc106437931)

5.2.48B9 /<x>/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ IDMSTokenEndPoint [97](#__RefHeading___Toc106437932)

5.2.48B10 /<x>/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/GroupKMSURI [98](#__RefHeading___Toc106437933)

5.2.48C1 /*<x>*/*<x>*/OnNetwork/ImplicitAffiliations [98](#__RefHeading___Toc106437934)

5.2.48C2 /*<x>*/<x>/OnNetwork/ImplicitAffiliations/<x> [98](#__RefHeading___Toc106437935)

5.2.48C3 /*<x>*/<x>/OnNetwork/ImplicitAffiliations/<x>/Entry [98](#__RefHeading___Toc106437936)

5.2.48C4 /*<x>*/<x>/OnNetwork/ImplicitAffiliations/<x>/Entry/ MCPTTGroupID [98](#__RefHeading___Toc106437937)

5.2.48C5 /*<x>*/*<x>*/OnNetwork/ImplicitAffiliations/<x>/Entry/DisplayName [99](#__RefHeading___Toc106437938)

5.2.48D /*<x>*/*<x>*/OnNetwork/AllowedRegroup [99](#__RefHeading___Toc106437939)

5.2.48E /*<x>*/*<x>*/OnNetwork/AllowedPresenceStatus [99](#__RefHeading___Toc106437940)

5.2.48F /*<x>*/*<x>*/OnNetwork/AllowedPresence [99](#__RefHeading___Toc106437941)

5.2.48G /*<x>*/*<x>*/OnNetwork/EnabledParticipation [100](#__RefHeading___Toc106437942)

5.2.48H /*<x>*/*<x>*/OnNetwork/AllowedTransmission [100](#__RefHeading___Toc106437943)

5.2.48I /*<x>*/*<x>*/OnNetwork/AllowedManualSwitch [100](#__RefHeading___Toc106437944)

5.2.48J /*<x>*/*<x>*/OnNetwork/PrivateCall [101](#__RefHeading___Toc106437945)

5.2.48K /*<x>*/*<x>*/OnNetwork/PrivateCall/EmergencyAlert [101](#__RefHeading___Toc106437946)

5.2.48L /*<x>*/*<x>*/OnNetwork/PrivateCall/EmergencyAlert/Entry [101](#__RefHeading___Toc106437947)

5.2.48M /*<x>*/*<x>*/OnNetwork/PrivateCall/EmergencyAlert/Entry/ID [101](#__RefHeading___Toc106437948)

5.2.48N /*<x>*/*<x>*/OnNetwork/PrivateCall/EmergencyAlert/Entry/ DisplayName [101](#__RefHeading___Toc106437949)

5.2.48O /*<x>*/*<x>*/OnNetwork/PrivateCall/EmergencyAlert/Entry/Usage [102](#__RefHeading___Toc106437950)

5.2.48P /*<x>*/*<x>*/OnNetwork/PrivateCall/AllowedCallBackRequest [102](#__RefHeading___Toc106437951)

5.2.48Q /<x>/<x>/OnNetwork/PrivateCall/AllowedCallBackCancelRequest [102](#__RefHeading___Toc106437952)

5.2.48R /*<x>*/*<x>*/OnNetwork/PrivateCall/ AllowedRemoteInitiatedAmbientListening [102](#__RefHeading___Toc106437953)

5.2.48S /<x>/<x>/OnNetwork/PrivateCall/ AllowedLocallyInitiatedAmbientListening [103](#__RefHeading___Toc106437954)

5.2.48T /*<x>*/*<x>*/OnNetwork/PrivateCall/ AllowedRequestFirstToAnswerCall [103](#__RefHeading___Toc106437955)

5.2.48U1 /*<x>*/*<x>*/OnNetwork/RemoteGroupSelection [103](#__RefHeading___Toc106437956)

5.2.48U2 /*<x>*/<x>/OnNetwork/RemoteGroupSelection/<x> [104](#__RefHeading___Toc106437957)

5.2.48U3 /*<x>*/<x>/OnNetwork/RemoteGroupSelection/<x>/Entry [104](#__RefHeading___Toc106437958)

5.2.48U4 /*<x>*/<x>/OnNetwork/RemoteGroupSelection/<x>/Entry/ MCPTTID [104](#__RefHeading___Toc106437959)

5.2.48U5 /*<x>*/*<x>*/OnNetwork/RemoteGroupSelection/<x>/Entry/ DisplayName [104](#__RefHeading___Toc106437960)

5.2.48V1 Void [105](#__RefHeading___Toc106437961)

5.2.48V2 Void [105](#__RefHeading___Toc106437962)

5.2.48V3 Void [105](#__RefHeading___Toc106437963)

5.2.48V4 Void [105](#__RefHeading___Toc106437964)

5.2.48V5 Void [105](#__RefHeading___Toc106437965)

5.2.48V6 Void [105](#__RefHeading___Toc106437966)

5.2.48V7 Void [105](#__RefHeading___Toc106437967)

5.2.48V8 Void [105](#__RefHeading___Toc106437968)

5.2.48V9 Void [105](#__RefHeading___Toc106437969)

5.2.48V10 Void [105](#__RefHeading___Toc106437970)

5.2.48V11 Void [105](#__RefHeading___Toc106437971)

5.2.48V12 Void [105](#__RefHeading___Toc106437972)

5.2.48V13 Void [105](#__RefHeading___Toc106437973)

5.2.48V14 Void [105](#__RefHeading___Toc106437974)

5.2.48V15 Void [105](#__RefHeading___Toc106437975)

5.2.48V16 Void [105](#__RefHeading___Toc106437976)

5.2.48V17 Void [105](#__RefHeading___Toc106437977)

5.2.48W1 /*<x>*/*<x>*/OnNetwork/AllowedRequestRemoteInitPrivateCall [105](#__RefHeading___Toc106437978)

5.2.48W2 /*<x>*/*<x>*/OnNetwork/AllowedRequestRemoteInitGroupCall [106](#__RefHeading___Toc106437979)

5.2.48W3 /*<x>*/*<x>*/OnNetwork/FunctionalAliasList [106](#__RefHeading___Toc106437980)

5.2.48W4 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x> [106](#__RefHeading___Toc106437981)

5.2.48W5 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry [106](#__RefHeading___Toc106437982)

5.2.48W6 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ FunctionalAlias [106](#__RefHeading___Toc106437983)

5.2.48W6A /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation [107](#__RefHeading___Toc106437984)

5.2.48W6A0 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x> [107](#__RefHeading___Toc106437985)

5.2.48W6A1 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/ Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea [107](#__RefHeading___Toc106437986)

5.2.48W6A2 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/PolygonArea [107](#__RefHeading___Toc106437987)

5.2.48W6A3 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ PolygonArea/<x> [108](#__RefHeading___Toc106437988)

5.2.48W6A3A /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ PolygonArea/<x>/PointCoordinateType [108](#__RefHeading___Toc106437989)

5.2.48W6A4 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ PolygonArea/<x>/PointCoordinateType/Longitude [108](#__RefHeading___Toc106437990)

5.2.48W6A5 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ PolygonArea/<x>/PointCoordinateType/Latitude [109](#__RefHeading___Toc106437991)

5.2.48W6A6 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ EllipsoidArcArea [109](#__RefHeading___Toc106437992)

5.2.48W6A7 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Center [109](#__RefHeading___Toc106437993)

5.2.48W6A7A /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType [110](#__RefHeading___Toc106437994)

5.2.48W6A8 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType/Longitude [110](#__RefHeading___Toc106437995)

5.2.48W6A9 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType/Latitude [110](#__RefHeading___Toc106437996)

5.2.48W6A10 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ EnterSpecificArea/EllipsoidArcArea/Radius [111](#__RefHeading___Toc106437997)

5.2.48W6A11 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ EnterSpecificArea/EllipsoidArcArea/OffsetAngle [111](#__RefHeading___Toc106437998)

5.2.48W6A12 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ EnterSpecificArea/EllipsoidArcArea/IncludedAngle [111](#__RefHeading___Toc106437999)

5.2.48W6A12A /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/Speed [112](#__RefHeading___Toc106438000)

5.2.48W6A12B /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/Speed/ MinimumSpeed [112](#__RefHeading___Toc106438001)

5.2.48W6A12C /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/Speed/ MaximumSpeed [112](#__RefHeading___Toc106438002)

5.2.48W6A12D /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/Heading [113](#__RefHeading___Toc106438003)

5.2.48W6A12E /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/Heading/ MinimumHeading [113](#__RefHeading___Toc106438004)

5.2.48W6A12F /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/Heading/ MaximumHeading [113](#__RefHeading___Toc106438005)

5.2.48W6A13 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ ExitSpecificArea [114](#__RefHeading___Toc106438006)

5.2.48W6A14 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ ExitSpecificArea/PolygonArea [114](#__RefHeading___Toc106438007)

5.2.48W6A15 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ ExitSpecificArea/PolygonArea/<x> [114](#__RefHeading___Toc106438008)

5.2.48W6A15A /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/ PolygonArea/<x>/PointCoordinateType [115](#__RefHeading___Toc106438009)

5.2.48W6A16 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude [115](#__RefHeading___Toc106438010)

5.2.48W6A17 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude [115](#__RefHeading___Toc106438011)

5.2.48W6A18 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ ExitSpecificArea/EllipsoidArcArea [116](#__RefHeading___Toc106438012)

5.2.48W6A19 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ ExitSpecificArea/EllipsoidArcArea/Center [116](#__RefHeading___Toc106438013)

5.2.48W6A19A /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType [116](#__RefHeading___Toc106438014)

5.2.48W6A20 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Longitude [117](#__RefHeading___Toc106438015)

5.2.48W6A21 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Latitude [117](#__RefHeading___Toc106438016)

5.2.48W6A22 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ ExitSpecificArea/EllipsoidArcArea/Radius [117](#__RefHeading___Toc106438017)

5.2.48W6A23 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ ExitSpecificArea/EllipsoidArcArea/OffsetAngle [118](#__RefHeading___Toc106438018)

5.2.48W6A24 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ ExitSpecificArea/EllipsoidArcArea/IncludedAngle [118](#__RefHeading___Toc106438019)

5.2.48W6A24A /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/Speed [118](#__RefHeading___Toc106438020)

5.2.48W6A24B /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/Speed/ MinimumSpeed [119](#__RefHeading___Toc106438021)

5.2.48W6A24C /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/Speed/ MaximumSpeed [119](#__RefHeading___Toc106438022)

5.2.48W6A24D /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/Heading [119](#__RefHeading___Toc106438023)

5.2.48W6A24E /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/Heading/ MinimumHeading [120](#__RefHeading___Toc106438024)

5.2.48W6A24F /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/Heading/ MaximumHeading [120](#__RefHeading___Toc106438025)

5.2.48W6B /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation [120](#__RefHeading___Toc106438026)

5.2.48W6B0 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x> [120](#__RefHeading___Toc106438027)

5.2.48W6B1 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea [121](#__RefHeading___Toc106438028)

5.2.48W6B2 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ PolygonArea [121](#__RefHeading___Toc106438029)

5.2.48W6B3 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ PolygonArea/<x> [121](#__RefHeading___Toc106438030)

5.2.48W6B3A /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ PolygonArea/<x>/PointCoordinateType [122](#__RefHeading___Toc106438031)

5.2.48W6B4 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ PolygonArea/<x>/PointCoordinateType/Longitude [122](#__RefHeading___Toc106438032)

5.2.48W6B5 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ PolygonArea/<x>/PointCoordinateType/Latitude [122](#__RefHeading___Toc106438033)

5.2.48W6B6 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ EllipsoidArcArea [123](#__RefHeading___Toc106438034)

5.2.48W6B7 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Center [123](#__RefHeading___Toc106438035)

5.2.48W6B7A /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType [123](#__RefHeading___Toc106438036)

5.2.48W6B8 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType/Longitude [124](#__RefHeading___Toc106438037)

5.2.48W6B9 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType/Latitude [124](#__RefHeading___Toc106438038)

5.2.48W6B10 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ EnterSpecificArea/EllipsoidArcArea/Radius [124](#__RefHeading___Toc106438039)

5.2.48W6B11 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ EnterSpecificArea/EllipsoidArcArea/OffsetAngle [125](#__RefHeading___Toc106438040)

5.2.48W6B12 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ EnterSpecificArea/EllipsoidArcArea/IncludedAngle [125](#__RefHeading___Toc106438041)

5.2.48W6B12A /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Speed [125](#__RefHeading___Toc106438042)

5.2.48W6B12B /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Speed/ MinimumSpeed [126](#__RefHeading___Toc106438043)

5.2.48W6B12C /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Speed/ MaximumSpeed [126](#__RefHeading___Toc106438044)

5.2.48W6B12D /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Heading [126](#__RefHeading___Toc106438045)

5.2.48W6B12E /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Heading/ MinimumHeading [127](#__RefHeading___Toc106438046)

5.2.48W6B12F /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Heading/ MaximumHeading [127](#__RefHeading___Toc106438047)

5.2.48W6B13 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ ExitSpecificArea [127](#__RefHeading___Toc106438048)

5.2.48W6B14 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ ExitSpecificArea/PolygonArea [128](#__RefHeading___Toc106438049)

5.2.48W6B15 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ ExitSpecificArea/PolygonArea/<x> [128](#__RefHeading___Toc106438050)

5.2.48W6B15A /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/ PolygonArea/<x>/PointCoordinateType [128](#__RefHeading___Toc106438051)

5.2.48W6B16 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude [129](#__RefHeading___Toc106438052)

5.2.48W6B17 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude [129](#__RefHeading___Toc106438053)

5.2.48W6B18 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ ExitSpecificArea/EllipsoidArcArea [129](#__RefHeading___Toc106438054)

5.2.48W6B19 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ ExitSpecificArea/EllipsoidArcArea/Center [130](#__RefHeading___Toc106438055)

5.2.48W6B19A /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType [130](#__RefHeading___Toc106438056)

5.2.48W6B20 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Longitude [130](#__RefHeading___Toc106438057)

5.2.48W6B21 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Latitude [131](#__RefHeading___Toc106438058)

5.2.48W6B22 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ ExitSpecificArea/EllipsoidArcArea/Radius [131](#__RefHeading___Toc106438059)

5.2.48W6B23 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ ExitSpecificArea/EllipsoidArcArea/OffsetAngle [131](#__RefHeading___Toc106438060)

5.2.48W6B24 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ ExitSpecificArea/EllipsoidArcArea/IncludedAngle [132](#__RefHeading___Toc106438061)

5.2.48W6B24A /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Speed [132](#__RefHeading___Toc106438062)

5.2.48W6B24B /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Speed/ MinimumSpeed [132](#__RefHeading___Toc106438063)

5.2.48W6B24C /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Speed/ MaximumSpeed [133](#__RefHeading___Toc106438064)

5.2.48W6B24D /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Heading [133](#__RefHeading___Toc106438065)

5.2.48W6B24E /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Heading/ MinimumHeading [133](#__RefHeading___Toc106438066)

5.2.48W6B24F /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Heading/ MaximumHeading [134](#__RefHeading___Toc106438067)

5.2.48W6C /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ ManualDeactivationNotAllowedIfLocationCriteriaMet [134](#__RefHeading___Toc106438068)

5.2.48W7 /*<x>*/*<x>*/OnNetwork/FunctionalAliasList/<x>/Entry/DisplayName [134](#__RefHeading___Toc106438069)

5.2.48W7A /*<x>*/*<x>*/OnNetwork/FunctionalAliasList/<x>/Entry/ MaxSimultaneousEmergencyGroupCalls [134](#__RefHeading___Toc106438070)

5.2.48W8 /*<x>*/*<x>*/OnNetwork/AllowedQueryFunctionalAliasOtherUser [135](#__RefHeading___Toc106438071)

5.2.48W9 /*<x>*/*<x>*/OnNetwork/AllowedTakeoverFunctionalAliasOtherUser [135](#__RefHeading___Toc106438072)

5.2.48W10 /*<x>*/*<x>*/OnNetwork/AllowedLocationInfoWhenTalking [135](#__RefHeading___Toc106438073)

5.2.48X /*<x>*/*<x>*/OnNetwork/AuthorisedIncomingAny [135](#__RefHeading___Toc106438074)

5.2.48Y1 /*<x>*/<x>/OnNetwork/UserList [136](#__RefHeading___Toc106438075)

5.2.48Y2 /*<x>*/<x>/OnNetwork/UserList/<x> [136](#__RefHeading___Toc106438076)

5.2.48Y3 /*<x>*/<x>/OnNetwork/UserList/<x>/Entry [136](#__RefHeading___Toc106438077)

5.2.48Y4 /*<x>*/<x>/OnNetwork/UserList/<x>/Entry/MCPTTID [136](#__RefHeading___Toc106438078)

5.2.48Y5 /*<x>*/<x>/OnNetwork/UserList/<x>/Entry/PrivateCallKMSURI [137](#__RefHeading___Toc106438079)

5.2.48Z /*<x>*/*<x>*/OnNetwork/AuthorisedReceiveNonAcknowledged [137](#__RefHeading___Toc106438080)

5.2.49 /*<x>*/*<x>*/OffNetwork [137](#__RefHeading___Toc106438081)

5.2.50 /*<x>*/*<x>*/OffNetwork/Authorised [137](#__RefHeading___Toc106438082)

5.2.51 /*<x>*/*<x>*/OffNetwork/MCPTTGroupInfo [138](#__RefHeading___Toc106438083)

5.2.52 /*<x>*/<x>/OffNetwork/MCPTTGroupInfo/<x> [138](#__RefHeading___Toc106438084)

5.2.52A /*<x>*/<x>/OffNetwork/MCPTTGroupInfo/<x>/Entry [138](#__RefHeading___Toc106438085)

5.2.53 /*<x>*/<x>/OffNetwork/MCPTTGroupInfo/<x>/Entry/MCPTTGroupID [138](#__RefHeading___Toc106438086)

5.2.53A /*<x>*/*<x>*/OffNetwork/MCPTTGroupInfo/<x>/Entry/DisplayName [138](#__RefHeading___Toc106438087)

5.2.53B /<x>/<x>/OffNetwork/MCPTTGroupInfo/<x>/Entry/ RelativePresentationPriority [139](#__RefHeading___Toc106438088)

5.2.53C /<x>/<x>/OffNetwork/MCPTTGroupInfo/<x>/Entry/GMSServID [139](#__RefHeading___Toc106438089)

5.2.53D /<x>/<x>/OffNetwork/MCPTTGroupInfo/<x>/Entry/ IDMSTokenEndPoint [139](#__RefHeading___Toc106438090)

5.2.53E /<x>/<x>/OffNetwork/MCPTTGroupInfo/<x>/Entry/GroupKMSURI [139](#__RefHeading___Toc106438091)

5.2.54 /*<x>*/*<x>*/OffNetwork/AllowedListen [140](#__RefHeading___Toc106438092)

5.2.55 /*<x>*/*<x>*/OffNetwork/AllowedTransmission [140](#__RefHeading___Toc106438093)

5.2.56 /*<x>*/*<x>*/OffNetwork/EmergencyCallChange [140](#__RefHeading___Toc106438094)

5.2.57 /*<x>*/*<x>*/OffNetwork/ImminentPerilCallChange [140](#__RefHeading___Toc106438095)

5.2.58 /*<x>*/*<x>*/OffNetwork/UserInfoID [141](#__RefHeading___Toc106438096)

5.2.58A1 Void [142](#__RefHeading___Toc106438097)

5.2.58A2 Void [142](#__RefHeading___Toc106438098)

5.2.58A3 Void [142](#__RefHeading___Toc106438099)

5.2.58A4 Void [142](#__RefHeading___Toc106438100)

5.2.58A5 Void [142](#__RefHeading___Toc106438101)

5.2.58A6 Void [142](#__RefHeading___Toc106438102)

5.2.58A7 Void [142](#__RefHeading___Toc106438103)

5.2.58A8 Void [142](#__RefHeading___Toc106438104)

5.2.58A9 Void [142](#__RefHeading___Toc106438105)

5.2.58A10 Void [142](#__RefHeading___Toc106438106)

5.2.58A11 Void [142](#__RefHeading___Toc106438107)

5.2.58A12 Void [142](#__RefHeading___Toc106438108)

5.2.58A13 Void [142](#__RefHeading___Toc106438109)

5.2.58A14 Void [142](#__RefHeading___Toc106438110)

5.2.58A15 Void [142](#__RefHeading___Toc106438111)

5.2.58A16 Void [142](#__RefHeading___Toc106438112)

5.2.58A17 Void [142](#__RefHeading___Toc106438113)

5.2.59 /*<x>*/Status [142](#__RefHeading___Toc106438114)

6 MCS group configuration MO [143](#__RefHeading___Toc106438115)

6.1 General [143](#__RefHeading___Toc106438116)

6.2 MCS group configuration MO parameters [146](#__RefHeading___Toc106438117)

6.2.1 General [146](#__RefHeading___Toc106438118)

6.2.2 Node: *<x>* [146](#__RefHeading___Toc106438119)

6.2.3 /*<x>*/Name [146](#__RefHeading___Toc106438120)

6.2.4 /*<x>*/Ext/ [147](#__RefHeading___Toc106438121)

6.2.5 /*<x>*/<x> [147](#__RefHeading___Toc106438122)

6.2.6 /*<x>*/<x>/Common [147](#__RefHeading___Toc106438123)

6.2.7 /*<x>*/<x>/Common/MCPTTGroupID [147](#__RefHeading___Toc106438124)

6.2.8 /*<x>*/<x>/Common/MCPTTGroupAlias [148](#__RefHeading___Toc106438125)

6.2.9 /*<x>*/<x>/Common/MCPTTGroupMemberList [148](#__RefHeading___Toc106438126)

6.2.10 /*<x>*/<x>/Common/MCPTTGroupMemberList/<x> [148](#__RefHeading___Toc106438127)

6.2.11 /*<x>*/<x>/Common/MCPTTGroupMemberList/<x>/MCPTTID [148](#__RefHeading___Toc106438128)

6.2.12 /*<x>*/<x>/Common/MCPTTGroupMemberList/<x>/UserPriority [149](#__RefHeading___Toc106438129)

6.2.13 /*<x>*/<x>/Common/MCPTTGroupMemberList/<x>/ParticipantType [149](#__RefHeading___Toc106438130)

6.2.14 Void [149](#__RefHeading___Toc106438131)

6.2.15 /*<x>*/<x>/Common/MCPTTGroupOwner [149](#__RefHeading___Toc106438132)

6.2.16 /*<x>*/<x>/Common/PreferredVoiceCodec [149](#__RefHeading___Toc106438133)

6.2.17 /*<x>*/<x>/Common/MCPTTGroupLevel [150](#__RefHeading___Toc106438134)

6.2.18 /*<x>*/<x>/Common/UserLevel [150](#__RefHeading___Toc106438135)

6.2.19 /*<x>*/<x>/Common/AllowedEmergencyCall [150](#__RefHeading___Toc106438136)

6.2.20 /*<x>*/<x>/Common/AllowedImminentPerilCall [151](#__RefHeading___Toc106438137)

6.2.21 /*<x>*/<x>/Common/AllowedEmergencyAlert [151](#__RefHeading___Toc106438138)

6.2.22 /*<x>*/<x>/Common/MediaProtectionRequired [151](#__RefHeading___Toc106438139)

6.2.23 /*<x>*/<x>/Common/FloorControlProtectionRequired [151](#__RefHeading___Toc106438140)

6.2.23A /*<x>*/<x>/Common/MediaProtectionSecurityMaterial [152](#__RefHeading___Toc106438141)

6.2.23B /*<x>*/<x>/Common/MCData [152](#__RefHeading___Toc106438142)

6.2.23C /*<x>*/<x>/Common/MCData/MediaProtectionRequired [152](#__RefHeading___Toc106438143)

6.2.23D /*<x>*/<x>/Common/MCData/TxControlProtectionRequired [153](#__RefHeading___Toc106438144)

6.2.23E /*<x>*/<x>/Common/MCData/MediaProtectionSecurityMaterial [153](#__RefHeading___Toc106438145)

6.2.23F /*<x>*/<x>/Common/MCData/AllowedSDS [153](#__RefHeading___Toc106438146)

6.2.23G /*<x>*/<x>/Common/MCData/AllowedFD [153](#__RefHeading___Toc106438147)

6.2.23H /*<x>*/<x>/Common/MCData/AllowedConvMgmt [154](#__RefHeading___Toc106438148)

6.2.23I /*<x>*/<x>/Common/MCData/AllowedTxControl [154](#__RefHeading___Toc106438149)

6.2.23J /*<x>*/<x>/Common/MCData/AllowedRxControl [154](#__RefHeading___Toc106438150)

6.2.23K /*<x>*/<x>/Common/MCData/AllowedEnhSvc [154](#__RefHeading___Toc106438151)

6.2.23L /*<x>*/<x>/Common/MCData/EnhSvcOpValues [155](#__RefHeading___Toc106438152)

6.2.23M /*<x>*/<x>/Common/MCData/EnhSvcOpValues/<x> [155](#__RefHeading___Toc106438153)

6.2.23N /*<x>*/<x>/Common/MCData/EnhSvcOpValues/<x>/EnhSvcOpValue [155](#__RefHeading___Toc106438154)

6.2.23NA /*<x>*/<x>/Common/MCData/EnhSvcOpValues/<x>/EnhSvcOpID [155](#__RefHeading___Toc106438155)

6.2.23O /*<x>*/<x>/Common/MCData/AllowedTransmitDataInGroup [155](#__RefHeading___Toc106438156)

6.2.23P /<x>/<x>/Common/MCData/MaxDataSingleRequest [156](#__RefHeading___Toc106438157)

6.2.23Q /<x>/<x>/Common/MCData/MaxTimeSingleRequest [156](#__RefHeading___Toc106438158)

6.2.23R /*<x>*/<x>/Common/MCVideo [156](#__RefHeading___Toc106438159)

6.2.23S /*<x>*/<x>/Common/MCVideo/MediaProtectionRequired [156](#__RefHeading___Toc106438160)

6.2.23T /*<x>*/<x>/Common/MCVideo/TxControlProtectionRequired [157](#__RefHeading___Toc106438161)

6.2.23U /*<x>*/<x>/Common/MCVideo/MediaProtectionSecurityMaterial [157](#__RefHeading___Toc106438162)

6.2.23V /*<x>*/<x>/Common/MCVideo/AllowedAudioCodecs [157](#__RefHeading___Toc106438163)

6.2.23W /*<x>*/<x>/Common/MCVideo/AllowedAudioCodecs/<x> [157](#__RefHeading___Toc106438164)

6.2.23X /*<x>*/<x>/Common/MCVideo/AllowedAudioCodecs/<x>/ AudioCodec [158](#__RefHeading___Toc106438165)

6.2.23Y /*<x>*/<x>/Common/MCVideo/AllowedVideoCodecs [158](#__RefHeading___Toc106438166)

6.2.23Z /*<x>*/<x>/Common/MCVideo/AllowedVideoCodecs/<x> [158](#__RefHeading___Toc106438167)

6.2.23AA /*<x>*/<x>/Common/MCVideo/AllowedVideoCodecs/ <x>/VideoCodec [158](#__RefHeading___Toc106438168)

6.2.23AB /*<x>*/<x>/Common/MCVideo/AllowedVideoResolutions [158](#__RefHeading___Toc106438169)

6.2.23AC /*<x>*/<x>/Common/MCVideo/AllowedVideoResolutions/<x> [159](#__RefHeading___Toc106438170)

6.2.23AD /*<x>*/<x>/Common/MCVideo/AllowedVideoResolutions/ <x>/VideoResolution [159](#__RefHeading___Toc106438171)

6.2.23AE /*<x>*/<x>/Common/MCVideo/AllowedVideoFrameRates [159](#__RefHeading___Toc106438172)

6.2.23AF /*<x>*/<x>/Common/MCVideo/AllowedVideoFrameRates/<x> [159](#__RefHeading___Toc106438173)

6.2.23AG /*<x>*/<x>/Common/MCVideo/AllowedVideoFrameRates/ <x>/FrameRate [160](#__RefHeading___Toc106438174)

6.2.23AH /*<x>*/<x>/Common/MCVideo/AllowedUrgentRealTimeMode [160](#__RefHeading___Toc106438175)

6.2.23AI /*<x>*/<x>/Common/MCVideo/AllowedNonUrgentRealTimeMode [160](#__RefHeading___Toc106438176)

6.2.23AJ /*<x>*/<x>/Common/MCVideo/AllowedNonRealTimeMode [160](#__RefHeading___Toc106438177)

6.2.23AK /*<x>*/<x>/Common/MCVideo/ActiveNonRealTimeMode [161](#__RefHeading___Toc106438178)

6.2.23AL /<x>/<x>/Common/MCVideo/MaxTransmitMembers [161](#__RefHeading___Toc106438179)

6.2.24 /*<x>*/<x>/OffNetwork [161](#__RefHeading___Toc106438180)

6.2.25 /*<x>*/<x>/OffNetwork/MCPTTGroupParameter [161](#__RefHeading___Toc106438181)

6.2.26 /*<x>*/<x>/OffNetwork/MCPTTGroupParameter/<x> [162](#__RefHeading___Toc106438182)

6.2.27 /*<x>*/<x>/OffNetwork/MCPTTGroupParameter/<x>/ ProSeLayer2GroupID [162](#__RefHeading___Toc106438183)

6.2.28 /*<x>*/<x>/OffNetwork/MCPTTGroupParameter/<x>/ IPMulticastAddress [162](#__RefHeading___Toc106438184)

6.2.29 /*<x>*/<x>/OffNetwork/MCPTTGroupParameter/<x>/ RelayServiceCode [162](#__RefHeading___Toc106438185)

6.2.30 /*<x>*/<x>/OffNetwork/MCPTTGroupParameter/<x>/IPVersions [163](#__RefHeading___Toc106438186)

6.2.31 /*<x>*/<x>/OffNetwork/EmergencyCallCancel [163](#__RefHeading___Toc106438187)

6.2.32 /*<x>*/<x>/OffNetwork/ImminentPerilCallCancel [163](#__RefHeading___Toc106438188)

6.2.33 /*<x>*/<x>/OffNetwork/HangTime [163](#__RefHeading___Toc106438189)

6.2.34 /*<x>*/<x>/OffNetwork/MaxDuration [164](#__RefHeading___Toc106438190)

6.2.34A /*<x>*/<x>/OffNetwork/QueueUsage [164](#__RefHeading___Toc106438191)

6.2.35 /*<x>*/<x>/OffNetwork/DefaultPPPP [164](#__RefHeading___Toc106438192)

6.2.36 /*<x>*/<x>/OffNetwork/DefaultPPPP/MCPTTGroupCallSignalling [165](#__RefHeading___Toc106438193)

6.2.37 /*<x>*/<x>/OffNetwork/DefaultPPPP/MCPTTGroupCallMedia [165](#__RefHeading___Toc106438194)

6.2.38 /*<x>*/<x>/OffNetwork/DefaultPPPP/ MCPTTEmergencyGroupCallSignalling [165](#__RefHeading___Toc106438195)

6.2.39 /*<x>*/<x>/OffNetwork/DefaultPPPP/ MCPTTEmergencyGroupCallMedia [166](#__RefHeading___Toc106438196)

6.2.40 /*<x>*/<x>/OffNetwork/DefaultPPPP/ MCPTTImminentPerilGroupCallSignalling [166](#__RefHeading___Toc106438197)

6.2.41 /*<x>*/<x>/OffNetwork/DefaultPPPP/ MCPTTImminentPerilGroupCallMedia [166](#__RefHeading___Toc106438198)

6.2.42 /*<x>*/<x>/OffNetwork/MCData [167](#__RefHeading___Toc106438199)

6.2.43 /*<x>*/<x>/OffNetwork/MCData/DefaultPPPP [167](#__RefHeading___Toc106438200)

6.2.44 /*<x>*/<x>/OffNetwork/MCData/DefaultPPPP/ MCDataGroupCallSignalling [167](#__RefHeading___Toc106438201)

6.2.45 /*<x>*/<x>/OffNetwork/MCData/DefaultPPPP/ MCDataGroupCallMedia [167](#__RefHeading___Toc106438202)

6.2.46 /*<x>*/<x>/OffNetwork/MCVideo [168](#__RefHeading___Toc106438203)

6.2.47 /*<x>*/<x>/OffNetwork/MCVideo/ArbitrationApproach [168](#__RefHeading___Toc106438204)

6.2.48 /<x>/<x>/OffNetwork/MCVideo/MaxTransmissions [168](#__RefHeading___Toc106438205)

6.2.49 /*<x>*/<x>/OffNetwork/MCVideo/DefaultPPPP [168](#__RefHeading___Toc106438206)

6.2.50 /*<x>*/<x>/OffNetwork/MCVideo/DefaultPPPP/ MCVideoGroupCallSignalling [169](#__RefHeading___Toc106438207)

6.2.51 /*<x>*/<x>/OffNetwork/MCVideo/DefaultPPPP/ MCVideoGroupCallMedia [169](#__RefHeading___Toc106438208)

6.2.52 /*<x>*/<x>/OffNetwork/MCVideo/DefaultPPPP/ MCVideoEmergencyGroupCallSignalling [169](#__RefHeading___Toc106438209)

6.2.53 /*<x>*/<x>/OffNetwork/MCVideo/DefaultPPPP/ MCVideoEmergencyGroupCallMedia [170](#__RefHeading___Toc106438210)

6.2.54 /*<x>*/<x>/OffNetwork/MCVideo/DefaultPPPP/ MCVideoImminentPerilGroupCallSignalling [170](#__RefHeading___Toc106438211)

6.2.55 /*<x>*/<x>/OffNetwork/MCVideo/DefaultPPPP/ MCVideoImminentPerilGroupCallMedia [170](#__RefHeading___Toc106438212)

6.2.56 /*<x>*/<x>/OffNetwork/MCVideo/MaxDuration [171](#__RefHeading___Toc106438213)

6.2.57 /*<x>*/<x>/OffNetwork/MCVideo/EmergencyCallCancel [171](#__RefHeading___Toc106438214)

6.2.58 /*<x>*/<x>/OffNetwork/MCVideo/ImminentPerilCallCancel [171](#__RefHeading___Toc106438215)

7 MCPTT service configuration MO [171](#__RefHeading___Toc106438216)

7.1 General [171](#__RefHeading___Toc106438217)

7.2 MCPTT service configuration MO parameters [172](#__RefHeading___Toc106438218)

7.2.1 General [172](#__RefHeading___Toc106438219)

7.2.2 Node: *<x>* [172](#__RefHeading___Toc106438220)

7.2.3 /*<x>*/Name [173](#__RefHeading___Toc106438221)

7.2.4 /*<x>*/Ext/ [173](#__RefHeading___Toc106438222)

7.2.5 /*<x>*/Common [173](#__RefHeading___Toc106438223)

7.2.6 /*<x>*/Common/BroadcastMCPTTGroupCall [173](#__RefHeading___Toc106438224)

7.2.7 /*<x>*/Common/BroadcastMCPTTGroupCall/ NumLevelGroupHierarchy [174](#__RefHeading___Toc106438225)

7.2.8 /*<x>*/Common/BroadcastMCPTTGroupCall/ NumLevelUserHierarchy [174](#__RefHeading___Toc106438226)

7.2.9 /*<x>*/Common/MinLengthAliasID [174](#__RefHeading___Toc106438227)

7.2.10 /*<x>*/OffNetwork [175](#__RefHeading___Toc106438228)

7.2.11 /*<x>*/OffNetwork/PrivateCall [175](#__RefHeading___Toc106438229)

7.2.12 /*<x>*/OffNetwork/PrivateCall/MaxDuration [175](#__RefHeading___Toc106438230)

7.2.13 /*<x>*/OffNetwork/PrivateCall/HangTime [175](#__RefHeading___Toc106438231)

7.2.14 /*<x>*/OffNetwork/PrivateCall/CancelTimeout [175](#__RefHeading___Toc106438232)

7.2.15 /*<x>*/OffNetwork/EmergencyCall [176](#__RefHeading___Toc106438233)

7.2.16 /*<x>*/OffNetwork/EmergencyCall/MCPTTGroupTimeout [176](#__RefHeading___Toc106438234)

7.2.17 /*<x>*/OffNetwork/NumLevelHierarchy [176](#__RefHeading___Toc106438235)

7.2.18 /*<x>*/OffNetwork/TransmitTimeout [176](#__RefHeading___Toc106438236)

7.2.19 /*<x>*/OffNetwork/TransmissionWarning [177](#__RefHeading___Toc106438237)

7.2.20 /*<x>*/OffNetwork/HangTimeWarning [177](#__RefHeading___Toc106438238)

7.2.21 /*<x>*/OffNetwork/DefaultPPPP [177](#__RefHeading___Toc106438239)

7.2.22 /*<x>*/OffNetwork/DefaultPPPP/MCPTTPrivateCallSignalling [177](#__RefHeading___Toc106438240)

7.2.23 /*<x>*/OffNetwork/DefaultPPPP/MCPTTPrivateCallMedia [178](#__RefHeading___Toc106438241)

7.2.24 /*<x>*/OffNetwork/DefaultPPPP/ MCPTTEmergencyPrivateCallSignalling [178](#__RefHeading___Toc106438242)

7.2.25 /*<x>*/OffNetwork/DefaultPPPP/ MCPTTEmergencyPrivateCallMedia [178](#__RefHeading___Toc106438243)

7.2.26 /*<x>*/OffNetwork/LogMetadata [179](#__RefHeading___Toc106438244)

8 MCS UE initial configuration MO [179](#__RefHeading___Toc106438245)

8.1 General [179](#__RefHeading___Toc106438246)

8.2 MCS UE initial configuration MO parameters [183](#__RefHeading___Toc106438247)

8.2.1 General [183](#__RefHeading___Toc106438248)

8.2.2 Node: *<x>* [183](#__RefHeading___Toc106438249)

8.2.3 /*<x>*/Name [184](#__RefHeading___Toc106438250)

8.2.4 /*<x>*/Ext/ [184](#__RefHeading___Toc106438251)

8.2.5 /*<x>*/DefaultUserProfile [184](#__RefHeading___Toc106438252)

8.2.6 /*<x>*/DefaultUserProfile/UserID [185](#__RefHeading___Toc106438253)

8.2.7 /*<x>*/DefaultUserProfile/UserProfileIndex [185](#__RefHeading___Toc106438254)

8.2.8 /*<x>*/OnNetwork [185](#__RefHeading___Toc106438255)

8.2.9 /*<x>*/OnNetwork/GMSURI [185](#__RefHeading___Toc106438256)

8.2.9A /*<x>*/OnNetwork/GroupCreationXUI [185](#__RefHeading___Toc106438257)

8.2.9B /*<x>*/OnNetwork/GMSXCAPRootURI [186](#__RefHeading___Toc106438258)

8.2.9C /*<x>*/OnNetwork/CMSXCAPRootURI [186](#__RefHeading___Toc106438259)

8.2.10 /*<x>*/OnNetwork/Timers [186](#__RefHeading___Toc106438260)

8.2.11 /*<x>*/OnNetwork/Timers/T100 [186](#__RefHeading___Toc106438261)

8.2.12 /*<x>*/OnNetwork/Timers/T101 [187](#__RefHeading___Toc106438262)

8.2.13 /*<x>*/OnNetwork/Timers/T103 [187](#__RefHeading___Toc106438263)

8.2.14 /*<x>*/OnNetwork/Timers/T104 [187](#__RefHeading___Toc106438264)

8.2.15 /*<x>*/OnNetwork/Timers/T132 [187](#__RefHeading___Toc106438265)

8.2.16 /*<x>*/OnNetwork/HPLMN [188](#__RefHeading___Toc106438266)

8.2.17 /*<x>*/OnNetwork/HPLMN/PLMN [188](#__RefHeading___Toc106438267)

8.2.18 /*<x>*/OnNetwork/HPLMN/Service [188](#__RefHeading___Toc106438268)

8.2.19 /*<x>*/OnNetwork/HPLMN/Service/MCPTTToConRef [188](#__RefHeading___Toc106438269)

8.2.20 /*<x>*/OnNetwork/HPLMN/Service/MCPTTToConRef/<x> [188](#__RefHeading___Toc106438270)

8.2.21 /*<x>*/OnNetwork/HPLMN/Service/MCPTTToConRef/<x>/ConRef [189](#__RefHeading___Toc106438271)

8.2.22 /*<x>*/OnNetwork/HPLMN/Service/MCCommonCoreToConRef [189](#__RefHeading___Toc106438272)

8.2.23 /*<x>*/OnNetwork/HPLMN/Service/MCCommonCoreToConRef/<x> [189](#__RefHeading___Toc106438273)

8.2.24 /*<x>*/OnNetwork/HPLMN/Service/ MCCommonCoreToConRef/<x>/ConRef [189](#__RefHeading___Toc106438274)

8.2.25 /*<x>*/OnNetwork/HPLMN/Service/MCIDMToConRef [190](#__RefHeading___Toc106438275)

8.2.26 /*<x>*/OnNetwork/HPLMN/Service/MCIDMToConRef/<x> [190](#__RefHeading___Toc106438276)

8.2.27 /*<x>*/OnNetwork/HPLMN/Service/MCIDMToConRef/<x>/ConRef [190](#__RefHeading___Toc106438277)

8.2.28 /*<x>*/OnNetwork/HPLMN/VPLMN [190](#__RefHeading___Toc106438278)

8.2.29 /*<x>*/OnNetwork/HPLMN/VPLMN/PLMN [190](#__RefHeading___Toc106438279)

8.2.30 /*<x>*/OnNetwork/HPLMN/VPLMN/Service [191](#__RefHeading___Toc106438280)

8.2.31 /*<x>*/OnNetwork/HPLMN/VPLMN/Service/MCPTTToConRef [191](#__RefHeading___Toc106438281)

8.2.32 /*<x>*/OnNetwork/HPLMN/VPLMN/Service/MCPTTToConRef/<x> [191](#__RefHeading___Toc106438282)

8.2.33 /*<x>*/OnNetwork/HPLMN/VPLMN/Service/ MCPTTToConRef/<x>/ConRef [191](#__RefHeading___Toc106438283)

8.2.34 /*<x>*/OnNetwork/HPLMN/VPLMN/Service/ MCCommonCoreToConRef [192](#__RefHeading___Toc106438284)

8.2.35 /*<x>*/OnNetwork/HPLMN/VPLMN/Service/ MCCommonCoreToConRef/<x> [192](#__RefHeading___Toc106438285)

8.2.36 /*<x>*/OnNetwork/HPLMN/VPLMN/Service/ MCCommonCoreToConRef/<x>/ConRef [192](#__RefHeading___Toc106438286)

8.2.37 /*<x>*/OnNetwork/HPLMN/VPLMN/Service/MCIDMToConRef [192](#__RefHeading___Toc106438287)

8.2.38 /*<x>*/OnNetwork/HPLMN/VPLMN/Service/MCIDMToConRef/<x> [193](#__RefHeading___Toc106438288)

8.2.39 /*<x>*/OnNetwork/HPLMN/VPLMN/Service/ MCIDMToConRef/<x>/ConRef [193](#__RefHeading___Toc106438289)

8.2.40 /*<x>*/OnNetwork/AppServerInfo [193](#__RefHeading___Toc106438290)

8.2.41 /*<x>*/OnNetwork/AppServerInfo/IDMSAuthEndpoint [193](#__RefHeading___Toc106438291)

8.2.41A /*<x>*/OnNetwork/AppServerInfo/IDMSTokenEndpoint [193](#__RefHeading___Toc106438292)

8.2.41B /*<x>*/OnNetwork/AppServerInfo/HTTPProxy [194](#__RefHeading___Toc106438293)

8.2.42 /*<x>*/OnNetwork/AppServerInfo/GMS [194](#__RefHeading___Toc106438294)

8.2.43 /*<x>*/OnNetwork/AppServerInfo/CMS [194](#__RefHeading___Toc106438295)

8.2.44 /*<x>*/OnNetwork/AppServerInfo/KMS [194](#__RefHeading___Toc106438296)

8.2.44A /*<x>*/OnNetwork/AppServerInfo/TLSTunnelAuthMethod [195](#__RefHeading___Toc106438297)

8.2.44B /*<x>*/OnNetwork/AppServerInfo/TLSTunnelAuthMethod/Mutual [195](#__RefHeading___Toc106438298)

8.2.44C /*<x>*/OnNetwork/AppServerInfo/TLSTunnelAuthMethod/X509 [195](#__RefHeading___Toc106438299)

8.2.44D /*<x>*/OnNetwork/AppServerInfo/TLSTunnelAuthMethod/Key [195](#__RefHeading___Toc106438300)

8.2.44E /*<x>*/OnNetwork/IntegrityProtection [195](#__RefHeading___Toc106438301)

8.2.44F /*<x>*/OnNetwork/ConfidentialityProtection [196](#__RefHeading___Toc106438302)

8.2.44G1 /*<x>*/OnNetwork/MCPTTServiceDetails [196](#__RefHeading___Toc106438303)

8.2.44G2 /*<x>*/OnNetwork/MCPTTServiceDetails/IPv6Required [196](#__RefHeading___Toc106438304)

8.2.44G3 /*<x>*/OnNetwork/MCPTTServiceDetails/ServerURI [196](#__RefHeading___Toc106438305)

8.2.44G4 /*<x>*/OnNetwork/MCVideoServiceDetails [197](#__RefHeading___Toc106438306)

8.2.44G5 /*<x>*/OnNetwork/MCVideoServiceDetails/IPv6Required [197](#__RefHeading___Toc106438307)

8.2.44G6 /*<x>*/OnNetwork/MCVideoServiceDetails/ServerURI [197](#__RefHeading___Toc106438308)

8.2.44G7 /*<x>*/OnNetwork/MCDataServiceDetails [197](#__RefHeading___Toc106438309)

8.2.44G8 /*<x>*/OnNetwork/MCDataServiceDetails/IPv6Required [198](#__RefHeading___Toc106438310)

8.2.44G9 /*<x>*/OnNetwork/MCDataServiceDetails/ServerURI [198](#__RefHeading___Toc106438311)

8.2.45 /*<x>*/OffNetwork [198](#__RefHeading___Toc106438312)

8.2.46 /*<x>*/OffNetwork/Timers [198](#__RefHeading___Toc106438313)

8.2.47 /*<x>*/OffNetwork/Timers/TFG1 [198](#__RefHeading___Toc106438314)

8.2.48 /*<x>*/OffNetwork/Timers/TFG2 [199](#__RefHeading___Toc106438315)

8.2.49 /*<x>*/OffNetwork/Timers/TFG3 [199](#__RefHeading___Toc106438316)

8.2.50 /*<x>*/OffNetwork/Timers/TFG4 [199](#__RefHeading___Toc106438317)

8.2.51 /*<x>*/OffNetwork/Timers/TFG5 [199](#__RefHeading___Toc106438318)

8.2.52 /*<x>*/OffNetwork/Timers/TFG11 [200](#__RefHeading___Toc106438319)

8.2.53 /*<x>*/OffNetwork/Timers/TFG12 [200](#__RefHeading___Toc106438320)

8.2.54 /*<x>*/OffNetwork/Timers/TFG13 [200](#__RefHeading___Toc106438321)

8.2.54A /*<x>*/OffNetwork/Timers/TFG14 [201](#__RefHeading___Toc106438322)

8.2.55 /*<x>*/OffNetwork/Timers/TFP1 [201](#__RefHeading___Toc106438323)

8.2.56 /*<x>*/OffNetwork/Timers/TFP2 [201](#__RefHeading___Toc106438324)

8.2.57 /*<x>*/OffNetwork/Timers/TFP3 [201](#__RefHeading___Toc106438325)

8.2.58 /*<x>*/OffNetwork/Timers/TFP4 [202](#__RefHeading___Toc106438326)

8.2.59 /*<x>*/OffNetwork/Timers/TFP5 [202](#__RefHeading___Toc106438327)

8.2.60 /*<x>*/OffNetwork/Timers/TFP6 [202](#__RefHeading___Toc106438328)

8.2.61 /*<x>*/OffNetwork/Timers/TFP7 [202](#__RefHeading___Toc106438329)

8.2.61A /*<x>*/OffNetwork/Timers/TFP9 [203](#__RefHeading___Toc106438330)

8.2.62 /*<x>*/OffNetwork/Timers/TFB1 [203](#__RefHeading___Toc106438331)

8.2.63 /*<x>*/OffNetwork/Timers/TFB2 [203](#__RefHeading___Toc106438332)

8.2.64 /*<x>*/OffNetwork/Timers/TFB3 [204](#__RefHeading___Toc106438333)

8.2.65 /*<x>*/OffNetwork/Timers/T201 [204](#__RefHeading___Toc106438334)

8.2.66 /*<x>*/OffNetwork/Timers/T203 [204](#__RefHeading___Toc106438335)

8.2.67 /*<x>*/OffNetwork/Timers/T204 [204](#__RefHeading___Toc106438336)

8.2.68 /*<x>*/OffNetwork/Timers/T205 [205](#__RefHeading___Toc106438337)

8.2.69 Void [205](#__RefHeading___Toc106438338)

8.2.70 /*<x>*/OffNetwork/Timers/T233 [205](#__RefHeading___Toc106438339)

8.2.71 /*<x>*/OffNetwork/Timers/TFE1 [205](#__RefHeading___Toc106438340)

8.2.72 /*<x>*/OffNetwork/Timers/TFE2 [205](#__RefHeading___Toc106438341)

8.2.73 /*<x>*/OffNetwork/Counters [206](#__RefHeading___Toc106438342)

8.2.74 /*<x>*/OffNetwork/Counters/CFP1 [206](#__RefHeading___Toc106438343)

8.2.75 /*<x>*/OffNetwork/Counters/CFP3 [206](#__RefHeading___Toc106438344)

8.2.76 /*<x>*/OffNetwork/Counters/CFP4 [206](#__RefHeading___Toc106438345)

8.2.77 /*<x>*/OffNetwork/Counters/CFP6 [207](#__RefHeading___Toc106438346)

8.2.78 /*<x>*/OffNetwork/Counters/CFG11 [207](#__RefHeading___Toc106438347)

8.2.79 /*<x>*/OffNetwork/Counters/CFG12 [207](#__RefHeading___Toc106438348)

8.2.80 /*<x>*/OffNetwork/Counters/C201 [207](#__RefHeading___Toc106438349)

8.2.81 /*<x>*/OffNetwork/Counters/C204 [208](#__RefHeading___Toc106438350)

8.2.82 /*<x>*/OffNetwork/Counters/C205 [208](#__RefHeading___Toc106438351)

9 MCData UE configuration MO [208](#__RefHeading___Toc106438352)

9.1 General [208](#__RefHeading___Toc106438353)

9.2 MCData UE configuration MO parameters [209](#__RefHeading___Toc106438354)

9.2.1 General [209](#__RefHeading___Toc106438355)

9.2.2 Node: *<x>* [210](#__RefHeading___Toc106438356)

9.2.3 /*<x>*/Name [210](#__RefHeading___Toc106438357)

9.2.4 /*<x>*/Ext/ [210](#__RefHeading___Toc106438358)

9.2.5 /*<x>*/Common [210](#__RefHeading___Toc106438359)

9.2.6 /*<x>*/Common/MCDataGroupTxns [211](#__RefHeading___Toc106438360)

9.2.7 /*<x>*/Common/MCDataGroupTxns/MaxSDSNc4 [211](#__RefHeading___Toc106438361)

9.2.8 /*<x>*/Common/MCDataGroupTxns/SDSPresentationPriority [211](#__RefHeading___Toc106438362)

9.2.9 /*<x>*/Common/MCDataGroupTxns/SDSPresentationPriority/<x> [211](#__RefHeading___Toc106438363)

9.2.10 /*<x>*/Common/MCDataGroupTxns/ SDSPresentationPriority/<x>/MCDataGroupID [211](#__RefHeading___Toc106438364)

9.2.11 /*<x>*/Common/MCDataGroupTxns/ SDSPresentationPriority/ <x>/MCDataGroupPriorityHierarchy [212](#__RefHeading___Toc106438365)

9.2.12 /*<x>*/Common/MCDataGroupTxns/MaxFDNc4 [212](#__RefHeading___Toc106438366)

9.2.13 /*<x>*/Common/MCDataGroupTxns/FDPresentationPriority [212](#__RefHeading___Toc106438367)

9.2.14 /*<x>*/Common/MCDataGroupTxns/FDPresentationPriority/<x> [212](#__RefHeading___Toc106438368)

9.2.15 /*<x>*/Common/MCDataGroupTxns/ FDPresentationPriority/<x>/MCDataGroupID [213](#__RefHeading___Toc106438369)

9.2.16 /*<x>*/Common/MCDataGroupTxns/FDPresentationPriority/ <x>/MCDataGroupPriorityHierarchy [213](#__RefHeading___Toc106438370)

9.2.17 /*<x>*/Common/MCDataGroupTxns/ConversationPresentationPriority [213](#__RefHeading___Toc106438371)

9.2.18 /*<x>*/Common/MCDataGroupTxns/ ConversationPresentationPriority/<x> [213](#__RefHeading___Toc106438372)

9.2.19 /*<x>*/Common/MCDataGroupTxns/ ConversationPresentationPriority/<x>/MCDataGroupID [214](#__RefHeading___Toc106438373)

9.2.20 /*<x>*/Common/MCDataGroupTxns/ ConversationPresentationPriority/<x>/ MCDataGroupPriorityHierarchy [214](#__RefHeading___Toc106438374)

9.2.21 /*<x>*/Common/MCDataGroupTxns/MaxTCNc4 [214](#__RefHeading___Toc106438375)

9.2.22 /*<x>*/Common/MCDataGroupTxns/MaxTCNc5 [214](#__RefHeading___Toc106438376)

9.2.23 /*<x>*/Common/MCDataGroupTxns/DataPresentationPriority [215](#__RefHeading___Toc106438377)

9.2.24 /*<x>*/Common/MCDataGroupTxns/DataPresentationPriority/<x> [215](#__RefHeading___Toc106438378)

9.2.25 /*<x>*/Common/MCDataGroupTxns/ DataPresentationPriority/<x>/MCDataGroupID [215](#__RefHeading___Toc106438379)

9.2.26 /*<x>*/Common/MCDataGroupTxns/DataPresentationPriority/ <x>/MCDataGroupPriorityHierarchy [215](#__RefHeading___Toc106438380)

9.2.27 /*<x>*/Common/MCDataGroupTxns/MaxRCNc4 [216](#__RefHeading___Toc106438381)

9.2.28 /*<x>*/Common/MCDataGroupTxns/MaxRCNc5 [216](#__RefHeading___Toc106438382)

9.2.29 /*<x>*/OnNetwork [216](#__RefHeading___Toc106438383)

9.2.30 /*<x>*/OnNetwork/RelayService [216](#__RefHeading___Toc106438384)

9.2.31 /*<x>*/OnNetwork/IPv6Preferred [216](#__RefHeading___Toc106438385)

9.2.32 /*<x>*/OnNetwork/RelayedMCDataGroup [217](#__RefHeading___Toc106438386)

9.2.33 /*<x>*/OnNetwork/RelayedMCDataGroup/<x> [217](#__RefHeading___Toc106438387)

9.2.34 /*<x>*/OnNetwork/RelayedMCDataGroup/<x>/MCDataGroupID [217](#__RefHeading___Toc106438388)

9.2.35 /*<x>*/OnNetwork/RelayedMCDataGroup/<x>/RelayServiceCode [217](#__RefHeading___Toc106438389)

10 MCData user profile MO [218](#__RefHeading___Toc106438390)

10.1 General [218](#__RefHeading___Toc106438391)

10.2 MCData user profile MO parameters [221](#__RefHeading___Toc106438392)

10.2.1 General [221](#__RefHeading___Toc106438393)

10.2.2 Node: *<x>* [221](#__RefHeading___Toc106438394)

10.2.3 /*<x>*/Name [221](#__RefHeading___Toc106438395)

10.2.4 /*<x>*/Ext/ [222](#__RefHeading___Toc106438396)

10.2.5 /*<x>*/<x> [222](#__RefHeading___Toc106438397)

10.2.6 /*<x>*/<x>/Common [222](#__RefHeading___Toc106438398)

10.2.7 /*<x>*/*<x>*/Common/MCDataUserID [222](#__RefHeading___Toc106438399)

10.2.8 /*<x>*/*<x>*/Common/MCDataUserProfileIndex [223](#__RefHeading___Toc106438400)

10.2.9 /*<x>*/*<x>*/Common/MCDataUserProfileName [223](#__RefHeading___Toc106438401)

10.2.9A /*<x>*/*<x>*/Common/MCDataUserIDKMSURI [223](#__RefHeading___Toc106438402)

10.2.10 /*<x>*/*<x>*/Common/PreSelectedIndication [223](#__RefHeading___Toc106438403)

10.2.11 /*<x>*/<x>/Common/UserAliases [224](#__RefHeading___Toc106438404)

10.2.12 /*<x>*/<x>/Common/UserAliases/<x> [224](#__RefHeading___Toc106438405)

10.2.13 /*<x>*/*<x>*/Common/UserAliases/<x>UserAlias [224](#__RefHeading___Toc106438406)

10.2.14 /*<x>*/*<x>*/Common/AuthorisedAlias [224](#__RefHeading___Toc106438407)

10.2.15 /*<x>*/<x>/Common/ParticipantType [225](#__RefHeading___Toc106438408)

10.2.16 /*<x>*/<x>/Common/Organization [225](#__RefHeading___Toc106438409)

10.2.16A /*<x>*/*<x>*/Common/OnetoOne [225](#__RefHeading___Toc106438410)

10.2.16B /*<x>*/<x>/Common/OnetoOne/UserList [225](#__RefHeading___Toc106438411)

10.2.16C /*<x>*/<x>/Common/OnetoOne/UserList/<x> [225](#__RefHeading___Toc106438412)

10.2.16D /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry [226](#__RefHeading___Toc106438413)

10.2.16E /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry/MCDataID [226](#__RefHeading___Toc106438414)

10.2.16F /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry/ DiscoveryGroupID [226](#__RefHeading___Toc106438415)

10.2.16G /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry/UserInfoID [226](#__RefHeading___Toc106438416)

10.2.16H /*<x>*/*<x>*/Common/OnetoOne/UserList/<x>/Entry/ MCDataIDKMSURI [227](#__RefHeading___Toc106438417)

10.2.16I /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry/DisplayName [227](#__RefHeading___Toc106438418)

10.2.16J /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation [227](#__RefHeading___Toc106438419)

10.2.16K /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry/ IPInformation/<x> [227](#__RefHeading___Toc106438420)

10.2.16L /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry/ IPInformation/<x>Entry [228](#__RefHeading___Toc106438421)

10.2.16M /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry/ IPInformation/<x>Entry/IPv4Information [228](#__RefHeading___Toc106438422)

10.2.16N /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry/ IPInformation/<x>Entry/IPv6Information [228](#__RefHeading___Toc106438423)

10.2.16O /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry/ IPInformation/<x>Entry/FQDN [228](#__RefHeading___Toc106438424)

10.2.17 /*<x>*/*<x>*/Common/FileDistribution [229](#__RefHeading___Toc106438425)

10.2.18 /*<x>*/<x>/Common/FileDistribution/CancelList [229](#__RefHeading___Toc106438426)

10.2.19 /*<x>*/<x>/Common/FileDistribution/CancelList/<x> [229](#__RefHeading___Toc106438427)

10.2.20 /*<x>*/<x>/Common/FileDistribution/CancelList/<x>/Entry [229](#__RefHeading___Toc106438428)

10.2.21 /*<x>*/<x>/Common/FileDistribution/CancelList/<x>/Entry/MCDataID [229](#__RefHeading___Toc106438429)

10.2.21A /*<x>*/<x>/Common/FileDistribution/CancelList/<x>/Entry/ MCDataIDKMSURI [230](#__RefHeading___Toc106438430)

10.2.22 /*<x>*/<x>/Common/FileDistribution/CancelList/<x>/Entry/ DisplayName [230](#__RefHeading___Toc106438431)

10.2.23 /*<x>*/*<x>*/Common/TxRxControl [230](#__RefHeading___Toc106438432)

10.2.24 /*<x>*/*<x>*/Common/TxRxControl/AuthorisedTransmit [230](#__RefHeading___Toc106438433)

10.2.25 /<x>/<x>/Common/TxRxControl/MaxData1To1 [231](#__RefHeading___Toc106438434)

10.2.26 /<x>/<x>/Common/TxRxControl/MaxTime1To1 [231](#__RefHeading___Toc106438435)

10.2.27 /*<x>*/<x>/Common/TxRxControl/ReleaseList [231](#__RefHeading___Toc106438436)

10.2.28 /*<x>*/<x>/Common/TxRxControl/ReleaseList/<x> [231](#__RefHeading___Toc106438437)

10.2.29 /*<x>*/<x>/Common/TxRxControl/ReleaseList/<x>/Entry [232](#__RefHeading___Toc106438438)

10.2.30 /*<x>*/<x>/Common/TxRxControl/ReleaseList/<x>/Entry/MCDataID [232](#__RefHeading___Toc106438439)

10.2.31 /*<x>*/<x>/Common/TxRxControl/ReleaseList/<x>/Entry/ DisplayName [232](#__RefHeading___Toc106438440)

10.2.32 /*<x>*/*<x>*/Common/MCDataGroupBroadcast [232](#__RefHeading___Toc106438441)

10.2.33 /*<x>*/*<x>*/Common/MCDataGroupBroadcast/Authorised [232](#__RefHeading___Toc106438442)

10.2.34 /*<x>*/*<x>*/Common/UserBroadcast [233](#__RefHeading___Toc106438443)

10.2.35 /*<x>*/*<x>*/Common/UserBroadcast/Authorised [233](#__RefHeading___Toc106438444)

10.2.36 /*<x>*/<x>/Common/GroupEmergencyAlert [233](#__RefHeading___Toc106438445)

10.2.37 /*<x>*/<x>/Common/GroupEmergencyAlert/Entry [233](#__RefHeading___Toc106438446)

10.2.38 /*<x>*/*<x>*/Common/GroupEmergencyAlert/Entry/ID [234](#__RefHeading___Toc106438447)

10.2.39 /*<x>*/*<x>*/Common/GroupEmergencyAlert/Entry/DisplayName [234](#__RefHeading___Toc106438448)

10.2.40 /*<x>*/*<x>*/Common/GroupEmergencyAlert/Entry/Usage [234](#__RefHeading___Toc106438449)

10.2.41 /*<x>*/*<x>*/Common/AllowedActivateAlert [234](#__RefHeading___Toc106438450)

10.2.42 /*<x>*/*<x>*/Common/AllowedCancelAlert [235](#__RefHeading___Toc106438451)

10.2.43 /*<x>*/*<x>*/OnNetwork [235](#__RefHeading___Toc106438452)

10.2.44 /*<x>*/*<x>*/OnNetwork/MCDataGroupList [235](#__RefHeading___Toc106438453)

10.2.45 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x> [235](#__RefHeading___Toc106438454)

10.2.46 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry [235](#__RefHeading___Toc106438455)

10.2.47 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ MCDataGroupID [236](#__RefHeading___Toc106438456)

10.2.48 /*<x>*/*<x>*/OnNetwork/MCDataGroupList/<x>/Entry/DisplayName [236](#__RefHeading___Toc106438457)

10.2.49 Void [236](#__RefHeading___Toc106438458)

10.2.50 Void [236](#__RefHeading___Toc106438459)

10.2.51 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/GMSServID [236](#__RefHeading___Toc106438460)

10.2.52 Void [237](#__RefHeading___Toc106438461)

10.2.53 Void [237](#__RefHeading___Toc106438462)

10.2.54 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ IdMSTokenEndPoint [237](#__RefHeading___Toc106438463)

10.2.54A /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/GroupKMSURI [237](#__RefHeading___Toc106438464)

10.2.55 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RelativePresentationPriority [237](#__RefHeading___Toc106438465)

10.2.55A /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation [237](#__RefHeading___Toc106438466)

10.2.55A0 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x> [238](#__RefHeading___Toc106438467)

10.2.55A1 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/ [238](#__RefHeading___Toc106438468)

10.2.55A2 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x> [238](#__RefHeading___Toc106438469)

10.2.55A3 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry [238](#__RefHeading___Toc106438470)

10.2.55A4 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea [239](#__RefHeading___Toc106438471)

10.2.55A5 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea [239](#__RefHeading___Toc106438472)

10.2.55A6 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea/<x> [239](#__RefHeading___Toc106438473)

10.2.55A7 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea/<x>/PointCoordinateType [240](#__RefHeading___Toc106438474)

10.2.55A8 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/ Longitude [240](#__RefHeading___Toc106438475)

10.2.55A9 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/ Latitude [240](#__RefHeading___Toc106438476)

10.2.55A10 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea [241](#__RefHeading___Toc106438477)

10.2.55A11 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Center [241](#__RefHeading___Toc106438478)

10.2.55A12 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType [241](#__RefHeading___Toc106438479)

10.2.55A13 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Longitude [242](#__RefHeading___Toc106438480)

10.2.55A14 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Latitude [242](#__RefHeading___Toc106438481)

10.2.55A15 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Radius [242](#__RefHeading___Toc106438482)

10.2.55A16 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/OffsetAngle [243](#__RefHeading___Toc106438483)

10.2.55A17 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/IncludedAngle [243](#__RefHeading___Toc106438484)

10.2.55A18 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Speed [243](#__RefHeading___Toc106438485)

10.2.55A19 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Speed/MinimumSpeed [244](#__RefHeading___Toc106438486)

10.2.55A20 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Speed/MaximumSpeed [244](#__RefHeading___Toc106438487)

10.2.55A21 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Heading [244](#__RefHeading___Toc106438488)

10.2.55A22 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Heading/MinimumHeading [245](#__RefHeading___Toc106438489)

10.2.55A23 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Heading/MaximumHeading [245](#__RefHeading___Toc106438490)

10.2.55A24 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea [245](#__RefHeading___Toc106438491)

10.2.55A25 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea [246](#__RefHeading___Toc106438492)

10.2.55A26 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea/<x> [246](#__RefHeading___Toc106438493)

10.2.55A27 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea/<x>/PointCoordinateType [246](#__RefHeading___Toc106438494)

10.2.55A28 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/ Longitude [247](#__RefHeading___Toc106438495)

10.2.55A29 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/ Latitude [247](#__RefHeading___Toc106438496)

10.2.55A30 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea [247](#__RefHeading___Toc106438497)

10.2.55A31 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Center [248](#__RefHeading___Toc106438498)

10.2.55A32 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType [248](#__RefHeading___Toc106438499)

10.2.55A33 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Longitude [248](#__RefHeading___Toc106438500)

10.2.55A34 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Latitude [249](#__RefHeading___Toc106438501)

10.2.55A35 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Radius [249](#__RefHeading___Toc106438502)

10.2.55A36 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/OffsetAngle [249](#__RefHeading___Toc106438503)

10.2.55A37 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/IncludedAngle [250](#__RefHeading___Toc106438504)

10.2.55A38 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Speed [250](#__RefHeading___Toc106438505)

10.2.55A39 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Speed/MinimumSpeed [250](#__RefHeading___Toc106438506)

10.2.55A40 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Speed/MaximumSpeed [251](#__RefHeading___Toc106438507)

10.2.55A41 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Heading [251](#__RefHeading___Toc106438508)

10.2.55A42 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Heading/MinimumHeading [251](#__RefHeading___Toc106438509)

10.2.55A43 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Heading/MaximumHeading [252](#__RefHeading___Toc106438510)

10.2.55A44 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfActiveFunctionalAliases [252](#__RefHeading___Toc106438511)

10.2.55A45 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfActiveFunctionalAliases/<x> [252](#__RefHeading___Toc106438512)

10.2.55A46 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfActiveFunctionalAliases/<x>/Entry [252](#__RefHeading___Toc106438513)

10.2.55A47 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfActiveFunctionalAliases/<x>/Entry/ FunctionalAlias [253](#__RefHeading___Toc106438514)

10.2.55B /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation [253](#__RefHeading___Toc106438515)

10.2.55B0 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x> [253](#__RefHeading___Toc106438516)

10.2.55B1 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/ [253](#__RefHeading___Toc106438517)

10.2.55B2 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x> [254](#__RefHeading___Toc106438518)

10.2.55B3 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry [254](#__RefHeading___Toc106438519)

10.2.55B4 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea [254](#__RefHeading___Toc106438520)

10.2.55B5 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea [254](#__RefHeading___Toc106438521)

10.2.55B6 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea/<x> [255](#__RefHeading___Toc106438522)

10.2.55B7 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea/<x>/PointCoordinateType [255](#__RefHeading___Toc106438523)

10.2.55B8 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/ Longitude [255](#__RefHeading___Toc106438524)

10.2.55B9 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/ Latitude [256](#__RefHeading___Toc106438525)

10.2.55B10 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea [256](#__RefHeading___Toc106438526)

10.2.55B11 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Center [256](#__RefHeading___Toc106438527)

10.2.55B12 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType [257](#__RefHeading___Toc106438528)

10.2.55B13 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Longitude [257](#__RefHeading___Toc106438529)

10.2.55B14 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Latitude [257](#__RefHeading___Toc106438530)

10.2.55B15 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Radius [258](#__RefHeading___Toc106438531)

10.2.55B16 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/OffsetAngle [258](#__RefHeading___Toc106438532)

10.2.55B17 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/IncludedAngle [258](#__RefHeading___Toc106438533)

10.2.55B18 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry /EnterSpecificArea/Speed [259](#__RefHeading___Toc106438534)

10.2.55B19 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Speed/MinimumSpeed [259](#__RefHeading___Toc106438535)

10.2.55B20 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Speed/MaximumSpeed [259](#__RefHeading___Toc106438536)

10.2.55B21 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Heading [260](#__RefHeading___Toc106438537)

10.2.55B22 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Heading/MinimumHeading [260](#__RefHeading___Toc106438538)

10.2.55B23 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Heading/MaximumHeading [260](#__RefHeading___Toc106438539)

10.2.55B24 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea [261](#__RefHeading___Toc106438540)

10.2.55B25 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea [261](#__RefHeading___Toc106438541)

10.2.55B26 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea/<x> [261](#__RefHeading___Toc106438542)

10.2.55B27 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea/<x>/PointCoordinateType [262](#__RefHeading___Toc106438543)

10.2.55B28 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/ Longitude [262](#__RefHeading___Toc106438544)

10.2.55B29 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/ Latitude [262](#__RefHeading___Toc106438545)

10.2.55B30 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea [263](#__RefHeading___Toc106438546)

10.2.55B31 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Center [263](#__RefHeading___Toc106438547)

10.2.55B32 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType [263](#__RefHeading___Toc106438548)

10.2.55B33 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Longitude [264](#__RefHeading___Toc106438549)

10.2.55B34 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry /ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Latitude [264](#__RefHeading___Toc106438550)

10.2.55B35 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Radius [264](#__RefHeading___Toc106438551)

10.2.55B36 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/OffsetAngle [265](#__RefHeading___Toc106438552)

10.2.55B37 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/IncludedAngle [265](#__RefHeading___Toc106438553)

10.2.55B38 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Speed [265](#__RefHeading___Toc106438554)

10.2.55B39 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Speed/MinimumSpeed [266](#__RefHeading___Toc106438555)

10.2.55B40 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Speed/MaximumSpeed [266](#__RefHeading___Toc106438556)

10.2.55B41 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Heading [266](#__RefHeading___Toc106438557)

10.2.55B42 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Heading/MinimumHeading [267](#__RefHeading___Toc106438558)

10.2.55B43 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Heading/MaximumHeading [267](#__RefHeading___Toc106438559)

10.2.55B44 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfActiveFunctionalAliases [267](#__RefHeading___Toc106438560)

10.2.55B45 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfActiveFunctionalAliases/<x> [268](#__RefHeading___Toc106438561)

10.2.55B46 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfActiveFunctionalAliases/<x>/Entry [268](#__RefHeading___Toc106438562)

10.2.55B47 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfActiveFunctionalAliases/<x>/Entry/ FunctionalAlias [268](#__RefHeading___Toc106438563)

10.2.55B48 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ ManualDeaffiliationNotAllowedIfAffiliationRulesAreMet [268](#__RefHeading___Toc106438564)

10.2.56 /*<x>*/*<x>*/OnNetwork/ImplicitAffiliations [269](#__RefHeading___Toc106438565)

10.2.57 /*<x>*/<x>/OnNetwork/ImplicitAffiliations/<x> [269](#__RefHeading___Toc106438566)

10.2.58 /*<x>*/<x>/OnNetwork/ImplicitAffiliations/<x>/Entry [269](#__RefHeading___Toc106438567)

10.2.59 /*<x>*/<x>/OnNetwork/ImplicitAffiliations/<x>/Entry/ MCDataGroupID [269](#__RefHeading___Toc106438568)

10.2.60 /*<x>*/*<x>*/OnNetwork/ImplicitAffiliations/<x>/Entry/ DisplayName [270](#__RefHeading___Toc106438569)

10.2.61 /*<x>*/*<x>*/OnNetwork/PresenceStatus [270](#__RefHeading___Toc106438570)

10.2.62 /*<x>*/<x>/OnNetwork/PresenceStatus/<x> [270](#__RefHeading___Toc106438571)

10.2.63 /*<x>*/<x>/OnNetwork/PresenceStatus/<x>/Entry [270](#__RefHeading___Toc106438572)

10.2.64 /*<x>*/<x>/OnNetwork/PresenceStatus/<x>/Entry/MCDataID [270](#__RefHeading___Toc106438573)

10.2.65 /*<x>*/*<x>*/OnNetwork/PresenceStatus/<x>/Entry/ DisplayName [271](#__RefHeading___Toc106438574)

10.2.66 /*<x>*/*<x>*/OnNetwork/RemoteGroupChange [271](#__RefHeading___Toc106438575)

10.2.67 /*<x>*/<x>/OnNetwork/RemoteGroupChange/<x> [271](#__RefHeading___Toc106438576)

10.2.68 /*<x>*/<x>/OnNetwork/RemoteGroupChange/<x>/Entry [271](#__RefHeading___Toc106438577)

10.2.69 /*<x>*/<x>/OnNetwork/RemoteGroupChange/<x>/Entry/ MCDataID [271](#__RefHeading___Toc106438578)

10.2.70 /*<x>*/*<x>*/OnNetwork/RemoteGroupChange/<x>/Entry/ DisplayName [272](#__RefHeading___Toc106438579)

10.2.71 /*<x>*/<x>/OnNetwork/MaxAffiliationsN2 [272](#__RefHeading___Toc106438580)

10.2.72 /*<x>*/*<x>*/OnNetwork/ConversationManagement [272](#__RefHeading___Toc106438581)

10.2.73 /*<x>*/<x>/OnNetwork/ConversationManagement/ GroupHangTime [272](#__RefHeading___Toc106438582)

10.2.74 /*<x>*/<x>/OnNetwork/ConversationManagement/ GroupHangTime/<x> [273](#__RefHeading___Toc106438583)

10.2.75 /*<x>*/<x>/OnNetwork/ConversationManagement/ GroupHangTime/<x>/Entry [273](#__RefHeading___Toc106438584)

10.2.76 /*<x>*/<x>/OnNetwork/ConversationManagement/ GroupHangTime/<x>/Entry/MCDataGroupID [273](#__RefHeading___Toc106438585)

10.2.77 /*<x>*/*<x>*/OnNetwork/ConversationManagement/ GroupHangTime/<x>/Entry/DisplayName [273](#__RefHeading___Toc106438586)

10.2.78 /*<x>*/<x>/OnNetwork/ConversationManagement/ GroupHangTime/<x>/Entry/HangTime [274](#__RefHeading___Toc106438587)

10.2.79 /*<x>*/<x>/OnNetwork/ConversationManagement/ DeliveredDisposition [274](#__RefHeading___Toc106438588)

10.2.80 /*<x>*/<x>/OnNetwork/ConversationManagement/ DeliveredDisposition/<x> [274](#__RefHeading___Toc106438589)

10.2.81 /*<x>*/<x>/OnNetwork/ConversationManagement/ DeliveredDisposition/<x>/Entry [274](#__RefHeading___Toc106438590)

10.2.82 /*<x>*/<x>/OnNetwork/ConversationManagement/ DeliveredDisposition/<x>/Entry/MCDataID [275](#__RefHeading___Toc106438591)

10.2.83 /*<x>*/*<x>*/OnNetwork/ConversationManagement/ DeliveredDisposition/<x>/Entry/DisplayName [275](#__RefHeading___Toc106438592)

10.2.84 /*<x>*/<x>/OnNetwork/ConversationManagement/ ReadDisposition [275](#__RefHeading___Toc106438593)

10.2.85 /*<x>*/<x>/OnNetwork/ConversationManagement/ ReadDisposition/<x> [275](#__RefHeading___Toc106438594)

10.2.86 /*<x>*/<x>/OnNetwork/ConversationManagement/ ReadDisposition/<x>/Entry [276](#__RefHeading___Toc106438595)

10.2.87 /*<x>*/<x>/OnNetwork/ConversationManagement/ ReadDisposition/<x>/Entry/MCDataID [276](#__RefHeading___Toc106438596)

10.2.88 /*<x>*/*<x>*/OnNetwork/ConversationManagement/ ReadDisposition/<x>/Entry/DisplayName [276](#__RefHeading___Toc106438597)

10.2.89 /*<x>*/<x>/OnNetwork/OneToOneEmergencyAlert [276](#__RefHeading___Toc106438598)

10.2.90 /*<x>*/<x>/OnNetwork/OneToOneEmergencyAlert/Entry [277](#__RefHeading___Toc106438599)

10.2.91 /*<x>*/*<x>*/OnNetwork/OneToOneEmergencyAlert/Entry/ID [277](#__RefHeading___Toc106438600)

10.2.92 /*<x>*/*<x>*/OnNetwork/OneToOneEmergencyAlert/Entry/ DisplayName [277](#__RefHeading___Toc106438601)

10.2.93 /*<x>*/*<x>*/OnNetwork/OneToOneEmergencyAlert/Entry/Usage [277](#__RefHeading___Toc106438602)

10.2.94 /*<x>*/*<x>*/OnNetwork/AllowedRegroup [278](#__RefHeading___Toc106438603)

10.2.95 /*<x>*/*<x>*/OnNetwork/AllowedPresenceStatus [278](#__RefHeading___Toc106438604)

10.2.96 /*<x>*/*<x>*/OnNetwork/AllowedPresence [278](#__RefHeading___Toc106438605)

10.2.97 /*<x>*/*<x>*/OnNetwork/AllowedManualSwitch [278](#__RefHeading___Toc106438606)

10.2.97A /*<x>*/<x>/OnNetwork/MCDataContentServerURI [279](#__RefHeading___Toc106438607)

10.2.97B /*<x>*/*<x>*/OnNetwork/FunctionalAliasList [279](#__RefHeading___Toc106438608)

10.2.97B1 /<x>/<x>/OnNetwork/FunctionalAliasList/<x> [279](#__RefHeading___Toc106438609)

10.2.97B2 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry [279](#__RefHeading___Toc106438610)

10.2.97B3 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ FunctionalAlias [280](#__RefHeading___Toc106438611)

10.2.97B3A /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ DisplayName [280](#__RefHeading___Toc106438612)

10.2.97B3B /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation [280](#__RefHeading___Toc106438613)

10.2.97B3B0 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x> [280](#__RefHeading___Toc106438614)

10.2.97B3B1 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea [281](#__RefHeading___Toc106438615)

10.2.97B3B2 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/PolygonArea [281](#__RefHeading___Toc106438616)

10.2.97B3B3 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/PolygonArea/ <x> [281](#__RefHeading___Toc106438617)

10.2.97B3B4 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/PolygonArea/ <x>/PointCoordinateType [282](#__RefHeading___Toc106438618)

10.2.97B3B5 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/PolygonArea/ <x>/PointCoordinateType/Longitude [282](#__RefHeading___Toc106438619)

10.2.97B3B6 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/PolygonArea/ <x>/PointCoordinateType/Latitude [282](#__RefHeading___Toc106438620)

10.2.97B3B7 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ EllipsoidArcArea [283](#__RefHeading___Toc106438621)

10.2.97B3B8 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Center [283](#__RefHeading___Toc106438622)

10.2.97B3B9 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType [283](#__RefHeading___Toc106438623)

10.2.97B3B10 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType/Longitude [284](#__RefHeading___Toc106438624)

10.2.97B3B11 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType/Latitude [284](#__RefHeading___Toc106438625)

10.2.97B3B12 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Radius [284](#__RefHeading___Toc106438626)

10.2.97B3B13 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ EllipsoidArcArea/OffsetAngle [285](#__RefHeading___Toc106438627)

10.2.97B3B14 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ EllipsoidArcArea/IncludedAngle [285](#__RefHeading___Toc106438628)

10.2.97B3B15 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/Speed [285](#__RefHeading___Toc106438629)

10.2.97B3B16 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/Speed/ MinimumSpeed [286](#__RefHeading___Toc106438630)

10.2.97B3B17 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/Speed/ MaximumSpeed [286](#__RefHeading___Toc106438631)

10.2.97B3B18 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/Heading [286](#__RefHeading___Toc106438632)

10.2.97B3B19 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/Heading/ MinimumHeading [287](#__RefHeading___Toc106438633)

10.2.97B3B20 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/Heading/ MaximumHeading [287](#__RefHeading___Toc106438634)

10.2.97B3B21 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea [287](#__RefHeading___Toc106438635)

10.2.97B3B22 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/PolygonArea [288](#__RefHeading___Toc106438636)

10.2.97B3B23 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/PolygonArea/ <x> [288](#__RefHeading___Toc106438637)

10.2.97B3B24 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/PolygonArea/ <x>/PointCoordinateType [288](#__RefHeading___Toc106438638)

10.2.97B3B25 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/PolygonArea/ <x>/PointCoordinateType/Longitude [289](#__RefHeading___Toc106438639)

10.2.97B3B26 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/PolygonArea/ <x>/PointCoordinateType/Latitude [289](#__RefHeading___Toc106438640)

10.2.97B3B27 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/ EllipsoidArcArea [289](#__RefHeading___Toc106438641)

10.2.97B3B28 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/ EllipsoidArcArea/Center [290](#__RefHeading___Toc106438642)

10.2.97B3B29 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType [290](#__RefHeading___Toc106438643)

10.2.97B3B30 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType/Longitude [290](#__RefHeading___Toc106438644)

10.2.97B3B31 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType/Latitude [291](#__RefHeading___Toc106438645)

10.2.97B3B32 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/ EllipsoidArcArea/Radius [291](#__RefHeading___Toc106438646)

10.2.97B3B33 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/ EllipsoidArcArea/OffsetAngle [291](#__RefHeading___Toc106438647)

10.2.97B3B34 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/ EllipsoidArcArea/IncludedAngle [292](#__RefHeading___Toc106438648)

10.2.97B3B35 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/Speed [292](#__RefHeading___Toc106438649)

10.2.97B3B36 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/Speed/ MinimumSpeed [292](#__RefHeading___Toc106438650)

10.2.97B3B37 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/Speed/ MaximumSpeed [293](#__RefHeading___Toc106438651)

10.2.97B3B38 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/Heading [293](#__RefHeading___Toc106438652)

10.2.97B3B39 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/Heading/ MinimumHeading [293](#__RefHeading___Toc106438653)

10.2.97B3B40 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/Heading/ MaximumHeading [294](#__RefHeading___Toc106438654)

10.2.97B3C /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation [294](#__RefHeading___Toc106438655)

10.2.97B3C0 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x> [294](#__RefHeading___Toc106438656)

10.2.97B3C1 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea [294](#__RefHeading___Toc106438657)

10.2.97B3C2 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ PolygonArea [295](#__RefHeading___Toc106438658)

10.2.97B3C3 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ PolygonArea/<x> [295](#__RefHeading___Toc106438659)

10.2.97B3C4 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ PolygonArea/<x>/PointCoordinateType [295](#__RefHeading___Toc106438660)

10.2.97B3C5 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ PolygonArea/<x>/PointCoordinateType/Longitude [296](#__RefHeading___Toc106438661)

10.2.97B3C6 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ PolygonArea/<x>/PointCoordinateType/Latitude [296](#__RefHeading___Toc106438662)

10.2.97B3C7 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ EllipsoidArcArea [296](#__RefHeading___Toc106438663)

10.2.97B3C8 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Center [297](#__RefHeading___Toc106438664)

10.2.97B3C9 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType [297](#__RefHeading___Toc106438665)

10.2.97B3C10 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType/Longitude [297](#__RefHeading___Toc106438666)

10.2.97B3C11 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType/Latitude [298](#__RefHeading___Toc106438667)

10.2.97B3C12 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Radius [298](#__RefHeading___Toc106438668)

10.2.97B3C13 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ EllipsoidArcArea/OffsetAngle [298](#__RefHeading___Toc106438669)

10.2.97B3C14 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ EllipsoidArcArea/IncludedAngle [299](#__RefHeading___Toc106438670)

10.2.97B3C15 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Speed [299](#__RefHeading___Toc106438671)

10.2.97B3C16 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Speed/ MinimumSpeed [299](#__RefHeading___Toc106438672)

10.2.97B3C17 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Speed/ MaximumSpeed [300](#__RefHeading___Toc106438673)

10.2.97B3C18 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Heading [300](#__RefHeading___Toc106438674)

10.2.97B3C19 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Heading/ MinimumHeading [300](#__RefHeading___Toc106438675)

10.2.97B3C20 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Heading/ MaximumHeading [301](#__RefHeading___Toc106438676)

10.2.97B3C21 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea [301](#__RefHeading___Toc106438677)

10.2.97B3C22 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/PolygonArea [301](#__RefHeading___Toc106438678)

10.2.97B3C23 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/ PolygonArea/<x> [302](#__RefHeading___Toc106438679)

10.2.97B3C24 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/ PolygonArea/<x>/PointCoordinateType [302](#__RefHeading___Toc106438680)

10.2.97B3C25 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/ PolygonArea/<x>/PointCoordinateType/Longitude [302](#__RefHeading___Toc106438681)

10.2.97B3C26 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/ PolygonArea/<x>/PointCoordinateType/Latitude [303](#__RefHeading___Toc106438682)

10.2.97B3C27 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/ EllipsoidArcArea [303](#__RefHeading___Toc106438683)

10.2.97B3C28 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/ EllipsoidArcArea/Center [303](#__RefHeading___Toc106438684)

10.2.97B3C29 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType [304](#__RefHeading___Toc106438685)

10.2.97B3C30 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType/Longitude [304](#__RefHeading___Toc106438686)

10.2.97B3C31 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType/Latitude [304](#__RefHeading___Toc106438687)

10.2.97B3C32 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/ EllipsoidArcArea/Radius [305](#__RefHeading___Toc106438688)

10.2.97B3C33 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/ EllipsoidArcArea/OffsetAngle [305](#__RefHeading___Toc106438689)

10.2.97B3C34 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/ EllipsoidArcArea/IncludedAngle [305](#__RefHeading___Toc106438690)

10.2.97B3C35 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Speed [306](#__RefHeading___Toc106438691)

10.2.97B3C36 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Speed/ MinimumSpeed [306](#__RefHeading___Toc106438692)

10.2.97B3C37 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Speed/ MaximumSpeed [306](#__RefHeading___Toc106438693)

10.2.97B3C38 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Heading [307](#__RefHeading___Toc106438694)

10.2.97B3C39 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Heading/ MinimumHeading [307](#__RefHeading___Toc106438695)

10.2.97B3C40 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Heading/ MaximumHeading [307](#__RefHeading___Toc106438696)

10.2.97B3D /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ ManualDeactivationNotAllowedIfLocationCriteriaMet [308](#__RefHeading___Toc106438697)

10.2.97C /<x>/<x>/OnNetwork/AllowedQueryFunctionalAliasOtherUser [308](#__RefHeading___Toc106438698)

10.2.97D /<x>/<x>/OnNetwork/AllowedTakeoverFunctionalAliasOtherUser [308](#__RefHeading___Toc106438699)

10.2.97E /*<x>*/<x>/OnNetwork/MessageStoreHostname [308](#__RefHeading___Toc106438700)

10.2.97F /*<x>*/*<x>*/OnNetwork/AuthorisedIncomingAny [309](#__RefHeading___Toc106438701)

10.2.97G /*<x>*/<x>/OnNetwork/IncomingUserList [309](#__RefHeading___Toc106438702)

10.2.97G1 /*<x>*/<x>/OnNetwork/IncomingUserList/<x> [309](#__RefHeading___Toc106438703)

10.2.97G2 /*<x>*/<x>/OnNetwork/IncomingUserList/<x>/Entry [309](#__RefHeading___Toc106438704)

10.2.97G3 /*<x>*/<x>/OnNetwork/IncomingUserList/<x>/Entry/MCDataID [310](#__RefHeading___Toc106438705)

10.2.97G4 /*<x>*/<x>/OnNetwork/IncomingUserList/<x>/Entry/ MCDataIDKMSURI [310](#__RefHeading___Toc106438706)

10.2.98 /*<x>*/*<x>*/OffNetwork [310](#__RefHeading___Toc106438707)

10.2.99 /*<x>*/*<x>*/OffNetwork/Authorised [310](#__RefHeading___Toc106438708)

10.2.100 /*<x>*/*<x>*/OffNetwork/MCDataGroupList [311](#__RefHeading___Toc106438709)

10.2.101 /*<x>*/<x>/OffNetwork/MCDataGroupList/<x> [311](#__RefHeading___Toc106438710)

10.2.102 /*<x>*/<x>/OffNetwork/MCDataGroupList/<x>/Entry [311](#__RefHeading___Toc106438711)

10.2.103 /*<x>*/<x>/OffNetwork/MCDataGroupList/<x>/Entry/ MCDataGroupID [311](#__RefHeading___Toc106438712)

10.2.104 /*<x>*/*<x>*/OffNetwork/MCDataGroupList/<x>/Entry/DisplayName [311](#__RefHeading___Toc106438713)

10.2.105 Void [312](#__RefHeading___Toc106438714)

10.2.106 Void [312](#__RefHeading___Toc106438715)

10.2.107 /*<x>*/<x>/OffNetwork/MCDataGroupList/<x>/Entry/GMSServID [312](#__RefHeading___Toc106438716)

10.2.108 Void [312](#__RefHeading___Toc106438717)

10.2.109 Void [312](#__RefHeading___Toc106438718)

10.2.110 /*<x>*/<x>/OffNetwork/MCDataGroupList/<x>/Entry/ IdMSTokenEndPoint [312](#__RefHeading___Toc106438719)

10.2.110A /*<x>*/<x>/OffNetwork/MCDataGroupList/<x>/Entry/GroupKMSURI [312](#__RefHeading___Toc106438720)

10.2.111 /*<x>*/<x>/OffNetwork/MCDataGroupList/<x>/Entry/ RelativePresentationPriority [313](#__RefHeading___Toc106438721)

10.2.112 /*<x>*/*<x>*/OffNetwork/UserInfoID [313](#__RefHeading___Toc106438722)

10.2.113 Void [313](#__RefHeading___Toc106438723)

10.2.114 Void [313](#__RefHeading___Toc106438724)

10.2.115 Void [313](#__RefHeading___Toc106438725)

10.2.116 Void [313](#__RefHeading___Toc106438726)

10.2.117 Void [313](#__RefHeading___Toc106438727)

10.2.118 Void [313](#__RefHeading___Toc106438728)

10.2.119 Void [313](#__RefHeading___Toc106438729)

10.2.120 Void [313](#__RefHeading___Toc106438730)

10.2.121 /*<x>*/Status [313](#__RefHeading___Toc106438731)

11 MCData service configuration MO [314](#__RefHeading___Toc106438732)

11.1 General [314](#__RefHeading___Toc106438733)

11.2 MCData service configuration MO parameters [314](#__RefHeading___Toc106438734)

11.2.1 General [314](#__RefHeading___Toc106438735)

11.2.2 Node: *<x>* [315](#__RefHeading___Toc106438736)

11.2.3 /*<x>*/Name [315](#__RefHeading___Toc106438737)

11.2.4 /*<x>*/Ext/ [315](#__RefHeading___Toc106438738)

11.2.5 /*<x>*/Common [315](#__RefHeading___Toc106438739)

11.2.6 /*<x>*/Common/TxRxControl [316](#__RefHeading___Toc106438740)

11.2.7 /*<x>*/Common/TxRxControl/TimeTempDataWaiting [316](#__RefHeading___Toc106438741)

11.2.8 /*<x>*/Common/TxRxControl/TimePeriodicAnnouncement [316](#__RefHeading___Toc106438742)

11.2.9 /*<x>*/OffNetwork [316](#__RefHeading___Toc106438743)

11.2.10 /*<x>*/OffNetwork/DefaultPPPP [317](#__RefHeading___Toc106438744)

11.2.11 /*<x>*/OffNetwork/DefaultPPPP/MCDataOneToOneCallSignalling [317](#__RefHeading___Toc106438745)

11.2.12 /*<x>*/OffNetwork/DefaultPPPP/MCDataOneToOneCallMedia [317](#__RefHeading___Toc106438746)

12 MCVideo UE configuration MO [317](#__RefHeading___Toc106438747)

12.1 General [317](#__RefHeading___Toc106438748)

12.2 MCVideo UE configuration MO parameters [318](#__RefHeading___Toc106438749)

12.2.1 General [318](#__RefHeading___Toc106438750)

12.2.2 Node: *<x>* [318](#__RefHeading___Toc106438751)

12.2.3 /*<x>*/Name [319](#__RefHeading___Toc106438752)

12.2.4 /*<x>*/Ext/ [319](#__RefHeading___Toc106438753)

12.2.5 /*<x>*/Common [319](#__RefHeading___Toc106438754)

12.2.5A /*<x>*/Common/PrivateCall [319](#__RefHeading___Toc106438755)

12.2.5B /*<x>*/Common/PrivateCall/MaxCallNc10 [320](#__RefHeading___Toc106438756)

12.2.6 /*<x>*/Common/MCVideoGroupCall [320](#__RefHeading___Toc106438757)

12.2.7 /*<x>*/Common/MCVideoGroupCall/MaxCallNc4 [320](#__RefHeading___Toc106438758)

12.2.8 /*<x>*/Common/MCVideoGroupCall/MaxTransmissionNc5 [320](#__RefHeading___Toc106438759)

12.2.9 /*<x>*/Common/MCVideoGroupCall/PrioritizedMCVideoGroup [320](#__RefHeading___Toc106438760)

12.2.10 /*<x>*/Common/MCVideoGroupCall/PrioritizedMCVideoGroup/<x> [321](#__RefHeading___Toc106438761)

12.2.11 /*<x>*/Common/MCVideoGroupCall/PrioritizedMCVideoGroup/ <x>/MCVideoGroupID [321](#__RefHeading___Toc106438762)

12.2.12 /*<x>*/Common/MCVideoGroupCall/ PrioritizedMCVideoGroup/<x>/MCVideoGroupPriorityHierarchy [321](#__RefHeading___Toc106438763)

12.2.13 /*<x>*/OnNetwork [321](#__RefHeading___Toc106438764)

12.2.14 /*<x>*/OnNetwork/RelayService [322](#__RefHeading___Toc106438765)

12.2.15 /*<x>*/OnNetwork/IPv6Preferred [322](#__RefHeading___Toc106438766)

12.2.16 /*<x>*/OnNetwork/RelayedMCVideoGroup [322](#__RefHeading___Toc106438767)

12.2.17 /*<x>*/OnNetwork/RelayedMCVideoGroup/<x> [322](#__RefHeading___Toc106438768)

12.2.18 /*<x>*/OnNetwork/RelayedMCVideoGroup/<x>/MCVideoGroupID [323](#__RefHeading___Toc106438769)

12.2.19 /*<x>*/OnNetwork/RelayedMCVideoGroup/<x>/RelayServiceCode [323](#__RefHeading___Toc106438770)

13 MCVideo user profile MO [323](#__RefHeading___Toc106438771)

13.1 General [323](#__RefHeading___Toc106438772)

13.2 MCVideo user profile MO parameters [326](#__RefHeading___Toc106438773)

13.2.1 General [326](#__RefHeading___Toc106438774)

13.2.2 Node: *<x>* [326](#__RefHeading___Toc106438775)

13.2.3 /*<x>*/Name [326](#__RefHeading___Toc106438776)

13.2.4 /*<x>*/Ext/ [326](#__RefHeading___Toc106438777)

13.2.5 /*<x>*/<x> [326](#__RefHeading___Toc106438778)

13.2.6 /*<x>*/<x>/Common [327](#__RefHeading___Toc106438779)

13.2.7 /*<x>*/*<x>*/Common/MCVideoUserID [327](#__RefHeading___Toc106438780)

13.2.8 /*<x>*/*<x>*/Common/MCVideoUserProfileIndex [327](#__RefHeading___Toc106438781)

13.2.9 /*<x>*/*<x>*/Common/MCVideoUserProfileName [327](#__RefHeading___Toc106438782)

13.2.10 /*<x>*/*<x>*/Common/PreSelectedIndication [328](#__RefHeading___Toc106438783)

13.2.11 /*<x>*/<x>/Common/UserAliases [328](#__RefHeading___Toc106438784)

13.2.12 /*<x>*/<x>/Common/UserAliases/<x> [328](#__RefHeading___Toc106438785)

13.2.13 /*<x>*/*<x>*/Common/UserAliases/<x>/UserAlias [328](#__RefHeading___Toc106438786)

13.2.14 Void [329](#__RefHeading___Toc106438787)

13.2.15 /*<x>*/<x>/Common/ParticipantType [329](#__RefHeading___Toc106438788)

13.2.16 /*<x>*/<x>/Common/Organization [329](#__RefHeading___Toc106438789)

13.2.17 /*<x>*/*<x>*/Common/MCVideoGroupBroadcast [329](#__RefHeading___Toc106438790)

13.2.18 /*<x>*/*<x>*/Common/MCVideoGroupBroadcast/Authorised [329](#__RefHeading___Toc106438791)

13.2.19 /*<x>*/*<x>*/Common/UserBroadcast [330](#__RefHeading___Toc106438792)

13.2.20 /*<x>*/*<x>*/Common/UserBroadcast/Authorised [330](#__RefHeading___Toc106438793)

13.2.21 Void [330](#__RefHeading___Toc106438794)

13.2.22 Void [330](#__RefHeading___Toc106438795)

13.2.23 Void [330](#__RefHeading___Toc106438796)

13.2.24 Void [330](#__RefHeading___Toc106438797)

13.2.25 Void [330](#__RefHeading___Toc106438798)

13.2.26 Void [330](#__RefHeading___Toc106438799)

13.2.27 Void [330](#__RefHeading___Toc106438800)

13.2.28 Void [330](#__RefHeading___Toc106438801)

13.2.29 /*<x>*/*<x>*/Common/AllowedActivateAlert [330](#__RefHeading___Toc106438802)

13.2.30 /*<x>*/*<x>*/Common/AllowedCancelAlert [331](#__RefHeading___Toc106438803)

13.2.31 Void [331](#__RefHeading___Toc106438804)

13.2.32 Void [331](#__RefHeading___Toc106438805)

13.2.33 Void [331](#__RefHeading___Toc106438806)

13.2.34 Void [331](#__RefHeading___Toc106438807)

13.2.35 Void [331](#__RefHeading___Toc106438808)

13.2.36 Void [331](#__RefHeading___Toc106438809)

13.2.37 Void [331](#__RefHeading___Toc106438810)

13.2.38 Void [331](#__RefHeading___Toc106438811)

13.2.38A /*<x>*/*<x>*/Common/MCVideoGroupCall [331](#__RefHeading___Toc106438812)

13.2.38A1 /*<x>*/*<x>*/Common/MCVideoGroupCall/EmergencyAlert [331](#__RefHeading___Toc106438813)

13.2.38A2 /*<x>*/*<x>*/Common/MCVideoGroupCall/EmergencyAlert/ Authorised [332](#__RefHeading___Toc106438814)

13.2.38A3 /*<x>*/*<x>*/Common/MCVideoGroupCall/EmergencyAlert/ Cancel [332](#__RefHeading___Toc106438815)

13.2.38A4 /*<x>*/<x>/Common/MCVideoGroupCall/EmergencyAlert/ Entry [332](#__RefHeading___Toc106438816)

13.2.38A5 /*<x>*/*<x>*/Common/MCVideoGroupCall/EmergencyAlert/ Entry/ID [332](#__RefHeading___Toc106438817)

13.2.38A6 /*<x>*/*<x>*/Common/MCVideoGroupCall/EmergencyAlert/ Entry/DisplayName [333](#__RefHeading___Toc106438818)

13.2.38A7 /*<x>*/*<x>*/Common/MCVideoGroupCall/EmergencyAlert/ Entry/Usage [333](#__RefHeading___Toc106438819)

13.2.38B /*<x>*/*<x>*/Common/MCVideoGroupCall/EmergencyCall [333](#__RefHeading___Toc106438820)

13.2.38C /*<x>*/*<x>*/Common/MCVideoGroupCall/EmergencyCall/ Enabled [334](#__RefHeading___Toc106438821)

13.2.38D /*<x>*/*<x>*/Common/MCVideoGroupCall/EmergencyCall/ CancelMCVideoGroup [334](#__RefHeading___Toc106438822)

13.2.38D1 /*<x>*/*<x>*/Common/MCVideoGroupCall/EmergencyCall/ MCVideoGroupInitiation [334](#__RefHeading___Toc106438823)

13.2.38D2 /*<x>*/<x>/Common/MCVideoGroupCall/EmergencyCall/ MCVideoGroupInitiation/Entry [334](#__RefHeading___Toc106438824)

13.2.38D3 /*<x>*/*<x>*/Common/MCVideoGroupCall/EmergencyCall/ MCVideoGroupInitiation/Entry/GroupID [335](#__RefHeading___Toc106438825)

13.2.38D4 /*<x>*/*<x>*/Common/MCVideoGroupCall/EmergencyCall/ MCVideoGroupInitiation/Entry/DisplayName [335](#__RefHeading___Toc106438826)

13.2.38D5 /*<x>*/*<x>*/Common/MCVideoGroupCall/EmergencyCall/ MCVideoGroupInitiation/Entry/Usage [335](#__RefHeading___Toc106438827)

13.2.38E /*<x>*/*<x>*/Common/MCVideoGroupCall/ImminentPerilCall [336](#__RefHeading___Toc106438828)

13.2.38F /*<x>*/*<x>*/Common/MCVideoGroupCall/ImminentPerilCall/ Authorised [336](#__RefHeading___Toc106438829)

13.2.38G /*<x>*/*<x>*/Common/MCVideoGroupCall/ImminentPerilCall/Cancel [336](#__RefHeading___Toc106438830)

13.2.38G1 /*<x>*/*<x>*/Common/MCVideoGroupCall/ImminentPerilCall/ MCVideoGroupInitiation [336](#__RefHeading___Toc106438831)

13.2.38G2 /*<x>*/<x>/Common/MCVideoGroupCall/ImminentPerilCall/ MCVideoGroupInitiation/Entry [337](#__RefHeading___Toc106438832)

13.2.38G3 /*<x>*/*<x>*/Common/MCVideoGroupCall/ImminentPerilCall/ MCVideoGroupInitiation/Entry/GroupID [337](#__RefHeading___Toc106438833)

13.2.38G4 /*<x>*/*<x>*/Common/MCVideoGroupCall/ImminentPerilCall/ MCVideoGroupInitiation/DisplayName [337](#__RefHeading___Toc106438834)

13.2.38G5 /*<x>*/*<x>*/Common/MCVideoGroupCall/ImminentPerilCall/ MCVideoGroupInitiation/Entry/Usage [337](#__RefHeading___Toc106438835)

13.2.38G6 /*<x>*/*<x>*/Common/MCVideoGroupCall/Priority [338](#__RefHeading___Toc106438836)

13.2.38G7 /*<x>*/*<x>*/Common/MCVideoGroupCall/ MaxSimultaneousCallsN6 [338](#__RefHeading___Toc106438837)

13.2.38H /*<x>*/*<x>*/Common/PrivateCall [338](#__RefHeading___Toc106438838)

13.2.38I /*<x>*/*<x>*/Common/PrivateCall/Authorised [338](#__RefHeading___Toc106438839)

13.2.38I1 /*<x>*/*<x>*/Common/PrivateCall/AuthorisedAny [339](#__RefHeading___Toc106438840)

13.2.38I2 /*<x>*/<x>/Common/PrivateCall/UserList [339](#__RefHeading___Toc106438841)

13.2.38I3 /*<x>*/<x>/Common/PrivateCall/UserList/<x> [339](#__RefHeading___Toc106438842)

13.2.38I4 /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry [339](#__RefHeading___Toc106438843)

13.2.38I5 /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry/ MCVideoID [339](#__RefHeading___Toc106438844)

13.2.38I6 /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry/ DiscoveryGroupID [340](#__RefHeading___Toc106438845)

13.2.38I7 /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry/UserInfoID [340](#__RefHeading___Toc106438846)

13.2.38I8 /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry/ DisplayName [340](#__RefHeading___Toc106438847)

13.2.38I9 /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry/ PrivateCallKMSURI [340](#__RefHeading___Toc106438848)

13.2.38J /*<x>*/*<x>*/Common/PrivateCall/ManualCommence [341](#__RefHeading___Toc106438849)

13.2.38K /*<x>*/*<x>*/Common/PrivateCall/AutoCommence [341](#__RefHeading___Toc106438850)

13.2.38L /*<x>*/*<x>*/Common/PrivateCall/FailRestrict [341](#__RefHeading___Toc106438851)

13.2.38M Void [341](#__RefHeading___Toc106438852)

13.2.38N /*<x>*/*<x>*/Common/PrivateCall/AllowedMediaProtection [341](#__RefHeading___Toc106438853)

13.2.38O /*<x>*/*<x>*/Common/PrivateCall/EmergencyCall [342](#__RefHeading___Toc106438854)

13.2.38P /*<x>*/*<x>*/Common/PrivateCall/EmergencyCall/Authorised [342](#__RefHeading___Toc106438855)

13.2.38Q /*<x>*/*<x>*/Common/PrivateCall/EmergencyCall/CancelPriority [342](#__RefHeading___Toc106438856)

13.2.38R /*<x>*/*<x>*/Common/PrivateCall/EmergencyCall/ MCVideoPrivateRecipient [343](#__RefHeading___Toc106438857)

13.2.38S /*<x>*/<x>/Common/PrivateCall/EmergencyCall/ MCVideoPrivateRecipient/Entry [343](#__RefHeading___Toc106438858)

13.2.38T /*<x>*/*<x>*/Common/PrivateCall/EmergencyCall/ MCVideoPrivateRecipient/Entry/ID [343](#__RefHeading___Toc106438859)

13.2.38U /*<x>*/<x>/Common/PrivateCall/EmergencyCall/ MCVideoPrivateRecipient/Entry/DiscoveryGroupID [343](#__RefHeading___Toc106438860)

13.2.38V /*<x>*/<x>/Common/PrivateCall/EmergencyCall/ MCVideoPrivateRecipient/Entry/UserInfoID [344](#__RefHeading___Toc106438861)

13.2.38W /*<x>*/*<x>*/Common/PrivateCall/EmergencyCall/ MCVideoPrivateRecipient/Entry/DisplayName [344](#__RefHeading___Toc106438862)

13.2.38X /*<x>*/*<x>*/Common/PrivateCall/EmergencyCall/ MCVideoPrivateRecipient/Entry/Usage [344](#__RefHeading___Toc106438863)

13.2.38Y /*<x>*/*<x>*/Common/PrivateCall/AutoAnswer [345](#__RefHeading___Toc106438864)

13.2.39 /*<x>*/*<x>*/OnNetwork [345](#__RefHeading___Toc106438865)

13.2.40 /*<x>*/*<x>*/OnNetwork/MCVideoGroupList [345](#__RefHeading___Toc106438866)

13.2.41 /*<x>*/<x>/OnNetwork/MCVideoGroupList/<x> [345](#__RefHeading___Toc106438867)

13.2.42 /*<x>*/<x>/OnNetwork/MCVideoGroupList/<x>/Entry [345](#__RefHeading___Toc106438868)

13.2.43 /*<x>*/<x>/OnNetwork/MCVideoGroupList/<x>/Entry/ MCVideoGroupID [346](#__RefHeading___Toc106438869)

13.2.44 /*<x>*/*<x>*/OnNetwork/MCVideoGroupList/<x>/Entry/ DisplayName [346](#__RefHeading___Toc106438870)

13.2.45 Void [346](#__RefHeading___Toc106438871)

13.2.46 Void [346](#__RefHeading___Toc106438872)

13.2.47 /*<x>*/<x>/OnNetwork/MCVideoGroupList/<x>/Entry/GMSServID [346](#__RefHeading___Toc106438873)

13.2.48 Void [347](#__RefHeading___Toc106438874)

13.2.49 Void [347](#__RefHeading___Toc106438875)

13.2.50 /*<x>*/<x>/OnNetwork/MCVideoGroupList/<x>/Entry/ IdMSTokenEndPoint [347](#__RefHeading___Toc106438876)

13.2.50A Void [347](#__RefHeading___Toc106438877)

13.2.50B Void [347](#__RefHeading___Toc106438878)

13.2.50C Void [347](#__RefHeading___Toc106438879)

13.2.50D /<x>/<x>/OnNetwork/MCVideoGroupList/<x>/Entry/ GroupKMSURI [347](#__RefHeading___Toc106438880)

13.2.51 /*<x>*/<x>/OnNetwork/MCVideoGroupList/<x>/Entry/ RelativePresentationPriority [347](#__RefHeading___Toc106438881)

13.2.52 /*<x>*/*<x>*/OnNetwork/ImplicitAffiliations [348](#__RefHeading___Toc106438882)

13.2.53 /*<x>*/<x>/OnNetwork/ImplicitAffiliations/<x> [348](#__RefHeading___Toc106438883)

13.2.54 /*<x>*/<x>/OnNetwork/ImplicitAffiliations/<x>/Entry [348](#__RefHeading___Toc106438884)

13.2.55 /*<x>*/<x>/OnNetwork/ImplicitAffiliations/<x>/Entry/ MCVideoGroupID [348](#__RefHeading___Toc106438885)

13.2.56 /*<x>*/*<x>*/OnNetwork/ImplicitAffiliations/<x>/Entry/ DisplayName [348](#__RefHeading___Toc106438886)

13.2.57 /*<x>*/*<x>*/OnNetwork/PresenceStatus [349](#__RefHeading___Toc106438887)

13.2.58 /*<x>*/<x>/OnNetwork/PresenceStatus/<x> [349](#__RefHeading___Toc106438888)

13.2.59 /*<x>*/<x>/OnNetwork/PresenceStatus/<x>/Entry [349](#__RefHeading___Toc106438889)

13.2.60 /*<x>*/<x>/OnNetwork/PresenceStatus/<x>/Entry/ MCVideoGroupID [349](#__RefHeading___Toc106438890)

13.2.61 /*<x>*/*<x>*/OnNetwork/PresenceStatus/<x>/Entry/DisplayName [350](#__RefHeading___Toc106438891)

13.2.62 Void [350](#__RefHeading___Toc106438892)

13.2.63 Void [350](#__RefHeading___Toc106438893)

13.2.64 Void [350](#__RefHeading___Toc106438894)

13.2.65 Void [350](#__RefHeading___Toc106438895)

13.2.66 Void [350](#__RefHeading___Toc106438896)

13.2.67 /*<x>*/<x>/OnNetwork/MaxAffiliationsN2 [350](#__RefHeading___Toc106438897)

13.2.68 /*<x>*/*<x>*/OnNetwork/AllowedRegroup [350](#__RefHeading___Toc106438898)

13.2.69 /*<x>*/*<x>*/OnNetwork/AllowedPresenceStatus [350](#__RefHeading___Toc106438899)

13.2.70 /*<x>*/*<x>*/OnNetwork/AllowedPresence [351](#__RefHeading___Toc106438900)

13.2.71 /*<x>*/*<x>*/OnNetwork/AllowedManualSwitch [351](#__RefHeading___Toc106438901)

13.2.72 Void [351](#__RefHeading___Toc106438902)

13.2.73 /*<x>*/*<x>*/OnNetwork/MaxSimultaneousVideoStreams [351](#__RefHeading___Toc106438903)

13.2.74 /*<x>*/<x>/OnNetwork/MaxSimultaneousVideoStreams/ MaxStreams [352](#__RefHeading___Toc106438904)

13.2.75 Void [352](#__RefHeading___Toc106438905)

13.2.76 Void [352](#__RefHeading___Toc106438906)

13.2.77 Void [352](#__RefHeading___Toc106438907)

13.2.78 Void [352](#__RefHeading___Toc106438908)

13.2.79 Void [352](#__RefHeading___Toc106438909)

13.2.80 Void [352](#__RefHeading___Toc106438910)

13.2.81 Void [352](#__RefHeading___Toc106438911)

13.2.82 Void [352](#__RefHeading___Toc106438912)

13.2.83 Void [352](#__RefHeading___Toc106438913)

13.2.84 Void [352](#__RefHeading___Toc106438914)

13.2.85 Void [352](#__RefHeading___Toc106438915)

13.2.86 Void [352](#__RefHeading___Toc106438916)

13.2.87 Void [352](#__RefHeading___Toc106438917)

13.2.87A /*<x>*/*<x>*/OnNetwork/EnabledParticipation [352](#__RefHeading___Toc106438918)

13.2.87A1 /*<x>*/*<x>*/OnNetwork/AllowedRemoteInitiatedAmbientViewing [353](#__RefHeading___Toc106438919)

13.2.87A2 /*<x>*/*<x>*/OnNetwork/AllowedLocallyInitiatedAmbientViewing [353](#__RefHeading___Toc106438920)

13.2.87D /*<x>*/*<x>*/OnNetwork/PrivateCall [353](#__RefHeading___Toc106438921)

13.2.87E /*<x>*/*<x>*/OnNetwork/PrivateCall/EmergencyAlert [353](#__RefHeading___Toc106438922)

13.2.87F /*<x>*/*<x>*/OnNetwork/PrivateCall/EmergencyAlert/Entry [354](#__RefHeading___Toc106438923)

13.2.87G /*<x>*/*<x>*/OnNetwork/PrivateCall/EmergencyAlert/Entry/ID [354](#__RefHeading___Toc106438924)

13.2.87H /*<x>*/*<x>*/OnNetwork/PrivateCall/EmergencyAlert/Entry/ DisplayName [354](#__RefHeading___Toc106438925)

13.2.87I /*<x>*/*<x>*/OnNetwork/PrivateCall/EmergencyAlert/Entry/Usage [354](#__RefHeading___Toc106438926)

13.2.87J /*<x>*/*<x>*/OnNetwork/RemoteGroupSelection [355](#__RefHeading___Toc106438927)

13.2.87K /*<x>*/<x>/OnNetwork/RemoteGroupSelection/<x> [355](#__RefHeading___Toc106438928)

13.2.87L /*<x>*/<x>/OnNetwork/RemoteGroupSelection/<x>/Entry [355](#__RefHeading___Toc106438929)

13.2.87M /*<x>*/<x>/OnNetwork/RemoteGroupSelection/<x>/Entry/ MCVideoID [355](#__RefHeading___Toc106438930)

13.2.87N /*<x>*/*<x>*/OnNetwork/RemoteGroupSelection/<x>/Entry/ DisplayName [355](#__RefHeading___Toc106438931)

13.2.88 /*<x>*/*<x>*/OffNetwork [356](#__RefHeading___Toc106438932)

13.2.89 /*<x>*/*<x>*/OffNetwork/Authorised [356](#__RefHeading___Toc106438933)

13.2.90 /*<x>*/*<x>*/OffNetwork/MCVideoGroupList [356](#__RefHeading___Toc106438934)

13.2.91 /*<x>*/<x>/OffNetwork/MCVideoGroupList/<x> [356](#__RefHeading___Toc106438935)

13.2.92 /*<x>*/<x>/OffNetwork/MCVideoGroupList/<x>/Entry [357](#__RefHeading___Toc106438936)

13.2.93 /*<x>*/<x>/OffNetwork/MCVideoGroupList/<x>/Entry/ MCVideoGroupID [357](#__RefHeading___Toc106438937)

13.2.94 /*<x>*/*<x>*/OffNetwork/MCVideoGroupList/<x>/Entry/DisplayName [357](#__RefHeading___Toc106438938)

13.2.95 Void [357](#__RefHeading___Toc106438939)

13.2.96 Void [357](#__RefHeading___Toc106438940)

13.2.97 /*<x>*/<x>/OffNetwork/MCVideoGroupList/<x>/Entry/GMSServID [357](#__RefHeading___Toc106438941)

13.2.98 Void [358](#__RefHeading___Toc106438942)

13.2.99 Void [358](#__RefHeading___Toc106438943)

13.2.100 /*<x>*/<x>/OffNetwork/MCVideoGroupList/<x>/Entry/ IdMSTokenEndPoint [358](#__RefHeading___Toc106438944)

13.2.100A Void [358](#__RefHeading___Toc106438945)

13.2.100B Void [358](#__RefHeading___Toc106438946)

13.2.100C /*<x>*/*<x>*/OffNetwork/MCVideoGroupList/<x>/Entry/ GroupKMSURI [358](#__RefHeading___Toc106438947)

13.2.101 /*<x>*/<x>/OffNetwork/MCVideoGroupList/<x>/Entry/ RelativePresentationPriority [358](#__RefHeading___Toc106438948)

13.2.102 /*<x>*/*<x>*/OffNetwork/UserInfoID [359](#__RefHeading___Toc106438949)

13.2.102A /*<x>*/*<x>*/OffNetwork/EmergencyCallChange [359](#__RefHeading___Toc106438950)

13.2.102B /*<x>*/*<x>*/OffNetwork/ImminentPerilCallChange [359](#__RefHeading___Toc106438951)

13.2.103 /*<x>*/Status [359](#__RefHeading___Toc106438952)

14 MCVideo service configuration MO [360](#__RefHeading___Toc106438953)

14.1 General [360](#__RefHeading___Toc106438954)

14.2 MCVideo service configuration MO parameters [360](#__RefHeading___Toc106438955)

14.2.1 General [360](#__RefHeading___Toc106438956)

14.2.2 Node: *<x>* [360](#__RefHeading___Toc106438957)

14.2.3 /*<x>*/Name [361](#__RefHeading___Toc106438958)

14.2.4 /*<x>*/Ext/ [361](#__RefHeading___Toc106438959)

14.2.5 /*<x>*/Common [361](#__RefHeading___Toc106438960)

14.2.6 /*<x>*/Common/BroadcastMCVideoGroupCall [361](#__RefHeading___Toc106438961)

14.2.7 /*<x>*/Common/BroadcastMCVideoGroupCall/ NumLevelGroupHierarchy [362](#__RefHeading___Toc106438962)

14.2.8 /*<x>*/Common/BroadcastMCVideoGroupCall/ NumLevelUserHierarchy [362](#__RefHeading___Toc106438963)

14.2.9 /*<x>*/Common/MinLengthAliasID [362](#__RefHeading___Toc106438964)

14.2.10 /*<x>*/OffNetwork [363](#__RefHeading___Toc106438965)

14.2.11 /*<x>*/OffNetwork/DefaultPPPP [363](#__RefHeading___Toc106438966)

14.2.12 /*<x>*/OffNetwork/DefaultPPPP/MCVideoPrivateCallSignalling [363](#__RefHeading___Toc106438967)

14.2.13 /*<x>*/OffNetwork/DefaultPPPP/MCVideoPrivateCallMedia [363](#__RefHeading___Toc106438968)

14.2.14 /*<x>*/OffNetwork/DefaultPPPP/ MCVideoEmergencyPrivateCallSignalling [364](#__RefHeading___Toc106438969)

14.2.15 /*<x>*/OffNetwork/DefaultPPPP/ MCVideoEmergencyPrivateCallMedia [364](#__RefHeading___Toc106438970)

14.2.16 /*<x>*/OffNetwork/PrivateCall [364](#__RefHeading___Toc106438971)

14.2.17 /*<x>*/OffNetwork/PrivateCall/MaxDuration [364](#__RefHeading___Toc106438972)

14.2.18 /*<x>*/OffNetwork/NumLevelHierarchy [365](#__RefHeading___Toc106438973)

Annex A (informative): MCPTT UE configuration MO DDF [366](#__RefHeading___Toc106438974)

Annex B (informative): MCPTT user profile MO DDF [367](#__RefHeading___Toc106438975)

Annex C (informative): MCS group configuration MO DDF [368](#__RefHeading___Toc106438976)

Annex D (informative): MCPTT service configuration MO DDF [369](#__RefHeading___Toc106438977)

Annex E (informative): MCS UE initial configuration MO DDF [370](#__RefHeading___Toc106438978)

Annex F (informative): MCVideo UE configuration MO DDF [371](#__RefHeading___Toc106438979)

Annex G (informative): MCVideo user profile configuration MO DDF [372](#__RefHeading___Toc106438980)

Annex H (informative): MCVideo service configuration MO DDF [373](#__RefHeading___Toc106438981)

Annex I (informative): MCData UE configuration MO DDF [374](#__RefHeading___Toc106438982)

Annex J (informative): MCData user profile configuration MO DDF [375](#__RefHeading___Toc106438983)

Annex K (informative): MCData service configuration MO DDF [376](#__RefHeading___Toc106438984)

Annex L (informative): Change history [377](#__RefHeading___Toc106438985)

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# 1 Scope

The present document defines a number of Mission Critical Services (MCSs) Management Objects (MO) that are configured for the UE for the operation of MCSs. The management objects are compatible with OMA Device Management protocol specifications, version 1.2 and upwards, and is defined using the OMA DM Device Description Framework as described in the Enabler Release Definition OMA OMA-ERELD\_DM-V1\_2 [2].

MCSs are services that require preferential handling compared to normal telecommunication services, e.g. in support of police or fire brigade.

MCSs can be used for public safety applications and also for general commercial applications (e.g., utility companies and railways).

The present document is applicable to an UE supporting on-line, off-line or both on-line and off-line configuration of the configuration management client.

The present document is applicable to an UE supporting off-line configuration of the group management client.

The parameters defined by the management objects in the present document are configured in the UE using on-line configuration over the CSC-4 reference point and using off-line configuration over the CSC-11 and CSC-12 reference points. Other specifications define how these parameters are used in the operation of MCSs, and whether they are applicable to on-network operation or off-network operation, or both:

- 3GPP TS 24.379 [7];

- 3GPP TS 24.380 [8];

- 3GPP TS 24.481 [9];

- 3GPP TS 24.482 [11];

- 3GPP TS 24.484 [12];

- 3GPP TS 24.282 [16];

- 3GPP TS 24.582 [17];

- 3GPP TS 24.281 [18]; and

- 3GPP TS 24.581 [19].

The common network operation means both on-network operation and off-network operation in the present document.

The following management objects are defined in the present document:

- MCPTT UE configuration MO;

- MCPTT user profile MO;

- MCS group configuration MO;

- MCPTT service configuration MO;

- MCS UE initial configuration MO;

- MCData UE configuration MO;

- MCData user profile MO;

- MCData service configuration MO;

- MCVideo UE configuration MO;

- MCVideo user profile MO; and

- MCVideo service configuration MO.

The MOs listed above define repositories of data in the ME.

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] OMA OMA-ERELD-DM-V1\_2-20070209-A: "Enabler Release Definition for OMA Device Management, Version 1.2".

[3] OMA OMA-TS-DM\_Protocol-V1\_2: "OMA Device Management Protocol".

[4] OMA OMA-TS-XDM\_Group-V1\_1-20120403-A: "Group XDM Specification".

[5] 3GPP TS 23.003: "Numbering, addressing and identification".

[6] 3GPP TS 23.303: "Proximity-based Services (ProSe); Stage 2".

[7] 3GPP TS 24.379: "Mission Critical Push To Talk (MCPTT) call control Protocol specification".

[8] 3GPP TS 24.380: "Mission Critical Push To Talk (MCPTT) media plane control Protocol specification".

[9] 3GPP TS 24.481: "Mission Critical Services (MCS) group management Protocol specification".

[10] 3GPP TS 31.102: "Characteristics of the USIM Application".

[11] 3GPP TS 24.482: "Mission Critical Services (MCS) identity management Protocol specification".

[12] 3GPP TS 24.484: "Mission Critical Services (MCS) configuration management Protocol specification".

[13] IETF RFC 4566 (July 2006): "Session Description Protocol".

[14] Void.

[15] 3GPP TS 23.179: "Functional architecture and information flows to support mission critical communication services; Stage 2".

[16] 3GPP TS 24.282: "Mission Critical Data (MCData) signalling control Protocol specification".

[17] 3GPP TS 24.582: "Mission Critical Data (MCData) media plane control Protocol specification".

[18] 3GPP TS 24.281: "Mission Critical Video (MCVideo) signalling control Protocol specification".

[19] 3GPP TS 24.581: "Mission Critical Video (MCVideo) media plane control Protocol specification".

[20] 3GPP TS 33.180: "Security of the mission critical service".

[21] 3GPP TS 23.032: "Universal Geographical Area Description (GAD)".

# 3 Definitions and abbreviations

## 3.1 Definitions

For the purpose of the present document, the following terms and definitions given in 3GPP TS 23.179 [15] apply:

**Pre-selected MCPTT user profile**

## 3.2 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

ACL Access Control List

CMS Configuration Management Server

DDF Device Description Framework

DM Device Management

GMS Group Management Server

MCS Mission Critical Service

MCSs Mission Critical Services

MCPTT Mission Critical Push To Talk

ME Mobile Equipment

MO Management Object

OMA Open Mobile Alliance

ProSe Proximity-based Services

RFC Request For Comments

URI Uniform Resource Identifier

URN Uniform Resource Name

XCAP XML Configuration Access Protocol

XML eXtensible Markup Language

XUI XCAP Unique Identifier

# 4 MCPTT UE configuration MO

## 4.1 General

The MCPTT UE configuration Management Object (MO) is used to configure MCPTT Client behaviour for the on-network or off-network MCPTT Service. The MCPTT UE configuration parameters may be stored in the ME, or in the USIM as specified in 3GPP TS 31.102 [10], or in both the ME and the USIM. If both the ME and the USIM contain the same parameters, the values stored in the USIM shall take precedence.

The Management Object Identifier is: urn:oma:mo:ext-3gpp-MCPTT-UE-configuration:1.0.

Protocol compatibility: This MO is compatible with OMA OMA DM 1.2 [3].

The OMA DM ACL property mechanism (see OMA OMA-ERELD-DM-V1\_2 [2]) may be used to grant or deny access rights to OMA DM servers in order to modify nodes and leaf objects of the MCPTT UE configuration MO.

The following nodes and leaf objects are possible under the MCPTT UE configuration node as described in figure 4.1.1.



Figure 4.1.1: The MCPTT UE configuration MO

## 4.2 MCPTT UE configuration MO parameters

### 4.2.1 General

This clause describes the parameters for the MCPTT UE configuration Management Object (MO).

### 4.2.2 Node: *<x>*

Table 4.2.2.1: Node: <x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get |  |
|  | This interior node acts as a placeholder for the MCPTT UE configuration Management Object (MO).  For the MCPTT UE configuration MO, the namespace specific string is: "urn:oma:mo:oma-dm-mcptt-ue-configuration:1.0" | | | | |

- Values: N/A

### 4.2.3 /*<x>*/Name

Table 4.2.3.1: /<x>/Name

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | chr | Get |  |
|  | The Name leaf is a name for the MCPTT UE configuration settings. | | | | |

- Values: <User displayable name>

### 4.2.4 /*<x>*/Ext/

Table 4.2.4.1: /<x>/Ext/

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Ext | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | The Ext is an interior node for where the vendor specific information about the MCPTT UE configuration MO is being placed. | | | | |

Usually the vendor extension is identified by vendor specific name under the ext node and contains the vendor meaning application vendor, device vendor etc. The tree structure under the vendor identified is not defined and can therefore include one or more un-standardized sub-trees.

- Values: N/A

### 4.2.5 /*<x>*/Common

Table 4.2.5.1: /*<x>*/Common

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | node | Get, Replace |  |
|  | This interior node represents a container for the common network operation which means both on-network operation and off-network operation. | | | | |

### 4.2.6 /*<x>*/Common/PrivateCall

Table 4.2.6.1: /*<x>*/Common/PrivateCall

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/PrivateCall | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the private call configuration. | | | | |

### 4.2.7 /*<x>*/Common/PrivateCall/MaxCallN10

Table 4.2.7.1: /*<x>*/Common/PrivateCall/MaxCallN10

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/PrivateCall/MaxCallN10 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the maximum number of private calls. | | | | |

- Values: 0-255

### 4.2.8 /*<x>*/Common/MCPTTGroupCall

Table 4.2.8.1: /*<x>*/Common/MCPTTGroupCall

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCPTTGroupCall | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the MCPTT group call configuration. | | | | |

### 4.2.9 /*<x>*/Common/MCPTTGroupCall/MaxCallN4

Table 4.2.9.1: /*<x>*/Common/MCPTTGroupCall/MaxCallN4

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCPTTGroupCall/MaxCallN4 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the maximum number of simultaneous group calls. | | | | |

- Values: 0-255

### 4.2.10 /*<x>*/Common/MCPTTGroupCall/MaxTransmissionN5

Table 4.2.10.1: /*<x>*/Common/MCPTTGroupCall/MaxTransmissionN5

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCPTTGroupCall/MaxTransmissionN5 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the maximum number of transmissions in a group. | | | | |

- Values: 0-255

### 4.2.11 /*<x>*/Common/MCPTTGroupCall/PrioritizedMCPTTGroup

Table 4.2.11.1: /*<x>*/Common/MCPTTGroupCall/PrioritizedMCPTTGroup

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCPTTGroupCall/PrioritizedMCPTTGroup | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the prioritized MCPTT group call configuration. | | | | |

### 4.2.12 /*<x>*/Common/MCPTTGroupCall/PrioritizedMCPTTGroup/<x>

Table 4.2.12.1: /*<x>*/Common/MCPTTGroupCall/PrioritizedMCPTTGroup/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCPTTGroupCall/PrioritizedMCPTTGroup /<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more prioritized MCPTT group call configuration. | | | | |

### 4.2.13 /*<x>*/Common/MCPTTGroupCall/PrioritizedMCPTTGroup/<x>/ MCPTTGroupID

Table 4.2.13.1: /*<x>*/Common/MCPTTGroupCall/PrioritizedMCPTTGroup/<x>/MCPTTGroupID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCPTTGroupCall/PrioritizedMCPTTGroup/<x>/MCPTTGroupID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the associated MCPTT group ID. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 4.2.14 /*<x>*/Common/MCPTTGroupCall/PrioritizedMCPTTGroup/<x>/ MCPTTGroupPriorityHierarchy

Table 4.2.14.1: /*<x>*/Common/MCPTTGroupCall/PrioritizedMCPTTGroup/<x>/MCPTTGroupPriorityHierarchy

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCPTTGroupCall/PrioritizedMCPTTGroup/<x>/MCPTTGroupPriorityHierarchy | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the requested presentation priority of group call. | | | | |

- Values: 0-7

The group with the lowest MCPTTGroupPriorityHierarchy value shall be considered as the group having the lowest priority among the groups.

### 4.2.15 /*<x>*/OnNetwork

Table 4.2.15.1: /*<x>*/OnNetwork

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | node | Get, Replace |  |
|  | This interior node represents a container for on-network operation. | | | | |

### 4.2.16 /*<x>*/OnNetwork/RelayService

Table 4.2.16.1: /*<x>*/OnNetwork/RelayService

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/RelayService | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to use a relay service. | | | | |

When set to "true" the MCPTT group is allowed to use a relay service.

When set to "false" the MCPTT group is not allowed to use a relay service.

### 4.2.17 /*<x>*/OnNetwork/IPv6Preferred

Table 4.2.17.1: /*<x>*/OnNetwork/IPv6Preferred

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/IPv6Preferred | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether IPv6 is preferred over IPv4 for on-network operation when the MCPTT UE has both IPv4 and IPv6 host configuration. | | | | |

If the MCPTT UE has both IPv4 and IPv6 host configuration and:

- if IPv6Preferred is set to "true" then the UE uses IPv6 for all on‑network signalling and media; otherwise

- if IPv6Preferred is set to "false" then the UE uses IPv4 for all on‑network signalling and media.

### 4.2.18 /*<x>*/OnNetwork/RelayedMCPTTGroup

Table 4.2.18.1: /*<x>*/OnNetwork/RelayedMCPTTGroup

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/RelayedMCPTTGroup | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node is a placeholder for the allowed relayed MCPTT groups. | | | | |

### 4.2.19 /*<x>*/OnNetwork/RelayedMCPTTGroup/<x>

Table 4.2.19.1: /*<x>*/OnNetwork/RelayedMCPTTGroup/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/RelayedMCPTTGroup/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more allowed relayed MCPTT groups. | | | | |

### 4.2.20 /*<x>*/OnNetwork/RelayedMCPTTGroup/<x>/MCPTTGroupID

Table 4.2.20.1: /*<x>*/OnNetwork/RelayedMCPTTGroup/<x>/MCPTTGroupID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/RelayedMCPTTGroup/<x>/MCPTTGroupID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the associated MCPTT group ID. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 4.2.21 /*<x>*/OnNetwork/RelayedMCPTTGroup/<x>/RelayServiceCode

Table 4.2.21.1: /*<x>*/OnNetwork/RelayedMCPTTGroup/<x>/RelayServiceCode

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/RelayedMCPTTGroup/<x>/RelayServiceCode | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the connectivity service that the ProSe UE-to-network relay provides to public safety applications as specified in 3GPP TS 23.303 [6]. | | | | |

# 5 MCPTT user profile MO

## 5.1 General

The MCPTT user profile configuration Management Object (MO) is used to configure the MCPTT Client behaviour for the on-network or off-network MCPTT Service. The MCPTT UE configuration parameters may be stored in the ME, or in the USIM as specified in 3GPP TS 31.102 [10], or in both the ME and the USIM. If both the ME and the USIM contain the same parameters, the values stored in the USIM shall take precedence.

The Management Object Identifier is: urn:oma:mo:ext-3gpp-MCPTT-user-profile:1.0.

Protocol compatibility: This MO is compatible with OMA OMA DM 1.2 [3].

The OMA DM ACL property mechanism (see OMA OMA-ERELD-DM-V1\_2 [2]) may be used to grant or deny access rights to OMA DM servers in order to modify nodes and leaf objects of the MCPTT user profile MO.

The following nodes and leaf objects are possible under the MCPTT user profile node as described in figure 5.1.1, figure 5.1.2, figure 5.1.3, figure 5.1.4, figure 5.1.5, figure 5.1.6, figure 5.1.7, and figure 5.1.8.



Figure 5.1.1: The MCPTT user profile MO (1 of 3)



Figure 5.1.2: The MCPTT user profile MO (2 of 3)



Figure 5.1.3: The MCPTT user profile MO (3 of 3)



NOTE 1: The LocationCriteriaForDeactivation MO contents are identical.

NOTE 2: This figure is referenced by figures 5.1.3 and 10.1.2.

Figure 5.1.4: LocationCriteriaForActivation MO contents



NOTE: The ExitSpecificArea MO contents are identical.

Figure 5.1.5: EnterSpecificArea MO contents



NOTE 1: The RulesForDeaffiliation MO contents are identical.

NOTE 2: This figure is referenced by figures 5.1.3 and 10.1.2.

Figure 5.1.6: RulesForAffiliation MO contents



Figure 5.1.7: ListOfLocationCriteria MO contents



Figure 5.1.8: ListOfFunctionalAliases MO contents

## 5.2 MCPTT user profile MO parameters

### 5.2.1 General

This clause describes the parameters for the MCPTT user profile Management Object (MO).

### 5.2.2 Node: *<x>*

Table 5.2.2.1: Node: *<x>*

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get |  |
|  | This interior node acts as a placeholder for the MCPTT user profile Management Object (MO).  For the MCPTT user profile MO, the namespace specific string is: "urn:oma:mo:oma-dm-mcptt-user-profile:1.0" | | | | |

- Values: N/A

### 5.2.3 /*<x>*/Name

Table 5.2.3.1: /*<x>*/Name

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | chr | Get |  |
|  | The Name leaf is a name for the MCPTT user profile settings. | | | | |

- Values: <User displayable name>

### 5.2.4 /*<x>*/Ext/

Table 5.2.4.1: /*<x>*/Ext/

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Ext | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | The Ext is an interior node for where the vendor specific information about the MCPTT user profile MO is being placed. | | | | |

Usually the vendor extension is identified by vendor specific name under the ext node and contains the vendor meaning application vendor, device vendor etc. The tree structure under the vendor identified is not defined and can therefore include one or more un-standardized sub-trees.

- Values: N/A

### 5.2.5 /*<x>*/<x>

Table 5.2.5.1: /*<x>*/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get, Replace |  |
|  | This interior node represents a container for on-network operation and off-network operation. | | | | |

### 5.2.6 /*<x>*/<x>/Common

Table 5.2.6.1: /*<x>*/<x>/Common

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node represents a container for the common network operation which means both on-network operation and off-network operation. | | | | |

### 5.2.7 /*<x>*/*<x>*/Common/MCPTTUserID

Table 5.2.7.1: /*<x>*/<x>/Common/MCPTTUserID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTUserID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates an MCPTT user identity (MCPTT ID) which is a globally unique identifier within the MCPTT service that represents the MCPTT user. | | | | |

### 5.2.7A /*<x>*/*<x>*/Common/MCPTTUserProfileIndex

Table 5.2.7A.1: /*<x>*/<x>/Common/MCPTTUserProfileIndex

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTUserProfileIndex | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates an index for the particular MCPTT user profile. | | | | |

- Values: 0-255

### 5.2.7B /*<x>*/*<x>*/Common/MCPTTUserProfileName

Table 5.2.7B.1: /*<x>*/<x>/Common/MCPTTUserProfileName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTUserProfileName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates a profile name for the particular MCPTT user profile. | | | | |

### 5.2.7C /*<x>*/*<x>*/Common/PreSelectedIndication

Table 5.2.7C.1: /*<x>*/<x>/Common/PreSelectedIndication

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PreSelectedIndication | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | null | Get, Replace |  |
|  | This leaf node indicates that this MCPTT user profile MO is designated to be the pre-selected MCPTT user profile as defined by 3GPP TS 23.179 [15] | | | | |

- Values: null

When this leaf node is present, this MCPTT user profile MO is designated as the pre-selected MCPTT user profile.

When this leaf node is absent, this MCPTT user profile MO is not designated as the pre-selected MCPTT user profile.

If more than one MCPTT user profile MO is specified for the MCPTT user, then only one MCPTT user profile MO for the MCPTT user shall contain the <x>/Common/PreSelectedIndication leaf node.

If there is only one MCPTT user profile MO specified for the MCPTT user, then it is optional to include the <x>/Common/PreSelectedIndication leaf node.

### 5.2.8 /*<x>*/*<x>*/Common/UserAliases

Table 5.2.8.1: /*<x>*/<x>/Common/UserAliases

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/UserAliases | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for a list of aliases of an MCPTT user. | | | | |

### 5.2.8A /*<x>*/*<x>*/Common/UserAliases/<x>

Table 5.2.8A.1: /*<x>*/<x>/Common/UserAliases/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/UserAliases/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more aliases of an MCPTT user. | | | | |

### 5.2.8B /*<x>*/*<x>*/Common/UserAliases/<x>/UserAlias

Table 5.2.8B.1: /*<x>*/<x>/Common/UserAliases/<x>/UserAlias

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/UserAliases/<x>/UserAlias | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates an alphanumeric alias of the MCPTT user. | | | | |

### 5.2.9 /*<x>*/*<x>*/Common/AuthorisedAlias

Table 5.2.9.1: /*<x>*/<x>/Common/AuthorisedAlias

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/AuthorisedAlias | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | bool | Get, Replace |  |
|  | This leaf node indicates authorisation to create and delete aliases of other MCPTT users and their associated MCPTT user profiles. | | | | |

When set to "true" the MCPTT user is authorised to create and delete aliases of other MCPTT users and their associated MCPTT user profiles.

When set to "false" the MCPTT user is not authorised to create and delete aliases of other MCPTT user and their associated MCPTT user profiles. This is the default if this leaf node is not present.

### 5.2.10 /*<x>*/<x>/Common/ParticipantType

Table 5.2.10.1: /*<x>*/<x>/Common/ParticipantType

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| *<x>*/Common/ParticipantType | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the participant type of the MCPTT user. | | | | |

The ParticipantType means the functional category of the participant (e.g., first responder, second responder, dispatch, dispatch supervisor), typically defined by the MCPTT administrators.

### 5.2.11 /*<x>*/<x>/Common/Organization

Table 5.2.11.1: /*<x>*/<x>/Common/Organization

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/Organization | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the organization an MCPTT user belongs to. | | | | |

### 5.2.12 /*<x>*/*<x>*/Common/PrivateCall

Table 5.2.12.1: /*<x>*/<x>/Common/PrivateCall

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the MCPTT private call configuration. | | | | |

### 5.2.13 /*<x>*/*<x>*/Common/PrivateCall/Authorised

Table 5.2.13.1: /*<x>*/<x>/Common/PrivateCall/Authorised

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/Authorised | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to make a MCPTT private call. | | | | |

When set to "true" the MCPTT user is allowed to make a MCPTT private call.

When set to "false" the MCPTT user is not allowed to make a MCPTT private call.

### 5.2.14 /*<x>*/*<x>*/Common/PrivateCall/AuthorisedAny

Table 5.2.14.1: /*<x>*/<x>/Common/PrivateCall/AuthorisedAny

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/AuthorisedAny | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to make a MCPTT private call to any MCPTT user. | | | | |

When set to "true" any MCPTT user is authorised to make an MCPTT private call to any MCPTT user.

When set to "false" any MCPTT user is not authorised to make an MCPTT private call to any MCPTT user.

### 5.2.15 /*<x>*/<x>/Common/PrivateCall/UserList

Table 5.2.15.1: /*<x>*/<x>/PrivateCall/UserList

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/UserList | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for a list of MCPTT user(s) who can be called in a MCPTT private call. | | | | |

### 5.2.16 /*<x>*/<x>/Common/PrivateCall/UserList/<x>

Table 5.2.16.1: /*<x>*/<x>/Common/PrivateCall/UserList/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/UserList/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more list of MCPTT users who can be called in a MCPTT private call. | | | | |

### 5.2.16A /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry

Table 5.2.16A.1: /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/UserList/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more MCPTT users who can be called in a private call. | | | | |

### 5.2.17 /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry/MCPTTID

Table 5.2.17.1: /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry/MCPTTID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/UserList/<x>/Entry/MCPTTID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates an MCPTT user identity (MCPTT ID) which is a globally unique identifier within the MCPTT service that represents the MCPTT user. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 5.2.18 /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry/ DiscoveryGroupID

Table 5.2.18.1: /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry/DiscoveryGroupID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/UserList/<x>/Entry/DiscoveryGroupID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | int | Get, Replace |  |
|  | This leaf node indicates a discovery group ID as specified in 3GPP TS 23.303 [6]. | | | | |

The value is used as the discovery group ID in the ProSe discovery procedures as specified in 3GPP TS 23.303 [6].

### 5.2.19 /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry/ UserInfoID

Table 5.2.19.1: /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry/UserInfoID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/UserList/<x>/Entry/UserInfoID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | int | Get, Replace |  |
|  | This leaf node indicates a ProSe user info ID as specified in 3GPP TS 23.303 [6]. | | | | |

### 5.2.19A /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry/ DisplayName

Table 5.2.19A.1: /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/UserList/<x>/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name. | | | | |

### 5.2.19B /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry/ PrivateCallKMSURI

Table 5.2.19B.1: /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry/PrivateCallKMSURI

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/UserList/<x>/Entry/PrivateCallKMSURI | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates the identity (URI) of the KMS associated with the MCPTTID. If the value is empty, the KMS leaf node present in the MCS UE initial configuration MO is used. | | | | |

### 5.2.20 /*<x>*/*<x>*/Common/PrivateCall/ManualCommence

Table 5.2.20.1: /*<x>*/<x>/Common/PrivateCall/ManualCommence

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/ManualCommence | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to make a MCPTT private call with manual commencement. | | | | |

When set to "true" the MCPTT user is authorised to make a MCPTT private call in manual commencement mode.

When set to "false" the MCPTT user is not authorised to make a MCPTT private call in manual commencement mode.

### 5.2.21 /*<x>*/*<x>*/Common/PrivateCall/AutoCommence

Table 5.2.21.1: /*<x>*/<x>/Common/PrivateCall/AutoCommence

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/AutoCommence | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to make a MCPTT private call with automatic commencement. | | | | |

When set to "true" the MCPTT user is authorised to make a MCPTT private call in automatic commencement mode.

When set to "false" the MCPTT user is not authorised to make a MCPTT private call in automatic commencement mode.

### 5.2.22 /*<x>*/*<x>*/Common/PrivateCall/AutoAnswer

Table 5.2.22.1: /*<x>*/<x>/Common/PrivateCall/AutoAnswer

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/AutoAnswer | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation of MCPTT user to force automatic answer for a MCPTT private call. | | | | |

When set to "true" the MCPTT user is authorised to force automatic answer for a MCPTT private call.

When set to "false" the MCPTT user is not authorised to force automatic answer for a MCPTT private call.

### 5.2.23 /*<x>*/*<x>*/Common/PrivateCall/FailRestrict

Table 5.2.23.1: /*<x>*/<x>/Common/PrivateCall/FailRestrict

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/FailRestrict | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to restrict the provision of a notification of call failure reason for a MCPTT private call. | | | | |

When set to "true" the MCPTT user is authorised to restrict notification of call failure reason for MCPTT private call.

When set to "false" the MCPTT user is not authorised to restrict notification of call failure reason for MCPTT private call.

### 5.2.24 /*<x>*/*<x>*/Common/PrivateCall/AllowedMediaProtection

Table 5.2.24.1: /*<x>*/<x>/Common/PrivateCall/AllowedMediaProtection

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/AllowedMediaProtection | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates authorisation to protect confidentiality and integrity of media for MCPTT private calls. | | | | |

When set to "true" the MCPTT user is authorised to protect confidentiality and integrity of media for MCPTT private calls.

When set to "false" the MCPTT user is not authorised to protect confidentiality and integrity of media for MCPTT private calls.

The default value is set to "true".

### 5.2.25 /*<x>*/*<x>*/Common/PrivateCall/AllowedFloorControlProtection

Table 5.2.25.1: /*<x>*/<x>/Common/PrivateCall/AllowedFloorControlProtection

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/AllowedFloorControlProtection | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates authorisation to protect confidentiality and integrity of floor control signalling for MCPTT private calls. | | | | |

When set to "true" the MCPTT user is authorised to protect confidentiality and integrity of floor control signalling for MCPTT private calls.

When set to "false" the MCPTT user is not authorised to protect confidentiality and integrity of floor control signalling for MCPTT private calls.

The default value is set to "true".

### 5.2.26 /*<x>*/*<x>*/Common/PrivateCall/EmergencyCall

Table 5.2.26.1: /*<x>*/<x>/Common/PrivateCall/EmergencyCall

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/EmergencyCall | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the MCPTT emergency call policy. | | | | |

### 5.2.27 /*<x>*/*<x>*/Common/PrivateCall/EmergencyCall/Authorised

Table 5.2.27.1: /*<x>*/<x>/Common/PrivateCall/EmergencyCall/Authorised

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/EmergencyCall/Authorised | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to make an MCPTT emergency private call. | | | | |

When set to "true" the MCPTT user is authorised to make an MCPTT emergency private call.

When set to "false" the MCPTT user is not authorised to make an MCPTT emergency private call.

### 5.2.28 /*<x>*/*<x>*/Common/PrivateCall/EmergencyCall/CancelPriority

Table 5.2.28.1: /*<x>*/<x>/Common/PrivateCall/EmergencyCall/CancelPriority

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/EmergencyCall/CancelPriority | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to cancel emergency priority in an MCPTT emergency private call by an authorised MCPTT user. | | | | |

When set to "true" the MCPTT user is authorised to cancel an emergency priority in an MCPTT private call.

When set to "false" the MCPTT user is not authorised to cancel an emergency priority in an MPCTT private call.

### 5.2.29 /*<x>*/*<x>*/Common/PrivateCall/EmergencyCall/ MCPTTPrivateRecipient

Table 5.2.29.1: /*<x>*/<x>/Common/PrivateCall/EmergencyCall/MCPTTPrivateRecipient

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/EmergencyCall/MCPTTPrivateRecipient | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the MCPTT private recipient for an MCPTT emergency private call. | | | | |

### 5.2.29A /*<x>*/<x>/Common/PrivateCall/EmergencyCall/ MCPTTPrivateRecipient/Entry

Table 5.2.29A.1: /*<x>*/<x>/Common/PrivateCall EmergencyCall/MCPTTPrivateRecipient/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/EmergencyCall/MCPTTPrivateRecipient/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the details of the MCPTT private recipient for an MCPTT emergency private call. | | | | |

### 5.2.29B /*<x>*/*<x>*/Common/PrivateCall/EmergencyCall/ MCPTTPrivateRecipient/Entry/ID

Table 5.2.29B.1: /*<x>*/<x>/Common/PrivateCall/EmergencyCall/MCPTTPrivateRecipient/Entry/ID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/EmergencyCall/MCPTTPrivateRecipient/Entry/ID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates the MCPTT private recipient used upon certain criteria on initiation of an MCPTT emergency private call. | | | | |

### 5.2.29C /*<x>*/<x>/Common/PrivateCall/EmergencyCall/ MCPTTPrivateRecipient/Entry/DiscoveryGroupID

Table 5.2.29C.1: /*<x>*/<x>/Common/PrivateCall/EmergencyCall/MCPTTPrivateRecipient/Entry/DiscoveryGroupID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/EmergencyCall/MCPTTPrivateRecipient/Entry/DiscoveryGroupID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | int | Get, Replace |  |
|  | This leaf node indicates the discovery group ID as specified in 3GPP TS 23.303 [6]. | | | | |

### 5.2.29D /*<x>*/<x>/Common/PrivateCall/EmergencyCall/ MCPTTPrivateRecipient/Entry/UserInfoID

Table 5.2.29D.1: /*<x>*/<x>/Common/PrivateCall/EmergencyCall/MCPTTPrivateRecipient/Entry/UserInfoID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/EmergencyCall/MCPTTPrivateRecipient/Entry/UserInfoID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | int | Get, Replace |  |
|  | This leaf node indicates a ProSe user info ID as specified in 3GPP TS 23.303 [6]. | | | | |

The "UserInfoID" element identifies the MCPTT private recipient when making an off-network private call.

### 5.2.29E /*<x>*/*<x>*/Common/PrivateCall/EmergencyCall/ MCPTTPrivateRecipient/Entry/DisplayName

Table 5.2.29E.1: /*<x>*/<x>/Common/PrivateCall/EmergencyCall/MCPTTPrivateRecipient/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/EmergencyCall/MCPTTPrivateRecipient/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name that corresponds to the MCPTT private recipient ID. | | | | |

### 5.2.29F /*<x>*/*<x>*/Common/PrivateCall/EmergencyCall/ MCPTTPrivateRecipient/Entry/Usage

Table 5.2.29F.1: /*<x>*/<x>/Common/PrivateCall/EmergencyCall/MCPTTPrivateRecipient/Entry/Usage

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/EmergencyCall/MCPTTPrivateRecipient/Entry/Usage | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the criteria to determine when initiation of an MCPTT emergency private call uses the MCPTT private recipient ID. | | | | |

The valid values are 'LocallyDetermined' and 'UsePreConfigured'.

When set to 'LocallyDetermined' then if the MCPTT user selects an MCPTT ID then use that MCPTT ID for the MCPTT emergency private call, if the MCPTT user does not select a MCPTT ID then use the MCPTT ID identified by the MCPTT private recipient ID in clause 5.2.29B for an on-network MCPTT emergency private call.

When set to 'UsePreConfigured' then use the MCPTT ID identified by the MCPTT private recipient ID in clause 5.2.29B for an on-network MCPTT emergency private call.

When set to 'LocallyDetermined' then if the MCPTT user selects an MCPTT user then use the UserInfoID that corresponds to that MCPTT user for the MCPTT emergency private call, if the MCPTT user does not select a MCPTT user then use the User Info ID identified by the UserInfoID in clause 5.2.29D for an off-network MCPTT emergency private call.

When set to 'UsePreConfigured' then use the User Info ID identified by the UserInfoID in clause 5.2.29D for an off-network MCPTT emergency private call.

### 5.2.30 /*<x>*/*<x>*/Common/MCPTTGroupCall

Table 5.2.30.1: /*<x>*/<x>/Common/MCPTTGroupCall

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupCall | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the MCPTT group call configuration. | | | | |

### 5.2.31 /*<x>*/*<x>*/Common/MCPTTGroupCall/ MaxSimultaneousCallsN6

Table 5.2.31.1: /*<x>*/<x>/Common/MCPTTGroupCall/MaxSimultaneousCallsN6

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupCall/MaxSimultaneousCallsN6 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the maximum number of simultaneously received MCPTT group calls (N6). | | | | |

### 5.2.32 /*<x>*/*<x>*/Common/MCPTTGroupCall/EmergencyCall

Table 5.2.32.1: /*<x>*/<x>/Common/MCPTTGroupCall/EmergencyCall

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupCall/EmergencyCall | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the MCPTT emergency call policy. | | | | |

### 5.2.33 /*<x>*/*<x>*/Common/MCPTTGroupCall/EmergencyCall/Enabled

Table 5.2.33.1: /*<x>*/<x>/Common/MCPTTGroupCall/EmergencyCall/Enabled

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupCall/EmergencyCall/Enabled | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to make an MCPTT emergency group call functionality enabled for MCPTT user. | | | | |

When set to "true" the MCPTT user is authorised to make an MCPTT emergency group call functionality enabled.

When set to "false" the MCPTT user is not authorised to make an MCPTT emergency group call functionality enabled.

### 5.2.34 /*<x>*/*<x>*/Common/MCPTTGroupCall/EmergencyCall/ MCPTTGroupInitiation

Table 5.2.34.1: /*<x>*/<x>/Common/MCPTTGroupCall/EmergencyCall/MCPTTGroupInitiation

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupCall/EmergencyCall/MCPTTGroupInitiation | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the group used on initiation of an MCPTT emergency group call. | | | | |

### 5.2.34A /*<x>*/<x>/Common/MCPTTGroupCall/EmergencyCall/ MCPTTGroupInitiation/Entry

Table 5.2.34A.1: /*<x>*/<x>/Common/MCPTTGroupCall/EmergencyCall/MCPTTGroupInitiation/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupCall/EmergencyCall/MCPTTGroupInitiation/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the details of the group used on initiation of an MCPTT emergency group call. | | | | |

### 5.2.34B /*<x>*/*<x>*/Common/MCPTTGroupCall/EmergencyCall/ MCPTTGroupInitiation/Entry/GroupID

Table 5.2.34BA.1: /*<x>*/<x>/Common/MCPTTGroupCall/EmergencyCall/MCPTTGroupInitiation/Entry/GroupID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupCall/EmergencyCall/MCPTTGroupInitiation/Entry/GroupID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates the group used upon certain criteria on initiation of an MCPTT emergency group call. | | | | |

### 5.2.34C /*<x>*/*<x>*/Common/MCPTTGroupCall/EmergencyCall/ MCPTTGroupInitiation/Entry/DisplayName

Table 5.2.34C.1: /*<x>*/<x>/Common/MCPTTGroupCall/EmergencyCall/MCPTTGroupInitiation/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupCall/EmergencyCall/MCPTTGroupInitiation/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name that corresponds to the Group ID. | | | | |

### 5.2.34D /*<x>*/*<x>*/Common/MCPTTGroupCall/EmergencyCall/ MCPTTGroupInitiation/Entry/Usage

Table 5.2.34D.1: /*<x>*/<x>/Common/MCPTTGroupCall/EmergencyCall/MCPTTGroupInitiation/Entry/Usage

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupCall/EmergencyCall/MCPTTGroupInitiation/Entry/Usage | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the criteria to determine when initiation of an MCPTT emergency group call uses the GroupID. | | | | |

The valid values are 'UseCurrentlySelectedGroup' and 'DedicatedGroup'.

When set to 'UseCurrentlySelectedGroup' then if the MCPTT user has currently selected an MCPTT group then use that MCPTT group for an on-network MCPTT emergency group call, if the MCPTT user does not have a currently selected MCPTT group then use the MCPTT group identified by the GroupID in clause 5.2.34B for an MCPTT emergency group call.

When set to 'DedicatedGroup' then use the MCPTT group identified by the GroupID in clause 5.2.34B for an MCPTT emergency group call.

### 5.2.35 /*<x>*/*<x>*/Common/MCPTTGroupCall/EmergencyCall/ CancelMCPTTGroup

Table 5.2.35.1: /*<x>*/<x>/Common/MCPTTGroupCall/EmergencyCall/CancelMCPTTGroup

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupCall/EmergencyCall/CancelMCPTTGroup | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to cancel an in progress MCPTT emergency group call associated with a group. | | | | |

When set to "true" the MCPTT user is authorised to cancel a MCPTT emergency group call.

When set to "false" the MCPTT user is not authorised to cancel a MCTT emergency group call.

### 5.2.36 /*<x>*/*<x>*/Common/MCPTTGroupCall/ImminentPerilCall

Table 5.2.36.1: /*<x>*/<x>/Common/MCPTTGroupCall/ImminentPerilCall

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupCall/ImminentPerilCall | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the MCPTT imminent peril call policy. | | | | |

### 5.2.37 /*<x>*/*<x>*/Common/MCPTTGroupCall/ImminentPerilCall/ Authorised

Table 5.2.37.1: /*<x>*/<x>/Common/MCPTTGroupCall/ImminentPerilCall/Authorised

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupCall/ImminentPerilCall/Authorised | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to make an Imminent Peril group call. | | | | |

When set to "true" the MCPTT user is authorised to create an MCPTT imminent peril group call.

When set to "false" the MCPTT user is not authorised to create an MCPTT imminent peril group call.

### 5.2.38 /*<x>*/*<x>*/Common/MCPTTGroupCall/ImminentPerilCall/ Cancel

Table 5.2.38.1: /*<x>*/<x>/Common/MCPTTGroupCall/ImminentPerilCall/Cancel

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupCall/ImminentPerilCall/Cancel | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation for in-progress MCPTT imminent peril cancelation. | | | | |

When set to "true" the MCPTT user is authorised to cancel an MCPTT imminent peril call.

When set to "false" the MCPTT user is not authorised to cancel an MCPTT imminent peril call.

### 5.2.39 /*<x>*/*<x>*/Common/MCPTTGroupCall/ImminentPerilCall/ MCPTTGroupInitiation

Table 5.2.39.1: /*<x>*/<x>/Common/MCPTTGroupCall/ImminentPerilCall/MCPTTGroupInitiation

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupCall/ImminentPerilCall/MCPTTGroupInitiation | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the group used on initiation of an MCPTT imminent peril group call. | | | | |

### 5.2.39A /*<x>*/<x>/Common/MCPTTGroupCall/ImminentPerilCall/ MCPTTGroupInitiation/Entry

Table 5.2.39A.1: /*<x>*/<x>/Common/MCPTTGroupCall/ImminentPerilCall//MCPTTGroupInitiation/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupCall/ImminentPerilCall/MCPTTGroupInitiation/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the details of the group used on initiation of an imminent peril call. | | | | |

### 5.2.39B /*<x>*/*<x>*/Common/MCPTTGroupCall/ImminentPerilCall/ MCPTTGroupInitiation/Entry/GroupID

Table 5.2.39B.1: /*<x>*/<x>/Common/MCPTTGroupCall/ImminentPerilCall/MCPTTGroupInitiation/Entry/GroupID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupCall/ImminentPerilCall/MCPTTGroupInitiation/Entry/GroupID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the group used upon certain criteria on initiation of an MCPTT imminent peril group call. | | | | |

### 5.2.39C /*<x>*/*<x>*/Common/MCPTTGroupCall/ImminentPerilCall/ MCPTTGroupInitiation/DisplayName

Table 5.2.39C.1: /*<x>*/<x>/Common/MCPTTGroupCall/ImminentPerilCall/MCPTTGroupInitiation/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupCall/ImminentPerilCall/MCPTTGroupInitiation/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name that corresponds to the Group ID. | | | | |

### 5.2.39D /*<x>*/*<x>*/Common/MCPTTGroupCall/ImminentPerilCall/ MCPTTGroupInitiation/Entry/Usage

Table 5.2.39D.1: /*<x>*/<x>/Common/MCPTTGroupCall/ImminentPerilCall/MCPTTGroupInitiation/Entry/Usage

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupCall/ImminentPerilCall/MCPTTGroupInitiation/Entry/Usage | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the criteria to determine when initiation of an MCPTT imminent peril group call uses the GroupID. | | | | |

The valid values are 'UseCurrentlySelectedGroup' and 'DedicatedGroup'.

When set to 'UseCurrentlySelectedGroup' then if the MCPTT user has currently selected an MCPTT group then use that MCPTT group for an on-network MCPTT imminent peril group call, if the MCPTT user does not have a currently selected MCPTT group then use the MCPTT group identified by the GroupID in clause 5.2.39B for an MCPTT imminent peril group call.

When set to 'DedicatedGroup' then use the MCPTT group identified by the GroupID in clause 5.2.39B for an MCPTT imminent peril group call.

### 5.2.40 /*<x>*/*<x>*/Common/MCPTTGroupCall/EmergencyAlert

Table 5.2.40.1: /*<x>*/<x>/Common/MCPTTGroupCall/EmergencyAlert

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupCall/EmergencyAlert | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the MCPTT emergency alert policy. | | | | |

### 5.2.41 /*<x>*/*<x>*/Common/MCPTTGroupCall/EmergencyAlert/ Authorised

Table 5.2.41.1: /*<x>*/<x>/Common/MCPTTGroupCall/EmergencyAlert/Authorised

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupCall/EmergencyAlert/Authorised | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to activate an MCPTT emergency alert. | | | | |

When set to "true" the MCPTT user is authorised to make an MCPTT emergency alert.

When set to "false" the MCPTT user is not authorised to make an MCPTT emergency alert.

### 5.2.42 /*<x>*/*<x>*/Common/MCPTTGroupCall/EmergencyAlert/ Cancel

Table 5.2.42.1: /*<x>*/<x>/Common/MCPTTGroupCall/EmergencyAlert/Cancel

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupCall/EmergencyAlert/Cancel | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to cancel an MCPTT emergency alert. | | | | |

When set to "true" the MCPTT user is authorised to cancel an MCPTT emergency alert.

When set to "false" the MCPTT user is not authorised to cancel an MCPTT emergency alert.

### 5.2.43 Void

### 5.2.43A /*<x>*/<x>/Common/MCPTTGroupCall/EmergencyAlert/Entry

Table 5.2.39A.1: /*<x>*/<x>/Common/MCPTTGroupCall/EmergencyAlert/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupCall/EmergencyAlert/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the details of the MCPTT group of an MCPTT emergency alert. | | | | |

### 5.2.43B /*<x>*/*<x>*/Common/MCPTTGroupCall/EmergencyAlert/Entry/ID

Table 5.2.439B.1: /*<x>*/<x>/Common/MCPTTGroupCall/EmergencyAlert/Entry/ID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupCall/EmergencyAlert/Entry/ID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the MCPTT group used upon certain criteria on initiation of an MCPTT emergency alert. | | | | |

### 5.2.43C Void

### 5.2.43D /*<x>*/*<x>*/Common/MCPTTGroupCall/EmergencyAlert/Entry/ DisplayName

Table 5.2.43D.1: /*<x>*/<x>/Common/MCPTTGroupCall/EmergencyAlert/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupCall/EmergencyAlert/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name that corresponds to the ID. | | | | |

### 5.2.43E /*<x>*/*<x>*/Common/MCPTTGroupCall/EmergencyAlert/Entry/Usage

Table 5.2.43E.1: /*<x>*/<x>/Common/MCPTTGroupCall/EmergencyAlert/Entry/Usage

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupCall/EmergencyAlert/Entry/Usage | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the criteria to determine when initiation of an MCPTT emergency alert uses the ID. | | | | |

The valid values are 'LocallyDetermined', 'UseCurrentlySelectedGroup', 'UsePreConfigured' and 'DedicatedGroup'.

When set to 'LocallyDetermined' then if the MCPTT user selects an MCPTT ID then use that MCPTT ID for an on-network MCPTT emergency alert, if the MCPTT user does not select a MCPTT ID then use the MCPTT ID identified by the ID in clause 5.2.43B for an on-network MCPTT emergency alert.

When set to 'UseCurrentlySelectedGroup' then if the MCPTT user has currently selected an MCPTT group then use that MCPTT group for an on-network MCPTT emergency alert, if the MCPTT user does not have a currently selected MCPTT group then use the MCPTT group identified by the ID in clause 5.2.43B for an MCPTT emergency alert.

When set to 'UsePreConfigured' then use the ID identified by the ID in clause 5.2.43B for an on-network MCPTT emergency alert.

When set to 'DedicatedGroup' then use the MCPTT group identified by the ID in clause 5.2.43B for an MCPTT emergency alert.

### 5.2.43F /*<x>*/*<x>*/Common/MCPTTGroupCall/Priority

Table 5.2.43F.1: /*<x>*/<x>/Common/MCPTTGroupCall/Priority

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupCall/Priority | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the priority of the MCPTT group calls. | | | | |

- Values: 0-255

The MCPTT group call with the lowest Priority value shall be considered as the MCPTT group call having the lowest level among the MCPTT group calls.

### 5.2.44 Void

### 5.2.45 /*<x>*/*<x>*/Common/MCPTTGroupBroadcast

Table 5.2.45.1: /*<x>*/<x>/Common/MCPTTGroupBroadcast

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupBroadcast | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the group-broadcast group policy. | | | | |

### 5.2.46 /*<x>*/*<x>*/Common/MCPTTGroupBroadcast/Authorised

Table 5.2.46.1: /*<x>*/<x>/Common/MCPTTGroupBroadcast/Authorised

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupBroadcast/Authorised | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to create a group-broadcast group. | | | | |

When set to "true" the MCPTT user is authorised to create a group-broadcast group.

When set to "false" the MCPTT user is not authorised to create a group-broadcast group.

### 5.2.47 /*<x>*/*<x>*/Common/UserBroadcast

Table 5.2.47.1: /*<x>*/<x>/Common/UserBroadcast

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/UserBroadcast | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the user-broadcast group policy. | | | | |

### 5.2.48 /*<x>*/*<x>*/Common/UserBroadcast/Authorised

Table 5.2.48.1: /*<x>*/<x>/Common/UserBroadcast/Authorised

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/UserBroadcast/Authorised | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to create a user-broadcast group. | | | | |

When set to "true" the MCPTT user is authorised to create a user-broadcast group.

When set to "false" the MCPTT user is not authorised to create a user-broadcast group.

### 5.2.48A /*<x>*/*<x>*/OnNetwork

Table 5.2.48A.1: /*<x>*/<x>/OnNetwork

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | node | Get, Replace |  |
|  | This interior node represents a container for on-network operation. | | | | |

### 5.2.48B1 /*<x>*/*<x>*/OnNetwork/MCPTTGroupList

Table 5.2.48B1.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the list of on-network MCPTT groups that the MCPTT user is allowed to affiliate to. | | | | |

### 5.2.48B2 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>

Table 5.2.48B2.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more list of on-network MCPTT groups that the MCPTT user is allowed to affiliate to. | | | | |

### 5.2.48B3 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry

Table 5.2.48B3.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the details of the on-network MCPTT groups that the MCPTT user is allowed to affiliate to. | | | | |

### 5.2.48B4 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ MCPTTGroupID

Table 5.2.48B4.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/MCPTTGroupID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/MCPTTGroupID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the MCPTT group ID for the on-network MCPTT group that the MCPTT user is allowed to affiliate to. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 5.2.48B4A /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation

Table 5.2.48B4A.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node is a placeholder for the rules that control automatic affiliation. | | | | |

### 5.2.48B4A0 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>

Table 5.2.48B4A0.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for the zero or more rules that control automatic affiliation. | | | | |

### 5.2.48B4A1 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/

Table 5.2.48B4A1.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the location portion of the rules that control automatic affiliation. | | | | |

### 5.2.48B4A2 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>

Table 5.2.48B84A2.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for the location portion of the rules that control automatic affiliation. | | | | |

### 5.2.48B4A3 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry

Table 5.2.48B4A3.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the location portion of the rules that control automatic affiliation. | | | | |

### 5.2.48B4A4 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea

Table 5.2.48B4A4.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |  |
|  | This interior node contains a geographical area which when entered by the MC service UE triggers evaluation of the rules. | | | | |  |

### 5.2.48B4A5 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea

Table 5.2.48B4A5.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |  |
|  | This interior node contains a geographical area described by a polygon. | | | | |  |

### 5.2.48B4A6 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea/<x>

Table 5.2.48B4A6.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea/<x>

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea/<x> | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | OneOrN | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the corners which define a polygon. The occurrence of this leaf node is "3 to 15" as per 3GPP TS 23.032 [21]. | | | | |  |

### 5.2.48B4A7 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea/<x>/PointCoordinateType

Table 5.2.48B4A7.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the type of the coordinates. | | | | |  |

### 5.2.48B4A8 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/ Longitude

Table 5.2.48B4A8.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the longitudinal coordinate of a corner. | | | | |  |

### 5.2.48B4A9 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude

Table 5.2.48B4A9.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the latitudinal coordinate of a corner. | | | | |  |

### 5.2.48B4A10 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea

Table 5.2.48B4A10.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |  |
|  | This interior node contains a geographical area described by an ellipsoid arc. | | | | |  |

### 5.2.48B4A11 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Center

Table 5.2.48B4A11.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |  |

### 5.2.48B4A12 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType

Table 5.2.48B4A12.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |  |

### 5.2.48B4A13 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Longitude

Table 5.2.48B4A13.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Longitude

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Longitude | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the longitudinal coordinate of the center. | | | | |  |

### 5.2.48B4A14 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Latitude

Table 5.2.48B4A14.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Latitude

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Latitude | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the latitudinal coordinate of a center. | | | | |  |

### 5.2.48B4A15 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Radius

Table 5.2.48B4A15.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Radius

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center/Radius | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the radius of the ellipsoid arc. | | | | |  |

### 5.2.48B4A16 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/OffsetAngle

Table 5.2.48B4A16.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/OffsetAngle

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/OffsetAngle | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the offset angle of the ellipsoid arc. | | | | |  |

### 5.2.48B4A17 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/IncludedAngle

Table 5.2.48B4A17.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/IncludedAngle

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/IncludedAngle | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the included angle of the ellipsoid arc. | | | | |  |

### 5.2.48B4A18 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Speed

Table 5.2.48B4A18.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Speed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Speed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | One | node | Get, Replace |  |  |
|  | This interior node contains the speed. | | | | |  |

### 5.2.48B4A19 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Speed/MinimumSpeed

Table 5.2.48B4A19.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Speed/MinimumSpeed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Speed/MinimumSpeed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the minimum speed. | | | | |  |

- Values: non-negative integer in units of kilometers/hour.

### 5.2.48B4A20 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Speed/MaximumSpeed

Table 5.2.48B4A20.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Speed/MaximumSpeed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Speed/MaximumSpeed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the maximum speed. | | | | |  |

- Values: non-negative integer in units of kilometers/hour.

### 5.2.48B4A21 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Heading

Table 5.2.48B4A21.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Heading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Heading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | One | node | Get, Replace |  |  |
|  | This interior node contains the heading. | | | | |  |

### 5.2.48B4A22 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Heading/MinimumHeading

Table 5.2.48B4A22.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Heading/MinimumHeading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Heading/MinimumHeading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the minimum heading. | | | | |  |

- Values: 0-359

### 5.2.48B4A23 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Heading/MaximumHeading

Table 5.2.48B4A23.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Heading/MaximumHeading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Heading/MaximumHeading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the maximum heading. | | | | |  |

- Values: 0-359

### 5.2.48B4A24 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea

Table 5.2.48B4A24.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |  |
|  | This interior node contains a geographical area which when entered by the MC service UE triggers evaluation of the rules. | | | | |  |

### 5.2.48B4A25 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea

Table 5.2.48B4A25.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |  |
|  | This interior node contains a geographical area described by a polygon. | | | | |  |

### 5.2.48B4A26 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea/<x>

Table 5.2.48B4A26.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea/<x>

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea/<x> | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | OneOrN | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the corners which define a polygon. The occurrence of this leaf node is "3 to 15" as per 3GPP TS 23.032 [21]. | | | | |  |

### 5.2.48B4A27 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea/<x>/PointCoordinateType

Table 5.2.48B4A27.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the type of the coordinates. | | | | |  |

### 5.2.48B4A28 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude

Table 5.2.48B4A28.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the longitudinal coordinate of a corner. | | | | |  |

### 5.2.48B4A29 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude

Table 5.2.48B4A29.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the latitudinal coordinate of a corner. | | | | |  |

### 5.2.48B4A30 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea

Table 5.2.48B4A30.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |  |
|  | This interior node contains a geographical area described by an ellipsoid arc. | | | | |  |

### 5.2.48B4A31 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Center

Table 5.2.48B4A31.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |  |

### 5.2.48B4A32 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType

Table 5.2.48B4A32.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |  |

### 5.2.48B4A33 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Longitude

Table 5.2.48B4A33.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Longitude

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Longitude | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the longitudinal coordinate of the center. | | | | |  |

### 5.2.48B4A34 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Latitude

Table 5.2.48B4A34.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Latitude

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Latitude | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the latitudinal coordinate of a center. | | | | |  |

### 5.2.48B4A35 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Radius

Table 5.2.48B4A35.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Radius

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center/Radius | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the radius of the ellipsoid arc. | | | | |  |

### 5.2.48B4A36 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/OffsetAngle

Table 5.2.48B4A36.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/OffsetAngle

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/OffsetAngle | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the offset angle of the ellipsoid arc. | | | | |  |

### 5.2.48B4A37 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/IncludedAngle

Table 5.2.48B4A37.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/IncludedAngle

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/IncludedAngle | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the included angle of the ellipsoid arc. | | | | |  |

### 5.2.48B4A38 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Speed

Table 5.2.48B4A38.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Speed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Speed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | One | node | Get, Replace |  |  |
|  | This interior node contains the speed. | | | | |  |

### 5.2.48B4A39 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Speed/MinimumSpeed

Table 5.2.48B4A39.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Speed/MinimumSpeed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Speed/MinimumSpeed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the minimum speed. | | | | |  |

- Values: non-negative integer in units of kilometers/hour.

### 5.2.48B4A40 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Speed/MaximumSpeed

Table 5.2.48B4A40.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Speed/MaximumSpeed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Speed/MaximumSpeed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the maximum speed. | | | | |  |

- Values: non-negative integer in units of kilometers/hour.

### 5.2.48B4A41 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Heading

Table 5.2.48B4A41.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Heading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Heading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | One | node | Get, Replace |  |  |
|  | This interior node contains the heading. | | | | |  |

### 5.2.48B4A42 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Heading/MinimumHeading

Table 5.2.48B4A42.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Heading/MinimumHeading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Heading/MinimumHeading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the minimum heading. | | | | |  |

- Values: 0-359

### 5.2.48B4A43 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Heading/MaximumHeading

Table 5.2.48B4A43.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Heading/MaximumHeading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Heading/MaximumHeading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the maximum heading. | | | | |  |

- Values: 0-359

### 5.2.48B4A44 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfActiveFunctionalAliases

Table 5.2.48B4A44.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfActiveFunctionalAliases

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfActiveFunctionalAliases | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the functional alias part of rules that control automatic affiliation. | | | | |

### 5.2.48B4A45 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfActiveFunctionalAliases/<x>

Table 5.2.48B4A45.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfActiveFunctionalAliases/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfActiveFunctionalAliases/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for the functional alias part of rules that control automatic affiliation. | | | | |

### 5.2.48B4A46 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfActiveFunctionalAliases/<x>/Entry

Table 5.2.48B4A46.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfActiveFunctionalAliases/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfActiveFunctionalAliases/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the functional alias part of rules that control automatic affiliation. | | | | |

### 5.2.48B4A47 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfActiveFunctionalAliases/<x>/Entry/ FunctionalAlias

Table 5.2.48B4A47.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfActiveFunctionalAliases/<x>/Entry/FunctionalAlias

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfActiveFunctionalAliases/<x>/Entry/FunctionalAlias | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | chr | Get, Replace |  |  |
|  | This leaf node contains a functional alias. | | | | |  |

### 5.2.48B4B /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation

Table 5.2.48B4B.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node is a placeholder for the rules that control automatic deaffiliation. | | | | |

### 5.2.48B4B0 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>

Table 5.2.48B4B0.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for the zero r morerules that control automatic deaffiliation. | | | | |

### 5.2.48B4B1 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/

Table 5.2.48B4B1.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the location portion of the rules that control automatic deaffiliation. | | | | |

### 5.2.48B4B2 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>

Table 5.2.48B84B2.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for the location portion of the rules that control automatic deaffiliation. | | | | |

### 5.2.48B4B3 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry

Table 5.2.48B4B3.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the location portion of the rules that control automatic deaffiliation. | | | | |

### 5.2.48B4B4 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea

Table 5.2.48B4B4.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |  |
|  | This interior node contains a geographical area which, when entered by the MC service UE triggers evaluation of the rules. | | | | |  |

### 5.2.48B4B5 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea

Table 5.2.48B4B5.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |  |
|  | This interior node contains a geographical area described by a polygon. | | | | |  |

### 5.2.48B4B6 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea/<x>

Table 5.2.48B4B6.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea/<x>

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea/<x> | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | OneOrN | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the corners which define a polygon. The occurrence of this leaf node is "3 to 15" as per 3GPP TS 23.032 [21]. | | | | |  |

### 5.2.48B4B7 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea/<x>/PointCoordinateType

Table 5.2.48B4B7.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesFordeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the type of the coordinates. | | | | |  |

### 5.2.48B4B8 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/ Longitude

Table 5.2.48B4B8.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the longitudinal coordinate of a corner. | | | | |  |

### 5.2.48B4B9 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude

Table 5.2.48B4B9.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the latitudinal coordinate of a corner. | | | | |  |

### 5.2.48B4B10 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea

Table 5.2.48B4B10.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |  |
|  | This interior node contains a geographical area described by an ellipsoid arc. | | | | |  |

### 5.2.48B4A11 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Center

Table 5.2.48B4B11.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |  |

### 5.2.48B4B12 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType

Table 5.2.48B4B12.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |  |

### 5.2.48B4B13 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Longitude

Table 5.2.48B4B13.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Longitude

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Longitude | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the longitudinal coordinate of the center. | | | | |  |

### 5.2.48B4B14 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Latitude

Table 5.2.48B4B14.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Latitude

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Latitude | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the latitudinal coordinate of a center. | | | | |  |

### 5.2.48B4B15 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Radius

Table 5.2.48B4B15.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Radius

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center/Radius | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the radius of the ellipsoid arc. | | | | |  |

### 5.2.48B4B16 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/OffsetAngle

Table 5.2.48B4B16.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/OffsetAngle

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/OffsetAngle | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the offset angle of the ellipsoid arc. | | | | |  |

### 5.2.48B4B17 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/IncludedAngle

Table 5.2.48B4B17.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/IncludedAngle

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/IncludedAngle | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the included angle of the ellipsoid arc. | | | | |  |

### 5.2.48B4B18 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Speed

Table 5.2.48B4B18.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Speed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Speed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | One | node | Get, Replace |  |  |
|  | This interior node contains the speed. | | | | |  |

### 5.2.48B4B19 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Speed/MinimumSpeed

Table 5.2.48B4B19.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Speed/MinimumSpeed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Speed/MinimumSpeed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the minimum speed. | | | | |  |

- Values: non-negative integer in units of kilometers/hour.

### 5.2.48B4B20 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Speed/MaximumSpeed

Table 5.2.48B4B20.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Speed/MaximumSpeed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Speed/MaximumSpeed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the maximum speed. | | | | |  |

- Values: non-negative integer in units of kilometers/hour.

### 5.2.48B4B21 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Heading

Table 5.2.48B4B21.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Heading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Heading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | One | node | Get, Replace |  |  |
|  | This interior node contains the heading. | | | | |  |

### 5.2.48B4B22 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Heading/MinimumHeading

Table 5.2.48B4B22.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Heading/MinimumHeading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Heading/MinimumHeading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the minimum heading. | | | | |  |

- Values: 0-359

### 5.2.48B4B23 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Heading/MaximumHeading

Table 5.2.48B4B23.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Heading/MaximumHeading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Heading/MaximumHeading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the maximum heading. | | | | |  |

- Values: 0-359

### 5.2.48B4B24 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea

Table 5.2.48B4B24.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |  |
|  | This interior node contains a geographical area which when entered by the MC service UE triggers evaluation of the rules. | | | | |  |

### 5.2.48B4B25 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea

Table 5.2.48B4B25.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |  |
|  | This interior node contains a geographical area described by a polygon. | | | | |  |

### 5.2.48B4B26 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea/<x>

Table 5.2.48B4B26.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea/<x>

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea/<x> | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | OneOrN | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the corners which define a polygon. The occurrence of this leaf node is "3 to 15" as per 3GPP TS 23.032 [21]. | | | | |  |

### 5.2.48B4B27 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea/<x>/PointCoordinateType

Table 5.2.48B4B27.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the type of the coordinates. | | | | |  |

### 5.2.48B4B28 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude

Table 5.2.48B4B28.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the longitudinal coordinate of a corner. | | | | |  |

### 5.2.48B4B29 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude

Table 5.2.48B4B29.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the latitudinal coordinate of a corner. | | | | |  |

### 5.2.48B4B30 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea

Table 5.2.48B4B30.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |  |
|  | This interior node contains a geographical area described by an ellipsoid arc. | | | | |  |

### 5.2.48B4B31 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Center

Table 5.2.48B431.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |  |

### 5.2.48B4B32 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType

Table 5.2.48B4B32.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |  |

### 5.2.48B4B33 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Longitude

Table 5.2.48B4B33.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Longitude

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Longitude | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the longitudinal coordinate of the center. | | | | |  |

### 5.2.48B4B34 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Latitude

Table 5.2.48B4B34.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Latitude

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Latitude | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the latitudinal coordinate of a center. | | | | |  |

### 5.2.48B4B35 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Radius

Table 5.2.48B4B35.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Radius

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center/Radius | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the radius of the ellipsoid arc. | | | | |  |

### 5.2.48B4B36 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/OffsetAngle

Table 5.2.48B4B36.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/OffsetAngle

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/OffsetAngle | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the offset angle of the ellipsoid arc. | | | | |  |

### 5.2.48B4B37 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/IncludedAngle

Table 5.2.48B4B37.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/IncludedAngle

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/IncludedAngle | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the included angle of the ellipsoid arc. | | | | |  |

### 5.2.48B4B38 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Speed

Table 5.2.48B4B38.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Speed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Speed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | One | node | Get, Replace |  |  |
|  | This interior node contains the speed. | | | | |  |

### 5.2.48B4B39 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Speed/MinimumSpeed

Table 5.2.48B4B39.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Speed/MinimumSpeed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Speed/MinimumSpeed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the minimum speed. | | | | |  |

- Values: non-negative integer in units of kilometers/hour.

### 5.2.48B4B40 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Speed/MaximumSpeed

Table 5.2.48B4B40.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Speed/MaximumSpeed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Speed/MaximumSpeed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the maximum speed. | | | | |  |

- Values: non-negative integer in units of kilometers/hour.

### 5.2.48B4B41 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Heading

Table 5.2.48B4B41.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Heading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Heading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | One | node | Get, Replace |  |  |
|  | This interior node contains the heading. | | | | |  |

### 5.2.48B4B42 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Heading/MinimumHeading

Table 5.2.48B4B42.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Heading/MinimumHeading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Heading/MinimumHeading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the minimum heading. | | | | |  |

- Values: 0-359

### 5.2.48B4B43 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Heading/MaximumHeading

Table 5.2.48B4B43.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Heading/MaximumHeading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Heading/MaximumHeading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the maximum heading. | | | | |  |

- Values: 0-359

### 5.2.48B4B44 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfActiveFunctionalAliases

Table 5.2.48B4B44.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfActiveFunctionalAliases

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfActiveFunctionalAliases | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the functional alias part of rules that control automatic deaffiliation. | | | | |

### 5.2.48B4B45 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfActiveFunctionalAliases/<x>

Table 5.2.48B4B45.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfActiveFunctionalAliases/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfActiveFunctionalAliases/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for the functional alias part of rules that control automatic deaffiliation. | | | | |

### 5.2.48B4B46 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfActiveFunctionalAliases/<x>/Entry

Table 5.2.48B4B46.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfActiveFunctionalAliases/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfActiveFunctionalAliases/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the functional alias part of rules that control automatic deaffiliation. | | | | |

### 5.2.48B4B47 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfActiveFunctionalAliases/<x>/Entry/ FunctionalAlias

Table 5.2.48B4B47.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfActiveFunctionalAliases/<x>/Entry/FunctionalAlias

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfActiveFunctionalAliases/<x>/Entry/FunctionalAlias | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | chr | Get, Replace |  |  |
|  | This leaf node contains a functional alias. | | | | |  |

### 5.2.48B5 /*<x>*/*<x>*/OnNetwork/MCPTTGroupList/<x>/Entry/DisplayName

Table 5.2.48B5.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name that corresponds to the MCPTT Group ID. | | | | |

### 5.2.48B6 /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ ManualDeaffiliationNotAllowedIfAffiliationRulesAreMet

Table 5.2.48B6.1: /*<x>*/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ManualDeaffiliationNotAllowedIfAffiliationRulesAreMet

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/ManualDeaffiliationNotAllowedIfAffiliationRulesAreMet | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCPTT user is authorised to deaffiliate if the affiliation criteria are met. | | | | |

### 5.2.48B7 /<x>/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ RelativePresentationPriority

Table 5.2.48B7.1: /<x>/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/RelativePresentationPriority

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| *<x>*/OnNetwork/MCPTTGroupList/<x>/Entry/RelativePresentationPriority | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | int | Get, Replace |  |
|  | This leaf node indicates the presentation priority of the on-network group, identified by the MCPTTGroupID, relative to other on-network groups and on-network users. | | | | |

- Values: 0-255

The lowest RelativePresentationPriority value shall be considered as the MCPTT group transaction having the lowest priority for presentation among other group MCPTT and one-to-one user transactions.

### 5.2.48B8 /<x>/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/GMSServID

Table 5.2.48B8.1: /<x>/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/GMSServID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/GMSServID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the identity (URI) of the GMS owning the group identified by the MCPTTGroupID. | | | | |

### 5.2.48B9 /<x>/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/ IDMSTokenEndPoint

Table 5.2.48B9.1: /<x>/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/IDMSTokenEndPoint

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/IDMSTokenEndPoint | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the identity (URI) of the IDMS token endpoint for the group identified by the MCPTTGroupID. If the value is empty, the IDMS identities (IDMSAuthEndpoint and IDMSTokenEndpoint) present in the MCS UE initial configuration MO are used. | | | | |

### 5.2.48B10 /<x>/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/GroupKMSURI

Table 5.2.48B10.1: /<x>/<x>/OnNetwork/MCPTTGroupList/<x>/Entry/GroupKMSURI

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCPTTGroupList/<x>/Entry/GroupKMSURI | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the identity (URI) of the KMS identity (URI) for the group identified by the MCPTTGroupID. If the value is empty, the KMS identity (URI) (kms) present in the MCS UE initial configuration MO is used. | | | | |

### 5.2.48C1 /*<x>*/*<x>*/OnNetwork/ImplicitAffiliations

Table 5.2.48C1.1: /*<x>*/<x>/OnNetwork/ImplicitAffiliations

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/ImplicitAffiliations | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the implicit affiliation configuration. | | | | |

### 5.2.48C2 /*<x>*/<x>/OnNetwork/ImplicitAffiliations/<x>

Table 5.2.48C2.1: /*<x>*/<x>/OnNetwork/ImplicitAffiliations/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/ImplicitAffiliations/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more implicit affiliation configuration. | | | | |

### 5.2.48C3 /*<x>*/<x>/OnNetwork/ImplicitAffiliations/<x>/Entry

Table 5.2.48C3.1: /*<x>*/<x>/OnNetwork/ImplicitAffiliations/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/ImplicitAffiliations/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the details of the on-network MCPTT groups that the MCPTT user is implicitly affiliated to. | | | | |

### 5.2.48C4 /*<x>*/<x>/OnNetwork/ImplicitAffiliations/<x>/Entry/ MCPTTGroupID

Table 5.2.48C4.1: /*<x>*/<x>/OnNetwork/ImplicitAffiliations/<x>/Entry/MCPTTGroupID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/ImplicitAffiliations/<x>/Entry/MCPTTGroupID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates a MCPTT group ID to which the MCPTT user is implicitly affiliated to. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 5.2.48C5 /*<x>*/*<x>*/OnNetwork/ImplicitAffiliations/<x>/Entry/DisplayName

Table 5.2.48C5.1: /*<x>*/<x>/OnNetwork/ImplicitAffiliations/<x>/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/ImplicitAffiliations/<x>/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name that corresponds to the MCPTT Group ID. | | | | |

### 5.2.48D /*<x>*/*<x>*/OnNetwork/AllowedRegroup

Table 5.2.48D.1: /*<x>*/<x>/OnNetwork/AllowedRegroup

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/AllowedRegroup | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCPTT user is authorised to perform dynamic regrouping operations. | | | | |

When set to "true" the MCPTT user is authorised to perform dynamic regrouping operations.

When set to "false" the MCPTT user is not authorised to perform dynamic regrouping operations.

### 5.2.48E /*<x>*/*<x>*/OnNetwork/AllowedPresenceStatus

Table 5.2.48E.1: /*<x>*/<x>/OnNetwork/AllowedPresenceStatus

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/AllowedPresenceStatus | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | bool | Get, Replace |  |
|  | This leaf node indicates the presence status on the network of this MCPTT user is available. | | | | |

When set to "true" the presence status on the network of this MCPTT user is available.

When set to "false" the presence status on the network of this MCPTT user is not available. This is the default if this leaf node is not present.

### 5.2.48F /*<x>*/*<x>*/OnNetwork/AllowedPresence

Table 5.2.48F.1: /*<x>*/<x>/OnNetwork/AllowedPresence

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/AllowedPresence | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCPTT user is authorised to obtain whether a particular MCPTT User is present on the network. | | | | |

When set to "true" the MCPTT user is authorised to obtain whether a particular MCPTT User is present on the network.

When set to "false" the MCPTT user is not authorised to obtain whether a particular MCPTT User is present on the network.

### 5.2.48G /*<x>*/*<x>*/OnNetwork/EnabledParticipation

Table 5.2.48G.1: /*<x>*/<x>/OnNetwork/EnabledParticipation

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/EnabledParticipation | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCPTT user is allowed to participate in MCPTT private calls that they are invited to. | | | | |

When set to "true" the MCPTT user is allowed to participate in MCPTT private calls that they are invited to.

When set to "false" the MCPTT user is not allowed to participate in MCPTT private calls that they are invited to.

### 5.2.48H /*<x>*/*<x>*/OnNetwork/AllowedTransmission

Table 5.2.48H.1: /*<x>*/<x>/OnNetwork/AllowedTransmission

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/AllowedTransmission | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCPTT user is authorised to override transmission in a MCPTT private call. | | | | |

When set to "true" the MCPTT user is authorised to override transmission in a MCPTT private call.

When set to "false" the MCPTT user is not authorised to override transmission in a MCPTT private call.

### 5.2.48I /*<x>*/*<x>*/OnNetwork/AllowedManualSwitch

Table 5.2.48I.1: /*<x>*/<x>/OnNetwork/AllowedManualSwitch

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/AllowedManualSwitch | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCPTT user is authorised to manually switch to off-network operation while in on-network operation. | | | | |

When set to "true" the MCPTT user is authorised to manually switch to off-network operation while in on-network operation.

When set to "false" the MCPTT user is not authorised to manually switch to off-network operation while in on-network operation.

### 5.2.48J /*<x>*/*<x>*/OnNetwork/PrivateCall

Table 5.2.48J.1: /*<x>*/<x>/OnNetwork/PrivateCall

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/PrivateCall | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the MCPTT private call configuration. | | | | |

### 5.2.48K /*<x>*/*<x>*/OnNetwork/PrivateCall/EmergencyAlert

Table 5.2.48K.1: /*<x>*/<x>/OnNetwork/PrivateCall/EmergencyAlert

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/PrivateCall/EmergencyAlert | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the MCPTT private emergency alert policy. | | | | |

### 5.2.48L /*<x>*/*<x>*/OnNetwork/PrivateCall/EmergencyAlert/Entry

Table 5.2.48L.1: /*<x>*/<x>/OnNetwork/PrivateCall/EmergencyAlert/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/PrivateCall/EmergencyAlert/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the details of an MCPTT private emergency alert for on-network. | | | | |

### 5.2.48M /*<x>*/*<x>*/OnNetwork/PrivateCall/EmergencyAlert/Entry/ID

Table 5.2.48M.1: /*<x>*/<x>/OnNetwork/PrivateCall/EmergencyAlert/Entry/ID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/PrivateCall/EmergencyAlert/Entry/ID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the MCPTT user ID used upon certain criteria on initiation of an MCPTT private emergency alert for on-network. | | | | |

### 5.2.48N /*<x>*/*<x>*/OnNetwork/PrivateCall/EmergencyAlert/Entry/ DisplayName

Table 5.2.48N.1: /*<x>*/<x>/OnNetwork/PrivateCall/EmergencyAlert/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/PrivateCall/EmergencyAlert/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name that corresponds to the ID. | | | | |

### 5.2.48O /*<x>*/*<x>*/OnNetwork/PrivateCall/EmergencyAlert/Entry/Usage

Table 5.2.48O.1: /*<x>*/<x>/OnNetwork/PrivateCall/EmergencyAlert/Entry/Usage

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/PrivateCall/EmergencyAlert/Entry/Usage | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the criteria to determine when initiation of an MCPTT private emergency alert uses the ID. | | | | |

The valid values are 'LocallyDetermined' and 'UsePreConfigured'.

When set to 'LocallyDetermined' then if the MCPTT user selects an MCPTT ID then use that MCPTT ID for an on-network MCPTT private emergency alert, if the MCPTT user does not select a MCPTT ID then use the MCPTT ID identified by the ID in clause 5.2.48M for an on-network MCPTT private emergency alert.

When set to 'UsePreConfigured' then use the ID identified by the ID in clause 5.2.48M for an on-network MCPTT private emergency alert.

### 5.2.48P /*<x>*/*<x>*/OnNetwork/PrivateCall/AllowedCallBackRequest

Table 5.2.48P.1: /*<x>*/<x>/OnNetwork/PrivateCall/AllowedCallBackRequest

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/PrivateCall/AllowedCallBackRequest | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCPTT user is allowed to request a private call call-back. | | | | |

When set to "true" the MCPTT user is allowed to request a private call call-back.

When set to "false" the MCPTT user is not allowed to request a private call call-back.

### 5.2.48Q /<x>/<x>/OnNetwork/PrivateCall/AllowedCallBackCancelRequest

Table 5.2.48Q.1: /<x>/<x>/OnNetwork/PrivateCall/AllowedCallBackCancelRequest

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/PrivateCall/AllowedCallBackCancelRequest | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCPTT user is allowed to cancel an outstanding private call call-back request. | | | | |

When set to "true" the MCPTT user is allowed to cancel an outstanding private call call-back request.

When set to "false" the MCPTT user is not allowed to cancel an outstanding private call call-back request.

### 5.2.48R /*<x>*/*<x>*/OnNetwork/PrivateCall/ AllowedRemoteInitiatedAmbientListening

Table 5.2.48R.1: /*<x>*/<x>/OnNetwork/PrivateCall/AllowedRemoteInitiatedAmbientListening

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/PrivateCall/AllowedRemoteInitiatedAmbientListening | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCPTT user is allowed to request a remote initiated ambient listening call. | | | | |

When set to "true" the MCPTT user is allowed to request a remote initiated ambient listening call.

When set to "false" the MCPTT user is not allowed to request a remote initiated ambient listening call.

### 5.2.48S /<x>/<x>/OnNetwork/PrivateCall/ AllowedLocallyInitiatedAmbientListening

Table 5.2.48S.1: /<x>/<x>/OnNetwork/PrivateCall/AllowedLocallyInitiatedAmbientListening

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/PrivateCall/AllowedLocallyInitiatedAmbientListening | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCPTT user is allowed to request a locally initiated ambient listening call. | | | | |

When set to "true" the MCPTT user is allowed to request a locally initiated ambient listening call.

When set to "false" the MCPTT user is not allowed to request a locally initiated ambient listening call.

### 5.2.48T /*<x>*/*<x>*/OnNetwork/PrivateCall/ AllowedRequestFirstToAnswerCall

Table 5.2.48T.1: /*<x>*/<x>/OnNetwork/PrivateCall/AllowedRequestFirstToAnswerCall

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/PrivateCall/AllowedRequestFirstToAnswerCall | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCPTT user is allowed to request a first to answer call. | | | | |

When set to "true" the MCPTT user is allowed to request a first to answer call.

When set to "false" the MCPTT user is not allowed to request a first to answer call.

### 5.2.48U1 /*<x>*/*<x>*/OnNetwork/RemoteGroupSelection

Table 5.2.48U1.1: /*<x>*/<x>/OnNetwork/RemoteGroupSelection

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/RemoteGroupSelection | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the remote group selection configuration. | | | | |

### 5.2.48U2 /*<x>*/<x>/OnNetwork/RemoteGroupSelection/<x>

Table 5.2.48U2.1: /*<x>*/<x>/OnNetwork/RemoteGroupSelection/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/RemoteGroupSelection/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more remote group selection configuration elements. | | | | |

### 5.2.48U3 /*<x>*/<x>/OnNetwork/RemoteGroupSelection/<x>/Entry

Table 5.2.48U3.1: /*<x>*/<x>/OnNetwork/RemoteGroupSelection/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/RemoteGroupSelection/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the details of the on-network MCPTT users whose selected MCPTT group is allowed to be remotely changed by the MCPTT user. | | | | |

### 5.2.48U4 /*<x>*/<x>/OnNetwork/RemoteGroupSelection/<x>/Entry/ MCPTTID

Table 5.2.48U4.1: /*<x>*/<x>/OnNetwork/RemoteGroupSelection/<x>/Entry/MCPTTID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/RemoteGroupSelection/<x>/Entry/MCPTTID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates a MCPTT ID of an MCPTT user whose selected MCPTT group is allowed to be remotely changed by the MCPTT user. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 5.2.48U5 /*<x>*/*<x>*/OnNetwork/RemoteGroupSelection/<x>/Entry/ DisplayName

Table 5.2.48U5.1: /*<x>*/<x>/OnNetwork/RemoteGroupSelection/<x>/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/RemoteGroupSelection/<x>/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name that corresponds to the MCPTT ID of the MCPTT user. | | | | |

### 5.2.48V1 Void

### 5.2.48V2 Void

### 5.2.48V3 Void

### 5.2.48V4 Void

### 5.2.48V5 Void

### 5.2.48V6 Void

### 5.2.48V7 Void

### 5.2.48V8 Void

### 5.2.48V9 Void

### 5.2.48V10 Void

### 5.2.48V11 Void

### 5.2.48V12 Void

### 5.2.48V13 Void

### 5.2.48V14 Void

### 5.2.48V15 Void

### 5.2.48V16 Void

### 5.2.48V17 Void

### 5.2.48W1 /*<x>*/*<x>*/OnNetwork/AllowedRequestRemoteInitPrivateCall

Table 5.2.48W1.1: /*<x>*/<x>/OnNetwork/AllowedRequestRemoteInitPrivateCall

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/AllowedRequestRemoteInitPrivateCall | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCPTT user is authorised to request a remotely initiated private call. | | | | |

When set to "true" the MCPTT user is authorised to request remotely initiated private calls.

When set to "false" the MCPTT user is not authorised to request remotely initiated private calls.

### 5.2.48W2 /*<x>*/*<x>*/OnNetwork/AllowedRequestRemoteInitGroupCall

Table 5.2.48W2.1: /*<x>*/<x>/OnNetwork/AllowedRequestRemoteInitGroupCall

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/AllowedRequestRemoteInitGroupCall | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCPTT user is authorised to request a remotely initiated group call. | | | | |

When set to "true" the MCPTT user is authorised to request remotely initiated group calls.

When set to "false" the MCPTT user is not authorised to request remotely initiated group calls.

### 5.2.48W3 /*<x>*/*<x>*/OnNetwork/FunctionalAliasList

Table 5.2.48W3.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the functional alias configuration. | | | | |

### 5.2.48W4 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>

Table 5.2.48W4.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more functional alias configuration elements. | | | | |

### 5.2.48W5 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry

Table 5.2.48W5.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the details of the functional alias. | | | | |

### 5.2.48W6 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ FunctionalAlias

Table 5.2.48W6.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/FunctionalAlias

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/FunctionalAlias | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates a functional alias that can be activated by the MCPTT user. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 5.2.48W6A /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation

Table 5.2.48W6A.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node contains the location criteria for activation of a functional alias. | | | | |

### 5.2.48W6A0 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>

Table 5.2.48W6A0.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrMore | node | Get, Replace |  |
|  | This interior node contains the zero or more location criteria for activation of a functional alias. | | | | |

### 5.2.48W6A1 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/ Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea

Table 5.2.48W6A1.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node contains a geographical area which when entered by the MC service UE triggers the functional alias activation. | | | | |

### 5.2.48W6A2 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/PolygonArea

Table 5.2.48W6A2.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/PolygonArea

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/PolygonArea | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node contains a geographical area described by a polygon. | | | | |

### 5.2.48W6A3 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ PolygonArea/<x>

Table 5.2.48W6A3.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/PolygonArea/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/PolygonArea/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrN | node | Get, Replace |  |
|  | This interior node contains the coordinates of the corners which define a polygon. The occurrence of this leaf node is "3 to 15" as per 3GPP TS 23.032 [21]. | | | | |

### 5.2.48W6A3A /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ PolygonArea/<x>/PointCoordinateType

Table 5.2.48W6A3A.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |  |

### 5.2.48W6A4 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ PolygonArea/<x>/PointCoordinateType/Longitude

Table 5.2.48W6A4.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the longitudinal coordinate of a corner. | | | | |

- Values: 0-16777215

### 5.2.48W6A5 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ PolygonArea/<x>/PointCoordinateType/Latitude

Table 5.2.48W6A5.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the latitudinal coordinate of a corner. | | | | |

- Values: 0-16777215

### 5.2.48W6A6 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ EllipsoidArcArea

Table 5.2.48W6A6.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/EllipsoidArcArea

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/EllipsoidArcArea | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node contains a geographical area described by an ellipsoid arc. | | | | |

### 5.2.48W6A7 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Center

Table 5.2.48W6A7.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/EllipsoidArcArea/Center

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/EllipsoidArcArea/Center | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |

### 5.2.48W6A7A /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType

Table 5.2.48W6A7A.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |  |

### 5.2.48W6A8 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType/Longitude

Table 5.2.48W6A8.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Longitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Longitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the longitudinal coordinate of the center. | | | | |

- Values: 0-16777215

### 5.2.48W6A9 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType/Latitude

Table 5.2.48W6A9.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Latitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Latitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the latitudinal coordinate of the center. | | | | |

- Values: 0-16777215

### 5.2.48W6A10 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ EnterSpecificArea/EllipsoidArcArea/Radius

Table 5.2.48W6A10.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/EllipsoidArcArea/Radius

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/EllipsoidArcArea/Radius | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the radius of the ellipsoid arc. | | | | |

- Values: non-negative integer

### 5.2.48W6A11 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ EnterSpecificArea/EllipsoidArcArea/OffsetAngle

Table 5.2.48W6A11.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/EllipsoidArcArea/OffsetAngle

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/EllipsoidArcArea/OffsetAngle | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the offset angle of the ellipsoid arc. | | | | |

- Values: 0-255

### 5.2.48W6A12 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ EnterSpecificArea/EllipsoidArcArea/IncludedAngle

Table 5.2.48W6A12.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/EllipsoidArcArea/IncludedAngle

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/EllipsoidArcArea/IncludedAngle | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the included angle of the ellipsoid arc. | | | | |

- Values: 0-255

### 5.2.48W6A12A /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/Speed

Table 5.2.48W6A12A.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/Speed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/Speed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | One | node | Get, Replace |  |  |
|  | This interior node contains the speed. | | | | |  |

### 5.2.48W6A12B /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/Speed/ MinimumSpeed

Table 5.2.48W6A12B.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/Speed/MinimumSpeed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/Speed/MinimumSpeed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the minimum speed. | | | | |  |

- Values: non-negative integer in units of kilometers/hour.

### 5.2.48W6A12C /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/Speed/ MaximumSpeed

Table 5.2.48W6A12C.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/Speed/MaximumSpeed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/Speed/MaximumSpeed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the maximum speed. | | | | |  |

- Values: non-negative integer in units of kilometers/hour.

### 5.2.48W6A12D /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/Heading

Table 5.2.48W6A12D.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/Heading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/Heading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | One | node | Get, Replace |  |  |
|  | This interior node contains the heading. | | | | |  |

### 5.2.48W6A12E /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/Heading/ MinimumHeading

Table 5.2.48W6A12E.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/Heading/MinimumHeading

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/Heading/MinimumHeading | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the minimum heading. | | | | |

- Values: 0-359

### 5.2.48W6A12F /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/Heading/ MaximumHeading

Table 5.2.48W6A12F.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/Heading/MaximumHeading

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/Heading/MaximmHeading | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the maximum heading. | | | | |

- Values: 0-359

### 5.2.48W6A13 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ ExitSpecificArea

Table 5.2.48W6A13.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node contains a geographical area which when exited by the MC service UE triggers the functional alias activation. | | | | |

### 5.2.48W6A14 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ ExitSpecificArea/PolygonArea

Table 5.2.48W6A14.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/PolygonArea

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/PolygonArea | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node contains a geographical area described by a polygon. | | | | |

### 5.2.48W6A15 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ ExitSpecificArea/PolygonArea/<x>

Table 5.2.48W6A15.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/PolygonArea/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/PolygonArea/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrN | node | Get, Replace |  |
|  | This interior node contains the coordinates of the corners which define a polygon. The occurrence of this leaf node is "3 to 15" as per 3GPP TS 23.032 [21]. | | | | |

### 5.2.48W6A15A /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/ PolygonArea/<x>/PointCoordinateType

Table 5.2.48W6A15A.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the type of the coordinates. | | | | |  |

### 5.2.48W6A16 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude

Table 5.2.48W6A16.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the longitudinal coordinate of a corner. | | | | |

- Values: 0-16777215

### 5.2.48W6A17 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude

Table 5.2.48W6A17.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the latitudinal coordinate of a corner. | | | | |

- Values: 0-16777215

### 5.2.48W6A18 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ ExitSpecificArea/EllipsoidArcArea

Table 5.2.48W6A18.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/EllipsoidArcArea

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/EllipsoidArcArea | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node contains a geographical area described by an ellipsoid arc. | | | | |

### 5.2.48W6A19 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ ExitSpecificArea/EllipsoidArcArea/Center

Table 5.2.48W6A19.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/EllipsoidArcArea/Center

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/EllipsoidArcArea/Center | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |

### 5.2.48W6A19A /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType

Table 5.2.48W6A19A.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |  |

### 5.2.48W6A20 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Longitude

Table 5.2.48W6A20.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Longitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Longitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the longitudinal coordinate of the center. | | | | |

- Values: 0-16777215

### 5.2.48W6A21 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Latitude

Table 5.2.48W6A21.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Latitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Latitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the latitudinal coordinate of the center. | | | | |

- Values: 0-16777215

### 5.2.48W6A22 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ ExitSpecificArea/EllipsoidArcArea/Radius

Table 5.2.48W6A22.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/EllipsoidArcArea/Radius

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/EllipsoidArcArea/Radius | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the radius of the ellipsoid arc. | | | | |

- Values: non-negative integer

### 5.2.48W6A23 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ ExitSpecificArea/EllipsoidArcArea/OffsetAngle

Table 5.2.48W6A23.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/EllipsoidArcArea/OffsetAngle

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/EllipsoidArcArea/OffsetAngle | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the offset angle of the ellipsoid arc. | | | | |

- Values: 0-255

### 5.2.48W6A24 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ ExitSpecificArea/EllipsoidArcArea/IncludedAngle

Table 5.2.48W6A24.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/EllipsoidArcArea/IncludedAngle

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/EllipsoidArcArea/IncludedAngle | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the included angle of the ellipsoid arc. | | | | |

- Values: 0-255

### 5.2.48W6A24A /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/Speed

Table 5.2.48W6A24A.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/Speed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/Speed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | One | node | Get, Replace |  |  |
|  | This interior node contains the speed. | | | | |  |

### 5.2.48W6A24B /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/Speed/ MinimumSpeed

Table 5.2.48W6A24B.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/Speed/MinimumSpeed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/Speed/MinimumSpeed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the minimum speed. | | | | |  |

- Values: non-negative integer in units of kilometers/hour.

### 5.2.48W6A24C /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/Speed/ MaximumSpeed

Table 5.2.48W6A24C.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/Speed/MaximumSpeed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/Speed/MaximumSpeed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the maximum speed. | | | | |  |

- Values: non-negative integer in units of kilometers/hour.

### 5.2.48W6A24D /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/Heading

Table 5.2.48W6A24D.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/Heading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/Heading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | One | node | Get, Replace |  |  |
|  | This interior node contains the heading. | | | | |  |

### 5.2.48W6A24E /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/Heading/ MinimumHeading

Table 5.2.48W6A24E.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/Heading/MinimumHeading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/Heading/MinimumHeading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the minimum heading. | | | | |  |

- Values: 0-359

### 5.2.48W6A24F /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/Heading/ MaximumHeading

Table 5.2.48W6A24E.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/Heading/MaximumHeading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/Heading/MaximumumHeading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the maximum heading. | | | | |  |

- Values: 0-359

### 5.2.48W6B /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation

Table 5.2.48W6B.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node contains the location criteria for de-activation of a functional alias. | | | | |

### 5.2.48W6B0 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>

Table 5.2.48W6B0.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrMore | node | Get, Replace |  |
|  | This interior node contains the zero or more location criteria for de-activation of a functional alias. | | | | |

### 5.2.48W6B1 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea

Table 5.2.48W6B1.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node contains a geographical area which when entered by the MC service UE triggers the functional alias de-activation. | | | | |

### 5.2.48W6B2 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ PolygonArea

Table 5.2.48W6B2.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/PolygonArea

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/PolygonArea | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node contains a geographical area described by a polygon. | | | | |

### 5.2.48W6B3 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ PolygonArea/<x>

Table 5.2.48W6B3.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/PolygonArea/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/PolygonArea/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrN | node | Get, Replace |  |
|  | This interior node contains the coordinates of the corners which define a polygon. The occurrence of this leaf node is "3 to 15" as per 3GPP TS 23.032 [21]. | | | | |

### 5.2.48W6B3A /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ PolygonArea/<x>/PointCoordinateType

Table 5.2.48W6B3A.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |  |

### 5.2.48W6B4 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ PolygonArea/<x>/PointCoordinateType/Longitude

Table 5.2.48W6B4.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the longitudinal coordinate of a corner. | | | | |

- Values: 0-16777215

### 5.2.48W6B5 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ PolygonArea/<x>/PointCoordinateType/Latitude

Table 5.2.48W6B5.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the latitudinal coordinate of a corner. | | | | |

- Values: 0-16777215

### 5.2.48W6B6 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ EllipsoidArcArea

Table 5.2.48W6B6.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/EllipsoidArcArea

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/EllipsoidArcArea | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node contains a geographical area described by an ellipsoid arc. | | | | |

### 5.2.48W6B7 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Center

Table 5.2.48W6B7.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/EllipsoidArcArea/Center

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/EllipsoidArcArea/Center | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |

### 5.2.48W6B7A /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType

Table 5.2.48W6B7A.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |  |

### 5.2.48W6B8 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType/Longitude

Table 5.2.48W6B8.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Longitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Longitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the longitudinal coordinate of the center. | | | | |

- Values: 0-16777215

### 5.2.48W6B9 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType/Latitude

Table 5.2.48W6B9.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Latitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Latitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the latitudinal coordinate of the center. | | | | |

- Values: 0-16777215

### 5.2.48W6B10 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ EnterSpecificArea/EllipsoidArcArea/Radius

Table 5.2.48W6B10.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/EllipsoidArcArea/Radius

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/EllipsoidArcArea/Radius | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the radius of the ellipsoid arc. | | | | |

- Values: non-negative integer

### 5.2.48W6B11 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ EnterSpecificArea/EllipsoidArcArea/OffsetAngle

Table 5.2.48W6B11.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/EllipsoidArcArea/OffsetAngle

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/EllipsoidArcArea/OffsetAngle | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the offset angle of the ellipsoid arc. | | | | |

- Values: 0-255

### 5.2.48W6B12 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ EnterSpecificArea/EllipsoidArcArea/IncludedAngle

Table 5.2.48W6B12.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/EllipsoidArcArea/IncludedAngle

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/EllipsoidArcArea/IncludedAngle | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the included angle of the ellipsoid arc. | | | | |

- Values: 0-255

### 5.2.48W6B12A /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Speed

Table 5.2.48W6B12A.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Speed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Speed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | One | node | Get, Replace |  |  |
|  | This interior node contains the speed. | | | | |  |

### 5.2.48W6B12B /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Speed/ MinimumSpeed

Table 5.2.48W6B12B.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Speed/MinimumSpeed

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Speed/MinimumSpeed | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the minimum speed. | | | | |

- Values: non-negative integer in units of kilometers/hour.

### 5.2.48W6B12C /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Speed/ MaximumSpeed

Table 5.2.48W6B12C.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Speed/MaximumSpeed

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Speed/MaximumSpeed | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the maximum speed. | | | | |

- Values: non-negative integer in units of kilometers/hour.

### 5.2.48W6B12D /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Heading

Table 10.2.97B3C18.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Heading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Heading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | One | node | Get, Replace |  |  |
|  | This interior node contains the heading. | | | | |  |

### 5.2.48W6B12E /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Heading/ MinimumHeading

Table 5.2.48W6B12E.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Heading/MinimumHeading

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Heading/MinimumHeading | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the minimum heading. | | | | |

- Values: 0-359

### 5.2.48W6B12F /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Heading/ MaximumHeading

Table 5.2.48W6B12F.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Heading/MaximumHeading

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Heading/MaximumHeading | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the maximum heading. | | | | |

- Values: 0-359

### 5.2.48W6B13 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ ExitSpecificArea

Table 5.2.48W6B13.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node contains a geographical area which when exited by the MC service UE triggers the functional alias de-activation. | | | | |

### 5.2.48W6B14 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ ExitSpecificArea/PolygonArea

Table 5.2.48W6B14.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/PolygonArea

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/PolygonArea | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node contains a geographical area described by a polygon. | | | | |

### 5.2.48W6B15 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ ExitSpecificArea/PolygonArea/<x>

Table 5.2.48W6B15.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/PolygonArea/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/PolygonArea/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrN | node | Get, Replace |  |
|  | This interior node contains the coordinates of the corners which define a polygon. The occurrence of this leaf node is "3 to 15" as per 3GPP TS 23.032 [21]. | | | | |

### 5.2.48W6B15A /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/ PolygonArea/<x>/PointCoordinateType

Table 5.2.48W6B15A.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |  |

### 5.2.48W6B16 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude

Table 5.2.48W6B16.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the longitudinal coordinate of a corner. | | | | |

- Values: 0-16777215

### 5.2.48W6B17 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude

Table 5.2.48W6B17.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the latitudinal coordinate of a corner. | | | | |

- Values: 0-16777215

### 5.2.48W6B18 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ ExitSpecificArea/EllipsoidArcArea

Table 5.2.48W6B18.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/EllipsoidArcArea

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/EllipsoidArcArea | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node contains a geographical area described by an ellipsoid arc. | | | | |

### 5.2.48W6B19 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ ExitSpecificArea/EllipsoidArcArea/Center

Table 5.2.48W6B19.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/EllipsoidArcArea/Center

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/EllipsoidArcArea/Center | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |

### 5.2.48W6B19A /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType

Table 5.2.48W6B19A.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |  |

### 5.2.48W6B20 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Longitude

Table 5.2.48W6B20.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Longitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Longitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the longitudinal coordinate of the center. | | | | |

- Values: 0-16777215

### 5.2.48W6B21 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Latitude

Table 5.2.48W6B21.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Latitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Latitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the latitudinal coordinate of the center. | | | | |

- Values: 0-16777215

### 5.2.48W6B22 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ ExitSpecificArea/EllipsoidArcArea/Radius

Table 5.2.48W6B22.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/EllipsoidArcArea/Radius

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/EllipsoidArcArea/Radius | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the radius of the ellipsoid arc. | | | | |

- Values: non-negative integer

### 5.2.48W6B23 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ ExitSpecificArea/EllipsoidArcArea/OffsetAngle

Table 5.2.48W6B23.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/EllipsoidArcArea/OffsetAngle

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/EllipsoidArcArea/OffsetAngle | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the offset angle of the ellipsoid arc. | | | | |

- Values: 0-255

### 5.2.48W6B24 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ ExitSpecificArea/EllipsoidArcArea/IncludedAngle

Table 5.2.48W6B24.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/EllipsoidArcArea/IncludedAngle

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/EllipsoidArcArea/IncludedAngle | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the included angle of the ellipsoid arc. | | | | |

- Values: 0-255

### 5.2.48W6B24A /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Speed

Table 5.2.48W6B24A.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Speed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Speed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | One | node | Get, Replace |  |  |
|  | This interior node contains the speed. | | | | |  |

### 5.2.48W6B24B /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Speed/ MinimumSpeed

Table 5.2.48W6B24B.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Speed/MinimumSpeed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Speed/MinimumSpeed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the minimum speed. | | | | |  |

- Values: non-negative integer in units of kilometers/hour.

### 5.2.48W6B24C /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Speed/ MaximumSpeed

Table 5.2.48W6B24C.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Speed/MaximumSpeed

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Speed/MaximumSpeed | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the maximum speed. | | | | |

- Values: non-negative integer in units of kilometers/hour.

### 5.2.48W6B24D /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Heading

Table 5.2.48W6B24D.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Heading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Heading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | One | node | Get, Replace |  |  |
|  | This interior node contains the heading. | | | | |  |

### 5.2.48W6B24E /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Heading/ MinimumHeading

Table 5.2.48W6B24E.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Heading/MinimumHeading

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Heading/MinimumHeading | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the minimum heading. | | | | |

- Values: 0-359

### 5.2.48W6B24F /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Heading/ MaximumHeading

Table 5.2.48W6B24F.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Heading/MaximumHeading

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Heading/MaximumHeading | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the maximum heading. | | | | |

- Values: 0-359

### 5.2.48W6C /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ ManualDeactivationNotAllowedIfLocationCriteriaMet

Table 5.2.48W6E.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ManualDeactivationNotAllowedIfLocationCriteriaMet

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/ManualDeactivationNotAllowedIfLocationCriteriaMet | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCPTT user is authorised to de-activate a functional alias if the location criteria is met. | | | | |

### 5.2.48W7 /*<x>*/*<x>*/OnNetwork/FunctionalAliasList/<x>/Entry/DisplayName

Table 5.2.48W7.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name that corresponds to a functional alias that can be activated by the MCPTT user. | | | | |

### 5.2.48W7A /*<x>*/*<x>*/OnNetwork/FunctionalAliasList/<x>/Entry/ MaxSimultaneousEmergencyGroupCalls

Table 5.2.48W7A.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/MaxSimultaneousEmergencyGroupCalls

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/MaxSimultaneousEmergencyGroupCalls | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | int | Get, Replace |  |
|  | This leaf node indicates the maximum number of simultaneous emergency group calls for a functional alias. | | | | |

### 5.2.48W8 /*<x>*/*<x>*/OnNetwork/AllowedQueryFunctionalAliasOtherUser

Table 5.2.48W8.1: /*<x>*/<x>/OnNetwork/AllowedQueryFunctionalAliasOtherUser

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/AllowedQueryFunctionalAliasOtherUser | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCPTT user is authorised query the functional alias(es) activated by another MCPTT user. | | | | |

When set to "true" the MCPTT user is authorised to query the functional alias(es) activated by another MCPTT user.

When set to "false" the MCPTT user is not authorised to query the functional alias(es) activated by another MCPTT user.

### 5.2.48W9 /*<x>*/*<x>*/OnNetwork/AllowedTakeoverFunctionalAliasOtherUser

Table 5.2.48W9.1: /*<x>*/<x>/OnNetwork/AllowedTakeoverFunctionalAliasOtherUser

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/AllowedTakeoverFunctionalAliasOtherUser | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCPTT user is authorised to take over the functional alias(es) previously activated by another MCPTT user. | | | | |

When set to "true" the MCPTT user is authorised to take over the functional alias(es) previously activated by another MCPTT user.

When set to "false" the MCPTT user is not authorised to take over the functional alias(es) previously activated by another MCPTT user.

### 5.2.48W10 /*<x>*/*<x>*/OnNetwork/AllowedLocationInfoWhenTalking

Table 5.2.48W10.1: /*<x>*/<x>/OnNetwork/AllowedLocationInfoWhenTalking

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/AllowedLocationInfoWhenTalking | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCPTT user is authorised to send its location information when it is requesting the floor. | | | | |

When set to "true" the MCPTT user is authorised to send its location information when it is requesting the floor.

When set to "false" the MCPTT user is not authorised to send its location information when it is requesting the floor.

### 5.2.48X /*<x>*/*<x>*/OnNetwork/AuthorisedIncomingAny

Table 5.2.48.1: /*<x>*/<x>/OnNetwork/AuthorisedIncomingAny

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/AuthorisedIncomingAny | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to receive a MCPTT private call by any MCPTT user. | | | | |

When set to "true" the MCPTT user is authorised to receive an MCPTT private call by any MCPTT user.

When set to "false" the MCPTT user is not authorised to receive an MCPTT private call by any MCPTT user.

### 5.2.48Y1 /*<x>*/<x>/OnNetwork/UserList

Table 5.2.48Y1.1: /*<x>*/<x>/OnNetwork/UserList

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/UserList | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for a list of MCPTT user(s) who can call this particular user in a MCPTT private call. | | | | |

### 5.2.48Y2 /*<x>*/<x>/OnNetwork/UserList/<x>

Table 5.2.48Y2.1: /*<x>*/<x>/OnNetwork/UserList/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/UserList/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more list of MCPTT users who can call this particular user in a MCPTT private call. | | | | |

### 5.2.48Y3 /*<x>*/<x>/OnNetwork/UserList/<x>/Entry

Table 5.2.48Y3.1: /*<x>*/<x>/OnNetwork/UserList/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/UserList/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more MCPTT users who can call the particular user in a private call. | | | | |

### 5.2.48Y4 /*<x>*/<x>/OnNetwork/UserList/<x>/Entry/MCPTTID

Table 5.2.48Y4.1: /*<x>*/<x>/OnNetwork/UserList/<x>/Entry/MCPTTID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/UserList/<x>/Entry/MCPTTID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates an MCPTT user identity (MCPTT ID) which is a globally unique identifier within the MCPTT service that represents the MCPTT user. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 5.2.48Y5 /*<x>*/<x>/OnNetwork/UserList/<x>/Entry/PrivateCallKMSURI

Table 5.2.48Y5.1: /*<x>*/<x>/OnNetwork/UserList/<x>/Entry/PrivateCallKMSURI

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/UserList/<x>/Entry/PrivateCallKMSURI | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates the identity (URI) of the KMS associated with the MCPTTID. If the value is empty, the KMS leaf node present in the MCS UE initial configuration MO is used. | | | | |

### 5.2.48Z /*<x>*/*<x>*/OnNetwork/AuthorisedReceiveNonAcknowledged

Table 5.2.48Z.1: /*<x>*/<x>/OnNetwork/AuthorisedReceiveNonAcknowledged

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/AuthorisedReceiveNonAcknowledged | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to receive the list of non-acknowledged MCPTT users to a group session invitation. | | | | |

When set to "true" the MCPTT user is authorised to receive information about the MCPTT Users that did not acknowledge a group session invitation.

When set to "false" the MCPTT user is not authorised to receive information about MCPTT Users that did not acknowledge a group session invitation.

### 5.2.49 /*<x>*/*<x>*/OffNetwork

Table 5.2.49.1: /*<x>*/<x>/OffNetwork

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | node | Get, Replace |  |
|  | This interior node represents a container for off-network operation. | | | | |

### 5.2.50 /*<x>*/*<x>*/OffNetwork/Authorised

Table 5.2.50.1: /*<x>*/<x>/OffNetwork/Authorised

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/Authorised | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation for off-network services. | | | | |

When set to "true" the MCPTT user is authorised for off-network.

When set to "false" the MCPTT user is not authorised for off-network operation.

### 5.2.51 /*<x>*/*<x>*/OffNetwork/MCPTTGroupInfo

Table 5.2.51.1: /*<x>*/<x>/OffNetwork/MCPTTGroupInfo

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCPTTGroupInfo | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for group information. | | | | |

### 5.2.52 /*<x>*/<x>/OffNetwork/MCPTTGroupInfo/<x>

Table 5.2.52.1: /*<x>*/<x>/OffNetwork/MCPTTGroupInfo/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCPTTGroupInfo/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more group information. | | | | |

### 5.2.52A /*<x>*/<x>/OffNetwork/MCPTTGroupInfo/<x>/Entry

Table 5.2.52A.1: /*<x>*/<x>/OffNetwork/MCPTTGroupInfo/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCPTTGroupInfo/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more off-network MCPTT groups for use by an MCPTT user. | | | | |

### 5.2.53 /*<x>*/<x>/OffNetwork/MCPTTGroupInfo/<x>/Entry/MCPTTGroupID

Table 5.2.53.1: /*<x>*/<x>/OffNetwork/MCPTTGroupInfo/<x>/Entry/MCPTTGroupID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCPTTGroupInfo/<x>/Entry/MCPTTGroupID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates an off-network MCPTT group for use by an MCPTT user. | | | | |

### 5.2.53A /*<x>*/*<x>*/OffNetwork/MCPTTGroupInfo/<x>/Entry/DisplayName

Table 5.2.53A.1: /*<x>*/<x>/OffNetwork/MCPTTGroupInfo/<x>/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCPTTGroupInfo/<x>/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name that corresponds to the MCPTT group represented by the MCPTT group ID. | | | | |

### 5.2.53B /<x>/<x>/OffNetwork/MCPTTGroupInfo/<x>/Entry/ RelativePresentationPriority

Table 5.2.53B.1: /<x>/<x>/OffNetwork/MCPTTGroupInfo/<x>/Entry/RelativePresentationPriority

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| *<x>*/OffNetwork/MCPTTGroupInfo/<x>/Entry/RelativePresentationPriority | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | int | Get, Replace |  |
|  | This leaf node indicates indicating the presentation priority of the off-network group for the MCPTT user relative to other off-network groups and off-network users. | | | | |

- Values: 0-255

The lowest RelativePresentationPriority value shall be considered as the MCPTT group transaction having the lowest priority for presentation among other group MCPTT and one-to-one user transactions.

### 5.2.53C /<x>/<x>/OffNetwork/MCPTTGroupInfo/<x>/Entry/GMSServID

Table 5.2.53C.1: /<x>/<x>/OffNetwork/MCPTTGroupInfo/<x>/Entry/GMSServID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCPTTGroupInfo/<x>/Entry/GMSServID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the identity (URI) of the GMS owning a specific group contained in the off-network MCPTTGroupList. | | | | |

### 5.2.53D /<x>/<x>/OffNetwork/MCPTTGroupInfo/<x>/Entry/ IDMSTokenEndPoint

Table 5.2.53D.1: /<x>/<x>/OffNetwork/MCPTTGroupInfo/<x>/Entry/IDMSTokenEndPoint

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCPTTGroupInfo/<x>/Entry/IDMSTokenEndPoint | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the identity (URI) of the IDMS token endpoint for a specific group contained in the off-network MCPTTGroupList. If the value is empty, the IDMS identities (IDMSAuthEndpoint and IDMSTokenEndpoint) present in the MCS UE initial configuration MO are used. | | | | |

### 5.2.53E /<x>/<x>/OffNetwork/MCPTTGroupInfo/<x>/Entry/GroupKMSURI

Table 5.2.53E.1: /<x>/<x>/OffNetwork/MCPTTGroupInfo/<x>/Entry/GroupKMSURI

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCPTTGroupInfo/<x>/Entry/GroupKMSURI | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the identity (URI) of the KMS identity (URI) for a specific group contained in the off-network MCPTTGroupList. If the value is empty, the KMS identity (URI) (kms) present in the MCS UE initial configuration MO is used. | | | | |

### 5.2.54 /*<x>*/*<x>*/OffNetwork/AllowedListen

Table 5.2.54.1: /*<x>*/<x>/OffNetwork/AllowedListen

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/AllowedListen | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCPTT user is allowed to listen both overriding and overridden. | | | | |

When set to "true" the MCPTT user is allowed to listen both overriding and overridden.

When set to "false" the MCPTT user is not allowed to listen both overriding and overridden.

### 5.2.55 /*<x>*/*<x>*/OffNetwork/AllowedTransmission

Table 5.2.55.1: /*<x>*/<x>/OffNetwork/AllowedTransmission

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/AllowedTransmission | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCPTT user is allowed to transmit in case of override (overriding and/or overridden). | | | | |

When set to "true" the MCPTT user is allowed to transmit in case of override (overriding and/or overridden).

When set to "false" the MCPTT user is not allowed to transmit in case of override (overriding and/or overridden).

### 5.2.56 /*<x>*/*<x>*/OffNetwork/EmergencyCallChange

Table 5.2.56.1: /*<x>*/<x>/OffNetwork/EmergencyCallChange

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/EmergencyCallChange | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorization for a participant to change an off-network group call in-progress to an off-network MCPTT emergency group call. | | | | |

When set to "true" the MCPTT user is authorised to change an MCPTT emergency group call.

When set to "false" the MCPTT user is not authorised to change an MCPTT emergency group call.

### 5.2.57 /*<x>*/*<x>*/OffNetwork/ImminentPerilCallChange

Table 5.2.57.1: /*<x>*/<x>/OffNetwork/ImminentPerilCallChange

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/ImminentPerilCallChange | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorization for a participant to change an off-network group call in-progress to an off-network MCPTT imminent peril group call. | | | | |

When set to "true" the MCPTT user is authorised to change an MCPTT imminent peril group call.

When set to "false" the MCPTT user is not authorised to change an MCPTT imminent peril group call.

### 5.2.58 /*<x>*/*<x>*/OffNetwork/UserInfoID

Table 5.2.58.1: /*<x>*/<x>/OffNetwork/UserInfoID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/UserInfoID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the ProSe user info ID as specified in 3GPP TS 23.303 [6]. | | | | |

### 5.2.58A1 Void

### 5.2.58A2 Void

### 5.2.58A3 Void

### 5.2.58A4 Void

### 5.2.58A5 Void

### 5.2.58A6 Void

### 5.2.58A7 Void

### 5.2.58A8 Void

### 5.2.58A9 Void

### 5.2.58A10 Void

### 5.2.58A11 Void

### 5.2.58A12 Void

### 5.2.58A13 Void

### 5.2.58A14 Void

### 5.2.58A15 Void

### 5.2.58A16 Void

### 5.2.58A17 Void

### 5.2.59 /*<x>*/Status

Table 5.2.59.1: /*<x>*/Status

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Status | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | bool | Get, Replace |  |
|  | This leaf node indicates whether this MCPTT user profile is enabled or disabled. | | | | |

When set to "true" this MCPTT user profile is enabled.

When set to "false" this MCPTT user profile is disabled.

# 6 MCS group configuration MO

## 6.1 General

The MCS group configuration Management Object (MO) is used to configure the MCS Client behaviour for the on-network or off-network MC services. The MCS group configuration parameters may be stored in the ME, or in the USIM as specified in 3GPP TS 31.102 [10], or in both the ME and the USIM. If both the ME and the USIM contain the same parameters, the values stored in the USIM shall take precedence.

NOTE: For historical reasons some of the elements in the MCS group configuration Management Object (MO) use the terminology "MCPTT", however this MO is common to all MCS with some MCPTT specific elements, some MCData specific elements and some MCVideo specific elements. Not all elements that contain the terminology "MCPTT" are just MCPTT specific. In the clauses that follow, it is made clear what aspects are specific to MCPTT and what aspects are specific to all MC services. MCData specific elements are contained under "MCData" nodes. MCVideo specific elements are contained under "MCVideo" nodes.

The Management Object Identifier is: urn:oma:mo:ext-3gpp-MCPTT-group-configuration:1.0.

Protocol compatibility: This MO is compatible with OMA OMA DM 1.2 [3].

The OMA DM ACL property mechanism (see OMA OMA-ERELD-DM-V1\_2 [2]) may be used to grant or deny access rights to OMA DM servers in order to modify nodes and leaf objects of the MCS group configuration MO.

The following nodes and leaf objects are possible under the MCS group configuration node as described in figure 6.1.1.



Figure 6.1.1: The MCS group configuration MO (1 of 5)



Figure 6.1.2: The MCS group configuration MO (2 of 5)



Figure 6.1.3: The MCS group configuration MO (3 of 5)



Figure 6.1.4: The MCS group configuration MO (4 of 5)



Figure 6.1.5: The MCS group configuration MO (5 of 5)

## 6.2 MCS group configuration MO parameters

### 6.2.1 General

This clause describes the parameters for the MCS group configuration Management Object (MO).

### 6.2.2 Node: *<x>*

Table 6.2.2.1: Node: *<x>*

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get |  |
|  | This interior node acts as a placeholder for the MCS group configuration Management Object (MO).  For the MCS group configuration MO, the namespace specific string is: "urn:oma:mo:oma-dm-mcptt-group configuration:1.0" | | | | |

- Values: N/A

### 6.2.3 /*<x>*/Name

Table 6.2.3.1: Node: *<x>*

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | chr | Get |  |
|  | The Name leaf is a name for the MCS group configuration settings. | | | | |

- Values: <User displayable name>

### 6.2.4 /*<x>*/Ext/

Table 6.2.4.1: /*<x>*/Ext/

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Ext | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | The Ext is an interior node for where the vendor specific information about the MCSgroup configuration MO is being placed. | | | | |

Usually the vendor extension is identified by vendor specific name under the ext node and contains the vendor meaning application vendor, device vendor etc. The tree structure under the vendor identified is not defined and can therefore include one or more un-standardized sub-trees.

- Values: N/A

### 6.2.5 /*<x>*/<x>

Table 6.2.5.1: /*<x>*/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrMore | node | Get, Replace |  |
|  | This interior node represents a container for on-network operation and off-network operation. | | | | |

### 6.2.6 /*<x>*/<x>/Common

Table 6.2.6.1: /*<x>*/<x>/Common

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | node | Get, Replace |  |
|  | This interior node represents a container for the common network operation which means both on-network operation and off-network operation. | | | | |

### 6.2.7 /*<x>*/<x>/Common/MCPTTGroupID

Table 6.2.7.1: /*<x>*/<x>/Common/MCPTTGroupID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the MCS group ID. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

NOTE: This element is common for all MC services.

### 6.2.8 /*<x>*/<x>/Common/MCPTTGroupAlias

Table 6.2.8.1: /*<x>*/<x>/Common/MCPTTGroupAlias

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupAlias | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the MCS group alias. | | | | |

The value is a <display-name> element specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

NOTE: This element is common for all MC services.

### 6.2.9 /*<x>*/<x>/Common/MCPTTGroupMemberList

Table 6.2.9.1: /*<x>*/<x>/Common/MCPTTGroupMemberList

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupMemberList | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for a list of MCS group members (group membership information). | | | | |

NOTE: This element is common for all MC services.

### 6.2.10 /*<x>*/<x>/Common/MCPTTGroupMemberList/<x>

Table 6.2.10.1: /*<x>*/<x>/Common/MCPTTGroupMemberList/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupMemberList/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more list(s) of MCS group members. | | | | |

NOTE: This element is common for all MC services.

### 6.2.11 /*<x>*/<x>/Common/MCPTTGroupMemberList/<x>/MCPTTID

Table 6.2.11.1: /*<x>*/<x>/Common/MCPTTGroupMemberList/<x>/MCPTTID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupMemberList/<x>/MCPTTID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates an MCS user identity (MC Service ID) which is a globally unique identifier within the MC service that represents the MCS user. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

NOTE: This element is common for all MC services.

### 6.2.12 /*<x>*/<x>/Common/MCPTTGroupMemberList/<x>/UserPriority

Table 6.2.12.1: /*<x>*/<x>/Common/MCPTTGroupMemberList/<x>/UserPriority

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupMemberList/<x>/UserPriority | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the user priority for the group. | | | | |

The value is a <user-priority> element specified in 3GPP TS 24.481 [9] clause 7.2.4.2.

NOTE: This element is common for all MC services.

### 6.2.13 /*<x>*/<x>/Common/MCPTTGroupMemberList/<x>/ParticipantType

Table 6.2.13.1: /*<x>*/<x>/Common/MCPTTGroupMemberList/<x>/ParticipantType

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupMemberList/<x>/ParticpantType | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the participant type for the group. | | | | |

The ParticipantType values are defined and configured by the Mission Critical Organisation (e.g.first responder, second responder, dispatcher, dispatch supervisor, MCS administrator).

NOTE: This element is common for all MC services.

### 6.2.14 Void

### 6.2.15 /*<x>*/<x>/Common/MCPTTGroupOwner

Table 6.2.15.1: /*<x>*/<x>/Common/MCPTTGroupOwner

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupOwner | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the group's owner (Mission Critical Organisation). | | | | |

NOTE: This element is common for all MC services.

### 6.2.16 /*<x>*/<x>/Common/PreferredVoiceCodec

Table 6.2.16.1: /*<x>*/<x>/Common/PreferredVoiceCodec

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PreferredVoiceCodec | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the MCPTT preferred voice codec for an MCS group. | | | | |

The value of the preferred voice codec is a RTP payload format name specified in IETF RFC 4566 [13].

NOTE: This element is specific for MCPTT.

### 6.2.17 /*<x>*/<x>/Common/MCPTTGroupLevel

Table 6.2.17.1: /*<x>*/<x>/Common/MCPTTGroupLevel

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCPTTGroupLevel | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the level within a group hierarchy (only applicable for group-broadcast group). | | | | |

- Values: 0-255

The group-broadcast group with the lowest MCPTTGroupLevel value shall be considered as the group-broadcast group having the lowest level among the groups.

NOTE: This element is common for all MC services.

### 6.2.18 /*<x>*/<x>/Common/UserLevel

Table 6.2.18.1: /*<x>*/<x>/Common/UserLevel

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/UserLevel | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the level within user hierarchy (only applicable for user-broadcast group). | | | | |

The user-broadcast group with the lowest UserLevel value shall be considered as the user-broadcast group having the lowest level among the groups.

NOTE: This element is common for all MC services.

### 6.2.19 /*<x>*/<x>/Common/AllowedEmergencyCall

Table 6.2.19.1: /*<x>*/<x>/Common/AllowedEmergencyCall

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/AllowedEmergencyCall | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether an MCPTT emergency group call is permitted on the MCS group. | | | | |

When set to "true" the MCPTT emergency group call is allowed on the group.

When set to "false" the MCPTT emergency group call is not allowed on the group.

NOTE: This element is specific for MCPTT.

### 6.2.20 /*<x>*/<x>/Common/AllowedImminentPerilCall

Table 6.2.20.1: /*<x>*/<x>/Common/AllowedImminentPerilCall

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/AllowedImminentPerilCall | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether an MCPTT imminent peril group call is permitted on the MCS group. | | | | |

When set to "true" the MCPTT imminent peril group call is allowed on the group.

When set to "false" the MCPTT imminent peril group call is not allowed on the group.

NOTE: This element is specific for MCPTT.

### 6.2.21 /*<x>*/<x>/Common/AllowedEmergencyAlert

Table 6.2.21.1: /*<x>*/<x>/Common/AllowedEmergencyAlert

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/AllowedEmergencyAlert | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether an MCPTT emergency alert is possible on the MCS group. | | | | |

When set to "true" the MCPTT emergency alert is allowed on the group.

When set to "false" the MCPTT emergency alert is not allowed on the group.

NOTE: This element is for specific for MCPTT.

### 6.2.22 /*<x>*/<x>/Common/MediaProtectionRequired

Table 6.2.22.1: /*<x>*/<x>/Common/MediaProtectionRequired

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MediaProtectionRequired | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether confidentiality and integrity of MCPTT media is required on the MCS group. | | | | |

When set to "true" confidentiality and integrity of media is required on the group.

When set to "false" confidentiality and integrity of media is not required on the group.

The default value is set to "true".

NOTE: This element is specific for MCPTT.

### 6.2.23 /*<x>*/<x>/Common/FloorControlProtectionRequired

Table 6.2.23.1: /*<x>*/<x>/Common/FloorControlProtectionRequired

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/FloorControlProtectionRequired | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether confidentiality and integrity of MCPTT floor control signalling is required on the MCS group. | | | | |

When set to "true" confidentiality and integrity of floor control signalling is requiredon the group.

When set to "false" confidentiality and integrity of floor control signalling is not requiredon the group.

The default value is set to "true".

NOTE: This element is specific for MCPTT.

### 6.2.23A /*<x>*/<x>/Common/MediaProtectionSecurityMaterial

Table 6.2.23A.1: /*<x>*/<x>/Common/MediaProtectionSecurityMaterial

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MediaProtectionSecurityMaterial | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates security material (as specified in 3GPP TS 33.180 [20]) for MCPTTmedia protection in the MCS group. | | | | |

NOTE: This element is specific for MCPTT.

### 6.2.23B /*<x>*/<x>/Common/MCData

Table 6.2.23B.1: /*<x>*/<x>/Common/MCData

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCData | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for a Common MCData group information | | | | |

### 6.2.23C /*<x>*/<x>/Common/MCData/MediaProtectionRequired

Table 6.2.23C.1: /*<x>*/<x>/Common/MCData/MediaProtectionRequired

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCData/MediaProtectionRequired | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether confidentiality and integrity of media is required for MCData transactions on the MCS group. | | | | |

When set to "true" confidentiality and integrity of MCData media is required on the group.

When set to "false" confidentiality and integrity of MCData media is not required on the group.

The default value is set to "true".

### 6.2.23D /*<x>*/<x>/Common/MCData/TxControlProtectionRequired

Table 6.2.23D.1: /*<x>*/<x>/Common/MCData/TxControlProtectionRequired

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCData/TxControlProtectionRequired | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether confidentiality and integrity protection is required for on-network and off-network MCData transmission control signalling on the MCS group | | | | |

When set to "true" confidentiality and integrity of MCData transmission control signalling is required on the group.

When set to "false" confidentiality and integrity of MCData transmission control signalling is not required on the group.

The default value is set to "true".

### 6.2.23E /*<x>*/<x>/Common/MCData/MediaProtectionSecurityMaterial

Table 6.2.23E.1: /*<x>*/<x>/Common/MCData/MediaProtectionSecurityMaterial

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCData/MediaProtectionSecurityMaterial | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates security material (as specified in 3GPP TS 33.180 [xx]) for MCData media protection in the MCS group. | | | | |

### 6.2.23F /*<x>*/<x>/Common/MCData/AllowedSDS

Table 6.2.23F.1: /*<x>*/<x>/Common/MCData/AllowedSDS

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCData/AllowedSDS | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether Short Data Service (SDS) is enabled for the group. | | | | |

When set to "true" the Short Data Service (SDS) is allowed on the group.

When set to "false" the Short Data Service (SDS) is not allowed on the group.

### 6.2.23G /*<x>*/<x>/Common/MCData/AllowedFD

Table 6.2.23G.1: /*<x>*/<x>/Common/MCData/AllowedFD

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCData/AllowedFD | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether File Distribution (FD) is enabled for the group. | | | | |

When set to "true" File Distribution (FD) is allowed on the group.

When set to "false" File Distribution (FD) is not allowed on the group.

### 6.2.23H /*<x>*/<x>/Common/MCData/AllowedConvMgmt

Table 6.2.23H.1: /*<x>*/<x>/Common/MCData/AllowedConvMgmt

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCData/AllowedConvMgmt | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether conversation management is enabled for the group. | | | | |

When set to "true" conversation management is allowed on the group.

When set to "false" conversation management is not allowed on the group.

### 6.2.23I /*<x>*/<x>/Common/MCData/AllowedTxControl

Table 6.2.23I.1: /*<x>*/<x>/Common/MCData/AllowedTxControl

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCData/AllowedTxControl | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether transmission control is enabled for the group. | | | | |

When set to "true" transmission control is allowed on the group.

When set to "false" transmission control is not allowed on the group.

### 6.2.23J /*<x>*/<x>/Common/MCData/AllowedRxControl

Table 6.2.23J.1: /*<x>*/<x>/Common/MCData/AllowedRxControl

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCData/AllowedRxControl | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether reception control is enabled for the group. | | | | |

When set to "true" reception control is allowed on the group.

When set to "false" reception control not allowed on the group.

### 6.2.23K /*<x>*/<x>/Common/MCData/AllowedEnhSvc

Table 6.2.23K.1: /*<x>*/<x>/Common/MCData/AllowedEnhSvc

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCData/AllowedEnhSvc | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether Enhanced Service is enabled for the group. | | | | |

When set to "true" Enhanced Service is allowed on the group.

When set to "false" Enhanced Service is not allowed on the group.

### 6.2.23L /*<x>*/<x>/Common/MCData/EnhSvcOpValues

Table 6.2.23L.1: /*<x>*/<x>/Common/MCData/EnhSvcOpValues

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCData/EnhSvcOpValues | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for a list of operational values for Enhanced Service. | | | | |

### 6.2.23M /*<x>*/<x>/Common/MCData/EnhSvcOpValues/<x>

Table 6.2.23M.1: /*<x>*/<x>/Common/MCData/EnhSvcOpValues/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCData/EnhSvcOpValues/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more list of operational values for Enhanced Service. | | | | |

### 6.2.23N /*<x>*/<x>/Common/MCData/EnhSvcOpValues/<x>/EnhSvcOpValue

Table 6.2.23N.1: /*<x>*/<x>/Common/MCData/EnhSvcOpValues/<x>/EnhSvcOpValue

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCData/EnhSvcOpValues/<x>/EnhSvcOpValue | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates an enhanced service operational value. | | | | |

### 6.2.23NA /*<x>*/<x>/Common/MCData/EnhSvcOpValues/<x>/EnhSvcOpID

Table 6.2.23NA.1: /*<x>*/<x>/Common/MCData/EnhSvcOpValues/<x>/EnhSvcOpID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCData/EnhSvcOpValues/<x>/EnhSvcOpID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | int | Get, Replace |  |
|  | This leaf node indicates a unique id associated with enhanced service operational value. | | | | |

### 6.2.23O /*<x>*/<x>/Common/MCData/AllowedTransmitDataInGroup

Table 6.2.23O.1: /*<x>*/<x>/Common/MCData/AllowedTransmitDataInGroup

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCData/AllowedTransmitDataInGroup | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether an MC data user is permitted to transmit data in the group. | | | | |

When set to "true" an MC data user is allowed to transmit data in the group.

When set to "false" an MC data user is not allowed to transmit data in the group.

### 6.2.23P /<x>/<x>/Common/MCData/MaxDataSingleRequest

Table 6.2.23P.1: /<x>/<x>/Common/MCData/MaxDataSingleRequest

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCData/MaxDataSingleRequest | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the maximum amount of data (in megabytes) that an MCData user can transmit in a single request during group communication. | | | | |

- Values: 0-65535

The MaxData1to1 size is in megabytes.

### 6.2.23Q /<x>/<x>/Common/MCData/MaxTimeSingleRequest

Table 6.2.23Q.1: /<x>/<x>/Common/MCData/MaxTimeSingleRequest

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCData/MaxTimeSingleRequest | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the maximum amount of time that an MCData user can transmit for in a single request during group communication. | | | | |

- Values: 0-65535

The MaxTime1To1 time is in seconds.

### 6.2.23R /*<x>*/<x>/Common/MCVideo

Table 6.2.23R.1: /*<x>*/<x>/Common/MCVideo

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideo | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for a Common MCVideo group information | | | | |

### 6.2.23S /*<x>*/<x>/Common/MCVideo/MediaProtectionRequired

Table 6.2.23S.1: /*<x>*/<x>/Common/MCVideo/MediaProtectionRequired

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideo/MediaProtectionRequired | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether confidentiality and integrity of media is required for MCVideo calls on the MCS group. | | | | |

When set to "true" confidentiality and integrity of MCvideo media is required on the group.

When set to "false" confidentiality and integrity of MCvideo media is not required on the group.

The default value is set to "true".

### 6.2.23T /*<x>*/<x>/Common/MCVideo/TxControlProtectionRequired

Table 6.2.23T.1: /*<x>*/<x>/Common/MCVideo/TxControlProtectionRequired

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideo/TxControlProtectionRequired | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether confidentiality and integrity protection is required for on-network and off-network MCVideo transmission control signalling on the MCS group | | | | |

When set to "true" confidentiality and integrity of MCVideo transmission control signalling is required on the group.

When set to "false" confidentiality and integrity of MCVideo transmission control signalling is not required on the group.

The default value is set to "true".

### 6.2.23U /*<x>*/<x>/Common/MCVideo/MediaProtectionSecurityMaterial

Table 6.2.23U.1: /*<x>*/<x>/Common/MCVideo/MediaProtectionSecurityMaterial

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideo/MediaProtectionSecurityMaterial | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates security material (as specified in 3GPP TS 33.180 [xx]) for MCVideo media protection in the MCS group. | | | | |

### 6.2.23V /*<x>*/<x>/Common/MCVideo/AllowedAudioCodecs

Table 6.2.23V.1: /*<x>*/<x>/Common/MCVideo/AllowedAudioCodecs

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideo/AllowedAudioCodecs | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for a list of allowed audio codecs for MCVideo sessions on the group | | | | |

### 6.2.23W /*<x>*/<x>/Common/MCVideo/AllowedAudioCodecs/<x>

Table 6.2.23W.1: /*<x>*/<x>/Common/MCVideo/AllowedAudioCodecs/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideo/AllowedAudioCodecs/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more list of allowed audio codecs for MCVideo sessions on the group | | | | |

### 6.2.23X /*<x>*/<x>/Common/MCVideo/AllowedAudioCodecs/<x>/ AudioCodec

Table 6.2.23X.1: /*<x>*/<x>/Common/MCVideo/AllowedAudioCodecs/<x>/AudioCodec

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideo/AllowedAudioCodecs/<x>/AudioCodec | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates the preferred RTP payload format to be used for audio encoding in MCVideo group sessions for the group. | | | | |

### 6.2.23Y /*<x>*/<x>/Common/MCVideo/AllowedVideoCodecs

Table 6.2.23Y.1: /*<x>*/<x>/Common/MCVideo/AllowedVideoCodecs

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideo/AllowedVideoCodecs | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for a list of allowed video codecs for MCVideo sessions on the group | | | | |

### 6.2.23Z /*<x>*/<x>/Common/MCVideo/AllowedVideoCodecs/<x>

Table 6.2.23Z.1: /*<x>*/<x>/Common/MCVideo/AllowedVideoCodecs/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideo/AllowedVideoCodecs/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more list of allowed video codecs for MCVideo sessions on the group | | | | |

### 6.2.23AA /*<x>*/<x>/Common/MCVideo/AllowedVideoCodecs/ <x>/VideoCodec

Table 6.2.23AA.1: /*<x>*/<x>/Common/MCVideo/AllowedVideoCodecs/<x>/VideoCodec

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideo/AllowedVideoCodecs/<x>/VideoCodec | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates the preferred RTP payload format to be used for video encoding in MCVideo group sessions for the group. | | | | |

### 6.2.23AB /*<x>*/<x>/Common/MCVideo/AllowedVideoResolutions

Table 6.2.23AB.1: /*<x>*/<x>/Common/MCVideo/AllowedVideoResolutions

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideo/AllowedVideoResolutions | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for a list of allowed video resolutions used in MCVideo group sessions for the group. | | | | |

### 6.2.23AC /*<x>*/<x>/Common/MCVideo/AllowedVideoResolutions/<x>

Table 6.2.23AC.1: /*<x>*/<x>/Common/MCVideo/AllowedVideoResolutions/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideo/AllowedVideoResolutions/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more list of allowed video resolutions used in MCVideo group sessions for the group. | | | | |

### 6.2.23AD /*<x>*/<x>/Common/MCVideo/AllowedVideoResolutions/ <x>/VideoResolution

Table 6.2.23AD.1: /*<x>*/<x>/Common/MCVideo/AllowedVideoResolutions/<x>/VideoResolution

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideo/AllowedVideoResolutions/<x>/VideoResolution | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates a video resolution (number of horizontal pixels x number of vertical pixels) to be used in MCVideo group sessions for the group. | | | | |

### 6.2.23AE /*<x>*/<x>/Common/MCVideo/AllowedVideoFrameRates

Table 6.2.23AE.1: /*<x>*/<x>/Common/MCVideo/AllowedVideoFrameRates

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideo/AllowedVideoFrameRates | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for a list of allowed video frame rates to be used in MCVideo group sessions for the group. | | | | |

### 6.2.23AF /*<x>*/<x>/Common/MCVideo/AllowedVideoFrameRates/<x>

Table 6.2.23AF.1: /*<x>*/<x>/Common/MCVideo/AllowedVideoFrameRates/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideo/AllowedVideoFrameRates/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more list of allowed video frame rates to be used in MCVideo group sessions for the group. | | | | |

### 6.2.23AG /*<x>*/<x>/Common/MCVideo/AllowedVideoFrameRates/ <x>/FrameRate

Table 6.2.23AG.1: /*<x>*/<x>/Common/MCVideo/AllowedVideoFrameRates/<x>/FrameRate

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideo/AllowedVideoFrameRates/<x>/FrameRate | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | int | Get, Replace |  |
|  | This leaf node indicates a video frame rate (in frames per second) to be used in MCVideo group sessions for the group. | | | | |

### 6.2.23AH /*<x>*/<x>/Common/MCVideo/AllowedUrgentRealTimeMode

Table 6.2.23AH.1: /*<x>*/<x>/Common/MCVideo/AllowedUrgentRealTimeMode

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideo/AllowedUrgentRealTimeMode | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether urgent real time mode is allowed for MCVideo sessions on the group. | | | | |

When set to "true" urgent real-time video mode is allowed for MCVideo sessions on the group.

When set to "false" urgent real-time video mode is not allowed for MCVideo sessions on the group.

### 6.2.23AI /*<x>*/<x>/Common/MCVideo/AllowedNonUrgentRealTimeMode

Table 6.2.23AI.1: /*<x>*/<x>/Common/MCVideo/AllowedNonUrgentRealTimeMode

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideo/AllowedNonUrgentRealTimeMode | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether non-urgent real time mode is allowed for MCVideo sessions on the group. | | | | |

When set to "true" non-urgent real-time video mode is allowed for MCVideo sessions on the group.

When set to "false" non-urgent real-time video mode is not allowed for MCVideo sessions on the group.

### 6.2.23AJ /*<x>*/<x>/Common/MCVideo/AllowedNonRealTimeMode

Table 6.2.23AJ.1: /*<x>*/<x>/Common/MCVideo/AllowedNonRealTimeMode

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideo/AllowedNonRealTimeMode | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether non-real time mode is allowed for MCVideo sessions on the group. | | | | |

When set to "true" non-real-time video mode is allowed for MCVideo sessions on the group.

When set to "false" non-real-time video mode is not allowed for MCVideo sessions on the group.

### 6.2.23AK /*<x>*/<x>/Common/MCVideo/ActiveNonRealTimeMode

Table 6.2.23AK.1: /*<x>*/<x>/Common/MCVideo/ActiveNonRealTimeMode

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideo/ActiveNonRealTimeMode | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the active non-real-time mode used for MCVideo sessions on the group. | | | | |

The valid values are:

a) "urgent-real-time";

b) "non-urgent-real-time"; and

c) "non-real-time".

### 6.2.23AL /<x>/<x>/Common/MCVideo/MaxTransmitMembers

Table 6.2.23AL.1: /<x>/<x>/Common/MCVideo/MaxTransmitMembers

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideo/MaxTransmitMembers | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the maximum number of simultaneous transmitting group members for MCVideo sessions on the group. | | | | |

- Values: 0-65535

### 6.2.24 /*<x>*/<x>/OffNetwork

Table 6.2.24.1: /*<x>*/<x>/OffNetwork

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | node | Get, Replace |  |
|  | This interior node represents a container for off-network operation. | | | | |

### 6.2.25 /*<x>*/<x>/OffNetwork/MCPTTGroupParameter

Table 6.2.25.1: /*<x>*/<x>/OffNetwork/MCPTTGroupParameter

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCPTTGroupParameter | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the group parameters. | | | | |

### 6.2.26 /*<x>*/<x>/OffNetwork/MCPTTGroupParameter/<x>

Table 6.2.26.1: /*<x>*/<x>/OffNetwork/MCPTTGroupParameter/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCPTTGroupParameter/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more group parameters. | | | | |

### 6.2.27 /*<x>*/<x>/OffNetwork/MCPTTGroupParameter/<x>/ ProSeLayer2GroupID

Table 6.2.27.1: /*<x>*/<x>/OffNetwork/MCPTTGroupParameter/<x>/ProSeLayer2GroupID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCPTTGroupParameter/<x>/ProSeLayer2GroupID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the Prose layer-2 group ID as specified in 3GPP TS 23.303 [6]. | | | | |

NOTE: This element is common for all MC services.

### 6.2.28 /*<x>*/<x>/OffNetwork/MCPTTGroupParameter/<x>/ IPMulticastAddress

Table 6.2.28.1: /*<x>*/<x>/OffNetwork/MCPTTGroupParameter/<x>/IPMulticastAddress

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCPTTGroupParameter/<x>/IPMulticastAddress | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the ProSe group IP multicast address as specified in 3GPP TS 23.303 [6]. | | | | |

The value is an IPv4 address or an IPv6 address.

NOTE: This element is common for all MC services.

### 6.2.29 /*<x>*/<x>/OffNetwork/MCPTTGroupParameter/<x>/ RelayServiceCode

Table 6.2.29.1: /*<x>*/<x>/OffNetwork/MCPTTGroupParameter/<x>/RelayServiceCode

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCPTTGroupParameter/<x>/RelayServiceCode | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the connectivity service that the ProSe UE-to-network relay provides to public safety applications as specified in 3GPP TS 23.303 [6]. | | | | |

NOTE: This element is common for all MC services.

### 6.2.30 /*<x>*/<x>/OffNetwork/MCPTTGroupParameter/<x>/IPVersions

Table 6.2.30.1: /*<x>*/<x>/OffNetwork/MCPTTGroupParameter/<x>/IPVersions

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCPTTGroupParameter/<x>/IPVersions | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates whether IPv4 or IPv6 is used for the MCS group as specified in 3GPP TS 23.303 [6]. | | | | |

The value is "IPv4" or "IPv6".

NOTE: This element is common for all MC services.

### 6.2.31 /*<x>*/<x>/OffNetwork/EmergencyCallCancel

Table 6.2.31.1: /*<x>*/<x>/OffNetwork/EmergencyCallCancel

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/EmergencyCallCancel | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the timeout value for the cancellation of an in progress emergency group call for MCPTT. | | | | |

- Values: 0-65535

The EmergencyCallCancel time is in seconds.

NOTE: This element is specific for MCPTT.

### 6.2.32 /*<x>*/<x>/OffNetwork/ImminentPerilCallCancel

Table 6.2.32.1: /*<x>*/<x>/OffNetwork/ImminentPerilCallCancel

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/ImminentPerilCallCancel | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the timeout value for the cancellation of an in progress MCPTT imminent peril group call. | | | | |

- Values: 0-65535

The ImminentPerilCallCancel time is in seconds.

NOTE: This element is specific for MCPTT.

### 6.2.33 /*<x>*/<x>/OffNetwork/HangTime

Table 6.2.33.1: /*<x>*/<x>/OffNetwork/HangTime

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/HangTime | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the group call hang timer. | | | | |

- Values: 0-65535

The HangTime is in seconds.

NOTE: This element is specific for MCPTT.

### 6.2.34 /*<x>*/<x>/OffNetwork/MaxDuration

Table 6.2.34.1: /*<x>*/<x>/OffNetwork/MaxDuration

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MaxDuration | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the max duration of group calls. | | | | |

- Values: 0-65535

The MaxDuration time is in seconds.

NOTE: This element is specific for MCPTT.

### 6.2.34A /*<x>*/<x>/OffNetwork/QueueUsage

Table 6.2.34A.1: /<x>/<x>/OffNetwork/QueueUsage

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/QueueUsage | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates if queuing is enabled or not. | | | | |

When set to "true" queueing floor requests is enabled on the group.

When set to "false" queueing floor requests is not enabled on the group.

The default value is set to "true".

NOTE: This element is specific for MCPTT.

### 6.2.35 /*<x>*/<x>/OffNetwork/DefaultPPPP

Table 6.2.35.1: /*<x>*/<x>/OffNetwork/DefaultPPPP

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/DefaultPPPP | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the default ProSe Per-Packet Priority (PPPP) configuration. | | | | |

### 6.2.36 /*<x>*/<x>/OffNetwork/DefaultPPPP/MCPTTGroupCallSignalling

Table 6.2.36.1: /*<x>*/<x>/OffNetwork/DefaultPPPP/MCPTTGroupCallSignalling

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/DefaultPPPP/MCPTTGroupCallSignalling | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the default ProSe Per-Packet Priority (PPPP) value (as specified in 3GPP TS 23.303 [6]) for the group call signalling for MCPTT. | | | | |

- Values: 1-8

The MCPTT user data with the lowest ProSe Per-Packet Priority value shall be considered as the MCPTT user data having the highest priority among the MCPTT user data.

NOTE: This element is specific for MCPTT.

### 6.2.37 /*<x>*/<x>/OffNetwork/DefaultPPPP/MCPTTGroupCallMedia

Table 6.2.37.1: /*<x>*/<x>/OffNetwork/DefaultPPPP/MCPTTGroupCallMedia

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/DefaultPPPP/MCPTTGroupCallMedia | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the default ProSe Per-Packet Priority (PPPP) value (as specified in 3GPP TS 23.303 [6]) for the group call media for MCPTT. | | | | |

- Values: 1-8

The MCPTT user data with the lowest ProSe Per-Packet Priority value shall be considered as the MCPTT user data having the highest priority among the MCPTT user data.

NOTE: This element is specific for MCPTT.

### 6.2.38 /*<x>*/<x>/OffNetwork/DefaultPPPP/ MCPTTEmergencyGroupCallSignalling

Table 6.2.38.1: /*<x>*/<x>/OffNetwork/DefaultPPPP/MCPTTEmergencyGroupCallSignalling

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/DefaultPPPP/MCPTTEmergencyGroupCallSignalling | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the default ProSe Per-Packet Priority (PPPP) value (as specified in 3GPP TS 23.303 [6]) for the MCPTT emerency group call signalling. | | | | |

- Values: 1-8

The MCPTT user data with the lowest ProSe Per-Packet Priority value shall be considered as the MCPTT user data having the highest priority among the MCPTT user data.

NOTE: This element is specific for MCPTT.

### 6.2.39 /*<x>*/<x>/OffNetwork/DefaultPPPP/ MCPTTEmergencyGroupCallMedia

Table 6.2.39.1: /*<x>*/<x>/OffNetwork/DefaultPPPP/MCPTTEmergencyGroupCallMedia

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/DefaultPPPP/MCPTTEmergencyGroupCallMedia | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the default ProSe Per-Packet Priority (PPPP) value (as specified in 3GPP TS 23.303 [6]) for the MCPTT emerency group call media. | | | | |

- Values: 1-8

The MCPTT user data with the lowest ProSe Per-Packet Priority value shall be considered as the MCPTT user data having the highest priority among the MCPTT user data.

NOTE: This element is specific for MCPTT.

### 6.2.40 /*<x>*/<x>/OffNetwork/DefaultPPPP/ MCPTTImminentPerilGroupCallSignalling

Table 6.2.40.1: /*<x>*/<x>/OffNetwork/DefaultPPPP/MCPTTImminentPerilGroupCallSignalling

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/DefaultPPPP/MCPTTImminentPerilGroupCallSignalling | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the default ProSe Per-Packet Priority (PPPP) value (as specified in 3GPP TS 23.303 [6]) for the MCPTT imminent peril group call signalling. | | | | |

- Values: 1-8

The MCPTT user data with the lowest ProSe Per-Packet Priority value shall be considered as the MCPTT user data having the highest priority among the MCPTT user data.

NOTE: This element is specific for MCPTT.

### 6.2.41 /*<x>*/<x>/OffNetwork/DefaultPPPP/ MCPTTImminentPerilGroupCallMedia

Table 6.2.41.1: /*<x>*/<x>/OffNetwork/DefaultPPPP/MCPTTImminentPerilGroupCallMedia

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/DefaultPPPP/MCPTTImminentPerilGroupCallMedia | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the default ProSe Per-Packet Priority (PPPP) value (as specified in 3GPP TS 23.303 [6]) for the MCPTT imminent peril group call media. | | | | |

- Values: 1-8

The MCPTT user data with the lowest ProSe Per-Packet Priority value shall be considered as the MCPTT user data having the highest priority among the MCPTT user data.

NOTE: This element is specific for MCPTT.

### 6.2.42 /*<x>*/<x>/OffNetwork/MCData

Table 6.2.42.1: /*<x>*/<x>/OffNetwork/MCData

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCData | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for off-network MCData configuration. | | | | |

### 6.2.43 /*<x>*/<x>/OffNetwork/MCData/DefaultPPPP

Table 6.2.43.1: /*<x>*/<x>/OffNetwork/MCData/DefaultPPPP

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCData/DefaultPPPP | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the default ProSe Per-Packet Priority (PPPP) configuration. | | | | |

### 6.2.44 /*<x>*/<x>/OffNetwork/MCData/DefaultPPPP/ MCDataGroupCallSignalling

Table 6.2.44.1: /*<x>*/<x>/OffNetwork/MCData/DefaultPPPP/MCDataGroupCallSignalling

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCData/DefaultPPPP/MCDataGroupCallSignalling | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the default ProSe Per-Packet Priority (PPPP) value (as specified in 3GPP TS 23.303 [6]) for the group call signalling for MCData. | | | | |

- Values: 1-8

The MCData user data with the lowest ProSe Per-Packet Priority value shall be considered as the MCData user data having the highest priority among the MCData user data.

### 6.2.45 /*<x>*/<x>/OffNetwork/MCData/DefaultPPPP/ MCDataGroupCallMedia

Table 6.2.45.1: /*<x>*/<x>/OffNetwork/MCData/DefaultPPPP/MCDataGroupCallMedia

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCData/DefaultPPPP/MCDataGroupCallMedia | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the default ProSe Per-Packet Priority (PPPP) value (as specified in 3GPP TS 23.303 [6]) for the group call media for MCData. | | | | |

- Values: 1-8

The MCData user data with the lowest ProSe Per-Packet Priority value shall be considered as the MCData user data having the highest priority among the MCData user data.

### 6.2.46 /*<x>*/<x>/OffNetwork/MCVideo

Table 6.2.46.1: /*<x>*/<x>/OffNetwork/MCVideo

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCVideo | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for off-network MCVideo group configuration. | | | | |

### 6.2.47 /*<x>*/<x>/OffNetwork/MCVideo/ArbitrationApproach

Table 6.2.47.1: /*<x>*/<x>/OffNetwork/MCVideo/ArbitrationApproach

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCVideo/ArbitrationApproach | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the arbitration approach used for off-network video tranmissions on the group | | | | |

The valid values are:

a) "single" which indicates transmission participants rely on a single participant designated as transmission arbitrator for the arbitration of transmission requests; and

b) "self" which indicates each transmission participant arbitrates its own transmission based on its view of the topology.

### 6.2.48 /<x>/<x>/OffNetwork/MCVideo/MaxTransmissions

Table 6.2.48.1: /<x>/<x>/OffNetwork/MCVideo/MaxTransmissions

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCVideo/MaxTransmissions | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates maximum number of simultaneous transmissions for off-network MCVideo procedures. | | | | |

- Values: 0-65535

### 6.2.49 /*<x>*/<x>/OffNetwork/MCVideo/DefaultPPPP

Table 6.2.49.1: /*<x>*/<x>/OffNetwork/MCVideo/DefaultPPPP

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCVideo/DefaultPPPP | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the default ProSe Per-Packet Priority (PPPP) configuration. | | | | |

### 6.2.50 /*<x>*/<x>/OffNetwork/MCVideo/DefaultPPPP/ MCVideoGroupCallSignalling

Table 6.2.50.1: /*<x>*/<x>/OffNetwork/MCVideo/DefaultPPPP/MCVideoGroupCallSignalling

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCVideo/DefaultPPPP/MCVideoGroupCallSignalling | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the default ProSe Per-Packet Priority (PPPP) value (as specified in 3GPP TS 23.303 [6]) for the group call signalling for MCVideo. | | | | |

- Values: 1-8

The MCVideo user data with the lowest ProSe Per-Packet Priority value shall be considered as the MCVideo user data having the highest priority among the MCVideo user data.

### 6.2.51 /*<x>*/<x>/OffNetwork/MCVideo/DefaultPPPP/ MCVideoGroupCallMedia

Table 6.2.51.1: /*<x>*/<x>/OffNetwork/MCVideo/DefaultPPPP/MCVideoGroupCallMedia

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCVideo/DefaultPPPP/MCVideoGroupCallMedia | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the default ProSe Per-Packet Priority (PPPP) value (as specified in 3GPP TS 23.303 [6]) for the group call media for MCVideo. | | | | |

- Values: 1-8

The MCVideo user data with the lowest ProSe Per-Packet Priority value shall be considered as the MCVideo user data having the highest priority among the MCVideo user data.

### 6.2.52 /*<x>*/<x>/OffNetwork/MCVideo/DefaultPPPP/ MCVideoEmergencyGroupCallSignalling

Table 6.2.52.1: /*<x>*/<x>/OffNetwork/MCVideo/DefaultPPPP/MCVideoEmergencyGroupCallSignalling

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCVideo/DefaultPPPP/MCVideoEmergencyGroupCallSignalling | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the default ProSe Per-Packet Priority (PPPP) value (as specified in 3GPP TS 23.303 [6]) for the MCVideo emerency group call signalling. | | | | |

- Values: 1-8

The MCVideo user data with the lowest ProSe Per-Packet Priority value shall be considered as the MCVideo user data having the highest priority among the MCVideo user data.

### 6.2.53 /*<x>*/<x>/OffNetwork/MCVideo/DefaultPPPP/ MCVideoEmergencyGroupCallMedia

Table 6.2.53.1: /*<x>*/<x>/OffNetwork/MCVideo/DefaultPPPP/MCVideoEmergencyGroupCallMedia

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCVideo/DefaultPPPP/MCVideoEmergencyGroupCallMedia | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the default ProSe Per-Packet Priority (PPPP) value (as specified in 3GPP TS 23.303 [6]) for the MCVideo emerency group call media. | | | | |

- Values: 1-8

The MCVideo user data with the lowest ProSe Per-Packet Priority value shall be considered as the MCVideo user data having the highest priority among the MCVideo user data.

### 6.2.54 /*<x>*/<x>/OffNetwork/MCVideo/DefaultPPPP/ MCVideoImminentPerilGroupCallSignalling

Table 6.2.54.1: /*<x>*/<x>/OffNetwork/MCVideo/DefaultPPPP/MCVideoImminentPerilGroupCallSignalling

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCVideo/DefaultPPPP/MCVideoImminentPerilGroupCallSignalling | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the default ProSe Per-Packet Priority (PPPP) value (as specified in 3GPP TS 23.303 [6]) for the MCVideo imminent peril group call signalling. | | | | |

- Values: 1-8

The MCVideo user data with the lowest ProSe Per-Packet Priority value shall be considered as the MCVideo user data having the highest priority among the MCVideo user data.

### 6.2.55 /*<x>*/<x>/OffNetwork/MCVideo/DefaultPPPP/ MCVideoImminentPerilGroupCallMedia

Table 6.2.55.1: /*<x>*/<x>/OffNetwork/MCVideo/DefaultPPPP/MCVideoImminentPerilGroupCallMedia

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCVideo/DefaultPPPP/MCVideoImminentPerilGroupCallMedia | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the default ProSe Per-Packet Priority (PPPP) value (as specified in 3GPP TS 23.303 [6]) for the MCVideo imminent peril group call media. | | | | |

- Values: 1-8

The MCVideo user data with the lowest ProSe Per-Packet Priority value shall be considered as the MCVideo user data having the highest priority among the MCVideo user data.

### 6.2.56 /*<x>*/<x>/OffNetwork/MCVideo/MaxDuration

Table 6.2.56.1: /*<x>*/<x>/OffNetwork/MCVideo/MaxDuration

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCVideo/MaxDuration | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the max duration of MCVideo group calls. | | | | |

- Values: 0-65535

The MaxDuration time is in seconds.

### 6.2.57 /*<x>*/<x>/OffNetwork/MCVideo/EmergencyCallCancel

Table 6.2.57.1: /*<x>*/<x>/OffNetwork/MCVideo/EmergencyCallCancel

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/EmergencyCallCancel | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the timeout value for the cancellation of an in progress MCVideo emergency group call for MCVideo. | | | | |

- Values: 0-65535

The EmergencyCallCancel time is in seconds.

### 6.2.58 /*<x>*/<x>/OffNetwork/MCVideo/ImminentPerilCallCancel

Table 6.2.58.1: /*<x>*/<x>/OffNetwork/MCVideo/ImminentPerilCallCancel

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/ImminentPerilCallCancel | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the timeout value for the cancellation of an in progress MCVideo imminent peril group call. | | | | |

- Values: 0-65535

The ImminentPerilCallCancel time is in seconds.

# 7 MCPTT service configuration MO

## 7.1 General

The MCPTT service configuration Management Object (MO) is used to configure MCPTT Client behaviour for the on-network or off-network MCPTT Service. The MCPTT service configuration parameters may be stored in the ME, or in the USIM as specified in 3GPP TS 31.102 [10], or in both the ME and the USIM. If both the ME and the USIM contain the same parameters, the values stored in the USIM shall take precedence.

The Management Object Identifier is: urn:oma:mo:ext-3gpp-MCPTT-service-configuration:1.0.

Protocol compatibility: This MO is compatible with OMA OMA DM 1.2 [3].

The OMA DM ACL property mechanism (see OMA OMA-ERELD-DM-V1\_2 [2]) may be used to grant or deny access rights to OMA DM servers in order to modify nodes and leaf objects of the MCPTT service configuration MO.

The following nodes and leaf objects are possible under the MCPTT service configuration node as described in figure 7.1.1.



Figure 7.1.1: The MCPTT service configuration MO

## 7.2 MCPTT service configuration MO parameters

### 7.2.1 General

This clause describes the parameters for the MCPTT service configuration Management Object (MO).

### 7.2.2 Node: *<x>*

Table 7.2.2.1: Node: *<x>*

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get |  |
|  | This interior node acts as a placeholder for the MCPTT service configuration Management Object (MO).  For the MCPTT service configuration MO, the namespace specific string is: "urn:oma:mo:oma-dm-mcptt-service configuration:1.0" | | | | |

- Values: N/A

### 7.2.3 /*<x>*/Name

Table 7.2.3.1: /*<x>*/Name

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | chr | Get |  |
|  | The Name leaf is a name for the MCPTT service configuration settings. | | | | |

- Values: <User displayable name>

### 7.2.4 /*<x>*/Ext/

Table 7.2.4.1: /*<x>*/Ext/

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Ext | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | The Ext is an interior node for where the vendor specific information about the MCPTT service configuration MO is being placed. | | | | |

Usually the vendor extension is identified by vendor specific name under the ext node and contains the vendor meaning application vendor, device vendor etc. The tree structure under the vendor identified is not defined and can therefore include one or more un-standardized sub-trees.

- Values: N/A

### 7.2.5 /*<x>*/Common

Table 7.2.5.1: /*<x>*/Common

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | node | Get, Replace |  |
|  | This interior node represents a container for the common network operation which means both on-network operation and off-network operation. | | | | |

### 7.2.6 /*<x>*/Common/BroadcastMCPTTGroupCall

Table 7.2.6.1: /*<x>*/Common/BroadcastMCPTTGroupCall

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/BroadcastMCPTTGroupCall | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for Broadcast MCPTT Group Call configuration. | | | | |

### 7.2.7 /*<x>*/Common/BroadcastMCPTTGroupCall/ NumLevelGroupHierarchy

Table 7.2.7.1: /*<x>*/Common/BroadcastMCPTTGroupCall/NumLevelGroupHierarchy

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/BroadcastMCPTTGroupCall/NumLevelGroupHierarchy | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the number of levels of group hierarchy for group-broadcast groups. | | | | |

- Values: 0-255

The group-broadcast group with the lowest NumLevelGroupHierarchy value shall be considered as the group-broadcast group having the lowest level among the groups.

### 7.2.8 /*<x>*/Common/BroadcastMCPTTGroupCall/ NumLevelUserHierarchy

Table 7.2.8.1: /*<x>*/Common/BroadcastMCPTTGroupCall/NumLevelUserHierarchy

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/BroadcastMCPTTGroupCall/NumLevelUserHierarchy | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the number of levels of user hierarchy for user-broadcast groups. | | | | |

- Values: 0-255

The user-broadcast group with the lowest NumLevelUserHierarchy value shall be considered as the user-broadcast group the lowest level among the groups.

### 7.2.9 /*<x>*/Common/MinLengthAliasID

Table 7.2.9.1: /*<x>*/Common/MinLengthAliasID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MinLengthAliasID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates minimum length of an alphanumeric identifier (i.e., alias) assigned by an MCPTT administrator. | | | | |

- Values: 0-255

### 7.2.10 /*<x>*/OffNetwork

Table 7.2.10.1: /*<x>*/OffNetwork

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | node | Get, Replace |  |
|  | This interior node represents a container for off-network operation. | | | | |

### 7.2.11 /*<x>*/OffNetwork/PrivateCall

Table 7.2.11.1: /*<x>*/OffNetwork/PrivateCall

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/PrivateCall | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for private call configuration. | | | | |

### 7.2.12 /*<x>*/OffNetwork/PrivateCall/MaxDuration

Table 7.2.12.1: /*<x>*/OffNetwork/PrivateCall/MaxDuration

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/PrivateCall/MaxDuration | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates max private call (with floor control) duration. | | | | |

- Values: 0-65535

The MaxDuration time is in seconds.

### 7.2.13 /*<x>*/OffNetwork/PrivateCall/HangTime

Table 7.2.13.1: /*<x>*/OffNetwork/PrivateCall/HangTime

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/PrivateCall/HangTime | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates hang timer for private calls (with floor control). | | | | |

- Values: 0-65535

The HangTime is in seconds.

### 7.2.14 /*<x>*/OffNetwork/PrivateCall/CancelTimeout

Table 7.2.14.1: /*<x>*/OffNetwork/PrivateCall/CancelTimeout

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/PrivateCall/CancelTimeout | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates timeout value for the cancellation of an in progress emergency for an MCPTT private call. | | | | |

- Values: 0-65535

The CancelTimeout is in seconds.

### 7.2.15 /*<x>*/OffNetwork/EmergencyCall

Table 7.2.15.1: /*<x>*/OffNetwork/EmergencyCall

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/EmergencyCall | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node indicates a placeholder for the MCPTT emergency call policy. | | | | |

### 7.2.16 /*<x>*/OffNetwork/EmergencyCall/MCPTTGroupTimeout

Table 7.2.16.1: /*<x>*/OffNetwork/EmergencyCall/MCPTTGroupTimeout

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/EmergencyCall/MCPTTGroupTimeout | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates time limit for an in progress MCPTT emergency call related to an MCPTT group. | | | | |

- Values: 0-65535

The GroupTimeout is in seconds.

### 7.2.17 /*<x>*/OffNetwork/NumLevelHierarchy

Table 7.2.17.1: /*<x>*/OffNetwork/NumLevelHierarchy

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/NumLevelHierarchy | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the number of levels of hierarchy for floor control override in off-network. | | | | |

- Values: 4-256

The request with the lowest NumLevelHierarchy value shall be considered as the request having the lowest priority level given to override an active transmission among the requests.

### 7.2.18 /*<x>*/OffNetwork/TransmitTimeout

Table 7.2.18.1: /*<x>*/OffNetwork/TransmitTimeout

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/TransmitTimeout | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates transmit time limit from a single request to transmit in a group or private call. | | | | |

- Values: 0-65535

The TransmitTimeout is in seconds.

### 7.2.19 /*<x>*/OffNetwork/TransmissionWarning

Table 7.2.19.1: /*<x>*/OffNetwork/TransmissionWarning

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/TransmissionWarning | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates configuration of warning time before time limit of transmission is reached (off-network). | | | | |

- Values: 0-255

The TransmissionWarning time is in seconds.

### 7.2.20 /*<x>*/OffNetwork/HangTimeWarning

Table 7.2.20.1: /*<x>*/OffNetwork/HangTimeWarning

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/HangTimeWarning | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates configuration of warning time before hang time is reached (off-network). | | | | |

- Values: 0-255

The HangTimeWarning time is in seconds.

### 7.2.21 /*<x>*/OffNetwork/DefaultPPPP

Table 7.2.21.1: /*<x>*/OffNetwork/DefaultPPPP

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/DefaultPPPP | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the default ProSe Per-Packet Priority (PPPP) configuration. | | | | |

### 7.2.22 /*<x>*/OffNetwork/DefaultPPPP/MCPTTPrivateCallSignalling

Table 7.2.22.1: /*<x>*/OffNetwork/DefaultPPPP/MCPTTPrivateCallSignalling

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/DefaultPPPP/MCPTTPrivateCallSignalling | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the default ProSe Per-Packet Priority (PPPP) value (as specified in 3GPP TS 23.303 [6]) for the MCPTT private call signalling. | | | | |

- Values: 1-8

The MCPTT user data with the lowest ProSe Per-Packet Priority value shall be considered as the MCPTT user data having the highest priority among the MCPTT user data.

### 7.2.23 /*<x>*/OffNetwork/DefaultPPPP/MCPTTPrivateCallMedia

Table 7.2.23.1: /*<x>*/OffNetwork/DefaultPPPP/MCPTTPrivateCallMedia

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/DefaultPPPP/MCPTTPrivateCallMedia | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the default ProSe Per-Packet Priority (PPPP) value (as specified in 3GPP TS 23.303 [6]) for the MCPTT private call media. | | | | |

- Values: 1-8

The MCPTT user data with the lowest ProSe Per-Packet Priority value shall be considered as the MCPTT user data having the highest priority among the MCPTT user data.

### 7.2.24 /*<x>*/OffNetwork/DefaultPPPP/ MCPTTEmergencyPrivateCallSignalling

Table 7.2.24.1: /*<x>*/OffNetwork/DefaultPPPP/MCPTTEmergencyPrivateCallSignalling

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/DefaultPPPP/MCPTTEmergencyPrivateCallSignalling | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the default ProSe Per-Packet Priority (PPPP) value (as specified in 3GPP TS 23.303 [6]) for the MCPTT emerency private call signalling. | | | | |

- Values: 1-8

The MCPTT user data with the lowest ProSe Per-Packet Priority value shall be considered as the MCPTT user data having the highest priority among the MCPTT user data.

### 7.2.25 /*<x>*/OffNetwork/DefaultPPPP/ MCPTTEmergencyPrivateCallMedia

Table 7.2.25.1: /*<x>*/OffNetwork/DefaultPPPP/MCPTTEmergencyPrivateCallMedia

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/DefaultPPPP/MCPTTEmergencyPrivateCallMedia | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the default ProSe Per-Packet Priority (PPPP) value (as specified in 3GPP TS 23.303 [6]) for the MCPTT emerency private call media. | | | | |

- Values: 1-8

The MCPTT user data with the lowest ProSe Per-Packet Priority value shall be considered as the MCPTT user data having the highest priority among the MCPTT user data.

### 7.2.26 /*<x>*/OffNetwork/LogMetadata

Table 7.2.26.1: /*<x>*/OffNetwork/LogMetadata

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/LogMetadata | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether logging of metadata for MCPTT group calls, MCPTT private calls and non-call activities is permitted. | | | | |

When set to "true" logging of metadata for MCPTT group calls, MCPTT private calls and non-call activities, is enabled.

When set to "false" logging of metadata for MCPTT group calls, MCPTT private calls and non-call activities, is not enabled.

# 8 MCS UE initial configuration MO

## 8.1 General

The MCS UE initial configuration Management Object (MO) is used to configure the MCS Client behaviour for the on-network or off-network MCS Service. The MCS UE initial configuration parameters may be stored in the ME, or in the USIM as specified in 3GPP TS 31.102 [10], or in both the ME and the USIM. If both the ME and the USIM contain the same parameters, the values stored in the USIM shall take precedence.

NOTE: For historical reasons some of the elements in the MCS UE initial MO uses the terminology "MCPTT", however this MO is common to all MCS with some MCPTT specific elements, some MCData specific elements and some MCVideo specific elements. Not all elements that contain the terminology "MCPTT" are just MCPTT specific.

The Management Object Identifier is: urn:oma:mo:ext-3gpp-MCPTT-UE-initial-configuration:1.0.

Protocol compatibility: This MO is compatible with OMA OMA DM 1.2 [3].

The OMA DM ACL property mechanism (see OMA OMA-ERELD-DM-V1\_2 [2]) may be used to grant or deny access rights to OMA DM servers in order to modify nodes and leaf objects of the MCPTT user profile MO.

The following nodes and leaf objects are possible under the MCPTT node as described in figure 8.1.1, figure 8.1.2, figure 8.1.3 and figure 8.1.4.



Figure 8.1.1: The MCS UE initial configuration MO (1 of 5)



Figure 8.1.2: The MCS UE initial configuration MO (2 of 5)



Figure 8.1.3: The MCS UE initial configuration MO (3 of 5)



Figure 8.1.4: The MCS UE initial configuration MO (4 of 5)



Figure 8.1.5: The MCS UE initial configuration MO (5 of 5)

## 8.2 MCS UE initial configuration MO parameters

### 8.2.1 General

This clause describes the parameters for the MCS UE initial configuration Management Object (MO).

### 8.2.2 Node: *<x>*

Table 8.2.2.1: Node: *<x>*

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get |  |
|  | This interior node acts as a placeholder for the MCS UE initial configuration Management Object (MO).  For the MCS UE initial configuration MO, the namespace specific string is: "urn:oma:mo:oma-dm-mcptt-ue-initial-configuration:1.0" | | | | |

- Values: N/A

### 8.2.3 /*<x>*/Name

Table 8.2.3.1: /*<x>*/Name

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | chr | Get |  |
|  | The Name leaf is a name for the MCPTT UE initial configuration settings. | | | | |

- Values: <User displayable name>

### 8.2.4 /*<x>*/Ext/

Table 8.2.4.1: /*<x>*/Ext/

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Ext | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | The Ext is an interior node for where the vendor specific information about the MCPTT UE initial configuration MO is being placed. | | | | |

Usually the vendor extension is identified by vendor specific name under the ext node and contains the vendor meaning application vendor, device vendor etc. The tree structure under the vendor identified is not defined and can therefore include one or more un-standardized sub-trees.

- Values: N/A

### 8.2.5 /*<x>*/DefaultUserProfile

Table 8.2.5.1: /*<x>*/Ext/DefaultUserProfile

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| DefaultUserProfile | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | node | Get, Replace |  |
|  | This interior node represents a container for the default user profile. | | | | |

The DefaultUserProfile nodes are:

- the same MCPTT user profile nodes defined in MCPTT user profile MO with a default MCPTT user ID;

- the same MCData user profile nodes defined in MCData user profile MO with a default MCData user ID; or

- the same MCVideo user profile nodes defined in MCVideo user profile MO with a default MCVideo user ID.

### 8.2.6 /*<x>*/DefaultUserProfile/UserID

Table 8.2.6.1: /*<x>*/Ext/DefaultUserProfile/UserID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| DefaultUserProfile/UserID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates a default MCS user identity. | | | | |

### 8.2.7 /*<x>*/DefaultUserProfile/UserProfileIndex

Table 8.2.7.1: /*<x>*/Ext/DefaultUserProfile/UserProfileIndex

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| DefaultUserProfile/UserProfileIndex | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node represents an indicator for the particular user profile. | | | | |

- Values: 0-255

### 8.2.8 /*<x>*/OnNetwork

Table 8.2.8.1: /<x>/OnNetwork

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | node | Get, Replace |  |
|  | This interior node represents a container for on-network operation. | | | | |

### 8.2.9 /*<x>*/OnNetwork/GMSURI

Table 8.2.9.1: <x>/OnNetwork/GMSURI

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/GMSURI | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the group management service URI information which contains the public service identity for performing subscription proxy function of the GMS. | | | | |

The value is a URI as specified in 3GPP TS 23.003 [5].

### 8.2.9A /*<x>*/OnNetwork/GroupCreationXUI

Table 8.2.9A.1: <x>/OnNetwork/GroupCreationXUI

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/GroupCreationXUI | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the group creation XUI information for creation of groups. | | | | |

The value is a URI as specified in 3GPP TS 23.003 [5].

### 8.2.9B /*<x>*/OnNetwork/GMSXCAPRootURI

Table 8.2.9B.1: <x>/OnNetwork/GMSXCAPRootURI

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/GMSXCAPRootURI | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the group management server XCAP Root URI information. | | | | |

The value is a URI as specified in 3GPP TS 23.003 [5].

### 8.2.9C /*<x>*/OnNetwork/CMSXCAPRootURI

Table 8.2.9C.1: <x>/OnNetwork/CMSXCAPRootURI

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/CMSXCAPRootURI | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the configuration management server XCAP Root URI information. | | | | |

The value is a URI as specified in 3GPP TS 23.003 [5].

### 8.2.10 /*<x>*/OnNetwork/Timers

Table 8.2.10.1: /*<x>*/OnNetwork/Timers

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/Timers | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for timer configuration. | | | | |

### 8.2.11 /*<x>*/OnNetwork/Timers/T100

Table 8.2.11.1: /*<x>*/OnNetwork/Timers/T100

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/Timers/T100 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT timer for floor release as specified in 3GPP TS 24.380 [8]. | | | | |

- Values: 0-255

The T100 is in seconds.

### 8.2.12 /*<x>*/OnNetwork/Timers/T101

Table 8.2.12.1: /*<x>*/OnNetwork/Timers/T101

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/Timers/T101 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT timer for floor request as specified in 3GPP TS 24.380 [8]. | | | | |

- Values: 0-255

The timer T101 is in seconds.

### 8.2.13 /*<x>*/OnNetwork/Timers/T103

Table 8.2.13.1: /*<x>*/OnNetwork/Timers/T103

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/Timers/T103 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT timer for end of RTP media as specified in 3GPP TS 24.380 [8]. | | | | |

- Values: 0-255

The timer T103 is in seconds.

### 8.2.14 /*<x>*/OnNetwork/Timers/T104

Table 8.2.14.1: /*<x>*/OnNetwork/Timers/T104

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/Timers/T104 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT timer for floor queue position request as specified in 3GPP TS 24.380 [8]. | | | | |

- Values: 0-255

The timer T104 is in seconds.

### 8.2.15 /*<x>*/OnNetwork/Timers/T132

Table 8.2.15.1: /*<x>*/OnNetwork/Timers/T132

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/Timers/T132 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT timer for queued request granted MCPTT user action as specified in 3GPP TS 24.380 [8]. | | | | |

- Values: 0-255

The timer T132 is in seconds.

### 8.2.16 /*<x>*/OnNetwork/HPLMN

Table 8.2.16.1: /*<x>*/OnNetwork/HPLMN

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/HPLMN | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the HPLMN configuration. | | | | |

### 8.2.17 /*<x>*/OnNetwork/HPLMN/PLMN

Table 8.2.17.1: /*<x>*/OnNetwork/HPLMN/PLMN

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/HPLMN/PLMN | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the HPLMN code. | | | | |

- Values: <PLMN>

The format of the PLMN is defined by 3GPP TS 23.003 [5].

### 8.2.18 /*<x>*/OnNetwork/HPLMN/Service

Table 8.2.18.1: /*<x>*/OnNetwork/HPLMN/Service

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/HPLMN/Service | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node indicates the MCS related services on a per HPLMN basis. | | | | |

### 8.2.19 /*<x>*/OnNetwork/HPLMN/Service/MCPTTToConRef

Table 8.2.19.1: /*<x>*/OnNetwork/HPLMN/Service/MCPTTToConRef

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/HPLMN/Service/MCPTTToConRef | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node contains the configuration parameters for establishment of the PDN connection for the MCS service on a per HPLMN basis. | | | | |

### 8.2.20 /*<x>*/OnNetwork/HPLMN/Service/MCPTTToConRef/<x>

Table 8.2.20.1: /*<x>*/OnNetwork/HPLMN/Service/MCPTTToConRef/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/HPLMN/Service/MCPTTToConRef/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneorMore | node | Get, Replace |  |
|  | This run-time node acts as a placeholder for each reference to the connectivity parameters on a per HPLMN basis. | | | | |

### 8.2.21 /*<x>*/OnNetwork/HPLMN/Service/MCPTTToConRef/<x>/ConRef

Table 8.2.21.1: /*<x>*/OnNetwork/HPLMN/Service/MCPTTToConRef/<x>/ConRef

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/HPLMN/Service/MCPTTToConRef/<x>/ConRef | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | The ConRef specifies a specific linkage to the connectivity parameters on a per HPLMN basis. | | | | |

- Values: <A network access point object>

### 8.2.22 /*<x>*/OnNetwork/HPLMN/Service/MCCommonCoreToConRef

Table 8.2.22.1: /*<x>*/OnNetwork/HPLMN/Service/MCCommonCoreToConRef

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/HPLMN/Service/MCCommonCoreToConRef | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node contains the configuration parameters for establishment of the PDN connection for the MC common core service on a per HPLMN basis. | | | | |

### 8.2.23 /*<x>*/OnNetwork/HPLMN/Service/MCCommonCoreToConRef/<x>

Table 8.2.23.1: /*<x>*/OnNetwork/HPLMN/Service/MCCommonCoreToConRef/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/HPLMN/Service/MCCommonCoreToConRef/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneorMore | node | Get, Replace |  |
|  | This run-time node acts as a placeholder for each reference to the connectivity parameters on a per HPLMN basis. | | | | |

### 8.2.24 /*<x>*/OnNetwork/HPLMN/Service/ MCCommonCoreToConRef/<x>/ConRef

Table 8.2.24.1: /*<x>*/OnNetwork/HPLMN/Service/MCCommonCoreToConRef/<x>/ConRef

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/HPLMN/Service/MCCommonCoreToConRef/<x>/ConRef | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | The ConRef specifies a specific linkage to the connectivity parameters on a per HPLMN basis. | | | | |

- Values: <A network access point object>

### 8.2.25 /*<x>*/OnNetwork/HPLMN/Service/MCIDMToConRef

Table 8.2.25.1: /*<x>*/OnNetwork/HPLMN/Service/MCIDMToConRef

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/HPLMN/Service/MCIDMToConRef | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node contains the configuration parameters for establishment of the PDN connection for the MC identity management service on a per HPLMN basis. | | | | |

### 8.2.26 /*<x>*/OnNetwork/HPLMN/Service/MCIDMToConRef/<x>

Table 8.2.26.1: /*<x>*/OnNetwork/HPLMN/Service/MCIDMToConRef/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/HPLMN/Service/MCIDMToConRef/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneorMore | node | Get, Replace |  |
|  | This run-time node acts as a placeholder for each reference to the connectivity parameters on a per HPLMN basis. | | | | |

### 8.2.27 /*<x>*/OnNetwork/HPLMN/Service/MCIDMToConRef/<x>/ConRef

Table 8.2.27.1: /*<x>*/OnNetwork/HPLMN/Service/MCIDMToConRef/<x>/ConRef

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/HPLMN/Service/MCIDMToConRef/<x>/ConRef | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | The ConRef specifies a specific linkage to the connectivity parameters on a per HPLMN basis. | | | | |

- Values: <A network access point object>

### 8.2.28 /*<x>*/OnNetwork/HPLMN/VPLMN

Table 8.2.28.1: /*<x>*/OnNetwork/HPLMN/VPLMN

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/HPLMN/VPLMN | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node is a placeholder for the VPLMN configuration. | | | | |

### 8.2.29 /*<x>*/OnNetwork/HPLMN/VPLMN/PLMN

Table 8.2.29.1: /*<x>*/OnNetwork/HPLMN/VPLMN/PLMN

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/HPLMN/VPLMN/PLMN | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the VPLMN code. | | | | |

- Values: <PLMN>

The format of the PLMN is defined by 3GPP TS 23.003 [5].

### 8.2.30 /*<x>*/OnNetwork/HPLMN/VPLMN/Service

Table 8.2.30.1: /*<x>*/OnNetwork/HPLMN/VPLMN/Service

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/HPLMN/VPLMN/Service | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node indicates the MCS related services on a per VPLMN and HPLMN basis. | | | | |

### 8.2.31 /*<x>*/OnNetwork/HPLMN/VPLMN/Service/MCPTTToConRef

Table 8.2.31.1: /*<x>*/OnNetwork/HPLMN/VPLMN/Service/MCPTTToConRef

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/HPLMN/VPLMN/Service/MCPTTToConRef | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node contains the configuration parameters for establishment of the PDN connection for the MCS service on a per VPLMN and HPLMN basis. | | | | |

### 8.2.32 /*<x>*/OnNetwork/HPLMN/VPLMN/Service/MCPTTToConRef/<x>

Table 8.2.32.1: /*<x>*/OnNetwork/HPLMN/Service/MCPTTToConRef/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/HPLMN/VPLMN/Service/MCPTTToConRef/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneorMore | node | Get, Replace |  |
|  | This run-time node acts as a placeholder for each reference to the connectivity parameters on a per VPLMN and HPLMN basis. | | | | |

### 8.2.33 /*<x>*/OnNetwork/HPLMN/VPLMN/Service/ MCPTTToConRef/<x>/ConRef

Table 8.2.33.1: /*<x>*/OnNetwork/HPLMN/VPLMN/Service/MCPTTToConRef/<x>/ConRef

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/HPLMN/VPLMN/Service/MCPTTToConRef/<x>/ConRef | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | The ConRef specifies a specific linkage to the connectivity parameters on a per VPLMN and HPLMN basis. | | | | |

- Values: <A network access point object>

### 8.2.34 /*<x>*/OnNetwork/HPLMN/VPLMN/Service/ MCCommonCoreToConRef

Table 8.2.34.1: /*<x>*/OnNetwork/HPLMN/VPLMN/Service/MCCommonCoreToConRef

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/HPLMN/VPLMN/Service/MCCommonCoreToConRef | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node contains the configuration parameters for establishment of the PDN connection for the MC common core service on a per VPLMN and HPLMN basis. | | | | |

### 8.2.35 /*<x>*/OnNetwork/HPLMN/VPLMN/Service/ MCCommonCoreToConRef/<x>

Table 8.2.35.1: /*<x>*/OnNetwork/HPLMN/VPLMN/Service/MCCommonCoreToConRef/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/HPLMN/VPLMN/Service/MCCommonCoreToConRef/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneorMore | node | Get, Replace |  |
|  | This run-time node acts as a placeholder for each reference to the connectivity parameters on a per VPLMN and HPLMN basis. | | | | |

### 8.2.36 /*<x>*/OnNetwork/HPLMN/VPLMN/Service/ MCCommonCoreToConRef/<x>/ConRef

Table 8.2.36.1: /*<x>*/OnNetwork/HPLMN/VPLMN/Service/MCCommonCoreToConRef/<x>/ConRef

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/HPLMN/VPLMN/Service/MCCommonCoreToConRef/<x>/ConRef | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | The ConRef specifies a specific linkage to the connectivity parameters on a per VPLMN and HPLMN basis. | | | | |

- Values: <A network access point object>

### 8.2.37 /*<x>*/OnNetwork/HPLMN/VPLMN/Service/MCIDMToConRef

Table 8.2.37.1: /*<x>*/OnNetwork/HPLMN/VPLMN/Service/MCIDMToConRef

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/HPLMN/VPLMN/Service/MCIDMToConRef | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node contains the configuration parameters for establishment of the PDN connection for the MC identity management service on a per VPLMN and HPLMN basis. | | | | |

### 8.2.38 /*<x>*/OnNetwork/HPLMN/VPLMN/Service/MCIDMToConRef/<x>

Table 8.2.38.1: /*<x>*/OnNetwork/HPLMN/VPLMN/Service/MCIDMToConRef/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/HPLMN/VPLMN/Service/MCIDMToConRef/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneorMore | node | Get, Replace |  |
|  | This run-time node acts as a placeholder for each reference to the connectivity parameters on a per VPLMN and HPLMN basis. | | | | |

### 8.2.39 /*<x>*/OnNetwork/HPLMN/VPLMN/Service/ MCIDMToConRef/<x>/ConRef

Table 8.2.39.1: /*<x>*/OnNetwork/HPLMN/VPLMN/Service/MCIDMToConRef/<x>/ConRef

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/HPLMN/VPLMN/Service/MCIDMToConRef/<x>/ConRef | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | The ConRef specifies a specific linkage to the connectivity parameters on a per VPLMN and HPLMN basis. | | | | |

- Values: <A network access point object>

### 8.2.40 /*<x>*/OnNetwork/AppServerInfo

Table 8.2.40.1: /*<x>*/OnNetwork/AppServerInfo

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/AppServerInfo | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the application plane server identity information configuration. | | | | |

### 8.2.41 /*<x>*/OnNetwork/AppServerInfo/IDMSAuthEndpoint

Table 8.2.41.1: /*<x>*/OnNetwork/AppServerInfo/IDMSAuthEndpoint

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/AppServerInfo/IDMSAuthEndpoint | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the identity management server authorisation endpoint identity information. | | | | |

The value is a URI as specified in 3GPP TS 23.003 [5].

### 8.2.41A /*<x>*/OnNetwork/AppServerInfo/IDMSTokenEndpoint

Table 8.2.41A.1: /*<x>*/OnNetwork/AppServerInfo/IDMSTokenEndpoint

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/AppServerInfo/IDMSTokenEndpoint | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the identity management server token endpoint identity information. | | | | |

The value is a URI as specified in 3GPP TS 23.003 [5].

### 8.2.41B /*<x>*/OnNetwork/AppServerInfo/HTTPProxy

Table 8.2.41B.1: /*<x>*/OnNetwork/AppServerInfo/HTTPProxy

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/AppServerInfo/HTTPProxy | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the HTTP Proxy identity information. | | | | |

The value is a URI as specified in 3GPP TS 23.003 [5].

### 8.2.42 /*<x>*/OnNetwork/AppServerInfo/GMS

Table 8.2.42.1: /*<x>*/OnNetwork/AppServerInfo/GMS

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/AppServerInfo/GMS | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the group management server identity information. | | | | |

The value is a URI as specified in 3GPP TS 23.003 [5].

### 8.2.43 /*<x>*/OnNetwork/AppServerInfo/CMS

Table 8.2.43.1: /*<x>*/OnNetwork/AppServerInfo/CMS

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/AppServerInfo/CMS | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the configuration management server identity information. | | | | |

The value is a URI as specified in 3GPP TS 23.003 [5].

### 8.2.44 /*<x>*/OnNetwork/AppServerInfo/KMS

Table 8.2.44.1: /*<x>*/OnNetwork/AppServerInfo/KMS

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/AppServerInfo/KMS | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates key management server identity information. | | | | |

The value is a URI as specified in 3GPP TS 23.003 [5].

### 8.2.44A /*<x>*/OnNetwork/AppServerInfo/TLSTunnelAuthMethod

Table 8.2.44A.1: /*<x>*/OnNetwork/AppServerInfo/TLSTunnelAuthMethod

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/AppServerInfo/TLSTunnelAuthMethod | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the TLS tunnel authentication method configuration. | | | | |

### 8.2.44B /*<x>*/OnNetwork/AppServerInfo/TLSTunnelAuthMethod/Mutual

Table 8.2.44B.1: /*<x>*/OnNetwork/AppServerInfo/TLSTunnelAuthMethod/Mutual

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/AppServerInfo/TLSTunnelAuthMethod/Mutual | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether mutual authentication is used for the TLS tunnel authentication. | | | | |

When set to "true" mutual authentication is used.

When set to "false" one-way authentication based on the server certificate is used.

The default value is "false".

### 8.2.44C /*<x>*/OnNetwork/AppServerInfo/TLSTunnelAuthMethod/X509

Table 8.2.44C.1: /*<x>*/OnNetwork/AppServerInfo/TLSTunnelAuthMethod/X509

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/AppServerInfo/TLSTunnelAuthMethod/X509 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains the X.509 certificate for mutual authentication for the TLS tunnel authentication. | | | | |

### 8.2.44D /*<x>*/OnNetwork/AppServerInfo/TLSTunnelAuthMethod/Key

Table 8.2.44D.1: /*<x>*/OnNetwork/AppServerInfo/TLSTunnelAuthMethod/Key

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/AppServerInfo/TLSTunnelAuthMethod/Key | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains the pre-shared key for mutual authentication for the TLS tunnel authentication. | | | | |

### 8.2.44E /*<x>*/OnNetwork/IntegrityProtection

Table 8.2.44E.1: /*<x>*/OnNetwork/IntegrityProtection

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/IntegrityProtection | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether integrity protection is enabled. | | | | |

When set to "true" integrity protection is enabled.

When set to "false" integrity protection is disabled.

The default value is "true".

### 8.2.44F /*<x>*/OnNetwork/ConfidentialityProtection

Table 8.2.44F.1: /*<x>*/OnNetwork/ConfidentialityProtection

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/ConfidentialityProtection | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether integrity protection is enabled. | | | | |

When set to "true" confidentiality protection is enabled.

When set to "false" confidentiality protection is disabled.

The default value is "true".

### 8.2.44G1 /*<x>*/OnNetwork/MCPTTServiceDetails

Table 8.2.44G1.1: /<x>/OnNetwork/MCPTTServiceDetails

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/MCPTTServiceDetails | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the details of the MCPTT service. | | | | |

### 8.2.44G2 /*<x>*/OnNetwork/MCPTTServiceDetails/IPv6Required

Table 8.2.44G2.1: /<x>/OnNetwork/MCPTTServiceDetails/IPv6Required

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/MCPTTServiceDetails/IPv6Required | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | Bool | Get, Replace |  |
|  | This leaf node indicates whether IP version 6 is required to use to access the MCPTT service. | | | | |

When set to "true", IPv6 shall be used to access the service.

When set to "false", IPv4 shall be used to access the service.

### 8.2.44G3 /*<x>*/OnNetwork/MCPTTServiceDetails/ServerURI

Table 8.2.44G3.1: /<x>/OnNetwork/MCPTTServiceDetails/ServerURI

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/MCPTTServiceDetails/ServerURI | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | Chr | Get, Replace |  |
|  | This leaf node indicates the URI to use to access the MCPTT service. | | | | |

The value is a URI as specified in 3GPP TS 23.003 [5].

### 8.2.44G4 /*<x>*/OnNetwork/MCVideoServiceDetails

Table 8.2.44G4.1: /<x>/OnNetwork/MCVideoServiceDetails

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/MCVideoServiceDetails | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the details of the MCVideo service. | | | | |

### 8.2.44G5 /*<x>*/OnNetwork/MCVideoServiceDetails/IPv6Required

Table 8.2.44G5.1: /<x>/OnNetwork/MCVideoServiceDetails/IPv6Required

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/MCVideoServiceDetails/IPv6Required | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | Bool | Get, Replace |  |
|  | This leaf node indicates the IP version to use to access the MCVideo service. | | | | |

When set to "true", IPv6 shall be used to access the service.

When set to "false", IPv4 shall be used to access the service.

### 8.2.44G6 /*<x>*/OnNetwork/MCVideoServiceDetails/ServerURI

Table 8.2.44G6.1: /<x>/OnNetwork/MCVideoServiceDetails/ServerURI

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/MCVideoServiceDetails/ServerURI | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | Chr | Get, Replace |  |
|  | This leaf node indicates the URI to use to access the MCVideo service. | | | | |

The value is a URI as specified in 3GPP TS 23.003 [5].

### 8.2.44G7 /*<x>*/OnNetwork/MCDataServiceDetails

Table 8.2.44G7.1: /<x>/OnNetwork/MCDataServiceDetails

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/MCDataServiceDetails | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the details of the MCData service. | | | | |

### 8.2.44G8 /*<x>*/OnNetwork/MCDataServiceDetails/IPv6Required

Table 8.2.44G8.1: /<x>/OnNetwork/MCDataServiceDetails/IPv6Required

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/MCDataServiceDetails/IPv6Required | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | Bool | Get, Replace |  |
|  | This leaf node indicates the IP version to use to access the MCData service. | | | | |

When set to "true", IPv6 shall be used to access the service.

When set to "false", IPv4 shall be used to access the service.

### 8.2.44G9 /*<x>*/OnNetwork/MCDataServiceDetails/ServerURI

Table 8.2.44G9.1: /<x>/OnNetwork/MCDataServiceDetails/ServerURI

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/MCDataServiceDetails/ServerURI | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | Chr | Get, Replace |  |
|  | This leaf node indicates the URI to use to access the MCData service. | | | | |

The value is a URI as specified in 3GPP TS 23.003 [5].

### 8.2.45 /*<x>*/OffNetwork

Table 8.2.45.1: /*<x>*/OffNetwork

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | node | Get, Replace |  |
|  | This interior node represents a container for the off-network operation. | | | | |

### 8.2.46 /*<x>*/OffNetwork/Timers

Table 8.2.46.1: /*<x>*/OffNetwork/Timers

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Timers | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the timer configuration. | | | | |

### 8.2.47 /*<x>*/OffNetwork/Timers/TFG1

Table 8.2.47.1: /*<x>*/OffNetwork/Timers/TFG1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Timers/TFG1 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT timer for wait for call announcement as specified in 3GPP TS 24.379 [7]. | | | | |

- Values: 0-65535

The timer TFG1 is in milliseconds.

### 8.2.48 /*<x>*/OffNetwork/Timers/TFG2

Table 8.2.48.1: /*<x>*/OffNetwork/Timers/TFG2

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Timers/TFG2 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT timer for call announcement as specified in 3GPP TS 24.379 [7]. | | | | |

- Values: 0-65535

The timer TFG2 is in milliseconds.

### 8.2.49 /*<x>*/OffNetwork/Timers/TFG3

Table 8.2.49.1: /*<x>*/OffNetwork/Timers/TFG3

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Timers/TFG3 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT timer for call probe retransmission as specified in 3GPP TS 24.379 [7]. | | | | |

- Values: 0-65535

The timer TFG3 is in milliseconds.

### 8.2.50 /*<x>*/OffNetwork/Timers/TFG4

Table 8.2.50.1: /*<x>*/OffNetwork/Timers/TFG4

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Timers/TFG4 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT timer for waiting for the MCPTT user as specified in 3GPP TS 24.379 [7]. | | | | |

- Values: 0-60

The timer TFG4 is in seconds.

### 8.2.51 /*<x>*/OffNetwork/Timers/TFG5

Table 8.2.51.1: /*<x>*/OffNetwork/Timers/TFG5

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Timers/TFG5 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT timer for not present incoming call announcements as specified in 3GPP TS 24.379 [7]. | | | | |

- Values: 0-255

The timer TFG5 is in seconds.

### 8.2.52 /*<x>*/OffNetwork/Timers/TFG11

Table 8.2.52.1: /*<x>*/OffNetwork/Timers/TFG11

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Timers/TFG11 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the timer for MCPTT emergency end retransmission as specified in 3GPP TS 24.379 [7]. | | | | |

- Values: 0-65535

The timer TFG11 is in milliseconds.

### 8.2.53 /*<x>*/OffNetwork/Timers/TFG12

Table 8.2.53.1: /*<x>*/OffNetwork/Timers/TFG12

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Timers/TFG12 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the timer for MCPTT imminent peril end retransmission as specified in 3GPP TS 24.379 [7]. | | | | |

- Values: 0-65535

The timer TFG12 is in milliseconds.

### 8.2.54 /*<x>*/OffNetwork/Timers/TFG13

Table 8.2.54.1: /*<x>*/OffNetwork/Timers/TFG13

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Timers/TFG13 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT timer for implicit priority downgrade as specified in 3GPP TS 24.379 [7]. | | | | |

- Values: 0-255

The timer TFG13 is in seconds.

### 8.2.54A /*<x>*/OffNetwork/Timers/TFG14

Table 8.2.54A.1: /*<x>*/OffNetwork/Timers/TFG14

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Timers/TFG14 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT timer for implicit priority downgrade (imminent peril) as specified in 3GPP TS 24.379 [7]. | | | | |

- Values: 0-255

The timer TFG14 is in seconds.

### 8.2.55 /*<x>*/OffNetwork/Timers/TFP1

Table 8.2.55.1: /*<x>*/OffNetwork/Timers/TFP1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Timers/TFP1 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT timer for private call request retransmission as specified in 3GPP TS 24.379 [7]. | | | | |

- Values: 0-65535

The timer TFP1 is in milliseconds.

### 8.2.56 /*<x>*/OffNetwork/Timers/TFP2

Table 8.2.56.1: /*<x>*/OffNetwork/Timers/TFP2

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Timers/TFP2 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT timer for waiting for the MCPTT user to respond to the setup request message when manual commencement mode is used as specified in 3GPP TS 24.379 [7]. | | | | |

- Values: 0-60

The timer TFP2 is in seconds.

### 8.2.57 /*<x>*/OffNetwork/Timers/TFP3

Table 8.2.57.1: /*<x>*/OffNetwork/Timers/TFP3

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Timers/TFP3 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT timer for private call release retransmission as specified in 3GPP TS 24.379 [7]. | | | | |

- Values: 0-65535

The timer TFP3 is in milliseconds.

### 8.2.58 /*<x>*/OffNetwork/Timers/TFP4

Table 8.2.58.1: /*<x>*/OffNetwork/Timers/TFP4

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Timers/TFP4 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT timer for private call accept retransmission as specified in 3GPP TS 24.379 [7]. | | | | |

- Values: 0-65535

The timer TFP4 is in milliseconds.

### 8.2.59 /*<x>*/OffNetwork/Timers/TFP5

Table 8.2.59.1: /*<x>*/OffNetwork/Timers/TFP5

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Timers/TFP5 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT timer for call release as specified in 3GPP TS 24.379 [7]. | | | | |

- Values: 0-600

The timer TFP5 is in seconds.

### 8.2.60 /*<x>*/OffNetwork/Timers/TFP6

Table 8.2.60.1: /*<x>*/OffNetwork/Timers/TFP6

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Timers/TFP6 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT timer for MCPTT emergency private call cancel retransmission as specified in 3GPP TS 24.379 [7]. | | | | |

- Values: 0-65535

The timer TFP6 is in milliseconds.

### 8.2.61 /*<x>*/OffNetwork/Timers/TFP7

Table 8.2.61.1: /*<x>*/OffNetwork/Timers/TFP7

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Timers/TFP7 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT timer for waiting for any message with same call identifier as specified in 3GPP TS 24.379 [7]. | | | | |

- Values: 0-255

The timer TFP7 is in seconds.

### 8.2.61A /*<x>*/OffNetwork/Timers/TFP9

Table 8.2.61A: /*<x>*/OffNetwork/Timers/TFP9

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Timers/TFP9 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT timer for waiting for call response message as specified in 3GPP TS 24.379 [7]. | | | | |

- Values: 0-60

The timer TFP9 is in seconds.

### 8.2.62 /*<x>*/OffNetwork/Timers/TFB1

Table 8.2.62.1: /*<x>*/OffNetwork/Timers/TFB1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Timers/TFB1 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT timer for max duration as specified in 3GPP TS 24.379 [7]. | | | | |

- Values: 0-600

The timer TFB1 is in seconds.

### 8.2.63 /*<x>*/OffNetwork/Timers/TFB2

Table 8.2.63.1: /*<x>*/OffNetwork/Timers/TFB2

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Timers/TFB2 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT timer for broadcast retransmission as specified in 3GPP TS 24.379 [7]. | | | | |

- Values: 0-10

The timer TFB2 is in seconds.

### 8.2.64 /*<x>*/OffNetwork/Timers/TFB3

Table 8.2.64.1: /*<x>*/OffNetwork/Timers/TFB3

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Timers/TFB3 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT timer for waiting for the MCPTT user as specified in 3GPP TS 24.379 [7]. | | | | |

- Values: 0-60

The timer TFB3 is in seconds.

### 8.2.65 /*<x>*/OffNetwork/Timers/T201

Table 8.2.65.1: /*<x>*/OffNetwork/Timers/T201

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Timers/T201 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT timer for floor request as specified in 3GPP TS 24.380 [8]. | | | | |

- Values: 0-65535

The timer T201 is in milliseconds.

### 8.2.66 /*<x>*/OffNetwork/Timers/T203

Table 8.2.66.1: /*<x>*/OffNetwork/Timers/T203

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Timers/T203 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT timer for end of RTP media as specified in 3GPP TS 24.380 [8]. | | | | |

- Values: 0-255

The timer T203 is in seconds.

### 8.2.67 /*<x>*/OffNetwork/Timers/T204

Table 8.2.67.1: /*<x>*/OffNetwork/Timers/T204

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Timers/T204 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT timer for floor queue position request as specified in 3GPP TS 24.380 [8]. | | | | |

- Values: 0-65535

The timer T204 is in milliseconds.

### 8.2.68 /*<x>*/OffNetwork/Timers/T205

Table 8.2.68.1: /*<x>*/OffNetwork/Timers/T205

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Timers/T205 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT timer for floor granted request as specified in 3GPP TS 24.380 [8]. | | | | |

- Values: 0-65535

The timer T205 is in milliseconds.

### 8.2.69 Void

### 8.2.70 /*<x>*/OffNetwork/Timers/T233

Table 8.2.70.1: /*<x>*/OffNetwork/Timers/T233

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Timers/T233 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT timer for pending user action as specified in 3GPP TS 24.380 [8]. | | | | |

- Values: 0-255

The timer T233 is in seconds.

### 8.2.71 /*<x>*/OffNetwork/Timers/TFE1

Table 8.2.71.1: /*<x>*/OffNetwork/Timers/TFE1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Timers/TFE1 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the timer for MCPTT emergency alert as specified in 3GPP TS 24.379 [7]. | | | | |

- Values: 0-65535

The timer TFE1 is in seconds.

### 8.2.72 /*<x>*/OffNetwork/Timers/TFE2

Table 8.2.72.1: /*<x>*/OffNetwork/Timers/TFE2

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Timers/TFE2 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the timer for MCPTT emergency alert retransmission as specified in 3GPP TS 24.379 [7]. | | | | |

- Values: 0-10

The timer TFE2 is in seconds.

### 8.2.73 /*<x>*/OffNetwork/Counters

Table 8.2.73.1: /*<x>*/OffNetwork/Counters

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Counters | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the counter configuration. | | | | |

### 8.2.74 /*<x>*/OffNetwork/Counters/CFP1

Table 8.2.74.1: /*<x>*/OffNetwork/Counters/CFP1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Counters/CFP1 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT counter for private call request retransmission as specified in 3GPP TS 24.379 [7]. | | | | |

- Values: 0-255

### 8.2.75 /*<x>*/OffNetwork/Counters/CFP3

Table 8.2.75.1: /*<x>*/OffNetwork/Counters/CFP3

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Counters/CFP3 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT counter for private call release retransmission as specified in 3GPP TS 24.379 [7]. | | | | |

- Values: 0-255

### 8.2.76 /*<x>*/OffNetwork/Counters/CFP4

Table 8.2.76.1: /*<x>*/OffNetwork/Counters/CFP4

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Counters/CFP4 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT counter for private call accept retransmission as specified in 3GPP TS 24.379 [7]. | | | | |

- Values: 0-255

### 8.2.77 /*<x>*/OffNetwork/Counters/CFP6

Table 8.2.77.1: /*<x>*/OffNetwork/Counters/CFP6

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Counters/CFP6 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT counter for emergency private call cancel retransmission as specified in 3GPP TS 24.379 [7]. | | | | |

- Values: 0-255

### 8.2.78 /*<x>*/OffNetwork/Counters/CFG11

Table 8.2.78.1: /*<x>*/OffNetwork/Counters/CFG11

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Counters/CFG11 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the counter for MCPTT group call emergency end retransmission as specified in 3GPP TS 24.379 [7]. | | | | |

- Values: 0-255

### 8.2.79 /*<x>*/OffNetwork/Counters/CFG12

Table 8.2.79.1: /*<x>*/OffNetwork/Counters/CFG12

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Counters/CFG12 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the counter for MCPTT imminent peril call emergency end retransmission as specified in 3GPP TS 24.379 [7]. | | | | |

- Values: 0-255

### 8.2.80 /*<x>*/OffNetwork/Counters/C201

Table 8.2.80.1: /*<x>*/OffNetwork/Counters/C201

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Counters/C201 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT counter for floor request as specified in 3GPP TS 24.380 [8]. | | | | |

- Values: 0-255

### 8.2.81 /*<x>*/OffNetwork/Counters/C204

Table 8.2.81.1: /*<x>*/OffNetwork/Counters/C204

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Counters/C204 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT counter for floor queue position request as specified in 3GPP TS 24.380 [8]. | | | | |

- Values: 0-255

### 8.2.82 /*<x>*/OffNetwork/Counters/C205

Table 8.2.82.1: /*<x>*/OffNetwork/Counters/C205

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/Counters/C205 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the MCPTT counter for floor granted request as specified in 3GPP TS 24.380 [8]. | | | | |

- Values: 0-255

# 9 MCData UE configuration MO

## 9.1 General

The MCData UE configuration Management Object (MO) is used to configure MCData Client behaviour for the on-network or off-network MCData Service. The MCData UE configuration parameters may be stored in the ME, or in the USIM as specified in 3GPP TS 31.102 [10], or in both the ME and the USIM. If both the ME and the USIM contain the same parameters, the values stored in the USIM shall take precedence.

The Management Object Identifier is: urn:oma:mo:ext-3gpp-MCData-UE-configuration:1.0.

Protocol compatibility: This MO is compatible with OMA OMA DM 1.2 [3].

The OMA DM ACL property mechanism (see OMA OMA-ERELD-DM-V1\_2 [2]) may be used to grant or deny access rights to OMA DM servers in order to modify nodes and leaf objects of the MCData UE configuration MO.

The following nodes and leaf objects are possible under the MCData UE configuration node as described in figure 9.1.1 and figure 9.1.2.



Figure 9.1.1: The MCData UE configuration MO (1 of 2)



Figure 9.1.2: The MCData UE configuration MO (2 of 2)

## 9.2 MCData UE configuration MO parameters

### 9.2.1 General

This clause describes the parameters for the MCData UE configuration Management Object (MO).

### 9.2.2 Node: *<x>*

Table 9.2.2.1: Node: <x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get |  |
|  | This interior node acts as a placeholder for the MCData UE configuration Management Object (MO).  For the MCData UE configuration MO, the namespace specific string is: "urn:oma:mo:oma-dm-mcdata-ue-configuration:1.0" | | | | |

- Values: N/A

### 9.2.3 /*<x>*/Name

Table 9.2.3.1: /<x>/Name

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | chr | Get |  |
|  | The Name leaf is a name for the MCData UE configuration settings. | | | | |

- Values: <User displayable name>

### 9.2.4 /*<x>*/Ext/

Table 9.2.4.1: /<x>/Ext/

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Ext | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | The Ext is an interior node for where the vendor specific information about the MCData UE configuration MO is being placed. | | | | |

Usually the vendor extension is identified by vendor specific name under the ext node and contains the vendor meaning application vendor, device vendor etc. The tree structure under the vendor identified is not defined and can therefore include one or more un-standardized sub-trees.

- Values: N/A

### 9.2.5 /*<x>*/Common

Table 9.2.5.1: /*<x>*/Common

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | node | Get, Replace |  |
|  | This interior node represents a container for the common network operation which means both on-network operation and off-network operation. | | | | |

### 9.2.6 /*<x>*/Common/MCDataGroupTxns

Table 9.2.6.1: /*<x>*/Common/MCDataGroupTxns

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCDataGroupTxns | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the MCData group transactions configuration. | | | | |

### 9.2.7 /*<x>*/Common/MCDataGroupTxns/MaxSDSNc4

Table 9.2.7.1: /*<x>*/Common/MCDataGroupTxns/MaxSDSNc4

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCDataGroupTxns/MaxSDSNc4 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the maximum number of simultaneous SDS transactions. | | | | |

- Values: 0-255

### 9.2.8 /*<x>*/Common/MCDataGroupTxns/SDSPresentationPriority

Table 9.2.8.1: /*<x>*/Common/MCDataGroupTxns/SDSPresentationPriority

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCDataGroupTxns/SDSPresentationPriority | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | node | Get, Replace |  |
|  | This interior node is a placeholder for the prioritized MCData SDS configuration. | | | | |

### 9.2.9 /*<x>*/Common/MCDataGroupTxns/SDSPresentationPriority/<x>

Table 9.2.9.1: /*<x>*/Common/MCDataGroupTxns/SDSPresentationPriority/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCDataGroupTxns/SDSPresentationPriority/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more prioritized MCData SDS configuration. | | | | |

### 9.2.10 /*<x>*/Common/MCDataGroupTxns/ SDSPresentationPriority/<x>/MCDataGroupID

Table 9.2.10.1: /*<x>*/Common/MCDataGroupTxns/SDSPresentationPriority/<x>/MCDataGroupID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCDataGroupTxns/SDSPresentationPriority/<x>/MCDataGroupID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the associated MCData group ID. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 9.2.11 /*<x>*/Common/MCDataGroupTxns/ SDSPresentationPriority/ <x>/MCDataGroupPriorityHierarchy

Table 9.2.11.1: /*<x>*/Common/MCDataGroupTxns/SDSPresentationPriority/<x>/MCDataGroupPriorityHierarchy

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCDataGroupTxns/SDSPresentationPriority/<x>/MCDataGroupPriorityHierarchy | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the requested presentation priority of SDS transactions. | | | | |

- Values: 0-255

The group with the lowest MCDataGroupPriorityHierarchy value shall be considered as the group having the lowest priority among the groups.

### 9.2.12 /*<x>*/Common/MCDataGroupTxns/MaxFDNc4

Table 9.2.12.1: /*<x>*/Common/MCDataGroupTxns/MaxFDNc4

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCDataGroupTxns/MaxFDNc4 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the maximum number of simultaneous FD transactions. | | | | |

- Values: 0-255

### 9.2.13 /*<x>*/Common/MCDataGroupTxns/FDPresentationPriority

Table 9.2.13.1: /*<x>*/Common/MCDataGroupTxns/FDPresentationPriority

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCDataGroupTxns/FDPresentationPriority | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | node | Get, Replace |  |
|  | This interior node is a placeholder for the prioritized MCData FD configuration. | | | | |

### 9.2.14 /*<x>*/Common/MCDataGroupTxns/FDPresentationPriority/<x>

Table 9.2.14.1: /*<x>*/Common/MCDataGroupTxns/FDPresentationPriority/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCDataGroupTxns/FDPresentationPriority /<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more prioritized MCData FD configuration. | | | | |

### 9.2.15 /*<x>*/Common/MCDataGroupTxns/ FDPresentationPriority/<x>/MCDataGroupID

Table 9.2.15.1: /*<x>*/Common/MCDataGroupTxns/FDPresentationPriority/<x>/MCDataGroupID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCDataGroupTxns/FDPresentationPriority/<x>/MCDataGroupID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the associated MCData group ID. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 9.2.16 /*<x>*/Common/MCDataGroupTxns/FDPresentationPriority/ <x>/MCDataGroupPriorityHierarchy

Table 9.2.16.1: /*<x>*/Common/MCDataGroupTxns/FDPresentationPriority/<x>/MCDataGroupPriorityHierarchy

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCDataGroupTxns/FDPresentationPriority/<x>/MCDataGroupPriorityHierarchy | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the requested presentation priority of FD transactions. | | | | |

- Values: 0-255

The group with the lowest MCDataGroupPriorityHierarchy value shall be considered as the group having the lowest priority among the groups.

### 9.2.17 /*<x>*/Common/MCDataGroupTxns/ConversationPresentationPriority

Table 9.2.17.1: /*<x>*/Common/MCDataGroupTxns/ConversationPresentationPriority

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCDataGroupTxns/ConversationPresentationPriority | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | node | Get, Replace |  |
|  | This interior node is a placeholder for the prioritized MCData conversation management configuration. | | | | |

### 9.2.18 /*<x>*/Common/MCDataGroupTxns/ ConversationPresentationPriority/<x>

Table 9.2.18.1: /*<x>*/Common/MCDataGroupTxns/ConversationPresentationPriority/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCDataGroupTxns/ConversationPresentationPriority /<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more prioritized MCData conversation management configuration. | | | | |

### 9.2.19 /*<x>*/Common/MCDataGroupTxns/ ConversationPresentationPriority/<x>/MCDataGroupID

Table 9.2.19.1: /*<x>*/Common/MCDataGroupTxns/ConversationPresentationPriority/<x>/MCDataGroupID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCDataGroupTxns/ConversationPresentationPriority/<x>/MCDataGroupID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the associated MCData group ID. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 9.2.20 /*<x>*/Common/MCDataGroupTxns/ ConversationPresentationPriority/<x>/ MCDataGroupPriorityHierarchy

Table 9.2.20.1: /*<x>*/Common/MCDataGroupTxns/ConversationPresentationPriority/<x>/MCDataGroupPriorityHierarchy

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCDataGroupTxns/ConversationPresentationPriority/<x>/MCDataGroupPriorityHierarchy | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the requested presentation priority of conversation management transactions. | | | | |

- Values: 0-255

The group with the lowest MCDataGroupPriorityHierarchy value shall be considered as the group having the lowest priority among the groups.

### 9.2.21 /*<x>*/Common/MCDataGroupTxns/MaxTCNc4

Table 9.2.21.1: /*<x>*/Common/MCDataGroupTxns/MaxTCNc4

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCDataGroupTxns/MaxTCNc4 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the maximum number of simultaneous data transmissions. | | | | |

- Values: 0-255

### 9.2.22 /*<x>*/Common/MCDataGroupTxns/MaxTCNc5

Table 9.2.22.1: /*<x>*/Common/MCDataGroupTxns/MaxTCNc5

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCDataGroupTxns/MaxTCN5 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the maximum number of data transmissions in a group. | | | | |

- Values: 0-255

### 9.2.23 /*<x>*/Common/MCDataGroupTxns/DataPresentationPriority

Table 9.2.23.1: /*<x>*/Common/MCDataGroupTxns/DataPresentationPriority

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCDataGroupTxns/DataPresentationPriority | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | node | Get, Replace |  |
|  | This interior node is a placeholder for the prioritized MCData Transmission Control configuration. | | | | |

### 9.2.24 /*<x>*/Common/MCDataGroupTxns/DataPresentationPriority/<x>

Table 9.2.24.1: /*<x>*/Common/MCDataGroupTxns/DataPresentationPriority/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCDataGroupTxns/DataPresentationPriority/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more prioritized MCData Transmission Control configuration. | | | | |

### 9.2.25 /*<x>*/Common/MCDataGroupTxns/ DataPresentationPriority/<x>/MCDataGroupID

Table 9.2.25.1: /*<x>*/Common/MCDataGroupTxns/DataPresentationPriority/<x>/MCDataGroupID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCDataGroupTxns/DataPresentationPriority/<x>/MCDataGroupID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the associated MCData group ID. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 9.2.26 /*<x>*/Common/MCDataGroupTxns/DataPresentationPriority/ <x>/MCDataGroupPriorityHierarchy

Table 9.2.26.1: /*<x>*/Common/MCDataGroupTxns/DataPresentationPriority/<x>/MCDataGroupPriorityHierarchy

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCDataGroupTxns/DataPresentationPriority/<x>/MCDataGroupPriorityHierarchy | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the requested presentation priority of data received. | | | | |

- Values: 0-255

The group with the lowest MCDataGroupPriorityHierarchy value shall be considered as the group having the lowest priority among the groups.

### 9.2.27 /*<x>*/Common/MCDataGroupTxns/MaxRCNc4

Table 9.2.27.1: /*<x>*/Common/MCDataGroupTxns/MaxRCNc4

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCDataGroupTxns/MaxRCNc4 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the maximum number of simultaneous data receptions. | | | | |

- Values: 0-255

### 9.2.28 /*<x>*/Common/MCDataGroupTxns/MaxRCNc5

Table 9.2.28.1: /*<x>*/Common/MCDataGroupTxns/MaxRCNc5

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCDataGroupTxns/MaxRCN5 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the maximum number of data receptions in a group. | | | | |

- Values: 0-255

### 9.2.29 /*<x>*/OnNetwork

Table 9.2.29.1: /*<x>*/OnNetwork

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | node | Get, Replace |  |
|  | This interior node represents a container for on-network operation. | | | | |

### 9.2.30 /*<x>*/OnNetwork/RelayService

Table 9.2.30.1: /*<x>*/OnNetwork/RelayService

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/RelayService | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to use a relay service. | | | | |

When set to "true" the MCData group is allowed to use a relay service.

When set to "false" the MCData group is not allowed to use a relay service.

### 9.2.31 /*<x>*/OnNetwork/IPv6Preferred

Table 9.2.31.1: /*<x>*/OnNetwork/IPv6Preferred

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/IPv6Preferred | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether IPv6 is preferred over IPv4 for on-network operation when the MCData UE has both IPv4 and IPv6 host configuration. | | | | |

If the MCData UE has both IPv4 and IPv6 host configuration and:

- if IPv6Preferred is set to "true" then the UE uses IPv6 for all on‑network signalling and media; otherwise

- if IPv6Preferred is set to "false" then the UE uses IPv4 for all on‑network signalling and media.

### 9.2.32 /*<x>*/OnNetwork/RelayedMCDataGroup

Table 9.2.32.1: /*<x>*/OnNetwork/RelayedMCDataGroup

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/RelayedMCDataGroup | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node is a placeholder for the allowed relayed MCData groups. | | | | |

### 9.2.33 /*<x>*/OnNetwork/RelayedMCDataGroup/<x>

Table 9.2.33.1: /*<x>*/OnNetwork/RelayedMCDataGroup/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/RelayedMCDataGroup/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more allowed relayed MCData groups. | | | | |

### 9.2.34 /*<x>*/OnNetwork/RelayedMCDataGroup/<x>/MCDataGroupID

Table 9.2.34.1: /*<x>*/OnNetwork/RelayedMCDataGroup/<x>/MCDataGroupID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/RelayedMCDataGroup/<x>/MCDataGroupID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the associated MCData group ID. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 9.2.35 /*<x>*/OnNetwork/RelayedMCDataGroup/<x>/RelayServiceCode

Table 9.2.35.1: /*<x>*/OnNetwork/RelayedMCDataGroup/<x>/RelayServiceCode

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/RelayedMCDataGroup/<x>/RelayServiceCode | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the connectivity service that the ProSe UE-to-network relay provides to public safety applications as specified in 3GPP TS 23.303 [6]. | | | | |

# 10 MCData user profile MO

## 10.1 General

The MCData user profile configuration Management Object (MO) is used to configure the MCData Client behaviour for the on-network or off-network MCData Service. The MCData user profile configuration parameters may be stored in the ME, or in the USIM as specified in 3GPP TS 31.102 [10], or in both the ME and the USIM. If both the ME and the USIM contain the same parameters, the values stored in the USIM shall take precedence.

The Management Object Identifier is: urn:oma:mo:ext-3gpp-MCData-user-profile:1.0.

Protocol compatibility: This MO is compatible with OMA OMA DM 1.2 [3].

The OMA DM ACL property mechanism (see OMA OMA-ERELD-DM-V1\_2 [2]) may be used to grant or deny access rights to OMA DM servers in order to modify nodes and leaf objects of the MCData user profile MO.

The following nodes and leaf objects are possible under the MCData user profile node as described in figures 10.1.1 through 10.1.4.



Figure 10.1.1: The MCData user profile MO (1 of 4)



Figure 10.1.2: The MCData user profile MO (2 of 4)



Figure 10.1.3: The MCData user profile MO (3 of 4)



Figure 10.1.4: The MCData user profile MO (4 of 4)

## 10.2 MCData user profile MO parameters

### 10.2.1 General

This clause describes the parameters for the MCData user profile Management Object (MO).

### 10.2.2 Node: *<x>*

Table 10.2.2.1: Node: *<x>*

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get |  |
|  | This interior node acts as a placeholder for the MCData user profile Management Object (MO).  For the MCData user profile MO, the namespace specific string is: "urn:oma:mo:oma-dm-mcdata-user-profile:1.0" | | | | |

- Values: N/A

### 10.2.3 /*<x>*/Name

Table 10.2.3.1: /*<x>*/Name

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | chr | Get |  |
|  | The Name leaf is a name for the MCData user profile settings. | | | | |

- Values: <User displayable name>

### 10.2.4 /*<x>*/Ext/

Table 10.2.4.1: /*<x>*/Ext/

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Ext | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | The Ext is an interior node for where the vendor specific information about the MCData user profile MO is being placed. | | | | |

Usually the vendor extension is identified by vendor specific name under the ext node and contains the vendor meaning application vendor, device vendor etc. The tree structure under the vendor identified is not defined and can therefore include one or more un-standardized sub-trees.

- Values: N/A

### 10.2.5 /*<x>*/<x>

Table 10.2.5.1: /*<x>*/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get, Replace |  |
|  | This interior node represents a container for on-network operation and off-network operation. | | | | |

### 10.2.6 /*<x>*/<x>/Common

Table 10.2.6.1: /*<x>*/<x>/Common

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node represents a container for the common network operation which means both on-network operation and off-network operation. | | | | |

### 10.2.7 /*<x>*/*<x>*/Common/MCDataUserID

Table 10.2.7.1: /*<x>*/<x>/Common/MCDataUserID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCDataUserID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates an MCData user identity (MCData ID) which is a globally unique identifier within the MCData service that represents the MCData user. | | | | |

### 10.2.8 /*<x>*/*<x>*/Common/MCDataUserProfileIndex

Table 10.2.8.1: /*<x>*/<x>/Common/MCDataUserProfileIndex

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCDataUserProfileIndex | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates an index for the particular MCData user profile. | | | | |

- Values: 0-255

### 10.2.9 /*<x>*/*<x>*/Common/MCDataUserProfileName

Table 10.2.9.1: /*<x>*/<x>/Common/MCDataUserProfileName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCDataUserProfileName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates a profile name for the particular MCData user profile. | | | | |

### 10.2.9A /*<x>*/*<x>*/Common/MCDataUserIDKMSURI

Table 10.2.9A.1: /*<x>*/<x>/Common/MCDataUserIDKMSURI

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCDataUserIDKMSURI | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates key management server URI for the security domain of the MCData user. | | | | |

The value is a URI as specified in 3GPP TS 23.003 [5].

### 10.2.10 /*<x>*/*<x>*/Common/PreSelectedIndication

Table 10.2.10.1: /*<x>*/<x>/Common/PreSelectedIndication

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PreSelectedIndication | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | null | Get, Replace |  |
|  | This leaf node indicates that this MCData user profile MO is designated to be the pre-selected MCData user profile as defined by 3GPP TS 23.179 [15] | | | | |

- Values: null

When this leaf node is present, this MCData user profile MO is designated as the pre-selected MCData user profile.

When this leaf node is absent, this MCData user profile MO is not designated as the pre-selected MCData user profile.

If more than one MCData user profile MO is specified for the MCData user, then only one MCData user profile MO for the MCData user shall contain the <x>/Common/PreSelectedIndication leaf node.

If there is only one MCData user profile MO specified for the MCData user, then it is optional to include the <x>/Common/PreSelectedIndication leaf node.

### 10.2.11 /*<x>*/<x>/Common/UserAliases

Table 10.2.11.1: /*<x>*/<x>/Common/UserAliases

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/UserAliases | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for a list of aliases of an MCData user. | | | | |

### 10.2.12 /*<x>*/<x>/Common/UserAliases/<x>

Table 10.2.12.1: /*<x>*/<x>/Common/UserAliases/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/UserAliases/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more aliases of an MCData user. | | | | |

### 10.2.13 /*<x>*/*<x>*/Common/UserAliases/<x>UserAlias

Table 10.2.13.1: /*<x>*/<x>/Common/UserAliases/<x>/UserAlias

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/UserAliases/<x>/UserAlias | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates an alphanumeric alias of the MCData user. | | | | |

### 10.2.14 /*<x>*/*<x>*/Common/AuthorisedAlias

Table 10.2.14.1: /*<x>*/<x>/Common/AuthorisedAlias

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/AuthorisedAlias | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | bool | Get, Replace |  |
|  | This leaf node indicates authorisation to create and delete aliases of other MCData users and their associated MCData user profiles. | | | | |

When set to "true" the MCData user is authorised to create and delete aliases of other MCData users and their associated MCData user profiles.

When set to "false" the MCData user is not authorised to create and delete aliases of other MCData user and their associated MCData user profiles. This is the default if this leaf node is not present.

### 10.2.15 /*<x>*/<x>/Common/ParticipantType

Table 10.2.15.1: /*<x>*/<x>/Common/ParticipantType

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| *<x>*/Common/ParticipantType | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the participant type of the MCData user. | | | | |

The ParticipantType means the functional category of the participant (e.g., first responder, second responder, dispatch, dispatch supervisor), typically defined by the MCData administrators.

### 10.2.16 /*<x>*/<x>/Common/Organization

Table 10.2.16.1: /*<x>*/<x>/Common/Organization

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/Organization | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the organization an MCData user belongs to. | | | | |

### 10.2.16A /*<x>*/*<x>*/Common/OnetoOne

Table 10.2.16A.1: /*<x>*/<x>/Common/OnetoOne

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/OnetoOne | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the MCData on-network or off-network one-to-one communication configuration. | | | | |

### 10.2.16B /*<x>*/<x>/Common/OnetoOne/UserList

Table 10.2.16B.1: /*<x>*/<x>/Common/OnetoOne/UserList

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/OnetoOne/UserList | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for a list of MCData users who can be involved in an on-network or off-network MCData one-to-one transaction. | | | | |

### 10.2.16C /*<x>*/<x>/Common/OnetoOne/UserList/<x>

Table 10.2.16C.1: /*<x>*/<x>/Common/OnetoOne/UserList/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/OnetoOne/UserList/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more list of MCData users who can be involved in an on-network or off-network MCData one-to-one transaction. | | | | |

### 10.2.16D /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry

Table 10.2.16D.1: /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/OnetoOne/UserList/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more MCData users who can be involved in an on-network or off-network MCData one-to-one transaction. | | | | |

### 10.2.16E /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry/MCDataID

Table 10.2.16E.1: /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry/MCDataID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/OnetoOne/UserList/<x>/Entry/MCDataID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates an MCData user identity (MCData ID) which is a globally unique identifier within the MCData service that represents the MCData user. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 10.2.16F /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry/ DiscoveryGroupID

Table 10.2.16F.1: /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry/DiscoveryGroupID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/OnetoOne/UserList/<x>/Entry/DiscoveryGroupID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | int | Get, Replace |  |
|  | This leaf node indicates a discovery group ID as specified in 3GPP TS 23.303 [6]. | | | | |

The value is used as the discovery group ID in the ProSe discovery procedures as specified in 3GPP TS 23.303 [6].

### 10.2.16G /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry/UserInfoID

Table 10.2.16G.1: /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry/UserInfoID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/OnetoOne/UserList/<x>/Entry/UserInfoID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | int | Get, Replace |  |
|  | This leaf node indicates a ProSe user info ID as specified in 3GPP TS 23.303 [6]. | | | | |

### 10.2.16H /*<x>*/*<x>*/Common/OnetoOne/UserList/<x>/Entry/ MCDataIDKMSURI

Table 10.2.16H.1: /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry/MCDataUserIDKMSURI

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/OnetoOne/UserList/<x>/Entry/MCDataUserIDKMSURI | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates key management server URI for the security domain of the MCData user of an MCData user that the configured MCData user is authorised to initiate a one-to-one communication with. | | | | |

The value is a URI as specified in 3GPP TS 23.003 [5].

### 10.2.16I /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry/DisplayName

Table 10.2.16I.1: /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/OnetoOne/UserList/<x>/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name. | | | | |

### 10.2.16J /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation

Table 10.2.16J.1: /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more list of IPInformation data that can be used in the setup of an IP Connectivity session for a specific MCData user in a one-to-one communication. | | | | |

### 10.2.16K /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry/ IPInformation/<x>

Table 10.2.16K.1: /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more list of IPInformation data that can be used in the setup of an IP Connectivity session for a specific MCData user in a one-to-one communication. | | | | |

### 10.2.16L /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry/ IPInformation/<x>Entry

Table 10.2.16L.1: /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more list of IPInformation data that can be used in the setup of an IP Connectivity session for a specific MCData user in a one-to-one communication. | | | | |

### 10.2.16M /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry/ IPInformation/<x>Entry/IPv4Information

Table 10.2.16M.1: /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation/<x>/Entry/IPv4Information

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation/<x>/Entry/IPv4Information | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates an IPv4 host address or an IPv4 network that can be addressed on an IP Connectivity session in a one-to-one communication for a specific MCData ID. | | | | |

### 10.2.16N /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry/ IPInformation/<x>Entry/IPv6Information

Table 10.2.16N.1: /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation/<x>/Entry/IPv6Information

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation/<x>/Entry/IPv6Information | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates an IPv6 host address or an IPv6 network that can be addressed on an IP Connectivity session in a one-to-one communication for a specific MCData ID. | | | | |

### 10.2.16O /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry/ IPInformation/<x>Entry/FQDN

Table 10.2.16O.1: /*<x>*/<x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation/<x>/Entry/FQDN

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/OnetoOne/UserList/<x>/Entry/IPInformation/<x>/Entry/FQDN | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates a fully qualified domain name for a specific host or domain that can be addressed on an IP Connectivity session in a one-to-one communication for a specific MCData ID. | | | | |

### 10.2.17 /*<x>*/*<x>*/Common/FileDistribution

Table 10.2.17.1: /*<x>*/<x>/Common/FileDistribution

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/FileDistribution | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the MCData file distribution configuration. | | | | |

### 10.2.18 /*<x>*/<x>/Common/FileDistribution/CancelList

Table 10.2.18.1: /*<x>*/<x>/Common/FileDistribution/CancelList

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/FileDistribution/CancelList | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for a list of MCData user(s) this MCData user is allowed to cancel distribution of files beings sent or waiting to be sent. | | | | |

### 10.2.19 /*<x>*/<x>/Common/FileDistribution/CancelList/<x>

Table 10.2.19.1: /*<x>*/<x>/Common/FileDistribution/CancelList/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/FileDistribution/CancelList/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for zero or more list of MCData users this MCData user is allowed to cancel distribution of files beings sent or waiting to be sent. | | | | |

### 10.2.20 /*<x>*/<x>/Common/FileDistribution/CancelList/<x>/Entry

Table 10.2.20.1: /*<x>*/<x>/Common/FileDistribution/CancelList/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/FileDistribution/CancelList/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more MCData users this MCData user is allowed to cancel distribution of files beings sent or waiting to be sent. | | | | |

### 10.2.21 /*<x>*/<x>/Common/FileDistribution/CancelList/<x>/Entry/MCDataID

Table 10.2.21.1: /*<x>*/<x>/Common/FileDistribution/CancelList/<x>/Entry/MCDataID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/FileDistribution/CancelList/<x>/Entry/MCDataID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates an MCData user identity (MCData ID) which is a globally unique identifier within the MCData service that represents the MCData user. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 10.2.21A /*<x>*/<x>/Common/FileDistribution/CancelList/<x>/Entry/ MCDataIDKMSURI

Table 10.2.21A.1: /*<x>*/<x>/Common/FileDistribution/CancelList/<x>/Entry/MCDataIDKMSURI

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/FileDistribution/CancelList/<x>/Entry/MCDataIDKMSURI | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates key management server URI for the security domain of the MCData user of an MCData user that the configured MCData user is authorised to cancel distribution of files being sent or waiting to be sent. | | | | |

The value is a URI as specified in 3GPP TS 23.003 [5].

### 10.2.22 /*<x>*/<x>/Common/FileDistribution/CancelList/<x>/Entry/ DisplayName

Table 10.2.22.1: /*<x>*/<x>/Common/FileDistribution/CancelList/<x>/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/FileDistribution/CancelList/<x>/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name. | | | | |

### 10.2.23 /*<x>*/*<x>*/Common/TxRxControl

Table 10.2.23.1: /*<x>*/<x>/Common/TxRxControl

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/TxRxControl | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the MCData transmission and reception control configuration. | | | | |

### 10.2.24 /*<x>*/*<x>*/Common/TxRxControl/AuthorisedTransmit

Table 10.2.24.1: /*<x>*/<x>/Common/TxRxControl/AuthorisedTransmit

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/TxRxControl/AuthorisedTransmit | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to transmit data. | | | | |

When set to "true" the MCData user is authorised to transmit data.

When set to "false" the MCData user is not authorised to transmit data.

### 10.2.25 /<x>/<x>/Common/TxRxControl/MaxData1To1

Table 10.2.25.1: /<x>/<x>/Common/TxRxControl/MaxData1To1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/TxRxControl/MaxData1To1 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the maximum amount of data (in megabytes) that an MCData user can transmit in a single request during one-to-one communication. | | | | |

- Values: 0-65535

The MaxData1to1 size is in megabytes.

### 10.2.26 /<x>/<x>/Common/TxRxControl/MaxTime1To1

Table 10.2.26.1: /<x>/<x>/Common/TxRxControl/MaxTime1To1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/TxRxControl/MaxTime1To1 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the maximum amount of time that an MCData user can transmit for in a single request during one-to-one communication. | | | | |

- Values: 0-65535

The MaxTime1To1 time is in seconds.

### 10.2.27 /*<x>*/<x>/Common/TxRxControl/ReleaseList

Table 10.2.27.1: /*<x>*/<x>/Common/TxRxControl/ReleaseList

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/TxRxControl/ReleaseList | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for a list of MCData users that this MCData user is allowed to request release of an ongoing transmission. | | | | |

### 10.2.28 /*<x>*/<x>/Common/TxRxControl/ReleaseList/<x>

Table 10.2.28.1: /*<x>*/<x>/Common/TxRxControl/ReleaseList/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/TxRxControl/ReleaseList/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for zero or more list of MCData users this MCData user is allowed to request release of an ongoing transmission. | | | | |

### 10.2.29 /*<x>*/<x>/Common/TxRxControl/ReleaseList/<x>/Entry

Table 10.2.29.1: /*<x>*/<x>/Common/TxRxControl/ReleaseList/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/TxRxControl/ReleaseList/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more MCData users this MCData user is allowed to request release of an ongoing transmission. | | | | |

### 10.2.30 /*<x>*/<x>/Common/TxRxControl/ReleaseList/<x>/Entry/MCDataID

Table 10.2.30.1: /*<x>*/<x>/Common/TxRxControl/ReleaseList/<x>/Entry/MCDataID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/TxRxControl/ReleaseList/<x>/Entry/MCDataID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates an MCData user identity (MCData ID) which is a globally unique identifier within the MCData service that represents the MCData user. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 10.2.31 /*<x>*/<x>/Common/TxRxControl/ReleaseList/<x>/Entry/ DisplayName

Table 10.2.31.1: /*<x>*/<x>/Common/TxRxControl/ReleaseList/<x>/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/TxRxControl/ReleaseList/<x>/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name. | | | | |

### 10.2.32 /*<x>*/*<x>*/Common/MCDataGroupBroadcast

Table 10.2.32.1: /*<x>*/<x>/Common/MCDataGroupBroadcast

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCDataGroupBroadcast | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the group-broadcast group policy. | | | | |

### 10.2.33 /*<x>*/*<x>*/Common/MCDataGroupBroadcast/Authorised

Table 10.2.33.1: /*<x>*/<x>/Common/MCDataGroupBroadcast/Authorised

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCDataGroupBroadcast/Authorised | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to create a group-broadcast group. | | | | |

When set to "true" the MCData user is authorised to create a group-broadcast group.

When set to "false" the MCData user is not authorised to create a group-broadcast group.

### 10.2.34 /*<x>*/*<x>*/Common/UserBroadcast

Table 10.2.34.1: /*<x>*/<x>/Common/UserBroadcast

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/UserBroadcast | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the user-broadcast group policy. | | | | |

### 10.2.35 /*<x>*/*<x>*/Common/UserBroadcast/Authorised

Table 10.2.35.1: /*<x>*/<x>/Common/UserBroadcast/Authorised

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/UserBroadcast/Authorised | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to create a user-broadcast group. | | | | |

When set to "true" the MCData user is authorised to create a user-broadcast group.

When set to "false" the MCData user is not authorised to create a user-broadcast group.

### 10.2.36 /*<x>*/<x>/Common/GroupEmergencyAlert

Table 10.2.36.1: /*<x>*/<x>/Common/GroupEmergencyAlert

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/GroupEmergencyAlert | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for Group Emergency Alert configuration. | | | | |

### 10.2.37 /*<x>*/<x>/Common/GroupEmergencyAlert/Entry

Table 10.2.37.1: /*<x>*/<x>/Common/GroupEmergencyAlert/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/GroupEmergencyAlert/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the details of the MCData group of an MCData emergency alert. | | | | |

### 10.2.38 /*<x>*/*<x>*/Common/GroupEmergencyAlert/Entry/ID

Table 10.2.38.1: /*<x>*/<x>/Common/GroupEmergencyAlert/Entry/ID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/GroupEmergencyAlert/Entry/ID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the MCData group used upon certain criteria on initiation of an MCData emergency alert. | | | | |

### 10.2.39 /*<x>*/*<x>*/Common/GroupEmergencyAlert/Entry/DisplayName

Table 10.2.39.1: /*<x>*/<x>/Common/GroupEmergencyAlert/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/GroupEmergencyAlert/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name that corresponds to the ID. | | | | |

### 10.2.40 /*<x>*/*<x>*/Common/GroupEmergencyAlert/Entry/Usage

Table 10.2.40.1: /*<x>*/<x>/Common/GroupEmergencyAlert/Entry/Usage

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/GroupEmergencyAlert/Entry/Usage | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the criteria to determine when initiation of an MCData emergency alert uses the ID. | | | | |

The valid values are 'UseCurrentlySelectedGroup' and 'DedicatedGroup'.

When set to 'UseCurrentlySelectedGroup' then if the MCData user has currently selected an MCData group then use that MCData group for an on-network MCData emergency alert, if the MCData user does not have a currently selected MCData group then use the MCData group identified by the ID in clause 10.2.38 for an MCData emergency alert.

When set to 'DedicatedGroup' then use the MCData group identified by the ID in clause 10.2.38 for an MCData emergency alert.

### 10.2.41 /*<x>*/*<x>*/Common/AllowedActivateAlert

Table 10.2.41.1: /*<x>*/<x>/Common/AllowedActivateAlert

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/AllowedActivateAlert | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCData user is authorised to activate an emergency alert | | | | |

When set to "true" the MCData user is authorised to activate an emergency alert.

When set to "false" the MCData user is not authorised to activate an emergency alert.

### 10.2.42 /*<x>*/*<x>*/Common/AllowedCancelAlert

Table 10.2.42.1: /*<x>*/<x>/Common/AllowedCancelAlert

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/AllowedCancelAlert | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCData user is allowed to cancel an emergency alert. | | | | |

When set to "true" the MCData user is authorised to cancel an emergency alert.

When set to "false" the MCData user is not authorised to cancel an emergency alert.

### 10.2.43 /*<x>*/*<x>*/OnNetwork

Table 10.2.43.1: /*<x>*/<x>/OnNetwork

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | node | Get, Replace |  |
|  | This interior node represents a container for on-network operation. | | | | |

### 10.2.44 /*<x>*/*<x>*/OnNetwork/MCDataGroupList

Table 10.2.44.1: /*<x>*/<x>/OnNetwork/MCDataGroupList

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the list of on-network MCData groups that the MCData user is allowed to use. | | | | |

### 10.2.45 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>

Table 10.2.45.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more list of on-network MCData groups that the MCData user is allowed to use. | | | | |

### 10.2.46 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry

Table 10.2.46.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the details of the on-network MCData groups that the MCData user is allowed to use. | | | | |

### 10.2.47 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ MCDataGroupID

Table 10.2.47.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/MCDataGroupID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/MCDataGroupID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the MCData group ID for the on-network MCData group that the MCData user is allowed to use. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 10.2.48 /*<x>*/*<x>*/OnNetwork/MCDataGroupList/<x>/Entry/DisplayName

Table 10.2.48.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name that corresponds to the MCData Group ID. | | | | |

### 10.2.49 Void

### 10.2.50 Void

### 10.2.51 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/GMSServID

Table 10.2.51.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/GMSServID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/GMSServID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates the identity (URI) of the group management server hosting the MCData Group ID. | | | | |

### 10.2.52 Void

### 10.2.53 Void

### 10.2.54 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ IdMSTokenEndPoint

Table 10.2.54.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/IdMSTokenEndPoint

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/IdMSTokenEndPoint | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates the identity (URI) of the IDMS token endpoint for the MCData Group ID in the MCDataGroupList. If the value is empty, the IDMS identities (IDMSAuthEndpoint and IDMSTokenEndpoint) present in the MCS UE initial configuration MO are used. | | | | |

### 10.2.54A /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/GroupKMSURI

Table 10.2.54A.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/GroupKMSURI

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/GroupKMSURI | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates key management server URI for the security domain of the MCData group identity (MCData Group ID) of the on-network MCData group | | | | |

The value is a URI as specified in 3GPP TS 23.003 [5].

### 10.2.55 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RelativePresentationPriority

Table 10.2.55.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RelativePresentationPriority

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RelativePresentationPriority | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | int | Get, Replace |  |
|  | This leaf node indicates indicating the presentation priority of the on-network group for the MCData user relative to other on-network groups and on-network users. | | | | |

- Values: 0-255

The lowest RelativePresentationPriority value shall be considered as the MCData group transaction having the lowest priority for presentation among other group MCData and one-to-one user transactions.

### 10.2.55A /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation

Table 10.2.55A.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node is a placeholder for the rules that control automatic affiliation. | | | | |

### 10.2.55A0 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>

Table 10.2.55A0.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for the zero or more rules that control automatic affiliation. | | | | |

### 10.2.55A1 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/

Table 10.2.55A1.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the location portion of the rules that control automatic affiliation. | | | | |

### 10.2.55A2 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>

Table 10.2.55A2.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for the location portion of the rules that control automatic affiliation. | | | | |

### 10.2.55A3 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry

Table 10.2.55A3.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the location portion of the rules that control automatic affiliation. | | | | |

### 10.2.55A4 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea

Table 10.2.55A4.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |  |
|  | This interior node contains a geographical area which when entered by the MC service UE triggers evaluation of the rules. | | | | |  |

### 10.2.55A5 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea

Table 10.2.55A5.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |  |
|  | This interior node contains a geographical area described by a polygon. | | | | |  |

### 10.2.55A6 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea/<x>

Table 10.2.55A6.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea/<x>

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea/<x> | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | OneOrN | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the corners which define a polygon. The occurrence of this leaf node is "3 to 15" as per 3GPP TS 23.032 [21]. | | | | |  |

### 10.2.55A7 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea/<x>/PointCoordinateType

Table 10.2.55A7.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the type of the coordinates. | | | | |  |

### 10.2.55A8 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/ Longitude

Table 10.2.55A8.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the longitudinal coordinate of a corner. | | | | |  |

### 10.2.55A9 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/ Latitude

Table 10.2.55A9.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the latitudinal coordinate of a corner. | | | | |

### 10.2.55A10 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea

Table 10.2.55A10.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |  |
|  | This interior node contains a geographical area described by an ellipsoid arc. | | | | |  |

### 10.2.55A11 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Center

Table 10.2.55A11.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |  |

### 10.2.55A12 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType

Table 10.2.55A12.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |  |

### 10.2.55A13 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Longitude

Table 10.2.55A13.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Longitude

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Longitude | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the longitudinal coordinate of the center. | | | | |  |

### 10.2.55A14 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Latitude

Table 10.2.55A14.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Latitude

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Latitude | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the latitudinal coordinate of a center. | | | | |  |

### 10.2.55A15 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Radius

Table 10.2.55A15.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Radius

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center/Radius | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the radius of the ellipsoid arc. | | | | |  |

### 10.2.55A16 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/OffsetAngle

Table 10.2.55A16.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/OffsetAngle

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/OffsetAngle | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the offset angle of the ellipsoid arc. | | | | |  |

### 10.2.55A17 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/IncludedAngle

Table 10.2.55A17.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/IncludedAngle

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/IncludedAngle | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the included angle of the ellipsoid arc. | | | | |  |

### 10.2.55A18 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Speed

Table 10.2.55A18.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Speed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Speed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | One | node | Get, Replace |  |  |
|  | This interior node contains the speed. | | | | |  |

### 10.2.55A19 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Speed/MinimumSpeed

Table 10.2.55A19.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Speed/MinimumSpeed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Speed/MinimumSpeed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the minimum speed. | | | | |  |

- Values: non-negative integer in units of kilometers/hour.

### 10.2.55A20 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Speed/MaximumSpeed

Table 10.2.55A20.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Speed/MaximumSpeed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Speed/MaximumSpeed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the maximum speed. | | | | |  |

- Values: non-negative integer in units of kilometers/hour.

### 10.2.55A21 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Heading

Table 10.2.55A21.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Heading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Heading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | One | node | Get, Replace |  |  |
|  | This interior node contains the heading. | | | | |  |

### 10.2.55A22 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Heading/MinimumHeading

Table 10.2.55A22.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Heading/MinimumHeading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Heading/MinimumHeading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the minimum heading. | | | | |  |

- Values: 0-359

### 10.2.55A23 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Heading/MaximumHeading

Table 10.2.55A23.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Heading/MaximumHeading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Heading/MaximumHeading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the maximum heading. | | | | |  |

- Values: 0-359

### 10.2.55A24 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea

Table 10.2.55A24.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |  |
|  | This interior node contains a geographical area which when entered by the MC service UE triggers evaluation of the rules. | | | | |  |

### 10.2.55A25 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea

Table 10.2.55A25.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |  |
|  | This interior node contains a geographical area described by a polygon. | | | | |  |

### 10.2.55A26 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea/<x>

Table 10.2.55A26.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea/<x>

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea/<x> | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | OneOrN | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the corners which define a polygon. The occurrence of this leaf node is "3 to 15" as per 3GPP TS 23.032 [21]. | | | | |  |

### 10.2.55A27 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea/<x>/PointCoordinateType

Table 10.2.55A27.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the type of the coordinates. | | | | |  |

### 10.2.55A28 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/ Longitude

Table 10.2.55A28.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the longitudinal coordinate of a corner. | | | | |  |

### 10.2.55A29 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/ Latitude

Table 10.2.55A29.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the latitudinal coordinate of a corner. | | | | |

### 10.2.55A30 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea

Table 10.2.55A30.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |  |
|  | This interior node contains a geographical area described by an ellipsoid arc. | | | | |  |

### 10.2.55A31 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Center

Table 10.2.55A31.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |  |

### 10.2.55A32 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType

Table 10.2.55A32.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |  |

### 10.2.55A33 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Longitude

Table 10.2.55A33.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Longitude

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Longitude | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the longitudinal coordinate of the center. | | | | |  |

### 10.2.55A34 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Latitude

Table 10.2.55A34.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Latitude

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Latitude | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the latitudinal coordinate of a center. | | | | |  |

### 10.2.55A35 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Radius

Table 10.2.55A35.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Radius

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center/Radius | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the radius of the ellipsoid arc. | | | | |  |

### 10.2.55A36 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/OffsetAngle

Table 10.2.55A36.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/OffsetAngle

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/OffsetAngle | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the offset angle of the ellipsoid arc. | | | | |  |

### 10.2.55A37 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/IncludedAngle

Table 10.2.55A37.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/IncludedAngle

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/IncludedAngle | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the included angle of the ellipsoid arc. | | | | |  |

### 10.2.55A38 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Speed

Table 10.2.55A38.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Speed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Speed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | One | node | Get, Replace |  |  |
|  | This interior node contains the speed. | | | | |  |

### 10.2.55A39 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Speed/MinimumSpeed

Table 10.2.55A39.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Speed/MinimumSpeed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Speed/MinimumSpeed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the minimum speed. | | | | |  |

- Values: non-negative integer in units of kilometers/hour.

### 10.2.55A40 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Speed/MaximumSpeed

Table 10.2.55A40.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Speed/MaximumSpeed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Speed/MaximumSpeed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the maximum speed. | | | | |  |

- Values: non-negative integer in units of kilometers/hour.

### 10.2.55A41 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Heading

Table 5. 10.2.55A41.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Heading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Heading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | One | node | Get, Replace |  |  |
|  | This interior node contains the heading. | | | | |  |

### 10.2.55A42 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Heading/MinimumHeading

Table 10.2.55A42.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Heading/MinimumHeading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Heading/MinimumHeading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the minimum heading. | | | | |  |

- Values: 0-359

### 10.2.55A43 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Heading/MaximumHeading

Table 10.2.55A43.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Heading/MaximumHeading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Heading/MaximumHeading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the maximum heading. | | | | |  |

- Values: 0-359

### 10.2.55A44 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfActiveFunctionalAliases

Table 10.2.55A44.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfActiveFunctionalAliases

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfActiveFunctionalAliases | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the functional alias part of rules that control automatic affiliation. | | | | |

### 10.2.55A45 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfActiveFunctionalAliases/<x>

Table 10.2.55A45.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfActiveFunctionalAliases/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfActiveFunctionalAliases/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for the functional alias part of rules that control automatic affiliation. | | | | |

### 10.2.55A46 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfActiveFunctionalAliases/<x>/Entry

Table 10.2.55A46.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfActiveFunctionalAliases/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfActiveFunctionalAliases/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the functional alias part of rules that control automatic affiliation. | | | | |

### 10.2.55A47 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForAffiliation/<x>/ListOfActiveFunctionalAliases/<x>/Entry/ FunctionalAlias

Table 10.2.55A47.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfActiveFunctionalAliases/<x>/Entry/FunctionalAlias

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForAffiliation/<x>/ListOfActiveFunctionalAliases/<x>/Entry/FunctionalAlias | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | chr | Get, Replace |  |  |
|  | This leaf node contains a functional alias. | | | | |  |

### 10.2.55B /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation

Table 10.2.55B.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node is a placeholder for the rules that control automatic deaffiliation. | | | | |

### 10.2.55B0 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>

Table 10.2.55B0.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for the zero or more rules that control automatic deaffiliation. | | | | |

### 10.2.55B1 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/

Table 10.2.55B1.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the location portion of the rules that control automatic deaffiliation. | | | | |

### 10.2.55B2 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>

Table 10.2.55B2.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for the location portion of the rules that control automatic deaffiliation. | | | | |

### 10.2.55B3 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry

Table 10.2.55B3.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the location portion of the rules that control automatic deaffiliation. | | | | |

### 10.2.55B4 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea

Table 10.2.55B4.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |  |
|  | This interior node contains a geographical area which, when entered by the MC service UE triggers evaluation of the rules. | | | | |  |

### 10.2.55B5 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea

Table 10.2.55B5.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |  |
|  | This interior node contains a geographical area described by a polygon. | | | | |  |

### 10.2.55B6 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea/<x>

Table 10.2.55B6.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea/<x>

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea/<x> | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | OneOrN | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the corners which define a polygon. The occurrence of this leaf node is "3 to 15" as per 3GPP TS 23.032 [21]. | | | | |  |

### 10.2.55B7 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea/<x>/PointCoordinateType

Table 10.2.55B7.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesFordeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the type of the coordinates. | | | | |  |

### 10.2.55B8 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/ Longitude

Table 10.2.55B8.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the longitudinal coordinate of a corner. | | | | |  |

### 10.2.55B9 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/ Latitude

Table 10.2.55B9.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the latitudinal coordinate of a corner. | | | | |

### 10.2.55B10 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea

Table 10.2.55B10.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |  |
|  | This interior node contains a geographical area described by an ellipsoid arc. | | | | |  |

### 10.2.55B11 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Center

Table 10.2.55B11.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |  |

### 10.2.55B12 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType

Table 10.2.55B12.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |  |

### 10.2.55B13 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Longitude

Table 10.2.55B13.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Longitude

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Longitude | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the longitudinal coordinate of the center. | | | | |  |

### 10.2.55B14 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Latitude

Table 10.2.55B14.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Latitude

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Latitude | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the latitudinal coordinate of a center. | | | | |  |

### 10.2.55B15 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/Radius

Table 10.2.55B15.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Radius

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/Center/Radius | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the radius of the ellipsoid arc. | | | | |  |

### 10.2.55B16 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/OffsetAngle

Table 10.2.55B16.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/OffsetAngle

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/OffsetAngle | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the offset angle of the ellipsoid arc. | | | | |  |

### 10.2.55B17 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/EllipsoidArcArea/IncludedAngle

Table 10.2.55B17.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/IncludedAngle

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/EllipsoidArcArea/IncludedAngle | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the included angle of the ellipsoid arc. | | | | |  |

### 10.2.55B18 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry /EnterSpecificArea/Speed

Table 10.2.55B18.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Speed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Speed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | One | node | Get, Replace |  |  |
|  | This interior node contains the speed. | | | | |  |

### 10.2.55B19 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Speed/MinimumSpeed

Table 10.2.55B19.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Speed/MinimumSpeed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Speed/MinimumSpeed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the minimum speed. | | | | |  |

- Values: non-negative integer in units of kilometers/hour.

### 10.2.55B20 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Speed/MaximumSpeed

Table 10.2.55B20.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Speed/MaximumSpeed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Speed/MaximumSpeed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the maximum speed. | | | | |  |

- Values: non-negative integer in units of kilometers/hour.

### 10.2.55B21 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Heading

Table 10.2.55B21.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Heading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Heading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | One | node | Get, Replace |  |  |
|  | This interior node contains the heading. | | | | |  |

### 10.2.55B22 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Heading/MinimumHeading

Table 10.2.55B22.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Heading/MinimumHeading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Heading/MinimumHeading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the minimum heading. | | | | |  |

- Values: 0-359

### 10.2.55B23 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ EnterSpecificArea/Heading/MaximumHeading

Table 10.2.55B23.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Heading/MaximumHeading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/EnterSpecificArea/Heading/Maximum | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the maximum heading. | | | | |  |

- Values: 0-359

### 10.2.55B24 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea

Table 10.2.55B24.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |  |
|  | This interior node contains a geographical area which when entered by the MC service UE triggers evaluation of the rules. | | | | |  |

### 10.2.55B25 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea

Table 10.2.55B25.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |  |
|  | This interior node contains a geographical area described by a polygon. | | | | |  |

### 10.2.55B26 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea/<x>

Table 10.2.55B26.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea/<x>

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea/<x> | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | OneOrN | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the corners which define a polygon. The occurrence of this leaf node is "3 to 15" as per 3GPP TS 23.032 [21]. | | | | |  |

### 10.2.55B27 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea/<x>/PointCoordinateType

Table 10.2.55B27.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the type of the coordinates. | | | | |  |

### 10.2.55B28 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/ Longitude

Table 10.2.55B28.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the longitudinal coordinate of a corner. | | | | |  |

### 10.2.55B29 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/ Latitude

Table 10.2.55B29.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the latitudinal coordinate of a corner. | | | | |

### 10.2.55B30 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea

Table 10.2.55B30.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |  |
|  | This interior node contains a geographical area described by an ellipsoid arc. | | | | |  |

### 10.2.55B31 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Center

Table 10.2.55B31.1:  
/*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |  |

### 10.2.55B32 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType

Table 10.2.55B32.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |  |

### 10.2.55B33 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Longitude

Table 10.2.55B33.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Longitude

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Longitude | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the longitudinal coordinate of the center. | | | | |  |

### 10.2.55B34 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry /ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/ Latitude

Table 10.2.55B34.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Latitude

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Latitude | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the latitudinal coordinate of a center. | | | | |  |

### 10.2.55B35 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/Radius

Table 10.2.55B35.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Radius

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/Center/Radius | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the radius of the ellipsoid arc. | | | | |  |

### 10.2.55B36 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/OffsetAngle

Table 10.2.55B36.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/OffsetAngle

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/OffsetAngle | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the offset angle of the ellipsoid arc. | | | | |  |

### 10.2.55B37 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/EllipsoidArcArea/IncludedAngle

Table 10.2.55B37.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/IncludedAngle

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/EllipsoidArcArea/IncludedAngle | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the included angle of the ellipsoid arc. | | | | |  |

### 10.2.55B38 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Speed

Table 10.2.55B38.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Speed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Speed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | One | node | Get, Replace |  |  |
|  | This interior node contains the speed. | | | | |  |

### 10.2.55B39 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Speed/MinimumSpeed

Table 10.2.55B39.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Speed/MinimumSpeed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Speed/MinimumSpeed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the minimum speed. | | | | |  |

- Values: non-negative integer in units of kilometers/hour.

### 10.2.55B40 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Speed/MaximumSpeed

Table 10.2.55B40.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Speed/MaximumSpeed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Speed/MaximumSpeed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the maximum speed. | | | | |  |

- Values: non-negative integer in units of kilometers/hour.

### 10.2.55B41 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Heading

Table 10.2.55B41.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Heading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Heading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | One | node | Get, Replace |  |  |
|  | This interior node contains the heading. | | | | |  |

### 10.2.55B42 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Heading/MinimumHeading

Table 10.2.55B42.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Heading/MinimumHeading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Heading/MinimumHeading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the minimum heading. | | | | |  |

- Values: in the range 0-359.

### 10.2.55B43 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ ExitSpecificArea/Heading/MaximumHeading

Table 10.2.55B43.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Heading/MaximumHeading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfLocationCriteria/<x>/Entry/ExitSpecificArea/Heading/MaximumHeading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the maximum heading. | | | | |  |

- Values: 0-359

### 10.2.55B44 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfActiveFunctionalAliases

Table 10.2.55B44.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfActiveFunctionalAliases

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfActiveFunctionalAliases | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the functional alias part of rules that control automatic deaffiliation. | | | | |

### 10.2.55B45 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfActiveFunctionalAliases/<x>

Table 10.2.55B45.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfActiveFunctionalAliases/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfActiveFunctionalAliases/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for the functional alias part of rules that control automatic deaffiliation. | | | | |

### 10.2.55B46 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfActiveFunctionalAliases/<x>/Entry

Table 10.2.55B46.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfActiveFunctionalAliases/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfActiveFunctionalAliases/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the functional alias part of rules that control automatic deaffiliation. | | | | |

### 10.2.55B47 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ RulesForDeaffiliation/<x>/ListOfActiveFunctionalAliases/<x>/Entry/ FunctionalAlias

Table 10.2.55B47.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfActiveFunctionalAliases/<x>/Entry/FunctionalAlias

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/RulesForDeaffiliation/<x>/ListOfActiveFunctionalAliases/<x>/Entry/FunctionalAlias | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node contains a functional alias. | | | | |

### 10.2.55B48 /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ ManualDeaffiliationNotAllowedIfAffiliationRulesAreMet

Table 10.2.55B48.1: /*<x>*/<x>/OnNetwork/MCDataGroupList/<x>/Entry/ManualDeaffiliationNotAllowedIfAffiliationRulesAreMet

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataGroupList/<x>/Entry/ManualDeaffiliationNotAllowedIfAffiliationRulesAreMet | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCData user is authorised to deaffiliate if the affiliation criteria are met. | | | | |

### 10.2.56 /*<x>*/*<x>*/OnNetwork/ImplicitAffiliations

Table 10.2.56.1: /*<x>*/<x>/OnNetwork/ImplicitAffiliations

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/ImplicitAffiliations | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the implicit affiliation configuration. | | | | |

### 10.2.57 /*<x>*/<x>/OnNetwork/ImplicitAffiliations/<x>

Table 10.2.57.1: /*<x>*/<x>/OnNetwork/ImplicitAffiliations/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/ImplicitAffiliations/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for zero or more implicit affiliation configuration. | | | | |

### 10.2.58 /*<x>*/<x>/OnNetwork/ImplicitAffiliations/<x>/Entry

Table 10.2.58.1: /*<x>*/<x>/OnNetwork/ImplicitAffiliations/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/ImplicitAffiliations/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the details of the on-network MCData groups that the MCData user is implicitly affiliated to. | | | | |

### 10.2.59 /*<x>*/<x>/OnNetwork/ImplicitAffiliations/<x>/Entry/ MCDataGroupID

Table 10.2.59.1: /*<x>*/<x>/OnNetwork/ImplicitAffiliations/<x>/Entry/MCDataGroupID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/ImplicitAffiliations/<x>/Entry/MCDataGroupID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates a MCData group ID to which the MCData user is implicitly affiliated to. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 10.2.60 /*<x>*/*<x>*/OnNetwork/ImplicitAffiliations/<x>/Entry/ DisplayName

Table 10.2.60.1: /*<x>*/<x>/OnNetwork/ImplicitAffiliations/<x>/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/ImplicitAffiliations/<x>/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name that corresponds to the MCData Group ID. | | | | |

### 10.2.61 /*<x>*/*<x>*/OnNetwork/PresenceStatus

Table 10.2.61.1: /*<x>*/<x>/OnNetwork/PresenceStatus

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/PresenceStatus | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the presence status configuration. | | | | |

### 10.2.62 /*<x>*/<x>/OnNetwork/PresenceStatus/<x>

Table 10.2.62.1: /*<x>*/<x>/OnNetwork/PresenceStatus/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/PresenceStatus/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for zero or more presence status configuration. | | | | |

### 10.2.63 /*<x>*/<x>/OnNetwork/PresenceStatus/<x>/Entry

Table 10.2.63.1: /*<x>*/<x>/OnNetwork/PresenceStatus/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/PresenceStatus/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the details of the MCData IDs of MCData users that the configured MCData user is authorised to obtain presence status. | | | | |

### 10.2.64 /*<x>*/<x>/OnNetwork/PresenceStatus/<x>/Entry/MCDataID

Table 10.2.64.1: /*<x>*/<x>/OnNetwork/PresenceStatus/<x>/Entry/MCDataID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/PresenceStatus/<x>/Entry/MCDataID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates an MCData ID of an MCData user that the configured MCData user is authorised to obtain presence status. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 10.2.65 /*<x>*/*<x>*/OnNetwork/PresenceStatus/<x>/Entry/ DisplayName

Table 10.2.65.1: /*<x>*/<x>/OnNetwork/PresenceStatus/<x>/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/PresenceStatus/<x>/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name that corresponds to the MCData ID. | | | | |

### 10.2.66 /*<x>*/*<x>*/OnNetwork/RemoteGroupChange

Table 10.2.66.1: /*<x>*/<x>/OnNetwork/RemoteGroupChange

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/RemoteGroupChange | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the remote group change configuration. | | | | |

### 10.2.67 /*<x>*/<x>/OnNetwork/RemoteGroupChange/<x>

Table 10.2.67.1: /*<x>*/<x>/OnNetwork/RemoteGroupChange/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/RemoteGroupChange/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for zero or more remote group change configuration. | | | | |

### 10.2.68 /*<x>*/<x>/OnNetwork/RemoteGroupChange/<x>/Entry

Table 10.2.68.1: /*<x>*/<x>/OnNetwork/RemoteGroupChange/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/RemoteGroupChange/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the details of the MCData IDs of MCData users whose selected groups are authorised to be remotely changed by the configured MCData user. | | | | |

### 10.2.69 /*<x>*/<x>/OnNetwork/RemoteGroupChange/<x>/Entry/ MCDataID

Table 10.2.69.1: /*<x>*/<x>/OnNetwork/RemoteGroupChange/<x>/Entry/MCDataID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/RemoteGroupChange/<x>/Entry/MCDataID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates an MCData ID of an MCData user whose selected groups are authorised to be remotely changed by the configured MCData user. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 10.2.70 /*<x>*/*<x>*/OnNetwork/RemoteGroupChange/<x>/Entry/ DisplayName

Table 10.2.70.1: /*<x>*/<x>/OnNetwork/RemoteGroupChange/<x>/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/RemoteGroupChange/<x>/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name that corresponds to the MCData ID. | | | | |

### 10.2.71 /*<x>*/<x>/OnNetwork/MaxAffiliationsN2

Table 10.2.71.1: /*<x>*/<x>/OnNetwork/MaxAffiliationsN2

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MaxAffiliationsN2 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | int | Get, Replace |  |
|  | This leaf node indicates the maximum number of MCData groups that the MCData user is authorised to affiliate with. | | | | |

- Values: 0-65535

### 10.2.72 /*<x>*/*<x>*/OnNetwork/ConversationManagement

Table 10.2.72.1: /*<x>*/<x>/OnNetwork/ConversationManagement

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/ConversationManagement | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for conversation management configuration | | | | |

### 10.2.73 /*<x>*/<x>/OnNetwork/ConversationManagement/ GroupHangTime

Table 10.2.73.1: /*<x>*/<x>/OnNetwork/ConversationManagement/GroupHangTime

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/ConversationManagement/GroupHangTime | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for group hang time configuration | | | | |

### 10.2.74 /*<x>*/<x>/OnNetwork/ConversationManagement/ GroupHangTime/<x>

Table 10.2.74.1: /*<x>*/<x>/OnNetwork/ConversationManagement/GroupHangTime/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/ConversationManagement/GroupHangTime/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more hang time configurations. | | | | |

### 10.2.75 /*<x>*/<x>/OnNetwork/ConversationManagement/ GroupHangTime/<x>/Entry

Table 10.2.75.1: /*<x>*/<x>/OnNetwork/ConversationManagement/GroupHangTime/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/ConversationManagement/GroupHangTime/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the conversation hang time configuration associated with the configured MCData group, for the MCData user. | | | | |

### 10.2.76 /*<x>*/<x>/OnNetwork/ConversationManagement/ GroupHangTime/<x>/Entry/MCDataGroupID

Table 10.2.76.1: /*<x>*/<x>/OnNetwork/ConversationManagement/GroupHangTime/<x>/Entry/MCDataGroupID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/ConversationManagement/GroupHangTime/<x>/Entry/MCDataGroupID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the MCData group ID for the on-network MCData group. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 10.2.77 /*<x>*/*<x>*/OnNetwork/ConversationManagement/ GroupHangTime/<x>/Entry/DisplayName

Table 10.2.77.1: /*<x>*/<x>/OnNetwork/ConversationManagement/GroupHangTime/<x>/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/ConversationManagement/GroupHangTime/<x>/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name that corresponds to the MCData Group ID. | | | | |

### 10.2.78 /*<x>*/<x>/OnNetwork/ConversationManagement/ GroupHangTime/<x>/Entry/HangTime

Table 10.2.78.1: /*<x>*/<x>/OnNetwork/ConversationManagement/GroupHangTime/<x>/Entry/HangTime

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/ConversationManagement/GroupHangTime/<x>/Entry/HangTime | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the group call hang timer of the MCData group for conversation management, for the MCData user. | | | | |

- Values: 0-65535

The HangTime is in seconds.

### 10.2.79 /*<x>*/<x>/OnNetwork/ConversationManagement/ DeliveredDisposition

Table 10.2.79.1: /*<x>*/<x>/OnNetwork/ConversationManagement/DeliveredDisposition

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/ConversationManagement/DeliveredDisposition | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for delivered disposition configuration | | | | |

### 10.2.80 /*<x>*/<x>/OnNetwork/ConversationManagement/ DeliveredDisposition/<x>

Table 10.2.80.1: /*<x>*/<x>/OnNetwork/ConversationManagement/DeliveredDisposition/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/ConversationManagement/DeliveredDisposition/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for zero or more delivered disposition configurations. | | | | |

### 10.2.81 /*<x>*/<x>/OnNetwork/ConversationManagement/ DeliveredDisposition/<x>/Entry

Table 10.2.81.1: /*<x>*/<x>/OnNetwork/ConversationManagement/DeliveredDisposition/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/ConversationManagement/DeliveredDisposition/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the delivered disposition configuration associated with the MCData user, indicating an MCData ID of an MCData user who is to be sent a message delivered disposition notification in addition to the message sender. | | | | |

### 10.2.82 /*<x>*/<x>/OnNetwork/ConversationManagement/ DeliveredDisposition/<x>/Entry/MCDataID

Table 10.2.82.1: /*<x>*/<x>/OnNetwork/ConversationManagement/DeliveredDisposition/<x>/Entry/MCDataID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/ConversationManagement/DeliveredDisposition/<x>/Entry/MCDataID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the MCData ID for the on-network MCData user. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 10.2.83 /*<x>*/*<x>*/OnNetwork/ConversationManagement/ DeliveredDisposition/<x>/Entry/DisplayName

Table 10.2.83.1: /*<x>*/<x>/OnNetwork/ConversationManagement/DeliveredDisposition/<x>/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/ConversationManagement/DeliveredDisposition/<x>/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name that corresponds to the MCData ID. | | | | |

### 10.2.84 /*<x>*/<x>/OnNetwork/ConversationManagement/ ReadDisposition

Table 10.2.84.1: /*<x>*/<x>/OnNetwork/ConversationManagement/ReadDisposition

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/ConversationManagement/ReadDisposition | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for read disposition configuration | | | | |

### 10.2.85 /*<x>*/<x>/OnNetwork/ConversationManagement/ ReadDisposition/<x>

Table 10.2.85.1: /*<x>*/<x>/OnNetwork/ConversationManagement/ReadDisposition/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/ConversationManagement/ReadDisposition/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for zero or more read disposition configurations. | | | | |

### 10.2.86 /*<x>*/<x>/OnNetwork/ConversationManagement/ ReadDisposition/<x>/Entry

Table 10.2.86.1: /*<x>*/<x>/OnNetwork/ConversationManagement/ReadDisposition/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/ConversationManagement/ReadDisposition/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the read disposition configuration associated with the MCData user, indicating an MCData ID of an MCData user who is to be sent a message read disposition notification in addition to the message sender. | | | | |

### 10.2.87 /*<x>*/<x>/OnNetwork/ConversationManagement/ ReadDisposition/<x>/Entry/MCDataID

Table 10.2.87.1: /*<x>*/<x>/OnNetwork/ConversationManagement/ReadDisposition/<x>/Entry/MCDataID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/ConversationManagement/ReadDisposition/<x>/Entry/MCDataID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the MCData ID for the on-network MCData user. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 10.2.88 /*<x>*/*<x>*/OnNetwork/ConversationManagement/ ReadDisposition/<x>/Entry/DisplayName

Table 10.2.88.1: /*<x>*/<x>/OnNetwork/ConversationManagement/ReadDisposition/<x>/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/ConversationManagement/ReadDisposition/<x>/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name that corresponds to the MCData ID. | | | | |

### 10.2.89 /*<x>*/<x>/OnNetwork/OneToOneEmergencyAlert

Table 10.2.89.1: /*<x>*/<x>/OnNetwork/OneToOneEmergencyAlert

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/OneToOneEmergencyAlert | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for on-network one-to-one emergency alert configuration. | | | | |

### 10.2.90 /*<x>*/<x>/OnNetwork/OneToOneEmergencyAlert/Entry

Table 10.2.90.1: /*<x>*/<x>/OnNetwork/OneToOneEmergencyAlert/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/OneToOneEmergencyAlert/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the details of the MCData ID of an MCData emergency alert. | | | | |

### 10.2.91 /*<x>*/*<x>*/OnNetwork/OneToOneEmergencyAlert/Entry/ID

Table 10.2.91.1: /*<x>*/<x>/OnNetwork/OneToOneEmergencyAlert/Entry/ID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/OneToOneEmergencyAlert/Entry/ID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the MCData user ID used upon certain criteria on initiation of a one-to-one MCData emergency alert. | | | | |

### 10.2.92 /*<x>*/*<x>*/OnNetwork/OneToOneEmergencyAlert/Entry/ DisplayName

Table 10.2.92.1: /*<x>*/<x>/OnNetwork/OneToOneEmergencyAlert/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/OneToOneEmergencyAlert/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name that corresponds to the ID. | | | | |

### 10.2.93 /*<x>*/*<x>*/OnNetwork/OneToOneEmergencyAlert/Entry/Usage

Table 10.2.93.1: /*<x>*/<x>/OnNetwork/OneToOneEmergencyAlert/Entry/Usage

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/OneToOneEmergencyAlert/Entry/Usage | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the criteria to determine when initiation of an MCData emergency alert uses the ID. | | | | |

The valid values are 'LocallyDetermined' and 'UsePreConfigured'.

When set to 'LocallyDetermined' then if the MCData user selects an MCData ID then use that MCData ID for an on-network MCData emergency alert, if the MCData user does not select a MCData ID then use the MCData ID identified by the ID in clause 10.2.91 for an on-network MCData emergency alert.

When set to 'UsePreConfigured' then use the ID identified by the ID in clause 10.2.91 for an on-network MCData emergency alert.

### 10.2.94 /*<x>*/*<x>*/OnNetwork/AllowedRegroup

Table 10.2.94.1: /*<x>*/<x>/OnNetwork/AllowedRegroup

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/AllowedRegroup | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCData user is authorised to perform dynamic regrouping operations. | | | | |

When set to "true" the MCData user is authorised to perform dynamic regrouping operations.

When set to "false" the MCData user is not authorised to perform dynamic regrouping operations.

### 10.2.95 /*<x>*/*<x>*/OnNetwork/AllowedPresenceStatus

Table 10.2.95.1: /*<x>*/<x>/OnNetwork/AllowedPresenceStatus

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/AllowedPresenceStatus | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | bool | Get, Replace |  |
|  | This leaf node indicates the presence status on the network of this MCData user is available. | | | | |

When set to "true" the presence status on the network of this MCData user is available.

When set to "false" the presence status on the network of this MCData user is not available. This is the default if this leaf node is not present.

### 10.2.96 /*<x>*/*<x>*/OnNetwork/AllowedPresence

Table 10.2.96.1: /*<x>*/<x>/OnNetwork/AllowedPresence

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/AllowedPresence | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCData user is authorised to obtain whether a particular MCData User is present on the network. | | | | |

When set to "true" the MCData user is authorised to obtain whether a particular MCData User is present on the network.

When set to "false" the MCData user is not authorised to obtain whether a particular MCData User is present on the network.

### 10.2.97 /*<x>*/*<x>*/OnNetwork/AllowedManualSwitch

Table 10.2.97.1: /*<x>*/<x>/OnNetwork/AllowedManualSwitch

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/AllowedManualSwitch | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCData user is authorised to manually switch to off-network operation while in on-network operation. | | | | |

When set to "true" the MCData user is authorised to manually switch to off-network operation while in on-network operation.

When set to "false" the MCData user is not authorised to manually switch to off-network operation while in on-network operation.

### 10.2.97A /*<x>*/<x>/OnNetwork/MCDataContentServerURI

Table 10.2.97A.1: /*<x>*/<x>/OnNetwork/MCDataContentServerURI

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCDataContentServerURI | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the absolute URI associated with the media storage function of the MCData content server. | | | | |

The value is a URI as specified in 3GPP TS 23.003 [5].

### 10.2.97B /*<x>*/*<x>*/OnNetwork/FunctionalAliasList

Table 10.2.97B.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the functional alias configuration. | | | | |

### 10.2.97B1 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>

Table 10.2.97B1.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more functional alias configuration elements. | | | | |

### 10.2.97B2 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry

Table 10.2.97B2.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the details of the functional alias. | | | | |

### 10.2.97B3 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ FunctionalAlias

Table 10.2.97B3.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/FunctionalAlias

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/FunctionalAlias | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates a functional alias that can be activated by the MCData user. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 10.2.97B3A /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ DisplayName

Table 10.2.97B3A.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name that corresponds to a functional alias that can be activated by the MCData user. | | | | |

### 10.2.97B3B /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation

Table 10.2.97B3B.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node contains the location criteria for activation of a functional alias. | | | | |

### 10.2.97B3B0 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>

Table 10.2.97B3B0.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrMore | node | Get, Replace |  |
|  | This interior node contains the zero or more location criteria for activation of a functional alias. | | | | |

### 10.2.97B3B1 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea

Table 10.2.97B3B1.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node contains a geographical area which when entered by the MC service UE triggers the functional alias activation. | | | | |

### 10.2.97B3B2 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/PolygonArea

Table 10.2.97B3B2.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/PolygonArea

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/PolygonArea | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node contains a geographical area described by a polygon. | | | | |

### 10.2.97B3B3 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/PolygonArea/ <x>

Table 10.2.97B3B3.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/PolygonArea/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/PolygonArea/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrN | node | Get, Replace |  |
|  | This interior node contains the coordinates of the corners which define a polygon. The occurrence of this leaf node is "3 to 15" as per 3GPP TS 23.032 [21]. | | | | |

### 10.2.97B3B4 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/PolygonArea/ <x>/PointCoordinateType

Table 10.2.97B3B4.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |  |

### 10.2.97B3B5 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/PolygonArea/ <x>/PointCoordinateType/Longitude

Table 10.2.97B3B5.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the longitudinal coordinate of a corner. | | | | |

- Values: 0-16777215

### 10.2.97B3B6 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/PolygonArea/ <x>/PointCoordinateType/Latitude

Table 10.2.97B3B6.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the latitudinal coordinate of a corner. | | | | |

- Values: 0-16777215

### 10.2.97B3B7 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ EllipsoidArcArea

Table 10.2.97B3B7.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/EllipsoidArcArea

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/EllipsoidArcArea | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node contains a geographical area described by an ellipsoid arc. | | | | |

### 10.2.97B3B8 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Center

Table 10.2.97B3B8.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/EllipsoidArcArea/Center

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/EllipsoidArcArea/Center | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |

### 10.2.97B3B9 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType

Table 10.2.97B3B9.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |  |

### 10.2.97B3B10 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType/Longitude

Table 10.2.97B3B8.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Longitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Longitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the longitudinal coordinate of the center. | | | | |

- Values: 0-16777215

### 10.2.97B3B11 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType/Latitude

Table 10.2.97B3B11.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Latitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Latitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the latitudinal coordinate of the center. | | | | |

- Values: 0-16777215

### 10.2.97B3B12 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Radius

Table 10.2.97B3B12.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/EllipsoidArcArea/Radius

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/EllipsoidArcArea/Radius | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the radius of the ellipsoid arc. | | | | |

- Values: non-negative integer

### 10.2.97B3B13 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ EllipsoidArcArea/OffsetAngle

Table 10.2.97B3B13.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/EllipsoidArcArea/OffsetAngle

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/EllipsoidArcArea/OffsetAngle | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the offset angle of the ellipsoid arc. | | | | |

- Values: 0-255

### 10.2.97B3B14 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/ EllipsoidArcArea/IncludedAngle

Table 10.2.97B3B14.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/EllipsoidArcArea/IncludedAngle

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/EllipsoidArcArea/IncludedAngle | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the included angle of the ellipsoid arc. | | | | |

- Values: 0-255

### 10.2.97B3B15 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/Speed

Table 10.2.97B3B15.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/Speed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/Speed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | One | node | Get, Replace |  |  |
|  | This interior node contains the speed. | | | | |  |

### 10.2.97B3B16 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/Speed/ MinimumSpeed

Table 10.2.97B3B16.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/Speed/MinimumSpeed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/Speed/MinimumSpeed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the minimum speed. | | | | |  |

- Values: non-negative integer in units of kilometers/hour.

### 10.2.97B3B17 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/Speed/ MaximumSpeed

Table 10.2.97B3B17.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/Speed/MaximumSpeed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/Speed/MaximumSpeed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the maximum speed. | | | | |  |

- Values: non-negative integer in units of kilometers/hour.

### 10.2.97B3B18 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/Heading

Table 10.2.97B3B18.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/Heading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/Heading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | One | node | Get, Replace |  |  |
|  | This interior node contains the heading. | | | | |  |

### 10.2.97B3B19 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/Heading/ MinimumHeading

Table 10.2.97B3B19.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/Heading/MinimumHeading

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/Heading/MinimumHeading | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the minimum heading. | | | | |

- Values: 0-359

### 10.2.97B3B20 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/EnterSpecificArea/Heading/ MaximumHeading

Table 10.2.97B3B20.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/Heading/MaximumHeading

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/EnterSpecificArea/Heading/MaximumHeading | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the maximum heading. | | | | |

- Values: 0-359

### 10.2.97B3B21 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea

Table 10.2.97B3B21.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node contains a geographical area which when exited by the MC service UE triggers the functional alias activation. | | | | |

### 10.2.97B3B22 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/PolygonArea

Table 10.2.97B3B22.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/PolygonArea

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/PolygonArea | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node contains a geographical area described by a polygon. | | | | |

### 10.2.97B3B23 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/PolygonArea/ <x>

Table 10.2.97B3B23.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/PolygonArea/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/PolygonArea/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrN | node | Get, Replace |  |
|  | This interior node contains the coordinates of the corners which define a polygon. The occurrence of this leaf node is "3 to 15" as per 3GPP TS 23.032 [21]. | | | | |

### 10.2.97B3B24 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/PolygonArea/ <x>/PointCoordinateType

Table 10.2.97B3B24.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the type of the coordinates. | | | | |  |

### 10.2.97B3B25 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/PolygonArea/ <x>/PointCoordinateType/Longitude

Table 10.2.97B3B25.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the longitudinal coordinate of a corner. | | | | |

- Values: 0-16777215

### 10.2.97B3B26 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/PolygonArea/ <x>/PointCoordinateType/Latitude

Table 10.2.97B3B26.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the latitudinal coordinate of a corner. | | | | |

- Values: 0-16777215

### 10.2.97B3B27 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/ EllipsoidArcArea

Table 10.2.97B3B27.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/EllipsoidArcArea

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/EllipsoidArcArea | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node contains a geographical area described by an ellipsoid arc. | | | | |

### 10.2.97B3B28 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/ EllipsoidArcArea/Center

Table 10.2.97B3B28.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/EllipsoidArcArea/Center

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/EllipsoidArcArea/Center | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |

### 10.2.97B3B29 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType

Table 10.2.97B3B29.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |  |

### 10.2.97B3B30 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType/Longitude

Table 10.2.97B3B30.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Longitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Longitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the longitudinal coordinate of the center. | | | | |

- Values: 0-16777215

### 10.2.97B3B31 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType/Latitude

Table 10.2.97B3B31.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Latitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Latitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the latitudinal coordinate of the center. | | | | |

- Values: 0-16777215

### 10.2.97B3B32 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/ EllipsoidArcArea/Radius

Table 10.2.97B3B32.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/EllipsoidArcArea/Radius

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/EllipsoidArcArea/Radius | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the radius of the ellipsoid arc. | | | | |

- Values: non-negative integer

### 10.2.97B3B33 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/ EllipsoidArcArea/OffsetAngle

Table 10.2.97B3B33.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/EllipsoidArcArea/OffsetAngle

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/EllipsoidArcArea/OffsetAngle | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the offset angle of the ellipsoid arc. | | | | |

- Values: 0-255

### 10.2.97B3B34 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/ EllipsoidArcArea/IncludedAngle

Table 10.2.97B3B34.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/EllipsoidArcArea/IncludedAngle

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/EllipsoidArcArea/IncludedAngle | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the included angle of the ellipsoid arc. | | | | |

- Values: 0-255

### 10.2.97B3B35 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/Speed

Table 10.2.97B3B35.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/Speed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/Speed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | One | node | Get, Replace |  |  |
|  | This interior node contains the speed. | | | | |  |

### 10.2.97B3B36 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/Speed/ MinimumSpeed

Table 10.2.97B3B36.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/Speed/MinimumSpeed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/Speed/MinimumSpeed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the minimum speed. | | | | |  |

- Values: non-negative integer in units of kilometers/hour.

### 10.2.97B3B37 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/Speed/ MaximumSpeed

Table 10.2.97B3B37.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/Speed/MaximumSpeed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/Speed/MaximumSpeed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the maximum speed. | | | | |  |

- Values: non-negative integer in units of kilometers/hour.

### 10.2.97B3B38 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/Heading

Table 10.2.97B3B38.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/Heading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/Heading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | One | node | Get, Replace |  |  |
|  | This interior node contains the heading. | | | | |  |

### 10.2.97B3B39 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/Heading/ MinimumHeading

Table 10.2.97B3B39.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/Heading/MinimumHeading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/Heading/MinimumHeading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the minimum heading. | | | | |  |

- Values: 0-359

### 10.2.97B3B40 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForActivation/<x>/ExitSpecificArea/Heading/ MaximumHeading

Table 10.2.97B3B40.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/Heading/MaximumHeading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForActivation/<x>/ExitSpecificArea/Heading/MaximumumHeading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the maximum heading. | | | | |  |

- Values: 0-359

### 10.2.97B3C /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation

Table 10.2.97B3C.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node contains the location criteria for de-activation of a functional alias. | | | | |

### 10.2.97B3C0 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>

Table 10.2.97B3C0.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrMore | node | Get, Replace |  |
|  | This interior node contains the zero or more location criteria for de-activation of a functional alias. | | | | |

### 10.2.97B3C1 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea

Table 10.2.97B3C1.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node contains a geographical area which when entered by the MC service UE triggers the functional alias de-activation. | | | | |

### 10.2.97B3C2 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ PolygonArea

Table 10.2.97B3C2.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/PolygonArea

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/PolygonArea | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node contains a geographical area described by a polygon. | | | | |

### 10.2.97B3C3 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ PolygonArea/<x>

Table 10.2.97B3C3.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/PolygonArea/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/PolygonArea/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrN | node | Get, Replace |  |
|  | This interior node contains the coordinates of the corners which define a polygon. The occurrence of this leaf node is "3 to 15" as per 3GPP TS 23.032 [21]. | | | | |

### 10.2.97B3C4 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ PolygonArea/<x>/PointCoordinateType

Table 10.2.97B3C4.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |  |

### 10.2.97B3C5 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ PolygonArea/<x>/PointCoordinateType/Longitude

Table 10.2.97B3C5.1: /</<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the longitudinal coordinate of a corner. | | | | |

- Values: 0-16777215

### 10.2.97B3C6 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ PolygonArea/<x>/PointCoordinateType/Latitude

Table 10.2.97B3C6.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the latitudinal coordinate of a corner. | | | | |

- Values: 0-16777215

### 10.2.97B3C7 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ EllipsoidArcArea

Table 10.2.97B3C7.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/EllipsoidArcArea

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/EllipsoidArcArea | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node contains a geographical area described by an ellipsoid arc. | | | | |

### 10.2.97B3C8 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Center

Table 10.2.97B3C8.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/EllipsoidArcArea/Center

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/EllipsoidArcArea/Center | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |

### 10.2.97B3C9 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType

Table 10.2.97B3C9.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |  |

### 10.2.97B3C10 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType/Longitude

Table 10.2.97B3C10.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Longitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Longitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the longitudinal coordinate of the center. | | | | |

- Values: 0-16777215

### 10.2.97B3C11 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType/Latitude

Table 10.2.97B3C11.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Latitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Latitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the latitudinal coordinate of the center. | | | | |

- Values: 0-16777215

### 10.2.97B3C12 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ EllipsoidArcArea/Radius

Table 10.2.97B3C12.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/EllipsoidArcArea/Radius

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/EllipsoidArcArea/Radius | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the radius of the ellipsoid arc. | | | | |

- Values: non-negative integer

### 10.2.97B3C13 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ EllipsoidArcArea/OffsetAngle

Table 10.2.97B3C13.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/EllipsoidArcArea/OffsetAngle

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/EllipsoidArcArea/OffsetAngle | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the offset angle of the ellipsoid arc. | | | | |

- Values: 0-255

### 10.2.97B3C14 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/ EllipsoidArcArea/IncludedAngle

Table 10.2.97B3C14.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/EllipsoidArcArea/IncludedAngle

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/EllipsoidArcArea/IncludedAngle | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the included angle of the ellipsoid arc. | | | | |

- Values: 0-255

### 10.2.97B3C15 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Speed

Table 10.2.97B3C15.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Speed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Speed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | One | node | Get, Replace |  |  |
|  | This interior node contains the speed. | | | | |  |

### 10.2.97B3C16 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Speed/ MinimumSpeed

Table 10.2.97B3C16.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Speed/MinimumSpeed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Speed/MinimumSpeed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the minimum speed. | | | | |  |

- Values: non-negative integer in units of kilometers/hour.

### 10.2.97B3C17 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Speed/ MaximumSpeed

Table 10.2.97B3C17.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Speed/MaximumSpeed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Speed/MaximumSpeed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the maximum speed. | | | | |  |

- Values: non-negative integer in units of kilometers/hour.

### 10.2.97B3C18 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Heading

Table 10.2.97B3C18.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Heading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Heading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | One | node | Get, Replace |  |  |
|  | This interior node contains the heading. | | | | |  |

### 10.2.97B3C19 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Heading/ MinimumHeading

Table 10.2.97B3C19.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Heading/MinimumHeading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Heading/MinimumHeading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the minimum heading. | | | | |  |

- Values: 0-359

### 10.2.97B3C20 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Heading/ MaximumHeading

Table 10.2.97B3C20.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Heading/MaximumHeading

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/EnterSpecificArea/Heading/MaximumHeading | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the maximum heading. | | | | |

- Values: 0-359

### 10.2.97B3C21 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea

Table 10.2.97B3C21.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node contains a geographical area which when exited by the MC service UE triggers the functional alias de-activation. | | | | |

### 10.2.97B3C22 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/PolygonArea

Table 10.2.97B3C22.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/PolygonArea

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/PolygonArea | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node contains a geographical area described by a polygon. | | | | |

### 10.2.97B3C23 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/ PolygonArea/<x>

Table 10.2.97B3C23.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/PolygonArea/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/PolygonArea/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrN | node | Get, Replace |  |
|  | This interior node contains the coordinates of the corners which define a polygon. The occurrence of this leaf node is "3 to 15" as per 3GPP TS 23.032 [21]. | | | | |

### 10.2.97B3C24 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/ PolygonArea/<x>/PointCoordinateType

Table 10.2.97B3C24.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |  |

### 10.2.97B3C25 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/ PolygonArea/<x>/PointCoordinateType/Longitude

Table 10.2.97B3C25.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Longitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the longitudinal coordinate of a corner. | | | | |

- Values: 0-16777215

### 10.2.97B3C26 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/ PolygonArea/<x>/PointCoordinateType/Latitude

Table 10.2.97B3C26.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/PolygonArea/<x>/PointCoordinateType/Latitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the latitudinal coordinate of a corner. | | | | |

- Values: 0-16777215

### 10.2.97B3C27 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/ EllipsoidArcArea

Table 10.2.97B3C27.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/EllipsoidArcArea

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/EllipsoidArcArea | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node contains a geographical area described by an ellipsoid arc. | | | | |

### 10.2.97B3C28 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/ EllipsoidArcArea/Center

Table 10.2.97B3C28.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/EllipsoidArcArea/Center

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/EllipsoidArcArea/Center | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |

### 10.2.97B3C29 /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType

Table 10.2.97B3C29.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | node | Get, Replace |  |  |
|  | This interior node contains the coordinates of the center point of the ellipsoid arc. | | | | |  |

### 10.2.97B3C30 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType/Longitude

Table 10.2.97B3C30.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Longitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Longitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the longitudinal coordinate of the center. | | | | |

- Values: 0-16777215

### 10.2.97B3C31 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/ EllipsoidArcArea/Center/PointCoordinateType/Latitude

Table 10.2.97B3C31.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Latitude

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/EllipsoidArcArea/Center/PointCoordinateType/Latitude | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the latitudinal coordinate of the center. | | | | |

- Values: 0-16777215

### 10.2.97B3C32 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/ EllipsoidArcArea/Radius

Table 10.2.97B3C32.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/EllipsoidArcArea/Radius

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/EllipsoidArcArea/Radius | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the radius of the ellipsoid arc. | | | | |

- Values: non-negative integer

### 10.2.97B3C33 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/ EllipsoidArcArea/OffsetAngle

Table 10.2.97B3C33.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/EllipsoidArcArea/OffsetAngle

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/EllipsoidArcArea/OffsetAngle | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the offset angle of the ellipsoid arc. | | | | |

- Values: 0-255

### 10.2.97B3C34 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/ EllipsoidArcArea/IncludedAngle

Table 10.2.97B3C34.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/EllipsoidArcArea/IncludedAngle

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/EllipsoidArcArea/IncludedAngle | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the included angle of the ellipsoid arc. | | | | |

- Values: 0-255

### 10.2.97B3C35 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Speed

Table 10.2.97B3C35.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Speed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Speed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | One | node | Get, Replace |  |  |
|  | This interior node contains the speed. | | | | |  |

### 10.2.97B3C36 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Speed/ MinimumSpeed

Table 10.2.97B3C36.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Speed/MinimumSpeed

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Speed/MinimumSpeed | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the minimum speed. | | | | |

- Values: non-negative integer in units of kilometers/hour.

### 10.2.97B3C37 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Speed/ MaximumSpeed

Table 10.2.97B3C37.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Speed/MaximumSpeed

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Speed/MaximumSpeed | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the maximum speed. | | | | |  |

- Values: non-negative integer in units of kilometers/hour.

### 10.2.97B3C38 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Heading

Table 10.2.97B3C38.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Heading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Heading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Optional | One | node | Get, Replace |  |  |
|  | This interior node contains the heading. | | | | |  |

### 10.2.97B3C39 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Heading/ MinimumHeading

Table 10.2.97B3C39.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Heading/MinimumHeading

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Heading/MinimumHeading | | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |  |
|  | Required | One | int | Get, Replace |  |  |
|  | This leaf node contains the minimum heading. | | | | |  |

- Values: 0-359

### 10.2.97B3C40 /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Heading/ MaximumHeading

Table 10.2.97B3C40.1: /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Heading/MaximumHeading

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/LocationCriteriaForDeactivation/<x>/ExitSpecificArea/Heading/MaximumHeading | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node contains the maximum heading. | | | | |

- Values: 0-359

### 10.2.97B3D /<x>/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ ManualDeactivationNotAllowedIfLocationCriteriaMet

Table 10.2.97B3D.1: /*<x>*/<x>/OnNetwork/FunctionalAliasList/<x>/Entry/ManualDeactivationNotAllowedIfLocationCriteriaMet

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/FunctionalAliasList/<x>/Entry/ManualDeactivationNotAllowedIfLocationCriteriaMet | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCData user is authorised to de-activate a functional alias if the location criteria are met. | | | | |

### 10.2.97C /<x>/<x>/OnNetwork/AllowedQueryFunctionalAliasOtherUser

Table 10.2.97C.1: /*<x>*/<x>/OnNetwork/AllowedQueryFunctionalAliasOtherUser

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/AllowedQueryFunctionalAliasOtherUser | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCData user is authorised query the functional alias(es) activated by another MCData user. | | | | |

When set to "true" the MCData user is authorised to query the functional alias(es) activated by another MCData user.

When set to "false" the MCData user is not authorised to query the functional alias(es) activated by another MCData user.

### 10.2.97D /<x>/<x>/OnNetwork/AllowedTakeoverFunctionalAliasOtherUser

Table 10.2.97D.1: /*<x>*/<x>/OnNetwork/AllowedTakeoverFunctionalAliasOtherUser

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/AllowedTakeoverFunctionalAliasOtherUser | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCData user is authorised to take over the functional alias(es) previously activated by another MCData user. | | | | |

When set to "true" the MCData user is authorised to take over the functional alias(es) previously activated by another MCData user.

When set to "false" the MCData user is not authorised to take over the functional alias(es) previously activated by another MCData user.

### 10.2.97E /*<x>*/<x>/OnNetwork/MessageStoreHostname

Table 10.2.97E.1: /*<x>*/<x>/OnNetwork/MessageStoreHostname

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MessageStoreHostname | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates value of the hostname identifying the message store function. | | | | |

The value is a string.

### 10.2.97F /*<x>*/*<x>*/OnNetwork/AuthorisedIncomingAny

Table 10.2.97F.1: /*<x>*/<x>/OnNetwork/AuthorisedIncomingAny

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/AuthorisedIncomingAny | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to receive MCData communication from any MCData user. | | | | |

When set to "true" the MCData user is authorised to receive MCData communication from any MCData user.

When set to "false" the MCData user is not authorised to receive an MCData communication from any MCData user, but only from the MCData users contained in the IncomingUserList.

### 10.2.97G /*<x>*/<x>/OnNetwork/IncomingUserList

Table 10.2.97G.1: /*<x>*/<x>/OnNetwork/IncomingUserList

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/IncomingUserList | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for a list of MCData user(s) who are authorised to initiate one-to-one MCData communication to the configured MCData user. | | | | |

### 10.2.97G1 /*<x>*/<x>/OnNetwork/IncomingUserList/<x>

Table 10.2.97G1.1: /*<x>*/<x>/OnNetwork/IncomingUserList/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/IncomingUserList/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more list of MCData users who are authorised to initiate one-to-one MCData communication to the configured MCData user. | | | | |

### 10.2.97G2 /*<x>*/<x>/OnNetwork/IncomingUserList/<x>/Entry

Table 10.2.97G2.1: /*<x>*/<x>/OnNetwork/IncomingUserList/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/IncomingUserList/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more MCData users who are authorised to initiate one-to-one MCData communication to the configured MCData user. | | | | |

### 10.2.97G3 /*<x>*/<x>/OnNetwork/IncomingUserList/<x>/Entry/MCDataID

Table 10.2.97G3.1: /*<x>*/<x>/OnNetwork/IncomingUserList/<x>/Entry/MCDataID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/IncomingUserList/<x>/Entry/MCDataID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates an MCData user identity (MCData ID) which is a globally unique identifier within the MCData service that represents the MCData user. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 10.2.97G4 /*<x>*/<x>/OnNetwork/IncomingUserList/<x>/Entry/ MCDataIDKMSURI

Table 10.2.97G4.1: /*<x>*/<x>/OnNetwork/IncomingUserList/<x>/Entry/MCDataIDKMSURI

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/IncomingUserList/<x>/Entry/MCDataIDKMSURI | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates the identity (URI) of the KMS associated with the MCDataID of an MCData user who is authorised to initiate a one-to-one communication to the configured MCData user. | | | | |

The value is a URI as specified in 3GPP TS 23.003 [5].

### 10.2.98 /*<x>*/*<x>*/OffNetwork

Table 10.2.98.1: /*<x>*/<x>/OffNetwork

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | node | Get, Replace |  |
|  | This interior node represents a container for off-network operation. | | | | |

### 10.2.99 /*<x>*/*<x>*/OffNetwork/Authorised

Table 10.2.99.1: /*<x>*/<x>/OffNetwork/Authorised

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/Authorised | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation for off-network services. | | | | |

When set to "true" the MCData user is authorised for off-network.

When set to "false" the MCData user is not authorised for off-network operation.

### 10.2.100 /*<x>*/*<x>*/OffNetwork/MCDataGroupList

Table 10.2.100.1: /*<x>*/<x>/OffNetwork/MCDataGroupList

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCDataGroupList | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the list of off-network MCData groups that the MCData user is allowed to use. | | | | |

### 10.2.101 /*<x>*/<x>/OffNetwork/MCDataGroupList/<x>

Table 10.2.101.1: /*<x>*/<x>/OffNetwork/MCDataGroupList/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCDataGroupList/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more list of off-network MCData groups that the MCData user is allowed to use. | | | | |

### 10.2.102 /*<x>*/<x>/OffNetwork/MCDataGroupList/<x>/Entry

Table 10.2.102.1: /*<x>*/<x>/OffNetwork/MCDataGroupList/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCDataGroupList/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the details of the off-network MCData groups that the MCData user is allowed to use. | | | | |

### 10.2.103 /*<x>*/<x>/OffNetwork/MCDataGroupList/<x>/Entry/ MCDataGroupID

Table 10.2.103.1: /*<x>*/<x>/OffNetwork/MCDataGroupList/<x>/Entry/MCDataGroupID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCDataGroupList/<x>/Entry/MCDataGroupID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the MCData group ID for the off-network MCData group that the MCData user is allowed to use. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 10.2.104 /*<x>*/*<x>*/OffNetwork/MCDataGroupList/<x>/Entry/DisplayName

Table 10.2.104.1: /*<x>*/<x>/OffNetwork/MCDataGroupList/<x>/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCDataGroupList/<x>/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name that corresponds to the MCData Group ID. | | | | |

### 10.2.105 Void

### 10.2.106 Void

### 10.2.107 /*<x>*/<x>/OffNetwork/MCDataGroupList/<x>/Entry/GMSServID

Table 10.2.107.1: /*<x>*/<x>/OffNetwork/MCDataGroupList/<x>/Entry/GMSServID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCDataGroupList/<x>/Entry/GMSServID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates the identity (URI) of the group management server hosting the MCData Group ID. | | | | |

### 10.2.108 Void

### 10.2.109 Void

### 10.2.110 /*<x>*/<x>/OffNetwork/MCDataGroupList/<x>/Entry/ IdMSTokenEndPoint

Table 10.2.110.1: /*<x>*/<x>/OffNetwork/MCDataGroupList/<x>/Entry/IdMSTokenEndPoint

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCDataGroupList/<x>/Entry/IdMSTokenEndPoint | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates the identity (URI) of the IDMS token endpoint for the MCData Group ID in the MCDataGroupList. If the value is empty, the IDMS identities (IDMSAuthEndpoint and IDMSTokenEndpoint) present in the MCS UE initial configuration MO are used. | | | | |

### 10.2.110A /*<x>*/<x>/OffNetwork/MCDataGroupList/<x>/Entry/GroupKMSURI

Table 10.2.110A.1: /*<x>*/<x>/OffNetwork/MCDataGroupList/<x>/Entry/GroupKMSURI

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCDataGroupList/<x>/Entry/GroupKMSURI | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates key management server URI for the security domain of the MCData group identity (MCData Group ID) of the off-network MCData group | | | | |

The value is a URI as specified in 3GPP TS 23.003 [5].

### 10.2.111 /*<x>*/<x>/OffNetwork/MCDataGroupList/<x>/Entry/ RelativePresentationPriority

Table 10.2.111.1: /*<x>*/<x>/OffNetwork/MCDataGroupList/<x>/Entry/RelativePresentationPriority

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCDataGroupList/<x>/Entry/RelativePresentationPriority | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | int | Get, Replace |  |
|  | This leaf node indicates indicating the presentation priority of the off-network group for the MCData user relative to other off-network groups and off-network users. | | | | |

- Values: 0-255

The lowest RelativePresentationPriority value shall be considered as the MCData group transaction having the lowest priority for presentation among other group MCData and one-to-one user transactions.

### 10.2.112 /*<x>*/*<x>*/OffNetwork/UserInfoID

Table 10.2.112.1: /*<x>*/<x>/OffNetwork/UserInfoID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/UserInfoID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the ProSe user info ID as specified in 3GPP TS 23.303 [6]. | | | | |

### 10.2.113 Void

### 10.2.114 Void

### 10.2.115 Void

### 10.2.116 Void

### 10.2.117 Void

### 10.2.118 Void

### 10.2.119 Void

### 10.2.120 Void

### 10.2.121 /*<x>*/Status

Table 10.2.121.1: /*<x>*/Status

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Status | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | bool | Get, Replace |  |
|  | This leaf node indicates whether this MCData user profile is enabled or disabled. | | | | |

When set to "true" this MCData user profile is enabled.

When set to "false" this MCData user profile is disabled.

# 11 MCData service configuration MO

## 11.1 General

The MCData service configuration Management Object (MO) is used to configure MCData Client behaviour for the on-network or off-network MCData Service. The MCData service configuration parameters may be stored in the ME, or in the USIM as specified in 3GPP TS 31.102 [10], or in both the ME and the USIM. If both the ME and the USIM contain the same parameters, the values stored in the USIM shall take precedence.

The Management Object Identifier is: urn:oma:mo:ext-3gpp-MCData-service-configuration:1.0.

Protocol compatibility: This MO is compatible with OMA OMA DM 1.2 [3].

The OMA DM ACL property mechanism (see OMA OMA-ERELD-DM-V1\_2 [2]) may be used to grant or deny access rights to OMA DM servers in order to modify nodes and leaf objects of the MCData service configuration MO.

The following nodes and leaf objects are possible under the MCData service configuration node as described in figure 11.1.1.



Figure 11.1.1: The MCData service configuration MO

## 11.2 MCData service configuration MO parameters

### 11.2.1 General

This clause describes the parameters for the MCData service configuration Management Object (MO).

### 11.2.2 Node: *<x>*

Table 11.2.2.1: Node: *<x>*

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get |  |
|  | This interior node acts as a placeholder for the MCData service configuration Management Object (MO).  For the MCData service configuration MO, the namespace specific string is: "urn:oma:mo:oma-dm-mcdata-service configuration:1.0" | | | | |

- Values: N/A

### 11.2.3 /*<x>*/Name

Table 11.2.3.1: /*<x>*/Name

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | chr | Get |  |
|  | The Name leaf is a name for the MCData service configuration settings. | | | | |

- Values: <User displayable name>

### 11.2.4 /*<x>*/Ext/

Table 11.2.4.1: /*<x>*/Ext/

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Ext | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | The Ext is an interior node for where the vendor specific information about the MCData service configuration MO is being placed. | | | | |

Usually the vendor extension is identified by vendor specific name under the ext node and contains the vendor meaning application vendor, device vendor etc. The tree structure under the vendor identified is not defined and can therefore include one or more un-standardized sub-trees.

- Values: N/A

### 11.2.5 /*<x>*/Common

Table 11.2.5.1: /*<x>*/Common

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | node | Get, Replace |  |
|  | This interior node represents a container for the common network operation which means both on-network operation and off-network operation. | | | | |

### 11.2.6 /*<x>*/Common/TxRxControl

Table 11.2.6.1: /*<x>*/Common/TxRxControl

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/TxRxControl | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for transmission and reception control configuration. | | | | |

### 11.2.7 /*<x>*/Common/TxRxControl/TimeTempDataWaiting

Table 11.2.7.1: /*<x>*/Common/TxRxControl/TimeTempDataWaiting

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/TxRxControl/TimeTempDataWaiting | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the time limit for the temporarily stored data that is waiting to be delivered to a receiving user. | | | | |

- Values: 0-65535

The TimeTempDataWaiting is in minutes.

### 11.2.8 /*<x>*/Common/TxRxControl/TimePeriodicAnnouncement

Table 11.2.8.1: /*<x>*/Common/TxRxControl/TimePeriodicAnnouncement

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/TxRxControl/TimePeriodicAnnouncement | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the timer for the periodic announcement which contains a list of available recently invited data group communications. | | | | |

- Values: 0-65535

The TimePeriodicAnnouncement is in minutes.

### 11.2.9 /*<x>*/OffNetwork

Table 11.2.9.1: /*<x>*/OffNetwork

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | node | Get, Replace |  |
|  | This interior node represents a container for off-network operation. | | | | |

### 11.2.10 /*<x>*/OffNetwork/DefaultPPPP

Table 11.2.10.1: /*<x>*/OffNetwork/DefaultPPPP

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/DefaultPPPP | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the default ProSe Per-Packet Priority (PPPP) configuration. | | | | |

### 11.2.11 /*<x>*/OffNetwork/DefaultPPPP/MCDataOneToOneCallSignalling

Table 11.2.11.1: /*<x>*/OffNetwork/DefaultPPPP/MCDataOneToOneCallSignalling

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/DefaultPPPP/MCDataOneToOneCallSignalling | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the default ProSe Per-Packet Priority (PPPP) value (as specified in 3GPP TS 23.303 [6]) for the MCData one-to-one call signalling. | | | | |

- Values: 1-8

The MCData user data with the lowest ProSe Per-Packet Priority value shall be considered as the MCData user data having the highest priority among the MCData user data.

### 11.2.12 /*<x>*/OffNetwork/DefaultPPPP/MCDataOneToOneCallMedia

Table 11.2.12.1: /*<x>*/OffNetwork/DefaultPPPP/MCDataOneToOneCallMedia

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/DefaultPPPP/MCDataOneToOneCallMedia | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the default ProSe Per-Packet Priority (PPPP) value (as specified in 3GPP TS 23.303 [6]) for the MCData private call media. | | | | |

- Values: 1-8

The MCData user data with the lowest ProSe Per-Packet Priority value shall be considered as the MCData user data having the highest priority among the MCData user data.

# 12 MCVideo UE configuration MO

## 12.1 General

The MCVideo UE configuration Management Object (MO) is used to configure MCVideo Client behaviour for the on-network or off-network MCVideo Service. The MCVideo UE configuration parameters may be stored in the ME, or in the USIM as specified in 3GPP TS 31.102 [10], or in both the ME and the USIM. If both the ME and the USIM contain the same parameters, the values stored in the USIM shall take precedence.

The Management Object Identifier is: urn:oma:mo:ext-3gpp-MCVideo-UE-configuration:1.0.

Protocol compatibility: This MO is compatible with OMA OMA DM 1.2 [3].

The OMA DM ACL property mechanism (see OMA OMA-ERELD-DM-V1\_2 [2]) may be used to grant or deny access rights to OMA DM servers in order to modify nodes and leaf objects of the MCVideo UE configuration MO.

The following nodes and leaf objects are possible under the MCVideo UE configuration node as described in figure 12.1.1.



Figure 12.1.1: The MCVideo UE configuration MO

## 12.2 MCVideo UE configuration MO parameters

### 12.2.1 General

This clause describes the parameters for the MCVideo UE configuration Management Object (MO).

### 12.2.2 Node: *<x>*

Table 12.2.2.1: Node: <x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get |  |
|  | This interior node acts as a placeholder for the MCVideo UE configuration Management Object (MO).  For the MCVideo UE configuration MO, the namespace specific string is: "urn:oma:mo:oma-dm-mcvideo-ue-configuration:1.0" | | | | |

- Values: N/A

### 12.2.3 /*<x>*/Name

Table 12.2.3.1: /<x>/Name

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | chr | Get |  |
|  | The Name leaf is a name for the MCVideo UE configuration settings. | | | | |

- Values: <User displayable name>

### 12.2.4 /*<x>*/Ext/

Table 12.2.4.1: /<x>/Ext/

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Ext | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | The Ext is an interior node for where the vendor specific information about the MCVideo UE configuration MO is being placed. | | | | |

Usually the vendor extension is identified by vendor specific name under the ext node and contains the vendor meaning application vendor, device vendor etc. The tree structure under the vendor identified is not defined and can therefore include one or more un-standardized sub-trees.

- Values: N/A

### 12.2.5 /*<x>*/Common

Table 12.2.5.1: /*<x>*/Common

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | node | Get, Replace |  |
|  | This interior node represents a container for the common network operation which means both on-network operation and off-network operation. | | | | |

### 12.2.5A /*<x>*/Common/PrivateCall

Table 12.2.5A.1: /*<x>*/Common/PrivateCall

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/PrivateCall | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the private call configuration. | | | | |

### 12.2.5B /*<x>*/Common/PrivateCall/MaxCallNc10

Table 12.2.5B.1: /*<x>*/Common/PrivateCall/MaxCallNc10

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/PrivateCall/MaxCallNc10 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the maximum number of private calls. | | | | |

- Values: 0-255

### 12.2.6 /*<x>*/Common/MCVideoGroupCall

Table 12.2.6.1: /*<x>*/Common/MCVideoGroupCall

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCVideoGroupCall | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the MCVideo group call configuration. | | | | |

### 12.2.7 /*<x>*/Common/MCVideoGroupCall/MaxCallNc4

Table 12.2.7.1: /*<x>*/Common/MCVideoGroupCall/MaxCallNc4

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCVideoGroupCall/MaxCallNc4 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the maximum number of simultaneous MCVideo group calls. | | | | |

- Values: 0-255

### 12.2.8 /*<x>*/Common/MCVideoGroupCall/MaxTransmissionNc5

Table 12.2.8.1: /*<x>*/Common/MCVideoGroupCall/MaxTransmissionNc5

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCVideoGroupCall/MaxTransmissionNc5 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the maximum number of video transmissions in a group. | | | | |

- Values: 0-255

### 12.2.9 /*<x>*/Common/MCVideoGroupCall/PrioritizedMCVideoGroup

Table 12.2.9.1: /*<x>*/Common/MCVideoGroupCall/PrioritizedMCVideoGroup

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCVideoGroupCall/PrioritizedMCVideoGroup | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the prioritized MCVideo group call configuration. | | | | |

### 12.2.10 /*<x>*/Common/MCVideoGroupCall/PrioritizedMCVideoGroup/<x>

Table 12.2.10.1: /*<x>*/Common/MCVideoGroupCall/PrioritizedMCVideoGroup/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCVideoGroupCall/PrioritizedMCVideoGroup/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more prioritized MCVideo group call configuration. | | | | |

### 12.2.11 /*<x>*/Common/MCVideoGroupCall/PrioritizedMCVideoGroup/ <x>/MCVideoGroupID

Table 12.2.11.1: /*<x>*/Common/MCVideoGroupCall/PrioritizedMCVideoGroup/<x>/MCVideoGroupID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCVideoGroupCall/PrioritizedMCVideoGroup/<x>/MCVideoGroupID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the associated MCVideo group ID. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 12.2.12 /*<x>*/Common/MCVideoGroupCall/ PrioritizedMCVideoGroup/<x>/MCVideoGroupPriorityHierarchy

Table 12.2.12.1: /*<x>*/Common/MCVideoGroupCall/PrioritizedMCVideoGroup/<x>/MCVideoGroupPriorityHierarchy

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MCVideoGroupCall/PrioritizedMCVideoGroup/<x>/MCVideoGroupPriorityHierarchy | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the requested presentation priority of MCVideo group call. | | | | |

- Values: 0-255

The group with the lowest MCVideoGroupPriorityHierarchy value shall be considered as the group having the lowest priority among the groups.

### 12.2.13 /*<x>*/OnNetwork

Table 12.2.13.1: /*<x>*/OnNetwork

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | node | Get, Replace |  |
|  | This interior node represents a container for on-network operation. | | | | |

### 12.2.14 /*<x>*/OnNetwork/RelayService

Table 12.2.14.1: /*<x>*/OnNetwork/RelayService

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/RelayService | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to use a relay service. | | | | |

When set to "true" the MCVideo group is allowed to use a relay service.

When set to "false" the MCVideo group is not allowed to use a relay service.

### 12.2.15 /*<x>*/OnNetwork/IPv6Preferred

Table 12.2.15.1: /*<x>*/OnNetwork/IPv6Preferred

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/IPv6Preferred | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether IPv6 is preferred over IPv4 for on-network operation when the MCVideo UE has both IPv4 and IPv6 host configuration. | | | | |

If the MCVideo UE has both IPv4 and IPv6 host configuration and:

- if IPv6Preferred is set to "true" then the UE uses IPv6 for all on‑network signalling and media; otherwise

- if IPv6Preferred is set to "false" then the UE uses IPv4 for all on‑network signalling and media.

### 12.2.16 /*<x>*/OnNetwork/RelayedMCVideoGroup

Table 12.2.16.1: /*<x>*/OnNetwork/RelayedMCVideoGroup

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/RelayedMCVideoGroup | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | This interior node is a placeholder for the allowed relayed MCVideo groups. | | | | |

### 12.2.17 /*<x>*/OnNetwork/RelayedMCVideoGroup/<x>

Table 12.2.17.1: /*<x>*/OnNetwork/RelayedMCVideoGroup/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/RelayedMCVideoGroup/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more allowed relayed MCVideo groups. | | | | |

### 12.2.18 /*<x>*/OnNetwork/RelayedMCVideoGroup/<x>/MCVideoGroupID

Table 12.2.18.1: /*<x>*/OnNetwork/RelayedMCVideoGroup/<x>/MCVideoGroupID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/RelayedMCVideoGroup/<x>/MCVideoGroupID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the associated MCVideo group ID. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 12.2.19 /*<x>*/OnNetwork/RelayedMCVideoGroup/<x>/RelayServiceCode

Table 12.2.19.1: /*<x>*/OnNetwork/RelayedMCVideoGroup/<x>/RelayServiceCode

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OnNetwork/RelayedMCVideoGroup/<x>/RelayServiceCode | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the connectivity service that the ProSe UE-to-network relay provides to public safety applications as specified in 3GPP TS 23.303 [6]. | | | | |

# 13 MCVideo user profile MO

## 13.1 General

The MCVideo user profile configuration Management Object (MO) is used to configure the MCVideo Client behaviour for the on-network or off-network MCVideo Service. The MCVideo user profile configuration parameters may be stored in the ME, or in the USIM as specified in 3GPP TS 31.102 [10], or in both the ME and the USIM. If both the ME and the USIM contain the same parameters, the values stored in the USIM shall take precedence.

The Management Object Identifier is: urn:oma:mo:ext-3gpp-MCVideo-user-profile:1.0.

Protocol compatibility: This MO is compatible with OMA OMA DM 1.2 [3].

The OMA DM ACL property mechanism (see OMA OMA-ERELD-DM-V1\_2 [2]) may be used to grant or deny access rights to OMA DM servers in order to modify nodes and leaf objects of the MCVideo user profile MO.

The following nodes and leaf objects are possible under the MCVideo user profile node as described in figure 13.1.1, figure 13.1.2 and figure 13.1.3.



Figure 13.1.1: The MCVideo user profile MO (1 of 3)



Figure 13.1.2: The MCVideo user profile MO (2 of 3)



Figure 13.1.3: The MCVideo user profile MO (3 of 3)

## 13.2 MCVideo user profile MO parameters

### 13.2.1 General

This clause describes the parameters for the MCVideo user profile Management Object (MO).

### 13.2.2 Node: *<x>*

Table 13.2.2.1: Node: *<x>*

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get |  |
|  | This interior node acts as a placeholder for the MCVideo user profile Management Object (MO).  For the MCVideo user profile MO, the namespace specific string is: "urn:oma:mo:oma-dm-mcvideo-user-profile:1.0" | | | | |

- Values: N/A

### 13.2.3 /*<x>*/Name

Table 13.2.3.1: /*<x>*/Name

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | chr | Get |  |
|  | The Name leaf is a name for the MCVideo user profile settings. | | | | |

- Values: <User displayable name>

### 13.2.4 /*<x>*/Ext/

Table 13.2.4.1: /*<x>*/Ext/

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Ext | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | The Ext is an interior node for where the vendor specific information about the MCVideo user profile MO is being placed. | | | | |

Usually the vendor extension is identified by vendor specific name under the ext node and contains the vendor meaning application vendor, device vendor etc. The tree structure under the vendor identified is not defined and can therefore include one or more un-standardized sub-trees.

- Values: N/A

### 13.2.5 /*<x>*/<x>

Table 13.2.5.1: /*<x>*/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get, Replace |  |
|  | This interior node represents a container for on-network operation and off-network operation. | | | | |

### 13.2.6 /*<x>*/<x>/Common

Table 13.2.6.1: /*<x>*/<x>/Common

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node represents a container for the common network operation which means both on-network operation and off-network operation. | | | | |

### 13.2.7 /*<x>*/*<x>*/Common/MCVideoUserID

Table 13.2.7.1: /*<x>*/<x>/Common/MCVideoUserID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideoUserID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates an MCVideo user identity (MCVideo ID) which is a globally unique identifier within the MCVideo service that represents the MCVideo user. | | | | |

### 13.2.8 /*<x>*/*<x>*/Common/MCVideoUserProfileIndex

Table 13.2.8.1: /*<x>*/<x>/Common/MCVideoUserProfileIndex

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideoUserProfileIndex | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates an index for the particular MCVideo user profile. | | | | |

- Values: 0-255

### 13.2.9 /*<x>*/*<x>*/Common/MCVideoUserProfileName

Table 13.2.9.1: /*<x>*/<x>/Common/MCVideoUserProfileName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideoUserProfileName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates a profile name for the particular MCVideo user profile. | | | | |

### 13.2.10 /*<x>*/*<x>*/Common/PreSelectedIndication

Table 13.2.10.1: /*<x>*/<x>/Common/PreSelectedIndication

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PreSelectedIndication | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | null | Get, Replace |  |
|  | This leaf node indicates that this MCVideo user profile MO is designated to be the pre-selected MCVideo user profile as defined by 3GPP TS 23.179 [15] | | | | |

- Values: null

When this leaf node is present, this MCVideo user profile MO is designated as the pre-selected MCVideo user profile.

When this leaf node is absent, this MCVideo user profile MO is not designated as the pre-selected MCVideo user profile.

If more than one MCVideo user profile MO is specified for the MCVideo user, then only one MCVideo user profile MO for the MCVideo user shall contain the <x>/Common/PreSelectedIndication leaf node.

If there is only one MCVideo user profile MO specified for the MCVideo user, then it is optional to include the <x>/Common/PreSelectedIndication leaf node.

### 13.2.11 /*<x>*/<x>/Common/UserAliases

Table 13.2.11.1: /*<x>*/<x>/Common/UserAliases

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/UserAliases | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for a list of aliases of an MCVideo user. | | | | |

### 13.2.12 /*<x>*/<x>/Common/UserAliases/<x>

Table 13.2.12.1: /*<x>*/<x>/Common/UserAliases/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/UserAliases/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more aliases of an MCVideo user. | | | | |

### 13.2.13 /*<x>*/*<x>*/Common/UserAliases/<x>/UserAlias

Table 13.2.13.1: /*<x>*/<x>/Common/UserAliases/<x>/UserAlias

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/UserAliases/<x>/UserAlias | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates an alphanumeric alias of the MCVideo user. | | | | |

### 13.2.14 Void

### 13.2.15 /*<x>*/<x>/Common/ParticipantType

Table 13.2.15.1: /*<x>*/<x>/Common/ParticipantType

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| *<x>*/Common/ParticipantType | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the participant type of the MCVideo user. | | | | |

The ParticipantType means the functional category of the participant (e.g., first responder, second responder, dispatch, dispatch supervisor), typically defined by the MCVideo administrators.

### 13.2.16 /*<x>*/<x>/Common/Organization

Table 13.2.16.1: /*<x>*/<x>/Common/Organization

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/Organization | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the organization an MCVideo user belongs to. | | | | |

### 13.2.17 /*<x>*/*<x>*/Common/MCVideoGroupBroadcast

Table 13.2.17.1: /*<x>*/<x>/Common/MCVideoGroupBroadcast

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideoGroupBroadcast | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the group-broadcast group policy. | | | | |

### 13.2.18 /*<x>*/*<x>*/Common/MCVideoGroupBroadcast/Authorised

Table 13.2.18.1: /*<x>*/<x>/Common/MCVideoGroupBroadcast/Authorised

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideoGroupBroadcast/Authorised | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to create a group-broadcast group. | | | | |

When set to "true" the MCVideo user is authorised to create a group-broadcast group.

When set to "false" the MCVideo user is not authorised to create a group-broadcast group.

### 13.2.19 /*<x>*/*<x>*/Common/UserBroadcast

Table 13.2.19.1: /*<x>*/<x>/Common/UserBroadcast

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/UserBroadcast | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the user-broadcast group policy. | | | | |

### 13.2.20 /*<x>*/*<x>*/Common/UserBroadcast/Authorised

Table 13.2.20.1: /*<x>*/<x>/Common/UserBroadcast/Authorised

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/UserBroadcast/Authorised | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to create a user-broadcast group. | | | | |

When set to "true" the MCVideo user is authorised to create a user-broadcast group.

When set to "false" the MCVideo user is not authorised to create a user-broadcast group.

### 13.2.21 Void

### 13.2.22 Void

### 13.2.23 Void

### 13.2.24 Void

### 13.2.25 Void

### 13.2.26 Void

### 13.2.27 Void

### 13.2.28 Void

### 13.2.29 /*<x>*/*<x>*/Common/AllowedActivateAlert

Table 13.2.29.1: /*<x>*/<x>/Common/AllowedActivateAlert

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/AllowedActivateAlert | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCVideo user is authorised to activate an emergency alert. | | | | |

When set to "true" the MCVideo user is authorised to activate an emergency alert.

When set to "false" the MCVideo user is not authorised to activate an emergency alert.

### 13.2.30 /*<x>*/*<x>*/Common/AllowedCancelAlert

Table 13.2.30.1: /*<x>*/<x>/Common/AllowedCancelAlert

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/AllowedCancelAlert | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCVideo user is allowed to cancel an emergency alert. | | | | |

When set to "true" the MCVideo user is authorised to cancel an emergency alert.

When set to "false" the MCVideo user is not authorised to cancel an emergency alert.

### 13.2.31 Void

### 13.2.32 Void

### 13.2.33 Void

### 13.2.34 Void

### 13.2.35 Void

### 13.2.36 Void

### 13.2.37 Void

### 13.2.38 Void

### 13.2.38A /*<x>*/*<x>*/Common/MCVideoGroupCall

Table 13.2.38A.1: /*<x>*/<x>/Common/MCVideoGroupCall

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideoGroupCall | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the MCVideo group call configuration. | | | | |

### 13.2.38A1 /*<x>*/*<x>*/Common/MCVideoGroupCall/EmergencyAlert

Table 13.2.38A1.1: /*<x>*/<x>/Common/MCVideoGroupCall/EmergencyAlert

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideoGroupCall/EmergencyAlert | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the MCVideo emergency alert policy. | | | | |

### 13.2.38A2 /*<x>*/*<x>*/Common/MCVideoGroupCall/EmergencyAlert/ Authorised

Table 13.2.38A2.1: /*<x>*/<x>/Common/MCVideoGroupCall/EmergencyAlert/Authorised

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideoGroupCall/EmergencyAlert/Authorised | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to activate an MCVideo emergency alert. | | | | |

When set to "true" the MCVideo user is authorised to make an MCVideo emergency alert.

When set to "false" the MCVideo user is not authorised to make an MCVideo emergency alert.

### 13.2.38A3 /*<x>*/*<x>*/Common/MCVideoGroupCall/EmergencyAlert/ Cancel

Table 13.2.38A3.1: /*<x>*/<x>/Common/MCVideoGroupCall/EmergencyAlert/Cancel

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideoGroupCall/EmergencyAlert/Cancel | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to cancel an MCVideo emergency alert. | | | | |

When set to "true" the MCVideo user is authorised to cancel an MCVideo emergency alert.

When set to "false" the MCVideo user is not authorised to cancel an MCVideo emergency alert.

### 13.2.38A4 /*<x>*/<x>/Common/MCVideoGroupCall/EmergencyAlert/ Entry

Table 13.2.338A4.1: /*<x>*/<x>/Common/MCVideoGroupCall/EmergencyAlert/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideoGroupCall/EmergencyAlert/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the details of the MCVideo group of an MCVideo emergency alert. | | | | |

### 13.2.38A5 /*<x>*/*<x>*/Common/MCVideoGroupCall/EmergencyAlert/ Entry/ID

Table 13.2.38A5.1: /*<x>*/<x>/Common/MCVideoGroupCall/EmergencyAlert/Entry/ID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideoGroupCall/EmergencyAlert/Entry/ID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the MCVideo group used upon certain criteria on initiation of an MCVideo emergency alert. | | | | |

### 13.2.38A6 /*<x>*/*<x>*/Common/MCVideoGroupCall/EmergencyAlert/ Entry/DisplayName

Table 13.2.38A6.1: /*<x>*/<x>/Common/MCVideoGroupCall/EmergencyAlert/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideoGroupCall/EmergencyAlert/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name that corresponds to the ID. | | | | |

### 13.2.38A7 /*<x>*/*<x>*/Common/MCVideoGroupCall/EmergencyAlert/ Entry/Usage

Table 13.2.38A7.1: /*<x>*/<x>/Common/MCVideoGroupCall/EmergencyAlert/Entry/Usage

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideoGroupCall/EmergencyAlert/Entry/Usage | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the criteria to determine when initiation of an MCVideo emergency alert uses the ID. | | | | |

The valid values are 'LocallyDetermined', 'UseCurrentlySelectedGroup', 'UsePreConfigured' and 'DedicatedGroup'.

When set to 'LocallyDetermined' then if the MCVideo user selects an MCVideo ID then use that MCVideo ID for an on-network MCVideo emergency alert, if the MCVideo user does not select a MCVideo ID then use the MCVideo ID identified by the ID in clause 13.2.38A5 for an on-network MCVideo emergency alert.

When set to 'UseCurrentlySelectedGroup' then if the MCVideo user has currently selected an MCVideo group then use that MCVideo group for an on-network MCVideo emergency alert, if the MCVideo user does not have a currently selected MCVideo group then use the MCVideo group identified by the ID in clause 13.2.38A5 for an MCVideo emergency alert.

When set to 'UsePreConfigured' then use the ID identified by the ID in clause 13.2.38A5 for an on-network MCVideo emergency alert.

When set to 'DedicatedGroup' then use the MCVideo group identified by the ID in clause 13.2.38A5 for an MCVideo emergency alert.

### 13.2.38B /*<x>*/*<x>*/Common/MCVideoGroupCall/EmergencyCall

Table 13.2. 38B.1: /*<x>*/<x>/Common/MCVideoGroupCall/EmergencyCall

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideoGroupCall/EmergencyCall | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the MCVideo emergency call policy. | | | | |

### 13.2.38C /*<x>*/*<x>*/Common/MCVideoGroupCall/EmergencyCall/ Enabled

Table 13.2.38C.1: /*<x>*/<x>/Common/MCVideoGroupCall/EmergencyCall/Enabled

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideoGroupCall/EmergencyCall/Enabled | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to make an MCVideo emergency group call functionality enabled for MCVideo user. | | | | |

When set to "true" the MCVideo user is authorised to make an MCVideo emergency group call functionality enabled.

When set to "false" the MCVideo user is not authorised to make an MCVideo emergency group call functionality enabled.

### 13.2.38D /*<x>*/*<x>*/Common/MCVideoGroupCall/EmergencyCall/ CancelMCVideoGroup

Table 13.2.38D.1: /*<x>*/<x>/Common/MCVideoGroupCall/EmergencyCall/CancelMCVideoGroup

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideoGroupCall/EmergencyCall/CancelMCVideoGroup | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to cancel an in progress MCVideo emergency group call associated with a group. | | | | |

When set to "true" the MCVideo user is authorised to cancel a MCVideo emergency group call.

When set to "false" the MCVideo user is not authorised to cancel a MCTT emergency group call.

### 13.2.38D1 /*<x>*/*<x>*/Common/MCVideoGroupCall/EmergencyCall/ MCVideoGroupInitiation

Table 13.2.38D1.1: /*<x>*/<x>/Common/MCVideoGroupCall/EmergencyCall/MCVideoGroupInitiation

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideoGroupCall/EmergencyCall/MCVideoGroupInitiation | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the group used on initiation of an MCVideo emergency group call. | | | | |

### 13.2.38D2 /*<x>*/<x>/Common/MCVideoGroupCall/EmergencyCall/ MCVideoGroupInitiation/Entry

Table 13.2.38D2.1: /*<x>*/<x>/Common/MCVideoGroupCall/EmergencyCall/MCVideoGroupInitiation/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideoGroupCall/EmergencyCall/MCVideoGroupInitiation/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the details of the group used on initiation of an MCVideo emergency group call. | | | | |

### 13.2.38D3 /*<x>*/*<x>*/Common/MCVideoGroupCall/EmergencyCall/ MCVideoGroupInitiation/Entry/GroupID

Table 13.2.38D3.1: /*<x>*/<x>/Common/MCVideoGroupCall/EmergencyCall/MCVideoGroupInitiation/Entry/GroupID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideoGroupCall/EmergencyCall/MCVideoGroupInitiation/Entry/GroupID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates the group used upon certain criteria on initiation of an MCVideo emergency group call. | | | | |

### 13.2.38D4 /*<x>*/*<x>*/Common/MCVideoGroupCall/EmergencyCall/ MCVideoGroupInitiation/Entry/DisplayName

Table 13.2.38D4.1: /*<x>*/<x>/Common/MCVideoGroupCall/EmergencyCall/MCVideoGroupInitiation/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideoGroupCall/EmergencyCall/MCVideoGroupInitiation/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name that corresponds to the Group ID. | | | | |

### 13.2.38D5 /*<x>*/*<x>*/Common/MCVideoGroupCall/EmergencyCall/ MCVideoGroupInitiation/Entry/Usage

Table 13.2.38D5.1: /*<x>*/<x>/Common/MCVideoGroupCall/EmergencyCall/MCVideoGroupInitiation/Entry/Usage

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideoGroupCall/EmergencyCall/MCVideoGroupInitiation/Entry/Usage | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the criteria to determine when initiation of an MCVideo emergency group call uses the GroupID. | | | | |

The valid values are 'UseCurrentlySelectedGroup' and 'DedicatedGroup'.

When set to 'UseCurrentlySelectedGroup' then if the MCVideo user has currently selected an MCVideo group then use that MCVideo group for an on-network MCVideo emergency group call, if the MCVideo user does not have a currently selected MCVideo group then use the MCVideo group identified by the GroupID in clause 13.2.38D3 for an MCVideo emergency group call.

When set to 'DedicatedGroup' then use the MCVideo group identified by the GroupID in clause 13.2.38D3 for an MCVideo emergency group call.

### 13.2.38E /*<x>*/*<x>*/Common/MCVideoGroupCall/ImminentPerilCall

Table 13.2.38E.1: /*<x>*/<x>/Common/MCVideoGroupCall/ImminentPerilCall

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideoGroupCall/ImminentPerilCall | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the MCVideo imminent peril call policy. | | | | |

### 13.2.38F /*<x>*/*<x>*/Common/MCVideoGroupCall/ImminentPerilCall/ Authorised

Table 13.2.38F.1: /*<x>*/<x>/Common/MCVideoGroupCall/ImminentPerilCall/Authorised

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideoGroupCall/ImminentPerilCall/Authorised | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to make an Imminent Peril group call. | | | | |

When set to "true" the MCVideo user is authorised to create an MCVideo imminent peril group call.

When set to "false" the MCVideo user is not authorised to create an MCVideo imminent peril group call.

### 13.2.38G /*<x>*/*<x>*/Common/MCVideoGroupCall/ImminentPerilCall/Cancel

Table 13.2.38G.1: /*<x>*/<x>/Common/MCVideoGroupCall/ImminentPerilCall/Cancel

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideoGroupCall/ImminentPerilCall/Cancel | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation for in-progress MCVideo imminent peril cancelation. | | | | |

When set to "true" the MCVideo user is authorised to cancel an MCVideo imminent peril call.

When set to "false" the MCVideo user is not authorised to cancel an MCVideo imminent peril call.

### 13.2.38G1 /*<x>*/*<x>*/Common/MCVideoGroupCall/ImminentPerilCall/ MCVideoGroupInitiation

Table 13.2.38G1.1: /*<x>*/<x>/Common/MCVideoGroupCall/ImminentPerilCall/MCVideoGroupInitiation

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideoGroupCall/ImminentPerilCall/MCVideoGroupInitiation | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the group used on initiation of an MCVideo imminent peril group call. | | | | |

### 13.2.38G2 /*<x>*/<x>/Common/MCVideoGroupCall/ImminentPerilCall/ MCVideoGroupInitiation/Entry

Table 13.2.38G2.1: /*<x>*/<x>/Common/MCVideoGroupCall/ImminentPerilCall/MCVideoGroupInitiation/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideoGroupCall/ImminentPerilCall/MCVideoGroupInitiation/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the details of the group used on initiation of an imminent peril call. | | | | |

### 13.2.38G3 /*<x>*/*<x>*/Common/MCVideoGroupCall/ImminentPerilCall/ MCVideoGroupInitiation/Entry/GroupID

Table 13.2.38G3.1: /*<x>*/<x>/Common/MCVideoGroupCall/ImminentPerilCall/MCVideoGroupInitiation/Entry/GroupID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideoGroupCall/ImminentPerilCall/MCVideoGroupInitiation/Entry/GroupID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the group used upon certain criteria on initiation of an MCVideo imminent peril group call. | | | | |

### 13.2.38G4 /*<x>*/*<x>*/Common/MCVideoGroupCall/ImminentPerilCall/ MCVideoGroupInitiation/DisplayName

Table 13.2.38G4.1: /*<x>*/<x>/Common/MCVideoGroupCall/ImminentPerilCall/MCVideoGroupInitiation/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideoGroupCall/ImminentPerilCall/MCVideoGroupInitiation/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name that corresponds to the Group ID. | | | | |

### 13.2.38G5 /*<x>*/*<x>*/Common/MCVideoGroupCall/ImminentPerilCall/ MCVideoGroupInitiation/Entry/Usage

Table 13.2.38G5.1: /*<x>*/<x>/Common/MCVideoGroupCall/ImminentPerilCall/MCVideoGroupInitiation/Entry/Usage

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideoGroupCall/ImminentPerilCall/MCVideoGroupInitiation/Entry/Usage | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the criteria to determine when initiation of an MCVideo imminent peril group call uses the GroupID. | | | | |

The valid values are 'UseCurrentlySelectedGroup' and 'DedicatedGroup'.

When set to 'UseCurrentlySelectedGroup' then if the MCVideo user has currently selected an MCVideo group then use that MCVideo group for an on-network MCVideo imminent peril group call, if the MCVideo user does not have a currently selected MCVideo group then use the MCVideo group identified by the GroupID in clause 13.2.38G3 for an MCVideo imminent peril group call.

When set to 'DedicatedGroup' then use the MCVideo group identified by the GroupID in clause 13.2.38G3 for an MCVideo imminent peril group call.

### 13.2.38G6 /*<x>*/*<x>*/Common/MCVideoGroupCall/Priority

Table 13.2.38G6.1: /*<x>*/<x>/Common/MCVideoGroupCall/Priority

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideoGroupCall/Priority | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the priority of the MCVideo group calls. | | | | |

- Values: 0-255

The MCVideo group call with the lowest Priority value shall be considered as the MCVideo group call having the lowest level among the MCVideo group calls.

### 13.2.38G7 /*<x>*/*<x>*/Common/MCVideoGroupCall/ MaxSimultaneousCallsN6

Table 13.2.38G7.1: /*<x>*/<x>/Common/MCVideoGroupCall/MaxSimultaneousCallsN6

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/MCVideoGroupCall/MaxSimultaneousCallsN6 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the maximum number of simultaneously received MCVideo group calls (N6). | | | | |

### 13.2.38H /*<x>*/*<x>*/Common/PrivateCall

Table 13.2.38H.1: /*<x>*/<x>/Common/PrivateCall

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the MCVideo private call configuration. | | | | |

### 13.2.38I /*<x>*/*<x>*/Common/PrivateCall/Authorised

Table 13.2.38I.1: /*<x>*/<x>/Common/PrivateCall/Authorised

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/Authorised | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to make a MCVideo private call. | | | | |

### 13.2.38I1 /*<x>*/*<x>*/Common/PrivateCall/AuthorisedAny

Table 13.2.38I1.1: /*<x>*/<x>/Common/PrivateCall/AuthorisedAny

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/AuthorisedAny | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to make a MCVideo private call to any MCVideo user. | | | | |

When set to "true" the MCVideo user is authorised to make an MCVideo private call to any MCVideo user.

When set to "false" the MCVideo user is not authorised to make an MCVideo private call to any MCVideo user.

### 13.2.38I2 /*<x>*/<x>/Common/PrivateCall/UserList

Table 13.2.38I2.1: /*<x>*/<x>/Common/PrivateCall/UserList

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/UserList | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for a list of MCVideo user(s) who can be called in a MCVideo private call. | | | | |

### 13.2.38I3 /*<x>*/<x>/Common/PrivateCall/UserList/<x>

Table 13.2.38I3.1: /*<x>*/<x>/Common/PrivateCall/UserList/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/UserList/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more list of MCVideo users who can be called in a MCVideo private call. | | | | |

### 13.2.38I4 /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry

Table 13.2.38I4.1: /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/UserList/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more MCVideo users who can be called in a private call. | | | | |

### 13.2.38I5 /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry/ MCVideoID

Table 13.2.38I5.1: /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry/MCVideoID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/UserList/<x>/Entry/MCVideoID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates an MCVideo user identity (MCVideo ID) which is a globally unique identifier within the MCVideo service that represents the MCVideo user. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 13.2.38I6 /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry/ DiscoveryGroupID

Table 13.2.38I6.1: /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry/DiscoveryGroupID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/UserList/<x>/Entry/DiscoveryGroupID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | int | Get, Replace |  |
|  | This leaf node indicates a discovery group ID as specified in 3GPP TS 23.303 [6]. | | | | |

The value is used as the discovery group ID in the ProSe discovery procedures as specified in 3GPP TS 23.303 [6].

### 13.2.38I7 /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry/UserInfoID

Table 13.2.38I7.1: /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry/UserInfoID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/UserList/<x>/Entry/UserInfoID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | int | Get, Replace |  |
|  | This leaf node indicates a ProSe user info ID as specified in 3GPP TS 23.303 [6]. | | | | |

### 13.2.38I8 /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry/ DisplayName

Table 13.2.38I8.1: /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/UserList/<x>/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name. | | | | |

### 13.2.38I9 /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry/ PrivateCallKMSURI

Table 13.2.38I9.1: /*<x>*/<x>/Common/PrivateCall/UserList/<x>/Entry/PrivateCallKMSURI

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/UserList/<x>/Entry/PrivateCallKMSURI | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates the identity (URI) of the KMS associated with the MCVideoID. If the value is empty, the KMS leaf node present in the MCS UE initial configuration MO is used. | | | | |

### 13.2.38J /*<x>*/*<x>*/Common/PrivateCall/ManualCommence

Table 13.2.38J.1: /*<x>*/<x>/Common/PrivateCall/ManualCommence

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/ManualCommence | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to make a MCVideo private call with manual commencement. | | | | |

When set to "true" the MCVideo user is authorised to make a MCVideo private call in manual commencement mode.

When set to "false" the MCVideo user is not authorised to make a MCVideo private call in manual commencement mode.

### 13.2.38K /*<x>*/*<x>*/Common/PrivateCall/AutoCommence

Table 13.2.38K.1: /*<x>*/<x>/Common/PrivateCall/AutoCommence

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/AutoCommence | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to make a MCVideo private call with automatic commencement. | | | | |

When set to "true" the MCVideo user is authorised to make a MCVideo private call in automatic commencement mode.

When set to "false" the MCVideo user is not authorised to make a MCVideo private call in automatic commencement mode.

### 13.2.38L /*<x>*/*<x>*/Common/PrivateCall/FailRestrict

Table 13.2.38L.1: /*<x>*/<x>/Common/PrivateCall/FailRestrict

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/FailRestrict | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to restrict the provision of a notification of call failure reason for a MCVideo private call. | | | | |

When set to "true" the MCVideo user is authorised to restrict notification of call failure reason for MCVideo private call.

When set to "false" the MCVideo user is not authorised to restrict notification of call failure reason for MCVideo private call.

### 13.2.38M Void

### 13.2.38N /*<x>*/*<x>*/Common/PrivateCall/AllowedMediaProtection

Table 13.2.38N.1: /*<x>*/<x>/Common/PrivateCall/AllowedMediaProtection

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/AllowedMediaProtection | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates authorisation to protect confidentiality and integrity of media for MCVideo private calls. | | | | |

When set to "true" the MCVideo user is authorised to protect confidentiality and integrity of media for MCVideo private calls.

When set to "false" the MCVideo user is not authorised to protect confidentiality and integrity of media for MCVideo private calls.

The default value is set to "true".

### 13.2.38O /*<x>*/*<x>*/Common/PrivateCall/EmergencyCall

Table 13.2.38O.1: /*<x>*/<x>/Common/PrivateCall/EmergencyCall

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/EmergencyCall | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the MCVideo emergency call policy. | | | | |

### 13.2.38P /*<x>*/*<x>*/Common/PrivateCall/EmergencyCall/Authorised

Table 13.2.38P.1: /*<x>*/<x>/Common/PrivateCall/EmergencyCall/Authorised

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/EmergencyCall/Authorised | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to make an MCVideo emergency private call. | | | | |

When set to "true" the MCVideo user is authorised to make an MCVideo emergency private call.

When set to "false" the MCVideo user is not authorised to make an MCVideo emergency private call.

### 13.2.38Q /*<x>*/*<x>*/Common/PrivateCall/EmergencyCall/CancelPriority

Table 13.2.38Q.1: /*<x>*/<x>/Common/PrivateCall/EmergencyCall/CancelPriority

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/EmergencyCall/CancelPriority | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation to cancel emergency priority in an MCVideo emergency private call by an authorised MCVideo user. | | | | |

When set to "true" the MCVideo user is authorised to cancel an emergency priority in an MCVideo private call.

When set to "false" the MCVideo user is not authorised to cancel an emergency priority in an MPCTT private call.

### 13.2.38R /*<x>*/*<x>*/Common/PrivateCall/EmergencyCall/ MCVideoPrivateRecipient

Table 13.2.38R.1: /*<x>*/<x>/Common/PrivateCall/EmergencyCall/MCVideoPrivateRecipient

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/EmergencyCall/MCVideoPrivateRecipient | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the MCVideo private recipient for an MCVideo emergency private call. | | | | |

### 13.2.38S /*<x>*/<x>/Common/PrivateCall/EmergencyCall/ MCVideoPrivateRecipient/Entry

Table 13.2.38S.1: /*<x>*/<x>/Common/PrivateCall/EmergencyCall/MCVideoPrivateRecipient/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/EmergencyCall/MCVideoPrivateRecipient/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the details of the MCVideo private recipient for an MCVideo emergency private call. | | | | |

### 13.2.38T /*<x>*/*<x>*/Common/PrivateCall/EmergencyCall/ MCVideoPrivateRecipient/Entry/ID

Table 13.2.38T.1: /*<x>*/<x>/Common/PrivateCall/EmergencyCall/MCVideoPrivateRecipient/Entry/ID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/EmergencyCall/MCVideoPrivateRecipient/Entry/ID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates the MCVideo private recipient used upon certain criteria on initiation of an MCVideo emergency private call. | | | | |

### 13.2.38U /*<x>*/<x>/Common/PrivateCall/EmergencyCall/ MCVideoPrivateRecipient/Entry/DiscoveryGroupID

Table 13.2.38U.1: /*<x>*/<x>/Common/PrivateCall/EmergencyCall/MCVideoPrivateRecipient/Entry/DiscoveryGroupID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/EmergencyCall/MCVideoPrivateRecipient/Entry/DiscoveryGroupID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | int | Get, Replace |  |
|  | This leaf node indicates the discovery group ID as specified in 3GPP TS 23.303 [6]. | | | | |

### 13.2.38V /*<x>*/<x>/Common/PrivateCall/EmergencyCall/ MCVideoPrivateRecipient/Entry/UserInfoID

Table 13.2.38V.1: /*<x>*/<x>/Common/PrivateCall/EmergencyCall/MCVideoPrivateRecipient/Entry/UserInfoID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/EmergencyCall/MCVideoPrivateRecipient/Entry/UserInfoID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | int | Get, Replace |  |
|  | This leaf node indicates a ProSe user info ID as specified in 3GPP TS 23.303 [6]. | | | | |

The "UserInfoID" element identifies the MCVideo private recipient when making an off-network private call.

### 13.2.38W /*<x>*/*<x>*/Common/PrivateCall/EmergencyCall/ MCVideoPrivateRecipient/Entry/DisplayName

Table 13.2.38W.1: /*<x>*/<x>/Common/PrivatepCall/EmergencyCall/MCVideoPrivateRecipient/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/EmergencyCall/MCVideoPrivateRecipient/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name that corresponds to the MCVideo private recipient ID. | | | | |

### 13.2.38X /*<x>*/*<x>*/Common/PrivateCall/EmergencyCall/ MCVideoPrivateRecipient/Entry/Usage

Table 13.2.38X.1: /*<x>*/<x>/Common/PrivateCall/EmergencyCall/MCVideoPrivateRecipient/Entry/Usage

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/EmergencyCall/MCVideoPrivateRecipient/Entry/Usage | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the criteria to determine when initiation of an MCVideo emergency private call uses the MCVideo private recipient ID. | | | | |

The valid values are 'LocallyDetermined' and 'UsePreConfigured'.

When set to 'LocallyDetermined' then if the MCVideo user selects an MCVideo ID then use that MCVideo ID for the MCVideo emergency private call, if the MCVideo user does not select a MCVideo ID then use the MCVideo ID identified by the MCVideo private recipient ID in clause 13.2.38T for an on-network MCVideo emergency private call.

When set to 'UsePreConfigured' then use the MCVideo ID identified by the MCVideo private recipient ID in clause 13.2.38T for an on-network MCVideo emergency private call.

When set to 'LocallyDetermined' then if the MCVideo user selects an MCVideo user then use the UserInfoID that corresponds to that MCVideo user for the MCVideo emergency private call, if the MCVideo user does not select a MCVideo user then use the User Info ID identified by the UserInfoID in clause 13.2.38T for an off-network MCVideo emergency private call.

When set to 'UsePreConfigured' then use the User Info ID identified by the UserInfoID in clause 13.2.38T for an off-network MCVideo emergency private call.

### 13.2.38Y /*<x>*/*<x>*/Common/PrivateCall/AutoAnswer

Table 13.2.38Y.1: /*<x>*/<x>/Common/PrivateCall/AutoAnswer

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/Common/PrivateCall/AutoAnswer | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation of MCVideo user to force automatic answer for a MCVideo private call. | | | | |

When set to "true" the MCVideo user is authorised to force automatic answer for a MCVideo private call.

When set to "false" the MCVideo user is not authorised to force automatic answer for a MCVideo private call.

### 13.2.39 /*<x>*/*<x>*/OnNetwork

Table 13.2.39.1: /*<x>*/<x>/OnNetwork

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | node | Get, Replace |  |
|  | This interior node represents a container for on-network operation. | | | | |

### 13.2.40 /*<x>*/*<x>*/OnNetwork/MCVideoGroupList

Table 13.2.40.1: /*<x>*/<x>/OnNetwork/MCVideoGroupList

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCVideoGroupList | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the list of on-network MCVideo groups that the MCVideo user is allowed to use. | | | | |

### 13.2.41 /*<x>*/<x>/OnNetwork/MCVideoGroupList/<x>

Table 13.2.41.1: /*<x>*/<x>/OnNetwork/MCVideoGroupList/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCVideoGroupList/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more list of on-network MCVideo groups that the MCVideo user is allowed to use. | | | | |

### 13.2.42 /*<x>*/<x>/OnNetwork/MCVideoGroupList/<x>/Entry

Table 13.2.42.1: /*<x>*/<x>/OnNetwork/MCVideoGroupList/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCVideoGroupList/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the details of the on-network MCVideo groups that the MCVideo user is allowed to use. | | | | |

### 13.2.43 /*<x>*/<x>/OnNetwork/MCVideoGroupList/<x>/Entry/ MCVideoGroupID

Table 13.2.43.1: /*<x>*/<x>/OnNetwork/MCVideoGroupList/<x>/Entry/MCVideoGroupID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCVideoGroupList/<x>/Entry/MCVideoGroupID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the MCVideo group ID for the on-network MCVideo group that the MCVideo user is allowed to use. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 13.2.44 /*<x>*/*<x>*/OnNetwork/MCVideoGroupList/<x>/Entry/ DisplayName

Table 13.2.44.1: /*<x>*/<x>/OnNetwork/MCVideoGroupList/<x>/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCVideoGroupList/<x>/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name that corresponds to the MCVideo Group ID. | | | | |

### 13.2.45 Void

### 13.2.46 Void

### 13.2.47 /*<x>*/<x>/OnNetwork/MCVideoGroupList/<x>/Entry/GMSServID

Table 13.2.47.1: /*<x>*/<x>/OnNetwork/MCVideoGroupList/<x>/Entry/GMSServID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCVideoGroupList/<x>/Entry/GMSServID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates the identity (URI) of the group management server hosting the MCVideo Group ID. | | | | |

### 13.2.48 Void

### 13.2.49 Void

### 13.2.50 /*<x>*/<x>/OnNetwork/MCVideoGroupList/<x>/Entry/ IdMSTokenEndPoint

Table 13.2.50.1: /*<x>*/<x>/OnNetwork/MCVideoGroupList/<x>/Entry/IdMSTokenEndPoint

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCVideoGroupList/<x>/Entry/IdMSTokenEndPoint | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates the identity (URI) of the identity management server hosting the MCVideo Group ID. | | | | |

### 13.2.50A Void

### 13.2.50B Void

### 13.2.50C Void

### 13.2.50D /<x>/<x>/OnNetwork/MCVideoGroupList/<x>/Entry/ GroupKMSURI

Table 13.2.50D.1: /*<x>*/<x>/OnNetwork/MCVideoGroupList/<x>/Entry/GroupKMSURI

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCVideoGroupList/<x>/Entry/GroupKMSURI | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the identity (URI) of the KMS identity (URI) for a specific group contained in the MCVideoGroupList. If the value is empty, the KMS identity (URI) (kms) present in the MCS UE initial configuration MO is used. | | | | |

### 13.2.51 /*<x>*/<x>/OnNetwork/MCVideoGroupList/<x>/Entry/ RelativePresentationPriority

Table 13.2.51.1: /*<x>*/<x>/OnNetwork/MCVideoGroupList/<x>/Entry/RelativePresentationPriority

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MCVideoGroupList/<x>/Entry/RelativePresentationPriority | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | int | Get, Replace |  |
|  | This leaf node indicates indicating the presentation priority of the on-network group for the MCVideo user relative to other on-network groups and on-network users. | | | | |

- Values: 0-255

The lowest RelativePresentationPriority value shall be considered as the MCVideo group transaction having the lowest priority for presentation among other group MCVideo and one-to-one user transactions.

### 13.2.52 /*<x>*/*<x>*/OnNetwork/ImplicitAffiliations

Table 13.2.52.1: /*<x>*/<x>/OnNetwork/ImplicitAffiliations

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/ImplicitAffiliations | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the implicit affiliation configuration. | | | | |

### 13.2.53 /*<x>*/<x>/OnNetwork/ImplicitAffiliations/<x>

Table 13.2.53.1: /*<x>*/<x>/OnNetwork/ImplicitAffiliations/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/ImplicitAffiliations/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for zero or more implicit affiliation configuration. | | | | |

### 13.2.54 /*<x>*/<x>/OnNetwork/ImplicitAffiliations/<x>/Entry

Table 13.2.54.1: /*<x>*/<x>/OnNetwork/ImplicitAffiliations/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/ImplicitAffiliations/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the details of the on-network MCVideo groups that the MCVideo user is implicitly affiliated to. | | | | |

### 13.2.55 /*<x>*/<x>/OnNetwork/ImplicitAffiliations/<x>/Entry/ MCVideoGroupID

Table 13.2.55.1: /*<x>*/<x>/OnNetwork/ImplicitAffiliations/<x>/Entry/MCVideoGroupID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/ImplicitAffiliations/<x>/Entry/MCVideoGroupID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates a MCVideo group ID to which the MCVideo user is implicitly affiliated to. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 13.2.56 /*<x>*/*<x>*/OnNetwork/ImplicitAffiliations/<x>/Entry/ DisplayName

Table 13.2.56.1: /*<x>*/<x>/OnNetwork/ImplicitAffiliations/<x>/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/ImplicitAffiliations/<x>/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name that corresponds to the MCVideo Group ID. | | | | |

### 13.2.57 /*<x>*/*<x>*/OnNetwork/PresenceStatus

Table 13.2.57.1: /*<x>*/<x>/OnNetwork/PresenceStatus

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/PresenceStatus | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the presence status configuration. | | | | |

### 13.2.58 /*<x>*/<x>/OnNetwork/PresenceStatus/<x>

Table 13.2.58.1: /*<x>*/<x>/OnNetwork/PresenceStatus/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/PresenceStatus/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for zero or more presence status configuration. | | | | |

### 13.2.59 /*<x>*/<x>/OnNetwork/PresenceStatus/<x>/Entry

Table 13.2.59.1: /*<x>*/<x>/OnNetwork/PresenceStatus/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/PresenceStatus/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the details of the MCVideo IDs of MCVideo users that the configured MCVideo user is authorised to obtain presence status. | | | | |

### 13.2.60 /*<x>*/<x>/OnNetwork/PresenceStatus/<x>/Entry/ MCVideoGroupID

Table 13.2.60.1: /*<x>*/<x>/OnNetwork/PresenceStatus/<x>/Entry/MCVideoGroupID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/PresenceStatus/<x>/Entry/MCVideoGroupID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates an MCVideo ID of an MCVideo user that the configured MCVideo user is authorised to obtain presence status. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 13.2.61 /*<x>*/*<x>*/OnNetwork/PresenceStatus/<x>/Entry/DisplayName

Table 13.2.61.1: /*<x>*/<x>/OnNetwork/PresenceStatus/<x>/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/PresenceStatus/<x>/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name that corresponds to the MCVideo ID. | | | | |

### 13.2.62 Void

### 13.2.63 Void

### 13.2.64 Void

### 13.2.65 Void

### 13.2.66 Void

### 13.2.67 /*<x>*/<x>/OnNetwork/MaxAffiliationsN2

Table 13.2.67.1: /*<x>*/<x>/OnNetwork/MaxAffiliationsN2

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MaxAffiliationsN2 | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | int | Get, Replace |  |
|  | This leaf node indicates the maximum number of MCVideo groups that the MCVideo user is authorised to affiliate with. | | | | |

- Values: 0-65535

### 13.2.68 /*<x>*/*<x>*/OnNetwork/AllowedRegroup

Table 13.2.68.1: /*<x>*/<x>/OnNetwork/AllowedRegroup

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/AllowedRegroup | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCVideo user is authorised to perform dynamic regrouping operations. | | | | |

When set to "true" the MCVideo user is authorised to perform dynamic regrouping operations.

When set to "false" the MCVideo user is not authorised to perform dynamic regrouping operations.

### 13.2.69 /*<x>*/*<x>*/OnNetwork/AllowedPresenceStatus

Table 13.2.69.1: /*<x>*/<x>/OnNetwork/AllowedPresenceStatus

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/AllowedPresenceStatus | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | bool | Get, Replace |  |
|  | This leaf node indicates the presence status on the network of this MCVideo user is available. | | | | |

When set to "true" the presence status on the network of this MCVideo user is available.

When set to "false" the presence status on the network of this MCVideo user is not available. This is the default if this leaf node is not present.

### 13.2.70 /*<x>*/*<x>*/OnNetwork/AllowedPresence

Table 13.2.70.1: /*<x>*/<x>/OnNetwork/AllowedPresence

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/AllowedPresence | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCVideo user is authorised to obtain whether a particular MCVideo User is present on the network. | | | | |

When set to "true" the MCVideo user is authorised to obtain whether a particular MCVideo User is present on the network.

When set to "false" the MCVideo user is not authorised to obtain whether a particular MCVideo User is present on the network. This is the default if this leaf node is not present.

### 13.2.71 /*<x>*/*<x>*/OnNetwork/AllowedManualSwitch

Table 13.2.71.1: /*<x>*/<x>/OnNetwork/AllowedManualSwitch

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/AllowedManualSwitch | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCVideo user is authorised to manually switch to off-network operation while in on-network operation. | | | | |

When set to "true" the MCVideo user is authorised to manually switch to off-network operation while in on-network operation.

When set to "false" the MCVideo user is not authorised to manually switch to off-network operation while in on-network operation.

### 13.2.72 Void

### 13.2.73 /*<x>*/*<x>*/OnNetwork/MaxSimultaneousVideoStreams

Table 13.2.73.1: /*<x>*/<x>/OnNetwork/MaxSimultaneousVideoStreams

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MaxSimultaneousVideoStreams | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for maximum number of simultaneous video streams that can be received. | | | | |

### 13.2.74 /*<x>*/<x>/OnNetwork/MaxSimultaneousVideoStreams/ MaxStreams

Table 13.2.74.1: /*<x>*/<x>/OnNetwork/MaxSimultaneousVideoStreams/MaxStreams

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/MaxSimultaneousVideoStreams/MaxStreams | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | int | Get, Replace |  |
|  | This leaf node indicates the maximum number of simultaneous video streams that can be received. | | | | |

- Values: 1-65535

### 13.2.75 Void

### 13.2.76 Void

### 13.2.77 Void

### 13.2.78 Void

### 13.2.79 Void

### 13.2.80 Void

### 13.2.81 Void

### 13.2.82 Void

### 13.2.83 Void

### 13.2.84 Void

### 13.2.85 Void

### 13.2.86 Void

### 13.2.87 Void

### 13.2.87A /*<x>*/*<x>*/OnNetwork/EnabledParticipation

Table 13.2.87A.1: /*<x>*/<x>/OnNetwork/EnabledParticipation

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/EnabledParticipation | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates whether the MCVideo user is allowed to participate in MCVideo private calls that they are invited to. | | | | |

When set to "true" the MCVideo user is allowed to participate in MCVideo private calls that they are invited to.

When set to "false" the MCVideo user is not allowed to participate in MCVideo private calls that they are invited to.

### 13.2.87A1 /*<x>*/*<x>*/OnNetwork/AllowedRemoteInitiatedAmbientViewing

Table 13.2.87A1.1: /*<x>*/<x>/AllowedRemoteInitiatedAmbientViewing

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/AllowedRemoteInitiatedAmbientViewing | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | bool | Get, Replace |  |
|  | This leaf node indicates the presence status on the network of this MCVideo user is available. | | | | |

When set to "true" the MCVideo user is authorised to remotely initiate ambient viewing at another MCVideo user's device.

When set to "false" the MCVideo user is not authorised to remotely initiate ambient viewing at another MCVideo user's device.

### 13.2.87A2 /*<x>*/*<x>*/OnNetwork/AllowedLocallyInitiatedAmbientViewing

Table 13.2.87A2.1: /*<x>*/<x>/OnNetwork/AllowedLocallyInitiatedAmbientViewing

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/AllowedLocallyInitiatedAmbientViewing | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | bool | Get, Replace |  |
|  | This leaf node indicates the presence status on the network of this MCVideo user is available. | | | | |

When set to "true" the MCVideo user is authorised to locally initiate ambient viewing.

When set to "false" the MCVideo user is not authorised to locally initiate ambient viewing.

### 13.2.87D /*<x>*/*<x>*/OnNetwork/PrivateCall

Table 13.2.87D.1: /*<x>*/<x>/OnNetwork/PrivateCall

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/PrivateCall | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the MCVideo private call configuration. | | | | |

### 13.2.87E /*<x>*/*<x>*/OnNetwork/PrivateCall/EmergencyAlert

Table 13.2.87E.1: /*<x>*/<x>/OnNetwork/PrivateCall/EmergencyAlert

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/PrivateCall/EmergencyAlert | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the MCVideo private emergency alert policy. | | | | |

### 13.2.87F /*<x>*/*<x>*/OnNetwork/PrivateCall/EmergencyAlert/Entry

Table 13.2.87F.1: /*<x>*/<x>/OnNetwork/PrivateCall/EmergencyAlert/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/PrivateCall/EmergencyAlert/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the details of an MCVideo private emergency alert for on-network. | | | | |

### 13.2.87G /*<x>*/*<x>*/OnNetwork/PrivateCall/EmergencyAlert/Entry/ID

Table 13.2.87G.1: /*<x>*/<x>/OnNetwork/PrivateCall/EmergencyAlert/Entry/ID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/PrivateCall/EmergencyAlert/Entry/ID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the MCVideo user ID used upon certain criteria on initiation of an MCVideo private emergency alert for on-network. | | | | |

### 13.2.87H /*<x>*/*<x>*/OnNetwork/PrivateCall/EmergencyAlert/Entry/ DisplayName

Table 13.2.87H.1: /*<x>*/<x>/OnNetwork/PrivateCall/EmergencyAlert/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/PrivateCall/EmergencyAlert/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name that corresponds to the ID. | | | | |

### 13.2.87I /*<x>*/*<x>*/OnNetwork/PrivateCall/EmergencyAlert/Entry/Usage

Table 13.2.87I.1: /*<x>*/<x>/OnNetwork/PrivateCall/EmergencyAlert/Entry/Usage

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/PrivateCall/EmergencyAlert/Entry/Usage | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the criteria to determine when initiation of an MCVideo private emergency alert uses the ID. | | | | |

The valid values are 'LocallyDetermined' and 'UsePreConfigured'.

When set to 'LocallyDetermined' then if the MCVideo user selects an MCVideo ID then use that MCVideo ID for an on-network MCVideo private emergency alert, if the MCVideo user does not select a MCVideo ID then use the MCVideo ID identified by the ID in clause 13.2.38I12 for an on-network MCVideo private emergency alert.

When set to 'UsePreConfigured' then use the ID identified by the ID in clause 13.2.38I12 for an on-network MCVideo private emergency alert.

### 13.2.87J /*<x>*/*<x>*/OnNetwork/RemoteGroupSelection

Table 13.2.87J.1: /*<x>*/<x>/OnNetwork/RemoteGroupSelection

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/RemoteGroupSelection | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the remote group selection configuration. | | | | |

### 13.2.87K /*<x>*/<x>/OnNetwork/RemoteGroupSelection/<x>

Table 13.2.87K.1: /*<x>*/<x>/OnNetwork/RemoteGroupSelection/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/RemoteGroupSelection/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more remote group selection configuration elements. | | | | |

### 13.2.87L /*<x>*/<x>/OnNetwork/RemoteGroupSelection/<x>/Entry

Table 13.2.87L.1: /*<x>*/<x>/OnNetwork/RemoteGroupSelection/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/RemoteGroupSelection/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the details of the on-network MCVideo users whose selected MCVideo group is allowed to be remotely changed by the MCVideo user. | | | | |

### 13.2.87M /*<x>*/<x>/OnNetwork/RemoteGroupSelection/<x>/Entry/ MCVideoID

Table 13.2.87M.1: /*<x>*/<x>/OnNetwork/RemoteGroupSelection/<x>/Entry/MCVideoID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/RemoteGroupSelection/<x>/Entry/MCVideoID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates a MCVideo ID of an MCVideo user whose selected MCVideo group is allowed to be remotely changed by the MCVideo user. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 13.2.87N /*<x>*/*<x>*/OnNetwork/RemoteGroupSelection/<x>/Entry/ DisplayName

Table 13.2.87N.1: /*<x>*/<x>/OnNetwork/RemoteGroupSelection/<x>/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OnNetwork/RemoteGroupSelection/<x>/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name that corresponds to the MCVideo ID of the MCVideo user. | | | | |

### 13.2.88 /*<x>*/*<x>*/OffNetwork

Table 13.2.88.1: /*<x>*/<x>/OffNetwork

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | node | Get, Replace |  |
|  | This interior node represents a container for off-network operation. | | | | |

### 13.2.89 /*<x>*/*<x>*/OffNetwork/Authorised

Table 13.2.89.1: /*<x>*/<x>/OffNetwork/Authorised

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/Authorised | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorisation for off-network services. | | | | |

When set to "true" the MCVideo user is authorised for off-network operation.

When set to "false" the MCVideo user is not authorised for off-network operation.

### 13.2.90 /*<x>*/*<x>*/OffNetwork/MCVideoGroupList

Table 13.2.90.1: /*<x>*/<x>/OffNetwork/MCVideoGroupList

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCVideoGroupList | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the list of off-network MCVideo groups that the MCVideo user is allowed to use. | | | | |

### 13.2.91 /*<x>*/<x>/OffNetwork/MCVideoGroupList/<x>

Table 13.2.91.1: /*<x>*/<x>/OffNetwork/MCVideoGroupList/<x>

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCVideoGroupList/<x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get, Replace |  |
|  | This interior node is a placeholder for one or more list of off-network MCVideo groups that the MCVideo user is allowed to use. | | | | |

### 13.2.92 /*<x>*/<x>/OffNetwork/MCVideoGroupList/<x>/Entry

Table 13.2.92.1: /*<x>*/<x>/OffNetwork/MCVideoGroupList/<x>/Entry

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCVideoGroupList/<x>/Entry | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the details of the off-network MCVideo groups that the MCVideo user is allowed to use. | | | | |

### 13.2.93 /*<x>*/<x>/OffNetwork/MCVideoGroupList/<x>/Entry/ MCVideoGroupID

Table 13.2.93.1: /*<x>*/<x>/OffNetwork/MCVideoGroupList/<x>/Entry/MCVideoGroupID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCVideoGroupList/<x>/Entry/MCVideoGroupID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the MCVideo group ID for the off-network MCVideo group that the MCVideo user is allowed to use. | | | | |

The value is a "uri" attribute specified in OMA OMA-TS-XDM\_Group-V1\_1 [4].

### 13.2.94 /*<x>*/*<x>*/OffNetwork/MCVideoGroupList/<x>/Entry/DisplayName

Table 13.2.94.1: /*<x>*/<x>/OffNetwork/MCVideoGroupList/<x>/Entry/DisplayName

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCVideoGroupList/<x>/Entry/DisplayName | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node contains a human readable name that corresponds to the MCVideo Group ID. | | | | |

### 13.2.95 Void

### 13.2.96 Void

### 13.2.97 /*<x>*/<x>/OffNetwork/MCVideoGroupList/<x>/Entry/GMSServID

Table 13.2.97.1: /*<x>*/<x>/OffNetwork/MCVideoGroupList/<x>/Entry/GMSServID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCVideoGroupList/<x>/Entry/GMSServID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates the identity (URI) of the group management server hosting the MCVideo Group ID. | | | | |

### 13.2.98 Void

### 13.2.99 Void

### 13.2.100 /*<x>*/<x>/OffNetwork/MCVideoGroupList/<x>/Entry/ IdMSTokenEndPoint

Table 13.2.100.1: /*<x>*/<x>/OffNetwork/MCVideoGroupList/<x>/Entry/IdMSTokenEndPoint

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCVideoGroupList/<x>/Entry/IdMSTokenEndPoint | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | chr | Get, Replace |  |
|  | This leaf node indicates the identity (URI) of the identity management server hosting the MCVideo Group ID. | | | | |

### 13.2.100A Void

### 13.2.100B Void

### 13.2.100C /*<x>*/*<x>*/OffNetwork/MCVideoGroupList/<x>/Entry/ GroupKMSURI

Table 13.2.100C.1: /*<x>*/<x>/OffNetwork/MCVideoGroupList/<x>/Entry/GroupKMSURI

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCVideoGroupList/<x>/Entry/GroupKMSURI | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the identity (URI) of the KMS identity (URI) for a specific group contained in the off-network MCVideoGroupList. If the value is empty, the KMS identity (URI) (kms) present in the MCS UE initial configuration MO is used. | | | | |

### 13.2.101 /*<x>*/<x>/OffNetwork/MCVideoGroupList/<x>/Entry/ RelativePresentationPriority

Table 13.2.101.1: /*<x>*/<x>/OffNetwork/MCVideoGroupList/<x>/Entry/RelativePresentationPriority

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/MCVideoGroupList/<x>/Entry/RelativePresentationPriority | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | int | Get, Replace |  |
|  | This leaf node indicates indicating the presentation priority of the off-network group for the MCVideo user relative to other off-network groups and off-network users. | | | | |

- Values: 0-255

The lowest RelativePresentationPriority value shall be considered as the MCVideo group transaction having the lowest priority for presentation among other group MCVideo and one-to-one user transactions.

### 13.2.102 /*<x>*/*<x>*/OffNetwork/UserInfoID

Table 13.2.102.1: /*<x>*/<x>/OffNetwork/UserInfoID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/UserInfoID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | chr | Get, Replace |  |
|  | This leaf node indicates the ProSe user info ID as specified in 3GPP TS 23.303 [6]. | | | | |

### 13.2.102A /*<x>*/*<x>*/OffNetwork/EmergencyCallChange

Table 13.2.102A.1: /*<x>*/<x>/OffNetwork/EmergencyCallChange

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/EmergencyCallChange | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorization for a participant to change an off-network group call in-progress to an off-network MCVideo emergency group call. | | | | |

When set to "true" the MCVideo user is authorised to change an MCVideo emergency group call.

When set to "false" the MCVideo user is not authorised to change an MCVideo emergency group call.

### 13.2.102B /*<x>*/*<x>*/OffNetwork/ImminentPerilCallChange

Table 13.2.102B.1: /*<x>*/<x>/OffNetwork/ImminentPerilCallChange

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x>/OffNetwork/ImminentPerilCallChange | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | bool | Get, Replace |  |
|  | This leaf node indicates the authorization for a participant to change an off-network group call in-progress to an off-network MCVideo imminent peril group call. | | | | |

When set to "true" the MCVideo user is authorised to change an MCVideo imminent peril group call.

When set to "false" the MCVideo user is not authorised to change an MCVideo imminent peril group call.

### 13.2.103 /*<x>*/Status

Table 13.2.103.1: /*<x>*/Status

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Status | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | One | bool | Get, Replace |  |
|  | This leaf node indicates whether this MCVideo user profile is enabled or disabled. | | | | |

When set to "true" this MCVideo user profile is enabled.

When set to "false" this MCVideo user profile is disabled.

# 14 MCVideo service configuration MO

## 14.1 General

The MCVideo service configuration Management Object (MO) is used to configure MCVideo Client behaviour for the on-network or off-network MCVideo Service. The MCVideo service configuration parameters may be stored in the ME, or in the USIM as specified in 3GPP TS 31.102 [10], or in both the ME and the USIM. If both the ME and the USIM contain the same parameters, the values stored in the USIM shall take precedence.

The Management Object Identifier is: urn:oma:mo:ext-3gpp-MCVideo-service-configuration:1.0.

Protocol compatibility: This MO is compatible with OMA OMA DM 1.2 [3].

The OMA DM ACL property mechanism (see OMA OMA-ERELD-DM-V1\_2 [2]) may be used to grant or deny access rights to OMA DM servers in order to modify nodes and leaf objects of the MCVideo service configuration MO.

The following nodes and leaf objects are possible under the MCVideo service configuration node as described in figure 14.1.1.



Figure 14.1.1: The MCVideo service configuration MO

## 14.2 MCVideo service configuration MO parameters

### 14.2.1 General

This clause describes the parameters for the MCVideo service configuration Management Object (MO).

### 14.2.2 Node: *<x>*

Table 14.2.2.1: Node: *<x>*

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| <x> | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | OneOrMore | node | Get |  |
|  | This interior node acts as a placeholder for the MCVideo service configuration Management Object (MO).  For the MCVideo service configuration MO, the namespace specific string is: "urn:oma:mo:oma-dm-mcvideo-service configuration:1.0" | | | | |

- Values: N/A

### 14.2.3 /*<x>*/Name

Table 14.2.3.1: /*<x>*/Name

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | chr | Get |  |
|  | The Name leaf is a name for the MCVideo service configuration settings. | | | | |

- Values: <User displayable name>

### 14.2.4 /*<x>*/Ext/

Table 14.2.4.1: /*<x>*/Ext/

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Ext | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Optional | ZeroOrOne | node | Get, Replace |  |
|  | The Ext is an interior node for where the vendor specific information about the MCVideo service configuration MO is being placed. | | | | |

Usually the vendor extension is identified by vendor specific name under the ext node and contains the vendor meaning application vendor, device vendor etc. The tree structure under the vendor identified is not defined and can therefore include one or more un-standardized sub-trees.

- Values: N/A

### 14.2.5 /*<x>*/Common

Table 14.2.5.1: /*<x>*/Common

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | node | Get, Replace |  |
|  | This interior node represents a container for the common network operation which means both on-network operation and off-network operation. | | | | |

### 14.2.6 /*<x>*/Common/BroadcastMCVideoGroupCall

Table 14.2.6.1: /*<x>*/Common/BroadcastMCVideoGroupCall

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/BroadcastMCVideoGroupCall | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for Broadcast MCVideo Group Call configuration. | | | | |

### 14.2.7 /*<x>*/Common/BroadcastMCVideoGroupCall/ NumLevelGroupHierarchy

Table 14.2.7.1: /*<x>*/Common/BroadcastMCVideoGroupCall/NumLevelGroupHierarchy

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/BroadcastMCVideoGroupCall/NumLevelGroupHierarchy | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the number of levels of group hierarchy for group-broadcast groups. | | | | |

- Values: 0-255

The group-broadcast group with the lowest NumLevelGroupHierarchy value shall be considered as the group-broadcast group having the lowest level among the groups.

### 14.2.8 /*<x>*/Common/BroadcastMCVideoGroupCall/ NumLevelUserHierarchy

Table 14.2.8.1: /*<x>*/Common/BroadcastMCVideoGroupCall/NumLevelUserHierarchy

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/BroadcastMCVideoGroupCall/NumLevelUserHierarchy | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the number of levels of user hierarchy for user-broadcast groups. | | | | |

- Values: 0-255

The user-broadcast group with the lowest NumLevelUserHierarchy value shall be considered as the user-broadcast group the lowest level among the groups.

### 14.2.9 /*<x>*/Common/MinLengthAliasID

Table 14.2.9.1: /*<x>*/Common/MinLengthAliasID

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Common/MinLengthAliasID | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates minimum length of an alphanumeric identifier (i.e., alias) assigned by an MCVideo administrator. | | | | |

- Values: 0-255

### 14.2.10 /*<x>*/OffNetwork

Table 14.2.10.1: /*<x>*/OffNetwork

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | ZeroOrOne | node | Get, Replace |  |
|  | This interior node represents a container for off-network operation. | | | | |

### 14.2.11 /*<x>*/OffNetwork/DefaultPPPP

Table 14.2.11.1: /*<x>*/OffNetwork/DefaultPPPP

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/DefaultPPPP | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for the default ProSe Per-Packet Priority (PPPP) configuration. | | | | |

### 14.2.12 /*<x>*/OffNetwork/DefaultPPPP/MCVideoPrivateCallSignalling

Table 14.2.12.1: /*<x>*/OffNetwork/DefaultPPPP/MCVideoPrivateCallSignalling

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/DefaultPPPP/MCVideoPrivateCallSignalling | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the default ProSe Per-Packet Priority (PPPP) value (as specified in 3GPP TS 23.303 [6]) for the MCVideo private call signalling. | | | | |

- Values: 1-8

The MCVideo user data with the lowest ProSe Per-Packet Priority value shall be considered as the MCVideo user data having the highest priority among the MCVideo user data.

### 14.2.13 /*<x>*/OffNetwork/DefaultPPPP/MCVideoPrivateCallMedia

Table 14.2.13.1: /*<x>*/OffNetwork/DefaultPPPP/MCVideoPrivateCallMedia

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/DefaultPPPP/MCVideoPrivateCallMedia | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the default ProSe Per-Packet Priority (PPPP) value (as specified in 3GPP TS 23.303 [6]) for the MCVideo private call media. | | | | |

- Values: 1-8

The MCVideo user data with the lowest ProSe Per-Packet Priority value shall be considered as the MCVideo user data having the highest priority among the MCVideo user data.

### 14.2.14 /*<x>*/OffNetwork/DefaultPPPP/ MCVideoEmergencyPrivateCallSignalling

Table 14.2.14.1: /*<x>*/OffNetwork/DefaultPPPP/MCVideoEmergencyPrivateCallSignalling

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/DefaultPPPP/MCVideoEmergencyPrivateCallSignalling | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the default ProSe Per-Packet Priority (PPPP) value (as specified in 3GPP TS 23.303 [6]) for the MCVideo emerency private call signalling. | | | | |

- Values: 1-8

The MCVideo user data with the lowest ProSe Per-Packet Priority value shall be considered as the MCVideo user data having the highest priority among the MCVideo user data.

### 14.2.15 /*<x>*/OffNetwork/DefaultPPPP/ MCVideoEmergencyPrivateCallMedia

Table 14.2.15.1: /*<x>*/OffNetwork/DefaultPPPP/MCVideoEmergencyPrivateCallMedia

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/DefaultPPPP/MCVideoEmergencyPrivateCallMedia | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the default ProSe Per-Packet Priority (PPPP) value (as specified in 3GPP TS 23.303 [6]) for the MCVideo emerency private call media. | | | | |

- Values: 1-8

The MCVideo user data with the lowest ProSe Per-Packet Priority value shall be considered as the MCVideo user data having the highest priority among the MCVideo user data.

### 14.2.16 /*<x>*/OffNetwork/PrivateCall

Table 14.2.16.1: /*<x>*/OffNetwork/PrivateCall

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/PrivateCall | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | node | Get, Replace |  |
|  | This interior node is a placeholder for private call configuration. | | | | |

### 14.2.17 /*<x>*/OffNetwork/PrivateCall/MaxDuration

Table 14.2.17.1: /*<x>*/OffNetwork/PrivateCall/MaxDuration

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/PrivateCall/MaxDuration | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates max private call duration. | | | | |

- Values: 0-65535

The MaxDuration time is in seconds.

### 14.2.18 /*<x>*/OffNetwork/NumLevelHierarchy

Table 14.2.18.1: /*<x>*/OffNetwork/NumLevelHierarchy

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| OffNetwork/NumLevelHierarchy | | | | | |
|  | Status | Occurrence | Format | Min. Access Types |  |
|  | Required | One | int | Get, Replace |  |
|  | This leaf node indicates the number of levels of hierarchy for transmission control override in off-network. | | | | |

- Values: 4-256

The request with the lowest NumLevelHierarchy value shall be considered as the request having the lowest priority level given to override an active transmission among the requests.

Annex A (informative):  
MCPTT UE configuration MO DDF

This DDF is the standardized minimal set. A vendor can define it's own DDF for the complete device. This DDF can include more features than this minimal standardized version. The DDF is included as an XML file.

Annex B (informative):  
MCPTT user profile MO DDF

This DDF is the standardized minimal set. A vendor can define it's own DDF for the complete device. This DDF can include more features than this minimal standardized version. The DDF is included as an XML file.

Annex C (informative):  
MCS group configuration MO DDF

This DDF is the standardized minimal set. A vendor can define its own DDF for the complete device. This DDF can include more features than this minimal standardized version. The DDF is included as an XML file.

Annex D (informative):  
MCPTT service configuration MO DDF

This DDF is the standardized minimal set. A vendor can define it's own DDF for the complete device. This DDF can include more features than this minimal standardized version. The DDF is included as an XML file.

Annex E (informative):  
MCS UE initial configuration MO DDF

This DDF is the standardized minimal set. A vendor can define its own DDF for the complete device. This DDF can include more features than this minimal standardized version. The DDF is included as an XML file.

Annex F (informative):  
MCVideo UE configuration MO DDF

This DDF is the standardized minimal set. A vendor can define its own DDF for the complete device. This DDF can include more features than this minimal standardized version. The DDF is included as an XML file.

Annex G (informative):  
MCVideo user profile configuration MO DDF

This DDF is the standardized minimal set. A vendor can define its own DDF for the complete device. This DDF can include more features than this minimal standardized version. The DDF is included as an XML file.

Annex H (informative):  
MCVideo service configuration MO DDF

This DDF is the standardized minimal set. A vendor can define its own DDF for the complete device. This DDF can include more features than this minimal standardized version. The DDF is included as an XML file.

Annex I (informative):  
MCData UE configuration MO DDF

This DDF is the standardized minimal set. A vendor can define its own DDF for the complete device. This DDF can include more features than this minimal standardized version. The DDF is included as an XML file.

Annex J (informative):  
MCData user profile configuration MO DDF

This DDF is the standardized minimal set. A vendor can define its own DDF for the complete device. This DDF can include more features than this minimal standardized version. The DDF is included as an XML file.

Annex K (informative):  
MCData service configuration MO DDF

This DDF is the standardized minimal set. A vendor can define its own DDF for the complete device. This DDF can include more features than this minimal standardized version. The DDF is included as an XML file.

Annex L (informative):  
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **TSG #** | **TSG Doc.** | **CR** | **Rev** | **Subject/Comment** | **Old** | **New** |
| 2015-07 |  |  |  |  | Initial proposal to CT1 | - | 0.0.0 |
| 2015-08 |  |  |  |  | Included skeleton from C1ah-150016 and scope from C1ah-150038 agreed at CT1#92bis | 0.0.0 | 0.10 |
| 2015-08 |  |  |  |  | Included CRs C1-152964 and C1-152965 agreed at CT1#93 | 0.1.0 | 0.2.0 |
| 2015-08 |  |  |  |  | Revision number changed due to cover sheet modifications | 0.2.0 | 0.2.1 |
| 2015-09 |  |  |  |  | Modifying the cover sheet to add the TS number. Changes by the rapporteur. | 0.2.1 | 0.2.2 |
| 2015-10 |  |  |  |  | Included CRs C1-153754,and C1-153755 agreed at CT1#94 | 0.2.2 | 0.3.0 |
| 2016-01 |  |  |  |  | Included CRs C1-160352, C1-160474, C1-160475, C1-160476, C1-160477 and C1-160478 agreed at CT1#95bis | 0.3.0 | 0.4.0 |
| 2016-01 |  |  |  |  | Editorial and formatting fixes | 0.4.0 | 0.4.1 |
| 2016-02 |  |  |  |  | Included CRs C1-161077, C1-161078, C1-161231, C1-161324, C1-161326, C1-161327, C1-161509 and C1-161510 agreed at CT1#96  Editorial and formatting fixes by the rapporteur. | 0.4.1 | 0.5.0 |
| 2016-03 | CT-71 | CP-160056 |  |  | Version 1.0.0 created for presentation for information and approval | 0.5.0 | 1.0.0 |
| 2016-03 | CT-71 |  |  |  | Version 13.0.0 created after approval | 1.0.0 | 13.0.0 |
| 2016-03 |  |  |  |  | An editorial change from TS rapporteur | 13.0.0 | 13.0.1 |
| 2016-06 | CT-72 | CP-160322 | 0002 | 1 | Corrections to the scope of MCPTT Management Object (MO) | 13.0.1 | 13.1.0 |
| 2016-06 | CT-72 | CP-160322 | 0003 | 3 | Correction for MCPTT UE configuration management object (MO) | 13.0.1 | 13.1.0 |
| 2016-06 | CT-72 | CP-160322 | 0004 | 3 | Correction for MCPTT user profile management object (MO) | 13.0.1 | 13.1.0 |
| 2016-06 | CT-72 | CP-160322 | 0005 | 2 | Correction for MCPTT group configuration management object (MO) | 13.0.1 | 13.1.0 |
| 2016-06 | CT-72 | CP-160322 | 0006 | 1 | Correction for MCPTT service configuration management object (MO) | 13.0.1 | 13.1.0 |
| 2016-06 | CT-72 | CP-160322 | 0007 | 3 | Correction for MCPTT UE initial configuration management object (MO) | 13.0.1 | 13.1.0 |
| 2016-06 | CT-72 | CP-160322 | 0011 |  | Correction for security configuration parameters in MCPTT management object (MO) | 13.0.1 | 13.1.0 |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2016-09 | CT#73 | CP-160565 | 0013 | 3 | F | Correction for configuration parameters in MCPTT user profile management object (MO) | 13.2.0 |
| 2016-09 | CT#73 | CP-160503 | 0014 | 1 | F | Correction for group related parameters in MCPTT UE initial configuration management object (MO) | 13.2.0 |
| 2016-09 | CT#73 | CP-160503 | 0015 | 1 | F | Correction for security material parameter in MCPTT group configuration management object (MO) | 13.2.0 |
| 2016-09 | CT#73 | CP-160503 | 0016 |  | F | Correction for "MCPTTGroupPriorityHierarchy" value in MCPTT UE configuration management object (MO) | 24.383 13.2.0 |
| 2016-12 | CT#74 |  |  |  |  | Change of spec number from 24.383 to 24.483 with wider scope and changed title | 24.483 13.2.1 |
| 2016-12 | CT#74 | CP-160733 | 0018 | 1 | F | Identity management endpoint UE initial configuration MO correction (24.383 CR) | 13.3.0 |
| 2016-12 | CT#74 | CP-160733 | 0019 | 1 | F | Correction for ProSe related configuration parameters (24.383 CR) | 13.3.0 |
| 2016-12 | CT#74 | CP-160733 | 0020 | 3 | F | Correction for MCPTT Private Call and Group Call in MCPTT user profile management (MO) (24.383 CR) | 13.3.0 |
| 2016-12 | CT#74 | CP-160733 | 0021 |  | F | Modify number of levels for priority hierarchy (24.383 CR) | 13.3.0 |
| 2016-12 | CT#74 | CP-160733 | 0022 | 1 | F | Identification of pre-selected MCPTT user profile in MCPTT user profile managed object. (24.383 CR) | 13.3.0 |
| 2016-12 | CT#74 | CP-160734 | 0023 | 2 | F | Off-network configuration parameter for queue (24.383 CR) | 13.3.0 |
| 2017-03 | CT#75 | CP-170117 | 0001 | 2 | F | Scope alignment with TS 24.483 title | 13.4.0 |
| 2017-03 | CT#75 | CP-170117 | 0004 |  | F | Corrections to upper limits | 13.4.0 |
| 2017-03 | CT#75 | CP-170127 | 0002 | 1 | F | Modifying references in TS 24.483 to cater for rel-14 Stage 2 and Stage 3 mission critical restructure | 14.0.0 |
| 2017-03 | CT#75 | CP-170127 | 0003 | 1 | F | Corrections and clean-up for 24.483 | 14.0.0 |
| 2017-03 | CT#75 | CP-170125 | 0005 | 1 | B | MCPTT user profile MO modifications in support of private call call-back | 14.0.0 |
| 2017-06 | CT#76 | CP-171080 | 0006 |  | B | Updating general parts of TS 24.483 for MCData, MCVideo and the initial configuration MO | 14.1.0 |
| 2017-06 | CT#76 | CP-171080 | 0007 | 2 | B | Modifications to the Group Configuration MO for MCData and MCVideo | 14.1.0 |
| 2017-06 | CT#76 | CP-171081 | 0008 | 1 | B | MCVideo UE configuration MO | 14.1.0 |
| 2017-06 | CT#76 | CP-171081 | 0009 | 2 | B | MCVideo user profile configuration MO | 14.1.0 |
| 2017-06 | CT#76 | CP-171081 | 0010 |  | B | MCVideo service configuration MO | 14.1.0 |
| 2017-06 | CT#76 | CP-171080 | 0011 | 2 | B | MCData UE configuration MO | 14.1.0 |
| 2017-06 | CT#76 | CP-171080 | 0012 | 2 | B | MCData user profile configuration MO | 14.1.0 |
| 2017-06 | CT#76 | CP-171080 | 0013 | 1 | B | MCData service configuration MO | 14.1.0 |
| 2017-06 | CT#76 | CP-171114 | 0014 | 1 | B | eMCPTT user profile MO updates | 14.1.0 |
| 2017-06 | CT#76 | CP-171113 | 0016 | 1 | A | AllowedFloorControlProtection configuration parameter | 14.1.0 |
| 2017-06 | CT#76 | CP-171113 | 0018 |  | A | QueueUsage configuration parameter | 14.1.0 |
| 2017-06 | CT#76 | CP-171082 | 0019 | 1 | F | Correction of User Aliases configuration parameter in the MCPTT user profile MO | 14.1.0 |
| 2017-09 | CT#77 | CP-172101 | 0020 | 1 | B | User profile MO additions for eMCPTT | 14.2.0 |
| 2017-09 | CT#77 | CP-172096 | 0022 | 1 | A | Clause 4 - Correction of occurrences of parameters | 14.2.0 |
| 2017-09 | CT#77 | CP-172104 | 0025 |  | F | Clause 6 - Correction of occurrences of parameters | 14.2.0 |
| 2017-09 | CT#77 | CP-172102 | 0026 | 1 | F | Clause 9 - Correction of occurrences of parameters | 14.2.0 |
| 2017-09 | CT#77 | CP-172143 | 0028 | 2 | F | Specify KMS-URI configuration for MCDATA in the MCData User Profile Management Object. | 14.2.0 |
| 2017-09 | CT#77 | CP-172144 | 0029 | 2 | F | Clause 10 - Correction of names and formats of some parameters | 14.2.0 |
| 2017-09 | CT#77 | CP-172104 | 0030 |  | F | Clause 12 - Correction of occurrences of parameters | 14.2.0 |
| 2017-09 | CT#77 | CP-172104 | 0031 |  | F | Clause 13 - Correction of occurrences of parameters and their graphical representation | 14.2.0 |
| 2017-09 | CT#77 | CP-172096 | 0032 | 2 | A | Clause 8 – Inclusion of missing timer TFG14 | 14.2.0 |
| 2017-09 | CT#77 | CP-172096 | 0034 | 1 | A | Include missing elements in MCPTT UE initial configuration MO | 14.2.0 |
| 2017-09 | CT#77 | CP-172134 | 0037 |  | F | DDF files for TS 24.483 | 14.2.0 |
| 2017-12 | CT#78 | CP-173066 | 0039 | 1 | F | Off-network MCVideo configurations | 14.3.0 |
| 2017-12 | CT#78 | CP-173073 | 0038 | 1 | B | Authorisation parameters for remotely initiated calls - user profile MO | 15.0.0 |
| 2018-03 | CT#79 | CP-180087 | 0040 | 1 | B | User profile MO updates for functional alias | 15.1.0 |
| 2018-03 | CT#79 | CP-180072 | 0042 | 1 | A | User profile presentation priority | 15.1.0 |
| 2018-06 | CT#80 | CP-181064 | 0043 |  | F | Unique ID leaf node for enhanced status operational value | 15.2.0 |
| 2018-09 | CT#81 | CP-182149 | 0045 | 2 | B | Location of Talker | 15.3.0 |
| 2018-09 | CT#81 | CP-182148 | 0046 |  | B | Reception Priority | 15.3.0 |
| 2019-03 | CT#83 | CP-190078 | 0051 | 1 | A | Correction of MO counter names CFx11 and CFx12 | 15.4.0 |
| 2019-03 | CT#83 | CP-190078 | 0055 | 1 | A | Remove T230 from TS 24.483 | 15.4.0 |
| 2019-03 | CT#83 | CP-190103 | 0048 | 2 | F | 24.483 Server URI and IP version additions | 16.0.0 |
| 2019-03 | CT#83 | CP-190103 | 0052 | 1 | F | Correction of Annex C and Annex E | 16.0.0 |
| 2019-09 | CT#85 | CP-192066 | 0057 | 1 | B | Restricting incoming private communications MO | 16.1.0 |
| 2019-12 | CT#86 | CP-193110 | 0058 | 1 | B | MO for limiting the number of emergency group calls for a specific functional alias | 16.2.0 |
| 2019-12 | CT#86 | CP-193110 | 0059 | 1 | B | Automatic activation and deactivation of functional aliases based on location | 16.2.0 |
| 2019-12 | CT#86 | CP-193082 | 0063 |  | A | Correction of single timer TFP2 mistakenly use for two different purposes | 16.2.0 |
| 2019-12 | CT#86 | CP-193110 | 0065 |  | B | List of MCPTT group members who did not acknowledge the group call request | 16.2.0 |
| 2020-03 | CT#87e | CP-200122 | 0064 | 3 | B | Automatic group affiliation and deaffiliation based on location or functional alias | 16.3.0 |
| 2020-03 | CT#87e | CP-200115 | 0066 | 1 | C | Included absolute URI associated with the media storage function of MCData content server | 16.3.0 |
| 2020-06 | CT#88e | CP-201124 | 0067 | 1 | B | IPConnectivity extension to include IP Information | 16.4.0 |
| 2020-06 | CT#88e | CP-201086 | 0071 | 1 | A | Correction of unit values for T204 and T205 | 16.4.0 |
| 2020-06 | CT#88e | CP-201124 | 0072 | 1 | B | Add PointCoordinate, Speed, Heading nodes in 5.2.48W | 16.4.0 |
| 2020-06 | CT#88e | CP-201124 | 0073 | 1 | D | Correct capitalisation in ListOfFunctionalaliases | 16.4.0 |
| 2020-06 | CT#88e | CP-201124 | 0074 | 1 | B | MCData FA (de)affiiation by location criteria MOs | 16.4.0 |
| 2020-06 | CT#88e | CP-201124 | 0075 | 1 | B | MCData Functional Alias by location criteria | 16.4.0 |
| 2020-06 | CT#88e | CP-201121 | 0076 |  | F | Correction of node formats | 16.4.0 |
| 2020-06 | CT#88e | CP-201112 | 0077 | 1 | B | Included the MessageStoreHostname element | 16.4.0 |
| 2020-06 | CT#88e | CP-201124 | 0078 | 1 | F | Restricting incoming MCData communications MO | 16.4.0 |
| 2020-09 | CT#89e | CP-202165 | 0081 |  | F | MOs Corrections related to MONASTERY2 CRs implementation | 16.5.0 |
| 2021-06 | CT#92e | CP-211125 | 0102 | 2 | A | Correct MCVideo MOs R16 | 16.6.0 |
| 2021-06 | CT#92e | CP-211125 | 0107 |  | A | Clause 12: name of node indicating the maximum number of private calls | 16.6.0 |
| 2021-06 | CT#92e | CP-211126 | 0110 |  | A | Invalid MCPTT user profile MO DDF | 16.6.0 |
| 2021-06 | CT#92e | CP-211132 | 0112 | 1 | F | Occurrence "ThreeToFifteen" in MCPTT user profile MO | 16.6.0 |
| 2021-06 | CT#92e | CP-211132 | 0114 | 1 | F | Occurrence "ThreeToFifteen" in MCData user profile MO | 16.6.0 |
| 2021-09 | CT#93e | CP-212113 | 0122 |  | A | MCPTT user profile MO: occurrence of the node "Common" | 16.7.0 |
| 2021-09 | CT#93e | CP-212115 | 0126 |  | A | MCData user profile MO: occurrence of the node "Common" | 16.7.0 |
| 2021-09 | CT#93e | CP-212115 | 0130 |  | A | MCVideo user profile MO: occurrence of the node "Common" | 16.7.0 |
| 2021-09 | CT#93e | CP-212123 | 0132 |  | F | Ocurrence of the ManualDeactivationNotAllowedIfLocationCriteriaMet | 16.7.0 |
| 2022-06 | CT#96 | CP-221193 | 0152 | 1 | A | Group info and presentation priorities, MO | 16.8.0 |