|  |  |
| --- | --- |
| 3GPP TS 24.571 V16.3.0 (2021-12) | |
| Technical Specification | |
| 3rd Generation Partnership Project;  Technical Specification Group Core Network and Terminals;  5G System (5GS);  Control plane Location Services (LCS) procedures;  Stage 3;  (Release 16) | |
|  | |
| *5G-logo_175px* | 3GPP-logo_web |
|  |
|  |
|  |
|  |
|  |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  http://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2021, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 5

1 Scope 7

2 References 7

3 Definitions of terms, symbols and abbreviations 7

3.1 Terms 7

3.2 Symbols 7

3.3 Abbreviations 7

4 General 8

4.1 Overview 8

4.1.1 NAS aspect 8

4.1.2 LCS aspect 8

4.2 LCS Support capabilities 8

4.2.1 UE support of LCS 8

4.2.2 Network support of LCS 9

5 Support of LCS signalling 9

5.1 General 9

5.2 LCS operations 9

5.2.1 Network initiated location services operations 9

5.2.1.1 Supplementary Services Location Notification 9

5.2.1.1.1 General 9

5.2.1.1.2 Normal operation 10

5.2.1.2 Positioning Information Transport 11

5.2.1.3 Supplementary Services Periodic or Triggered Location 12

5.2.1.3.1 General 12

5.2.1.3.2 Normal operation 13

5.2.1.4 Supplementary Services Cancel Deferred Location 15

5.2.1.4.1 General 15

5.2.1.4.2 Normal operation 16

5.2.2 Mobile initiated location services operations 17

5.2.2.1 Mobile Originiated Location Request(MO-LR) 17

5.2.2.1.1 General 17

5.2.2.1.2 Normal operation 18

5.2.2.2 UE initiated Cancel Deferred Location 22

5.2.2.2.1 General 22

5.2.2.2.2 Normal operation 23

5.2.2.3 UE initiated Positioning Information Transport 24

5.2.2.4 UE initiated Event Reporting Procedure 25

5.2.2.4.1 General 25

5.2.2.4.2 Normal operation 26

5.2.2.5 UE Location Privacy Setting Procedure 27

5.2.2.5.1 General 27

5.2.2.5.2 Normal operation 28

5.2.2.6 UE initiated Event Reporting Procedure for Low Power Event Reporting and Triggered 5GC-MT-LR 29

5.2.2.6.1 General 29

5.2.2.6.2 Normal operation 30

5.3 LCS message and coding 30

5.3.1 Messages for Location services operations 30

5.3.2 Messages for LTE Positioning Protocol (LPP) 31

5.3.2.1 Downlink Positioning Information Transport using LPP messages 31

5.3.2.2 Uplink Positioning Information Transport using LPP messages 31

Annex A (informative): Change history 32

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

In the present document, certain modal verbs have the following meanings:

**shall** indicates a mandatory requirement to do something

**shall not** indicates an interdiction (prohibition) to do something

NOTE 1: The constructions "shall" and "shall not" are confined to the context of normative provisions, and do not appear in Technical Reports.

NOTE 2: The constructions "must" and "must not" are not used as substitutes for "shall" and "shall not". Their use is avoided insofar as possible, and they are not used in a normative context except in a direct citation from an external, referenced, non-3GPP document, or so as to maintain continuity of style when extending or modifying the provisions of such a referenced document.

**should** indicates a recommendation to do something

**should not** indicates a recommendation not to do something

**may** indicates permission to do something

**need not** indicates permission not to do something

NOTE 3: The construction "may not" is ambiguous and is not used in normative elements. The unambiguous constructions "might not" or "shall not" are used instead, depending upon the meaning intended.

**can** indicates that something is possible

**cannot** indicates that something is impossible

NOTE 4: The constructions "can" and "cannot" shall not to be used as substitutes for "may" and "need not".

**will** indicates that something is certain or expected to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**will not** indicates that something is certain or expected not to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**might** indicates a likelihood that something will happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

**might not** indicates a likelihood that something will not happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

In addition:

**is** (or any other verb in the indicative mood) indicates a statement of fact

**is not** (or any other negative verb in the indicative mood) indicates a statement of fact

NOTE 5: The constructions "is" and "is not" do not indicate requirements.

# 1 Scope

The present document specifies the operations and information coding for the Non-Access Stratum (NAS) layer protocol for supporting the Location Services (LCS) in the NG-RAN.

The present document is applicable to the User Equipment (UE) and to the Access and Mobility Management Function (AMF) or Location Management Function (LMF) in the 5G System (5GS).

The present document is developed in accordance to the general principles stated in 3GPP TS 23.273 [2].

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 23.273: "5G System (5GS) Location Services (LCS); Stage 2".

[3] 3GPP TS 24.501: "Non-Access-Stratum (NAS) protocol for 5G System (5GS); Stage 3".

[4] 3GPP TS 36.355: "Evolved Universal Terrestrial Radio Access (E-UTRA); LTE Positioning Protocol (LPP)".

[5] 3GPP TS 24.080: "Mobile radio interface layer 3 supplementary services specification; Formats and coding".

[6] 3GPP TS 29.572: "5G System; Location Management Services; Stage 3".

# 3 Definitions of terms, symbols and abbreviations

## 3.1 Terms

For the purposes of the present document, the terms given in 3GPP TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in 3GPP TR 21.905 [1].

## 3.2 Symbols

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

5GCN 5G Core Network

5GS 5G System

AMF Access and Mobility Management Function

DL Downlink

IE Information Element

GMLC Gateway Mobile Location Centre

LCS Location Services

LDR Location Deferred Request

LMF Location Management Function

LPP LTE Positioning Protocol

MO-LR Mobile Originated Location Request

MT-LR Mobile Terminated Location Request

NAS Non-access Stratum

UE User Equipment

UL Uplink

# 4 General

## 4.1 Overview

### 4.1.1 NAS aspect

To enable transfer of Location Services (LCS) signaling messages between the 5G core network (5GCN) and the UE, two Payload container types are defined in the downlink (DL NAS TRANSPORT message) and the uplink (UL NAS TRANSPORT message). The message protocol and procedures are described in 3GPP TS 24.501 [3].

### 4.1.2 LCS aspect

LCS uses the defined payload container to transfer LCS signalling messages between the UE and the network.

The corresponding LCS signaling messages include:

a) LTE Positioning Protocol (LPP) messages (see 3GPP TS 36.355 [4])

- Both downlink and uplink LPP messages are supported

- Routing information is transported as the Additional information IE in UL/DL NAS TRANSPORT message for LPP messages (see 3GPP TS 24.501 [3])

b) Location services messages

- Messages for MO-LR operations (see 3GPP TS 24.080 [5])

- Messages for LocationNotification operations (see 3GPP TS 24.080 [5])

- Messages for EventReport operations (see 3GPP TS 24.080 [5])

- Messages for PeriodicTriggeredInvoke operations (see 3GPP TS 24.080 [5])

- Messages for CancelDeferredLocation operations (see 3GPP TS 24.080 [5])

- Messages for MSCancelDeferredLocation operations (see 3GPP TS 24.080 [5])

- Messages for LocationPrivacySetting operations (see 3GPP TS 24.080 [5])

Routing information associated with the LMF is transported as the Additional information IE in UL/DL NAS TRANSPORT message for Location services messages that are transported from/to the LMF (see 3GPP TS 24.501 [3])

## 4.2 LCS Support capabilities

### 4.2.1 UE support of LCS

The UE announces to the network its ability to support LCS notification mechanism or LPP messages or both, using the 5GMM capability IE defined in 3GPP TS 24.501 [3].

### 4.2.2 Network support of LCS

The network announces to the UE its ability to support LCS in 5GC using the 5GS network feature support IE defined in 3GPP TS 24.501 [3]. The information is taken into account by the UE, in addition to UE's LCS capabilities, for the UE to determine whether to initiate MO-LR procedure in NG-RAN as specified in 3GPP TS 23.273 [3], subclause 6.2.

# 5 Support of LCS signalling

## 5.1 General

This clause defines the NG-RAN LCS operations (subclause 5.2) and the format and coding of the messages (subclause 5.3).

The messages defined in this subclause can be transported in the UL/DL NAS Transport message defined in 3GPP TS 24.501 [3].

## 5.2 LCS operations

### 5.2.1 Network initiated location services operations

#### 5.2.1.1 Supplementary Services Location Notification

##### 5.2.1.1.1 General

The supplementary services Location Notification operation enables the AMF to trigger the end-user notification verification process on the UE using NAS signalling. The supplementary services messages are transported using the DL NAS Transport message and the UL NAS Transport message defined in 3GPP TS 24.501 [3]. UE Location Privacy Indication information may be included in Location Notification Return Result to indicate whether subsequent LCS requests will be allowed or disallowed by the UE. Figure 5.2.1.1.1.1 illustrates an example of the NAS signalling transport applicable to a 5GC-MT-LR procedure for immediate or deferred location.



Figure 5.2.1.1.1.1: NAS signalling transport for Supplementary Services Location Notification

NOTE: The optional Additional Information IE of the DL/UL NAS Transport message is not used when the LCS Location Notification signalling is transported in the Payload container.

##### 5.2.1.1.2 Normal operation

The network invokes a location notification procedure by sending a REGISTER message containing an LCS-LocationNotification invoke component to the UE as defined in 3GPP TS 24.080 [5]. This may be sent either to request verification for a 5GC-MT-LR or to notify the UE about an already authorized 5GC-MT-LR.

In case of privacy verification, the UE shall respond to the request by sending a RELEASE COMPLETE message containing the user's response and optionally UE Location Privacy Indication information in a return result component (see figure 5.2.1.1.2.1).

If the timer T(LCSN) defined in 3GPP TS 24.080 [5] expires in the network before any response from the UE (e.g. due to no response from the user), the network shall interpret this by applying the default treatment defined in 3GPP TS 23.273 [2] (i.e. disallow location if barred by subscription or allow location if allowed by subscription).

In the case of location notification, the UE shall terminate the dialogue immediately by sending a RELEASE COMPLETE message containing a LocationNotification return result.

If the UE is unable to process the request received from the network, it shall return an error indication by sending a RELEASE COMPLETE message containing a return error component. Error values are specified in 3GPP TS 24.080 [5].

**UE Network**

REGISTER

<------------------------------------------------------------------------------------------------------------------------

Facility (Invoke = LCS-LocationNotification (notificationType, locationType, lcsClientExternalID, lcsClientName, lcsCodeword, lcsServiceTypeId, deferredLocationExt))

RELEASE COMPLETE

------------------------------------------------------------------------------------------------------------------------>

Facility (Return result = LCS-LocationNotification (verificationResponse, locationPrivacyIndication, validTimePeriod))

RELEASE COMPLETE

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - ->

Facility (Return error (Error))

RELEASE COMPLETE

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - ->

Facility (Reject (Invoke\_problem))

RELEASE COMPLETE

<- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

Figure 5.2.1.1.2.1: Location Notification

#### 5.2.1.2 Positioning Information Transport

The AMF sends an LPP message and an associated Correlation Identifier in the DL NAS Transport message (refer to 3GPP TS 24.501 [3] and 3GPP TS 23.273 [2] clause 6.11.1). Figure 5.2.1.2.1 illustrates an example of the NAS signalling transport for downlink LPP messages.



Figure 5.2.1.2.1: NAS signalling transport for downlink LPP messages

#### 5.2.1.3 Supplementary Services Periodic or Triggered Location

##### 5.2.1.3.1 General

The supplementary services LCS PeriodicTriggered Invoke operation enables the LMF to initiate periodic or triggered location event reporting by a target UE as described in clause 6.3.1 of 3GPP TS 23.272 [2]. The supplementary services LCS PeriodicTriggered Invoke message is transferred to the target UE via the serving AMF in a DL NAS Transport message. A response from the target UE is similarly returned to the LMF via the serving AMF and is transferred to the AMF in an UL NAS Transport message.

Figure 5.2.1.3.1.1 illustrates an example of the NAS signalling transport for initiation of periodic or triggered location,



Figure 5.2.1.3.1.1: NAS signalling transport for LCS PeriodicTriggered messages

##### 5.2.1.3.2 Normal operation

The LMF sends a REGISTER message to the UE containing the supplementary services LCS PeriodicTriggered Invoke component as defined in 3GPP TS 24.080 [5]. The REGISTER message is transported to the UE via the serving AMF as described in figure 5.2.1.3.1.1.

If the UE can support the periodic or triggered location, the UE returns a RELEASE COMPLETE message to the LMF containing an LCS PeriodicTriggered return result. The RELEASE COMPLETE message is transported to the LMF via the serving AMF as described in figure 5.2.1.3.1.1.

If the UE is unable to process or support the request received from the network, it shall return an error indication by sending a RELEASE COMPLETE message containing a return error component or reject component. Error values are specified in 3GPP TS 24.080 [5].

Figure 5.2.1.3.2.1 illustrates the signalling for normal operation between the UE and the network.

**UE Network**

REGISTER

<------------------------------------------------------------------------------------------------------------------------

Facility (Invoke = LCS-PeriodicTriggered (referenceNumber, qos, periodicLocation, areaEventReporting, motionEventReporting, referenceNumberExt, h-gmlc-callBackUri, supportedGADShapes, deferredRoutingIdentifier, reportingAccessTypes, multiplePositioningProtocolPDUs, controlPlane-CIoT-5GS-Optimisation))

RELEASE COMPLETE

------------------------------------------------------------------------------------------------------------------------>

Facility (Return result = LCS-PeriodicTriggered)

RELEASE COMPLETE

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - ->

Facility (Return error (Error))

RELEASE COMPLETE

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - ->

Facility (Reject (Invoke\_problem))

RELEASE COMPLETE

<- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

Figure 5.2.1.3.2.1: Periodic or Triggered Location Invocation

#### 5.2.1.4 Supplementary Services Cancel Deferred Location

##### 5.2.1.4.1 General

The supplementary services Cancel Deferred Location operation enables the AMF to cancel ongoing periodic or triggered location in a target UE using NAS signalling as described in 3GPP TS 23.273 [2] clause 6.3.3. The supplementary services Cancel Deferred Location messages are transported using the DL NAS Transport message and the UL NAS Transport message defined in 3GPP TS 24.501 [3]. Figure 5.2.1.4.1-1 illustrates an example of the NAS signalling transport.



Figure 5.2.1.4.1.1: NAS signalling transport for Cancel Deferred Location

NOTE: The optional Additional Information IE of the DL/UL NAS Transport message is not used when the LCS CancelDeferredLocation signalling is transported in the Payload container.

##### 5.2.1.4.2 Normal operation

The AMF invokes a cancel deferred location procedure by sending a REGISTER message containing an LCS-CancelDeferredLocation invoke component to the UE as defined in 3GPP TS 24.080 [5].

The UE shall terminate the ongoing periodic or triggered location if this can be identified from the information in the LCS-CancelDeferredLocation invoke component.

The UE shall then return a RELEASE COMPLETE message containing an LCS-CancelDeferredLocation return result component (see figure 5.2.1.4.2.1).

If the UE is unable to process the request received from the network or cannot identify the ongoing periodic or triggered location to be terminated, it shall return an error indication by sending a RELEASE COMPLETE message containing a return error component. Error values are specified in 3GPP TS 24.080 [5].

**UE Network**

REGISTER

<------------------------------------------------------------------------------------------------------------------------

Facility (Invoke = LCS-CancelDeferredLocation (referenceNumberExt, h-gmlc-callBackUri))

RELEASE COMPLETE

------------------------------------------------------------------------------------------------------------------------>

Facility (Return result = LCS-CancelDeferredLocation)

RELEASE COMPLETE

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - ->

Facility (Return error (Error))

RELEASE COMPLETE

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - ->

Facility (Reject (Invoke\_problem))

RELEASE COMPLETE

<- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

Figure 5.2.1.4.2.1: Cancel Deferred Location

### 5.2.2 Mobile initiated location services operations

#### 5.2.2.1 Mobile Originiated Location Request(MO-LR)

##### 5.2.2.1.1 General

The supplementary services MO-LR operation enables the UE to launch MO positioning session or request location assistance data using NAS signaling. The NAS signaling are transported using the DL NAS Transport message and the Uplink NAS Transport message defined in 3GPP TS 24.501 [3]. Figure 5.2.2.1.1-1 illustrates an example of the NAS signaling transport for an MO-LR session.



Figure 5.2.2.1.1-1: NAS signaling transport for MO-LR

NOTE: The optional Additional Information IE of the UL/DL NAS TRANSPORT message is not used when the MO-LR signaling is transported in the Payload container.

##### 5.2.2.1.2 Normal operation

The UE invokes a MO-LR by sending a REGISTER message to the network containing a LCS-MOLR invoke component. SS Version Indicator value 1 or above shall be used.

The receiving network entity shall initiate the handling of location request in the network. The network shall pass the result of the location procedure to the UE by sending a FACILITY message to the UE containing a LCS-MOLR return result component. When location estimate is kept in the network entity and this information satisfies the requested accuracy and the requested maximum age of location, then the network may reuse this information and the positioning measurement procedure may be skipped.

The network shall pass the result of the location procedure to the UE only if the location estimate is given in a format that the UE supports, as indicated by either the presence (and content) or the absence of the parameter supportedGADShapes, which may be sent by the UE in the LCS-MOLR operation.

The UE may terminate the dialogue by sending a RELEASE COMPLETE message in the case of single location request (see figure 5.2.2.1.1-1). The UE may also initiate another location request operation by sending a FACILITY message to the network containing a LCS-MOLR invoke component (see figure 5.2.2.1.1-2). After the last location request operation the UE shall terminate the dialogue by sending a RELEASE COMPLETE message.

If the network is unable to successfully fulfil the request received from the UE (e.g. to provide a location estimate or location assistance information), it shall clear the transaction by sending a RELEASE COMPLETE message containing a return error component. Error values are specified in 3GPP TS 24.080 [5]. If the network is unable to provide a location estimate due to lack of support in the UE for the type of shape of the location estimate, then it shall use the error Facility Not Supported.

If the network has returned a result to the UE in a FACILITY message but, after some PLMN administered time period has elapsed, has not received either a new location request operation in a FACILITY message or a RELEASE COMPLETE message from the UE, the network may clear the transaction by sending a RELEASE COMPLETE message.

During the MO-LR operation the UE shall run a timer T(LCSL). This timer is started when the operation is sent, and stopped when a response is received from the network. If this timer expires the UE shall assume that the operation has failed, and may terminate the dialogue by sending a RELEASE COMPLETE message, and shall inform the user of the failure.

**UE Network**

REGISTER

------------------------------------------------------------------------------------------------------------------------>

Facility (Invoke = LCS-MOLR (molr-Type, lcs-QoS, lcsClientExternalID, mlc-Number, supportedGADShapes, lcsServiceTypeID, ageOfLocationInfo, locationType, pseudonymIndicator, multiplePositioningProtocolPDUs))

FACILITY

<------------------------------------------------------------------------------------------------------------------------

Facility (Return result = LCS-MOLR (locationEstimate, velocityEstimate, add-LocationEstimate, decipheringKeys))

RELEASE COMPLETE

<- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

Facility (Return error (Error))

RELEASE COMPLETE

<- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

Facility (Reject (Invoke\_problem))

RELEASE COMPLETE

------------------------------------------------------------------------------------------------------------------------>

Figure 5.2.2.1.1-1: Single mobile originated location request

**UE Network**

REGISTER

------------------------------------------------------------------------------------------------------------------------>

Facility (Invoke = LCS-MOLR (molr-Type, lcs-QoS, lcsClientExternalID, mlc-Number, supportedGADShapes, lcsServiceTypeID, ageOfLocationInfo, locationType, pseudonymIndicator, multiplePositioningProtocolPDUs))

FACILITY

<------------------------------------------------------------------------------------------------------------------------

(Return result = LCS-MOLR (locationEstimate, velocityEstimate, add-LocationEstimate, decipheringKeys))

RELEASE COMPLETE

<- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

Facility (Return error (Error))

RELEASE COMPLETE

<- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

Facility (Reject (Invoke\_problem))

FACILITY

------------------------------------------------------------------------------------------------------------------------>

Facility (Invoke = LCS-MOLR (molr-Type, lcs-QoS, lcsClientExternalID, mlc-Number, supportedGADShapes, lcsServiceTypeID, ageOfLocationInfo, locationType, pseudonymIndicator, multiplePositioningProtocolPDUs))

FACILITY

<------------------------------------------------------------------------------------------------------------------------

(Return result = LCS-MOLR (locationEstimate, velocityEstimate, add-LocationEstimate, decipheringKeys))

RELEASE COMPLETE

<- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

Facility (Return error (Error))

RELEASE COMPLETE

<- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

Facility (Reject (Invoke\_problem))

RELEASE COMPLETE

------------------------------------------------------------------------------------------------------------------------>

Figure 5.2.2.1.1-2: Multiple mobile originated location requests

NOTE: Only the following IEs defined in MO-LR operations in 3GPP TS 24.080 [5] are used for NG-RAN LCS:

- molr-Type

- lcs-QoS

- lcsServiceTypeID

- ageOfLocationInformation

- locationType

- mlc-Number

- lcsClientExternalID

- pseudonymIndicator

- supportedGADShapes

- multiplePositioningProtocolPDUs

- locationEstimate

- decipheringKeys

NOTE: multiplePositioningProtocolPDUs IE is added to the MO-LR Request to allow for passing multiple UE positioning information LPP messages (e.g. UE location measurements or UE capabilities) to the LMF for NG-RAN LCS. Its ASN.1 description is given in 3GPP TS 24.080 [5].

#### 5.2.2.2 UE initiated Cancel Deferred Location

##### 5.2.2.2.1 General

The supplementary services MSCancelDeferredLocation operation enables the UE to cancel ongoing periodic or triggered location in a target LMF using NAS signalling as described in 3GPP TS 23.273  subclause 6.3.3 [2]. The supplementary services MCancelDeferredLocation messages are transported using the UL NAS TRANSPORT message and the DL NAS TRANSPORT message defined in 3GPP TS 24.501 [3]. Figure 5.2.2.2.1-1 illustrates an example of the NAS signalling transport.



Figure 5.2.2.2.1-1: NAS signaling transport for UE initiated Cancel Deferred Location

##### 5.2.2.2.2 Normal operation

The UE invokes a cancel deferred location procedure by sending a REGISTER message containing a LCS-MSCancelDeferredLocation invoke component to the LMF as defined in 3GPP TS 24.080 [5].

The LMF shall terminate the ongoing periodic or triggered location if this can be identified from the information in the LCS-MSCancelDeferredLocation invoke component.

The LMF shall then return a RELEASE COMPLETE message containing an LCS-MSCancelDeferredLocation return result component (see Figure 5.2.2.2.2-1).

If the LMF is unable to process the request received from the UE or can not identify the ongoing periodic or triggered location to be terminated, it shall return an error indication by sending a RELEASE COMPLETE message containing a return error component. Error values are specified in 3GPP TS 24.080 [5].

**UE Network**

REGISTER

------------------------------------------------------------------------------------------------------------------------>

Facility (Invoke = LCS-MSCancelDeferredLocation (referenceNumberExt, h-gmlc-callBackUri))

RELEASE COMPLETE

<------------------------------------------------------------------------------------------------------------------------

Facility (Return result = LCS-MSCancelDeferredLocation)

RELEASE COMPLETE

<- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

Facility (Return error (Error))

RELEASE COMPLETE

<- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

Facility (Reject (Invoke\_problem))

RELEASE COMPLETE

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - ->

Figure 5.2.2.2.2-1: Cancel Deferred Location

NOTE: Only the following IEs defined in MSCancelDeferredLocation operations in 3GPP TS 24.080 [5] are used for NG-RAN LCS:

- referenceNumberExt

- h-gmlc-callBackUri

#### 5.2.2.3 UE initiated Positioning Information Transport

The UE sends LPP message and the associated Routing Identifier in the UL NAS Transport message (refer to 3GPP TS 24.501 [3] and 3GPP TS 23.273 [2] clause 6.11.1). Figure 5.2.2.3-1 illustrates an example of the NAS signalling transport for uplink LPP messages.



Figure 5.2.2.3-1: NAS signalling transport for uplink LPP messages

#### 5.2.2.4 UE initiated Event Reporting Procedure

##### 5.2.2.4.1 General

The supplmentary services EventReport operation enables the UE to report the periodic or triggered location event invoked by the LMF via LCS PeriodicTriggered Invoke operation as described in clause 6.3.1 of 3GPP TS 23.273 [2] when some certain events are detected in the UE. The supplmentary services EventReport message is transferred to the LMF via the serving AMF in a UL NAS TRANSPORT message defined in 3GPP TS 24.501 [3]. A response from the LMF may be returned to the UE via the serving AMF and be transferred to the UE in a DL NAS TRANSPORT message.

Figure 5.2.2.4.1-1 illustrates an example of the NAS signalling transport for EventReport messages,



Figure 5.2.2.4.1-1: NAS signalling transport for EventReport messages

##### 5.2.2.4.2 Normal operation

The UE invokes an EventReport procedure by sending a REGISTER message containing an EventReport component to the LMF as defined in 3GPP TS 24.080 [5].

The LMF shall return a supplementary services acknowledgement of event report if it can handle this event report.

The LMF shall then return a RELEASE COMPLETE message containing an EventReport Acknowledge component (see Figure 5.2.2.4.2-1).

If the LMF is unable to process the request received from the UE or can not identify the ongoing periodic or triggered location to be terminated, it shall return an error indication by sending a RELEASE COMPLETE message containing a return error component. Error values are specified in 3GPP TS 24.080 [5].

**UE Network**

REGISTER

------------------------------------------------------------------------------------------------------------------------>

Facility (Invoke = LCS-EventReport (eventType, referenceNumberExt, h-gmlc-callBackUri, lcs-QoS, locationInfo, supportedGADShapes, multiplePositioningProtocolPDUs, terminationCause))

RELEASE COMPLETE

<------------------------------------------------------------------------------------------------------------------------

Facility (Return result = LCS-EventReport Acknowledgement)

RELEASE COMPLETE

<- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

Facility (Return error (Error))

RELEASE COMPLETE

<- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

Facility (Reject (Invoke\_problem))

RELEASE COMPLETE

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - ->

Figure 5.2.2.4.2-1: EventReport

NOTE: Only the following IEs defined in EventReport operations in 3GPP TS 24.080 [5] are used for NG-RAN LCS:

- eventType

- referenceNumberExt

- h-gmlc-callBackUri

- lcs-QoS

- locationInfo

- supportedGADShapes

- multiplePositioningProtocolPDUs

- terminationCause

#### 5.2.2.5 UE Location Privacy Setting Procedure

##### 5.2.2.5.1 General

The supplmentary services LocationPrivacySetting operation enables the UE to update the UE Location Privacy Indication information via UE Location Privacy Setting procedure as described in clause 6.12.1 of 3GPP TS 23.273 [2] when the UE has generated or updated the UE Location Privacy Indication. The supplementary services LocationPrivacySetting message is transferred to the serving AMF in a UL NAS TRANSPORT message and an acknowledgement from the serving AMF may be returned to the UE in DL NAS TRANSPORT message defined in 3GPP TS 24.501 [3].

Figure 5.2.2.5.1-1 illustrates an example of the NAS signalling transport for UE Location Privacy Setting procedure,



Figure 5.2.2.5.1-1: NAS signalling transport for LocationPrivacySetting messages

##### 5.2.2.5.2 Normal operation

The UE invokes a Location Privacy Setting procedure by sending a REGISTER message containing an LocationPrivacySetting message as defined in 3GPP TS 24.080 [5]. UE's Location Privacy Indication information is included in LocationPrivacySetting message.

The AMF shall transfers the UE Location Privacy Indication information in LocationPrivacySetting message to UDM and response a supplementary services acknowledgement of LocationPrivacyIndication message

The AMF shall then return a RELEASE COMPLETE message containing a LocationPrivacySetting Acknowledgement component (see figure 5.2.2.5.2-1) if it can handle this LocationPrivacySetting message correctly.

If the AMF is unable to process the request received from the UE or can not identify that provisioning the parameters of UE Location Privacy Setting information to UDM is executed successfully, it shall return an error indication by sending a RELEASE COMPLETE message containing a return error component. Error values are specified in 3GPP TS 24.080 [5].

**UE Network**

REGISTER

------------------------------------------------------------------------------------------------------------------------>

Facility (Invoke = LCS-LocationPrivacySetting (locationPrivacyIndication, validTimePeriod)

RELEASE COMPLETE

<------------------------------------------------------------------------------------------------------------------------

Facility (Return result = LCS-LocationPrivacySetting Acknowledgement)

RELEASE COMPLETE

<- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

Facility (Return error (Error))

RELEASE COMPLETE

<- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

Facility (Reject (Invoke\_problem))

RELEASE COMPLETE

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - ->

Figure 5.2.2.5.2-1: LocationPrivacySetting

NOTE: Only the following IEs defined in LocationPrivacySetting operations in 3GPP TS 24.080 [5] are used for NG-RAN LCS:

- locationPrivacyIndication

- validTimePeriod

#### 5.2.2.6 UE initiated Event Reporting Procedure for Low Power Event Reporting and Triggered 5GC-MT-LR

##### 5.2.2.6.1 General

The supplementary services EventReport operation enables the UE to report the periodic or triggered location event invoked by the LMF via LCS PeriodicTriggered Invoke operation as described in clause 6.7.1 of 3GPP TS 23.273 [2] when certain events are detected in the UE and when the UE supports and the LMF allows the use of Control Plane CIoT 5GS Optimisation. The supplementary services EventReport message is transferred to the LMF via the serving AMF in a CONTROL PLANE SERVICE REQUEST message defined in 3GPP TS 24.501 [3]. A response from the LMF may be returned to the UE via the serving AMF and be transferred to the UE in a DL NAS TRANSPORT message defined in 3GPP TS 24.501 [3].

Figure 5.2.2.x.1-1 illustrates an example of the NAS signalling transport for EventReport messages,



Figure 5.2.2.6.1-1: NAS signalling transport for EventReport messages using Low Power Event Reporting and Triggered 5GC-MT-LR

##### 5.2.2.6.2 Normal operation

Normal operation is as described for the UE initiated Event Reporting Procedure in clause 5.2.2.4.2.

## 5.3 LCS message and coding

### 5.3.1 Messages for Location services operations

The LCS message format and information elements coding for the MO-LR, LocationNotification, EventReport, PeriodicTriggeredInvoke, CancelDeferredLocation and LocationPrivacySetting operations (subclause 5.2) are defined in 3GPP TS 24.080 [5] for the following messages:

- Register message

- Facility message

- Release Complete message

### 5.3.2 Messages for LTE Positioning Protocol (LPP)

#### 5.3.2.1 Downlink Positioning Information Transport using LPP messages

The AMF shall set the Payload container type to "LPP message container" in the DL NAS TRANSPORT message.

The AMF includes a Routing Identifier in the Additional information IE of the DL NAS TRANSPORT message which identifies the LMF and the positioning session between the AMF and LMF when a positioning session is being used.

The Routing identifier is the Correlation ID, which is defined in 3GPP TS 29.572 [6], so that the AMF can map the Routing identifier to the LMF and the Correlation identifier when the AMF receives a UL NAS TRANSPORT message including the responding LPP message.

#### 5.3.2.2 Uplink Positioning Information Transport using LPP messages

The UE shall set the Payload container type to "LPP message container" in the UL NAS TRANSPORT message.

The UE includes a Routing Identifier received in the Additional Information IE of the DL NAS TRANSPORT message in the Additional Information IE of the UL NAS TRANSPORT message. This association of the Routing Identifier is provided at the LPP level: the UL NAS TRANSPORT message carries an LPP message that is a response to or instigated by the LPP message in the DL NAS TRANSPORT message. The Routing identifier is the Correlation ID, which is defined in 3GPP TS 29.572 [6], so that the AMF can map the Routing identifier to the Correlation identifier when the AMF receives the UL NAS TRANSPORT message.

Annex A (informative):  
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2019-08 | CT1#119 |  |  |  |  | Draft skeleton provided by the rapporteur | 0.0.0 |
| 2019-10 | CT1#120 |  |  |  |  | Includes the following contribution agreed by CT1 at CT1#120:C1-196563 | 0.1.0 |
| 2019-11 | CT1#121 |  |  |  |  | Includes the following contributions agreed by CT1 at CT1#121:C1-198290, C1-198720 | 0.2.0 |
| 2019-12 | CT#86 | CP-193155 |  |  |  | Presentation for information to TSG CT | 1.0.0 |
| 2020-03 | CT#87e | CP-200287 |  |  |  | Implementation of pCRs CP-200102 and 103 approved by TSG CT. Presentation for approval to TSG CT. | 2.0.0 |
| 2020-03 | CT#87e |  |  |  |  | Version 16.0.0 created after approval | 16.0.0 |
| 2020-03 | CT#87e |  |  |  |  | Editorial corrections | 16.0.1 |
| 2020-06 | CT#88e | CP-201098 | 0001 |  | B | Adding Location Privacy Setting operation | 16.1.0 |
| 2020-09 | CT#89e | CP-202148 | 0002 | 3 | B | UE initiated Event Reporting Procedure for Low Power Event Reporting | 16.2.0 |
| 2020-09 | CT#89e | CP-202148 | 0003 |  | F | Additional function of MO-LR procedure | 16.2.0 |
| 2021-12 | CT#84e | CP-213042 | 0005 | - | F | Removal of h-gmlc-address | 16.3.0 |