3GPP TS 25.106 V16.0.0 (2020-06)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Radio Access Network;

UTRA repeater radio transmission and reception

(Release 16)



The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP..  
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.  
This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword [5](#__RefHeading___Toc518916780)

1 Scope [6](#__RefHeading___Toc518916781)

2 References [6](#__RefHeading___Toc518916782)

3 Definitions, symbols and abbreviations [6](#__RefHeading___Toc518916783)

3.1 Definitions [6](#__RefHeading___Toc518916784)

3.2 Symbols [7](#__RefHeading___Toc518916785)

3.3 Abbreviations [7](#__RefHeading___Toc518916786)

4 General [7](#__RefHeading___Toc518916787)

4.1 Relationship between Minimum Requirements and Test Requirements [7](#__RefHeading___Toc518916788)

4.2 Regional requirements [8](#__RefHeading___Toc518916789)

5 Frequency bands and channel arrangement [9](#__RefHeading___Toc518916790)

5.1 Frequency bands [9](#__RefHeading___Toc518916791)

5.2 TX - RX frequency separation [9](#__RefHeading___Toc518916792)

5.3 Channel arrangement [10](#__RefHeading___Toc518916793)

5.3.1 Channel spacing [10](#__RefHeading___Toc518916794)

5.3.2 Channel raster [10](#__RefHeading___Toc518916795)

5.3.3 Channel number [10](#__RefHeading___Toc518916796)

6 Output power [12](#__RefHeading___Toc518916797)

6.1 Maximum output power [13](#__RefHeading___Toc518916798)

6.1.1 Minimum Requirements [13](#__RefHeading___Toc518916799)

7 Frequency stability [13](#__RefHeading___Toc518916800)

7.1 Minimum requirement [13](#__RefHeading___Toc518916801)

8 Out of band gain [13](#__RefHeading___Toc518916802)

8.1 Minimum requirement [13](#__RefHeading___Toc518916803)

9 Unwanted emission [14](#__RefHeading___Toc518916804)

9.1 Out of band emission [14](#__RefHeading___Toc518916805)

9.1.1 Void [14](#__RefHeading___Toc518916806)

9.1.2 Operating band unwanted emissions [14](#__RefHeading___Toc518916807)

9.1.3. Protection of the BS receiver in the operating band [19](#__RefHeading___Toc518916808)

9.1.3.1 Minimum Requirement [19](#__RefHeading___Toc518916809)

9.1.4 Co-existence with services in adjacent frequency bands [19](#__RefHeading___Toc518916810)

9.1.4.1 Minimum requirement [19](#__RefHeading___Toc518916811)

9.2 Spurious emissions [19](#__RefHeading___Toc518916812)

9.2.1 General Requirements [20](#__RefHeading___Toc518916813)

9.2.1.1 Minimum Requirement (Category A) [20](#__RefHeading___Toc518916814)

9.2.1.2 Minimum Requirement (Category B) [20](#__RefHeading___Toc518916815)

9.2.2 Void [21](#__RefHeading___Toc518916816)

9.2.3 Co-existence with other systems in the same geographical area [21](#__RefHeading___Toc518916817)

9.2.3.1 Minimum Requirements [22](#__RefHeading___Toc518916818)

9.2.4 Co-existence with co-located and co-sited Base Stations [25](#__RefHeading___Toc518916819)

9.2.4.1 Minimum Requirements [26](#__RefHeading___Toc518916820)

9.2.5 Co-existence with PHS [28](#__RefHeading___Toc518916821)

9.2.5.1 Minimum Requirement [28](#__RefHeading___Toc518916822)

9.2.6 Co-existence with UTRA-TDD and/or E-UTRA TDD [29](#__RefHeading___Toc518916823)

9.2.6.1 Operation in the same geographic area [29](#__RefHeading___Toc518916824)

9.2.6.1.1 Minimum Requirement [29](#__RefHeading___Toc518916825)

9.2.6.2 Co-located Repeaters and UTRA-TDD and/or E-UTRA TDD base stations [31](#__RefHeading___Toc518916826)

9.2.6.2.1 Minimum Requirement [31](#__RefHeading___Toc518916827)

9.2.7 Void [33](#__RefHeading___Toc518916828)

9.2.8 Protection of public safety operations [33](#__RefHeading___Toc518916829)

9.2.8.1 Minimum Requirement [33](#__RefHeading___Toc518916830)

10 Modulation accuracy [33](#__RefHeading___Toc518916831)

10.1 Error Vector Magnitude [33](#__RefHeading___Toc518916832)

10.1.1 Minimum requirement [34](#__RefHeading___Toc518916833)

10.2 Peak code domain error [34](#__RefHeading___Toc518916834)

10.2.1 Minimum requirement [34](#__RefHeading___Toc518916835)

10.3 Relative Code Domain Error (RCDE) for 64QAM modulation [34](#__RefHeading___Toc518916836)

10.3.1 Minimum requirement [34](#__RefHeading___Toc518916837)

11 Input Intermodulation [34](#__RefHeading___Toc518916838)

11.1 General Requirement [34](#__RefHeading___Toc518916839)

11.1.1 Minimum requirement [34](#__RefHeading___Toc518916840)

11.2 Co-location with BS in other systems [35](#__RefHeading___Toc518916841)

11.2.1 Minimum requirements - Co-location with GSM, DCS, PCS, UTRA FDD and/or E-UTRA FDD [35](#__RefHeading___Toc518916842)

11.2.2 Minimum Requirement - Co-location with UTRA-TDD and/or E-UTRA TDD [38](#__RefHeading___Toc518916843)

11.3 Co-existence with other systems [39](#__RefHeading___Toc518916844)

11.3.1 Minimum requirements [39](#__RefHeading___Toc518916845)

12 Output intermodulation [42](#__RefHeading___Toc518916846)

12.1 Minimum requirement [42](#__RefHeading___Toc518916847)

13 Adjacent Channel Rejection Ratio (ACRR) [43](#__RefHeading___Toc518916848)

13.1 Definitions and applicability [43](#__RefHeading___Toc518916849)

13.2 Minimum Requirements [43](#__RefHeading___Toc518916850)

Annex A (informative): Change History [44](#__RefHeading___Toc518916851)

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document..

# 1 Scope

The present document establishes the minimum radio frequency performance of UTRA FDD repeaters.

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] ITU-R Recommendation SM.329: "Unwanted emissions in the spurious domain".

[2] 3GPP TS 25.143: "UTRA Repeater Conformance Testing".

[3] 3GPP TS 25.113: "Base Station and Repeater Electromagnetic Compatibility".

[4] ETSI ETR 273-1-2: "Electromagnetic compatibility and Radio spectrum Matters (ERM); Improvement of radiated methods of measurement (using test sites) and evaluation of the corresponding measurement uncertainties; Part 1: Uncertainties in the measurement of mobile radio equipment characteristics; Sub-part 2: Examples and annexes".

[5] 3GPP TR 25.942: "RF System Scenarios".

[6] 3GPP TS 25.104: "UTRA(BS) FDD; Radio transmission and Reception".

[7] CEPT ECC Decision (13)03, "The harmonised use of the frequency band 1452-1492 MHz for Mobile/Fixed Communications Networks Supplemental Downlink (MFCN SDL) ".

[8] 3GPP TS 36.104: "Evolved Universal Terrestrial Radio Access (E-UTRA); Base Station (BS) radio transmission and reception".

# 3 Definitions, symbols and abbreviations

## 3.1 Definitions

For the purposes of the present document, the following terms and definitions apply:

**Donor coupling loss:** is the coupling loss between the repeater and the donor base station.

**Down-link**: Signal path where base station transmits and mobile receives.

**Operating band**: the frequency range in which UTRA FDD operates, that is defined with a specific set of technical requirements.

NOTE 1: The operating band(s) for an UTRA Repeater is declared by the manufacturer according to the designations in clause 5.1, Table 5.1.

NOTE 2: Unless specified, operating band refers to the uplink operating band and downlink operating band.

**Pass band:** The frequency range in which the repeater operates in with operational configuration. This frequency range can correspond to one or several consecutive nominal 5 MHz channels. If they are not consecutive each subset of channels shall be considered as an individual pass band. A repeater can have one or several pass bands.

**Repeater:** A device that receives, amplifies and transmits the radiated or conducted RF carrier both in the down-link direction (from the base station to the mobile area) and in the up-link direction (from the mobile to the base station). In operating bands specified with only down-link or up-link, only the up-link or down-link as specified for the operating band is repeated.

**Up-link:** Signal path where mobile transmits and base station receives.

## 3.2 Symbols

(void)

## 3.3 Abbreviations

For the purposes of the present document, the following abbreviations apply:

BS Base Transceiver Station

DL Down Link (forward link)

DTT Digital Terrestrial Television

EVM Error Vector Magnitude

EIRP Effective Isotropic Radiated Power

FDD Frequency Division Duplex

FFS For Further Study

IMT2000 International Mobile Telecommunication-2000

ITU International Telecommunication Union

RCDE Relative Code Domain Error.

RF Radio Frequency

UARFCN UTRA Absolute Radio Frequency Channel Number

UL Up Link (reverse link)

UMTS Universal Mobile Telecommunication System

UTRA Universal Terrestrial Radio Access

WCDMA Wide band Code Division Multiple Access

# 4 General

This specification applies only to UTRA-FDD repeaters.

Unless otherwise stated, all requirements in this specification apply to both the up-link and down-link directions, where applicable.

## 4.1 Relationship between Minimum Requirements and Test Requirements

The Minimum Requirements given in this specification make no allowance for measurement uncertainty. The repeater test specification 25.143 section 5 [2] defines Test Tolerances. These Test Tolerances are individually calculated for each test. The Test Tolerances are used to relax the Minimum Requirements in this specification to create Test Requirements.

The measurement results returned by the Test System are compared - without any modification - against the Test Requirements as defined by the shared risk principle.

The Shared Risk principle is defined in ETR 273 Part 1 sub-part 2 section 6.5 [4].

## 4.2 Regional requirements

Some requirements in TS 25.106 may only apply in certain regions. Table 4.1 lists all requirements that may be applied differently in different regions.

Table 4.1: List of regional requirements.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Clause number | Requirement | | Comments | |
| 5.1 | Frequency bands | | Some bands may be applied regionally. | |
| 5.2 | TX – RX frequency separation | | The requirement is applied according to which frequency bands in Clause 5.1 that are supported by the Repeater. | |
| 5.3 | Channel arrangement | | The requirement is applied according to what frequency bands in clause 5.1 that are supported by the Repeater. | |
| 6.1 | Maximum output power | | In certain regions, the minimum requirement for normal conditions may apply also for some conditions outside the ranges of conditions defined as normal. | |
| 9.1. 2 | Operating band unwanted emissions | | The mask specified may be mandatory in certain regions. In other regions this mask may not be applied. Additional spectrum protection may apply regionally. | |
| 9.2.1.1 | Spurious emissions (Category A) | | These requirements shall be met in cases where Category A limits for spurious emissions, as defined in ITU-R Recommendation SM.329 [1], are applied. | |
| 9.2.1.2 | Spurious emissions (Category B) | | These requirements shall be met in cases where Category B limits for spurious emissions, as defined in ITU-R Recommendation SM.329 [1], are applied. | |
| 9.2.3 | | Spurious emissions: Co-existence with other systems in the same geographical area | | These requirements may apply in geographic areas in which both UTRA FDD Repeater and GSM900 DCS1800, PCS1900, GSM850 and/or UTRA FDD operating in another frequency band are deployed. |
| 9.2.4 | | Spurious emissions: Co-existence with co-located and co-sited base stations | | These requirements may be applied for the protection of other BS receivers when GSM900 DCS1800, PCS1900, GSM850 and/or FDD BS operating in another frequency band are co-located with a UTRA FDD Repeater. |
| 9.2.5 | Spurious emissions: Co-existence with PHS | | This requirement may be applied for the protection of PHS in geographic areas in which both PHS and UTRA FDD Repeaters are deployed. | |
| 9.2.6.1 | Spurious emissions: Co-existence with UTRA-TDD and/or E-UTRA TDD - Operation in the same geographic area | | This requirement may be applied for the protection of UTRA UE in geographic areas in which both UTRA TDD BS and UTRA FDD Repeaters are deployed. | |
| 9.2.6.2 | Spurious emissions: Co-existence with UTRA-TDD and/or E-UTRA TDD - Co-location | | This requirement may be applied for the protection of UTRA TDD BS receivers when UTRA TDD BS and UTRA FDD Repeaters are co-located. | |
| 9.2.8 | Spurious emissions: Protection of public safety operations | | This requirement may be applied for the protection of public safety systems in geographic areas in which both UTRA FDD Repeater and public safety systems are deployed. | |
| 11.2 | Input Intermodulation: Co-location with BS in other systems | | The requirement may be applied when GSM900, DCS1800, PCS1900, GSM850 and/or UTRA FDD BS operating in another frequency band and UTRA-FDD Repeaters are co-located. | |
| 11.3 | Input Intermodulation: Co-existence with other systems | | These requirements may apply in geographic areas in which both UTRA FDD Repeater and GSM900, DCS1800, PCS1900, GSM850 and/or UTRA FDD operating in another frequency band are deployed. | |

# 5 Frequency bands and channel arrangement

## 5.1 Frequency bands

a) A UTRA/FDD Repeater is designed to operate in one or several pass bands within either of the following operating bands;

Table 5.1: Frequency bands

|  |  |  |
| --- | --- | --- |
| Operating Band | UL Frequencies  UE transmit, Node B receive | DL frequencies  UE receive, Node B transmit |
| I | 1920 - 1980 MHz | 2110 -2170 MHz |
| II | 1850 -1910 MHz | 1930 -1990 MHz |
| III | 1710 - 1785 MHz | 1805 - 1880 MHz |
| IV | 1710 - 1755 MHz | 2110 - 2155 MHz |
| V | 824 - 849MHz | 869 - 894MHz |
| VI | 830 - 840 MHz | 875 - 885 MHz |
| VII | 2500 - 2570 MHz | 2620 - 2690 MHz |
| VIII | 880 - 915 MHz | 925 - 960 MHz |
| IX | 1749.9 - 1784.9 MHz | 1844.9 - 1879.9 MHz |
| X | 1710 - 1770 MHz | 2110 - 2170 MHz |
| XI | 1427.9 - 1447.9 MHz | 1475.9 - 1495.9 MHz |
| XII | 698 - 716 MHz | 728 - 746 MHz |
| XIII | 777 - 787 MHz | 746 - 756 MHz |
| XIV | 788 - 798 MHz | 758 - 768 MHz |
| XV | Reserved | Reserved |
| XVI | Reserved | Reserved |
| XVII | Reserved | Reserved |
| XVII | Reserved | Reserved |
| XIX | 830 – 845 MHz | 875 – 890 MHz |
| XX | 832 – 862 MHz | 791 – 821 MHz |
| XXI | 1447.9 – 1462.9 MHz | 1495.9 – 1510.9 MHz |
| XXII | 3410 – 3490 MHz | 3510 – 3590 MHz |
| XXV | 1850 – 1915 MHz | 1930 – 1995 MHz |
| XXVI | 814 – 849 MHz | 859 – 894 MHz |
| XXXII | N/A | 1452 – 1496 MHz |

b) Deployment in other frequency bands is not precluded.

## 5.2 TX - RX frequency separation

a) A UTRA/FDD repeaters is designed to operate with the following TX to RX frequency separation

Table 5.2: TX-RX frequency separation

|  |  |
| --- | --- |
| Operating Band | TX-RX frequency separation |
| I | 190 MHz |
| II | 80 MHz. |
| III | 95 MHz |
| IV | 400 MHz |
| V | 45 MHz |
| VI | 45 MHz |
| VII | 120 MHz |
| VIII | 45 MHz |
| IX | 95 MHz |
| X | 400 MHz |
| XI | 48 MHz |
| XII | 30 MHz |
| XIII | 31 MHz |
| XIV | 30 MHz |
| XIX | 45 MHz |
| XX | 41 MHz |
| XXI | 48 MHz |
| XXII | 100 MHz |
| XXV | 80 MHz |
| XXVI | 45 MHz |

b) A UTRA/FDD repeater can support both fixed and variable up-link to down-link frequency separation.

c) The use of other up-link to down-link frequency separations in existing or other frequency bands shall not be precluded.

## 5.3 Channel arrangement

### 5.3.1 Channel spacing

The nominal channel spacing is 5 MHz, but this can be adjusted to optimise performance in a particular deployment scenario.

### 5.3.2 Channel raster

The channel raster is 200 kHz for all bands, which means that the centre frequency must be an integer multiple of 200 kHz. In addition, a number of additional centre frequencies are specified according to the table 5.3, which means that and the centre frequencies for these channels are shifted 100 kHz relative to the general raster.

### 5.3.3 Channel number

The carrier frequency is designated by the UTRA Absolute Radio Frequency Channel Number (UARFCN).

For each operating band, the UARFCN values are defined as follows.

Uplink: NU =5 \* (FUL - FUL\_Offset), for the carrier frequency range FUL\_low FUL  FUL\_high

Downlink: ND =5 \* (FDL - FDL\_Offset), for the carrier frequency range FDL\_low FDL  FDL\_high

For each operating Band, FUL\_Offset, FUL\_low FUL\_high, FDL\_Offset,, FDL\_lowand FDL\_high are defined in Table 5.3 for the general UARFCN. For the additional UARFCN, FUL\_Offset, FDL\_Offset and the specific FUL and FDL are defined in Table 5.4.

Table 5.3: UARFCN definition (general)

| Band | UPLINK (UL)  UE transmit, Node B receive | | | DOWNLINK (DL)  UE receive, Node B transmit | | |
| --- | --- | --- | --- | --- | --- | --- |
| UARFCN formula offset  FUL\_Offset [MHz] | Carrier frequency (FUL) range [MHz] | | UARFCN formula offset  FDL\_Offset [MHz] | Carrier frequency (FDL) range [MHz] | |
| FUL\_low | FUL\_high | **FDL\_low** | **FDL\_high** |
| I | 0 | 1922.4 | 1977.6 | 0 | 2112.4 | 2167.6 |
| II | 0 | 1852.4 | 1907.6 | 0 | 1932.4 | 1987.6 |
| III | 1525 | 1712.4 | 1782.6 | 1575 | 1807.4 | 1877.6 |
| IV | 1450 | 1712.4 | 1752.6 | 1805 | 2112.4 | 2152.6 |
| V | 0 | 826.4 | 846.6 | 0 | 871.4 | 891.6 |
| VI | 0 | 832.4 | 837.6 | 0 | 877.4 | 882.6 |
| VII | 2100 | 2502.4 | 2567.6 | 2175 | 2622.4 | 2687.6 |
| VIII | 340 | 882.4 | 912.6 | 340 | 927.4 | 957.6 |
| IX | 0 | 1752.4 | 1782.4 | 0 | 1847.4 | 1877.4 |
| X | 1135 | 1712.4 | 1767.6 | 1490 | 2112.4 | 2167.6 |
| XI | 733 | 1430.4 | 1450.4 | 736 | 1478.4 | 1498.4 |
| XII | -22 | 700.4 | 713.6 | -37 | 730.4 | 743.6 |
| XIII | 21 | 779.4 | 784.6 | -55 | 748.4 | 753.6 |
| XIV | 12 | 790.4 | 795.6 | -63 | 760.4 | 765.6 |
| XIX | 770 | 832.4 | 842.6 | 735 | 877.4 | 887.6 |
| XX | -23 | 834.4 | 859.6 | -109 | 793.4 | 818.6 |
| XXI | 1358 | 1450.4 | 1460.4 | 1326 | 1498.4 | 1508.4 |
| XXII | 2525 | 3412.4 | 3487.6 | 2580 | 3512.4 | 3587.6 |
| XXV | 875 | 1852.4 | 1912.6 | 910 | 1932.4 | 1992.6 |
| XXVI | -291 | 816.4 | 846.6 | -291 | 861.4 | 891.6 |
| XXXII | - | N/A | N/A | 131 | 1454.4 | 1493.6 |

Table 5.4: UARFCN definition (additional channels)

| Band | UPLINK (UL)  UE transmit, Node B receive | | DOWNLINK (DL)  UE receive, Node B transmit | |
| --- | --- | --- | --- | --- |
| UARFCN formula offset  FUL\_Offset [MHz] | Carrier frequency [MHz]  (FUL) | UARFCN formula offset  FDL\_Offset [MHz] | Carrier frequency [MHz]  (FDL) |
| I | - | **-** | **-** | **-** |
| II | 1850.1 | 1852.5, 1857.5, 1862.5, 1867.5, 1872.5, 1877.5, 1882.5, 1887.5, 1892.5, 1897.5, 1902.5, 1907.5 | 1850.1 | 1932.5, 1937.5, 1942.5, 1947.5, 1952.5, 1957.5, 1962.5, 1967.5, 1972.5, 1977.5, 1982.5, 1987.5 |
| III | - | - | - | - |
| IV | 1380.1 | 1712.5, 1717.5, 1722.5, 1727.5, 1732.5, 1737.5 1742.5, 1747.5, 1752.5 | 1735.1 | 2112.5, 2117.5, 2122.5, 2127.5, 2132.5, 2137.5, 2142.5, 2147.5, 2152.5 |
| V | 670.1 | 826.5, 827.5, 831.5, 832.5, 837.5, 842.5 | 670.1 | 871.5, 872.5, 876.5,  877.5, 882.5, 887.5 |
| VI | 670.1 | 832.5, 837.5 | 670.1 | 877.5, 882.5 |
| VII | 2030.1 | 2502.5, 2507.5, 2512.5,  2517.5, 2522.5, 2527.5,  2532.5, 2537.5, 2542.5,  2547.5, 2552.5, 2557.5,  2562.5, 2567.5 | 2105.1 | 2622.5, 2627.5, 2632.5,  2637.5, 2642.5, 2647.5,  2652.5, 2657.5, 2662.5,  2667.5, 2672.5, 2677.5,  2682.5, 2687.5 |
| VIII | - | - | - | - |
| IX | - | - | - | - |
| X | 1075.1 | 1712.5, 1717.5, 1722.5, 1727.5, 1732.5, 1737.5, 1742.5, 1747.5, 1752.5, 1757.5, 1762.5, 1767.5 | 1430.1 | 2112.5, 2117.5, 2122.5, 2127.5, 2132.5, 2137.5, 2142.5, 2147.5, 2152.5, 2157.5, 2162.5, 2167.5 |
| XI | - | - | - | - |
| XII | -39.9 | 700.5, 701.5, 706.5, 707.5, 712.5, 713.5 | -54.9 | 730.5, 731.5, 736.5, 737.5, 742.5, 743.5 |
| XIII | 11.1 | 779.5, 784.5 | -64.9 | 748.5, 753.5 |
| XIV | 2.1 | 790.5, 795.5 | -72.9 | 760.5, 765.5 |
| XIX | 755.1 | 832.5, 837.5, 842.5 | 720.1 | 877.5, 882.5, 887.5 |
| XX | - | - | - | - |
| XXI | - | - | - | - |
| XXII | - | - | - | - |
| XXV | 810.1 | 1852.5, 1857.5, 1862.5, 1867.5, 1872.5, 1877.5, 1882.5, 1887.5, 1892.5, 1897.5, 1902.5, 1907.5, 1912.5 | 845.1 | 1932.5, 1937.5, 1942.5, 1947.5, 1952.5, 1957.5, 1962.5, 1967.5, 1972.5, 1977.5, 1982.5, 1987.5, 1992.5 |
| XXVI | -325.9 | 816.5, 821.5, 826.5, 827.5, 831.5, 832.5, 836.5, 837.5, 841.5, 842.5, 846.5 | -325.9 | 861.5, 866.5, 871.5, 872.5, 876.5, 877.5, 881.5, 882.5, 886.5, 887.5, 891.5 |
| XXXII | - | - | 87.1 | 1454.5, 1459.5, 1464.5, 1469.5, 1474.5, 1479.5, 1484.5, 1489.5 |

# 6 Output power

Output power, Pout, of the repeater is the mean power of one carrier at maximum repeater gain delivered to a load with resistance equal to the nominal load impedance of the transmitter.

Rated output power, PRAT, of the repeater is the mean power level per carrier at maximum repeater gain that the manufacturer has declared to be available at the antenna connector.

## 6.1 Maximum output power

Maximum output power, Pmax, of the repeater is the mean power level per carrier measured at the antenna connector in specified reference condition.

### 6.1.1 Minimum Requirements

The requirements shall apply at maximum gain, with WCDMA signals in the pass band of the repeater, at levels that produce the maximum rated output power per channel.

When the power of all signals is increased by 10 dB, compared to the power level that produce the maximum rated output power, the requirements shall still be met.

In normal conditions, the Repeater maximum output power shall remain within limits specified in Table 6.1 relative to the manufacturer's rated output power.

Table 6.1: Repeater output power; normal conditions

|  |  |
| --- | --- |
| Rated output power | Limit |
| P  43 dBm | +2 dB and -2 dB |
| 39  P < 43 dBm | +2 dB and -2 dB |
| 31  P < 39 dBm | +2 dB and -2 dB |
| P < 31 dBm | +3 dB and -3 dB |

In extreme conditions, the Repeater maximum output power shall remain within the limits specified in Table 6.2 relative to the manufacturer's rated output power.

Table 6.2: Repeater output power; extreme conditions

|  |  |
| --- | --- |
| Rated output power | Limit |
| P  43 dBm | +2,5 dB and -2,5 dB |
| 39  P < 43 dBm | +2,5 dB and -2,5 dB |
| 31  P < 39 dBm | +2,5 dB and -2,5 dB |
| P < 31 dBm | +4 dB and -4 dB |

In certain regions, the minimum requirement for normal conditions may apply also for some conditions outside the ranges of conditions defined as normal.

# 7 Frequency stability

Frequency stability is the ability to maintain the same frequency on the output signal with respect to the input signal.

## 7.1 Minimum requirement

The frequency deviation of the output signal with respect to the input signal shall be no more than ±0,01 ppm.

# 8 Out of band gain

Out of band gain refers to the gain of the repeater outside the pass band.

## 8.1 Minimum requirement

The intended use of a repeater in a system is to amplify the in band signals and not to amplify the out of band emission of the donor base station.

In the intended application of the repeater, the out of band gain is less than the donor coupling loss.

The repeater minimum donor coupling loss shall be declared by the manufacturer. This is this the minimum required attenuation between the donor BS and the repeater for proper repeater operation.

The gain outside the pass band shall not exceed the maximum level specified in table 8.1, where:

- f\_offset is the distance from the centre frequency of the first or last 5 MHz channel within the pass band.

Table 8.1: Out of band gain limits 1

|  |  |
| --- | --- |
| Frequency offset from the carrier frequency, f\_offset | Maximum gain |
| 2,7  f\_offset < 3,5 MHz | 60 dB |
| 3,5  f\_offset < 7,5 MHz | 45 dB |
| 7,5  f\_offset < 12,5 MHz | 45 dB |
| 12,5 MHz  f\_offset | 35 dB |

For 12,5 MHz  f\_offset the out of band gain shall not exceed the maximum gain of table 8.2 or the maximum gain stated in table 8.1 whichever is lower.

Table 8.2: Out of band gain limits 2

|  |  |
| --- | --- |
| Repeater maximum output power as in 9.1.1.1 | Maximum gain |
| P < 31 dBm | Out of band gain  minimum donor coupling loss |
| 31 dBm  P < 43 dBm | Out of band gain  minimum donor coupling loss |
| P  43 dBm | Out of band gain  minimum donor coupling loss - (P-43dBm) |
| NOTE 1: The out of band gain is considered with 12,5 MHz  f\_offset | |

# 9 Unwanted emission

Unwanted emissions consist of out-of-band emissions and spurious emissions [1]. Out of band emissions are unwanted emissions immediately outside the pass band bandwidth resulting from the modulation process and non-linearity in the transmitter, but excluding spurious emissions. Spurious emissions are emissions which are caused by unwanted transmitter effects such as harmonics emission, parasitic emission, intermodulation products and frequency conversion products, but exclude out of band emissions.

The out-of-band emissions requirement for repeater is specified both in terms operating band unwanted emissions and protection of the BS receiver in the operating band. The Operating band unwanted emissions define all unwanted emissions in the repeater operating band plus the frequency ranges 10 MHz above and 10 MHz below that band. Unwanted emissions outside of this frequency range are limited by a spurious emissions requirement.

## 9.1 Out of band emission

### 9.1.1 Void

### 9.1.2 Operating band unwanted emissions

Operating band unwanted emissions comprise an emission mask applied outside the repeater passband and a general requirement applied outside the mask but inside the frequency range of the operating band unwanted emissions.

The general operating band unwanted emissions limits are given in table 9.0.

Table 9.0: General operating band unwanted emissions requirements

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Frequency range of operating band | Category A | Category B | Measurement bandwidth | Notes |
|  1 GHz | -13 dBm | -16 dBm | 100 kHz | 1,2 |
|  1 GHz | -13 dBm | -15 dBm | 1 MHz | 2,3 |

NOTE 1: Bandwidth as in ITU-R Recommendation SM.329 [1], s4.1.

NOTE 2: Limit based on ITU-R Recommendation SM.329 [1], s4.3 and Annex 7.

NOTE 3: Bandwidth as in ITU-R Recommendation SM.329 [1], s4.1. Upper frequency as in ITU-R SM.329 [1], s2.5 table 1.

The mask defined in tables 9.1 to 9.4 below may be mandatory in certain regions. In other regions this mask may not be applied.

For regions where this clause applies, the requirement shall be met by a repeater's RF-signal output at maximum gain with WCDMA signals in the pass band of the repeater, at levels that produce the maximum rated output power per channel. The requirements shall also apply at maximum gain without WCDMA signals in the pass band.

Emissions shall not exceed the maximum level specified in tables 9.1 to 9.4 for the appropriate repeater maximum output power, in the frequency range from f = 2,5 MHz to fmax from the 5 MHz channel, where:

- f is the separation between the centre frequency of first or last 5 MHz channel used in the pass band and the nominal -3 dB point of the measuring filter closest to the carrier frequency.

- f\_offset is the separation between the centre frequency of first or last 5 MHz channel in the pass band and the centre of the measuring filter.

- f\_offsetmax is 12,5 MHz.

- f max is equal to f\_offsetmax minus half of the bandwidth of the measurement filter.



Figure 9.1: Illustrative diagram of emission mask

Table 9.1: Emission mask values, maximum output power P  43 dBm

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency offset of measurement filter -3dB point, f | Frequency offset of measurement filter centre frequency, f\_offset | Minimum requirement | Measurement bandwidth (Note 2) |
| 2,5 MHz  f < 2,7 MHz | 2,515MHz  f\_offset < 2,715MHz | -14 dBm | 30 kHz |
| 2,7 MHz  f < 3,5 MHz | 2,715MHz  f\_offset < 3,515MHz |  | 30 kHz |
| (Note 1) | 3,515MHz  f\_offset < 4,0MHz | -26 dBm | 30 kHz |
| 3,5 MHz  f  f max | 4,0MHz  f\_offset < f\_offsetmax | -13 dBm | 1 MHz |

Table 9.2: Emission mask values, maximum output power 39  P < 43 dBm

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency offset of measurement filter -3dB point, f | Frequency offset of measurement filter centre frequency, f\_offset | Minimum requirement | Measurement bandwidth (Note 2) |
| 2,5 MHz  f < 2,7 MHz | 2,515MHz  f\_offset < 2,715MHz | -14 dBm | 30 kHz |
| 2,7 MHz  f < 3,5 MHz | 2,715MHz  f\_offset < 3,515MHz |  | 30 kHz |
| (Note 1) | 3,515MHz  f\_offset < 4,0MHz | -26 dBm | 30 kHz |
| 3,5 MHz  f < 7,5 MHz | 4,0MHz  f\_offset < 8,0MHz | -13 dBm | 1 MHz |
| 7,5 MHz  f  f max | 8,0MHz  f\_offset < f\_offsetmax | P - 56 dB | 1 MHz |

Table 9.3: Emission mask values, maximum output power 31  P < 39 dBm

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency offset of measurement filter -3dB point, f | Frequency offset of measurement filter centre frequency, f\_offset | Minimum requirement | Measurement bandwidth (Note 2) |
| 2,5 MHz  f < 2,7 MHz | 2,515MHz  f\_offset < 2,715MHz | P - 53 dB | 30 kHz |
| 2,7 MHz  f < 3,5 MHz | 2,715MHz  f\_offset < 3,515MHz |  | 30 kHz |
| (Note 1) | 3,515MHz  f\_offset < 4,0MHz | P-65 dB | 30 kHz |
| 3,5 MHz  f < 7,5 MHz | 4,0MHz  f\_offset < 8,0MHz | P - 52 dB | 1 MHz |
| 7,5 MHz  f  f max | 8,0MHz  f\_offset < f\_offsetAmax | P - 56 dB | 1 MHz |

Table 9.4: Emission mask values, maximum output power P < 31 dBm

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency offset of measurement filter -3dB point, f | Frequency offset of measurement filter centre frequency, f\_offset | Minimum requirement | Measurement bandwidth (Note 2) |
| 2,5 MHz  f < 2,7 MHz | 2,515MHz  f\_offset < 2,715MHz | -22 dBm | 30 kHz |
| 2,7 MHz  f < 3,5 MHz | 2,715MHz  f\_offset < 3,515MHz |  | 30 kHz |
| ( Note 1) | 3,515MHz  f\_offset < 4,0MHz | -34 dBm | 30 kHz |
| 3,5 MHz  f < 7,5 MHz | 4,0MHz  f\_offset < 8,0MHz | -21 dBm | 1 MHz |
| 7,5 MHz  f  f max | 8,0MHz  f\_offset < f\_offsetmax | -25 dBm | 1 MHz |

For operation in band II, IV, V, X, XII, XIII, XIV, XXV and XXVI, the applicable additional requirement in Tables 9.4A, 9.4B or 9.4C apply in addition to the minimum requirements in Tables 9.1 to 9.4.

Table 9.4A: Additional emission mask values for Bands II, IV, X, XXV

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency offset of measurement filter ‑3dB point, f | Frequency offset of measurement filter centre frequency, f\_offset | Additional requirement | Measurement bandwidth(Note 2) |
| 2.5 MHz  f < 3.5 MHz | 2.515MHz  f\_offset < 3.515MHz | -15 dBm | 30 kHz |
| 3.5 MHz  f  fmax | 4.0MHz  f\_offset < f\_offsetmax | -13 dBm | 1 MHz |

Table 9.4B: Additional emission mask values for Band V and XXVI

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency offset of measurement filter ‑3dB point, f | Frequency offset of measurement filter centre frequency, f\_offset | Additional requirement | Measurement bandwidth(Note 2) |
| 2.5 MHz  f < 3.5 MHz | 2.515MHz  f\_offset < 3.515MHz | -15 dBm | 30 kHz |
| 3.5 MHz  f  fmax | 3.55MHz  f\_offset < f\_offsetmax | -13 dBm | 100 kHz |

Table 9.4C: Additional emission mask values for Bands XII, XIII, XIV

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency offset of measurement filter ‑3dB point, f | Frequency offset of measurement filter centre frequency, f\_offset | Additional requirement | Measurement bandwidth(Note 2) |
| 2.5 MHz  f < 2.6 MHz | 2.515MHz  f\_offset < 2.615MHz | -13 dBm | 30 kHz |
| 2.6 MHz  f  fmax | 2.65MHz  f\_offset < f\_offsetmax | -13 dBm | 100 kHz |

In certain regions the following requirement may apply for protection of DTT. For UTRA Repeater operating in Band XX, the level of emissions in the band 470-790 MHz, measured in an 8MHz filter bandwidth on centre frequencies Ffilter according to Table 9.4.D, shall not exceed the maximum emission level PEM,N declared by the manufacturer.

Table 9.4.D: Declared emissions levels for protection of DTT

|  |  |  |
| --- | --- | --- |
| Filter centre frequency, Ffilter | Measurement bandwidth | Declared emission level [dBm] |
| Ffilter = 8\*N + 306 (MHz);  21 ≤ N ≤ 60 | 8 MHz | PEM,N |

NOTE: The regional requirement is defined in terms of EIRP (effective isotropic radiated power), which is dependent on both the repeater emissions at the antenna connector and the deployment (including antenna gain and feeder loss). The requirement defined above provides the characteristics of the repeater needed to verify compliance with the regional requirement. Compliance with the regional requirement can be determined using the method outlined in TS 25.104 [6] Annex D.

Note for Tables 9.1, 9.2, 9.3, 9.4, 9.4A, 9.4B and 9.4C:

NOTE 1: This frequency range ensures that the range of values of f\_offset is continuous.

In certain regions, the following requirements may apply to UTRA repeaters operating in Band XXXII within 1452-1492 MHz. The level of unwanted emissions, measured on centre frequencies f\_offset with filter bandwidth, according to Table 9.4E shall neither exceed the maximum emission level PEM,B32,a , PEM,B32,b nor PEM,B32,c declared by the manufacturer.

Table 9.4E: Declared operating band XXXII unwanted emission within 1452-1492 MHz

|  |  |  |
| --- | --- | --- |
| Frequency offset of measurement filter centre frequency, f\_offset | Declared emission level [dBm] | Measurement bandwidth |
| 5 MHz | PEM,B32,a | 5 MHz |
| 10 MHz | PEM,B32,b | 5 MHz |
| 15 MHz ≤ f\_offset ≤ f\_offsetmax, B32 | PEM,B32,c | 5 MHz |
| NOTE: f\_offsetmax, B32 denotes the frequency difference between the lower channel carrier frequency and 1454.5 MHz, and the frequency difference between the upper channel carrier frequency and 1489.5 MHz for the set channel position. | | |

NOTE: The regional requirement, included in [7], is defined in terms of EIRP per antenna, which is dependent on both the repeater emissions at the antenna connector and the deployment (including antenna gain and feeder loss). The requirement defined above provides the characteristics of the base station needed to verify compliance with the regional requirement. The assessment of the EIRP level is described in Annex H of TS36.104 [8].

In certain regions, the following requirement may apply to UTRA repeaters operating in Band XXXII within 1452-1492 MHz for the protection of services in spectrum adjacent to the frequency range 1452-1492 MHz. The level of emissions, measured on centre frequencies Ffilter with filter bandwidth according to Table 9.4F shall neither exceed the maximum emission level PEM,B32,d nor PEM,B32,e declared by the manufacturer. This requirement applies in the frequency range 1429-1518 MHz even though part of the range falls in the spurious domain.

Table 9.4F: Operating band XXXII declared emission outside 1452-1492 MHz

| Filter centre frequency, Ffilter | Declared emission level [dBm] | Measurement bandwidth |
| --- | --- | --- |
| 1429.5 MHz ≤ Ffilter ≤ 1448.5 MHz | PEM,B32,d | 1 MHz |
| Ffilter = 1450.5 MHz | PEM,B32,e | 3 MHz |
| Ffilter = 1493.5 MHz | PEM,B32,e | 3 MHz |
| 1495.5 MHz ≤ Ffilter ≤ 1517.5 MHz | PEM,B32,d | 1 MHz |

NOTE: The regional requirement, included in [7], is defined in terms of EIRP, which is dependent on both the repeater emissions at the antenna connector and the deployment (including antenna gain and feeder loss). The requirement defined above provides the characteristics of the base station needed to verify compliance with the regional requirement. The assessment of the EIRP level is described in Annex H of TS36.104 [8].

### 9.1.3. Protection of the BS receiver in the operating band

This requirement shall be applied for the protection of UTRA FDD BS receiver in geographic areas in which UTRA-FDD Repeater and UTRA-FDD BS are deployed.

The requirement applies outside the emission mask.

#### 9.1.3.1 Minimum Requirement

This requirement applies to the uplink of the repeater, at maximum gain.

The power of any operating band unwanted emission shall not exceed the limits in Table 9.7A.

Table 9.7A: Uplink operating band unwanted emissions limits for protection of the BS receiver

|  |  |  |
| --- | --- | --- |
| Maximum Level | Measurement Bandwidth | Note |
| -53 dBm | 100 kHz |  |

NOTE 1: These requirements in Table 9.7A: for the uplink direction of the Repeater reflect what can be achieved with present state of the art technology and are based on a coupling loss of 73 dB between a Repeater and a UTRA FDD BS receiver.

NOTE 2: The requirements shall be reconsidered when the state of the art technology progresses.

NOTE 3: The protection of R-GSM is for further study.

### 9.1.4 Co-existence with services in adjacent frequency bands

This requirement may be applied for the protection in bands adjacent to bands I, or VII, as defined in clause 5.1 in geographic areas in which both an adjacent band service and UTRA are deployed.

The requirement applies only to the down-link direction of the repeater.

#### 9.1.4.1 Minimum requirement

The power of any spurious emission shall not exceed:

Table 9.16: UTRA Repeater down-link spurious emissions limits for protection of adjacent band services

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Operating Band | Band | Maximum Level | Measurement Bandwidth | Note |
| I | 2100-2105 MHz | -30 + 3.4 (f - 2100 MHz) dBm | 1 MHz |  |
| 2175-2180 MHz | -30 + 3.4 (2180 MHz - f) dBm | 1 MHz |  |
| VII | 2610-2615 MHz | -30 + 3.4 (f ‑ 2610 MHz) dBm | 1 MHz |  |
| 2695-2700 MHz | -30 + 3.4 (2700 MHz ‑ f) dBm | 1 MHz |  |

## 9.2 Spurious emissions

Spurious emissions are emissions which are caused by unwanted transmitter effects such as harmonics emission, parasitic emission, intermodulation products and frequency conversion products, but exclude out of band emissions. This is measured at the repeaters RF output port.

The spurious emission limits apply from 9 kHz to 12.75 GHz (or above, as indicated in Table 9.5 and 9.5A), excluding the frequency range from 10 MHz below the lowest frequency of the repeaters operating band up to 10 MHz above the highest frequency of the repeaters operating band. Exceptions are the requirement in Table 9.13 and 9.16 that apply also closer than 10 MHz from repeaters operating band.

Unless otherwise stated, all requirements are measured as mean power.

### 9.2.1 General Requirements

The requirements of either subclause 9.2.1.1 or subclause 9.2.1.2 shall apply whatever the type of repeater considered (one or several pass bands). It applies for all configurations foreseen by the manufacturer’s specification.

#### 9.2.1.1 Minimum Requirement (Category A)

The following requirements shall be met in cases where Category A limits for spurious emissions, as defined in ITU-R Recommendation SM.329 [1], are applied.

At maximum repeater gain, with WCDMA signals in the pass band of the repeater, at levels that produce the maximum rated output power per channel, the power of any spurious emission shall not exceed the limits specified in table 9.5. The requirements shall also apply at maximum gain without WCDMA signals in the pass band.

When the power in all channels is increased by 10 dB, compared to the input level producing the maximum rated output power, the requirement shall still be met.

Table 9.5: Up-link and down-link: General spurious emissions limits, Category A

|  |  |  |  |
| --- | --- | --- | --- |
| Band | Maximum level | Measurement Bandwidth | Note |
| 9kHz - 150kHz | -13 dBm | 1 kHz | Note 1 |
| 150kHz - 30MHz | 10 kHz | Note 1 |
| 30MHz - 1GHz | 100 kHz | Note 1 |
| 1GHz - 12,75 GHz | 1 MHz | Note 2 |
| 12,75GHz – 5th harmonic of the upper frequency edge of the DL or UL operating band for DL or UL spurious emissions, respectively | 1 MHz | Note 2, Note 3 |
| NOTE 1: Bandwidth as in ITU-R SM.329 [1], s4.1  NOTE 2: Upper frequency as in ITU-R SM.329 [1], s2.5 table 1  NOTE 3: Applies only for Band XXII | | | |

#### 9.2.1.2 Minimum Requirement (Category B)

The following requirements shall be met in cases where Category B limits for spurious emissions, as defined in ITU-R Recommendation SM.329 [1], are applied.

At maximum repeater gain, with WCDMA signals in the pass band of the repeater, at levels that produce the maximum rated power output per channel, the power of any spurious emission shall not exceed the limits specified in table 9.5A for the down- and up-link.

The requirements shall also apply at maximum gain without WCDMA signals in the pass band.

When the power in all channels is increased by 10 dB, compared to the input level producing the maximum rated output power, the requirement shall still be met.

Table 9.5A: General spurious emissions limits (Category B)

|  |  |  |  |
| --- | --- | --- | --- |
| Band | Maximum Level | Measurement Bandwidth | Note |
| 9 kHz  150 kHz | -36 dBm | 1 kHz | Note 1 |
| 150 kHz  30 MHz | -36 dBm | 10 kHz | Note 1 |
| 30 MHz  1 GHz | -36 dBm | 100 kHz | Note 1 |
| 1 GHz  12.75 GHz | -30 dBm | 1 MHz | Note 2 |
| 12.75 GHz  5th harmonic of the upper frequency edge of the DL or UL operating band for DL or UL spurious emissions, respectively | -30 dBm | 1 MHz | Note 2, Note 3 |
| NOTE 1: Bandwidth as in ITU-R Recommendation SM.329 [1], s4.1  NOTE 2: Bandwidth as in ITU-R Recommendation SM.329 [1], s4.1. Upper frequency as in ITU-R SM.329 [1], s2.5 table 1  NOTE 3: Applies only for Band XXII | | | |

Table 9.6: (Void)

Table 9.6A: (Void)

Table 9.6B: (Void)

Table 9.6C: (Void)

Table 9.6D: (Void)

Table 9.6E: (Void)

Table 9.6F: (Void)

### 9.2.2 Void

### 9.2.3 Co-existence with other systems in the same geographical area

These requirements may be applied for the protection of UE, MS and/or BS operating in other frequency bands in the same geographical area. The requirements may apply in geographic areas in which both UTRA FDD Repeater and a system operating in another frequency band than the FDD operating band are deployed. The system operating in the other frequency band may be GSM900, DCS1800, PCS1900, GSM850, E-UTRA FDD and/or UTRA FDD.

#### 9.2.3.1 Minimum Requirements

The power of any spurious emission shall not exceed the limits of Table 9.9 for a UTRA FDD Repeater where requirements for co-existence with the system listed in the first column apply.

Table 9.9: UTRA Repeater up-link and down-link spurious emissions limits in geographic coverage area of systems operating in other frequency bands

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| System type operating in the same geographical area | Band for co-existence requirement | Maximum Level | Measurement Bandwidth | Note |
| GSM900 | 921 ‑ 960 MHz | -57 dBm | 100 kHz | This requirement does not apply to UTRA FDD Repeater operating in band VIII |
| 876 - 915 MHz | -61 dBm | 100 kHz | This requirement does not apply to the UL of the UTRA FDD Repeater operating in band VIII, since it is already covered by the requirement in sub-clause 9.1.3 |
| DCS1800 | 1805 ‑ 1880 MHz | -47 dBm | 100 kHz | This requirement does not apply to UTRA FDD Repeater operating in band III. |
| 1710 - 1785 MHz | -61 dBm | 100 kHz | This requirement does not apply to the UL of the UTRA FDD Repeater operating in band III, since it is already covered by the requirement in sub-clause 9.1.3. |
| PCS1900 | 1930 ‑ 1990 MHz | -47 dBm | 100 kHz | This requirement does not apply to UTRA FDD Repeater operating in frequency band II or band XXV. |
| 1850 ‑ 1910 MHz | -61 dBm | 100 kHz | This requirement does not apply to the UL of the UTRA FDD Repeater operating in frequency band II or band XXV, since it is already covered by the requirement in sub-clause 9.1.3. |
| GSM850 or CDMA850 | 869 - 894 MHz | -57 dBm | 100 kHz | This requirement does not apply to UTRA FDD Repeater operating in frequency band V or XXVI. |
| 824 ‑ 849 MHz | -61 dBm | 100 kHz | This requirement does not apply to the UL of the UTRA FDD Repeater operating in frequency band V or XXVI, since it is already covered by the requirement in sub-clause 9.1.3. |
| UTRA FDD Band I or E‑UTRA Band 1 | 2110 - 2170 MHz | -52 dBm | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band I. |
| 1920 - 1980 MHz | -49 dBm | 1 MHz | This requirement does not apply to the UL of the UTRA FDD Repeater operating in band I, since it is already covered by the requirement in sub-clause 9.1.3. |
| UTRA FDD Band II or E‑UTRA Band 2 | 1930 - 1990 MHz | -52 dBm | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band II or band XXV. |
| 1850 - 1910 MHz | -49 dBm | 1 MHz | This requirement does not apply to the UL of the UTRA FDD Repeater operating in band II or band XXV, since it is already covered by the requirement in sub-clause 9.1.3. |
| UTRA FDD Band III or E‑UTRA Band 3 | 1805 - 1880 MHz | -52 dBm | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band III or band IX. |
| 1710 - 1785 MHz | -49 dBm | 1 MHz | This requirement does not apply to the UL of the UTRA FDD Repeater operating in band III, since it is already covered by the requirement in sub-clause 9.1.3.  This requirement does not apply to the uplink of UTRA FDD Repeater operating in band IX in the frequency Range from 1749,9 MHz to 1784,9 MHz, since it is already covered by the requirement in clause 9.1.3. |
| UTRA FDD Band IV or E‑UTRA Band 4 | 2110 - 2155 MHz | -52 dBm | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band IV or band X. |
| 1710 - 1755 MHz | -49 dBm | 1 MHz | This requirement does not apply to the UL of the UTRA FDD Repeater operating in band IV or band X, since it is already covered by the requirement in sub-clause 9.1.3. |
| UTRA FDD Band V or E‑UTRA Band 5 | 869 - 894 MHz | -52 dBm | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band V or XXVI. |
| 824 - 849 MHz | -49 dBm | 1 MHz | This requirement does not apply to the UL of the UTRA FDD Repeater operating in band V or XXVI, since it is already covered by the requirement in sub-clause 9.1.3. |
| UTRA FDD Band VI or XIX or E‑UTRA Band 6, 18 or 19 | 860 - 890 MHz | -52 dBm | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band V, VI, XIX, XX or XXVI. |
| 815 - 830 MHz | -49 dBm | 1 MHz | This requirement does not apply to the UL of the UTRA FDD Repeater operating in band V, VI, XIX, XX or XXVI. |
| 830 – 845 MHz | -49 dBm | 1 MHz | This requirement does not apply to the UL of UTRA FDD Repeater operating in band VI or XIX, since it is already covered by the requirement in sub-clause 9.1.3. This requirement does not apply to the UL of the UTRA FDD Repeater operating in band V, XX or XXVI. |
| UTRA FDD Band VII or E‑UTRA Band 7 | 2620 - 2690 MHz | -52 dBm | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band VII. |
| 2500 - 2570 MHz | -49 dBm | 1 MHz | This requirement does not apply to the UL of the UTRA FDD Repeater operating in band VII, since it is already covered by the requirement in sub-clause 9.1.3. |
| UTRA FDD Band VIII or E‑UTRA Band 8 | 925 - 960 MHz | -52 dBm | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band VIII. |
| 880 - 915 MHz | -49 dBm | 1 MHz | This requirement does not apply to the UL of the UTRA FDD Repeater operating in band VIII, since it is already covered by the requirement in sub-clause 9.1.3. |
| UTRA FDD Band IX or E‑UTRA Band 9 | 1844.9 - 1879.9 MHz | -52 dBm | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band III or band IX. |
| 1749. 9 - 1784.9 MHz | -49 dBm | 1 MHz | This requirement does not apply to the UL of the UTRA FDD Repeater operating in band III or band IX, since it is already covered by the requirement in sub-clause 9.1.3. |
| UTRA FDD Band X or E‑UTRA Band 10 | 2110 - 2170 MHz | -52 dBm | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band IV or band X. |
| 1710 - 1770 MHz | -49 dBm | 1 MHz | This requirement does not apply to the UL of the UTRA FDD Repeater operating in band X, since it is already covered by the requirement in sub-clause 9.1.3.  This requirement does not apply to the uplink of UTRA FDD Repeater operating in band IV in the frequency Range from 1710 MHz to 1755 MHz, since it is already covered by the requirement in clause 9.1.3. |
| UTRA FDD Band XI or XXI or E‑UTRA Band 11 or 21 | 1475.9 - 1510.9 MHz | -52 dBm | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band XI, band XXI or XXXII. |
| 1427.9 - 1447.9 MHz | -49 dBm | 1 MHz | This requirement does not apply to the UL of the UTRA FDD Repeater operating in band XI, since it is already covered by the requirement in sub-clause 9.1.3. For UTRA repeaters operating in band XXXII, this requirement applies for carriers allocated within 1475.9MHz and 1495.9MHz. |
| 1447.9 - 1462.9 MHz | -49 dBm | 1 MHz | This requirement does not apply to the UL of the UTRA FDD Repeater operating in band XXI, since it is already covered by the requirement in sub-clause 9.1.3. For UTRA repeaters operating in band XXXII, this requirement applies for carriers allocated within 1475.9MHz and 1495.9MHz. |
| UTRA FDD Band XII or E‑UTRA Band 12 | 728 - 746 MHz | -52 dBm | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band XII. |
| 698 - 716 MHz | -49 dBm | 1 MHz | This requirement does not apply to the UL of the UTRA FDD Repeater operating in band XII, since it is already covered by the requirement in sub-clause 9.1.3. |
| UTRA FDD Band XIII or E‑UTRA Band 13 | 746 - 756 MHz | -52 dBm | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band XIII. |
| 777 - 787 MHz | -49 dBm | 1 MHz | This requirement does not apply to the UL of the UTRA FDD Repeater operating in band XIII, since it is already covered by the requirement in sub-clause 9.1.3. |
| UTRA FDD Band XIV or E‑UTRA Band 14 | 758 - 768 MHz | -52 dBm | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band XIV. |
| 788 - 798 MHz | -49 dBm | 1 MHz | This requirement does not apply to the UL of the UTRA FDD Repeater operating in band XIV, since it is already covered by the requirement in sub-clause 9.1.3. |
| E‑UTRA Band 17 | 734 - 746 MHz | -52 dBm | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band XII. |
| 704 - 716 MHz | -49 dBm | 1 MHz | This requirement does not apply to the UL of the UTRA FDD Repeater operating in band XII, since it is already covered by the requirement in sub-clause 9.1.3. |
| UTRA FDD Band XX or E‑UTRA Band 20 | 791 - 821 MHz | -52 dBm | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band XX. |
| 832 - 862 MHz | -49 dBm | 1 MHz | This requirement does not apply to the UL of the UTRA FDD Repeater operating in band XIII, since it is already covered by the band XX requirement in sub-clause 9.1.3. |
| UTRA FDD Band XXII or  E-UTRA Band 22 | 3510 - 3590 MHz | -52 dBm | 1 MHz | This requirement does not apply to UTRA FDD repeater operating in band XXII. |
| 3410 - 3490 MHz | -49 dBm | 1 MHz | This requirement does not apply to the uplink of the UTRA FDD repeater operating in band XXII, since it is already covered by the requirement in sub-clause 9.1.3. |
| E-UTRA Band 23 | 2180 - 2200 MHz | -52 dBm | 1 MHz |  |
| 2000 - 2020 MHz | -49 dBm | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band II or band XXV, where the limits are defined separately. |
| 2000 – 2010 MHz | -30 dBm | 1 MHz | This requirement only applies to UTRA FDD Repeater operating in band II or band XXV. This requirement applies starting 5 MHz above the band XXV DL operating band. |
| 2010 – 2020 MHz | -49 dBm | 1 MHz |
| E-UTRA Band 24 | 1525 – 1559 MHz | -52 dBm | 1 MHz |  |
| 1626.5 – 1660.5 MHz | -49 dBm | 1 MHz |  |
| UTRA FDD Band XXV or  E-UTRA Band 25 | 1930 - 1995 MHz | -52 dBm | 1 MHz | This requirement does not apply to UTRA FDD repeater operating in band II or band XXV. |
| 1850 - 1915 MHz | -49 dBm | 1 MHz | This requirement does not apply to the UL of the UTRA FDD repeater operating in band XXV since it is already covered by the requirement in sub-clause 9.1.3. For UTRA FDD repeater operating in band II, it applies for 1910 MHz to 1915 MHz, while the rest is covered in sub-clause 9.1.3. |
| UTRA FDD Band XXVI or  E-UTRA Band 26 | 859 - 894 MHz | -52 dBm | 1 MHz | This requirement does not apply to UTRA FDD repeater operating in band V or band XXVI. |
| 814 - 849 MHz | -49 dBm | 1 MHz | This requirement does not apply to the UL of the UTRA FDD repeater operating in band XXVI since it is already covered by the requirement in sub-clause 9.1.3. For UTRA FDD repeater operating in band V, it applies for 814 MHz to 824 MHz, while the rest is covered in sub-clause 9.1.3. |
| E-UTRA Band 27 | 852 - 869 MHz | -52 dBm | 1 MHz | This requirement does not apply to UTRA FDD repeater operating in band V or band XXVI. |
| 807 - 824 MHz | -49 dBm | 1 MHz | For UTRA FDD repeater operating in band XXVI, it applies for 807 MHz to 814 MHz, while the rest is covered in sub-clause 9.1.3. |
| E-UTRA Band 28 | 758 - 803 MHz | -52 dBm | 1 MHz |  |
| 703 - 748 MHz | -49 dBm | 1 MHz |  |
| E-UTRA Band 29 | 717 – 728 MHz | -52 dBm | 1 MHz |  |
| E-UTRA Band 30 | 2350 - 2360 MHz | -52 dBm | 1 MHz |  |
| 2305 - 2315 MHz | -49 dBm | 1 MHz |  |
| E-UTRA Band 31 | 462.5 – 467.5 MHz | -52 dBm | 1 MHz |  |
| 452.5 – 457.5 MHz | -49 dBm | 1 MHz |  |
| UTRA FDD Band XXXII or E-UTRA Band 32 | 1452 – 1496 MHz | -52 dBm | 1 MHz | This requirement does not apply to UTRA repeater operating in Band XI, XXI, or XXXII |
| NOTE 1: The co-existence requirements do not apply for the 10 MHz frequency range immediately outside the repeaters operating band (see Table 5.1). Emission limits for this excluded frequency range may be covered by local or regional requirements.  NOTE 2: The table above assumes that two operating bands, where the frequency ranges would be overlapping, are not deployed in the same geographical area. For such a case of operation with overlapping frequency arrangements in the same geographical area, special co-existence requirements may apply that are not covered by the 3GPP specifications. | | | | |

### 9.2.4 Co-existence with co-located and co-sited Base Stations

These requirements may be applied for the protection of other BS receivers when GSM900 and/or DCS1800, PCS1900, GSM850, E-UTRA FDD and/or UTRA FDD BS are co-located with a UTRA FDD Repeater.

#### 9.2.4.1 Minimum Requirements

The power of any spurious emission shall not exceed the limits of Table 9.10 for a UTRA FDD Repeater where requirements for co-location with the Base Station listed in the first column apply.

Table 9.10: UTRA Repeater up-link and down-link spurious emissions limits for Repeater co-located with Base Stations

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Type of co-located Base Station | | Band for co-location requirement | | Maximum Level | | Measurement Bandwidth | | Note |
| GSM900 | | 876 - 915 MHz | | -98 dBm | | 100 kHz | | This requirement does not apply to the UL of UTRA FDD Repeater operating in band VIII. The sub-clause 9.1.3 requirement applies, but requires a 75dB coupling loss between BS and the repeater UL transmit port. |
| DCS1800 | | 1710 - 1785 MHz | | -98 dBm | | 100 kHz | | This requirement does not apply to the UL of UTRA FDD Repeater operating in band III. The sub-clause 9.1.3 requirement applies, but requires a 75dB coupling loss between BS and the repeater UL transmit port. |
| PCS1900 | | 1850 - 1910 MHz | | -98 dBm | | 100 kHz | | This requirement does not apply to the UL of UTRA FDD Repeater operating in band II or band XXV. The sub-clause 9.1.3 requirement applies, but requires a 75dB coupling loss between BS and the repeater UL transmit port. |
| GSM850 or CDMA850 | | 824 - 849 MHz | | -98 dBm | | 100 kHz | | This requirement does not apply to the UL of UTRA FDD Repeater operating in band V or band XXVI. The sub-clause 9.1.3 requirement applies, but requires a 75dB coupling loss between BS and the repeater UL transmit port. |
| UTRA FDD Band I or E‑UTRA Band 1 | | 1920 - 1980 MHz | | -96 dBm | | 100 kHz | | This requirement does not apply to the UL of UTRA FDD Repeater operating in band I. The sub-clause 9.1.3 requirement applies, but requires a 73dB coupling loss between BS and the repeater UL transmit port. |
| UTRA FDD Band II or E‑UTRA Band 2 | | 1850 - 1910 MHz | | -96 dBm | | 100 kHz | | This requirement does not apply to the UL of UTRA FDD Repeater operating in band II or band XXV. The sub-clause 9.1.3 requirement applies, but requires a 73dB coupling loss between BS and the repeater UL transmit port. |
| UTRA FDD Band III or E‑UTRA Band 3 | | 1710 - 1785 MHz | | -96 dBm | | 100 kHz | | This requirement does not apply to the UL of UTRA FDD Repeater operating in band III. The sub-clause 9.1.3 requirement applies, but requires a 73dB coupling loss between BS and the repeater UL transmit port. This requirement does not apply to the uplink of UTRA FDD Repeater operating in band IX in the frequency Range from 1749,9 MHz to 1784,9 MHz, since it is already covered by the requirement in clause 9.1.3, but requires a 73dB coupling loss between base station and the repeater UL transmit port. |
| UTRA FDD Band IV or E‑UTRA Band 4 | | 1710 - 1755 MHz | | -96 dBm | | 100 kHz | | This requirement does not apply to the UL of UTRA FDD Repeater operating in band IV or band X. The sub-clause 9.1.3 requirement applies, but requires a 73dB coupling loss between BS and the repeater UL transmit port. |
| UTRA FDD Band V or E‑UTRA Band 5 | | 824 - 849 MHz | | -96 dBm | | 100 kHz | | This requirement does not apply to the UL of UTRA FDD Repeater operating in band V or band XXVI. The sub-clause 9.1.3 requirement applies, but requires a 73dB coupling loss between BS and the repeater UL transmit port. |
| UTRA FDD Band VI or XIX or E‑UTRA Band 6, 18 or 19 | | 815 - 830 MHz | | -96 dBm | | 100 kHz | | This requirement does not apply to the UL of UTRA FDD Repeater operating in band V, VI, XIX, XX or XXVI. |
| 830 – 845 MHz | | -96 dBm | | 100 kHz | | This requirement does not apply to the UL of UTRA FDD Repeater operating in band VI or XIX. The sub-clause 9.1.3 requirement applies, but requires a 73dB coupling loss between BS and the repeater UL transmit port. This requirement does not apply to the UL of UTRA FDD Repeater operating in band V, XX or XXVI. |
| UTRA FDD Band VII or E‑UTRA Band 7 | 2500 - 2570 MHz | | -96 dBm | | 100 kHz | | This requirement does not apply to the UL of UTRA FDD Repeater operating in band VII. The sub-clause 9.1.3 requirement applies, but requires a 73dB coupling loss between BS and the repeater UL transmit port. | |
| UTRA FDD Band VIII or E‑UTRA Band 8 | 880 - 915 MHz | | -96 dBm | | 100 kHz | | This requirement does not apply to the UL of UTRA FDD Repeater operating in band VIII. The sub-clause 9.1.3 requirement applies, but requires a 73dB coupling loss between BS and the repeater UL transmit port. | |
| UTRA FDD Band IX or E‑UTRA Band 9 | 1749.9 - 1784.9 MHz | | -96 dBm | | 100 kHz | | This requirement does not apply to the UL of UTRA FDD Repeater operating in band III or band IX. The sub-clause 9.1.3 requirement applies, but requires a 73dB coupling loss between BS and the repeater UL transmit port. | |
| UTRA FDD Band X or E‑UTRA Band 10 | 1710 - 1770 MHz | | -96 dBm | | 100 kHz | | This requirement does not apply to the UL of UTRA FDD Repeater operating in band X. The sub-clause 9.1.3 requirement applies, but requires a 73dB coupling loss between BS and the repeater UL transmit port. This requirement does not apply to the uplink of E-UTRA FDD Repeater operating in band IV in the frequency range from 1710 MHz to 1755 MHz, since it is already covered by the requirement in clause 9.1.3, but requires a 73dB coupling loss between base station and the repeater UL transmit port. | |
| UTRA FDD Band XI or XXI or E‑UTRA Band 11 or 21 | 1427.9 - 1447.9 MHz | | -96 dBm | | 100 kHz | | This requirement does not apply to the UL of UTRA FDD Repeater operating in band XI. The sub-clause 9.1.3 requirement applies, but requires a 73dB coupling loss between BS and the repeater UL transmit port. This requirement applies only for operation between 1475.9 MHz and 1495.9 MHz for UTRA FDD repeater operating in band XXXII. | |
| 1447.9 - 1462.9 MHz | | -96 dBm | | 100 kHz | | This requirement does not apply to the UL of UTRA FDD Repeater operating in band XXI. The sub-clause 9.1.3 requirement applies, but requires a 73dB coupling loss between BS and the repeater UL transmit port. This requirement applies only for operation between 1475.9 MHz and 1495.9 MHz for UTRA FDD repeater operating in band XXXII. | |
| UTRA FDD Band XII or E‑UTRA Band 12 | 698 - 716 MHz | | -96 dBm | | 100 kHz | | This requirement does not apply to the UL of UTRA FDD Repeater operating in band XII. The sub-clause 9.1.3 requirement applies, but requires a 73dB coupling loss between BS and the repeater UL transmit port. | |
| UTRA FDD Band XIII or E‑UTRA Band 13 | 777 - 787 MHz | | -96 dBm | | 100 kHz | | This requirement does not apply to the UL of UTRA FDD Repeater operating in band XIII. The sub-clause 9.1.3 requirement applies, but requires a 73dB coupling loss between BS and the repeater UL transmit port. | |
| UTRA FDD Band XIV or E‑UTRA Band 14 | 788 - 798 MHz | | -96 dBm | | 100 kHz | | This requirement does not apply to the UL of UTRA FDD Repeater operating in band XIV. The sub-clause 9.1.3 requirement applies, but requires a 73dB coupling loss between BS and the repeater UL transmit port. | |
| E‑UTRA Band 17 | 704 - 716 MHz | | -96 dBm | | 100 kHz | | This requirement does not apply to the UL of UTRA FDD Repeater operating in band XII. The sub-clause 9.1.3 requirement applies, but requires a 73dB coupling loss between BS and the repeater UL transmit port. | |
| UTRA FDD Band XX or E‑UTRA Band 20 | 832 – 862 MHz | | -96 dBm | | 100 kHz | | This requirement does not apply to the UL of UTRA FDD Repeater operating in band XX. The sub-clause 9.1.3 requirement applies, but requires a 73dB coupling loss between BS and the repeater UL transmit port. | |
| UTRA FDD Band XXII or E‑UTRA Band 22 | 3410 - 3490 MHz | | -96 dBm | | 100 kHz | | This requirement does not apply to the UL of UTRA FDD Repeater operating in band XXII. The sub-clause 9.1.3 requirement applies, but requires a 73dB coupling loss between BS and the repeater UL transmit port. | |
| E‑UTRA Band 23 | 2000 - 2020 MHz | | -96 dBm | | 100 kHz | |  | |
| E‑UTRA Band 24 | 1626.5 - 1660.5 MHz | | -96 dBm | | 100 kHz | |  | |
| UTRA FDD Band XXV or E‑UTRA Band 25 | 1850 - 1915 MHz | | -96 dBm | | 100 kHz | | This requirement does not apply to the UL of UTRA FDD Repeater operating in band XXV. The sub-clause 9.1.3 requirement applies, but requires a 73dB coupling loss between BS and the repeater UL transmit port. For UTRA FDD Repeater operating in band 2, it applies from 1910MHz to 1915MHz, while the rest is covered in sub-clause 9.1.3, but requires a 73dB coupling loss between BS and the repeater UL transmit port. | |
| UTRA FDD Band XXVI or E UTRA Band 26 | 814 – 849 MHz | | -96 dBm | | 100 kHz | | This requirement does not apply to the UL of UTRA FDD Repeater operating in band XXVI. The sub-clause 9.1.3 requirement applies, but requires a 73dB coupling loss between BS and the repeater UL transmit port. For UTRA FDD Repeater operating in band V, it applies from 814 MHz to 824MHz, while the rest is covered in sub-clause 9.1.3, but requires a 73dB coupling loss between BS and the repeater UL transmit port. | |
| E-UTRA Band 27 | 807 – 824 MHz | | -96 dBm | | 100 kHz | | For UTRA FDD Repeater operating in band XXVI, this requirement applies from 807 MHz to 814MHz, while the rest is covered in sub-clause 9.1.3, but requires a 73dB coupling loss between BS and the repeater UL transmit port. | |
| E-UTRA Band 28 | 703 – 748 MHz | | -96 dBm | | 100 kHz | |  | |
| E-UTRA Band 30 | 2305 – 2315 MHz | | -96 dBm | | 100 kHz | |  | |
| E.UTRA Band 31 | 452.5 – 457.5 MHz | | -96 dBm | | 100 kHz | |  | |
| NOTE 1: The co-location requirements do not apply for the 10 MHz frequency range immediately outside the repeater operating band (see Table 5.1). The current state-of-the-art technology does not allow a single generic solution for co-location with other system on adjacent frequencies for 30 dB UTRA Repeater-BS minimum coupling loss. However, there are certain site-engineering solutions that can be used. These techniques are addressed in TR 25.942 [5].  NOTE 2: The table above assumes that two operating bands, where the frequency ranges would be overlapping, are not deployed in the same geographical area. For such a case of operation with overlapping frequency arrangements in the same geographical area, special co-existence requirements may apply that are not covered by the 3GPP specifications. | | | | | | | | |

### 9.2.5 Co-existence with PHS

This requirement may be applied for the protection of PHS in geographic areas in which both PHS and UTRA-FDD Repeaters are deployed. This requirement is also applicable at specified frequencies falling between 12,5 MHz below the centre frequency of the first 5 MHz channel or more than 12,5 MHz above the centre frequency of the last 5 MHz channel in the pass band.

#### 9.2.5.1 Minimum Requirement

The power of any spurious emission shall not exceed:

Table 9.13: UTRA Repeater up-link and down-link spurious emissions limits for in geographic coverage area of PHS

|  |  |  |  |
| --- | --- | --- | --- |
| Band | Maximum Level | Measurement Bandwidth | Note |
| 1884,5 ‑ 1915,7 MHz | -41 dBm | 300 kHz |  |

### 9.2.6 Co-existence with UTRA-TDD and/or E-UTRA TDD

#### 9.2.6.1 Operation in the same geographic area

This requirement may be applied to geographic areas in which both UTRA-TDD and/or E-UTRA TDD and UTRA-FDD Repeaters are deployed.

##### 9.2.6.1.1 Minimum Requirement

In the down-link direction of the Repeater the power of any spurious emission shall not exceed:

Table 9.14: UTRA Repeater down-link spurious emissions limits in geographic coverage area of UTRA-TDD and/or E-UTRA TDD

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| System type operating in the same geographical area | Band for co-existence requirement | Maximum Level | Measurement Bandwidth | Note |
| UTRA TDD Band a) or E-UTRA Band 33 | 1900 ‑ 1920 MHz | -52 dBm | 1 MHz |  |
| UTRA TDD Band a) or E-UTRA Band 34 | 2010 ‑ 2025 MHz | -52 dBm | 1 MHz |  |
| UTRA TDD Band d) or E-UTRA Band 38 | 2570 ‑ 2620 MHz | -52 dBm | 1 MHz |  |
| UTRA TDD Band f) or E-UTRA Band 39 | 1880 – 1920 MHz | -52 dBm | 1 MHz | Applicable in China. |
| UTRA TDD in Band e) or E-UTRA Band 40 | 2300 – 2400 MHz | -52 dBm | 1 MHz |  |
| E-UTRA Band 41 | 2496 - 2690 MHz | -52 dBm | 1 MHz |  |
| E-UTRA Band 42 | 3400 – 3600 MHz | -52 dBm | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band XXII. |
| E-UTRA Band 43 | 3600 – 3800 MHz | -52 dBm | 1 MHz |  |
| E-UTRA Band 44 | 703 – 803 MHz | -52 dBm | 1 MHz |  |
| NOTE 1: The co-existence requirements do not apply for the 10 MHz frequency range immediately outside the repeaters operating band (see Table 4.1). Emission limits for this excluded frequency range may be covered by local or regional requirements.  NOTE 2: The table above assumes that two operating bands, where the frequency ranges would be overlapping, are not deployed in the same geographical area. For such a case of operation with overlapping frequency arrangements in the same geographical area, special co-existence requirements may apply that are not covered by the 3GPP specifications. | | | | |

In the up-link direction of the Repeater the power of any spurious emission shall not exceed:

Table 9.14A: UTRA Repeater up-link spurious emissions limits in geographic coverage area of UTRA-TDD and/or E-UTRA TDD

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| System type operating in the same geographical area | Band for co-existence requirement | Maximum Level | Measurement Bandwidth | Note |
| UTRA TDD Band a) or  E-UTRA Band 33 | 1900 ‑ 1920 MHz | -53 dBm | 100 kHz | This requirement is applied only to UTRA FDD Repeater operating in band I, band II or band XXV. |
| 1900 ‑ 1920 MHz | -52 dBm | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band I, band II or band XXV. |
| UTRA TDD Band a) or  E-UTRA Band 34 | 2010 ‑ 2025 MHz | -52 dBm | 1 MHz |  |
| UTRA TDD Band d) or  E-UTRA Band 38 | 2570 ‑ 2620 MHz | -53 dBm | 100 kHz | This requirement is applied only to UTRA FDD Repeater operating in band VII. |
| 2570 ‑ 2620 MHz | -52 dBm | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band VII. |
| UTRA TDD Band f) or  E-UTRA Band 39 | 1880 – 1920 MHz | -53 dBm | 100 kHz | Applicable in China.  This requirement is applied only to UTRA FDD Repeater operating in band II or band XXV. |
| 1880 – 1920 MHz | -52 dBm | 1 MHz | Applicable in China.  This requirement does not apply to UTRA FDD Repeater operating in band II or band XXV. |
| UTRA TDD in Band e) or E-UTRA Band 40 | 2300 – 2400 MHz | -52 dBm | 1 MHz |  |
| E-UTRA Band 41 | 2496 - 2690 MHz | -52 dBm | 1 MHz |  |
| E-UTRA Band 42 | 3400 – 3600 MHz | -52 dBm | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band XXII. |
| E-UTRA Band 43 | 3600 – 3800 MHz | -52 dBm | 1 MHz |  |
| E-UTRA Band 44 | 703 – 803 MHz | -52 dBm | 1 MHz |  |
| NOTE 3: The co-existence requirements do not apply for the 10 MHz frequency range immediately outside the repeaters operating band (see Table 4.1). Emission limits for this excluded frequency range may be covered by local or regional requirements.  NOTE 4: The table above assumes that two operating bands, where the frequency ranges would be overlapping, are not deployed in the same geographical area. For such a case of operation with overlapping frequency arrangements in the same geographical area, special co-existence requirements may apply that are not covered by the 3GPP specifications. | | | | |

NOTE 1: The requirements of -53dBm/100kHz in Table 9.14 and Table 9.14A, which are respectively for the down link and up link direction of the Repeater reflect what can be achieved with present state of the art technology and are based on a coupling loss of 73 dB between a Repeater and a UTRA TDD BS receiver.

NOTE 2: The requirements shall be reconsidered when the state of the art technology progresses.

#### 9.2.6.2 Co-located Repeaters and UTRA-TDD and/or E-UTRA TDD base stations

This requirement may be applied for the protection of UTRA-TDD BS receivers when UTRA-TDD BS and UTRA-FDD Repeater are co-located.

##### 9.2.6.2.1 Minimum Requirement

In the down-link direction of the Repeater the power of any spurious emission shall not exceed:

Table 9.15: UTRA Repeater down-link spurious emissions limits for protection of co-located UTRA TDD and/or E-UTRA TDD BS receiver

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Type of co-located Base Station | Band for co-location requirement | Maximum Level | Measurement Bandwidth | Note |
| UTRA TDD Band a) or  E-UTRA Band 33 | 1900 ‑ 1920 MHz | -86 dBm | 1 MHz |  |
| UTRA TDD Band a) or  E-UTRA Band 34 | 2010 ‑ 2025 MHz | -86 dBm | 1 MHz |  |
| UTRA TDD Band d) or  E-UTRA Band 38 | 2570 ‑ 2620 MHz | -86 dBm | 1 MHz |  |
| UTRA TDD Band f) or  E-UTRA Band 39 | 1880 - 1920MHz | -86 dBm | 1 MHz | Applicable in China |
| UTRA TDD Band e) or  E-UTRA Band 40 | 2300 - 2400MHz | -86 dBm | 1 MHz |  |
| E-UTRA Band 41 | 2496 - 2690 MHz | -86 dBm | 1 MHz | This requirement does not apply to E-UTRA FDD Repeater operating in band VII. |
| E-UTRA Band 42 | 3400 - 3600 MHz | -86 dBm | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band XXII. |
| E-UTRA Band 43 | 3600 - 3800 MHz | -86 dBm | 1 MHz |  |
| E-UTRA Band 44 | 703 – 803 MHz | -86 dBm | 1 MHz |  |
| NOTE 1: The co-location requirements do not apply for the 10 MHz frequency range immediately outside the repeaters operating band (see Table 4.1). Emission limits for this excluded frequency range may be covered by local or regional requirements.  NOTE 2: The table above assumes that two operating bands, where the frequency ranges would be overlapping, are not deployed in the same geographical area. For such a case of operation with overlapping frequency arrangements in the same geographical area, special co-existence requirements may apply that are not covered by the 3GPP specifications. | | | | |

In the up-link direction of the Repeater the power of any spurious emission shall not exceed:

Table 9.15A: UTRA Repeater up-link spurious emissions limits for protection of co-located UTRA TDD and/or E-UTRA TDD BS receiver

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Type of co-located Base Station | Band for co-location requirement | Maximum Level | Measurement Bandwidth | Note |
| UTRA TDD Band a) or  E-UTRA Band 33 | 1900 ‑ 1920 MHz | -53 dBm | 100 kHz | This requirement is applied only to UTRA FDD Repeater operating in band I, band II or band XXV. |
| 1900 ‑ 1920 MHz | -86 dBm | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band I, II or band XXV. |
| UTRA TDD Band a) or  E-UTRA Band 34 | 2010 ‑ 2025 MHz | -83 dBm | 100 kHz | This requirement is applied only to UTRA FDD Repeater operating in band I. |
| 2010 ‑ 2025 MHz | -86 dBm | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band I |
| UTRA TDD Band d) or  E-UTRA Band 38 | 2570 ‑ 2620 MHz | -53 dBm | 100 kHz | This requirement is applied only to UTRA FDD Repeater operating in band VII. |
| 2570 ‑ 2620 MHz | -86 dBm | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band VII. |
| UTRA TDD Band f) or  E-UTRA Band 39 | 1880 – 1920 MHz | -53 dBm | 100 kHz | Applicable in China.  This requirement is applied only to UTRA FDD Repeater operating in band II or band XXV. |
| 1880 – 1920 MHz | -86 dBm | 1 MHz | Applicable in China.  This requirement does not apply to UTRA FDD Repeater operating in band II or band XXV. |
| UTRA TDD in Band e) or  E-UTRA Band 40 | 2300 – 2400 MHz | -86 dBm | 1 MHz |  |
| E-UTRA Band 41 | 2496 - 2690 MHz | -86 dBm | 1 MHz | This requirement does not apply to E-UTRA FDD Repeater operating in band VII. |
| E-UTRA Band 42 | 3400 – 3600 MHz | -86 dBm | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band XXII. |
| E-UTRA Band 43 | 3600 – 3800 MHz | -86 dBm | 1 MHz |  |
| E-UTRA Band 44 | 703 – 803 MHz | -86 dBm | 1 MHz |  |
| NOTE 4: The co-location requirements do not apply for the 10 MHz frequency range immediately outside the repeaters operating band (see Table 4.1). Emission limits for this excluded frequency range may be covered by local or regional requirements.  NOTE 5: The table above assumes that two operating bands, where the frequency ranges would be overlapping, are not deployed in the same geographical area. For such a case of operation with overlapping frequency arrangements in the same geographical area, special co-location requirements may apply that are not covered by the 3GPP specifications. | | | | |

NOTE 1: The requirements of -53dBm/100kHz in Table 9.15 and Table 9.15A , which are respectively for the down link and up link direction of the Repeater reflect what can be achieved with present state of the art technology and are based on a coupling loss of 73 dB between a Repeater and a UTRA TDD BS receiver.

NOTE 2: The requirements of -83dBm/100kHz in Table 9.15A for the up link direction of the Repeater reflect what can be achieved with present state of the art technology and are based on a coupling loss of 43 dB between a Repeater and a UTRA TDD BS receiver.

NOTE 3: The requirements shall be reconsidered when the state of the art technology progresses.

### 9.2.7 Void

### 9.2.8 Protection of public safety operations

This requirement shall be applied to Repeater operating in Bands XIII and XIV to ensure that appropriate interference protection is provided to 700 MHz public safety operations. This requirement is also applicable at specified frequencies falling between 12.5 MHz below the first carrier frequency used and 12.5 MHz above the last carrier frequency used.

#### 9.2.8.1 Minimum Requirement

The power of any spurious emission shall not exceed:

Table 9.16: Spurious emissions limits for the up-link and down-link of UTRA Repeater for protection of 700 MHz public safety operations

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Operating Band | Band | Maximum Level | Measurement Bandwidth | Note |
| XIII | 763 - 775 MHz | -46 dBm | 6.25 kHz |  |
| XIII | 793 - 805 MHz | -46 dBm | 6.25 kHz |  |
| XIV | 769 - 775 MHz | -46 dBm | 6.25 kHz |  |
| XIV | 799 - 805 MHz | -46 dBm | 6.25 kHz |  |

This requirement shall be applied to repeaters operating in Band XXVI to ensure that appropriate interference protection is provided to 800 MHz public safety operations. This requirement is also applicable at specified frequencies falling between 12.5 MHz below the first carrier frequency used and 12.5 MHz above the last carrier frequency used.

The power of any spurious emission shall not exceed:

Table 6.16A: Spurious emissions limits for the up-link and down-link of UTRA Repeater for protection of 800 MHz public safety operations

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Operating Band | Band | Maximum Level | Measurement Bandwidth | Note |
| XXVI | 851 - 859 MHz | -13 dBm | 100 kHz | Applicable for offsets > 37.5kHz from the channel edge |

# 10 Modulation accuracy

## 10.1 Error Vector Magnitude

The modulation accuracy is defined by the Error Vector Magnitude (EVM), which is a measure of the difference between the theoretical waveform and a modified version of the measured waveform. This difference is called the error vector. The measured waveform is modified by first passing it through a matched root raised cosine filter with bandwidth 3.84 MHz and roll-off =0.22. The waveform is then further modified by selecting the frequency, absolute phase, absolute amplitude and chip clock timing so as to minimise the error vector. The EVM result is defined as root of the ratio of the mean error vector power to the mean reference signal power expressed as a %.

The measurement interval is one power control group (timeslot). The repeater shall operate with an ideal WCDMA signal in the pass band of the repeater at a level, which produce the maximum rated output power per channel, as specified by the manufacturer.

### 10.1.1 Minimum requirement

The Error Vector Magnitude shall not be worse than 12,5 %.

## 10.2 Peak code domain error

The peak code domain error is computed by projecting the power of the error vector (as defined in subclause 10.1) onto the code domain at a specified spreading factor. The code domain error for every code in the domain is defined as the ratio of the mean power of the projection onto that code, to the mean power of the composite reference waveform. This ratio is expressed in dB. The peak code domain error is defined as the maximum value for the code domain error for all codes. The measurement interval is one power control group (timeslot).

### 10.2.1 Minimum requirement

The peak code domain error shall not exceed -35 dB at spreading factor 256.

## 10.3 Relative Code Domain Error (RCDE) for 64QAM modulation

The Relative Code Domain Error is computed by projecting the error vector (as defined in 10.1) onto the code domain at a specified spreading factor. Only the active code channels in the composite reference waveform are considered for this requirement. The Relative Code Domain Error for every active code is defined as the ratio of the mean power of the error projection onto that code, to the mean power of the active code in the composite reference waveform. This ratio is expressed in dB. The measurement interval is one frame.

The requirement for Relative Code Domain Error is only applicable for Repeater supporting 64QAM modulated codes.

### 10.3.1 Minimum requirement

The average Relative Code Domain Error for 64QAM modulated codes shall not exceed -21 dB at spreading factor 16.

# 11 Input Intermodulation

The input intermodulation is a measure of the capability of the repeater to inhibit the generation of interference in the pass band, in the presence of interfering signals on frequencies other than the pass band.

## 11.1 General Requirement

The following requirement applies for interfering signals in the frequency bands defined in sub-clause 5.1, depending on the repeaters pass band. The requirement shall bet met with the repeater operating at maximum gain.

### 11.1.1 Minimum requirement

For the parameters specified in table 11.1, the power in the pass band, shall not increase with more than 10 dB at the output of the repeater as measured in the centre of the pass band, compared to the level obtained without interfering signals applied.

The frequency separation between the two interfering signals shall be adjusted so that the 3rd order intermodulation product is positioned in the centre of the pass band.

Table 11.1 specifies the parameters for two interfering signals, where:

- f\_offset is the separation between the centre frequency of first or last 5 MHz channel in the pass band and one the interfering signals.

Table 11.1: Input intermodulation requirement

|  |  |  |  |
| --- | --- | --- | --- |
| f\_offset | Interfering Signal Levels | Type of signals | Measurement bandwidth |
| 3,5 MHz | -40 dBm | 2 CW carriers | 1 MHz |

## 11.2 Co-location with BS in other systems

The requirement shall bet met with the repeater operating at maximum gain.

### 11.2.1 Minimum requirements - Co-location with GSM, DCS, PCS, UTRA FDD and/or E-UTRA FDD

This additional input intermodulation requirement may be applied for the protection of FDD Repeater input when GSM900, DCS1800, PCS1900, GSM850, E-UTRA FDD and/or UTRA FDD BS are co-located with a UTRA FDD Repeater.

For the parameters specified in table 11.2, the power in the pass band shall not increase with more than 10 dB at the output of the repeater as measured in the centre of the pass band, compared to the level obtained without interfering signals applied.

The frequency separation between the two interfering signals shall be adjusted so that the lowest order intermodulation product is positioned in the centre of the pass band.

NOTE 1: The lowest intermodulation product corresponds to the 4th and 3rd order for the GSM 900 and DCS 1800 bands, respectively.

Table 11.2: Input intermodulation requirements for interfering signals in other systems

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Co-located other systems | Frequency of interfering signals | Interfering Signal Levels | Type of signals | Measurement bandwidth | Note |
| GSM900 | 921 ‑ 960 MHz | +16 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band VIII, since it is already covered by the requirement in sub-clause 11.1, but requires a 86dB coupling loss between BS and the repeater DL receive port. |
| DCS1800 | 1805 ‑ 1880 MHz | +16 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band III, since it is already covered by the requirement in sub-clause 11.1, but requires a 86dB coupling loss between BS and the repeater DL receive port. |
| PCS1900 | 1930 - 1990 MHz | +16 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band II or band XXV, since it is already covered by the requirement in sub-clause 11.1, but requires a 86dB coupling loss between BS and the repeater DL receive port. |
| GSM850 or CDMA850 | 869 - 894 MHz | +16 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band V or XXVI, since it is already covered by the requirement in sub-clause 11.1, but requires a 86dB coupling loss between BS and the repeater DL receive port. |
| UTRA-FDD Band I or E‑UTRA Band 1 | 2110 - 2170 MHz | +16 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band I, since it is already covered by the requirement in sub-clause 11.1, but requires a 86dB coupling loss between BS and the repeater DL receive port. |
| UTRA-FDD Band II or E‑UTRA Band 2 | 1930 - 1990 MHz | +16 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band II or band XXV, since it is already covered by the requirement in sub-clause 11.1, but requires a 86dB coupling loss between BS and the repeater DL receive port. |
| UTRA-FDD Band III or E‑UTRA Band 3 | 1805 - 1880 MHz | +16 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band III or band IX, since it is already covered by the requirement in sub-clause 11.1, but requires a 86dB coupling loss between BS and the repeater DL receive port. |
| UTRA-FDD Band IV or E‑UTRA Band 4 | 2110 - 2155 MHz | +16 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band IV or band X, since it is already covered by the requirement in sub-clause 11.1, but requires a 86dB coupling loss between BS and the repeater DL receive port. |
| UTRA-FDD Band V or E‑UTRA Band 5 | 869 - 894 MHz | +16 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band V or band XXVI, since it is already covered by the requirement in sub-clause 11.1, but requires a 86dB coupling loss between BS and the repeater DL receive port. |
| UTRA-FDD Band VI or XIX or E‑UTRA Band 6, 18 or 19 | 860 - 890 MHz | +16 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band VI, XIX or XXVI, since it is already covered by the requirement in sub-clause 11.1, but requires a 86dB coupling loss between BS and the repeater DL receive port. |
| UTRA-FDD Band VII or E‑UTRA Band 7 | 2620 - 2690 MHz | +16 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band VII, since it is already covered by the requirement in sub-clause 11.1, but requires a 86dB coupling loss between BS and the repeater DL receive port. |
| UTRA-FDD Band VIII or E‑UTRA Band 8 | 925 - 960 MHz | +16 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band VIII, since it is already covered by the requirement in sub-clause 11.1, but requires a 86dB coupling loss between BS and the repeater DL receive port. |
| UTRA-FDD Band IX or E‑UTRA Band 9 | 1844.9 - 1879.9 MHz | +16 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band III or band IX, since it is already covered by the requirement in sub-clause 11.1, but requires a 86dB coupling loss between BS and the repeater DL receive port. |
| UTRA-FDD Band X or E‑UTRA Band 10 | 2110 - 2170 MHz | +16 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band IV or band X, since it is already covered by the requirement in sub-clause 11.1, but requires a 86dB coupling loss between BS and the repeater DL receive port. |
| UTRA-FDD Band XI or XXI or E‑UTRA Band 11 or 21 | 1475.9 - 1510.9 MHz | +16 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band XI or band XXI, since it is already covered by the requirement in sub-clause 11.1, but requires a 86dB coupling loss between BS and the repeater DL receive port. This requirement does not apply to UTRA FDD Repeater operating in band XXXII, between 1475.9 MHz and 1496 MHz, since it is already covered by the requirement in sub-clause 11.1, but requires a 86dB coupling loss between base station and the repeater DL receive port. |
| UTRA-FDD Band XII or E‑UTRA Band 12 | 728 - 746 MHz | +16 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band XII, since it is already covered by the requirement in sub-clause 11.1, but requires a 86dB coupling loss between BS and the repeater DL receive port. |
| UTRA-FDD Band XIII or E‑UTRA Band 13 | 746 - 756 MHz | +16 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band XIII, since it is already covered by the requirement in sub-clause 11.1, but requires a 86dB coupling loss between BS and the repeater DL receive port. |
| UTRA-FDD Band XIV or E‑UTRA Band 14 | 758 - 768 MHz | +16 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band XIV, since it is already covered by the requirement in sub-clause 11.1, but requires a 86dB coupling loss between BS and the repeater DL receive port. |
| E‑UTRA Band 17 | 734 - 746 MHz | +16 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band XII, since it is already covered by the requirement in sub-clause 11.1, but requires a 86dB coupling loss between BS and the repeater DL receive port. |
| UTRA-FDD Band XX or E‑UTRA Band 20 | 791 - 821 MHz | +16 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band XX, since it is already covered by the requirement in sub-clause 11.1, but requires a 86dB coupling loss between BS and the repeater DL receive port. |
| UTRA-FDD Band XXII or E-UTRA Band 22 | 3510 - 3590 MHz | +16 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band XXII, since it is already covered by the requirement in sub-clause 11.1, but requires a 86dB coupling loss between BS and the repeater DL receive port. |
| E-UTRA Band 23 | 2180 - 2200 MHz | +16 dBm | 2 CW carriers | 1 MHz |  |
| E-UTRA Band 24 | 1525 – 1559 MHz | +16 dBm | 2 CW carriers | 1 MHz |  |
| UTRA-FDD Band XXV or E-UTRA Band 25 | 1930 - 1995 MHz | +16 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band XXV, since it is already covered by the requirement in sub-clause 11.1, but requires a 86dB coupling loss between BS and the repeater DL receive port. For UTRA FDD Repeater operating in band II, it applies from 1990MHz to 1995MHz, while the rest is covered in sub-clause 11.1, but requires a 86dB coupling loss between BS and the repeater DL receive port. |
| UTRA-FDD Band XXVI or E-UTRA Band 26 | 859 - 894 MHz | +16 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band XXVI, since it is already covered by the requirement in sub-clause 11.1, but requires a 86dB coupling loss between BS and the repeater DL receive port. For UTRA FDD Repeater operating in band V, it applies from 859 MHz to 869 MHz, while the rest is covered in sub-clause 11.1, but requires a 86dB coupling loss between BS and the repeater DL receive port. |
| E-UTRA Band 27 | 852 - 869 MHz | +16 dBm | 2 CW carriers | 1 MHz | For UTRA FDD Repeater operating in band XXVI, it applies from 852 MHz to 859 MHz, while the rest is covered in sub-clause 11.1, but requires a 86dB coupling loss between BS and the repeater DL receive port. |
| E-UTRA Band 28 | 758 - 803 MHz | +16 dBm | 2 CW carriers | 1 MHz |  |
| E-UTRA Band 29 | 717 - 728 MHz | +16 dBm | 2 CW carriers | 1 MHz |  |
| E-UTRA Band 30 | 2350 - 2360 MHz | +16 dBm | 2 CW carriers | 1 MHz |  |
| E-UTRA Band 31 | 462.5 – 467.5 MHz | +16 dBm | 2 CW carriers | 1 MHz |  |
| UTRA-FDD Band XXXII or E-UTRA Band 32 | 1452 - 1496 MHz | +16 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band XI, XXI or XXXII, since it is already covered by the requirement in sub-clause 11.1, but requires a 86dB coupling loss between BS and the repeater DL receive port. |
| NOTE 1: The co-location requirements in the table 11.2 do not apply when the repeaters pass band frequency range is adjacent to the frequency range of the co-location requirement in the table 11.2. The current state-of-the-art technology does not allow a single generic solution for co-location with other system on adjacent frequencies for 30 dB Repeater-BS minimum coupling loss. However, there are certain site-engineering solutions that can be used. These techniques are addressed in TR 25.942 [5].  NOTE 2: The table above assumes that two operating bands, where the frequency ranges would be overlapping, are not deployed in the same geographical area. For such a case of operation with overlapping frequency arrangements in the same geographical area, special co-existence requirements may apply that are not covered by the 3GPP specifications. | | | | | |

### 11.2.2 Minimum Requirement - Co-location with UTRA-TDD and/or E-UTRA TDD

An additional input intermodulation requirement may be applied for the protection of FDD BS receivers when UTRA TDD and/or E-UTRA TDD is co-located with a UTRA FDD Repeater.

The requirements in this chapter assume a 30 dB coupling loss between transmitter and receiver.

The current state-of-the-art technology does not allow a single generic solution for co-location with UTRA-TDD on adjacent frequencies for 30dB BS-Repeater minimum coupling loss.

However, there are certain site-engineering solutions that can be used. These techniques are addressed in TR 25.942 [5].

Table 11.2A: Input intermodulation requirements for interfering signals in UTRA and E-UTRA TDD systems

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Co-located other system | Frequency of interfering signals | Interfering Signal Levels | Type of signals | Measurement bandwidth |
| UTRA TDD Band a) or E-UTRA Band 33 | 1900 - 1920 MHz | +16 dBm | 2 CW carriers | 1 MHz |
| UTRA TDD Band a) or  E-UTRA Band 34 | 2010 – 2025 MHz | +16 dBm | 2 CW carriers | 1 MHz |
| UTRA-TDD Band d) or E-UTRA TDD Band 38 | 2570 - 2620 MHz | +16 dBm | 2 CW carriers | 1 MHz |
| UTRA TDD Band f) or  E-UTRA Band 39 | 1880 - 1920MHz | +16 dBm | 2 CW carriers | 1 MHz |
| UTRA TDD Band e) or  E-UTRA Band 40 | 2300 - 2400MHz | +16 dBm | 2 CW carriers | 1 MHz |
| E-UTRA Band 41 | 2496 - 2690 MHz | +16 dBm | 2 CW carriers | 1 MHz |
| E-UTRA Band 42 | 3400 - 3600 MHz | +16 dBm | 2 CW carriers | 1 MHz |
| E-UTRA Band 43 | 3600 - 3800 MHz | +16 dBm | 2 CW carriers | 1 MHz |
| E-UTRA Band 44 | 703 - 803 MHz | +16 dBm | 2 CW carriers | 1 MHz |
| NOTE 1: The co-location requirements in Table 11.2A do not apply when the repeaters pass band frequency range is adjacent to the frequency range of the co-location requirement in the Table 11.2A. The current state-of-the-art technology does not allow a single generic solution for co-location with other system on adjacent frequencies for 30 dB Repeater-BS minimum coupling loss. However, there are certain site-engineering solutions that can be used. These techniques are addressed in TR 25.942 [5]  NOTE 2: The table above assumes that two operating bands, where the frequency ranges would be overlapping, are not deployed in the same geographical area. For such a case of operation with overlapping frequency arrangements in the same geographical area, special co-existence requirements may apply that are not covered by the 3GPP specifications. | | | | |

## 11.3 Co-existence with other systems

The following requirement may be applied when GSM 900, DCS 1800, PCS1900, GSM850, E-UTRA FDD, E-UTRA TDD BS and/or UTRA FDD, UTRA TDD BS operating in another frequency band and UTRA-FDD Repeaters co-exist. The requirement shall bet met with the repeater operating at maximum gain.

### 11.3.1 Minimum requirements

For the parameters specified in table 11.3 and table 11.3A, the power in the pass band shall not increase with more than 10 dB at the output of the repeater as measured in the centre of the pass band, compared to the level obtained without interfering signals applied.

The frequency separation between the two interfering signals shall be adjusted so that the lowest order intermodulation product is positioned in the centre of the pass band.

NOTE 1: The lowest intermodulation product corresponds to the 4th and 3rd order for the GSM 900 and DCS 1800 bands, respectively.

Table 11.3: Input intermodulation requirements for interfering signals in other systems

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Co-existence with other systems | Frequency of interfering signals | Interfering Signal Levels | Type of signals | Measurement bandwidth | Note |
| GSM900 | 876 - 915 MHz | -15 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band VIII, since it is already covered by the requirement in sub-clause 11.1. |
| DCS1800 | 1710 ‑ 1785 MHz | -15 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band III, since it is already covered by the requirement in sub-clause 11.1. |
| PCS1900 | 1850 ‑ 1910 MHz | -15 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band II or band XXV, since it is already covered by the requirement in sub-clause 11.1. |
| GSM850 or CDMA850 | 824 ‑ 849 MHz | -15 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band V or band XXVI, since it is already covered by the requirement in sub-clause 11.1. |
| UTRA-FDD Band I or E‑UTRA Band 1 | 1920 - 1980 MHz | -15 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band I, since it is already covered by the requirement in sub-clause 11.1. |
| UTRA-FDD Band II or E‑UTRA Band 2 | 1850 - 1910 MHz | -15 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band II or band XXV, since it is already covered by the requirement in sub-clause 11.1. |
| UTRA-FDD Band III or E‑UTRA Band 3 | 1710 - 1785 MHz | -15 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band III or band IX, since it is already covered by the requirement in sub-clause 11.1. |
| UTRA-FDD Band IV or E‑UTRA Band 4 | 1710 - 1755 MHz | -15 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band IV or band X, since it is already covered by the requirement in sub-clause 11.1. |
| UTRA-FDD Band V or E‑UTRA Band 5 | 824 - 849 MHz | -15 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band V or band XXVI, since it is already covered by the requirement in sub-clause 11.1. |
| UTRA-FDD Band VI or XIX or E‑UTRA Band 6, 18 or 19 | 815 - 8845 MHz | -15 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band VI or band XIX, since it is already covered by the requirement in sub-clause 11.1. This requirement does not apply to the UL of the UTRA FDD Repeater operating in band V or XX. |
| UTRA-FDD Band VII or E‑UTRA Band 7 | 2500 - 2570 MHz | -15 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band VII, since it is already covered by the requirement in sub-clause 11.1. |
| UTRA-FDD Band VIII or E‑UTRA Band 8 | 880 - 915 MHz | -15 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band VIII, since it is already covered by the requirement in sub-clause 11.1. |
| UTRA-FDD Band IX or E‑UTRA Band 9 | 1749,9 - 1784,9 MHz | -15 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band III or band IX, since it is already covered by the requirement in sub-clause 11.1. |
| UTRA-FDD Band X or E‑UTRA Band 10 | 1710 - 1770 MHz | -15 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band IV or band X, since it is already covered by the requirement in sub-clause 11.1. |
| UTRA-FDD Band XI or XXI or E‑UTRA Band 11 or 21 | 1427.9 - 1447.9 MHz | -15 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band XI, since it is already covered by the requirement in sub-clause 11.1. |
| 1447.9 - 1462.9 MHz | -15 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band XXI, since it is already covered by the requirement in sub-clause 11.1. For UTRA FDD Repeater operating in band XXXII, it applies from 1447.9 MHz to 1452 MHz, while the rest is covered in sub-clause 11. 1. |
| UTRA-FDD Band XII or E‑UTRA Band 12 | 698 - 716 MHz | -15 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band XII, since it is already covered by the requirement in sub-clause 11.1. |
| UTRA-FDD Band XIII or E‑UTRA Band 13 | 777 - 787 MHz | -15 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band XIII, since it is already covered by the requirement in sub-clause 11.1. |
| UTRA-FDD Band XIV or E‑UTRA Band 14 | 788 - 798 MHz | -15 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band XIV, since it is already covered by the requirement in sub-clause 11.1. |
| E‑UTRA Band 17 | 704 - 716 MHz | -15 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band XII, since it is already covered by the requirement in sub-clause 11.1. |
| UTRA-FDD Band XX or E‑UTRA Band 20 | 832 - 862 MHz | -15 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band XX, since it is already covered by the requirement in sub-clause 11.1. |
| UTRA-FDD Band XXII or E‑UTRA Band 22 | 3410 - 3490 MHz | -15 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band XXII, since it is already covered by the requirement in sub-clause 11.1. |
| E‑UTRA Band 23 | 2000 - 2020 MHz | -15 dBm | 2 CW carriers | 1 MHz |  |
| E‑UTRA Band 24 | 1626.5 – 1660.5 MHz | -15 dBm | 2 CW carriers | 1 MHz |  |
| UTRA-FDD Band XXV or E‑UTRA Band 25 | 1850 - 1915 MHz | -15 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band XXV, since it is already covered by the requirement in sub-clause 11.1. For UTRA FDD Repeater operating in band II, it applies from 1910MHz to 1915MHz, while the rest is covered in sub-clause 11.1. |
| UTRA-FDD Band XXVI or E‑UTRA Band 26 | 814 - 849 MHz | -15 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band XXVI, since it is already covered by the requirement in sub-clause 11.1. For UTRA FDD Repeater operating in band V, it applies from 814MHz to 824 MHz, while the rest is covered in sub-clause 11.1. |
| E‑UTRA Band 27 | 807 - 824 MHz | -15 dBm | 2 CW carriers | 1 MHz | For UTRA FDD Repeater operating in band XXVI, this requirement applies from 807MHz to 814 MHz, while the rest is covered in sub-clause 11.1. |
| E‑UTRA Band 28 | 703 - 748 MHz | -15 dBm | 2 CW carriers | 1 MHz |  |
| E‑UTRA Band 30 | 2305 - 2315 MHz | -15 dBm | 2 CW carriers | 1 MHz |  |
| E‑UTRA Band 31 | 452.5 – 457.5 MHz | -15 dBm | 2 CW carriers | 1 MHz |  |
| NOTE 1: The co-existence requirements in Table 11.3 do not apply when the repeaters pass band frequency range is adjacent to the frequency range of the co-existence requirement in the Table 11.3. The current state-of-the-art technology does not allow a single generic solution for co-existence.  NOTE 2: The table above assumes that two operating bands, where the frequency ranges would be overlapping, are not deployed in the same geographical area. For such a case of operation with overlapping frequency arrangements in the same geographical area, special co-existence requirements may apply that are not covered by the 3GPP specifications. | | | | | |

Table 11.3A: Input intermodulation requirements for interfering signals in UTRA and E-UTRA TDD systems

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Co-existence with other systems | Frequency of interfering signals | Interfering Signal Levels | Type of signals | Measurement bandwidth | Note |
| UTRA TDD Band a) or E-UTRA Band 33 | 1900 – 1920 MHz | -15 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band I, band II or band XXV. |
| UTRA TDD Band a) or  E-UTRA Band 34 | 2010 – 2025 MHz | -15 dBm | 2 CW carriers | 1 MHz |  |
| UTRA-TDD Band d) and or  E-UTRA TDD Band 38 | 2570 – 2620 MHz | -15 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band VII. |
| UTRA TDD Band f) or  E-UTRA Band 39 | 1880 - 1920MHz | -15 dBm | 2 CW carriers | 1 MHz | Applicable in China.  This requirement does not apply to UTRA FDD Repeater operating in band II or band XXV. |
| UTRA TDD Band e) or  E-UTRA Band 40 | 2300 - 2400MHz | -15 dBm | 2 CW carriers | 1 MHz |  |
| E-UTRA Band 41 | 2496 - 2690 MHz | -15 dBm | 2 CW carriers | 1 MHz |  |
| E-UTRA Band 42 | 3400 - 3600 MHz | -15 dBm | 2 CW carriers | 1 MHz | This requirement does not apply to UTRA FDD Repeater operating in band XXII. |
| E-UTRA Band 43 | 3600 - 3800 MHz | -15 dBm | 2 CW carriers | 1 MHz |  |
| E-UTRA Band 44 | 703 - 803 MHz | -15 dBm | 2 CW carriers | 1 MHz |  |
| NOTE 1: The co-existence requirements in Table 11.3A do not apply when the repeaters pass band frequency range is adjacent to the frequency range of the co-location requirement in the Table 11.3A. The current state-of-the-art technology does not allow a single generic solution for co-location with other system on adjacent frequencies for 30 dB Repeater-BS minimum coupling loss. However, there are certain site-engineering solutions that can be used. These techniques are addressed in TR 25.942 [5]  NOTE 2: The table above assumes that two operating bands, where the frequency ranges would be overlapping, are not deployed in the same geographical area. For such a case of operation with overlapping frequency arrangements in the same geographical area, special co-existence requirements may apply that are not covered by the 3GPP specifications. | | | | | |

## 12 Output intermodulation

The output intermodulation requirement is a measure of the ability of the repeater to inhibit the generation of intermodulation products signals created by the presence of an interfering signal reaching the repeater via the output port.

The output intermodulation level is the power of the intermodulation products when a WCDMA modulated interference signal is injected into the output port at a level of 30 dB lower than that of the wanted signal. The frequency of the interference signal shall be 5 MHz, 10 MHz and 15 MHz offset from the wanted signal, but within the frequency band allocated for UTRA FDD downlink as specified in subclause 4.1.

The requirement is applicable for downlink signals.

### 12.1 Minimum requirement

The output intermodulation level shall not exceed the out of band emission or the spurious emission requirements of section 9.1 and 9.2.

# 13 Adjacent Channel Rejection Ratio (ACRR)

## 13.1 Definitions and applicability

Adjacent Channel Rejection Ratio (ACRR) is the ratio of the RRC weighted gain per carrier of the repeater in the pass band to the RRC weighted gain of the repeater on an adjacent channel.

The requirement shall apply to the Uplink and Downlink of Repeater where the donor link is maintained via antennas (over the air Repeater).

## 13.2 Minimum Requirements

In normal conditions the ACRR shall be higher than the value specified in the Table 13.1.

Table 13.1: Repeater ACRR

|  |  |  |
| --- | --- | --- |
| Repeater maximum output power as in 9.1.1 | Channel offset from the centre frequency of the first or last 5 MHz channel within the pass band. | ACRR limit |
| P  31 dBm | 5 MHz | 33dB |
| P  31 dBm | 10 MHz | 33dB |
| P < 31 dBm | 5 MHz | 20dB |
| P < 31 dBm | 10 MHz | 20dB |

Annex A (informative):  
Change History

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| TSG | Doc | CR | R | Title | Cat | Curr | New | Work Item |
| RP-31 |  |  |  | Rel-7 version created; based on v6.4.0 |  |  | 7.0.0 |  |
| RP-31 | RP-060100 | 0042 | 2 | Introduction of operating band III to IX requirements in 25.106 | B | 6.3.0 | 7.0.0 | TEI7 |
| RP-31 | RP-060110 | 0043 |  | Correction of spurious emissions for coexistence with GSM900 in same geographic area | F | 6.3.0 | 7.0.0 | RInImp-UMTS900 |
| RP-33 | RP-060520 | 0046 | 1 | Clean up of Spurious emissions | A | 7.0.0 | 7.1.0 | TEI5 |
| RP-33 | RP-060521 | 0049 | 1 | New UTRA Repeater up-link spurious emissions limits for co-existence/co-location with TDD | A | 7.0.0 | 7.1.0 | TEI5 |
| RP-34 | RP-060811 | 0052 | 1 | Corrections to input intermodulation | A | 7.1.0 | 7.2.0 | TEI5 |
| RP-36 | RP-070370 | 0056 |  | Category B spurious emission limits for UTRA Repeater | A | 7.2.0 | 7.3.0 | TEI4 |
| RP-36 | RP-070373 | 0057 |  | Introduction of operating band X into the repeater specification | B | 7.2.0 | 7.3.0 | TEI7 |
| RP-39 | RP-080126 | 0058 |  | Introduction of UMTS1500 requirements | B | 7.3.0 | 8.0.0 | RInImp8-UMTS1500 |
|  |  |  |  | Minor correction to CR implementation |  | 8.0.0 | 8.0.1 |  |
|  |  |  |  | Update of history table |  | 8.0.1 | 8.0.2 |  |
| RP-42 | RP-080943 | 60 | 1 | Introduction of operating band unwanted emission | F | 8.0.2 | 8.1.0 | TEI8 |
| RP-45 | RP-080819 | 61 |  | Introduction of band XII, XIII, XIV | F | 8.1.0 | 8.2.0 | TEI8 |
| RP-45 | RP-080819 | 62 |  | CR to limit the scope to FDD only to 25.106 | F | 8.1.0 | 8.2.0 | TEI8 |
| RP-46 | RP-091277 | 063 |  | Corrections on additional spectrum emission limits for Bands XII, XIII, XIV | F | 8.2.0 |  | TEI8 |
|  |  |  |  | Automatic upgrade from previous Release |  | 8.3.0 | 9.0.0 | TEI9 |
| RP-49 | RP-100925 | 064 |  | Introduction of operating band XIX, XX and XXI and correction of band XI | F | 9.0.0 | 9.1.0 | TEI9 |
| RP-49 | RP-100913 | 067 | 1 | RCDE for 64QAM modulated codes for FDD Repeater | A | 9.0.0 | 9.1.0 | TEI7 |
| RP-50 | RP-101336 | 072 |  | Protection of cdma and E-UTRA bands | A | 9.1.0 | 9.2.0 | TEI8 |
| RP-50 | RP-101337 | 074 |  | Removal of brackets | A | 9.1.0 | 9.2.0 | TEI8 |
| RP-50 | RP-101347 | 068 |  | Remove test settings for unwanted emissions from core spec | F | 9.1.0 | 9.2.0 | TEI9 |
| RP-50 | RP-101347 | 069 |  | Corrections to the symbols and abbreviations clause related to DTT requirement | F | 9.1.0 | 9.2.0 | TEI9 |
| RP-50 | RP-101347 | 070 |  | Co-existence with services in adjacent frequency bands | F | 9.1.0 | 9.2.0 | TEI9 |
| RP-51 | RP-110352 | 0075 | - | Inclusion of E-UTRA TDD text to co-location on 25.106 | F | 9.2.0 | 10.0.0 | TEI10 |
| RP-55 | RP-120303 | 078 | 1 | Correction on the table of Regional requirements | F | 10.0.0 | 10.1.0 | TEI10 |
| RP-55 | RP-120303 | 079 | 1 | Introduction of operating frequency band XXII | B | 10.0.0 | 10.1.0 | TEI10 |
| RP-55 | RP-120303 | 080 | 1 | Introduction of operating frequency band XXV and protection limits towards E-UTRA Band 23 | B | 10.0.0 | 10.1.0 | TEI10 |
| RP-56 | RP-120783 | 082 | 2 | Update of the Definition clause with repeaters operating band definition and introduction of minor editorial changes for better alignment with BS core specification | F | 10.1.0 | 10.2.0 | TEI10 |
| RP-56 | RP-120765 | 085 |  | Additional spurious emissions requirements for PHS | A | 10.1.0 | 10.2.0 | TEI8 |
| RP-57 | RP-121313 | 088 | 2 | Introduction of missing Spurious Emission limits and Input Intermodulation requirements towards E-UTRA FDD Band 24 | F | 10.2.0 | 10.3.0 | TEI10 |
| SP-57 | - | - | - | Update to Rel-11 version (MCC) | - | 10.3.0 | 11.0.0 | - |
| RP-58 | RP-121867 | 095 |  | Introduction of Spurious Emission limits and Input Intermodulation requirements towards missing UTRA and E-UTRA TDD frequency bands | A | 11.0.0 | 11.1.0 | TEI10 |
| RP-58 | RP-121867 | 096 |  | Introduction of a Note on non deployment of operating bands with overlapping frequency ranges for the tables for Input Intermodulation requirements | A | 11.0.0 | 11.1.0 | TEI10 |
| RP-58 | RP-121858 | 097 |  | Modifications of frequency ranges for E-UTRA Band 6, 18, 19 in the Tables for Spurious Emission limits and Input Intermodulation requirements | A | 11.0.0 | 11.1.0 | RInImp9-UMTSLTE800 |
| RP-58 | RP-121867 | 100 |  | The special cases for protection of UTRA Band III and Band X in co-existence and co-location with UTRA Repeaters | A | 11.0.0 | 11.1.0 | TEI10 |
| SP-65 | - | - | - | Update to Rel-12 version (MCC) | - | 11.1.0 | 12.0.0 |  |
| RP-66 | RP-142154 | 103 |  | Update with regard to operating bands of TS25.106 | F | 12.0.0 | 12.1.0 | LTE\_UTRA\_SDL\_BandL-Core, LTE450\_Brazil-Core, LTE\_WCS\_band-Core, LTE\_DL\_FDD700-Core, LTE\_APAC700-Core, LTE\_e850\_LB-Core,E850\_UB-Core |
| SP-70 | - | - | - | Update to Rel-13 version (MCC) | - | 12.1.0 | 13.0.0 |  |
| RP-75 | - | - | - | Update to Rel-14 version (MCC) | - | 13.0.0 | 14.0.0 |  |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2018-06 | SA#80 | - | - | - | - | Update to Rel-15 version (MCC) | 15.0.0 |
| 2020-06 | SA#88 | - | - | - | - | Update to Rel-16 version (MCC) | **16.0.0** |