3GPP TS 25.111 V16.0.0 (2020-06)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Radio Access Network;

Location Measurement Unit (LMU) performance specification;

User Equipment (UE) positioning in UTRAN

(Release 16)



The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP..  
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.  
This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

Keywords

UMTS, radio

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword [4](#__RefHeading___Toc518918281)

Introduction [5](#__RefHeading___Toc518918282)

1 Scope [6](#__RefHeading___Toc518918283)

2 References [6](#__RefHeading___Toc518918284)

3 Definitions and abbreviations [6](#__RefHeading___Toc518918285)

3.1 Definitions [6](#__RefHeading___Toc518918286)

3.2 Abbreviations [6](#__RefHeading___Toc518918287)

4 General [7](#__RefHeading___Toc518918288)

4.1 Main concepts [7](#__RefHeading___Toc518918289)

4.2 LMU Classes [7](#__RefHeading___Toc518918290)

4.3 U-TDOA architecture [7](#__RefHeading___Toc518918291)

5 LMU radio characteristics [8](#__RefHeading___Toc518918292)

5.1 Frequency bands [8](#__RefHeading___Toc518918293)

5.2 Channel arrangement [8](#__RefHeading___Toc518918294)

5.3 Reference sensitivity level [9](#__RefHeading___Toc518918295)

5.4 Dynamic range [9](#__RefHeading___Toc518918296)

5.5 Adjacent Channel Selectivity (ACS) [9](#__RefHeading___Toc518918297)

5.6 Blocking characteristics [9](#__RefHeading___Toc518918298)

5.7 Intermodulation characteristics [13](#__RefHeading___Toc518918299)

5.8 Spurious emissions [14](#__RefHeading___Toc518918300)

6 LMU measurement requirements [15](#__RefHeading___Toc518918301)

6.1 General [15](#__RefHeading___Toc518918302)

6.2 RRC States supported [15](#__RefHeading___Toc518918303)

6.3 Maximum response times [15](#__RefHeading___Toc518918304)

6.4 Nominal time accuracy [15](#__RefHeading___Toc518918305)

6.5 Multipath scenarios [16](#__RefHeading___Toc518918306)

6.6 Moving scenario [16](#__RefHeading___Toc518918307)

6.7 Cross correlation [16](#__RefHeading___Toc518918308)

Annex A (informative): Change history [17](#__RefHeading___Toc518918309)

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

Y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# Introduction

In order to ensure correctness and consistency of the specifications (i.e., technical specifications and technical reports) under responsibility of the Technical Specification Groups (TSG) of the 3rd Generation Partnership Project (3GPP), clear, manageable and efficient mechanisms are necessary to handle version control, change control, document updating, distribution and management.

Also, the fact that the specifications are/will be implemented by industry almost in parallel with the writing of them requires strict and fast procedures for handling of changes to the specifications.

It is very important that the changes that are brought into the standard, from the past, at present and in the future, are well documented and controlled, so that technical consistency and backwards tracing are ensured.

The 3GPP TSGs, and their sub-groups together with the Support Team are responsible for the technical content and consistency of the specifications whilst the Support Team alone is responsible for the proper management of the entire documentation, including specifications, meeting documents, administrative information and information exchange with other bodies.

# 1 Scope

The present document establishes the Location Measurement Unit (LMU) minimum RF characteristics of the FDD mode of UTRA.

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TS 25.104: “Base Station (BS) radio transmission and reception (FDD)”.

[2] 3GPP TS 45.004: “Modulation”.

[3] 3GPP TS 25.141: “Base Station (BS) conformance testing (FDD)”.

[4] 3GPP TR 25.942: “Radio Frequency (RF) system scenarios”.

[5] 3GPP TR 21.905: “Vocabulary for 3GPP Specifications”.

# 3 Definitions and abbreviations

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in TR 21.905 [5] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in TR 21.905 [5].

**Mean power:** When applied to a W-CDMA modulated signal this is the power (transmitted or received) in a bandwidth of at least (1+  times the chip rate of the radio access mode. The period of measurement shall be at least one timeslot unless otherwise stated.

NOTE: The roll-off factor  is defined in clause 6.8.1 of [1].

## 3.2 Abbreviations

For the purposes of the present document, the abbreviations given in TR 21.905 [5] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in TR 21.905 [5].

ACS Adjacent Channel Selectivity

BS Base Station

BER Bit Error Ratio

BLER Block Error Ratio

CW Continuous Wave (unmodulated signal)

DL Down Link (forward link)

FDD Frequency Division Duplexing

GSM Global System for Mobile Communications

LMU Location Measurement Unit

UARFCN UTRA Absolute Radio Frequency Channel Number

UE User Equipment

UL Up Link (reverse link)

U-TDOA Uplink Time Difference Of Arrival

WCDMA Wideband Code Division Multiple Access

# 4 General

## 4.1 Main concepts

The LMU is either located as a separate unit in an existing network or typically located at Node B or BTS sites. Therefore the LMU radio requirements assume that the isolation between the LMU and any other network to be protected is to be at least 30dB.

The communication link between LMU and Stand-Alone SMLC is not a radio interface over the air. Requirements in this document therefore do not cover the situation when the LMU is transmitting over the air on this interface between LMU and Stand-Alone SMLC.

## 4.2 LMU Classes

The requirements in this specification apply to Wide Area LMUs and Medium Range LMUs.

Wide Area LMUs are characterised by requirements derived from Macro Cell scenarios with an LMU to UE minimum coupling loss equal to 70 dB.

Medium Range LMUs are characterised by requirements derived from Micro Cell scenarios with an LMU to UE minimum coupling loss equal to 53 dB.

For Pico Cell scenarios, the location of the BS provides sufficient accuracy; therefore, a Local Area LMUs class is not specified.

## 4.3 U-TDOA architecture

A sample architecture is shown in Figure 3.1 depicting the LMU’s relationship with other network elements. The LMU is typically located at the Node B. The LMUs communicate with the SMLC that distributes UTDOA reference data from the reference LMU to other cooperating LMUs when performing UE positioning.



Figure 3.1: Example of UTDOA deployment

# 5 LMU radio characteristics

An LMU performs BS receiver functions to obtain reference data for use at a cooperating LMU. The following clause describes the required LMU radio characteristics when performing these functions.

## 5.1 Frequency bands

a) The LMU is designed to operate in the following bands:

Table 4.1: Frequency bands

|  |  |
| --- | --- |
| Operating Band | UL Frequencies UE transmit, LMU receive |
| I | 1920 – 1980 MHz |
| II | 1850 -1910 MHz |
| III | 1710-1785 MHz |
| IV | 1710-1755 MHz |
| V | 824 – 849MHz |
| VI | 830-840 MHz |
| VII | 2500 – 2570 MHz |
| VIII | 880 – 915 MHz |
| IX | 1749.9 – 1784.9 MHz |
| X | 1710-1770 MHz |

b) Deployment in other frequency bands is not precluded

## 5.2 Channel arrangement

The channel arrangement shall be as specified in Section 5.4 of [1].

## 5.3 Reference sensitivity level

Using the reference measurement channel specification in TS 25.104 Annex A [1], the reference sensitivity level and performance of the LMU shall be as specified in Table 4.2.

Table 4.2: LMU reference sensitivity levels

|  |  |  |  |
| --- | --- | --- | --- |
| LMU Class | Reference measurement channel data rate | LMU sensitivity level (dBm) | BER |
| Wide Area LMU | 12.2 kbps | -121 | BER shall not exceed 0.001 |
| Medium Range LMU | 12.2 kbps | -111 | BER shall not exceed 0.001 |

## 5.4 Dynamic range

Receiver dynamic range is the receiver ability to handle a rise of interference in the reception frequency channel. The receiver shall fulfil a specified BER requirement for a specified sensitivity degradation of the wanted signal in the presence of an interfering AWGN signal in the same reception frequency channel.

The BER shall not exceed 0.001 for the parameters specified in Table 4.3.

Table 4.3: Dynamic range

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Level Wide Area LMU | Level Medium Range LMU | Unit |
| Reference measurement channel data rate | 12.2 | 12.2 | kbps |
| Wanted signal mean power | -91 | -81 | dBm |
| Interfering AWGN signal | -73 | -63 | dBm/3.84 MHz |

## 5.5 Adjacent Channel Selectivity (ACS)

Adjacent channel selectivity (ACS) is a measure of the LMU receiver ability to receive a wanted signal at its assigned channel frequency in the presence of an adjacent channel signal at a given frequency offset from the centre frequency of the assigned channel. ACS is the ratio of the LMU receiver filter attenuation on the assigned channel frequency to the receiver filter attenuation on the adjacent channel(s).

The interference signal is offset from the wanted signal by the frequency offset Fuw. The interference signal shall be a W-CDMA signal as specified in Annex C of TS 25.104 [1].

The BER shall not exceed 0.001 for the parameters specified in Table 4.4.

Table 4.4: LMU Adjacent channel selectivity

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Level Wide Area LMU | Level  Medium Range LMU | Unit |
| Data rate | 12.2 | 12.2 | kbps |
| Wanted signal mean power | -115 | -105 | dBm |
| Interfering signal mean power | -52 | -42 | dBm |
| Fuw offset (Modulated) | 5 | 5 | MHz |

## 5.6 Blocking characteristics

The blocking characteristics are a measure of the LMU receiver ability to receive a wanted signal at its assigned channel frequency in the presence of an unwanted interferer on frequencies other than those of the adjacent channels. The performance as specified in Table 4.5-4.10 shall be met with a wanted and an interfering signal coupled to the LMU antenna input using the following parameters for the blocking and narrowband blocking requirements:

Table 4.5: Blocking performance requirement for Wide Area LMU

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Operating Band | Center Frequency of Interfering Signal | Interfering Signal mean power | Wanted Signal mean power | Minimum Offset of Interfering Signal | Type of Interfering Signal |
| I | 1920 – 1980 MHz | -40 dBm | -115 dBm | 10 MHz | WCDMA signal \* |
| 1900 – 1920 MHz  1980 – 2000 MHz | -40 dBm | -115 dBm | 10 MHz | WCDMA signal \* |
| 1 MHz -1900 MHz  2000 MHz – 12750 MHz | -15 dBm | -115 dBm |  | CW carrier |
| II | 1850 – 1910 MHz | -40 dBm | -115 dBm | 10 MHz | WCDMA signal \* |
| 1830 – 1850 MHz  1910 – 1930 MHz | -40 dBm | -115 dBm | 10 MHz | WCDMA signal \* |
| 1 MHz – 1830 MHz  1930 MHz – 12750 MHz | -15 dBm | -115 dBm |  | CW carrier |
| III | 1710 – 1785 MHz | -40 dBm | -115 dBm | 10 MHz | WCDMA signal \* |
| 1690 – 1710 MHz  1785 – 1805 MHz | -40 dBm | -115 dBm | 10 MHz | WCDMA signal \* |
| 1 MHz – 1690 MHz  1805 MHz – 12750 MHz | -15 dBm | -115 dBm |  | CW carrier |
| IV | 1710 – 1755 MHz | -40 dBm | -115 dBm | 10 MHz | WCDMA signal \* |
| 1690 – 1710 MHz  1755 – 1775 MHz | -40 dBm | -115 dBm | 10 MHz | WCDMA signal \* |
| 1 MHz – 1690 MHz  1775 MHz – 12750 MHz | -15 dBm | -115 dBm |  | CW carrier |
| V | 824-849 MHz | -40 dBm | -115 dBm | 10 MHz | WCDMA signal \* |
| 804-824 MHz  849-869 MHz | -40 dBm | -115 dBm | 10 MHz | WCDMA signal \* |
| 1 MHz – 804 MHz  869 MHz – 12750 MHz | -15 dBm | -115 dBm |  | CW carrier |
| VI | 810 – 830 MHz  840 – 860 MHz | -40 dBm | -115 dBm | 10 MHz | WCDMA signal \* |
| 1 MHz – 810 MHz  860 MHz – 12750 MHz | -15 dBm | -115 dBm |  | CW carrier |
| VII | 2500 – 2570 MHz | -40 dBm | -115 dBm | 10 MHz | WCDMA signal \* |
|  | 2480 – 2500 MHz  2570 – 2590 MHz | -40 dBm | -115 dBm | 10 MHz | WCDMA signal \* |
|  | 1 MHz -2480 MHz  2590 MHz – 12750 MHz | -15 dBm | -115 dBm |  | CW carrier |
| VIII | 880 – 915 MHz | -40 dBm | -115 dBm | 10 MHz | WCDMA signal \* |
|  | 860 – 880 MHz  915 – 925 MHz | -40 dBm | -115 dBm | 10 MHz | WCDMA signal \* |
|  | 1 MHz -860 MHz  925 MHz – 12750 MHz | -15 dBm | -115 dBm |  | CW carrier |
| IX | 1749.9 – 1784.9 MHz | -40 dBm | -115 dBm | 10 MHz | WCDMA signal \* |
| 1729.9 – 1749.9 MHz  1784.9 – 1804.9 MHz | -40 dBm | -115 dBm | 10 MHz | WCDMA signal \* |
| 1 MHz – 1729.9 MHz  1804.9 MHz – 12750 MHz | -15 dBm | -115 dBm |  | CW carrier |
| X | 1710 – 1770 MHz | -40 dBm | -115 dBm | 10 MHz | WCDMA signal \* |
|  | 1690 – 1710 MHz  1770 – 1790 MHz | -40 dBm | -115 dBm | 10 MHz | WCDMA signal \* |
|  | 1 MHz – 1690 MHz  1790 MHz – 12750 MHz | -15 dBm | -115 dBm |  | CW carrier |
| NOTE \*: The characteristics of the W-CDMA interference signal are specified in Annex C of [1] | | | | | |

Table 4.6: Blocking performance requirement for the Medium range LMU

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Operating Band | Center Frequency of Interfering Signal | Interfering Signal mean power | Wanted Signal mean power | Minimum Offset of Interfering Signal | Type of Interfering Signal |
| I | 1920 – 1980 MHz | -35 dBm | -105 dBm | 10 MHz | WCDMA signal \* |
| 1900 – 1920 MHz  1980 – 2000 MHz | -35 dBm | -105 dBm | 10 MHz | WCDMA signal \* |
| 1 MHz -1900 MHz  2000 MHz – 12750 MHz | -15 dBm | -105 dBm |  | CW carrier |
| II | 1850 – 1910 MHz | -35 dBm | -105 dBm | 10 MHz | WCDMA signal \* |
| 1830 – 1850 MHz  1910 – 1930 MHz | -35 dBm | -105 dBm | 10 MHz | WCDMA signal \* |
| 1 MHz – 1830 MHz  1930 MHz – 12750 MHz | -15 dBm | -105 dBm |  | CW carrier |
| III | 1710 – 1785 MHz | -35 dBm | -105 dBm | 10 MHz | WCDMA signal \* |
| 1690 – 1710 MHz  1785 – 1805 MHz | -35 dBm | -105 dBm | 10 MHz | WCDMA signal \* |
| 1 MHz – 1690 MHz  1805 MHz – 12750 MHz | -15 dBm | -105 dBm |  | CW carrier |
| IV | 1710 – 1755 MHz | -35 dBm | -105 dBm | 10 MHz | WCDMA signal \* |
| 1690 – 1710 MHz  1755 – 1775 MHz | -35 dBm | -105 dBm | 10 MHz | WCDMA signal \* |
| 1 MHz – 1690 MHz  1775 MHz – 12750 MHz | -15 dBm | -105 dBm |  | CW carrier |
| V | 824-849 MHz | -35 dBm | -105 dBm | 10 MHz | WCDMA signal \* |
| 804-824 MHz  849-869 MHz | -35 dBm | -105 dBm | 10 MHz | WCDMA signal \* |
| 1 MHz – 804 MHz  869 MHz – 12750 MHz | -15 dBm | -105 dBm |  | CW carrier |
| VI | 810 – 830 MHz  840 – 860 MHz | -35 dBm | -105 dBm | 10 MHz | WCDMA signal \* |
| 1 MHz – 810 MHz  860 MHz – 12750 MHz | -15 dBm | -105 dBm |  | CW carrier |
| VII | 2500 – 2570 MHz | -35 dBm | -105 dBm | 10 MHz | WCDMA signal \* |
| 2480 – 2500 MHz  2570 – 2590 MHz | -35 dBm | -105 dBm | 10 MHz | WCDMA signal \* |
| 1 MHz -2480 MHz  2590 MHz – 12750 MHz | -15 dBm | -105 dBm |  | CW carrier |
| VIII | 880 – 915 MHz | -35 dBm | -105 dBm | 10 MHz | WCDMA signal \* |
| 860 – 880 MHz  915 – 925 MHz | -35 dBm | -105 dBm | 10 MHz | WCDMA signal \* |
| 1 MHz -860 MHz  925 MHz – 12750 MHz | -15 dBm | -105 dBm |  | CW carrier |
| IX | 1749.9 – 1784.9 MHz | -35 dBm | -105 dBm | 10 MHz | WCDMA signal \* |
| 1729.9 – 1749.9 MHz  1784.9 – 1804.9 MHz | -35 dBm | -105 dBm | 10 MHz | WCDMA signal \* |
| 1 MHz – 1729.9 MHz  1804.9 MHz – 12750 MHz | -15 dBm | -105 dBm |  | CW carrier |
| X | 1710 – 1770 MHz | -35 dBm | -105 dBm | 10 MHz | WCDMA signal \* |
|  | 1690 – 1710 MHz  1770 – 1790 MHz | -35 dBm | -105 dBm | 10 MHz | WCDMA signal \* |
|  | 1 MHz – 1690 MHz  1790 MHz – 12750 MHz | -15 dBm | -105 dBm |  | CW carrier |
| NOTE \*: The characteristics of the W-CDMA interference signal are specified in Annex C of [1] | | | | | |

Table 4.7: Blocking performance requirement (narrowband) for the Wide Area LMU

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Operating Band | Center Frequency of Interfering Signal | Interfering Signal mean power | Wanted Signal mean power | Minimum Offset of Interfering Signal | Type of Interfering Signal |
| II | 1850 – 1910 MHz | - 47 dBm | -115 dBm | 2.7 MHz | GMSK modulated\* |
| III | 1710 – 1785 MHz | - 47 dBm | -115 dBm | 2.8 MHz | GMSK modulated\* |
| IV | 1710 – 1755 MHz | - 47 dBm | -115 dBm | 2.7 MHz | GMSK modulated\* |
| V | 824 – 849 MHz | - 47 dBm | -115 dBm | 2.7 MHz | GMSK modulated\* |
| VIII | 880 – 915 MHz | - 47 dBm | -115 dBm | 2.8 MHz | GMSK modulated\* |
| X | 1710 – 1770 MHz | - 47 dBm | -115 dBm | 2.7 MHz | GMSK modulated\* |
| NOTE \*: GMSK modulation as defined in TS 45.004 [2]. | | | | | |

Table 4.8: Narrowband blocking performance requirement for the Medium Range LMU

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Operating Band | Center Frequency of Interfering Signal | Interfering Signal mean power | Wanted Signal mean power | Minimum Offset of Interfering Signal | Type of Interfering Signal |
| II | 1850 – 1910 MHz | - 42 dBm | -105 dBm | 2.7 MHz | GMSK modulated\* |
| III | 1710 – 1785 MHz | - 42 dBm | -105 dBm | 2.8 MHz | GMSK modulated\* |
| IV | 1710 – 1755 MHz | - 42 dBm | -105 dBm | 2.7 MHz | GMSK modulated\* |
| V | 824 – 849 MHz | - 42 dBm | -105 dBm | 2.7 MHz | GMSK modulated\* |
| VIII | 880 – 915 MHz | - 42 dBm | -105 dBm | 2.8 MHz | GMSK modulated\* |
| X | 1710 – 1770 MHz | - 42 dBm | -105 dBm | 2.7 MHz | GMSK modulated\* |
| NOTE \*: GMSK modulation as defined in TS 45.004 [2]. | | | | | |

Additional blocking requirements shall be applied for the protection of the LMU receiver in the presence of GSM900, DCS1800, PCS1900, GSM850, UTRA TDD, and UTRA FDD in bands I to X.

Table 4.9: Additional blocking performance requirement for Wide Area LMU.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Co-located BS type | Center Frequency of Interfering Signal | Interfering Signal mean power | Wanted Signal mean power | Type of Interfering Signal |
| Macro GSM900 | 921 – 960 MHz | +16 dBm | -115 dBm | CW carrier |
| Macro DCS1800 | 1805 – 1880 MHz | +16 dBm | -115 dBm | CW carrier |
| Macro PCS1900 | 1930 – 1990 MHz | +16 dBm | -115 dBm | CW carrier |
| Macro GSM850 | 869 – 894 MHz | +16 dBm | -115 dBm | CW carrier |
| WA UTRA-FDD Band I | 2110 – 2170 MHz | +16 dBm | -115 dBm | CW carrier |
| WA UTRA-FDD Band II | 1930 – 1990 MHz | +16 dBm | -115 dBm | CW carrier |
| WA UTRA-FDD Band III | 1805 – 1880 MHz | +16 dBm | -115 dBm | CW carrier |
| WA UTRA-FDD Band IV | 2110 – 2155 MHz | +16 dBm | -115 dBm | CW carrier |
| WA UTRA-FDD Band V | 869 – 894 MHz | +16 dBm | -115 dBm | CW carrier |
| WA UTRA-FDD Band VI | 875 – 885 MHz | +16 dBm | -115 dBm | CW carrier |
| WA UTRA-FDD Band VII | 2620 – 2690 MHz | +16 dBm | -115 dBm | CW carrier |
| WA UTRA-FDD Band VIII | 925 – 960 MHz | +16 dBm | -115 dBm | CW carrier |
| WA UTRA-FDD Band IX | 1844.9 – 1879.9 MHz | +16 dBm | -115 dBm | CW carrier |
| WA UTRA-FDD Band X | 2110 – 2170 MHz | +16 dBm | -115 dBm | CW carrier |

Table 4.10: Additional blocking performance requirements for the LMU

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Co-located BS type | Center Frequency of Interfering Signal | Interfering Signal mean power | Wanted Signal mean power | Type of Interfering Signal |
| Micro GSM900 | 921 – 960 MHz | -3 dBm | -105 dBm | CW carrier |
| Micro DCS1800 | 1805 – 1880 MHz | +5 dBm | -105 dBm | CW carrier |
| Micro PCS1900 | 1930 – 1990 MHz | +5 dBm | -105 dBm | CW carrier |
| Micro GSM850 | 869 – 894 MHz | -3 dBm | -105 dBm | CW carrier |
| MR UTRA-FDD Band I | 2110 – 2170 MHz | +8 dBm | -105 dBm | CW carrier |
| MR UTRA-FDD Band II | 1930 – 1990 MHz | +8 dBm | -105 dBm | CW carrier |
| MR UTRA-FDD Band III | 1805 – 1880 MHz | +8 dBm | -105 dBm | CW carrier |
| MR UTRA-FDD Band IV | 2110 – 2155 MHz | +8 dBm | -105 dBm | CW carrier |
| MR UTRA-FDD Band V | 869 – 894 MHz | +8 dBm | -105 dBm | CW carrier |
| MR UTRA-FDD Band VI | 875 – 885 MHz | +8 dBm | -105 dBm | CW carrier |
| MR UTRA-FDD Band VII | 2620 – 2690 MHz | +8 dBm | -105 dBm | CW carrier |
| MR UTRA-FDD Band VIII | 925 – 960 MHz | +8 dBm | -105 dBm | CW carrier |
| MR UTRA-FDD Band IX | 1844.9 – 1879.9 MHz | +8 dBm | -105 dBm | CW carrier |
| MR UTRA-FDD Band X | 2110 – 2170 MHz | +8 dBm | -105 dBm | CW carrier |

An additional blocking requirement may be applied for the protection of the LMU receivers when UTRA TDD is co-located with an LMU.

The current state-of-the-art technology does not allow a single generic solution for co-location with UTRA-TDD on adjacent frequencies for 30dB BS-BS minimum coupling loss.

However, there are certain site-engineering solutions that can be used in these cases. These techniques are addressed in TR 25.942 [4].

For an LMU, the static reference performance as specified in clause 5.3 should be met with a wanted and an interfering signal coupled to BS antenna input using the parameters in Table 4.11.

Table 4.11: Blocking performance requirement for a Wide Area LMU when co-located with UTRA TDD BS in other bands.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Co-located BS type | Center Frequency of Interfering Signal | Interfering Signal mean power | Wanted Signal mean power | Type of Interfering Signal |
| Wide Area TDD | 2585 – 2620 MHz | +16 dBm | -115 dBm | CW carrier |

## 5.7 Intermodulation characteristics

Third and higher order mixing of the two interfering RF signals can produce an interfering signal in the band of the desired channel. Intermodulation response rejection is a measure of the capability of the receiver to receive a wanted signal on its assigned channel frequency in the presence of two or more interfering signals which have a specific frequency relationship to the wanted signal.

The static reference performance as specified in clause 5.3 shall be met for a LMU when the following signals are coupled to LMU antenna input:

- A wanted signal at the assigned channel frequency with a mean power of ‑115 dBm.

- Two interfering signals with the following parameters.

Table 4.12: Intermodulation performance requirement (Wide Area LMU)

|  |  |  |  |
| --- | --- | --- | --- |
| Operating band | Interfering Signal mean power | Offset | Type of Interfering Signal |
| All bands | - 48 dBm | 10 MHz | CW signal |
| - 48 dBm | 20 MHz | WCDMA signal \* |
| Note\*: The characteristics of the W-CDMA interference signal are specified in Annex C of [1] | | | |

Table 4.13: Narrowband intermodulation performance requirement (Wide Area LMU)

|  |  |  |  |
| --- | --- | --- | --- |
| Operating band | Interfering Signal mean power | Offset | Type of Interfering Signal |
| II, III, IV, V, VIII, X | - 47 dBm | 3.5 MHz | CW signal |
| - 47 dBm | 5.9 MHz | GMSK modulated\* |
| \* GMSK as defined in TS45.004 [2] | | | |

The static reference performance as specified in clause 5.3 shall be met for a Medium Range LMU when the following signals are coupled to LMU antenna input:

- A wanted signal at the assigned channel frequency with a mean power of ‑105 dBm.

- Two interfering signals with the following parameters.

Table 4.14: Intermodulation performance requirement (Medium Range LMU)

|  |  |  |  |
| --- | --- | --- | --- |
| Operating band | Interfering Signal mean power | Offset | Type of Interfering Signal |
| All bands | - 44 dBm | 10 MHz | CW signal |
| - 44 dBm | 20 MHz | WCDMA signal \* |
| Note\*: The characteristics of the W-CDMA interference signal are specified in Annex C of [1] | | | |

Table 4.15: Narrowband intermodulation performance requirement (Medium Range LMU)

|  |  |  |  |
| --- | --- | --- | --- |
| Operating band | Interfering Signal mean power | Offset | Type of Interfering Signal |
| II, III, IV, V, VIII, X | - 43 dBm | 3.5 MHz | CW signal |
| - 43 dBm | 5.9 MHz | GMSK modulated\* |
| \* GMSK as defined in TS45.004 [2] | | | |

## 5.8 Spurious emissions

The spurious emissions power is the power of emissions generated or amplified in a receiver that appear at the LMU antenna connector.

The power of any spurious emission shall not exceed:

Table 4.16: General LMU spurious emission requirement

|  |  |  |  |
| --- | --- | --- | --- |
| Band | Maximum level | Measurement Bandwidth | Note |
| 30MHz – 1 GHz | -57 dBm | 100 kHz |  |
| 1 GHz – 12.75 GHz | -47 dBm | 1 MHz | With the exception of frequencies between 12.5 MHz below the first carrier frequency and 12.5 MHz above the last carrier frequency used by the LMU. |

In addition the following requirements shall be applied for the protection of UE, MS, and Node B, BS of the same and other systems, where the power of any spurious emission shall not exceed the limits:

Table 4.17: Additional LMU Spurious emissions limits

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Operating Band | Band | Maximum level | Measurement Bandwidth | Note |
| I | 1920 – 1980 MHz | -78 dBm | 3.84 MHz |  |
| II | 1850 – 1910 MHz | -78 dBm | 3.84 MHz |  |
| III | 1710 – 1785 MHz | -78 dBm | 3.84 MHz |  |
| IV | 1710 – 1755 MHz | -78 dBm | 3.84 MHz |  |
| V | 824 – 849 MHz | -78 dBm | 3.84 MHz |  |
| VI | 815 – 850 MHz | -78 dBm | 3.84 MHz |  |
| VII | 2500 – 2570 MHz | -78 dBm | 3.84 MHz |  |
| VIII | 880 – 915 MHz | -78 dBm | 3.84 MHz |  |
| IX | 1749.9 – 1784.9 MHz | -78 dBm | 3.84 MHz |  |
| X | 1710 – 1770 MHz | -78 dBm | 3.84 MHz |  |

In addition, the requirement in Table 4.18 may be applied to geographic areas in which both UTRA-TDD and UTRA-FDD are deployed.

Table 4.18: Additional spurious emission requirements for the TDD bands

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Operating Band | Band | Maximum level | Measurement Bandwidth | Note |
| I | 1900 – 1920 MHz  2010 – 2025 MHz | -78 dBm | 3.84 MHz | Not applicable in Japan |
| 2010 – 2025 MHz | -52 dBm | 1MHz | Applicable in Japan |
| VI, IX | 2010 – 2025 MHz | -52 dBm | 1MHz |  |

# 6 LMU measurement requirements

## 6.1 General

All tests at specified detection levels require that the LMU detection threshold be set such that the false alarm rate is at or below 5 % when no signal is present (noise only).

## 6.2 RRC States supported

UTDOA positioning technique does work in CELL\_DCH and CELL\_FACH state, not in URA\_PCH nor CELL\_PCH state.

## 6.3 Maximum response times

1) The maximum time for a Master LMU to establish a reference signal shall be, after the data capture has started, less than 5 seconds.

2) The maximum time for the distribution of the reference signal to another LMU involved in the positioning shall be less than 3 seconds.

3) The maximum time of detection of the time of arrival in an LMU given the reference signal shall be less than 15 seconds.

## 6.4 Nominal time accuracy

Nominal Time Accuracy requirement verifies the difference between the detected time of arrival and the real time of arrival.

In an AWGN environment with no fading or multi-paths, the standard deviation of the timing error of the LMU shall be less than 30 ns when the signal presence is correctly detected.

## 6.5 Multipath scenarios

The purpose of the test case is to verify the LMU receiver’s performance in multipath.

For the 12.2 kbps reference measurement channel specified in 3GPP TS 25.104 Annex A [1], and with Rx diversity (using both diversity paths), the LMU shall be capable of detecting the earliest path, for at least 90 % of the location attempts, at the levels in Table 5.1.

Nominal time accuracy for multipath fading scenarios includes an additional chip duration of 260 nanoseconds over that in Section 5.4.

Table 5.1: Multipath detection level

|  |  |  |
| --- | --- | --- |
| **Propagation condition** | **Detection level: Signal to Noise level in (dB)** | **Note** |
| Static (AWGN) | -51.2 dB | NOTE 1 |
| Multipath fading Case 1 | -47.2dB | NOTE 2 |
| Multipath fading Case 2 | - 43.8 dB | NOTE 2 |
| Multipath fading Case 3 | - 41.9 dB | NOTE 2 |
| Multipath fading Case 4 | - 39.8 dB | NOTE 2 |

NOTE 1: Static propagation condition is described in 3GPP TS 25.104 Annex B.1 [1].

NOTE 2: Multipath-fading case 1-4 is described in 3GPP TS 25.104 Annex B.2 [1].

## 6.6 Moving scenario

The purpose of the test case is to verify the LMU receiver’s performance to Doppler shift.

In an AWGN environment with no fading or multi-paths, and at a speed of 250km/h, the detectability of the LMU shall be degraded by no more than 1.5 dB.

## 6.7 Cross correlation

The ability of the LMU to detect a weak terminal signal in the presence of a strong other terminal is covered in Section 5.5 when the other terminal interference is modelled as AWGN.

Annex A (informative):  
Change history

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | | |
| **Date** | **TSG** | **Doc.** | **CR** | **Rev** | **Subject/Comment** | **Cat** | **Old** | **New** |
| 2005-08 |  |  |  |  | Initial version created |  |  | 0.1.0 |
| 2007-11 |  |  |  |  | Incorporate simulation results and synchronize with TS.104 |  | 0.1.0 | 1.0.0 |
| 2007-12 | 38 | RP-071015 |  |  | Approved version at RAN TSG # 38 |  | 1.0.0 | 7.0.0 |
| 2008-03 | 39 | RP-080122 | 1 |  | Correcting multipath detection level in LMU performance specification | F | 7.0.0 | 7.1.0 |
| 2008-12 | SP-42 |  |  |  | Upgraded unchanged from Rel-7 |  |  | 8.0.0 |
| 2009-12 | SP-46 |  |  |  | Upgraded unchanged from Rel-8 |  |  | 9.0.0 |
|  | SP-51 |  |  |  | Upgraded unchanged from Rel-9 |  | 9.0.0 | 10.0.0 |
| 2012-09 | SP-57 | - | - | - | Update to Rel-11 version (MCC) |  | 10.0.0 | 11.0.0 |
| 2014-09 | SP-65 | - | - | - | Update to Rel-12 version (MCC) |  | 11.0.0 | 12.0.0 |
| 2016-01 | SP-70 | - | - | - | Update to Rel-13 version (MCC) |  | 12.0.0 | 13.0.0 |
| 2017-03 | RP-75 | - | - | - | Update to Rel-14 version (MCC) |  | 13.0.0 | 14.0.0 |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2018-06 | SA#80 | - | - | - | - | Update to Rel-15 version (MCC) | 15.0.0 |
| 2020-06 | SA#88 | - | - | - | - | Update to Rel-16 version (MCC) | **16.0.0** |