

3GPP TS 25.212 V16.0.0 (2020-07)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Radio Access Network;

Multiplexing and channel coding (FDD)

(Release 16)

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.  
The present document has not been subject to any approval process by the 3GPPOrganisational Partners and shall not be implemented.  
This Specification is provided for future development work within 3GPPonly. The Organisational Partners accept no liability for any use of this Specification.  
Specifications and reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organisational Partners' Publications Offices.

Keywords

UMTS, radio, mux

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword [9](#__RefHeading___Toc492492005)

1 Scope [10](#__RefHeading___Toc492492006)

2 References [10](#__RefHeading___Toc492492007)

3 Definitions, symbols and abbreviations [10](#__RefHeading___Toc492492008)

3.1 Definitions [10](#__RefHeading___Toc492492009)

3.2 Symbols [12](#__RefHeading___Toc492492010)

3.3 Abbreviations [13](#__RefHeading___Toc492492011)

4 Multiplexing, channel coding and interleaving [14](#__RefHeading___Toc492492012)

4.1 General [14](#__RefHeading___Toc492492013)

4.2 General coding/multiplexing of TrCHs [14](#__RefHeading___Toc492492014)

4.2.0 Transport channel concatenation [19](#__RefHeading___Toc492492015)

4.2.1 CRC attachment [19](#__RefHeading___Toc492492016)

4.2.1.1 CRC Calculation [19](#__RefHeading___Toc492492017)

4.2.1.2 Relation between input and output of the CRC attachment block [20](#__RefHeading___Toc492492018)

4.2.2 Transport block concatenation and code block segmentation [20](#__RefHeading___Toc492492019)

4.2.2.1 Concatenation of transport blocks [20](#__RefHeading___Toc492492020)

4.2.2.2 Code block segmentation [20](#__RefHeading___Toc492492021)

4.2.3 Channel coding [21](#__RefHeading___Toc492492022)

4.2.3.1 Convolutional coding [22](#__RefHeading___Toc492492023)

4.2.3.2 Turbo coding [23](#__RefHeading___Toc492492024)

4.2.3.2.1 Turbo coder [23](#__RefHeading___Toc492492025)

4.2.3.2.2 Trellis termination for Turbo coder [23](#__RefHeading___Toc492492026)

4.2.3.2.3 Turbo code internal interleaver [24](#__RefHeading___Toc492492027)

4.2.3.3 Concatenation of encoded blocks [27](#__RefHeading___Toc492492028)

4.2.4 Radio frame size equalisation [27](#__RefHeading___Toc492492029)

4.2.5 1st interleaving [28](#__RefHeading___Toc492492030)

4.2.5.1 Void [28](#__RefHeading___Toc492492031)

4.2.5.2 1st interleaver operation [28](#__RefHeading___Toc492492032)

4.2.5.3 Relation between input and output of 1st interleaving in uplink [29](#__RefHeading___Toc492492033)

4.2.5.4 Relation between input and output of 1st interleaving in downlink [29](#__RefHeading___Toc492492034)

4.2.6 Radio frame segmentation [29](#__RefHeading___Toc492492035)

4.2.6.1 Relation between input and output of the radio frame segmentation block in uplink [30](#__RefHeading___Toc492492036)

4.2.6.2 Relation between input and output of the radio frame segmentation block in downlink [30](#__RefHeading___Toc492492037)

4.2.7 Rate matching [30](#__RefHeading___Toc492492038)

4.2.7.1 Determination of rate matching parameters in uplink [32](#__RefHeading___Toc492492039)

4.2.7.1.1 Determination of SF and number of PhCHs needed [32](#__RefHeading___Toc492492040)

4.2.7.2 Determination of rate matching parameters in downlink [35](#__RefHeading___Toc492492041)

4.2.7.2.1 Determination of rate matching parameters for fixed positions of TrCHs [35](#__RefHeading___Toc492492042)

4.2.7.2.1A Determination of rate matching parameters for pseudo-flexible positions of TrCHs [37](#__RefHeading___Toc492492043)

4.2.7.2.2 Determination of rate matching parameters for flexible positions of TrCHs [37](#__RefHeading___Toc492492044)

4.2.7.3 Bit separation and collection in uplink [39](#__RefHeading___Toc492492045)

4.2.7.3.1 Bit separation [41](#__RefHeading___Toc492492046)

4.2.7.3.2 Bit collection [41](#__RefHeading___Toc492492047)

4.2.7.4 Bit separation and collection in downlink [42](#__RefHeading___Toc492492048)

4.2.7.4.1 Bit separation [43](#__RefHeading___Toc492492049)

4.2.7.4.2 Bit collection [43](#__RefHeading___Toc492492050)

4.2.7.5 Rate matching pattern determination [44](#__RefHeading___Toc492492051)

4.2.8 TrCH multiplexing [45](#__RefHeading___Toc492492052)

4.2.9 Insertion of discontinuous transmission (DTX) indication bits [45](#__RefHeading___Toc492492053)

4.2.9.1 1st insertion of DTX indication bits [45](#__RefHeading___Toc492492054)

4.2.9.2 2nd insertion of DTX indication bits [46](#__RefHeading___Toc492492055)

4.2.10 Physical channel segmentation [47](#__RefHeading___Toc492492056)

4.2.10.1 Relation between input and output of the physical segmentation block in uplink [47](#__RefHeading___Toc492492057)

4.2.10.2 Relation between input and output of the physical segmentation block in downlink [47](#__RefHeading___Toc492492058)

4.2.11 2nd interleaving [47](#__RefHeading___Toc492492059)

4.2.11.1 2nd interleaving for Secondary CCPCH with 16QAM [48](#__RefHeading___Toc492492060)

4.2.12 Physical channel mapping [49](#__RefHeading___Toc492492061)

4.2.12.1 Uplink [49](#__RefHeading___Toc492492062)

4.2.12.1.1 UL\_DPCH\_10ms\_Mode is not configured by higher layers, or, no compressed-mode transmission gap overlaps with the first radio frame in the 20ms CI [49](#__RefHeading___Toc492492063)

4.2.12.1.2 UL\_DPCH\_10ms\_Mode is configured by higher layers, and, a compressed-mode transmission gap overlaps with the first radio frame in 20ms CI [49](#__RefHeading___Toc492492064)

4.2.12.2 Downlink [50](#__RefHeading___Toc492492065)

4.2.13 Restrictions on different types of CCTrCHs [50](#__RefHeading___Toc492492066)

4.2.13.1 Uplink Dedicated channel (DCH) [50](#__RefHeading___Toc492492067)

4.2.13.2 Random Access Channel (RACH) [51](#__RefHeading___Toc492492068)

4.2.13.3 Void [51](#__RefHeading___Toc492492069)

4.2.13.4 Downlink Dedicated Channel (DCH) [51](#__RefHeading___Toc492492070)

4.2.13.5 Void [51](#__RefHeading___Toc492492071)

4.2.13.6 Broadcast channel (BCH) [51](#__RefHeading___Toc492492072)

4.2.13.7 Forward access and paging channels (FACH and PCH) [51](#__RefHeading___Toc492492073)

4.2.13.8 High Speed Downlink Shared Channel (HS-DSCH) associated with a DCH [51](#__RefHeading___Toc492492074)

4.2.13.9 Enhanced Dedicated Channel (E-DCH) [52](#__RefHeading___Toc492492075)

4.2.14 Multiplexing of different transport channels into one CCTrCH, and mapping of one CCTrCH onto physical channels [52](#__RefHeading___Toc492492076)

4.2.14.1 Allowed CCTrCH combinations for one UE [53](#__RefHeading___Toc492492077)

4.2.14.1.1 Allowed CCTrCH combinations on the uplink [53](#__RefHeading___Toc492492078)

4.2.14.1.2 Allowed CCTrCH combinations on the downlink [53](#__RefHeading___Toc492492079)

4.3 Transport format detection [53](#__RefHeading___Toc492492080)

4.3.1 Blind transport format detection [54](#__RefHeading___Toc492492081)

4.3.1A Single transport format detection [54](#__RefHeading___Toc492492082)

4.3.2 Transport format detection based on TFCI [54](#__RefHeading___Toc492492083)

4.3.3 Coding of Transport-Format-Combination Indicator (TFCI) [55](#__RefHeading___Toc492492084)

4.3.4 Void [56](#__RefHeading___Toc492492085)

4.3.5 Mapping of TFCI words [56](#__RefHeading___Toc492492086)

4.3.5.1 Mapping of TFCI word in normal mode in downlink, and in uplink when uplink DPCCH slot format is not 5 [56](#__RefHeading___Toc492492087)

4.3.5.1A Mapping of TFCI word in normal mode in uplink when uplink DPCCH slot format is 5 [56](#__RefHeading___Toc492492088)

4.3.5.1.1 Mapping of TFCI bits for Secondary CCPCH with 16QAM [56](#__RefHeading___Toc492492089)

4.3.5.2 Mapping of TFCI word in compressed mode [56](#__RefHeading___Toc492492090)

4.3.5.2.1 Uplink compressed mode [57](#__RefHeading___Toc492492091)

4.3.5.2.2 Downlink compressed mode [57](#__RefHeading___Toc492492092)

4.3A Mapping of DL FET ACK/NACK bits [58](#__RefHeading___Toc492492093)

4.4 Compressed mode [59](#__RefHeading___Toc492492094)

4.4.1 Frame structure in the uplink [59](#__RefHeading___Toc492492095)

4.4.2 Frame structure types in the downlink [59](#__RefHeading___Toc492492096)

4.4.2A Frame structure in the downlink for F-DPCH [60](#__RefHeading___Toc492492097)

4.4.2B Frame structure in the downlink for F-TPICH [60](#__RefHeading___Toc492492098)

4.4.3 Transmission time reduction method [60](#__RefHeading___Toc492492099)

4.4.3.1 Void [60](#__RefHeading___Toc492492100)

4.4.3.2 Compressed mode by reducing the spreading factor by 2 [60](#__RefHeading___Toc492492101)

4.4.3.3 Compressed mode by higher layer scheduling [60](#__RefHeading___Toc492492102)

4.4.4 Transmission gap position [61](#__RefHeading___Toc492492103)

4.4.5 Transmission gap position for E‑DCH [62](#__RefHeading___Toc492492104)

4.4.5.1 E‑DPDCH Transmission Gap Position during Initial Transmissions [62](#__RefHeading___Toc492492105)

4.4.5.2 E‑DPDCH Transmission Gap Position during Retransmissions [63](#__RefHeading___Toc492492106)

4.4.5.3 E‑DPCCH Transmission Gap Position [63](#__RefHeading___Toc492492107)

4.5 Coding for HS-DSCH [63](#__RefHeading___Toc492492108)

4.5.1 CRC attachment for HS-DSCH [64](#__RefHeading___Toc492492109)

4.5.1.1 CRC attachment method 1 for HS-DSCH [64](#__RefHeading___Toc492492110)

4.5.1.2 CRC attachment method 2 for HS-DSCH [65](#__RefHeading___Toc492492111)

4.5.1A Bit scrambling for HS-DSCH [65](#__RefHeading___Toc492492112)

4.5.2 Code block segmentation for HS-DSCH [65](#__RefHeading___Toc492492113)

4.5.3 Channel coding for HS-DSCH [66](#__RefHeading___Toc492492114)

4.5.4 Hybrid ARQ for HS-DSCH [66](#__RefHeading___Toc492492115)

4.5.4.1 HARQ bit separation [66](#__RefHeading___Toc492492116)

4.5.4.2 HARQ First Rate Matching Stage [66](#__RefHeading___Toc492492117)

4.5.4.3 HARQ Second Rate Matching Stage [67](#__RefHeading___Toc492492118)

4.5.4.4 HARQ bit collection [68](#__RefHeading___Toc492492119)

4.5.5 Physical channel segmentation for HS-DSCH [68](#__RefHeading___Toc492492120)

4.5.6 Interleaving for HS-DSCH [69](#__RefHeading___Toc492492121)

4.5.7 Constellation re-arrangement for 16 QAM and 64QAM [69](#__RefHeading___Toc492492122)

4.5.8 Physical channel mapping for HS-DSCH [70](#__RefHeading___Toc492492123)

4.6 Coding for HS-SCCH type 1 [70](#__RefHeading___Toc492492124)

4.6.1 Overview [70](#__RefHeading___Toc492492125)

4.6.2 HS-SCCH information field mapping [72](#__RefHeading___Toc492492126)

4.6.2.1 Redundancy and constellation version coding [72](#__RefHeading___Toc492492127)

4.6.2.2 Modulation scheme mapping [73](#__RefHeading___Toc492492128)

4.6.2.3 Channelization code-set mapping [73](#__RefHeading___Toc492492129)

4.6.2.4 UE identity mapping [74](#__RefHeading___Toc492492130)

4.6.2.5 HARQ process identifier mapping [74](#__RefHeading___Toc492492131)

4.6.2.6 Transport block size index mapping [74](#__RefHeading___Toc492492132)

4.6.3 Multiplexing of HS-SCCH information [74](#__RefHeading___Toc492492133)

4.6.4 CRC attachment for HS-SCCH [74](#__RefHeading___Toc492492134)

4.6.5 Channel coding for HS-SCCH [75](#__RefHeading___Toc492492135)

4.6.6 Rate matching for HS-SCCH [75](#__RefHeading___Toc492492136)

4.6.7 UE specific masking for HS-SCCH [75](#__RefHeading___Toc492492137)

4.6.8 Physical channel mapping for HS-SCCH [75](#__RefHeading___Toc492492138)

4.6A Coding for HS-SCCH type 2 [75](#__RefHeading___Toc492492139)

4.6A.1 Overview [75](#__RefHeading___Toc492492140)

4.6A.2 HS-SCCH Type 2 information field mapping [76](#__RefHeading___Toc492492141)

4.6A.2.1 The first transmission [76](#__RefHeading___Toc492492142)

4.6A.2.2 The second and the third transmissions [77](#__RefHeading___Toc492492143)

4.6A.2.2.1 Special Information mapping [77](#__RefHeading___Toc492492144)

4.6A.2.2.1.1 Transport-block size information mapping [77](#__RefHeading___Toc492492145)

4.6A.2.2.1.2 Pointer to the previous transmission mapping [77](#__RefHeading___Toc492492146)

4.6A.2.2.1.3 Second or third transmission mapping [77](#__RefHeading___Toc492492147)

4.6A.2.2.2 Redundancy and Constellation Version mapping [78](#__RefHeading___Toc492492148)

4.6A.2.2.3 Modulation scheme mapping [78](#__RefHeading___Toc492492149)

4.6A.2.2.4 Channelization code-set mapping [78](#__RefHeading___Toc492492150)

4.6A.2.2.5 UE identity mapping [78](#__RefHeading___Toc492492151)

4.6A.3 Multiplexing of HS-SCCH Type 2 information [78](#__RefHeading___Toc492492152)

4.6A.4 CRC attachment for HS-SCCH Type 2 [78](#__RefHeading___Toc492492153)

4.6A.5 Channel coding for HS-SCCH Type 2 [78](#__RefHeading___Toc492492154)

4.6A.6 Rate matching for HS-SCCH Type 2 [78](#__RefHeading___Toc492492155)

4.6A.7 UE specific masking for HS-SCCH Type 2 [78](#__RefHeading___Toc492492156)

4.6A.8 Physical channel mapping for HS-SCCH Type 2 [78](#__RefHeading___Toc492492157)

4.6B Coding for HS-SCCH type 3 [79](#__RefHeading___Toc492492158)

4.6B.1 Overview [79](#__RefHeading___Toc492492159)

4.6B.2 HS-SCCH type 3 information field mapping [80](#__RefHeading___Toc492492160)

4.6B.2.1 Redundancy and constellation version coding [80](#__RefHeading___Toc492492161)

4.6B.2.2 Modulation scheme and number of transport blocks mapping [81](#__RefHeading___Toc492492162)

4.6B.2.3 Channelization code-set mapping [81](#__RefHeading___Toc492492163)

4.6B.2.4 UE identity mapping [82](#__RefHeading___Toc492492164)

4.6B.2.5 HARQ process identifier mapping [82](#__RefHeading___Toc492492165)

4.6B.2.6 Transport block size index mapping [82](#__RefHeading___Toc492492166)

4.6B.2.7 Precoding Weight Information mapping [82](#__RefHeading___Toc492492167)

4.6B.3 Multiplexing of HS-SCCH type 3 information [83](#__RefHeading___Toc492492168)

4.6B.4 CRC attachment for HS-SCCH type 3 [83](#__RefHeading___Toc492492169)

4.6B.5 Channel coding for HS-SCCH type 3 [84](#__RefHeading___Toc492492170)

4.6B.6 Rate matching for HS-SCCH type 3 [84](#__RefHeading___Toc492492171)

4.6B.7 UE specific masking for HS-SCCH type 3 [84](#__RefHeading___Toc492492172)

4.6B.8 Physical channel mapping for HS-SCCH type 3 [84](#__RefHeading___Toc492492173)

4.6C Coding for HS-SCCH orders [85](#__RefHeading___Toc492492174)

4.6C.1 Overview [85](#__RefHeading___Toc492492175)

4.6C.2 HS-SCCH Order information field mapping in the CELL\_DCH state [85](#__RefHeading___Toc492492176)

4.6C.2.1 Order type mapping [85](#__RefHeading___Toc492492177)

4.6C.2.2 Order mapping [85](#__RefHeading___Toc492492178)

4.6C.2.2.1 Orders for activation and deactivation of DTX, DRX and HS-SCCH-less operation and for HS-DSCH serving cell change [85](#__RefHeading___Toc492492179)

4.6C.2.2.2 Orders for activation and deactivation of Secondary serving HS-DSCH cells and Secondary uplink frequency [86](#__RefHeading___Toc492492180)

4.6C.2.2.3 Orders for Switching between Uplink Closed Loop Transmit Diversity Activation states [93](#__RefHeading___Toc492492181)

4.6C.2.2.4 Orders for activating and de-activating demodulation common pilots (D-CPICH) when the UE is configured in MIMO mode with four transmit antennas [93](#__RefHeading___Toc492492182)

4.6C.2.2.5 Orders for switching the E-DCH TTI, and for start/stop a simplified HS-SCCH type 1 transmission interval [94](#__RefHeading___Toc492492183)

4.6C.2.3 UE identity mapping [95](#__RefHeading___Toc492492184)

4.6C.3 HS-SCCH order information field mapping in the CELL\_FACH and CELL\_PCH states [95](#__RefHeading___Toc492492185)

4.6C.3.1 Order type mapping [95](#__RefHeading___Toc492492186)

4.6C.3.2 Order mapping [95](#__RefHeading___Toc492492187)

4.6C.3.2.1 Orders for network triggered HS-DPCCH transmission [95](#__RefHeading___Toc492492188)

4.6C.3.2.2 Orders for HS-DSCH reception during CELL\_FACH HS-SCCH DRX operation [95](#__RefHeading___Toc492492189)

4.6D Coding for HS-SCCH type 4 [95](#__RefHeading___Toc492492190)

4.6D.1 Overview [95](#__RefHeading___Toc492492191)

4.6D.2 HS-SCCH type 4 information field mapping [96](#__RefHeading___Toc492492192)

4.6D.2.1 Redundancy and constellation version coding [96](#__RefHeading___Toc492492193)

4.6D.2.2 Modulation scheme and number of transport blocks mapping [97](#__RefHeading___Toc492492194)

4.6D.2.3 Channelization code-set mapping [98](#__RefHeading___Toc492492195)

4.6D.2.4 UE identity mapping [99](#__RefHeading___Toc492492196)

4.6D.2.5 HARQ process identifier mapping [99](#__RefHeading___Toc492492197)

4.6D.2.6 Transport block size index mapping [99](#__RefHeading___Toc492492198)

4.6D.2.7 Precoding Weight Information mapping [100](#__RefHeading___Toc492492199)

4.6D.3 Multiplexing of HS-SCCH type 4 information [101](#__RefHeading___Toc492492200)

4.6D.4 CRC attachment for HS-SCCH type 4 [102](#__RefHeading___Toc492492201)

4.6D.5 Channel coding for HS-SCCH type 4 [102](#__RefHeading___Toc492492202)

4.6D.6 Rate matching for HS-SCCH type 4 [102](#__RefHeading___Toc492492203)

4.6D.7 UE specific masking for HS-SCCH type 4 [103](#__RefHeading___Toc492492204)

4.6D.8 Physical channel mapping for HS-SCCH type 4 [103](#__RefHeading___Toc492492205)

4.7 Coding for HS-DPCCH [103](#__RefHeading___Toc492492206)

4.7.1 Overview [103](#__RefHeading___Toc492492207)

4.7.2 Channel coding for HS-DPCCH when the UE is not configured in MIMO mode and not configured in MIMO mode with four transmit antennas in the serving HS-DSCH cell and Secondary\_Cell\_Enabled is 0 or 1 and Secondary\_Cell\_Active is 0 [108](#__RefHeading___Toc492492208)

4.7.2.1 Channel coding for HS-DPCCH HARQ-ACK [108](#__RefHeading___Toc492492209)

4.7.2.2 Channel coding for HS-DPCCH channel quality indication [108](#__RefHeading___Toc492492210)

4.7.3 Channel coding for HS-DPCCH when the UE is configured in MIMO mode in the serving HS-DSCH cell and Secondary\_Cell\_Enabled is 0 [109](#__RefHeading___Toc492492211)

4.7.3.1 Channel coding for HS-DPCCH HARQ-ACK [109](#__RefHeading___Toc492492212)

4.7.3.2 Channel coding for HS-DPCCH composite precoding control indication and channel quality indication [110](#__RefHeading___Toc492492213)

4.7.3.2.1 Bit mapping of Type A channel quality indication [110](#__RefHeading___Toc492492214)

4.7.3.2.2 Bit mapping of Type B channel quality indication [110](#__RefHeading___Toc492492215)

4.7.3.2.3 Bit mapping of precoding control indication [110](#__RefHeading___Toc492492216)

4.7.3.2.4 Composite precoding control indication and channel quality indication bits [110](#__RefHeading___Toc492492217)

4.7.3.2.5 Block encoding of composite precoding control indication and channel quality indication bits [111](#__RefHeading___Toc492492218)

4.7.3A Channel coding for HS-DPCCH when the UE is not configured in MIMO mode in any cell and Secondary\_Cell\_Enabled is 1 and Secondary\_Cell\_Active is 1 [112](#__RefHeading___Toc492492219)

4.7.3A.1 Channel coding for the composite HS-DPCCH HARQ-ACK [112](#__RefHeading___Toc492492220)

4.7.3A.2 Channel coding for HS-DPCCH composite channel quality indication [113](#__RefHeading___Toc492492221)

4.7.3A.2.1 Composite channel quality indication bits [113](#__RefHeading___Toc492492222)

4.7.3A.2.2 Block encoding of composite channel quality indication bits [114](#__RefHeading___Toc492492223)

4.7.3B Channel coding for HS-DPCCH when Secondary\_Cell\_Enabled is at least 3 or when the UE is configured in MIMO mode in at least one cell and Secondary\_Cell\_Enabled is greater than 0 [114](#__RefHeading___Toc492492224)

4.7.3B.1 Channel coding for the composite HS-DPCCH HARQ-ACK [114](#__RefHeading___Toc492492225)

4.7.3B.2 Channel coding for HS-DPCCH composite precoding control indication and channel quality indication [116](#__RefHeading___Toc492492226)

4.7.3C Channel coding for HS-DPCCH when the UE is not configured in MIMO mode in any cell and Secondary\_Cell\_Enabled is 2 [116](#__RefHeading___Toc492492227)

4.7.3C.1 Channel coding for the composite HS-DPCCH HARQ-ACK [116](#__RefHeading___Toc492492228)

4.7.3C.2 Channel coding for HS-DPCCH channel quality indication [117](#__RefHeading___Toc492492229)

4.7.3D Channel coding for HS-DPCCH when the UE is configured in Multiflow mode [117](#__RefHeading___Toc492492230)

4.7.3D.1 Channel coding for the composite HS-DPCCH HARQ-ACK [117](#__RefHeading___Toc492492231)

4.7.3D.2 Channel coding for HS-DPCCH channel quality indication [118](#__RefHeading___Toc492492232)

4.7.3E Channel coding for HS-DPCCH when the UE is configured in MIMO mode with 4 transmit antennas [118](#__RefHeading___Toc492492233)

4.7.3E.1 Channel coding for HS-DPCCH when the UE is configured in MIMO mode with four transmit antennas and Secondary\_Cell\_Enabled is 0 [118](#__RefHeading___Toc492492234)

4.7.3E.1.1 Channel coding for HS-DPCCH HARQ-ACK [118](#__RefHeading___Toc492492235)

4.7.3E.1.2 Channel coding for HS-DPCCH composite number of transport blocks preferred, precoding control indication and channel quality indication [120](#__RefHeading___Toc492492236)

4.7.3E.2 Channel coding for HS-DPCCH when the UE is configured in MIMO mode with four transmit antennas in any cell and Secondary\_Cell\_Enabled is 1 [122](#__RefHeading___Toc492492237)

4.7.3E.2.1 Channel coding for the composite HS-DPCCH HARQ-ACK [122](#__RefHeading___Toc492492238)

4.7.3E.2.2 Channel coding for HS-DPCCH composite number of transport blocks preferred, precoding control indication and channel quality indication [123](#__RefHeading___Toc492492239)

4.7.3E.3 Channel coding for HS-DPCCH when the UE is configured in MIMO mode with four transmit antennas in any cell and Secondary\_Cell\_Enabled is 2 [123](#__RefHeading___Toc492492240)

4.7.3E.3.1 Channel coding for the composite HS-DPCCH HARQ-ACK [123](#__RefHeading___Toc492492241)

4.7.3E.3.2 Channel coding for HS-DPCCH composite number of transport blocks preferred, precoding control indication and channel quality indication [123](#__RefHeading___Toc492492242)

4.7.3E.4 Channel coding for HS-DPCCH when the UE is configured in MIMO mode with four transmit antennas in any cell and Secondary\_Cell\_Enabled is 3 [123](#__RefHeading___Toc492492243)

4.7.3E.4.1 Channel coding for the composite HS-DPCCH HARQ-ACK [124](#__RefHeading___Toc492492244)

4.7.3E.4.2 Channel coding for HS-DPCCH composite number of transport blocks preferred, precoding control indication and channel quality indication [124](#__RefHeading___Toc492492245)

4.7.4 Physical channel mapping for HS-DPCCH [124](#__RefHeading___Toc492492246)

4.7.4.1 Physical Channel mapping for HS-DPCCH HARQ-ACK [124](#__RefHeading___Toc492492247)

4.7.4.2 Physical Channel mapping for HS-DPCCH PCI/CQI [127](#__RefHeading___Toc492492248)

4.7.4.3 Physical Channel mapping for HS-DPCCH HARQ-ACK and PCI/CQI when the UE is configured in Multiflow mode [132](#__RefHeading___Toc492492249)

4.7.4.3.1 Physical Channel mapping for HS-DPCCH HARQ-ACK and PCI/CQI when the UE is configured with one serving and one assisting serving HS-DSCH cell [132](#__RefHeading___Toc492492250)

4.7.4.3.2 Physical Channel mapping for HS-DPCCH HARQ-ACK and PCI/CQI when the UE is configured with two serving and one assisting serving or one serving and two assisting serving HS-DSCH cells [133](#__RefHeading___Toc492492251)

4.7.4.3.3 Physical Channel mapping for HS-DPCCH HARQ-ACK and PCI/CQI when the UE is configured with two serving and two assisting serving HS-DSCH cells [135](#__RefHeading___Toc492492252)

4.7.4.3.4 Physical Channel mapping for HS-DPCCH HARQ-ACK and PCI/CQI when the UE is configured with three serving and one assisting serving HS-DSCH cells or one serving and three assisting serving HS-DSCH cells [135](#__RefHeading___Toc492492253)

4.7.4.4 Physical Channel mapping for HS-DPCCH when the UE is configured in MIMO mode with four transmit antennas in at least one cell [137](#__RefHeading___Toc492492254)

4.7.4.4.1 Physical Channel mapping for HS-DPCCH HARQ-ACK [137](#__RefHeading___Toc492492255)

4.7.4.4.2 Physical Channel mapping for HS-DPCCH NTBP/PCI/CQI [138](#__RefHeading___Toc492492256)

4.8 Coding for E‑DCH [140](#__RefHeading___Toc492492257)

4.8.1 CRC attachment for E-DCH [142](#__RefHeading___Toc492492258)

4.8.2 Code block segmentation for E-DCH [142](#__RefHeading___Toc492492259)

4.8.3 Channel coding for E-DCH [142](#__RefHeading___Toc492492260)

4.8.4 Physical layer HARQ functionality and rate matching for E-DCH [142](#__RefHeading___Toc492492261)

4.8.4.1 Determination of SF, modulation scheme and number of E-DPDCH PhCHs needed [142](#__RefHeading___Toc492492262)

4.8.4.1A Determination of SF, modulation scheme and number of S-E-DPDCH PhCHs needed [144](#__RefHeading___Toc492492263)

4.8.4.2 HARQ bit separation [145](#__RefHeading___Toc492492264)

4.8.4.3 HARQ Rate Matching Stage [145](#__RefHeading___Toc492492265)

4.8.4.4 HARQ bit collection [146](#__RefHeading___Toc492492266)

4.8.5 Physical channel segmentation for E‑DCH [146](#__RefHeading___Toc492492267)

4.8.6 Interleaving for E‑DCH [146](#__RefHeading___Toc492492268)

4.8.7 Physical channel mapping for E‑DCH [147](#__RefHeading___Toc492492269)

4.9 Coding for E‑DPCCH [147](#__RefHeading___Toc492492270)

4.9.1 Overview [148](#__RefHeading___Toc492492271)

4.9.2 E‑DPCCH information field mapping [148](#__RefHeading___Toc492492272)

4.9.2.1 Information field mapping of E‑TFCI [148](#__RefHeading___Toc492492273)

4.9.2.2 Information field mapping of retransmission sequence number [148](#__RefHeading___Toc492492274)

4.9.2.3 Information field mapping of the "Happy" bit [149](#__RefHeading___Toc492492275)

4.9.3 Multiplexing of E‑DPCCH information [149](#__RefHeading___Toc492492276)

4.9.4 Channel coding for E‑DPCCH [149](#__RefHeading___Toc492492277)

4.9.5 Physical channel mapping for E‑DPCCH [149](#__RefHeading___Toc492492278)

4.9A Coding for S-E‑DPCCH [150](#__RefHeading___Toc492492279)

4.9A.1 Overview [150](#__RefHeading___Toc492492280)

4.9A.2 S-E‑DPCCH information field mapping [150](#__RefHeading___Toc492492281)

4.9A.2.1 Information field mapping of E‑TFCI [150](#__RefHeading___Toc492492282)

4.9A.2.2 Information field mapping of retransmission sequence number [150](#__RefHeading___Toc492492283)

4.9A.2.3 Information field mapping of the Spare bit [150](#__RefHeading___Toc492492284)

4.9A.3 Multiplexing of S-E‑DPCCH information [150](#__RefHeading___Toc492492285)

4.9A.4 Channel coding for S-E‑DPCCH [150](#__RefHeading___Toc492492286)

4.9A.5 Physical channel mapping for S-E‑DPCCH [150](#__RefHeading___Toc492492287)

4.10 Coding for E‑AGCH [150](#__RefHeading___Toc492492288)

4.10.1 Overview [150](#__RefHeading___Toc492492289)

4.10.1A E-AGCH information field mapping [151](#__RefHeading___Toc492492290)

4.10.1A.1 Information field mapping of the Absolute Grant Value [151](#__RefHeading___Toc492492291)

4.10.1A.2 Information field mapping of the Absolute Grant Scope [153](#__RefHeading___Toc492492292)

4.10.1B Multiplexing of E-AGCH information [153](#__RefHeading___Toc492492293)

4.10.2 CRC attachment for E‑AGCH [154](#__RefHeading___Toc492492294)

4.10.3 Channel coding for E‑AGCH [154](#__RefHeading___Toc492492295)

4.10.4 Rate matching for E‑AGCH [154](#__RefHeading___Toc492492296)

4.10.5 Physical channel mapping for E‑AGCH [154](#__RefHeading___Toc492492297)

4.10A Coding for E-ROCH [154](#__RefHeading___Toc492492298)

4.10A.1 Overview [154](#__RefHeading___Toc492492299)

4.10A.2 E-ROCH information field mapping [155](#__RefHeading___Toc492492300)

4.10A.2.1 Information field mapping of the S-ETFC Offset [155](#__RefHeading___Toc492492301)

4.10A.2.2 Information field mapping of the Rank Indication [156](#__RefHeading___Toc492492302)

4.10A.3 Multiplexing of E-ROCH information [156](#__RefHeading___Toc492492303)

4.10A.4 CRC attachment for E-ROCH [156](#__RefHeading___Toc492492304)

4.10A.5 Channel coding for E-ROCH [157](#__RefHeading___Toc492492305)

4.10A.6 Rate matching for E-ROCH [157](#__RefHeading___Toc492492306)

4.10A.7 Physical channel mapping for E-ROCH [157](#__RefHeading___Toc492492307)

4.11 Mapping for E‑RGCH Relative Grant [157](#__RefHeading___Toc492492308)

4.11.1 Overview [157](#__RefHeading___Toc492492309)

4.11.2 Relative Grant mapping [157](#__RefHeading___Toc492492310)

4.12 Mapping for E-HICH ACK/NACK [157](#__RefHeading___Toc492492311)

4.12.1 Overview [157](#__RefHeading___Toc492492312)

4.12.2 ACK/NACK mapping [157](#__RefHeading___Toc492492313)

Annex A (informative): Blind transport format detection [159](#__RefHeading___Toc492492314)

A.1 Blind transport format detection using fixed positions [159](#__RefHeading___Toc492492315)

A.1.1 Blind transport format detection using received power ratio [159](#__RefHeading___Toc492492316)

A.1.2 Blind transport format detection using CRC [159](#__RefHeading___Toc492492317)

A.2 Blind transport format detection using pseudo-flexible positions [161](#__RefHeading___Toc492492318)

Annex B (informative): Compressed mode idle lengths [162](#__RefHeading___Toc492492319)

B.1 Idle lengths for DL, UL and DL+UL compressed mode for DPCH [162](#__RefHeading___Toc492492320)

Annex C (informative): Change history [164](#__RefHeading___Toc492492321)

# Foreword

This Technical Specification (TS) has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# 1 Scope

The present document describes the characteristics of the Layer 1 multiplexing and channel coding in the FDD mode of UTRA.

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies.

[1] 3GPP TS 25.201: "Physical layer - General Description".

[2] 3GPP TS 25.211: "Physical channels and mapping of transport channels onto physical channels (FDD)".

[3] 3GPP TS 25.213: "Spreading and modulation (FDD)".

[4] 3GPP TS 25.214: "Physical layer procedures (FDD)".

[5] 3GPP TS 25.215: "Physical layer – Measurements (FDD)".

[6] 3GPP TS 25.221: "Physical channels and mapping of transport channels onto physical channels (TDD)".

[7] 3GPP TS 25.222: "Multiplexing and channel coding (TDD)".

[8] 3GPP TS 25.223: "Spreading and modulation (TDD)".

[9] 3GPP TS 25.224: "Physical layer procedures (TDD)".

[10] 3GPP TS 25.225: "Physical layer – Measurements (TDD)".

[11] 3GPP TS 25.302: "Services Provided by the Physical Layer".

[12] 3GPP TS 25.402: "Synchronization in UTRAN, Stage 2".

[13] 3GPP TS 25.331: "Radio Resource Control (RRC); Protocol Specification".

[14] ITU-T Recommendation X.691 (12/97) "Information technology - ASN.1 encoding rules: Specification of Packed Encoding Rules (PER)"

[15] 3GPP TS 25.306: "UE Radio Access capabilities".

[16] 3GPP TS 25.321: "Medium Access Control (MAC) protocol specification".

# 3 Definitions, symbols and abbreviations

## 3.1 Definitions

For the purposes of the present document, the following terms and definitions apply:

**Assisting secondary serving HS-DSCH Cell(s):** In addition to the serving HS-DSCH cell, a cell in the secondary downlink frequency, where the UE is configured to simultaneously monitor a HS-SCCH set and receive HS-DSCH if it is scheduled in that cell. There can be up to two assisting secondary serving HS-DSCH cells.

**Assisting serving HS-DSCH Cell:** In addition to the serving HS-DSCH cell, a cell in the same frequency, where the UE is configured to simultaneously monitor a HS-SCCH set and receive HS-DSCH if it is scheduled in that cell.

**Cell group**: A group of (one, two, or three) Multiflow mode cells that have the same CPICH timing. The cells that belong to a cell group are indicated by higher layers.

**DL FET:** DL FET refers to early termination of DL DPCH transmission upon receiving an acknowledgement message. In this context, a DL FET ACK/NACK message represents an acknowledge message sent on UL DPCCH for DL FET.

**DL\_DCH\_FET\_Config**: Higher layers signal this configuration parameter to indicate enhanced DCH physical layer configuration. The possible values are 0 and 1. The value 0 indicates Mode 0 configuration where DL transport channels concatenation and DL FET ACK/NACK signalling on UL are not configured. The value 1 indicates Mode 1 where DL transport channel concatenation and DL FET ACK/NACK signalling on UL are configured.

**MIMO mode:** This term refers to the downlink MIMO configuration with two transmit antennas

**MIMO mode with four transmit antennas:** This term refers to the downlink MIMO configuration with four transmit antennas

**Multiflow mode:** The UE is configured in Multiflow mode when it is configured with assisting serving HS-DSCH cell.

**Primary uplink frequency:** If a single uplink frequency is configured for the UE, then it is the primary uplink frequency. In case more than one uplink frequency is configured for the UE, then the primary uplink frequency is the frequency on which the E-DCH corresponding to the serving E-DCHcellassociated with the serving HS-DSCH cell is transmitted. The association between a pair of uplink and downlink frequencies is indicated by higher layers.

**Secondary uplink frequency:** A secondary uplink frequency is a frequency on which an E-DCH corresponding to a serving E-DCH cell associated with a secondary serving HS-DSCH cell is transmitted. The association between a pair of uplink and downlink frequencies is indicated by higher layers.

**TG:** Transmission Gap is consecutive empty slots that have been obtained with a transmission time reduction method. The transmission gap can be contained in one or two consecutive radio frames.

**TGL:** Transmission Gap Length is the number of consecutive empty slots that have been obtained with a transmission time reduction method. 0 *TGL* 14. The CFNs of the radio frames containing the first empty slot of the transmission gaps, the CFNs of the radio frames containing the last empty slot, the respective positions Nfirst and Nlast within these frames of the first and last empty slots of the transmission gaps, and the transmission gap lengths can be calculated with the compressed mode parameters described in [5].

**TrCH number:** The transport channel number identifies a TrCH in the context of L1. The L3 transport channel identity (TrCH ID) maps onto the L1 transport channel number. The mapping between the transport channel number and the TrCH ID is as follows: TrCH 1 corresponds to the TrCH with the lowest TrCH ID, TrCH 2 corresponds to the TrCH with the next lowest TrCH ID and so on.

**UL DPCH 10ms Mode**: When configured by higher layers for the TTI to be transmitted [16], UL DPCH follows physical channel procedures specific to this mode.UL DPCH 10ms Mode can only happen when DL\_DCH\_FET\_Config is configured.

**UL 20ms Compression Interval (CI):** A time interval of 20ms duration aligned to a 20ms TTI defined for UL DPCH physical layer procedures when DL\_DCH\_FET\_Config is configured by higher layers.

**1st secondary serving HS-DSCH cell**: If the UE is configured with two uplink frequencies, the 1st secondary serving HS-DSCH cell is the secondary serving HS-DSCH cell that is associated with the secondary uplink frequency. If the UE is configured with a single uplink frequency, the 1st secondary serving HS-DSCH cell is a secondary serving HS-DSCH cell whose index is indicated by higher layers.

**2nd secondary serving HS-DSCH cell**: If the UE is configured with more than two serving HS-DSCH cells, the 2nd secondary serving HS-DSCH cell is a secondary serving HS-DSCH cell whose index is indicated by higher layers.

**3rd secondary serving HS-DSCH cell**: If the UE is configured with more than three serving HS-DSCH cells, the 3rd secondary serving HS-DSCH cell is a secondary serving HS-DSCH cell whose index is indicated by higher layers.

**4th secondary serving HS-DSCH cell**: If the UE is configured with more than four serving HS-DSCH cells, the 4th secondary serving HS-DSCH cell is a secondary serving HS-DSCH cell whose index is indicated by higher layers.

**5th secondary serving HS-DSCH cell**: If the UE is configured with more than five serving HS-DSCH cells, the 5th secondary serving HS-DSCH cell is a secondary serving HS-DSCH cell whose index is indicated by higher layers.

**6th secondary serving HS-DSCH cell**: If the UE is configured with more than six serving HS-DSCH cells, the 6th secondary serving HS-DSCH cell is a secondary serving HS-DSCH cell whose index is indicated by higher layers.

**7th secondary serving HS-DSCH cell**: If the UE is configured with eight serving HS-DSCH cells, the 7th secondary serving HS-DSCH cell is a secondary serving HS-DSCH cell whose index is indicated by higher layers.

## 3.2 Symbols

For the purposes of the present document, the following symbols apply:

*x* round towards **, i.e. integer such that *x  x < x+*1

*x* round towards -**, i.e. integer such that *x-*1 *< x  x*

*x* absolute value of *x*

sgn(*x*)signum function, i.e. 

*Nfirst* The first slot in the *TG*, located in the first compressed radio frame if the TG spans two frames.

*Nlast* The last slot in the *TG*, located in the second compressed radio frame if the TG spans two frames.

*Ntr* Number of transmitted slots in a radio frame.

Unless otherwise is explicitly stated when the symbol is used, the meaning of the following symbols is:

** List of transport channels numbers *i1, i2, …, iB,* corresponding to downlink transport channels to be concatenated when DL\_DCH\_FET\_Config = 1.

*i* TrCH number

*j* TFC number

*k* Bit number

*l* TF number

*m* Transport block number

*ni* Radio frame number of TrCH *i*.

*p* PhCH number

r Code block number

*I* Number of TrCHs in a CCTrCH.

*Ci* Number of code blocks in one TTI of TrCH *i*.

*Fi* Number of radio frames in one TTI of TrCH *i,* except for uplink when UL\_DPCH\_10ms\_Mode is configured. In uplink, when UL\_DPCH\_10ms\_Mode is configured, *Fi* is the number of radio frames in the transmission time interval of TrCH *i* divided by 2*.*

*Mi* Number of transport blocks in one TTI of TrCH *i*.

*Ndata,j* Number of data bits that are available for the CCTrCH in a radio frame with TFC *j*.

** Number of data bits that are available for the CCTrCH in a compressed radio frame with TFC *j*.

*P* Number of PhCHs used for one CCTrCH.

*PL* Puncturing Limit for the uplink. Signalled from higher layers

*RMi* Rate Matching attribute for TrCH *i*. Signalled from higher layers, or determined as specified in clause 4.2.0.

Temporary variables, i.e. variables used in several (sub)clauses with different meaning.

x, X

y, Y

z, Z

## 3.3 Abbreviations

For the purposes of the present document, the following abbreviations apply:

ARQ Automatic Repeat Request

BCH Broadcast Channel

BER Bit Error Rate

BLER Block Error Rate

BS Base Station

CCPCH Common Control Physical Channel

CCTrCH Coded Composite Transport Channel

CFN Connection Frame Number

CLTD Closed Loop Transmit Diversity

CRC Cyclic Redundancy Check

DCH Dedicated Channel

DL Downlink (Forward link)

DPCCH Dedicated Physical Control Channel

DPCCH2 Dedicated Physical Control Channel 2

DPCH Dedicated Physical Channel

DPDCH Dedicated Physical Data Channel

DS-CDMA Direct-Sequence Code Division Multiple Access

DTX Discontinuous Transmission

FACH Forward Access Channel

E-AGCH E-DCH Absolute Grant Channel

E-DCH Enhanced Dedicated Channel

E-DPCCH E-DCH Dedicated Physical Control Channel

E-DPDCH E-DCH Dedicated Physical Data Channel

E-HICH E-DCH Hybrid ARQ Indicator Channel

E-RGCH E-DCH Relative Grant Channel

E-RNTI E-DCH Radio Network Temporary Identifier

E-ROCH E-DCH Rank and Offset Channel

FDD Frequency Division Duplex

F-DPCH Fractional Dedicated Physical Channel

F-TPICH Fractional Transmitted Precoding Indicator Channel

FER Frame Error Rate

GF Galois Field

HARQ Hybrid Automatic Repeat reQuest

HS-DPCCH Dedicated Physical Control Channel (uplink) for HS-DSCH

HS-DPCCH2 Secondary Dedicated Physical Control Channel (uplink) for HS-DSCH, when Secondary\_Cell\_Enabled is greater than 3

HS-DSCH High Speed Downlink Shared Channel

HS-PDSCH High Speed Physical Downlink Shared Channel

HS-SCCH Shared Control Channel for HS-DSCH

MAC Medium Access Control

MBSFN MBMS over a Single Frequency Network

Mcps Mega Chip Per Second

MIMO Multiple Input Multiple Output

MS Mobile Station

OVSF Orthogonal Variable Spreading Factor (codes)

PCCC Parallel Concatenated Convolutional Code

PCH Paging Channel

PhCH Physical Channel

PRACH Physical Random Access Channel

RACH Random Access Channel

RSC Recursive Systematic Convolutional Coder

RV Redundancy Version

RX Receive

SCH Synchronization Channel

SF Spreading Factor

SFN System Frame Number

SIR Signal-to-Interference Ratio

SNR Signal to Noise Ratio

S-DPCCH Secondary Dedicated Physical Control Channel

S-E-DPCCH Secondary Dedicated Physical Control Channel for E-DCH

S-E-DPDCH Secondary Dedicated Physical Data Channel for E-DCH

S-E-RNTI Secondary E-RNTI

TF Transport Format

TFC Transport Format Combination

TFCI Transport Format Combination Indicator

TPC Transmit Power Control

TPI Transmitted Precoding Indicator

TrCH Transport Channel

TTI Transmission Time Interval

TX Transmit

UL Uplink (Reverse link)

# 4 Multiplexing, channel coding and interleaving

## 4.1 General

Data stream from/to MAC and higher layers (Transport block / Transport block set) is encoded/decoded to offer transport services over the radio transmission link. Channel coding scheme is a combination of error detection, error correcting, rate matching, interleaving and transport channels mapping onto/splitting from physical channels.

## 4.2 General coding/multiplexing of TrCHs

This section only applies to the transport channels: DCH, RACH, BCH, FACH and PCH. Other transport channels which do not use the general method are described separately below.

Data arrives to the coding/multiplexing unit in form of transport block sets once every transmission time interval. The transmission time interval is transport-channel specific from the set {10 ms, 20 ms, 40 ms, 80 ms}, where 80 ms TTI for DCH shall not be used unless SF=512.

The following coding/multiplexing steps can be identified:

- add CRC to each transport block (see subclause 4.2.1);

- transport block concatenation and code block segmentation (see subclause 4.2.2);

- channel coding (see subclause 4.2.3);

- radio frame equalisation (see subclause 4.2.4);

- rate matching (see subclause 4.2.7);

- insertion of discontinuous transmission (DTX) indication bits (see subclause 4.2.9);

- interleaving (two steps, see subclauses 4.2.5 and 4.2.11);

- radio frame segmentation (see subclause 4.2.6);

- multiplexing of transport channels (see subclause 4.2.8);

- physical channel segmentation (see subclause 4.2.10);

- mapping to physical channels (see subclause 4.2.12).

The coding/multiplexing steps for uplink and downlink are shown in figure 1 and figure 2 respectively.



Figure 1: Transport channel multiplexing structure for uplink



Figure 2: Downlink transport channel multiplexing structure for transport channels that are not concatenated.



Figure 2A: Downlink transport channel processing for transport channels that are concatenated. The concatenated transport channel inherits the parameters of the transport channel *i1*.

The single output data stream from the TrCH multiplexing, including DTX indication bits in downlink, is denoted *Coded Composite Transport Channel (CCTrCH)*. A CCTrCH can be mapped to one or several physical channels.

### 4.2.0 Transport channel concatenation

When DL\_DCH\_FET\_Config is configured with value 1, downlink transport blocks of transport channels with a transport channel number *il*   are concatenated to form a concatenated transport channel. In this case, higher layers ensure that TTI values of transport channels that are concatenated are the same.

Let *i1, i2, i3,…,iB* denote in ascending order the transport channel numbers in  *i1 < i2 < i3 <… < iB* he concatenated transport channel is treated as a regular transport channel in layer 1, inheriting the parameters of transport channel number *i1,* e.g., the transport channel number, and the rate matching attribute of the concatenated transport channel are *i1* and  respectively.All transport blocks of all the transport channels to be concatenated are serially concatenated into a single transport block, in ascending order. The bits input to the transport channel concatenation are denoted by for , and *m* = 1, …, , where *ik* denotes the TrCH number, *m* denotes the transport block number for the transport channel *ik* , and is the number of bits in each transport block of transport channel *ik*. The bits after transport channel concatenation are denoted by , where *A* =**denotes the total number of bits in the signle transport block of the concatenated transport channel. The  bits are defined by the following set of relations:

,

for *m* = 1, …,, and .

### 4.2.1 CRC attachment

Error detection is provided on transport blocks through a Cyclic Redundancy Check (CRC). The size of the CRC is 24, 16, 12, 8 or 0 bits and it is signalled from higher layers what CRC size that should be used for each TrCH.

#### 4.2.1.1 CRC Calculation

The entire transport block is used to calculate the CRC parity bits for each transport block. The parity bits are generated by one of the following cyclic generator polynomials:

- gCRC24(*D*) = *D*24 + *D*23 + *D*6 + *D*5 + *D* + 1;

- gCRC16(*D*) = *D*16 + *D*12 + *D*5 + 1;

- gCRC12(*D*) = *D*12 + *D*11 + *D*3 + *D*2 + *D* + 1;

- gCRC8(*D*) = *D*8 + *D*7 + *D*4 + *D*3 + *D* + 1.

Denote the bits in a transport block delivered to layer 1 by , and the parity bits by . *Ai* is the size of a transport block of TrCH *i, m* is the transport block number, and *Li* is the number of parity bits. *Li* can take the values 24, 16, 12, 8, or 0 depending on what is signalled from higher layers, except for a concatenated transport channel (Subclause 4.2.0) where the number of parity bits is always 16.

The encoding is performed in a systematic form, which means that in GF(2), the polynomial:



yields a remainder equal to 0 when divided by gCRC24(*D*), polynomial:



yields a remainder equal to 0 when divided by gCRC16(*D*), polynomial:



yields a remainder equal to 0 when divided by gCRC12(*D*) and polynomial:



yields a remainder equal to 0 when divided by gCRC8(*D*).

If no transport blocks are input to the CRC calculation (*Mi* = 0), no CRC attachment shall be done. If transport blocks are input to the CRC calculation (*Mi*  0) and the size of a transport block is zero (*Ai* = 0), CRC shall be attached, i.e. all parity bits equal to zero.

#### 4.2.1.2 Relation between input and output of the CRC attachment block

The bits after CRC attachment are denoted by , where *Bi* = *Ai*+ *Li*. The relation between *aimk* and *bimk* is:

 *k* = 1, 2, 3, …, *Ai*

 *k* = *Ai* + 1, *Ai* + 2, *Ai* + 3, …, *Ai* + *Li*

### 4.2.2 Transport block concatenation and code block segmentation

All transport blocks in a TTI are serially concatenated. If the number of bits in a TTI is larger than *Z*, the maximum size of a code block in question, then code block segmentation is performed after the concatenation of the transport blocks. The maximum size of the code blocks depends on whether convolutional coding or turbo coding is used for the TrCH.

#### 4.2.2.1 Concatenation of transport blocks

The bits input to the transport block concatenation are denoted by  where *i* is the TrCH number, *m* is the transport block number, and *Bi* is the number of bits in each block (including CRC). The number of transport blocks on TrCH *i* is denoted by *Mi*. The bits after concatenation are denoted by , where *i* is the TrCH number and *Xi=MiBi*. They are defined by the following relations:

 *k =* 1, 2*, …, Bi*

 *k = Bi* *+* 1*, Bi* *+* 2*, …,* 2*Bi*

 *k =* 2*Bi* *+* 1, 2*Bi* *+* 2*, …,* 3*Bi*

**

 *k =* (*Mi* - 1)*Bi* *+* 1*,* (*Mi* - 1)*Bi* *+* 2*, …, MiBi*

#### 4.2.2.2 Code block segmentation

Segmentation of the bit sequence from transport block concatenation is performed if *Xi>Z.* The code blocks after segmentation are of the same size. The number of code blocks on TrCH *i* is denoted by *Ci*. If the number of bits input to the segmentation, *Xi*, is not a multiple of *Ci*, filler bits are added to the beginning of the first block. If turbo coding is selected and *Xi <* 40, filler bits are added to the beginning of the code block. The filler bits are transmitted and they are always set to 0. The maximum code block sizes are:

- convolutional coding: *Z* = 504;

- turbo coding: *Z* = 5114.

The bits output from code block segmentation, for *Ci*  0, are denoted by , where *i* is the TrCH number, *r* is the code block number, and *Ki* is the number of bits per code block.

Number of code blocks:



Number of bits in each code block (applicable for *Ci*  0 only):

if *Xi* < 40 and Turbo coding is used, then

*Ki* = 40

else

*Ki = Xi / Ci*

end if

Number of filler bits: *Yi = CiKi - Xi*

for *k =* 1 to *Yi* -- Insertion of filler bits



end for

for *k = Yi+*1 to *Ki*



end for

*r =* 2 -- Segmentation

while *r  Ci*

for *k =* 1 to *Ki*

*I*

end for

*r = r+*1

end while

### 4.2.3 Channel coding

Code blocks are delivered to the channel coding block. They are denoted by , where *i* is the TrCH number, *r* is the code block number, and *Ki* is the number of bits in each code block. The number of code blocks on TrCH *i* is denoted by *Ci*. After encoding the bits are denoted by , where *Yi* is the number of encoded bits. The relation between *oirk* and *yirk* and between *Ki* and *Yi* is dependent on the channel coding scheme.

The following channel coding schemes can be applied to TrCHs:

- convolutional coding;

- turbo coding.

Usage of coding scheme and coding rate for the different types of TrCH is shown in table 1.

The values of *Yi* in connection with each coding scheme:

- convolutional coding with rate 1/2: *Yi* = 2*\*Ki +* 16; rate 1/3: *Yi* = 3*\*Ki +* 24;

- turbo coding with rate 1/3: *Yi* = 3*\*Ki +* 12.

Table 1: Usage of channel coding scheme and coding rate

|  |  |  |
| --- | --- | --- |
| Type of TrCH | Coding scheme | Coding rate |
| BCH | Convolutional coding | 1/2 |
| PCH |
| RACH |
| DCH, FACH | 1/3, 1/2 |
| Turbo coding\* | 1/3 |

\* For DCH, turbo coding is not allowed when DL\_DCH\_FET\_Config is configured by higher layers.

#### 4.2.3.1 Convolutional coding

Convolutional codes with constraint length 9 and coding rates 1/3 and 1/2 are defined.

The configuration of the convolutional coder is presented in figure 3.

Output from the rate 1/3 convolutional coder shall be done in the order output0, output1, output2, output0, output1, output 2, output 0,…,output2. Output from the rate 1/2 convolutional coder shall be done in the order output 0, output 1, output 0, output 1, output 0, …, output 1.

8 tail bits with binary value 0 shall be added to the end of the code block before encoding.

The initial value of the shift register of the coder shall be "all 0" when starting to encode the input bits.



Figure 3: Rate 1/2 and rate 1/3 convolutional coders

#### 4.2.3.2 Turbo coding

##### 4.2.3.2.1 Turbo coder

The scheme of Turbo coder is a Parallel Concatenated Convolutional Code (PCCC) with two 8-state constituent encoders and one Turbo code internal interleaver. The coding rate of Turbo coder is 1/3. The structure of Turbo coder is illustrated in figure 4.

The transfer function of the 8-state constituent code for PCCC is:

*G*(*D*) = ,

where

*g*0(*D*) = 1 + *D*2 + *D*3,

*g*1(*D*) = 1 + *D* + *D*3.

The initial value of the shift registers of the 8-state constituent encoders shall be all zeros when starting to encode the input bits.

Output from the Turbo coder is

*x*1, *z*1, *z*'1, *x*2, *z*2, *z*'2, …, *xK*, *zK*, *z*'*K*,

where *x*1, *x*2, …, *xK* are the bits input to the Turbo coder i.e. both first 8-state constituent encoder and Turbo code internal interleaver, and *K* is the number of bits, and *z*1, *z*2, …, *zK* and *z*'1, *z*'2, …, *z*'*K* are the bits output from first and second 8-state constituent encoders, respectively.

The bits output from Turbo code internal interleaver are denoted by *x*'1, *x*'2, …, *x*'*K*, and these bits are to be input to the second 8-state constituent encoder.



Figure 4: Structure of rate 1/3 Turbo coder (dotted lines apply for trellis termination only)

##### 4.2.3.2.2 Trellis termination for Turbo coder

Trellis termination is performed by taking the tail bits from the shift register feedback after all information bits are encoded. Tail bits are padded after the encoding of information bits.

The first three tail bits shall be used to terminate the first constituent encoder (upper switch of figure 4 in lower position) while the second constituent encoder is disabled. The last three tail bits shall be used to terminate the second constituent encoder (lower switch of figure 4 in lower position) while the first constituent encoder is disabled.

The transmitted bits for trellis termination shall then be:

*xK*+1, *zK*+1, *xK*+2, *zK*+2, *xK*+3, *zK*+3, *x*'*K*+1, *z*'*K*+1, *x*'*K*+2, *z*'*K*+2, *x*'*K*+3, *z*'*K*+3.

##### 4.2.3.2.3 Turbo code internal interleaver

The Turbo code internal interleaver consists of bits-input to a rectangular matrix with padding, intra-row and inter-row permutations of the rectangular matrix, and bits-output from the rectangular matrix with pruning. The bits input to the Turbo code internal interleaver are denoted by , where *K* is the integer number of the bits and takes one value of 40  *K*  5114. The relation between the bits input to the Turbo code internal interleaver and the bits input to the channel coding is defined by  and *K* = *Ki*.

The following subclause specific symbols are used in subclauses 4.2.3.2.3.1 to 4.2.3.2.3.3:

*K* Number of bits input to Turbo code internal interleaver

*R* Number of rows of rectangular matrix

*C* Number of columns of rectangular matrix

*p* Prime number

*v* Primitive root

 Base sequence for intra-row permutation

*qi* Minimum prime integers

*ri* Permuted prime integers

 Inter-row permutation pattern

 Intra-row permutation pattern of *i*-th row

*i* Index of row number of rectangular matrix

*j* Index of column number of rectangular matrix

*k* Index of bit sequence

4.2.3.2.3.1 Bits-input to rectangular matrix with padding

The bit sequence  input to the Turbo code internal interleaver is written into the rectangular matrix as follows.

(1) Determine the number of rows of the rectangular matrix, *R*, such that:

.

The rows of rectangular matrix are numbered 0, 1, …, *R* - 1 from top to bottom.

(2) Determine the prime number to be used in the intra-permutation, *p*, and the number of columns of rectangular matrix, *C*, such that:

if (481  *K*  530) then

*p = 53* and *C* = *p*.

else

Find minimum prime number *p* from table 2 such that

,

and determine *C* such that

.

end if

The columns of rectangular matrix are numbered 0, 1, …, *C* - 1 from left to right.

Table 2: List of prime number *p* and associated primitive root *v*

| *p* | *v* | *p* | *v* | *p* | *v* | *p* | *v* | *p* | *v* |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 7 | 3 | 47 | 5 | 101 | 2 | 157 | 5 | 223 | 3 |
| 11 | 2 | 53 | 2 | 103 | 5 | 163 | 2 | 227 | 2 |
| 13 | 2 | 59 | 2 | 107 | 2 | 167 | 5 | 229 | 6 |
| 17 | 3 | 61 | 2 | 109 | 6 | 173 | 2 | 233 | 3 |
| 19 | 2 | 67 | 2 | 113 | 3 | 179 | 2 | 239 | 7 |
| 23 | 5 | 71 | 7 | 127 | 3 | 181 | 2 | 241 | 7 |
| 29 | 2 | 73 | 5 | 131 | 2 | 191 | 19 | 251 | 6 |
| 31 | 3 | 79 | 3 | 137 | 3 | 193 | 5 | 257 | 3 |
| 37 | 2 | 83 | 2 | 139 | 2 | 197 | 2 |  |  |
| 41 | 6 | 89 | 3 | 149 | 2 | 199 | 3 |  |  |
| 43 | 3 | 97 | 5 | 151 | 6 | 211 | 2 |  |  |

(3) Write the input bit sequence  into the *R* *C* rectangular matrix row by row starting with bit *y*1 in column 0 of row 0:



where *y*k = *x*k for *k* = 1, 2, …, *K* and if *R**C**K*, the dummy bits are padded such that  for *k* = *K* + 1, *K* + 2, …, *R**C*. These dummy bits are pruned away from the output of the rectangular matrix after intra-row and inter-row permutations.

4.2.3.2.3.2 Intra-row and inter-row permutations

After the bits-input to the *R**C* rectangular matrix, the intra-row and inter-row permutations for the *R**C* rectangular matrix are performed stepwise by using the following algorithm with steps (1) – (6):

(1) Select a primitive root *v* from table 2 in clause 4.2.3.2.3.1, which is indicated on the right side of the prime number *p*.

(2) Construct the base sequence  for intra-row permutation as:

, *j* = 1, 2,…, (*p* - 2), and *s*(0) = 1.

(3) Assign *q*0 = 1 to be the first prime integer in the sequence , and determine the prime integer *qi* in the sequence  to be a least prime integer such that g.c.d(*qi*, *p* - 1) = 1*,* *qi* > 6, and *qi* > *q*(*i* - 1) for each *i* = 1, 2, …, *R* – 1. Here g.c.d. is greatest common divisor.

(4) Permute the sequence  to make the sequence  such that

*rT*(*i*) = *qi*, *i* = 0, 1, …, *R* - 1,

where  is the inter-row permutation pattern defined as the one of the four kind of patterns, which are shown in table 3, depending on the number of input bits *K*.

Table 3: Inter-row permutation patterns for Turbo code internal interleaver

|  |  |  |
| --- | --- | --- |
| Number of input bits  *K* | Number of rows *R* | Inter-row permutation patterns  <*T*(0), *T*(1), …, *T*(*R* - 1)> |
| (40*K*159) | 5 | <4, 3, 2, 1, 0> |
| (160*K*200) or (481*K*530) | 10 | <9, 8, 7, 6, 5, 4, 3, 2, 1, 0> |
| (2281*K*2480) or (3161*K*3210) | 20 | <19, 9, 14, 4, 0, 2, 5, 7, 12, 18, 16, 13, 17, 15, 3, 1, 6, 11, 8, 10> |
| *K* = any other value | 20 | <19, 9, 14, 4, 0, 2, 5, 7, 12, 18, 10, 8, 13, 17, 3, 1, 16, 6, 15, 11> |

(5) Perform the *i*-th (*i* = 0, 1, …, *R* - 1) intra-row permutation as:

if (*C* = *p*) then

, *j* = 0, 1, …, (*p* - 2), and *Ui*(*p* - 1) = 0,

where *Ui*(*j*) is the original bit position of *j*-th permuted bit of *i*-th row.

end if

if (*C* = *p* + 1) then

, *j* = 0, 1, …, (*p* - 2). *Ui*(*p* - 1) = 0, and *Ui*(*p*) = *p*,

where *Ui*(*j*) is the original bit position of *j*-th permuted bit of *i*-th row, and

if (*K* = *R**C*) then

Exchange *UR*-1(*p*) with *UR*-1(0).

end if

end if

if (*C* = *p* - 1) then

, *j* = 0, 1, …, (*p* - 2),

where *Ui*(*j*) is the original bit position of *j*-th permuted bit of *i*-th row.

end if

(6) Perform the inter-row permutation for the rectangular matrix based on the pattern ,

where *T*(*i*) is the original row position of the *i*-th permuted row.

4.2.3.2.3.3 Bits-output from rectangular matrix with pruning

After intra-row and inter-row permutations, the bits of the permuted rectangular matrix are denoted by *y*'*k*:



The output of the Turbo code internal interleaver is the bit sequence read out column by column from the intra-row and inter-row permuted *R* ** *C* rectangular matrix starting with bit *y*'1 in row 0 of column 0 and ending with bit *y*'*CR* in row *R* - 1 of column *C* - 1. The output is pruned by deleting dummy bits that were padded to the input of the rectangular matrix before intra-row and inter row permutations, i.e. bits *y*'*k* that corresponds to bits *yk* with *k > K* are removed from the output. The bits output from Turbo code internal interleaver are denoted by *x*'1, *x*'2, …, *x*'*K*, where *x*'1 corresponds to the bit *y*'*k* with smallest index *k* after pruning, *x*'2 to the bit *y*'*k* with second smallest index *k* after pruning, and so on. The number of bits output from Turbo code internal interleaver is *K* and the total number of pruned bits is:

*R*  *C* – *K*.

#### 4.2.3.3 Concatenation of encoded blocks

After the channel coding for each code block, if *Ci* is greater than 1, the encoded blocks are serially concatenated so that the block with lowest index *r* is output first from the channel coding block, otherwise the encoded block is output from channel coding block as it is. The bits output are denoted by , where *i* is the TrCH number and *Ei* = *CiYi*. The output bits are defined by the following relations:

 *k =* 1, 2*, …, Yi*

 *k = Yi* *+* 1*, Yi* *+* 2*, …,* 2*Yi*

 *k =* 2*Yi* *+* 1, 2*Yi* *+* 2*, …,* 3*Yi*



 *k =* (*Ci* - 1)*Yi* *+* 1*,* (*Ci* - 1)*Yi* *+* 2*, …, CiYi*

If no code blocks are input to the channel coding (*Ci* = 0), no bits shall be output from the channel coding, i.e. *Ei* = 0.

### 4.2.4 Radio frame size equalisation

Radio frame size equalisation is padding the input bit sequence in order to ensure that the output can be segmented in *Fi* data segments of same size as described in subclause 4.2.7. Radio frame size equalisation is only performed in the UL.

The input bit sequence to the radio frame size equalisation is denoted by, where *i* is TrCH number and *Ei* the number of bits. The output bit sequence is denoted by, where *Ti* is the number of bits. The output bit sequence is derived as follows:

- *tik* = *cik*, for k = 1… *Ei*; and

- *tik* = {0, 1} for k= *Ei* +1… *Ti*, if *Ei* < *Ti*;

where

- T*i* = *Fi* \* *Ni*; and

-  is the number of bits per segment after size equalisation.

### 4.2.5 1st interleaving

#### 4.2.5.1 Void

#### 4.2.5.2 1st interleaver operation

The 1st interleaving is a block interleaver with inter-column permutations. The input bit sequence to the block interleaver is denoted by , where *i* is TrCH number and *Xi* the number of bits. Here *Xi* is guaranteed to be an integer multiple of *Fi*. The output bit sequence from the block interleaver is derived as follows:

(1) Select the number of columns C1 from Table 4 or 4A depending on the TTI. The columns are numbered 0, 1, …, C1 - 1 from left to right. Table 4A is used in uplink when UL\_DPCH\_10ms\_Mode is configured by higher layers, and Table 4 is used in all other cases.

(2) Determine the number of rows of the matrix, R1 defined as

R1 = *Xi* / C1.

The rows of the matrix are numbered 0, 1, …, R1 - 1 from top to bottom.

(3) Write the input bit sequence into the R1  C1 matrix row by row starting with bit  in column 0 of row 0 and ending with bit  in column C1 - 1 of row R1 - 1:



(4) Perform the inter-column permutation for the matrix based on the pattern  shown in table 4, where P1C1 (*j*) is the original column position of the *j*-th permuted column. After permutation of the columns, the bits are denoted by *yik*:



(5) Read the output bit sequence  of the block interleaver column by column from the inter-column permuted R1  C1 matrix. Bit  corresponds to row 0 of column 0 and bit  corresponds to row R1 - 1 of column C1 - 1.

Table 4: Inter-column permutation patterns for 1st interleaving for downlink, and for uplink when UL\_DPCH\_10ms\_Mode is not configured by higher layers

|  |  |  |
| --- | --- | --- |
| TTI | Number of columns C1 | Inter-column permutation patterns  <P1C1(0), P1C1(1), …, P1C1(C1-1)> |
| 10 ms | 1 | <0> |
| 20 ms | 2 | <0,1> |
| 40 ms | 4 | <0,2,1,3> |
| 80 ms | 8 | <0,4,2,6,1,5,3,7> |

Table 4A: Inter-column permutation patterns for 1st interleaving for uplink when UL\_DPCH\_10ms\_Mode is configured by higher layers

|  |  |  |
| --- | --- | --- |
| TTI | Number of columns C1 | Inter-column permutation patterns  <P1C1(0), P1C1(1), …, P1C1(C1-1)> |
| 20 ms | 1 | <0> |
| 40 ms | 2 | <0,1> |
| 80 ms | 4 | <0,2,1,3> |

#### 4.2.5.3 Relation between input and output of 1st interleaving in uplink

The bits input to the 1st interleaving are denoted by , where *i* is the TrCH number and *Ti* the number of bits. Hence, x*i,k = ti,k* and X*i* *=* *Ti*.

The bits output from the 1st interleaving are denoted by , and d*i,k = yi,k*.

#### 4.2.5.4 Relation between input and output of 1st interleaving in downlink

If fixed positions of the TrCHs in a radio frame is used then the bits input to the 1st interleaving are denoted by , where *i* is the TrCH number. Hence, x*ik = hik* and X*i = Di*.

If flexible positions of the TrCHs in a radio frame is used then the bits input to the 1st interleaving are denoted by , where *i* is the TrCH number. Hence, x*ik = gik* and X*i = Gi*.

The bits output from the 1st interleaving are denoted by , where *i* is the TrCH number and *Qi* is the number of bits. Hence, *qik = yik*, *Qi* = *FiHi* if fixed positions are used, and *Qi* = *Gi* if flexible positions are used. *Hi* is defined in subclause 4.2.9.1.

### 4.2.6 Radio frame segmentation

When the transmission time interval is longer than 10 ms, the input bit sequence is segmented and mapped onto *Fi* segments. Following rate matching in the DL and radio frame size equalisation in the UL the input bit sequence length is guaranteed to be an integer multiple of *Fi*.

The input bit sequence is denoted by  where *i* is the TrCH number and *Xi* is the number bits. The *Fi* output bit sequences per TTI are denoted by where *ni* is the segment number and *Yi* is the number of bits per radio frame for TrCH *i*. The output sequences are defined as follows:

= , *ni* = 1…*Fi*, *k* = 1…*Yi*

where

*Yi* = (*Xi* / *Fi*) is the number of bits per segment.

In downlink, the *ni* -th segment is mapped to the radio frame *ni* -1 of the transmission time interval.

In uplink when UL\_DPCH\_10ms\_Mode is not configured by higher layers, the *ni* -th segment, 1  *ni*  *Fi* is mapped to radio frame *ni* -1 of the transmission time interval.

In uplink when UL\_DPCH\_10ms\_Mode is configured by higher layers, the *ni*th segment, 1  *ni*  *Fi*, is mapped to theradio frame 2*ni* – 2 of the transmission time interval. No bits are input to the radio frame 2*ni* – 1.

#### 4.2.6.1 Relation between input and output of the radio frame segmentation block in uplink

The input bit sequence to the radio frame segmentation is denoted by , where *i* is the TrCH number and *Ti* the number of bits. Hence, *xik = dik* and *Xi = Ti*.

The output bit sequence corresponding to radio frame *ni* is denoted by , where *i* is the TrCH number and *Ni* is the number of bits. Hence, and *Ni = Yi*.

#### 4.2.6.2 Relation between input and output of the radio frame segmentation block in downlink

The bits input to the radio frame segmentation are denoted by , where *i* is the TrCH number and *Qi* the number of bits. Hence, *xik = qik* and *Xi = Qi*.

The output bit sequence corresponding to radio frame *ni* is denoted by , where *i* is the TrCH number and *Vi* is the number of bits. Hence, and *Vi = Yi*.

### 4.2.7 Rate matching

Rate matching means that bits on a transport channel are repeated or punctured. Higher layers assign a rate-matching attribute for each transport channel. This attribute is semi-static and can only be changed through higher layer signalling. The rate-matching attribute is used when the number of bits to be repeated or punctured is calculated.

The number of bits on a transport channel can vary between different transmission time intervals. In the downlink the transmission is interrupted if the number of bits is lower than maximum. When the number of bits between different transmission time intervals in uplink is changed, bits are repeated or punctured to ensure that the total bit rate after TrCH multiplexing is identical to the total channel bit rate of the allocated dedicated physical channels.

If no bits are input to the rate matching for all TrCHs within a CCTrCH, the rate matching shall output no bits for all TrCHs within the CCTrCH and no uplink DPDCH will be selected in the case of uplink rate matching.

**Notation used in subclause 4.2.7 and subclauses:**

*Ni,j:* For uplink: Number of bits in a radio frame before rate matching on TrCH *i* with transport format combination *j* . When UL\_DPCH\_10ms Mode is configured by higher layers, the derivation of *Ni,j* is described in detail in subclauses 4.2.6 and 4.2.6.1.

For downlink: An intermediate calculation variable (not an integer but a multiple of 1/8).

*:* Number of bits in a transmission time interval before rate matching on TrCH *i* with transport format *l*. Used in downlink only.

*:* For uplink: If positive - number of bits that should be repeated in each radio frame on TrCH *i* with transport format combination *j*.

If negative - number of bits that should be punctured in each radio frame on TrCH *i* with transport format combination *j*.

For downlink : An intermediate calculation variable (not an integer but a multiple of 1/8).

*:* If positive - number of bits to be repeated in each transmission time interval on TrCH *i* with transport format *l*.

If negative - number of bits to be punctured in each transmission time interval on TrCH *i* with transport format *l*.

Used in downlink only.

*NTGL*: Positive or null: number of bits in the radio frame corresponding to the gap for compressed mode for the CCTrCH.

*RMi:* Semi-static rate matching attribute for transport channel *i*. *RMi* is provided by higher layers or takes a value as indicated in subclause 4.2.13 or subclause 4.2.0.

*PL:* Puncturing limit for uplink. This value limits the amount of puncturing that can be applied in order to avoid multicode or to enable the use of a higher spreading factor. Signalled from higher layers. The allowed puncturing in % is actually equal to (1-PL)\*100.

*Ndata,j:* Total number of bits that are available for the CCTrCH in a radio frame with transport format combination *j*.

*I:* Number of TrCHs in the CCTrCH.

*Zi,j:* Intermediate calculation variable.

*Fi:* Number of radio frames in the transmission time interval of TrCH *i,* except for uplink when UL\_DPCH\_10ms\_Mode is configured. In uplink, when UL\_DPCH\_10ms\_Mode is configured, *Fi* is the number of radio frames in the transmission time interval of TrCH *i* divided by 2.

*ni:* Radio frame number in the transmission time interval of TrCH *i*. In downlink, and in uplink when UL\_DPCH\_10ms\_Mode is not configured by higher layers, *0  ni < Fi*. In uplink when UL\_DPCH\_10ms\_Mode is configured by higher layers, *0  ni <* 2*Fi*.

*q:* Average puncturing or repetition distance (normalised to only show the remaining rate matching on top of an integer number of repetitions). Used in uplink only.

P1*F(ni):* The column permutation function of the 1st interleaver, P1*F*(x) is the original position of column with number x after permutation. P1 is defined on table 4 of clause 4.2.5.2 (note that the P1F is self-inverse). Used for rate matching in uplink only.

*S*[*n*]*:* The shift of the puncturing or repetition pattern for radio frame *ni* when . Used in uplink only.

*TFi*(*j*)*:* Transport format of TrCH *i* for the transport format combination *j*.

*TFS*(*i*) The set of transport format indexes *l* for TrCH *i*.

*TFCS* The set of transport format combination indexes *j.*

*eini*  Initial value of variable *e* in the rate matching pattern determination algorithm of subclause 4.2.7.5.

eplus Increment of variable *e* in the rate matching pattern determination algorithm of subclause4.2.7.5.

eminus Decrement of variable *e* in the rate matching pattern determination algorithm of subclause 4.2.7.5.

*b:* Indicates systematic and parity bits

*b*=1: Systematic bit. *xk* in subclause 4.2.3.2.1.

*b*=2: 1st parity bit (from the upper Turbo constituent encoder). *zk* in subcaluse 4.2.3.2.1.

*b*=3: 2nd parity bit (from the lower Turbo constituent encoder). *z*'*k* in subclause 4.2.3.2.1.

The \* (star) notation is used to replace an index *x* when the indexed variable *Xx* does not depend on the index *x.* In the left wing of an assignment the meaning is that "*X\** = *Y*" is equivalent to "**for all** *x* **do** *Xx* = *Y* ". In the right wing of an assignment, the meaning is that "*Y* = *X\** " is equivalent to "**take any** *x* **and do** *Y = Xx*".

The following relations, defined for all TFC *j*, are used when calculating the rate matching parameters:



 for all *i* = 1 … *I* (1)

 for all *i* = 1 … *I*

#### 4.2.7.1 Determination of rate matching parameters in uplink

##### 4.2.7.1.1 Determination of SF and number of PhCHs needed

In uplink, puncturing can be applied to match the CCTrCH bit rate to the PhCH bit rate. The bit rate of the PhCH(s) is limited by the UE capability and restrictions imposed by UTRAN, through limitations on the PhCH spreading factor. The maximum amount of puncturing that can be applied is 1-PL, PL is signalled from higher layers. The number of available bits in the radio frames of one PhCH for all possible spreading factors is given in [2]. Denote these values by *N256, N128, N64, N32, N16, N8,* and *N4,* where the index refers to the spreading factor. The possible number of bits available to the CCTrCH on all PhCHs, *Ndata*, then are { *N*256, *N*128, *N*64, *N*32, *N*16, *N*8, *N*4,2*N*4,3*N*4,4*N*4,5*N*4*,* 6*N*4}*.*

For a RACH CCTrCH SET0 represents the set of *Ndata* values allowed by the UTRAN, as set by the minimum SF provided by higher layers. SET0 may be a sub-set of { *N*256, *N*128, *N*64, *N*32 }. SET0 does not take into account the UE’s capability.

For other CCTrCHs, SET0 denotes the set of  *Ndata*values allowed by the UTRAN and supported by the UE, as part of the UE’s capability. SET0 can be a subset of { *N*256, *N*128, *N*64, *N*32, *N*16, *N*8, *N*4,2*N*4,3*N*4,4*N*4,5*N*4*,* 6*N*4}*.* When UL DPCH 10ms Mode is configured, SET0 shall include *Ndata* values associated with spreading factors larger than or equal to the minimum SF provided by higher layers divided by 2. *Ndata, j*for the transport format combination *j* is determined by executing the following algorithm:

SET1 = { *Ndata* in SET0 such that  is non negative }

If SET1 is not empty and the smallest element of SET1 requires just one PhCH then

*Ndata,j* = min SET1

else

SET2 = { *Ndata* in SET0 such that  is non negative }

Sort SET2 in ascending order

*Ndata* = min SET2

While *Ndata* is not the max of SET2 and the follower of *Ndata* requires no additional PhCH do

*Ndata* = follower of *Ndata* in SET2

End while

*Ndata*,*j* = *Ndata*

End if

For a RACH CCTrCH, if *Ndata,j* is not part of the UE’s capability then the TFC *j* cannot be used.

4.2.7.1.2 Determination of parameters needed for calculating the rate matching pattern

The number of bits to be repeated or punctured, *Ni,j*, within one radio frame for each TrCH *i* is calculated with equation 1 forall possible transport format combinations *j* and selected every radio frame. *Ndata,j* is given from subclause 4.2.7.1.1.

In a compressed radio frame when UL\_DPCH\_10ms\_Mode is not configured by higher layers,  is replaced by in Equation 1.  is given as follows:

In a radio frame compressed by higher layer scheduling,  is obtained by executing the algorithm in subclause 4.2.7.1.1 but with the number of bits in one radio frame of one PhCH reduced to  of the value in normal mode.

*Ntr* is the number of transmitted slots in a compressed radio frame and is defined by the following relation:

|  |  |
| --- | --- |
|  | , if *Nfirst + TGL*  15  , in first frame if *Nfirst + TGL* > 15  , in second frame if *Nfirst + TGL* > 15 |

*Nfirst* and *TGL* are defined in subclause 4.4.

In a radio frame compressed by spreading factor reduction, , where 

If *Ni,j* = 0 then the output data of the rate matching is the same as the input data and the rate matching algorithm of subclause 4.2.7.5 does not need to be executed.

If *Ni,j*  0 the parameters listed in subclauses 4.2.7.1.2.1 and 4.2.7.1.2.2 shall be used for determining *eini*, *eplus*, and *eminus* (regardless if the radio frame is compressed or not).

4.2.7.1.2.1 Convolutionally encoded TrCHs

*R* = *Ni*,*j* mod *Ni*,*j* -- note: in this context *Ni*,*j* mod *Ni*,*j* is in the range of0to *Nij*-1i.e. -1 mod 10 = 9.

if *R*  0and2*R*  *Nij*

then q =  *Ni,j*/ *R* 

else

q =  *Ni*,*j* / (*R* - *Ni*,*j*) 

endif

-- note: q is a signed quantity.

if q is even

then q' = q + gcd(q, *Fi*)/ *Fi* -- where gcd (q, *Fi*) means greatest common divisor of q and *Fi*

-- note that q' is not an integer, but a multiple of 1/8

else

q' = q

endif

for *x* = 0 to *Fi* - 1

S[ *x*q'  mod *Fi*] = ( *x*q'  div *Fi*)

end for

*Ni* = *Ni*,*j*

a = 2

For each radio frame, the rate-matching pattern is calculated with the algorithm in subclause 4.2.7.5, where :

*Xi* = *Ni*,*j*., and

*eini* = (aS[P1*Fi*(*ni*)]|*Ni* | + 1) mod (a*Nij*).

*e*plus = a*Ni*,*j*

*e*minus =a|*Ni*|

puncturing for *N* <0, repetition otherwise.

4.2.7.1.2.2 Turbo encoded TrCHs

If repetition is to be performed on turbo encoded TrCHs, i.e. *Ni,j >*0, the parameters in subclause 4.2.7.1.2.1 are used.

If puncturing is to be performed, the parameters below shall be used. Index *b* is used to indicate systematic (*b*=1), 1st parity (*b*=2), and 2nd parity bit (*b*=3).

*a=2* when *b*=2

*a=1* when *b*=3



If  is calculated as 0 for *b*=2 or *b*=3, then the following procedure and the rate matching algorithm of subclause 4.2.7.5 don't need to be performed for the corresponding parity bit stream.

Xi = Ni,j /3 ,

q = Xi /|Ni| 

if(q2)

for *r=*0 to *Fi*-1

S[(3*r*+b-1) mod *FI*] = *r* mod 2;

end for

else

if *q* is even

then q' = q – *gcd(* q*,* *Fi)*/ *Fi*  -- where *gcd (* q*, Fi)* means greatest common divisor of q and *Fi*   
 -- note that q' is not an integer, but a multiple of 1/8

else q' = q

endif

for *x*=0 to *Fi* -1

r = *x*q' mod *Fi*;

S[(3r+b-1) mod *Fi*] = *x*q' div *Fi*;

endfor

endif

For each radio frame, the rate-matching pattern is calculated with the algorithm in subclause 4.2.7.5, where:

*Xi* is as above:

eini = (aS[P1*Fi*(*ni*)] |Ni| + Xi) mod (a*Xi*), if eini =0 then *eini* = a*Xi*

eplus = a*Xi*

eminus = a*Ni*

#### 4.2.7.2 Determination of rate matching parameters in downlink

For downlink channels, *Ndata,j* does not depend on the transport format combination *j*. *Ndata,\** is given by the channelization code(s) assigned by higher layers.

Denote the number of physical channels used for the CCTrCH by *P*. *Ndata,\** is the number of bits available to the CCTrCH in one radio frame and defined as *Ndata,\**=*P*15(*Ndata*1+*Ndata*2), where *Ndata1* and *Ndata2* are defined in [2]. Note that contrary to the uplink, the same rate matching patterns are used in TTIs containing no compressed radio frames and in TTIs containing radio frames compressed by spreading factor reduction or higher layer scheduling.

##### 4.2.7.2.1 Determination of rate matching parameters for fixed positions of TrCHs

4.2.7.2.1.1 Calculation of *Ni*,max for normal mode and compressed mode by spreading factor reduction

First an intermediate calculation variable  is calculated for all transport channels *i* by the following formula:



In order to compute the  parameters for all TrCH *i* and all TF *l*, we first compute an intermediate parameter *Ni,*max by the following formula, where  is derived from  by the formula given at subclause 4.2.7:



If  then, for TrCH *i*, the output data of the rate matching is the same as the input data and the rate matching algorithm of subclause 4.2.7.5 does not need to be executed. In this case we have :



If  the parameters listed in subclauses 4.2.7.2.1.3 and 4.2.7.2.1.4 shall be used for determining *eini*, *eplus*, and *eminus,* and .

4.2.7.2.1.2 Void

4.2.7.2.1.3 Determination of rate matching parameters for convolutionally encoded TrCHs



*a*=2



For each transmission time interval of TrCH *i* with TF *l*, the rate-matching pattern is calculated with the algorithm in subclause 4.2.7.5. The following parameters are used as input:



1





Puncturing if , repetition otherwise. The values of may be computed by counting repetitions or puncturing when the algorithm of subclause 4.2.7.5 is run. The resulting values of  can be represented with following expression.



4.2.7.2.1.4 Determination of rate matching parameters for Turbo encoded TrCHs

If repetition is to be performed on turbo encoded TrCHs, i.e., the parameters in subclause 4.2.7.2.1.3 are used.

If puncturing is to be performed, the parameters below shall be used. Index *b* is used to indicate systematic (*b*=1), 1st parity (*b*=2), and 2nd parity bit (*b*=3).

*a=2* when *b=*2

*a=1* when *b=*3

The bits indicated by *b*=1 shall not be punctured.

**



For each transmission time interval of TrCH *i* with TF *l*, the rate-matching pattern is calculated with the algorithm in subcaluse 4.2.7.5. The following parameters are used as input:









The values of may be computed by counting puncturing when the algorithm of subclause 4.2.7.5 is run. The resulting values of  can be represented with following expression.



In the above equation, the first term of the right hand side represents the amount of puncturing for *b*=2 and the second term represents the amount of puncturing for *b*=3.

##### 4.2.7.2.1A Determination of rate matching parameters for pseudo-flexible positions of TrCHs

Pseudo-flexible rate matching is identical to fixed-position rate matching, with a difference that in psueduo-flexible rate matching, rate matching parameters are re-evaluated for each maximum TTI, and the value of *RMi* is set to 0 in Equation (1) of subclause 4.2.7 if *Mi* =0 (i.e., no transport blocks are sent in the TTI) for each transport channel *i* with the maximum TTI value among all the transport channels multiplexed into the CCTrCH.

When there is a configuration with more than one transport channel having the maximum TTI and more than one of those transport channels having a transport format with no transport blocks multiplexed into a CCTrCH, the UE behaviour is unspecified.

As a consequence of re-evaluating rate-matching parameters per maximum TTI in pseudo-flexible rate matching, derived parameters dependent on rate matching, for example the parameters corresponding to DTX indication bits in Section 4.2.9.1, can change from one maximum TTI to another in pseudo-flexible rate matching, unlike in fixed position rate matching.

##### 4.2.7.2.2 Determination of rate matching parameters for flexible positions of TrCHs

4.2.7.2.2.1 Calculations for normal mode, compressed mode by higher layer scheduling, and compressed mode by spreading factor reduction

First an intermediate calculation variable  is calculated for all transport channels *i* and all transport format combinations *j* by the following formula:



Then rate matching ratios *RFi* are calculated for each the transport channel *i* in order to minimise the number of DTX bits when the bit rate of the CCTrCH is maximum. The *RFi* ratios are defined by the following formula:



The computation of  parameters is then performed in two phases. In a first phase, tentative temporary values of  are computed, and in the second phase they are checked and corrected. The first phase, by use of the *RFi* ratios, ensures that the number of DTX indication bits inserted is minimum when the CCTrCH bit rate is maximum, but it does not ensure that the maximum CCTrCH bit rate is not greater than *Ndata,\**. per 10ms. The latter condition is ensured through the checking and possible corrections carried out in the second phase.

At the end of the second phase, the latest value of is the definitive value.

The first phase defines the tentative temporary  for all transport channel *i* and any of its transport format *l* by use of the following formula:



The second phase is defined by the following algorithm:

for all  in *TFCS* in ascending order of TFCI do -- for all TFC

**** -- CCTrCH bit rate (bits per 10ms) for TFC *j*

if  then

for *i* = 1 to *I* do -- for all TrCH

 --   is derived from  by the formula given at subclause 4.2.7.

if then



end-if

end-for

end-if

end-for

If  then, for TrCH *i* at TF *l*, the output data of the rate matching is the same as the input data and the rate matching algorithm of subclause 4.2.7.5 does not need to be executed.

If  the parameters listed in subclauses 4.2.7.2.2.2 and 4.2.7.2.2.3 shall be used for determining *eini*, *eplus*, and *eminus*.

4.2.7.2.2.2 Determination of rate matching parameters for convolutionally encoded TrCHs



*a=2*

For each transmission time interval of TrCH *i* with TF *l*, the rate-matching pattern is calculated with the algorithm in subclause 4.2.7.5. The following parameters are used as input:



1





puncturing for , repetition otherwise.

4.2.7.2.2.3 Determination of rate matching parameters for Turbo encoded TrCHs

If repetition is to be performed on turbo encoded TrCHs, i.e. , the parameters in subclause 4.2.7.2.2.2 are used.

If puncturing is to be performed, the parameters below shall be used. Index *b* is used to indicate systematic (*b*=1), 1st parity (*b*=2), and 2nd parity bit (*b*=3).

*a=2* when *b*=2

*a=1* when *b=*3

The bits indicated by *b*=1 shall not be punctured.

**

For each transmission time interval of TrCH *i* with TF *l*, the rate-matching pattern is calculated with the algorithm in subclause 4.2.7.5. The following parameters are used as input:

,

,

**



#### 4.2.7.3 Bit separation and collection in uplink

The systematic bits of turbo encoded TrCHs shall not be punctured, the other bits may be punctured. The systematic bits, first parity bits, and second parity bits in the bit sequence input to the rate matching block are therefore separated into three sequences.

The first sequence contains:

- All of the systematic bits that are from turbo encoded TrCHs.

- From 0 to 2 first and/or second parity bits that are from turbo encoded TrCHs. These bits come into the first sequence when the total number of bits in a block after radio frame segmentation is not a multiple of three.

- Some of the systematic, first parity and second parity bits that are for trellis termination.

The second sequence contains:

- All of the first parity bits that are from turbo encoded TrCHs, except those that go into the first sequence when the total number of bits is not a multiple of three.

- Some of the systematic, first parity and second parity bits that are for trellis termination.

The third sequence contains:

- All of the second parity bits that are from turbo encoded TrCHs, except those that go into the first sequence when the total number of bits is not a multiple of three.

- Some of the systematic, first parity and second parity bits that are for trellis termination.

The second and third sequences shall be of equal length, whereas the first sequence can contain from 0 to 2 more bits. Puncturing is applied only to the second and third sequences.The bit separation function is transparent for convolutionally encoded TrCHs and for turbo encoded TrCHs with repetition. The bit separation and bit collection are illustrated in figures 5 and 6.



Figure 5: Puncturing of turbo encoded TrCHs in uplink



Figure 6: Rate matching for convolutionally encoded TrCHs  
and for turbo encoded TrCHs with repetition in uplink

The bit separation is dependent on the 1st interleaving and offsets are used to define the separation for different TTIs. *b* indicates the three sequences defined in this section, with *b*=1 indicating the first sequence, *b* = 2 the second one, and *b* = 3 the third one. The offsets *b* for these sequences are listed in table 5.

Table 5: TTI dependent offset needed for bit separation

|  |  |  |  |
| --- | --- | --- | --- |
| TTI (ms) | **1 | **2 | **3 |
| 10, 40 | 0 | 1 | 2 |
| 20, 80 | 0 | 2 | 1 |

The bit separation is different for different radio frames in the TTI. A second offset is therefore needed. The radio frame number for TrCH *i* is denoted by *ni*. and the offset by .

Table 6: Radio frame dependent offset needed for bit separation

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| TTI (ms) | **0 | **1 | **2 | **3 | **4 | **5 | **6 | **7 |
| 10 | 0 | NA | NA | NA | NA | NA | NA | NA |
| 20 | 0 | 1 | NA | NA | NA | NA | NA | NA |
| 40 | 0 | 1 | 2 | 0 | NA | NA | NA | NA |
| 80 | 0 | 1 | 2 | 0 | 1 | 2 | 0 | 1 |

##### 4.2.7.3.1 Bit separation

The bits input to the rate matching are denoted by, where *i* is the TrCH number and *Ni* is the number of bits input to the rate matching block. Note that the transport format combination number *j* for simplicity has been left out in the bit numbering, i.e. *Ni*=*Nij*. The bits after separation are denoted by. For turbo encoded TrCHs with puncturing, *b* indicates the three sequences defined in clause 4.2.7.3, with *b*=1 indicating the first sequence, and so forth. For all other cases *b* is defined to be 1. *Xi* is the number of bits in each separated bit sequence. The relation between *eik* and *xbik* is given below.

For turbo encoded TrCHs with puncturing:

 *k* = 1, 2, 3, …, *Xi Xi =* *Ni* /3

 *k* = 1, …, *Ni* mod 3 Note: When (*Ni* mod 3) = 0 this row is not needed.

 *k* = 1, 2, 3, …, *Xi*  *Xi*  = *Ni* /3

 *k* = 1, 2, 3, …, *Xi*  *Xi* = *Ni* /3

For convolutionally encoded TrCHs and turbo encoded TrCHs with repetition:

 *k* = 1, 2, 3, …, *Xi* *Xi = Ni*

##### 4.2.7.3.2 Bit collection

The bits *xbik* are input to the rate matching algorithm described in subclause 4.2.7.5. The bits output from the rate matching algorithm are denoted.

Bit collection is the inverse function of the separation. The bits after collection are denoted by *.* After bit collection, the bits indicated as punctured are removed and the bits are then denoted by, where *i* is the TrCH number and *Vi*= *Nij*+*Nij*. The relations between *ybik*, *zbik*, and *fik* are given below.

For turbo encoded TrCHs with puncturing(*Yi=Xi*):

 *k* = 1, 2, 3, …, *Yi*

 *k* = 1, …, *Ni* mod 3 Note: When (*Ni* mod 3) = 0 this row is not needed.

 *k* = 1, 2, 3, …, *Yi*

 *k* = 1, 2, 3, …, *Yi*

After the bit collection, bits *zi,k* with value **, where **{0, 1}, are removed from the bit sequence. Bit *fi,*1 corresponds to the bit *zi,k* with smallest index *k* after puncturing, bit *fi,*2 corresponds to the bit *zi,k* with second smallest index *k* after puncturing, and so on.

For convolutionally encoded TrCHs and turbo encoded TrCHs with repetition:

 *k* = 1, 2, 3, …, *Yi*

When repetition is used, *fi,k*=*zi,k* and *Yi*=*Vi*.

When puncturing is used, *Yi*=*Xi* and bits *zi,k* with value **, where **{0, 1}, are removed from the bit sequence. Bit *fi,*1 corresponds to the bit *zi,k* with smallest index *k* after puncturing, bit *fi,*2 corresponds to the bit *zi,k* with second smallest index *k* after puncturing, and so on.

#### 4.2.7.4 Bit separation and collection in downlink

The systematic bits of turbo encoded TrCHs shall not be punctured, the other bits may be punctured.

The systematic bits, first parity bits and second parity bits in the bit sequence input to the rate matching block are therefore separated into three sequences of equal lengths.

The first sequence contains :

- All of the systematic bits that are from turbo encoded TrCHs.

- Some of the systematic, first parity and second parity bits that are for trellis termination.

The second sequence contains:

- All of the first parity bits that are from turbo encoded TrCHs.

- Some of the systematic, first parity and second parity bits that are for trellis termination.

The third sequence contains:

- All of the second parity bits that are from turbo encoded TrCHs.

- Some of the systematic, first parity and second parity bits that are for trellis termination.

Puncturing is applied only to the second and third sequences.

The bit separation function is transparent for convolutionally encoded TrCHs and for turbo encoded TrCHs with repetition. The bit separation and bit collection are illustrated in figures 7 and 8.



Figure 7: Puncturing of turbo encoded TrCHs in downlink



Figure 8: Rate matching for convolutionally encoded TrCHs  
and for turbo encoded TrCHs with repetition in downlink

##### 4.2.7.4.1 Bit separation

The bits input to the rate matching are denoted by, where *i* is the TrCH number and *Ei* is the number of bits input to the rate matching block. Note that *Ei* is a multiple of 3 for turbo encoded TrCHs and that the transport format *l* for simplicity has been left out in the bit numbering, i.e. *Ei*=. The bits after separation are denoted by. For turbo encoded TrCHs with puncturing, *b* indicates the three sequences defined in clause 4.2.7.4, with b=1 indicating the first sequence, and so forth. For all other cases *b* is defined to be 1. *Xi* is the number of bits in each separated bit sequence. The relation between *cik* and *xbik* is given below.

For turbo encoded TrCHs with puncturing:

 *k* = 1, 2, 3, …, *Xi Xi = Ei* /3

 *k* = 1, 2, 3, …, *Xi*  *Xi*  = *Ei* /3

 *k* = 1, 2, 3, …, *Xi*  *Xi* = *Ei* /3

For convolutionally encoded TrCHs and turbo encoded TrCHs with repetition:

 *k* = 1, 2, 3, …, *Xi* *Xi = Ei*

##### 4.2.7.4.2 Bit collection

The bits *xbik* are input to the rate matching algorithm described in subclause 4.2.7.5. The bits output from the rate matching algorithm are denoted.

Bit collection is the inverse function of the separation. The bits after collection are denoted by *.* After bit collection, the bits indicated as punctured are removed and the bits are then denoted by, where *i* is the TrCH number and *Gi*= +. The relations between *ybik*, *zbik*, and *gik* are given below.

For turbo encoded TrCHs with puncturing(*Yi=Xi*):

 *k* = 1, 2, 3, …, *Yi*

 *k* = 1, 2, 3, …, *Yi*

 *k* = 1, 2, 3, …, *Yi*

After the bit collection, bits *zi,k* with value **, where **{0, 1}, are removed from the bit sequence. Bit *gi,*1 corresponds to the bit *zi,k* with smallest index *k* after puncturing, bit *gi,*2 corresponds to the bit *zi,k* with second smallest index *k* after puncturing, and so on.

For convolutionally encoded TrCHs and turbo encoded TrCHs with repetition:

 *k* = 1, 2, 3, …, *Yi*

When repetition is used, *gi,k*=*zi,k* and *Yi*=*Gi*.

When puncturing is used, *Yi*=*Xi* and bits *zi,k* with value **, where **{0, 1}, are removed from the bit sequence. Bit *gi,*1 corresponds to the bit *zi,k* with smallest index *k* after puncturing, bit *gi,*2 corresponds to the bit *zi,k* with second smallest index *k* after puncturing, and so on.

#### 4.2.7.5 Rate matching pattern determination

Denote the bits before rate matching by:

, where *i* is the TrCH number and the sequence is defined in 4.2.7.3 for uplink or in 4.2.7.4 for downlink. Parameters *Xi*, eini, eplus, and eminus are given in 4.2.7.1 for uplink or in 4.2.7.2 for downlink.

The rate matching rule is as follows:

if puncturing is to be performed

e = eini  -- initial error between current and desired puncturing ratio

m = 1 -- index of current bit

do while m <= Xi

e = e – eminus -- update error

if e <= 0 then -- check if bit number m should be punctured

set bit xi,m to ** where **{0, 1}

e = e + eplus -- update error

end if

m = m + 1 -- next bit

end do

else

e = eini -- initial error between current and desired puncturing ratio

m = 1 -- index of current bit

do while m <= Xi

e = e – eminus -- update error

do while e <= 0 -- check if bit number m should be repeated

repeat bit *xi,m*

*e = e + eplus -- update error*

end do

*m = m + 1 -- next bit*

end do

end if

A repeated bit is placed directly after the original one.

### 4.2.8 TrCH multiplexing

Every 10 ms, one radio frame from each TrCH is delivered to the TrCH multiplexing. These radio frames are serially multiplexed into a coded composite transport channel (CCTrCH).

The bits input to the TrCH multiplexing are denoted by , where *i* is the TrCH number and *Vi* is the number of bits in the radio frame of TrCH *i*. The number of TrCHs is denoted by *I*. The bits output from TrCH multiplexing are denoted by , where *S* is the number of bits, i.e. . The TrCH multiplexing is defined by the following relations:

 *k =* 1, 2*, …, V*1

 *k = V*1*+*1*, V*1*+*2*, …, V*1*+V*2

 *k = (V*1*+V*2*)+*1*, (V*1*+V*2*)+*2*, …, (V*1*+V*2*)+V*3

**

 *k = (V*1*+V*2*+…+VI*-1*)+*1*, (V*1*+V*2*+…+VI*-1*)+*2*, …, (V*1*+V*2*+…+VI*-1*)+VI*

### 4.2.9 Insertion of discontinuous transmission (DTX) indication bits

In the downlink, DTX is used to fill up the radio frame with bits. The insertion point of DTX indication bits depends on whether fixed or flexible positions of the TrCHs in the radio frame are used. It is up to the UTRAN to decide for each CCTrCH whether fixed, pseudo-flexible (Subclause 4.2.7.2.1A), or flexible positions are used during the connection. DTX indication bits only indicate when the transmission should be turned off, they are not transmitted. Pseudo-flexible rate matching is always used when DL\_DCH\_FET\_Config is configured by higher layers. Otherwise pseudo-flexible rate matching is not used.

#### 4.2.9.1 1st insertion of DTX indication bits

This step of inserting DTX indication bits is used only if the positions of the TrCHs in the radio frame are fixed. With fixed position scheme a fixed number of bits is reserved for each TrCH in the radio frame.

The bits from rate matching are denoted by , where *Gi* is the number of bits in one TTI of TrCH *i*. Denote the number of bits in one radio frame of TrCH *i* by *Hi*. Denote *Di* the number of bits output of the first DTX insertion block.

In TTIs containing no compressed frames or frames compressed by spreading factor reduction, *Hi* is constant and corresponds to the maximum number of bits from TrCH *i* in one radio frame for any transport format of TrCH *i* and *Di* *=* *Fi*  *Hi*.

The bits output from the DTX insertion are denoted by *h i1, h i2, h i3, …, h iDi* Note that these bits are three valued. They are defined by the following relations:

* k =* 1, 2, 3, …, *Gi*

* k = Gi+*1*, Gi+*2*, Gi+*3*, …, Di*

where DTX indication bits are denoted by **. Here *gik* {0, 1}and ** {0, 1}.

In pseudo-flexible rate matching, the 1st insertion of DTX indication bits is the same as the above for fixed position rate matching, with a difference that the above procedure is applied to each TTI independently of others.

#### 4.2.9.2 2nd insertion of DTX indication bits

The DTX indication bits inserted in this step shall be placed at the end of the radio frame. Note that the DTX will be distributed over all slots after 2nd interleaving.

The bits input to the DTX insertion block are denoted by ,where *S* is the number of bits from TrCH multiplexing. The number of PhCHs is denoted by *P* and the number of bits in one radio frame, including DTX indication bits, for each PhCH by *R*..

In non-compressed frames, , where *Ndata*1 and *Ndata*2 are defined in [2].

For compressed frames, *N'data,\** is defined as . and  are the number of bits in the data fields of the slot format used for the current compressed frame, i.e. slot format A or B as defined in [2] corresponding to the spreading factor and the number of transmitted slots in use.

In frames compressed by higher layer scheduling, additional DTX with respect to normal mode shall be inserted if the transmission time reduction does not exactly create a transmission gap of the desired *TGL*.

The number of bits available to the CCTrCH in one radio frame compressed by spreading factor reduction or by higher layer scheduling is denoted by  and .

For frames compressed by spreading factor reduction .

For frames compressed by higher layer scheduling the exact value of  is dependent on the *TGL* which is signalled from higher layers. It can be calculated as.

*NTGL* is the number of bits that are located within the transmission gap and defined as:

|  |  |
| --- | --- |
|  | , if *Nfirst + TGL*  15  , in first frame if *Nfirst + TGL* > 15  , in second frame if *Nfirst + TGL* > 15 |

*Nfirst* and *TGL* are defined in subclause 4.4.

The bits output from the DTX insertion block are denoted by . Note that these bits are three valued. They are defined by the following relations:

 k = 1, 2, 3, …, S

 k = S+1, S+2, S+3, …, *PR*

where DTX indication bits are denoted by **. Here *s*k {0,1, p}and ** {0,1}.

### 4.2.10 Physical channel segmentation

When more than one PhCH is used, physical channel segmentation divides the bits among the different PhCHs. The bits input to the physical channel segmentation are denoted by , where *X* is the number of bits input to the physical channel segmentation block. The number of PhCHs is denoted by *P.*

The bits after physical channel segmentation are denoted , where *p* is PhCH number and *U* is the number of bits in one radio frame for each PhCH, i.e. **. The relation between *xk* and *up,k* is given below.

For all modes, some bits of the input flow are mapped to each code until the number of bits on the code is *U*. All bits of the input flow are taken to be mapped to the codes.

Bits on first PhCH after physical channel segmentation:

*u1, k = xk k =* 1, 2 , …, *U*

Bits on second PhCH after physical channel segmentation:

*u2, k = xk+U*  *k =* 1, 2 , …, *U*

…

Bits on the *Pth* PhCH after physical channel segmentation:

*uP,k = x k+(P-1)**U* *k =* 1, 2 , …, *U*

#### 4.2.10.1 Relation between input and output of the physical segmentation block in uplink

The bits input to the physical segmentation are denoted by . Hence, *xk = sk* and *Y = S*.

#### 4.2.10.2 Relation between input and output of the physical segmentation block in downlink

The bits input to the physical segmentation are denoted by . Hence, *xk = wk* and *Y = PU*.

### 4.2.11 2nd interleaving

The 2nd interleaving is a block interleaver and consists of bits input to a matrix with padding, the inter-column permutation for the matrix and bits output from the matrix with pruning. The bits input to the block interleaver are denoted by , where *p* is PhCH number and *U* is the number of bits in one radio frame for one PhCH. The output bit sequence from the block interleaver is derived as follows:

(1) Assign C2 *=* 30 to be the number of columns of the matrix. The columns of the matrix are numbered 0, 1, 2, …, C2 *-* 1 from left to right.

(2) Determine the number of rows of the matrix, R2, by finding minimum integer R2such that:

*U* ** R2  C2*.*

The rows of rectangular matrix are numbered 0, 1, 2, …, R2 - 1 from top to bottom.

(3) Write the input bit sequence  into the R2 ** C2 matrix row by row starting with bit  in column 0 of row 0:



where  for *k* = 1, 2, …, *U* and if R2  C2 > *U*, the dummy bits are padded such that  = 0 or 1 for *k* = *U* + 1, *U* + 2, …, R2  C2. These dummy bits are pruned away from the output of the matrix after the inter-column permutation.

(4) Perform the inter-column permutation for the matrix based on the pattern  that is shown in table 7, where P2(*j*) is the original column position of the *j*-th permuted column. After permutation of the columns, the bits are denoted by .



(5) The output of the block interleaver is the bit sequence read out column by column from the inter-column permuted R2 ** C2 matrix. The output is pruned by deleting dummy bits that were padded to the input of the matrix before the inter-column permutation, i.e. bits  that corresponds to bits  with *k>U* are removed from the output. The bits after 2nd interleaving are denoted by , where *vp,*1 corresponds to the bit  with smallest index *k* after pruning, *vp,*2 to the bit  with second smallest index *k* after pruning, and so on.

Table 7 Inter-column permutation pattern for 2nd interleaving

|  |  |
| --- | --- |
| Number of columns C2 | Inter-column permutation pattern  < P2(0), P2(1), …, P2(C2-1) > |
| 30 | <0, 20, 10, 5, 15, 25, 3, 13, 23, 8, 18, 28, 1, 11, 21,  6, 16, 26, 4, 14, 24, 19, 9, 29, 12, 2, 7, 22, 27, 17> |

#### 4.2.11.1 2nd interleaving for Secondary CCPCH with 16QAM

For MBSFN transmissions with 16QAM, the 2nd interleaving for Secondary CCPCH is done as illustrated in figure 8a below. The basic block interleaver is as described in Clause 4.2.11. For 16QAM modulated bits, there are two identical basic block interleavers of size R2×30, where R2 is the minimum integer fulfilling

,

The output bits from the physical channel segmentation are divided two by two between the interleavers: bits *up,k* and up,k+1 go to the first interleaver and bits *up,k+2* and *up,k+3* go to the second interleaver. Bits are collected two by two from the interleavers: bits *vp,k* and *vp,k+1*are obtained from the first interleaver and bits *vp,k+2* and *vp,k+3* are obtained from the second interleaver, where k mod 4=1.



Figure 8a: Interleaver structure for Secondary CCPCH

### 4.2.12 Physical channel mapping

The PhCH for both uplink and downlink is defined in [2]. The bits input to the physical channel mapping are denoted by , where *p* is the PhCH number and *U* is the number of bits in one radio frame for one PhCH. The bits *vp,k* are mapped to the PhCHs so that the bits for each PhCH are transmitted over the air in ascending order with respect to *k*.

In compressed mode, no bits are mapped to certain slots of the PhCH(s). If *Nfirst* + *TGL*  15, no bits are mapped to slots *Nfirst* to *Nlast*. If *Nfirst* + *TGL* > 15, i.e. the transmission gap spans two consecutive radio frames, the mapping is as follows:

- In the first radio frame, no bits are mapped to slots *Nfirst, Nfirst*+1, *Nfirst*+2, …, 14.

- In the second radio frame, no bits are mapped to the slots 0, 1, 2, …, *Nlast*.

*TGL, Nfirst*, and *Nlast* are defined in subclause 4.4.

#### 4.2.12.1 Uplink

When UL\_DPCH\_10ms\_Mode is configured, uplink physical channel mapping depends on whether a compressed-mode transmission gap overlaps with the first radio frame in 20ms CI. A distinction is made between the following cases:

##### 4.2.12.1.1 UL\_DPCH\_10ms\_Mode is not configured by higher layers, or, no compressed-mode transmission gap overlaps with the first radio frame in the 20ms CI

In uplink, the PhCHs used during a radio frame are either completely filled with bits that are transmitted over the air or not used at all. The only exception is when the UE is in compressed mode. The transmission can then be turned off during consecutive slots of the radio frame.

##### 4.2.12.1.2 UL\_DPCH\_10ms\_Mode is configured by higher layers, and, a compressed-mode transmission gap overlaps with the first radio frame in 20ms CI

In this case, physical channel mapping is performed over 20ms Compression Intervals (20m CI). Note that as a consequence of radio frame segmentation procedure in Subclause 4.2.6, there are no bit inputs to the second radio frame in one 20ms CI. Denote the bit inputs to the physical channel mapping in a 20ms CI by , where *p* is the PhCH number and *U* is the number of bits in one radio frame for one PhCH. Then, the 15 slots used to map the bits are the first 15 slots in the 20ms CI excluding slots in the compressed-mode transmission gap. In other words,

if *Nfirst* + *TGL*  15, i.e., the transmission gap spans only one radio frame, and the mapping is as follows

The 15 slots used for mapping are slots 0 to *Nfirst* – 1 in the first 10ms radio frame in the 20ms CI, slots *Nlast* + 1 to slot 14 in in the first 10ms radio frame in the 20ms CI, and slots 0 to TGL – 1 in the second radio frame of the 20ms CI.

Else if *Nfirst* + *TGL* > 15, i.e., the transmission gap spans two consecutive radio frames, the mapping is as follows:

If the transmission gap occurs at the beginning of the first radio frame of the 20ms CI, then the 15 slots used for mapping are slots *Nlast +* 1 to slot 14 of the first radio frame of the 20ms CI and slots 0 to *Nlast* of the second radio frame of the 20ms CI;

Else, if the transmission gap occurs at the end of the first radio frame of the 20ms CI, then the 15 slots used for mapping are slots 0 to *Nfirst –* 1 of the first radio frame of the 20ms CI and slots *Nlast* + 1 to *Nlast* + 15 - *Nfirst* of the second radio frame of the 20ms CI.

#### 4.2.12.2 Downlink

In downlink, the PhCHs do not need to be completely filled with bits that are transmitted over the air. Values *vp,k* {0, 1} correspond to DTX indicators, which are mapped to the DPCCH/DPDCH fields but are not transmitted over the air.

In compressed mode when DL\_DCH\_FET\_Config is configured by higher layers, the mapping of data bits onto the slots of the PhCH is the same as normal mode, with a difference that the data bits that are mapped to slots in a transmission gap are not transmitted over the air.

During compressed mode by reducing the spreading factor by 2, the data bits are always mapped into 7.5 slots within a compressed frame. No bits are mapped to the DPDCH field as follows:

If *Nfirst* + *TGL*  15, i.e. the transmission gap spans one radio frame,

if *Nfirst* + 7  14

no bits are mapped to slots *Nfirst*,*Nfirst* + 1, *Nfirst* +2,…, *Nfirst+6*

no bits are mapped to the first (NData1+ NData2)/2 bit positions of slot *Nfirst+7*

else

no bits are mapped to slots *Nfirst*, *Nfirst* + 1, *Nfirst* + 2,…, 14

no bits are mapped to slots *Nfirst* - 1, *Nfirst* - 2, *Nfirst* - 3, …, *8*

no bits are mapped to the last (NData1+ NData2)/2 bit positions of slot 7

end if

If *Nfirst* + *TGL* > 15, i.e. the transmission gap spans two consecutive radio frames,

In the first radio frame, no bits are mapped to last (NData1+ NData2)/2 bit positions in slot 7 as well as to slots 8, 9, 10, ..., 14.

In the second radio frame, no bits are mapped to slots 0, 1, 2, ..., 6 as well as to first (NData1+ NData2)/2 bit positions in slot 7.

NData1and NData2 are defined in [2].

### 4.2.13 Restrictions on different types of CCTrCHs

Restrictions on the different types of CCTrCHs are described in general terms in TS 25.302[11]. In this subclause those restrictions are given with layer 1 notation.

#### 4.2.13.1 Uplink Dedicated channel (DCH)

The maximum value of the number of TrCHs *I* in a CCTrCH, the maximum value of the number of transport blocks *Mi* on each transport channel, and the maximum value of the number of DPDCHs *P* are given from the UE capability class.

#### 4.2.13.2 Random Access Channel (RACH)

- There can only be one TrCH in each RACH CCTrCH, i.e. *I*=1, *sk = f*1*k* and *S* = *V*1.

- The maximum value of the number of transport blocks *M*1 on the transport channel is given from the UE capability class.

- The transmission time interval is either 10 ms or 20 ms.

- Only one PRACH is used, i.e. *P*=1, *u*1*k* = *sk*, and *U* = *S*.

- The Static rate matching parameter *RM*1 is not provided by higher layer signalling on the System information as the other transport channel parameters. Any value may be used as there is one transport channel in the CCTrCH, hence one transport channel per Transport Format Combination and no need to do any balancing between multiple transport channels.

#### 4.2.13.3 Void

#### 4.2.13.4 Downlink Dedicated Channel (DCH)

The maximum value of the number of TrCHs *I* in a CCTrCH, the maximum value of the number of transport blocks *Mi* on each transport channel, and the maximum value of the number of DPDCHs *P* are given from the UE capability class.

#### 4.2.13.5 Void

#### 4.2.13.6 Broadcast channel (BCH)

- There can only be one TrCH in a BCH CCTrCH, i.e. *I*=1, *sk = f*1*k*, and *S* = *V*1.

- There can only be one transport block in each transmission time interval, i.e. *M*1 = 1.

- All transport format attributes have predefined values which are provided in [11] apart from the rate matching *RM*1.

- The Static rate matching parameter *RM*1 is not provided by higher layer signalling neither fixed. Any value may be used as there is one transport channel in the CCTrCH, hence one transport channel per Transport Format Combination and no need to do any balancing between multiple transport channels.

- Only one primary or secondary CCPCH is used per CCTrCH, i.e. *P*=1.

#### 4.2.13.7 Forward access and paging channels (FACH and PCH)

- The maximum value of the number of TrCHs *I* in a CCTrCH and the maximum value of the number of transport blocks *Mi* on each transport channel are given from the UE capability class.

- The transmission time interval for TrCHs of PCH type is always 10 ms.

- Only one secondary CCPCH is used per CCTrCH, i.e. *P*=1.

#### 4.2.13.8 High Speed Downlink Shared Channel (HS-DSCH) associated with a DCH

- There can be only one TrCH in an HS-DSCH CCTrCH, i.e. *I* = 1,

- In case the UE is not configured in MIMO mode and not in MIMO mode with four transmit antennas or the UE is configured in MIMO mode and single-stream restriction is configured, there can only be one transport block in each transmission time interval, i.e. *M1* = 1. In case the UE is configured in MIMO mode, there can be one or two transport blocks in each transmission time interval and in case the UE is configured in MIMO mode with four transmit antennas, there can be up to four transport blocks in each transmission time interval.

- The transmission time interval for TrCHs of HS-DSCH type is always 2 ms.

- The maximum value of the number of HS-PDSCHs *P* are given from the UE capability class.

#### 4.2.13.9 Enhanced Dedicated Channel (E-DCH)

- There can be only one TrCH in the E-DCH CCTrCH, i.e. *I* = 1.

- If the UL\_MIMO\_Enabled is not set to TRUE, there can only be one transport block in each transmission time interval, i.e. *M1* = 1. If the UL\_MIMO\_Enabled is set to TRUE, there can be one or two transport blocks in each transmission time interval..

- The transmission time interval for TrCHs of E-DCH type is 2 ms or 10 ms. If the UL\_MIMO\_Enabled is set to TRUE, the transmission time interval for TrCHs of E-DCH type is always set to 2 ms.

- The maximum value of the number of E-DPDCHs *P* are given from the UE capabilities.

### 4.2.14 Multiplexing of different transport channels into one CCTrCH, and mapping of one CCTrCH onto physical channels

The following rules shall apply to the different transport channels which are part of the same CCTrCH:

1) Transport channels multiplexed into one CCTrCh shall have co-ordinated timings. When the TFCS of a CCTrCH is changed because one or more transport channels are added to the CCTrCH or reconfigured within the CCTrCH, or removed from the CCTrCH, the change may only be made at the start of a radio frame with CFN fulfilling the relation

CFN mod Fmax = 0,

where Fmax denotes the maximum number of radio frames within the transmission time intervals of all transport channels which are multiplexed into the same CCTrCH, including any transport channels *i* which are added, reconfigured or have been removed, and CFN denotes the connection frame number of the first radio frame of the changed CCTrCH.

After addition or reconfiguration of a transport channel *i* within a CCTrCH, the TTI of transport channel *i* may only start in radio frames with CFN fulfilling the relation:

CFN mod Fi = 0.

2) Only transport channels with the same active set can be mapped onto the same CCTrCH.

3) Different CCTrCHs cannot be mapped onto the same PhCH.

4) One CCTrCH shall be mapped onto one or several PhCHs. These physical channels shall all have the same SF, except for the case of four E-DPDCHs, where two E-DPDCHs have spreading factor 2 and the other two E-DPDCHs have spreading factor 4, and for the case of four S-E-DPDCHs, where two S-E-DPDCHs have spreading factor 2 and the other two S-E-DPDCHs have spreading factor 4.

All physical channels belonging to the same CCTrCH shall use the same modulation scheme with the exception that, when transmitted, the modulation scheme used by the four S-E-DPDCHsmay be different from that used by the four E-DPDCHs.

The 4PAM modulation shall only be used for orthogonal PhCH pairs which are orthogonal in phase and use the same OVSF code.

The 8PAM modulation shall only be used for orthogonal PhCH pairs which are orthogonal in phase and use the same OVSF code.

5) Dedicated Transport channels and common transport channels cannot be multiplexed into the same CCTrCH.

6) For the common transport channels, only the FACH and PCH may belong to the same CCTrCH.

There are hence two types of CCTrCH:

1) CCTrCH of dedicated type, corresponding to the result of coding and multiplexing of one or several DCHs or one E-DCH.

2) CCTrCH of common type, corresponding to the result of the coding and multiplexing of a common channel, RACH in the uplink, HS-DSCH, BCH, or FACH/PCH for the downlink.

#### 4.2.14.1 Allowed CCTrCH combinations for one UE

##### 4.2.14.1.1 Allowed CCTrCH combinations on the uplink

The following CCTrCH combinations for one UE are allowed:

1) one CCTrCH of dedicated type or

1a) two CCTrCHs of dedicated type, one being of DCH type and the other one of E-DCH type or

2) one CCTrCH of common type.

##### 4.2.14.1.2 Allowed CCTrCH combinations on the downlink

The following CCTrCH combinations for one UE are allowed:

- x CCTrCH of dedicated type + y CCTrCH of common type. The allowed combination of CCTrCHs of dedicated and common type are given from UE radio access capabilities. There can be a maximum of one CCTrCH of common type for HS-DSCH. The maximum number of CCTrCHs of common type for FACH is determined from UE capabilities. With one CCTrCH of common type for HS-DSCH, there shall be only one CCTrCH of dedicated type.

NOTE 1: There is only one DPCCH in the uplink, hence one TPC bits flow on the uplink to control possibly the different DPDCHs on the downlink, part of the same or several CCTrCHs.

NOTE 2: There is only one DPCCH in the downlink, even with multiple CCTrCHs. With multiple CCTrCHs, the DPCCH is transmitted on one of the physical channels of that CCTrCH which has the smallest SF among the multiple CCTrCHs. Thus there is only one TPC command flow and only one TFCI word in downlink even with multiple CCTrCHs.

NOTE 3: in the current release, only 1 CCTrCH of dedicated type is supported.

## 4.3 Transport format detection

If the transport format set of a TrCH *i* contains more than one transport format, the transport format can be detected according to one of the following methods:

- TFCI based detection: This method is applicable when the transport format combination is signalled using the TFCI field;

- explicit blind detection: This method typically consists of detecting the TF of TrCH *i* by use of channel decoding and CRC check;

- guided detection: This method is applicable when there is at least one other TrCH *i'*, hereafter called guiding TrCH, such that:

- the guiding TrCH has the same TTI duration as the TrCH under consideration, i.e. Fi' = Fi;

- different TFs of the TrCH under consideration correspond to different TFs of the guiding TrCH;

- explicit blind detection is used on the guiding TrCH.

If the transport format set for a TrCH *i* does not contain more than one transport format with more than zero transport blocks, no explicit blind transport format detection needs to be performed for this TrCH. The UE can use guided detection for this TrCH or single transport format detection, where the UE always assumes the transport format corresponding to more than zero transport blocks for decoding.

For uplink, blind transport format detection is a network controlled option. For downlink, the UE shall be capable of performing blind transport format detection, if certain restrictions on the configured transport channels are fulfilled.

### 4.3.1 Blind transport format detection

When no TFCI is available then explicit blind detection or guided detection shall be performed on all TrCHs within the CCTrCH that have more than one transport format and that do not use single transport format detection. The UE shall only be required to support blind transport format detection if all of the following restrictions are fulfilled:

1. either only one CCTrCH is received, or one CCTrCH of dedicated type and one CCTrCH of common type for HS-DSCH are received by the UE;

If only one CCTrCH is received by the UE, the following conditions apply to that CCTrCH and those TrCHs that are multiplexed on the CCTrCH. If one CCTrCH of dedicated type and one CCTrCH of common type for HS-DSCH are received by the UE, the following conditions apply to the dedicated type CCTrCH and the TrCHs that are multiplexed on the dedicated type CCTrCH.

2. the number of CCTrCH bits received per radio frame is 600 or less;

3. the number of transport format combinations of the CCTrCH is 64 or less;

4. fixed positions of the transport channels is used on the CCTrCH to be detectable;

5. convolutional coding is used on all explicitly detectable TrCHs;

6. CRC with non-zero length is appended to all transport blocks on all explicitly detectable TrCHs;

7. at least one transport block shall be transmitted per TTI on each explicitly detectable TrCH;

8. the number of explicitly detectable TrCHs is 3 or less;

9. for all explicitly detectable TrCHs *i*, the number of code blocks in one TTI (Ci) shall not exceed 1;

10. the sum of the transport format set sizes of all explicitly detectable TrCHs, is 16 or less. The transport format set size is defined as the number of transport formats within the transport format set;

11. there is at least one TrCH that can be used as the guiding transport channel for all transport channels using guided detection.

Examples of blind transport format detection methods are given in annex A.

### 4.3.1A Single transport format detection

When no TFCI is available, then single transport format detection shall be applied on all TrCHs within the CCTrCH that have a transport format set not containing more than one transport format with more than zero transport blocks and that do not use guided detection. The UE shall only be required to support single transport format detection if the following restrictions are fulfilled:

1. For each transport channel that is single transport format detected, CRC with non-zero length is appended to all transport blocks within the non-zero transport block transport format;

2. fixed positions of the transport channels is used on the CCTrCH to be detectable.

### 4.3.2 Transport format detection based on TFCI

If a TFCI is available, then TFCI based detection shall be applicable to all TrCHs within the CCTrCH. The TFCI informs the receiver about the transport format combination of the CCTrCHs. As soon as the TFCI is detected, the transport format combination, and hence the transport formats of the individual transport channels are known.

If higher layers indicate that S-CCPCHs can be soft combined during a period of consecutive TTIs, then the same TFC is used on those S-CCPCHs for each combinable TTI. The UE may therefore detect TFCI on one S-CCPCH to determine the TFC on all S-CCPCHs that can be soft combined. (S-CCPCH soft combining is further specified in [4]).

### 4.3.3 Coding of Transport-Format-Combination Indicator (TFCI)

The TFCI is encoded using a (32, 10) sub-code of the second order Reed-Muller code. The coding procedure is as shown in figure 9.



Figure 9: Channel coding of TFCI information bits

If the TFCI consist of less than 10 bits, it is padded with zeros to 10 bits, by setting the most significant bits to zero. The length of the TFCI code word is 32 bits.

The code words of the (32,10) sub-code of second order Reed-Muller code are linear combination of 10 basis sequences. The basis sequences are as in the following table 8.

Table 8: Basis sequences for (32,10) TFCI code

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| i | Mi,0 | Mi,1 | Mi,2 | Mi,3 | Mi,4 | Mi,5 | Mi,6 | Mi,7 | Mi,8 | Mi,9 |
| 0 | 1 | 0 | 0 | 0 | 0 | 1 | 0 | 0 | 0 | 0 |
| 1 | 0 | 1 | 0 | 0 | 0 | 1 | 1 | 0 | 0 | 0 |
| 2 | 1 | 1 | 0 | 0 | 0 | 1 | 0 | 0 | 0 | 1 |
| 3 | 0 | 0 | 1 | 0 | 0 | 1 | 1 | 0 | 1 | 1 |
| 4 | 1 | 0 | 1 | 0 | 0 | 1 | 0 | 0 | 0 | 1 |
| 5 | 0 | 1 | 1 | 0 | 0 | 1 | 0 | 0 | 1 | 0 |
| 6 | 1 | 1 | 1 | 0 | 0 | 1 | 0 | 1 | 0 | 0 |
| 7 | 0 | 0 | 0 | 1 | 0 | 1 | 0 | 1 | 1 | 0 |
| 8 | 1 | 0 | 0 | 1 | 0 | 1 | 1 | 1 | 1 | 0 |
| 9 | 0 | 1 | 0 | 1 | 0 | 1 | 1 | 0 | 1 | 1 |
| 10 | 1 | 1 | 0 | 1 | 0 | 1 | 0 | 0 | 1 | 1 |
| 11 | 0 | 0 | 1 | 1 | 0 | 1 | 0 | 1 | 1 | 0 |
| 12 | 1 | 0 | 1 | 1 | 0 | 1 | 0 | 1 | 0 | 1 |
| 13 | 0 | 1 | 1 | 1 | 0 | 1 | 1 | 0 | 0 | 1 |
| 14 | 1 | 1 | 1 | 1 | 0 | 1 | 1 | 1 | 1 | 1 |
| 15 | 1 | 0 | 0 | 0 | 1 | 1 | 1 | 1 | 0 | 0 |
| 16 | 0 | 1 | 0 | 0 | 1 | 1 | 1 | 1 | 0 | 1 |
| 17 | 1 | 1 | 0 | 0 | 1 | 1 | 1 | 0 | 1 | 0 |
| 18 | 0 | 0 | 1 | 0 | 1 | 1 | 0 | 1 | 1 | 1 |
| 19 | 1 | 0 | 1 | 0 | 1 | 1 | 0 | 1 | 0 | 1 |
| 20 | 0 | 1 | 1 | 0 | 1 | 1 | 0 | 0 | 1 | 1 |
| 21 | 1 | 1 | 1 | 0 | 1 | 1 | 0 | 1 | 1 | 1 |
| 22 | 0 | 0 | 0 | 1 | 1 | 1 | 0 | 1 | 0 | 0 |
| 23 | 1 | 0 | 0 | 1 | 1 | 1 | 1 | 1 | 0 | 1 |
| 24 | 0 | 1 | 0 | 1 | 1 | 1 | 1 | 0 | 1 | 0 |
| 25 | 1 | 1 | 0 | 1 | 1 | 1 | 1 | 0 | 0 | 1 |
| 26 | 0 | 0 | 1 | 1 | 1 | 1 | 0 | 0 | 1 | 0 |
| 27 | 1 | 0 | 1 | 1 | 1 | 1 | 1 | 1 | 0 | 0 |
| 28 | 0 | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 0 |
| 29 | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 |
| 30 | 0 | 0 | 0 | 0 | 0 | 1 | 0 | 0 | 0 | 0 |
| 31 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 0 | 0 | 0 |

When UL\_DPCH\_10ms\_Mode is not configured by higher layers, the TFCI information bits a0 , a1 , a2 , a3 , a4 , a5 , a6 , a7 , a8 , a9 (where a0 is LSB and a9 is MSB) shall correspond to the TFC index (expressed in unsigned binary form) defined by the RRC layer to reference the TFC of the CCTrCH in the associated DPCH radio frame.

When UL\_DPCH\_10ms\_Mode is configured by higher layers, the TFCI information bits a0 , a1 , a2 , a3 , a4 , a5 , a6 , a7 , a8 , a9 (where a0 is LSB and a9 is MSB) shall correspond to unsigned binary expression of the sum of the TFC index and the size of TFCS.

The output code word bits bi are given by:



where *i* = 0, …, 31.

The output bits are denoted by *bk*, *k* = 0, 1, 2, …, 31.

In downlink, when the SF < 128 the encoded TFCI code words are repeated yielding 8 encoded TFCI bits per slot in normal mode and 16 encoded TFCI bits per slot in compressed mode. Mapping of repeated bits to slots is explained in subclause 4.3.5.

### 4.3.4 Void

### 4.3.5 Mapping of TFCI words

#### 4.3.5.1 Mapping of TFCI word in normal mode in downlink, and in uplink when uplink DPCCH slot format is not 5

The bits of the code word are directly mapped to the slots of the radio frame. Within a slot the bit with lower index is transmitted before the bit with higher index. The coded bits *bk*, are mapped to the transmitted TFCI bits *dk*, according to the following formula:

*dk* = *bk* mod 32

For uplink physical channels regardless of the SF and downlink physical channels, if SF128, *k* = 0, 1, 2, …, 29. Note that this means that bits *b30* and *b31* are not transmitted.

For downlink physical channels whose SF < 128, *k* = 0, 1, 2, …, 119. Note that this means that bits *b0* to *b23* are transmitted four times and bits *b24* to *b31* are transmitted three times.

#### 4.3.5.1A Mapping of TFCI word in normal mode in uplink when uplink DPCCH slot format is 5

In each 20ms CI, the first 10 slots of uplink DPCCH contain TFCI bits. The bits of the codeword are directly mapped to the slots of the radio frame. Within a slot, the bit with lower index is transmitted before the bit with higher index. The coded bits *bk*, are mapped to the transmitted TFCI bits *dk*, according to the following formula:

*dk* = *bk, ,* for *k* = 0,…, 19*.*

##### 4.3.5.1.1 Mapping of TFCI bits for Secondary CCPCH with 16QAM

For MBSFN transmissions with 16QAM, the coded bits *bk*, are mapped to the transmitted TFCI bits according to the following formulas:

*d4k* = *b*2k mod 32  ,

*d4k+*1 = *b2k*+1 mod 32 ,

*d4k+*2 = ( *d4k* *+ d4k+*1 ) mod 2,

*d4k+*3 = (1 *+ d4k* *+ d4k+*1 ) mod 2,

where *k* = 0, 1, 2,…, 59 for SF < 128 and *k* = 0, 1, 2,…, 14 for SF128.

#### 4.3.5.2 Mapping of TFCI word in compressed mode

The mapping of the TFCI bits in compressed mode is different for uplink, downlink with SF  128 and downlink with SF < 128.

##### 4.3.5.2.1 Uplink compressed mode

4.3.5.2.1.1 Uplink DPCCH slot formats other than 5

For uplink compressed mode, the slot format is changed so that no TFCI coded bits are lost. The different slot formats in compressed mode do not match the exact number of TFCI coded bits for all possible TGLs. Repetition of the TFCI bits is therefore used.

Denote the number of bits available in the TFCI fields of one compressed radio frame by *D* and the number of bits in the TFCI field in a slot by NTFCI. The parameter *E* is used to determine the number of the first TFCI bit to be repeated.

*E*= Nfirst NTFCI, if the start of the transmission gap is allocated to the current frame.

*E* = *0*, if the start of the transmission gap is allocated to the previous frame and the end of the transmission gap is allocated to the current frame.

The TFCI coded bits *bk* are mapped to the bits in the TFCI fields *dk*. The following relations define the mapping for each compressed frame.

*dk* = *bk*

where *k* = 0, 1, 2, …, min (31, *D*-1).

If *D* > 32, the remaining positions are filled by repetition (in reversed order):

*dD-k*-1 = *b*(*E+k*) mod 32

where *k* = 0, …, *D*-33.

4.3.5.2.1.2 Uplink DPCCH slot format 5

In each 20ms CI, the first 10 UL DPCCH slots that are not in a compressed mode transmission gap contain TFCI information. The bits of the codeword are directly mapped to these slots. Within a slot, the bit with lower index is transmitted before the bit with higher index. The coded bits *bk*, are mapped to the transmitted TFCI bits *dk*, according to the following formula:

*dk* = *bk, ,* for *k* = 0,…, 19*.*

##### 4.3.5.2.2 Downlink compressed mode

For downlink compressed mode, the slot format is changed so that no TFCI coded bits are lost. The different slot formats in compressed mode do not match the exact number of TFCI bits for all possible TGLs. DTX is therefore used if the number of bits available in the TFCI fields in one compressed frame exceeds the number of TFCI bits given from the slot format. The block of bits in the TFCI fields where DTX is used starts on the first TFCI field after the transmission gap. If there are more bits available in the TFCI fields before the transmission gap than TFCI bits, DTX is also used on the bits in the last TFCI fields before the transmission gap.

Denote the number of bits available in the TFCI fields of one compressed radio frame by *D* and the number of bits in the TFCI field in a slot by NTFCI. The parameter *E* is used to determine the position of the first bit in the TFCI field on which DTX is used.

*E* = Nfirst NTFCI, if the start of the transmission gap is allocated to the current frame.

*E* = 0, if the start of the transmission gap is allocated to the previous frame and the end of the transmission gap is allocated to the current frame.

Denote the total number of TFCI bits to be transmitted by *F*. *F* = 32 for slot formats *n*A or *n*B, where *n* = 0, 1, …, 11 (see table 11 in [2]). Otherwise, *F* = 128. The TFCI coded bits *bk* are mapped to the bits in the TFCI fields *dk*. The following relations define the mapping for each compressed frame.

If *E* > 0,

*dk* = *bk* mod 32

where *k* = 0, 1, 2, …, min (*E*, *F*)-1.

If *E* < *F*,

*dk+D-F* = *bk* mod 32

where *k* = *E*, ..., *F* -1.

DTX is used on *dk* where *k* = min (*E*, *F*), ..., min (*E*, *F*) +*D* - *F* -1.

## 4.3A Mapping of DL FET ACK/NACK bits

When slot format 5 is used for uplink DPCCH, TFCI fields in each 20ms TTI contain DL FET ACK/NACK indicators in all transmitted slots that do not contain TFCI bits (see subclauses 4.3.5.1A and 4.3.5.2.1.2). Each DL FET ACK/NACK indicator is encoded as specified in Table 9. When DL\_DCH\_FET\_Config = 0, the bits that replace DL FET ACK/NACK indicators are unspecified.

Table 9: ACK/NACK transmission on uplink DPCCH

|  |  |
| --- | --- |
| DL FET ACK/NACK indicator | bits in slot *i* |
| ACK | 1 |
| NACK | 0 |

Let the slots in a 20ms CI be numbered 0,1,…29. For each *i* =0,1,…29, if slot *i* is not in a compressed-mode gap and does not contain TFCI bits, then a DL FET NACK indicator is transmitted in slot *i* if at least one of the following conditions holds:

a) At least one of the transport blocks transmitted on downlink DPDCH with a TTI that includes slot *i* has not been successfully decoded by the UE.

b) *i* belongs in the set S={11, 13, 15, 17, 19, 21, 23, 25, 27, 29}, and a DL FET ACK indication has not been sent in any prior slot *j,*0 *≤ j* < *i,* in this 20ms TTI.

c) A downlink slot containing bits of a non-zero transport block of a maximum TTI TrCH overlaps with slot i.

A DL FET ACK indicator is sent in all transmitted UL DPCCH slots that do not fall in a compressed mode gap and do not contain a DL FET NACK indicator or TFCI bit. If a 20ms CI contains a DL FET ACK indication, it always contains at least two slots carrying a DL FET ACK indication.

## 4.4 Compressed mode

In compressed frames, TGL slots from Nfirst to Nlast are not used for transmission of data. As illustrated in figure 11, the instantaneous transmit power is increased in the compressed frame in order to keep the quality (BER, FER, etc.) unaffected by the reduced processing gain. The amount of power increase depends on the transmission time reduction method (see subclause 4.4.3). What frames are compressed, are decided by the network. When in compressed mode, compressed frames can occur periodically, as illustrated in figure 11, or requested on demand. The rate and type of compressed frames is variable and depends on the environment and the measurement requirements.



Figure 11: Compressed mode transmission

### 4.4.1 Frame structure in the uplink

The frame structure for uplink compressed frames is illustrated in figure 12.



Figure 12: Frame structure in uplink compressed transmission

### 4.4.2 Frame structure types in the downlink

There are two different types of frame structures defined for downlink compressed frames. Type A maximises the transmission gap length and type B is optimised for power control. The frame structure type A or B is set by higher layers independent from the downlink slot format type A or B.

- With frame structure of type A, the pilot field of the last slot in the transmission gap is transmitted. Transmission is turned off during the rest of the transmission gap (figure 13(a)). In case the length of the pilot field is 2 bits and STTD is used on the radio link, the pilot bits in the last slot of the transmission gap shall be STTD encoded assuming DTX indicators as the two last bits in the Data2 field.

- With frame structure of type B, the TPC field of the first slot in the transmission gap and the pilot field of the last slot in the transmission gap is transmitted. Transmission is turned off during the rest of the transmission gap (figure 13(b)). In case the length of the pilot field is 2 bits and STTD is used on the radio link, the pilot bits in the last slot of the transmission gap shall be STTD encoded assuming DTX indicators as the two last bits of the Data2 field. Similarly, the TPC bits in the first slot of the transmission gap shall be STTD encoded assuming DTX indicators as the two last bits in the Data1 field.



(a) Frame structure type A



(b) Frame structure type B

Figure 13: Frame structure types in downlink compressed transmission

### 4.4.2A Frame structure in the downlink for F-DPCH

There is only one type of frame structure defined for downlink F-DPCH compressed frames: transmission is turned off during the whole transmission gap i.e. in slots Nfirst to Nlast.

### 4.4.2B Frame structure in the downlink for F-TPICH

There is only one type of frame structure defined for downlink F-TPICH compressed frames: transmission is turned off during the whole transmission gap i.e. in slots Nfirst to Nlast. TPI will not be transmitted in either of the both slots in the case where only one of the two slots carrying the TPI information overlaps with the transmission gap.

### 4.4.3 Transmission time reduction method

When in compressed mode, the information normally transmitted during a 10 ms frame is compressed in time. The mechanisms provided for achieving this are reduction of the spreading factor by a factor of two , and higher layer scheduling. In the downlink and the uplink, all methods are supported. The maximum idle length is defined to be 7 slots per one 10 ms frame. The slot formats that are used in compressed frames are listed in [2].

In downlink when DL\_DCH\_FET\_Config is configured by higher layers, and in uplink when UL\_DPCH\_10ms\_Mode is configured by higher layers, the same slot format is used in compressed frames and normal frames.

In case F-DPCH is configured in the downlink, no transmission time reduction method is needed during compressed frames. The same slot format is used in compressed frames and normal frames.

#### 4.4.3.1 Void

#### 4.4.3.2 Compressed mode by reducing the spreading factor by 2

The spreading factor (SF) can be reduced by 2 during one compressed radio frame to enable the transmission of the information bits in the remaining time slots of the compressed frame. This method is not supported for SF=4.

On the downlink, UTRAN can also order the UE to use a different scrambling code in a compressed frame than in a non-compressed frame. If the UE is ordered to use a different scrambling code in a compressed frame, then there is a one-to-one mapping between the scrambling code used in the non-compressed frame and the one used in the compressed frame, as described in [3] subclause 5.2.1.

#### 4.4.3.3 Compressed mode by higher layer scheduling

Compressed frames can be obtained by higher layer scheduling. Higher layers then set restrictions so that only a subset of the allowed TFCs are used in a compressed frame. The maximum number of bits that will be delivered to the physical layer during the compressed radio frame is then known and a transmission gap can be generated. Note that in the downlink, the TFCI field is expanded on the expense of the data fields and this shall be taken into account by higher layers when setting the restrictions on the TFCs. Compressed mode by higher layer scheduling shall not be used with fixed starting positions of the TrCHs in the radio frame. Compressed mode by higher layer scheduling shall not be used when DL\_DCH\_FET\_Config is configured by higher layers.

### 4.4.4 Transmission gap position

Transmission gaps can be placed at different positions as shown in figures 14 and 15 for each purpose such as interfrequency power measurement, acquisition of control channel of other system/carrier, and actual handover operation.

The restrictions listed below apply to DPCCH/DPCCH2/S-DPCCH/DPDCH in the uplink and DPCH or F-DPCH in the downlink.

When using single frame method, the transmission gap is located within the compressed frame depending on the transmission gap length (TGL) as shown in figure 14 (1). When using double frame method, the transmission gap is located on the center of two connected frames as shown in figure 14 (2).



Figure 14: Transmission gap position

Parameters of the transmission gap positions are calculated as follows.

TGL is the number of consecutive idle slots during the compressed mode transmission gap:

TGL = 3, 4, 5, 7, 10, 14

Nfirst specifies the starting slot of the consecutive idle slots,

Nfirst = 0,1,2,3,…,14.

Nlast shows the number of the final idle slot and is calculated as follows;

If Nfirst + TGL  15, then Nlast = Nfirst + TGL –1 ( in the same frame ),

If Nfirst + TGL > 15, then Nlast = (Nfirst + TGL – 1) mod 15 ( in the next frame ).

When the transmission gap spans two consecutive radio frames, Nfirst and TGL must be chosen so that at least 8 slots in each radio frame are transmitted.



Figure 15: Transmission gap positions with different Nfirst

### 4.4.5 Transmission gap position for E‑DCH

In the following, the transmission gap position for E‑DCH during compressed frames is specified for the case when E‑DCH TTI length is 10 ms. Slots that are not idle due to uplink compressed mode are termed "available".

The parameter *nfirst* and *nlast* are used to determine the transmission gap position due to uplink compressed mode in the current radio frame. If the start of the transmission gap is allocated in the current frame *nfirst*=*Nfirst* else *nfirst*=0. If the end of a transmission gap is allocated in the current frame *nlast*=*Nlast* else *nlast*=14.

#### 4.4.5.1 E‑DPDCH Transmission Gap Position during Initial Transmissions

If an initial transmission overlaps with a compressed frame the starting slot of the consecutive E‑DPDCH idle slots within the E‑DCH TTI is *nfirst*, and *nlast* is the final idle slot within the 10 ms E‑DCH TTI. The number of transmitted slots *ntx1* is given by *ntx1*=14+*nfirst*-*nlast*.

If the initial transmission occurs in a non‑compressed uplink frame, *ntx1*=15.

#### 4.4.5.2 E‑DPDCH Transmission Gap Position during Retransmissions

If the current retransmission occurs in a compressed frame the maximum number of slots available for the retransmission is given by *nmax*=14+*nfirst*-*nlast*. Else the maximum number of slots available for the retransmission *nmax* is 15.

If the initial transmission was compressed and in the retransmission more than *ntx1* slots are available for transmission (*nmax*>*ntx1*), the last *ndtx*=*nmax*-*ntx1* available slots of the E‑DPDCH frame are E‑DPDCH idle slots. The parameter *ntx1* refers to the number of transmitted slots calculated as defined in 4.4.5.1 for the corresponding initial transmission.

The E‑DPDCH transmission gap in case a retransmission occurs in a compressed frame or a retransmission occurs in a non‑compressed frame for which initial transmission was compressed is defined as follows:

If *nmax*  *ntx1*

E‑DPDCH idle slots are slots *nfirst*, *nfirst*+1, .., *nlast*

Else

If a retransmission occurs in a compressed frame and *nfirst* < *ntx1*

E‑DPDCH idle slots are the slots *nfirst*, *nfirst*+1, .., *nlast* and 15-*ndtx*, 15-*ndtx*+1, ..,14

Else

E‑DPDCH idle slots are the slots *ntx1, ntx1+1,* ..,14

#### 4.4.5.3 E‑DPCCH Transmission Gap Position

If a transmission overlaps with an uplink compressed frame the starting slot of the compressed mode gap within the E‑DCH TTI is *nfirst*, and *nlast* is the final E‑DPCCH idle slot within the 10 ms E‑DCH TTI.

## 4.5 Coding for HS-DSCH

Data arrives to the coding unit in form of a maximum of one transport block once every transmission time interval. The transmission time interval is 2 ms which is mapped to a radio sub-frame of 3 slots.

The following coding steps can be identified:

- add CRC to each transport block (see subclause 4.5.1);

- bit scrambling (see subclause 4.5.1A);

- code block segmentation (see subclause 4.5.2);

- channel coding (see subclause 4.5.3);

- hybrid ARQ (see subclause 4.5.4);

- physical channel segmentation (see subclause 4.5.5);

- interleaving for HS-DSCH (see subclause 4.5.6);

- constellation re-arrangement for 16QAM and 64QAM (see subclause 4.5.7);

- mapping to physical channels (see subclause 4.5.8).

The coding steps for HS-DSCH are shown in the figure below.



Figure 16: Coding chain for HS-DSCH

In the following the number of transport blocks and the number of transport channels is always one i.e. m=1, i=1. When referencing non HS-DSCH formulae which are used in correspondence with HS-DSCH formulae the convention is used that transport block subscripts may be omitted (e.g. X1 may be written X).

### 4.5.1 CRC attachment for HS-DSCH

#### 4.5.1.1 CRC attachment method 1 for HS-DSCH

CRC attachment method 1 for the HS-DSCH transport channel shall be done using the general method described in 4.2.1 above with the following specific parameters.

The CRC length shall always be L1 = 24 bits.

#### 4.5.1.2 CRC attachment method 2 for HS-DSCH

CRC attachment method 2 for the HS-DSCH transport channel shall be done according to the following method.

From the sequence of bits *a1, a2, a3,…, aA* , where *A* is the size of the HS-DSCH transport block*,* a CRC of length L1 = 24 bits is calculated according to Clause 4.2.1.1 above. This gives a sequence of bits *cim1, cim2, cim3,…, cim24*  where

*k=1,2,…,24*

This sequence of bits is then masked with the UE Identity *xue,1, xue,2, …, xue,16* and then appended to the sequence of bits *a1, a2, a3,…, aA* to form the sequence of bits *b1, b2, b3,…, bB*, where *B* = *A* + 24, and

*bk = ak k=1,2,…,A*

*bk = ck-A k=A+1,…,A+8*

*bk =* (*ck-A* + *xue*,*k-A-8*) mod 2 *k=A+9, …,A+24*

### 4.5.1A Bit scrambling for HS-DSCH

The bits output from the HS-DSCH CRC attachment are scrambled in the bit scrambler. The bits input to the bit scrambler are denoted by , where *B* is the number of bits input to the HS-DSCH bit scrambler The bits after bit scrambling are denoted .

Bit scrambling is defined by the following relation:

*k* = 1,2,…,*B*

and results from the following operation:

-15 < *γ*< 1

*γ*= 1

,

where ,

*k* = 1,2,…,*B*.

### 4.5.2 Code block segmentation for HS-DSCH

Code block segmentation for the HS-DSCH transport channel shall be done with the general method described in 4.2.2.2 above with the following specific parameters.

There will be a maximum of one transport block, i=1. The bits *dim1, dim2, dim3,…dimB* input to the block are mapped to the bits xi1, xi2, xi3,…xiXi directly. It follows that X1 = B. Note that the bits x referenced here refer only to the internals of the code block segmentation function. The output bits from the code block segmentation function are oir1, oir2, oir3,…oirK.

The value of Z = 5114 for turbo coding shall be used.

### 4.5.3 Channel coding for HS-DSCH

Channel coding for the HS-DSCH transport channel shall be done with the general method described in 4.2.3 above with the following specific parameters.

There will be a maximum of one transport block, i=1. The rate 1/3 turbo coding shall be used.

### 4.5.4 Hybrid ARQ for HS-DSCH

The hybrid ARQ functionality matches the number of bits at the output of the channel coder to the total number of bits of the HS-PDSCH set to which the HS-DSCH is mapped. The hybrid ARQ functionality is controlled by the redundancy version (RV) parameters. The exact set of bits at the output of the hybrid ARQ functionality depends on the number of input bits, the number of output bits, and the RV parameters.

The hybrid ARQ functionality consists of two rate-matching stages and a virtual buffer as shown in the figure below.

The first rate matching stage matches the number of input bits to the virtual IR buffer, information about which is provided by higher layers. Note that, if the number of input bits does not exceed the virtual IR buffering capability, the first rate-matching stage is transparent.

The second rate matching stage matches the number of bits after first rate matching stage to the number of physical channel bits available in the HS-PDSCH set in the TTI.



Figure 17: HS-DSCH hybrid ARQ functionality

#### 4.5.4.1 HARQ bit separation

The HARQ bit separation function shall be performed in the same way as bit separation for turbo encoded TrCHs with puncturing in 4.2.7.4.1 above.

#### 4.5.4.2 HARQ First Rate Matching Stage

HARQ first stage rate matching for the HS-DSCH transport channel shall be done with the general method described in 4.2.7.2.2.3 above with the following specific parameters.

The maximum number of soft channel bits available in the virtual IR buffer is NIR which is signalled from higher layers for each HARQ process. The number of coded bits in a TTI before rate matching is NTTI this is deduced from information signalled from higher layers and parameters signalled on the HS-SCCH for each TTI. Note that HARQ processing and physical layer storage occurs independently for each HARQ process currently active.

If NIR is greater than or equal to NTTI (i.e. all coded bits of the corresponding TTI can be stored) the first rate matching stage shall be transparent. This can, for example, be achieved by setting *eminus* = 0. Note that no repetition is performed.

If NIR is smaller than NTTI the parity bit streams are punctured as in 4.2.7.2.2.3 above by setting the rate matching parameter where the subscripts i and l refer to transport channel and transport format in the referenced sub-clause. Note the negative value is expected when the rate matching implements puncturing. Bits selected for puncturing which appear as  in the algorithm in 4.2.7 above shall be discarded and not counted in the totals for the streams through the virtual IR buffer.

#### 4.5.4.3 HARQ Second Rate Matching Stage

HARQ second stage rate matching for the HS-DSCH transport channel shall be done with the general method described in 4.2.7.5 above with the following specific parameters. Bits selected for puncturing which appear as ** in the algorithm in 4.2.7.5 above shall be discarded and are not counted in the streams towards the bit collection.

The parameters of the second rate matching stage depend on the value of the RV parameters s and r. The parameter s can take the value 0 or 1 to distinguish between transmissions that prioritise systematic bits (s = 1) and non systematic bits (s = 0). The parameter r (range 0 to *rmax-1*) changes the initial error variable *eini* in the case of puncturing. In case of repetition both parameters *r* and *s* change the initial error variable *eini*. The parameters Xi, eplus and eminus are calculated as per table 10 below.

Denote the number of bits before second rate matching as *Nsys* for the systematic bits, *Np1*for the parity 1 bits, and *Np2* for the parity 2 bits, respectively. Denote the number of physical channels used for the HS-DSCH by *P*. *Ndata* is the number of bits available to the HS-DSCH in one TTI and defined as *Ndata*=*P*3*Ndata*1, where *Ndata1* is defined in [2]. The rate matching parameters are determined as follows.

For , puncturing is performed in the second rate matching stage. The number of transmitted systematic bits in a transmission is for a transmission that prioritises systematic bits and for a transmission that prioritises non systematic bits.

For repetition is performed in the second rate matching stage. A similar repetition rate in all bit streams is achieved by setting the number of transmitted systematic bits to .

The number of parity bits in a transmission is: and for the parity 1 and parity 2 bits, respectively.

Table 10 below summarizes the resulting parameter choice for the second rate matching stage.

Table 10: Parameters for HARQ second rate matching

|  |  |  |  |
| --- | --- | --- | --- |
|  | *Xi* | *eplus* | *eminus* |
| Systematic RM S |  |  |  |
| Parity 1 RM P1\_2 |  |  |  |
| Parity 2 RM P2\_2 |  |  |  |

The rate matching parameter *eini* is calculated for each bit stream according to the RV parameters r and s using

in the case of puncturing , i.e.,, and

for repetition, i.e., . Where and  is the total number of redundancy versions allowed by varying  as defined in 4.6.2. Note that rmax varies depending on the modulation mode, i.e. for 16QAM and 64QAM, *rmax* = 2 and for QPSK *rmax* = 4.

Note: For the modulo operation the following clarification is used: the value of (x mod y) is strictly in the range of 0 to *y*-1 (i.e. -1 mod 10 = 9).

#### 4.5.4.4 HARQ bit collection

The HARQ bit collection is achieved using a rectangular interleaver of size .

The number of rows and columns are determined from:

for 64QAM, for 16QAM and for QPSK

where *Ndata* is used as defined in 4.5.4.3.

Data is written into the interleaver column by column, and read out of the interleaver column by column starting from the first column.

*Nt,sys* is the number of transmitted systematic bits. Intermediate values *Nr* and *Nc* are calculated using:

and .

If *Nc*=0 and *Nr* > 0, the systematic bits are written into rows 1…*Nr*.

Otherwise systematic bits are written into rows 1…*Nr+1* in the first *Nc* columns and, if *Nr* > 0, also into rows 1…*Nr* in the remaining *Ncol-Nc* columns.

The remaining space is filled with parity bits. The parity bits are written column wise into the remaining rows of the respective columns. Parity 1 and 2 bits are written in alternating order, starting with a parity 2 bit in the first available column with the lowest index number.

In the case of 64QAM for each column the bits are read out of the interleaver in the order row 1, row 2, row 3, row 4, row 5, row 6. In the case of 16QAM for each column the bits are read out of the interleaver in the order row 1, row 2, row 3, row 4. In the case of QPSK for each column the bits are read out of the interleaver in the order row1, row2.

### 4.5.5 Physical channel segmentation for HS-DSCH

When more than one HS-PDSCH is used, physical channel segmentation divides the bits among the different physical channels. The bits input to the physical channel segmentation are denoted by w1, w2, w3,…wR, where Ris the number of bits input to the physical channel segmentation block. The number of PhCHs is denoted by *P.*

The bits after physical channel segmentation are denoted , where *p* is PhCH number and *U* is the number of bits in one radio sub-frame for each HS-PDSCH, i.e. . The relation between w*k* and *up,k* is given below.

For all modes, some bits of the input flow are mapped to each code until the number of bits on the code is *U*.

Bits on first PhCH after physical channel segmentation:

*u1, k = wk k =* 1, 2 , …, *U*

Bits on second PhCH after physical channel segmentation:

*u2, k = wk+U* *k =* 1, 2 , …, *U*

…

Bits on the *Pth* PhCH after physical channel segmentation:

*uP,k = wk+(P-1)**U* *k =* 1, 2 , …, *U*

### 4.5.6 Interleaving for HS-DSCH

The interleaving for FDD is done as shown in figure 18 below, separately for each physical channel. The bits input to the block interleaver are denoted by , where *p* is PhCH number and *U* is the number of bits in one TTI for one PhCH. For QPSK *U* = 960, for 16QAM *U* = 1920 and for 64QAM *U* = 2880. The basic interleaver is as the 2nd interleaver described in Clause 4.2.11. The interleaver is of fixed size: R2=32 rows and C2=30 columns.



Figure 18: Interleaver structure for HS-DSCH

For 16QAM, there are two identical interleavers of the same fixed size R2×C2 = 32×30. The output bits from the physical channel segmentation are divided two by two between the interleavers: bits *up,k* and up,k+1 go to the first interleaver and bits *up,k+2* and *up,k+3* go to the second interleaver. Bits are collected two by two from the interleavers: bits *vp,k* and *vp,k+1*are obtained from the first interleaver and bits *vp,k+2* and *vp,k+3* are obtained from the second interleaver, where k mod 4=1.

For 64QAM, there are three identical interleavers of the same fixed size R2×C2 = 32×30. The output bits from the physical channel segmentation are divided two by two between the interleavers: bits *up,k* and up,k+1 go to the first interleaver, bits *up,k+2* and *up,k+3* go to the second interleaver and bits *up,k+4* and *up,k+5* go to the third interleaver. Bits are collected two by two from the interleavers: bits *vp,k* and *vp,k+1*are obtained from the first interleaver, bits *vp,k+2* and *vp,k+3* are obtained from the second interleaver and bits *vp,k+4* and *vp,k+5* are obtained from the third interleaver, where k mod 6=1.

### 4.5.7 Constellation re-arrangement for 16 QAM and 64QAM

This function only applies to 16QAM and 64QAM modulated bits. In case of QPSK it is transparent.

Table 11 describes the operations that produce the different rearrangements for 16QAM. The bits of the input sequence are mapped in groups of 4 so that *vp,k, vp,k+1, vp,k+2, vp,k+3* are used, where k mod 4 = 1. The output bit sequences map to the output bits in groups of 4, i.e. *rp,k, rp,k+1, rp,k+2, rp,k+3*, where k mod 4 = 1.

Table 11: Constellation re-arrangement for 16QAM

|  |  |  |
| --- | --- | --- |
| constellation version parameter *b* | Output bit sequence | Operation |
| 0 |  | None |
| 1 |  | Swapping MSBs with LSBs |
| 2 |  | Inversion of the logical values of LSBs |
| 3 |  | Swapping MSBs with LSBs and inversion of logical values of LSBs |

Table 11A describes the operations that produce the different rearrangements for 64QAM. The bits of the input sequence are mapped in groups of 6 so that *vp,k, vp,k+1, vp,k+2, vp,k+3, vp,k+4, vp,k+5* are used, where k mod 6 = 1. The output bit sequences map to the output bits in groups of 6, i.e. *rp,k, rp,k+1, rp,k+2, rp,k+3, rp,k+4, rp,k+5*, where k mod 6 = 1.

Table 11A: Constellation re-arrangement for 64QAM

|  |  |  |
| --- | --- | --- |
| constellation version parameter *b* | Output bit sequence | Operation |
| 0 |  | None |
| 1 |  | Swapping MSBs and LSBs. Inversion of Middle SBs |
| 2 |  | Left circular shift of pair of SBs. Inversion of Middle SBs |
| 3 |  | Inversion of Middle SBs |

### 4.5.8 Physical channel mapping for HS-DSCH

The HS-PDSCH is defined in [2]. The bits input to the physical channel mapping are denoted by *rp,1*, *rp,2*,...,*rp,U*, where *p* is the physical channel number and *U* is the number of bits in one radio sub-frame for one HS-PDSCH. The bits *rp,k* are mapped to the PhCHs so that the bits for each PhCH are transmitted over the air in ascending order with respect to *k*.

## 4.6 Coding for HS-SCCH type 1

### 4.6.1 Overview

HS-SCCH shall be of type 1 when the following two conditions are both true:

- the UE is not configured in MIMO mode and not in MIMO mode with four transmit antennas, and

- the conditions for usage of HS-SCCH type 2 are not met.

In this section, the terms “HS-SCCH” and “HS-SCCH type 1” are used interchangeably.

The following information is transmitted by means of the HS-SCCH type 1 physical channel.

- Channelization-code-set information (7 bits): *xccs,1, xccs,2, …, xccs,7*

- Modulation scheme information (1 bit): *xms,1*

- Transport-block size information (6 bits): *xtbs,1, xtbs,2, …, xtbs,6*

- Hybrid-ARQ process information (3 bits): *xhap,1, xhap,2, xhap,3*

- Redundancy and constellation version (3 bits): *xrv,1, xrv,2, xrv,3*

- New data indicator (1 bit): *xnd,1*

- UE identity (16 bits): *xue,1, xue,2, …, xue,16*

For an HS-SCCH order,

- xccs,1, xccs,2, …, xccs,7, xms,1 shall be set to ''11100000’

- xtbs,1, xtbs,2, …, xtbs,4 shall be set to ''1111’

- xtbs,5, tbs,6 shall be set to xeodt,1, xeodt,2

- xhap,1, xhap,2, xhap,3, xrv,1, xrv,2, xrv,3 shall be set to xodt,1, xodt,2, xodt,3, xord,1, xord,2, xord,3

- xnd,1 is reserved

where *xeodt,1, xeodt,2, xodt,1, xodt,2, xodt,3, xord,1, xord,2, xord,3* are defined in subclause 4.6C.

Figure 19 below illustrates the overall coding chain for HS-SCCH type 1.



Figure 19: Coding chain for HS-SCCH type 1

### 4.6.2 HS-SCCH information field mapping

#### 4.6.2.1 Redundancy and constellation version coding

The redundancy version (RV) parameters *r*, *s* and constellation version parameter *b* are coded jointly to produce the value Xrv. Xrv is alternatively represented as the sequence xrv,1, xrv,2, xrv,3 where xrv,1 is the MSB. This is done according to tables 12 and 13 according to the modulation mode used:

Table 12: RV coding for 16QAM and 64QAM

|  |  |  |  |
| --- | --- | --- | --- |
| Xrv (value) | s | R | b |
| 0 | 1 | 0 | 0 |
| 1 | 0 | 0 | 0 |
| 2 | 1 | 1 | 1 |
| 3 | 0 | 1 | 1 |
| 4 | 1 | 0 | 1 |
| 5 | 1 | 0 | 2 |
| 6 | 1 | 0 | 3 |
| 7 | 1 | 1 | 0 |

Table 13: RV coding for QPSK

|  |  |  |
| --- | --- | --- |
| Xrv (value) | s | r |
| 0 | 1 | 0 |
| 1 | 0 | 0 |
| 2 | 1 | 1 |
| 3 | 0 | 1 |
| 4 | 1 | 2 |
| 5 | 0 | 2 |
| 6 | 1 | 3 |
| 7 | 0 | 3 |

#### 4.6.2.2 Modulation scheme mapping

The value of *xms,1* is derived from the modulation and given by the following:

#### 4.6.2.3 Channelization code-set mapping

The channelization code-set bits xccs,1, xccs,2, …, xccs,7 are coded according to the following:

Given P (multi-)codes starting at code O, and given the HS-SCCH number if 64QAM is configured for the UE and xms,1=1, calculate the information-field using the unsigned binary representation of integers calculated by the expressions,

for the first three bits (code group indicator) of which *xccs,1* is the MSB:

*xccs,1, xccs,2, xccs,3* = min(P-1,15-P)

If 64QAM is not configured for the UE, or if 64QAM is configured and xms,1=0, then

for the last four bits (code offset indicator) of which *xccs,4* is the MSB:

*xccs,4, xccs,5, xccs,6, xccs,7* = |O-1-P/8 \*15|

Otherwise (i.e. if 64QAM is configured for the UE and xms,1=1),

*P* and *O* shall fulfil |O-1-P/8 \*15| mod 2 = (HS‑SCCH number) mod 2, and then

*xccs,4, xccs,5, xccs,6, xccs,dummy* = |O-1-P/8 \*15|, where *xccs,dummy* is a dummy bit that is not transmitted on HS-SCCH.

Furthermore,

.

The definitions of P and O are given in [3]. The HS-SCCH number is given by the position in the list of HS-SCCH Channelisation Code Informations signalled by higher layers. The HS-SCCH number is associated with the code offset indicator and code group indicator as described above if 64QAM is configured for the UE and xms,1=1.

#### 4.6.2.4 UE identity mapping

The UE identity is the HS-DSCH Radio Network Identifier (H-RNTI) defined in [13]. This is mapped such that xue,1  corresponds to the MSB and xue,16 to the LSB, cf. [14].

#### 4.6.2.5 HARQ process identifier mapping

Hybrid-ARQ process information (3 bits) *xhap,1, xhap,2, xhap,3* is the unsigned binary representation of the HARQ process identifier where *xhap,1* is MSB.

#### 4.6.2.6 Transport block size index mapping

Transport-block size information (6 bits) *xtbs,1, xtbs,2, …, xtbs,6*  is unsigned binary representation of the transport block size index where *xtbs,1* is MSB.

### 4.6.3 Multiplexing of HS-SCCH information

The channelization-code-set information *xccs,1, xccs,2, …, xccs,7* and modulation-scheme information *xms,1* are multiplexed together. This gives a sequence of bits *x1,1, x1,2, …, x1,8* where

*x1,i = xccs,i i=1,2,…,7*

*x1,i = xms,i-7 i=8*

The transport-block-size information *xtbs,1, xtbs,2, …, xtbs,6*, Hybrid-ARQ-process information *xhap,1,xhap,2, xhap,3*, redundancy-version information *xrv,1, xrv,2*, xrv,3 and new-data indicator *xnd,1* are multiplexed together. This gives a sequence of bits *x2,1, x2,2, …, x2,13* where

*x2,i = xtbs,i i=1,2,…,6*

*x2,i = xhap,i-6 i=7,8,9*

*x2,i = xrv,i-9 i=10,11,12*

*x2,i = xnd,i-12 i=13*

### 4.6.4 CRC attachment for HS-SCCH

From the sequence of bits *x1,1, x1,2, …, x1,8, x2,1, x2,2, …, x2,13* a 16 bits CRC is calculated according to Clause 4.2.1.1. This gives a sequence of bits *c1, c2, …, c16* where

*k=1,2,…,16*

This sequence of bits is then masked with the UE Identity *xue,1, xue,2, …, xue,16* and then appended to the sequence of bits *x2,1, x2,2, …, x2,13* to form the sequence of bits *y1, y2, …, y29*, where

*yi = x2,i i=1,2,…,13*

*yi =* (*ci-13* + *xue*,i-13 ) mod 2 *i=14,15,…,29*

### 4.6.5 Channel coding for HS-SCCH

Rate 1/3 convolutional coding, as described in Clause 4.2.3.1, is applied to the sequence of bits x*1,1,x1,2, …,x1,8*. This gives a sequence of bits *z1,1, z1,2, …, z1,48*.

Rate 1/3 convolutional coding, as described in Clause 4.2.3.1, is applied to the sequence of bits *y1, y2, …, y29*. This gives a sequence of bits *z2,1, z2,2, …, z2,111*.

Note that the coded sequence lengths result from the termination of K=9 convolutional coding being fully applied.

### 4.6.6 Rate matching for HS-SCCH

From the input sequence *z1,1, z1,2, …, z1,48* the bits *z1,1, z1,2, z1,4, z1,8, z1,42, z1,45, z1,47, z1,48* are punctured to obtain the output sequence *r1,1,r1,2…r1,40*.

From the input sequence *z2,1, z2,2, …, z2,111* the bits *z2,1, z2,2, z2,3, z2,4, z2,5, z2,6, z2,7, z2,8, z2,12, z2,14, z2,15, z2,24, z2,42, z2,48, z2,54, z2,57, z2,60, z2,66, z2,69, z2,96, z2,99, z2,101, z2,102, z2,104, z2,105, z2,106, z2,107, z2,108, z2,109, z2,110, z2,111* are punctured to obtain the output sequence *r2,1,r2,2…r2,80*.

### 4.6.7 UE specific masking for HS-SCCH

The rate matched bits *r1,1,r1,2…r1,40* shall be masked in an UE specific way using the UE identity *xue,1, xue,2, …, xue,16,*to produce the bits *s1,1,s1,2…s1,40*.

Intermediate code word bits bi, i=1,2…,48, are defined by encoding the UE identity bits using the rate ½ convolutional coding described in Clause 4.2.3.1. Eight bits out of the resulting 48 convolutionally encoded bits are punctured using the rate matching rule of Clause 4.6.6 for the HS-SCCH part 1 sequence, that is, the intermediate code word bits b1, b2, b4, b8, b42, b45, b47, b48, arepunctured to obtain the 40 bit UE specific scrambling sequence c1, c2, ….c40. .

The mask output bits *s1,1,s1,2…s1,40* are calculated as follows:

*s1,k =*(*r1,k + ck*) *mod 2* for k = 1,2…40

### 4.6.8 Physical channel mapping for HS-SCCH

The HS-SCCH sub-frame is described in[2].

The sequence of bits *s1,1, s1,2,, …, s1,40* is mapped to the first slot of the HS-SCCH sub frame. The bits *s1,k* are mapped to the PhCHs so that the bits for each PhCH are transmitted over the air in ascending order with respect to *k*.

The sequence of bits *r2,1, r2,2,, …,,r2,80* is mapped to the second and third slot of the HS-SCCH sub frame. The bits *r2,k* are mapped to the PhCHs so that the bits for each PhCH are transmitted over the air in ascending order with respect to *k*.

## 4.6A Coding for HS-SCCH type 2

### 4.6A.1 Overview

HS-SCCH type 2 is used for HS-SCCH-less operation. HS-SCCH type 2 is not used when the UE is configured in MIMO mode or in MIMO mode with four transmit antennas. During second and third transmission, the following information is transmitted by means of the HS-SCCH type 2 physical channel.

- Channelization-code-set information (7 bits): *xccs,1, xccs,2, …, xccs,7*

- Modulation scheme information (1 bit): *xms,1*

- Special Information type (6 bits): *xtype,1, xtype,2, …, xtype,6*

- Special Information (7 bits): *xinfo,1, xinfo,2, xinfo,3, xinfo,4, xinfo,5, xinfo,6, xinfo,7*

- UE identity (16 bits): *xue,1, xue,2, …, xue,16*

Figure 19A below illustrates the overall coding chain for HS-SCCH type 2.



Figure 19A: Coding chain for HS-SCCH type 2

### 4.6A.2 HS-SCCH Type 2 information field mapping

##### 4.6A.2.1 The first transmission

When HS-SCCH\_less\_mode=1 for a UE (as defined in [4]), the first transmission of an HS-DSCH transport block using CRC attachment method 2 shall be sent without an associated HS-SCCH. In this case, the UE shall use the following signalling values in order to attempt to decode the transport block:

- Channelization-code-set information: *Configured by higher layers*

- Modulation scheme information: *QPSK*

- Transport-block size information: *Each of four possible sizes configured by higher layers*

- Redundancy and constellation version: Xrv *=0* (see 4.6.2.1)

- UE identity: *Configured by higher layers*

##### 4.6A.2.2 The second and the third transmissions

For HS-SCCH\_less\_mode=1 there are at maximum 3 transmissions for a HS-DSCH transport block using CRC attachment method 2. The 2nd and 3rd transmissions of a transport block that was sent without an associated HS-SCCH in the first transmission, as described in subclause 4.6A.2.1.1, are associated with an HS-SCCH of type 2.

###### 4.6A.2.2.1 Special Information mapping

The Special Information type *xtype,1, xtype,2, …, xtype,6* shall be set to ''111110’ to indicate HS-SCCH less operation.

The Special Information bits *xinfo,1, xinfo,2, …, xinfo,7* are comprised of:

- Transport-block size information (2 bits): *xinfo,1, xinfo,2* = *xtbs,1, xtbs,2*

- Pointer to the previous transmission (3 bits): *xinfo,3, xinfo,4, xinfo,5*  = *xptr,1, xptr,2, xptr,3*

- Second or third transmission (1 bit): *xinfo,6* = *xsec,1*

- Reserved (1 bit): *xinfo,7* = *xres,1*

4.6A.2.2.1.1 Transport-block size information mapping

The Transport-block size information (2 bits) *xtbs,1, xtbs,2* is the unsigned binary representation of a reference to one of the four Transport-block sizes and the associated number of HS-PDSCH codes for the first transmission configured by higher layers.

|  |  |
| --- | --- |
| xtbs,1, xtbs,2 | **Entry in “Transport Block size list” as signalled in the HS-SCCH-less Information of HS\_SCCH\_LESS\_PARAMS [13]** |
| ''00’ | 1st entry |
| ''01’ | 2nd entry |
| ''10’ | 3rd entry |
| ''11’ | 4th entry |

4.6A.2.2.1.2 Pointer to the previous transmission mapping

Pointer to the previous transmission (3 bits) *xptr,1, xptr,2, xptr,3*  is the unsigned binary representation of s, such that the previous transmission of the same transport block started (6+s) subframes before the start of this transmission.

4.6A.2.2.1.3 Second or third transmission mapping

Second or Third transmission (1 bit) indicates whether this is the second or third transmission.

If *xsec,1*= *''0’*, this is a second transmission.

If *xsec,1*= *''1’*, this is a third transmission.

###### 4.6A.2.2.2 Redundancy and Constellation Version mapping

The redundancy version Xrv for the second and third transmissions shall be equal to 3 and 4 respectively, as defined in Table 13.

###### 4.6A.2.2.3 Modulation scheme mapping

The value of *xms,1* shall be set to ''0’ (QPSK).

###### 4.6A.2.2.4 Channelization code-set mapping

The channelization code-set bits *xccs,1, xccs,2, …, xccs,7* are coded as per clause 4.6.2.3 where the value of P shall be set to either 1 or 2.

###### 4.6A.2.2.5 UE identity mapping

The UE identity is encoded as per clause 4.6.2.4.

### 4.6A.3 Multiplexing of HS-SCCH Type 2 information

The channelization-code-set information *xccs,1, xccs,2, …, xccs,7* and modulation-scheme information *xms,1* are multiplexed together. This gives a sequence of bits *x1,1, x1,2, …, x1,8* where

*x1,i = xccs,i i=1,2,…,7*

*x1,i = xms,i-7 i=8*

The Special Information type *xtype,1, xtype,2, …, xtype,6*, and Special Information *xinfo,1, xinfo,2, xinfo,3, xinfo,4, xinfo,5, xinfo,6, xinfo,7* are multiplexed together. This gives a sequence of bits *x2,1, x2,2, …, x2,13* where

*x2,i = xtype,i i=1,2,…,6*

*x2,i = xinfo,i-6 i=7,8,…,13*

### 4.6A.4 CRC attachment for HS-SCCH Type 2

The sequence of bits *y1, y2, …, y29*, is calculated according to Clause 4.6.4.

### 4.6A.5 Channel coding for HS-SCCH Type 2

Channel coding is performed according to Clause 4.6.5.

### 4.6A.6 Rate matching for HS-SCCH Type 2

Rate matching is performed according to Clause 4.6.6.

### 4.6A.7 UE specific masking for HS-SCCH Type 2

The mask output bits *s1,1,s1,2…s1,40* are calculated according to Clause 4.6.7.

### 4.6A.8 Physical channel mapping for HS-SCCH Type 2

Physical channel mapping is performed according to Clause 4.6.8.

## 4.6B Coding for HS-SCCH type 3

### 4.6B.1 Overview

HS-SCCH type 3 is used when the UE is configured in MIMO mode. If one transport block is transmitted on the associated HS-PDSCH(s) or an HS-SCCH order is transmitted, the following information is transmitted by means of the HS-SCCH type 3 physical channel:

- Channelization-code-set information (7 bits): *xccs,1, xccs,2, …, xccs,7*

- Modulation scheme and number of transport blocks information (3 bits): *xms,1, xms,2, xms,3*

- Precoding weight information (2 bits): *xpwipb,1, xpwipb,2*

- Transport-block size information (6 bits): *xtbspb,1, xtbspb,2, …, xtbspb,6*

- Hybrid-ARQ process information (4 bits): *xhap,1, xhap,2, …, xhap,4*

- Redundancy and constellation version (2 bits): *xrvpb,1, xrvpb,2*

- UE identity (16 bits): *xue,1, xue,2, …, xue,16*

For an HS-SCCH order,

- xccs,1, xccs,2, …, xccs,7, xms,1, xms,2, xms,3, xpwipb,1, xpwipb,2 shall be set to ''111000000000’

- xtbspb,1, xtbspb,2, …, xtbspb,4 shall be set to ''1111’

- xtbspb,5, xtbspb,6 shall be set to xeodt,1, xeodt,2

- xhap,1, xhap,2, xhap,3, xhap,4, xrvpb,1, xrvpb,2 shall be set to xodt,1, xodt,2, xodt,3, xord,1, xord,2, xord,3

where *xeodt,1, xeodt,2*, *xodt,1, xodt,2, xodt,3, xord,1, xord,2, xord,3* are defined in subclause 4.6C.

If two transport blocks are transmitted on the associated HS-PDSCHs (not applicable when single-stream restriction is configured), the following information is transmitted by means of the HS-SCCH type 3 physical channel:

- Channelization-code-set information (7 bits): *xccs,1, xccs,2, …, xccs,7*

- Modulation scheme and number of transport blocks information (3 bits): *xms,1, xms,2, xms,3*

- Precoding weight information for the primary transport block (2 bits): *xpwipb,1, xpwipb,2*

- Transport-block size information for the primary transport block (6 bits): *xtbspb,1, xtbspb,2, …, xtbspb,6*

- Transport-block size information for the secondary transport block (6 bits): *xtbssb,1, xtbssb,2, …, xtbssb,6*

- Hybrid-ARQ process information (4 bits): *xhap,1, xhap,2,…, xhap,4*

- Redundancy and constellation version for the primary transport block (2 bits): *xrvpb,1, xrvpb,2*

- Redundancy and constellation version for the secondary transport block (2 bits): *xrvsb,1, xrvsb,2*

- UE identity (16 bits): *xue,1, xue,2, …, xue,16*

Figure 19B below illustrates the overall coding chain for HS-SCCH type 3. Note that some information shown is not present if only one transport block is transmitted on the associated HS-PDSCH(s).



Figure 19B: Coding chain for HS-SCCH type 3

### 4.6B.2 HS-SCCH type 3 information field mapping

#### 4.6B.2.1 Redundancy and constellation version coding

For each of the primary transport block and a secondary transport block if two transport blocks are transmitted on the associated HS-PDSCH(s), the redundancy version (RV) parameters *r*, *s* and constellation version parameter *b* are coded jointly to produce the values Xrvpb and Xrvsb respectively. The transmitted sequences xrvpb,1, xrvpb,2 and xrvsb,1, xrvsb,2 are the binary representations of Xrvpb and Xrvsb, respectively, where xrvpb,1 and xrvsb,1 are the MSBs.

For the primary transport block if only one transport block is transmitted on the associated HS-PDSCH(s), the redundancy version (RV) parameters *r*, *s* and constellation version parameter *b* are coded jointly to produce the value Xrvpb. The transmitted sequence xrvpb,1, xrvpb,2 is the binary representation of Xrvpb, where xrvpb,1 is the MSB.

Joint coding of parameters *r*, *s* and constellation version parameter *b* is done according to tables 13A and 13B according to the modulation mode used. If Xrvpb = 0 or Xrvsb = 0, the UE shall treat the corresponding transport block as an initial transmission.

Table 13A: RV coding for 16QAM and 64QAM for HS-SCCH type 3

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Xrvpb or Xrvsb (value)** | ***Nsys* / *Ndata* < 1/2** | | | ***Nsys* / *Ndata* ≥ 1/2** | | |
| **s** | **r** | **b** | **s** | **r** | **b** |
| 0 | 1 | 0 | 0 | 1 | 0 | 0 |
| 1 | 1 | 1 | 1 | 0 | 1 | 1 |
| 2 | 1 | 0 | 2 | 0 | 0 | 0 |
| 3 | 1 | 0 | 3 | 1 | 0 | 2 |

Table 13B: RV coding for QPSK for HS-SCCH type 3

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Xrvpb or Xrvsb (value)** | ***Nsys* / *Ndata* <1/2** | | ***Nsys* / *Ndata* ≥1/2** | |
| **s** | **r** | **s** | **r** |
| 0 | 1 | 0 | 1 | 0 |
| 1 | 1 | 1 | 0 | 1 |
| 2 | 1 | 2 | 0 | 3 |
| 3 | 1 | 3 | 1 | 2 |

#### 4.6B.2.2 Modulation scheme and number of transport blocks mapping

The number of transport blocks transmitted on the associated HS-PDSCH(s) and the modulation scheme information are jointly coded as shown in Table 14:

Table 14: Mapping of xms

|  |  |  |  |
| --- | --- | --- | --- |
| xms,1, xms,2,  xms,3 | Modulation for primary transport block | Modulation for secondary transport block | Number of transport blocks |
| 111 | 16QAM | 16QAM | 2 |
| 110 | 16QAM | QPSK | 2 |
| 101 | 64QAM | Indicated by xccs,7 | Indicated by xccs,7 |
| 100 | 16QAM | n/a | 1 |
| 011 | QPSK | QPSK | 2 |
| 010 | 64QAM | 64QAM | 2 |
| 001 | 64QAM | 16QAM | 2 |
| 000 | QPSK | n/a | 1 |

In case *xms,1*, *xms,2*, *xms,3* equals “101” xccs,7 is used as an extra bit in modulation scheme information.

#### 4.6B.2.3 Channelization code-set mapping

The channelization code-set bits *xccs,1, xccs,2, …, xccs,7* are coded according to the following:

Given P (multi-)codes starting at code O, and given the HS-SCCH number if 64QAM is configured for the UE and *xms,1*, *xms,2*, *xms,3* is equal to “101”, calculate the information-field using the unsigned binary representation of integers calculated by the expressions,

for the first three bits (code group indicator) of which *xccs,1* is the MSB:

*xccs,1, xccs,2, xccs,3* = min(P-1,15-P)

If 64QAM is not configured for the UE, or if 64QAM is configured and *xms,1, xms,2, xms,3* is not equal to “101”, then

for the last four bits (code offset indicator) of which *xccs,4* is the MSB:

*xccs,4, xccs,5, xccs,6, xccs,7* = |O-1-P/8 \*15|

Otherwise (i.e. if 64QAM is configured for the UE and *xms,1, xms,2, xms,3* is equal to “101”),

*P* and *O* shall fulfil |O-1-P/8 \*15| mod 2 = (HS‑SCCH number) mod 2, and then

*xccs,4, xccs,5, xccs,6, xccs,dummy* = |O-1-P/8 \*15|, where *xccs,dummy* is a dummy bit that is not transmitted on HS-SCCH.

Furthermore,

*xccs,7* = 0 if the modulation for the secondary transport block is QPSK, and

*xccs,7* = 1 if the number of transport blocks = 1.

The definitions of P and O are given in [3]. The HS-SCCH number is given by the position in the list of HS-SCCH Channelisation Code Informations signalled by higher layers. The HS-SCCH number is associated with the code offset indicator and code group indicator as described above if 64QAM is configured for the UE and *xms,1*, *xms,2*, *xms,3* is equal to “101”.

If two transport blocks are transmitted on the associated HS-PDSCH(s), the same set of channelization codes shall be used for both transport blocks.

#### 4.6B.2.4 UE identity mapping

The UE identity is the HS-DSCH Radio Network Identifier (H-RNTI) defined in [13]. This is mapped such that xue,1  corresponds to the MSB and xue,16 to the LSB, cf. [14].

#### 4.6B.2.5 HARQ process identifier mapping

If two transport blocks are transmitted on the associated HS-PDSCH(s), the mapping relationship between the hybrid-ARQ processes and the transport blocks is such that when the HARQ-process with identifier *HAPpb* is mapped to the primary transport block, the HARQ-process with the identifier given by shall be mapped to the secondary transport block, where *Nproc* is the number of HARQ processes configured by higher layers. The combination of HARQ-processes is indicated by the hybrid-ARQ process information (4 bits) *xhap,1, xhap,2, xhap,3, xhap,4* which are the unsigned binary representation of *HAPpb* where *xhap,1* is MSB.

If only one transport block is transmitted on the associated HS-PDSCH(s), the above mapping is ignored and the hybrid-ARQ process information *xhap,1, xhap,2, xhap,3, xhap,4* is the unsigned binary representation of the HARQ process identifier where *xhap,1* is MSB.

#### 4.6B.2.6 Transport block size index mapping

The transport-block size information *xtbspb,1, xtbspb,2, …, xtbspb,6*  is the unsigned binary representation of the transport block size index for the primary transport block, where *xtbspb,1* is the MSB.

If two transport blocks are transmitted on the associated HS-PDSCH(s), the transport-block size information *xtbssb,1, xtbssb,2, …, xtbssb,6*  is the unsigned binary representation of the transport block size index for the secondary transport block, where *xtbssb,1* is the MSB.

#### 4.6B.2.7 Precoding Weight Information mapping

The precoding weight information for the primary transport block *xpwipb,1, xpwipb,2* is derived from the precoding weight factor w2 as defined in [4], according to Table 14A.

Table 14A: Mapping of precoding weight information for primary transport block

|  |  |
| --- | --- |
| w2 | xpwipb,1, xpwipb,2 |
|  | 00 |
|  | 01 |
|  | 10 |
|  | 11 |

### 4.6B.3 Multiplexing of HS-SCCH type 3 information

The channelization-code-set information *xccs,1, xccs,2, …, xccs,7,* modulation-scheme and number of transport blocks information *xms,1, xms,2, xms,3* and precoding weight information *xpwipb,1, xpwipb,2* are multiplexed together. This gives a sequence of bits *x1,1, x1,2, …, x1,12,* where

*x1,i = xccs,i i=1,2,…,7*

*x1,i = xms,i-7 i=8,9,10*

*x1,i = xpwipb,i-10 i=11,12*

If one transport block is transmitted on the associated HS-PDSCH(s), the transport-block-size information *xtbspb,1, xtbspb,2, …, xtbspb,6*, Hybrid-ARQ-process information *xhap,1,xhap,2, …, xhap,4* and redundancy-version information *xrvpb,1, xrvpb,2* are multiplexed together. This gives a sequence of bits *x2,1, x2,2, …, x2,12* where

*x2,i = xtbs,i i=1,2,…,6*

*x2,i = xhap,i-6 i=7,8,…,10*

*x2,i = xrv,i-10 i=11,12*

If two transport blocks are transmitted on the associated HS-PDSCHs, the transport-block-size information for the primary transport block *xtbspb,1, xtbspb,2, …, xtbspb,6*, transport-block-size information for the secondary transport block *xtbssb,1, xtbssb,2, …, xtbssb,6*, Hybrid-ARQ-process information *xhap,1,xhap,2, …, xhap,4*, redundancy-version information for the primary transport block *xrvpb,1, xrvpb,2*, and redundancy-version information for the secondary transport block *xrvsb,1, xrvsb,2* are multiplexed together. This gives a sequence of bits *x2,1, x2,2, …, x2,20* where

*x2,i = xtbspb,i  i=1,2,…,6*

*x2,i = xtbssb,i-6 i=7,8,…,12*

*x2,i = xhap,i-12 i=13,14,...,16*

*x2,i = xrvpb,i-16 i=17,18*

*x2,i = xrvsb,i-18 i=19,20*

### 4.6B.4 CRC attachment for HS-SCCH type 3

If one transport block is transmitted on the associated HS-PDSCH(s), from the sequence of bits *x1,1, x1,2, …, x1,12, x2,1, x2,2, …, x2,12* a 16-bit CRC is calculated according to Clause 4.2.1.1. This gives a sequence of bits *c1, c2, …, c16* where

*k=1,2,…,16*

This sequence of bits is then masked with the UE Identity *xue,1, xue,2, …, xue,16* and then appended to the sequence of bits *x2,1, x2,2, …, x2,12* to form the sequence of bits *y1, y2, …, y28*, where

*yi = x2,i i=1,2,…,12*

*yi =* (*ci-12* + *xue*,i-12 ) mod 2 *i=13,14,…,28*

If two transport blocks are transmitted on the associated HS-PDSCHs, from the sequence of bits *x1,1, x1,2, …, x1,12, x2,1, x2,2, …, x2,20* a 16-bit CRC is calculated according to Clause 4.2.1.1. This gives a sequence of bits *c1, c2, …, c16* where

*k=1,2,…,16*

This sequence of bits is then masked with the UE Identity *xue,1, xue,2, …, xue,16* and then appended to the sequence of bits *x2,1, x2,2, …, x2,20* to form the sequence of bits *y1, y2, …, y36*, where

*yi = x2,i i=1,2,…,20*

*yi =* (*ci-20* + *xue*,i-20) mod 2 *i=21,22,…,36*

### 4.6B.5 Channel coding for HS-SCCH type 3

Rate 1/3 convolutional coding, as described in Clause 4.2.3.1, is applied to the sequence of bits x*1,1,x1,2, …,x1,12*. This gives a sequence of bits *z1,1, z1,2, …, z1,60*.

If one transport block is transmitted on the associated HS-PDSCH(s), rate 1/3 convolutional coding, as described in Clause 4.2.3.1, is applied to the sequence of bits *y1, y2, …, y28*. This gives a sequence of bits *z2,1, z2,2, …, z2,108*.

If two transport blocks are transmitted on the associated HS-PDSCHs, rate 1/3 convolutional coding, as described in Clause 4.2.3.1, is applied to the sequence of bits *y1, y2, …, y36*. This gives a sequence of bits *z2,1, z2,2, …, z2,132*.

Note that the coded sequence lengths result from the termination of K=9 convolutional coding being fully applied.

### 4.6B.6 Rate matching for HS-SCCH type 3

From the input sequence *z1,1, z1,2, …, z1, 60* the bits *z1,1, z1,2, z1,4, z1,6, z1,8, z1,12, z1,15, z1,18, z1,21, z1,24, z1,37, z1,40, z1,43, z1,46, z1,49, z1,53, z1,55, z1,57, z1,59, z1,60* are punctured to obtain the output sequence *r1,1,r1,2…r1,40*.

If one transport block is transmitted on the associated HS-PDSCH(s), from the input sequence *z2,1, z2,2, …, z2,108* the bits *z2,1, z2,2, z2,3, z2,4, z2,5, z2,6, z2,7, z2,8, z2,12, z2,14, z2,15, z2,24, z2,42, z2,48, z2,63, z2,66, z2,93, z2,96, z2,98, z2,99, z2,101, z2,102, z2,103, z2,104, z2,105, z2,106, z2,107, z2,108* are punctured to obtain the output sequence *r2,1,r2,2…r2,80*.

If two transport blocks are transmitted on the associated HS-PDSCHs, from the input sequence *z2,1, z2,2, …, z2,132* the bits *z2,1, z2,2, z2,3, z2,4, z2,5, z2,6, z2,7, z2,8, z2,10, z2,11, z2,13, z2,14, z2,16, z2,19, z2,22, z2,25, z2,28, z2,31, z2,34, z2,37, z2,40, z2,43, z2,46, z2,49, z2,55, z2,61, z2,72, z2,78, z2,84, z2,87, z2,90, z2,93, z2,96, z2,99, z2,102 , z2,105, z2,108, z2,111, z2,114, z2,117, z2,119, z2,120, z2,122, z2,123, z2,125, z2,126, z2,127, z2,128, z2,129, z2,130, z2,131, z2,132* are punctured to obtain the output sequence *r2,1,r2,2…r2,80*.

### 4.6B.7 UE specific masking for HS-SCCH type 3

The output bits *s1,1,s1,2…s1,40* are calculated as described in subclause 4.6.7.

### 4.6B.8 Physical channel mapping for HS-SCCH type 3

The HS-SCCH sub-frame is described in [2]. The physical channel mapping is carried out as described in subclause 4.6.8.

## 4.6C Coding for HS-SCCH orders

### 4.6C.1 Overview

HS-SCCH orders are commands sent to the UE using HS-SCCH. No HS-PDSCH is associated with HS-SCCH orders.

The following information is transmitted by means of the HS-SCCH order physical channel.

- Extended order type (2bits) *xeodt,1, xeodt,2*

- Order type (3 bits): *xodt,1, xodt,2, xodt,3*

- Order (3 bits):  *xord,1, xord,2, xord,3*

- UE identity (16 bits): *xue,1, xue,2, …, xue,16*

The coding for HS-SCCH orders is specified in subclause 4.6.1 for a cell where the UE is not configured in MIMO mode and not configured in MIMO mode with four transmit antennas or if the UE is in CELL\_FACH state and in subclause 4.6B.1 for a cell where the UE is configured in MIMO mode, in subclause 4.6D.1 for a cell where the UE is configured in MIMO mode with four transmit antennas with the exception of HS-DSCH serving cell change order, which is always transmitted using HS-SCCH type 1 specified in subclause 4.6.1.

### 4.6C.2 HS-SCCH Order information field mapping in the CELL\_DCH state

#### 4.6C.2.1 Order type mapping

If the extended Order type *xeodt,1, xeodt,2* = ’01’ and the Order type *xodt,1, xodt,2, xodt,3* = *''000’*, then the mapping for *xord,1, xord,2, xord,3* is according to subclause 4.6C.2.2.1.

If the extended Order type *xeodt,1, xeodt,2* = ’01’ and the Order type *xodt,1, xodt,2, xodt,3* = *''011’*, then the mapping for *xord,1, xord,2, xord,3* is according to subclause 4.6C.2.2.3.

If the extended Order type *xeodt,1, xeodt,2* = ’11’ and the Order type *xodt,1, xodt,2, xodt,3* = *''010’*, then the mapping for *xord,1, xord,2, xord,3* is according to subclause 4.6C.2.2.4.

If the extended Order type *xeodt,1, xeodt,2* = "11" and the Order type *xodt,1, xodt,2, xodt,3* = *''011"*, then the mapping for *xord,1,xord,2, xord,3* is according to subclause 4.6C.2.2.5.

Otherwise the mapping for *xeodt,1* , *xeodt,2*, *xodt,1, xodt,2, xodt,3*, *xord,1, xord,2, xord,3* is according to subclause 4.6C.2.2.2.

#### 4.6C.2.2 Order mapping

##### 4.6C.2.2.1 Orders for activation and deactivation of DTX, DRX and HS-SCCH-less operation and for HS-DSCH serving cell change

If the order is transmitted from the serving HS-DSCH cell or a secondary serving HS-DSCH cell, for this Order type, *xord,1, xord,2, xord,3* is comprised of:

- DRX activation (1 bit): *xord,1* = *xdrx,1*

- DTX activation (1 bit): *xord,2* = *xdtx,1*

- HS-SCCH-less operation activation (1 bit): *xord,3* = *xhs-scch-less,1*

If *xdrx,1*= *''0’*, then the HS-SCCH order is a DRX De-activation order.

If *xdrx,1*= *''1’*, then the HS-SCCH order is a DRX Activation order.

If *xdtx,1*= *''0’*, then the HS-SCCH order is a DTX De-activation order.

If *xdtx,1*= *''1’*, then the HS-SCCH order is a DTX Activation order.

If *xhs-scch-less,1*= *''0’*, then the HS-SCCH order is a HS-SCCH-less operation De-activation order.

If *xhs-scch-less,1*= *''1’*, then the HS-SCCH order is a HS-SCCH-less operation Activation order.

If the order is transmitted from a non-serving cell using HS-SCCH type 1 specified in subclause 4.6.1 and *xord,1, xord,2, xord,3* = *''000’*, then it is an HS-DSCH serving cell change order .

*xdrx,1, xdtx,1* = *''10’* is a reserved combination (not used in this release).

##### 4.6C.2.2.2 Orders for activation and deactivation of Secondary serving HS-DSCH cells and Secondary uplink frequency

For these Extended Order types and Order types, the meaning of the orders is listed in Table 14B for the case where Secondary\_Cell\_Enabled is less than 4. For the case where Secondary\_Cell\_Enabled is greater than 3 the meaning of the orders is listed in Table 14B.1.

When Secondary\_Cell\_Enabled is 1,

- the order type *xodt,1*, *xodt,2*, *xodt,3* = '010’ is unused;

- regardless of the signaled value of *xord,1* the UE shall assume *xord,1* = *'0’*;

*- xord,2*, *xord,3* = *''10’* is an unused combination.

When the UE is configured in Multiflow mode the following exceptions to the definitions in table 14B apply:

- For the orders received from the Serving or the Secondary Serving HS-DSCH cell, the UE shall consider the 1st Secondary Serving cell to refer to the Secondary Serving HS-DSCH cell and apply the received order to that cell. The activation status of all other cells shall remain unchanged.

- For the orders received from the Assisting Serving or Assisting Secondary Serving HS-DSCH cell the UE shall consider the 1st Secondary Serving cell to refer to the Assisting Secondary Serving HS-DSCH cell and apply the received order to that cell. The activation status of all other cells shall remain unchanged.

- For the orders received from the Assisting Serving or Assisting Secondary Serving HS-DSCH cell the UE shall ignore activation status related to the Secondary Uplink Frequency and maintain the activation status of the Secondary Uplink Frequency unchanged.

- The order contents related to the 2nd and 3rd Secondary Serving HS-DSCH cells shall be ignored.

Table 14B: Orders for activation and deactivation of Secondary serving HS-DSCH cells and Secondary uplink frequency when Secondary\_Cell\_Enabled is less than 4, or when the UE is configured in Multiflow mode.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Extended Order Type | Order Type | Order Mapping | | | Activation Status of Secondary Serving HS-DSCH cells and Secondary Uplink Frequency A= Activate; D = De-activate | | | |
| xeodt,1, xeodt,2 | *xodt,1, xodt,2, xodt,3* | *xord,1* | *xord,2* | *xord,3* | **1st Secondary Serving HS-DSCH cell** | **2nd Secondary Serving HS-DSCH cell** | **3rd Secondary Serving HS-DSCH cell** | **Secondary Uplink Frequency** |
| 01 | 001 | 0 | 0 | 0 | D | D | D | D |
| 0 | 0 | 1 | A | D | D | D |
| 0 | 1 | 1 | A | D | D | A |
| 0 | 1 | 0 | D | A | D | D |
| 1 | 0 | 0 | A | A | D | D |
| 1 | 0 | 1 | A | A | D | A |
| 1 | 1 | 0 | D | D | A | D |
| 1 | 1 | 1 | A | D | A | D |
| 010 | 0 | 0 | 0 | A | D | A | A |
| 0 | 0 | 1 | D | A | A | D |
| 0 | 1 | 0 | A | A | A | D |
| 0 | 1 | 1 | A | A | A | A |
| 1 | 0 | 0 | Unused (Reserved) | | | |
| 1 | 0 | 1 | Unused (Reserved) | | | |
| 1 | 1 | 0 | Unused (Reserved) | | | |
| 1 | 1 | 1 | Unused (Reserved) | | | |

Table 14B.1: Orders for activation and deactivation of Secondary serving HS-DSCH cells and Secondary uplink frequency when Secondary\_Cell\_Enabled is greater than 3.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Extended Order Type | | Order Type | Order Mapping | | | Activation Status of Secondary Serving HS-DSCH cells and Secondary Uplink Frequency A= Activate; D = De-activate | | | | | | | |
| xeodt,,1 | xeodt,,2 | *xodt,1, xodt,2, xodt,3* | *xord,1* | *xord,2* | *xord,3* | **1st Sec Serving HS-DSCH cell** | **2nd Sec Serving HS-DSCH cell** | **3rd Sec Serving HS-DSCH cell** | **4th Sec Serving HS-DSCH cell** | **5th Sec Serving HS-DSCH cell** | **6th Sec Serving HS-DSCH cell** | **7th Sec Serving HS-DSCH cell** | **Sec Uplink Freq** |
| 00 | | 000 | 0 | 0 | 0 | A | D | A | D | A | D | A | A |
| 0 | 0 | 1 | D | A | A | D | A | D | A | D |
| 0 | 1 | 1 | A | A | A | D | A | D | A | A |
| 0 | 1 | 0 | A | A | A | D | A | D | A | D |
| 1 | 0 | 0 | D | D | D | A | A | D | A | D |
| 1 | 0 | 1 | A | D | D | A | A | D | A | D |
| 1 | 1 | 0 | D | A | D | A | A | D | A | D |
| 1 | 1 | 1 | A | D | D | A | A | D | A | A |
| 00 | | 001 | 0 | 0 | 0 | A | A | D | A | A | D | A | D |
| 0 | 0 | 1 | A | A | D | A | A | D | A | A |
| 0 | 1 | 1 | A | D | A | A | A | D | A | D |
| 0 | 1 | 0 | D | D | A | A | A | D | A | D |
| 1 | 0 | 0 | A | D | A | A | A | D | A | A |
| 1 | 0 | 1 | D | A | A | A | A | D | A | D |
| 1 | 1 | 0 | A | A | A | A | A | D | A | D |
| 1 | 1 | 1 | A | A | A | A | A | D | A | A |
| 00 | | 010 | 0 | 0 | 0 | D | D | D | D | D | A | A | D |
| 0 | 0 | 1 | A | D | D | D | D | A | A | D |
| 0 | 1 | 1 | A | D | D | D | D | A | A | A |
| 0 | 1 | 0 | D | A | D | D | D | A | A | D |
| 1 | 0 | 0 | A | A | D | D | D | A | A | D |
| 1 | 0 | 1 | A | A | D | D | D | A | A | A |
| 1 | 1 | 0 | D | D | A | D | D | A | A | D |
| 1 | 1 | 1 | A | D | A | D | D | A | A | D |
| 00 | | 011 | 0 | 0 | 0 | A | D | A | D | D | A | A | A |
| 0 | 0 | 1 | D | A | A | D | D | A | A | D |
| 0 | 1 | 1 | A | A | A | D | D | A | A | A |
| 0 | 1 | 0 | A | A | A | D | D | A | A | D |
| 1 | 0 | 0 | D | D | D | A | D | A | A | D |
| 1 | 0 | 1 | A | D | D | A | D | A | A | D |
| 1 | 1 | 0 | D | A | D | A | D | A | A | D |
| 1 | 1 | 1 | A | D | D | A | D | A | A | A |
| 00 | | 100 | 0 | 0 | 0 | A | A | D | A | D | A | A | D |
| 0 | 0 | 1 | A | A | D | A | D | A | A | A |
| 0 | 1 | 1 | A | D | A | A | D | A | A | D |
| 0 | 1 | 0 | D | D | A | A | D | A | A | D |
| 1 | 0 | 0 | A | D | A | A | D | A | A | A |
| 1 | 0 | 1 | D | A | A | A | D | A | A | D |
| 1 | 1 | 0 | A | A | A | A | D | A | A | D |
| 1 | 1 | 1 | A | A | A | A | D | A | A | A |
| 00 | | 101 | 0 | 0 | 0 | D | D | D | D | A | A | A | D |
| 0 | 0 | 1 | A | D | D | D | A | A | A | D |
| 0 | 1 | 1 | A | D | D | D | A | A | A | A |
| 0 | 1 | 0 | D | A | D | D | A | A | A | D |
| 1 | 0 | 0 | A | A | D | D | A | A | A | D |
| 1 | 0 | 1 | A | A | D | D | A | A | A | A |
| 1 | 1 | 0 | D | D | A | D | A | A | A | D |
| 1 | 1 | 1 | A | D | A | D | A | A | A | D |
| 00 | | 110 | 0 | 0 | 0 | A | D | A | D | A | A | A | A |
| 0 | 0 | 1 | D | A | A | D | A | A | A | D |
| 0 | 1 | 1 | A | A | A | D | A | A | A | A |
| 0 | 1 | 0 | A | A | A | D | A | A | A | D |
| 1 | 0 | 0 | D | D | D | A | A | A | A | D |
| 1 | 0 | 1 | A | D | D | A | A | A | A | D |
| 1 | 1 | 0 | D | A | D | A | A | A | A | D |
| 1 | 1 | 1 | A | D | D | A | A | A | A | A |
| 00 | | 111 | 0 | 0 | 0 | A | A | D | A | A | A | A | D |
| 0 | 0 | 1 | A | A | D | A | A | A | A | A |
| 0 | 1 | 1 | A | D | A | A | A | A | A | D |
| 0 | 1 | 0 | D | D | A | A | A | A | A | D |
| 1 | 0 | 0 | A | D | A | A | A | A | A | A |
| 1 | 0 | 1 | D | A | A | A | A | A | A | D |
| 1 | 1 | 0 | A | A | A | A | A | A | A | D |
| 1 | 1 | 1 | A | A | A | A | A | A | A | A |
| 01 | | 001 | 0 | 0 | 0 | D | D | D | D | D | D | D | D |
| 0 | 0 | 1 | A | D | D | D | D | D | D | D |
| 0 | 1 | 1 | A | D | D | D | D | D | D | A |
| 0 | 1 | 0 | D | A | D | D | D | D | D | D |
| 1 | 0 | 0 | A | A | D | D | D | D | D | D |
| 1 | 0 | 1 | A | A | D | D | D | D | D | A |
| 1 | 1 | 0 | D | D | A | D | D | D | D | D |
| 1 | 1 | 1 | A | D | A | D | D | D | D | D |
| 01 | | 010 | 0 | 0 | 0 | A | D | A | D | D | D | D | A |
| 0 | 0 | 1 | D | A | A | D | D | D | D | D |
| 0 | 1 | 1 | A | A | A | D | D | D | D | A |
| 0 | 1 | 0 | A | A | A | D | D | D | D | D |
| 1 | 0 | 0 | D | D | D | A | D | D | D | D |
| 1 | 0 | 1 | A | D | D | A | D | D | D | D |
| 1 | 1 | 0 | D | A | D | A | D | D | D | D |
| 1 | 1 | 1 | A | D | D | A | D | D | D | A |
| 01 | | 100 | 0 | 0 | 0 | D | D | D | D | A | D | D | D |
| 0 | 0 | 1 | A | D | D | D | A | D | D | D |
| 0 | 1 | 1 | A | D | D | D | A | D | D | A |
| 0 | 1 | 0 | D | A | D | D | A | D | D | D |
| 1 | 0 | 0 | A | A | D | D | A | D | D | D |
| 1 | 0 | 1 | A | A | D | D | A | D | D | A |
| 1 | 1 | 0 | D | D | A | D | A | D | D | D |
| 1 | 1 | 1 | A | D | A | D | A | D | D | D |
| 01 | | 101 | 0 | 0 | 0 | A | D | A | D | A | D | D | A |
| 0 | 0 | 1 | D | A | A | D | A | D | D | D |
| 0 | 1 | 1 | A | A | A | D | A | D | D | A |
| 0 | 1 | 0 | A | A | A | D | A | D | D | D |
| 1 | 0 | 0 | D | D | D | A | A | D | D | D |
| 1 | 0 | 1 | A | D | D | A | A | D | D | D |
| 1 | 1 | 0 | D | A | D | A | A | D | D | D |
| 1 | 1 | 1 | A | D | D | A | A | D | D | A |
| 01 | | 110 | 0 | 0 | 0 | A | A | D | A | A | D | D | D |
| 0 | 0 | 1 | A | A | D | A | A | D | D | A |
| 0 | 1 | 1 | A | D | A | A | A | D | D | D |
| 0 | 1 | 0 | D | D | A | A | A | D | D | D |
| 1 | 0 | 0 | A | D | A | A | A | D | D | A |
| 1 | 0 | 1 | D | A | A | A | A | D | D | D |
| 1 | 1 | 0 | A | A | A | A | A | D | D | D |
| 1 | 1 | 1 | A | A | A | A | A | D | D | A |
| 01 | | 111 | 0 | 0 | 0 | D | D | D | D | D | A | D | D |
| 0 | 0 | 1 | A | D | D | D | D | A | D | D |
| 0 | 1 | 1 | A | D | D | D | D | A | D | A |
| 0 | 1 | 0 | D | A | D | D | D | A | D | D |
| 1 | 0 | 0 | A | A | D | D | D | A | D | D |
| 1 | 0 | 1 | A | A | D | D | D | A | D | A |
| 1 | 1 | 0 | D | D | A | D | D | A | D | D |
| 1 | 1 | 1 | A | D | A | D | D | A | D | D |
| 10 | | 000 | 0 | 0 | 0 | A | D | A | D | D | A | D | A |
| 0 | 0 | 1 | D | A | A | D | D | A | D | D |
| 0 | 1 | 1 | A | A | A | D | D | A | D | A |
| 0 | 1 | 0 | A | A | A | D | D | A | D | D |
| 1 | 0 | 0 | D | D | D | A | D | A | D | D |
| 1 | 0 | 1 | A | D | D | A | D | A | D | D |
| 1 | 1 | 0 | D | A | D | A | D | A | D | D |
| 1 | 1 | 1 | A | D | D | A | D | A | D | A |
| 10 | | 001 | 0 | 0 | 0 | A | A | D | A | D | A | D | D |
| 0 | 0 | 1 | A | A | D | A | D | A | D | A |
| 0 | 1 | 1 | A | D | A | A | D | A | D | D |
| 0 | 1 | 0 | D | D | A | A | D | A | D | D |
| 1 | 0 | 0 | A | D | A | A | D | A | D | A |
| 1 | 0 | 1 | D | A | A | A | D | A | D | D |
| 1 | 1 | 0 | A | A | A | A | D | A | D | D |
| 1 | 1 | 1 | A | A | A | A | D | A | D | A |
| 10 | | 010 | 0 | 0 | 0 | D | D | D | D | A | A | D | D |
| 0 | 0 | 1 | A | D | D | D | A | A | D | D |
| 0 | 1 | 1 | A | D | D | D | A | A | D | A |
| 0 | 1 | 0 | D | A | D | D | A | A | D | D |
| 1 | 0 | 0 | A | A | D | D | A | A | D | D |
| 1 | 0 | 1 | A | A | D | D | A | A | D | A |
| 1 | 1 | 0 | D | D | A | D | A | A | D | D |
| 1 | 1 | 1 | A | D | A | D | A | A | D | D |
| 10 | | 011 | 0 | 0 | 0 | A | D | A | D | A | A | D | A |
| 0 | 0 | 1 | D | A | A | D | A | A | D | D |
| 0 | 1 | 1 | A | A | A | D | A | A | D | A |
| 0 | 1 | 0 | A | A | A | D | A | A | D | D |
| 1 | 0 | 0 | D | D | D | A | A | A | D | D |
| 1 | 0 | 1 | A | D | D | A | A | A | D | D |
| 1 | 1 | 0 | D | A | D | A | A | A | D | D |
| 1 | 1 | 1 | A | D | D | A | A | A | D | A |
| 10 | | 100 | 0 | 0 | 0 | A | A | D | A | A | A | D | D |
| 0 | 0 | 1 | A | A | D | A | A | A | D | A |
| 0 | 1 | 1 | A | D | A | A | A | A | D | D |
| 0 | 1 | 0 | D | D | A | A | A | A | D | D |
| 1 | 0 | 0 | A | D | A | A | A | A | D | A |
| 1 | 0 | 1 | D | A | A | A | A | A | D | D |
| 1 | 1 | 0 | A | A | A | A | A | A | D | D |
| 1 | 1 | 1 | A | A | A | A | A | A | D | A |
| 10 | | 101 | 0 | 0 | 0 | D | D | D | D | D | D | A | D |
| 0 | 0 | 1 | A | D | D | D | D | D | A | D |
| 0 | 1 | 1 | A | D | D | D | D | D | A | A |
| 0 | 1 | 0 | D | A | D | D | D | D | A | D |
| 1 | 0 | 0 | A | A | D | D | D | D | A | D |
| 1 | 0 | 1 | A | A | D | D | D | D | A | A |
| 1 | 1 | 0 | D | D | A | D | D | D | A | D |
| 1 | 1 | 1 | A | D | A | D | D | D | A | D |
| 10 | | 110 | 0 | 0 | 0 | A | D | A | D | D | D | A | A |
| 0 | 0 | 1 | D | A | A | D | D | D | A | D |
| 0 | 1 | 1 | A | A | A | D | D | D | A | A |
| 0 | 1 | 0 | A | A | A | D | D | D | A | D |
| 1 | 0 | 0 | D | D | D | A | D | D | A | D |
| 1 | 0 | 1 | A | D | D | A | D | D | A | D |
| 1 | 1 | 0 | D | A | D | A | D | D | A | D |
| 1 | 1 | 1 | A | D | D | A | D | D | A | A |
| 10 | | 111 | 0 | 0 | 0 | A | A | D | A | D | D | A | D |
| 0 | 0 | 1 | A | A | D | A | D | D | A | A |
| 0 | 1 | 1 | A | D | A | A | D | D | A | D |
| 0 | 1 | 0 | D | D | A | A | D | D | A | D |
| 1 | 0 | 0 | A | D | A | A | D | D | A | A |
| 1 | 0 | 1 | D | A | A | A | D | D | A | D |
| 1 | 1 | 0 | A | A | A | A | D | D | A | D |
| 1 | 1 | 1 | A | A | A | A | D | D | A | A |
| 11 | | 000 | 0 | 0 | 0 | D | D | D | D | A | D | A | D |
| 0 | 0 | 1 | A | D | D | D | A | D | A | D |
| 0 | 1 | 1 | A | D | D | D | A | D | A | A |
| 0 | 1 | 0 | D | A | D | D | A | D | A | D |
| 1 | 0 | 0 | A | A | D | D | A | D | A | D |
| 1 | 0 | 1 | A | A | D | D | A | D | A | A |
| 1 | 1 | 0 | D | D | A | D | A | D | A | D |
| 1 | 1 | 1 | A | D | A | D | A | D | A | D |
| 11 | | 001 | 0 | 0 | 0 | A | A | D | A | D | D | D | D |
| 0 | 0 | 1 | A | A | D | A | D | D | D | A |
| 0 | 1 | 1 | A | D | A | A | D | D | D | D |
| 0 | 1 | 0 | D | D | A | A | D | D | D | D |
| 1 | 0 | 0 | A | D | A | A | D | D | D | A |
| 1 | 0 | 1 | D | A | A | A | D | D | D | D |
| 1 | 1 | 0 | A | A | A | A | D | D | D | D |
| 1 | 1 | 1 | A | A | A | A | D | D | D | A |

##### 4.6C.2.2.3 Orders for Switching between Uplink Closed Loop Transmit Diversity Activation states

For this Order type, the meaning of the orders is listed in Table 14B.2.

When the UE is configured in Multiflow mode, if any of the orders related to uplink CLTD activation states as defined in Table 14B.2 are received from the Assisting Serving or Assisting Secondary Serving HS-DSCH cell, then the UE shall ignore the orders and maintain the uplink CLTD activation state unchanged.

Table 14B.2: Orders for UE when UL\_CLTD\_Enabled is TRUE

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Extended Order Type | **Order Type** | **Order Mapping** | | | **Activation States  A= Activate; D = De-activate** | | |
| xeodt,1, xeodt,2 | *xodt,1, xodt,2, xodt,3* | *xord,1* | *xord,2* | *xord,3* | **1** | **2** | **3** |
| **Tx on Antenna 1 and Antenna 2 with Beamforming (Note 1)** | **Single Tx on Antenna 1 with no S-DPCCH** | **Single Tx on Antenna 2 with no S-DPCCH** |
| 01 | 011 | 1 | 1 | 1 | A | D | D |
| 0 | 0 | 1 | D | A | D |
| 0 | 1 | 0 | D | D | A |
| 1 | 0 | 1 | Unused (Reserved) | | |
| 1 | 1 | 0 | Unused (Reserved) | | |
| 0 | 0 | 0 | Unused (Reserved) | | |
| 0 | 1 | 1 | Unused (Reserved) | | |
| 1 | 0 | 0 | Unused (Reserved) | | |

Note 1: The precoding weights for beamforming are defined in [4].

##### 4.6C.2.2.4 Orders for activating and de-activating demodulation common pilots (D-CPICH) when the UE is configured in MIMO mode with four transmit antennas

For this Order type, the meaning of the orders is listed in Table 14B.3.

Table 14B.3: Orders when the UE is configured in MIMO mode with four transmit antennas

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Extended Order Type | Order Type | Order Mapping | | | D-CPICH Activation States  A= Activate; D = De-activate |
| xeodt,1, xeodt,2 | *xodt,1, xodt,2, xodt,3* | *xord,1* | *xord,2* | *xord,3* |
| 11 | 010 | 1 | 1 | 1 | **A** |
| 0 | 0 | 0 | **D** |
| 0 | 0 | 1 | Unused (Reserved) |
| 0 | 1 | 0 | Unused (Reserved) |
| 0 | 1 | 1 | Unused (Reserved) |
| 1 | 0 | 0 | Unused (Reserved) |
| 1 | 0 | 1 | Unused (Reserved) |
| 1 | 1 | 0 | Unused (Reserved) |

Note 1: The activation and de-activation status corresponds to individual HS-DSCH cell.

Note 2: Activation and de-activation indication applies for all the demodulation common pilots configured in the cell.

##### 4.6C.2.2.5 Orders for switching the E-DCH TTI, and for start/stop a simplified HS-SCCH type 1 transmission interval

If the order is transmitted from the serving HS-DSCH cell or a secondary serving HS-DSCH cell, for this Order type, the meaning of the orders for single cell E-DCH is listed in Table 14B.3A and the meaning of the orders for dual cell E-DCH is listed in Table 14B.3B.

Table 14B.3A: Orders for switching the E-DCH TTI for single cell E-DCH and for start/stop a simplified HS-SCCH type 1 transmission interval

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Extended Order Type | Order Type | Order Mapping | | | Interpretation |
| xeodt,1, xeodt,2 | xodt,1, xodt,2, xodt,3 | xord,1 | xord,2 | xord,3 |
| 11 | 011 | 0 | 0 | 0 | TTI switch order from 2ms to 10ms |
| 0 | 0 | 1 | TTI switch order from 10ms to 2ms |
| 0 | 1 | 0 | Start simplified HS-SCCH type 1 transmission interval order |
| 0 | 1 | 1 | Stop simplified HS-SCCH type 1 transmission interval order |
| 1 | 0 | 0 | Unused (Reserved) for single cell E-DCH |
| 1 | 0 | 1 | Unused (Reserved) for single cell E-DCH |
| 1 | 1 | 0 | Unused (Reserved) for single cell E-DCH |
| 1 | 1 | 1 | Unused (Reserved) for single cell E-DCH |

Table 14B.3B: Orders for switching the E-DCH TTI for dual cell E-DCH

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Extended Order Type | Order Type | Order Mapping | | | Interpretation |
| xeodt,1, xeodt,2 | xodt,1, xodt,2, xodt,3 | xord,1 | xord,2 | xord,3 |
| 11 | 011 | 0 | 0 | 0 | Unused (Reserved for dual cell E-DCH) |
| 0 | 0 | 1 | Unused (Reserved for dual cell E-DCH) |
| 0 | 1 | 0 | TTI switch order to 2ms+10ms |
| 0 | 1 | 1 | TTI switch order to 10ms+2ms |
| 1 | 0 | 0 | TTI switch order to 2ms+2ms |
| 1 | 0 | 1 | TTI switch order to 10ms+10ms |
| 1 | 1 | 0 | Unused (Reserved for dual cell E-DCH) |
| 1 | 1 | 1 | Unused (Reserved for dual cell E-DCH) |

NOTE 1: (Table 14B.3B): For the TTI switch orders the TTI length displayed on the left hand side applies to the primary uplink frequency, while the TTI length displayed on the right hand side applies to the secondary uplink frequency.

NOTE 2: (Table 14B.3B): The TTI switch orders also apply if the secondary uplink frequency is deactivated, but it becomes effective on the secondary uplink frequency upon its re-activation.

#### 4.6C.2.3 UE identity mapping

The UE identity is the HS-DSCH Radio Network Identifier (H-RNTI) defined in [13]. This is mapped such that xue,1  corresponds to the MSB and xue,16 to the LSB, cf. [14].

### 4.6C.3 HS-SCCH order information field mapping in the CELL\_FACH and CELL\_PCH states

#### 4.6C.3.1 Order type mapping

If the extended Order type *xeodt,1, xeodt,2* = ’01’ and the Order type *xodt,1, xodt,2, xodt,3* = *''000’*, then the mapping for *xord,1, xord,2, xord,3* is according to subclause 4.6C.3.2.

#### 4.6C.3.2 Order mapping

##### 4.6C.3.2.1 Orders for network triggered HS-DPCCH transmission

For this Order type, the Order mapping *xord,1, xord,2, xord,3* and the associated meaning is as follows:

If *xord,1, xord,2, xord,3* = *''001’*, then the HS-SCCH order is an order for triggering the random access procedure in CELL\_FACH as specified in subclause 6.1A in [4].

##### 4.6C.3.2.2 Orders for HS-DSCH reception during CELL\_FACH HS-SCCH DRX operation

For this Order type, the Order mapping *xord,1, xord,2, xord,3* and the associated meaning is as follows:

If *xord,1, xord,2, xord,3* = *''110”* then the HS-SCCH order is an order for notifying about an HS-DSCH transmission during CELL\_FACH HS-SCCH DRX operation as specified in [4] subclause 6A.1.3.2.

## 4.6D Coding for HS-SCCH type 4

### 4.6D.1 Overview

HS-SCCH type 4 is used when the UE is configured in MIMO mode with four transmit antennas. If one transport block is transmitted on the associated HS-PDSCH(s) or an HS-SCCH order is transmitted, the following information is transmitted by means of the HS-SCCH type 4 physical channel:

- Channelization-code-set information (7 bits): *xccs,1, xccs,2, …, xccs,7*

- Modulation scheme and number of transport blocks information (5 bits): *xms,1, xms,2, xms,3, xms,4, xms,5*

- Precoding weight information (4 bits): *xpwipb,1, xpwipb,2, xpwipb,3, xpwipb,4*

- Transport-block size information (6 bits): *xtbspb,1, xtbspb,2, …, xtbspb,6*

- Hybrid-ARQ process information (4 bits): *xhap,1, xhap,2, …, xhap,4*

- Redundancy and constellation version (2 bits): *xrvpb,1, xrvpb,2*

- UE identity (16 bits): *xue,1, xue,2, …, xue,16*

For an HS-SCCH order,

- xccs,1, xccs,2, …, xccs,7, xms,1, xms,2, xms,3, xms,4, xms,5, xpwipb,1, xpwipb,2, xpwipb,3, xpwipb,4 shall be set to ''1110000000000000’

- xtbspb,1, xtbspb,2, …, xtbspb,4 shall be set to ''1111’

- xtbspb,5, xtbspb,6 shall be set to xeodt,1, xeodt,2

- xhap,1, xhap,2, xhap,3, xhap,4, xrvpb,1, xrvpb,2 shall be set to xodt,1, xodt,2, xodt,3, xord,1, xord,2, xord,3

where *xeodt,1, xeodt,2*, *xodt,1, xodt,2, xodt,3, xord,1, xord,2, xord,3* are defined in subclause 4.6C.

If more than one transport block is transmitted on the associated HS-PDSCHs, the following information is transmitted by means of the HS-SCCH type 4 physical channel:

- Channelization-code-set information (7 bits): *xccs,1, xccs,2, …, xccs,7*

- Modulation scheme and number of transport blocks information (5 bits): *xms,1, xms,2, xms,3, xms,4, xms,5*

- Precoding weight information (4 bits): *xpwipb,1, xpwipb,2, xpwipb,3, xpwipb,4*

- Transport-block size information for the primary or/and fourth transport block (6 bits): *xtbspb,1, xtbspb,2, …, xtbspb,6*

- Transport-block size information for the second or/and third transport block (6 bits): *xtbssb,1, xtbssb,2, …, xtbssb,6*

- Hybrid-ARQ process information (4 bits): *xhap,1, xhap,2,…, xhap,4*

- Redundancy and constellation version for the primary or/and fourth transport block (2 bits): *xrvpb,1, xrvpb,2*

- Redundancy and constellation version for the second or/and third transport block (2 bits): *xrvsb,1, xrvsb,2*

- UE identity (16 bits): *xue,1, xue,2, …, xue,16*

The overall coding chain for HS-SCCH type 4 is same as that of HS-SCCH type 3 as shown in Figure 19 B.

### 4.6D.2 HS-SCCH type 4 information field mapping

#### 4.6D.2.1 Redundancy and constellation version coding

If four transport blocks are transmitted on the associated HS-PDSCH(s), the redundancy version (RV) parameters *r*, *s* and constellation version parameter *b* are coded jointly to produce the values Xrvpb for the primary and the fourth transport blocks and Xrvsb for the second and the third transport blocks respectively. The transmitted sequences xrvpb,1, xrvpb,2 and xrvsb,1, xrvsb,2 are the binary representations of Xrvpb and Xrvsb, respectively, where xrvpb,1 and xrvsb,1 are the MSBs.

If three transport blocks are transmitted on the associated HS-PDSCH(s), the redundancy version (RV) parameters *r*, *s* and constellation version parameter *b* are coded jointly to produce the values Xrvpb for the primary transport block and Xrvsb for the second and the third transport blocks respectively. The transmitted sequences xrvpb,1, xrvpb,2 and xrvsb,1, xrvsb,2 are the binary representations of Xrvpb and Xrvsb, respectively, where xrvpb,1 and xrvsb,1 are the MSBs.

For each of the primary transport block and a second transport block if two transport blocks are transmitted on the associated HS-PDSCH(s), the redundancy version (RV) parameters *r*, *s* and constellation version parameter *b* are coded jointly to produce the values Xrvpb and Xrvsb respectively. The transmitted sequences xrvpb,1, xrvpb,2 and xrvsb,1, xrvsb,2 are the binary representations of Xrvpb and Xrvsb, respectively, where xrvpb,1 and xrvsb,1 are the MSBs.

For the primary transport block if only one transport block is transmitted on the associated HS-PDSCH(s), the redundancy version (RV) parameters *r*, *s* and constellation version parameter *b* are coded jointly to produce the value Xrvpb. The transmitted sequence xrvpb, 1, xrvpb, 2 is the binary representation of Xrvpb, where xrvpb,1 is the MSB.

Joint coding of parameters *r*, *s* and constellation version parameter *b* is done according to tables 14B.4 and 14B.5 according to the modulation mode used. If Xrvpb = 0 or Xrvsb = 0, the UE shall treat the corresponding transport block as an initial transmission.

Table 14B.4: RV coding for 16QAM and 64QAM for HS-SCCH type 4

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Xrvpb or Xrvsb (value)** | ***Nsys* / *Ndata* < 1/2** | | | ***Nsys* / *Ndata* ≥ 1/2** | | |
| **s** | **r** | **b** | **s** | **r** | **b** |
| 0 | 1 | 0 | 0 | 1 | 0 | 0 |
| 1 | 1 | 1 | 1 | 0 | 1 | 1 |
| 2 | 1 | 0 | 2 | 0 | 0 | 0 |
| 3 | 1 | 0 | 3 | 1 | 0 | 2 |

Table 14B.5: RV coding for QPSK for HS-SCCH type 4

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Xrvpb or Xrvsb (value)** | ***Nsys* / *Ndata* <1/2** | | ***Nsys* / *Ndata* ≥1/2** | |
| **s** | **r** | **s** | **r** |
| 0 | 1 | 0 | 1 | 0 |
| 1 | 1 | 1 | 0 | 1 |
| 2 | 1 | 2 | 0 | 3 |
| 3 | 1 | 3 | 1 | 2 |

#### 4.6D.2.2 Modulation scheme and number of transport blocks mapping

The number of transport blocks transmitted on the associated HS-PDSCH(s) and the modulation scheme information are jointly coded as shown in Table 14B.6:

Table 14B.6: Mapping of xms

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| xms,1, xms,2,  xms,3, xms,4,  xms,5 | Modulation for  primary transport block | Modulation for second transport block | Modulation for  third  transport block | Modulation for  fourth transport block | Number  of transport blocks |
| 00000 | QPSK | Unused | Unused | Unused | 1 |
| 00001 | 16QAM | Unused | Unused | Unused | 1 |
| 00010 | 64 QAM | Unused | Unused | Unused | 1 |
| 00011 | QPSK | QPSK | Unused | Unused | 2 |
| 00100 | QPSK | 16QAM | Unused | Unused | 2 |
| 00101 | QPSK | 64QAM | Unused | Unused | 2 |
| 00110 | 16QAM | QPSK | Unused | Unused | 2 |
| 00111 | 16QAM | 16QAM | Unused | Unused | 2 |
| 1000 | 16QAM | 64QAM | Unused | Unused | 2 |
| 01001 | 64QAM | QPSK | Unused | Unused | 2 |
| 01010 | 64QAM | 16QAM | Unused | Unused | 2 |
| 01011 | 64QAM | 64QAM | Unused | Unused | 2 |
| 01100 | QPSK | QPSK | QPSK | Unused | 3 |
| 01101 | QPSK | 16QAM | 16QAM | Unused | 3 |
| 01110 | QPSK | 64QAM | 64QAM | Unused | 3 |
| 01111 | 16QAM | QPSK | QPSK | Unused | 3 |
| 10000 | 16QAM | 16QAM | 16QAM | Unused | 3 |
| 10001 | 16QAM | 64QAM | 64QAM | Unused | 3 |
| 10010 | 64QAM | QPSK | QPSK | Unused | 3 |
| 10011 | 64QAM | 16QAM | 16QAM | Unused | 3 |
| 10100 | 64QAM | 64QAM | 64QAM | Unused | 3 |
| 10101 | QPSK | QPSK | QPSK | QPSK | 4 |
| 10110 | QPSK | 16QAM | 16QAM | QPSK | 4 |
| 10111 | QPSK | 64QAM | 64QAM | QPSK | 4 |
| 11000 | 16QAM | QPSK | QPSK | 16QAM | 4 |
| 11001 | 16QAM | 16QAM | 16QAM | 16QAM | 4 |
| 11010 | 16QAM | 64QAM | 64QAM | 16QAM | 4 |
| 11011 | 64QAM | QPSK | QPSK | 64QAM | 4 |
| 11100 | 64QAM | 16QAM | 16QAM | 64QAM | 4 |
| 11101 | 64 QAM | 64QAM | 64QAM | 64 QAM | 4 |
| 11110 | Unused (Reserved) | | | | |
| 11111 | Unused (Reserved) | | | | |

#### 4.6D.2.3 Channelization code-set mapping

The channelization code-set bits xccs,1, xccs,2, …, xccs,7 are coded according to the following:

Given P (multi-)codes starting at code O calculate the information-field using the unsigned binary representation of integers calculated by the expressions,

for the first three bits (code group indicator) of which *xccs,1* is the MSB:

*xccs,1, xccs,2, xccs,3* = min(P-1,15-P)

for the last four bits (code offset indicator) of which *xccs,4* is the MSB:

*xccs,4, xccs,5, xccs,6, xccs,7* = |O-1-P/8 \*15|

The definitions of P and O are given in [3].

If more than one transport blocks are transmitted on the associated HS-PDSCH(s), the same set of channelization codes shall be used for all transport blocks.

#### 4.6D.2.4 UE identity mapping

The UE identity is the HS-DSCH Radio Network Identifier (H-RNTI) defined in [13]. This is mapped such that xue,1  corresponds to the MSB and xue,16 to the LSB, cf. [14].

#### 4.6D.2.5 HARQ process identifier mapping

If four transport blocks are transmitted on the associated HS-PDSCH(s), the mapping relationship between the hybrid-ARQ processes and the transport blocks is such that when the HARQ-process with identifier *HAPpb* is mapped to the primary and the fourth transport block, the HARQ-process with the identifier given by shall be mapped to the second and the third transport block, where *Nproc* is the number of HARQ processes configured by higher layers. The combination of HARQ-processes is indicated by the hybrid-ARQ process information (4 bits) *xhap,1, xhap,2, xhap,3, xhap,4* which are the unsigned binary representation of *HAPpb* where *xhap,1* is MSB.

If three transport blocks are transmitted on the associated HS-PDSCH(s), the mapping relationship between the hybrid-ARQ processes and the transport blocks is such that when the HARQ-process with identifier *HAPpb* is mapped to the primary transport block, the HARQ-process with the identifier given by shall be mapped to the second and the third transport block, where *Nproc* is the number of HARQ processes configured by higher layers. The combination of HARQ-processes is indicated by the hybrid-ARQ process information (4 bits) *xhap,1, xhap,2, xhap,3, xhap,4* which are the unsigned binary representation of *HAPpb* where *xhap,1* is MSB.

If two transport blocks are transmitted on the associated HS-PDSCH(s), the mapping relationship between the hybrid-ARQ processes and the transport blocks is such that when the HARQ-process with identifier *HAPpb* is mapped to the primary transport block, the HARQ-process with the identifier given by shall be mapped to the second transport block, where *Nproc* is the number of HARQ processes configured by higher layers. The combination of HARQ-processes is indicated by the hybrid-ARQ process information (4 bits) *xhap,1, xhap,2, xhap,3, xhap,4* which are the unsigned binary representation of *HAPpb* where *xhap,1* is MSB.

If only one transport block is transmitted on the associated HS-PDSCH(s), the above mapping is ignored and the hybrid-ARQ process information *xhap, 1, xhap,2, xhap,3, xhap,4* is the unsigned binary representation of the HARQ process identifier where *xhap,1* is MSB.

#### 4.6D.2.6 Transport block size index mapping

The transport-block size information *xtbspb,1, xtbspb,2, …, xtbspb,6*  is the unsigned binary representation of the transport block size index for the primary transport block, where *xtbspb,1* is the MSB.

If two transport blocks are transmitted on the associated HS-PDSCH(s), the transport-block size information *xtbssb,1, xtbssb,2, …, xtbssb,6*  is the unsigned binary representation of the transport block size index for the second transport block, where *xtbssb,1* is the MSB. If the number of transport blocks indicated is equal to 2, if Xrvpb = 0 and if the transport-block size information *xtbspb,1, xtbspb,2, …, xtbspb,6*  is set to ''111111’, then the primary transport block is not transmitted. If the number of transport blocks indicated is equal to 2, if Xrvsb = 0 and if the transport-block size information *xtbssb,1, xtbssb,2, …, xtbssb,6*  is set to ''111111’, then the second transport block is not transmitted.

If three transport blocks are transmitted on the associated HS-PDSCH(s), the transport-block size information *xtbspb,1, xtbspb,2, …, xtbspb,6*  is the unsigned binary representation of the transport block size index for the primary transport block, where *xtbspb,1* is the MSB and the transport-block size information *xtbssb,1, xtbssb,2, …, xtbssb,6*  is the unsigned binary representation of the transport block size index for the second and the third transport blocks, where *xtbssb,1* is the MSB. If the number of transport blocks indicated is equal to 3, if Xrvpb = 0 and if the transport-block size information *xtbspb,1, xtbspb,2, …, xtbspb,6*  is set to ''111111’, then the primary transport block is not transmitted. If the number of transport blocks indicated is equal to 3, if Xrvsb = 0 and if the transport-block size information *xtbssb,1, xtbssb,2, …, xtbssb,6*  is set to ''111111’, then the second and the third transport blocks are not transmitted.

If four transport blocks are transmitted on the associated HS-PDSCH(s), the transport-block size information *xtbspb,1, xtbspb,2, …, xtbspb,6*  is the unsigned binary representation of the transport block size index for the primary and the fourth transport blocks, where *xtbspb,1* is the MSB and the transport-block size information *xtbssb,1, xtbssb,2, …, xtbssb,6*  is the unsigned binary representation of the transport block size index for the second and the third transport blocks, where *xtbssb,1* is the MSB. If the number of transport blocks indicated is equal to 4 if Xrvpb = 0 and if the transport-block size information *xtbspb,1, xtbspb,2, …, xtbspb,6*  is set to ''111111’, then the primary and fourth transport blocks are not transmitted. If the number of transport blocks indicated is equal to 4 if Xrvsb = 0 and if the transport-block size information *xtbssb,1, xtbssb,2, …, xtbssb,6*  is set to ''111111’, then the second and the third transport blocks are not transmitted.

#### 4.6D.2.7 Precoding Weight Information mapping

The precoding weight information *xpwipb,1, xpwipb,2, xpwipb,3, xpwipb,4* is mapped according to Table 14B.7. The quantity denotes the matrix defined by the columns given by the set from the expression where *I* is the identity matrix and the vector is given by Table 14B.7.

Table 14B.7: precoding weight information

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| xpwipb,1, xpwipb,2, xpwipb,3, xpwipb,4, |  | Number of transport blocks | | | |
|  |  | 1 | 2 | 3 | 4 |
| 0000 |  |  |  |  |  |
| 0001 |  |  |  |  |  |
| 0010 |  |  |  |  |  |
| 0011 |  |  |  |  |  |
| 0100 |  |  |  |  |  |
| 0101 |  |  |  |  |  |
| 0110 |  |  |  |  |  |
| 0111 |  |  |  |  |  |
| 1000 |  |  |  |  |  |
| 1001 |  |  |  |  |  |
| 1010 |  |  |  |  |  |
| 1011 |  |  |  |  |  |
| 1100 |  |  |  |  |  |
| 1101 |  |  |  |  |  |
| 1110 |  |  |  |  |  |
| 1111 |  |  |  |  |  |

### 4.6D.3 Multiplexing of HS-SCCH type 4 information

The channelization-code-set information *xccs,1, xccs,2, …, xccs,7,* modulation-scheme and number of transport blocks information *xms,1, xms,2, xms,3, xms,4, xms,5* and precoding weight information *xpwipb,1, xpwipb,2, xpwipb,3, xpwipb,4* are multiplexed together. This gives a sequence of bits *x1,1, x1,2, …, x1,16,* where

*x1,i = xccs,i i=1,2,…,7*

*x1,i = xms,i-7 i=8,9,10,11,12*

*x1,i = xpwipb,i-12 i=13,14,15,16*

If one transport block is transmitted on the associated HS-PDSCH(s), the transport-block-size information *xtbspb,1, xtbspb,2, …, xtbspb,6*, Hybrid-ARQ-process information *xhap,1,xhap,2, …, xhap,4* and redundancy-version information *xrvpb,1, xrvpb,2* are multiplexed together. This gives a sequence of bits *x2,1, x2,2, …, x2,12* where

*x2,i = xtbs,i i=1,2,…,6*

*x2,i = xhap,i-6 i=7,8,…,10*

*x2,i = xrv,i-10 i=11,12*

If two transport blocks are transmitted on the associated HS-PDSCHs, the transport-block-size information for the primary transport block *xtbspb,1, xtbspb,2, …, xtbspb,6*, transport-block-size information for the second transport block *xtbssb,1, xtbssb,2, …, xtbssb,6*, Hybrid-ARQ-process information *xhap,1,xhap,2, …, xhap,4*, redundancy-version information for the primary transport block *xrvpb,1, xrvpb,2*, and redundancy-version information for the second transport block *xrvsb,1, xrvsb,2* are multiplexed together. This gives a sequence of bits *x2,1, x2,2, …, x2,20* where

*x2,i = xtbspb,i  i=1,2,…,6*

*x2,i = xtbssb,i-6 i=7,8,…,12*

*x2,i = xhap,i-12 i=13,14,...,16*

*x2,i = xrvpb,i-16 i=17,18*

*x2,i = xrvsb,i-18 i=19,20*

If three transport blocks are transmitted on the associated HS-PDSCHs, the transport-block-size information for the primary transport block *xtbspb,1, xtbspb,2, …, xtbspb,6*, transport-block-size information for the second and the third transport blocks *xtbssb,1, xtbssb,2, …, xtbssb,6*, Hybrid-ARQ-process information *xhap,1,xhap,2, …, xhap,4*, redundancy-version information for the primary transport block *xrvpb,1, xrvpb,2*, and redundancy-version information for the second and the third transport blocks *xrvsb,1, xrvsb,2* are multiplexed together. This gives a sequence of bits *x2,1, x2,2, …, x2,20* where

*x2,i = xtbspb,i  i=1,2,…,6*

*x2,i = xtbssb,i-6 i=7,8,…,12*

*x2,i = xhap,i-12 i=13,14,...,16*

*x2,i = xrvpb,i-16 i=17,18*

*x2,i = xrvsb,i-18 i=19,20*

If four transport blocks are transmitted on the associated HS-PDSCHs, the transport-block-size information for the primary and the fourth transport blocks *xtbspb,1, xtbspb,2, …, xtbspb,6*, transport-block-size information for the second and the third transport blocks *xtbssb,1, xtbssb,2, …, xtbssb,6*, Hybrid-ARQ-process information *xhap,1,xhap,2, …, xhap,4*, redundancy-version information for the primary and the fourth transport blocks *xrvpb,1, xrvpb,2*, and redundancy-version information for the second and the third transport blocks *xrvsb,1, xrvsb,2* are multiplexed together. This gives a sequence of bits *x2,1, x2,2, …, x2,20* where

*x2,i = xtbspb,i  i=1,2,…,6*

*x2,i = xtbssb,i-6 i=7,8,…,12*

*x2,i = xhap,i-12 i=13,14,...,16*

*x2,i = xrvpb,i-16 i=17,18*

*x2,i = xrvsb,i-18 i=19,20*

### 4.6D.4 CRC attachment for HS-SCCH type 4

If one transport block is transmitted on the associated HS-PDSCH(s), from the sequence of bits *x1,1, x1,2, …, x1,16,, x2,1, x2,2, …, x2,12* a 16-bit CRC is calculated according to Clause 4.2.1.1. This gives a sequence of bits *c1, c2, …, c16* where

*k=1,2,…,16*

This sequence of bits is then masked with the UE Identity *xue,1, xue,2, …, xue,16* and then appended to the sequence of bits *x2,1, x2,2, …, x2,12* to form the sequence of bits *y1, y2, …, y28*, where

*yi = x2,i i=1,2,…,12*

*yi =* (*ci-12* + *xue*,i-12 ) mod 2 *i=13,14,…,28*

If more than one transport blocks are transmitted on the associated HS-PDSCHs, from the sequence of bits *x1,1, x1,2, …, x1,16, x2,1, x2,2, …, x2,20* a 16-bit CRC is calculated according to Clause 4.2.1.1. This gives a sequence of bits *c1, c2, …, c16* where

*k=1,2,…,16*

This sequence of bits is then masked with the UE Identity *xue,1, xue,2, …, xue,16* and then appended to the sequence of bits *x2,1, x2,2, …, x2,20* to form the sequence of bits *y1, y2, …, y36*, where

*yi = x2,i i=1,2,…,20*

*yi =* (*ci-20* + *xue*,i-20) mod 2 *i=21,22,…,36*

### 4.6D.5 Channel coding for HS-SCCH type 4

Rate 1/2 convolutional coding, as described in Clause 4.2.3.1, is applied to the sequence of bits x*1,1,x1,2, …,x1,16*. This gives a sequence of bits *z1,1, z1,2, …, z1,48*.

If one transport block is transmitted on the associated HS-PDSCH(s), rate 1/3 convolutional coding, as described in Clause 4.2.3.1, is applied to the sequence of bits *y1, y2, …, y28*. This gives a sequence of bits *z2,1, z2,2, …, z2,108*.

If more than one transport blocks are transmitted on the associated HS-PDSCHs, rate 1/3 convolutional coding, as described in Clause 4.2.3.1, is applied to the sequence of bits *y1, y2, …, y36*. This gives a sequence of bits *z2,1, z2,2, …, z2,132*.

Note that the coded sequence lengths result from the termination of K=9 convolutional coding being fully applied.

### 4.6D.6 Rate matching for HS-SCCH type 4

From the input sequence *z1,1, z1,2, …, z1, 48* the bits *z1,1, z1,2, z1,4, z1,8, z1,42, z1,45, z1,47, z1,48* are punctured to obtain the output sequence *r1,1,r1,2…r1,40*.

If one transport block is transmitted on the associated HS-PDSCH(s), from the input sequence *z2,1, z2,2, …, z2,108* the bits *z2,1, z2,2, z2,3, z2,4, z2,5, z2,6, z2,7, z2,8, z2,12, z2,14, z2,15, z2,24, z2,42, z2,48, z2,63, z2,66, z2,93, z2,96, z2,98, z2,99, z2,101, z2,102, z2,103, z2,104, z2,105, z2,106, z2,107, z2,108* are punctured to obtain the output sequence *r2,1,r2,2…r2,80*.

If more than one transport blocks are transmitted on the associated HS-PDSCHs, from the input sequence *z2,1, z2,2, …, z2,132* the bits *z2,1, z2,2, z2,3, z2,4, z2,5, z2,6, z2,7, z2,8, z2,10, z2,11, z2,13, z2,14, z2,16, z2,19, z2,22, z2,25, z2,28, z2,31, z2,34, z2,37, z2,40, z2,43, z2,46, z2,49, z2,55, z2,61, z2,72, z2,78, z2,84, z2,87, z2,90, z2,93, z2,96, z2,99, z2,102 , z2,105, z2,108, z2,111, z2,114, z2,117, z2,119, z2,120, z2,122, z2,123, z2,125, z2,126, z2,127, z2,128, z2,129, z2,130, z2,131, z2,132* are punctured to obtain the output sequence *r2,1,r2,2…r2,80*.

### 4.6D.7 UE specific masking for HS-SCCH type 4

The output bits *s1,1,s1,2…s1,40* are calculated as described in subclause 4.6.7.

### 4.6D.8 Physical channel mapping for HS-SCCH type 4

The HS-SCCH sub-frame is described in [2]. The physical channel mapping is carried out as described in subclause 4.6.8.

## 4.7 Coding for HS-DPCCH

### 4.7.1 Overview

Data arrives to the coding unit in form of indicators for measurement indication and HARQ acknowledgement.

The following coding/multiplexing steps can be identified:

- channel coding (see subclauses 4.7.2, 4.7.3, 4.7.3A, 4.7.3B, 4.7.3C, 4.7.3D and 4.7.3E);

- mapping to physical channels (see subclause 4.7.4).

The coding/multiplexing for HS-DPCCH is defined separately for the following cases:

- when the UE is not configured in MIMO mode and not configured in MIMO mode with four transmit antennas in the serving HS-DSCH cell, and Secondary\_Cell\_Enabled is 0 or 1 and Secondary\_Cell\_Active is 0 (see subclause 4.7.2);

- when the UE is configured in MIMO mode in the serving HS-DSCH cell and Secondary\_Cell\_Enabled is 0 (see subclause 4.7.3);

- when the UE is configured in MIMO mode in at least the serving HS-DSCH cell, and Secondary\_Cell\_Enabled is 1 and Secondary\_Cell\_Active is 0 (see subclause 4.7.3B);

- when the UE is not configured in MIMO mode in any cell and Secondary\_Cell\_Enabled is 1 and Secondary\_Cell\_Active is 1 (see subclause 4.7.3A);

- when the UE is configured in MIMO mode in at least one cell and Secondary\_Cell\_Enabled is 1 and Secondary\_Cell\_Active is 1 (see subclause 4.7.3B);

- when Secondary\_Cell\_Enabled is equal to 2 or 3 (see applicable subclauses in Table 14C and 14D)

- when Secondary\_Cell\_Enabled is more than 3 (see applicable subclauses in Table 14C.1 and 14D.1)

- when the UE is configured in Multiflow mode, see subclause 4.7.3D

- when the UE is configured in MIMO mode with four transmit antennas at least in one cell, see subclause 4.7.3E

where Secondary\_Cell\_Enabled and Secondary\_Cell\_Active are defined in [4].

Table 14C: Coding for HARQ-ACK when Secondary\_Cell\_Enabled is 2 or 3

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **Secondary Cell Enabled is 2 UE is configured with two secondary serving HS-DSCH cells** | | | | |
| **Secondary\_Cell\_Active** | **Condition** | **Serving HS-DSCH cell** | **1st Secondary Serving HS-DSCH cell** | **2nd Secondary Serving HS-DSCH cell** | **3rd Secondary Serving HS-DSCH cell** |
| 0, 1, 2 | MIMO mode and MIMO mode with four transmit antennas is not configured in any cell | 4.7.3C.1 (Note 1) | | | N/A |
| 0 | MIMO mode is configured in at least one cell | 4.7.3B.1 (Note 3) | | | N/A |
| 1 | MIMO mode is configured in at least one cell | 4.7.3B.1 (Note 2) | | | N/A |
| 2 | MIMO mode is configured in at least one cell | 4.7.3B.1 | | 4.7.3B.1 (Note 4) | N/A |
|  | **Secondary Cell Enabled is 3 UE is configured with three secondary serving HS-DSCH cells** | | | | |
| **Secondary\_Cell\_Active** | **Condition** | **Serving HS-DSCH cell** | **1st Secondary Serving HS-DSCH cell** | **2nd Secondary Serving HS-DSCH cell** | **3rd Secondary Serving HS-DSCH cell** |
| 0 | - | 4.7.3B.1 (Note 3) | | | |
| 1 | - | 4.7.3B.1 (Note 2) | | | |
| 2, 3 | - | 4.7.3B.1 (Note 1) | | 4.7.3B.1 (Note 1) | |

Note 1: When a cell is deactivated, DTX message is indicated for that cell.

Note 2: HARQ-ACK information is jointly encoded for the pair of serving HS-DSCH cell and the active secondary serving HS-DSCH cell and repeated to fill the whole HARQ-ACK slot in the HS-DPCCH sub-frame as described in subclause 4.7.4.1.

Note 3: HARQ-ACK information for the serving HS-DSCH cell is repeated to fill the whole HARQ-ACK slot in the HS-DPCCH sub-frame as described in subclause 4.7.4.1.

Note 4: HARQ-ACK information for the 2nd secondary serving HS-DSCH cell is jointly encoded with a DTX message in place of the 3rd secondary serving HS-DSCH cell as described in subclause 4.7.3B.1.

Table 14C.1: Coding for HARQ-ACK of HS-DPCCH when Secondary\_Cell\_Enabled is more than 3

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **Secondary Cell Enabled is more than 3 UE is configured with more than 3 secondary serving HS-DSCH cells** | | | |
| **Number of active cells mapped to the HS-DPCCH** | **Serving HS-DSCH cell** | **1st Secondary Serving HS-DSCH cell** | **2nd Secondary Serving HS-DSCH cell** | **3rd Secondary Serving HS-DSCH cell** |
| **1** | 4.7.3B.1 (Note 1) | | | |
| **2** | 4.7.3B.1 (Note 2) | | | |
| **3** | 4.7.3B.1 (Note 3) | | 4.7.3B.1 (Note 3) | |
| **4** | 4.7.3B.1 | | 4.7.3B.1 | |

Note 1: The HARQ-ACK information is repeated to the fill the whole HARQ-ACK slot of HS-DPCCH sub-frame as described in subclause 4.7.4.1.

Note 2: HARQ-ACK information is jointly encoded for the pair of serving HS-DSCH cell and the active secondary serving HS-DSCH cell and repeated to fill the whole HARQ-ACK slot in the HS-DPCCH sub-frame as described in subclause 4.7.4.1.

Note 3: If one of the 1st, 2nd, or 3rd secondary serving HS-DSCH cells is deactivated a DTX message is indicated for the deactivated cell.

Table 14C.2: Coding for HARQ-ACK transmitted on HS-DPCCH2 when Secondary\_Cell\_Enabled is more than 3

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **Secondary Cell Enabled is more than 3 UE is configured with more than 3 secondary serving HS-DSCH cells** | | | |
| **Number of active cells mapped to the HS-DPCCH2** | **4th secondary serving HS-DSCH cell** | **5th Secondary Serving HS-DSCH cell** | **6th Secondary Serving HS-DSCH cell** | **7th Secondary Serving HS-DSCH cell** |
| **1** | 4.7.3B.1 (Note 1) | | | |
| **2** | 4.7.3B.1 (Note 2) | | | |
| **3** | 4.7.3B.1 (Note 3) | | 4.7.3B.1 (Note 3) | |
| **4** | 4.7.3B.1 | | 4.7.3B.1 | |

Note 1: The HARQ-ACK information is repeated to the fill the whole HARQ-ACK slot of HS-DPCCH2 sub-frame as described in subclause 4.7.4.1.

Note 2: The HARQ-ACK information for the two activated secondary serving HS-DSCH cells are jointly encoded and repeated to fill the whole HARQ-ACK slot in the HS-DPCCH2 sub-frame as described in subclause 4.7.4.1.

Note 3: If one of the 4th, 5th, 6th, and 7th secondary serving HS-DSCH cells is deactivated a DTX message is indicated for the deactivated cell.

The order of the cells in HARQ-ACK joint encoding is specified in detail in subclause 4.7.4.1.

Table 14D: Coding for PCI/CQI when Secondary\_Cell\_Enabled is 2 or 3

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **Secondary Cell Enabled is 2 UE is configured with two secondary serving HS-DSCH cells** | | | |
| **Secondary\_Cell\_Active** | **Serving HS-DSCH cell** | **1st Secondary Serving HS-DSCH cell** | **2nd Secondary Serving HS-DSCH cell** | **3rd Secondary Serving HS-DSCH cell** |
| 0, 1 | The CQI information for a cell not configured in MIMO mode and not configured in MIMO mode with four transmit antennas is encoded according to subclause 4.7.2.2(Note 1)The composite PCI/CQI information for a cell configured with MIMO mode is encoded according to subclause 4.7.3.2 (Note 3) | | | N/A |
| 2 MIMO is not configured in any cell | The CQI information for the serving HS-DSCH cell is encoded using subclause 4.7.2.2 | The CQI information for the 1st secondary serving HS-DSCH cell and the 2nd secondary serving HS-DSCH cell is encoded according to subclause 4.7.3A.2 | | N/A |
| 2 (Otherwise) Note 4 | The CQI information for a cell not configured in MIMO mode and not configured in MIMO mode with four transmit antennas is encoded according to subclause 4.7.2.2. The composite PCI/CQI information for a cell configured with MIMO mode is encoded according to subclause 4.7.3.2 | | | N/A |
|  | **Secondary Cell Enabled is 3 UE is configured with three secondary serving HS-DSCH cells** | | | |
| **Secondary\_Cell\_Active** | **Serving HS-DSCH cell** | **1st Secondary Serving HS-DSCH cell** | **2nd Secondary Serving HS-DSCH cell** | **3rd Secondary Serving HS-DSCH cell** |
| 0, 1 Note 3 | The CQI information for a cell not configured in MIMO mode and not configured in MIMO mode with four transmit antennas is encoded according to subclause 4.7.2.2. The composite PCI/CQI information for a cell configured with MIMO mode is encoded according to subclause 4.7.3.2 | | | |
| 2, 3 Note 2 |

Note 1: If the UE is configured with MIMO mode in at least one cell, the CQI field for each active cell is repeated to fill the two slot CQI field in the HS-DPCCH sub-frame as described in subclause 4.7.4.2.

Note 2: In the deactivated cell, the PCI/CQI field is DTXed.

Note 3: The CQI or PCI/CQI for each active cell is repeated to fill the two slot CQI or PCI/CQI field in the HS-DPCCH sub-frame as described in subclause 4.7.4.2.

Note 4: The PCI/CQI field for the 3rd secondary serving HS-DSCH cell is DTXed.

Table 14D.1: Coding for PCI/CQI transmitted on HS-DPCCH when Secondary\_Cell\_Enabled is more than 3

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Secondary Cell Enabled more than 3 UE is configured with more than 3 secondary serving HS-DSCH cells | | | |
| Number of active cells mapped to the HS-DPCCH | Serving HS-DSCH cell | 1st Secondary Serving HS-DSCH cell | 2nd Secondary Serving HS-DSCH cell | 3rd Secondary Serving HS-DSCH cell |
| 1, 2  Note 1 | The CQI information for a cell not configured in MIMO mode and not configured in MIMO mode with four transmit antennas is encoded according to subclause 4.7.2.2. The composite PCI/CQI information for a cell configured with MIMO mode is encoded according to subclause 4.7.3.2. | | | |
| 3, 4  Note 2 |

Note 1: The CQI or PCI/CQI for each active cell is repeated to fill the two slot CQI or PCI/CQI field in the corresponding HS-DPCCH sub-frame as described in subclause 4.7.4.2.

Note 2: In the deactivated cell, the PCI/CQI field is DTXed.

Table 14D.2: Coding for PCI/CQI transmitted on HS-DPCCH2 when Secondary\_Cell\_Enabled is more than 3

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Secondary Cell Enabled more than 3 UE is configured with more than 3 secondary serving HS-DSCH cells | | | |
| Number of active cells mapped to the HS-DPCCH2 | 4th Secondary serving HS-DSCH cell | 5th Secondary Serving HS-DSCH cell | 6th Secondary Serving HS-DSCH cell | 7th Secondary Serving HS-DSCH cell |
| 1, 2  Note 1 | The CQI information for a cell not configured in MIMO mode and not configured in MIMO mode with four transmit antennas is encoded according to subclause 4.7.2.2. The composite PCI/CQI information for a cell configured with MIMO mode is encoded according to subclause 4.7.3.2. | | | |
| 3, 4  Note 2 |

Note 1: The CQI or PCI/CQI for each active cell is repeated to fill the two slot CQI or PCI/CQI field in the corresponding HS-DPCCH sub-frame as described in subclause 4.7.4.2.

Note 2: In the deactivated cell, the PCI/CQI field is DTXed.

For each HS-DPCCH the general coding flow when the UE is not configured in MIMO mode and not configured in MIMO mode with four transmit antennas is shown in the figure 20. This is done in parallel for the HARQ-ACK and CQI as the flows are not directly multiplexed but are transmitted at different times.



Figure 20: Coding for each HS-DPCCH when the UE is not configured in MIMO mode and not configured in MIMO mode with four transmit antennas

In case the UE is configured in MIMO mode, the measurement indication consists of precoding control indication (PCI) and channel quality indication (CQI). For each HS-DPCCH the general coding flow when the UE is configured in MIMO mode is shown in the figure 20A. This is done in parallel for the flow of HARQ-ACK and for the flow of composite PCI/CQI reports as the two flows are not directly multiplexed but are transmitted at different times



Figure 20A: Coding for each HS-DPCCH when the UE is configured in MIMO mode

In case the UE is configured in MIMO mode with four transmit antennas, the measurement indication consists of number of transport blocks preferred (NTBP), precoding control indication (PCI) and channel quality indication (CQI). For each HS-DPCCH the general coding flow when the UE is configured in MIMO mode with four transmit antennas is shown in the figure 20A.1. This is done in parallel for the flow of HARQ-ACK and for the flow of composite NTBP/PCI/CQI reports as the two flows are not directly multiplexed but are transmitted at different times



Figure 20A.1: Coding for each HS-DPCCH when the UE is configured in MIMO mode with four transmit antennas

### 4.7.2 Channel coding for HS-DPCCH when the UE is not configured in MIMO mode and not configured in MIMO mode with four transmit antennas in the serving HS-DSCH cell and Secondary\_Cell\_Enabled is 0 or 1 and Secondary\_Cell\_Active is 0

Two forms of channel coding are used, one for the channel quality indication (CQI) and another for HARQ-ACK (acknowledgement).

#### 4.7.2.1 Channel coding for HS-DPCCH HARQ-ACK

The HARQ acknowledgement message to be transmitted, as defined in [4], shall be coded to 10 bits as shown in Table 15. The output is denoted w0, w1,…w9.

Table 15: Channel coding of HARQ-ACK when the UE is not configured in MIMO mode and not configured in MIMO mode with four transmit antennas in the serving HS-DSCH cell and Secondary\_Cell\_Enabled is 0 or 1 and Secondary\_Cell\_Active is 0

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| HARQ-ACK message to be transmitted | w0 | w1 | w2 | w3 | w4 | w5 | w6 | w7 | w8 | w9 |
| ACK | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 |
| NACK | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 |
| PRE | 0 | 0 | 1 | 0 | 0 | 1 | 0 | 0 | 1 | 0 |
| POST | 0 | 1 | 0 | 0 | 1 | 0 | 0 | 1 | 0 | 0 |

#### 4.7.2.2 Channel coding for HS-DPCCH channel quality indication

The channel quality indication is coded using a (20,5) code. The code words of the (20,5) code are a linear combination of the 5 basis sequences denoted Mi,n defined in the table below.

Table 15A: Basis sequences for (20,5) code

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| i | Mi,0 | Mi,1 | Mi,2 | Mi,3 | Mi,4 |
| 0 | 1 | 0 | 0 | 0 | 1 |
| 1 | 0 | 1 | 0 | 0 | 1 |
| 2 | 1 | 1 | 0 | 0 | 1 |
| 3 | 0 | 0 | 1 | 0 | 1 |
| 4 | 1 | 0 | 1 | 0 | 1 |
| 5 | 0 | 1 | 1 | 0 | 1 |
| 6 | 1 | 1 | 1 | 0 | 1 |
| 7 | 0 | 0 | 0 | 1 | 1 |
| 8 | 1 | 0 | 0 | 1 | 1 |
| 9 | 0 | 1 | 0 | 1 | 1 |
| 10 | 1 | 1 | 0 | 1 | 1 |
| 11 | 0 | 0 | 1 | 1 | 1 |
| 12 | 1 | 0 | 1 | 1 | 1 |
| 13 | 0 | 1 | 1 | 1 | 1 |
| 14 | 1 | 1 | 1 | 1 | 1 |
| 15 | 0 | 0 | 0 | 0 | 1 |
| 16 | 0 | 0 | 0 | 0 | 1 |
| 17 | 0 | 0 | 0 | 0 | 1 |
| 18 | 0 | 0 | 0 | 0 | 1 |
| 19 | 0 | 0 | 0 | 0 | 1 |

The CQI values 0 ... 30 as defined in [4] are converted from decimal to binary to map them to the channel quality indication bits (1 0 0 0 0) to (1 1 1 1 1) respectively. The information bit pattern (0 0 0 0 0) shall not be used in this release. The channel quality indication bits are a0 , a1 , a2 , a3 , a4 (where a0 is LSB and a4 is MSB). The output code word bits bi are given by:

where *i* = 0, …, 19.

### 4.7.3 Channel coding for HS-DPCCH when the UE is configured in MIMO mode in the serving HS-DSCH cell and Secondary\_Cell\_Enabled is 0

Two forms of channel coding are used, one for the composite precoding control indication (PCI) and channel quality indication (CQI) and another for HARQ-ACK (acknowledgement).

#### 4.7.3.1 Channel coding for HS-DPCCH HARQ-ACK

The HARQ acknowledgement message to be transmitted, as defined in [4], shall be coded to 10 bits as shown in Table 15B. The output is denoted w0, w1,…w9.

Table 15B: Channel coding of HARQ-ACK when the UE is configured in MIMO mode in the serving HS-DSCH cell and Secondary\_Cell\_Enabled is 0

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| HARQ-ACK message to be transmitted | | w0 | w1 | w2 | w3 | w4 | w5 | w6 | w7 | w8 | w9 |
| HARQ-ACK in response to a single scheduled transport block | | | | | | | | | | | |
| ACK | | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 |
| NACK | | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 |
| HARQ-ACK in response to two scheduled transport blocks | | | | | | | | | | | |
| Response to primary transport block | Response to secondary transport block |  | | | | | | | | | |
| ACK | ACK | 1 | 0 | 1 | 0 | 1 | 1 | 1 | 1 | 0 | 1 |
| ACK | NACK | 1 | 1 | 0 | 1 | 0 | 1 | 0 | 1 | 1 | 1 |
| NACK | ACK | 0 | 1 | 1 | 1 | 1 | 0 | 1 | 0 | 1 | 1 |
| NACK | NACK | 1 | 0 | 0 | 1 | 0 | 0 | 1 | 0 | 0 | 0 |
| PRE/POST indication | | | | | | | | | | | |
| PRE | | 0 | 0 | 1 | 0 | 0 | 1 | 0 | 0 | 1 | 0 |
| POST | | 0 | 1 | 0 | 0 | 1 | 0 | 0 | 1 | 0 | 0 |

#### 4.7.3.2 Channel coding for HS-DPCCH composite precoding control indication and channel quality indication

When the UE is configured in MIMO mode and single-stream restriction is not configured, two types of CQI reports shall be supported by the UE. According to the definition of the CQI reporting procedure in [4], type A CQI reports use values 0 … 255 and type B CQI reports use values 0 … 30, respectively. When the UE is configured in MIMO mode and single-stream restriction is configured, only type B shall be supported by the UE.

##### 4.7.3.2.1 Bit mapping of Type A channel quality indication

In case a type A CQI shall be reported, the CQI values 0 ... 255 as defined in [4] are converted from decimal to binary to map them to the channel quality indication bits (0 0 0 0 0 0 0 0) to (1 1 1 1 1 1 1 1), respectively. The channel quality indication bits are cqi0 , cqi1 , cqi2 , cqi3 , cqi4, cqi5, cqi6, cqi7 (where cqi0 is LSB and cqi7 is MSB).

##### 4.7.3.2.2 Bit mapping of Type B channel quality indication

In case a type B CQI shall be reported, the CQI values 0 ... 30 as defined in [4] are converted from decimal to binary to map them to the channel quality indication bits (1 0 0 0 0) to (1 1 1 1 1), respectively. The information bit pattern (0 0 0 0 0) shall not be used in this release. The channel quality indication bits are cqi0, cqi1, cqi2, cqi3, cqi4 (where cqi0 is LSB and cqi4 is MSB).

##### 4.7.3.2.3 Bit mapping of precoding control indication

According to the PCI definition in [4], the range of possible PCI values is 0 ... 3. The PCI values 0 ... 3 as defined in [4] are converted from decimal to binary to map them to the precoding control indication bits (0 0) to (1 1) respectively. The precoding control indication bits are pci0 , pci1 (where pci0 is LSB and pci1 is MSB).

##### 4.7.3.2.4 Composite precoding control indication and channel quality indication bits

Two formats for composite PCI/CQI information words are possible depending on the type of the reported CQI value. The two formats shall be constructed according to the scheme depicted in Figure 20B.



Figure 20B: Construction of composite PCI/CQI report

In case a type A CQI shall be reported, the precoding control indication bits pci0 , pci1, and the channel quality indication bits cqi0 , cqi1 , cqi2 , cqi3 , cqi4, cqi5, cqi6, cqi7 are concatenated to the composite precoding control indication and channel quality indication bits according to the relation

In case a type B CQI shall be reported, the precoding control indication bits pci0 , pci1, and the channel quality indication bits cqi0 , cqi1 , cqi2 , cqi3 , cqi4 are concatenated to the composite precoding control indication and channel quality indication bits according to the relation

##### 4.7.3.2.5 Block encoding of composite precoding control indication and channel quality indication bits

In case a type A CQI needs to be reported, the composite precoding control indication and channel quality indication is coded using a (20,10) code. The code words of the (20,10) code are a linear combination of the 10 basis sequences denoted Mi,n defined in the table 15C below.

Table 15C: Basis sequences for channel encoding of composite PCI/CQI reports

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| i | Mi,0 | Mi,1 | Mi,2 | Mi,3 | Mi,4 | Mi,5 | Mi,6 | Mi,7 | Mi,8 | Mi,9 | Mi,10 |
| 0 | 1 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 |
| 1 | 0 | 1 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 |
| 2 | 0 | 0 | 0 | 1 | 0 | 0 | 0 | 0 | 0 | 0 | 0 |
| 3 | 0 | 0 | 0 | 0 | 1 | 0 | 0 | 0 | 0 | 0 | 0 |
| 4 | 0 | 0 | 0 | 0 | 0 | 1 | 0 | 0 | 0 | 0 | 0 |
| 5 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 1 | 0 | 0 | 0 |
| 6 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 1 | 0 | 1 |
| 7 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 1 | 1 |
| 8 | 1 | 0 | 1 | 0 | 0 | 0 | 1 | 1 | 1 | 0 | 1 |
| 9 | 1 | 1 | 0 | 1 | 0 | 0 | 0 | 1 | 1 | 1 | 1 |
| 10 | 0 | 1 | 1 | 0 | 1 | 0 | 0 | 0 | 1 | 1 | 1 |
| 11 | 1 | 0 | 1 | 1 | 0 | 1 | 0 | 0 | 0 | 1 | 0 |
| 12 | 1 | 1 | 0 | 1 | 1 | 0 | 1 | 0 | 0 | 0 | 0 |
| 13 | 1 | 1 | 1 | 0 | 1 | 1 | 0 | 1 | 0 | 0 | 0 |
| 14 | 0 | 1 | 1 | 1 | 0 | 1 | 1 | 0 | 1 | 0 | 1 |
| 15 | 0 | 0 | 1 | 1 | 1 | 0 | 1 | 1 | 0 | 1 | 0 |
| 16 | 0 | 0 | 0 | 1 | 1 | 1 | 0 | 1 | 1 | 0 | 1 |
| 17 | 1 | 0 | 0 | 0 | 1 | 1 | 1 | 0 | 1 | 1 | 1 |
| 18 | 0 | 1 | 0 | 0 | 0 | 1 | 1 | 1 | 0 | 1 | 0 |
| 19 | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 |

The output code word bits bi are given by:

where *i* = 0, …, 19.

In case a type B CQI needs to be reported, the composite precoding control indication and channel quality indication is coded using a (20,7) code. The code words of the (20,7) code are a linear combination of the basis sequences denoted Mi,n defined in the table 15C for.

The output code word bits bi are given by:

where *i* = 0, …, 19.

### 4.7.3A Channel coding for HS-DPCCH when the UE is not configured in MIMO mode in any cell and Secondary\_Cell\_Enabled is 1 and Secondary\_Cell\_Active is 1

Two forms of channel coding are used, one for the composite channel quality indication (CQI) and another for the composite HARQ-ACK (acknowledgement).

#### 4.7.3A.1 Channel coding for the composite HS-DPCCH HARQ-ACK

The composite HARQ acknowledgement message to be transmitted, as defined in [4], shall be coded to 10 bits as shown in Table 15C.1. The output is denoted w0, w1,…w9.

Table 15C.1: Channel coding of HARQ-ACK when the UE is not configured in MIMO mode in a pair of serving HS-DSCH cells and Secondary\_Cell\_Enabled is 1 and Secondary\_Cell\_Active is 1

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| HARQ-ACK message to be transmitted | | w0 | w1 | w2 | w3 | w4 | w5 | w6 | w7 | w8 | w9 |
| HARQ-ACK when UE detects a single scheduled transport block on the serving HS-DSCH cell | | | | | | | | | | | |
| ACK | | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 |
| NACK | | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 |
| HARQ-ACK when UE detects a single scheduled transport block on the secondary serving HS-DSCH cell | | | | | | | | | | | |
| ACK | | 1 | 1 | 1 | 1 | 1 | 0 | 0 | 0 | 0 | 0 |
| NACK | | 0 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 1 | 1 |
| HARQ-ACK when UE detects a single scheduled transport block on each of the serving and secondary serving HS-DSCH cells | | | | | | | | | | | |
| Response to transport block from serving HS-DSCH cell | Response to transport block from secondary serving HS-DSCH cell |  | | | | | | | | | |
| ACK | ACK | 1 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 | 0 |
| ACK | NACK | 1 | 1 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 1 |
| NACK | ACK | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 1 | 0 | 0 |
| NACK | NACK | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 |
| PRE/POST indication | | | | | | | | | | | |
| PRE | | 0 | 0 | 1 | 0 | 0 | 1 | 0 | 0 | 1 | 0 |
| POST | | 0 | 1 | 0 | 0 | 1 | 0 | 0 | 1 | 0 | 0 |

#### 4.7.3A.2 Channel coding for HS-DPCCH composite channel quality indication

##### 4.7.3A.2.1 Composite channel quality indication bits

The composite CQI report is constructed from two individual CQI reports that are represented by CQI1 and CQI2. CQI1 corresponds to the serving HS-DSCH cell and CQI2 corresponds to the secondary serving HS-DSCH cell.

Each constituent CQI report uses values 0 … 30 in accordance with the definition of the CQI reporting procedure in [4]. The individual CQI values are converted from decimal to binary to map them to the channel quality indication bits (1 0 0 0 0) to (1 1 1 1 1) respectively. The information bit pattern (0 0 0 0 0) shall not be used in this release.

The channel quality indication bits corresponding to CQI1 are cqi10, cqi11, cqi12, cqi13, cqi14 (where cqi10 is LSB and cqi14 is MSB) and those corresponding to CQI2 are cqi20, cqi21, cqi22, cqi23, cqi24 (where cqi20 is LSB and cqi24 is MSB).

The composite CQI report is constructed according to the scheme depicted in Figure 20C



Figure 20C: Construction of composite CQI report

The two individual CQI reports are concatenated to form the composite channel quality indication according to the relation

##### 4.7.3A.2.2 Block encoding of composite channel quality indication bits

The composite channel quality indication is coded using a (20,10) code. The code words of the (20,10) code are a linear combination of the 10 basis sequences denoted Mi,n defined in Table 15C.

The output code word bits bi are given by:

where *i* = 0, …, 19 and *a0,…, a9* are defined in the previous subclause.

### 4.7.3B Channel coding for HS-DPCCH when Secondary\_Cell\_Enabled is at least 3 or when the UE is configured in MIMO mode in at least one cell and Secondary\_Cell\_Enabled is greater than 0

Two forms of channel coding are used, one for the composite precoding control indication (PCI) and channel quality indication (CQI) and another for the composite HARQ-ACK (acknowledgement).

#### 4.7.3B.1 Channel coding for the composite HS-DPCCH HARQ-ACK

The composite HARQ acknowledgement message to be transmitted, as defined in [4], shall be coded to 10 bits as shown in Table 15C.2. The feedback related to the first cell is given before the divider sign and the feedback related to the second cell is given after the divider sign. ''A’ means ''ACK’, ''N’ means ''NACK’ and ''D’ means ''no transmission’ (''DTX’). ''AA’, ''AN’, ''NA’ and ''NN’ refer to feedback for dual-stream transmission in a cell. For example, ''AN’ means ACK on the primary stream and NACK on the secondary stream. The output is denoted w0, w1,…w9.

When Secondary\_Cell\_Enabled is 2, and when Secondary\_Cell\_Active is 2, HARQ-ACK information for the 2nd secondary serving HS-DSCH cell is jointly encoded with a DTX message in place of the 3rd secondary serving HS-DSCH cell.

When Secondary\_Cell\_Enabled is 4, and when Secondary\_Cell\_Active is 4, HARQ-ACK information for the 4th secondary serving HS-DSCH cell is jointly encoded with a DTX message in place of the 5th secondary serving HS-DSCH cell.

When Secondary\_Cell\_Enabled is 6, and when Secondary\_Cell\_Active is 6, HARQ-ACK information for the 6th secondary serving HS-DSCH cell is jointly encoded with a DTX message in place of the 7th secondary serving HS-DSCH cell.

Table 15C.2: Channel coding of HARQ-ACK when Secondary\_Cell\_Enabled is at least 3 or the UE is configured in MIMO mode in at least one cell and Secondary\_Cell\_Enabled is greater than 0

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| HARQ-ACK message to be transmitted | w0 | w1 | w2 | w3 | w4 | w5 | w6 | w7 | w8 | w9 |  | HARQ-ACK message to be transmitted | w0 | w1 | w2 | w3 | w4 | w5 | w6 | w7 | w8 | w9 |
| A/D | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 |  | AA/A | 0 | 1 | 1 | 0 | 0 | 0 | 0 | 1 | 0 | 0 |
| N/D | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | AA/N | 1 | 1 | 1 | 0 | 0 | 1 | 1 | 0 | 1 | 0 |
| AA/D | 1 | 0 | 1 | 0 | 1 | 1 | 1 | 1 | 0 | 1 | AN/A | 1 | 0 | 1 | 1 | 1 | 0 | 0 | 1 | 1 | 0 |
| AN/D | 1 | 1 | 0 | 1 | 0 | 1 | 0 | 1 | 1 | 1 | AN/N | 0 | 0 | 1 | 1 | 0 | 1 | 0 | 0 | 0 | 1 |
| NA/D | 0 | 1 | 1 | 1 | 1 | 0 | 1 | 0 | 1 | 1 | NA/A | 0 | 1 | 0 | 1 | 1 | 1 | 1 | 1 | 0 | 0 |
| NN/D | 1 | 0 | 0 | 1 | 0 | 0 | 1 | 0 | 0 | 0 | NA/N | 1 | 1 | 0 | 0 | 1 | 0 | 0 | 0 | 0 | 1 |
| D/A | 0 | 0 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 1 | NN/A | 0 | 0 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 0 |
| D/N | 1 | 1 | 1 | 1 | 1 | 1 | 0 | 0 | 0 | 0 | NN/N | 0 | 1 | 0 | 0 | 0 | 1 | 1 | 0 | 0 | 1 |
| D/AA | 1 | 0 | 0 | 0 | 1 | 0 | 0 | 0 | 1 | 1 | AA/AA | 0 | 1 | 1 | 0 | 1 | 1 | 0 | 1 | 1 | 1 |
| D/AN | 0 | 1 | 0 | 0 | 0 | 0 | 1 | 1 | 0 | 1 | AA/AN | 1 | 0 | 1 | 1 | 0 | 0 | 1 | 1 | 1 | 1 |
| D/NA | 0 | 0 | 0 | 1 | 1 | 1 | 1 | 1 | 1 | 0 | AA/NA | 1 | 1 | 0 | 1 | 1 | 1 | 1 | 0 | 0 | 1 |
| D/NN | 1 | 1 | 1 | 1 | 1 | 0 | 0 | 1 | 0 | 0 | AA/NN | 0 | 1 | 1 | 1 | 0 | 1 | 1 | 1 | 0 | 0 |
| A/A | 1 | 1 | 0 | 1 | 0 | 0 | 0 | 0 | 1 | 1 | AN/AA | 0 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 0 | 1 |
| A/N | 0 | 0 | 1 | 1 | 1 | 0 | 1 | 0 | 0 | 1 | AN/AN | 1 | 1 | 1 | 0 | 0 | 0 | 0 | 0 | 0 | 1 |
| N/A | 1 | 0 | 0 | 1 | 0 | 1 | 1 | 1 | 0 | 0 | AN/NA | 1 | 0 | 0 | 0 | 0 | 1 | 0 | 1 | 0 | 0 |
| N/N | 0 | 1 | 1 | 0 | 0 | 1 | 0 | 1 | 0 | 1 | AN/NN | 0 | 0 | 1 | 1 | 0 | 1 | 0 | 0 | 0 | 1 |
| A/AA | 1 | 0 | 1 | 0 | 0 | 1 | 1 | 0 | 0 | 0 | NA/AA | 1 | 1 | 0 | 0 | 1 | 0 | 1 | 1 | 1 | 0 |
| A/AN | 1 | 0 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 1 | NA/AN | 0 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | 0 | 0 |
| A/NA | 0 | 0 | 1 | 1 | 1 | 0 | 1 | 0 | 0 | 1 | NA/NA | 1 | 0 | 1 | 1 | 1 | 1 | 0 | 0 | 1 | 0 |
| A/NN | 0 | 1 | 1 | 1 | 0 | 1 | 0 | 0 | 1 | 1 | NA/NN | 1 | 1 | 1 | 0 | 0 | 1 | 1 | 0 | 1 | 0 |
| N/AA | 1 | 1 | 0 | 1 | 0 | 0 | 1 | 0 | 1 | 0 | NN/AA | 0 | 1 | 0 | 1 | 0 | 0 | 0 | 0 | 1 | 0 |
| N/AN | 1 | 1 | 0 | 0 | 0 | 1 | 0 | 1 | 1 | 0 | NN/AN | 0 | 0 | 1 | 0 | 0 | 0 | 0 | 1 | 1 | 0 |
| N/NA | 0 | 1 | 1 | 0 | 1 | 0 | 1 | 0 | 1 | 0 | NN/NA | 0 | 1 | 0 | 0 | 1 | 1 | 0 | 0 | 0 | 0 |
| N/NN | 0 | 0 | 1 | 0 | 1 | 1 | 0 | 1 | 0 | 1 | NN/NN | 0 | 0 | 0 | 0 | 0 | 1 | 1 | 0 | 1 | 1 |
| PRE/POST | | | | | | | | | | | | | | | | | | | | | | |
| PRE | 0 | 0 | 1 | 0 | 0 | 1 | 0 | 0 | 1 | 0 |  | POST | 0 | 1 | 0 | 0 | 1 | 0 | 0 | 1 | 0 | 0 |

When Secondary\_Cell\_Active is 2 or 3, and when DTX message is indicated for a cell pair, whose HARQ-ACK information is jointly encoded, the specific DTX code word as defined in Table 15C.2A is transmitted for that cell pair except for the case when DTX message is indicated for all active cells, in which case the HARQ-ACK slot is DTXed. The slot containing HARQ-ACK information is either transmitted or DTXed. If Secondary\_Cell\_Active is larger than 3 and when DTX message is indicated for both cell pairs transmitted on one of the two HS-DPCCHs and there is at least one HARQ-ACK message associated with the other HS-DPCCH that does not correspond to DTX message, then the specific DTX code word as defined in Table 15C.2A is transmitted for all cell pairs for which a DTX message is indicated. If the DTX message is indicated for all active cell pairs then the ­slot on each respective HS-DPCCH containing the HARQ-ACK information is DTXed.

Table 15C.2A: Channel coding of HARQ-ACK for a pair of DTX messages when Secondary\_Cell\_Active is greater than 2

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| HARQ-ACK message to be transmitted | w0 | w1 | w2 | w3 | w4 | w5 | w6 | w7 | w8 | w9 |
| D/D | 0 | 0 | 1 | 1 | 0 | 1 | 1 | 0 | 1 | 0 |

#### 4.7.3B.2 Channel coding for HS-DPCCH composite precoding control indication and channel quality indication

The channel coding for CQI associated with a cell for which the UE is not configured in MIMO mode is specified in subclause 4.7.2.2.

The channel coding for PCI and CQI associated with a cell for which the UE is configured in MIMO mode is specified in subclause 4.7.3.2.

### 4.7.3C Channel coding for HS-DPCCH when the UE is not configured in MIMO mode in any cell and Secondary\_Cell\_Enabled is 2

Two forms of channel coding are used, one for the composite channel quality indication (CQI) and another for the composite HARQ-ACK (acknowledgement).

#### 4.7.3C.1 Channel coding for the composite HS-DPCCH HARQ-ACK

Table 15C.3: Channel coding of HARQ-ACK when the UE is not configured in MIMO mode in any cell and Secondary\_Cell\_Enabled is 2

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| HARQ-ACK message to be transmitted | | | | | w0 | | | w1 | | | w2 | | | w3 | | w4 | w5 | | | w6 | | | w7 | | | w8 | | | w9 | |
| A/D/D | | | | | 1 | | | 1 | | | 1 | | | 1 | | 1 | 1 | | | 1 | | | 1 | | | 1 | | | 1 | |
| N/D/D | | | | | 0 | | | 0 | | | 0 | | | 0 | | 0 | 0 | | | 0 | | | 0 | | | 0 | | | 0 | |
| D/A/D | | | | | 1 | | | 1 | | | 1 | | | 1 | | 1 | 0 | | | 0 | | | 0 | | | 0 | | | 0 | |
| D/N/D | | | | | 0 | | | 0 | | | 0 | | | 0 | | 0 | 1 | | | 1 | | | 1 | | | 1 | | | 1 | |
| D/D/A | | | | | 1 | | | 1 | | | 0 | | | 0 | | 0 | 1 | | | 1 | | | 0 | | | 0 | | | 0 | |
| D/D/N | | | | | 0 | | | 0 | | | 1 | | | 1 | | 1 | 0 | | | 0 | | | 1 | | | 1 | | | 1 | |
| A/A/D | | | | | 1 | | | 0 | | | 1 | | | 0 | | 1 | 0 | | | 1 | | | 0 | | | 1 | | | 0 | |
| A/N/D | | | | | 1 | | | 1 | | | 0 | | | 0 | | 1 | 1 | | | 0 | | | 0 | | | 1 | | | 1 | |
| N/A/D | | | | | 0 | | | 0 | | | 1 | | | 1 | | 0 | 0 | | | 1 | | | 1 | | | 0 | | | 0 | |
| N/N/D | | | | | 0 | | | 1 | | | 0 | | | 1 | | 0 | 1 | | | 0 | | | 1 | | | 0 | | | 1 | |
| A/D/A | | | | | 1 | | | 0 | | | 1 | | | 1 | | 0 | 1 | | | 1 | | | 0 | | | 0 | | | 1 | |
| A/D/N | | | | | 0 | | | 1 | | | 0 | | | 1 | | 1 | 0 | | | 1 | | | 0 | | | 0 | | | 1 | |
| N/D/A | | | | | 0 | | | 0 | | | 0 | | | 1 | | 1 | 1 | | | 1 | | | 0 | | | 1 | | | 0 | |
| N/D/N | | | | | 1 | | | 0 | | | 0 | | | 1 | | 1 | 1 | | | 0 | | | 1 | | | 0 | | | 0 | |
| D/A/A | | | | | 0 | | | 1 | | | 1 | | | 1 | | 0 | 1 | | | 0 | | | 0 | | | 1 | | | 0 | |
| D/A/N | | | | | 1 | | | 0 | | | 1 | | | 0 | | 0 | 1 | | | 0 | | | 1 | | | 1 | | | 0 | |
| D/N/A | | | | | 0 | | | 1 | | | 1 | | | 0 | | 0 | 0 | | | 1 | | | 0 | | | 1 | | | 1 | |
| D/N/N | | | | | 0 | | | 0 | | | 0 | | | 0 | | 1 | 0 | | | 1 | | | 0 | | | 1 | | | 1 | |
| A/A/A | | | | | 1 | | | 1 | | | 0 | | | 1 | | 0 | 0 | | | 1 | | | 1 | | | 1 | | | 0 | |
| A/A/N | | | | | 0 | | | 1 | | | 1 | | | 0 | | 1 | 1 | | | 1 | | | 1 | | | 0 | | | 0 | |
| A/N/A | | | | | 1 | | | 0 | | | 0 | | | 1 | | 0 | 0 | | | 0 | | | 0 | | | 1 | | | 1 | |
| A/N/N | | | | | 0 | | | 0 | | | 1 | | | 0 | | 1 | 1 | | | 0 | | | 0 | | | 0 | | | 1 | |
| N/A/A | | | | | 1 | | | 1 | | | 1 | | | 0 | | 0 | 0 | | | 0 | | | 1 | | | 0 | | | 1 | |
| N/A/N | | | | | 0 | | | 1 | | | 0 | | | 0 | | 1 | 0 | | | 0 | | | 1 | | | 1 | | | 0 | |
| N/N/A | | | | | 1 | | | 0 | | | 0 | | | 0 | | 1 | 0 | | | 1 | | | 1 | | | 0 | | | 1 | |
| N/N/N | | | | | 1 | | | 1 | | | 1 | | | 1 | | 0 | 1 | | | 0 | | | 1 | | | 0 | | | 0 | |
| PRE/POST | | | | | | | | | | | | | | | | | | | | | | | | | | | | | | |
| PRE | 0 | 0 | 1 | 0 | 0 | 1 | 0 | | 0 | 1 | | 0 |  | | POST | | | 0 | 1 | | 0 | 0 | | 1 | 0 | | 0 | 1 | 0 | 0 |

#### 4.7.3C.2 Channel coding for HS-DPCCH channel quality indication

The channel coding for CQI is specified in subclause 4.7.2.2 for the serving HS-DSCH cell, and in subclause 4.7.3A.2 for the 1st and 2nd secondary serving HS-DSCH cells.

### 4.7.3D Channel coding for HS-DPCCH when the UE is configured in Multiflow mode

#### 4.7.3D.1 Channel coding for the composite HS-DPCCH HARQ-ACK

Subclause 4.7.4.3 defines the applicable HARQ-ACK encoding to be used with the following exception

- When the UE is configured with one serving and one assisting HS-DSCH cell and at least one of the two cells is configured in MIMO mode the HARQ-ACK encoding is defined in Table 15C.3A.

Table 15C.3A: Channel coding of HARQ-ACK when the UE is configured with one serving and one assisting HS-DSCH cell and at least one cell is configured in MIMO mode

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| HARQ-ACK message to be transmitted | w0 | w1 | w2 | w3 | w4 | w5 | w6 | w7 | w8 | w9 |  | HARQ-ACK message to be transmitted | w0 | w1 | w2 | w3 | w4 | w5 | w6 | w7 | w8 | w9 |
| A/D | 1 | 1 | 1 | 0 | 0 | 0 | 0 | 1 | 0 | 1 |  | AA/A | 1 | 0 | 0 | 1 | 0 | 1 | 0 | 1 | 1 | 0 |
| N/D | 1 | 1 | 0 | 0 | 1 | 0 | 1 | 0 | 0 | 1 | AA/N | 1 | 0 | 1 | 0 | 0 | 1 | 1 | 0 | 0 | 1 |
| AA/D | 1 | 1 | 1 | 0 | 0 | 0 | 0 | 1 | 0 | 1 | AN/A | 1 | 1 | 0 | 1 | 0 | 0 | 1 | 0 | 1 | 0 |
| AN/D | 1 | 0 | 1 | 1 | 0 | 0 | 0 | 0 | 0 | 0 | AN/N | 0 | 1 | 1 | 0 | 0 | 0 | 1 | 0 | 0 | 0 |
| NA/D | 0 | 0 | 0 | 1 | 0 | 1 | 1 | 0 | 1 | 1 | NA/A | 0 | 0 | 1 | 0 | 1 | 0 | 1 | 1 | 1 | 0 |
| NN/D | 1 | 1 | 0 | 0 | 1 | 0 | 1 | 0 | 0 | 1 | NA/N | 0 | 1 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 1 |
| D/A | 0 | 1 | 1 | 1 | 1 | 0 | 1 | 0 | 1 | 1 | NN/A | 0 | 0 | 0 | 1 | 1 | 0 | 1 | 1 | 0 | 1 |
| D/N | 0 | 0 | 1 | 0 | 1 | 0 | 0 | 0 | 0 | 1 | NN/N | 0 | 1 | 1 | 1 | 1 | 1 | 0 | 0 | 0 | 0 |
| D/AA | 0 | 1 | 1 | 1 | 1 | 0 | 1 | 0 | 1 | 1 | AA/AA | 1 | 0 | 0 | 1 | 0 | 1 | 0 | 1 | 1 | 0 |
| D/AN | 1 | 1 | 1 | 1 | 1 | 0 | 1 | 1 | 0 | 0 | AA/AN | 1 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 1 | 1 |
| D/NA | 0 | 1 | 0 | 0 | 0 | 0 | 1 | 1 | 1 | 1 | AA/NA | 1 | 1 | 1 | 0 | 0 | 1 | 1 | 1 | 1 | 0 |
| D/NN | 0 | 0 | 1 | 0 | 1 | 0 | 0 | 0 | 0 | 1 | AA/NN | 1 | 0 | 1 | 0 | 0 | 1 | 1 | 0 | 0 | 1 |
| A/A | 1 | 0 | 0 | 1 | 0 | 1 | 0 | 1 | 1 | 0 | AN/AA | 1 | 1 | 0 | 1 | 0 | 0 | 1 | 0 | 1 | 0 |
| A/N | 1 | 0 | 1 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | AN/AN | 1 | 1 | 1 | 1 | 0 | 1 | 0 | 0 | 1 | 1 |
| N/A | 0 | 0 | 0 | 1 | 1 | 0 | 1 | 1 | 0 | 1 | AN/NA | 1 | 0 | 0 | 0 | 0 | 0 | 1 | 1 | 0 | 0 |
| N/N | 0 | 1 | 1 | 1 | 1 | 1 | 0 | 0 | 0 | 0 | AN/NN | 0 | 1 | 1 | 0 | 0 | 0 | 1 | 0 | 0 | 0 |
| A/AA | 1 | 0 | 0 | 1 | 0 | 1 | 0 | 1 | 1 | 0 | NA/AA | 0 | 0 | 1 | 0 | 1 | 0 | 1 | 1 | 1 | 0 |
| A/AN | 1 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 1 | 1 | NA/AN | 0 | 1 | 1 | 0 | 1 | 1 | 1 | 1 | 0 | 1 |
| A/NA | 1 | 1 | 1 | 0 | 0 | 1 | 1 | 1 | 1 | 0 | NA/NA | 0 | 0 | 0 | 1 | 1 | 0 | 0 | 0 | 1 | 0 |
| A/NN | 1 | 0 | 1 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | NA/NN | 0 | 1 | 0 | 0 | 1 | 1 | 0 | 0 | 1 | 1 |
| N/AA | 0 | 0 | 0 | 1 | 1 | 0 | 1 | 1 | 0 | 1 | NN/AA | 0 | 0 | 0 | 1 | 1 | 0 | 1 | 1 | 0 | 1 |
| N/AN | 0 | 1 | 0 | 1 | 0 | 0 | 0 | 0 | 0 | 1 | NN/AN | 0 | 1 | 0 | 1 | 0 | 0 | 0 | 0 | 0 | 1 |
| N/NA | 1 | 1 | 1 | 0 | 1 | 0 | 0 | 0 | 1 | 0 | NN/NA | 1 | 1 | 1 | 0 | 1 | 0 | 0 | 0 | 1 | 0 |
| N/NN | 0 | 1 | 1 | 1 | 1 | 1 | 0 | 0 | 0 | 0 | NN/NN | 0 | 1 | 1 | 1 | 1 | 1 | 0 | 0 | 0 | 0 |
| PRE/POST | | | | | | | | | | | | | | | | | | | | | | |
| PRE | 0 | 0 | 1 | 0 | 0 | 1 | 0 | 0 | 1 | 0 |  | POST | 0 | 1 | 0 | 0 | 1 | 0 | 0 | 1 | 0 | 0 |

#### 4.7.3D.2 Channel coding for HS-DPCCH channel quality indication

Subclause 4.7.4.3 defines the applicable CQI encoding to be used with different Multiflow configurations.

### 4.7.3E Channel coding for HS-DPCCH when the UE is configured in MIMO mode with 4 transmit antennas

The coding for HS-DPCCH is defined separately for the following cases:

- when the UE is configured in MIMO mode with four transmit antennas and Secondary\_Cell\_Enabled is 0 (see subclause 4.7.3E.1);

- when the UE is configured in MIMO mode with four transmit antennas in any cell, and Secondary\_Cell\_Enabled is 1 (see subclause 4.7.3E.2);

- when the UE is configured in MIMO mode with four transmit antennas in any cell, and Secondary\_Cell\_Enabled is 2 (see subclause 4.7.3E.3);

- when the UE is configured in MIMO mode with four transmit antennas in any cell, and Secondary\_Cell\_Enabled is 3 (see subclause 4.7.3E.4);

#### 4.7.3E.1 Channel coding for HS-DPCCH when the UE is configured in MIMO mode with four transmit antennas and Secondary\_Cell\_Enabled is 0

Two forms of channel coding are used, one for the composite number of transport blocks preferred (NTBP), precoding control indication (PCI) and channel quality indication (CQI) and another for HARQ-ACK (acknowledgement).

##### 4.7.3E.1.1 Channel coding for HS-DPCCH HARQ-ACK

The HARQ acknowledgement message to be transmitted, as defined in [4], shall be coded to 10 bits as shown in Table 15C.3B. The output is denoted g0, g1,…g9.

When three or four transport blocks are received, the second and the third transport blocks are positively acknowledged (ACK) only if both transport blocks are received correctly. Otherwise both the second and the third transport blocks are negatively acknowledged (NACK).

When four transport blocks are received, the first and the fourth transport blocks are positively acknowledged (ACK) only if both transport blocks are received correctly. Otherwise both the first and the fourth transport blocks are negatively acknowledged (NACK).

Table 15C.3B: Channel coding of HARQ-ACK when the UE is configured in MIMO mode with four transmit antennas in the serving HS-DSCH cell and Secondary\_Cell\_Enabled is 0

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| HARQ-ACK message to be transmitted | | g0 | g1 | g2 | g3 | g4 | g5 | g6 | g7 | g8 | g9 |
| HARQ-ACK in response to a single scheduled transport block | | | | | | | | | | | |
| ACK | | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 |
| NACK | | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 |
| HARQ-ACK in response to two scheduled transport blocks | | | | | | | | | | | |
| Response to primary transport block | Response to second transport block |  | | | | | | | | | |
| ACK | ACK | 1 | 0 | 1 | 0 | 1 | 1 | 1 | 1 | 0 | 1 |
| ACK | NACK | 1 | 1 | 0 | 1 | 0 | 1 | 0 | 1 | 1 | 1 |
| NACK | ACK | 0 | 1 | 1 | 1 | 1 | 0 | 1 | 0 | 1 | 1 |
| NACK | NACK | 1 | 0 | 0 | 1 | 0 | 0 | 1 | 0 | 0 | 0 |
| HARQ-ACK in response to three scheduled transport blocks | | | | | | | | | | | |
| Response to primary transport block | Response to second and third transport blocks |  | | | | | | | | | |
| ACK | ACK | 1 | 0 | 1 | 0 | 1 | 1 | 1 | 1 | 0 | 1 |
| ACK | NACK | 1 | 1 | 0 | 1 | 0 | 1 | 0 | 1 | 1 | 1 |
| NACK | ACK | 0 | 1 | 1 | 1 | 1 | 0 | 1 | 0 | 1 | 1 |
| NACK | NACK | 1 | 0 | 0 | 1 | 0 | 0 | 1 | 0 | 0 | 0 |
| HARQ-ACK in response to four scheduled transport blocks | | | | | | | | | | | |
| Response to primary and fourth transport blocks | Response to second and third transport blocks |  | | | | | | | | | |
| ACK | ACK | 1 | 0 | 1 | 0 | 1 | 1 | 1 | 1 | 0 | 1 |
| ACK | NACK | 1 | 1 | 0 | 1 | 0 | 1 | 0 | 1 | 1 | 1 |
| NACK | ACK | 0 | 1 | 1 | 1 | 1 | 0 | 1 | 0 | 1 | 1 |
| NACK | NACK | 1 | 0 | 0 | 1 | 0 | 0 | 1 | 0 | 0 | 0 |
| PRE/POST indication | | | | | | | | | | | |
| PRE | | 0 | 0 | 1 | 0 | 0 | 1 | 0 | 0 | 1 | 0 |
| POST | | 0 | 1 | 0 | 0 | 1 | 0 | 0 | 1 | 0 | 0 |

The output bits g0, g1,…g9 are repeated as shown in Figure 20C.0



Figure 20C.0: Repetition of HARQ-ACK message

In Figure 20C.0, the repetition is according to the relation:

##### 4.7.3E.1.2 Channel coding for HS-DPCCH composite number of transport blocks preferred, precoding control indication and channel quality indication

When the UE is configured in MIMO mode with four transmit antennas two types of CQI reports shall be supported by the UE. According to the definition of the CQI reporting procedure in [4], in type A CQI reporting the number of transport blocks preferred is up to four and in type B CQI reporting the number of transport blocks preferred is one.

4.7.3E.1.2.1 Bit mapping of Type A channel quality indication

In case a type A CQI shall be reported, the CQI values 0 ... 255 as defined in [4] are converted from decimal to binary to map them to the channel quality indication bits (0 0 0 0 0 0 0 0) to (1 1 1 1 1 1 1 1), respectively. The channel quality indication bits are cqi0 , cqi1 , cqi2 , cqi3 , cqi4, cqi5, cqi6, cqi7 (where cqi0 is LSB and cqi7 is MSB).

In case the number of transport blocks preferred is one, the CQI values 0 ... 30 as defined in [4] are converted from decimal to binary to map them to the channel quality indication bits (1 0 0 0 0) to (1 1 1 1 1), respectively. The information bit pattern (0 0 0 0 0) shall not be used in this release. The channel quality indication bits are cqi0, cqi1, cqi2, cqi3, cqi4 (where cqi0 is LSB and cqi4 is MSB) and (0 0 0) is used for indicating cqi5, cqi6, cqi7 (where cqi5 is LSB and cqi7 is MSB). .

4.7.3E.1.2.2 Bit mapping of Type B channel quality indication

In case a type B CQI shall be reported, the CQI values 0 ... 30 as defined in [4] are converted from decimal to binary to map them to the channel quality indication bits (1 0 0 0 0) to (1 1 1 1 1), respectively. The information bit pattern (0 0 0 0 0) shall not be used in this release. The channel quality indication bits are cqi0, cqi1, cqi2, cqi3, cqi4 (where cqi0 is LSB and cqi4 is MSB).

4.7.3E.1.2.3 Bit mapping of number of transport blocks preferred

According to the number of transport blocks preferred definition in [4], the range of possible values is 0 ... 3. The number of transport blocks preferred values 0 ... 3 as defined in [4] are converted from decimal to binary to map them to the number of transport blocks preferred bits (0 0) to (1 1) respectively. The number of transport blocks preferred bits are ri0 ,ri1 (where ri0 is LSB and ri1 is MSB).

4.7.3E.1.2.4 Bit mapping of precoding control indication

According to the PCI definition in [4], the range of possible PCI values is 0 ... 15. The PCI values 0 ... 15 as defined in [4] are converted from decimal to binary to map them to the precoding control indication bits (0 0,0,0) to (1 1,1,1) respectively. The precoding control indication bits are pci0 , pci1,, pci2, pci3  (where pci0 is LSB and pci3 is MSB).

4.7.3E.1.2.5 Composite number of transport blocks preferred , precoding control indication and channel quality indication bits

For type A CQI report the composite NTBP/PCI/CQI shall be constructed according to the scheme depicted in Figure 20C.1.



Figure 20C.1: Construction of composite NTBP/PCI/CQI for Type A CQI report

In case a type A CQI shall be reported, the number of transport blocks preferred bits ri0 ,ri1, precoding control indication bits pci0 , pci1, pci2, pci3, and the channel quality indication bits cqi0 , cqi1 , cqi2 , cqi3 , cqi4, cqi5, cqi6, cqi7 are concatenated to the composite number of transport blocks preferred, precoding control indication and channel quality indication bits according to the relation

For type B CQI report the composite PCI/CQI shall be constructed according to the scheme depicted in Figure 20C.2.



Figure 20C.2: Construction of composite NTBP/PCI/CQI for Type B CQI report

In case a type B CQI shall be reported, the precoding control indication bits pci0 , pci1, pci2, pci3, and the channel quality indication bits cqi0 , cqi1 , cqi2 , cqi3 , cqi4 are concatenated to the composite precoding control indication and channel quality indication bits according to the relation

4.7.3E.1.2.6 Channel coding for composite number of transport blocks preferred, precoding control indication and channel quality indication bits

In case a type A CQI needs to be reported, rate 1/2 convolutional coding, as described in Clause 4.2.3.1 is applied to the sequence of bits *a0*, *a1*, …, *a13*, resulting in the sequence of bits *d0*, *d1*, …, *d43*.

Note that the coded sequence lengths result from the termination of K=9 convolutional coding being fully applied.

In case a type B CQI needs to be reported, rate 1/3 convolutional coding, as described in Clause 4.2.3.1 is applied to the sequence of bits *a0*, *a1*, …, *a8*, resulting in the sequence of bits *d0*, *d1*, …, *d50*.

Note that the coded sequence lengths result from the termination of K=9 convolutional coding being fully applied.

4.7.3E.1.2.7 Rate matching for composite number of transport blocks preferred, precoding control indication and channel quality indication bits

In case a type A CQI needs to be reported, from the input sequence *d0*, *d1*, …, *d43* the bits *d0*, *d2*, *d41*, *d43* are punctured to obtain the output sequence b0, b1, …, b39 .

In case a type B CQI needs to be reported, from the input sequence *d0*, *d1*, …, *d50* the bits *d0*, *d2*, *d3*, *d4*, *d6*, *d44*, *d45*, *d46*, *d47*, *d48*, *d50* are punctured to obtain the output sequence b0, b1, …, b39 .

#### 4.7.3E.2 Channel coding for HS-DPCCH when the UE is configured in MIMO mode with four transmit antennas in any cell and Secondary\_Cell\_Enabled is 1

Two forms of channel coding are used, one for the composite number of transport blocks preferred (NTBP), precoding control indication (PCI) and channel quality indication (CQI) and another for HARQ-ACK (acknowledgement).

##### 4.7.3E.2.1 Channel coding for the composite HS-DPCCH HARQ-ACK

The HARQ acknowledgement message associated with a cell for which the UE is configured in MIMO mode with four transmit antennas shall be coded to 10 bits as in Table 15C.3B in subclause 4.7.3E.1.1.

The HARQ acknowledgement message associated with a cell for which the UE is configured in MIMO mode shall be coded to 10 bits as in Table 15B in subclause 4.7.3.1.

The HARQ acknowledgement message associated with a cell for which the UE is configured not in MIMO mode and not in MIMO mode with four transmit antennas shall be coded to 10 bits as specified in Table 15 in subclause 4.7.2.

The HARQ acknowledgement messages corresponding to the serving HS-DSCH cell and secondary serving HS-DSCH cell in that order are encoded and concatenated into the same slot according to Figure 20D in clause 4.7.4.1.

##### 4.7.3E.2.2 Channel coding for HS-DPCCH composite number of transport blocks preferred, precoding control indication and channel quality indication

The channel coding for NTBP, PCI and CQI associated with a cell for which the UE is configured in MIMO mode with four transmit antennas is specified in subclause 4.7.3E.1.2.

The channel coding for PCI and CQI associated with a cell for which the UE is configured in MIMO mode is specified in subclause 4.7.3.2.

The channel coding for CQI associated with a cell for which the UE is configured not in MIMO mode and not in MIMO mode with four transmit antennas is specified in subclause 4.7.2.2.

#### 4.7.3E.3 Channel coding for HS-DPCCH when the UE is configured in MIMO mode with four transmit antennas in any cell and Secondary\_Cell\_Enabled is 2

Two forms of channel coding are used, one for the composite number of transport blocks preferred (NTBP), precoding control indication (PCI) and channel quality indication (CQI) and another for HARQ-ACK (acknowledgement).

##### 4.7.3E.3.1 Channel coding for the composite HS-DPCCH HARQ-ACK

The HARQ acknowledgement message associated with a cell for which the UE is configured in MIMO mode with four transmit antennas shall be coded to 10 bits as in Table 15C.3B in subclause 4.7.3E.1.1.

The HARQ acknowledgement message associated with a cell for which the UE is configured in MIMO mode shall be coded to 10 bits as in Table 15B in subclause 4.7.3.1.

The HARQ acknowledgement message associated with a cell for which the UE is not configured in MIMO mode and not configured in MIMO mode with four transmit antennas shall be coded to 10 bits as specified in Table 15 in subclause 4.7.2.

The HARQ acknowledgement messages corresponding to the serving HS-DSCH cell and 1st secondary serving HS-DSCH cell in that order are encoded and concatenated into the same slot according to Figure 20D in clause 4.7.4.1.

##### 4.7.3E.3.2 Channel coding for HS-DPCCH composite number of transport blocks preferred, precoding control indication and channel quality indication

The channel coding for NTBP, PCI and CQI associated with a cell for which the UE is configured in MIMO mode with four transmit antennas is specified in subclause 4.7.3E.1.2.

The channel coding for PCI and CQI associated with a cell for which the UE is configured in MIMO mode is specified in subclause 4.7.3.2.

The channel coding for PCI and CQI associated with a cell for which the UE is configured not in MIMO mode and not in MIMO mode with four transmit antennas is specified in subclause 4.7.2.2.

#### 4.7.3E.4 Channel coding for HS-DPCCH when the UE is configured in MIMO mode with four transmit antennas in any cell and Secondary\_Cell\_Enabled is 3

Two forms of channel coding are used, one for the composite number of transport blocks preferred (NTBP), precoding control indication (PCI) and channel quality indication (CQI) and another for HARQ-ACK (acknowledgement).

##### 4.7.3E.4.1 Channel coding for the composite HS-DPCCH HARQ-ACK

The HARQ acknowledgement message associated with a cell for which the UE is configured in MIMO mode with four transmit antennas shall be coded to 10 bits as in Table 15C.3B in subclause 4.7.3E.1.1.

The HARQ acknowledgement message associated with a cell for which the UE is configured in MIMO mode shall be coded to 10 bits as in Table 15B in subclause 4.7.3.1.

The HARQ acknowledgement message associated with a cell for which the UE is configured not in MIMO mode and not in MIMO mode with four transmit antennas shall be coded to 10 bits as specified in Table 15 in subclause 4.7.2.

The HARQ acknowledgement messages corresponding to the serving HS-DSCH cell and 1st secondary serving HS-DSCH cell in that order are encoded and concatenated into the same slot according to Figure 20D in clause 4.7.4.1.

The HARQ acknowledgement messages corresponding to the 2nd secondary serving HS-DSCH cell and the 3rd secondary serving HS-DSCH cell in that order are encoded and concatenated into the same slot according to Figure 20D.1 in clause 4.7.4.1.

##### 4.7.3E.4.2 Channel coding for HS-DPCCH composite number of transport blocks preferred, precoding control indication and channel quality indication

The channel coding for NTBP, PCI and CQI associated with a cell for which the UE is configured in MIMO mode with four transmit antennas is specified in subclause 4.7.3E.1.2.

The channel coding for PCI and CQI associated with a cell for which the UE is configured in MIMO mode is specified in subclause 4.7.3.2.

The channel coding for PCI and CQI associated with a cell for which the UE is configured not in MIMO mode and not in MIMO mode with four transmit antennas is specified in subclause 4.7.2.2.

### 4.7.4 Physical channel mapping for HS-DPCCH

#### 4.7.4.1 Physical Channel mapping for HS-DPCCH HARQ-ACK

This section is not applicable when the UE is configured in MIMO mode with four transmit antennas in at least one cell.

If the HS-DPCCH slot format 0 as defined in [2] is used, the HS-DPCCH physical channel mapping function shall map the input bits wk directly to physical channel so that bits are transmitted over the air in ascending order with respect to k.

If the HS-DPCCH slot format 1 as defined in [2], is used, the HS-DPCCH physical channel mapping function shall map the input bits wk to the physical channel so that bits are transmitted over the air in ascending order with respect to k as follows:

- If Secondary\_Cell\_Enabled is equal to 7 and Secondary\_Cell\_Active is equal to 7

- The following two HARQ-ACK messages are transmitted on HS-DPCCH according to Figure 20D:

- HARQ-ACK1 comprising the HARQ acknowledgement messages for the pair of serving HS-DSCH cell and 1st secondary serving HS-DSCH cell in that order and

- HARQ-ACK2 comprising the HARQ acknowledgement messages for the pair of the 2nd secondary serving HS-DSCH cell and the 3rd secondary serving HS-DSCH cell in that order

- The following two HARQ-ACK messages are transmitted on HS-DPCCH2 according to Figure 20D.1:

- HARQ-ACK3 comprising the HARQ acknowledgement messages for the pair of the 4th secondary serving HS-DSCH cell and the 5th secondary serving HS-DSCH cell in that order

- HARQ-ACK4 comprising the HARQ acknowledgement messages for the pair of the 6th secondary serving HS-DSCH cell and the 7th secondary serving HS-DSCH cell in that order

- If Secondary\_Cell\_Enabled is equal to 6 and Secondary\_Cell\_Active is equal to 6

- The following two HARQ-ACK messages are transmitted on HS-DPCCH according to Figure 20D:

- HARQ-ACK1 comprising the HARQ acknowledgement messages for the pair of serving HS-DSCH cell and 1st secondary serving HS-DSCH cell in that order and

- HARQ-ACK2 comprising the HARQ acknowledgement messages for the pair of the 2nd secondary serving HS-DSCH cell and the 3rd secondary serving HS-DSCH cell in that order

- The following two HARQ-ACK messages are transmitted on HS-DPCCH2 according to Figure 20D.1:

- HARQ-ACK3 comprising the HARQ acknowledgement messages for the pair of the 4th secondary serving HS-DSCH cell and the 5th secondary serving HS-DSCH cell in that order

- HARQ-ACK4 comprising the HARQ acknowledgement messages for the 6th secondary serving HS-DSCH cell and a DTX message in that order

- If Secondary\_Cell\_Enabled is equal to 5 and Secondary\_Cell\_Active is equal to 5

- The following two HARQ-ACK messages are transmitted on HS-DPCCH according to Figure 20D:

- HARQ-ACK1 comprising the HARQ acknowledgement messages for the pair of serving HS-DSCH cell and 1st secondary serving HS-DSCH cell in that order and

- HARQ-ACK2 comprising the HARQ acknowledgement messages for the pair of the 2nd secondary serving HS-DSCH cell and the 3rd secondary serving HS-DSCH cell in that order

- The following HARQ-ACK message is transmitted on HS-DPCCH2:

- The HARQ acknowledgement messages for the pair of the 4th secondary serving HS-DSCH cell and the 5th secondary serving HS-DSCH cell are repeated according to Figure 20E.

- If Secondary\_Cell\_Enabled is equal to 4 and Secondary\_Cell\_Active is equal to 4

- The following two HARQ-ACK messages are transmitted on HS-DPCCH according to Figure 20D:

- HARQ-ACK1 comprising the HARQ acknowledgement messages for the pair of serving HS-DSCH cell and 1st secondary serving HS-DSCH cell in that order and

- HARQ-ACK2 comprising the HARQ acknowledgement messages for the pair of the 2nd secondary serving HS-DSCH cell and the 3rd secondary serving HS-DSCH cell in that order

- The following two HARQ-ACK messages are transmitted on HS-DPCCH2:

- The HARQ-ACK comprising the HARQ acknowledgement the 4th secondary serving HS-DSCH cell and a DTX message in that order and it is repeated according to Figure 20E.

- If Secondary\_Cell\_Enabled is greater than 3 and Secondary\_Cell\_Active is less than Secondary\_Cell\_Enabled:

- If none of the 4th, 5th, 6th, or 7th secondary serving HS-DSCH cell is activated the HARQ-ACK transmissions on HS-DPCCH2 are DTXed

- If at most one of the 1st, 2nd, or 3rd secondary serving HS-DSCH cell is activated the HARQ-ACK message is repeated according to Figure 20E

- If one of the 4th, 5th, 6th, and 7th secondary serving HS-DSCH cell is activated the HARQ-ACK message is repeated according to Figure 20E.

- If two of the 4th, 5th, 6th and 7th secondary serving HS-DSCH cell are active the HARQ-ACK comprises the HARQ acknowledgement messages for the pair of the secondary serving HS-DSCH cell with lowest index as indicated by higher layers and the other activated secondary serving HS-DSCH cell in that order. The HARQ-ACK message is repeated according to Figure 20E.

- Otherwise the transmissions of the HARQ-ACK messages is the same as if Secondary\_Cell\_Active was equal to Secondary\_Cell\_Enabled but where DTX message(s) is transmitted in place of deactivated secondary serving HS-DSCH cells.

- If Secondary\_Cell\_Enabled is 3 and Secondary\_Cell\_Active is 2 or 3 then the following two HARQ-ACK messages are encoded and concatenated into the same slot according to Figure 20D :

- HARQ-ACK1 comprising the HARQ acknowledgement messages for the pair of serving HS-DSCH cell and 1st secondary serving HS-DSCH cell in that order and

- HARQ-ACK2 comprising the HARQ acknowledgement messages for the pair of 2nd secondary serving HS-DSCH cell and the 3rd secondary serving HS-DSCH cell in that order

- If Secondary\_Cell\_Enabled is 2 with MIMO configured in at least one of the cells and Secondary\_Cell\_Active is 2 then the following two HARQ-ACK messages, are encoded and concatenated into the same slot according to Figure 20D:

- HARQ-ACK1 comprising the HARQ acknowledgement messages for the pair of serving HS-DSCH cell and 1st secondary serving HS-DSCH cell in that order and

- HARQ-ACK2 comprising the HARQ acknowledgement messages for the 2nd secondary serving HS-DSCH cell and a DTX message in that order

- If Secondary\_Cell\_Enabled is more than 1 and Secondary\_Cell\_Active is 0 or 1 then the transmission of the HARQ-ACK message is repeated according to Figure 20E.



Figure 20D: Concatenation of 2 HARQ-ACK messages

In Figure 20D, the concatenation of the 2 HARQ-ACK messages is according to the relation:



Figure 20D.1: Concatenation of 2 HARQ-ACK messages on HS-DPCCH2



Figure 20E: Repetition of HARQ-ACK message

In Figure 20E, the repetition of the HARQ-ACK message is according to the relation:

#### 4.7.4.2 Physical Channel mapping for HS-DPCCH PCI/CQI

Table 15C.4 lists the CQI and PCI/CQI report mapping scenarios when Secondary\_Cell\_Enabled is less than 4. Tables 15C.5 and 15C.6 list the CQI and PCI/CQI report mapping scenarios when Secondary\_Cell\_Enabled is greater than 3. The transmission timing and repetition of the 1st and the 2nd CQI and PCI/CQI report is defined in [4].

Table 15C.4: The CQI and PCI/CQI report mapping scenarios when Secondary\_Cell\_Enabled is less than 4

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Case | Secondary\_ Cell\_ Enabled | MIMO configured in any cell | HS-DPCCH slot format | Secondary\_ Cell\_ Active | 1st CQI or PCI/CQI report | | 2nd CQI or PCI/CQI report | |
|  | | | | | CQI or  PCI/CQI Type A/B | | CQI or  PCI/CQI Type A/B | |
| 1 | 0 | No | 0 | 0 | CQI | | Not applicable | |
| 2 | Yes | 0 | 0 | PCI/CQI | | Not applicable | |
| 3 | 1  Note 2 | No | 0 | 1 | CQI0 & CQI1  Note 5 | | Not applicable | |
| 4 | 0 | CQI0 | | Not applicable | |
| 5 | Yes  Note 1 | 0 | 1 | PCI/CQI0 | | PCI/CQI1 | |
| 6 | 0 | PCI/CQI0 | | DTX | |
| 7 | 2  Note 2 | No | 0 | 2 | CQI0 | | CQI1 & CQI2  Note 5 | |
| 8 | 1 | CQI0 | | CQIn  Note 4 | |
| 9 | 0 | CQI0 | | DTX | |
|  | | | | | CQI 1 or PCI/CQI 1 Type A/B | CQI 2 or PCI/CQI 2 Type A/B | CQI 1 or PCI/CQI 1 Type A/B | CQI 2 or PCI/CQI 2 Type A/B |
| 10 | 2  Note 2 | Yes Note 1 | 1 | 2 | PCI/CQI0 | PCI/CQI2 | PCI/CQI1 | DTX |
| 11 | 1 | PCI/CQI0 | PCI/CQI0 | PCI/CQIn  Note 4 | PCI/CQIn  Note 4 |
| 12 | 0 | PCI/CQI0 | PCI/CQI0 | DTX | |
| 13 | 3  Note 2 | No | 1 | 3 | CQI0 | CQI2 | CQI1 | CQI3 |
| 14 | 2 | CQI0 | CQI2  Note 3 | CQI1  Note 3 | CQI3  Note 3 |
| 15 | 1 | CQI0 | CQI0 | CQIn  Note 4 | CQIn  Note 4 |
| 16 | 0 | CQI0 | CQI0 | DTX | |
| 17 | Yes  Note 1 | 1 | 3 | PCI/CQI0 | PCI/CQI2 | PCI/CQI1 | PCI/CQI3 |
| 18 | 2 | PCI/CQI0 | PCI/CQI2  Note 3 | PCI/CQI1  Note 3 | PCI/CQI3  Note 3 |
| 19 | 1 | PCI/CQI0 | PCI/CQI0 | PCI/CQIn  Note 4 | PCI/CQIn  Note 4 |
| 20 | 0 | PCI/CQI0 | PCI/CQI0 | DTX | |

Note 1: If the UE is configured in MIMO mode in at least one cell, but not in all cells, a CQI value is reported instead of PCI/CQI value for the non-MIMO cell(s).

Note 2: The CQI0 and PCI/CQI0 refer to the serving HS-DSCH cell’s CQI and PCI/CQI reports respectively, the CQIn and PCI/CQIn refer to the nth secondary serving HS-DSCH cell’s reports.

Note 3: The deactivated secondary cell’s CQI or PCI/CQI is not transmitted (DTX’d).

Note 4: The CQI or the PCI/CQI of the single active secondary cell is transmitted.

Note 5: The two CQI values are jointly encoded.

Table 15C.5: The CQI and PCI/CQI report mapping for HS-DPCCH when Secondary\_Cell\_Enabled is greater than 3.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Case | Secondary\_ Cell\_ Enabled | MIMO configured in any cell | HS-DPCCH slot format | Active secondary cells out of 1st, 2nd, 3rd secondary cell | 1st CQI or PCI/CQI report | | 2nd CQI or PCI/CQI report | |
|  | | | | | CQI 1 or PCI/CQI 1 Type A/B | CQI 2 or PCI/CQI 2 Type A/B | CQI 1 or PCI/CQI 1 Type A/B | CQI 2 or PCI/CQI 2 Type A/B |
| 21a | 4-7  Note 2 | No | 1 | 3 | CQI0 | CQI2 | CQI1 | CQI3 |
| 22a | 2 | CQI0 | CQI2  Note 3 | CQI1  Note 3 | CQI3  Note 3 |
| 23a | 1 | CQI0 | CQI0 | CQIn  Note 4 | CQIn  Note 4 |
| 24a | 0 | CQI0 | CQI0 | DTX | |
| 25a | Yes  Note 1 | 1 | 3 | PCI/CQI0 | PCI/CQI2 | PCI/CQI1 | PCI/CQI3 |
| 26a | 2 | PCI/CQI0 | PCI/CQI2  Note 3 | PCI/CQI1  Note 3 | PCI/CQI3  Note 3 |
| 27a | 1 | PCI/CQI0 | PCI/CQI0 | PCI/CQIn  Note 4 | PCI/CQIn  Note 4 |
| 28a | 0 | PCI/CQI0 | PCI/CQI0 | DTX | |

Note 1: If the UE is configured in MIMO mode in at least one cell, but not in all cells, a CQI value is reported instead of PCI/CQI value for the non-MIMO cell(s).

Note 2: The CQI0 and PCI/CQI0 refer to the serving HS-DSCH cell’s CQI and PCI/CQI reports respectively, the CQIn and PCI/CQIn refer to the nth secondary serving HS-DSCH cell’s reports, and n ⊂ {1,2,3}.

Note 3: The deactivated secondary cell’s CQI or PCI/CQI is not transmitted (DTX’d).

Note 4: The CQI or the PCI/CQI of the single active secondary cell is transmitted.

Table 15C.6: The CQI and PCI/CQI report mapping for HS-DPCCH2 when Secondary\_Cell\_Enabled is greater than 3.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Case | Secondary\_ Cell\_ Enabled | MIMO configured in any cell | HS-DPCCH slot format | Active secondary cells out of 4th, 5th, 6th and 7th secondary cell | 3rd CQI or PCI/CQI report | | 4th CQI or PCI/CQI report | |
|  | | | | | CQI 3 or PCI/CQI 3 Type A/B | CQI 4 or PCI/CQI 4 Type A/B | CQI 3 or PCI/CQI 3 Type A/B | CQI 4 or PCI/CQI 4 Type A/B |
| 21b | 4-7  Note 2 | No | 1 | 4 | CQI4 | CQI6 | CQI5 | CQI7 |
| 22b | 3 | CQI4  Note 3 | CQI6  Note 3 | CQI5  Note 3 | CQI7  Note 3 |
| 23b | 2 | CQIn  Note 2 | CQIn  Note 2 | CQIm  Note 2 | CQIm  Note 2 |
| 24b | 1 | CQIn  Note 4 | CQIn  Note 4 | DTX | |
| 25b | 0 | DTX | | DTX | |
| 26b | Yes  Note 1 | 1 | 4 | PCI/CQI4 | PCI/CQI6 | PCI/CQI5 | PCI/CQI7 |
| 27b | 3 | PCI/CQI4  Note 3 | PCI/CQI6  Note 3 | PCI/CQI5  Note 3 | PCI/CQI7  Note 3 |
| 28b | 2 | PCI/CQIn  Note 2 | PCI/CQIn  Note 2 | PCI/CQIm  Note 2 | PCI/CQIm  Note 2 |
| 29b | 1 | PCI/CQIn  Note 4 | PCI/CQIn  Note 4 | DTX | |
| 30b | 0 | DTX | | DTX | |

Note 1: If the UE is configured in MIMO mode in at least one cell, but not in all cells, a CQI value is reported instead of PCI/CQI value for the non-MIMO cell(s).

Note 2: The CQIn and PCI/CQIn refer to the nth secondary serving HS-DSCH cell’s reports, and the CQIm and PCI/CQIm refer to the mth secondary serving HS-DSCH cell’s reports, where n < m and {n, m} ⊂ {4,5,6,7}.

Note 3: The deactivated secondary cells’ CQI or PCI/CQI is not transmitted (DTX’d).

Note 4: The CQI or the PCI/CQI of the single active secondary cell out of the 4th, 5th, 6th and 7th secondary cells is transmitted.

If the HS-DPCCH slot format 0 as defined in [2] is used, the HS-DPCCH physical channel mapping function shall map the input bits bk directly to physical channel so that bits are transmitted over the air in ascending order with respect to k. When Secondary\_Cell\_Active is 2, the CQI reports for each of the following groups are mapped to separate subframes as specified in [4]:

- The report for the serving HS-DSCH cell (CQI) is mapped according to the physical channel mapping of CQI in Figure 20.

- The report for the 1st secondary serving HS-DSCH cell (CQI 1) and the 2nd secondary serving HS-DSCH cell (CQI 2) are mapped according to Figure 20C and according to the physical channel mapping of CQI in Figure 20.

If the HS-DPCCH slot format 1 as defined in [2] is used and Secondary\_Cell\_Enabled is less than 4, the HS-DPCCH physical channel mapping function shall map the input bits bk to the physical channel so that bits are transmitted over the air in ascending order with respect to k as follows:

- When Secondary\_Cell\_Active is 3, the CQI or PCI/CQI reports for each of the following pairs are mapped to separate subframes as specified in [4]:

- The report for the serving HS-DSCH cell (CQI 1 or PCI/CQI 1) and the 2nd secondary serving HS-DSCH cell (CQI 2 or PCI/CQI 2) are mapped according to Figure 20F.

- The report for the 1st secondary serving HS-DSCH cell (CQI 1 or PCI/CQI 1) and the 3rd secondary serving HS-DSCH cell (CQI 2 or PCI/CQI 2) are mapped according to Figure 20F.

- When Secondary\_Cell\_Active is 2, the mapping of the CQI or PCI/CQI reports is the same as the case when Secondary\_Cell\_Active is 3 with the following exception: In the subframe in which only one active cell is mapped, the HS-DPCCH physical channel mapping function shall map the input bits bk directly to the physical channel in the corresponding slot of the CQI (or PCI/CQI) field of that subframe while the other slot of the CQI (or PCI/CQI) field is DTXed.

- When Secondary\_Cell\_Active is 0 or 1, the CQI or PCI/CQI report for each active cell is mapped to a separate subframe as specified in [4]. In each subframe, the HS-DPCCH physical channel mapping function shall map the input bits to the physical channel according to Figure 20G.

If the HS-DPCCH slot format 1 as defined in [2] is used and Secondary\_Cell\_Enabled is greater than 3, the HS-PDCCH physical channel mapping function shall map the input bits bk to the physical channel so that bits are transmitted over the air in ascending order with respect to k as follows:

- When Secondary\_Cell\_Active is 7, the CQI or PCI/CQI reports for each of the following pairs are mapped to separate subframes as specified in [4]:

- The following is transmitted on HS-DPCCH:

- The report for the serving HS-DSCH cell (CQI1 or PCI/CQI1) and the 2nd secondary serving HS-DSCH cell (CQI2 or PCI/CQI2) are mapped according to Figure 20F.

- The report for the 1st secondary serving HS-DSCH cell (CQI1 or PCI/CQI1) and the 3rd secondary serving HS-DSCH cell (CQI2 or PCI/CQI2) are mapped according to Figure 20F.

- The following is transmitted on HS-DPCCH2:

- The report for the 4th secondary serving HS-DSCH cell (CQI3 or PCI/CQI3) and the 6th secondary serving HS-DSCH cell (CQI4 or PCI/CQI4) are mapped according to Figure 20F.1.

- The report for the 5th secondary serving HS-DSCH cell (CQI3 or PCI/CQI3) and the 7th secondary serving HS-DSCH cell (CQI4 or PCI/CQI4) are mapped according to Figure 20F.1.

- When Secondary\_Cell\_Active is less than 7 the mapping of the CQI or PCI/CQI reports is the same as the case when Secondary\_Cell\_Active is 7 with the following exceptions:

- When one of the 1st, 2nd or 3rd secondary serving HS-DSCH cell is deactivated the HS-DPCCH physical channel mapping function shall map the input bits bk directly to the physical channel in the corresponding slot of the CQI (or PCI/CQI) field of that subframe while the other slot of the CQI (or PCI/CQI) field is DTXed in the subframe in which only one active cell is mapped.

- When one of the 4th, 5th, 6th or 7th secondary serving HS-DSCH cell is deactivated the HS-DPCCH physical channel mapping function shall map the input bits bk directly to the physical channel in the corresponding slot of the CQI (or PCI/CQI) field of that subframe while the other slot of the CQI (or PCI/CQI) field is DTXed in the subframe in which only one active cell is mapped.

- If at most one of the 1st, 2nd, or 3rd secondary serving HS-DSCH cell is activated the CQI or PCI/CQI report for each active cell is mapped to a separate subframe as specified in [4]. In each subframe, the HS-DPCCH physical channel mapping function shall map the input bits to the physical channel according to Figure 20G.

- If at most two of the 4th, 5th, 6th or 7th secondary serving HS-DSCH cell is activated the CQI or PCI/CQI report for each active cell is mapped to a separate subframe as specified in [4]. In each subframe, the HS-DPCCH physical channel mapping function shall map the input bits to the physical channel according to Figure 20G.



Figure 20F: Concatenation of CQI (or PCI/CQI) reports in the CQI (or PCI/CQI) field of a sub-frame

In Figure 20F, the two individual CQI (or PCI/CQI) reports are concatenated to form the composite channel quality indication according to the relation



Figure 20F.1: Concatenation of CQI (or PCI/CQI) reports in the CQI (or PCI/CQI) field of a sub-frame on HS-DPCCH2.



Figure 20G: Repetition of CQI or PCI/CQI reports

In Figure 20G, the CQI (or PCI/CQI) report is repeated according to the relation

#### 4.7.4.3 Physical Channel mapping for HS-DPCCH HARQ-ACK and PCI/CQI when the UE is configured in Multiflow mode

The notation used in the following subclauses is as defined below:

Cell activation status ''A’: Indicates a cell that is active (not deactivated by an HS-SCCH order).

Cell activation status ''-’: Indicates a cell that is inactive (deactivated by an HS-SCCH order).

Cell group n: A group of (one, two, or three) Multiflow mode cells that have the same CPICH timing. The cells that belong to a cell group are indicated by higher layers.

Ai & Aj: HARQ-ACK field for jointly encoded HARQ-ACK information of cell i and cell j.

Ai & Aj & Ak: HARQ-ACK field for jointly encoded HARQ-ACK information of cell i, cell j and cell k.

Ai & D: HARQ-ACK field for jointly encoded HARQ-ACK information of cell i and DTX indication.

Ai & Aj & D: HARQ-ACK field for jointly encoded HARQ-ACK information of cell i, cell j and DTX indication.

Ai & D & Aj: HARQ-ACK field for jointly encoded HARQ-ACK information of cell i, DTX indication, and HARQ-ACK information of cell j.

CQIi: CQI field for CQI information of cell i.

PCI/CQIi: PCI/CQI field for jointly encoded PCI and CQI information of cell i.

CQIi & CQIj: Jointly encoded CQI field for CQI information of cell i and cell j.

##### 4.7.4.3.1 Physical Channel mapping for HS-DPCCH HARQ-ACK and PCI/CQI when the UE is configured with one serving and one assisting serving HS-DSCH cell

When MIMO is not configured in any cell;

- The HS-DPCCH mapping follows the table 15C.8.

- The HARQ-ACK and CQI encoding follow the definition in subclause 4.7.3A.

- HS-DPCCH is transmitted using slot format #0.

Table 15C.8: The UE is configured with one serving and one assisting serving HS-DSCH cell and no cells are in MIMO mode

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **MF case** | **Cell activation status** | | **HS-DPCCH subframe** | | |
| **Cell group 1** | **Cell group 2** | **Slot 0** | **Slot 1** | **Slot 2** |
| **Cell0** | **Cell1** |
| 1 | A | A | A0 & A1 | CQI0 & CQI1 | |

In this table cell 0 refers to the serving HS-DSCH cell, and cell 1 refers to the assisting serving HS-DSCH cell.

When MIMO is configured in at least one cell;

- The HS-DPCCH mapping follows the table 15C.9.

- The HARQ-ACK encoding follows the subclause 4.7.3D.1.

- The channel coding for CQI associated with a cell for which the UE is not configured in MIMO mode is specified in subclause 4.7.2.2.

- The channel coding for PCI and CQI associated with a cell for which the UE is configured in MIMO mode is specified in subclause 4.7.3.2.

- HS-DPCCH is transmitted using slot format #0.

Table 15C.9: The UE is configured with one serving and one assisting serving HS-DSCH cell and at least one cell is configured in MIMO mode

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **MF case** | **Cell activation status** | | **HS-DPCCH subframe #1** | | | **HS-DPCCH subframe #2** | | |
| **Cell group 1** | **Cell group 2** | **Slot 0** | **Slot 1** | **Slot 2** | **Slot 0** | **Slot 1** | **Slot 2** |
| **Cell0** | **Cell1** |
| 2 | A | A | A0 & A1 | PCI/CQI0 | | A0 & A1 | PCI/CQI1 | |

In this table cell 0 refers to the serving HS-DSCH cell, and cell 1 refers to the assisting serving HS-DSCH cell.

##### 4.7.4.3.2 Physical Channel mapping for HS-DPCCH HARQ-ACK and PCI/CQI when the UE is configured with two serving and one assisting serving or one serving and two assisting serving HS-DSCH cells

When MIMO is not configured in any cell;

- If the UE is configured with two serving and one assisting serving HS-DSCH cells the HS-DPCCH mapping follows the table 15C.10

- If the UE is configured with one serving and two assisting serving HS-DSCH cells the HS-DPCCH mapping follows the table 15C.11.

- The HARQ-ACK encoding follow the definition in subclause 4.7.3C.1.

- The CQI encoding for composite CQI reports containing channel quality indication for two cells follows the definition in subclause 4.7.3A.2

- The CQI encoding for the separately encoded CQI reports follows the definition in subclause 4.7.2.2.

- HS-DPCCH is transmitted using slot format #0.

Table 15C.10: The UE is configured with two serving and one assisting serving HS-DSCH cells and no cells are in MIMO mode

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **MF case** | **Cell activation status** | | | **HS-DPCCH subframe #1** | | | **HS-DPCCH subframe #2** | | |
| **Cell group 1** | | **Cell group 2** | **Slot 0** | **Slot 1** | **Slot 2** | **Slot 0** | **Slot 1** | **Slot 2** |
|  | **Cell0** | **Cell1** | **Cell2** |
| 3 | A | A | A | A0&A1&A2 | CQI0 & CQI1 | | A0&A1&A2 | CQI2 | |
| 4 | A | - | A | A0&D&A2 | CQI0 | | A0&D&A2 | CQI2 | |

In this table cell 0 refers to the serving HS-DSCH cell, cell 1 refers to the secondary serving HS-DSCH cell and cell 2 refers to the assisting serving HS-DSCH cell.

Table 15C.11: The UE is configured with one serving and two assisting serving HS-DSCH cells and no cells are in MIMO mode

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **MF case** | **Cell activation status** | | | **HS-DPCCH subframe #1** | | | **HS-DPCCH subframe #2** | | |
| **Cell group 1** | **Cell group 2** | | **Slot 0** | **Slot 1** | **Slot 2** | **Slot 0** | **Slot 1** | **Slot 2** |
|  | **Cell0** | **Cell1** | **Cell2** |
| 5 | A | A | A | A0&A1&A2 | CQI0 | | A0&A1&A2 | CQI1 & CQI2 | |
| 6 | A | A | - | A0&A1&D | CQI0 | | A0&A1&D | CQI1 | |

In this table cell 0 refers to the serving HS-DSCH cell, cell 1 refers to the assisting serving HS-DSCH cell and cell 2 refers to the assisting secondary serving HS-DSCH cell.

When MIMO is configured in at least one cell;

- If the UE is configured with two serving and one assisting serving HS-DSCH cells the HS-DPCCH mapping follows the table 15C.12

- If the UE is configured with one serving and two assisting serving HS-DSCH cells the HS-DPCCH mapping follows the table 15C.13.

- The channel coding for HARQ-ACK for all cells is specified in subclause 4.7.3B.1.

- The channel coding for CQI associated with a cell for which the UE is not configured in MIMO mode is specified in subclause 4.7.2.2.

- The channel coding for PCI and CQI associated with a cell for which the UE is configured in MIMO mode is specified in subclause 4.7.3.2.

- HS-DPCCH is transmitted using slot format #1.

Table 15C.12: The UE is configured with two serving and one assisting serving HS-DSCH cells and at least one cell is configured in MIMO mode

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **MF case** | **Cell activation status** | | | **HS-DPCCH subframe #1** | | | | **HS-DPCCH subframe #2** | | | |
| **Cell group 1** | | **Cell group 2** | **Slot 0** | | **Slot 1** | **Slot 2** | **Slot 0** | | **Slot 1** | **Slot 2** |
|  | **Cell0** | **Cell1** | **Cell2** |
| 7 | A | A | A | A0&A1 | A2&D | PCI/CQI0 | PCI/CQI1 | A0&A1 | A2&D | PCI/CQI2 | PCI/CQI2 |
| 8 | A | - | A | A0&D | A2&D | PCI/CQI0 | PCI/CQI0 | A0&D | A2&D | PCI/CQI2 | PCI/CQI2 |

In this table cell 0 refers to the serving HS-DSCH cell, cell 1 refers to the secondary serving HS-DSCH cell and cell 2 refers to the assisting serving HS-DSCH cell.

Table 15C.13: The UE is configured with one serving and two assisting serving HS-DSCH cells and at least one cell is configured in MIMO mode

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **MF case** | **Cell activation status** | | | **HS-DPCCH subframe #1** | | | | **HS-DPCCH subframe #2** | | | |
| **Cell group 1** | **Cell group 2** | | **Slot 0** | | **Slot 1** | **Slot 2** | **Slot 0** | | **Slot 1** | **Slot 2** |
|  | **Cell0** | **Cell1** | **Cell2** |
| 9 | A | A | A | A0&D | A1&A2 | PCI/CQI0 | PCI/CQI0 | A0&D | A1&A2 | PCI/CQI1 | PCI/CQI2 |
| 10 | A | A | - | A0&D | A1&D | PCI/CQI0 | PCI/CQI0 | A0&D | A1&D | PCI/CQI1 | PCI/CQI1 |

In this table cell 0 refers to the serving HS-DSCH cell, cell 1 refers to the assisting serving HS-DSCH cell and cell 2 refers to the assisting secondary serving HS-DSCH cell.

##### 4.7.4.3.3 Physical Channel mapping for HS-DPCCH HARQ-ACK and PCI/CQI when the UE is configured with two serving and two assisting serving HS-DSCH cells

When MIMO is not configured in any cell;

- The HS-DPCCH mapping follows the table 15C.14

- The channel coding for HARQ-ACK is specified in subclause 4.7.3B.1.

- The channel coding for CQI is specified in subclause 4.7.2.2.

- HS-DPCCH is transmitted using slot format #1.

Table 15C.14: The UE is configured with two serving and two assisting serving HS-DSCH cells and no cells are in MIMO mode

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **MF case** | **Cell activation status** | | | | **HS-DPCCH subframe #1** | | | | **HS-DPCCH subframe #2** | | | |
| **Cell group 1** | | **Cell group 2** | | **Slot 0** | | **Slot 1** | **Slot 2** | **Slot 0** | | **Slot 1** | **Slot 2** |
|  | **Cell0** | **Cell1** | **Cell2** | **Cell3** |
| 11 | A | A | A | A | A0&A1 | A2&A3 | CQI0 | CQI1 | A0&A1 | A2&A3 | CQI2 | CQI3 |
| 12 | A | A | A | - | A0&A1 | A2&D | CQI0 | CQI1 | A0&A1 | A2&D | CQI2 | CQI2 |
| 13 | A | - | A | A | A0&D | A2&A3 | CQI0 | CQI0 | A0&D | A2&A3 | CQI2 | CQI3 |
| 14 | A | - | A | - | A0&D | A2&D | CQI0 | CQI0 | A0&D | A2&D | CQI2 | CQI2 |

In this table cell 0 refers to the serving HS-DSCH cell, cell 1 refers to the secondary serving HS-DSCH cell, cell 2 refers to the assisting serving HS-DSCH cell and cell 3 refers to the assisting secondary serving HS-DSCH cell.

When MIMO is configured in at least one cell;

- The HS-DPCCH mapping follows the table 15C.15

- The channel coding for HARQ-ACK for all cells is specified in subclause 4.7.3B.1.

- The channel coding for CQI associated with a cell for which the UE is not configured in MIMO mode is specified in subclause 4.7.2.2.

- The channel coding for PCI and CQI associated with a cell for which the UE is configured in MIMO mode is specified in subclause 4.7.3.2.

- HS-DPCCH is transmitted using slot format #1.

Table 15C.15: The UE is configured with two serving and two assisting serving HS-DSCH cells and at least one cell is configured in MIMO mode

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **MF case** | **Cell activation status** | | | | **HS-DPCCH subframe #1** | | | | **HS-DPCCH subframe #2** | | | |
| **Cell group 1** | | **Cell group 2** | | **Slot 0** | | **Slot 1** | **Slot 2** | **Slot 0** | | **Slot 1** | **Slot 2** |
|  | **Cell0** | **Cell1** | **Cell2** | **Cell3** |
| 15 | A | A | A | A | A0&A1 | A2&A3 | PCI/CQI0 | PCI/CQI1 | A0&A1 | A2&A3 | PCI/CQI2 | PCI/CQI3 |
| 16 | A | A | A | - | A0&A1 | A2&D | PCI/CQI0 | PCI/CQI1 | A0&A1 | A2&D | PCI/CQI2 | PCI/CQI2 |
| 17 | A | - | A | A | A0&D | A2&A3 | PCI/CQI0 | PCI/CQI0 | A0&D | A2&A3 | PCI/CQI2 | PCI/CQI3 |
| 18 | A | - | A | - | A0&D | A2&D | PCI/CQI0 | PCI/CQI0 | A0&D | A2&D | PCI/CQI2 | PCI/CQI2 |

In this table cell 0 refers to the serving HS-DSCH cell, cell 1 refers to the secondary serving HS-DSCH cell, cell 2 refers to the assisting serving HS-DSCH cell and cell 3 refers to the assisting secondary serving HS-DSCH cell.

##### 4.7.4.3.4 Physical Channel mapping for HS-DPCCH HARQ-ACK and PCI/CQI when the UE is configured with three serving and one assisting serving HS-DSCH cells or one serving and three assisting serving HS-DSCH cells

When MIMO is not configured in any cell;

- If the UE is configured with three serving and one assisting serving HS-DSCH cells, the HS-DPCCH mapping follows the table 15C.16.

- If the UE is configured with one serving and three assisting serving HS-DSCH cells, the HS-DPCCH mapping follows the table 15C.17.

- The channel coding for HARQ-ACK is specified in subclause 4.7.3B.1.

- The channel coding for CQI is specified in subclause 4.7.2.2.

- HS-DPCCH is transmitted using slot format #1.

Table 15C.16: The UE is configured with three serving and one assisting serving HS-DSCH cells and no cells are in MIMO mode

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| MF case | Cell activation status | | | | HS-DPCCH subframe #1 | | | | HS-DPCCH subframe #2 | | | |
| Cell group 1 | | | CG2 | Slot 0 | | Slot 1 | Slot 2 | Slot 0 | | Slot 1 | Slot 2 |
|  | Cell0 | Cell1 | Cell2 | Cell3 |
| 19 | A | A | A | A | A0&A1 | A2&A3 | CQI0 | CQI1 | A0&A1 | A2&A3 | CQI2 | CQI3 |
| 20 | A | - | A | A | A0&D | A2&A3 | CQI0 | CQI0 | A0&D | A2&A3 | CQI2 | CQI3 |
| 21 | A | A | - | A | A0&A1 | D&A3 | CQI0 | CQI1 | A0&A1 | D&A3 | DTX | CQI3 |
| 22 | A | - | - | A | A0&D | D&A3 | CQI0 | CQI0 | A0&D | D&A3 | DTX | CQI3 |

In this table cell 0 refers to the serving HS-DSCH cell, cell 1 refers to the 1st secondary serving HS-DSCH cell, cell 2 refers to the 2nd secondary serving HS-DSCH cell and cell 3 refers to the assisting serving HS-DSCH cell.

Table 15C.17: The UE is configured with one serving and three assisting serving HS-DSCH cells and no cells are in MIMO mode

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| MF case | Cell activation status | | | | HS-DPCCH subframe #1 | | | | HS-DPCCH subframe #2 | | | |
| CG1 | Cell group 2 | | | Slot 0 | | Slot 1 | Slot 2 | Slot 0 | | Slot 1 | Slot 2 |
|  | Cell0 | Cell1 | Cell2 | Cell3 |
| 23 | A | A | A | A | A0&A1 | A2&A3 | CQI0 | CQI1 | A0&A1 | A2&A3 | CQI2 | CQI3 |
| 24 | A | A | - | A | A0&A1 | D&A3 | CQI0 | CQI1 | A0&A1 | D&A3 | DTX | CQI3 |
| 25 | A | A | A | - | A0&A1 | A2&D | CQI0 | CQI1 | A0&A1 | A2&D | CQI2 | DTX |
| 26 | A | A | - | - | A0&A1 | D | CQI0 | CQI1 | A0&A1 | D | DTX | DTX |

In this table cell 0 refers to the serving HS-DSCH cell, cell 1 refers to the assisting serving HS-DSCH cell, cell 2 refers to the 1st assisting secondary serving HS-DSCH cell and cell 3 refers to the 2nd assisting secondary serving HS-DSCH cell.

When MIMO is configured in at least one cell;

- If the UE is configured with three serving and one assisting serving HS-DSCH cells, the HS-DPCCH mapping follows the table 15C.18.

- If the UE is configured with one serving and three assisting serving HS-DSCH cells, the HS-DPCCH mapping follows the table 15C.19.

- The channel coding for HARQ-ACK for all cells is specified in subclause 4.7.3B.1, with the following exceptions:

- The second half (last 10 bits) of the Slot0 in Table 15C.18, where the channel coding is specified in subclause 4.7.3D.1.

- The first half (first 10 bits) of the Slot0 in Table 15C.19, where the channel coding is specified in subclause 4.7.3D.1

- The channel coding for CQI associated with a cell for which the UE is not configured in MIMO mode is specified in subclause 4.7.2.2.

- The channel coding for PCI and CQI associated with a cell for which the UE is configured in MIMO mode is specified in subclause 4.7.3.2.

- HS-DPCCH is transmitted using slot format #1.

Table 15C.18: The UE is configured with three serving and one assisting serving HS-DSCH cells and at least one cell is configured in MIMO mode

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| MF case | Cell activation status | | | | HS-DPCCH subframe #1 | | | | HS-DPCCH subframe #2 | | | |
| Cell group 1 | | | CG2 | Slot 0 | | Slot 1 | Slot 2 | Slot 0 | | Slot 1 | Slot 2 |
|  | Cell0 | Cell1 | Cell2 | Cell3 |
| 27 | A | A | A | A | A0&A1 | A2&A3 | PCI/CQI0 | PCI/CQI1 | A0&A1 | A2&A3 | PCI/CQI2 | PCI/CQI3 |
| 28 | A | - | A | A | A0&D | A2&A3 | PCI/CQI0 | PCI/CQI0 | A0&D | A2&A3 | PCI/CQI2 | PCI/CQI3 |
| 29 | A | A | - | A | A0&A1 | D&A3 | PCI/CQI0 | PCI/CQI1 | A0&A1 | D&A3 | DTX | PCI/CQI3 |
| 30 | A | - | - | A | A0&D | D&A3 | PCI/CQI0 | PCI/CQI0 | A0&D | D&A3 | DTX | PCI/CQI3 |

In this table cell 0 refers to the serving HS-DSCH cell, cell 1 refers to the 1st secondary serving HS-DSCH cell, cell 2 refers to the 2nd secondary serving HS-DSCH cell and cell 3 refers to the assisting serving HS-DSCH cell.

Table 15C.19: The UE is configured with one serving and three assisting serving HS-DSCH cells and at least one cell is configured in MIMO mode

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| MF case | Cell activation status | | | | HS-DPCCH subframe #1 | | | | HS-DPCCH subframe #2 | | | |
| CG1 | Cell group 2 | | | Slot 0 | | Slot 1 | Slot 2 | Slot 0 | | Slot 1 | Slot 2 |
|  | Cell0 | Cell1 | Cell2 | Cell3 |
| 31 | A | A | A | A | A0&A1 | A2&A3 | PCI/CQI0 | PCI/CQI1 | A0&A1 | A2&A3 | PCI/CQI2 | PCI/CQI3 |
| 32 | A | A | - | A | A0&A1 | A2&D | PCI/CQI0 | PCI/CQI1 | A0&A1 | D&A3 | DTX | PCI/CQI3 |
| 33 | A | A | A | - | A0&A1 | D&A3 | PCI/CQI0 | PCI/CQI1 | A0&A1 | A2&D | PCI/CQI2 | DTX |
| 34 | A | A | - | - | A0&A1 | D | PCI/CQI0 | PCI/CQI1 | A0&A1 | D | DTX | DTX |

In this table cell 0 refers to the serving HS-DSCH cell, cell 1 refers to the assisting serving HS-DSCH cell, cell 2 refers to the 1st assisting secondary serving HS-DSCH cell and cell 3 refers to the 2nd assisting secondary serving HS-DSCH cell.

#### 4.7.4.4 Physical Channel mapping for HS-DPCCH when the UE is configured in MIMO mode with four transmit antennas in at least one cell

##### 4.7.4.4.1 Physical Channel mapping for HS-DPCCH HARQ-ACK

If the HS-DPCCH slot format 0 as defined in [2], is used, the HS-DPCCH physical channel mapping function shall map the input bits wk directly to physical channel so that bits are transmitted over the air in ascending order with respect to k.

If the HS-DPCCH slot format 1 as defined in [2], is used, the HS-DPCCH physical channel mapping function shall map the input bits wk to the physical channel so that bits are transmitted over the air in ascending order with respect to k as follows:

- If Secondary\_Cell\_Enabled is equal to 3 and Secondary\_Cell\_Active is equal to 3

- The following HARQ-ACK messages are transmitted on HS-DPCCH:

- HARQ-ACK comprising the HARQ acknowledgement messages for the pair of serving HS-DSCH cell and 1st secondary serving HS-DSCH cell in that order

- The following HARQ-ACK messages are transmitted on HS-DPCCH2 :

- HARQ-ACK comprising the HARQ acknowledgement messages for the pair of the 2nd secondary serving HS-DSCH cell and the 3rd secondary serving HS-DSCH cell in that order

- If Secondary\_Cell\_Enabled is equal to 2 and Secondary\_Cell\_Active is equal to 2

- The following HARQ-ACK messages are transmitted on HS-DPCCH:

- HARQ-ACK comprising the HARQ acknowledgement messages for the pair of serving HS-DSCH cell and 1st secondary serving HS-DSCH cell in that order

- The following HARQ-ACK messages are transmitted on HS-DPCCH2 :

- HARQ-ACK comprising the HARQ acknowledgement message for the 2nd secondary serving HS-DSCH cell

- If Secondary\_Cell\_Enabled is equal to 1 and Secondary\_Cell\_Active is equal to 1

- The following two HARQ-ACK messages are transmitted on HS-DPCCH

- HARQ-ACK comprising the HARQ acknowledgement messages for the pair of serving HS-DSCH cell and 1st secondary serving HS-DSCH cell in that order

- If Secondary\_Cell\_Enabled is equal to 3 and Secondary\_Cell\_Active is less than Secondary\_Cell\_Enabled:

- If none of the 2nd or 3rd secondary serving HS-DSCH cell is activated HS-DPCCH2 is not transmitted

- If only one of the 2nd or 3rd secondary serving HS-DSCH cell is activated the HARQ-ACK is repeated according to the Figure 20E

- If the 1st secondary serving HS-DSCH cell is not activated the HARQ-ACK is repeated according to the Figure 20E

- Otherwise the transmissions of the HARQ-ACK messages are the same as if Secondary\_Cell\_Active was equal to Secondary\_Cell\_Enabled.

- If Secondary\_Cell\_Enabled is equal to 2 and Secondary\_Cell\_Active is less than Secondary\_Cell\_Enabled:

- If the 2nd secondary serving HS-DSCH cell is not activated the HARQ-ACK transmissions on HS-DPCCH2 are DTXed

- If the 1st secondary serving HS-DSCH cell is not activated the HARQ-ACK is repeated according to the Figure 20E

- Otherwise the transmissions of the HARQ-ACK messages are the same as if Secondary\_Cell\_Active was equal to Secondary\_Cell\_Enabled.

- If Secondary\_Cell\_Enabled is equal to 1 and Secondary\_Cell\_Active is 0 then the transmission of the HARQ-ACK message is repeated according to Figure 20E.

##### 4.7.4.4.2 Physical Channel mapping for HS-DPCCH NTBP/PCI/CQI

If the HS-DPCCH slot format 0 as defined in [2] is used, the HS-DPCCH physical channel mapping function shall map the input bits bk directly to physical channel so that bits are transmitted over the air in ascending order with respect to k.

If the HS-DPCCH slot format 1 as defined in [2] is used, the HS-DPCCH physical channel mapping function shall map the input bits bk directly to physical channel so that bits are transmitted over the air in ascending order with respect to k.

- If Secondary\_Cell\_Enabled is equal to 3 and Secondary\_Cell\_Active is equal to 3

- The following is transmitted on HS-DPCCH:

- The report for the serving HS-DSCH cell (CQI1 or PCI/CQI1 or NTBP/PCI/CQI1) and the 1st secondary serving HS-DSCH cell (CQI2 or PCI/CQI2 or NTBP/PCI/CQI2) are mapped to a separate subframe as specified in [4].

- If the serving cell is configured in MIMO mode with four transmit antennas and the 1st secondary serving cell is not configured in MIMO mode with four transmit antennas, the CQI2 or PCI/CQI2 of the 1st secondary serving cell is repeated.

- If the serving cell is not configured in MIMO mode with four transmit antennas and the 1st secondary serving cell is configured in MIMO mode with four transmit antennas, the CQI1 or PCI/CQI1 of the serving cell is repeated.

- If both the serving cell and 1st secondary serving cell are not configured in MIMO mode with four transmit antennas the CQI1 or PCI/CQI1 and CQI2 or PCI/CQI2 are mapped to a separate subframe as specified in [4].

- The following is transmitted on HS-DPCCH2:

- The report for the 2nd secondary HS-DSCH cell (CQI3 or PCI/CQI3 or NTBP/PCI/CQI3) and the 3rd secondary HS-DSCH cell (CQI4 or PCI/CQI4 or NTBP/PCI/CQI4) are mapped to a separate subframe as specified in [4].

- If the 2nd serving cell is configured in MIMO mode with four transmit antennas and the 3rd secondary serving cell is not configured in MIMO mode with four transmit antennas, the CQI4 or PCI/CQI4 of the 3rd secondary serving cell is repeated.

- If the 2nd serving cell is not configured in MIMO mode with four transmit antennas and the 3rd secondary serving cell is configured in MIMO mode with four transmit antennas, the CQI3 or PCI/CQI3 of the 2nd serving cell is repeated.

- If both the 2nd serving cell and 3rd secondary serving cell are not configured in MIMO mode with four transmit antennas the CQI3 or PCI/CQI3 and CQI4 or PCI/CQI4 are mapped to a separate subframe as specified in [4].

- If Secondary\_Cell\_Enabled is equal to 2 and Secondary\_Cell\_Active is equal to 2

- The following is transmitted on HS-DPCCH:

- The report for the serving HS-DSCH cell (CQI1 or PCI/CQI1 or NTBP/PCI/CQI1) and the 1st secondary serving HS-DSCH cell (CQI2 or PCI/CQI2 or NTBP/PCI/CQI2) are mapped to a separate subframe as specified in [4].

- If the serving cell is configured in MIMO mode with four transmit antennas and the 1st secondary serving cell is not configured in MIMO mode with four transmit antennas, the CQI2 or PCI/CQI2 of the 1st secondary serving cell is repeated.

- If the serving cell is not configured in MIMO mode with four transmit antennas and the 1st secondary serving cell is configured in MIMO mode with four transmit antennas, the CQI1 or PCI/CQI1 of the serving cell is repeated.

- If both the serving cell and 1st secondary serving cell are not configured in MIMO mode with four transmit antennas the CQI1 or PCI/CQI1 and CQI2 or PCI/CQI2 are mapped to a separate subframe as specified in [4].

- The following is transmitted on HS-DPCCH2:

- If the 2nd serving cell is configured in MIMO mode with four transmit antennas the HS-DPCCH2 physical channel mapping function shall map NTBP/ PCI/CQI3 to the physical channel.

- If the 2nd serving cell is not configured in MIMO mode with four transmit antennas the HS-DPCCH2 physical channel mapping function shall map CQI3 or PCI/CQI3 to the physical channel.

- If Secondary\_Cell\_Enabled is equal to 1 and Secondary\_Cell\_Active is equal to 1

- The following is transmitted on HS-DPCCH:

- The report for the serving HS-DSCH cell (CQI1 or PCI/CQI1 or NTBP/PCI/CQI1) and the 1st secondary serving HS-DSCH cell (CQI2 or PCI/CQI2 or NTBP/PCI/CQI2) are mapped to a separate subframe as specified in [4].

- If the serving cell is configured in MIMO mode with four transmit antennas and the 1st secondary serving cell is not configured in MIMO mode with four transmit antennas, the CQI2 or PCI/CQI2 of the 1st secondary serving cell is repeated.

- If the serving cell is not configured in MIMO mode with four transmit antennas and the 1st secondary serving cell is configured in MIMO mode with four transmit antennas, the CQI1 or PCI/CQI1 of the serving cell is repeated.

- If Secondary\_Cell\_Enabled is equal to 1 and Secondary\_Cell\_Active is less than Secondary\_Cell\_Enabled:

- The following is transmitted on HS-DPCCH:

- The report for the serving HS-DSCH cell (CQI1 or PCI/CQI1 or NTBP/PCI/CQI1) and the 1st secondary serving HS-DSCH cell (CQI2 or PCI/CQI2 or NTBP/PCI/CQI2) are mapped to a separate subframe as specified in [4]. The slots corresponding to the (CQI2 or PCI/CQI2 or NTBP/PCI/CQI2) are DTXed.

- If Secondary\_Cell\_Enabled is equal to 2 and Secondary\_Cell\_Active is less than Secondary\_Cell\_Enabled:

- If the 2nd serving cell is not activated HS-DPCCH2 is not transmitted.

- The following is transmitted on HS-DPCCH:

- The report for the serving HS-DSCH cell (CQI1 or PCI/CQI1 or NTBP/PCI/CQI1) and the 1st secondary serving HS-DSCH cell (CQI2 or PCI/CQI2 or NTBP/PCI/CQI2) are mapped to a separate subframe as specified in [4]. The slots corresponding to the (CQI2 or PCI/CQI2 or NTBP/PCI/CQI2) are DTXed.

- The following is transmitted on HS-DPCCH2:

- If the 2nd serving cell is configured in MIMO mode with four transmit antennas the HS-DPCCH2 physical channel mapping function shall map NTBP/ PCI/CQI3 to the physical channel

- If the 2nd serving cell is not configured in MIMO mode with four transmit antennas the HS-DPCCH2 physical channel mapping function shall map CQI3 or PCI/CQI3 to the physical channel.

- If Secondary\_Cell\_Enabled is equal to 3 and Secondary\_Cell\_Active is less than Secondary\_Cell\_Enabled:

- If none of the 2nd or 3rd secondary serving HS-DSCH cell is activated HS-DPCCH2 is not transmitted and the rules in case Secondary\_Cell\_Enabled is equal to 1 and Secondary\_Cell\_Active is equal to 1 are followed for HS-DPCCH

- The following is transmitted on HS-DPCCH:

- The report for the serving HS-DSCH cell (CQI1 or PCI/CQI1 or NTBP/PCI/CQI1) and the 1st secondary serving HS-DSCH cell (CQI2 or PCI/CQI2 or NTBP/PCI/CQI2) are mapped to a separate subframe as specified in [4]. The slots corresponding to the (CQI2 or PCI/CQI2 or NTBP/PCI/CQI2) are DTXed.

- The following is transmitted on HS-DPCCH2:

- If the 3rd secondary serving HS-DSCH cell is not activated, the report for the 2nd secondary HS-DSCH cell (CQI3 or PCI/CQI3 or NTBP/PCI/CQI3) and the 3rd secondary serving HS-DSCH cell (CQI4 or PCI/CQI4 or NTBP/PCI/CQI4) are mapped to a separate subframe as specified in [4]. The slots corresponding to the (CQI4 or PCI/CQI4 or NTBP/PCI/CQI4) are DTXed.

- If the 2rd secondary serving HS-DSCH cell is not activated, the report for the 3rd secondary HS-DSCH cell (CQI4 or PCI/CQI4 or NTBP/PCI/CQI4) and the 2nd secondary serving HS-DSCH cell (CQI3 or PCI/CQI3 or NTBP/PCI/CQI3) are mapped to a separate subframe as specified in [4]. The slots corresponding to the (CQI3 or PCI/CQI3 or NTBP/PCI/CQI3) are DTXed.

- If Secondary\_Cell\_Enabled is equal to 0

- The following is transmitted on HS-DPCCH:

- The physical channel mapping function shall map NTBP/ PCI/CQI1 to the physical channel.

## 4.8 Coding for E‑DCH

Figure 21 shows the processing structure for the E‑DCH transport channel mapped onto a separate CCTrCH.

If UL\_MIMO\_Enabled is not set to TRUE, or UL\_MIMO\_Enabled is set to TRUE and UL\_CLTD\_Active is not 1, data arrives to the coding unit in form of a maximum of one transport block once every transmission time interval (TTI).

If UL\_MIMO\_Enabled is set to TRUE and UL\_CLTD\_Active = 1, data arrives to the coding unit in form of a maximum of two transport blocks once every TTI.

- If a single transport block arrives to the coding unit in a TTI, the transport block is processed as when UL\_MIMO\_Enabled is not set to TRUE.

- If two transport blocks arrive to the coding unit in a TTI, each transport block is separately processed as when UL\_MIMO\_Enabled is not set to TRUE, with the exception of the rank-dependent determinations of SF, modulation, number of E-DPDCHs and S-E-DPDCHs, and the physical channel mapping.

The following coding steps can be identified:

- Add CRC to the transport block

- Code block segmentation

- Channel coding

- Physical layer hybrid ARQ and rate matching

- Physical channel segmentation

- Interleaving

- Physical channel mapping

The coding steps for E-DCH transport channel are shown in the figure below.



Figure 21: Transport channel processing for E-DCH

In the following the number of transport blocks per TTI and the number of transport channels is always one i.e. *m*=1 and *i*=1. When referencing non E-DCH formulae which are used in correspondence with E-DCH formulae the convention is used that transport block subscripts may be omitted (e.g. *X1* may be written *X*).

### 4.8.1 CRC attachment for E-DCH

CRC attachment for the E-DCH transport channel shall be performed according to the general method described in 4.2.1 above with the following specific parameters.

The CRC length shall always be *L1*=24 bits.

### 4.8.2 Code block segmentation for E-DCH

Code block segmentation for the E-DCH transport channel shall be performed according to the general method described in 4.2.2.2 with the following specific parameters.

There is a maximum of one transport block. The bits input to the block are mapped to the bits directly. It follows that *Xi* = *Bi*. Note that the bits *x* referenced here refer only to the internals of the code block segmentation function. The output bits from the code block segmentation function are *oir1*, *oir2*, *oir3*, …, *oirK*.

The value of *Z* = 5114 for turbo coding shall be used.

### 4.8.3 Channel coding for E-DCH

Channel coding for the E-DCH transport channel shall be performed according to the general method described in clause 4.2.3 above with the following specific parameters.

There is a maximum of one transport block, *i*=1. The rate 1/3 turbo coding shall be used.

### 4.8.4 Physical layer HARQ functionality and rate matching for E-DCH

The hybrid ARQ functionality matches the number of bits at the output of the channel coder to the total number of bits of the E-DPDCH or S-E-DPDCH set to which the E-DCH transport channel is mapped. The hybrid ARQ functionality is controlled by the redundancy version (RV) parameters.



Figure 22: E‑DCH hybrid ARQ functionality

#### 4.8.4.1 Determination of SF, modulation scheme and number of E-DPDCH PhCHs needed

The maximum amount of puncturing that can be applied is

- 1-*PLnon-max* if the modulation scheme or the number of code channels is less than the maximum allowed by the UE capability and restrictions imposed by UTRAN.

- 1-*PLmod\_switch* if the modulation scheme is BPSK, the number of E-DPDCH code channels equals to 4 and the usage of 4PAM is allowed by the UE capability and restrictions imposed by UTRAN.

- 1-*PLmod\_switch\_2* if the modulation scheme is 4PAM, the number of E-DPDCH code channels equals to 4 and the usage of 8PAM is allowed by the UE capability and restrictions imposed by UTRAN.

- 1-*PLmax* if the modulation scheme and the number of code channels equals to the maximum allowed by the UE capability and restrictions imposed by UTRAN.

The number of available bits per TTI of one E-DPDCH for all possible spreading factors and modulation schemes is denoted by *N256, N128, N64, N32, N16, N8, N4,N2,* *M4, M2*, *L4* and *L2* where the index refers to the spreading factor. *N* refers to BPSK modulation, *M* to 4PAM modulation and *L* to 8PAM modulation.

The possible number of bits available to the CCTrCH of E-DCH type on all E-DPDCHs, *Ne,data*, then are {*N256, N128, N*64, *N*32, *N*16, *N*8, *N*4,2*N*4,2*N*2,2*N*2+2*N*4, 2*M*2+2*M*4, 2*L*2+2*L*4}.

SET0 denotes the set of *Ne,data*values allowed by the UTRAN and supported by the UE, as part of the UE’s capability. SET0 can be a subset of {*N256, N128, N*64, *N*32, *N*16, *N*8, *N*4,2*N*4,2*N*2,2*N*2+2*N*4, 2*M*2+2*M*4, 2*L*2+2*L*4}.

The total number of bits in a TTI on all E-DPDCHs before rate matching with transport format j is *Ne,j*. The total number of bits available for the E‑DCH transmission per TTI on all E-DPDCHs with transport format j, *Ne,data,j*, is determined by executing the following algorithm, where

*- PLnon-max* is signalled from higher layers,

*- PLmod\_,switch* is equal to 0.468,

*- PLmod\_switch\_2* is equal to 0.4,

*- PLmax* is equal to 0.44 , except when the *Ne,data* = 2*N*2+2*N*4, 2*M*2+2*M*4 or 2*L*2+2*L*4 is allowed by the UTRAN and supported by the UE, in which case *PLmax* is equal to 0.33:

If the UE transmits only one transport block:

SET1 = { *Ne,data* in SET0 such that *Ne,data* – *Ne,j* is non negative }

If SET1 is not empty and the smallest element of SET1 requires just one E-DPDCH then

*Ne,data,j* = min SET1

Else

SET2 = { *Ne,data* in SET0 without 2*N*2+2*N*4, 2*M*2+2*M*4 and 2*L*2+2*L*4 such that *Ne,data* – *PLnon-max* × *Ne,j* is non negative }

If SET2 is not empty then

Sort SET2 in ascending order

*Ne,data* = min SET2

While *Ne,data* is not the max of SET2 and the follower of *Ne,data* requires only one E-DPDCH do

*Ne,data* = follower of *Ne,data* in SET2

End while

*Ne,data,j* = *Ne,data*

Else

If SET0 includes 2*N*2+2*N*4

*Ne,data* = 2*N*2+2*N*4

If *Ne,data* / *Ne,j* < *PLmod\_switch* and SET0 includes 2*M*2+2*M*4

*Ne,data* = 2*M*2+2*M*4

End if

If *Ne,data* is equal to 2*M*2+2*M*4 and *Ne,data* / *Ne,j* < *PLmod\_switch\_2* and SET0 includes 2*L*2+2*L*4

*Ne,data* = 2*L*2+2*L*4

End if

*Ne,data,j* = *Ne,data* provided that *Ne,data,j* - *PLmax* × *Ne,j* is non negative

Else

*Ne,data,j* = max SET0 provided that *Ne,data,j* - *PLmax* × *Ne,j* is non negative

End if

End if

End if

Else (when UE transmits two transport blocks)

*Ne,data* = 2*N*2+2*N*4

If *Ne,data* / *Ne,j* < *PLmod\_switch* and SET0 includes 2*M*2+2*M*4

*Ne,data* = 2*M*2+2*M*4

End if

If *Ne,data* is equal to 2*M*2+2*M*4, *Ne,data* / *Ne,j* < *PLmod\_switch\_2* and SET0 includes 2*L*2+2*L*4

*Ne,data* = 2*L*2+2*L*4

End if

*Ne,data,j* = *Ne,data* provided that *Ne,data* - *PLmax* × *Ne,j* is non negative

End if

While E‑DCH TTI length is 10 ms, if an initial transmission occurs in a compressed frame, or a retransmission occurs in a compressed frame, or a retransmission occurs in a non‑compressed frame for which initial transmission was compressed, the number of available bits per TTI of one E‑DPDCH for all possible spreading factors denoted by *N256, N128, N64, N32, N16, N8, N4* and *N2* used in the algorithm above is replaced by *k*×*N256, k*×*N128, k*×*N64, k*×*N32, k*×*N16, k*×*N8, k*×*N4* and *k*×*N2.* The parameter *k* is equal to *ntx1*/15 and *ntx1* is defined in 4.4.5.1.

#### 4.8.4.1A Determination of SF, modulation scheme and number of S-E-DPDCH PhCHs needed

S-E-DPDCHs are only present when the UE transmits two transport blocks. When present, the number of S-E-DPDCHs is always 4.

The maximum amount of puncturing that can be applied is

- 1-*PLnon-max* if the modulation scheme is less than the maximum allowed by the UE capability and restrictions imposed by UTRAN.

- 1-*PLmod\_switch* if the modulation scheme is BPSK and the usage of 4PAM is allowed by the UE capability and restrictions imposed by UTRAN.

- 1-*PLmod\_switch\_2* if the modulation scheme is 4PAM and the usage of 8PAM is allowed by the UE capability and restrictions imposed by UTRAN.

- 1-*PLmax* if the modulation scheme equals to the maximum allowed by the UE capability and restrictions imposed by UTRAN.

The number of available bits per TTI of one S-E-DPDCH for all possible spreading factors and modulation schemes is denoted by *N4, N2,* *M4*, *M2*, *L4* and *L2*, where the index refers to the spreading factor. *N* refers to BPSK modulation, *M* to 4PAM modulation and *L* to 8PAM modulation.

The possible number of bits available to the CCTrCH of E-DCH type on all S-E-DPDCHs, *Ne,data*, then are {2*N*2+2*N*4, 2*M*2+2*M*4, 2*L*2+2*L*4}.

SET0 denotes the set of *Ne,data*values allowed by the UTRAN and supported by the UE, as part of the UE’s capability. SET0 can be a subset of {2*N*2+2*N*4, 2*M*2+2*M*4, 2*L*2+2*L*4}.

The total number of bits in a TTI on all S-E-DPDCHs before rate matching with transport format j is *Ne,j*. The total number of bits available for the E‑DCH transmission per TTI on all S-E-DPDCHs with transport format j, *Ne,data,j*, is determined by executing the following algorithm, where

*- PLmod\_switch* is equal to 0.468,

*- PLmod\_switch\_2* is equal to 0.4,

*- PLmax* is equal to 0.33:

*Ne,data* = 2*N*2+2*N*4

If *Ne,data* / *Ne,j* < *PLmod\_switch* and SET0 includes 2*M*2+2*M*4

*Ne,data* = 2*M*2+2*M*4

End if

If *Ne,data* is equal to 2*M*2+2*M*4, *Ne,data* / *Ne,j* < *PLmod\_switch\_2* and SET0 includes 2*L*2+2*L*4

*Ne,data* = 2*L*2+2*L*4

End if

*Ne,data,j* = *Ne,data* provided that *Ne,data* - *PLmax* × *Ne,j* is non negative

#### 4.8.4.2 HARQ bit separation

The HARQ bit separation function shall be performed in the same way as bit separation for turbo encoded TrCHs with puncturing in 4.2.7.4.1 above.

#### 4.8.4.3 HARQ Rate Matching Stage

The hybrid ARQ rate matching for the E-DCH transport channel shall be done with the general method described in 4.2.7.5 with the following specific parameters.

The parameters of the rate matching stage depend on the value of the RV parameters *s* and *r*. The *s* and *r* combinations corresponding to each RV allowed for the E-DCH are listed in the table below.

Table 15D: RV for E-DCH

|  |  |  |
| --- | --- | --- |
| E-DCH RV Index | *s* | *r* |
| 0 | 1 | 0 |
| 1 | 0 | 0 |
| 2 | 1 | 1 |
| 3 | 0 | 1 |

The parameter *eplus*, *eminus* and *eini* are calculated with the general method for QPSK as described in 4.5.4.3 above. The following parameters are used as input:

*Nsys* = *Np1* = *Np2* = *Ne,j*/3

*Ndata* = *Ne,data,j*

*rmax* = 2

During uplink compressed frames while E‑DCH TTI length is 10 ms and if *Ndata*>*Ne,j*:

- If *Ndata* mod 3 = 1, one *δ* bit is added to the *Nt,sys* bits as the last systematic bit and another δ bit is added to the *Nt,p1* bits as the last *Nt,p1* bit.

- If *Ndata* mod 3 = 2, one *δ* bit is added to the *Nt,sys* bits as the last systematic bit.

#### 4.8.4.4 HARQ bit collection

The HARQ bit collection shall be performed according to the general method for bit collection for turbo encoded TrCHs with puncturing as specified in 4.2.7.4.2 including the removal of the bits with value **.

### 4.8.5 Physical channel segmentation for E‑DCH

When more than one E-DPDCH or S-E-DPDCH is used, physical channel segmentation distributes the bits among the different physical channels. The bits input to the physical channel segmentation are denoted by *s1*, *s2*, *s3*, …,*sR*, where *R* is the number of bits input to the physical channel segmentation block. The number of PhCHs is denoted by *P.*

The bits after physical channel segmentation are denoted *up,k* where *p* is the PhCH number. *U(p)* is the number of physical channel bits in one E-DCH TTI for the pth E-DPDCH or S-E-DPDCH. The relation between s*k* and *up,k* is given below.

Bits on first PhCH after physical channel segmentation:

*k* = 1, 2, ..., *U(1)*

Bits on pth PhCH after physical channel segmentation:

*k* = 1, 2, ..., *U*(p)

### 4.8.6 Interleaving for E‑DCH

The interleaving is done as shown in figure 22A below, separately for each physical channel. The bits input to the block interleaver are denoted by , where *p* is PhCH number and *U*=*U(p)* is the number of bits in one TTI for one PhCH.



Figure 22A: Interleaver structure for E-DCH

The basic interleaver is as the 2nd interleaver described in Clause 4.2.11.

For 4PAM, there are two identical interleavers of the same size R2×30, where R2 is the minimum integer fulfilling . The output bits from the physical channel segmentation are divided one by one between the interleavers: bit *up,k* goes to the first interleaver and bit *up,k+1* goes to the second interleaver. Bits are collected one by one from the interleavers: bit *vp,k* is obtained from the first interleaver and bit *vp,k+1* is obtained from the second interleaver, where k mod 2=1.

For 8PAM, there are three identical interleavers of the same size R2×30, where R2 is the minimum integer fulfilling . The output bits from the physical channel segmentation are divided one by one between the interleavers: bit *up,k* goes to the first interleaver, bit *up,k+1* goes to the second interleaver and bit *up,k+2* goes to the third interleaver. Bits are collected one by one from the interleavers: bit *vp,k* is obtained from the first interleaver, bit *vp,k+1* is obtained from the second interleaver and bit *vp,k+2* is obtained from the third interleaver, where k mod 3=1.

### 4.8.7 Physical channel mapping for E‑DCH

The E-DCH structure is described in [2]. The bits input to the physical channel mapping are denoted *p,1*, *p,2*, ..., *p,U(p)*. The bits *p,k* are mapped to the PhCHs such that the bits for each PhCH are transmitted over the air in ascending order with respect to *k*.

During compressed frames in the uplink and when E‑DCH TTI is 10 ms:

- For the initial transmission the bits shall be consecutively mapped to the non‑idle slots. The UE shall not map any bit to the E‑DPDCH idle slots specified in 4.4.5.1.

- In case a retransmission occurs in a compressed frame or a retransmission occurs in a non‑compressed frame for which initial transmission was compressed:

- If *ntx1*>*nmax*: The bits shall be consecutively mapped to the *nmax* available slots. The remaining bits are not transmitted.

- If *ntx1**nmax*: The bits shall be consecutively mapped to the *ntx1* non‑idle slots, whilst no bits are mapped to the idle slots.

- The transmission gap position and the parameters *ntx1* and *nmax* are specified in 4.4.5.2.

## 4.9 Coding for E‑DPCCH

The following information is transmitted by means of the E-DPCCH:

- Retransmission sequence number (RSN): *xrsn,1*, *xrsn,2*

- E-TFCI: *xtfci,1*, *xtfci,2*, ..., *xtfci,7*

- "Happy" bit: *xh,1*

### 4.9.1 Overview

The figure below illustrates the overall coding chain for E-DPCCH.



Figure 23: Coding chain for E‑DPCCH

### 4.9.2 E‑DPCCH information field mapping

#### 4.9.2.1 Information field mapping of E‑TFCI

The E‑TFCI is mapped such that *xtfci,1* corresponds to the MSB.

#### 4.9.2.2 Information field mapping of retransmission sequence number

To indicate the redundancy version (RV) of each HARQ transmission and to assist the Node B soft buffer management a two bit retransmission sequence number (RSN) is signalled from the UE to the Node B. The Node B can avoid soft buffer corruption by flushing the soft buffer associated to one HARQ process in case more than 3 consecutive E‑DPCCH transmissions on that HARQ process can not be decoded or the last received RSN is incompatible with the current one.

The RSN is set by higher layers as described in [16]. The RSN is mapped such that *xrsn,1* corresponds to the MSB.

The applied E-DCH RV index specifying the used RV (*s* and *r* parameter) depends on the RSN, on *Nsys* / *Ne,data,j*, and if RSN=3 also on the TTIN (TTI number). For 10 ms TTI the TTI number is equal to the CFN, for 2 ms TTI

TTIN = 5\*CFN + subframe number

where the subframe number counts the five TTIs which are within a given CFN, starting from 0 for the first TTI to 4 for the last TTI. NARQ is the number of Hybrid ARQ processes.

Table 16: Relation between RSN value and E-DCH RV Index

|  |  |  |
| --- | --- | --- |
| **RSN Value** | *Nsys* / *Ne,data,j* **<1/2** | **1/2 ≤** *Nsys* / *Ne,data,j* |
| **E-DCH RV Index** | **E-DCH RV Index** |
| 0 | 0 | 0 |
| 1 | 2 | 3 |
| 2 | 0 | 2 |
| 3 | [ TTIN/NARQ **mod** 2 ] x 2 | TTIN/NARQ **mod** 4 |

The UE shall use either

- an RV index as indicated in Table 16 and according to the RSN

- or, if signalled by higher layers only E-DCH RV index 0 independently of the RSN.

#### 4.9.2.3 Information field mapping of the "Happy" bit

The UE shall set *xh,1* as specified in Table 16A.

Table 16A: Mapping of "Happy" bit

|  |  |
| --- | --- |
| "Happy" bit | *xh,1* |
| Happy | 1 |
| Not happy | 0 |

### 4.9.3 Multiplexing of E‑DPCCH information

The E‑TFCI *xtfci,1, xtfci,2, …, xtfci,7*, the retransmission sequence number *xrsn,1*, *xrsn,2*and the "happy" bit *xh,1* are multiplexed together. This gives a sequence of bits *x1, x2, …, x10* where

xk = xh,1 k=1

xk = xrsn,4-k k=2,3

xk = xtfci,11-k k=4,5,…,10

### 4.9.4 Channel coding for E‑DPCCH

Channel coding of the E‑DPCCH is done using a sub-code of the second order Reed-Muller code. Coding is applied to the output *x1*, *x2*, ..., *x10* from the E-DPCCH multiplexing, resulting in:

*i*=*0, 1, ..., 29*

The basis sequences are as described in 4.3.3 for *i*=0, 1, ..., 29.

### 4.9.5 Physical channel mapping for E‑DPCCH

The E-DPCCH is described in [2]. The sequence of bits *z0*, *z1*, ..., *z29* output from the E-DPCCH channel coding is mapped to the corresponding E-DPCCH sub frame. The bits are mapped so that they are transmitted over the air in ascending order with respect to *i*. If the E‑DCH TTI is equal to 10 ms the sequence of bits is transmitted in all the E‑DPCCH sub frames of the E‑DPCCH radio frame.

For compressed frames in the uplink and the case when E‑DCH TTI length is 10 ms, the bits mapped to the E‑DPCCH idle slots specified in 4.4.5.3 shall not be transmitted.

## 4.9A Coding for S-E‑DPCCH

The following information related to the transport block transmitted on the secondary stream is transmitted by means of the S-E-DPCCH:

- Retransmission sequence number (RSN): *xrsn,1*, *xrsn,2*

- E-TFCI: *xtfci,1*, *xtfci,2*, ..., *xtfci,7*

- Spare: *xh,1*

### 4.9A.1 Overview

Overall coding chain for S-E-DPCCH follows that of the E-DPCCH described in clause 4.9.1.

### 4.9A.2 S-E‑DPCCH information field mapping

#### 4.9A.2.1 Information field mapping of E‑TFCI

The E‑TFCI mapping for S-E-DPCCH follows that of the E-DPCCH described in clause 4.9.2.1.

#### 4.9A.2.2 Information field mapping of retransmission sequence number

The RSN mapping for S-E-DPCCH follows that of the E-DPCCH described in clause 4.9.2.2.

#### 4.9A.2.3 Information field mapping of the Spare bit

This bit is fixed to ''0’ in this release of the specifications.

### 4.9A.3 Multiplexing of S-E‑DPCCH information

The S-E-DPCCH multiplexing follows that of the E-DPCCH multiplexing described in clause 4.9.3.

### 4.9A.4 Channel coding for S-E‑DPCCH

Channel coding for S-E-DPCCH follows the channel coding for E-DPCCH described in clause 4.9.4.

### 4.9A.5 Physical channel mapping for S-E‑DPCCH

Physical channel mapping for S-E-DPCCH follows the physical channel mapping for E-DPCCH described in clause 4.9.5.

## 4.10 Coding for E‑AGCH

The following information is transmitted by means of the absolute grant channel (E‑AGCH):

- Absolute Grant Value: *xagv,1, xagv,2, …, xagv,5*

- Absolute Grant Scope: *xags,1*

### 4.10.1 Overview

Figure 24 below illustrates the overall coding chain for the E‑AGCH.



Figure 24: Coding for E‑AGCH

### 4.10.1A E-AGCH information field mapping

#### 4.10.1A.1Information field mapping of the Absolute Grant Value

The Absolute Grant Value information is specified in Table 16B and Table 16.B.1. The values are mapped such that *xagv,1* corresponds to the MSB of the index.

Based on higher layer signalling, either Table 16B or Table 16.B.1 is selected.

Table 16B: Mapping of Absolute Grant Value

|  |  |
| --- | --- |
| Absolute Grant Value | Index |
| (168/15)2x6 | 31 |
| (150/15)2x6 | 30 |
| (168/15)2x4 | 29 |
| (150/15)2x4 | 28 |
| (134/15)2x4 | 27 |
| (119/15)2x4 | 26 |
| (150/15)2x2 | 25 |
| (95/15)2x4 | 24 |
| (168/15)2 | 23 |
| (150/15)2 | 22 |
| (134/15)2 | 21 |
| (119/15)2 | 20 |
| (106/15)2 | 19 |
| (95/15)2 | 18 |
| (84/15)2 | 17 |
| (75/15)2 | 16 |
| (67/15)2 | 15 |
| (60/15)2 | 14 |
| (53/15)2 | 13 |
| (47/15)2 | 12 |
| (42/15)2 | 11 |
| (38/15)2 | 10 |
| (34/15)2 | 9 |
| (30/15)2 | 8 |
| (27/15)2 | 7 |
| (24/15)2 | 6 |
| (19/15)2 | 5 |
| (15/15)2 | 4 |
| (11/15)2 | 3 |
| (7/15)2 | 2 |
| ZERO\_GRANT\* | 1 |
| INACTIVE\* | 0 |

NOTE \*: These values are specified in [16].

Table 16B.1: Alternative Mapping of Absolute Grant Value

|  |  |
| --- | --- |
| Absolute Grant Value | Index |
| (377/15)2x4 | 31 |
| (237/15)2x6 | 30 |
| (168/15)2\*6 | 29 |
| (150/15)2\*6 | 28 |
| (168/15)2\*4 | 27 |
| (150/15)2x4 | 26 |
| (134/15)2x4 | 25 |
| (119/15)2x4 | 24 |
| (150/15)2x2 | 23 |
| (95/15)2x4 | 22 |
| (168/15)2 | 21 |
| (150/15)2 | 20 |
| (134/15)2 | 19 |
| (119/15)2 | 18 |
| (106/15)2 | 17 |
| (95/15)2 | 16 |
| (84/15)2 | 15 |
| (75/15)2 | 14 |
| (67/15)2 | 13 |
| (60/15)2 | 12 |
| (53/15)2 | 11 |
| (47/15)2 | 10 |
| (42/15)2 | 9 |
| (38/15)2 | 8 |
| (34/15)2 | 7 |
| (30/15)2 | 6 |
| (27/15)2 | 5 |
| (24/15)2 | 4 |
| (19/15)2 | 3 |
| (15/15)2 | 2 |
| ZERO\_GRANT\* | 1 |
| INACTIVE\* | 0 |

NOTE \*: These values are specified in [16].

#### 4.10.1A.2 Information field mapping of the Absolute Grant Scope

The value of *xags,1* is set as specified in Table 16C.

Table 16C: Mapping of Absolute Grant Scope

|  |  |
| --- | --- |
| Absolute Grant Scope | *xags,1* |
| "Per HARQ process" | 1 |
| "All HARQ processes" | 0 |

### 4.10.1B Multiplexing of E-AGCH information

The Absolute Grant Value information *xagv,1, xagv,2, …, xagv,5* and the Absolute Grant Scope information *xags,1* are multiplexed together. This gives a sequence of bits *xag,1*, *xag,2*, ..., *xag, 6* where

*xag,k = xagv,k* *k=1,2,…,5*

*xag,k = xags,7-k k=6*

### 4.10.2 CRC attachment for E‑AGCH

The E-RNTI is the E‑DCH Radio Network Identifier defined in [13]. It is mapped such that *xid,1* corresponds to the MSB.

From the sequence of bits *xag,1*, *xag,2*, ..., *xag,6* a 16 bit CRC is calculated according to clause 4.2.1.1. That gives the sequence of bits *c1*, *c2*, ..., *c16* where

*k=1,2,…,16*

This sequence of bits is then masked with *xid,1, xid,2, ...,xid,16* and appended to the sequence of bits *xag,1*, *xag,2*, ..., *xag,6* to form the sequence of bits *y1*, *y2*, ..., *y22* where

*yi=xag,i i=1,2, ...,6*

*yi=(ci-6 + xid,i-6) mod 2 i= 7, ..., 22*

### 4.10.3 Channel coding for E‑AGCH

Rate 1/3 convolutional coding, as described in Clause 4.2.3.1 is applied to the sequence of bits *y1*, *y2*, …, *y22*, resulting in the sequence of bits *z1*, *z2*, …, *z90*.

### 4.10.4 Rate matching for E‑AGCH

From the input sequence z1, z2, …, z90 the bits z1, z2, z5, z6, z7, z11, z12, z14, z15, z17, z23, z24, z31, z37, z44, z47, z61, z63, z64, z71, z72, z75, z77, z80, z83, z84, z85, z87, z88, z90 are punctured to obtain the output sequence r1, r2, …, r60.

### 4.10.5 Physical channel mapping for E‑AGCH

The E‑AGCH sub frame is described in [2]. The sequence of bits *r1*, *r2*, …, *r60*  is mapped to the corresponding E‑AGCH sub frame. The bits *rk* are mapped so that they are transmitted over the air in ascending order with respect to k. If the E‑DCH TTI is equal to 10 ms the same sequence of bits is transmitted in all the E‑AGCH sub frames of the E‑AGCH radio frame.

## 4.10A Coding for E-ROCH

The following information is transmitted by means of the E-DCH rank and offset channel (E-ROCH):

- S-ETFC Offset: *xseo,1, xseo,2, …, xseo,5*

- Rank Indication: *xri,1*

### 4.10A.1 Overview

The E-ROCH coding chain uses the same coding chain as the E-AGCH. Figure 24B below illustrates the overall coding chain for the E-ROCH.



Figure 24B: Coding for E-ROCH

### 4.10A.2 E-ROCH information field mapping

#### 4.10A.2.1Information field mapping of the S-ETFC Offset

The S-ETFC Offset information is specified in Table 16D. The values are mapped such that *xseo,1* corresponds to the MSB of the index.

Table 16D: Mapping of S-ETFC Offset value

|  |  |
| --- | --- |
| **S-ETFC Offset Value** | **Index** |
| 60/30 | 31 |
| 55/30 | 30 |
| 50/30 | 29 |
| 45/30 | 28 |
| 40/30 | 27 |
| 35/30 | 26 |
| 30/30 | 25 |
| 28/30 | 24 |
| 26/30 | 23 |
| 24/30 | 22 |
| 22/30 | 21 |
| 21/30 | 20 |
| 20/30 | 19 |
| 19/30 | 18 |
| 18/30 | 17 |
| 17/30 | 16 |
| 16/30 | 15 |
| 15/30 | 14 |
| 14/30 | 13 |
| 13/30 | 12 |
| 12/30 | 11 |
| 11/30 | 10 |
| 10/30 | 9 |
| 9/30 | 8 |
| 8/30 | 7 |
| 7/30 | 6 |
| 6/30 | 5 |
| 5/30 | 4 |
| 4/30 | 3 |
| 3/30 | 2 |
| 2/30 | 1 |
| 1/30 | 0 |

#### 4.10A.2.2 Information field mapping of the Rank Indication

The value of *xri,1* is set as specified in Table 16E.

Table 16E: Mapping of Rank Indication

|  |  |
| --- | --- |
| Rank Indication | *xri,1* |
| "Rank 2 allowed" | 1 |
| "Rank 2 not allowed" | 0 |

### 4.10A.3 Multiplexing of E-ROCH information

The S-ETFC Offset information *xseo,1, xseo,2, …, xseo,5* and the Rank Indication information *xri,1* are multiplexed together. This gives a sequence of bits *xro,1*, *xro,2*, ..., *xro, 6* where

*xro,k = xseo,k* *k=1,2,…,5*

*xro,6 = xri,1*

### 4.10A.4 CRC attachment for E-ROCH

The S-E-RNTI is the E‑DCH Radio Network Identifier specific to E-ROCH defined in [13]. It is mapped such that *xid,1* corresponds to the MSB.

From the sequence of bits *xro,1*, *xro,2*, ..., *xro,6* a 16 bit CRC is calculated according to clause 4.2.1.1. That gives the sequence of bits *c1*, *c2*, ..., *c16* where

*k=1,2,…,16*

This sequence of bits is then masked with *xid,1, xid,2, ...,xid,16* and appended to the sequence of bits *xro,1*, *xro,2*, ..., *xro,6* to form the sequence of bits *y1*, *y2*, ..., *y22* where

*yi=xro,i i=1,2, ...,6*

*yi=(ci-6 + xid,i-6) mod 2 i= 7, ..., 22*

### 4.10A.5 Channel coding for E-ROCH

Rate 1/3 convolutional coding, as described in Clause 4.2.3.1 is applied to the sequence of bits *y1*, *y2*, …, *y22*, resulting in the sequence of bits *z1*, *z2*, …, *z90*.

### 4.10A.6 Rate matching for E-ROCH

From the input sequence z1, z2, …, z90 the bits z1, z2, z5, z6, z7, z11, z12, z14, z15, z17, z23, z24, z31, z37, z44, z47, z61, z63, z64, z71, z72, z75, z77, z80, z83, z84, z85, z87, z88, z90 are punctured to obtain the output sequence r1, r2, …, r60.

### 4.10A.7 Physical channel mapping for E-ROCH

The E-ROCH sub frame is described in [2]. The sequence of bits *r1*, *r2*, …, *r60*  is mapped to the corresponding E-ROCH sub frame. The bits *rk* are mapped so that they are transmitted over the air in ascending order with respect to k.

## 4.11 Mapping for E‑RGCH Relative Grant

### 4.11.1 Overview

The relative grant is transmitted on the E-RGCH as described in [2].

### 4.11.2 Relative Grant mapping

The relative grant (RG) command is mapped to the relative grant value as described in the table below.

Table 17: Mapping of RG value

|  |  |  |
| --- | --- | --- |
| Command | RG Value (serving E-DCH RLS) | RG Value (other radio links) |
| UP | +1 | not allowed |
| HOLD | 0 | 0 |
| DOWN | -1 | -1 |

## 4.12 Mapping for E-HICH ACK/NACK

### 4.12.1 Overview

The ACK/NACK is transmitted on the E‑HICH as described in [2].

### 4.12.2 ACK/NACK mapping

The ACK/NACK command is mapped to the HARQ acknowledgement indicator as described in the table below.

Table 18: Mapping of HARQ Acknowledgement

|  |  |
| --- | --- |
| Command | HARQ acknowledgement indicator |
| ACK | +1 |
| NACK (RLSs not containing the serving E-DCH cell) | 0 |
| NACK (RLS containing the serving E-DCH cell) | -1 |

Annex A (informative):  
Blind transport format detection

# A.1 Blind transport format detection using fixed positions

## A.1.1 Blind transport format detection using received power ratio

For the dual transport format case (the possible data rates are 0 and full rate, and CRC is only transmitted for full rate), blind transport format detection using received power ratio can be used.

The transport format detection is then done using average received power ratio of DPDCH to DPCCH. Define the following:

*- Pc:* Received power per bit of DPCCH calculated from all pilot and TPC bits per slot over a radio frame;

*- Pd:* Received power per bit of DPDCH calculated from *X* bits per slot over a radio frame;

*- X:* the number of DPDCH bits per slot when transport format corresponds to full rate;

*- T:* Threshold of average received power ratio of DPDCH to DPCCH for transport format detection.

The decision rule can then be formulated as:

If *Pd/Pc >T* then:

- full rate transport format detected;

else

- zero rate transport format detected.

## A.1.2 Blind transport format detection using CRC

For the multiple transport format case (the possible data rates are 0, …, (full rate)/r, …, full rate, and CRC is transmitted for all transport formats), blind transport format detection using CRC can be used.

At the transmitter, the data stream with variable number of bits from higher layers is block-encoded using a cyclic redundancy check (CRC) and then convolutionally encoded. CRC parity bits are attached just after the data stream with variable number of bits as shown in figure A.1.

The receiver knows only the possible transport formats (or the possible end bit position {nend}) by Layer-3 negotiation. The receiver performs Viterbi-decoding on the soft decision sample sequence. The correct trellis path of the Viterbi-decoder ends at the zero state at the correct end bit position.

The blind transport format detection method using CRC traces back the surviving trellis path ending at the zero state (hypothetical trellis path) at each possible end bit position to recover the data sequence. For each recovered data sequence error-detection is performed by checking the CRC, and if there is no error, the recovered sequence is declared to be correct.

The following variable is defined:

s(nend) = - 10 log ( (a0(nend) – amin(nend) ) / (amax(nend)-amin(nend) ) ) [dB] (Eq. 1)

where amax(nend) and amin(nend) are the maximum and minimum path-metric values among all survivors at end bit position nend, and a0(nend) is the path-metric value at zero state.

In order to reduce the probability of false detection (this happens if the selected path is wrong but the CRC misses the error detection), a path selection threshold D is introduced. The threshold D determines whether the hypothetical trellis path connected to the zero state should be traced back or not at each end bit position nend. If the hypothetical trellis path connected to the zero state that satisfies:

s(nend)  D (Eq. 2)

is found, the path is traced back to recover the frame data, where D is the path selection threshold and a design parameter.

If more than one end bit positions satisfying Eq. 2 is found, the end bit position which has minimum value of s(nend) is declared to be correct. If no path satisfying Eq. 2 is found even after all possible end bit positions have been exhausted, the received frame data is declared to be in error.

Figure A-2 shows the procedure of blind transport format detection using CRC.



Figure A.1: An example of data with variable number of bits.  
Four possible transport formats, and transmitted end bit position nend = 3



Figure A.2: Basic processing flow of blind transport format detection

# A.2 Blind transport format detection using pseudo-flexible positions

The blind detection procedure for each TTI begins by assuming a hypothesis for all values of *RMi* of Equation (1) of subclause 4.2.7, based on a corresponding hypothesis regarding whether certain TrCHs are delivering a transport block during that TTI. Based on this hypothesis, the blind detection then proceeds similar to blind transport format detection with fixed positions. If this hypothesis results in a successful detection of at least one transport format based on a passing CRC, the assumed hypothesis is considered to be validated to be correct. If there is no passing CRC, this process is repeated with another hypothesis, until all hypotheses are exhausted.

Annex B (informative):  
Compressed mode idle lengths

The tables B.1-B.3 show the resulting idle lengths for different transmission gap lengths, UL/DL modes and DL frame types when DPCCH/DPDCH are used in the uplink and DPCH in the downlink. The idle lengths given are calculated purely from the slot and frame structures and the UL/DL offset. They do not contain margins for e.g. synthesizer switching.

# B.1 Idle lengths for DL, UL and DL+UL compressed mode for DPCH

Table B.1: Parameters for DL compressed mode

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| TGL | DL Frame Type | Spreading Factor | Idle length [ms] | Transmission time  Reduction method | Idle frame  Combining |
| 3 | A | 512 – 4 | 1.73 – 1.99 | Spreading factor division by 2 or  Higher layer scheduling | (S)  (D) =(1,2) or (2,1) |
| B | 1.60 – 1.86 |
| 4 | A | 2.40 – 2.66 | (S)  (D) =(1,3), (2,2) or (3,1) |
| B | 2.27 – 2.53 |
| 5 | A | 3.07 – 3.33 | (S)  (D) = (1,4), (2,3), (3, 2) or (4,1) |
| B | 2.93 – 3.19 |
| 7 | A | 4.40 – 4.66 | (S)  (D)=(1,6), (2,5), (3,4), (4,3), (5,2) or (6,1) |
| B | 4.27 – 4.53 |
| 10 | A | 6.40 – 6.66 | (D)=(3,7), (4,6), (5,5), (6,4) or (7,3) |
| B | 6.27 – 6.53 |
| 14 | A | 9.07 – 9.33 | (D) =(7,7) |
| B | 8.93 – 9.19 |

Table B.2: Parameters for UL compressed mode

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| TGL | Spreading Factor | Idle length [ms] | Transmission time  Reduction method | Idle frame  Combining |
| 3 | 256 – 4 | 2.00 | Spreading factor division by 2 or  Higher layer scheduling | (S)  (D) =(1,2) or (2,1) |
| 4 | 2.67 | (S)  (D) =(1,3), (2,2) or (3,1) |
| 5 | 3.33 | (S)  (D) = (1,4), (2,3), (3, 2) or (4,1) |
| 7 | 4.67 | (S)  (D)=(1,6), (2,5), (3,4), (4,3), (5,2) or (6,1) |
| 10 | 6.67 | (D)=(3,7), (4,6), (5,5), (6,4) or (7,3) |
| 14 | 9.33 | (D) =(7,7) |

Table B.3: Parameters for combined UL/DL compressed mode

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| TGL | DL Frame Type | Spreading Factor | Idle length [ms] | Transmission time  Reduction method | Idle frame  Combining |
| 3 | A or B | DL: 512 – 4  UL:  256 – 4 | 1.47 – 1.73 | Spreading factor division by 2 or  Higher layer scheduling | (S)  (D) =(1,2) or (2,1) |
| 4 | 2.13 – 2.39 | (S)  (D) =(1,3), (2,2) or (3,1) |
| 5 | 2.80 – 3.06 | (S)  (D) = (1,4), (2,3), (3, 2) or (4,1) |
| 7 | 4.13 – 4.39 | (S)  (D)=(1,6), (2,5), (3,4), (4,3), (5,2) or (6,1) |
| 10 | 6.13 – 6.39 | (D)=(3,7), (4,6), (5,5), (6,4) or (7,3) |
| 14 | 8.80 – 9.06 | (D) =(7,7) |

(S): Single-frame method as shown in figure 14 (1).

(D): Double-frame method as shown in figure 14 (2). (x,y) indicates x: the number of idle slots in the first frame, y: the number of idle slots in the second frame.

NOTE: Compressed mode by spreading factor reduction is not supported when SF=4 is used in normal mode

Annex C (informative):  
Change history

| Change history | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Date** | **TSG #** | **TSG Doc.** | **CR** | **Rev** | **Subject/Comment** | **Old** | **New** |
|  | RP\_05 | RP-99588 | - |  | Approved at TSG RAN #5 and placed under Change Control | - | 3.0.0 |
| 14/01/00 | RP\_06 | RP-99680 | 001 | 3 | Correction of rate matching parameters for repetition after 1st unterleaving in 25.212 | 3.0.0 | 3.1.0 |
| 14/01/00 | RP\_06 | RP-99680 | 004 | - | Changing the initial offset value for convolutional code rate matching | 3.0.0 | 3.1.0 |
| 14/01/00 | RP\_06 | RP-99681 | 005 | 1 | Introduction of compressed mode by higher layer scheduling | 3.0.0 | 3.1.0 |
| 14/01/00 | RP\_06 | RP-99679 | 008 | - | Editorial corrections to TS 25.212 | 3.0.0 | 3.1.0 |
| 14/01/00 | RP\_06 | RP-99680 | 009 | - | Removal of SFN multiplexing | 3.0.0 | 3.1.0 |
| 14/01/00 | RP\_06 | RP-99680 | 010 | 1 | Clarification of bit separation and collection | 3.0.0 | 3.1.0 |
| 14/01/00 | RP\_06 | RP-99680 | 011 | 2 | Connection between TTI and CFN | 3.0.0 | 3.1.0 |
| 14/01/00 | RP\_06 | RP-99680 | 012 | 2 | Zero length transport blocks | 3.0.0 | 3.1.0 |
| 14/01/00 | RP\_06 | RP-99679 | 014 | - | Update of channel coding sections | 3.0.0 | 3.1.0 |
| 14/01/00 | RP\_06 | RP-99680 | 016 | - | Removal of TrCH restriction in DSCH CCTrCH | 3.0.0 | 3.1.0 |
| 14/01/00 | RP\_06 | RP-99681 | 017 | - | 20 ms RACH message length | 3.0.0 | 3.1.0 |
| 14/01/00 | RP\_06 | RP-99680 | 018 | - | Minimum SF in UL | 3.0.0 | 3.1.0 |
| 14/01/00 | RP\_06 | RP-99680 | 024 | - | Rate matching parameter determination in DL and fixed positions | 3.0.0 | 3.1.0 |
| 14/01/00 | RP\_06 | RP-99680 | 026 | 1 | Corrections to TS 25.212 | 3.0.0 | 3.1.0 |
| 14/01/00 | RP\_06 | RP-99679 | 027 | - | Modification of BTFD description in 25.212 Annex | 3.0.0 | 3.1.0 |
| 14/01/00 | RP\_06 | RP-99681 | 028 | - | TFCI coding and mapping including compressed mode | 3.0.0 | 3.1.0 |
| 14/01/00 | - | - | - |  | Change history was added by the editor | 3.1.0 | 3.1.1 |
| 31/03/00 | RP\_07 | RP-000061 | 025 | 2 | CR for parity bit attachment to 0 bit transport block | 3.1.1 | 3.2.0 |
| 31/03/00 | RP\_07 | RP-000061 | 029 | 1 | Limitations of blind transport format detection | 3.1.1 | 3.2.0 |
| 31/03/00 | RP\_07 | RP-000061 | 034 | 1 | Clarification of fixed position rate matching | 3.1.1 | 3.2.0 |
| 31/03/00 | RP\_07 | RP-000061 | 035 | 1 | Clarification of DL compressed mode | 3.1.1 | 3.2.0 |
| 31/03/00 | RP\_07 | RP-000061 | 036 | - | Reconfiguration of TFCS | 3.1.1 | 3.2.0 |
| 31/03/00 | RP\_07 | RP-000061 | 037 | 1 | Removal of fixed gap position in 25.212 | 3.1.1 | 3.2.0 |
| 31/03/00 | RP\_07 | RP-000061 | 038 | 2 | Definition clarification for TS 25.212 | 3.1.1 | 3.2.0 |
| 31/03/00 | RP\_07 | RP-000061 | 039 | 1 | Clarification on TFCI coding input | 3.1.1 | 3.2.0 |
| 31/03/00 | RP\_07 | RP-000061 | 041 | 2 | Correction of UL compressed mode by higher layer scheduling | 3.1.1 | 3.2.0 |
| 31/03/00 | RP\_07 | RP-000061 | 042 | 5 | Downlink Compressed Mode by puncturing | 3.1.1 | 3.2.0 |
| 31/03/00 | RP\_07 | RP-000061 | 044 | - | Modification of Turbo code internal interleaver | 3.1.1 | 3.2.0 |
| 31/03/00 | RP\_07 | RP-000061 | 045 | - | Editorial corrections | 3.1.1 | 3.2.0 |
| 31/03/00 | RP\_07 | RP-000061 | 046 | - | SF/2 method: DTX insertion after 2nd interleaver | 3.1.1 | 3.2.0 |
| 31/03/00 | RP\_07 | RP-000061 | 047 | 1 | TFCI coding for FDD | 3.1.1 | 3.2.0 |
| 31/03/00 | RP\_07 | RP-000061 | 048 | - | Mapping of TFCI in downlink compressed mode | 3.1.1 | 3.2.0 |
| 31/03/00 | RP\_07 | RP-000061 | 049 | - | Editorial changes to Annex A | 3.1.1 | 3.2.0 |
| 31/03/00 | RP\_07 | RP-000061 | 050 | - | Removal of rate matching attribute setting for RACH | 3.1.1 | 3.2.0 |
| 31/03/00 | RP\_07 | RP-000061 | 052 | - | Padding Function for Turbo coding of small blocks | 3.1.1 | 3.2.0 |
| 31/03/00 | RP\_07 | RP-000061 | 055 | 2 | Clarifications relating to DSCH | 3.1.1 | 3.2.0 |
| 31/03/00 | RP\_07 | RP-000061 | 056 | - | Editorial modification of uplink shifting parameter calculation for turbo code puncturing | 3.1.1 | 3.2.0 |
| 31/03/00 | RP\_07 | RP-000062 | 059 | 1 | Revision: Editorial correction to the calculation of Rate Matching parameters | 3.1.1 | 3.2.0 |
| 31/03/00 | RP\_07 | RP-000062 | 060 | 1 | Editorial changes of channel coding section | 3.1.1 | 3.2.0 |
| 31/03/00 | RP\_07 | RP-000062 | 061 | - | Removal of DL compressed mode by higher layer scheduling with fixed positions | 3.1.1 | 3.2.0 |
| 26/06/00 | RP\_08 | RP-000266 | 066 | 1 | Clause 4.4.5 and table 9 is moved to informative annex | 3.2.0 | 3.3.0 |
| 26/06/00 | RP\_08 | RP-000266 | 068 | - | Editorial modifications of 25.212 | 3.2.0 | 3.3.0 |
| 26/06/00 | RP\_08 | RP-000266 | 069 | - | Removal of BTFD for flexible positions in Release 99 | 3.2.0 | 3.3.0 |
| 26/06/00 | RP\_08 | RP-000266 | 070 | 1 | Editorial modifications | 3.2.0 | 3.3.0 |
| 26/06/00 | RP\_08 | RP-000266 | 071 | 1 | Corrections and editorial modifications of 25.212 for 2nd insertion of DTX bits for CM | 3.2.0 | 3.3.0 |
| 26/06/00 | RP\_08 | RP-000266 | 072 | 4 | Corrections to 25.212 (Rate Matching, p-bit insertion, PhCH segmentation) | 3.2.0 | 3.3.0 |
| 26/06/00 | RP\_08 | RP-000266 | 073 | - | Editorial correction in 25.212 coding/multiplexing | 3.2.0 | 3.3.0 |
| 26/06/00 | RP\_08 | RP-000266 | 074 | 2 | Bit separation of the Turbo encoded data | 3.2.0 | 3.3.0 |
| 26/06/00 | RP\_08 | RP-000266 | 076 | 1 | Revision of code block segmentation description | 3.2.0 | 3.3.0 |
| 26/06/00 | RP\_08 | RP-000266 | 077 | - | Clarifications for TFCI coding | 3.2.0 | 3.3.0 |
| 26/06/00 | RP\_08 | RP-000266 | 078 | 2 | Clarifying the rate matching parameter setting for the RACH and BCH | 3.2.0 | 3.3.0 |
| 26/06/00 | RP\_08 | RP-000266 | 080 | - | Clarification on BTFD utilisation (single CCTrCH) | 3.2.0 | 3.3.0 |
| 26/06/00 | RP\_08 | RP-000266 | 081 | - | Correction of order of checking TFC during flexible position RM parameter determination | 3.2.0 | 3.3.0 |
| 26/06/00 | RP\_08 | RP-000266 | 082 | - | Editorial corrections in channel coding section | 3.2.0 | 3.3.0 |
| 26/06/00 | RP\_08 | RP-000266 | 083 | - | Correction for bit separation and bit collection | 3.2.0 | 3.3.0 |
| 26/06/00 | RP\_08 | RP-000266 | 084 | 1 | Correction on the spreading factor selection for the RACH | 3.2.0 | 3.3.0 |
| 23/09/00 | RP\_09 | RP-000341 | 079 | - | Clarification of compressed mode terminology | 3.3.0 | 3.4.0 |
| 23/09/00 | RP\_09 | RP-000341 | 085 | 1 | Editorial corrections in Turbo code internal interleaver section | 3.3.0 | 3.4.0 |
| 23/09/00 | RP\_09 | RP-000341 | 086 | 1 | Clarification on DL slot format for compressed mode by SF/2 | 3.3.0 | 3.4.0 |
| 23/09/00 | RP\_09 | RP-000341 | 087 | - | Corrections | 3.3.0 | 3.4.0 |
| 23/09/00 | RP\_09 | RP-000341 | 088 | 1 | Clarifications to TS 25.212 | 3.3.0 | 3.4.0 |
| 23/09/00 | RP\_09 | RP-000341 | 089 | - | Correction regarding DSCH | 3.3.0 | 3.4.0 |
| 23/09/00 | RP\_09 | RP-000341 | 090 | - | Correction regarding CPCH | 3.3.0 | 3.4.0 |
| 23/09/00 | RP\_09 | RP-000341 | 092 | 1 | Bit separation and collection for rate matching | 3.3.0 | 3.4.0 |
| 23/09/00 | RP\_09 | RP-000341 | 093 | - | Puncturing Limit definition in WG1 specification | 3.3.0 | 3.4.0 |
| 15/12/00 | RP\_10 | RP-000538 | 094 | 2 | Correction of BTFD limitations | 3.4.0 | 3.5.0 |
| 15/12/00 | RP\_10 | RP-000538 | 096 | - | Compressed mode by puncturing | 3.4.0 | 3.5.0 |
| 15/12/00 | RP\_10 | RP-000538 | 097 | - | Clarification on the Ci formula | 3.4.0 | 3.5.0 |
| 15/12/00 | RP\_10 | RP-000538 | 099 | - | Editorial modification in RM section | 3.4.0 | 3.5.0 |
| 15/12/00 | RP\_10 | RP-000538 | 100 | 1 | Editorial corrections in TS 25.212 | 3.4.0 | 3.5.0 |
| 15/12/00 | RP\_10 | RP-000538 | 101 | - | Correction to code block segmentation | 3.4.0 | 3.5.0 |
| 16/03/01 | RP\_11 | - | - | - | Approved as Release 4 specification (v4.0.0) at TSG RAN #11 | 3.5.0 | 4.0.0 |
| 15/06/01 | RP\_12 | RP-010332 | 106 | - | Correction of compressed mode by puncturing | 4.0.0 | 4.1.0 |
| 15/06/01 | RP\_12 | RP-010332 | 108 | 1 | Dual transport format detection | 4.0.0 | 4.1.0 |
| 15/06/01 | RP\_12 | RP-010332 | 112 | 1 | Correction for downlink rate matching for the DSCH | 4.0.0 | 4.1.0 |
| 21/09/01 | RP\_13 | RP-010519 | 115 | - | Correction of PDSCH spreading factor signalling | 4.1.0 | 4.2.0 |
| 14/12/01 | RP\_14 | RP-010737 | 118 | - | Clarification of compressed mode | 4.2.0 | 4.3.0 |
| 14/12/01 | RP\_14 | RP-010737 | 122 | - | Support of multiple CCTrChs of dedicated type | 4.2.0 | 4.3.0 |
| 08/03/02 | RP\_15 | RP-020231 | 128 | 2 | Removal of channel coding option “no coding” for FDD | 4.3.0 | 4.4.0 |
| 08/03/02 | RP\_15 | RP-020054 | 123 | 4 | Inclusion of flexible hard split mode TFCI operation | 4.3.0 | 5.0.0 |
| 08/03/02 | RP\_15 | RP-020058 | 126 | 1 | Changes to 25.212 for HSDPA work item | 4.3.0 | 5.0.0 |
| 07/06/02 | RP\_16 | RP-020308 | 136 | - | Downlink bit mapping | 5.0.0 | 5.1.0 |
| 07/06/02 | RP\_16 | RP-020316 | 130 | 5 | Correction of Errata noted by RAN1 delegates | 5.0.0 | 5.1.0 |
| 07/06/02 | RP\_16 | RP-020316 | 131 | 2 | Removal of inconsistencies and ambiguities in the HARQ description | 5.0.0 | 5.1.0 |
| 07/06/02 | RP\_16 | RP-020316 | 132 | - | Rate Matching and Channel Coding for HS-SCCH | 5.0.0 | 5.1.0 |
| 07/06/02 | RP\_16 | RP-020316 | 137 | - | Basis sequences for HS-DPCCH Channel Quality information code | 5.0.0 | 5.1.0 |
| 07/06/02 | RP\_16 | RP-020316 | 145 | 5 | UE specific masking for HS-SCCH part1 | 5.0.0 | 5.1.0 |
| 14/09/02 | RP\_17 | RP-020582 | 141 | 1 | Bit scrambling for HS-DSCH | 5.1.0 | 5.2.0 |
| 15/09/02 | RP\_17 | RP-020582 | 148 |  | Physical channel mapping for HS-DPCCH | 5.1.0 | 5.2.0 |
| 15/09/02 | RP\_17 | RP-020582 | 149 |  | HARQ bit collection | 5.1.0 | 5.2.0 |
| 15/09/02 | RP\_17 | RP-020582 | 150 | 1 | Coding for HS-SCCH | 5.1.0 | 5.2.0 |
| 15/09/02 | RP\_17 | RP-020582 | 151 |  | Correction to UE specific masking for HS-SCCH part1 | 5.1.0 | 5.2.0 |
| 15/09/02 | RP\_17 | RP-020568 | 155 | 2 | Clarification of the definition of layer 1 transport channel numbers | 5.1.0 | 5.2.0 |
| 15/09/02 | RP\_17 | RP-020573 | 157 |  | Numbering Corrections | 5.1.0 | 5.2.0 |
| 15/09/02 | RP\_17 | RP-020645 | 158 | 1 | Specification of H-RNTI to UE identity mapping | 5.1.0 | 5.2.0 |
| 20/12/02 | RP\_18 | RP-020846 | 163 | - | Correction of CQI index to bit mapping | 5.2.0 | 5.3.0 |
| 20/12/02 | RP\_18 | RP-020846 | 164 | - | Correction of mapping of HARQ-ACK | 5.2.0 | 5.3.0 |
| 26/03/03 | RP\_19 | RP-030134 | 165 | 1 | Correction of CQI index to bit mapping | 5.3.0 | 5.4.0 |
| 26/03/03 | RP\_19 | RP-030134 | 166 | 3 | Correction of bit scrambling of HS-DSCH | 5.3.0 | 5.4.0 |
| 26/03/03 | RP\_19 | RP-030134 |  |  | Correction of subscript for modulation scheme information | 5.3.0 | 5.4.0 |
| 23/06/03 | RP\_20 | RP-030272 | 172 | 1 | Clarification of TPC and Pilot transmission with STTD in compressed mode | 5.4.0 | 5.5.0 |
| 23/06/03 | RP\_20 | RP-030272 | 173 | 2 | Correction on the flexible TFCI coding in the DSCH hard split mode for Rel5 | 5.4.0 | 5.5.0 |
| 21/09/03 | RP\_21 | RP-030456 | 178 | 4 | Clarification on Single Transport Format Detection | 5.5.0 | 5.6.0 |
| 21/09/03 | RP\_21 | RP-030456 | 179 | - | Correction on table number in first interleave description | 5.5.0 | 5.6.0 |
| 21/09/03 | RP\_21 | RP-030456 | 180 | 3 | Broadening the conditions that require UEs to perform BTFD for the case of HS-DSCH reception | 5.5.0 | 5.6.0 |
| 06/01/04 | RP\_22 | RP-030647 | 183 | - | Clarification of the CRC attachment procedure for HS-SCCH | 5.6.0 | 5.7.0 |
| 06/01/04 | RP\_22 | RP-030647 | 184 | 1 | Correction of UE identity notation | 5.6.0 | 5.7.0 |
| 06/01/04 | RP\_22 | RP-030644 | 185 | - | HARQ process identifier mapping | 5.6.0 | 5.7.0 |
| 06/01/04 | RP\_22 | RP-030712 | 186 |  | Alignment of terminology across 3GPP documentation | 5.6.0 | 5.7.0 |
| 13/01/04 | RP\_22 | - | - | - | Created for M.1457 update | 5.7.0 | 6.0.0 |
| 23/03/04 | RP\_23 | RP-040085 | 187 | 1 | CCTrCH definition extension to HS-DSCH | 6.0.0 | 6.1.0 |
| 09/06/04 | RP\_24 | RP-040230 | 191 | 1 | Clarification of Channelization Code-Set Mapping | 6.1.0 | 6.2.0 |
| 13/12/04 | RP\_26 | RP-040446 | 192 | 2 | Introduction of MBMS Soft Combining | 6.2.0 | 6.3.0 |
| 13/12/04 | RP\_26 | RP-040527 | 195 | - | Preamble and Postamble to reduce HS-DPCCH transmit power | 6.2.0 | 6.3.0 |
| 13/12/04 | RP\_26 | RP-040449 | 196 | 2 | Introduction of E-DCH | 6.2.0 | 6.3.0 |
| 14/03/05 | RP\_27 | RP-050088 | 193 | 1 | Introduction of F-DPCH | 6.3.0 | 6.4.0 |
| 14/03/05 | RP\_27 | RP-050044 | 198 | 1 | PLnon-max and PLmax | 6.3.0 | 6.4.0 |
| 14/03/05 | RP\_27 | RP-050045 | 199 | - | HARQ bit collection for E-DCH | 6.3.0 | 6.4.0 |
| 16/06/05 | RP\_28 | RP-050241 | 203 | - | Correction of HSDPA Bit Separation | 6.4.0 | 6.5.0 |
| 16/06/05 | RP\_28 | RP-050252 | 204 | 2 | E-DCH Corrections | 6.4.0 | 6.5.0 |
| 16/06/05 | RP\_28 | RP-050252 | 205 | 1 | Compressed mode operation for the Enhanced Uplink | 6.4.0 | 6.5.0 |
| 16/06/05 | RP\_28 | RP-050357 | 206 | 1 | E-HICH and E-RGCH serving/non-serving definition clarification | 6.4.0 | 6.5.0 |
| 16/06/05 | RP\_28 | RP-050250 | 208 | 1 | Feature Clean Up: Removal of “CPCH” | 6.4.0 | 6.5.0 |
| 16/06/05 | RP\_28 | RP-050248 | 210 | - | Feature Clean Up: Removal of DSCH (FDD mode) | 6.4.0 | 6.5.0 |
| 16/06/05 | RP\_28 | RP-050243 | 212 | 1 | Feature Clean-Up: Removal of 80 ms TTI for DCH for all other cases but when the UE supports SF512 | 6.4.0 | 6.5.0 |
| 16/06/05 | RP\_28 | RP-050252 | 215 | - | Clarification on E-AGCH bit mapping | 6.4.0 | 6.5.0 |
| 16/06/05 | RP\_28 | RP-050252 | 216 | - | Determination of SF and number of PhCHs considering SF2 | 6.4.0 | 6.5.0 |
| 16/06/05 | RP\_28 | RP-050251 | 217 | 1 | MBMS related corrections | 6.4.0 | 6.5.0 |
| 16/06/05 | RP\_28 | RP-050249 | 218 | 1 | Feature clean up: Removal of the 'compressed mode by puncturing' | 6.4.0 | 6.5.0 |
| 16/06/05 | RP\_28 | RP-050252 | 219 | - | Re-ordering of the E-DPCCH bit mapping | 6.4.0 | 6.5.0 |
| 16/06/05 | RP\_28 | RP-050252 | 220 | - | Coding for E‑AGCH | 6.4.0 | 6.5.0 |
| 26/09/05 | RP\_29 | RP-050450 | 0222 | - | SF max for E-DPDCH | 6.5.0 | 6.6.0 |
| 26/09/05 | RP\_29 | RP-050450 | 0223 | 1 | Compressed mode operation for the Enhanced Uplink | 6.5.0 | 6.6.0 |
| 26/09/05 | RP\_29 | RP-050450 | 0225 | 1 | Absolute grant values | 6.5.0 | 6.6.0 |
| 26/09/05 | RP\_29 | RP-050450 | 0227 | - | Removal of description on RSN setting | 6.5.0 | 6.6.0 |
| 12/12/05 | RP\_30 | RP-050727 | 0228 | - | PLmax alignment over all UE categories | 6.6.0 | 6.7.0 |
| 12/12/05 | RP\_30 | RP-050727 | 0229 | - | Correction of SF when a CCTrCH is mapped onto four E-DPDCHs | 6.6.0 | 6.7.0 |
| 12/12/05 | RP\_30 | RP-050727 | 0231 | 1 | Usage of 2xSF4 with puncturing | 6.6.0 | 6.7.0 |
| 20/03/06 | RP\_31 | - | - | - | Creation of Release 7 specification (v.7.0.0) at RAN#31 | 6.7.0 | 7.0.0 |
| 12/06/06 | RP\_32 | RP-060370 | 0236 | - | Clarification of E-TFCI terminology | 7.0.0 | 7.1.0 |
| 29/09/06 | RP\_33 | RP-060490 | 0240 | - | Correction to the E-DCH HARQ rate matching for compressed mode | 7.1.0 | 7.2.0 |
| 11/12/06 | RP\_34 | RP-060727 | 0244 | 1 | Clarification on the number of physical channels, transmission gap positioning and physical channel mapping for E-DCH in relation to compressed mode | 7.2.0 | 7.3.0 |
| 07/03/07 | RP\_35 | RP-070115 | 0238 | 5 | Support of CPC feature | 7.3.0 | 7.4.0 |
| 07/03/07 | RP\_35 | RP-070114 | 0241 | 4 | Coding of HS-SCCH to support FDD MIMO | 7.3.0 | 7.4.0 |
| 07/03/07 | RP\_35 | RP-070114 | 0242 | 7 | Coding of HS-DPCCH to support operation of FDD MIMO | 7.3.0 | 7.4.0 |
| 07/03/07 | RP\_35 | RP-070116 | 0245 | 4 | Introduction of 64QAM for HSDPA | 7.3.0 | 7.4.0 |
| 30/05/07 | RP\_36 | RP-070387 | 0249 | - | MIMO HS-SCCH rate matching | 7.4.0 | 7.5.0 |
| 30/05/07 | RP\_36 | RP-070387 | 0248 | 1 | Correction to coding of HS-SCCH to support FDD MIMO | 7.4.0 | 7.5.0 |
| 30/05/07 | RP\_36 | RP-070387 | 0251 | 1 | HS-SCCH orders in MIMO mode | 7.4.0 | 7.5.0 |
| 30/05/07 | RP\_36 | RP-070388 | 0246 | 5 | Introduction of 16QAM for HSUPA | 7.4.0 | 7.5.0 |
| 30/05/07 | RP\_36 | RP-070384 | 0247 | 1 | Support for DL only SFN operation for MBMS FDD | 7.4.0 | 7.5.0 |
| 11/09/07 | RP\_37 | RP-070644 | 0252 | - | 16QAM modulation selection for HSUPA | 7.5.0 | 7.6.0 |
| 11/09/07 | RP\_37 | RP-070642 | 0253 | - | Clarifications of MIMO | 7.5.0 | 7.6.0 |
| 11/09/07 | RP\_37 | RP-070641 | 0254 | - | Clarifications of CPC and MIMO | 7.5.0 | 7.6.0 |
| 27/11/07 | RP\_38 | RP-070941 | 0257 | - | Correction of decimal to binary mapping in case of type B CQI | 7.6.0 | 7.7.0 |
| 27/11/07 | RP\_38 | RP-070941 | 0259 | - | Correction of number of TBs in a TTI in case of MIMO | 7.6.0 | 7.7.0 |
| 28/11/07 | RP\_38 | RP-070950 | 0256 | - | HS-SCCH information field mapping for 64QAM MIMO | 7.7.0 | 8.0.0 |
| 05/04/08 | RP\_39 | RP-080146 | 0261 | - | Correction to RV-coding in case of simultaneous usage of 64QAM and MIMO | 8.0.0 | 8.1.0 |
| 28/05/08 | RP\_40 | RP-080440 | 0262 | 1 | HS-SCCH orders for HS-SCCH-less operation | 8.1.0 | 8.2.0 |
| 28/05/08 | RP\_40 | RP-080349 | 0264 | 2 | Clarification to number of HS-PDSCH codes in HS-SCCH less operations | 8.1.0 | 8.2.0 |
| 09/09/08 | RP\_41 | RP-080673 | 270 | 2 | Introduction of HS-PDSCH Serving Cell Change Enhancements | 8.2.0 | 8.3.0 |
| 09/09/08 | RP\_41 | RP-080665 | 272 | - | Correction to the table name and the quoted name | 8.2.0 | 8.3.0 |
| 03/12/08 | RP\_42 | RP-080989 | 267 | 5 | Introduction of Dual-Cell HSDPA Operation on Adjacent Carriers | 8.3.0 | 8.4.0 |
| 03/12/08 | RP\_42 | RP-080988 | 270 | 3 | Introduction of HS-PDSCH Serving Cell Change Enhancements | 8.3.0 | 8.4.0 |
| 03/03/09 | RP\_43 | RP-090228 | 274 | 1 | Correction to the puncturing limit allowed when UL 4PAM modulation is allowed | 8.4.0 | 8.5.0 |
| 15/09/09 | RP\_45 | RP-090885 | 278 | 1 | Reservation of HS-SCCH order combination not used by CPC | 8.5.0 | 8.6.0 |
| 15/09/09 | RP\_45 | RP-090889 | 280 | 1 | Alignment with RAN2 decisions on HS-SCCH orders for activation and deactivation of DTX and DRX operation | 8.5.0 | 8.6.0 |
| 18/09/09 | RP\_45 | RP-090975 | 276 | 4 | Introduction of TxAA extension for non-MIMO UEs | 8.6.0 | 9.0.0 |
| 18/09/09 | RP\_45 | RP-090974 | 282 | 1 | Combination of DC-HSDPA with MIMO | 8.6.0 | 9.0.0 |
| 01/12/09 | RP\_46 | RP-091170 | 281 | 2 | Introduction of DC-HSUPA | 9.0.0 | 9.1.0 |
| 01/12/09 | RP\_46 | RP-091171 | 283 | 3 | MIMO configuration per downlink frequency in DC-MIMO operation | 9.0.0 | 9.1.0 |
| 16/03/10 | RP\_47 | RP-100206 | 286 | 1 | Clarification of MIMO configuration per downlink frequency in DC-MIMO operation | 9.1.0 | 9.2.0 |
| 14/09/10 | RP\_49 | RP-100897 | 287 | 1 | Clarification of uplink frequencies | 9.2.0 | 9.3.0 |
| 16/09/10 | RP\_49 | RP-100902 | 288 | 3 | Release 10 created with the introduction of 4C-HSDPA | 9.3.0 | 10.0.0 |
| 07/12/10 | RP\_50 | RP-101318 | 290 | 3 | Clarification of 4C-HSDPA | 10.0.0 | 10.1.0 |
| 07/12/10 | RP\_50 | RP-101318 | 295 | - | 4C-HSDPA summary of CQI reporting configurations | 10.0.0 | 10.1.0 |
| 05/12/11 | RP\_54 | RP-111671 | 296 | 8 | Introduction of 8C-HSDPA | 10.1.0 | 11.0.0 |
| 05/12/11 | RP\_54 | RP-111672 | 297 | 1 | Introduction of Uplink Closed Loop Transmit Diversity for HSPA | 10.1.0 | 11.0.0 |
| 28/02/12 | RP\_55 | RP-120280 | 301 | - | Clarification to Target cell HS-SCCH order type | 11.0.0 | 11.1.0 |
| 28/02/12 | RP\_55 | RP-120284 | 303 | - | Correction to 4C-HSDPA CQI report mapping scenarios table | 11.0.0 | 11.1.0 |
| 28/02/12 | RP\_55 | RP-120287 | 304 | 1 | Introduction of 8C-HSDPA CQI report mapping scenarios table | 11.0.0 | 11.1.0 |
| 28/02/12 | RP\_55 | RP-120288 | 305 | - | Corrections to Uplink Closed Loop Transmit Diversity | 11.0.0 | 11.1.0 |
| 13/06/12 | RP\_56 | RP-120740 | 307 | 1 | Addition of missing 8C-HSDPA CQI reporting case indices | 11.1.0 | 11.2.0 |
| 13/06/12 | RP\_56 | RP-120741 | 306 | - | Clarification of CLTD Features | 11.1.0 | 11.2.0 |
| 04/09/12 | RP\_57 | RP-121271 | 308 | 2 | Introduction of Multiflow | 11.2.0 | 11.3.0 |
| 04/09/12 | RP\_57 | RP-121267 | 310 | 1 | Correction of the number of CQI information bits for MC-HSDPA | 11.2.0 | 11.3.0 |
| 04/09/12 | RP\_57 | RP-121268 | 311 | - | Correction of HS-SCCH order information | 11.2.0 | 11.3.0 |
| 04/09/12 | RP\_57 | RP-121270 | 314 | - | Introduction of Further Enhancements to CELL\_FACH | 11.2.0 | 11.3.0 |
| 04/12/12 | RP\_58 | RP-121845 | 312 | 5 | Introduction of uplink MIMO and 64QAM | 11.3.0 | 11.4.0 |
| 04/12/12 | RP\_58 | RP-121843 | 313 | 5 | Introduction of 4Tx\_HSDPA in 25.212 | 11.3.0 | 11.4.0 |
| 04/12/12 | RP\_58 | RP-121840 | 316 | 1 | Clarification of HS-SCCH order for MC-HSPA | 11.3.0 | 11.4.0 |
| 04/12/12 | RP\_58 | RP-121844 | 317 | 1 | Clarifications and corrections to HSDPA Multiflow | 11.3.0 | 11.4.0 |
| 04/12/12 | RP\_58 | RP-121842 | 318 | 1 | Clarification of HS-SCCH order information | 11.3.0 | 11.4.0 |
| 11/06/13 | RP\_60 | RP-130745 | 319 | 2 | Correction to the HS-SCCH Type 4 Structure | 11.4.0 | 11.5.0 |
| 11/06/13 | RP\_60 | RP-130748 | 320 | 1 | Clarification of HS-SCCH orders with the UE is configured in Multiflow and CLTD | 11.4.0 | 11.5.0 |
| 03/09/13 | RP\_61 | RP-131245 | 321 | - | Correction of HS-SCCH type 4 order | 11.5.0 | 11.6.0 |
| 03/03/14 | RP\_63 | RP-140285 | 326 | - | Correction of HS-SCCH type 4 orderCorrection to HS-SCCH special information mapping for HS-SCCH less HSDPA | 11.6.0 | 11.7.0 |
| 10/09/14 | RP\_65 | RP-141483 | 327 | 2 | Introduction of Further EUL Enhancements | 11.7.0 | 12.0.0 |
| 10/09/14 | RP\_65 | RP-141482 | 328 | 2 | Introduction of Enhanced Broadcast of System Information | 11.7.0 | 12.0.0 |
| 10/09/14 | RP\_65 | RP-141480 | 329 | 4 | Introduction of DCH Enhancements | 11.7.0 | 12.0.0 |
| 10/09/14 | RP\_65 | RP-141481 | 330 | 1 | Introduction of UMTS Heterogeneous Networks enhancements | 11.7.0 | 12.0.0 |
| 08/12/14 | RP\_66 | RP-142101 | 332 | 1 | Correction of DL FET | 12.0.0 | 12.1.0 |
| 08/12/14 | RP\_66 | RP-142101 | 333 | - | Correction to TFCI bit mapping index in Rel-12 DCH Enhancements | 12.0.0 | 12.1.0 |
| 14/09/15 | RP\_69 | RP-151469 | 334 | 6 | Introduction of the Multiflow 3F-4C configuration | 12.1.0 | 13.0.0 |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2016-06 | RP-72 | RP-161144 | 0340 |  | F | Clarifications on DCH enhancements feature | 13.1.0 |
| 2016-06 | RP-72 | RP-161283 | 0338 | 2 | F | Clarification on UL DPCH 10ms Mode | 13.1.0 |
| 2016-12 | RP-74 | RP-162354 | 0344 | - | B | Introduction of HS-SCCH Order for HS-SCCH DRx feature in enhanced Cell Fach | 14.0.0 |
| 2016-12 | RP-74 | RP-162363 | 0345 | 1 | B | Introduction of multi-carrier enhancements for UMTS | 14.0.0 |
| 2017-09 | RP-77 | RP-171592 | 0347 | - | B | Introduction of the HS-SCCH orders for the additional triggering mechanism based on HS-SCCH orders | 15.0.0 |
| 2020-07 | RP-88e | - | - | - | - | Upgrade to Rel-16 version without technical change | 16.0.0 |