

3GPP TS 25.213 V16.0.0 (2020-07)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Radio Access Network;

Spreading and modulation (FDD)

(Release 16)

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.  
The present document has not been subject to any approval process by the 3GPPOrganisational Partners and shall not be implemented.   
This Specification is provided for future development work within 3GPPonly. The Organisational Partners accept no liability for any use of this Specification.  
Specifications and reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organisational Partners' Publications Offices.

Keywords

UMTS, radio, modulation, layer 1

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword [5](#__RefHeading___Toc517794533)

1 Scope [6](#__RefHeading___Toc517794534)

2 References [6](#__RefHeading___Toc517794535)

3 Symbols, abbreviations and definitions [6](#__RefHeading___Toc517794536)

3.1 Symbols [6](#__RefHeading___Toc517794537)

3.2 Abbreviations [6](#__RefHeading___Toc517794538)

3.3 Definitions [7](#__RefHeading___Toc517794539)

4 Uplink spreading and modulation [8](#__RefHeading___Toc517794540)

4.1 Overview [8](#__RefHeading___Toc517794541)

4.2 Spreading [8](#__RefHeading___Toc517794542)

4.2.1 Dedicated physical channels [8](#__RefHeading___Toc517794543)

4.2.1.1 DPCCH/DPDCH [10](#__RefHeading___Toc517794544)

4.2.1.2 HS-DPCCH [12](#__RefHeading___Toc517794545)

4.2.1.3 E-DPDCH/E-DPCCH [13](#__RefHeading___Toc517794546)

4.2.1.4 S-DPCCH [21](#__RefHeading___Toc517794547)

4.2.1.4.1 S-DPCCH gain factor setting while not transmitting rank-2 [21](#__RefHeading___Toc517794548)

4.2.1.4.2 S-DPCCH gain factor setting while transmitting rank-2 [22](#__RefHeading___Toc517794549)

4.2.1.5 S-E-DPCCH [22](#__RefHeading___Toc517794550)

4.2.1.6 S-E-DPDCH [23](#__RefHeading___Toc517794551)

4.2.1.7 DPCCH2 [24](#__RefHeading___Toc517794552)

4.2.2 PRACH [25](#__RefHeading___Toc517794553)

4.2.2.1 PRACH preamble part [25](#__RefHeading___Toc517794554)

4.2.2.2 PRACH message part [25](#__RefHeading___Toc517794555)

4.2.3 Void [25](#__RefHeading___Toc517794556)

4.2.4 Channel combining for UL CLTD and UL MIMO [25](#__RefHeading___Toc517794557)

4.3 Code generation and allocation [26](#__RefHeading___Toc517794558)

4.3.1 Channelisation codes [26](#__RefHeading___Toc517794559)

4.3.1.1 Code definition [26](#__RefHeading___Toc517794560)

4.3.1.2 Code allocation for dedicated physical channels [27](#__RefHeading___Toc517794561)

4.3.1.2.1 Code allocation for DPCCH/ S-DPCCH/DPDCH/DPCCH2 [27](#__RefHeading___Toc517794562)

4.3.1.2.2 Code allocation for HS-DPCCH when the UE is not configured in MIMO mode with four transmit antennas in any cell [28](#__RefHeading___Toc517794563)

4.3.1.2.2A Code allocation for HS-DPCCH when the UE is configured in MIMO mode with four transmit antennas in at least one cell [29](#__RefHeading___Toc517794564)

4.3.1.2.3 Code allocation for E-DPCCH/E-DPDCH [30](#__RefHeading___Toc517794565)

4.3.1.2.4 Code allocation for S-E-DPCCH/S-E-DPDCH [31](#__RefHeading___Toc517794566)

4.3.1.3 Code allocation for PRACH message part [31](#__RefHeading___Toc517794567)

4.3.1.4 Void [31](#__RefHeading___Toc517794568)

4.3.1.5 Void [31](#__RefHeading___Toc517794569)

4.3.2 Scrambling codes [31](#__RefHeading___Toc517794570)

4.3.2.1 General [31](#__RefHeading___Toc517794571)

4.3.2.2 Long scrambling sequence [32](#__RefHeading___Toc517794572)

4.3.2.3 Short scrambling sequence [33](#__RefHeading___Toc517794573)

4.3.2.4 Dedicated physical channels scrambling code [34](#__RefHeading___Toc517794574)

4.3.2.5 PRACH message part scrambling code [34](#__RefHeading___Toc517794575)

4.3.2.6 Void [35](#__RefHeading___Toc517794576)

4.3.2.7 Void [35](#__RefHeading___Toc517794577)

4.3.3 PRACH preamble codes [35](#__RefHeading___Toc517794578)

4.3.3.1 Preamble code construction [35](#__RefHeading___Toc517794579)

4.3.3.2 Preamble scrambling code [35](#__RefHeading___Toc517794580)

4.3.3.3 Preamble signature [35](#__RefHeading___Toc517794581)

4.3.4 Void [36](#__RefHeading___Toc517794582)

4.4 Modulation [36](#__RefHeading___Toc517794583)

4.4.1 Modulating chip rate [36](#__RefHeading___Toc517794584)

4.4.2 Modulation [36](#__RefHeading___Toc517794585)

5 Downlink spreading and modulation [37](#__RefHeading___Toc517794586)

5.1 Spreading [37](#__RefHeading___Toc517794587)

5.1.1 Modulation mapper [37](#__RefHeading___Toc517794588)

5.1.1.1 QPSK [37](#__RefHeading___Toc517794589)

5.1.1.2 16QAM [38](#__RefHeading___Toc517794590)

5.1.1.3 64QAM [38](#__RefHeading___Toc517794591)

5.1.2 Channelisation [39](#__RefHeading___Toc517794592)

5.1.3 IQ combining [39](#__RefHeading___Toc517794593)

5.1.4 Scrambling [39](#__RefHeading___Toc517794594)

5.1.5 Channel combining [39](#__RefHeading___Toc517794595)

5.2 Code generation and allocation [40](#__RefHeading___Toc517794596)

5.2.1 Channelisation codes [40](#__RefHeading___Toc517794597)

5.2.2 Scrambling code [41](#__RefHeading___Toc517794598)

5.2.3 Synchronisation codes [43](#__RefHeading___Toc517794599)

5.2.3.1 Code generation [43](#__RefHeading___Toc517794600)

5.2.3.2 Code allocation of SSC [43](#__RefHeading___Toc517794601)

5.3 Modulation [45](#__RefHeading___Toc517794602)

5.3.1 Modulating chip rate [45](#__RefHeading___Toc517794603)

5.3.2 Modulation [45](#__RefHeading___Toc517794604)

Annex A (informative): Generalised Hierarchical Golay Sequences [46](#__RefHeading___Toc517794605)

A.1 Alternative generation [46](#__RefHeading___Toc517794606)

Annex B (informative): Uplink modulation for operation on adjacent frequencies [47](#__RefHeading___Toc517794607)

Annex B1 (informative): Uplink modulation for UL CLTD [48](#__RefHeading___Toc517794608)

Annex B2 (informative): Uplink modulation for operation on dual band frequencies [49](#__RefHeading___Toc517794609)

Annex C (informative): Change history [50](#__RefHeading___Toc517794610)

# Foreword

This Technical Specification (TS) has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# 1 Scope

The present document describes spreading and modulation for UTRA Physical Layer FDD mode.

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TS 25.201: "Physical layer - general description".

[2] 3GPP TS 25.211: "Physical channels and mapping of transport channels onto physical channels (FDD)."

[3] 3GPP TS 25.101: "UE Radio transmission and Reception (FDD)".

[4] 3GPP TS 25.104: "UTRA (BS) FDD; Radio transmission and Reception".

[5] 3GPP TS 25.308: "UTRA High Speed Downlink Packet Access (HSDPA); Overall description".

[6] 3GPP TS 25.214: "Physical layer procedures (FDD)".

[7] 3GPP TS 25.212: "Multiplexing and channel coding (FDD)".

# 3 Symbols, abbreviations and definitions

## 3.1 Symbols

For the purposes of the present document, the following symbols apply:

Cch,SF,n: n:th channelisation code with spreading factor SF

Cpre,n,s: PRACH preamble code for *n*:th preamble scrambling code and signature *s*

Csig,s: PRACH signature code for signature *s*

Sdpch,n: *n*:th DPCCH/DPDCH uplink scrambling code

Sr-pre,n: *n*:th PRACH preamble scrambling code

Sr-msg,n: *n*:th PRACH message scrambling code

Sdl,n: DL scrambling code

Cpsc: PSC code

Cssc,n: n:th SSC code

## 3.2 Abbreviations

For the purposes of the present document, the following abbreviations apply:

16QAM 16 Quadrature Amplitude Modulation

4PAM 4 Pulse Amplitude Modulation

64QAM 64 Quadrature Amplitude Modulation

8PAM 8 Pulse Amplitude Modulation

AICH Acquisition Indicator Channel

BCH Broadcast Channel

CCPCH Common Control Physical Channel

CLTD Closed Loop Transmit Diversity

CPICH Common Pilot Channel

DCH Dedicated Channel

DPCH Dedicated Physical Channel

DPCCH Dedicated Physical Control Channel

DPCCH2 Dedicated Physical Control Channel 2

DPDCH Dedicated Physical Data Channel

E-AGCH E-DCH Absolute Grant Channel

E-DPCCH E-DCH Dedicated Physical Control Channel

E-DPDCH E-DCH Dedicated Physical Data Channel

E-HICH E-DCH Hybrid ARQ Indicator Channel

E-RGCH E-DCH Relative Grant Channel

E-ROCH E-DCH Rank and Offset Channel

FDD Frequency Division Duplex

F-DPCH Fractional Dedicated Physical Channel

F-TPICH Fractional Transmitted Precoding Indicator Channel

HS-DPCCH Dedicated Physical Control Channel (uplink) for HS-DSCH

HS-DPCCH2 Secondary Dedicated Physical Control Channel (uplink) for HS-DSCH, when Secondary\_Cell\_Enabled is greater than 3

HS-DSCH High Speed Downlink Shared Channel

HS-PDSCH High Speed Physical Downlink Shared Channel

HS-SCCH Shared Control Physical Channel for HS-DSCH

MBSFN MBMS over a Single Frequency Network

Mcps Mega Chip Per Second

MICH MBMS Indication Channel

OVSF Orthogonal Variable Spreading Factor (codes)

TPI Transmitted Precoding Indicator

PICH Page Indication Channel

PRACH Physical Random Access Channel

PSC Primary Synchronisation Code

RACH Random Access Channel

SCH Synchronisation Channel

S-DPCCH Secondary Dedicated Physical Control Channel

S-E-DPCCH Secondary Dedicated Physical Control Channel for E-DCH

S-E-DPDCH Secondary Dedicated Physical Data Channel for E-DCH

SSC Secondary Synchronisation Code

SF Spreading Factor

UE User Equipment

## 3.3 Definitions

**Activated uplink frequency:** For a specific UE, an uplink frequency is said to be activated if the UE is allowed to transmit on that frequency. The primary uplink frequency is always activated when configured while a secondary uplink frequency has to be activated by means of an HS-SCCH order in order to become activated. Similarly, for a specific UE, an uplink frequency is said to be deactivated if it is configured but disallowed by the NodeB to transmit on that frequency.

**Configured uplink frequency**: For a specific UE, an uplink frequency is said to be configured if the UE has received all relevant information from higher layers in order to perform transmission on that frequency.

**Primary uplink frequency:** If a single uplink frequency is configured for the UE, then it is the primary uplink frequency. In case more than one uplink frequency is configured for the UE, then the primary uplink frequency is the frequency on which the E-DCH corresponding to the serving E-DCHcellassociated with the serving HS-DSCH cell is transmitted. The association between a pair of uplink and downlink frequencies is indicated by higher layers.

**Secondary uplink frequency:** A secondary uplink frequency is a frequency on which an E-DCH corresponding to a serving E-DCH cell associated with a secondary serving HS-DSCH cell is transmitted. The association between a pair of uplink and downlink frequencies is indicated by higher layers.

# 4 Uplink spreading and modulation

## 4.1 Overview

Spreading is applied to the physical channels. It consists of two operations. The first is the channelisation operation, which transforms every data symbol into a number of chips, thus increasing the bandwidth of the signal. The number of chips per data symbol is called the Spreading Factor (SF). The second operation is the scrambling operation, where a scrambling code is applied to the spread signal.

With the channelisation, data symbols on so-called I- and Q-branches are independently multiplied with an OVSF code. With the scrambling operation, the resultant signals on the I- and Q-branches are further multiplied by complex-valued scrambling code, where I and Q denote real and imaginary parts, respectively.

## 4.2 Spreading

### 4.2.1 Dedicated physical channels

The possible combinations of the maximum number of respective dedicated physical channels which may be configured simultaneously for a UE in addition to the DPCCH are specified in table 0. The actual UE capability may be lower than the values specified in table 0; the actual dedicated physical channel configuration is indicated by higher layer signalling. The actual number of configured DPDCHs, denoted Nmax‑dpdch, is equal to the largest number of DPDCHs from all the TFCs in the TFCS. Nmax‑dpdch is not changed by frame-by-frame TFCI change or temporary TFC restrictions.

Table 0: Maximum number of simultaneously-configured uplink dedicated channels

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | **DPDCH** | **HS-DPCCH** | **E-DPDCH** | **E-DPCCH** | **S-E-DPDCH** | **S-E-DPCCH** |
| Case 1 | 6 | 1 | - | - | - | - |
| Case 2 | 1 | 1 | 2 | 1 | - | - |
| Case 3 | - | 1 on the primary uplink frequency, 0 on any secondary uplink frequency | 4 per uplink frequency | 1 per uplink frequency | - | - |
| Case 4 | 1 | 2 | 2 | 1 | - | - |
| Case 5 | - | 2 on the primary uplink frequency, 0 on any secondary uplink frequency | 4 per uplink frequency | 1 per uplink frequency | - | - |
| Case 6 | - | 2 | 4 | 1 | 4 | 1 |
| Case X | 1 on the primary uplink frequency | 2 on the primary uplink frequency, 0 on any secondary uplink frequency | 2 on the primary uplink frequency, 4 on the secondary uplink frequency | 1 per uplink frequency | - | - |

Figure 1 illustrates the principle of the spreading of uplink dedicated physical channels (DPCCH, DPDCHs, HS-DPCCH, DPCCH2, E-DPCCH, E-DPDCHs, S-E-DPCCH). Figure 1.1 illustrates the principle of the spreading of uplink S-DPCCH and S-E-DPDCHs.

In case of BPSK modulation , the binary input sequences of all physical channels are converted to real valued sequences, i.e. the binary value "0" is mapped to the real value +1, the binary value "1" is mapped to the real value –1, and the value "DTX" (HS-DPCCH only) is mapped to the real value 0.

In case of 4PAM modulation, the binary input sequences of all E-DPDCH and S-E-DPDCH physical channels are converted to real valued sequences, i.e. a set of two consecutive binary symbols *nk*, *nk+1* (with *k* mod 2 = 0) in each binary sequence is converted to a real valued sequence following the mapping described in Table 0A.

In case of 8PAM modulation, the binary input sequences of all E-DPDCH and S-E-DPDCH physical channels are converted to real valued sequences, i.e. a set of three consecutive binary symbols *nk*, *nk+1*, *nk+2* (with *k* mod 3 = 0) in each binary sequence is converted to a real valued sequence following the mapping described in Table 0B.

Table 0A: Mapping of E-DPDCH and S-E-DPDCH  
with 4PAM modulation

|  |  |
| --- | --- |
| ***nk*, *nk+1*** | **Mapped real value** |
| 00 | 0.4472 |
| 01 | 1.3416 |
| 10 | -0.4472 |
| 11 | -1.3416 |

Table 0B: Mapping of E-DPDCH and S-E-DPDCH   
with 8PAM modulation

|  |  |
| --- | --- |
| ***nk*, *nk+1*, *nk+2*** | **Mapped real value** |
| 000 | 0.6547 |
| 001 | 0.2182 |
| 010 | 1.0911 |
| 011 | 1.5275 |
| 100 | -0.6547 |
| 101 | -0.2182 |
| 110 | -1.0911 |
| 111 | -1.5275 |



Figure 1: Spreading for uplink dedicated channels



Figure 1.1: Spreading for uplink S-DPCCH and S-E-DPDCHs

The spreading operation is specified in subclauses 4.2.1.1 to 4.2.1.4 for each of the dedicated physical channels; it includes a spreading stage, a weighting stage, and an IQ mapping stage. In the process, the streams of real-valued chips on the I and Q branches are summed; this results in a complex-valued stream of chips for each set of channels.

As described in figure 1, the resulting complex-valued streams Sdpch, Sdpcch2, Shs-dpcch, Se-dpch and Ss-e-dpcch are summed into a single complex-valued stream which is then scrambled by the complex-valued scrambling codeSdpch,n resulting in the complex-valued signal S. As described in Figure 1.1, the resulting complex-valued streams Ss-dpcch and Ss-e-dpdch are summed into a single complex-valued stream which is scrambled by the same complex-valued scrambling code Sdpch,n resulting in the complex-valued signal S'. The scrambling code shall be applied aligned with the radio frames, i.e. the first scrambling chip corresponds to the beginning of a radio frame.

NOTE: Although subclause 4.2.1 has been reorganized in this release, the spreading operation for the DPCCH, DPDCH remains unchanged as compared to the previous release.

#### 4.2.1.1 DPCCH/DPDCH

Figure 1a illustrates the spreading operation for the uplink DPCCH and DPDCHs.



Figure 1A: Spreading for uplink DPCCH/DPDCHs

The DPCCH is spread to the chip rate by the channelisation code cc. The *n*:th DPDCH called DPDCHn is spread to the chip rate by the channelisation code cd,n.

After channelisation, the real-valued spread signals are weighted by gain factors, c for DPCCH, d for all DPDCHs.

The c and d values are signalled by higher layers or derived as described in [6] 5.1.2.5 and 5.1.2.5C. At every instant in time, at least one of the values c and d has the amplitude 1.0. The c and d values are quantized into 4 bit words. The quantization steps are given in table 1.

Table 1: The quantization of the gain parameters

|  |  |
| --- | --- |
| Signalled values for  c and d | Quantized amplitude ratios  c and d |
| 15 | 1.0 |
| 14 | 14/15 |
| 13 | 13/15 |
| 12 | 12/15 |
| 11 | 11/15 |
| 10 | 10/15 |
| 9 | 9/15 |
| 8 | 8/15 |
| 7 | 7/15 |
| 6 | 6/15 |
| 5 | 5/15 |
| 4 | 4/15 |
| 3 | 3/15 |
| 2 | 2/15 |
| 1 | 1/15 |
| 0 | Switch off |

#### 4.2.1.2 HS-DPCCH

Figure 1B illustrates the spreading operation for the HS-DPCCH when Secondary\_Cell\_Enabled is less than 4 in case the UE is not configured in MIMO mode with four transmit antennas in any cell, or less than 2 in case the UE is configured in MIMO mode with four transmit antennas in at least one cell. Figure 1B.1 illustrates the spreading operation for the HS-DPCCHs when Secondary\_Cell\_Enabled is greater than 3 in case the UE is not configured in MIMO mode with four transmit antennas in any cell, or greater than 1 in case the UE is configured in MIMO mode with four transmit antennas in at least one cell..



Figure 1B: Spreading for uplink HS-DPCCH when Secondary\_Cell\_Enabled is less than 4 in case the UE is not configured in MIMO mode with four transmit antennas in any cell, or less than 2 in case the UE is configured in MIMO mode with four transmit antennas in at least one cell



Figure 1B.1: Spreading for uplink HS-DPCCHs when Secondary\_Cell\_Enabled is greater than 3 in case the UE is not configured in MIMO mode with four transmit antennas in any cell, or greater than 1 in case the UE is configured in MIMO mode with four transmit antennas in at least one cell

Each HS-DPCCH shall be spread to the chip rate by the channelisation code chs.

After channelisation, the real-valued spread signals are weighted by gain factor hs

The hs values are derived from the quantized amplitude ratios Ahs which are translated from ACK , ACK and CQI signalled by higher layers as described in [6] 5.1.2.5A.

The translation of  ACK,ACK and CQI into quantized amplitude ratios Ahs =hs/c in the case that DPCCH2 is not configured, and Ahs =hs/c2 in the case that DPCCH2 is configured is shown in Table 1A.

Table 1A: The quantization of the power offset

|  |  |
| --- | --- |
| Signalled values for  ACK,ACK and CQI | Quantized amplitude ratios  Ahs =hs/c or hs/c2 |
| 12 | 76/15 |
| 11 | 60/15 |
| 10 | 48/15 |
| 9 | 38/15 |
| 8 | 30/15 |
| 7 | 24/15 |
| 6 | 19/15 |
| 5 | 15/15 |
| 4 | 12/15 |
| 3 | 9/15 |
| 2 | 8/15 |
| 1 | 6/15 |
| 0 | 5/15 |

If Secondary\_Cell\_Enabled is less than 4 in case the UE is not configured in MIMO mode with four transmit antennas in any cell, or less than 2 in case the UE is configured in MIMO mode with four transmit antennas in at least one cell, HS-DPCCH shall be mapped to the I branch in case Nmax-dpdch is 2, 4 or 6, and to the Q branch otherwise (Nmax-dpdch = 0, 1, 3 or 5). If Secondary\_Cell\_Enabled is greater than 3 in case the UE is not configured in MIMO mode with four transmit antennas in any cell, or greater than 1 in case the UE is configured in MIMO mode with four transmit antennas in at least one cell, HS-DPCCH shall be mapped to the Q branch and HS-DPCCH2 shall be mapped to the I branch.

#### 4.2.1.3 E-DPDCH/E-DPCCH

Figure 1C illustrates the spreading operation for the E-DPDCHs and the E-DPCCH.



Figure 1C: Spreading for E-DPDCH/E-DPCCH

The E-DPCCH shall be spread to the chip rate by the channelisation code cec. The *k*:th E-DPDCH, denominated E‑DPDCHk, shall be spread to the chip rate using channelisation code ced,k.

After channelisation, the real-valued spread E-DPCCH and E-DPDCHk signals shall respectively be weighted by gain factor ec and ed,k.

*E-TFCIec,boost* may be signalled by higher layers. If *E-TFCIec,boost* is not signalled by higher layers a default value 127 shall be used. When UL\_MIMO\_Enabled is TRUE the UE shall assume *E-TFCIec,boost* = -1 for rank-2 transmissions.

When E-TFCI ≤ *E-TFCIec,boost* the value of ec shall be derived as specified in [6] based on the quantized amplitude ratio Aec which is translated from E-DPCCH signalled by higher layers. The translation of E-DPCCH into quantized amplitude ratios Aec =ec/c is specified in Table 1B.

Table 1B: Quantization for E-DPCCH for E-TFCI ≤ *E-TFCIec,boost*

|  |  |
| --- | --- |
| Signalled values for   E-DPCCH | Quantized amplitude ratios  Aec =ec/c |
| 15 | 151/15 |
| 14 | 120/15 |
| 13 | 95/15 |
| 12 | 76/15 |
| 11 | 60/15 |
| 10 | 48/15 |
| 9 | 38/15 |
| 8 | 30/15 |
| 7 | 24/15 |
| 6 | 19/15 |
| 5 | 15/15 |
| 4 | 12/15 |
| 3 | 9/15 |
| 2 | 8/15 |
| 1 | 6/15 |
| 0 | 5/15 |

When E-TFCI > *E-TFCIec,boost* in order to provide an enhanced phase referencethe value of ec shall be derived as specified in [6] based on a traffic to total pilot power offset T2TP, configured by higher layers as specified in Table 1B.0 and the quantization of the ratio ec/c as specified in Table 1B.0A.

Table 1B.0: T2TP

|  |  |
| --- | --- |
| Signalled values for   T2TP | Power offset values   T2TP [dB] |
| 6 | 16 |
| 5 | 15 |
| 4 | 14 |
| 3 | 13 |
| 2 | 12 |
| 1 | 11 |
| 0 | 10 |

Table 1B.0A: Quantization for *ec*/*c* for E-TFCI > *E-TFCIec,boost*

|  |  |
| --- | --- |
| Quantized amplitude ratios  *ec*/*c* | E-DPDCH modulation schemes which may be used in the same subframe |
| 239/15 | 4PAM, 8PAM |
| 190/15 | 4PAM, 8PAM |
| 151/15 | 4PAM, 8PAM |
| 120/15 | BPSK, 4PAM, 8PAM |
| 95/15 | BPSK, 4PAM, 8PAM |
| 76/15 | BPSK, 4PAM, 8PAM |
| 60/15 | BPSK, 4PAM, 8PAM |
| 48/15 | BPSK, 4PAM, 8PAM |
| 38/15 | BPSK, 4PAM, 8PAM |
| 30/15 | BPSK, 4PAM, 8PAM |
| 24/15 | BPSK, 4PAM, 8PAM |
| 19/15 | BPSK, 4PAM, 8PAM |
| 15/15 | BPSK, 4PAM, 8PAM |
| 12/15 | BPSK, 4PAM, 8PAM |
| 9/15 | BPSK |
| 8/15 | BPSK, 4PAM, 8PAM |
| 6/15 | BPSK, 4PAM, 8PAM |
| 5/15 | BPSK |

The value of ed,k shall be computed as specified in [6] subclause 5.1.2.5B.2, based on the reference gain factors, the spreading factor for E-DPDCHk, the HARQ offsets, and the quantization of the ratio ed,k/c into amplitude ratios specified in Table 1B.2 for the case when E-TFCI ≤ *E-TFCIec,boost* and Table 1.B.2B, for the case when E-TFCI > *E-TFCIec,boost*.

The reference gain factors are derived from the quantised amplitude ratios Aed which is translated from E-DPDCH signalled by higher layers. The translation of E-DPDCH into quantized amplitude ratios Aed =ed/c is specified in Table 1B.1 for the case when E-TFCI ≤ *E-TFCIec,boost* and Table 1.B.2A for the case when E-TFCI > *E-TFCIec,boost*.

When the UE is configured in MIMO mode and transmitting two transport blocks, one with a set of E-DPDCHs and another with a set of S-E-DPDCHs, the amplitude ratios Aed for the primary stream are modified to take the inter-stream interference into account. Note that the amplitude ratios for the secondary stream are not modified. The amplitude ratios Aed for the primary stream are then given by

Aed = Aed, ISI­ x AISI

Aed,ISI, is translated from ∆E-DPDCH signalled by higher layers. The translation of ∆E-DPDCH into quantized amplitude ratios Aed,ISI is specified in Table 1B.2A. AISI is an inter-stream interference compensation factor that is translated from ∆ISI signalled by higher layers according to Table 1B.0B. Note that this procedure does not affect the power used for the transmission of the primary stream E-TFC, but rather lowers the size of the primary stream transport block in order to compensate for the inter-stream interference.

Table 1B.0B: Quantization of ΔISI

|  |  |
| --- | --- |
| Signalled values for  ISI | Quantized amplitude ratios  ISI |
| 15 | 30/15 |
| 14 | 29/15 |
| 13 | 28/15 |
| 12 | 27/15 |
| 11 | 26/15 |
| 10 | 25/15 |
| 9 | 24/15 |
| 8 | 23/15 |
| 7 | 22/15 |
| 6 | 21/15 |
| 5 | 20/15 |
| 4 | 19/15 |
| 3 | 18/15 |
| 2 | 17/15 |
| 1 | 16/15 |
| 0 | 15/15 |

Table 1B.1: Quantization for E-DPDCH for E-TFCI ≤ *E-TFCIec,boost*

|  |  |  |
| --- | --- | --- |
| Signalled values for  E-DPDCH | Quantized amplitude ratios  Aed =ed/c | E-DPDCH modulation schemes which may be used in the same subframe |
| 29 | 168/15 | BPSK |
| 28 | 150/15 | BPSK |
| 27 | 134/15 | BPSK |
| 26 | 119/15 | BPSK |
| 25 | 106/15 | BPSK |
| 24 | 95/15 | BPSK |
| 23 | 84/15 | BPSK |
| 22 | 75/15 | BPSK |
| 21 | 67/15 | BPSK |
| 20 | 60/15 | BPSK |
| 19 | 53/15 | BPSK, 4PAM |
| 18 | 47/15 | BPSK, 4PAM |
| 17 | 42/15 | BPSK, 4PAM |
| 16 | 38/15 | BPSK, 4PAM |
| 15 | 34/15 | BPSK, 4PAM |
| 14 | 30/15 | BPSK, 4PAM |
| 13 | 27/15 | BPSK, 4PAM |
| 12 | 24/15 | BPSK, 4PAM |
| 11 | 21/15 | BPSK, 4PAM |
| 10 | 19/15 | BPSK, 4PAM |
| 9 | 17/15 | BPSK |
| 8 | 15/15 | BPSK |
| 7 | 13/15 | BPSK |
| 6 | 12/15 | BPSK |
| 5 | 11/15 | BPSK |
| 4 | 9/15 | BPSK |
| 3 | 8/15 | BPSK |
| 2 | 7/15 | BPSK |
| 1 | 6/15 | BPSK |
| 0 | 5/15 | BPSK |

Table 1B.2: Quantization for *ed,k*/*c* for E-TFCI ≤ *E-TFCIec,boost*

|  |  |
| --- | --- |
| Quantized amplitude ratios  *ed,k*/*c* | E-DPDCH modulation schemes which may be used in the same subframe |
| 168/15 | BPSK |
| 150/15 | BPSK |
| 134/15 | BPSK |
| 119/15 | BPSK |
| 106/15 | BPSK |
| 95/15 | BPSK |
| 84/15 | BPSK |
| 75/15 | BPSK |
| 67/15 | BPSK |
| 60/15 | BPSK |
| 53/15 | BPSK, 4PAM |
| 47/15 | BPSK, 4PAM |
| 42/15 | BPSK, 4PAM |
| 38/15 | BPSK, 4PAM |
| 34/15 | BPSK, 4PAM |
| 30/15 | BPSK, 4PAM |
| 27/15 | BPSK, 4PAM |
| 24/15 | BPSK, 4PAM |
| 21/15 | BPSK, 4PAM |
| 19/15 | BPSK, 4PAM |
| 17/15 | BPSK |
| 15/15 | BPSK |
| 13/15 | BPSK |
| 12/15 | BPSK |
| 11/15 | BPSK |
| 9/15 | BPSK |
| 8/15 | BPSK |
| 7/15 | BPSK |
| 6/15 | BPSK |
| 5/15 | BPSK |

Table 1B.2A: Quantization for E-DPDCH for E-TFCI > *E-TFCIec,boost*

|  |  |  |
| --- | --- | --- |
| Signalled values for  E-DPDCH | Quantized amplitude ratios  Aed =ed/c | E-DPDCH modulation schemes which may be used in the same subframe |
| 31 | 377/15 | 4PAM, 8PAM (applicable only for SF2 code in a 2xSF2+2xSF4 configuration) |
| 30 | 336/15 | 4PAM, 8PAM (applicable only for SF2 code in a 2xSF2+2xSF4 configuration) |
| 29 | 299/15 | 4PAM, 8PAM |
| 28 | 267/15 | BPSK (applicable only for SF2 code in a 2xSF2+2xSF4 configuration), 4PAM, 8PAM |
| 27 | 237/15 | BPSK (applicable only for SF2 code in a 2xSF2+2xSF4 configuration), 4PAM, 8PAM |
| 26 | 212/15 | BPSK, 4PAM, 8PAM |
| 25 | 189/15 | BPSK, 4PAM, 8PAM |
| 24 | 168/15 | BPSK, 4PAM, 8PAM |
| 23 | 150/15 | BPSK, 4PAM, 8PAM |
| 22 | 134/15 | BPSK, 4PAM, 8PAM |
| 21 | 119/15 | BPSK, 4PAM, 8PAM |
| 20 | 106/15 | BPSK, 4PAM, 8PAM |
| 19 | 95/15 | BPSK, 4PAM, 8PAM |
| 18 | 84/15 | BPSK, 4PAM, 8PAM |
| 17 | 75/15 | BPSK, 4PAM, 8PAM |
| 16 | 67/15 | BPSK, 4PAM, 8PAM |
| 15 | 60/15 | BPSK, 4PAM, 8PAM |
| 14 | 53/15 | BPSK, 4PAM, 8PAM |
| 13 | 47/15 | BPSK, 4PAM, 8PAM |
| 12 | 42/15 | BPSK, 4PAM, 8PAM |
| 11 | 38/15 | BPSK |
| 10 | 34/15 | BPSK |
| 9 | 30/15 | BPSK |
| 8 | 27/15 | BPSK |
| 7 | 24/15 | BPSK |
| 6 | 21/15 | BPSK |
| 5 | 19/15 | BPSK |
| 4 | 17/15 | BPSK |
| 3 | 15/15 | BPSK |
| 2 | 13/15 | BPSK |
| 1 | 11/15 | BPSK |
| 0 | 8/15 | BPSK |

Table 1B.2B: Quantization for *ed,k*/*c* for E-TFCI > *E-TFCIec,boost*

|  |  |
| --- | --- |
| Quantized amplitude ratios  *ed,k*/*c* | E-DPDCH modulation schemes which may be used in the same subframe |
| 377/15 | 4PAM, 8PAM (applicable only for SF2 code in a 2xSF2+2xSF4 configuration) |
| 336/15 | 4PAM, 8PAM (applicable only for SF2 code in a 2xSF2+2xSF4 configuration) |
| 299/15 | 4PAM, 8PAM |
| 267/15 | BPSK (applicable only for SF2 code in a 2xSF2+2xSF4 configuration), 4PAM, 8PAM |
| 237/15 | BPSK (applicable only for SF2 code in a 2xSF2+2xSF4 configuration), 4PAM, 8PAM |
| 212/15 | BPSK, 4PAM, 8PAM |
| 189/15 | BPSK, 4PAM, 8PAM |
| 168/15 | BPSK, 4PAM, 8PAM |
| 150/15 | BPSK, 4PAM, 8PAM |
| 134/15 | BPSK, 4PAM, 8PAM |
| 119/15 | BPSK, 4PAM, 8PAM |
| 106/15 | BPSK, 4PAM, 8PAM |
| 95/15 | BPSK, 4PAM, 8PAM |
| 84/15 | BPSK, 4PAM, 8PAM |
| 75/15 | BPSK, 4PAM, 8PAM |
| 67/15 | BPSK, 4PAM, 8PAM |
| 60/15 | BPSK, 4PAM, 8PAM |
| 53/15 | BPSK, 4PAM, 8PAM |
| 47/15 | BPSK, 4PAM, 8PAM |
| 42/15 | BPSK, 4PAM, 8PAM |
| 38/15 | BPSK |
| 34/15 | BPSK |
| 30/15 | BPSK |
| 27/15 | BPSK |
| 24/15 | BPSK |
| 21/15 | BPSK |
| 19/15 | BPSK |
| 17/15 | BPSK |
| 15/15 | BPSK |
| 13/15 | BPSK |
| 11/15 | BPSK |
| 8/15 | BPSK |

The HARQ offsets harq to be used for support of different HARQ profile are configured by higher layers as specified in Table 1B.3.

Table 1B.3: HARQ offset harq

|  |  |
| --- | --- |
| Signalled values for harq | Power offset values harq [dB] |
| 6 | 6 |
| 5 | 5 |
| 4 | 4 |
| 3 | 3 |
| 2 | 2 |
| 1 | 1 |
| 0 | 0 |

After weighting, the real-valued spread signals shall be mapped to the I branch or the Q branch according to the iqec value for the E-DPCCH and to iqed,k for E-DPDCHk and summed together.

The E-DPCCH shall always be mapped to the I branch, i.e. iqec = 1.

The IQ branch mapping for the E-DPDCHs depends on Nmax-dpdch and on whether an HS-DSCH is configured for the UE; the IQ branch mapping shall be as specified in table 1C.

Table 1C: IQ branch mapping for E-DPDCH

|  |  |  |  |
| --- | --- | --- | --- |
| Nmax-dpdch | **HS-DSCH configured** | **E-DPDCHk** | **iqed,k** |
| 0 | No/Yes | E-DPDCH1 | 1 |
| E-DPDCH2 | j |
| E-DPDCH3 | 1 |
| E-DPDCH4 | j |
| 1 | No | E-DPDCH1 | j |
| E-DPDCH2 | 1 |
| 1 | Yes | E-DPDCH1 | 1 |
| E-DPDCH2 | j |

NOTE: In case the UE transmits more than 2 E-DPDCHs, the UE then always transmits E‑DPDCH3 and E‑DPDCH4 simultaneously.

#### 4.2.1.4 S-DPCCH

Figure 1D illustrates the spreading operation for the uplink S-DPCCH.



Figure 1D: Spreading for uplink S-DPCCH

The S-DPCCH is spread to the chip rate by the channelisation code csc.

After channelisation, the real-valued spread signal is weighted by the gain factor sc for S-DPCCH.

##### 4.2.1.4.1 S-DPCCH gain factor setting while not transmitting rank-2

When no transmission on E-DCH is taking place, or when E-DCH transmission is taking place and E-TFCI ≤ *E-TFCIec,boost* the sc shall be derived based on the quantized amplitude ratios Asc which is translated from S-DPCCH signalled by higher layers as described in [6] subclause 5.1.2.5D. The translation of S-DPCCH into quantized amplitude ratios Asc =sc/c is specified in Table 1C.1.

Table 1C.1: The quantization for S-DPCCH when no transmission on E-DCH is taking place, and when E-DCH transmission is taking place and E-TFCI ≤ *E-TFCIec,boost*

|  |  |
| --- | --- |
| Signalled values for  S-DPCCH | Quantized amplitude ratios  sc |
| 6 | 1.0 |
| 5 | 12/15 |
| 4 | 11/15 |
| 3 | 10/15 |
| 2 | 9/15 |
| 1 | 8/15 |
| 0 | Switch off |

When E-TFCI > *E-TFCIec,boost* in order to provide an enhanced phase reference the value of sc shall be derived as specified in [6] based on the traffic to secondary pilot power offset T2SP, configured by higher layers, and following the definition of T2TP as specified in Table 1B.0 and the quantization of the ratio sc/c following the quantization of ec/c as specified in Table 1B.0A.

##### 4.2.1.4.2 S-DPCCH gain factor setting while transmitting rank-2

When a set of S-E-DPDCHs are present in a TTI, the S-DPCCH gain factor *sc* is set equal to *ec* for that TTI as defined in sub-clause 4.2.1.3.

#### 4.2.1.5 S-E-DPCCH

Figure 1E illustrates the spreading operation for the S-E-DPCCH.



Figure 1E: Spreading for S-E-DPCCH

The S-E-DPCCH shall be spread to the chip rate by the channelisation code csec.

After channelisation, the real-valued spread S-E-DPCCH shall be weighted by gain factor *sec*.

The S-E-DPCCHvalue is signalled by higher layers and the gain factor *sec* shall be derived based on the quantized amplitude ratios. The translation of S-E-DPCCHinto quantized amplitude ratios *sec*/*c* is specified in Table 1C.2.

The S-E-DPCCH shall always be mapped to the Q branch.

Table 1C.2: Quantization gain factors for S-E-DPCCH

|  |  |
| --- | --- |
| Signaled values for S-E-DPCCH | Quantized amplitude ratios *βsec*/*βc* |
| 17 | 239/15 |
| 16 | 190/15 |
| 15 | 151/15 |
| 14 | 120/15 |
| 13 | 95/15 |
| 12 | 76/15 |
| 11 | 60/15 |
| 10 | 48/15 |
| 9 | 38/15 |
| 8 | 30/15 |
| 7 | 24/15 |
| 6 | 19/15 |
| 5 | 15/15 |
| 4 | 12/15 |
| 3 | 9/15 |
| 2 | 8/15 |
| 1 | 6/15 |
| 0 | 5/15 |

#### 4.2.1.6 S-E-DPDCH

Figure 1F illustrates the spreading operation for the S-E-DPDCHs.



Figure 1F: Spreading for S-E-DPDCH

The *k*:th S-E-DPDCH, denominated S-E‑DPDCHk, shall be spread to the chip rate using channelisation code csed,k.

After channelisation, the real-valued spread S-E-DPDCHk signals shall respectively be weighted by gain factor *sed,k*. The value of *sed,k* for S-E-DPDCHk shall follow that of the corresponding *ed,k* for E-DPDCHk transmitted in the same TTI as defined in table 1C.3.

Table 1C.3: Gain factor setting for S-E-DPDCHs

|  |  |
| --- | --- |
| **S-E-DPDCHk** | Quantized amplitude ratios  *sed,k*/*c* |
| S-E-DPDCH1 | *sed,1*/*c* = *ed,1*/*c* |
| S-E-DPDCH2 | *sed,2*/*c* = *ed,2*/*c* |
| S-E-DPDCH3 | *sed,3*/*c* = *ed,3*/*c* |
| S-E-DPDCH4 | *sed,4*/*c* = *ed,4*/*c* |

NOTE: Either no S-E-DPDCHs are transmitted, or all four S-E-DPDCHs are transmitted together and simultaneously with four E-DPDCHs.

After weighting, the real-valued spread signals shall be mapped to the I branch or the Q branch according to the iqsed,k for S-E-DPDCHk and summed together. The IQ branch mapping for the S-E-DPDCHs shall be as specified in table 1C.4.

Table 1C.4: IQ branch mapping for S-E-DPDCHs

|  |  |
| --- | --- |
| **S-E-DPDCHk** | **iqsed,k** |
| S-E-DPDCH1 | 1 |
| S-E-DPDCH2 | j |
| S-E-DPDCH3 | 1 |
| S-E-DPDCH4 | j |

#### 4.2.1.7 DPCCH2

Figure 1G illustrates the spreading operation for the uplink DPCCH2.



Figure 1G: Spreading for uplink DPCCH2

The DPCCH2 is spread to the chip rate by the channelisation code cc2.

After channelisation, the real-valued spread signal is weighted by the gain factor c2 for DPCCH2.

At every instant in time, the value of c2 is set to 1.0.

### 4.2.2 PRACH

#### 4.2.2.1 PRACH preamble part

The PRACH preamble part consists of a complex-valued code, described in subclause 4.3.3.

#### 4.2.2.2 PRACH message part

Figure 2 illustrates the principle of the spreading and scrambling of the PRACH message part, consisting of data and control parts. The binary control and data parts to be spread are represented by real-valued sequences, i.e. the binary value "0" is mapped to the real value +1, while the binary value "1" is mapped to the real value –1. The control part is spread to the chip rate by the channelisation code cc, while the data part is spread to the chip rate by the channelisation code cd.



Figure 2: Spreading of PRACH message part

After channelisation, the real-valued spread signals are weighted by gain factors, c for the control part andd for the data part. At every instant in time, at least one of the values c and d has the amplitude 1.0. The -values are quantized into 4 bit words. The quantization steps are given in subclause 4.2.1.

After the weighting, the stream of real-valued chips on the I- and Q-branches are treated as a complex-valued stream of chips. This complex-valued signal is then scrambled by the complex-valued scrambling code Sr-msg,n. The 10 ms scrambling code is applied aligned with the 10 ms message part radio frames, i.e. the first scrambling chip corresponds to the beginning of a message part radio frame.

### 4.2.3 Void

### 4.2.4 Channel combining for UL CLTD and UL MIMO

Figure 3, 3A, and 3B illustrate how different uplink channels are combined if UL\_CLTD\_Enabled is TRUE.

- For the case that UL\_CLTD\_Active is 1,

- Each complex-valued spread channel, corresponding to point S in Figure 1, and point S' in Figure 1.1 , shall be separately pre-coded by a precoding vector {w1,w2} and {w3,w4} as described in [6]. After precoding, the complex-valued signals T and T' are obtained; see Figure 3.

- For the case that UL\_CLTD\_Active is 2,

- Complex-valued spread channel, corresponding to point S in Figure 1, shall be mapped to T, as shown in Figure 3A.

- For the case that UL\_CLTD\_Active is 3,

- Complex-valued spread channel, corresponding to point S in Figure 1, shall be mapped to T', as shown in Figure 3B.



Figure 3: Combining of uplink physical channels when UL\_CLTD\_Enabled is TRUE and UL\_CLTD\_Active is 1



Figure 3A: Combining of uplink physical channels when UL\_CLTD\_Enabled is TRUE and UL\_CLTD\_Active is 2



Figure 3B: Combining of uplink physical channels when UL\_CLTD\_Enabled is TRUE and UL\_CLTD\_Active is 3

## 4.3 Code generation and allocation

### 4.3.1 Channelisation codes

#### 4.3.1.1 Code definition

The channelisation codes of figure 1 are Orthogonal Variable Spreading Factor (OVSF) codes that preserve the orthogonality between a user's different physical channels. The OVSF codes can be defined using the code tree of figure 4.



Figure 4: Code-tree for generation of Orthogonal Variable Spreading Factor (OVSF) codes

In figure 4, the channelisation codes are uniquely described as Cch,SF,k, where SF is the spreading factor of the code and *k* is the code number, 0  *k*  SF-1.

Each level in the code tree defines channelisation codes of length SF, corresponding to a spreading factor of SF in figure 4.

The generation method for the channelisation code is defined as:

,

The leftmost value in each channelisation code word corresponds to the chip transmitted first in time.

#### 4.3.1.2 Code allocation for dedicated physical channels

NOTE: Although subclause 4.3.1.2 has been reorganized in this release, the spreading operation for DPCCH and DPDCH remains unchanged as compared to the previous release.

##### 4.3.1.2.1 Code allocation for DPCCH/ S-DPCCH/DPDCH/DPCCH2

For the DPCCH, S-DPCCH and DPDCHs the following applies:

- The DPCCH shall always be spread by code cc = Cch,256,0.

- The S-DPCCH shall always be spread by code csc = Cch,256,31.

- The DPCCH2 shall be spread with code cc2 as specified in table 1C.5.

- When only one DPDCH is to be transmitted, DPDCH1 shall be spread by code cd,1 = Cch,SF,k where SF is the spreading factor of DPDCH1 and k= SF / 4.

- When more than one DPDCH is to be transmitted, all DPDCHs have spreading factors equal to 4. DPDCHn shall be spread by the the code cd,n = Cch,4,k , where *k* = 1 if *n*  {1, 2}, *k* = 3 if *n*  {3, 4}, and *k* = 2 if *n*  {5, 6}.

Table 1C.5: Channelisation code of DPCCH2

|  |  |
| --- | --- |
| Nmax-dpdch  (as defined in subclause 4.2.1) | **Channelisation code cc2** |
| 0 | Cch,256,34 |
| ≥1 | Cch,256,3 |

If a power control preamble is used to initialise a DCH, the channelisation code for the DPCCH during the power control preamble shall be the same as that to be used afterwards.

##### 4.3.1.2.2 Code allocation for HS-DPCCH when the UE is not configured in MIMO mode with four transmit antennas in any cell

The HS-DPCCH shall be spread with code chs as specified in table 1D. If Secondary\_Cell\_Enabled is greater than 3 HS-DPCCH2 shall be spread with code chs as specified in table 1D.1.

If Secondary\_Cell\_Enabled as defined in [6] is 0 or 1 or if Secondary\_Cell\_Enabled is 2 and MIMO is not configured in any cell, HS-DPCCH slot format #0 as defined in [2] is used.

If Secondary\_Cell\_Enabled is 2 and MIMO is configured in at least one cell or if Secondary\_Cell\_Enabled is 3, HS-DPCCH slot format #1 as defined in [2] is used.

If Secondary\_Cell\_Enabled is greater than 3, HS-DPCCH slot format #1 as defined in [2] is used.

Table 1D: channelisation code of HS-DPCCH

|  |  |  |  |
| --- | --- | --- | --- |
| Nmax-dpdch  (as defined in subclause 4.2.1) | Channelisation code chs | | |
| Secondary\_Cell\_Enabled is 0, 1, 2 or 3 | | Secondary\_Cell\_Enabled is greater than 3 |
| HS-DPCCH slot format #0 [2] | HS-DPCCH slot format #1 [2] | HS-DPCCH slot format #1 [2] |
| 0 | C ch,256,33 | C ch,128,16 | C ch,128,16 |
| 1 | Cch,256,64 | C ch,128,32 | C ch,128,16 |
| 2,4,6 | Cch,256,1 | N/A | N/A |
| 3,5 | Cch,256,32 | N/A | N/A |

Table 1D.1: channelisation code of HS-DPCCH2 if Secondary\_Cell\_Enabled is greater than 3.

|  |  |
| --- | --- |
| Nmax-dpdch  (as defined in subclause 4.2.1) | Channelisation code chs |
| Secondary\_Cell\_Enabled is greater than 3 |
| HS-DPCCH slot format #1 [2] |
| 0 | C ch,128,16 |
| 1 | C ch,128,16 |

##### 4.3.1.2.2A Code allocation for HS-DPCCH when the UE is configured in MIMO mode with four transmit antennas in at least one cell

If Secondary\_Cell\_Enabled as defined in [6] is 0 or 1, HS-DPCCH slot format #1 as defined in [2] is used. HS-DPCCH shall be spread with code chs as specified in table 1D.2.

If Secondary\_Cell\_Enabled is 2:

- If the UE is configured in MIMO mode with four transmit antennas in all cells, HS-DPCCH slot format #1 as defined in [2] is used for both HS-DPCCH and HS-DPCCH2. HS-DPCCH shall be spread with code chs as specified in table 1D.2 and HS-DPCCH2 spread with code chs as specified in table 1D.3.

- If the number of cells configured in MIMO mode with four transmit antennas is less than 3 and if the UE is configured in MIMO mode with four transmit antennas either in the primary or in the 1st secondary serving cell or both, then HS-DPCCH slot format #1 as defined in [2] is used for HS-DPCCH. HS-DPCCH shall be spread with code chs as specified in table 1D.2.

- If the number of cells configured in MIMO mode with four transmit antennas is less than 3 and if the UE is not configured in MIMO mode with four transmit antennas in the primary and the 1st secondary serving cell then HS-DPCCH slot format #0 as defined in [2] is used for HS-DPCCH. HS-DPCCH shall be spread with code chs as specified in table 1D.4.

- If the number of cells configured in MIMO mode with four transmit antennas is less than 3 and if the UE is configured in MIMO mode with four transmit antennas in the 2nd secondary serving cell then HS-DPCCH slot format #1 as defined in [2] is used for HS-DPCCH2. HS-DPCCH2 spread with code chs as specified in table 1D.3.

- If the number of cells configured in MIMO mode with four transmit antennas is less than 3 and if the UE is not configured in MIMO mode with four transmit antennas in the 2nd secondary serving cell then HS-DPCCH slot format #0 as defined in [2] is used for HS-DPCCH2. HS-DPCCH2 spread with code chs as specified in table 1D.5.

If Secondary\_Cell\_Enabled is 3:

- If the UE is configured in MIMO mode with four transmit antennas in more than 2 cells HS-DPCCH slot format #1 as defined in [2] is used for both HS-DPCCH and HS-DPCCH2. HS-DPCCH shall be spread with code chs as specified in table 1D.2 and HS-DPCCH2 spread with code chs as specified in table 1D.3.

- If the number of cells configured in MIMO mode with four transmit antennas is less than 3 and if the UE is configured in MIMO mode with four transmit antennas either in the primary or in the 1st secondary serving cell or both, then HS-DPCCH slot format #1 as defined in [2] is used for HS-DPCCH. HS-DPCCH shall be spread with code chs as specified in table 1D.2.

- If the number of cells configured in MIMO mode with four transmit antennas is less than 3 and if the UE is not configured in MIMO mode with four transmit antennas in the primary and the 1st secondary serving cell then HS-DPCCH slot format #0 as defined in [2] is used for HS-DPCCH. HS-DPCCH shall be spread with code chs as specified in table 1D.4.

- If the number of cells configured in MIMO mode with four transmit antennas is less than 3 and if the UE is configured in MIMO mode with four transmit antennas in the 2nd serving or in the 3rd serving secondary cell or both then HS-DPCCH slot format #1 as defined in [2] is used for HS-DPCCH2. HS-DPCCH2 spread with code chs as specified in table 1D.3.

- If the number of cells configured in MIMO mode with four transmit antennas is less than 3 and if the UE is not configured in MIMO mode with four transmit antennas in the 2nd and the 3rd secondary serving cell then HS-DPCCH slot format #0 as defined in [2] is used for HS-DPCCH2. HS-DPCCH2 spread with code chs as specified in table 1D.5.

Table 1D.2: channelisation code of HS-DPCCH if Secondary\_Cell\_Enabled is 0 or 1 or 2 or 3 and the UE is configured in MIMO mode with four transmit antennas in any cell

|  |  |  |
| --- | --- | --- |
| Nmax-dpdch  (as defined in subclause 4.2.1) | Channelisation code chs, Secondary\_Cell\_Enabled is 0, 1 | Channelisation code chs, Secondary\_Cell\_Enabled is 2, 3 |
| HS-DPCCH slot format #1 [2] | HS-DPCCH slot format #1 [2] |
| 0 | Cch,128,16 | Cch,128,16 |
| 1 | Cch,128,32 | Cch,128,16 |

Table 1D.3: channelisation code of HS-DPCCH2 if Secondary\_Cell\_Enabled is 2 or 3 and the UE is configured in MIMO mode with four transmit antennas in any cell

|  |  |  |
| --- | --- | --- |
| Nmax-dpdch  (as defined in subclause 4.2.1) | Channelisation code chs | Channelisation code chs |
| HS-DPCCH slot format #0 [2] | HS-DPCCH slot format #1 [2] |
| 0 | Cch,256,32 | Cch,128,16 |
| 1 | Cch,256,32 | Cch,128,16 |

Table 1D.4: channelisation code of HS-DPCCH if Secondary\_Cell\_Enabled is greater than 1 and the UE is not configured in MIMO mode with four transmit antennas in the primary and the 1st secondary serving cell.

|  |  |
| --- | --- |
| Nmax-dpdch  (as defined in subclause 4.2.1) | Channelisation code chs |
| Secondary\_Cell\_Enabled is greater than 1 |
| HS-DPCCH slot format #0 [2] |
| 0 | C ch,256,33 |
| 1 | C ch,256,64 |

Table 1D.5: channelisation code of HS-DPCCH2 if Secondary\_Cell\_Enabled is equal to 3 and the UE is not configured in MIMO mode with four transmit antennas in the 2nd and the 3rd secondary serving cell or if Secondary\_Cell\_Enabled is equal to 2 and the UE is not configured in MIMO mode with four transmit antennas in the 2nd secondary serving cell.

|  |  |
| --- | --- |
| Nmax-dpdch  (as defined in subclause 4.2.1) | Channelisation code chs |
| Secondary\_Cell\_Enabled is greater than 1 |
| HS-DPCCH slot format #0 [2] |
| 0 | C ch,256,33 |
| 1 | C ch,256,64 |

##### 4.3.1.2.3 Code allocation for E-DPCCH/E-DPDCH

The E-DPCCH shall be spread with channelisation code cec = Cch,256,1.

E-DPDCHk shall be spread with channelisation code ced,k. The sequence ced,k depends on Nmax-dpdch and the spreading factor selected for the corresponding frame or sub-frame as specified in [7]; it shall be selected according to table 1E.

Table 1E: Channelisation code for E-DPDCH

|  |  |  |
| --- | --- | --- |
| Nmax-dpdch | E-DPDCHk | Channelisation codeCed,k |
| 0 | E-DPDCH1 | Cch,SF,SF/4 if SF  4  Cch,2,1 if SF = 2 |
| E-DPDCH2 | Cch,4,1 if SF = 4  Cch,2,1 if SF = 2 |
| E-DPDCH3  E-DPDCH4 | Cch,4,1 |
| 1 | E-DPDCH1 | Cch,SF,SF/2 |
| E-DPDCH2 | Cch,4,2 if SF = 4  Cch,2,1 if SF = 2 |

NOTE: When more than one E-DPDCH is transmitted, the respective channelisation codes used for E-DPDCH1 and E-DPDCH2 are always the same.

##### 4.3.1.2.4 Code allocation for S-E-DPCCH/S-E-DPDCH

The S-E-DPCCH shall be spread with channelisation code csec = Cch,256,1.

S-E-DPDCHk shall be spread with channelisation code csed,k. The sequence csed,k shall be selected according to table 1F.

Table 1F: Channelisation code for S-E-DPDCH

|  |  |  |
| --- | --- | --- |
| Nmax-dpdch | S-E-DPDCHk | Channelisation codeCsed,k |
| 0 | S-E-DPDCH1  S-E-DPDCH2 | Cch,2,1 |
| S-E-DPDCH3  S-E-DPDCH4 | Cch,4,1 |

NOTE: Either none or all four S-E-DPDCHs are transmitted.

#### 4.3.1.3 Code allocation for PRACH message part

The preamble signature *s*, 0  *s*  15, points to one of the 16 nodes in the code-tree that corresponds to channelisation codes of length 16. The sub-tree below the specified node is used for spreading of the message part. The control part is spread with the channelisation code cc (as shown in subclause 4.2.2.2) of spreading factor 256 in the lowest branch of the sub-tree, i.e. cc = Cch,256,m where m = 16s + 15. The data part uses any of the channelisation codes from spreading factor 32 to 256 in the upper-most branch of the sub-tree. To be exact, the data part is spread by channelisation code cd =  Cch,SF,m and SF is the spreading factor used for the data part and m = SFs/16.

#### 4.3.1.4 Void

#### 4.3.1.5 Void

### 4.3.2 Scrambling codes

#### 4.3.2.1 General

All uplink physical channels on an activated uplink frequency shall be scrambled with a complex-valued scrambling code. The dedicated physical channels may be scrambled by either a long or a short scrambling code, defined in subclause 4.3.2.4. The PRACH message part shall be scrambled with a long scrambling code, defined in subclause 4.3.2.5. There are 224 long and 224 short uplink scrambling codes. Uplink scrambling codes are assigned by higher layers.

The long scrambling code is built from constituent long sequences defined in subclause 4.3.2.2, while the constituent short sequences used to build the short scrambling code are defined in subclause 4.3.2.3.

#### 4.3.2.2 Long scrambling sequence

The long scrambling sequences clong,1,n and clong,2,n are constructed from position wise modulo 2 sum of 38400 chip segments of two binary *m*-sequences generated by means of two generator polynomials of degree 25. Let *x*, and *y* be the two *m*-sequences respectively. The *x* sequence is constructed using the primitive (over GF(2)) polynomial  *X25+X3+1.* The *y* sequence is constructed using the polynomial  *X25+X3+X2+X+1.* The resulting sequences thus constitute segments of a set of Gold sequences.

The sequence clong,2,n is a 16777232 chip shifted version of the sequence clong,1,n.

Let *n23 … n0* be the 24 bit binary representation of the scrambling sequence number *n* with *n0* being the least significant bit. The *x* sequence depends on the chosen scrambling sequence number *n* and is denoted *xn*, in the sequel. Furthermore, let *xn(i)* and *y(i)* denote the *i:*th symbol of the sequence *xn* and *y,* respectively.

The *m*-sequences *xn* and *y* are constructed as:

Initial conditions:

- xn(0)=n0 , xn(1)= n1 , … =xn(22)= n22 ,xn(23)= n23, xn(24)=1.

- y(0)=y(1)= … =y(23)= y(24)=1.

Recursive definition of subsequent symbols:

- xn(i+25) =xn(i+3) + xn(i) modulo 2, i=0,…, 225-27.

- y(i+25) = y(i+3)+y(i+2) +y(i+1) +y(i) modulo 2, i=0,…, 225-27.

Define the binary Gold sequence *zn* by:

*- zn*(*i*) *= xn*(*i*) *+ y*(*i*) modulo 2*, i* = 0, 1, 2, …, 225-2.

The real valued Gold sequence *Zn* is defined by:

Now, the real-valued long scrambling sequences clong,1,n and clong,2,n are defined as follows:

clong,1,n(*i*) *= Zn*(*i*), *i =* 0, 1, 2, …, 225 – 2 and

clong,2,n(*i*) *= Zn*((*i +* 16777232) modulo (225 – 1)), *i =* 0, 1, 2, …, 225 – 2.

Finally, the complex-valued long scrambling sequence Clong, n, is defined as:

where *i* = 0, 1, …, 225 – 2 and  denotes rounding to nearest lower integer.



Figure 5: Configuration of uplink scrambling sequence generator

#### 4.3.2.3 Short scrambling sequence

The short scrambling sequences *c*short,1,*n*(*i*) and *c*short,2,*n*(*i*) are defined from a sequence from the family of periodically extended S(2) codes.

Let *n*23*n*22…*n*0 be the 24 bit binary representation of the code number *n*.

The *n*:th quaternary S(2) sequence *zn*(*i*), 0 £ *n* £ 16777215, is obtained by modulo 4 addition of three sequences, a quaternary sequence *a*(*i*) and two binary sequences *b*(*i*) and *d*(*i*), where the initial loading of the three sequences is determined from the code number *n*. The sequence *zn*(*i*) of length 255 is generated according to the following relation:

*- zn*(*i*) = *a*(*i*) + 2*b*(*i*) + 2*d*(*i*) modulo 4, *i* = 0, 1, …, 254;

where the quaternary sequence *a*(*i*) is generated recursively by the polynomial *g*0(*x*)= *x8+3x5+x3+3x2+2x+3* as:

*- a*(*0*) = 2*n0* + 1 modulo 4;

*- a*(*i*) = 2*ni* modulo 4, *i* = 1, 2, …, 7;

*- a*(*i)* = 3*a*(*i*-3) + *a*(*i*-5) + 3*a*(*i*-6) + 2*a*(*i*-7) + 3*a*(*i*-8) modulo 4, *i* = 8, 9, …, 254;

and the binary sequence *b*(*i*) is generated recursively by the polynomial *g*1(*x*)= *x8+x7+x5+x+1* as

*b*(*i*) = *n*8+*i* modulo 2, *i* = 0, 1, …, 7,

*b*(*i*) = *b*(*i-1*) *+ b*(*i-3*) + *b*(*i-7*) + *b*(*i-8*) modulo 2, *i* = 8, 9, …, 254,

and the binary sequence *d*(*i*) is generated recursively by the polynomial *g*2(*x*)= *x8+x7+x5+x4+1* as:

*d*(*i*) = *n*16+*i* modulo 2, *i* = 0, 1, …, 7;

*d*(*i*) = *d*(*i-1*) + *d*(*i-3*) + *d*(*i-4*) + *d*(*i-8*) modulo 2, *i* = 8, 9, …, 254.

The sequence *zn*(*i*) is extended to length 256 chips by setting *zn*(255) = *zn*(0).

The mapping from *zn*(*i*) to the real-valued binary sequences *c*short,1,*n*(*i*) and *c*short,2,*n*(*i*), , *i* = 0, 1, …, 255 is defined in Table 2.

Table 2: Mapping from *zn*(*i*) to *cshort,1,n*(*i*) and *cshort,2,n*(*i*), *i* = 0, 1, …, 255

|  |  |  |
| --- | --- | --- |
| *zn*(*i*) | *cshort,1,n*(*i*) | *cshort,2,n*(*i*) |
| 0 | +1 | +1 |
| 1 | -1 | +1 |
| 2 | -1 | -1 |
| 3 | +1 | -1 |

Finally, the complex-valued short scrambling sequence Cshort, n, is defined as:

where *i* = 0, 1, 2, … and  denotes rounding to nearest lower integer.

An implementation of the short scrambling sequence generator for the 255 chip sequence to be extended by one chip is shown in Figure 6.



Figure 6: Uplink short scrambling sequence generator for 255 chip sequence

#### 4.3.2.4 Dedicated physical channels scrambling code

The code used for scrambling of the uplink dedicated physical channels may be of either long or short type. The *n*:th uplink scrambling code, denoted Sdpch, n, is defined as:

Sdpch,n(*i*) = Clong,n(*i*), *i* = 0, 1, …, 38399, when using long scrambling codes;

where the lowest index corresponds to the chip transmitted first in time and Clong,n is defined in subclause 4.3.2.2.

The *n*:th uplink scrambling code, denoted Sdpch, n, is defined as:

Sdpch,n(*i*) = Cshort,n(*i*), *i* = 0, 1, …, 38399, when using short scrambling codes;

where the lowest index corresponds to the chip transmitted first in time and Cshort,n is defined in subclause 4.3.2.3.

#### 4.3.2.5 PRACH message part scrambling code

The scrambling code used for the PRACH message part is 10 ms long, and there are 8192 different PRACH scrambling codes defined.

The *n*:th PRACH message part scrambling code, denoted Sr-msg,n, where *n =* 0, 1, …, 8191, is based on the long scrambling sequence and is defined as:

Sr-msg,n(*i*) = Clong,n(*i* + 4096), *i* = 0, 1, …, 38399

where the lowest index corresponds to the chip transmitted first in time and Clong,n is defined in subclause 4.3.2.2.

The message part scrambling code has a one-to-one correspondence to the scrambling code used for the preamble part. For one PRACH, the same code number is used for both scrambling codes, i.e. if the PRACH preamble scrambling code used is Sr-pre,m then the PRACH message part scrambling code is Sr-msg,m, where the number *m* is the same for both codes.

#### 4.3.2.6 Void

#### 4.3.2.7 Void

### 4.3.3 PRACH preamble codes

#### 4.3.3.1 Preamble code construction

The random access preamble code Cpre,n, is a complex valued sequence. It is built from a preamble scrambling code Sr‑pre,n and a preamble signature Csig,s as follows:

- Cpre,n,s(k) = Sr-pre,n(k)  Csig,s(k)  , k = 0, 1, 2, 3, …, 4095;

where k=0 corresponds to the chip transmitted first in time and Sr-pre,n and Csig,s are defined in 4.3.3.2 and 4.3.3.3 below respectively.

#### 4.3.3.2 Preamble scrambling code

The scrambling code for the PRACH preamble part is constructed from the long scrambling sequences. There are 8192 PRACH preamble scrambling codes in total.

The *n*:th preamble scrambling code, *n =* 0, 1, …, 8191*,* is defined as:

Sr-pre,n(*i*) = clong,1,n(*i*), *i* = 0, 1, …, 4095;

where the sequence clong,1,n is defined in subclause 4.3.2.2.

The 8192 PRACH preamble scrambling codes are divided into 512 groups with 16 codes in each group. There is a one-to-one correspondence between the group of PRACH preamble scrambling codes in a cell and the primary scrambling code used in the downlink of the cell. The *k*:th PRACH preamble scrambling code within the cell with downlink primary scrambling code *m*, *k* = 0, 1, 2, …, 15 and *m* = 0, 1, 2, …, 511, is Sr-pre,n(*i*) as defined above with *n* = 16*m* + *k*.

#### 4.3.3.3 Preamble signature

The preamble signature corresponding to a signature s consists of 256 repetitions of a length 16 signature Ps(n), n=0…15. This is defined as follows:

- Csig,*s*(*i*) = *Ps(i* modulo 16*), i* = 0, 1, …, 4095.

The signature Ps(n) is from the set of 16 Hadamard codes of length 16. These are listed in table 3.

Table 3: Preamble signatures

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Preamble signature | Value of *n* | | | | | | | | | | | | | | | |
| 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15 |
| P0(n) | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 |
| P1(n) | 1 | -1 | 1 | -1 | 1 | -1 | 1 | -1 | 1 | -1 | 1 | -1 | 1 | -1 | 1 | -1 |
| P2(n) | 1 | 1 | -1 | -1 | 1 | 1 | -1 | -1 | 1 | 1 | -1 | -1 | 1 | 1 | -1 | -1 |
| P3(n) | 1 | -1 | -1 | 1 | 1 | -1 | -1 | 1 | 1 | -1 | -1 | 1 | 1 | -1 | -1 | 1 |
| P4(n) | 1 | 1 | 1 | 1 | -1 | -1 | -1 | -1 | 1 | 1 | 1 | 1 | -1 | -1 | -1 | -1 |
| P5(n) | 1 | -1 | 1 | -1 | -1 | 1 | -1 | 1 | 1 | -1 | 1 | -1 | -1 | 1 | -1 | 1 |
| P6(n) | 1 | 1 | -1 | -1 | -1 | -1 | 1 | 1 | 1 | 1 | -1 | -1 | -1 | -1 | 1 | 1 |
| P7(n) | 1 | -1 | -1 | 1 | -1 | 1 | 1 | -1 | 1 | -1 | -1 | 1 | -1 | 1 | 1 | -1 |
| P8(n) | 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 | -1 | -1 | -1 | -1 | -1 | -1 | -1 | -1 |
| P9(n) | 1 | -1 | 1 | -1 | 1 | -1 | 1 | -1 | -1 | 1 | -1 | 1 | -1 | 1 | -1 | 1 |
| P10(n) | 1 | 1 | -1 | -1 | 1 | 1 | -1 | -1 | -1 | -1 | 1 | 1 | -1 | -1 | 1 | 1 |
| P11(n) | 1 | -1 | -1 | 1 | 1 | -1 | -1 | 1 | -1 | 1 | 1 | -1 | -1 | 1 | 1 | -1 |
| P12(n) | 1 | 1 | 1 | 1 | -1 | -1 | -1 | -1 | -1 | -1 | -1 | -1 | 1 | 1 | 1 | 1 |
| P13(n) | 1 | -1 | 1 | -1 | -1 | 1 | -1 | 1 | -1 | 1 | -1 | 1 | 1 | -1 | 1 | -1 |
| P14(n) | 1 | 1 | -1 | -1 | -1 | -1 | 1 | 1 | -1 | -1 | 1 | 1 | 1 | 1 | -1 | -1 |
| P15(n) | 1 | -1 | -1 | 1 | -1 | 1 | 1 | -1 | -1 | 1 | 1 | -1 | 1 | -1 | -1 | 1 |

### 4.3.4 Void

## 4.4 Modulation

### 4.4.1 Modulating chip rate

The modulating chip rate is 3.84 Mcps.

### 4.4.2 Modulation

Modulation of the complex-valued chip sequence generated by the spreading process is shown below in Figure 7 for a UE with a single configured uplink frequency when UL\_CLTD\_Enabled is FALSE:



Figure 7: Uplink modulation when a single uplink frequency is configured and UL\_CLTD\_Enabled is FALSE

An example of uplink modulation for a UE with adjacent primary and secondary uplink frequencies is given in Annex B. An example of uplink modulation for a UE with primary and secondary uplink frequencies in two different bands is given in Annex B2. The pulse-shaping characteristics are described in [3].

An example of uplink modulation for a UE when a single uplink frequency is configured and UL\_CLTD\_Enabled is TRUE is given in Annex B1. The pulse-shaping characteristics are described in [3].

# 5 Downlink spreading and modulation

## 5.1 Spreading

Figure 8 illustrates the spreading operation for all physical channel except SCH. The spreading operation includes a modulation mapper stage successively followed by a channelisation stage, an IQ combining stage and a scrambling stage. All the downlink physical channels are then combined as specified in sub subclause 5.1.5.

The non-spread downlink physical channels, except SCH, AICH, E-HICH and E-RGCH consist of a sequence of 3-valued digits taking the values 0, 1 and "DTX". Note that "DTX" is only applicable to those downlink physical channels that support DTX transmission.



Figure 8: Spreading for all downlink physical channels except SCH

NOTE: Although subclause 5.1 has been reorganized in this release, the spreading operation as specified for the DL channels in the previous release remains unchanged.

### 5.1.1 Modulation mapper

Table 3A defines which of the IQ mapping specified in subclauses 5.1.1.1 and 5.1.1.2 may be used for the physical channel being processed.

Table 3A: IQ mapping

|  |  |
| --- | --- |
| Physical channel | IQ mapping |
| HS-PDSCH | QPSK, 16QAM or 64QAM |
| S-CCPCH used for MBSFN | QPSK or 16QAM |
| All other channels  (except the SCH) | QPSK |

#### 5.1.1.1 QPSK

For all channels, except AICH, E-HICH and E‑RGCH, the input digits shall be mapped to real-valued symbols as follows: the binary value "0" is mapped to the real value +1, the binary value "1" is mapped to the real value –1 and "DTX" is mapped to the real value 0.

For the indicator channels using signatures (AICH), the real-valued input symbols depend on the exact combination of the indicators to be transmitted as specified in [2] subclauses 5.3.3.7, 5.3.3.8 and 5.3.3.9.For the E-HICH and the E‑RGCH the input is a real valued symbol sequence as specified in [2]

Each pair of two consecutive real-valued symbols is first converted from serial to parallel and mapped to an I and Q branch. The definition of the modulation mapper is such that even and odd numbered symbols are mapped to the I and Q branch respectively. For all QPSK channels except the indicator channels using signatures, symbol number zero is defined as the first symbol in each frame or sub-frame. For the indicator channels using signatures, symbol number zero is defined as the first symbol in each access slot.

#### 5.1.1.2 16QAM

In case of 16QAM, a set of four consecutive binary symbols *nk*, *nk+1*, *nk+2*, *nk+3* (with *k* mod 4 = 0) is serial-to-parallel converted to two consecutive binary symbols (*i1*= *nk*, *i2*= *nk+2*) on the I branch and two consecutive binary symbols (*q1*= *nk+1*, *q2*= *nk+3*) on the Q branch and then mapped to 16QAM by the modulation mapper as defined in table 3B.

The I and Q branches are then both spread to the chip rate by the same real-valued channelisation code Cch,16,m. The channelisation code sequence shall be aligned in time with the symbol boundary. The sequences of real-valued chips on the I and Q branch are then treated as a single complex-valued sequence of chips. This sequence of chips from all multi-codes is summed and then scrambled (complex chip-wise multiplication) by a complex-valued scrambling code Sdl,n. The scrambling code is applied aligned with the scrambling code applied to the P-CCPCH.

Table 3B: 16QAM modulation mapping

|  |  |  |
| --- | --- | --- |
| **i1q1i2q2** | **I branch** | **Q branch** |
| 0000 | 0.4472 | 0.4472 |
| 0001 | 0.4472 | 1.3416 |
| 0010 | 1.3416 | 0.4472 |
| 0011 | 1.3416 | 1.3416 |
| 0100 | 0.4472 | -0.4472 |
| 0101 | 0.4472 | -1.3416 |
| 0110 | 1.3416 | -0.4472 |
| 0111 | 1.3416 | -1.3416 |
| 1000 | -0.4472 | 0.4472 |
| 1001 | -0.4472 | 1.3416 |
| 1010 | -1.3416 | 0.4472 |
| 1011 | -1.3416 | 1.3416 |
| 1100 | -0.4472 | -0.4472 |
| 1101 | -0.4472 | -1.3416 |
| 1110 | -1.3416 | -0.4472 |
| 1111 | -1.3416 | -1.3416 |

In the case of 16-QAM on S-CCPCH, a sequence of four consecutive symbols *nk*, *nk+1*, *nk+2*, *nk+3* (with *k* mod 4 = 0) at the input to the modulation mapper may contain values from the set 0, 1, and "DTX". In the event that all 4 bits of the quadruple are DTX bits, the output from the modulation mapping on both the I and Q branches is equal to the real value 0.

For all other cases, all DTX bits in the quadruple are replaced with other non-DTX bits from the quadruple according to the following:

The quadruple consists of two bit pairs, {nk,nk+2} on the I branch, and {nk+1,nk+3} on the Q branch. For any bit pair, if a non-DTX bit is available in the same pair, the DTX bit shall be replaced with the non-DTX bit value. If a non-DTX bit is not available in the same pair, the two DTX bits in that pair shall be replaced by the non-DTX bits in the other pair (using the same bit ordering when the other pair contains two non-DTX bits).

The bit positions and values of non-DTX bits in the quadruple are not affected.

#### 5.1.1.3 64QAM

In case of 64QAM, a set of six consecutive binary symbols *nk*, *nk+1*, *nk+2*, *nk+3*, *nk+4*, *nk+5* (with *k* mod 6 = 0) is serial-to-parallel converted to three consecutive binary symbols (*i1*= *nk*, *i2*= *nk+2*, *i3*= *nk+4*) on the I branch and three consecutive binary symbols (*q1*= *nk+1*, *q2*= *nk+3*, *q3*= *nk+5*) on the Q branch and then mapped to 64QAM by the modulation mapper as defined in table 3C.

The I and Q branches are then both spread to the chip rate by the same real-valued channelisation code Cch,16,m. The channelisation code sequence shall be aligned in time with the symbol boundary. The sequences of real-valued chips on the I and Q branch are then treated as a single complex-valued sequence of chips. This sequence of chips from all multi-codes is summed and then scrambled (complex chip-wise multiplication) by a complex-valued scrambling code Sdl,n. The scrambling code is applied aligned with the scrambling code applied to the P-CCPCH.

Table 3C: 64QAM modulation mapping

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **i1q1i2q2 i3q3** | **I branch** | **Q branch** |  | **i1q1i2q2 i3q3** | **I branch** | **Q branch** |
| 000000 | 0.6547 | 0.6547 |  | 100000 | -0.6547 | 0.6547 |
| 000001 | 0.6547 | 0.2182 |  | 100001 | -0.6547 | 0.2182 |
| 000010 | 0.2182 | 0.6547 |  | 100010 | -0.2182 | 0.6547 |
| 000011 | 0.2182 | 0.2182 |  | 100011 | -0.2182 | 0.2182 |
| 000100 | 0.6547 | 1.0911 |  | 100100 | -0.6547 | 1.0911 |
| 000101 | 0.6547 | 1.5275 |  | 100101 | -0.6547 | 1.5275 |
| 000110 | 0.2182 | 1.0911 |  | 100110 | -0.2182 | 1.0911 |
| 000111 | 0.2182 | 1.5275 |  | 100111 | -0.2182 | 1.5275 |
| 001000 | 1.0911 | 0.6547 |  | 101000 | -1.0911 | 0.6547 |
| 001001 | 1.0911 | 0.2182 |  | 101001 | -1.0911 | 0.2182 |
| 001010 | 1.5275 | 0.6547 |  | 101010 | -1.5275 | 0.6547 |
| 001011 | 1.5275 | 0.2182 |  | 101011 | -1.5275 | 0.2182 |
| 001100 | 1.0911 | 1.0911 |  | 101100 | -1.0911 | 1.0911 |
| 001101 | 1.0911 | 1.5275 |  | 101101 | -1.0911 | 1.5275 |
| 001110 | 1.5275 | 1.0911 |  | 101110 | -1.5275 | 1.0911 |
| 001111 | 1.5275 | 1.5275 |  | 101111 | -1.5275 | 1.5275 |
| 010000 | 0.6547 | -0.6547 |  | 110000 | -0.6547 | -0.6547 |
| 010001 | 0.6547 | -0.2182 |  | 110001 | -0.6547 | -0.2182 |
| 010010 | 0.2182 | -0.6547 |  | 110010 | -0.2182 | -0.6547 |
| 010011 | 0.2182 | -0.2182 |  | 110011 | -0.2182 | -0.2182 |
| 010100 | 0.6547 | -1.0911 |  | 110100 | -0.6547 | -1.0911 |
| 010101 | 0.6547 | -1.5275 |  | 110101 | -0.6547 | -1.5275 |
| 010110 | 0.2182 | -1.0911 |  | 110110 | -0.2182 | -1.0911 |
| 010111 | 0.2182 | -1.5275 |  | 110111 | -0.2182 | -1.5275 |
| 011000 | 1.0911 | -0.6547 |  | 111000 | -1.0911 | -0.6547 |
| 011001 | 1.0911 | -0.2182 |  | 111001 | -1.0911 | -0.2182 |
| 011010 | 1.5275 | -0.6547 |  | 111010 | -1.5275 | -0.6547 |
| 011011 | 1.5275 | -0.2182 |  | 111011 | -1.5275 | -0.2182 |
| 011100 | 1.0911 | -1.0911 |  | 111100 | -1.0911 | -1.0911 |
| 011101 | 1.0911 | -1.5275 |  | 111101 | -1.0911 | -1.5275 |
| 011110 | 1.5275 | -1.0911 |  | 111110 | -1.5275 | -1.0911 |
| 011111 | 1.5275 | -1.5275 |  | 111111 | -1.5275 | -1.5275 |

### 5.1.2 Channelisation

For all physical channels (except SCH) the I and Q branches shall be spread to the chip rate by the same real-valued channelisation code Cch,SF,m, i.e. the output for each input symbol on the I and the Q branches shall be a sequence of SF chips corresponding to the channelisation code chip sequence multiplied by the real-valued symbol. The channelisation code sequence shall be aligned in time with the symbol boundary.

### 5.1.3 IQ combining

The real valued chip sequence on the Q branch shall be complex multiplied with j and summed with the corresponding real valued chip sequence on the I branch, thus resulting in a single complex valued chip sequence.

### 5.1.4 Scrambling

The sequence of complex valued chips shall be scrambled (complex chip-wise multiplication) by a complex-valued scrambling code Sdl,n. In case of P-CCPCH, the scrambling code shall be applied aligned with the P-CCPCH frame boundary, i.e. the first complex chip of the spread P-CCPCH frame is multiplied with chip number zero of the scrambling code. In case of other downlink channels, the scrambling code shall be applied aligned with the scrambling code applied to the P‑CCPCH. In this case, the scrambling code is thus not necessarily applied aligned with the frame boundary of the physical channel to be scrambled.

### 5.1.5 Channel combining

Figure 9 illustrates how different downlink channels are combined. Each complex-valued spread channel, corresponding to point S in Figure 8, may be separately weighted by a weight factor Gi. The complex-valued P-SCH and S-SCH, as described in [2], subclause 5.3.3.5, may be separately weighted by weight factors Gp and Gs. All downlink physical channels shall then be combined using complex addition.



Figure 9: Combining of downlink physical channels

## 5.2 Code generation and allocation

### 5.2.1 Channelisation codes

The channelisation codes of figure 8 are the same codes as used in the uplink, namely Orthogonal Variable Spreading Factor (OVSF) codes that preserve the orthogonality between downlink channels of different rates and spreading factors. The OVSF codes are defined in figure 4 in subclause 4.3.1.

The channelisation code for the Primary CPICH is fixed to Cch,256,0 and the channelisation code for the Primary CCPCH is fixed to Cch,256,1.The channelisation codes for all other physical channels are assigned by UTRAN.

With the spreading factor 512 a specific restriction is applied. When the code word Cch,512,n, with n=0,2,4….510, is used in soft handover, then the code word Cch,512,n+1 is not allocated in the cells where timing adjustment is to be used. Respectively if Cch,512,n, with n=1,3,5….511 is used, then the code word Cch,512,n-1 is not allocated in the cells where timing adjustment is to be used. This restriction shall not apply in cases where timing adjustments in soft handover are not used with spreading factor 512.

When compressed mode is implemented by reducing the spreading factor by 2, the OVSF code used for compressed frames is:

- Cch,SF/2,n/2 if ordinary scrambling code is used.

- Cch,SF/2,n mod SF/2 if alternative scrambling code is used (see subclause 5.2.2);

where Cch,SF,n is the channelisation code used for non-compressed frames.

For F-DPCH, the spreading factor is always 256.

For HS-PDSCH, the spreading factor is always 16.

For HS-SCCH, the spreading factor is always 128.

Channelisation-code-set information over HS-SCCH is mapped in following manner: the OVSF codes shall be allocated in such a way that they are positioned in sequence in the code tree. That is, for P multicodes at offset O the following codes are allocated:

Cch,16,O … Cch,16, O+P-1

The number of multicodes and the corresponding offset for HS-PDSCHs mapped from a given HS-DSCH is signalled by HS-SCCH.

For E-HICH and for E-RGCH, the spreading factor shall always be 128. In each cell, the E‑RGCH and E-HICH assigned to a UE shall be configured with the same channelisation code.

For E-AGCH, the spreading factor shall always be 256.

For F-TPICH, the spreading factor shall always be 256.

For E-ROCH, the spreading factor shall always be 256.

### 5.2.2 Scrambling code

A total of 218-1 = 262,143 scrambling codes, numbered 0…262,142 can be generated. However not all the scrambling codes are used. The scrambling codes are divided into 512 sets each of a primary scrambling code and 15 secondary scrambling codes.

The primary scrambling codes consist of scrambling codes n=16\*i where i=0…511. The i:th set of secondary scrambling codes consists of scrambling codes 16\*i+k, where k=1…15.

There is a one-to-one mapping between each primary scrambling code and 15 secondary scrambling codes in a set such that i:th primary scrambling code corresponds to i:th set of secondary scrambling codes.

Hence, according to the above, scrambling codes k = 0, 1, …, 8191 are used. Each of these codes are associated with a left alternative scrambling code and a right alternative scrambling code, that may be used for compressed frames. The left alternative scrambling code corresponding to scrambling code k is scrambling code number k + 8192, while the right alternative scrambling code corresponding to scrambling code k is scrambling code number k + 16384. The alternative scrambling codes can be used for compressed frames. In this case, the left alternative scrambling code is used if n<SF/2 and the right alternative scrambling code is used if nSF/2, where cch,SF,n is the channelisation code used for non-compressed frames. The usage of alternative scrambling code for compressed frames is signalled by higher layers for each physical channel respectively.

In case F-DPCH is configured in the downlink, the same scrambling code and OVSF code shall be used in F-DPCH compressed frames and normal frames.

In the case that F-TPICH is configured in the downlink, the same scrambling code and OVSF code shall be used in F-TPICH compressed frames and normal frames.

The set of primary scrambling codes is further divided into 64 scrambling code groups, each consisting of 8 primary scrambling codes. The j:th scrambling code group consists of primary scrambling codes 16\*8\*j+16\*k, where j=0..63 and k=0..7.

Each cell is allocated one and only one primary scrambling code. The primary CCPCH, primary CPICH, PICH, MICH, AICH and S-CCPCH carrying PCH or BCH shall always be transmitted using the primary scrambling code. The other downlink physical channels may be transmitted with either the primary scrambling code or a secondary scrambling code from the set associated with the primary scrambling code of the cell.

In MBSFN operations, the S-CCPCH carries FACH only and shall always be transmitted using the primary scrambling code. The same primary CCPCH, primary CPICH, MICH and S-CCPCH may be transmitted from multiple cells using the same primary scrambling code when part of MBSFN operations.

The mixture of primary scrambling code and no more than one secondary scrambling code for one CCTrCH is allowable. In compressed mode during compressed frames, these can be changed to the associated left or right scrambling codes as described above, i.e. in these frames, the total number of different scrambling codes may exceed two.

In the case of CCTrCH of type of HS-DSCH then all the HS-PDSCH channelisation codes and HS-SCCH that a single UE may receive from a single cell shall be under a single scrambling code (either the primary or a secondary scrambling code).

In each cell, the F-DPCH, E‑RGCH, E-HICH, E-AGCH, E-ROCH and F-TPICH assigned to a UE shall be configured with same scrambling code as the assigned phase reference (primary or secondary CPICH).

In each cell the UE may be configured simultaneously with at most two scrambling codes.

The scrambling code sequences are constructed by combining two real sequences into a complex sequence. Each of the two real sequences are constructed as the position wise modulo 2 sum of 38400 chip segments of two binary *m*-sequences generated by means of two generator polynomials of degree 18. The resulting sequences thus constitute segments of a set of Gold sequences. The scrambling codes are repeated for every 10 ms radio frame. Let *x* and *y* be the two sequences respectively. The *x* sequence is constructed using the primitive (over GF(2)) polynomial *1+X7+X18 .* The y sequence is constructed using the polynomial *1+X5+X7+ X10+X18 .*

The sequence depending on the chosen scrambling code number *n* is denoted *zn*, in the sequel. Furthermore, let *x(i)*, *y(i)* and *zn(i)* denote the *i:*th symbol of the sequence *x*, *y,* and *zn*, respectively.

The *m*-sequences *x*and *y* are constructed as:

Initial conditions:

- x is constructed with x(0)=1, x(1)= x(2)=...= x (16)= x (17)=0.

- y(0)=y(1)= … =y(16)= y(17)=1.

Recursive definition of subsequent symbols:

- x(i+18) =x(i+7) + x(i) modulo 2, i=0,…,218-20.

- y(i+18) = y(i+10)+y(i+7)+y(i+5)+y(i) modulo 2, i=0,…, 218-20.

The n:th Gold code sequence *zn, n=0,1,2,…,218-2,* is then defined as:

- zn(i) = x((i+n) modulo (218 - 1)) + y(i) modulo 2, i=0,…, 218-2.

These binary sequences are converted to real valued sequences Zn by the following transformation:

Finally, the n:th complex scrambling code sequence *Sdl,n* is defined as:

- Sdl,n(i) = Zn(i) + j Zn((i+131072) modulo (218-1)), i=0,1,…,38399.

Note that the pattern from phase 0 up to the phase of 38399 is repeated.



Figure 10: Configuration of downlink scrambling code generator

### 5.2.3 Synchronisation codes

#### 5.2.3.1 Code generation

The primary synchronisation code (PSC), Cpsc is constructed as a so-called generalised hierarchical Golay sequence. The PSC is furthermore chosen to have good aperiodic auto correlation properties.

Define:

- a = <x1, x2, x3, …, x16> = <1, 1, 1, 1, 1, 1, -1, -1, 1, -1, 1, -1, 1, -1, -1, 1>

The PSC is generated by repeating the sequence *a* modulated by a Golay complementary sequence, and creating a complex-valued sequence with identical real and imaginary components. The PSC Cpsc is defined as:

- Cpsc = (1 + j)  <a, a, a, -a, -a, a, -a, -a, a, a, a, -a, a, -a, a, a>;

where the leftmost chip in the sequence corresponds to the chip transmitted first in time.

The 16 secondary synchronization codes (SSCs), {Cssc,1,…,C ssc,16}, are complex-valued with identical real and imaginary components, and are constructed from position wise multiplicationof a Hadamard sequence and a sequence *z*, defined as:

- z = <b, b, b, -b, b, b, -b, -b, b, -b, b, -b, -b, -b, -b, -b>, where

*- b* = <*x*1, *x*2, *x*3, *x*4, *x*5, *x*6, *x*7, *x*8, *-x*9, -*x*10, *-x*11, -*x*12, *-x*13, -*x*14, -*x*15, -*x*16> and *x*1, *x*2 , …, *x*15, *x*16, are same as in the definition of the sequence *a* above.

The Hadamard sequences are obtained as the rows in a matrix *H*8 constructed recursively by:

The rows are numbered from the top starting with row *0* (the all ones sequence).

Denote the *n*:th Hadamard sequence as a row of *H8* numbered from the top, n = 0, 1, 2, …, 255,in the sequel.

Furthermore, let *hn(i)* and *z(i)* denote the *i:*th symbol of the sequence *hn* and *z,* respectively where *i* = 0, 1, 2, …, 255 and *i* = 0 corresponds to the leftmost symbol.

The *k*:th SSC, Cssc,k, *k* = 1, 2, 3, …, 16 is then defined as:

- Cssc,k = (1 + *j*)  <*hm*(0)  *z*(0), *hm*(1)  *z*(1), *hm*(2)  *z*(2), …, *hm*(255)  *z*(255)>;

where *m* = 16(*k* – 1) and the leftmost chip in the sequence corresponds to the chip transmitted first in time.

#### 5.2.3.2 Code allocation of SSC

The 64 secondary SCH sequences are constructed such that their cyclic-shifts are unique, i.e., a non-zero cyclic shift less than 15 of any of the 64 sequences is not equivalent to some cyclic shift of any other of the 64 sequences. Also, a non-zero cyclic shift less than 15 of any of the sequences is not equivalent to itself with any other cyclic shift less than 15. Table 4 describes the sequences of SSCs used to encode the 64 different scrambling code groups. The entries in table 4 denote what SSC to use in the different slots for the different scrambling code groups, e.g. the entry "7" means that SSC Cssc,7 shall be used for the corresponding scrambling code group and slot.

Table 4: Allocation of SSCs for secondary SCH

| Scrambling  Code Group | slot number | | | | | | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| #0 | #1 | #2 | #3 | #4 | #5 | #6 | #7 | #8 | #9 | #10 | #11 | #12 | #13 | #14 |
| Group 0 | 1 | 1 | 2 | 8 | 9 | 10 | 15 | 8 | 10 | 16 | 2 | 7 | 15 | 7 | 16 |
| Group 1 | 1 | 1 | 5 | 16 | 7 | 3 | 14 | 16 | 3 | 10 | 5 | 12 | 14 | 12 | 10 |
| Group 2 | 1 | 2 | 1 | 15 | 5 | 5 | 12 | 16 | 6 | 11 | 2 | 16 | 11 | 15 | 12 |
| Group 3 | 1 | 2 | 3 | 1 | 8 | 6 | 5 | 2 | 5 | 8 | 4 | 4 | 6 | 3 | 7 |
| Group 4 | 1 | 2 | 16 | 6 | 6 | 11 | 15 | 5 | 12 | 1 | 15 | 12 | 16 | 11 | 2 |
| Group 5 | 1 | 3 | 4 | 7 | 4 | 1 | 5 | 5 | 3 | 6 | 2 | 8 | 7 | 6 | 8 |
| Group 6 | 1 | 4 | 11 | 3 | 4 | 10 | 9 | 2 | 11 | 2 | 10 | 12 | 12 | 9 | 3 |
| Group 7 | 1 | 5 | 6 | 6 | 14 | 9 | 10 | 2 | 13 | 9 | 2 | 5 | 14 | 1 | 13 |
| Group 8 | 1 | 6 | 10 | 10 | 4 | 11 | 7 | 13 | 16 | 11 | 13 | 6 | 4 | 1 | 16 |
| Group 9 | 1 | 6 | 13 | 2 | 14 | 2 | 6 | 5 | 5 | 13 | 10 | 9 | 1 | 14 | 10 |
| Group 10 | 1 | 7 | 8 | 5 | 7 | 2 | 4 | 3 | 8 | 3 | 2 | 6 | 6 | 4 | 5 |
| Group 11 | 1 | 7 | 10 | 9 | 16 | 7 | 9 | 15 | 1 | 8 | 16 | 8 | 15 | 2 | 2 |
| Group 12 | 1 | 8 | 12 | 9 | 9 | 4 | 13 | 16 | 5 | 1 | 13 | 5 | 12 | 4 | 8 |
| Group 13 | 1 | 8 | 14 | 10 | 14 | 1 | 15 | 15 | 8 | 5 | 11 | 4 | 10 | 5 | 4 |
| Group 14 | 1 | 9 | 2 | 15 | 15 | 16 | 10 | 7 | 8 | 1 | 10 | 8 | 2 | 16 | 9 |
| Group 15 | 1 | 9 | 15 | 6 | 16 | 2 | 13 | 14 | 10 | 11 | 7 | 4 | 5 | 12 | 3 |
| Group 16 | 1 | 10 | 9 | 11 | 15 | 7 | 6 | 4 | 16 | 5 | 2 | 12 | 13 | 3 | 14 |
| Group 17 | 1 | 11 | 14 | 4 | 13 | 2 | 9 | 10 | 12 | 16 | 8 | 5 | 3 | 15 | 6 |
| Group 18 | 1 | 12 | 12 | 13 | 14 | 7 | 2 | 8 | 14 | 2 | 1 | 13 | 11 | 8 | 11 |
| Group 19 | 1 | 12 | 15 | 5 | 4 | 14 | 3 | 16 | 7 | 8 | 6 | 2 | 10 | 11 | 13 |
| Group 20 | 1 | 15 | 4 | 3 | 7 | 6 | 10 | 13 | 12 | 5 | 14 | 16 | 8 | 2 | 11 |
| Group 21 | 1 | 16 | 3 | 12 | 11 | 9 | 13 | 5 | 8 | 2 | 14 | 7 | 4 | 10 | 15 |
| Group 22 | 2 | 2 | 5 | 10 | 16 | 11 | 3 | 10 | 11 | 8 | 5 | 13 | 3 | 13 | 8 |
| Group 23 | 2 | 2 | 12 | 3 | 15 | 5 | 8 | 3 | 5 | 14 | 12 | 9 | 8 | 9 | 14 |
| Group 24 | 2 | 3 | 6 | 16 | 12 | 16 | 3 | 13 | 13 | 6 | 7 | 9 | 2 | 12 | 7 |
| Group 25 | 2 | 3 | 8 | 2 | 9 | 15 | 14 | 3 | 14 | 9 | 5 | 5 | 15 | 8 | 12 |
| Group 26 | 2 | 4 | 7 | 9 | 5 | 4 | 9 | 11 | 2 | 14 | 5 | 14 | 11 | 16 | 16 |
| Group 27 | 2 | 4 | 13 | 12 | 12 | 7 | 15 | 10 | 5 | 2 | 15 | 5 | 13 | 7 | 4 |
| Group 28 | 2 | 5 | 9 | 9 | 3 | 12 | 8 | 14 | 15 | 12 | 14 | 5 | 3 | 2 | 15 |
| Group 29 | 2 | 5 | 11 | 7 | 2 | 11 | 9 | 4 | 16 | 7 | 16 | 9 | 14 | 14 | 4 |
| Group 30 | 2 | 6 | 2 | 13 | 3 | 3 | 12 | 9 | 7 | 16 | 6 | 9 | 16 | 13 | 12 |
| Group 31 | 2 | 6 | 9 | 7 | 7 | 16 | 13 | 3 | 12 | 2 | 13 | 12 | 9 | 16 | 6 |
| Group 32 | 2 | 7 | 12 | 15 | 2 | 12 | 4 | 10 | 13 | 15 | 13 | 4 | 5 | 5 | 10 |
| Group 33 | 2 | 7 | 14 | 16 | 5 | 9 | 2 | 9 | 16 | 11 | 11 | 5 | 7 | 4 | 14 |
| Group 34 | 2 | 8 | 5 | 12 | 5 | 2 | 14 | 14 | 8 | 15 | 3 | 9 | 12 | 15 | 9 |
| Group 35 | 2 | 9 | 13 | 4 | 2 | 13 | 8 | 11 | 6 | 4 | 6 | 8 | 15 | 15 | 11 |
| Group 36 | 2 | 10 | 3 | 2 | 13 | 16 | 8 | 10 | 8 | 13 | 11 | 11 | 16 | 3 | 5 |
| Group 37 | 2 | 11 | 15 | 3 | 11 | 6 | 14 | 10 | 15 | 10 | 6 | 7 | 7 | 14 | 3 |
| Group 38 | 2 | 16 | 4 | 5 | 16 | 14 | 7 | 11 | 4 | 11 | 14 | 9 | 9 | 7 | 5 |
| Group 39 | 3 | 3 | 4 | 6 | 11 | 12 | 13 | 6 | 12 | 14 | 4 | 5 | 13 | 5 | 14 |
| Group 40 | 3 | 3 | 6 | 5 | 16 | 9 | 15 | 5 | 9 | 10 | 6 | 4 | 15 | 4 | 10 |
| Group 41 | 3 | 4 | 5 | 14 | 4 | 6 | 12 | 13 | 5 | 13 | 6 | 11 | 11 | 12 | 14 |
| Group 42 | 3 | 4 | 9 | 16 | 10 | 4 | 16 | 15 | 3 | 5 | 10 | 5 | 15 | 6 | 6 |
| Group 43 | 3 | 4 | 16 | 10 | 5 | 10 | 4 | 9 | 9 | 16 | 15 | 6 | 3 | 5 | 15 |
| Group 44 | 3 | 5 | 12 | 11 | 14 | 5 | 11 | 13 | 3 | 6 | 14 | 6 | 13 | 4 | 4 |
| Group 45 | 3 | 6 | 4 | 10 | 6 | 5 | 9 | 15 | 4 | 15 | 5 | 16 | 16 | 9 | 10 |
| Group 46 | 3 | 7 | 8 | 8 | 16 | 11 | 12 | 4 | 15 | 11 | 4 | 7 | 16 | 3 | 15 |
| Group 47 | 3 | 7 | 16 | 11 | 4 | 15 | 3 | 15 | 11 | 12 | 12 | 4 | 7 | 8 | 16 |
| Group 48 | 3 | 8 | 7 | 15 | 4 | 8 | 15 | 12 | 3 | 16 | 4 | 16 | 12 | 11 | 11 |
| Group 49 | 3 | 8 | 15 | 4 | 16 | 4 | 8 | 7 | 7 | 15 | 12 | 11 | 3 | 16 | 12 |
| Group 50 | 3 | 10 | 10 | 15 | 16 | 5 | 4 | 6 | 16 | 4 | 3 | 15 | 9 | 6 | 9 |
| Group 51 | 3 | 13 | 11 | 5 | 4 | 12 | 4 | 11 | 6 | 6 | 5 | 3 | 14 | 13 | 12 |
| Group 52 | 3 | 14 | 7 | 9 | 14 | 10 | 13 | 8 | 7 | 8 | 10 | 4 | 4 | 13 | 9 |
| Group 53 | 5 | 5 | 8 | 14 | 16 | 13 | 6 | 14 | 13 | 7 | 8 | 15 | 6 | 15 | 7 |
| Group 54 | 5 | 6 | 11 | 7 | 10 | 8 | 5 | 8 | 7 | 12 | 12 | 10 | 6 | 9 | 11 |
| Group 55 | 5 | 6 | 13 | 8 | 13 | 5 | 7 | 7 | 6 | 16 | 14 | 15 | 8 | 16 | 15 |
| Group 56 | 5 | 7 | 9 | 10 | 7 | 11 | 6 | 12 | 9 | 12 | 11 | 8 | 8 | 6 | 10 |
| Group 57 | 5 | 9 | 6 | 8 | 10 | 9 | 8 | 12 | 5 | 11 | 10 | 11 | 12 | 7 | 7 |
| Group 58 | 5 | 10 | 10 | 12 | 8 | 11 | 9 | 7 | 8 | 9 | 5 | 12 | 6 | 7 | 6 |
| Group 59 | 5 | 10 | 12 | 6 | 5 | 12 | 8 | 9 | 7 | 6 | 7 | 8 | 11 | 11 | 9 |
| Group 60 | 5 | 13 | 15 | 15 | 14 | 8 | 6 | 7 | 16 | 8 | 7 | 13 | 14 | 5 | 16 |
| Group 61 | 9 | 10 | 13 | 10 | 11 | 15 | 15 | 9 | 16 | 12 | 14 | 13 | 16 | 14 | 11 |
| Group 62 | 9 | 11 | 12 | 15 | 12 | 9 | 13 | 13 | 11 | 14 | 10 | 16 | 15 | 14 | 16 |
| Group 63 | 9 | 12 | 10 | 15 | 13 | 14 | 9 | 14 | 15 | 11 | 11 | 13 | 12 | 16 | 10 |

## 5.3 Modulation

### 5.3.1 Modulating chip rate

The modulating chip rate is 3.84 Mcps.

### 5.3.2 Modulation

Modulation of the complex-valued chip sequence generated by the spreading process is shown in Figure 11 below.



Figure 11: Downlink modulation

The pulse-shaping characteristics are described in [4].

Annex A (informative):  
Generalised Hierarchical Golay Sequences

# A.1 Alternative generation

The generalised hierarchical Golay sequences for the PSC described in 5.2.3.1 may be also viewed as generated (in real valued representation) by the following methods:

Method 1.

The sequence y is constructed from two constituent sequences *x1* and *x2* of length *n1* and *n2* respectively using the following formula:

- y(i) = x2(i mod n2) \* x1(i div n2), i = 0 ... (n1\* n2) - 1.

The constituent sequences *x1* and *x2* are chosen to be the following length 16 (i.e. *n1* = *n2* =16) sequences:

- x1 is defined to be the length 16 (N(1)=4) Golay complementary sequence obtained by the delay matrix D(1) = [8, 4, 1,2] and weight matrix W(1) = [1, -1, 1,1].

- x2 is a generalised hierarchical sequence using the following formula, selecting s=2 and using the two Golay complementary sequences x3 and x4 as constituent sequences. The length of the sequence x3 and x4 is called n3 respectively n4.

*- x2(i) = x4(i* mod *s + s\*(i* div *sn3)) \* x3((i* div *s)* mod *n3),* *i* = 0 ... (*n3\* n4*) - 1.

- x3 and x4 are defined to be identical and the length 4 (N(3)= N(4)=2) Golay complementary sequence obtained by the delay matrix D(3) = D(4) = [1, 2] and weight matrix W(3) = W(4) = [1, 1].

The Golay complementary sequences x1,x3 and x4 are defined using the following recursive relation:

*a*0(*k*) = (*k*) and *b*0(*k*) = (*k*);

*an*(*k*) = *an*-1(*k*) + *W(j)n*·*bn*-1(*k*-*D(j)n*);

*bn*(*k*) = *an*-1(*k*) - *W(j)n*·*bn*-1(*k*-*D(j)n*);

*k* = 0, 1, 2, …, 2\*\*N(j) -1;

*n* = 1, 2, …, N*(j)*.

The wanted Golay complementary sequence xj is defined by an  assuming n=N(j). The Kronecker delta function is described by , k,j and n are integers.

Method 2

The sequence y can be viewed as a pruned Golay complementary sequence and generated using the following parameters which apply to the generator equations for a and b above:

(a) Let j = 0, N(0) = 8.

(b) [D10,D20,D30,D40,D50,D60,D70,D80] = [128, 64, 16, 32, 8, 1, 4, 2].

(c) [W10,W20,W30,W40,W50,W60,W70,W80] = [1, -1, 1, 1, 1, 1, 1, 1].

(d) For n = 4, 6, set b4(k) = a4(k), b6(k) = a6(k).

Annex B (informative):   
Uplink modulation for operation on adjacent frequencies

An example of modulation of the complex-valued chip sequence generated by the spreading process is shown below in Figure B-1. In Figure B-1, ωL and ωH are the lower and higher assigned channel frequencies.



Figure B-1: Uplink modulation for a UE with adjacent primary and secondary uplink frequencies

Annex B1 (informative):   
Uplink modulation for UL CLTD

In the case that UL\_CLTD\_Enabled is TRUE, modulation of the complex-valued chip sequence T and T', obtained from channel combining operation for UL CLTD in section 4.2.4, is shown in Figure B1-1.



Figure B1-1: Uplink modulation when UL\_CLTD\_Enabled is TRUE

Annex B2 (informative):   
Uplink modulation for operation on dual band frequencies

An example of modulation of the complex-valued chip sequence generated by the spreading process is shown below in Figure B2-1 for two uplink frequencies in two distinct bands. In Figure B2-1, ωB1 and ωB2 are the assigned primary and secondary uplink channel frequencies in two distinct bands.



Figure B2-1: Uplink modulation for a UE with primary and secondary uplink frequencies on two different bands

Annex C (informative):   
Change history

| **Change history** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Date** | **TSG #** | **TSG Doc.** | **CR** | **Rev** | **Subject/Comment** | **Old** | **New** |
| 14/01/00 | RAN\_05 | RP-99589 | - |  | Approved at TSG RAN #5 and placed under Change Control | - | 3.0.0 |
| 14/01/00 | RAN\_06 | RP-99682 | 005 | 1 | Harmonization of notations for downlink scrambling codes | 3.0.0 | 3.1.0 |
| 14/01/00 | RAN\_06 | RP-99683 | 006 | - | Update of downlink spreading description | 3.0.0 | 3.1.0 |
| 14/01/00 | RAN\_06 | RP-99682 | 007 | 1 | Update of TS 25.213 uplink parts | 3.0.0 | 3.1.0 |
| 14/01/00 | RAN\_06 | RP-99683 | 008 | - | Updated modulation description | 3.0.0 | 3.1.0 |
| 14/01/00 | RAN\_06 | RP-99683 | 009 | - | Restriction for spreading factor 512 allocation in the UTRA FDD Downlink | 3.0.0 | 3.1.0 |
| 14/01/00 | RAN\_06 | RP-99683 | 011 | 1 | CPCH codes in power control preamble | 3.0.0 | 3.1.0 |
| 14/01/00 | RAN\_06 | RP-99683 | 012 | 2 | Support of short codes for CPCH | 3.0.0 | 3.1.0 |
| 14/01/00 | RAN\_06 | RP-99682 | 014 | 1 | Editorial Change | 3.0.0 | 3.1.0 |
| 14/01/00 | RAN\_06 | RP-99683 | 016 | - | Channelization Code Allocation for USTS | 3.0.0 | 3.1.0 |
| 14/01/00 | RAN\_06 | RP-99683 | 017 | 1 | Correction (Editorial Change) | 3.0.0 | 3.1.0 |
| 14/01/00 | RAN\_06 | RP-99683 | 019 | - | Correction to code allocation for compressed mode | 3.0.0 | 3.1.0 |
| 14/01/00 | - | - | - |  | Change history was added by the editor | 3.1.0 | 3.1.1 |
| 31/03/00 | RAN\_07 | RP-000063 | 020 | 1 | Consistent numbering of scrambling code groups | 3.1.1 | 3.2.0 |
| 31/03/00 | RAN\_07 | RP-000063 | 021 | - | Downlink signal flow corrections | 3.1.1 | 3.2.0 |
| 31/03/00 | RAN\_07 | RP-000063 | 022 | - | Uplink signal flow corrections | 3.1.1 | 3.2.0 |
| 31/03/00 | RAN\_07 | RP-000063 | 023 | 1 | Number of RACH scrambling codes | 3.1.1 | 3.2.0 |
| 31/03/00 | RAN\_07 | RP-000063 | 024 | 1 | Editorial changes to 25.213 | 3.1.1 | 3.2.0 |
| 31/03/00 | RAN\_07 | RP-000063 | 025 | 3 | Number of PCPCH scrambling codes per cell | 3.1.1 | 3.2.0 |
| 31/03/00 | RAN\_07 | RP-000063 | 027 | - | A typo correction for 5.2.2 and clarification for 5.2.3.1 of TS 25.213V3.1.1 | 3.1.1 | 3.2.0 |
| 31/03/00 | RAN\_07 | RP-000063 | 028 | 2 | Channelization code allocation method for PCPCH message part | 3.1.1 | 3.2.0 |
| 31/03/00 | RAN\_07 | RP-000063 | 029 | - | Clarifications to DSCH scrambling and modulation in 25.213 | 3.1.1 | 3.2.0 |
| 31/03/00 | RAN\_07 | RP-000063 | 032 | - | Clean up of USTS related specifications | 3.1.1 | 3.2.0 |
| 26/06/00 | RAN\_08 | RP-000267 | 033 | - | Clarifications to power control preamble sections | 3.2.0 | 3.3.0 |
| 26/06/00 | RAN\_08 | RP-000267 | 034 | 2 | Numbering of the PCPCH access preamble and collision detection preamble scrambling codes | 3.2.0 | 3.3.0 |
| 26/06/00 | RAN\_08 | RP-000267 | 035 | - | DPDCH/DPCCH gain factors | 3.2.0 | 3.3.0 |
| 16/12/00 | RAN\_10 | RP-000539 | 037 | 1 | Proposed removal of the option of secondary scrambling code for some downlink common channels | 3.3.0 | 3.4.0 |
| 16/03/01 | RAN\_11 | - | - | - | Approved as Release 4 specification (v4.0.0) at TSG RAN #11 | 3.4.0 | 4.0.0 |
| 16/03/01 | RAN\_11 | RP-010059 | 038 | - | Clarification of channelization codes when SF=512 | 3.4.0 | 4.0.0 |
| 16/03/01 | RAN\_11 | RP-010059 | 039 | 1 | Clarification of the scrambling code of a power control preamble | 3.4.0 | 4.0.0 |
| 15/06/01 | RAN\_12 | RP-010333 | 041 | 1 | Clarification of DL channelization code alignment | 4.0.0 | 4.1.0 |
| 15/06/01 | RAN\_12 | RP-010333 | 043 | 1 | Clarification of PDSCH root channelisation code definition | 4.0.0 | 4.1.0 |
| 14/12/01 | RAN\_14 | RP-010738 | 047 | - | Correction of section number reference | 4.1.0 | 4.2.0 |
| 08/03/02 | RAN\_15 | RP-020058 | 049 | - | The inclusion of HSDPA into 25.213 | 4.2.0 | 5.0.0 |
| 07/06/02 | RAN\_16 | RP-020309 | 053 | 1 | Downlink bit mapping | 5.0.0 | 5.1.0 |
| 07/06/02 | RAN\_16 | RP-020316 | 050 | - | Consistency of Signal Point Constellation for QPSK and 16QAM | 5.0.0 | 5.1.0 |
| 07/06/02 | RAN\_16 | RP-020316 | 054 | - | Clarification of uplink DTX handling and modulation | 5.0.0 | 5.1.0 |
| 07/06/02 | RAN\_16 | RP-020316 | 055 | - | Removal of code mapping description over HS-SCCH | 5.0.0 | 5.1.0 |
| 07/06/02 | RAN\_16 | RP-020316 | 056 | 3 | I/Q mapping of HS-DPCCH | 5.0.0 | 5.1.0 |
| 07/06/02 | RAN\_16 | RP-020316 | 057 | - | Definition of the amplitude gain factor for HS-DPCCH | 5.0.0 | 5.1.0 |
| 16/09/02 | RAN\_17 | RP-020583 | 058 | 1 | Numbering corrections | 5.1.0 | 5.2.0 |
| 16/09/02 | RAN\_17 | RP-020583 | 059 |  | Correction on the maximum DPDCH in Figure1 | 5.1.0 | 5.2.0 |
| 16/09/02 | RAN\_17 | RP-020592 | 060 |  | Power offset values for HS-DPCCH | 5.1.0 | 5.2.0 |
| 26/03/03 | RAN\_19 | RP-030135 | 061 | 1 | Removal of the tiny text in Figure 1 and minor corrections to 4.2.1 | 5.2.0 | 5.3.0 |
| 21/09/03 | RAN\_21 | RP-030457 | 062 | - | Clarification of 16QAM modulation description | 5.3.0 | 5.4.0 |
| 06/01/04 | RAN\_22 | RP-030648 | 064 | 1 | Correction of figure in combining of downlink physical channels | 5.4.0 | 5.5.0 |
| 06/01/04 | RAN\_22 | RP-030648 | 065 | 1 | Correction of reference to calculation of HS-DPCCH gain factor | 5.4.0 | 5.5.0 |
| 06/01/04 | RAN\_22 | RP-030727 | 067 | 2 | Restriction of DL secondary scrambling codes per CCTrCH | 5.4.0 | 5.5.0 |
| 13/01/04 | RAN\_22 | - | - | - | Created for M.1457 update | 5.5.0 | 6.0.0 |
| 13/12/04 | RAN\_26 | RP-040539 | 071 | 3 | Introduction of E-DCH | 6.0.0 | 6.1.0 |
| 13/12/04 | RAN\_26 | RP-040450 | 069 | - | Introduction of MICH | 6.0.0 | 6.1.0 |
| 14/03/05 | RAN\_27 | RP-050088 | 070 | 1 | Introduction of F-DPCH | 6.1.0 | 6.2.0 |
| 14/03/05 | RAN\_27 | RP-050046 | 072 | - | Correction on E-DPCCH power offset | 6.1.0 | 6.2.0 |
| 14/03/05 | RAN\_27 | RP-050047 | 073 | 1 | Defining E-DPDCH power offset | 6.1.0 | 6.2.0 |
| 16/06/05 | RAN\_28 | RP-050252 | 074 | 2 | Power offset values for E-DPDCH/E-DPCCH | 6.2.0 | 6.3.0 |
| 16/06/05 | RAN\_28 | RP-050252 | 075 | 3 | Support of different HARQ profiles | 6.2.0 | 6.3.0 |
| 16/06/05 | RAN\_28 | RP-050250 | 077 | 2 | Feature Clean Up: Removal of "CPCH" | 6.2.0 | 6.3.0 |
| 16/06/05 | RAN\_28 | RP-050248 | 079 | - | Feature Clean Up: Removal of DSCH (FDD mode) | 6.2.0 | 6.3.0 |
| 16/06/05 | RAN\_28 | RP-050256 | 080 | - | Correction to short scrambling code polynomial | 6.2.0 | 6.3.0 |
| 26/09/05 | RAN\_29 | RP-050450 | 0081 | - | Clarification on derivation of c and d | 6.3.0 | 6.4.0 |
| 26/09/05 | RAN\_29 | RP-050450 | 0082 | 1 | DL Scrambling Code and Phase Reference Combinations | 6.3.0 | 6.4.0 |
| 26/09/05 | RAN\_29 | RP-050450 | 0083 | 1 | Clarification on power offset quantization | 6.3.0 | 6.4.0 |
| 20/03/06 | RAN\_31 | RP-060076 | 0084 | 1 | Correction to number of configured DPDCHs when E-DPDCH is configured | 6.4.0 | 6.5.0 |
| 20/03/06 | RAN\_31 | - | - | - | Creation of Release 7 specification (v7.0.0) at RAN#31 | 6.5.0 | 7.0.0 |
| 07/03/07 | RAN\_35 | RP-070116 | 0085 | 2 | Introduction of 64QAM for HSDPA | 7.0.0 | 7.1.0 |
| 30/05/07 | RAN\_36 | RP-070388 | 0086 | 4 | Introduction of 16-QAM for HSUPA | 7.1.0 | 7.2.0 |
| 30/05/07 | RAN\_36 | RP-070384 | 0087 | 1 | Support for DL only SFN operation for MBMS FDD | 7.1.0 | 7.2.0 |
| 30/05/07 | RAN\_36 | RP-070387 | 0089 | - | CQI and ACK/NACK power setting for MIMO | 7.1.0 | 7.2.0 |
| 11/09/07 | RAN\_37 | RP-070644 | 0090 | - | Editorial changes in 25.213 for 16QAM specification | 7.2.0 | 7.3.0 |
| 27/11/07 | RAN\_38 | RP-070944 | 0091 | 1 | Editorial changes in 25.213 for 16QAM specification | 7.3.0 | 7.4.0 |
| 04/03/08 | RAN\_39 | - | - | - | Release 8 version further to RAN\_39 decision | 7.4.0 | 8.0.0 |
| 28/05/08 | RAN\_40 | RP-080439 | 0093 | 1 | Range of E-DCH amplitude ratios | 8.0.0 | 8.1.0 |
| 09/09/08 | RAN\_41 | RP-080709 | 0098 | - | Restricted Beta Factor Combinations for EUL | 8.1.0 | 8.2.0 |
| 03/12/08 | RAN\_42 | RP-080989 | 0099 | - | Clarification to scrambling codes in dual cell HSDPA operation | 8.2.0 | 8.3.0 |
| 03/03/09 | RAN\_43 | RP-090238 | 0101 | 2 | Correction to DTX bit insertion for MBSFN 16-QAM | 8.3.0 | 8.4.0 |
| 18/09/09 | RAN\_45 | - | - | - | Release 9 created further to RAN\_45 decision | 8.4.0 | 9.0.0 |
| 01/12/09 | RAN\_46 | RP-091170 | 0103 | 2 | Introduction of DC-HSUPA | 9.0.0 | 9.1.0 |
| 01/12/09 | RAN\_46 | RP-091161 | 0106 | - | Clarification of the quantization of E-DPDCH power offset without E-DPCCH boosting | 9.0.0 | 9.1.0 |
| 14/09/10 | RAN\_49 | RP-100897 | 0107 | 1 | Clarification of uplink frequencies | 9.1.0 | 9.2.0 |
| 16/09/10 | RAN\_49 | RP-100902 | 0108 | 2 | Release 10 created with the introduction of 4C HSDPA | 9.2.0 | 10.0.0 |
| 05/12/11 | RAN\_54 | RP-111671 | 0109 | 7 | Introduction of 8C-HSDPA | 10.0.0 | 11.0.0 |
| 05/12/11 | RAN\_54 | RP-111672 | 0110 | 1 | Introduction of Uplink Closed Loop Transmit Diversity for HSPA | 10.0.0 | 11.0.0 |
| 28/02/12 | RAN\_55 | RP-120288 | 0111 | - | Corrections to Uplink Closed Loop Transmit Diversity | 11.0.0 | 11.1.0 |
| 13/06/12 | RAN\_56 | RP-120741 | 0112 | 1 | Clarification of CLTD Features | 11.1.0 | 11.2.0 |
| 04/09/12 | RAN\_57 | RP-121271 | 0113 | 2 | Introduction of Multiflow | 11.2.0 | 11.3.0 |
| 04/09/12 | RAN\_57 | RP-121384 | 0114 | 1 | Correction to the gain factor definition for S-DPCCH | 11.2.0 | 11.3.0 |
| 04/12/12 | RAN\_58 | RP-121845 | 0115 | 6 | Introduction of uplink MIMO and 64QAM | 11.3.0 | 11.4.0 |
| 04/12/12 | RAN\_58 | RP-121843 | 0116 | 6 | Introduction of 4Tx\_HSDPA in 25.213 | 11.3.0 | 11.4.0 |
| 10/09/14 | RAN\_65 | RP-141482 | 0117 | 2 | Introduction of Enhanced Broadcast of System Information | 11.4.0 | 12.0.0 |
| 10/09/14 | RAN\_65 | RP-141481 | 0118 | 1 | Introduction of UMTS Heterogeneous Networks enhancements | 11.4.0 | 12.0.0 |
| 07/12/15 | RAN\_70 | RP-152023 | 0119 | 4 | Introduction of Dual Carrier HSUPA enhancements for UTRAN CS in TS 25.213 | 12.0.0 | 13.0.0 |
| 07/12/15 | RAN\_70 | RP-152030 | 0121 | 1 | Introduction of HSPA Dual-Band UL carrier aggregation | 12.0.0 | 13.0.0 |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2017-03 | RP-75 | - | - | - | - | Promotion to Release 14 without technical change (MCC) | 14.0.0 |
| 2018-06 | RP-80 | - | - | - | - | Promotion to Release 15 without technical change (MCC) | 15.0.0 |
| 2020-07 | RP-88e | - | - | - | - | Upgrade to Rel-16 version without technical change | 16.0.0 |