

3GPP TS 25.215 V16.0.0 (2020-07)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Radio Access Network;

Physical layer;  
Measurements (FDD)

(Release 16)

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.  
The present document has not been subject to any approval process by the 3GPPOrganisational Partners and shall not be implemented.   
This Specification is provided for future development work within 3GPPonly. The Organisational Partners accept no liability for any use of this Specification.  
Specifications and reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organisational Partners' Publications Offices.

Keywords

UMTS, radio, layer 1

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword [5](#__RefHeading___Toc517795313)

1 Scope [6](#__RefHeading___Toc517795314)

2 References [6](#__RefHeading___Toc517795315)

3 Definitions and Abbreviations [7](#__RefHeading___Toc517795316)

3.1 Definitions [7](#__RefHeading___Toc517795317)

3.2 Abbreviations [7](#__RefHeading___Toc517795318)

4 Control of UE/UTRAN measurements [7](#__RefHeading___Toc517795319)

5 Measurement abilities for UTRA FDD [8](#__RefHeading___Toc517795320)

5.1 UE measurement abilities [8](#__RefHeading___Toc517795321)

5.1.1 CPICH RSCP [9](#__RefHeading___Toc517795322)

5.1.2 PCCPCH RSCP [9](#__RefHeading___Toc517795323)

5.1.3 UTRA carrier RSSI [9](#__RefHeading___Toc517795324)

5.1.4 GSM carrier RSSI [9](#__RefHeading___Toc517795325)

5.1.5 CPICH Ec/No [10](#__RefHeading___Toc517795326)

5.1.6 Transport channel BLER [10](#__RefHeading___Toc517795327)

5.1.7 UE transmitted power [10](#__RefHeading___Toc517795328)

5.1.8 SFN-CFN observed time difference [11](#__RefHeading___Toc517795329)

5.1.9 SFN-SFN observed time difference [11](#__RefHeading___Toc517795330)

5.1.10 UE Rx-Tx time difference [12](#__RefHeading___Toc517795331)

5.1.11 Void [12](#__RefHeading___Toc517795332)

5.1.12 UE GPS Timing of Cell Frames for UE positioning [12](#__RefHeading___Toc517795333)

5.1.13 UE GPS code phase [12](#__RefHeading___Toc517795334)

5.1.14 UE transmission power headroom [12](#__RefHeading___Toc517795335)

5.1.15 UE GANSS Timing of Cell Frames for UE positioning [13](#__RefHeading___Toc517795336)

5.1.16 UE GANSS code measurements [13](#__RefHeading___Toc517795337)

5.1.17 E-UTRA RSRP [13](#__RefHeading___Toc517795338)

5.1.18 Void [13](#__RefHeading___Toc517795339)

5.1.19 E-UTRA RSRQ [14](#__RefHeading___Toc517795340)

5.1.20 IEEE 802.11 Beacon RSSI [14](#__RefHeading___Toc517795341)

5.2 UTRAN measurement abilities [14](#__RefHeading___Toc517795342)

5.2.1 Received total wide band power [15](#__RefHeading___Toc517795343)

5.2.2 SIR [15](#__RefHeading___Toc517795344)

5.2.3 SIRerror [15](#__RefHeading___Toc517795345)

5.2.4 Transmitted carrier power [16](#__RefHeading___Toc517795346)

5.2.5 Transmitted code power [16](#__RefHeading___Toc517795347)

5.2.6 Transport channel BER [16](#__RefHeading___Toc517795348)

5.2.7 Physical channel BER [16](#__RefHeading___Toc517795349)

5.2.8 Round trip time [17](#__RefHeading___Toc517795350)

5.2.9 UTRAN GPS Timing of Cell Frames for UE positioning [17](#__RefHeading___Toc517795351)

5.2.10 PRACH Propagation delay [17](#__RefHeading___Toc517795352)

5.2.11 Acknowledged PRACH preambles [17](#__RefHeading___Toc517795353)

5.2.12 Void [18](#__RefHeading___Toc517795354)

5.2.13 Void [18](#__RefHeading___Toc517795355)

5.2.14 SFN-SFN observed time difference [18](#__RefHeading___Toc517795356)

5.2.15 Transmitted carrier power of all codes not used for HS-PDSCH, HS-SCCH, E-AGCH, E-RGCH or E-HICH transmission [18](#__RefHeading___Toc517795357)

5.2.16 DL Transmission Branch Load [18](#__RefHeading___Toc517795358)

5.2.17 Received scheduled E-DCH power share (RSEPS) [19](#__RefHeading___Toc517795359)

5.2.18 UTRAN GANSS Timing of Cell Frames for UE positioning [19](#__RefHeading___Toc517795360)

6 Measurements for UTRA FDD [19](#__RefHeading___Toc517795361)

6.1 UE measurements [19](#__RefHeading___Toc517795362)

6.1.1 Compressed mode [19](#__RefHeading___Toc517795363)

6.1.1.1 Use of compressed mode for monitoring [19](#__RefHeading___Toc517795364)

6.1.1.2 Parameterisation of the compressed mode [20](#__RefHeading___Toc517795365)

Annex A (informative): Change history [23](#__RefHeading___Toc517795366)

# Foreword

This Technical Specification (TS) has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# 1 Scope

The present document contains the description and definition of the measurements for FDD done at the UE and network in order to support operation in idle mode and connected mode.

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TS 25.211: "Physical channels and mapping of transport channels onto physical channels (FDD)".

[2] 3GPP TS 25.212: "Multiplexing and channel coding (FDD)".

[3] 3GPP TS 25.213: "Spreading and modulation (FDD)".

[4] 3GPP TS 25.214: "Physical layer procedures (FDD)".

[5] 3GPP TS 25.215: "Physical layer - Measurements (FDD)".

[6] 3GPP TS 25.221: "Physical channels and mapping of transport channels onto physical channels (TDD)".

[7] 3GPP TS 25.222: "Multiplexing and channel coding (TDD)".

[8] 3GPP TS 25.223: "Spreading and modulation (TDD)".

[9] 3GPP TS 25.224: "Physical layer procedures (TDD)".

[10] 3GPP TS 25.301: "Radio Interface Protocol Architecture".

[11] 3GPP TS 25.302: "Services provided by the Physical layer".

[12] 3GPP TS 25.303: "UE functions and interlayer procedures in connected mode".

[13] 3GPP TS 25.304: "UE procedures in idle mode".

[14] 3GPP TS 25.331: "RRC Protocol Specification".

[15] 3GPP TR 25.922: "Radio Resource Management Strategies".

[16] 3GPP TR 25.923: "Report on Location Services (LCS)".

[17] 3GPP TR 25.401: "UTRAN Overall Description".

[18] 3GPP TS 25.101: "UE Radio transmission and Reception (FDD)".

[19] 3GPP TS 25.104: "UTRA (BS) FDD; Radio transmission and Reception".

[20] 3GPP TS 25.133: " Requirements for Support of Radio Resource Management (FDD)"

[21] 3GPP TS 25.225: " Physical layer – Measurements (TDD)".

[22] 3GPP TS 25.321: "Medium Access Control (MAC) protocol specification"

[23] 3GPP TS 36.211: "E-UTRA; Physical Channels and Modulation"

[24] 3GPP TS 36.214: "E-UTRA; Physical layer – Measurements"

[25] IEEE 802.11, Part 11: "Wireless LAN Medium Access Control (MAC) and Physical Layer (PHY) specifications, IEEE Std.".

# 3 Definitions and Abbreviations

## 3.1 Definitions

For the purposes of the present document, the following terms and definitions apply.

**cell portion**: A geographical part of a cell for which a Node B measurement can be reported to the RNC. A cell portion is semi-static, and identical for both the UL and the DL. Within a cell, a cell portion is uniquely identified by a cell portion ID.

Note 1: a cell portion is not necessarily analogous to actual beams used for transmission and/or reception of e.g. a DPCH at the Node B.

Note 2: RNC may associate physical channels with cell portions.

**DL\_DCH\_FET\_Config**: Higher layers signal this configuration parameter to indicate enhanced DCH physical layer configuration. The possible values are 0 and 1. The value 0 indicates Mode 0 configuration where DL transport channels concatenation and UL ACK/NACK signalling are not configured. The value 1 indicates Mode 1 where DL transport channel concatenation and UL ACK/NACK signalling for DL FET are configured.

## 3.2 Abbreviations

For the purposes of the present document, the following abbreviations apply:

BER Bit Error Rate

BLER Block Error Rate

Ec/No Received energy per chip divided by the power density in the band

E-UTRA Evolved Universal Terrestrial Radio Access

F-DPCH Fractional Dedicated Physical Channel

GANSS Galileo and Additional Navigation Satellite Systems

GNSS Global Navigation Satellite System

GPS Global Positioning System

ISCP Interference Signal Code Power

RL Radio Link

RSCP Received Signal Code Power

RSRP Reference Signal Received Power

RSRQ Reference Signal Received Quality

RSSI Received Signal Strength Indicator

SIR Signal to Interference Ratio

# 4 Control of UE/UTRAN measurements

In this chapter the general measurement control concept of the higher layers is briefly described to provide an understanding on how L1 measurements are initiated and controlled by higher layers.

L1 provides with the measurement specifications a toolbox of measurement abilities for the UE and the UTRAN. These measurements can be differentiated in different reported measurement types: intra-frequency, inter-frequency, inter-system, traffic volume, quality and UE internal measurements (see [14]).

In the L1 measurement specifications the measurements, see chapter 5, are distinguished between measurements in the UE (the messages will be described in the RRC Protocol or MAC Protocol [22]) and measurements in the UTRAN (the messages will be described in the NBAP and the Frame Protocol).

To initiate a specific measurement the UTRAN transmits a 'measurement control message' to the UE including a measurement ID and type, a command (setup, modify, release), the measurement objects and quantity, the reporting quantities, criteria (periodical/event-triggered) and mode (acknowledged/unacknowledged), see [14].

When the reporting criteria is fulfilled the UE shall answer with a 'measurement report message' to the UTRAN including the measurement ID and the results.

In idle mode the measurement control message is broadcast in a System Information.

Intra-frequency reporting events, traffic volume reporting events and UE internal measurement reporting events described in [14] define events which trigger the UE to send a report to the UTRAN. This defines a toolbox from which the UTRAN can choose the needed reporting events.

# 5 Measurement abilities for UTRA FDD

In this chapter the physical layer measurements reported to higher layers are defined. The GSM measurements are required only from the GSM capable terminals. The TDD measurements are required only from the terminals that are capable to operate in TDD mode.

## 5.1 UE measurement abilities

The structure of the table defining a UE measurement quantity is shown below.

|  |  |
| --- | --- |
| **Column field** | Comment |
| **Definition** | Contains the definition of the measurement. |
| **Applicable for** | States in which RRC state according to [14] a measurement shall be possible to perform. For RRC connected mode states information is also given on the possibility to perform the measurement on intra-frequency and/or inter-frequency.  The following terms are used in the tables:  Idle = Shall be possible to perform in idle mode;  URA\_PCH = Shall be possible to perform in URA\_PCH;  CELL\_PCH = Shall be possible to perform in CELL\_PCH;  CELL\_FACH = Shall be possible to perform in CELL\_FACH;  CELL\_DCH = Shall be possible to perform in CELL\_DCH;  For all RRC connected mode states i.e. URA\_PCH, CELL\_PCH, CELL\_FACH and CELL\_DCH  Intra appended to the RRC state = Shall be possible to perform in the corresponding RRC state on an intra-frequency cell;  Inter appended to the RRC state = Shall be possible to perform in the corresponding RRC state on an inter-frequency cell.  Inter-RAT appended to the RRC state = Shall be possible to perform in the corresponding RRC state on an inter-RAT cell. |

The term "antenna connector of the UE" used in this sub-clause to define the reference point for the UE measurements is defined in [18]. Performance and reporting requirements for the UE measurements are defined in [20].

### 5.1.1 CPICH RSCP

|  |  |
| --- | --- |
| **Definition** | Received Signal Code Power, the received power on one code measured on the Primary CPICH. The reference point for the RSCP shall be the antenna connector of the UE. If Tx diversity is applied on the Primary CPICH the received code power from each antenna shall be separately measured and summed together in [W] to a total received code power on the Primary CPICH. If receiver diversity is in use by the UE, the measured CPICH RSCP value shall not be lower than the corresponding CPICH RSCP of any of the individual receive antenna branches. |
| **Applicable for** | Idle,  URA\_PCH intra, URA\_PCH inter,  CELL\_PCH intra, CELL\_PCH inter,  CELL\_FACH intra, CELL\_FACH inter,  CELL\_DCH intra, CELL\_DCH inter |

### 5.1.2 PCCPCH RSCP

|  |  |
| --- | --- |
| **Definition** | Received Signal Code Power, the received power on one code measured on the PCCPCH from a TDD cell. The reference point for the RSCP shall be the antenna connector of the UE.  See [21] for further details on this measurement. |
| **Applicable for** | Idle,  URA\_PCH inter,  CELL\_PCH inter,  CELL\_FACH inter,  CELL\_DCH inter |

### 5.1.3 UTRA carrier RSSI

|  |  |
| --- | --- |
| **Definition** | The received wide band power, including thermal noise and noise generated in the receiver, within the bandwidth defined by the receiver pulse shaping filter. The reference point for the measurement shall be the antenna connector of the UE. If receiver diversity is in use by the UE, the measured UTRA carrier RSSI value shall not be lower than the corresponding UTRA carrier RSSI of any of the individual receive antenna branches. |
| **Applicable for** | CELL\_DCH intra, CELL\_DCH inter |

### 5.1.4 GSM carrier RSSI

|  |  |
| --- | --- |
| **Definition** | Received Signal Strength Indicator, the wide-band received power within the relevant channel bandwidth. Measurement shall be performed on a GSM BCCH carrier. The reference point for the RSSI shall be the antenna connector of the UE. |
| **Applicable for** | Idle,  URA\_PCH inter-RAT  CELL\_PCH inter-RAT  CELL\_FACH inter-RAT  CELL\_DCH inter-RAT |

### 5.1.5 CPICH Ec/No

|  |  |
| --- | --- |
| **Definition** | The received energy per chip divided by the power density in the band. If receiver diversity is not in use by the UE, the CPICH Ec/No is identical to CPICH RSCP/UTRA Carrier RSSI. Measurement shall be performed on the Primary CPICH. The reference point for the CPICH Ec/No shall be the antenna connector of the UE. If Tx diversity is applied on the Primary CPICH the received energy per chip (Ec) from each antenna shall be separately measured and summed together in [Ws] to a total received chip energy per chip on the Primary CPICH, before calculating the Ec/No. If receiver diversity is in use by the UE the measured CPICH Ec/No value shall not be lower than the corresponding CPICH RSCP*i*/UTRA Carrier RSSI*i* of receive antenna branch i. |
| **Applicable for** | Idle,  URA\_PCH intra, URA\_PCH inter,  CELL\_PCH intra, CELL\_PCH inter,  CELL\_FACH intra, CELL\_FACH inter,  CELL\_DCH intra, CELL\_DCH inter |

### 5.1.6 Transport channel BLER

|  |  |
| --- | --- |
| **Definition** | Estimation of the transport channel block error rate (BLER). The BLER estimation shall be based on evaluating the CRC of each transport block associated with the measured transport channel after RL combination. The BLER shall be computed over the measurement period as the ratio between the number of received transport blocks resulting in a CRC error and the number of received transport blocks.  When either TFCI or guided detection is used, the measurement "Transport channel BLER" may only be requested for a transport channel when the associated CRC size is non zero and at least one transport format in the associated transport format set includes at least one transport block.  When neither TFCI nor guided detection is used, the measurement "Transport channel BLER" may only be requested for a transport channel when the associated CRC size is non zero and all transport formats in the associated transport format set include at least one transport block.  The measurement "Transport channel BLER" does not apply to transport channels mapped on a P-CCPCH and a S-CCPCH. The UE shall be able to perform the measurement "Transport channel BLER" on any transport channel configured such that the measurement "Transport channel BLER" can be requested as defined in this section. |
| **Applicable for** | CELL\_DCH intra |

### 5.1.7 UE transmitted power

|  |  |
| --- | --- |
| **Definition** | The sum of the total UE transmitted power on all configured uplink carriers. The reference point for the UE transmitted power shall be the antenna connector of the UE. In the case where transmissions from multiple branches take place the transmitted power for each branch shall be measured and summed together in [W]. |
| **Applicable for** | CELL\_FACH intra, CELL\_DCH intra |

### 5.1.8 SFN-CFN observed time difference

|  |  |
| --- | --- |
| **Definition** | The SFN-CFN observed time difference to cell is defined as: OFF38400+ Tm, where:  Tm= (TUETx-T0) - TRxSFN, given in chip units with the range [0, 1, …, 38399] chips  TUETx is the time when the UE transmits an uplink DPCCH frame.  T0 is defined in [1].  TRxSFN is the time at the beginning of the neighbouring P-CCPCH frame received most recent in time before the time instant TUETx-T0in the UE. If the beginning of the neighbouring P-CCPCH frame is received exactly at TUETx-T0 then TRxSFN=TUETx-T0 (which leads to Tm=0).  and  OFF=(SFN-CFNTx) mod 256, given in number of frames with the range [0, 1, …, 255] frames  CFNTx is the connection frame number for the UE transmission of an uplink DPCCH frame at the time TUETx.  SFN is the system frame number for the neighbouring P-CCPCH frame received in the UE at the time TRxSFN.  The reference point for the SFN-CFN observed time difference shall be the antenna connector of the UE.  In case the inter-frequency measurement is done with compressed mode, the UE is not required to read the cell SFN of the target inter-frequency neighbour cell and the value for the parameter OFF is always reported to be 0.  In case that the SFN measurement indicator indicates that the UE does not need to read cell SFN of the target neighbour cell, the value of the parameter OFF is always be set to 0. |
| **Applicable for** | CELL\_DCH intra, CELL\_DCH inter |

### 5.1.9 SFN-SFN observed time difference

|  |  |
| --- | --- |
| **Definition** | **Type 1:**  The SFN-SFN observed time difference to cell is defined as: OFF38400+ Tm, where:  Tm= TRxSFNj  - TRxSFNi, given in chip units with the range [0, 1, …, 38399] chips  TRxSFNj is the time at the beginning of a received neighbouring P-CCPCH frame from cell j.  TRxSFNi is the time at the beginning of the P-CCPCH frame from serving cell i of most recent in time before the time instant TRxSFNj in the UE. If the next neighbouring P-CCPCH frame is exactly at TRxSFNj then TRxSFNj= TRxSFNi (which leads to Tm=0).  and  OFF=(SFNi- SFNj) mod 256, given in number of frames with the range [0, 1, …, 255] frames  SFNj is the system frame number for downlink P-CCPCH frame from cell j in the UE at the time TRxSFNj.  SFNi is the system frame number for the P-CCPCH frame from serving cell i in the UE at the time TRxSFNi.  The reference point for the SFN-SFN observed time difference type 1 shall be the antenna connector of the UE.  **Type 2:**  The relative timing difference between cell j and cell i, defined as TCPICHRxj - TCPICHRxi, where:  TCPICHRxj is the time when the UE receives one Primary CPICH slot from cell j  TCPICHRxi is the time when the UE receives the Primary CPICH slot from cell i that is closest in time to the Primary CPICH slot received from cell j.  The reference point for the SFN-SFN observed time difference type 2 shall be the antenna connector of the UE. |
| **Applicable for** | **Type 1:** Idle, URA\_PCH intra, CELL\_PCH intra, CELL\_FACH intra  **Type 2:**  URA\_PCH intra, URA\_PCH inter,  CELL\_PCH intra, CELL\_PCH inter,  CELL\_FACH intra, CELL\_FACH inter  CELL\_DCH intra, CELL\_DCH inter |

### 5.1.10 UE Rx-Tx time difference

|  |  |
| --- | --- |
| **Definition** | The difference in time between the UE uplink DPCCH frame transmission and the first detected path (in time), of the downlink DPCH or F-DPCH frame from the measured radio link. Type 1 and Type 2 are defined. For Type 1, the reference Rx path shall be the first detected path (in time) amongst the paths (from the measured radio link) used in the demodulation process. For Type 2, the reference Rx path shall be the first detected path (in time) amongst all paths (from the measured radio link) detected by the UE. The reference path used for the measurement may therefore be different for Type 1 and Type 2. The reference point for the UE Rx-Tx time difference shall be the antenna connector of the UE. Measurement shall be made for each cell included in the active set. |
| **Applicable for** | CELL\_DCH intra |

### 5.1.11 Void

### 5.1.12 UE GPS Timing of Cell Frames for UE positioning

|  |  |
| --- | --- |
| **Definition** | The timing between cell j and GPS Time Of Week. TUE-GPSj is defined as the time of occurrence of a specified UTRAN event according to GPS time. The specified UTRAN event is the beginning of a particular frame (identified through its SFN) in the first detected path (in time) of the cell j CPICH, where cell j is a cell chosen by the UE. The reference point for TUE-GPSj shall be the antenna connector of the UE. |
| **Applicable for** | CELL\_FACH intra, CELL\_DCH intra |

### 5.1.13 UE GPS code phase

|  |  |
| --- | --- |
| **Definition** | The whole and fractional phase of the spreading code of the ith GPS satellite signal. The reference point for the GPS code phase shall be the antenna connector of the UE. |
| **Applicable for** | Void (this measurement is not related to UTRAN/GSM signals; its applicability is therefore independent of the UE RRC state) |

### 5.1.14 UE transmission power headroom

|  |  |
| --- | --- |
| **Definition** | For each uplink DPCCH, UE transmission power headroom (UPH) is the ratio of the maximum UE transmission power and the DPCCH code power, and shall be calculated as following:  where:  *Pmax,tx*= min {*Maximum allowed UL TX Power*, *Pmax*} is the UE maximum transmission power;  *Maximum allowed UL TX Power* is set by UTRAN and defined in [14];  *Pmax* is the UE nominal maximum output power according to the UE power class and specified in [18] table 6.1;  *PDPCCH* is the transmitted code power on the DPCCH.  The reference point for the UE transmission power headroom shall be the antenna connector of the UE. |
| **Applicable for** | CELL\_FACH intra, CELL\_DCH intra |

### 5.1.15 UE GANSS Timing of Cell Frames for UE positioning

|  |  |
| --- | --- |
| **Definition** | The timing between cell j and GANSS Time Of Day for a given GANSS system. TUE-GANSS is defined as the time of occurrence of a specified UTRAN event according to GANSS time for a given GANSS Id. The specified UTRAN event is the beginning of a particular frame (identified through its SFN) in the first detected path (in time) of the cell j CPICH, where cell j is a cell chosen by the UE. The reference point for TUE-GANSSj shall be the antenna connector of the UE. |
| **Applicable for** | CELL\_FACH intra, CELL\_DCH intra |

### 5.1.16 UE GANSS code measurements

|  |  |
| --- | --- |
| **Definition** | The GANSS code phase and GANSS Integer code phase of the spreading code of the ith GANSS satellite signal. The reference point for the GANSS code phase shall be the antenna connector of the UE. |
| **Applicable for** | Void (this measurement is not related to UTRAN/GSM signals; its applicability is therefore independent of the UE RRC state) |

### 5.1.17 E-UTRA RSRP

|  |  |
| --- | --- |
| **Definition** | Reference signal received power (RSRP), is defined as the linear average over the power contributions (in [W]) of the resource elements that carry cell-specific reference signals within the considered measurement frequency bandwidth.  For RSRP determination the cell-specific reference signals R0 according to TS 36.211 [23] shall be used. If the UE can reliably detect that R1 is available it may use R1 in addition to R0 to determine RSRP.  The reference point for the RSRP shall be the antenna connector of the UE.  If receiver diversity is in use by the UE, the reported value shall not be lower than the corresponding RSRP of any of the individual diversity branches. |
| **Applicable for** | Idle,  URA\_PCH inter-RAT  CELL\_PCH inter-RAT  CELL\_DCH inter-RAT |

NOTE 1: The number of resource elements within the considered measurement frequency bandwidth and within the measurement period that are used by the UE to determine RSRP is left up to the UE implementation with the limitation that corresponding measurement accuracy requirements have to be fulfilled.

NOTE 2: The power per resource element is determined from the energy received during the useful part of the symbol, excluding the CP.

### 5.1.18 Void

### 5.1.19 E-UTRA RSRQ

|  |  |
| --- | --- |
| **Definition** | Reference Signal Received Quality (RSRQ) is defined as the ratio *N*×RSRP/(E-UTRA carrier RSSI), where *N* is the number of resource blocks of the E-UTRA carrier RSSI measurement bandwidth. The measurements in the numerator and denominator shall be made over the same set of resource blocks.  E-UTRA Carrier Received Signal Strength Indicator (RSSI), comprises the linear average of the total received power (in [W]) observed only in certain OFDM symbols of measurement subframes, in the measurement bandwidth, over *N* number of resource blocks by the UE from all sources, including co-channel serving and non-serving cells, adjacent channel interference, thermal noise etc.  Unless indicated otherwise by higher layers, RSSI is measured only from OFDM symbols containing reference symbols for antenna port 0 of measurement subframes. If higher layers indicate all OFDM symbols for performing RSRQ measurements, then RSSI is measured from all OFDM symbols of the DL part of measurement subframes.  The reference point for the RSRQ shall be the antenna connector of the UE.  If receiver diversity is in use by the UE, the reported value shall not be lower than the corresponding RSRQ of any of the individual diversity branches. |
| **Applicable for** | Idle,  URA\_PCH inter-RAT  CELL\_PCH inter-RAT  CELL\_DCH inter-RAT |

### 5.1.20 IEEE 802.11 Beacon RSSI

|  |  |
| --- | --- |
| **Definition** | The IEEE 802.11 Beacon RSSI is defined in [25]. |
| **Applicable for** | Idle,  URA\_PCH inter-RAT  CELL\_PCH inter-RAT  CELL\_FACH inter-RAT  CELL\_DCH inter-RAT |

## 5.2 UTRAN measurement abilities

The structure of the table defining a UTRAN measurement quantity is shown below.

|  |  |
| --- | --- |
| **Column field** | Comment |
| **Definition** | Contains the definition of the measurement. |

The term "antenna connector" used in this sub-clause to define the reference point for the UTRAN measurements refers to the "BS antenna connector" test port A and test port B as described in [19]. The term "antenna connector" refers to Rx or Tx antenna connector as described in the respective measurement definitions.

### 5.2.1 Received total wide band power

|  |  |
| --- | --- |
| **Definition** | The received wide band power, including noise generated in the receiver, within the bandwidth defined by the receiver pulse shaping filter. The reference point for the measurement shall be the Rx antenna connector. In case of receiver diversity the reported value shall be linear average of the power in the diversity branches. When cell portions are defined in the cell, the total received wideband power shall be measured for each cell portion. |

### 5.2.2 SIR

|  |  |
| --- | --- |
| **Definition** | Type 1:  Signal to Interference Ratio, is defined as: (RSCP/ISCP)SF. The measurement shall be performed on the DPCCH of a Radio Link Set. In compressed mode the SIR shall not be measured in the transmission gap. The reference point for the SIR measurements shall be the Rx antenna connector. If the radio link set contains more than one radio link, the reported value shall be the linear summation of the SIR from each radio link of the radio link set. If Rx diversity is used in the Node B for a cell, the SIR for a radio link shall be the linear summation of the SIR from each Rx antenna for that radio link. When cell portions are defined in the cell, the SIR measurement shall be possible in each cell portion.  where:  RSCP = Received Signal Code Power, unbiased measurement of the received power on one code.  ISCP = Interference Signal Code Power, the interference on the received signal.  SF=The spreading factor used on the DPCCH.  Type 2:  Signal to Interference Ratio, is defined as: (RSCP/ISCP)SF. The measurement shall be performed on the PRACH control part. The reference point for the SIR measurements shall be the Rx antenna connector. When cell portions are defined in the cell, the SIR measurement shall be possible in each cell portion.  where:  RSCP = Received Signal Code Power, unbiased measurement of the received power on the code.  ISCP = Interference Signal Code Power, the interference on the received signal.  SF=The spreading factor used on the control part of the PRACH. |

### 5.2.3 SIRerror

|  |  |
| --- | --- |
| **Definition** | SIRerror = SIR – SIRtarget\_ave, where:  SIR = the SIR measured by UTRAN, defined in section 5.2, given in dB.  SIRtarget\_ave = the SIRtarget averaged over the same time period as the SIR used in the SIRerror calculation. In compressed mode SIRtarget=SIRcm\_target shall be used when calculating SIRtarget\_ave. In compressed mode the SIRtarget\_ave shall not be calculated over the transmission gap. The averaging of SIRtarget shall be made in a linear scale and SIRtarget\_ave shall be given in dB. |

### 5.2.4 Transmitted carrier power

|  |  |
| --- | --- |
| **Definition** | Transmitted carrier power, is the ratio between the total transmitted power on one DL carrier from one UTRAN access point, and the maximum transmission power possible to use on that DL carrier at this moment of time. Total transmission power is the mean power [W] on one carrier from one UTRAN access point. Maximum transmission power is the mean power [W] on one carrier from one UTRAN access point when transmitting at the configured maximum power for the cell. Measurement shall be possible on any carrier transmitted from the UTRAN access point. The reference point for the transmitted carrier power measurement shall be the Tx antenna connector. In case of Tx diversity the transmitted carrier power is the ratio between the sum of the total transmitted powers of all branches and the maximum transmission power. When cell portions are defined in the cell, the transmitted carrier power for each cell portion shall be measured and reported to higher layers. |

### 5.2.5 Transmitted code power

|  |  |
| --- | --- |
| **Definition** | Transmitted code power, is the transmitted power on one channelisation code on one given scrambling code on one given carrier. For DPCH, measurement shall be possible on the DPCCH-field of any dedicated radio link transmitted from the UTRAN access point and shall reflect the power on the pilot bits of the DPCCH-field, except for the downlink DPCH slot formats 17 and 18, in which case the measurement shall be possible on the TPC-field and shall reflect the power on the TPC bits. For F-DPCH, measurement shall be possible on the TPC-field and shall reflect the power on the TPC bits. When measuring the transmitted code power in compressed mode all slots shall be included in the measurement, e.g. also the slots in the transmission gap shall be included in the measurement. The reference point for the transmitted code power measurement shall be the Tx antenna connector. In case of Tx diversity the transmitted code power for each branch shall be measured and summed together in [W]. |

### 5.2.6 Transport channel BER

|  |  |
| --- | --- |
| **Definition** | The transport channel BER is an estimation of the average bit error rate (BER) of the DPDCH data of a Radio Link Set. The transport channel (TrCH) BER is measured from the data considering only non-punctured bits at the input of the channel decoder in Node B. It shall be possible to report an estimate of the transport channel BER for a TrCH after the end of each TTI of the TrCH. The reported TrCH BER shall be an estimate of the BER during the latest TTI for that TrCH. |

### 5.2.7 Physical channel BER

|  |  |
| --- | --- |
| **Definition** | The Physical channel BER is an estimation of the average bit error rate (BER) on the DPCCH of a Radio Link Set. An estimate of the Physical channel BER shall be possible to be reported after the end of each TTI of any of the transferred TrCHs. The reported physical channel BER shall be an estimate of the BER averaged over the latest TTI of the respective TrCH. |

### 5.2.8 Round trip time

|  |  |
| --- | --- |
| **Definition** | Round trip time (RTT), is defined as  RTT = TRX – TTX, where  TTX = The time of transmission of the beginning of a downlink DPCH or F-DPCH frame to a UE. The reference point for TTX shall be the Tx antenna connector.  TRX = The time of reception of the beginning (the first detected path, in time) of the corresponding uplink DPCCH frame from the UE. The reference point for TRX shall be the Rx antenna connector.  Measurement shall be possible on DPCH or F-DPCH for each RL transmitted from an UTRAN access point and DPDCH for each RL received in the same UTRAN access point. |

### 5.2.9 UTRAN GPS Timing of Cell Frames for UE positioning

|  |  |
| --- | --- |
| **Definition** | TUTRAN-GPS is defined as the time of the occurrence of a specified UTRAN event according to GPS Time Of Week. The specified UTRAN event is the beginning of the transmission of a particular frame in the cell. The reference point for TUTRAN-GPS shall be the Tx antenna connector. |

### 5.2.10 PRACH Propagation delay

|  |  |
| --- | --- |
| **Definition** | Propagation delay is defined as one-way propagation delay as measured during PRACH access:  PRACH :  Propagation delay = (TRX – TTX – 2560)/2, where:  TTX = The transmission time of AICH access slot (n-2-AICH transmission timing), where 0(n-2-AICH Transmission Timing)14 and AICH\_Transmission\_Timing can have values 0 or 1. The reference point for TTX shall be the Tx antenna connector.  TRX = The time of reception of the beginning (the first detected path, in time) of the PRACH message from the UE at PRACH access slot n. The reference point for TRX shall be the Rx antenna connector. |

### 5.2.11 Acknowledged PRACH preambles

|  |  |
| --- | --- |
| **Definition** | The Acknowledged PRACH preambles measurement is defined as the total number of acknowledged PRACH preambles per access frame per PRACH. This is equivalent to the number of positive acquisition indicators transmitted per access frame per AICH. |

### 5.2.12 Void

### 5.2.13 Void

### 5.2.14 SFN-SFN observed time difference

|  |  |
| --- | --- |
| **Definition** | The relative timing difference between cell j and cell i, defined as TCPICHRxj - TCPICHRxi, where:  TCPICHRxj is the time when the LMU receives the beginning of one Primary CPICH frame from cell j and  TCPICHRxi is the time when the LMU receives the beginning of the Primary CPICH frame from cell i that is closest in time to the beginning of Primary CPICH frame received from cell j.  The reference point for the measurements shall be the Rx antenna connector. |

### 5.2.15 Transmitted carrier power of all codes not used for HS-PDSCH, HS-SCCH, E-AGCH, E-RGCH or E-HICH transmission

|  |  |
| --- | --- |
| **Definition** | Transmitted carrier power of all codes not used for HS-PDSCH, HS-SCCH, E-AGCH, E-RGCH or E-HICH transmission is the ratio between the total transmitted power of all codes not used for HS-PDSCH, HS-SCCH, E-AGCH, E-RGCH or E-HICH transmission on one DL carrier from one UTRAN access point, and the maximum transmission power possible to use on that DL carrier at this moment of time. Total transmission power of all codes not used for HS-PDSCH, HS-SCCH, E-AGCH, E-RGCH or E-HICH transmission is the mean power [W] of all codes not used for HS-PDSCH, HS-SCCH, E-AGCH, E-RGCH or E-HICH transmission on one carrier from one UTRAN access point. Maximum transmission power is the mean power [W] on one carrier from one UTRAN access point when transmitting at the configured maximum power for the cell. The measurement shall be possible on any carrier transmitted from the UTRAN access point. The reference point for the measurement shall be the Tx antenna connector. In case of Tx diversity the measurement is the ratio between the sum of the total transmitted powers of all codes not used for HS-PDSCH, HS-SCCH, E-AGCH, E-RGCH or E-HICH transmission of all branches and the maximum transmission power. When cell portions are defined in the cell, the measurement shall be performed and reported to higher layers for each cell portion. |

### 5.2.16 DL Transmission Branch Load

|  |  |
| --- | --- |
| **Definition** | The 'DL transmission branch load' is the maximum of the transmission branch loads calculated for each branch.  A 'transmission branch load' is the ratio between the total transmitted power [W] on the considered branch and the 'maximum DL branch capability' on this branch.  The 'maximum DL branch capability' defines the maximum transmission power possible to use on that branch.  The reference point for the transmission branch load measurement shall be the TX antenna connector. |

### 5.2.17 Received scheduled E-DCH power share (RSEPS)

|  |  |
| --- | --- |
| **Definition** | The 'Received scheduled E-DCH power share' is defined as a report of 2 values for a considered cell:  1. RSEPS: defined as a quotient:  sum of all scheduled E-DPCCH and E-DPDCH power contributions determined in the RSEPS measurement period T=t2-t1>0 for all UEs for which this cell is the serving E-DCH cell  divided by  the corresponding received total wideband power value determined for this cell during T.  2. RTWP\*: This is the received total wideband power (RTWP) measured for this cell as defined in section 5.2.1 but determined for the same time period T starting at t1 and ending at t2 during which RSEPS is determined.  The reference point for the RSEPS and RTWP\* measurements shall be the Rx antenna connector.  When cell portions are defined in the cell, RSEPS (and RTWP\*) shall be measured for each cell portion.  The sum in the numerator of RSEPS is determined under the following conditions:  - The contributions are summed up TTI wise and only TTIs which are ending between the time instants t1 and t2 are considered.  - In case a UE has not only a radio link to the considered cell but also other radio links to the same Node B ('softer handover'): It is allowed to take into account the power value combined for these radio links of the same Node B and divided by the number of combined radio links.  Note: For improved measurement performance it is possible to consider only the power contribution determined for the considered cell. |

### 5.2.18 UTRAN GANSS Timing of Cell Frames for UE positioning

|  |  |
| --- | --- |
| **Definition** | TUTRAN-GANSS is defined as the time of the occurrence of a specified UTRAN event according to GANSS Time Of Day. The specified UTRAN event is the beginning of the transmission of a particular frame in the cell. The reference point for TUTRAN-GANSS shall be the Tx antenna connector. |

# 6 Measurements for UTRA FDD

## 6.1 UE measurements

### 6.1.1 Compressed mode

#### 6.1.1.1 Use of compressed mode for monitoring

On command from the UTRAN, a UE shall monitor cells on other FDD frequencies and on other modes and radio access technologies that are supported by the UE (i.e. TDD, GSM, E-UTRA). To allow the UE to perform measurements, UTRAN shall command that the UE enters in compressed mode, depending on the UE capabilities.

The UE capabilities define whether a UE requires compressed mode in order to monitor cells on other FDD frequencies and on other modes and radio access technologies. UE capabilities indicate the need for compressed mode separately for the uplink and downlink and for each mode, radio access technology and frequency band.

A UE shall support compressed mode for all cases for which the UE indicates that compressed mode is required.

A UE does not need to support compressed mode for cases for which the UE indicates that compressed mode is not required. For these cases, the UE shall support an alternative means of making the measurements.

The UE shall support one single measurement purpose for one transmission gap pattern sequence. The measurement purpose of the transmission gap pattern sequence is signalled by higher layers.

The following subclause provides rules to parameterise the compressed mode.

#### 6.1.1.2 Parameterisation of the compressed mode

In response to a request from higher layers, the UTRAN shall signal to the UE the compressed mode parameters.

A transmission gap pattern sequence consists of consecutive occurrences of transmission gap pattern 1, where transmission gap pattern 1 consists of one or two transmission gaps. See figure 1.

The following parameters characterise a transmission gap pattern:

- TGSN (Transmission Gap Starting Slot Number): A transmission gap pattern begins in a radio frame, henceforward called first radio frame of the transmission gap pattern, containing at least one transmission gap slot. TGSN is the slot number of the first transmission gap slot within the first radio frame of the transmission gap pattern;

- TGL1 (Transmission Gap Length 1): This is the duration of the first transmission gap within the transmission gap pattern, expressed in number of slots;

- TGL2 (Transmission Gap Length 2): This is the duration of the second transmission gap within the transmission gap pattern, expressed in number of slots. If this parameter is not explicitly set by higher layers, then TGL2 = TGL1;

- TGD (Transmission Gap start Distance): This is the duration between the starting slots of two consecutive transmission gaps within a transmission gap pattern, expressed in number of slots. The resulting position of the second transmission gap within its radio frame(s) shall comply with the limitations of [2]. If this parameter is not set by higher layers, then there is only one transmission gap in the transmission gap pattern;

- TGPL1 (Transmission Gap Pattern Length): This is the duration of transmission gap pattern 1, expressed in number of frames;

The following parameters control the transmission gap pattern sequence start and repetition:

- TGPRC (Transmission Gap Pattern Repetition Count): This is the number of transmission gap patterns within the transmission gap pattern sequence;

- TGCFN (Transmission Gap Connection Frame Number): This is the CFN of the first radio frame of the first pattern 1 within the transmission gap pattern sequence.

In addition to the parameters defining the positions of transmission gaps, each transmission gap pattern sequence is characterised by:

- UL/DL compressed mode selection: This parameter specifies whether compressed mode is used in UL only, DL only or both UL and DL;

- UL compressed mode method: The methods for generating the uplink compressed mode gap are spreading factor division by two or higher layer scheduling and are described in [2]. This parameter does not impact the compressed mode method used when DL\_DCH\_FET\_Config is configured by higher layers;

- DL compressed mode method: The methods for generating the downlink compressed mode gap are spreading factor division by two or higher layer scheduling and are described in [2]. This parameter does not impact the compressed mode method used when DL\_DCH\_FET\_Config is configured by higher layers;

- downlink frame type: This parameter defines if frame structure type 'A' or 'B' shall be used in downlink compressed mode. The frame structures are defined in [2];

- scrambling code change: This parameter indicates whether the alternative scrambling code is used for compressed mode method 'SF/2'. Alternative scrambling codes are described in [3];

- RPP: Recovery Period Power control mode specifies the uplink power control algorithm applied during recovery period after each transmission gap in compressed mode. RPP can take 2 values (0 or 1). The different power control modes are described in [4];

- ITP: Initial Transmit Power mode selects the uplink power control method to calculate the initial transmit power after the gap. ITP can take two values (0 or 1) and is described in [4].

The UE shall support simultaneous compressed mode pattern sequences which can be used for different measurements. The following measurement purposes can be signalled from higher layers:

- FDD

- TDD

- GSM carrier RSSI measurement

- Initial BSIC identification

- BSIC re-confirmation

- E-UTRA.

The UE shall support one compressed mode pattern sequence for each measurement purpose while operating in FDD mode, assuming the UE needs compressed mode to perform the respective measurement. In case the UE supports several of the measurement purposes, it shall support in parallel one compressed mode pattern sequence for each supported measurement purpose where the UE needs compressed mode to perform the measurement. The capability of the UE to operate in compressed mode in uplink and downlink is given from the UE capabilities.

The GSM measurements Initial BSIC identification and BSIC re-confirmation are defined in [20].

Higher layers will ensure that the compressed mode gaps do not overlap and are not scheduled to overlap the same frame. The behaviour when an overlap occurs is described in [11]. UE is not required to support two compressed mode gaps in a frame.

In all cases, higher layers have control of individual UE parameters. Any pattern sequence can be stopped on higher layers' command.

The parameters TGSN, TGL1, TGL2, TGD, TGPL1, TGPRC and TGCFN shall all be integers.



Figure 1: Illustration of compressed mode pattern parameters

Annex A (informative):  
Change history

| Change history | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Date** | **TSG #** | **TSG Doc.** | **CR** | **Rev** | **Subject/Comment** | **Old** | **New** |
| 14/01/00 | RAN\_05 | RP-99590 | - |  | Approved at TSG RAN #5 and placed under Change Control | - | 3.0.0 |
| 14/01/00 | RAN\_06 | RP-99688 | 001 | 3 | Clarifications for compressed mode parameters | 3.0.0 | 3.1.0 |
| 14/01/00 | RAN\_06 | RP-99689 | 002 | - | Definition of PCCPCH RSCP | 3.0.0 | 3.1.0 |
| 14/01/00 | RAN\_06 | RP-99689 | 003 | - | Definition of observed time difference to GSM cell | 3.0.0 | 3.1.0 |
| 14/01/00 | RAN\_06 | RP-99688 | 004 | - | Measurements are done on Primary CPICH | 3.0.0 | 3.1.0 |
| 14/01/00 | RAN\_06 | RP-99689 | 005 | 1 | Physical channel BER on DPCCH | 3.0.0 | 3.1.0 |
| 14/01/00 | RAN\_06 | RP-99688 | 006 | - | Definition of SIR measurement | 3.0.0 | 3.1.0 |
| 14/01/00 | RAN\_06 | RP-99689 | 007 | 2 | Ranges and resolution of timing measurements | 3.0.0 | 3.1.0 |
| 14/01/00 | RAN\_06 | RP-99688 | 009 | 2 | Range and resolution for RF related measurements | 3.0.0 | 3.1.0 |
| 14/01/00 | RAN\_06 | RP-99689 | 010 | 2 | New subclauses: 5.1.15 - UE GPS Timing of Cell Frames for LCS; 5.2.8 UTRAN GPS Timing of Cell Frames for LCS | 3.0.0 | 3.1.0 |
| 14/01/00 | RAN\_06 | RP-99688 | 011 | - | Removal of Annex A from TS 25.215 | 3.0.0 | 3.1.0 |
| 14/01/00 | RAN\_06 | RP-99688 | 013 | - | Definition of Transmitted code power | 3.0.0 | 3.1.0 |
| 14/01/00 | RAN\_06 | RP-99688 | 014 | 2 | Range and resolution of BLER measurements | 3.0.0 | 3.1.0 |
| 14/01/00 | RAN\_06 | RP-99688 | 015 | 2 | Range and resolution of BER measurements | 3.0.0 | 3.1.0 |
| 14/01/00 | RAN\_06 | RP-99688 | 020 | - | Correction of SFN-SFN observed time difference | 3.0.0 | 3.1.0 |
| 14/01/00 | RAN\_06 | RP-99688 | 021 | 1 | CFN-SFN measurement with compressed mode | 3.0.0 | 3.1.0 |
| 14/01/00 | - | - | - |  | Change history was added by the editor | 3.1.0 | 3.1.1 |
| 31/03/00 | RAN\_07 | RP-000066 | 024 | 1 | Definition of Transmitted carrier power | 3.1.1 | 3.2.0 |
| 31/03/00 | RAN\_07 | RP-000066 | 025 | - | Clarification of Observed time difference to GSM cell | 3.1.1 | 3.2.0 |
| 31/03/00 | RAN\_07 | RP-000066 | 027 | - | Naming of BER/BLER mapping | 3.1.1 | 3.2.0 |
| 31/03/00 | RAN\_07 | RP-000066 | 028 | - | Minor corrections in TS 25.215 | 3.1.1 | 3.2.0 |
| 31/03/00 | RAN\_07 | RP-000066 | 029 | - | Re-definition of timing measurements | 3.1.1 | 3.2.0 |
| 31/03/00 | RAN\_07 | RP-000066 | 030 | 2 | Mapping of timing measurements | 3.1.1 | 3.2.0 |
| 31/03/00 | RAN\_07 | RP-000066 | 031 | - | Removal of note in Round trip time measurement | 3.1.1 | 3.2.0 |
| 31/03/00 | RAN\_07 | RP-000066 | 033 | - | Removal of fixed gap position in 25.215 | 3.1.1 | 3.2.0 |
| 31/03/00 | RAN\_07 | RP-000066 | 036 | 4 | Corrections to 25.215 compressed mode parameter list | 3.1.1 | 3.2.0 |
| 31/03/00 | RAN\_07 | RP-000066 | 037 | 3 | Definition and range of physical channel BER | 3.1.1 | 3.2.0 |
| 31/03/00 | RAN\_07 | RP-000066 | 040 | - | Clarification of CPICH measurements in Tx diversity | 3.1.1 | 3.2.0 |
| 31/03/00 | RAN\_07 | RP-000066 | 042 | 1 | UTRAN RSSI measurement | 3.1.1 | 3.2.0 |
| 31/03/00 | RAN\_07 | RP-000066 | 043 | 1 | UTRAN Propagation delay | 3.1.1 | 3.2.0 |
| 31/03/00 | RAN\_07 | RP-000066 | 044 | 2 | Correction to subclauses: 5.1.15 UE GPS Timing of Cell Frames for LCS; 5.2.8 UTRAN GPS Timing of Cell Frames for LCS, including timing mapping | 3.1.1 | 3.2.0 |
| 31/03/00 | RAN\_07 | RP-000066 | 047 | - | Removal of RSCP measurement | 3.1.1 | 3.2.0 |
| 31/03/00 | RAN\_07 | RP-000066 | 048 | - | UE BER measurement removal and clarification for use of uplink compressed mode | 3.1.1 | 3.2.0 |
| 26/06/00 | RAN\_08 | RP-000270 | 049 | 1 | Propagation delay for PCPCH | 3.2.0 | 3.3.0 |
| 26/06/00 | RAN\_08 | RP-000270 | 050 | 1 | Maximum number of simultaneous compressed mode pattern sequences | 3.2.0 | 3.3.0 |
| 26/06/00 | RAN\_08 | RP-000270 | 051 | 1 | Clarification of Physical channel BER | 3.2.0 | 3.3.0 |
| 26/06/00 | RAN\_08 | RP-000270 | 052 | - | Clarification of transmitted code power | 3.2.0 | 3.3.0 |
| 26/06/00 | RAN\_08 | RP-000270 | 053 | - | Editorial correction in TS 25.215 | 3.2.0 | 3.3.0 |
| 26/06/00 | RAN\_08 | RP-000270 | 055 | - | Proposed CR for Measurements of RACH in FDD | 3.2.0 | 3.3.0 |
| 26/06/00 | RAN\_08 | RP-000270 | 056 | - | Proposed CR for Measurements of CPCH in FDD | 3.2.0 | 3.3.0 |
| 26/06/00 | RAN\_08 | RP-000270 | 057 | - | Transfer of information from TS 25.212 table 9 to TS 25.215 | 3.2.0 | 3.3.0 |
| 26/06/00 | RAN\_08 | RP-000270 | 058 | - | Correction to CM parameter list | 3.2.0 | 3.3.0 |
| 26/06/00 | RAN\_08 | RP-000270 | 062 | - | Clarification of radio link measurements in compressed mode | 3.2.0 | 3.3.0 |
| 26/06/00 | RAN\_08 | RP-000270 | 063 | - | Clarification of the Transmitted code power measurement in Tx diversity | 3.2.0 | 3.3.0 |
| 26/06/00 | RAN\_08 | RP-000270 | 064 | 1 | Removal of Range/mapping | 3.2.0 | 3.3.0 |
| 26/06/00 | RAN\_08 | RP-000270 | 066 | - | Removal of UTRAN TrCH BLER measurement | 3.2.0 | 3.3.0 |
| 23/09/00 | RAN\_09 | RP-000343 | 067 | - | Insertion of UTRAN SIRerro measurement in 25.215 | 3.3.0 | 3.4.0 |
| 23/09/00 | RAN\_09 | RP-000343 | 068 | - | Reporting of UTRAN Transmitted carrier power | 3.3.0 | 3.4.0 |
| 23/09/00 | RAN\_09 | RP-000343 | 070 | - | Clarification of UTRAN SIR measurement | 3.3.0 | 3.4.0 |
| 23/09/00 | RAN\_09 | RP-000343 | 071 | - | Clarification of first significant path | 3.3.0 | 3.4.0 |
| 23/09/00 | RAN\_09 | RP-000343 | 072 | - | Clarification of radio link set as the measured object | 3.3.0 | 3.4.0 |
| 15/12/00 | RAN\_10 | RP-000541 | 069 | 3 | Support of parallel compressed mode patterns | 3.4.0 | 3.5.0 |
| 15/12/00 | RAN\_10 | RP-000541 | 074 | 1 | Clarification of SIRerror measurement during compressed mode | 3.4.0 | 3.5.0 |
| 15/12/00 | RAN\_10 | RP-000541 | 075 | 2 | Definition of UTRAN RSSI | 3.4.0 | 3.5.0 |
| 15/12/00 | RAN\_10 | RP-000541 | 076 | 1 | Clarification of GPS timing measurements | 3.4.0 | 3.5.0 |
| 15/12/00 | RAN\_10 | RP-000541 | 077 | 2 | Clarification of reference point for UE/UTRAN measurements | 3.4.0 | 3.5.0 |
| 15/12/00 | RAN\_10 | RP-000541 | 078 | 1 | Correction to measurement "Rx-Tx time difference" | 3.4.0 | 3.5.0 |
| 15/12/00 | RAN\_10 | RP-000541 | 080 | 1 | Clarifications to compressed mode usage | 3.4.0 | 3.5.0 |
| 16/03/01 | RAN\_11 | - | - | - | Approved as Release 4 specification (v4.0.0) at TSG RAN #11 | 3.5.0 | 4.0.0 |
| 16/03/01 | RAN\_11 | RP-010061 | 079 | 2 | Correction of the observed time difference to GSM measurement | 3.5.0 | 3.6.0 |
| 16/03/01 | RAN\_11 | RP-010061 | 081 | - | Removal of UE SIR measurement | 3.5.0 | 3.6.0 |
| 16/03/01 | RAN\_11 | RP-010061 | 082 | 1 | Correction of GSM reference | 3.5.0 | 3.6.0 |
| 16/03/01 | RAN\_11 | RP-010061 | 083 | - | Correction of GPS Timing measurement | 3.5.0 | 3.6.0 |
| 16/03/01 | RAN\_11 | RP-010061 | 086 | - | Correction on transport channel BLER | 3.5.0 | 3.6.0 |
| 16/03/01 | RAN\_11 | RP-010072 | 085 | - | RTD measurement in UTRAN for FDD | 3.5.0 | 4.0.0 |
| 15/06/01 | RAN\_12 | RP-010335 | 088 | - | Renaming of LCS measurements | 4.0.0 | 4.1.0 |
| 15/06/01 | RAN\_12 | RP-010456 | 090 | 2 | Correction the TrCH BLER measurement | 4.0.0 | 4.1.0 |
| 21/09/01 | RAN\_13 | RP-010521 | 096 | - | Removal of the BLER measurement of the BCH | 4.1.0 | 4.2.0 |
| 14/12/01 | RAN\_14 | RP-010740 | 098 | - | Clarification of internal measurements | 4.2.0 | 4.3.0 |
| 14/12/01 | RAN\_14 | RP-010740 | 103 | - | Clarification of P-CCPCH RSCP in 25.215 | 4.2.0 | 4.3.0 |
| 14/12/01 | RAN\_14 | RP-010740 | 105 | - | Revised definitions of CPICH Ec/No and UTRA carrier RSSI | 4.2.0 | 4.3.0 |
| 14/12/01 | RAN\_14 | RP-010745 | 099 | 2 | UE GPS code phase measurement | 4.2.0 | 4.3.0 |
| 14/12/01 | RAN\_14 | RP-010745 | 106 | 1 | UTRAN SFN-SFN observed time difference measurement | 4.2.0 | 4.3.0 |
| 08/03/02 | RAN\_15 | RP-020245 | 114 | 3 | Clarification of UE measurements Applicability | 4.3.0 | 4.4.0 |
| 08/03/02 | RAN\_15 | RP-020048 | 116 | - | Correction to the definition of UTRAN GPS timing of cell frames for UE positioning | 4.3.0 | 4.4.0 |
| 08/03/02 | RAN\_15 | RP-020048 | 117 | - | Correction to the definition of UE GPS timing of cell frames for UE positioning | 4.3.0 | 4.4.0 |
| 08/03/02 | RAN\_15 | RP-020231 | 111 | 1 | Removal of channel coding option "no coding" for FDD | 4.3.0 | 4.4.0 |
| 08/03/02 | RAN\_15 | - | - | - | Raised up to v5.0.0 together with other specs. | 4.4.0 | 5.0.0 |
| 18/09/02 | RAN\_17 | RP-020530 | 119 | 4 | Transmitted carrier power measurement correction | 5.0.0 | 5.1.0 |
| 18/09/02 | RAN\_17 | RP-020575 | 121 | - | Measurements for observed time difference to GSM cell | 5.0.0 | 5.1.0 |
| 18/09/02 | RAN\_17 | RP-020575 | 130 | - | Compressed mode limitation | 5.0.0 | 5.1.0 |
| 18/09/02 | RAN\_17 | RP-020558 | 128 | - | Correction of UE SFN-SFN type 1 measurement | 5.0.0 | 5.1.0 |
| 21/12/02 | RAN\_18 | RP-020842 | 131 | 1 | Received Total Wide Band Power Measurement Definition | 5.1.0 | 5.2.0 |
| 26/03/03 | RAN\_19 | RP-030017 | 133 | 3 | Correction of UTRAN SIR measurement definition | 5.2.0 | 5.3.0 |
| 26/03/03 | RAN\_19 | RP-030081 | 134 | 1 | Non-HSDPA power measurement | 5.2.0 | 5.3.0 |
| 23/06/03 | RAN\_20 | RP-030270 | 142 | - | Correction of transmitted carrier power definition in case of Tx diversity | 5.3.0 | 5.4.0 |
| 23/06/03 | RAN\_20 | RP-030274 | 143 | - | Correction of transmitted carrier power of all codes not used for HS-PDSCH or HS-SCCH transmission definition in case of Tx diversity | 5.3.0 | 5.4.0 |
| 22/09/03 | RAN\_21 | RP-030452 | 144 | 1 | Beamforming Enhancement related measurements | 5.4.0 | 5.5.0 |
| 07/01/04 | RAN\_22 | - | - | - | Approved to promote to a Release 6 TS and created for M.1457 update | 5.5.0 | 6.0.0 |
| 07/01/04 | RAN\_22 | RP-030726 | 145 | 2 | Beamforming Enhancement related measurements | 5.5.0 | 6.0.0 |
| 13/12/04 | RAN\_26 | RP-040449 | 149 | 1 | Introduction of E-DCH | 6.0.0 | 6.1.0 |
| 14/03/05 | RAN\_27 | RP-050050 | 147 | 4 | Introduction of 'DL Transmission Branch Load' measurement | 6.1.0 | 6.2.0 |
| 14/03/05 | RAN\_27 | RP-050038 | 153 | 1 | Removal of TGPL2 | 6.1.0 | 6.2.0 |
| 14/03/05 | RAN\_27 | RP-050092 | 154 | - | Clarification of the cell on SFN-SFN observed time difference | 6.1.0 | 6.2.0 |
| 14/03/05 | RAN\_27 | RP-050088 | 155 | - | Introduction of F-DPCH without pilot field | 6.1.0 | 6.2.0 |
| 16/06/05 | RAN\_28 | RP-050250 | 161 | - | Feature Clean Up: Removal of "CPCH" | 6.2.0 | 6.3.0 |
| 16/06/05 | RAN\_28 | RP-050245 | 163 | - | Feature Clean Up: Removal of observed time difference to GSM cell measurement | 6.2.0 | 6.3.0 |
| 16/06/05 | RAN\_28 | RP-050249 | 165 | - | Feature clean up: Removal of the 'compressed mode by puncturing' | 6.2.0 | 6.3.0 |
| 26/09/05 | RAN\_29 | RP-050453 | 0166 | 1 | UE power headroom measurement | 6.3.0 | 6.4.0 |
| 26/09/05 | RAN\_29 | RP-050440 | 0167 | - | Non-HS power measurement | 6.3.0 | 6.4.0 |
| 20/03/06 | RAN\_31 | - | - | - | Creation of Release 7 specification (v.7.0.0) at RAN#31 | 6.4.0 | 7.0.0 |
| 29/09/06 | RAN\_33 | RP-060495 | 0170 | 3 | Introduction of a Node B measurement for E-DCH RRM | 7.0.0 | 7.1.0 |
| 30/05/07 | RAN\_36 | RP-070391 | 0172 | 5 | Clarification of UE measurement definitions for RX diversity | 7.1.0 | 7.2.0 |
| 11/09/07 | RAN\_37 | RP-070648 | 0176 | 1 | Adding GANSS related measurements in the FDD physical layer measurements | 7.2.0 | 7.3.0 |
| 27/11/07 | RAN\_38 | RP-070946 | 0177 | - | Clarification of UE measurement definitions for RX diversity | 7.3.0 | 7.4.0 |
| 04/03/08 | RAN\_39 | - | - | - | Release 8 version further to RAN\_39 decision | 7.4.0 | 8.0.0 |
| 28/05/08 | RAN\_40 | RP-080436 | 188 | - | E-UTRA measurements for UTRA – E-UTRA interworking | 8.0.0 | 8.1.0 |
| 09/09/08 | RAN\_41 | RP-080672 | 189 | - | UPH measurement support for Enhanced Uplink for CELL\_FACH state | 8.1.0 | 8.2.0 |
| 09/09/08 | RAN\_41 | RP-080666 | 190 | - | Modification of RSRQ and removal of RSSI | 8.1.0 | 8.2.0 |
| 09/09/08 | RAN\_41 | RP-080666 | 192 | - | Modification of RSRP definition | 8.1.0 | 8.2.0 |
| 03/03/09 | RAN\_43 | RP-090232 | 194 | 1 | RSRP and RSRQ Measurement Definitions | 8.2.0 | 8.3.0 |
| 15/09/09 | RAN\_45 | RP-090888 | 195 | 1 | Clarification on reference point of RSRP and RSRQ for EUTRA | 8.3.0 | 8.4.0 |
| 18/09/09 | RAN\_45 | - | - | - | Release 9 created further to RAN\_45 decision | 8.4.0 | 9.0.0 |
| 01/12/09 | RAN\_46 | RP-091170 | 196 | 2 | Introduction of DC-HSUPA | 9.0.0 | 9.1.0 |
| 16/03/10 | RAN\_47 | RP-100205 | 197 | 2 | Modification of RSRQ definition | 9.1.0 | 9.2.0 |
| 21/03/11 | SP\_51 | - | - | - | Release 10 created further to SP\_51 decision | 9.2.0 | 10.0.0 |
| 05/12/11 | RAN\_54 | RP-111672 | 199 | - | Introduction of Uplink Closed Loop Transmit Diversity for HSPA | 10.0.0 | 11.0.0 |
| 10/09/14 | RAN\_65 | RP-141480 | 201 | 1 | Introduction of DCH Enhancements | 11.0.0 | 12.0.0 |
| 10/09/14 | RAN\_65 | RP-141484 | 202 | 2 | Inclusion of definition of WLAN Beacon RSSI in UMTS specifications | 11.0.0 | 12.0.0 |
| 09/03/15 | RAN\_67 | RP-150361 | 200 | 2 | New E-UTRA RSRQ measurement definition | 12.0.0 | 12.1.0 |
| 07/12/15 | SP\_70 |  |  |  | Release 13 created further to SP\_70 decision | 12.1.0 | 13.0.0 |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2016-06 | RP-72 | RP-161144 | 0206 |  | F | Clarification on measuring the transmitted code power for the downlink DPCH slot formats #17 and #18 | 13.1.0 |
| 2017-03 | RP-75 | - | - | - | - | Promotion to Release 14 without technical change (MCC) | 14.0.0 |
| 2018-06 | RP-80 | - | - | - | - | Promotion to Release 15 without technical change (MCC) | 15.0.0 |
| 2020-07 | RP-88e | - | - | - | - | Upgrade to Rel-16 version without technical change | 16.0.0 |