3GPP TS 25.306 V16.1.0 (2020-09)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Radio Access Network;

UE Radio Access capabilities

(Release 16)



The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.

The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.

This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

Keywords

UMTS, radio, access

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

[http://www.3gpp.org](http://www.3gpp.org/)

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword [4](#__RefHeading___Toc52560236)

1 Scope [5](#__RefHeading___Toc52560237)

2 References [5](#__RefHeading___Toc52560238)

3 Definitions, symbols and abbreviations [6](#__RefHeading___Toc52560239)

3.1 Definitions [6](#__RefHeading___Toc52560240)

3.2 Symbols [6](#__RefHeading___Toc52560241)

3.3 Abbreviations [6](#__RefHeading___Toc52560242)

4 UE radio access capability parameters [6](#__RefHeading___Toc52560243)

4.1 PDCP parameters [7](#__RefHeading___Toc52560244)

4.2 Void [8](#__RefHeading___Toc52560245)

4.3 RLC, MAC-hs, MAC-ehs and MAC-i/is parameters [8](#__RefHeading___Toc52560246)

4.4 Void [8](#__RefHeading___Toc52560247)

4.5 PHY parameters [9](#__RefHeading___Toc52560248)

4.5.1 Transport channel parameters in downlink [9](#__RefHeading___Toc52560249)

4.5.2 Transport channel parameters in uplink [10](#__RefHeading___Toc52560250)

4.5.3 FDD Physical channel parameters in downlink [11](#__RefHeading___Toc52560251)

4.5.4 FDD physical channel parameters in uplink [16](#__RefHeading___Toc52560252)

4.5.5 TDD physical channel parameters in downlink [18](#__RefHeading___Toc52560253)

4.5.5.1 3.84 Mcps TDD and 7.68 Mcps TDD physical channel parameters in downlink [19](#__RefHeading___Toc52560254)

4.5.5.2 1.28 Mcps TDD physical channel parameters in downlink [19](#__RefHeading___Toc52560255)

4.5.6 TDD physical channel parameters in uplink [21](#__RefHeading___Toc52560256)

4.5.6.1 3.84 Mcps TDD and 7.68 Mcps TDD physical channel parameters in uplink [21](#__RefHeading___Toc52560257)

4.5.6.2 1.28 Mcps TDD physical channel parameters in uplink [22](#__RefHeading___Toc52560258)

4.5.7 RF parameters [22](#__RefHeading___Toc52560259)

4.6 Multi-mode related parameters [23](#__RefHeading___Toc52560260)

4.7 Multi-RAT related parameters [23](#__RefHeading___Toc52560261)

4.7a Security parameters [25](#__RefHeading___Toc52560262)

4.8 UE positioning related parameters [25](#__RefHeading___Toc52560263)

4.9 Measurement related capabilities (FDD only) [26](#__RefHeading___Toc52560264)

4.9a Measurement related capabilities (TDD only) [28](#__RefHeading___Toc52560265)

4.10 General capabilities [28](#__RefHeading___Toc52560266)

4.11 DL capabilities with simultaneous HS-DSCH [29](#__RefHeading___Toc52560267)

4.12 UL capabilities with simultaneous E-DCH [29](#__RefHeading___Toc52560268)

4.13 UE minimum capabilities for reception of MBMS not provided in MBSFN mode [30](#__RefHeading___Toc52560269)

4.13a UE minimum capabilities for reception of MBMS provided in MBSFN mode [34](#__RefHeading___Toc52560270)

4.14 Home Node B Inbound Mobility Related Parameters [39](#__RefHeading___Toc52560271)

4.14.1 CSG Proximity Indication Parameters [39](#__RefHeading___Toc52560272)

4.14.2 Neighbour Cell SI Acquisition Parameters [39](#__RefHeading___Toc52560273)

4.14a IMS Voice Parameters [39](#__RefHeading___Toc52560274)

4.15 UE based network performance measurements parameters [40](#__RefHeading___Toc52560275)

5 Possible UE radio access capability parameter settings [40](#__RefHeading___Toc52560276)

5.1 Value ranges [40](#__RefHeading___Toc52560277)

5.2 Reference UE radio access capability combinations [64](#__RefHeading___Toc52560278)

5.2.1 Combinations of common UE Radio Access Parameters for UL and DL [64](#__RefHeading___Toc52560279)

5.2.2 Combinations of UE Radio Access Parameters for DL [66](#__RefHeading___Toc52560280)

5.2.3 Combinations of UE Radio Access Parameters for UL [69](#__RefHeading___Toc52560281)

Annex A (informative): Change history [71](#__RefHeading___Toc52560282)

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# 1 Scope

The present document identifies the parameters of the access stratum part of the UE radio access capabilities. Furthermore, some reference configurations of these values are defined. The intention is that these configurations will be used for test specifications.

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non specific.

-- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TS 25.323: "Packet Data Convergence Protocol (PDCP) specification".

[2] 3GPP TS 34.108: "Common Test Environments for User Equipment (UE) Conformance Testing".

[3] 3GPP TS 34.123-2: "User Equipment (UE) conformance specification; Part 2: Implementation Conformance Statement (ICS) proforma specification".

[4] 3GPP TS 25.101 "UE Radio Transmission and Reception (FDD)".

[5] 3GPP TS 25.102 "UTRA (UE) TDD; Radio transmission and reception".

[6] 3GPP TS 25.215 "Physical layer; Measurements (FDD)".

[7] RFC 2507: "IP Header Compression".

[8] RFC 3095: "RObust Header Compression (ROHC): Framework and four profiles".

[9] 3GPP TS 25.321 "Medium Access Control (MAC) protocol specification".

[10] 3GPP TS 25.322 "Radio Link Control (RLC) protocol specification".

[11] 3GPP TS 25.211 "Physical channels and mapping of transport channels onto physical channels (FDD)".

[12] 3GPP TS 25.331 "Radio Resource Control (RRC); Protocol Specification".

[13] 3GPP TS 25.308 "High Speed Downlink Packet Access (HSDPA); Overall description; Stage 2".

[14] 3GPP TS 25.221 "Physical channels and mapping of transport channels onto physical channels (TDD)".

[15] RFC 4815: "RObust Header Compression (ROHC): Corrections and Clarifications to RFC 3095".

[16] 3GPP TS 25.307: " Requirement on User Equipments (UEs) supporting a release-independent frequency band".

[17] 3GPP TS 36.331: "Evolved Universal Terrestrial Radio Access (E-UTRA); Radio Resource Control (RRC); Protocol Specification".

[18] 3GPP TS 36.101: "User Equipment (UE) radio transmission and reception".

[19] 3GPP TS 25.300: "Universal Terrestrial Radio Access Network (UTRAN); General description; Stage 2".

[20] 3GPP TS 25.133: "Requirements for support of radio resource management (FDD)".

[21] 3GPP TS 25.225: "Physical layer – Measurements (TDD)".

[22] 3GPP TS 25.304: "User Equipment (UE) procedures in idle mode and procedures for cell reselection in connected mode".

[23] 3GPP TS 24.312: "Access Network Discovery and Selection Function (ANDSF) Management Object (MO)".

[24] 3GPP TS 36.133: "Evolved Universal Terrestrial Radio Access (E-UTRA); Requirements for support of radio resource management".

[25] 3GPP TS 25.214 "Physical layer procedures (FDD)".

# 3 Definitions, symbols and abbreviations

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in TR 21.905 [1].

**<defined term>**: <definition>

## 3.2 Symbols

For the purposes of the present document, the following symbols apply:

<symbol> <Explanation>

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in TR 21.905 [1].

AMD Acknowledged Mode Data

ANDSF Access Network Discovery and Selection Function

ANR Automatic Neighbour Relation

BDS BeiDou Navigation Satellite System

EGNOS European Geostationary Navigation Overlay Service

GAN Generic Access Network

GANSS Galileo and Additional Navigation Satellite Systems

IPDL Idle Period DownLink

MBS Metropolitan Beacon System

MSAS Multi-functional Satellite Augmentation System

QoE Quality of Experience

QZSS Quasi-Zenith Satellite System

rSRVCC reverse Single Radio Voice Call Continuity

SPS Semi-Persistent Scheduling

SRVCC Single Radio Voice Call Continuity

WLAN Wireless Local Area Network

# 4 UE radio access capability parameters

In the following the UE radio capability parameters are defined. When using the RRC configuration parameters, UTRAN needs to respect the UE capabilities. Only parameters for which there is a need to set different values for different UEs are considered as UE capability parameters. Therefore, the capabilities that are the same for all UEs, including baseline capabilities, are not listed here.

UTRAN needs to respect the UE capabilities when configuring the RBs. Actions in the UE when capabilities are in conflict with a UTRAN request are specified in RRC.

## 4.1 PDCP parameters

Support for RFC 2507

This parameter defines whether the UE supports header compression according to RFC 2507 as defined in [1] or not.

Support for RFC 3095

This parameter defines whether the UE supports robust header compression according to [8] and [15], as defined in [1] or not. 'IMS capable UEs supporting voice' shall support ROHC profiles 0x0000, 0x0001, 0x0002 and be able to compress and decompress headers of PDCP SDUs at a PDCP SDU rate corresponding to supported IMS voice codecs.

Support for RFC 3095 context relocation

This parameter defines whether the UE supports ROHC, [8] and [15], context relocation as defined in [1] or not.

Support for loss-less SRNS relocation

Defines whether the UE supports loss-less SRNS relocation as defined in [1] or not.

Support for lossless DL RLC PDU size change

Defines whether the UE supports lossless DL RLC PDU size change as defined in [1] or not.

Maximum header compression context space

This parameter is only applicable if the UE supports header compression according to RFC 2507. It is defined as the maximum header compression context size supported by the UE for all RFC 2507 protocol entities for all RBs. UTRAN controls that the UE capability can be fulfilled through the following parameters:

1. MAX\_HEADER;

2. TCP\_SPACE;

3. NON\_TCP\_SPACE;

The context space for a single RFC 2507 protocol entity calculates from:

(2 \* (TCP\_SPACE + 1 + NON\_ TCP\_SPACE + 1) \* MAX\_HEADER).

The following criterion must be fulfilled in the configuration:

Maximum header compression context space  sum of context spaces for all RFC 2507 protocol entities for all RBs.

Maximum number of ROHC context sessions

This parameter is only applicable if the UE supports header compression according to [8] and [15]. It is defined as the maximum number of header compression context sessions supported by the UE.

Support for Reverse Decompression

This parameter determines whether reverse decompression is supported or not and the maximum number of packets that can be reverse decompressed by the decompressor in the UE.

Support for CS voice over HSPA

Defines whether the UE is able to route CS voice (AMR and AMR WB) data over HS-DSCH and E-DCH transport channels. If the UE supports CS voice over HS-DSCH and E-DCH, then the UE shall also support HS-PDSCH and E-DPDCH in CELL\_DCH and DPCCH Discontinuous Transmission and MAC-ehs.

## 4.2 Void

## 4.3 RLC, MAC-hs, MAC-ehs and MAC-i/is parameters

Total RLC AM and MAC-hs buffer size

When HS-DSCH is not configured this is defined as the maximum total buffer size across all RLC AM entities supported by the UE. When HS-DSCH is configured this is defined as the maximum total buffer size across all MAC-hs reordering entities and all RLC AM entities supported by the UE. The memory signalled in this capability is dynamically shared by RLC AM entities and MAC-hs reordering entities at any time.

In order to evaluate memory consumption in the UE, it shall be assumed that:

- a stored AMD PDU of N octets requires a memory equal to N octets;

- a stored MAC-hs PDU of N bits requires a memory equal to (N – 10) bits.

The UE shall only consider itself in a memory shortage situation as defined in [9] [10] when the amount of stored AM RLC PDUs and MAC-hs PDUs exceeds its capability.

Maximum number of AM entities

This is defined as the maximum number of RLC AM entities supported by the UE.

Maximum RLC AM Window Size

This is defined as the maximum transmission and receiving window size of RLC AM entities supported by the UE.

Support of MAC-ehs

Defines whether the UE supports reception of MAC-ehs operation. If the UE supports MAC-ehs operation then the UE shall also support HS-PDSCH in CELL\_DCH, flexible RLC AM PDU size in downlink, octet aligned transport block table, using special value of HE field to indicate end of an SDU for RLC AM and the possibility that different HS-SCCHs can be used in contiguous TTIs.

Support of Two Logical Channels

Defines whether the UE supports an AM RLC entity configurationed with two logical channels.

Support of MAC-i/is

Defines whether the UE supports MAC-i/is operation. If the UE supports MAC-i/is operation then the UE shall also support MAC-ehs operation, E-DPDCH in CELL\_DCH and flexible RLC AM PDU size in uplink.

Support of MAC-ehs window size extension

For 1.28Mcps TDD only, this capability defines whether the UE supports MAC-ehs window size extension.

Support of UM RLC re-establishment via reconfiguration

Defines whether the UE supports UM RLC re-establishment procedure triggered by an RRC reconfiguration message.

## 4.4 Void

## 4.5 PHY parameters

### 4.5.1 Transport channel parameters in downlink

Maximum sum of number of bits of all transport blocks being received at an arbitrary time instant

NOTE 1: "Being received" refers to all bits in the active TFC within the TFCS over all simultaneous transport channels received by the UE. "Arbitrary time instant" means that the time instant corresponding to the highest sum of number of bits is relevant. This note also applies to similar parameter definitions below.

This parameter is defined as:

i(Ni)

where Ni is defined as the number of bits in transport block #i, and the sum is over all transport blocks being received at an arbitrary time instant. All transport blocks that are to be simultaneously received by the UE on DCH, FACH, PCH and DSCH transport channels are included in the parameter.

NOTE 2: A UE does not need to support a TFC within the TFCS for which the sum of *Number of Transport Blocks* \* *Transport Block size* over all simultaneous transport channels is larger than what the UE capability indicates.

This UE capability also limits the maximum number of bits before de-rate-matching as follows: The maximum number of bits before de-rate matching being received at an arbitrary time instant (DPCH, PDSCH, S-CCPCH) shall be less or equal to 6.6 times the Maximum sum of number of bits of all transport blocks being received at an arbitrary time instant.

Maximum sum of number of bits of all convolutionally coded transport blocks being received at an arbitrary time instant.

This parameter is defined similar to the parameter above, but the sum includes only transport blocks that are to be convolutionally coded.

Maximum sum of number of bits of all turbo coded transport blocks being received at an arbitrary time instant.

This parameter is defined similar to the parameter above, but the sum includes only transport blocks that are to be turbo coded.

Maximum number of simultaneous transport channels

This is defined as the maximum number of downlink Transport Channels that the UE is capable to process simultaneously, not taking into account the rate of each Transport Channel.

NOTE: The number of simultaneous transport channels affects how the total memory space and processing capacity can be shared among the transport channels. A UE does not need to support more simultaneous transport channels than the UE capability allows for.

Maximum number of simultaneous CCTrCH

This is defined as the maximum number of downlink CCTrCH that the UE is capable to process simultaneously. CCTrCH should be interpreted as consisting of DCH, FACH or DSCH.

Maximum total number of transport blocks received within TTIs that end within the same 10 ms interval

All transport blocks that are to be simultaneously received by the UE on DCH, FACH, PCH and DSCH transport channels are included in the parameter.

NOTE: Relates to processing requirements for CRC in downlink. A UE does not need to support a TFC within the TFCS for which the sum of *Number of Transport Blocks* is larger than what the UE capability indicates. In the case of several CCTrCHs, the combination of the TFCs within the respective TFCSs for simultaneous TTIs at an arbitrary time instant shall not exceed this parameter.

Maximum number of TFC

Defines the maximum number of transport format combinations the UE can store, where all transport format combinations for all downlink transport format combination sets are counted. Different channelisation code mapping shall be counted as separate TFC in case of DSCH.

Maximum number of TF

The maximum total number of downlink transport formats the UE can store, where all transport formats for all downlink transport channels are counted.

Support for turbo decoding

Defines whether turbo decoding is supported or not.

Maximum number of bits of an HS-DSCH transport block received within an HS-DSCH TTI

Defines the maximum number of bits of an HS-DSCH transport block received within an HS-DSCH TTI the UE is capable of receiving within a HS-DSCH TTI.

### 4.5.2 Transport channel parameters in uplink

Maximum sum of number of bits of all transport blocks being transmitted at an arbitrary time instant

NOTE 1: "Being transmitted" refers to all bits in the active TFC within the TFCS over all simultaneous transport channels transmitted by the UE. "Arbitrary time instant" means that the time instant corresponding to the highest sum of number of bits is relevant. This note also applies to similar parameter definitions below.

This parameter is defined as:

i(Ni)

where Ni is defined as the number of bits in transport block #i, and the sum is over all transport blocks being transmitted at an arbitrary time instant.

NOTE 2: This parameter is related to memory requirements for uplink data received from MAC before it can be transmitted over the radio interface. As shown in Figure 4.1 the worst case occurs for the maximum TTI. A UE does not need to support a TFC within the TFCS for which the sum of *Number of Transport Blocks* \* *Transport Block size* over all simultaneous transport channels is larger than what the UE capability indicates.

Maximum sum of number of bits of all convolutionally coded transport blocks being transmitted at an arbitrary time instant

This parameter is defined similar to the parameter above, but the sum includes only transport blocks that are to be convolutionally coded.

Maximum sum of number of bits of all turbo coded transport blocks being transmitted at an arbitrary time instant

This parameter is defined similar to the parameter above, but the sum includes only transport blocks that are to be turbo coded.

Maximum number of simultaneous transport channels

This is defined as the maximum number of uplink transport channels that the UE is capable to process simultaneously, not taking into account the rate of each transport channel.

NOTE: A UE does not need to support a TFC within the TFCS for which the sum of *Number of Transport Blocks* \* *Transport Block size* over all simultaneous transport channels is larger than what the UE capability indicates.

Maximum number of simultaneous CCTrCH

This parameter is applicable for TDD only. For FDD there is always only one CCTrCH at a time. The parameter is defined as the maximum number of uplink CCTrCH that the UE is capable to process simultaneously.

Maximum total number of transport blocks transmitted within TTIs that start at the same time

Defines the maximum number of transport blocks that the UE is capable to transmit within TTIs that start at the same time. An example is shown in figure 4.1.

NOTE: Relates to processing requirements for CRC in uplink.

Maximum number of TFC

Defines the maximum number of transport format combinations the UE can store, where all transport format combinations for all uplink transport format combination sets are counted.

Maximum number of TF

The maximum total number of uplink transport formats the UE can store, where all transport formats for all uplink transport channels are counted.

Support for turbo encoding

Defines whether turbo encoding is supported or not.



Figure 4.1: UE transport channel processing limitations in uplink

### 4.5.3 FDD Physical channel parameters in downlink

Maximum number of DPCH codes to be simultaneously received

Defines the number of codes the UE is capable of receiving in parallel. For DPCH in soft/softer handover, each DPCH is only calculated once in this capability. The capability does not include codes used for S-CCPCH.

Maximum number of physical channel bits received in any 10 ms interval (DPCH, S-CCPCH)

Defines the number of physical channel bits the UE is capable of receiving. For DPCH in soft/softer handover, each DPCH is only calculated once in this capability.

The number of DPCH channel bits indicates the capability of the UE when operating in non-compressed mode.

The parameter also indicates the capability of the UE to support compressed mode by spreading factor reduction as follows. The UE shall:

- for parameter values up to and including 9600 bits:

- support compressed mode by spreading factor reduction when operating at any value up to the reported capability.

- for parameter values greater than 9600 bits:

- support compressed mode by spreading factor reduction when operating at any value up to the greater of:

- half the reported capability; or

- 9600bits.

NOTE: Compressed mode by spreading factor reduction is not applicable when operating at spreading factor 4.

Support for SF 512 and 80 ms TTI for DPCH

Defines whether the UE supports spreading factor 512 and 80 ms TTI in downlink DPCH or not.

Support of HS-PDSCH

Defines whether the UE supports HS-PDSCH in CELL\_DCH state or not. If the UE supports HS-PDSCH in CELL\_DCH state then the UE shall support also F-DPCH.

Support of HS-SCCHless HS-DSCH

Defines whether the UE supports HS-PDSCH reception in CELL\_DCH without prior reception of HS-SCCH. If the UE supports HS-SCCHless HS-DSCH then the UE shall support HS-PDSCH in CELL\_DCH and E-DPDCH.

Support of HS-PDSCH in CELL\_FACH

Defines whether the UE supports HS-PDSCH in CELL\_FACH state or not. If the UE supports HS-PDSCH in CELL\_FACH then the UE shall support also HS-PDSCH in CELL\_DCH and MAC-ehs.

Support of HS-PDSCH in CELL\_PCH and URA\_PCH

Defines whether the UE supports HS-PDSCH in CELL\_PCH and URA\_PCH states or not. If the UE supports HS-PDSCH in CELL\_PCH then the UE shall support also HS-PDSCH in CELL\_FACH.

Support of Enhanced F-DPCH

Defines whether the UE supports enhanced F-DPCH operation. If the UE supports Enhanced F-DPCH then the UE shall also support HS-PDSCH in CELL\_DCH and E-DPDCH.

Maximum number of HS-DSCH codes received

Defines the maximum number of HS-DSCH codes the UE is capable of receiving. When the UE supports either MIMO or dual cell operation, this parameter defines the maximum number of HS-DSCH codes that the UE is capable of receiving per transport block.

Total number of soft channel bits in HS-DSCH

Defines the maximum number of soft channel bits over all HARQ processes. When explicit signalling is used, UTRAN configures Process Memory Size for each HARQ process so that the following criterion must be fulfilled in the configuration:

Total number of soft channel bits in HS-DSCH  sum of Process Memory Size of all the HARQ processes.

Minimum inter-TTI interval in HS-DSCH

Defines the distance from the beginning of a TTI to the beginning of the next TTI that can be assigned to the UE.

Support of Target Cell Pre-Configuration

Defines if the UE supports simultaneous HS-DSCH reception from serving cell and decoding of an HS-SCCH sent from another cell in the active set. If the UE supports Target Cell Pre-Configuration then the UE shall also support Enhanced F-DPCH.

Support of Enhanced Serving Cell Change for Event 1C

Defines if the UE supports simultaneous HS-DSCH reception from serving cell and decoding of an HS-SCCH sent from another cell in the active set when an Event 1C measurement report requesting serving HS-DSCH cell change is triggered. If the UE supports Enhanced Serving Cell Change for Event 1C then the UE shall also support Target Cell Pre-Configuration.

Support of HS-DSCH DRX operation

Defines whether the UE supports HS-DSCH DRX operation in CELL\_FACH state as defined in [13]. If the UE supports HS-DSCH DRX operation in CELL\_FACH state then the UE shall also support HS-PDSCH in CELL\_FACH.

Support for Two DRX schemes in URA\_PCH and CELL\_PCH

Defines whether UE supports Two DRX schemes in URA\_PCH and CELL\_PCH.

Support of TX Diversity on DL Control Channels by MIMO Capable UE when MIMO operation is active

Defines whether the UE supports TX diversity on DL Control Channels (HS-SCCH, F-DPCH, E-AGCH, E-HICH, E-RGCH) when MIMO is active, P-CPICH is configured on antenna 1, and S-CPICH on antenna 2.

Support for cell-specific Tx diversity configuration for dual-cell operation

Defines whether the UE supports cell specific Tx diversity configuration when configured for dual-cell operation.

Support of MIMO only with single-stream restriction

Defines whether the UE supports MIMO only with restriction to single stream operation. UE supporting this capability shall belong to any HS-DSCH physical layer category not supporting MIMO or the UE shall belong to category 17 or 18. If the UE supports MIMO only with single-stream restriction, the UE shall also support MAC-ehs.

Support of MIMO mode with four transmit antennas per band capability

Defines whether the UE supports MIMO mode with four transmit antennas in CELL\_DCH. The capability is defined per frequency band.

Support of MIMO mode with four transmit antennas operation only with dual-stream restriction

Defines whether the UE supports MIMO mode with four transmit antennas only with restriction to dual stream operation. UE supporting this capability shall belong to category 28, 30, 32, 34 or 36. If a UE supporting this capability belongs to category 34 or 36, then only up to 4 carriers can be configured with this capability. The dual-stream restriction capability shall not be signalled when UE supports either category 37 or 38. If the UE supports MIMO mode with four transmit antennas only with dual-stream restriction, the UE shall also support MAC-ehs.

Support of dual band operation

Defines whether the UE supports dual cell operation in the band combinations indicated in the Radio Access Capability Band Combination List [12]. If the UE supports dual band operation, the UE shall also support dual cell operation on adjacent frequencies.

Support for dual cell with MIMO operation in different bands

Defines whether the UE supports dual cell with MIMO operation in different bands. If the UE supports dual cell with MIMO operation in different bands, the UE shall also support dual band operation.

Support for Multiflow operation

A UE capability to receive simultaneously two HS-DSCH transport channels per carrier frequency, where the HS-DSCH transport channels may belong to the same or different Node Bs. If a UE supports Multiflow operation, it shall also support Dual Cell HSDPA operation on adjacent frequencies and the HS-DPCCH power offset extension.

Support of NodeB triggered HS-DPCCH transmission

Defines whether the UE supports NodeB triggered HS-DPCCH transmission in CELL\_FACH state. If the UE supports both HS-PDSCH in CELL\_PCH and URA\_PCH states and NodeB triggered HS-DPCCH transmission, then the UE shall also support NodeB triggered HS-DPCCH transmission in CELL\_PCH state. If the UE supports NodeB triggered HS-DPCCH transmission, then the UE shall also support Common E-DCH.

Support of HS-DSCH DRX operation with second DRX cycle

Defines whether the UE supports HS-DSCH DRX operation with second DRX cycle in CELL\_FACH state as defined in [13]. If the UE supports HS-DSCH DRX operation with second DRX cycle in CELL\_FACH state then the UE shall also support HS-PDSCH in CELL\_FACH, HS-DSCH DRX operation, and common E-DCH. If the UE supports UTRAN ANR and HS-DSCH DRX operation with second DRX cycle, then the UE shall also support measurement and logging in CELL\_FACH state when second DRX cycle is used for Automatic Neighbour Relation (ANR) in UTRAN. If the UE supports logged measurements in Idle mode and PCH States and HS-DSCH DRX operation with second DRX cycle, then the UE shall also support logged measurements in CELL\_FACH state when second DRX cycle is used in UTRAN.

Non-contiguous multi-cell

Defines whether the UE supports non-contiguous multi-cell operation on two, three or four cells with single gap in one band. If the UE supports non-contiguous multi-cell operation in a certain band, it shall also support dual cell operation on adjacent frequencies in that band.

Support of HS-DPCCH power offset extension

Defines whether the UE supports the values 9 and 10 of deltaACK, deltaNACK and deltaCQI power offset as specified in [12].

Support of STTD on DL Control Channels when Multiflow operation is active

Defines whether a Multiflow capable UE supports STTD on DL Control Channels (HS-SCCH, F-DPCH, E-AGCH, E-HICH, E-RGCH, F-TPICH) when Multiflow operation is active, as specified in [12].

Non-contiguous multi-cell with MIMO

Defines whether the UE supports non-contiguous multi-cell operation on two, three or four cells with single gap in one band with MIMO. If the UE supports non-contiguous multi-cell with MIMO, it shall also support non-contiguous multi-cell.

Support of multi-cell configuration in inter-RAT handover

Defines whether the UE supports multi-cell configuration at inter-RAT handover to UTRAN. The UE shall support it for all multi-cell capabilities supported by the UE (i.e. multi-cell operation on two or more than two cells, multi-cell operation in the band combinations indicated in the Radio Access Capability Band Combination List [12], non-contiguous multi-cell operation on two, three or four cells with single gap in one band, dual cell E-DCH), except for multi-cell operation on more than four cells.

Support of DPCCH2

Defines whether the UE supports DPCCH2 transmission in CELL\_DCH state. If the UE supports DPCCH2, it shall also support HS-PDSCH in CELL\_DCH.

Support for DCH Enhancements

Defines whether the UE supports DCH Enhancements.

Basic capability indicates that the UE supports the following sub-features in DCH enhancements ([19]):

- Basic mode of DL FET (Mode 0)

- Pilot-free DL DPCH slot formats #17 and #18

- Pseudo flexible rate matching

- Uplink DPCCH slot format #5

- Uplink DPDCH dynamic 10ms transmission

Full capability indicates that the UE supports the following sub-features in DCH enhancements ([19]):

- Basic mode of DL FET (Mode 0)

- Full mode of DL FET (Mode 1)

- Pilot-free DL DPCH slot formats #17 and #18

- Pseudo flexible rate matching and transport channel concatenation in L1

- Uplink DPCCH slot format #5 with DL FET ACK/NACK indication

- Uplink DPDCH dynamic 10ms transmission

Simultaneous support for DCH Enhancements and Compressed Mode operation

Defines whether the UE supports simultaneous operation of DCH Enhancements and Compressed Mode. If the UE supports simultaneous operation of DCH Enhancements with Full capability and Compressed Mode, then the UE shall support simultaneous operation of DCH Enhancements with Basic capability and Compressed Mode.

Simultaneous support for DCH Enhancements and DPCCH Discontinuous Transmission

Defines whether the UE supports simultaneous operation of DCH Enhancements and DPCCH Discontinuous Transmission. If the UE supports simultaneous operation of DCH Enhancements with Full capability and DPCCH Discontinuous Transmission, then the UE shall support simultaneous operation of DCH Enhancements with Basic capability and DPCCH Discontinuous Transmission.

DRX enhancements

Defines whether the UE supports DRX enhancements, as defined in subclause 6C.3 in [25], or not.

HS-DPCCH overhead reduction

Defines whether the UE supports HS-DPCCH overhead reduction for multi-RAB with DCH or not.

Support of F-TPICH feedback from the Multiflow assisting cell

Defines whether the UE supports reception of the F-TPICH feedback from the Multiflow assisting serving HS-DSCH cell. If the UE supports this feature, it shall also support uplink closed loop transmit diversity and Multiflow operation.

Support of power control algorithm 3

Defines whether the UE supports power control algorithm 3.

Support of blind HARQ retransmissions for HSDPA

Defines whether the UE supports blind HARQ retransmissions for HSDPA.

Support of HS-SCCH DRX operation

Defines whether the UE supports HS-SCCH DRX operation in CELL\_FACH state.

Support of simplified HS-SCCH type 1 operation

Defines whether the UE supports simplified HS-SCCH type 1 operation.

### 4.5.4 FDD physical channel parameters in uplink

Maximum number of DPDCH bits per 10 ms

Defines the maximum number of the DPDCH bits the UE is capable to transmit per 10 ms.

If the reported capability is lower than 9600, the number of DPDCH channel bits indicates the capability of the UE when operating in non-compressed mode; if the reported capability is equal to or greater than 9600 it indicates the maximum capability of the UE considering both compressed and non compressed mode operation.

NOTE 1: This capability combines the 'Max number of DPDCH' and 'Minimum SF' capabilities into one capability. Note that no flexibility is lost due to this, as multiple DPDCH is only used for SF = 4, i.e. when the number of DPDCH bits exceed a certain value.

NOTE 2: Compressed mode by spreading factor reduction is not applicable when operating at spreading factor 4.

Support of E-DPDCH

Defines whether the UE supports E-DPDCH in CELL\_DCH or not.

Maximum number of E-DCH codes transmitted per transport block

Defines the maximum number of E-DCH codes and spreading factors the UE is capable of transmitting per transport block. The UE can support 1, 2 or 4 E-DPDCHs using either SF=2 or/and SF=4.

Support of 2ms TTI for E-DCH

Defines whether the UE supports 2ms TTI or not.

Support of DPCCH Discontinuous Transmission

Defines whether the UE supports DPCCH Discontinuous Transmission in CELL\_DCH. If the UE supports DPCCH Discontinuous Transmission then the UE shall also support

- HS-PDSCH in CELL\_DCH

- E-DPDCH in CELL-DCH

- Uplink DRX with E-DCH start time restriction in CELL-DCH as definied in [13]

- The configuration of the Downlink DRX as definied in [13].

Support of Slot Format #4

Defines whether the UE supports slot format #4.

Support for E-DPDCH power interpolation formula

Defines whether the UE supports E-DPDCH power interpolation formula when 16QAM is not configured.

Support for E-DPCCH power boosting

Defines whether the UE supports E-DPCCH power boosting.

Support of common E-DCH

Defines whether the UE supports E-DCH enhanced random access in CELL\_FACH state and Idle mode. If the UE supports common E-DCH then the UE shall also support

- MAC-i/is

- FDD E-DCH physical layer category 2, 4, 6 or 7

- Enhanced F-DPCH

- HS-PDSCH in CELL\_FACH

Support of uplink open loop transmit diversity

Defines whether the UE supports uplink open loop transmit diversity in CELL\_DCH.

Support of uplink closed loop transmit diversity

Defines whether the UE supports uplink closed loop transmit diversity in CELL\_DCH.

Support of Common E-RGCH based interference control

Defines whether the UE supports Common E-RGCH based interference control in CELL\_FACH state. If the UE supports Common E-RGCH based interference control, then the UE shall also support Common E-DCH.

Support of Fallback to R99 PRACH

Defines whether the UE supports Fallback to R99 PRACH in CELL\_FACH state and IDLE mode. If the UE supports Fallback to R99 PRACH, then the UE shall also support Common E-DCH.

Support of Concurrent deployment

Defines whether the UE supports Concurrent deployment of 2ms and 10ms TTI in a cell in CELL\_FACH state and IDLE mode. If the UE supports Concurrent deployment of 2ms and 10ms TTI in a cell, then the UE shall also support Common E-DCH.

Support of TTI alignment and Per HARQ process

Defines whether the UE supports TTI alignment and Per HARQ process activation and de-activation in CELL\_FACH state and IDLE mode. If the UE supports TTI alignment and Per HARQ process activation and de-activation, then the UE shall also support Common E-DCH and Concurrent deployment of 2ms and 10ms TTI in a cell.

Support of Uplink MIMO

Defines whether the UE supports Uplink MIMO in CELL\_DCH. If the UE supports Uplink MIMO, it shall also support Uplink Closed Loop Transmit Diversity.

Support of Cell Reselection Indication Reporting

Defines whether the UE supports Cell Reselection Indication Reporting in CELL\_FACH state when common E-DCH resource is allocated. If the UE supports Cell Reselection Indication Reporting, then the UE shall also support Common E-RGCH based interference control or NodeB triggered HS-DPCCH transmission, or both.

Support of Serving E-DCH cell decoupling

Defines whether the UE supports a configuration in which the Serving HS-DSCH and Serving E-DCH cell are different.

Support of Radio Links without DPCH/F-DPCH

Defines whether the UE supports to not receive both DPCH and F-DPCH downlink channels from the indicated Non-serving E-DCH cell(s).

Access Groups based access control

Defines whether the UE supports network control of DTCH transmissions in CELL\_FACH and DCCH/CCCH due to uplink DTCH data transmissions in CELL\_PCH state and URA\_PCH state.

Enhanced TTI switching

Defines whether the UE supports Enhanced EUL TTI switching or not. If the UE supports Enhanced TTI switching, then the UE shall also support Enhanced UPH reporting.

Implicit Grant handling

Defines whether the UE supports handling of Implicit Grants on the Secondary Uplink frequency or not. If the UE supports Implicit Grant handling, then the UE shall also support Dual cell E-DCH operation.

DTX enhancements

Defines whether the UE supports DTX enhancements or not. If the UE supports DTX enhancements, then the UE shall also support Implicit Grant handling.

Support of Dual Cell E-DCH transmission with DPDCH

Defines whether the UE supports Dual Cell E-DCH transmission with DPDCH. If a UE supports Dual Cell E-DCH transmission with DPDCH, then the UE shall also support Dual cell E-DCH operation.

Support for Dual Band Dual Cell E-DCH operation

Defines whether the UE supports Dual Band Dual Cell E-DCH operation in the band combinations indicated in the Radio Access Capability Band Combination List [12]. If the UE supports Dual Band Dual Cell E-DCH operation, the UE shall also support dual band operation in downlink. If the UE supports Dual Band Dual Cell E-DCH operation, the UE shall also support Dual Cell E-DCH transmission.

Support of Dual Cell E-DCH operation enhancements

Defines whether the UE supports 10ms TTI on both Primary and Secondary Uplink Frequency or a combination of 2ms TTI and 10ms TTI. If the UE supports Dual Cell E-DCH operation enhancements, the UE shall also support Dual Cell E-DCH operation.

### 4.5.5 TDD physical channel parameters in downlink

#### 4.5.5.1 3.84 Mcps TDD and 7.68 Mcps TDD physical channel parameters in downlink

Maximum number of timeslots per frame

Defines the maximum number of timeslots per frame that the UE can receive.

Maximum number of physical channels per frame

This parameter defines how many physical channels can be received during one frame. The distribution of the received physical channels on the received timeslots can be arbitrary.

Minimum SF

Defines the minimum SF supported by the UE.

Support of PDSCH

Defines whether PDSCH is supported or not.

Support of HS-PDSCH

Defines whether the UE supports HS-PDSCH or not.

Maximum number of physical channels per timeslot

This parameter defines how many physical channels can be received within one timeslot.

Maximum number of HS-DSCH codes per timeslot

This is the maximum number of channelisation codes that can be used for the HS-DSCH in a given downlink timeslot. Where the parameter "Maximum number of physical channels per timeslot" is larger than "Maximum number of HS-DSCH codes per timeslot", this indicates that the UE is able to receive HS-SCCH or associated DPCH transmissions in the same timeslot as HS-PDSCHs, even if the maximum HS-DSCH code allocation for that slot is being used.

Maximum number of HS-DSCH timeslots per TTI

This is the maximum number of timeslots in a given 10 ms frame that can be used for HS-DSCH transmissions.

Maximum number of bits of an HS-DSCH transport block received within an HS-DSCH TTI

Defines maximum number of bits of an HS-DSCH transport block received within an HS-DSCH TTI the UE is capable of receiving within an HS-DSCH TTI.

Total number of soft channel bits

Defines the maximum number of soft channel bits over all HARQ processes.

#### 4.5.5.2 1.28 Mcps TDD physical channel parameters in downlink

Maximum number of timeslots per subframe

Defines the maximum number of timeslots per subframe that the UE can receive.

Maximum number of physical channels per subframe

This parameter defines how many physical channels can be received during one subframe. The distribution of the received physical channels on the received timeslots can be arbitrary.

Minimum SF

Defines the minimum SF supported by the UE.

Support of PDSCH

Defines whether PDSCH is supported or not.

Support of HS-PDSCH

Defines whether the UE supports HS-PDSCH or not.

Support of HS-PDSCH in CELL\_FACH

Defines whether the UE supports HS-PDSCH in CELL\_FACH, CELL\_PCH and URA\_PCH state or not. If the UE supports HS-PDSCH in CELL\_FACH, CELL\_PCH and URA\_PCH state then the UE shall also support:

- MAC-ehs,

- HS-PDSCH in CELL\_DCH,

- HS-PDSCH physical layer category at least 9,

- HS-DSCH DRX operation in CELL\_FACH,

- E-DCH in CELL\_FACH.

Maximum number of physical channels per timeslot

This parameter defines how many physical channels can be received within one timeslot.

Support of 8PSK

Defines whether 8PSK modulation is supported or not.

Maximum number of HS-DSCH codes per timeslot

This is the maximum number of channelisation codes that can be used for the HS-DSCH in a given downlink timeslot. Where the parameter "Maximum number of physical channels per timeslot" is larger than "Maximum number of HS-DSCH codes per timeslot", this indicates that the UE is able to receive HS-SCCH or associated DPCH transmissions in the same timeslot as HS-PDSCHs, even if the maximum HS-DSCH code allocation for that slot is being used.

Maximum number of HS-DSCH timeslots per TTI

This is the maximum number of timeslots in a given 5 ms subframe that can be used for HS-DSCH transmissions.

Maximum number of bits of an HS-DSCH transport block received within an HS-DSCH TTI

Defines maximum number of bits of an HS-DSCH transport block received within an HS-DSCH TTI the UE is capable of receiving within an HS-DSCH TTI.

Total number of soft channel bits

Defines the maximum number of soft channel bits over all HARQ processes.

Maximum number of the total HS-DSCH timeslots on the all assigned carriers per TTI (Multi-frequency HS-DSCH operation mode only)

This is the maximum number of the total timeslots of all the carriers in a given 5 ms subframe that can be used for HS-DSCH transmissions. This is used by the UE which has the multi-carrier capability.

NOTE: If it is not specified explicitly, these parameters in this section are defined for single frequency operation mode.

UE specific capability Information LCR TDD

Defines the maximum number of frequencies supported in the multi-carrier HS-DSCH transmission.

Support of SPS

Defines whether semi-persistent scheduling is supported or not on downlink and uplink.

Support of HS-SCCH/E-AGCH Discontinuous Reception

Defines whether the UE supports HS-SCCH and E-AGCH Discontinuous Reception in CELL\_DCH and CELL\_FACH state.

Support of SF Mode For HS-PDSCH dual stream

Defines which SF is supported in dual HS-PDSCH stream operation for a 1.28Mcps TDD MIMO capable UE.

Support of Enhanced TS0

Defines whether the UE supports DPCH, HS-PDSCH, HS-SCCH, E-AGCH and E-HICH reception in timeslot 0 on the secondary carriers.

Support of Non-rectangular Resource Allocation

Defines whether the UE supports non-rectangular resource allocation in CELL\_DCH on downlink and uplink.

### 4.5.6 TDD physical channel parameters in uplink

#### 4.5.6.1 3.84 Mcps TDD and 7.68 Mcps TDD physical channel parameters in uplink

Maximum Number of timeslots per frame

Defines the maximum number of timeslots per frame that the UE can transmit.

Maximum number of physical channels per timeslot

Defines the maximum number physical channels transmitted in parallel during one timeslot.

Minimum SF

Defines the minimum SF supported by the UE.

Support of PUSCH

Defines whether PUSCH is supported or not.

Support of E-PUCH

Defines whether the UE supports E-PUCH or not.

Maximum number of physical channel bits on E-PUCH that can be transmitted in a 10ms TTI

Defines the maximum number of physical channel bits, *Ndata*, that the UE is capable of transmitting on E-PUCH in a 10ms TTI.

Maximum number of bits of an E-DCH transport block that can be transmitted within a 10ms E-DCH TTI

Defines the maximum number of bits of an E-DCH transport block that the UE is capable of transmitting within a 10ms E-DCH TTI.

#### 4.5.6.2 1.28 Mcps TDD physical channel parameters in uplink

Maximum Number of timeslots per subframe

Defines the maximum number of timeslots per subframe that the UE can transmit.

Maximum number of physical channels per timeslot

Defines the maximum number of physical channels transmitted in parallel during one timeslot.

Minimum SF

Defines the minimum SF supported by the UE.

Support of PUSCH

Defines whether PUSCH is supported or not.

Support of 8PSK

Defines whether 8PSK modulation is supported or not.

Support of E-PUCH

Defines whether the UE supports E-PUCH or not.

Support of E-DCH in CELL\_FACH

Defines whether the UE supports E-DCH transmission in CELL\_FACH state and Idle mode. If the UE supports E-DCH in CELL\_FACH then the UE shall also support:

- MAC-i/is,

- E-DCH in CELL\_DCH,

- E-DCH physical layer category 3, 4, 5, or 6,

- HS-PDSCH in CELL\_FACH.

Maximum number of physical channel bits on E-PUCH that can be transmitted in a 5ms TTI

Defines the maximum number of physical channel bits, *Ndata*, that the UE is capable of transmitting on E-PUCH in a 5ms TTI.

Maximum number of bits of an E-DCH transport block that can be transmitted within a 5ms E-DCH TTI

Defines the maximum number of bits of an E-DCH transport block that the UE is capable of transmitting within a 5ms E-DCH TTI.

### 4.5.7 RF parameters

UE power class

Indicates the UE power class as defined in [4] for FDD and [5] for TDD.

Radio frequency bands

Defines the uplink and downlink frequency bands supported by the UE as defined in [4] for FDD and [5] for TDD.

UEs that support band XIX shall also support band VI.

Tx/Rx frequency separation

This parameter is only applicable for FDD. It defines the uplink/downlink frequency separations supported by the UE. The value range depends on the radio frequency band the UE supports, as defined in [4].

Support of Multiple Frequency Band Indicators

This parameter is only applicable for FDD. It indicates if the UE supports the signalling requirements of multiple radio frequency bands in a cell, as defined in [16], and if the UE understands the UARFCN signalling for all bands, that overlap with the band(s) supported by the UE, and that are defined in the earliest version of [4] that includes all UE supported bands.

## 4.6 Multi-mode related parameters

Support of UTRA FDD

Defines whether UTRA FDD is supported.

There is no explicit configuration parameter.

Support of UTRA TDD 3.84 Mcps

Defines whether UTRA TDD 3.84 Mcps is supported.

There is no explicit configuration parameter.

Support of UTRA TDD 7.68 Mcps

Defines whether UTRA TDD 7.68 Mcps is supported.

There is no explicit configuration parameter.

Support of UTRA TDD 1.28 Mcps

Defines whether UTRA TDD 1.28 Mcps is supported.

There is no explicit configuration parameter.

## 4.7 Multi-RAT related parameters

Support of GSM

Defines whether GSM is supported or not. There is a separate parameter for each GSM frequency band.

Support of multi-carrier

Defines whether multi-carrier is supported or not.

Support of UTRAN to GERAN NACC

Defines whether UTRAN to GERAN NACC is supported or not.

Support of Handover to GAN

Defines whether CS Handover to GAN is supported or not.

Support of Inter-RAT PS Handover

Defines whether Inter-RAT PS Handover to GERAN is supported or not.

Support of PS Handover to GAN

Defines whether PS Handover to GAN is supported or not.

Support of E-UTRA FDD

Defines whether E-UTRA FDD is supported or not. There is a separate parameter for each E-UTRA frequency band. If the UE supports E-UTRA FDD, it shall also support absolute priority based cell re-selection to GERAN if GERAN is supported by the UE.

Support of Inter-RAT PS Handover to E-UTRA FDD

Defines whether Inter-RAT PS Handover to E-UTRA FDD is supported or not.

Support of E-UTRA FDD measurements and reporting in CELL\_FACH

Defines whether E-UTRA measurement for CELL\_FACH for E-UTRA FDD is supported or not.

Support of E-UTRA TDD

Defines whether E-UTRA TDD is supported or not. There is a separate parameter for each E-UTRA frequency band. If the UE supports E-UTRA TDD, it shall also support absolute priority based cell re-selection to GERAN if GERAN is supported by the UE.

Support of Inter-RAT PS Handover to E-UTRA TDD

Defines whether Inter-RAT PS Handover to E-UTRA TDD is supported or not.

Support of E-UTRA TDD measurements and reporting in CELL\_FACH

Defines whether E-UTRA measurement for CELL\_FACH for E-UTRA TDD is supported or not.

Support of E-UTRA Multiple Frequency Band Indicators

This parameter is only applicable for a UE supporting E-UTRA. It indicates if the UE supports the signalling requirements of multiple radio frequency bands in a cell, as defined in [17],and if the UE understands the EARFCN signalling for all bands, that overlap with the band(s) supported by the UE, and that are defined in the earliest version of [18] that includes all UE supported bands.

Support of RAN-assisted WLAN interworking based on RAN rules

This parameter defines whether the UE supports RAN-assisted WLAN interworking based on access network selection and traffic steering rules specified in TS 25.304 [22]. A UE which supports RAN-assisted WLAN interworking based on access network selection and traffic steering rules specified in TS 25.304 [22] shall support to receive, via system information and dedicated signalling, the RAN assistance parameters relevant for those rules.

Support of RAN-assisted WLAN interworking based on ANDSF policies

This parameter defines whether the UE supports RAN-assisted WLAN interworking based on ANDSF policies specified in TS 24.312 [23]. A UE which supports RAN-assisted WLAN interworking based on ANDSF policies specified in TS 24.312 [23] shall support to receive, via system information and dedicated signalling, the RAN assistance parameters relevant for those policies.

Support of extended E-UTRA frequency priority

This parameter defines whether the UE supports extended E-UTRA frequency priority. If the UE supports extended E-UTRA frequency priority, it shall also support E-UTRA.

## 4.7a Security parameters

Ciphering algorithm capability

This capability defines the ciphering algorithms supported by the UE. In this version of the protocol, the UE shall support UEA0, UEA1 and UEA2.

Integrity protection algorithm capability

This capability defines the integrity protection algorithms supported by the UE. In this version of the protocol, the UE shall support UIA1 and UIA2.

## 4.8 UE positioning related parameters

Standalone location method(s) supported

Defines if a UE can measure its location by some means unrelated to UTRAN (e.g. if the UE has access to a standalone GPS receiver).

UE based OTDOA supported

Defines if a UE supports the OTDOA UE based schemes.

Network Assisted GPS support

Defines if a UE supports either of the two types of assisted GPS schemes, namely "Network based", "UE based", "Both", or "none".

Network Assisted GANSS support List

Defines if a UE supports assisted GANSS schemes. The GANSS gathers Galileo and Additional Navigation Satellite Systems. It defines which GANSS(s) is/are supported, and for each supported GANSS it further defines:

- the GANSS mode supported (namely "Network based", "UE based", "Both", or "none");

- the GANSS signals supported;

- the capability to perform GANSS timing of cell frames measurement;

- the capability to perform GANSS carrier phase measurement;

- the capability to support non-native assistance data choices.

Support for GPS timing of cell frames measurement

Defines if a UE has the capability to measure GPS reference time as defined in [6].

Support for IPDL

Defines if a UE has the capability to use IPDL to enhance its "SFN-SFN observed time difference –type 2" measurement.

Support for Rx-Tx time difference type 2 measurement

Defines if a UE has the capability to perform the Rx-Tx time difference type 2 measurement.

Support for UE Positioning assisted GPS measurement validity in CELL\_PCH and URA\_PCH RRC states

Defines if UE Positioning measurements using the assisted GPS method are valid in CELL\_PCH and URA\_PCH RRC states.

Support for SFN-SFN observed time difference type 2 measurement

Defines if the UE has the capability to perform the SFN-SFN observed time difference type 2 measurement.

Additional Positioning method support List

Defines if a UE supports Additional Positioning methods. It defines which Additional Positioning method(s) is/are supported, and for each supported method it further defines:

- the positioning mode supported (namely "Standalone", "UE assisted", "Both").

## 4.9 Measurement related capabilities (FDD only)

Need for downlink compressed mode

Defines whether the UE needs compressed mode in the downlink in order to perform inter-frequency or inter-RAT measurements. There are separate parameters for measurements on each UTRA mode, on each RAT, and in each frequency band.

Need for uplink compressed mode

Defines whether the UE needs compressed mode in the uplink in order to perform inter-frequency or inter-RAT measurements. There are separate parameters for measurements on each UTRA mode, on each RAT, and in each frequency band.

Support for absolute priority based cell re-selection in UTRAN

Defines whether absolute priority based cell re-selection in UTRAN is supported or not. If the UE supports absolute priority based cell re-selection in UTRAN, it shall also support absolute priority based cell re-selection to GERAN if GERAN is supported by the UE.

Adjacent Frequency measurements without compressed mode

Defines whether the UE needs compressed mode to perform measurements on an adjacent frequency, i.e. a frequency whose center is within 5MHz of the center of the currently used frequency and belongs to the same frequency band as that of the currently used frequency.

Inter-band Frequency measurements without compressed mode

Defines whether the UE needs compressed mode to perform measurements on an inter-band frequency, i.e. a frequency belonging to a frequency band in the band combinations as reported in the IE "Radio Access Capability Band Combination List" but not belonging to the same frequency band as that of the currently used frequency.

Support for System Information Block type 11bis

Defines whether the UE supports System Information Block type 11bis.

Enhanced inter-frequency measurements without compressed mode

Defines whether the UE needs compressed mode to perform measurements on two additional frequencies other than the frequency associated with the serving HS-DSCH cell, where each frequency belongs either to the frequency band of the currently used frequency or to a frequency band in the band combinations as reported in the IE "Radio Access Capability Band Combination List". The two additional frequencies to be measured without compressed mode together with currently used frequency cannot belong to more than two frequency bands.

Frequency specific compressed mode

For the dual band operation, defines whether the UE can apply compressed mode only to the frequencies associated with the secondary serving HS-DSCH cells, which are in the frequency band other than the serving HS-DSCH cell.

Frequency specific compressed mode for non-contiguous operation

For the intra-band non-contiguous operation, defines whether the UE can apply compressed mode only to the frequencies associated with the secondary serving HS-DSCH cells, which are in the block of configured carriers other than the serving HS-DSCH cell.

Extended measurements ID support

Defines whether the UE supports extended measurement identity range 17 to 32. In this release of the specification the UE shall support Extended measurements ID.

Inter-frequency detected set measurements

Defines whether the UE supports measurements of inter-frequency detected set cells. If the UE supports Inter-frequency detected set measurements then the UE shall also support Cells excluded from detected set measurements.

Inter-frequency measurements on configured carriers without compressed mode

Defines whether the UE requires compressed mode to perform measurements on the frequencies which are configured for HS-DSCH operation and associated with the secondary serving HS-DSCH cells.

Cells excluded from detected set measurements

Defines whether the UE supports exclusion of cells from intra-frequency detected set measurements. If the UE supports Inter-frequency detected set measurements, then this capability also defines whether the UE supports exclusion of cells from inter-frequency detected set measurements.

Wideband RSRQ FDD measurements

Defines whether the UE is able to perform wideband RSRQ FDD measurements.

Wideband RSRQ TDD measurements

Defines whether the UE is able to perform wideband RSRQ TDD measurements.

Event 2g reporting on a configured secondary downlink frequency

Defines whether the UE supports reporting event 2g on a configured secondary downlink frequency. If a UE supports event 2g reporting on a configured secondary downlink frequency, it shall also support Inter-frequency measurements on configured carriers without compressed mode.

Enhanced UPH reporting

Defines whether the UE supports reporting of filtered UPH measurement or not.

RRC measurement events for UPH reporting

Defines whether the UE supports RRC measurement events 6h and 6i for UPH reporting or not.

Increased UE carrier monitoring UTRA

Defines whether the UE supports increased number of UTRA carrier monitoring in connected and idle mode as defined in [20].

Increased UE carrier monitoring E-UTRA

Defines whether the UE supports increased number of E-UTRA carrier monitoring in connected and idle mode as defined in [20]. In this release of the specification, if the UE supports E-UTRA and if it is not category 0, the UE shall support Increased UE carrier monitoring E-UTRA.

Extended RSRQ lower value range

Defines whether the UE supports the extended RSRQ lower value range from -34dB to-19.5 dB in measurement configuration and reporting as specified in [24].

RSRQ measurement on all symbols

Defines whether the UE supports the RSRQ measurement on all OFDM symbols as specified in [6] and [21] and the extended RSRQ upper value range from -3dB to 2.5dB in measurement configuration and reporting as specified in [24]. If the UE supports RSRQ measurement on all OFDM symbols and Wideband RSRQ FDD or TDD measurements it shall also support the RSRQ measurement on all OFDM symbols with wider bandwidth for FDD or TDD respectively.

QoE Measurement Collection for streaming services

Defines whether the UE supports QoE Measurement Collection for streaming services.

QoE Measurement Collection for MTSI services

Defines whether the UE supports QoE Measurement Collection for MTSI services.

## 4.9a Measurement related capabilities (TDD only)

Need for idle interval

Defines whether the UE needs idle interval in order to perform E-UTRAN measurements. There are separate parameters for measurements in each frequency band.

## 4.10 General capabilities

Access stratum release indicator

This is defined as the release of the UTRA layer 1, 2, and 3 specifications that is applicable for the UE e.g. R'99, Rel-4.

Device type

Defines whether UE benefits from NW-based battery consumption optimisation or not.

Support of DSAC and PPAC update in CELL\_DCH

Defines whether the UE supports DSAC and PPAC update in CELL\_DCH or not.

Support of retrievable configurations

Defines whether the UE supports retrievable configurations.

Support of URA\_PCH with seamless transition

Defines whether the UE supports seamless transition from URA\_PCH to CELL\_FACH. If the UE supports URA\_PCH with seamless transition then the UE shall also support common E-DCH.

Support of improved synchronized RRC procedures

Defines whether the UE supports improved synchronized RRC procedures.

Support of enhanced state transition

Defines whether the UE supports enhanced state transition.

Support of simultaneous setup and release of RABs and RBs

Defines whether the UE supports simultaneous setup and release of RABs and RBs.

## 4.11 DL capabilities with simultaneous HS-DSCH

DL capability with simultaneous HS-DSCH configuration

Defines the modification of reception capabilities in downlink in terms of DPCH in case an HS-DSCH is configured simultaneously. The parameter values in table 4.11-1 replace the signalled values in case an HS-DSCH is configured simultaneously depending on the setting of the parameter DL DPCH capability with simultaneous HS-DSCH configuration. Other parameters are valid irrespective whether HS-DSCH is configured simultaneously or not.

Table 4.11-1: DL capabilities with simultaneous HS-DSCH

| DL DPCH capability with simultaneous HS-DSCH configuration | 32 kbps | 64 kbps | 128 kbps | 384 kbps |
| --- | --- | --- | --- | --- |
| Transport channel parameters |  |  |  |  |
| Maximum sum of number of bits of all transport blocks being received at an arbitrary time instant | 640 | 3840 | 3840 | 6400 |
| Maximum sum of number of bits of all convolutionally coded transport blocks being received at an arbitrary time instant | 640 | 640 | 640 | 640 |
| Maximum sum of number of bits of all turbo coded transport blocks being received at an arbitrary time instant | NA | 3840 | 3840 | 6400 |
| Maximum number of simultaneous transport channels | 8 | 8 | 8 | 8 |
| Maximum number of simultaneous CCTrCH (FDD) | 1 | 1 | 1 | 1 |
| Maximum number of simultaneous CCTrCH (TDD) | 2 | 3 | 3 | 3 |
| Maximum total number of transport blocks received within TTIs that end at the same time | 8 | 8 | 16 | 32 |
| Maximum number of TFC | 32 | 48 | 96 | 128 |
| Maximum number of TF | 32 | 64 | 64 | 64 |
| Support for turbo decoding | No | Yes | Yes | Yes |
| Physical channel parameters (FDD) |  |  |  |  |
| Maximum number of DPCH codes to be simultaneously received | 1 | 1 | 1 | 3 |
| Maximum number of physical channel bits received in any 10 ms interval (DPCH, S-CCPCH). | 1200 | 2400 | 4800 | 19200 |
| Physical channel parameters (TDD 3.84 Mcps) |  |  |  |  |
| Maximum number of timeslots per frame | 1 | 2 | 4 | 5 |
| Maximum number of physical channels per frame | 8 | 9 | 14 | 28 |
| Support of PDSCH | No | No | No | No |
| Maximum number of physical channels per timeslot | 8 | 9 | 9 | 9 |
| **Physical channel parameters (TDD 7.68 Mcps)** |  |  |  |  |
| Maximum number of timeslots per frame | 1 | 2 | 4 | 5 |
| Maximum number of physical channels per frame | 8 | 9 | 14 | 28 |
| Support of PDSCH | No | No | No | No |
| Maximum number of physical channels per timeslot | 8 | 9 | 9 | 9 |
| Physical channel parameters (TDD 1.28 Mcps) |  |  |  |  |
| Maximum number of timeslots per subframe | 1 | 2 | 3 | 4 |
| Maximum number of physical channels per subframe | 8 | 12 | 18 | 43 |
| Support of PDSCH | No | No | No | No |
| Maximum number of physical channels per timeslot | 8 | 11 | 14 | 14 |

## 4.12 UL capabilities with simultaneous E-DCH

UL capability with simultaneous E-DCH configuration

Defines the modification of transmission capabilities in uplink in terms of DPCH in case an E-DCH is configured simultaneously. The parameter values in table 4.12-1 replace the signalled values in case an E-DCH is configured simultaneously depending on the setting of the parameter UL DPCH capability with simultaneous E-DCH configuration. Other parameters are valid irrespective whether E-DCH is configured simultaneously or not.

Table 4.12-1: UL capabilities with simultaneous E-DCH

| UL DPCH capability with simultaneous E-DCH configuration | 64 kbps |
| --- | --- |
| Transport channel parameters |  |
| Maximum sum of number of bits of all transport blocks being transmitted at an arbitrary time instant | 3840 |
| Maximum sum of number of bits of all convolutionally coded transport blocks being transmitted at an arbitrary time instant | 640 |
| Maximum sum of number of bits of all turbo coded transport blocks being transmitted at an arbitrary time instant | 3840 |
| Maximum number of simultaneous transport channels | 8 |
| Maximum total number of transport blocks transmitted within TTIs that end at the same time | 8 |
| Maximum number of TFC | 32 |
| Maximum number of TF | 32 |
| Support for turbo encoding | Yes |
| **Physical channel parameters (FDD)** |  |
| Maximum number of DPDCH bits transmitted per 10 ms | 2400 |
| **Physical channel parameters (3.84Mcps TDD)** |  |
| Maximum number of timeslots per frame | 2 |
| Maximum number of physical channels per timeslot | 1 |
| Minimum SF | 2 |
| **Physical channel parameters (7.68Mcps TDD)** |  |
| Maximum number of timeslots per frame | 2 |
| Maximum number of physical channels per timeslot | 1 |
| Minimum SF | 4 |
| **Physical channel parameters (1.28Mcps TDD)** |  |
| Maximum number of timeslots per frame | 2 |
| Maximum number of physical channels per timeslot | 1 |
| Minimum SF | 2 |

## 4.13 UE minimum capabilities for reception of MBMS not provided in MBSFN mode

For FDD, the minimum UE capability for MBMS reception for MBMS services that are not provided in MBSFN mode consists of two separate and independent parts ("MBMS capability part A" and "MBMS capability part B").

MBMS capability part A parameters defined in Table 4.13-1 are the same as the 64kbps UE reference class for DL described in subclause 5.2 and provides capability to enable reception of logical channels other than MTCHs and MSCH when MBMS PTM is received simultaneously.

Table 4.13-1: MBMS capability part A (FDD)

|  |  |
| --- | --- |
| Capability for reception of DL DPCH or S-CCPCH carrying logical channels other than MTCH during MTCH reception | 64 kbps  Class |
| Transport channel parameters | Value |
| Maximum sum of number of bits of all transport blocks being received at an arbitrary time instant | 3840 |
| Maximum sum of number of bits of all convolutionally coded transport blocks being received at an arbitrary time instant | 640 |
| Maximum sum of number of bits of all turbo coded transport blocks being received at an arbitrary time instant | 3840 |
| Maximum number of simultaneous transport channels | 8 |
| Maximum number of simultaneous CCTrCH (FDD) | 1 |
| Maximum total number of transport blocks received within TTIs that end at the same time | 8 |
| Maximum number of TFC | 48 |
| Maximum number of TF | 64 |
| Support for turbo decoding | Yes |
| Physical channel parameters (FDD) |  |
| Number of DPCH or S-CCPCH codes (Note 1) | 1 |
| Maximum number of physical channel bits received in any 10 ms interval (DPCH or S-CCPCH). | 2400 |

NOTE: Capability for reception of DPCH is applicable only if UE supports MBMS PTM reception in CELL\_DCH state for reception of MBMS services that are not provided in MBSFN mode.

MBMS capability part B for reception of MBMS services that are not provided in MBSFN mode is defined in the following Table 4.13-2. MBMS capability part B enables reception of the S-CCPCHs onto which at least MTCH is multiplexed. MBMS capability part B supports selection combining and soft combining of S-CCPCHs on different cells. The UE is not required to support simultaneous selection combining and soft combining.

The exhaustive lists of supported configurations (slot formats, TTI and combining parameters) for capability part B is given in Table 4.13-3. Only FACH can be mapped on the S-CCPCHs listed in table 4.13-3. In addition to MTCH, the MSCH, BCCH, CCCH, DCCH and DTCH can be multiplexed onto the S-CCPCHs listed in table 4.13-3. The FACH TTI restrictions in table 4.13-3 only apply to FACHs carrying MTCH or MSCH.

Table 4.13-2: MBMS capability part B (FDD)

| Combination of UE Radio Access capability parameters in DL for all S-CCPCHs that carry at least MTCH |  |
| --- | --- |
| Transport channel parameters | Value |
| Maximum sum of number of bits of all transport blocks being received at an arbitrary time instant | 21504 |
| Maximum sum of number of bits of all convolutionally coded transport blocks being received at an arbitrary time instant | 640 |
| Maximum sum of number of bits of all turbo coded transport blocks being received at an arbitrary time instant | 21504 |
| Maximum number of transport channels for the configuration | 12 |
| Maximum total number of transport blocks received within TTIs that end at the same time | 32 |
| Maximum number of TFC per S-CCPCH | 32 |
| Maximum number of TF | 64 |
| Support for turbo decoding | Yes |
| Number of CRC bits | 16 |
| Support for slot formats that do not contain TFCI | No |
| Supported slot formats and TTI combinations | See table 4.13-3 |
| Physical channel parameters |  |
| Maximum number of S-CCPCHs simultaneously received per cell for S-CCPCH Selection Combining or Soft Combining | 1 |
| Maximum number of cells for S-CCPCH Selection Combining or Soft Combining | See table 4.13-3 |

Table 4.13-3: Supported slot formats and FACH TTI combinations for MBMS capability part B (FDD)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| S-CCPCH slot format (see [11]) | FACH TTI (ms)  for FACHs carrying MTCH or MSCH | Maximum Number of cells for S-CCPCH Selection Combining  (Note 1) | Maximum Number of cells for S-CCPCH Soft Combining  (Note 1) | Maximum Number of Simultaneous Transport Channels per S-CCPCH |
| 14 (SF=8) | 40 | 2 | None | 1 |
| 14 (SF=8) | 40 | None | 3 | 1 |
| 12 (SF=16) | 40 | 3 | None | 1 |
| 12 (SF=16) | 80 | 2 | None | 1 |
| 12 (SF=16) | 80 | None | 3 | 1 |
| 10 (SF=32) | 80 | 3 | None | 4 |
| 10(SF=32) | 80 | None | 3 | 1 |
| 8 (SF=64) | 80 | 3 | None | 4 |
| 8 (SF=64) | 80 | None | 3 | 1 |
| 6 (SF=128) | 80 | 3 | None | 4 |
| 6 (SF=128) | 80 | None | 3 | 1 |
| 2 (SF=256) | 80 | 3 | None | 4 |
| 2 (SF=256) | 80 | None | 3 | 1 |

NOTE: 'None' indicates that either selection combining or soft combining is not required for the respective combination.

Since MBMS capability part A and B are independent, the maximum total number of S-CCPCHs, including the S-CCPCH that the UE is required to monitor by subclause 8.5.19 of [12], that the UE is required to receive is 4.

MBMS Capability part B may be used to receive MCCH in the following cases:

- When the UE is in CELL\_FACH state, and the MCCH is on a different S-CCPCH than the S-CCPCH that the UE is required to monitor by subclause 8.5.19 of [12].

- When the UE is in CELL\_DCH, if the UE supports MBMS PTM reception in CELL\_DCH.

Furthermore, in case MBMS PTM reception is ongoing, the UE may soft or selectively combine one less cell than shown in table 4.13-3 while receiving the S-CCPCH carrying the MCCH.

Further restrictions on the supported configurations of the S-CCPCH carrying the MCCH apply. The exhaustive lists of supported slot formats, TTI size, and maximum number of configured transport channels that can be received, depend on the capability of the UE to support MBMS PTM reception in CELL\_DCH. Table 4.13-3a applies when UE does support MBMS PTM reception in CELL\_DCH, while Table 4.13-3b applies when UE does not support MBMS PTM reception in CELL\_DCH. In addition to MCCH, the BCCH, PCCH, CCCH, DCCH and DTCH can be multiplexed onto the S-CCPCHs listed in tables 4.13-3a and 4.13-3b. The FACH TTI restrictions in tables 4.13-3a and 4.13-3b only apply to FACH carrying MCCH.

Table 4.13-3a: Alternate supported slot formats and FACH TTI for MBMS capability part B (FDD)

|  |  |  |
| --- | --- | --- |
| S-CCPCH slot format (see [11]) | FACH TTI (ms)  for FACH carrying MCCH | Maximum Number of Configured Transport Channels |
| 10 (SF=32) | 20,10 | 4 |
| 8 (SF=64) | 20,10 | 4 |
| 6 (SF=128) | 20,10 | 4 |
| 2 (SF=256) | 20,10 | 4 |

NOTE: One of the transport channels could be PCH.

Table 4.13-3b: Alternate supported slot formats and FACH TTI for MBMS capability part B (FDD)

|  |  |  |
| --- | --- | --- |
| S-CCPCH slot format (see [11]) | FACH TTI (ms)  for FACH carrying MCCH | Maximum Number of Configured Transport Channels |
| 8 (SF=64) | 10 | 1 |
| 6 (SF=128) | 10 | 1 |
| 2 (SF=256) | 20, 10 | 1 |

For FDD, the UE only supports reception of the MCCH, MTCH and MSCH on S-CCPCHs configured with flexible position.

For 3.84 Mcps TDD, a UE which supports the minimum capabilities defined in Table 4.13-4 should be capable of supporting transport channel combining of up to three radio links.

Table 4.13-4: MBMS Capabilities (3.84 Mcps TDD)

|  |  |
| --- | --- |
| Combination of UE Radio Access capability parameters in DL for MBMS |  |
| Maximum sum of number of bits of all transport blocks being received at an arbitrary time instant for S-CCPCH carrying MTCH (and MCCH/MSCH) | 10752 |
| Maximum sum of number of bits of all convolutionally coded transport blocks being received at an arbitrary time instant for S-CCPCH carrying MTCH (and MCCH/MSCH) | 640 |
| Maximum number of bits of all turbo coded transport blocks being received at an arbitrary time instant for S-CCPCH carrying MTCH (and MCCH/MSCH) | 10752 |
| Maximum number of bits before de-rate matching being received at an arbitrary time instant for S-CCPCH which carries MTCH (and MCCH/MSCH) | 31856 |
| Maximum number of physical channel bits received in any 10ms interval | 13248 |
| Maximum number of simultaneous transport channels per S-CCPCH carrying MTCH (and MCCH/MSCH) | 16 |
| Maximum number of physical channels per timeslot | 16 |
| Maximum number of synchronised radio links per frame which carry MTCH (and MCCH/MSCH) | 3 |
| Support for turbo decoding | Yes |

NOTE: In the above table, the S-CCPCH refers to the CCTrCH carrying FACH

For 7.68 Mcps TDD, a UE which supports the minimum capabilities defined in Table 4.13-4a should be capable of supporting transport channel combining of up to three radio links.

Table 4.13-4a: MBMS Capabilities (7.68 Mcps TDD)

|  |  |
| --- | --- |
| Combination of UE Radio Access capability parameters in DL for MBMS |  |
| Maximum sum of number of bits of all transport blocks being received at an arbitrary time instant for S-CCPCH carrying MTCH (and MCCH/MSCH) | 21504 |
| Maximum sum of number of bits of all convolutionally coded transport blocks being received at an arbitrary time instant for S-CCPCH carrying MTCH (and MCCH/MSCH) | 1280 |
| Maximum number of bits of all turbo coded transport blocks being received at an arbitrary time instant for S-CCPCH carrying MTCH (and MCCH/MSCH) | 21504 |
| Maximum number of bits before de-rate matching being received at an arbitrary time instant for S-CCPCH which carries MTCH (and MCCH/MSCH) | 63712 |
| Maximum number of physical channel bits received in any 10ms interval | 26496 |
| Maximum number of simultaneous transport channels per S-CCPCH carrying MTCH (and MCCH/MSCH) | 16 |
| Maximum number of physical channels per timeslot | 16 |
| Maximum number of synchronised radio links per frame which carriy MTCH (and MCCH/MSCH) | 3 |
| Support for turbo decoding | Yes |

NOTE: In the above table, the S-CCPCH refers to the CCTrCH carrying FACH.

For 1.28 Mcps TDD, a UE which supports the minimum capabilities defined in Table 4.13-5 should be capable of supporting transport channel combining of up to three radio links.

Table 4.13-5: DL Capabilities with simultaneous MBMS (1.28Mcps TDD)

|  |  |
| --- | --- |
| Combination of UE Radio Access capability parameters in DL for MBMS |  |
| Maximum sum of number of bits of all transport blocks being received at an arbitrary time instant for S-CCPCH carrying MTCH (and MCCH/MSCH) | 10752 |
| Maximum sum of number of bits of all convolutionally coded transport blocks being received at an arbitrary time instant for S-CCPCH carrying MTCH (and MCCH/MSCH) | 640 |
| Maximum number of bits of all turbo coded transport blocks being received at an arbitrary time instant for S-CCPCH carrying MTCH (and MCCH/MSCH) | 10752 |
| Maximum number of bits before de-rate matching being received at an arbitrary time instant for S-CCPCH which carries MTCH (and MCCH/MSCH) | 23920 |
| Maximum number of physical channel bits received in any 5ms interval | 4224 |
| Maximum number of simultaneous transport channels per S-CCPCH carrying MTCH (and MCCH/MSCH) | 16 |
| Maximum number of physical channels per timeslot | 16 |
| Maximum number of synchronised radio links received per frame which carry MTCH (and MCCH/MSCH) | 3 |
| Support for turbo decoding | Yes |

NOTE: In the above table, the S-CCPCH refers to the CCTrCH carrying FACH

## 4.13a UE minimum capabilities for reception of MBMS provided in MBSFN mode

For FDD, the minimum UE capability for reception of MBMS on cells that are operating in MBSFN mode consists of two separate and independent parts ("MBMS capability part C" and "MBMS capability part D").

For FDD MBSFN capability part C parameters defined in Table 4.13a-1 are the same as the 64kbps UE reference class for DL described in subclause 5.2 and provides capability to enable reception of MCCH when MBMS PTM is received simultaneously, and is applicable when a cell is operating in MBSFN mode.

Table 4.13a-1: MBSFN capability part C (FDD)

|  |  |
| --- | --- |
| Capability for reception of S-CCPCH carrying logical channels other than MTCH during MTCH reception in MBSFN Mode |  |
| Transport channel parameters | Value |
| Maximum sum of number of bits of all transport blocks being received at an arbitrary time instant | 1280 |
| Maximum sum of number of bits of all convolutionally coded transport blocks being received at an arbitrary time instant | 640 |
| Maximum sum of number of bits of all turbo coded transport blocks being received at an arbitrary time instant | 1280 |
| Maximum number of simultaneous transport channels | 1 |
| Maximum number of simultaneous CCTrCH (FDD) | 1 |
| Maximum total number of transport blocks received within TTIs that end at the same time | 8 |
| Maximum number of TFC | 32 |
| Maximum number of TF | 32 |
| Support for turbo decoding | Yes |
| Physical channel parameters (FDD) |  |
| Number of S-CCPCH codes | 1 |
| Maximum number of physical channel bits received in any 10 ms interval (S-CCPCH). | 1200 |

For FDD, MBSFNcapability part D for cells that do operate in MBSFN mode is defined in Table 4.13a-2 for the reception of MTCH and MSCH on a S-CCPCH. This allows the UE to receive at least one service sent on a S-CCPCH of a cell operating in MBSFN mode.

The exhaustive lists of supported configurations (slot formats and TTI) for capability part D is given in Table 4.13a-3. Only FACH can be mapped on the S-CCPCHs listed in table 4.13a-2.

Table 4.13a-2: MBSFN capability part D (FDD)

|  |  |
| --- | --- |
| **Combination of UE Radio Access capability parameters in DL for MBMS reception in MBSFN Mode** |  |
| Maximum number of bits of all transport blocks being received at an arbitrary time instant for S-CCPCHs carrying MTCH (and MSCH) | 81920 / 40960 Note 1 |
| Maximum sum of number of bits of all convolutionally coded transport blocks being received at an arbitrary time instant | 640 |
| Maximum sum of number of bits of all turbo coded transport blocks being received at an arbitrary time instant | 81920 / 40960  Note 1 |
| Maximum number of transport channels for the configuration | 8 |
| Maximum total number of transport blocks received within TTIs that end at the same time | 128 |
| Maximum number of TFC per S-CCPCH | 128 |
| Maximum number of TF | 64 |
| Support for turbo decoding | Yes |
| Number of CRC bits | 16 |
| Support for slot formats that do not contain TFCI | No |
| Supported slot formats and TTI combinations | See table 4.13-3 |
| Maximum Number of Simultaneous Transport Channels per S-CCPCH | 2 (Note 2) |

NOTE 1: 81920 is only applicable for combinations in table 4.13a-3 where scheduling is restriced by a value bigger than 1 of MBMS minimum inter-TTI interval.

NOTE 2: Only one MTCH at a time and in addition possibly MSCH.

Table 4.13a-3: Supported slot formats and FACH TTI combinations for MBSFN capability part D (FDD)

|  |  |  |
| --- | --- | --- |
| S-CCPCH slot format (see [11]) | FACH TTI (ms) | MBMS minimum inter-TTI interval |
| 23 (SF=8, 16QAM) | 80 | 2 |
| 23 (SF=8, 16QAM) | 40 | 1 |
| 22 (SF=16, 16QAM) | 80 | 1 |
| 21 (SF=32, 16QAM) | 80 | 1 |
| 20 (SF=64, 16QAM) | 80 | 1 |
| 19 (SF=128, 16QAM) | 80 | 1 |
| 18 (SF=256, 16QAM) | 80 | 1 |
| 16 (SF=4, QPSK) | 80 | 2 |
| 14 (SF=8, QPSK) | 80 | 1 |
| 12 (SF=16, QPSK) | 80 | 1 |
| 10 (SF=32, QPSK) | 80 | 1 |
| 8 (SF=64, QPSK) | 80 | 1 |
| 6 (SF=128, QPSK) | 80 | 1 |
| 4 (SF=128, QPSK) | 80 | 1 |
| 2 (SF=256, QPSK) | 80 | 1 |
| 0 (SF=256, QPSK) | 80 | 1 |

The MBMS minimum inter-TTI interval for MBSFN reception defines the minimum distance from the beginning of a TTI in which a given transport channel is scheduled to the beginning of the next TTI which corresponds to the earliest TTI in which which the same transport channel is allowed to be scheduled according to table 4.13a-3.

For 3.84 Mcps TDD, a MBSFN (MBMS over a Single Frequency Network) capable UE should support the minimum capabilities defined in Table 4.13a-4

Table 4.13a-4: MBSFN Capabilities (3.84 Mcps TDD)

|  |  |
| --- | --- |
| Combination of UE Radio Access capability parameters in DL for MBMS reception in MBSFN Mode |  |
| Maximum number of bits of all transport blocks being received at an arbitrary time instant for S-CCPCHs carrying MTCH (and MCCH/MSCH) | 43603 |
| Maximum number of bits before de-rate matching being received at an arbitrary time instant for S-CCPCHs which carry MTCH (and MCCH/MSCH) | 69696 |
| Maximum number of physical channel bits received in any 10ms interval | 8712 |
| Maximum number of simultaneous transport channels per S-CCPCH carrying MTCH (and MCCH/MSCH) | 4 |
| Maximum total number of transport blocks received within TTIs that end at the same time | 130 |
| Maximum number of TFC per S-CCPCH carrying MTCH (and MCCH / MSCH) | 32 |
| Maximum number of physical channels per timeslot | 16 |
| Maximum number of physical channels per frame | 33 |
| Maximum number of timeslots per frame | 3 |

NOTE 3: In the above table, the S-CCPCH refers to the CCTrCH carrying FACH. Only turbo coding is supported.

For 7.68 Mcps TDD, a MBSFN (MBMS over a Single Frequency Network) capable UE should support the minimum capabilities defined in Table 4.13a-5.

Table 4.13a-5: MBSFN Capabilities (7.68 Mcps TDD)

|  |  |
| --- | --- |
| Combination of UE Radio Access capability parameters in DL for MBMS reception in MBSFN Mode |  |
| Maximum number of bits of all transport blocks being received at an arbitrary time instant for S-CCPCHs carrying MTCH (and MCCH/MSCH) | 84572 |
| Maximum number of bits before de-rate matching being received at an arbitrary time instant for S-CCPCHs which carry MTCH (and MCCH/MSCH) | 137280 |
| Maximum number of physical channel bits received in any 10ms interval | 17160 |
| Maximum number of simultaneous transport channels per S-CCPCH carrying MTCH (and MCCH/MSCH) | 4 |
| Maximum total number of transport blocks received within TTIs that end at the same time | 130 |
| Maximum number of TFC per S-CCPCH carrying MTCH (and MCCH / MSCH) | 32 |
| Maximum number of physical channels per timeslot | 32 |
| Maximum number of physical channels per frame | 65 |
| Maximum number of timeslots per frame | 3 |

NOTE 4: In the above table, the S-CCPCH refers to the CCTrCH carrying FACH. Only turbo coding is supported.

For 1.28 Mcps TDD, a MBSFN (MBMS over a Single Frequency Network) capable for mixed-carrier UE should support the minimum capabilities defined in Table 4.13a-6

Table 4.13a-6: MBSFN Capabilities for Mixed-carrier (1.28 Mcps TDD)

|  |  |
| --- | --- |
| Combination of UE Radio Access capability parameters in DL for MBMS reception in MBSFN Mode |  |
| Maximum number of bits of all transport blocks being received at an arbitrary time instant for S-CCPCH carrying MTCH (and MCCH/MSCH) | 16448 |
| Maximum number of bits before de-rate matching being received at an arbitrary time instant for S-CCPCH which carries MTCH (and MCCH/MSCH) | 23232 |
| Maximum number of physical channel bits received in any 10ms interval | 5808 |
| Maximum number of simultaneous transport channels per S-CCPCH carrying MTCH (and MCCH/MSCH) | 1 |
| Maximum total number of transport blocks received within TTIs that end at the same time | 49 |
| Maximum number of TFC per S-CCPCH carrying MTCH (and MCCH / MSCH) | 32 |
| Maximum number of physical channels per timeslot | 16 |
| Maximum number of physical channels per frame | 17 |
| Maximum number of timeslots per frame | 2 |

NOTE: In the above table, the S-CCPCH refers to the CCTrCH carrying FACH.

For 1.28 Mcps TDD, a MBSFN (MBMS over a Single Frequency Network) capable for dedicated-carrier UE should support the minimum capabilities defined in Table 4.13a-7

Table 4.13a-7: MBSFN Capabilities for Dedicated-carrier (1.28 Mcps TDD)

|  |  |
| --- | --- |
| Combination of UE Radio Access capability parameters in DL for MBMS reception in MBSFN Mode |  |
| Maximum number of bits of all transport blocks being received at an arbitrary time instant for S-CCPCH carrying MTCH (and MCCH/MSCH) | 16448 |
| Maximum number of bits before de-rate matching being received at an arbitrary time instant for S-CCPCH which carries MTCH (and MCCH/MSCH) | 25224 |
| Maximum number of physical channel bits received in any 10ms interval | 6306 |
| Maximum number of simultaneous transport channels per S-CCPCH carrying MTCH (and MCCH/MSCH) | 1 |
| Maximum total number of transport blocks received within TTIs that end at the same time | 49 |
| Maximum number of TFC per S-CCPCH carrying MTCH (and MCCH / MSCH) | 32 |
| Maximum number of physical channels per timeslot | 16 |
| Maximum number of physical channels per frame | 35 |
| Maximum number of timeslots per frame | 3 |

NOTE: In the above table, the S-CCPCH refers to the CCTrCH carrying FACH.

For MBSFN Integrated Mobile Broadcast (3.84 Mcps TDD IMB), the minimum UE capability for reception of MBMS on cells that are operating in MBSFN mode consists of two separate and independent parts ("MBMS capability part E" and "MBMS capability part F").

For 3.84 Mcps TDD MBSFN IMB, capability part E parameters defined in Table 4.13a-8 enable reception of MCCH on S-CCPCH frame type 1 when MBMS PTM is received simultaneously, and is applicable when a cell is operating in MBSFN mode.

Table 4.13a-8: MBSFN capability part E (3.84 Mcps TDD MBSFN IMB)

|  |  |
| --- | --- |
| Capability for reception of S-CCPCH frame type 1 carrying logical channels other than MTCH during MTCH reception in MBSFN Mode |  |
| Transport channel parameters | Value |
| Maximum sum of number of bits of all transport blocks being received at an arbitrary time instant | 1280 |
| Maximum sum of number of bits of all convolutionally coded transport blocks being received at an arbitrary time instant | 1280 |
| Maximum number of simultaneous transport channels | 1 |
| Maximum number of simultaneous CCTrCH | 1 |
| Maximum total number of transport blocks received within TTIs that end at the same time | 8 |
| Maximum number of TFC | 32 |
| Maximum number of TF | 32 |
| Support for turbo decoding | No |
| Physical channel parameters |  |
| Number of S-CCPCH frame type 1 codes | 1 |
| Maximum number of physical channel bits received in any 10 ms interval (S-CCPCH frame type 1). | 270 |

For 3.84 Mcps TDD MBSFN IMB, capability part F for cells that do operate in MBSFN mode is defined in Table 4.13a-9 for the reception of an MTCH (and MSCH) on S-CCPCH frame type 2. This allows the UE to receive at least one service sent on S-CCPCHs frame type 2 of a cell operating in MBSFN mode.

Table 4.13a-9: MBSFN capability part F (3.84 Mcps TDD MBSFN IMB)

|  |  |
| --- | --- |
| Combination of UE Radio Access capability parameters in DL for MBMS reception in MBSFN Mode |  |
| Maximum number of bits of all transport blocks being received at an arbitrary time instant for S-CCPCHs frame type 2 carrying MTCH (and MSCH) | 40960 |
| Maximum sum of number of bits of all convolutionally coded transport blocks being received at an arbitrary time instant | 0 |
| Maximum sum of number of bits of all turbo coded transport blocks being received at an arbitrary time instant | 40960 |
| Maximum number of transport channels for the configuration | 8 |
| Maximum total number of transport blocks received within TTIs that end at the same time | 128 |
| Maximum number of TFC per S-CCPCH frame type 2 | 32 |
| Maximum number of TF | 32 |
| Support for turbo decoding | Yes |
| Number of CRC bits | 16 |
| Support for CCTrCH that do not contain TFCI | No |
| Maximum Number of Simultaneous Transport Channels per S-CCPCH type 2 | 2 (Note 5) |
| **Physical channel parameters** |  |
| Maximum number of S-CCPCH frame type 2 codes using QPSK modulation | 10 |
| Maximum number of S-CCPCH frame type 2 codes using 16-QAM modulation | 5 |
| Maximum number of physical channel bits received in any 10 ms interval (S-CCPCH frame type 2). | 8640 |

NOTE 5: Only one MTCH at a time and in addition possibly MSCH

For 3.84 Mcps TDD MBSFN IMB, the permitted FACH TTI values for the supported configurations of the S-CCPCH carrying the MCCH are given by capability part G. For 3.84 Mcps TDD MBSFN IMB, capability part G is defined in Table 4.13a-10 for the reception of an MCCH on S-CCPCH frame type 1.

Table 4.13a-10: Slot formats and FACH TTI for MBSFN capability part G (3.84 Mcps TDD MBSFN IMB)

|  |  |  |
| --- | --- | --- |
| S-CCPCH slot format (see [14]) | FACH TTI (ms)  for FACH carrying MCCH | Maximum Number of Configured Transport Channels |
| 0 (SF=256, QPSK) | 80,40,20,10 | 1 |
| 1 (SF=256, QPSK) | 80,40,20,10 | 1 |

## 4.14 Home Node B Inbound Mobility Related Parameters

### 4.14.1 CSG Proximity Indication Parameters

Support of intra-frequency proximity indication

Defines whether the UE supports proximity indication for intra-frequency cells whose CSG Identities are in the UE’s CSG Whitelist.

Support of inter-frequency proximity indication

Defines whether the UE supports proximity indication for inter-frequency cells whose CSG Identities are in the UE’s CSG Whitelist.

Support of E-UTRA proximity indication

Defines whether the UE supports proximity indication for E-UTRAN cells whose CSG IDs are in the UE’s CSG Whitelist.

### 4.14.2 Neighbour Cell SI Acquisition Parameters

Support of intra-frequency SI acquisition for HO

Defines whether the UE supports, upon configuration of "Intra-frequency SI Acquisition", acquisition of relevant informationfrom a neighbouring intra-frequency cell by reading the SI of the neighbouring cell and reporting the acquired informationto the network.

Support of inter-frequency SI acquisition for HO

Defines whether the UE supports, upon configuration of "Inter-frequency SI Acquisition", acquisition of relevant informationfrom a neighbouring inter-frequency cell by reading the SI of the neighbouring cell using autonomous gaps and reporting the acquired informationto the network.

Support of E-UTRA SI acquisition for HO

Defines whether the UE supports, upon configuration of "E-UTRA SI Acquisition", acquisition of relevant informationfrom a neighbouring E-UTRA cell by reading the SI of the neighbouring cell using autonomous gaps and reporting the acquired informationto the network.

## 4.14a IMS Voice Parameters

Voice over UTRA PS HS Support

Defines whether the UE supports IMS Voice in UTRA according to GSMA IR 58 profile. If UE supports E-UTRA and IMS voice in UTRA, UE also supports IMS voice in E-UTRA. If the UE supports IMS Voice in UTRA PS HS, then the UE shall also support the UM RLC re-establishment via reconfiguration.

SRVCC Support from UTRA to UTRA

Defines whether the UE supports SRVCC handover from UTRA PS HS to UTRA CS.

SRVCC Support from UTRA to GERAN

Defines whether the UE supports SRVCC handover from UTRA PS HS to GERAN CS.

rSRVCC support from UTRA CS to E-UTRAN FDD

Defines whether the UE supports rSRVCC handover from UTRA CS to E-UTRAN FDD.

rSRVCC support from UTRA CS to E-UTRAN TDD

Defines whether the UE supports rSRVCC handover from UTRA CS to E-UTRAN TDD.

## 4.15 UE based network performance measurements parameters

Support of logged measurements in Idle mode and PCH States

Defines whether the UE supports logged measurements upon request from the network in Idle mode, URA\_PCH and CELL\_PCH states. A UE that supports logged measurements in Idle mode, Cell\_PCH and URA\_PCH states shall also support a minimum of 64 kB of memory for log storage. If the UE supports logged measurements in Idle mode and PCH States and HS-DSCH DRX operation with second DRX cycle, then the UE shall also support logged measurements in CELL\_FACH state when second DRX cycle is used in UTRAN.

Support of UTRAN ANR

Defines whether the UE supports measurement and logging in Idle mode, CELL\_PCH and URA\_PCH states for Automatic Neighbour Relation (ANR) in UTRAN. If the UE supports UTRAN ANR and HS-DSCH DRX operation with second DRX cycle, then the UE shall also support measurement and logging in CELL\_FACH state when second DRX cycle is used for Automatic Neighbour Relation (ANR) in UTRAN.

# 5 Possible UE radio access capability parameter settings

## 5.1 Value ranges

Table 5.1: UE radio access capability parameter value ranges

|  | | UE radio access capability parameter | Value range |
| --- | --- | --- | --- |
| PDCP parameters | | Support for RFC 2507 | Yes/No |
| Support for RFC 3095 | Yes/No |
| Support for RFC 3095 context relocation | Yes/No |
| Support for loss-less SRNS relocation | Yes/No |
| Support for loss-less DL RLC PDU size change | Yes/No |
| Maximum header compression context space | 1024, 2048, 4096, 8192, 16384, 32768, 65536, 131072 bytes |
| Maximum number of ROHC context sessions | 2, 4, 8, 12, 16, 24, 32, 48, 64, 128, 256, 512, 1024, 16384 |
| Support for Reverse Decompression | Not supported, 1..65535 |
| Support for CS voice over HSPA | Yes/No |
| RLC, MAC-hs, MAC-ehs and MAC-i/is parameters | | Total RLC AM, MAC-hs and MAC-ehs buffer size | 2, 10, 50, 100, 150, 200, 300, 400, 500, 750, 1000, 1150, 1250, 1800, 2000, 2300, 2550, 3400, 3500, 4400, 4500, 5000 kBytes |
| Maximum number of AM entities | 3, 4, 5, 6, 8, 16, 30 |
| Maximum RLC AM window size | 2047, 4095 |
| Support for MAC-ehs | Yes/No |
| Support for two logical channels | Yes/No |
| Support of MAC-i/is | Yes/No |
| Support of MAC-ehs window size extension | Yes/No |
| Support of UM RLC re-establishment via reconfiguration | Yes/No |
| PHY parameters | Transport channel parameters in downlink | Maximum sum of number of bits of all transport blocks being received at an arbitrary time instant | 640, 1280, 2560, 3840, 5120, 6400, 7680, 8960, 10240, 20480, 40960, 81920, 163840, 204640 |
| Maximum sum of number of bits of all convolutionally coded transport blocks being received at an arbitrary time instant | 640, 1280, 2560, 3840, 5120, 6400, 7680, 8960, 10240, 20480, 40960, 81920, 163840, 204640 |
| Maximum sum of number of bits of all turbo coded transport blocks being received at an arbitrary time instant | 640, 1280, 2560, 3840, 5120, 6400, 7680, 8960, 10240, 20480, 40960, 81920, 163840, 204640 |
| Maximum number of simultaneous transport channels | 4, 8, 16, 32 |
| Maximum number of simultaneous CCTrCH | 1, 2, 3, 4, 5, 6, 7, 8 |
| Maximum total number of transport blocks received within TTIs that end within the same 10 ms interval | 4, 8, 16, 32, 48, 64, 96, 128, 256, 512 |
| Maximum number of TFC | 16, 32, 48, 64, 96, 128, 256, 512, 1024 |
| Maximum number of TF | 32, 64, 128, 256, 512, 1024 |
| Support for turbo decoding | Yes/No |
| Transport channel parameters in uplink | Maximum sum of number of bits of all transport blocks being transmitted at an arbitrary time instant | 640, 1280, 2560, 3840, 5120, 6400, 7680, 8960, 10240, 20480, 40960, 81920, 163840 |
| Maximum sum of number of bits of all convolutionally coded transport blocks being transmitted at an arbitrary time instant | 640, 1280, 2560, 3840, 5120, 6400, 7680, 8960, 10240, 20480, 40960, 81920, 163840 |
| Maximum sum of number of bits of all turbo coded transport blocks being transmitted at an arbitrary time instant | 640, 1280, 2560, 3840, 5120, 6400, 7680, 8960, 10240, 20480, 40960, 81920, 163840 |
| Maximum number of simultaneous transport channels | 2, 4, 8, 16, 32 |
| Maximum number of simultaneous CCTrCH of DCH type (TDD only) | 1, 2, 3, 4, 5, 6, 7, 8 |
| Maximum total number of transport blocks transmitted within TTIs that start at the same time | 2, 4, 8, 16, 32, 48, 64, 96, 128, 256, 512 |
| Maximum number of TFC | 4, 8, 16, 32, 48, 64, 96, 128, 256, 512, 1024 |
| Maximum number of TF | 32, 64, 128, 256, 512, 1024 |
| Support for turbo encoding | Yes/No |
|  | FDD Physical channel parameters in downlink | Maximum number of DPCHcodes to be simultaneously received | 1, 2, 3, 4, 5, 6, 7, 8 |
| Maximum number of physical channel bits received in any 10 ms interval (DPCH, S-CCPCH) | 600, 1200, 2400, 3600, 4800, 7200, 9600, 14400, 19200, 28800, 38400, 48000, 57600, 67200, 76800 |
| Support for SF 512 and 80 ms TTI for DPCH | Yes/No |
| Support of HS-PDSCH in CELL\_DCH | Yes/No |
| Support of HS-SCCHless HS-DSCH | Yes/No |
| Support of HS-PDSCH in CELL\_FACH | Yes/No |
| Support of HS-PDSCH in CELL\_PCH and URA\_PCH | Yes/No |
| Support of Enhanced F-DPCH | Yes/No |
| Support of Target Cell Pre-Configuration | Yes/No |
| Support of Enhanced Serving Cell Change for Event 1C | Yes/No |
| Support of HS-DSCH DRX operation | Yes/No |
| Support of Node B triggered HS-DPCCH transmission | Yes/No |
| Support of HS-DSCH DRX operation with second DRX cycle | Yes/No |
| Support for Two DRX schemes in URA\_PCH and CELL\_PCH | Yes/No |
| Support of TX Diversity on DL Control Channels by MIMO Capable UE when MIMO operation is active | Yes/No |
| Support for cell-specific Tx diversity configuration for dual-cell operation | Yes/No |
| Support of MIMO only with single-stream restriction | Yes/No |
| Support for dual cell with MIMO operation in different bands | Yes/No |
| Support of MIMO mode with four transmit antennas operation only with dual-stream restriction | Yes/No |
| Support of dual band operation (Radio Access Capability Band Combination List) | 1..16 |
| >Band Combination | 1..256 |
| >Supported Carrier Combination List |  |
| >>Carrier Combination (1,2) | Yes/No |
| >>Carrier Combination (2,1) | Yes/No |
| >>Carrier Combination (1,3) | Yes/No |
| >>Carrier Combination (3,1) | Yes/No |
| >>Carrier Combination (2,2) | Yes/No |
| >>Carrier Combination (1,4) | Yes/No |
| >>Carrier Combination (4,1) | Yes/No |
| >>Carrier Combination (1,5) | Yes/No |
| >>Carrier Combination (5,1) | Yes/No |
| >>Carrier Combination (1,6) | Yes/No |
| >>Carrier Combination (6,1) | Yes/No |
| >>Carrier Combination (1,7) | Yes/No |
| >>Carrier Combination (7,1) | Yes/No |
| >>Carrier Combination (2,3) | Yes/No |
| >>Carrier Combination (3,2) | Yes/No |
| >>Carrier Combination (2,4) | Yes/No |
| >>Carrier Combination (4,2) | Yes/No |
| >>Carrier Combination (2,5) | Yes/No |
| >>Carrier Combination (5,2) | Yes/No |
| >>Carrier Combination (2,6) | Yes/No |
| >>Carrier Combination (6,2) | Yes/No |
| >>Carrier Combination (3,3) | Yes/No |
| >>Carrier Combination (3,4) | Yes/No |
| >>Carrier Combination (4,3) | Yes/No |
| >>Carrier Combination (4,4) | Yes/No |
| >>Carrier Combination (3,5) | Yes/No |
| >>Carrier Combination (5,3) | Yes/No |
| Support for Multiflow | Yes/No (per frequency band) |
| >Support for Multiflow and MIMO | No/Single stream/Dual stream  NOTE: If a UE supports single-stream MIMO transmission with Multiflow, then single-stream MIMO is supported in all the frequency bands where Multiflow operation is supported. The dual-stream MIMO transmission with Multiflow support is per frequency band. |
| >Support for Multiflow with non-contiguous carrier allocation | 5, 10, any gap size (per frequency band) |
| Support for Multiflow in different bands | Yes/No (per frequency band combination) |
| Support for Multiflow with MIMO operation in different bands | No/Single stream/Dual stream  NOTE1: If a UE does not support "Multiflow with MIMO operation in different bands", then no MIMO is supported in any of the band combinations where Multiflow is supported.  NOTE2: If a UE supports single-stream "Multiflow with MIMO operation in different bands", then single-stream MIMO is supported in all the band combinations where Multiflow is supported.  NOTE3: If a UE supports dual-stream "Multiflow with MIMO operation in different bands", then dual-stream MIMO transmission is supported in all the band combinations, in which the UE supports Multiflow and dual-stream MIMO in both bands of the corresponding band combination. Otherwise the UE supports single-stream MIMO in that band combination. |
| Support of MIMO mode with four transmit antennas operation | Yes/No (per frequency band) |
| Non-contiguous multi-cell | 1..3 |
| >Aggregated cells | 2, 3, 4 |
| >Gap size | 5, 10, any gap size |
| >Non-contiguous multi-cell Combination (2,2) | Yes/No |
| >Non-contiguous multi-cell Combination (3,1) (1,3) | Yes/No |
| Support of HS-DPCCH power offset extension | Yes/No |
| Support of STTD on DL Control Channels when Multiflow operation is active | Yes/No |
| Non-contiguous multi-cell with MIMO | Yes/No |
| Support of multi-cell configuration in inter-RAT handover | Yes/No |
| Support of DPCCH2 | Yes/No |
| Support for DCH Enhancements | Basic/Full |
| Simultaneous support for DCH Enhancements and Compressed Mode operation | Yes/No |
| Simultaneous support for DCH Enhancements and DPCCH Discontinuous Transmission | Yes/No |
| DRX enhancements | Yes/No |
| HS-DPCCH overhead reduction | Yes/No |
| Support of F-TPICH feedback from the Multiflow assisting cell | Yes/No |
| Support of power control algorithm 3 | Yes/No |
| Support of blind HARQ retransmissions for HSDPA | Yes/No |
| Support of HS-SCCH DRX operation | Yes/No |
| Support of simplified HS-SCCH type 1 operation | Yes/No |
| FDD Physical channel parameters in uplink | Maximum number of DPDCH bits transmitted per 10 ms | 600, 1200, 2400, 4800, 9600, 19200, 28800, 38400, 48000, 57600 |
| Support of E-DPDCH | Yes/No |
| Support of Discontinuous Transmission in CELL\_DCH | Yes/No |
| Support of Slot Format #4 | Yes/No |
| Support for E-DPCCH power interpolation formula | Yes/No |
| Support for E-DPCCH power boosting | Yes/No |
| Support of common E-DCH | Yes/No |
| Support of Common E-RGCH based interference control | Yes/No |
| Support of Fallback to R99 PRACH | Yes/No |
| Support of Concurrent deployment | Yes/No |
| Support of TTI alignment and Per HARQ process | Yes/No |
| Support of uplink open loop transmit diversity | Yes/No (per frequency band) |
| Support of uplink closed loop transmit diversity | Yes/No (per frequency band) |
| Support of Uplink MIMO | Yes/No (per frequency band) |
| Support of Serving E-DCH cell decoupling | Yes/No |
| Support of Radio Links without DPCH/F-DPCH | Yes/No |
| Support of Cell Reselection Indication Reporting | Yes/No |
| Access Groups based access control | Yes/No |
| Enhanced TTI switching | Yes/No |
| Implicit Grant handling | Yes/No |
| DTX enhancements | Yes/No |
| Support of Dual Cell E-DCH transmission with DPDCH | Yes/No |
| Support for Dual Band Dual Cell E-DCH operation | Yes/No |
| Support of Dual Cell E-DCH operation enhancements | Yes/No |
| TDD 3.84 Mcps physical channel parameters in downlink | Maximum number of timeslots per frame | 1..14 |
| Maximum number of physical channels per frame | 1, 2, 3..224 |
| Minimum SF | 16, 1 |
| Support of PDSCH | Yes/No |
| Support of HS-PDSCH | Yes/No |
| Maximum number of physical channels per timeslot | 1..16 |
| TDD 3.84 Mcps physical channel parameters in uplink | Maximum Number of timeslots per frame | 1..14 |
| Maximum number of physical channels per timeslot | 1, 2 |
| Minimum SF | 16, 8, 4, 2, 1 |
| Support of PUSCH | Yes/No |
| Support of E-PUCH | Yes/No |
| TDD 7.68 Mcps physical channel parameters in downlink  TDD 7.68 Mcps physical channel parameters in downlink | Maximum number of timeslots per frame | 1..14 |
| Maximum number of physical channels per frame | 1, 2, 3..448 |
| Minimum SF | 32, 1 |
| Support of PDSCH | Yes/No |
| Support of HS-PDSCH | Yes/No |
| Maximum number of physical channels per timeslot | 1..32 |
| TDD 7.68 Mcps physical channel parameters in uplink | Maximum Number of timeslots per frame | 1..14 |
| Maximum number of physical channels per timeslot | 1, 2 |
| Minimum SF | 32, 16, 8, 4, 2, 1 |
| Support of PUSCH | Yes/No |
| Support of E-PUCH | Yes/No |
| TDD 1.28 Mcps physical channel parameters in downlink | Maximum number of timeslots per subframe | 1..6 |
| Maximum number of physical channels per subframe | 1, 2, 3, …, 96 |
| Minimum SF | 16, 1 |
| Support of PDSCH | Yes/No |
| Support of HS-PDSCH | Yes/No |
| Maximum number of physical channels per timeslot | 1..16 |
| Support 8PSK | Yes/No |
| UE specific capability Information LCR TDD | Enumerated (NF, TriRxUniTx, TriRxTriTx, HexRxUniTx, HexRxTriTx, HexRxHexTx, TwoRxUniTxDiscontiguous, TwoRxTwoTxDiscontiguous,  TwoRxUniTxContiguous, TwoRxTwoTxContiguous)  NOTE: If three frequencies are supported, the three frequencies shall be configured within 5 MHz; if six frequencies are supported, the six frequencies shall be configured within 10MHz; TwoRxUniTxDiscontiguous and TwoRxTwoTxDiscontiguous mean that the UE is capable of supporting two non-adjacent carriers; TwoRxUniTxContiguous and TwoRxTwoTxContiguous mean that the UE is only capable of supporting two adjacent carriers; if two non-adjacent carriers are supported, the two carriers can be in the same band or in two different bands. |
| Support of HS-PDSCH in CELL\_FACH | Yes/No |
| Support of SPS | Yes/No |
| Support of HS-SCCH/E-AGCH Discontinuous Reception | Yes/No |
| Support of SF Mode For HS-PDSCH dual stream | Yes/No |
| Support of Enhanced TS0 | Yes/No |
| Support of Non-rectangular Resource Allocation | Yes/No |
| TDD 1.28 Mcps physical channel parameters in uplink | Maximum number of timeslots per subframe | 1..6 |
| Maximum number of physical channels per timeslot | 1, 2 |
| Minimum SF | 16, 8, 4, 2, 1 |
| Support of 8PSK | Yes/No |
| Support of PUSCH | Yes/No |
| Support of E-PUCH | Yes/No |
| Support of E-DCH in CELL\_FACH | Yes/No |
| RF parameters | FDD RF parameters | UE power class | 3, 4  NOTE: Only power classes 3 and 4 are part of this release of the specification |
| Radio frequency bands | The radio frequency bands defined in [4].  UEs that support band XIX shall also support band VI |
| Tx/Rx frequency separation | Defined in [4] for the respective supported radio frequency band |
| Support of Multiple Frequency Band Indicators | Yes/No |
| RF parameters | TDD 3.84 Mcps RF parameters | UE power class | 2, 3  NOTE: Only power classes 2 and 3 are part of this release of the specification |
| Radio frequency bands | The radio frequency bands defined in [5] |
| TDD 1.28 Mcps RF parameters | UE power class | 2, 3 |
| Radio frequency bands | The radio frequency bands defined in [5] |
| Multi-mode related parameters | | Support of UTRA FDD | Yes/No |
| Support of UTRA TDD 3.84 Mcps | Yes/No |
| Support of UTRA TDD 1.28 Mcps | Yes/No |
| Multi-RAT related parameters | | Support of GSM | Yes/No (per GSM frequency band) |
| Support of multi-carrier | Yes/No |
| Support of UTRAN to GERAN Network Assisted Cell Change | Yes/No |
| Support of Handover to GAN | Yes/No |
| Support of Inter-RAT PS Handover | Yes/No |
| Support of PS Handover to GAN | Yes/No |
| Support of E-UTRA FDD | Yes/No (per E-UTRA frequency band) |
| Support of Inter-RAT PS Handover to E-UTRA FDD | Yes/No |
| Support of E-UTRA FDD measurements and reporting in CELL\_FACH | Yes/No |
| Support of E-UTRA TDD | Yes/No (per E-UTRA frequency band) |
| Support of Inter-RAT PS Handover to E-UTRA TDD | Yes/No |
| Support of E-UTRA Multiple Frequency Band Indicators | Yes/No |
| Support of E-UTRA TDD measurements and reporting in CELL\_FACH | Yes/No |
| Support of RAN-assisted WLAN interworking based on RAN rules | Yes/No |
| Support of RAN-assisted WLAN interworking based on ANDSF policies | Yes/No |
| Support of extended E-UTRA frequency priority | Yes/No |
| Security parameters | | Support of ciphering algorithm UEA0 | Yes |
| Support of ciphering algorithm UEA1 | Yes |
| Support of ciphering algorithm UEA2 | Yes |
| Support of integrity protection algorithm UIA1 | Yes |
| Support of integrity protection algorithm UIA2 | Yes |
| UE positioning related parameters | | Standalone location method(s) supported | Yes/No |
| UE based OTDOA supported | Yes/No |
| Network assisted GPS support | Network based / UE based / Both/ None |
| Network Assisted GANSS support List: | per GANSS |
| >GANSS ID | Galileo / SBAS / Modernized GPS / QZSS / GLONASS/ BDS |
| >SBAS IDs | WAAS / EGNOS / MSAS / GAGAN |
| >GANSS mode | Network based / UE based / Both/ None |
| >GANSS Signal ID | 0..7 |
| >GANSS Signal IDs | Yes/No (per GANSS signal) |
| >Support for GANSS timing of cell frames measurement | Yes/No |
| >Support for GANSS Carrier-Phase Measurement | Yes/No |
| >Support for non-native assistance choices | Yes/No |
| Support for GPS timing of cell frames measurement | Yes/No |
| Support for IPDL | Yes/No |
| Support for Rx-Tx time difference type 2 measurement | Yes/No |
| Support for UE Positioning assisted GPS measurement validity in CELL\_PCH and URA\_PCH RRC states | Yes |
| Support for SFN-SFN observed time difference type 2 measurement | Yes/No |
| Additional Positioning method support List | Per Additional Positioning method |
| >AddPos ID | Barometric Pressure, WLAN, Bluetooth, MBS |
| >AddPos mode | Standalone / UE assisted / Both |
| Measurement related capabilities | | Need for downlink compressed mode | Yes/No (per frequency band, UTRA mode and RAT) |
| Need for uplink compressed mode | Yes/No (per frequency band, UTRA mode and RAT) |
| Support for absolute priority based cell re-selection in UTRAN | Yes/No |
| Support for System Information Block type 11bis | Yes |
| Adjacent Frequency measurements without compressed mode | Yes/No |
| Inter-band Frequency measurements without compressed mode | Yes/No |
| Enhanced inter-frequency measurements without compressed mode | Yes/No |
| Extended measurements ID support | Yes |
| Frequency specific compressed mode | Yes/No |
| Frequency specific compressed mode for non-contiguous operation | Yes/No |
| Inter-frequency detected set measurements | Yes/No |
| Inter-frequency measurements on configured carriers without compressed mode | Yes/No |
| Cells excluded from detected set measurements | Yes/No |
| Wideband RSRQ FDD measurements | Yes/No |
| Wideband RSRQ TDD measurements | Yes/No |
| Event 2g reporting on a configured secondary downlink frequency | Yes/No |
| Enhanced UPH reporting | Yes/No |
| RRC measurement events 6h and 6i for UPH reporting | Yes/No |
| Increased UE carrier monitoring UTRA | Yes/No |
| Increased UE carrier monitoring E-UTRA | Yes/No |
| Extended RSRQ lower value range | Yes/No |
| RSRQ measurement on all symbols | Yes/No |
| QoE Measurement Collection for streaming services | Yes/No |
| QoE Measurement Collection for MTSI services | Yes/No |
| General capabilities | | Access Stratum release indicator | R99, REL-4, REL-5, REL-6, REL-7, REL-8, REL-9, REL-10, REL-11, REL-12, REL-13, REL-14, REL-15, REL-16 |
| Device type | Benefits from NW-based battery consumption optimisation / Does not benefit from NW-based battery consumption optimisation |
| Support of DSAC and PPAC update in CELL\_DCH | Yes/No |
| Support of retrievable configurations | Yes/No |
| Support of URA\_PCH with seamless transition | Yes/No |
| Support of improved synchronized RRC procedures | Yes/No |
| Support of enhanced state transition | Yes/No |
| Support of simultaneous setup and release of RABs and RBs | Yes/No |
| DL capabilities with simultaneous HS-DSCH | | DL capability with simultaneous HS-DSCH configuration | 32 kbps, 64 kbps, 128 kbps, 384 kbps |
| UL capabilities with simultaneous E-DCH | | UL capabilities with simultaneous E-DCH | 64 kbps |
| UE based network performance measurements parameters | | Support of logged measurements in Idle mode and PCH States | Yes/No |
| Support of UTRAN ANR | Yes/No |
| Home Node B Inbound Mobility Related Parameters | CSG Proximity Indication capabilities | Support of intra-frequency proximity indication | Yes/No |
| Support of inter-frequency proximity indication | Yes/No |
| Support of E-UTRA proximity indication | Yes/No |
| Neighbour Cell SI Acquisition capabilities | Support of intra-frequency SI acquisition for HO | Yes/No |
| Support of inter-frequency SI acquisition for HO | Yes/No |
| Support of E-UTRA SI acquisition for HO | Yes/No |
| IMS Voice Parameters | | Voice over UTRA PS HS Support | Yes/No |
| SRVCC Support from UTRA to UTRA | Yes/No |
| SRVCC Support from UTRA to GERAN | Yes/No |
| rSRVCC support from UTRA CS to E-UTRAN FDD | Yes/No |
| rSRVCC support from UTRA CS to E-UTRAN TDD | Yes/No |

Table 5.1a: FDD HS-DSCH physical layer categories

| HS-DSCH category | Maximum number of HS-DSCH codes received | Minimum inter-TTI interval | Maximum number of bits of an HS-DSCH transport block received within  an HS-DSCH TTI NOTE 1 | Total number of soft channel bits | Total Numb-er of serving/secondary serving HS-DSCH cells | Total Number of serving/secondary serving HS-DSCH cells in which MIMO mode with two transmit antennas can be configured | Total Number of serving/secondary serving HS-DSCH cells in which MIMO mode with four transmit antennas can be configured | Supported modula-tions without MIMO operation or aggregated cell operation | Supported modula-tions with MIMO operation and without aggregated cell operation | Supported modula-tions without MIMO operation with aggregated cell operation | Supported modula-tions with MIMO operation and aggregated cell operation |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Category 1 | 5 | 3 | 7298 | 19200 | 1 | 0 | - | QPSK, 16QAM | Not applicable  (MIMO not supported) | Not applicable (aggregated carriers operation not supported) | Not applicable (simultaneous aggregated carriers and MIMO operation not supported) |
| Category 2 | 5 | 3 | 7298 | 28800 | 1 | 0 | - |
| Category 3 | 5 | 2 | 7298 | 28800 | 1 | 0 | - |
| Category 4 | 5 | 2 | 7298 | 38400 | 1 | 0 | - |
| Category 5 | 5 | 1 | 7298 | 57600 | 1 | 0 | - |
| Category 6 | 5 | 1 | 7298 | 67200 | 1 | 0 | - |
| Category 7 | 10 | 1 | 14411 | 115200 | 1 | 0 | - |
| Category 8 | 10 | 1 | 14411 | 134400 | 1 | 0 | - |
| Category 9 | 15 | 1 | 20251 | 172800 | 1 | 0 | - |
| Category 10 | 15 | 1 | 27952 | 172800 | 1 | 0 | - |
| Category 11 | 5 | 2 | 3630 | 14400 | 1 | 0 | - | QPSK |
| Category 12 | 5 | 1 | 3630 | 28800 | 1 | 0 | - |
| Category 13 | 15 | 1 | 35280 | 259200 | 1 | 0 | - | QPSK, 16QAM, 64QAM |
| Category 14 | 15 | 1 | 42192 | 259200 | 1 | 0 | - |
| Category 15 | 15 | 1 | 23370 | 345600 | 1 | 1 | - | QPSK, 16QAM | |
| Category 16 | 15 | 1 | 27952 | 345600 | 1 | 1 | - |
| Category 17 NOTE 2 | 15 | 1 | 35280 | 259200 | 1 | 0 | - | QPSK, 16QAM, 64QAM | – |
| 23370 | 345600 | 1 | 1 | - | – | QPSK, 16QAM |
| Category 18 NOTE 3 | 15 | 1 | 42192 | 259200 | 1 | 0 | - | QPSK, 16QAM, 64QAM | – |
| 27952 | 345600 | 1 | 1 | - | – | QPSK, 16QAM |
| Category 19 | 15 | 1 | 35280 | 518400 | 1 | 1 | - | QPSK, 16QAM, 64QAM | |
| Category 20 | 15 | 1 | 42192 | 518400 | 1 | 1 | - |
| Category 21 | 15 | 1 | 23370 | 345600 | 2 | 0 | - | - | - | QPSK, 16QAM |
| Category 22 | 15 | 1 | 27952 | 345600 | 2 | 0 | - |
| Category 23 | 15 | 1 | 35280 | 518400 | 2 | 0 | - | QPSK, 16QAM, 64QAM |
| Category 24 | 15 | 1 | 42192 | 518400 | 2 | 0 | - |
| Category 25 | 15 | 1 | 23370 | 691200 | 2 | 2 | - | - | - | - | QPSK, 16QAM |
| Category 26 | 15 | 1 | 27952 | 691200 | 2 | 2 | - |
| Category 27 | 15 | 1 | 35280 | 1036800 | 2 | 2 | - | - | - | - | QPSK, 16QAM, 64QAM |
| Category 28 | 15 | 1 | 42192 | 1036800 | 2 | 2 | - |
| Category 29 | 15 | 1 | 42192 | 777600 | 3 | 0 | - | - | - | QPSK,  16QAM,  64QAM | - |
| Category 30 | 15 | 1 | 42192 | 1555200 | 3 | 3 | - | - | - | QPSK,  16QAM,  64QAM | QPSK,  16QAM,  64QAM |
| Category 31 | 15 | 1 | 42192 | 1036800 | 4 | 0 | - | - | - | QPSK,  16QAM,  64QAM | - |
| Category 32 | 15 | 1 | 42192 | 2073600 | 4 | 4 | - | - | - | QPSK,  16QAM,  64QAM | QPSK,  16QAM,  64QAM |
| Category 33 | 15 | 1 | 42192 | 1555200 | 6 | 0 | - | - | - | QPSK, 16QAM, 64QAM | - |
| Category 34 | 15 | 1 | 42192 | 3110400 | 6 | 6 | - | - | - | QPSK, 16QAM, 64QAM | QPSK, 16QAM, 64QAM |
| Category 35 | 15 | 1 | 42192 | 2073600 | 8 | 0 | - | - | - | QPSK, 16QAM, 64QAM | - |
| Category 36 | 15 | 1 | 42192 | 4147200 | 8 | 8 | - | - | - | QPSK, 16QAM, 64QAM | QPSK, 16QAM, 64QAM |
| Category 37 | 15 | 1 | 42192 | 2073600 | 2 | 2 | 2 | - | - | QPSK, 16QAM, 64QAM | QPSK, 16QAM, 64QAM |
| Category 38 | 15 | 1 | 42192 | 4147200 | 4 | 4 | 4 | - | - | QPSK, 16QAM, 64QAM | QPSK, 16QAM, 64QAM |

For any category, in addition to the requirements in Table 5.1a, an HS-SCCH less capable UE shall allocate 24960 raw channel bits for HS-SCCH less operation in order to buffer the last 13 subframes and 13599 soft channel bits to receive 3 parallel HARQ processes.

UE Categories 1 to 4 and Category 11 do not support HS-DSCH reception in CELL\_FACH, CELL\_PCH or URA\_PCH states.

UEs of Category 13 are only required to support code rates up to 0.823 when 64QAM is used, which is represented by a limitation in the maximum value of *Ki*. in the transport block calculation in [9]. For other modulation formats, this restriction does not apply.

UEs of Category 15 are only required to support code rates up to 0.823 for 16QAM when two transport blocks are received in the same TTI, which is represented by a limitation in the maximum value of *Ki* in the transport block calculation in [9]. For other modulation formats or when a single transport block is received, this restriction does not apply.

UEs of Category 19 are only required to support code rates up to 0.823 when 64QAM is used when two transport blocks are received in the same TTI, which is represented by a limitation in the maximum value of *Ki*. in the transport block calculation in [9]. For other modulation formats or when a single transport block is received, this restriction does not apply.

UEs of Category 21 are only required to support code rates up to 0.823 when 16QAM is used, which is represented by a limitation in the maximum value of *Ki*. in the transport block calculation in [9]. For other modulation formats, this restriction does not apply.

UEs of Category 23 are only required to support code rates up to 0.823 when 64QAM is used, which is represented by a limitation in the maximum value of *Ki*. in the transport block calculation in [9]. For other modulation formats, this restriction does not apply.

UEs of category 25 are only required to support code rates up to 0.823 for 16QAM for one cell when two transport blocks are received in the same TTI on that cell, which is represented by a limitation in the maximum value of Ki in the transport block calculation. For other modulation formats or when a single transport block is received in a cell, this restriction does not apply on that cell.

UEs of category 27 are only required to support code rates up to 0.823 for 64QAM for one cell when two transport blocks are received in the same TTI on that cell, which is represented by a limitation in the maximum value of Ki in the transport block calculation. For other modulation formats or when a single transport block is received in a cell, this restriction does not apply on that cell.

A UE that supports categories greater or equal to category 13, also supports E-DPDCH.

A UE that supports categories greater or equal to category 13, also supports MAC-ehs.

NOTE 1: Depending on the HS-DSCH configuration, the indicated maximum number of bits of an HS-DSCH transport block does not have to correspond exactly to an entry in the transport block size table to be applied [9].

NOTE 2: A UE of category 17 supports the physical capabilities of categories 13 and 15, but not simultaneously. The first row of category 17 in table 5.1a specifies the capabilities when MIMO is not configured and the capabilities of category 13 apply, the second row specifies the capabilities when MIMO is configured and the capabilities of category 15 apply.

NOTE 3: A UE of category 18 supports the physical capabilities of categories 14 and 16, but not simultaneously. The first row of category 18 in table 5.1a specifies the capabilities when MIMO is not configured and the capabilities of category 14 apply, the second row specifies the capabilities when MIMO is configured and the capabilities of category 16 apply.

Table 5.1b: RLC and MAC-hs/MAC-ehs parameters for FDD HS-DSCH physical layer categories

| HS-DSCH category | Maximum number of AM RLC entities | Minimum total RLC AM and MAC-hs/MAC-ehs buffer size [kBytes] |
| --- | --- | --- |
| Category 1 | 6 | 50 |
| Category 2 | 6 | 50 |
| Category 3 | 6 | 50 |
| Category 4 | 6 | 50 |
| Category 5 | 6 | 50 |
| Category 6 | 6 | 50 |
| Category 7 | 8 | 100 |
| Category 8 | 8 | 100 |
| Category 9 | 8 | 150 |
| Category 10 | 8 | 150 |
| Category 11 | 6 | 50 |
| Category 12 | 6 | 50 |
| Category 13 | 8 | 300 |
| Category 14 | 8 | 300 |
| Category 15 | 8 | 400 |
| Category 16 | 8 | 400 |
| Category 17 | 8 | 400 |
| Category 18 | 8 | 400 |
| Category 19 | 8 | 600 |
| Category 20 | 8 | 600 |
| Category 21 | 8 | 400 |
| Category 22 | 8 | 400 |
| Category 23 | 8 | 600 |
| Category 24 | 8 | 600 |
| Category 25 | 8 | 1200 |
| Category 26 | 8 | 1200 |
| Category 27 | 8 | 1700 |
| Category 28 | 8 | 1700 |
| Category 29 | 8 | 1000 |
| Category 30 | 8 | 1800 |
| Category 31 | 8 | 1250 |
| Category 32 | 8 | 2300 |
| Category 33 | 8 | 1800 |
| Category 34 | 8 | 3400 |
| Category 35 | 8 | 2300 |
| Category 36 | 8 | 4400 |
| Category 37 | 8 | 2300 |
| Category 38 | 8 | 4400 |

Table 5.1c: 1.28 Mcps TDD HS-DSCH physical layer categories

| HS-DSCH category | Maximum number of HS-DSCH codes per timeslot | Maximum number of HS-DSCH timeslots per TTI | Maximum number of HS-DSCH transport channel bits that can be received within an HS-DSCH TTI | Total number of soft channel bits | Supported modulations without MIMO operation | Supported modulations simultaneous with MIMO operation |
| --- | --- | --- | --- | --- | --- | --- |
| Category 1 | 16 | 2 | 2788 | 11264 | QPSK | Not applicable  (MIMO not supported) |
| Category 2 | 16 | 2 | 2788 | 22528 |
| Category 3 | 16 | 2 | 2788 | 33792 |
| Category 4 | 16 | 2 | 5600 | 22528 | QPSK,16QAM |
| Category 5 | 16 | 2 | 5600 | 45056 |
| Category 6 | 16 | 2 | 5600 | 67584 |
| Category 7 | 16 | 3 | 8416 | 33792 |
| Category 8 | 16 | 3 | 8416 | 67584 |
| Category 9 | 16 | 3 | 8416 | 101376 |
| Category 10 | 16 | 4 | 11226 | 45056 |
| Category 11 | 16 | 4 | 11226 | 90112 |
| Category 12 | 16 | 4 | 11226 | 135168 |
| Category 13 | 16 | 5 | 14043 | 56320 |
| Category 14 | 16 | 5 | 14043 | 112640 |
| Category 15 | 16 | 5 | 14043 | 168960 |
| Category 16 | 16 | 3 | 12636 | 50688 | QPSK,16QAM, 64QAM | Not applicable  (MIMO not supported) |
| Category 17 | 16 | 3 | 12636 | 101376 |
| Category 18 | 16 | 3 | 12636 | 152064 |
| Category 19 | 16 | 4 | 16856 | 67584 |
| Category 20 | 16 | 4 | 16856 | 135168 |
| Category 21 | 16 | 4 | 16856 | 202752 |
| Category 22 | 16 | 5 | 21076 | 84480 |
| Category 23 | 16 | 5 | 21076 | 168960 |
| Category 24 | 16 | 5 | 21076 | 253440 |
| Category 25  NOTE 1 | 16 | 3 | 12636 | 152064 | QPSK,16QAM, 64QAM | -- |
| 8416 | 202752 | -- | QPSK,16QAM |
| Category 26  NOTE 2 | 16 | 4 | 16856 | 202752 | QPSK,16QAM, 64QAM | -- |
| 11226 | 270336 | -- | QPSK,16QAM |
| Category 27  NOTE 3 | 16 | 5 | 21076 | 253440 | QPSK,16QAM, 64QAM | -- |
| 14043 | 337920 | -- | QPSK,16QAM |
| Category 28 | 16 | 3 | 12636 | 304128 | QPSK,16QAM, 64QAM | QPSK,16QAM, 64QAM |
| Category 29 | 16 | 4 | 16856 | 405504 |
| Category 30 | 16 | 5 | 21076 | 506880 |

A UE in CELL\_FACH, CELL\_PCH or URA\_PCH state with HS-DSCH reception shall support the HS-DSCH physical layer category 9 and may support the total number of soft channel bits larger than that of the category 9 in table 5.1c. When HS-DSCH reception in CELL\_FACH, CELL\_PCH or URA\_PCH state is configured, the octet aligned table of transport block size for the HS-DSCH physical layer category 9 shall be used (see [9]).

NOTE 1: A UE of category 25 supports the physical capabilities of categories 18. The first row of category 25 in table 5.1c specifies the capabilities when MIMO is not configured and the capabilities of category 18 apply .The second row of category 25 in table 5.1c specifies the capabilities when MIMO is configured.

NOTE 2: A UE of category 26 supports the physical capabilities of categories 21. The first row of category 26 in table 5.1c specifies the capabilities when MIMO is not configured and the capabilities of category 21 apply .The second row of category 26 in table 5.1c specifies the capabilities when MIMO is configured.

NOTE 3: A UE of category 27 supports the physical capabilities of categories 24. The first row of category 27 in table 5.1c specifies the capabilities when MIMO is not configured and the capabilities of category 24 apply .The second row of category 27 in table 5.1c specifies the capabilities when MIMO is configured.

Table 5.1d: RLC and MAC-hs parameters for 1.28 Mcps TDD HS-DSCH physical layer categories

| HS-DSCH category | Maximum number of AM RLC entities | Minimum total RLC AM and MAC-hs buffer size [kBytes] |
| --- | --- | --- |
| Category 1 | 6 | 50 |
| Category 2 | 6 | 50 |
| Category 3 | 6 | 50 |
| Category 4 | 6 | 50 |
| Category 5 | 6 | 50 |
| Category 6 | 6 | 50 |
| Category 7 | 6 | 50 |
| Category 8 | 6 | 50 |
| Category 9 | 6 | 50 |
| Category 10 | 6 | 50 |
| Category 11 | 6 | 50 |
| Category 12 | 6 | 50 |
| Category 13 | 6 | 100 |
| Category 14 | 6 | 100 |
| Category 15 | 6 | 100 |
| Category 16 | 6 | 100 |
| Category 17 | 6 | 100 |
| Category 18 | 6 | 100 |
| Category 19 | 6 | 100 |
| Category 20 | 6 | 100 |
| Category 21 | 6 | 100 |
| Category 22 | 6 | 100 |
| Category 23 | 6 | 100 |
| Category 24 | 6 | 100 |
| Category 25 | 6 | 150 |
| Category 26 | 6 | 200 |
| Category 27 | 6 | 300 |
| Category 28 | 6 | 300 |
| Category 29 | 6 | 300 |
| Category 30 | 6 | 300 |

Table 5.1d-a: 1.28 Mcps TDD HS-DSCH physical layer categories (Multi-frequency HS-DSCH operation mode only)

| HS-DSCH category | Maximum number of the total HS-DSCH timeslots on the all assigned carriers per TTI | Maximum number of HS-DSCH transport channel bits that can be received within an HS-DSCH TTI | Total number of soft channel bits |
| --- | --- | --- | --- |
| Category 1 | 30 | 84258 | 1013760 |
| Category 2 | 30 | 84258 | 675840 |
| Category 3 | 30 | 84258 | 337920 |
| Category 4 | 24 | 67356 | 811008 |
| Category 5 | 24 | 67356 | 540672 |
| Category 6 | 24 | 67356 | 270336 |
| Category 7 | 18 | 50496 | 608256 |
| Category 8 | 18 | 50496 | 405504 |
| Category 9 | 18 | 50496 | 202752 |
| Category 10 | 15 | 42129 | 506880 |
| Category 11 | 15 | 42129 | 337920 |
| Category 12 | 15 | 42129 | 168960 |
| Category 13 | 12 | 33678 | 405504 |
| Category 14 | 12 | 33678 | 270336 |
| Category 15 | 12 | 33678 | 135168 |
| Category 16 | 9 | 25248 | 304128 |
| Category 17 | 9 | 25248 | 202752 |
| Category 18 | 9 | 25248 | 101376 |
| Category 19 | 30 | 126456 | 1520640 |
| Category 20 | 30 | 126456 | 1013760 |
| Category 21 | 30 | 126456 | 506880 |
| Category 22 | 24 | 101136 | 1216512 |
| Category 23 | 24 | 101136 | 811008 |
| Category 24 | 24 | 101136 | 405504 |
| Category 25 | 18 | 75816 | 912384 |
| Category 26 | 18 | 75816 | 608256 |
| Category 27 | 18 | 75816 | 304128 |
| Category 28 | 15 | 63228 | 760320 |
| Category 29 | 15 | 63228 | 506880 |
| Category 30 | 15 | 63228 | 253440 |
| Category 31 | 12 | 50568 | 608256 |
| Category 32 | 12 | 50568 | 405504 |
| Category 33 | 12 | 50568 | 202752 |
| Category 34 | 9 | 37908 | 456192 |
| Category 35 | 9 | 37908 | 304128 |
| Category 36 | 9 | 37908 | 152064 |
| Category 37 | 8 | 33712 | 405504 |
| Category 38 | 8 | 33712 | 270336 |
| Category 39 | 8 | 22452 | 270336 |
| Category 40 | 8 | 22452 | 180224 |
| Category 41 | 6 | 25272 | 304128 |
| Category 42 | 6 | 25272 | 202752 |
| Category 43 | 6 | 16832 | 202752 |
| Category 44 | 6 | 16832 | 135168 |

NOTE: UEs of Categories 1 to 18, 39, 40, 43 and 44 support QPSK and 16QAM. UEs of Categories 19 to 38, 41, and 42 support QPSK, 16QAM and 64QAM.

Table 5.1d-b: RLC and MAC-hs parameters for 1.28 Mcps TDD HS-DSCH physical layer categories (Multi-frequency HS-DSCH operation mode only)

| HS-DSCH category | Maximum number of AM RLC entities | Minimum total RLC AM and MAC-hs buffer size [kBytes] |
| --- | --- | --- |
| Category 1 | 6 | 500 |
| Category 2 | 6 | 500 |
| Category 3 | 6 | 500 |
| Category 4 | 6 | 400 |
| Category 5 | 6 | 400 |
| Category 6 | 6 | 400 |
| Category 7 | 6 | 300 |
| Category 8 | 6 | 300 |
| Category 9 | 6 | 250 |
| Category 10 | 6 | 250 |
| Category 11 | 6 | 250 |
| Category 12 | 6 | 200 |
| Category 13 | 6 | 200 |
| Category 14 | 6 | 200 |
| Category 15 | 6 | 200 |
| Category 16 | 6 | 150 |
| Category 17 | 6 | 150 |
| Category 18 | 6 | 150 |
| Category 19 | 6 | 1000 |
| Category 20 | 6 | 1000 |
| Category 21 | 6 | 1000 |
| Category 22 | 6 | 900 |
| Category 23 | 6 | 900 |
| Category 24 | 6 | 900 |
| Category 25 | 6 | 800 |
| Category 26 | 6 | 800 |
| Category 27 | 6 | 800 |
| Category 28 | 6 | 700 |
| Category 29 | 6 | 700 |
| Category 30 | 6 | 700 |
| Category 31 | 6 | 600 |
| Category 32 | 6 | 600 |
| Category 33 | 6 | 600 |
| Category 34 | 6 | 550 |
| Category 35 | 6 | 550 |
| Category 36 | 6 | 550 |
| Category 37 | 6 | 250 |
| Category 38 | 6 | 250 |
| Category 39 | 6 | 200 |
| Category 40 | 6 | 200 |
| Category 41 | 6 | 200 |
| Category 42 | 6 | 200 |
| Category 43 | 6 | 150 |
| Category 44 | 6 | 150 |

Table 5.1e: 3.84 Mcps TDD HS-DSCH physical layer categories

| HS-DSCH category | Maximum number of HS-DSCH codes per timeslot | Maximum number of HS-DSCH timeslots per TTI | Maximum number of HS-DSCH transport channel bits that can be received within an HS-DSCH TTI | Total number of soft channel bits |
| --- | --- | --- | --- | --- |
| Category 1 | 16 | 2 | 12000 | 52992 |
| Category 2 | 16 | 12 | 12000 | 52992 |
| Category 3 | 16 | 4 | 24000 | 105984 |
| Category 4 | 16 | 12 | 24000 | 105984 |
| Category 5 | 16 | 6 | 36000 | 158976 |
| Category 6 | 16 | 12 | 36000 | 158976 |
| Category 7 | 16 | 12 | 53000 | 211968 |
| Category 8 | 16 | 12 | 73000 | 264960 |
| Category 9 | 16 | 12 | 102000 | 317952 |

Table 5.1f: RLC and MAC-hs parameters for 3.84 Mcps TDD HS-DSCH physical layer categories

| HS-DSCH category | Maximum number of AM RLC entities | Minimum total RLC AM and MAC-hs buffer size [kBytes] |
| --- | --- | --- |
| Category 1 | 6 | 50 |
| Category 2 | 6 | 50 |
| Category 3 | 6 | 50 |
| Category 4 | 6 | 50 |
| Category 5 | 6 | 100 |
| Category 6 | 6 | 100 |
| Category 7 | 6 | 150 |
| Category 8 | 8 | 150 |
| Category 9 | 8 | 200 |

Table 5.1f-a: 7.68 Mcps TDD HS-DSCH physical layer categories

| HS-DSCH category | Maximum number of HS-DSCH codes per timeslot | Maximum number of HS-DSCH timeslots per TTI | Maximum number of HS-DSCH transport channel bits that can be received within an HS-DSCH TTI | Total number of soft channel bits |
| --- | --- | --- | --- | --- |
| Category 1 | 32 | 1 | 12000 | 52992 |
| Category 2 | 32 | 12 | 12000 | 52992 |
| Category 3 | 32 | 2 | 24000 | 105984 |
| Category 4 | 32 | 12 | 24000 | 105984 |
| Category 5 | 32 | 3 | 36000 | 158976 |
| Category 6 | 32 | 12 | 36000 | 158976 |
| Category 7 | 32 | 4 | 53000 | 211968 |
| Category 8 | 32 | 12 | 53000 | 211968 |
| Category 9 | 32 | 5 | 73000 | 264960 |
| Category 10 | 32 | 12 | 73000 | 264960 |
| Category 11 | 32 | 8 | 106000 | 423936 |
| Category 12 | 32 | 12 | 106000 | 423936 |
| Category 13 | 32 | 12 | 204000 | 635904 |

Table 5.1f-b: RLC and MAC-hs parameters for 7.68 Mcps TDD HS-DSCH physical layer categories

| HS-DSCH category | Maximum number of AM RLC entities | Minimum total RLC AM and MAC-hs buffer size [kBytes] |
| --- | --- | --- |
| Category 1 | 6 | 50 |
| Category 2 | 6 | 50 |
| Category 3 | 6 | 50 |
| Category 4 | 6 | 50 |
| Category 5 | 6 | 100 |
| Category 6 | 6 | 100 |
| Category 7 | 6 | 150 |
| Category 8 | 6 | 150 |
| Category 9 | 8 | 150 |
| Category 10 | 8 | 150 |
| Category 11 | 8 | 200 |
| Category 12 | 8 | 200 |
| Category 13 | 8 | 400 |

Table 5.1g: FDD E-DCH physical layer categories

| E-DCH category | Maximum number of E-DCH codes transmittedper transport block | **Minimum spreading factor** | Support for 10 and 2 ms TTI EDCH | Maximum number of bits of an E-DCH transport block transmitted within a 10 ms E-DCH TTI | Maximum number of bits of an E-DCH transport block transmitted within a 2 ms E-DCH TTI |
| --- | --- | --- | --- | --- | --- |
| Category 1 | 1 | SF4 | 10 ms TTI only | 7110 | - |
| Category 2 | 2 | SF4 | 10 ms and 2 ms TTI | 14484 | 2798 |
| Category 3 | 2 | SF4 | 10 ms TTI only | 14484 | - |
| Category 4 | 2 | SF2 | 10 ms and 2 ms TTI | 20000 | 5772 |
| Category 5 | 2 | SF2 | 10 ms TTI only | 20000 | - |
| Category 6 | 4 | SF2 | 10 ms and 2 ms TTI | 20000 | 11484 |
| Category 7 | 4 | SF2 | 10ms and 2 ms TTI | 20000 | 22996 |
| Category 8 | 4 | SF2 | 2 ms TTI | - | 11484 |
| Category 9 | 4 | SF2 | 2 ms TTI | - | 22996 |
| Category 10 | 4 | SF2 | 2 ms TTI | - | 34507 |
| Category 11 | 4 | SF2 | 2 ms TTI | - | 22996 |
| Category 12 | 4 | SF2 | 2 ms TTI | - | 34507 |
| NOTE: When 4 codes are transmitted in parallel, two codes shall be transmitted with SF2 and two with SF4 | | | | | |

UEs of Categories 1 to 6 support QPSK only.

UEs of Category 7 supports QPSK (2 ms TTI, 10 ms TTI) and 16QAM (2 ms TTI).

UEs of Category 8 support only QPSK in Dual Cell E-DCH operation.

UEs of Category 9 support QPSK and 16QAM in Dual Cell E-DCH operation.

UEs of Category 10 support QPSK, 16QAM and 64QAM.

UEs of Category 11 support Uplink MIMO with QPSK and 16QAM.

UEs of Category 12 support Uplink MIMO with QPSK, 16QAM and 64QAM.

UEs of Category 8, 9, 10, 11 and 12 support MAC-i/is.

The values in the following Table 5.1h reflect the total buffer sizes of HS-DSCH and E-DCH categories for simultaneous HS-DSCH/E-DCH operation.

Table 5.1h: Total RLC and MAC-hs parameters for FDD HS-DSCH and E-DCH physical layer categories

| HS-DSCH category  E-DCH category | Cat. 1 to 4  [kBytes] | Cat. 5 and 6  [kBytes] | Cat. 7 and 8  [kBytes] | Category 9  [kBytes] | Cat. 10  [kBytes] | Cat. 11  [kBytes] | Cat. 12  [kBytes] |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Category 1** | 100 | 100 | 200 | 300 | 300 | 50 | 50 |
| **Categories 2 and 3** | 100 | 150 | 200 | 300 | 300 | 50 | 100 |
| **Category 5** | 100 | 150 | 200 | 300 | 300 | 100 | 100 |
| **Category 4** | - | 150 | 300 | 300 | 400 | 100 | 100 |
| **Category 6** | - | 200 | 300 | 400 | 400 | 150 | 150 |
| **Category 7** | - | 300 | 300 | 400 | 500 | 200 | 200 |
| **Category 8** | - | - | - | - | - | - | - |
| **Category 9** | - | - | - | - | - | - | - |
| **Category 10** | - | - | - | - | - | - | - |
| **Category 11** | - | - | - | - | - | - | - |
| **Category 12** | - | - | - | - | - | - | - |

| HS-DSCH category  E-DCH category | Categories 13 and 14  [kBytes] | Categories 15 and 16  [kBytes] | Categories 17 and 18  [kBytes] | Categories 19 and 20 [kBytes] | Categories 21 and 22 [kBytes] | Categories 23 and 24 [kBytes] |
| --- | --- | --- | --- | --- | --- | --- |
| **Category 1** | - | - | - | - | - | - |
| **Categories 2 and 3** | - | - | - | - | - | - |
| **Category 5** | 400 | - | - | - | - | - |
| **Category 4** | 400 | 400 | 400 | - | 400 | - |
| **Category 6** | 400 | 500 | 500 | 750 | 500 | 750 |
| **Category 7** | 500 | 500 | 500 | 750 | 500 | 750 |
| **Category 8** | - | - | - | - | 500 | 750 |
| **Category 9** | - | - | - | - | 750 | 750 |
| **Category 10** | - | - | - | 750 | 500 | 750 |
| **Category 11** | - | - | - | 750 | 750 | 750 |
| **Category 12** | - | - | - | 1000 | 750 | 1000 |

| HS-DSCH category  E-DCH category | Categories 25 and 26 [kBytes] | Categories 27 and 28 [kBytes] |
| --- | --- | --- |
| **Category 1** | - | - |
| **Categories 2 and 3** | - | - |
| **Category 5** | - | - |
| **Category 4** | 750 | - |
| **Category 6** | 750 | 1150 |
| **Category 7** | 1000 | 1150 |
| **Category 8** | 1000 | 1150 |
| **Category 9** | 1000 | 1250 |
| **Category 10** | 1000 | 1250 |
| **Category 11** | 1000 | 1250 |
| **Category 12** | 1000 | 1800 |

| HS-DSCH category  E-DCH category | Cat. 29  [kBytes] | Cat. 30  [kBytes] | Cat. 31  [kBytes] | Cat. 32  [kBytes] | Cat. 33  [kBytes] | Cat. 34  [kBytes] | Cat. 35  [kBytes] | Cat. 36  [kBytes] |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Category 6** | 1000 | 1800 | 1150 | 2300 | 1800 | 3400 | 2300 | 4400 |
| **Category 7** | 1000 | 1800 | 1150 | 2300 | 1800 | 3400 | 2300 | 4400 |
| **Category 8** | 1000 | 1800 | 1150 | 2300 | 1800 | 3400 | 2300 | 4400 |
| **Category 9** | 1000 | 1800 | 1250 | 2300 | 1800 | 3400 | 2300 | 4400 |
| **Category 10** | 1000 | 1800 | 1250 | 2300 | 1800 | 3400 | 2300 | 4400 |
| **Category 11** | 1000 | 1800 | 1250 | 2300 | 1800 | 3400 | 2300 | 4400 |
| **Category 12** | 1150 | 2000 | 1800 | 2550 | 2000 | 3500 | 2550 | 4500 |

| HS-DSCH category  E-DCH category | Category 37  [kBytes] | Category 38  [kBytes] |
| --- | --- | --- |
| **Category 6** | 2300 | 4400 |
| **Category 7** | 2300 | 4400 |
| **Category 8** | 2300 | 4400 |
| **Category 9** | 2300 | 4400 |
| **Category 10** | 2300 | 4400 |
| **Category 11** | 2300 | 4400 |
| **Category 12** | 2550 | 4500 |

NOTE: Maximum number of AM RLC entities for simultaneous HS-DSCH/E-DCH operation is defined in Table 5.1b.

Table 5.1i: 3.84Mcps TDD E-DCH physical layer categories

|  |  |  |
| --- | --- | --- |
| E-DCH category | maximum number of physical channel bits on E-UCH that can be transmitted in a 10ms TTI | Maximum number of bits of an E-DCH transport block that can be transmitted within a 10ms E-DCH TTI |
| Category 1 | 17360 | 12146 |
| Category 2 | 34752 | 24161 |
| Category 3 | 52416 | 36782 |
| Category 4 | 69536 | 53896 |
| Category 5 | 104864 | 92014 |

NOTE: A UE of any 3.84Mcps TDD category can transmit E-DCH on up to (and including) 12 timeslots at spreading factors between 1 and 16 subject to the capabilities in table 5.1i.

The values in the following Table 5.1j reflect the total buffer sizes of HS-DSCH and E-DCH categories for simultaneous HS-DSCH/E-DCH operation.

Table 5.1j - Total RLC and MAC-hs parameters for 3.84Mcps TDD HS-DSCH and E-DCH physical layer categories

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| HS-DSCH category  E-DCH category | Categories 1 / 2 [Kbytes] | Categories 3 / 4 [Kbytes] | Categories 5 / 6 [Kbytes] | Category 7 [Kbytes] | Category 8 [Kbytes] | Category 9 [Kbytes] |
| Category 1 | 100 | 100 | 150 | 200 | 300 | 400 |
| Category 2 | 100 | 150 | 200 | 300 | 300 | 400 |
| Category 3 | 150 | 150 | 200 | 300 | 300 | 400 |
| Category 4 | 150 | 200 | 300 | 300 | 300 | 400 |
| Category 5 | 300 | 300 | 300 | 300 | 300 | 400 |

NOTE: Maximum number of AM RLC entities for simultaneous HS-DSCH/E-DCH operation is defined in Table 5.1f.

Table 5.1k: 7.68Mcps TDD E-DCH physical layer categories

|  |  |  |
| --- | --- | --- |
| **E-DCH category** | **maximum number of physical channel bits on E-UCH that can be transmitted in a 10ms TTI** | **Maximum number of bits of an E-DCH transport block that can be transmitted within a 10ms E-DCH TTI** |
| Category 1 | 17360 | 12347 |
| Category 2 | 34752 | 24830 |
| Category 3 | 52416 | 36782 |
| Category 4 | 69536 | 54488 |
| Category 5 | 87200 | 73967 |
| Category 6 | 139104 | 104891 |
| Category 7 | 209760 | 177130 |

NOTE: A UE of any 7.68Mcps TDD category can transmit E-DCH on up to (and including) 12 timeslots at spreading factors between 1 and 32 subject to the capabilities in table 5.1k.

The values in the following Table 5.1l reflect the total buffer sizes of HS-DSCH and E-DCH categories for simultaneous HS-DSCH/E-DCH operation.

Table 5.1l: Total RLC and MAC-hs parameters for 7.68Mcps TDD HS-DSCH and E-DCH physical layer categories

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **HS-DSCH category**  **E-DCH category** | **Categories 1 / 2 [Kbytes]** | **Categories 3 / 4 [Kbytes]** | **Categories 5 / 6 [Kbytes]** | **Categories 7 / 8 [Kbytes]** | **Categories 9 / 10 [Kbytes]** | **Categories 11 / 12 [Kbytes]** | **Category 13 [Kbytes]** |
| Category 1 | 100 | 100 | 150 | 200 | 300 | 400 | 700 |
| Category 2 | 100 | 150 | 200 | 300 | 300 | 400 | 700 |
| Category 3 | 150 | 150 | 200 | 300 | 300 | 400 | 700 |
| Category 4 | 150 | 200 | 300 | 300 | 400 | 500 | 700 |
| Category 5 | 200 | 300 | 300 | 300 | 400 | 500 | 700 |
| Category 6 | 300 | 300 | 400 | 400 | 500 | 700 | 700 |
| Category 7 | 400 | 400 | 500 | 500 | 500 | 700 | 700 |

NOTE: Maximum number of AM RLC entities for simultaneous HS-DSCH/E-DCH operation is defined in Table 5.1f-b.

Table 5.1m: 1.28 Mcps TDD E-DCH physical layer categories

| E-DCH category | Maximum number of E – DCH timeslots per TTI | Maximum number of E – DCH transport channel bits that can be received within an E-DCH TTI |
| --- | --- | --- |
| Category 1 | 2 (Note 1, 3) | 2754 |
| Category 2 | 3 (Note 1, 3) | 4162 |
| Category 3 | 2 (Note 2, 3) | 5532 |
| Category 4 | 3 (Note 2, 3) | 8348 |
| Category 5 | 4 (Note 2, 3) | 11160 |
| Category 6 | 5 (Note 2, 3) | 11160 |

A UE in CELL\_FACH state with E-DCH transmission shall support the E-DCH physical layer category 3 in table 5.1m. When E-DCH transmission in CELL\_FACH state is configured, the formula to calculate the Transport Block Size shall be used according to the E-DCH physical layer category 3 (see [9]).

NOTE 1: Category 1 and category 2 UEs support QPSK only.

NOTE 2: Category 3, 4, 5 and 6 UEs support QPSK and 16QAM.

NOTE 3: All category UEs support up to 2 physical channels per timeslot unless 16QAM is adopted.

Table 5.1m-a: 1.28 Mcps TDD multi-carrier E-DCH physical layer categories

| E-DCH category | Maximum number of E – DCH timeslots per TTI |
| --- | --- |
| Category 1 | 4 |
| Category 2 | 6 |
| Category 3 | 9 |
| Category 4 | 12 |
| Category 5 | 15 |
| Category 6 | 18 |
| Category 7 | 24 |
| Category 8 | 30 |

The maximum number of E-DCH transport channel bits for multi-carrier E-DCH transmission equals to the sum of maximum number of E-DCH transport channel bits on each carrier which is determined by the UE’s single carrier categories as specified in Table 5.1m. For instance, if the UE reports multi-carrier category 2 and single carrier category 4 with 2 uplink carriers, the maximum number of E-DCH transport channel bits is 8348\*2=16696.

NOTE: All categorys UEs support QPSK and 16QAM.

The values in the following Table 5.1n reflect the total buffer sizes of HS-DSCH and E-DCH categories for simultaneous HS-DSCH/E-DCH operation.

Table 5.1n: Total RLC and MAC-hs parameters for 1.28 Mcps TDD HS-DSCH and E-DCH physical layer categories

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **HS-DSCH category**  **E-DCH category** | **Categories**  **1/2/3 [Kbytes]** | **Categories**  **4/5/6 [Kbytes]** | **Categories**  **7/8/9**  **[Kbytes]** | **Category**  **10/11/12**  **[Kbytes]** | **Category**  **13/14/15**  **[Kbytes]** |
| Category 1 | 100 | 100 | 150 | 200 | 300 |
| Category 2 | 100 | 150 | 200 | 300 | 300 |
| Category 3 | 150 | 150 | 200 | 300 | 300 |
| Category 4 | 150 | 150 | 200 | 300 | 300 |
| Category 5 | 150 | 200 | 300 | 300 | 400 |
| Category 6 | 200 | 300 | 300 | 300 | 400 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **HS-DSCH category**  **E-DCH category** | **Categories**  **16/17/18 [Kbytes]** | **Categories**  **19/20/21 [Kbytes]** | **Categories**  **22/23/24**  **[Kbytes]** | **Category**  **25[Kbytes]** | **Category**  **26 [Kbytes]** |
| Category 1 | 150 | 150 | 200 | 200 | 200 |
| Category 2 | 150 | 200 | 200 | 200 | 200 |
| Category 3 | 150 | 200 | 300 | 200 | 200 |
| Category 4 | 200 | 200 | 300 | 200 | 300 |
| Category 5 | 200 | 200 | 300 | 200 | 300 |
| Category 6 | 200 | 200 | 300 | 200 | 300 |

|  |  |  |
| --- | --- | --- |
| **HS-DSCH category**  **E-DCH category** | **Categories**  **27/28/29**  **[Kbytes]** | **Category**  **30**  **[Kbytes]** |
| Category 1 | 300 | 300 |
| Category 2 | 300 | 300 |
| Category 3 | 300 | 400 |
| Category 4 | 300 | 400 |
| Category 5 | 300 | 400 |
| Category 6 | 300 | 400 |

The values in the following Table 5.1n-a reflect the total buffer sizes of HS-DSCH and E-DCH categories for simultaneous HS-DSCH/E-DCH operation.

Table 5.1n-a: Total RLC and MAC-hs parameters for 1.28 Mcps TDD HS-DSCH and E-DCH physical layer categories (Multi-frequency HS-DSCH operation mode only)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **HS-DSCH category**  **E-DCH category** | **Categories**  **1/2/3 [Kbytes]** | **Categories**  **4/5/6 [Kbytes]** | **Categories**  **7/8/9**  **[Kbytes]** | **Category**  **10/11/12**  **[Kbytes]** | **Category**  **13/14/15**  **[Kbytes]** | **Category**  **16/17/18**  **[Kbytes]** |
| Category 1 | 500 | 400 | 300 | 250 | 200 | 150 |
| Category 2 | 500 | 400 | 300 | 250 | 200 | 150 |
| Category 3 | 500 | 400 | 300 | 250 | 200 | 150 |
| Category 4 | 500 | 400 | 300 | 300 | 200 | 150 |
| Category 5 | 600 | 400 | 300 | 300 | 250 | 200 |
| Category 6 | 600 | 500 | 400 | 300 | 250 | 200 |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **HS-DSCH category**  **E-DCH category** | **Categories**  **19/20/21 [Kbytes]** | **Categories**  **22/23/24 [Kbytes]** | **Categories**  **25/26/27**  **[Kbytes]** | **Category**  **28/29/30**  **[Kbytes]** | **Category**  **31/32/33**  **[Kbytes]** | **Category**  **34/35/36**  **[Kbytes]** |
| Category 1 | 750 | 600 | 500 | 400 | 300 | 300 |
| Category 2 | 750 | 600 | 500 | 400 | 300 | 300 |
| Category 3 | 750 | 600 | 500 | 400 | 400 | 300 |
| Category 4 | 750 | 600 | 500 | 400 | 400 | 300 |
| Category 5 | 750 | 600 | 500 | 400 | 400 | 300 |
| Category 6 | 750 | 600 | 500 | 400 | 400 | 300 |

|  |  |  |  |
| --- | --- | --- | --- |
| **HS-DSCH category**  **E-DCH category** | **Category**  **37/38**  **[Kbytes]** | **Category**  **39/40/43/44**  **[Kbytes]** | **Category**  **41/42**  **[Kbytes]** |
| Category 1 | 300 | 200 | 200 |
| Category 2 | 300 | 200 | 200 |
| Category 3 | 300 | 300 | 200 |
| Category 4 | 300 | 300 | 200 |

The values in the following Table 5.1n-b reflect the total buffer sizes of HS-DSCH and E-DCH categories for simultaneous multi-frequency HS-DSCH/E-DCH operation.

Table 5.1n-b: Total RLC and MAC-hs/MAC-ehs parameters for 1.28 Mcps TDD HS-DSCH and E-DCH physical layer categories (Multi-frequency E-DCH and HS-DSCH operation mode only)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **HS-DSCH category**  **E-DCH category** | **Categories**  **1/2/3 [Kbytes]** | **Categories**  **4/5/6 [Kbytes]** | **Categories**  **7/8/9**  **[Kbytes]** | **Category**  **10/11/12**  **[Kbytes]** | **Category**  **13/14/15**  **[Kbytes]** | **Category**  **16/17/18**  **[Kbytes]** |
| Category 1 | 1500 | 1150 | 1000 | 500 | 400 | 300 |
| Category 2 | 1500 | 1150 | 1000 | 500 | 400 | 300 |
| Category 3 | 1500 | 1150 | 1000 | 500  (Note) | 400  (Note) | 300  (Note) |
| Category 4 | 1500 | 1150 | 1000 | 500  (Note) | 400  (Note) | 400  (Note) |
| Category 5 | 1500 | 1150 | 1000 | 500  (Note) | 400  (Note) | 400  (Note) |
| Category 6 | 1500 | 1150 | 1000 | - | - | - |
| Category 7 | 1500 | 1150 | 1000 | - | - | - |
| Category 8 | 1500 | 1150 | 1000 | - | - | - |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **HS-DSCH category**  **E-DCH category** | **Categories**  **19/20/21 [Kbytes]** | **Categories**  **22/23/24 [Kbytes]** | **Categories**  **25/26/27**  **[Kbytes]** | **Category**  **28/29/30**  **[Kbytes]** | **Category**  **31/32/33**  **[Kbytes]** | **Category**  **34/35/36**  **[Kbytes]** |
| Category 1 | 2300 | 1800 | 1150 | 750 | 500 | 400 |
| Category 2 | 2300 | 1800 | 1150 | 750 | 500 | 400 |
| Category 3 | 2300 | 1800 | 1250 | 750  (Note) | 750  (Note) | 400  (Note) |
| Category 4 | 2300 | 1800 | 1250 | 750  (Note) | 750  (Note) | 500  (Note) |
| Category 5 | 2300 | 1800 | 1250 | 750  (Note) | 750  (Note) | 500  (Note) |
| Category 6 | 2300 | 1800 | 1250 | - | - | - |
| Category 7 | 2300 | 1800 | 1500 | - | - | - |
| Category 8 | 2300 | 1800 | 1500 | - | - | - |

|  |  |  |  |
| --- | --- | --- | --- |
| **HS-DSCH category**  **E-DCH category** | **Categories**  **37/38/**  **[Kbytes]** | **Categories**  **39/40/43/44 [Kbytes]** | **Categories**  **41/42 [Kbytes]** |
| Category 1 | 400 | 300 | 250 |
| Category 2 | 400 | 300 | 250 |

NOTE: Total RLC and MAC-hs/MAC-ehs parameters for E-DCH category 3, 4, 5 and HS-DSCH category form 10 to 18, 28 to 36 apply only for the UEs support smaller or equal to 3 carrier reception and transmission.

## 5.2 Reference UE radio access capability combinations

Based on required UE radio access capabilities to support reference RABs as defined in [2], this clause lists reference UE Radio Access capability combinations. Subclause 5.2.1 defines reference combinations of UE radio access capability parameters common for UL and DL. Subclauses 5.2.2 and 5.2.3 define reference combinations of UE radio access capability parameters that are separate for DL and UL respectively. A reference combination for common UL and DL parameters, one combination for UL parameters and one combination for DL parameters together relate to a UE with a certain implementation complexity, that allows support for one or several combined reference RABs. Combinations for UL and DL can be chosen independently. The bit rate supported by the selected combination of common UL and DL parameters needs to be at least as high as the maximum out of the supported bit rates of the selected combination of DL parameters and the selected combination of UL parameters. Different combinations have different levels of implementation complexity.

For defined reference RABs, it is possible to require a UE to meet a certain reference UE radio access capability combination. Each UE needs to have capabilities complying with a given reference radio access capability combination. Each individual radio access capability parameter as defined in subclause 5.1 shall be signalled.

The reference combination numbers shall not be used in the signalling of UE radio access capabilities between the UE and UTRAN. Reference UE radio access capability combinations provide default configurations that should be used as a basis for conformance testing against reference RABs.

The UE shall support at least the UE radio access capability parameter values as specified for the 12kbps UE reference class for both UL and DL.

Allowed values of UE capability parameters are limited by the defined range and granularity of values in subclause 5.1. Values might change depending on further definition of reference RABs for testing.

### 5.2.1 Combinations of common UE Radio Access Parameters for UL and DL

NOTE: Measurement-related capabilities are not included in the combinations. These capabilities are independent from the supported RABs.

Table 5.2.1.1: UE radio access capability parameter combinations,  
parameters common for UL and DL

| Reference combination of UE Radio Access capability parameters common for UL and DL | 12 kbps class | 32 kbps class | 64 kbps class | 128 kbps class | 384 kbps class | 768 kbps class | 2048 kbps class |
| --- | --- | --- | --- | --- | --- | --- | --- |
| PDCP parameters |  |  |  |  |  |  |  |
| Support for RFC 2507 | No | No | No/Yes NOTE 1 | No/Yes NOTE 1 | No/Yes NOTE 1 | No/Yes NOTE 1 | No/Yes NOTE 1 |
| Support for RFC 3095 | No/Yes NOTE 1 | No/Yes NOTE 1 | No/Yes NOTE 1 | No/Yes NOTE 1 | No/Yes NOTE 1 | No/Yes NOTE 1 | No/Yes NOTE 1 |
| Support for RFC 3095 context relocation | No/Yes  NOTE 1 | | | | | | |
| Support for loss-less SRNS relocation | No/Yes  NOTE 1 | | | | | | |
| Maximum header compression context space | Not applicable for conformance testing | | | | | | |
| Maximum number of ROHC context sessions | Not applicable for conformance testing | | | | | | |
| Support for Reverse decompression | No/Yes  NOTE 1 | | | | | | |
| RLC parameters |  |  |  |  |  |  |  |
| Total RLC AM buffer size (kbytes) | 10 | 10 | 10 | 50 | 50 | 100 | 500 |
| Maximum number of AM entities | 4 | 4 | 4 | 5 | 6 | 8 | 8 |
| Maximum RLC AM window size | 2047/4095  NOTE 1 | 2047/4095  NOTE 1 | 2047/4095  NOTE 1 | 2047/4095  NOTE 1 | 2047/4095  NOTE 1 | 2047/4095  NOTE 1 | 2047/4095  NOTE 1 |
| Multi-mode related parameters |  | | | | | | |
| Support of UTRA FDD | Yes/No  NOTE 1 | | | | | | |
| Support of UTRA TDD 3.84 Mcps | Yes/No  NOTE 1 | | | | | | |
| Support of UTRA TDD 1.28 Mcps | Yes/No  NOTE 1 | | | | | | |
| Multi-RAT related parameters |  | | | | | | |
| Support of GSM | Yes/No NOTE 1 | | | | | | |
| Support of multi-carrier | Yes/No  NOTE 1 | | | | | | |
| Support of UTRAN to GERAN Network Assisted Cell Change | Yes/No | | | | | | |
| Support of E-UTRA FDD | Yes/No  NOTE 1 | | | | | | |
| Support of E-UTRA TDD | Yes/No  NOTE 1 | | | | | | |
| **Security parameters** |  | | | | | | |
| Support of ciphering algorithm UEA0 | Yes | | | | | | |
| Support of ciphering algorithm UEA1 | Yes | | | | | | |
| Support of ciphering algorithm UEA2 | Yes | | | | | | |
| Support of integrity protection algorithm UIA1 | Yes | | | | | | |
| Support of integrity protection algorithm UIA2 | Yes | | | | | | |
| UE positioning related parameters |  | | | | | | |
| Standalone location method(s) supported | Yes/No  NOTE 1 | | | | | | |
| UE based OTDOA supported | Yes/No  NOTE 1 | | | | | | |
| Network assisted GPS support | Network based / UE based / Both/ None  NOTE 1 | | | | | | |
| Network Assisted GANSS support List | Per supported GANSS  NOTE 1 | | | | | | |
| >GANSS ID | Galileo / SBAS / Modernized GPS / QZSS / GLONASS/ BDS  NOTE 1 | | | | | | |
| >SBAS IDs | WAAS / EGNOS / MSAS / GAGAN  NOTE 1 | | | | | | |
| >GANSS mode | Network based / UE based / Both/ None  NOTE 1 | | | | | | |
| >GANSS Signal ID | 0..7  NOTE 1 | | | | | | |
| >GANSS Signal IDs | Yes/No (per GANSS signal)  NOTE 1 | | | | | | |
| >Support for GANSS timing of cell frames measurement | Yes/No  NOTE 1 | | | | | | |
| >Support for GANSS Carrier-Phase Measurement | Yes/No  NOTE 1 | | | | | | |
| >Support for non-native assistance choices | Yes/No  NOTE 1 | | | | | | |
| Support for GPS timing of cell frames measurement | Yes/No  NOTE 1 | | | | | | |
| Support for IPDL | Yes/No  NOTE 1 | | | | | | |
| Support for Rx-Tx time difference type 2 measurement | Yes/No  NOTE 1 | | | | | | |
| Support for UE Positioning assisted GPS measurement validity in CELL\_PCH and URA\_PCH RRC states | Yes | | | | | | |
| Support for SFN-SFN observed time difference type 2 measurement | Yes/No  NOTE 1 | | | | | | |
| Additional Positioning method support List | Per Additional Positioning method  NOTE 1 | | | | | | |
| >AddPos ID | Barometric Pressure, WLAN, Bluetooth, MBS  NOTE 1 | | | | | | |
| >AddPos mode | Standalone / UE assisted / Both  NOTE 1 | | | | | | |
| RF parameters for FDD |  | | | | | | |
| Radio frequency bands | The radio frequency bands defined in [4] | | | | | | |
| UE power class | 3 / 4 NOTE 1 | | | | | | |
| Tx/Rx frequency separation | Defined in [4] for the respective supported radio frequency band | | | | | | |
| RF parameters for TDD 3.84 Mcps |  | | | | | | |
| Radio frequency bands | A / b / c / a+b / a+c / b+c / a+b+c  NOTE 1 | | | | | | |
| UE power class | 2 / 3  NOTE 1 | | | | | | |
| **RF parameters for TDD 7.68 Mcps** |  | | | | | | |
| Radio frequency bands | A / b / c / a+b / a+c / b+c / a+b+c  NOTE 1 | | | | | | |
| UE power class | 2 / 3  NOTE 1 | | | | | | |
| **RF parameters for TDD 1.28 Mcps** |  | | | | | | |
| Radio frequency bands | A / b / c / a+b / a+c / b+c/ a+b+c  NOTE 1 | | | | | | |
| UE power class | 2 / 3  NOTE 1 | | | | | | |

NOTE 1: Options represent different combinations that should be supported with Conformance Tests.

### 5.2.2 Combinations of UE Radio Access Parameters for DL

Table 5.2.2.1: UE radio access capability parameter combinations, DL parameters

| Reference combination of UE Radio Access capability parameters in DL | 12 kbps class | 32 kbps class | 64 kbps class | 128 kbps class | 384 kbps class | 768 kbps class | 2048 kbps class |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Transport channel parameters |  |  |  |  |  |  |  |
| Maximum sum of number of bits of all transport blocks being received at an arbitrary time instant | 640 (FDD)  1280(TDD) | 1280 | 3840 | 3840 | 6400 | 10240 | 20480 |
| Maximum sum of number of bits of all convolutionally coded transport blocks being received at an arbitrary time instant | 640 | 640 | 640 | 640 | 640 | 640 | 640 |
| Maximum sum of number of bits of all turbo coded transport blocks being received at an arbitrary time instant | NA (FDD)  1280(TDD) | 1280 | 3840 | 3840 | 6400 | 10240 | 20480(1)  10240(2)  NOTE 5 |
| Maximum number of simultaneous transport channels | 4 | 8  NOTE 4 | 8  NOTE 4 | 8  NOTE 4 | 8  NOTE 4 | 8  NOTE 4 | 16  NOTE 4 |
| Maximum number of simultaneous CCTrCH (FDD) | 1 | 1  NOTE 3 | 1  NOTE 3 | 1  NOTE 3 | 1  NOTE 3 | 1  NOTE 3 | 1  NOTE 3 |
| Maximum number of simultaneous CCTrCH (TDD) | 1  NOTE 3 | 2  NOTE 3 | 3  NOTE 3 | 3  NOTE 3 | 3  NOTE 3 | 4  NOTE 3 | 4  NOTE 3 |
| Maximum total number of transport blocks received within TTIs that end at the same time | 4 | 8 | 8 | 16 | 32 | 64 | 96 |
| Maximum number of TFC | 16 | 32 | 48 | 96 | 128 | 256 | 1024 |
| Maximum number of TF | 32 | 32 | 64 | 64 | 64 | 128 | 256 |
| Support for turbo decoding | No (FDD)  Yes (TDD) | Yes | Yes | Yes | Yes | Yes | Yes |
| Support for loss-less DL RLC PDU size change | No | No | Yes/No | Yes/No | Yes/No | Yes/No | Yes/No |
| Physical channel parameters (FDD) |  |  |  |  |  |  |  |
| Maximum number of DPCH codes to be simultaneously received | 1 | 1 | 1 | 1 | 3 | 3 | 3 |
| Maximum number of physical channel bits received in any 10 ms interval (DPCH, S-CCPCH). | 1200 | 1200 | 2400 | 4800 | 19200 | 28800 | 57600 |
| Support for SF 512 and 80 ms TTI for DPCH | No | No | No | No | No | No | No |
| Support of HS-PDSCH | No | No | Yes/No  NOTE 1 | Yes/No  NOTE 1 | Yes/No  NOTE 1 | Yes/No  NOTE 1 | Yes/No  NOTE 1 |
| Physical channel parameters (TDD 3.84 Mcps) |  |  |  |  |  |  |  |
| Maximum number of timeslots per frame | 1 | 1 | 2 | 4 | 5 | 10 | 12 |
| Maximum number of physical channels per frame | 5 | 8 | 9 | 14 | 28 | 64 | 136 |
| Minimum SF | 16 | 16 | 16 | 16 | 1/16  NOTE 1 | 1/16  NOTE 1 | 1/16  NOTE 1 |
| Support of PDSCH | No | Yes/No  NOTE 1 | Yes | Yes | Yes | Yes | Yes |
| Support of HS-PDSCH | No | No | Yes/No  NOTE 1 | Yes/No  NOTE 1 | Yes/No  NOTE 1 | Yes/No  NOTE 1 | Yes/No  NOTE 1 |
| Maximum number of physical channels per timeslot | 5 | 8 | 9 | 9 | 9 | 9 | 13 |
| **Physical channel parameters (TDD 7.68 Mcps)** |  |  |  |  |  |  |  |
| Maximum number of timeslots per frame | 1 | 1 | 2 | 4 | 5 | 10 | 12 |
| Maximum number of physical channels per frame | 5 | 8 | 9 | 14 | 28 | 64 | 136 |
| Minimum SF | 32 | 32 | 32 | 32 | 1/32  NOTE 1 | 1/32  NOTE 1 | 1/32  NOTE 1 |
| Support of PDSCH | No | Yes/No  NOTE 1 | Yes | Yes | Yes | Yes | Yes |
| Support of HS-PDSCH | No | No | Yes/No  NOTE 1 | Yes/No  NOTE 1 | Yes/No  NOTE 1 | Yes/No  NOTE 1 | Yes/No  NOTE 1 |
| Maximum number of physical channels per timeslot | 5 | 8 | 9 | 9 | 9 | 9 | 13 |
| Physical channel parameters (TDD 1.28 Mcps) |  |  |  |  |  |  |  |
| Maximum number of timeslots per subframe | 1 | 1 | 2 | 3 | 4 | 6 | 6 |
| Maximum number of physical channels per subframe | 5 | 8 | 12 | 18 | 43 | 77 | 77 |
| Minimum SF | 16 | 16 | 16 | 16 | 1/16  NOTE 1 | 1/16  NOTE 1 | 1 |
| Support of PDSCH | No | Yes/No NOTE 1 | Yes | Yes | Yes | Yes | Yes |
| Support of HS-PDSCH | No | No | Yes/No  NOTE 1 | Yes/No  NOTE 1 | Yes/No  NOTE 1 | Yes/No  NOTE 1 | Yes/No  NOTE 1 |
| Maximum number of physical channels per timeslot | 5 | 8 | 11 | 14 | 14 | 14 | 14 |
| Support of 8PSK | No | No | No | No | No | No | Yes |

NOTE 1: Options represent different combinations that should be supported with conformance tests.

NOTE 3: The given number does not contain the BCH CCTrCH of the current cell nor of the neighbour cells.

NOTE 4: The given number does not contain the BCH of the neighbour cell.

NOTE 5: (1) For FDD and 3.84/7.68 Mcps TDD (2) For 1.28 Mcps TDD.

The reference combinations for HS-DSCH capabilities are shown in tables 5.2.2.2, 5.2.2.3 and 5.2.2.4.

Table 5.2.2.2: FDD UE radio access capability parameter combinations, DL HS-DSCH parameters

| Reference combination | 1.2 Mbps class | 3.6 Mbps class | 7 Mbps class | 10 Mbps class |
| --- | --- | --- | --- | --- |
| FDD HS-DSCH category | Category 1 | Category 5 | Category 7 | Category 9 |

Table 5.2.2.3: 1.28 Mcps TDD UE radio access capability parameter combinations, DL HS-DSCH parameters

| Reference combination | 0.5 Mbps class | 1.1 Mbps  class | 1.6 Mbps class | 2.2 Mbps class | 2.8 Mbps class |
| --- | --- | --- | --- | --- | --- |
| 1.28 Mcps TDD HS-DSCH Category | Category 1 | Category 4 | Category 7 | Category 10 | Category 13 |

Table 5.2.2.3-a: 1.28 Mcps TDD UE radio access capability parameter combinations, DL HS-DSCH parameters (Multi-frequency HS-DSCH operation mode only)

| **Reference combination** | **14 Mbps class** | **11.2 Mbps**  **class** | **8.4 Mbps class** | **7.0 Mbps class** | **5.6 Mbps class** | **4.2 Mbps class** |
| --- | --- | --- | --- | --- | --- | --- |
| 1.28 Mcps TDD HS-DSCH Category | Category 1 | Category 4 | Category 7 | Category 10 | Category 13 | Category 10 |

Table 5.2.2.4: 3.84 Mcps TDD UE radio access capability parameter combinations, DL HS-DSCH parameters

| Reference combination | 1.2 Mbps class | 2.4 Mbps class | 3.6 Mbps class | 7.3 Mbps class | 10.2 Mbps class |
| --- | --- | --- | --- | --- | --- |
| 3.84Mcps TDD HS-DSCH category | Category 1 | Category 3 | Category 5 | Category 8 | Category 9 |

Table 5.2.2.4a: 7.68 Mcps TDD UE radio access capability parameter combinations, DL HS-DSCH parameters

| Reference combination | 1.2 Mbps class | 2.4 Mbps class | 3.6 Mbps class | 7.3 Mbps class | 10.6 Mbps class |
| --- | --- | --- | --- | --- | --- |
| 7.68Mcps TDD HS-DSCH category | Category 1 | Category 3 | Category 5 | Category 9 | Category 11 |

The reference combinations for E-DCH capabilities are shown in tables 5.2.2.5, 5.2.2.6 and 5.2.2.7.

Table 5.2.2.5: FDD UE radio access capability parameter combinations, UL E-DCH parameters

| Reference combination | 0.7296 Mbps class | 1.4592 Mbps class | 2 Mbps class | 2.9185 Mbps class | 5.76 Mbps class |
| --- | --- | --- | --- | --- | --- |
| FDD E-DCH category | Category 1 | Categories 2 and 3 | Category 5 | Category 4 | Category 6 |

Table 5.2.2.6: 3.84Mcps TDD UE radio access capability parameter combinations, UL E-DCH parameters

| Reference combination | 1.2 Mbps class | 2.4 Mbps class | 3.6 Mbps class | 5.3 Mbps class | 9.2 Mbps class |
| --- | --- | --- | --- | --- | --- |
| 3.84Mcps TDD E-DCH category | Category 1 | Category 2 | Category 3 | Category 4 | Category 6 |

Table 5.2.2.7: 7.68Mcps TDD UE radio access capability parameter combinations, UL E-DCH parameters

| Reference combination | 1.2 Mbps class | 2.4 Mbps class | 3.6 Mbps class | 5.3 Mbps class | 10.6 Mbps class |
| --- | --- | --- | --- | --- | --- |
| 7.68Mcps TDD E-DCH category | Category 1 | Category 2 | Category 3 | Category 4 | Category 6 |

Table 5.2.2.8: 1.28Mcps TDD UE radio access capability parameter combinations, UL E-DCH parameters

| Reference combination | 0.5 Mbps class | 0.8 Mbps class | 1.1 Mbps class | 1.6 Mbps class | 2.2 Mbps class |
| --- | --- | --- | --- | --- | --- |
| 1.28Mcps TDD E-DCH category | Category 1 | Category 2 | Category 3 | Category 4 | Category 5 and 6 |

### 5.2.3 Combinations of UE Radio Access Parameters for UL

Table 5.2.3.1: UE radio access capability parameter combinations, UL parameters

| Reference combination of UE Radio Access capability parameters in UL | 12 kbps class | 32 kbps class | 64 kbps class | 128 kbps class | 384 kbps class | 768 kbps class |
| --- | --- | --- | --- | --- | --- | --- |
| Transport channel parameters |  |  |  |  |  |  |
| Maximum sum of number of bits of all transport blocks being transmitted at an arbitrary time instant | 640 | 640(FDD)  1280 (TDD) | 3840 | 3840 | 6400 | 10240 |
| Maximum sum of number of bits of all convolutionally coded transport blocks being transmitted at an arbitrary time instant | 640 | 640 | 640 | 640 | 640 | 640 |
| Maximum sum of number of bits of all turbo coded transport blocks being transmitted at an arbitrary time instant | NA | NA(FDD)  1280 (TDD) | 3840 | 3840 | 6400 | 10240 |
| Maximum number of simultaneous transport channels | 4 | 4 | 8 | 8 | 8 | 8 |
| Maximum number of simultaneous CCTrCH(TDD only) | 1  NOTE 3 | 1  NOTE 3 | 2  NOTE 3 | 2  NOTE 3 | 2  NOTE 3 | 2  NOTE 3 |
| Maximum total number of transport blocks transmitted within TTIs that start at the same time | 4 | 4 | 8 | 8 | 16 | 32 |
| Maximum number of TFC | 16 | 16 | 32 | 48 | 64 | 128 |
| Maximum number of TF | 32 | 32 | 32 | 32 | 32 | 64 |
| Support for turbo encoding | No | No (FDD)  Yes (TDD) | Yes | Yes | Yes | Yes |
| Physical channel parameters (FDD) |  |  |  |  |  |  |
| Maximum number of DPDCH bits transmitted per 10 ms | 600 | 1200 | 2400 | 4800 | 9600 | 19200 |
| Support of E-DPDCH | No | No | Yes/No | Yes/No | Yes/No | Yes/No |
| Physical channel parameters (TDD 3.84 Mcps) |  |  |  |  |  |  |
| Maximum Number of timeslots per frame | 1 | 1 | 2 | 3 | 7 | 9 |
| Maximum number of physical channels per timeslot | 1 | 1 | 1 | 1 | 1 | 2 |
| Minimum SF | 8 | 4 | 2 | 2 | 2 | 2 |
| Support of PUSCH | No | Yes/No  NOTE 1 | Yes | Yes | Yes | Yes |
| Support of E-PUCH | No | Yes/No | Yes | Yes | Yes | Yes |
| **Physical channel parameters (TDD 7.68 Mcps)** |  |  |  |  |  |  |
| Maximum Number of timeslots per frame | 1 | 1 | 2 | 3 | 7 | 9 |
| Maximum number of physical channels per timeslot | 1 | 1 | 1 | 1 | 1 | 2 |
| Minimum SF | 16 | 8 | 4 | 4 | 4 | 4 |
| Support of PUSCH | No | Yes/No  NOTE 1 | Yes | Yes | Yes | Yes |
| Support of E-PUCH | No | Yes/No | Yes | Yes | Yes | Yes |
| Physical channel parameters (TDD 1.28 Mcps) |  |  |  |  |  |  |
| Maximum Number of timeslots per subframe | 1 | 1 | 2 | 3 | 5 | 5 |
| Maximum number of physical channels per timeslot | 1 | 2/1  NOTE 1 | 2 | 2 | 2 | 2 |
| Minimum SF | 8 | 4 | 2 | 2 | 2 | 2 |
| Support of PUSCH | No | Yes/No  NOTE 1 | Yes | Yes | Yes | Yes |
| Support of 8PSK | No | No | No | No | No | No |
| Support of E-PUCH | No | Yes/No | Yes | Yes | Yes | Yes |

NOTE 1: Options represent different combinations that should be supported with conformance tests.

NOTE 3: This number does not contain the RACH CCTrCH.

Annex A (informative):  
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history TR 25.926** | | | | | | | |
| **Date** | **TSG #** | **TSG Doc.** | **CR** | **Rev** | **Subject/Comment** | **Old** | **New** |
| 03/2000 | RP-07 | RP-000052 | - | - | Approved at TSG-RAN #7 and placed under Change Control | - | 3.0.0 |
| 06/2000 | RP-08 | RP-000229 | 003 | 4 | Updated Ad Hoc changes | 3.0.0 | 3.1.0 |
|  | RP-08 | RP-000229 | 008 |  | CPCH note to the parameter definitions | 3.0.0 | 3.1.0 |
| 09/2000 | RP-09 | RP-000368 | 010 | 1 | TDD DL Physical Channel Capability per Timeslot | 3.1.0 | 3.2.0 |
|  | RP-09 | RP-000368 | 012 |  | Change to UE Capability definition | 3.1.0 | 3.2.0 |
|  | RP-09 | RP-000368 | 013 |  | Physical parameter changes | 3.1.0 | 3.2.0 |
| 12/2000 | RP-10 | RP-000578 | 014 |  | Removal of example RABs | 3.2.0 | 25.306 3.0.0 |
|  | RP-10 | RP-000578 | 015 | 2 | Correction on parameter "Maximum total number of transport blocks…" | 3.2.0 | 25.306 3.0.0 |
|  | RP-10 | RP-000578 | 016 |  | Change to UE multi-RAT capability | 3.2.0 | 25.306 3.0.0 |
|  | RP-10 | RP-000578 | 017 |  | Change from TR 25.926 to TS 25.306 | 3.2.0 | 25.306 3.0.0 |

| **Change history TS 25.306** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Date** | **TSG #** | **TSG Doc.** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New** |
| 03/2001 | RP-11 | RP-010024 | 001 |  |  | Downlink rate matching limitation | 3.1.0 |
|  | RP-11 | RP-010024 | 005 |  |  | Miscellaneous corrections and editorial clean-up | 3.1.0 |
|  | RP-11 | RP-010024 | 007 |  |  | Maximum number of AM entity | 3.1.0 |
|  | RP-11 | RP-010024 | 008 | 1 |  | Clarification of maximum number of TF | 3.1.0 |
|  | RP-11 | RP-010024 | 010 | 1 |  | Removal of the RLC PU concept | 3.1.0 |
|  | RP-11 | RP-010039 | 003 | 1 |  | 1.28 Mcps TDD | 4.0.0 |
|  | RP-11 | RP-010043 | 006 | 1 |  | DSCH related updates for UE capabilities for the UE Radio Access Capability parameter combinations | 4.0.0 |
|  | RP-11 | RP-010039 | 011 | 1 |  | Addition of ROHC | 4.0.0 |
| 06/2001 | RP-12 | RP-010307 | 013 |  |  | Clarification on the number of CCTrCHs to be received simultaneously by the UE | 4.1.0 |
|  | RP-12 | RP-010321 | 009 | 6 |  | Modified UE Capability for CPCH | 4.1.0 |
| 09/2001 | RP-13 | RP-010540 | 017 |  |  | Maximum number of simultaneous transport channels | 4.2.0 |
|  | RP-13 | RP-010540 | 019 |  |  | Clarification of FDD physical channel parameters | 4.2.0 |
|  | RP-13 | RP-010540 | 021 |  |  | Support of dedicated pilots for channel estimation | 4.2.0 |
|  | RP-13 | RP-010540 | 023 |  |  | Correction of UE capabilities regarding Rx-Tx time difference type 2 measurements | 4.2.0 |
| 12/2001 | RP-14 | RP-010758 | 026 |  |  | Correction on UL parameter "Maximum number of DPDCH bits per 10 ms" | 4.3.0 |
| 03/2002 | RP-15 | RP-020228 | 035 |  |  | Clarification on ICS version within UE radio access capabilities | 4.4.0 |
|  | RP-15 | RP-020242 | 037 | 1 |  | Clarification of Maximum number of TFC in the TFCS | 4.4.0 |
|  | RP-15 | RP-020237 | 039 |  |  | Support of UP measurement reporting in CELL\_PCH/URA\_PCH | 4.4.0 |
|  | RP-15 | RP-020094 | 029 | 2 |  | HSDPA UE capabilities | 5.0.0 |
| 06/2002 | RP-16 | RP-020325 | 044 |  |  | Security Capabilities | 5.1.0 |
|  | RP-16 | RP-020439 | 040 | 1 |  | Corrections in HSDPA UE capabilities | 5.1.0 |
|  | RP-16 | RP-020341 | 041 |  |  | HSDPA TDD UE capabilities | 5.1.0 |
|  | RP-16 | RP-020341 | 045 |  |  | DPCH capabilities with simultaneous HSDPA configuration | 5.1.0 |
|  | RP-16 | RP-020345 | 046 |  |  | RFC 3095 context relocation | 5.1.0 |
|  | RP-17 | RP-020555 | 047 |  |  | Introduction of HS-PDSCH capability definition and QPSK-only UE categories | 5.2.0 |
|  | RP-17 | RP-020555 | 048 |  |  | Mandatory Support of dedicated pilots for channel estimation | 5.2.0 |
| 12/2002 | RP-18 | RP-020717 | 054 | 1 |  | UE capability for RLC window size | 5.3.0 |
|  | RP-18 | RP-020857 | 051 |  |  | UE capability for RFC3095 operation | 5.3.0 |
|  | RP-18 | RP-020733 | 049 | 3 |  | HSDPA L2 buffer sizes | 5.3.0 |
|  | RP-18 | RP-020733 | 056 |  |  | Correction to Access Stratum release indicator | 5.3.0 |
|  | RP-18 | RP-020733 | 057 |  |  | Dedicated pilot bits for HS-DSCH | 5.3.0 |
| 03/2003 | RP-19 | RP-030113 | 061 |  |  | Network Assisted Cell Change from UTRAN to GERAN | 5.4.0 |
|  | RP-19 | RP-030113 | 062 |  |  | Modification to the number of soft channel bits required for HS-DSCH (TDD) | 5.4.0 |
| 06/2003 | RP-20 | RP-030291 | 067 |  |  | Extension of 32 kbps UE capability class | 5.5.0 |
|  | RP-20 | RP-030301 | 068 |  |  | Correction of maximum transport block sizes for UE categories | 5.5.0 |
|  | RP-20 | RP-030301 | 069 |  |  | SF1 corrections for TDD | 5.5.0 |
| 09/2003 | RP-21 | RP-030493 | 072 |  |  | Addition of memory unit in UE Radio Access Capabilities tables | 5.6.0 |
|  | RP-21 | RP-030482 | 075 |  |  | Correction of Maximum hc context space capability | 5.6.0 |
|  | RP-21 | RP-030482 | 078 |  |  | UE positioning support in the UE | 5.6.0 |
| 12/2003 | RP-22 | RP-030623 | 082 |  |  | Removal of reference combinations for HS-DSCH capabilities | 5.7.0 |
|  | RP-22 | RP-030614 | 085 |  |  | Definition of minimum UE capability class | 5.7.0 |
|  | RP-22 | RP-030614 | 088 |  |  | TDD Radio Access Parameters for UL 32kbs class UE’s | 5.7.0 |
|  | RP-22 | RP-030623 | 089 |  |  | Correction to HSDPA capability | 5.7.0 |
|  | RP-22 | - | - |  |  | Upgrade to Release 6 - no technical change | 6.0.0 |
| 03/2004 | RP-23 | RP-040102 | 093 |  |  | Simultaneous Reception of S-CCPCH and HS-DSCH | 6.1.0 |
|  | RP-23 | RP-040102 | 095 |  |  | Correction to memory check in the UE | 6.1.0 |
| 06/2004 | RP-24 | RP-040223 | 096 |  |  | Correction to memory handling in the UE | 6.2.0 |
| 12/2004 | RP-26 | RP-040479 | 098 |  |  | Alignment of MaxHcContextSpace | 6.3.0 |
| 03/2005 | RP-27 | RP-050065 | 101 |  |  | Support of DSCH | 6.4.0 |
|  | RP-27 | RP-050067 | 103 |  |  | Lossless DL RLC PDU size change | 6.4.0 |
|  | RP-27 | RP-050154 | 104 | 2 |  | Inclusion of UE capabilities for Enhanced Uplink | 6.4.0 |
|  | RP-27 | RP-050083 | 105 |  |  | Support of ROHC mandatory | 6.4.0 |
| 04/2005 |  |  |  |  |  | Inclusion of RP-27 change history in this table. | 6.4.1 |
| 06/2005 | RP-28 | RP-050314 | 0107 |  |  | Introduction of MBMS capability Part A and B | 6.5.0 |
|  | RP-28 | RP-050305 | 0109 |  |  | Feature Clean Up: Removal of 80 ms TTI for DCH for all other cases but when the UE supports SF512 | 6.5.0 |
|  | RP-28 | RP-050308 | 0111 |  |  | Feature Clean-up: Removal of DSCH (FDD) | 6.5.0 |
|  | RP-28 | RP-050309 | 0113 |  |  | Feature Clean Up: Removal of CPCH | 6.5.0 |
|  | RP-28 | RP-050310 | 0115 |  |  | Feature Clean Up: Removal of dedicated pilot as sole phase reference | 6.5.0 |
|  | RP-28 | RP-050311 | 0117 |  |  | Feature Clean Up: Removal of DRAC | 6.5.0 |
|  | RP-28 | RP-050327 | 0118 |  |  | E-DCH L2 Buffer sizes | 6.5.0 |
|  | RP-28 | RP-050317 | 0119 |  |  | RLC LI Optimization for VoiP | 6.5.0 |
| 09/2005 | RP-29 | RP-050480 | 0120 |  |  | Removal RLC-SDU alignment capability | 6.6.0 |
|  | RP-29 | RP-050480 | 0121 |  |  | Feature Clean Up: Removal of DRAC | 6.6.0 |
|  | RP-29 | RP-050480 | 0122 |  |  | Adding the UE capability for FDD Radio frequency bands | 6.6.0 |
|  | RP-29 | RP-050475 | 0123 |  |  | F-DPCH support for HS-DSCH supporting Ues | 6.6.0 |
|  | RP-29 | RP-050468 | 0124 |  |  | Introduction of MBMS capability for TDD | 6.6.0 |
|  | RP-29 | RP-050468 | 0125 |  |  | Correction of UE capability for MBMS | 6.6.0 |
|  | RP-29 | RP-050470 | 0126 |  |  | Correction on table 5.1g (FDD E-DCH physical layer categories) | 6.6.0 |
|  | RP-29 | RP-050470 | 0127 |  |  | E-DCH L2 Buffer sizes | 6.6.0 |
|  | RP-29 | RP-050469 | 0128 |  |  | Removal of fixed position for S-CCPCHs carrying MBMS channels | 6.6.0 |
|  | RP-29 | RP-50461 | 0130 |  |  | Correction of TB size and soft channel bits number for 1.28 Mcps TDD | 6.6.0 |
|  | RP-29 | RP-050484 | 0131 |  |  | Introduction of battery-limited device indication in UE capability | 6.6.0 |
|  | RP-29 | RP-050480 | 0132 |  |  | Introduction of REL-6 Access Stratum release indicator | 6.6.0 |
| 12/2005 | RP-30 | RP-050796 | 0133 |  |  | Tx/Rx frequency separation capability (FDD) | 6.7.0 |
|  | RP-30 | RP-050784 | 0134 |  |  | Feature cleanup and other leftovers | 6.7.0 |
|  | RP-30 | RP-050790 | 0135 | 1 |  | E-DCH L2 Buffer sizes | 6.7.0 |
|  | RP-30 | RP-050861 | 0136 | 1 |  | Introduction of Support of Handover to GAN | 6.7.0 |
| 03/2006 | RP-31 | RP-060090 | 0138 |  |  | Correction to number of RLC AM instances for HS | 6.8.0 |
|  | RP-31 | RP-060093 | 0141 | 1 |  | Inter-RAT PS Handover capability | 6.8.0 |
|  | RP-31 | RP-060098 | 0139 |  |  | 7.68 Mpcs TDD Option (Release 7) | 7.0.0 |
|  | RP-31 | RP-060099 | 0140 |  |  | Introduction of REL-7 access stratum release indicator | 7.0.0 |
| 09/2006 | RP-33 | RP-060614 | 0144 |  |  | Introduction of SIB 11bis | 7.1.0 |
|  | RP-33 | RP-060586 | 0145 |  |  | Introduction of 3.84 Mcps and 7.68 McpsTDD E-DCH | 7.1.0 |
| 12/2006 | RP-34 | RP-060713 | 0146 | 1 |  | Introduction of the new security algorithms UEA2 and UIA2 | 7.2.0 |
| 03/2007 | RP-35 | RP-070151 | 0147 |  |  | TTI values for MCCH RB configuration | 7.3.0 |
|  | RP-35 | RP-070150 | 0150 |  |  | Correction of the HS-DSCH physical layger categories of 1.28Mcps TDD | 7.3.0 |
|  | RP-35 | RP-070157 | 0152 |  |  | Introduction of 1.28 Mcps TDD E-DCH | 7.3.0 |
|  | RP-35 | RP-070161 | 0153 | 2 |  | Introducing MIMO in UE Capability specification | 7.3.0 |
|  | RP-35 | RP-070163 | 0155 |  |  | Introduction of 64QAM downlink in 25.306 | 7.3.0 |
| 06/2007 | RP-36 | RP-070402 | 0151 | 2 |  | Introducing 16QAM uplink support | 7.4.0 |
|  | RP-36 | RP-070395 | 0156 |  |  | Introduction of GAN PS handover | 7.4.0 |
|  | RP-36 | RP-070406 | 0158 |  |  | Support of RFC 3095 (ROHC) Compression | 7.4.0 |
|  | RP-36 | RP-070400 | 0159 |  |  | MBMS FDD and TDD Physical Layer Improvements | 7.4.0 |
|  | RP-36 | RP-070398 | 0160 |  |  | GANSS support to UE capabilities | 7.4.0 |
|  | RP-36 | RP-070403 | 0161 |  |  | UE capabilities for HS-DSCH reception in CELL\_PCH, URA\_PCH and CELL\_FACH states | 7.4.0 |
| 09/2007 | RP-37 | RP-070670 | 0163 | 1 |  | Introduction of HS-DSCH category for combined MIMO and DL64QAM | 7.5.0 |
|  | RP-37 | RP-070670 | 0164 |  |  | Code rate limitation for UE HSDPA Categories 13 and 15 | 7.5.0 |
|  | RP-37 | RP-070625 | 0166 |  |  | MBMS UE Capability for mapping MTCH/MSCH to legacy S-CCPCH | 7.5.0 |
|  | RP-37 | RP-070670 | 0167 |  |  | HSPA+ L2 Buffering | 7.5.0 |
|  | RP-37 | RP-070634 | 0168 | 1 |  | UE capabilities for Rel-7, with 'improved L2' optional | 7.5.0 |
|  | RP-37 | RP-070627 | 0171 | 2 |  | Specification of HS-SCCH less memory requirement | 7.5.0 |
|  | RP-37 | RP-070650 | 0173 |  |  | Introduction of the Multi-Carrier HS-DSCH physical layer categories for 1.28Mcps TDD | 7.5.0 |
|  | RP-37 | RP-070764 | 0174 |  |  | For the creation of RRC Rel-8 | 8.0.0 |
| 12/2007 | RP-38 | RP-070900 | 0176 | 1 |  | Correction to memory requirement for HS-SCCH less operation | 8.1.0 |
|  | RP-38 | RP-070903 | 0178 |  |  | Introduction of an additional UE category for 1.28Mcps TDD E-DCH | 8.1.0 |
|  | RP-38 | RP-070901 | 0180 |  |  | Clarification on MIMO and 64QAM UE categories | 8.1.0 |
|  | RP-38 | RP-070902 | 0182 |  |  | More improvement on dedicated carrier for 1.28 Mcps TDD MBMS | 8.1.0 |
|  | RP-38 | RP-070900 | 0184 |  |  | UE capability for E-DCH transmission time restriction and UE DRX in CPC | 8.1.0 |
|  | RP-38 | RP-070905 | 0186 |  |  | Correction to Control Information transmission with two logical channels | 8.1.0 |
|  | RP-38 | RP-070910 | 0187 |  |  | Introduction of CS voice over HSPA | 8.1.0 |
|  | RP-38 | RP-070907 | 0188 |  |  | Introduction of HS-DSCH category for combined MIMO and DL64QAM | 8.1.0 |
| 03/2008 | RP-39 | RP-080185 | 0190 | - |  | Clarification of uplink multicode capability for 1.28Mcps TDD | 8.2.0 |
|  | RP-39 | RP-080188 | 0192 | - |  | Code rate limitations for HS-DSCH UE cat 13 and 15 | 8.2.0 |
| 05/2008 | RP-40 | RP-080417 | 0193 | 1 |  | Introduction of 64QAM in UE capability specification for LCR TDD | 8.3.0 |
| 09/2008 | RP-41 | RP-080682 | 0195 | - |  | Ki restriction for UE HS-DSCH categories 13 and 15 | 8.4.0 |
|  | RP-41 | RP-080694 | 0196 | 1 |  | Introduction of E-UTRA support | 8.4.0 |
| 12/2008 | RP-42 | RP-081024 | 0200 | - |  | Introduction of additional UE categories for 1.28Mcps TDD 64QAM DL | 8.5.0 |
|  | RP-42 | RP-081022 | 0201 | 2 |  | Introduction of support of “Enhanced Uplink for CELL\_FACH State in FDD” and “Improved L2 for uplink” | 8.5.0 |
|  | RP-42 | RP-081030 | 0202 | 2 |  | Addition of UE categories for dual cell HSDPA | 8.5.0 |
|  | RP-42 | RP-081029 | 0203 | - |  | UE positioning capabilities for support of additional navigation satellite systems | 8.5.0 |
|  | RP-42 | RP-081102 | 0206 | 1 |  | 25.306 CR Introduction of UE Measurement Capability on frequency adjacent to intra-frequency | 8.5.0 |
|  | RP-42 | RP-081033 | 0207 | - |  | Introduction of optional features in Release 8 | 8.5.0 |
|  | RP-42 | RP-081127 | 0208 | 2 |  | Support for 3.84 Mcps MBSFN IMB operation | 8.5.0 |
| 03/2009 | RP-43 | RP-090114 | 0213 | - |  | Correction of RF parameters in 25.306 | 8.6.0 |
|  | RP-43 | RP-090147 | 0214 | - |  | 25.306 CR on Introduction of CPC for 1.28Mcps TDD | 8.6.0 |
|  | RP-43 | RP-090151 | 0216 | - |  | Value range for UE Measurement Capability on a frequency adjacent to intra-frequency | 8.6.0 |
|  | RP-43 | RP-090144 | 0218 | - |  | Update to UE capability for IMB MCCH reception | 8.6.0 |
|  | RP-43 | RP-090149 | 0219 | - |  | Introduction of MIMO for 1.28Mcps TDD | 8.6.0 |
| 06/2009 | RP-44 | RP-090506 | 0220 | 1 |  | Add description about the parameter of Need for Idle Interval | 8.7.0 |
|  | RP-44 | RP-090519 | 0223 | - |  | Clarification for the code rate restriction for Cat19 | 8.7.0 |
| 09/2009 | RP-45 | RP-090908 | 0228 | 1 |  | E-DCH TTI restriction for 16QAM | 8.8.0 |
|  | RP-45 | RP-090902 | 0232 | - |  | Making features “Using special value of HE field to indicate end of an SDU for RLC AM” optional, “Removing the constraint that the same HS-SCCH should be used in contiguous TTIs” and octet aligned HS-DSCH transport block table optional for non-64QAM UEs | 8.8.0 |
|  | RP-45 | RP-090910 | 0233 | 1 |  | Clarification on UE category of enhanced CELL\_FACH for 1.28Mcps TDD | 8.8.0 |
|  | RP-45 | RP-090901 | 0246 | - |  | Enhancing the Category Handling in UMTS | 8.8.0 |
| 09/2009 | RP-45 | RP-090921 | 0224 | 1 |  | Introduction of Band XIX | 9.0.0 |
|  | RP-45 | RP-090925 | 0230 | - |  | Introduction of TxAA extension for non-MIMO UEs | 9.0.0 |
|  | RP-45 | RP-090924 | 0231 | - |  | Introduction of Dual Cell operation with MIMO | 9.0.0 |
| 12/2009 | RP-46 | RP-091315 | 0248 | 1 |  | Making features “Absolute priority reselection to GERAN”, “Absolute priority reselection to UTRA inter-frequency” optional (Option1) | 9.1.0 |
|  | RP-46 | RP-091338 | 0249 | 1 |  | L2 buffer sizes for DC-MIMO and E-DCH category combinations | 9.1.0 |
|  | RP-46 | RP-091336 | 0250 | - |  | Email discussion outcome for [67b#17] UMTS: DC-HSUPA in 25.306 | 9.1.0 |
|  | RP-46 | RP-091339 | 0252 | - |  | RAN1 RAN2 alignment on TxAA | 9.1.0 |
|  | RP-46 | RP-091347 | 0253 | 2 |  | Introduction of TS0 capability for 1.28Mcps TDD | 9.1.0 |
|  | RP-46 | RP-091259 | 0255 | - |  | Support for carrier-specific STTD configuration for DC-HSDPA | 9.1.0 |
| 03/2010 | RP-47 | RP-100298 | 0256 | - |  | Clarification of code rates limitation for category 25/27 | 9.2.0 |
|  | RP-47 | RP-100306 | 0258 | - |  | Release 9 UE Capability: UTRA Home Node B Inbound Mobility related features | 9.2.0 |
|  | RP-47 | RP-100299 | 0264 | - |  | UE cat17/18 and signalling of Single Stream MiMo capability | 9.2.0 |
|  | RP-47 | RP-100297 | 0265 | 1 |  | dual band capability | 9.2.0 |
|  | RP-47 | RP-100282 | 0266 | - |  | Bounds to RoHC requirements for UEs supporting IMS | 9.2.0 |
| 06/2010 | RP-48 | RP-100547 | 0267 | 1 |  | Corrections to Inter-band measurement capability | 9.3.0 |
|  | RP-48 | RP-100549 | 0268 | - |  | Support MAC-ehs in Single Stream MIMO case | 9.3.0 |
| 09/2010 | RP-49 | RP-100846 | 0272 | - |  | Clarification on the code rate restriction in HS-DSCH UE Categories 19 | 9.4.0 |
|  | RP-49 | RP-100857 | 0273 | - |  | Clarification on the code rate restriction in HS-DSCH UE Categories 25 and 27 | 9.4.0 |
|  | RP-49 | - | - | - |  | v10.0.0 created based on v9.4.0 | 10.0.0 |
|  | RP-49 | RP-100863 | 0275 | 1 |  | Introduction of 4C-HSDPA categories | 10.0.0 |
| 12/2010 | RP-50 | RP-101366 | 0278 | 1 |  | Correction for value range of total RLC AM, MAC-hs and MAC-ehs buffer size | 10.1.0 |
|  | RP-50 | RP-101211 | 0279 | - |  | Correction for value range of total RLC AM, MAC-hs and MAC-ehs buffer size | 10.1.0 |
|  | RP-50 | RP-101213 | 0280 | 1 |  | Introduction of REL-10 access stratum release indicator | 10.1.0 |
|  | RP-50 | RP-101212 | 0282 | 1 |  | Introduction of REL-9 access stratum release indicator | 10.1.0 |
|  | RP-50 | RP-101366 | 0283 | - |  | Corrections on 25.306 for 4C-HSDPA | 10.1.0 |
|  | RP-50 | RP-101365 | 0284 | - |  | introduction of MC-HSUPA for 1.28Mcps TDD | 10.1.0 |
| 03/2011 | RP-51 | RP-110268 | 0287 | - |  | Correction of buffer sizes for 64QAM+MIMO, DC-HSDPA categories | 10.2.0 |
|  | RP-51 | RP-110279 | 0289 | - |  | Extend the carrier capability for Multi-Carrier HSDPA for 1.28Mcps TDD | 10.2.0 |
|  | RP-51 | RP-110264 | 0293 | - |  | Clarification to the carrier capability in Multi-Carrier HSDPA for 1.28Mcps TDD | 10.2.0 |
|  | RP-51 | RP-110282 | 0295 | - |  | Counter proposal to R2-110749 on UE capabilities for MDT | 10.2.0 |
|  | RP-51 | RP-110332 | 0297 | 1 |  | Combination of DB-HSDPA and MIMO | 10.2.0 |
| 06/2011 | RP-52 | RP-110825 | 0298 | 1 |  | Removing RoHC discrepancy | 10.3.0 |
|  | RP-52 | RP-110829 | 0301 | 2 |  | Addition of the missing Total RLC and MAC-hs parameters in UE HS-DSCH categories for 1.28Mcps TDD | 10.3.0 |
|  | RP-52 | RP-110838 | 0302 | 1 |  | Addition of the missing Total RLC and MAC-hs parameters in UE dual-carrier HS-DSCH categories for 1.28Mcps TDD | 10.3.0 |
|  | RP-52 | RP-110838 | 0303 | - |  | Correction to UE capability Support of MIMO with dual cell dual band operation | 10.3.0 |
|  | RP-52 | RP-110829 | 0306 | 1 |  | Correction to HS-DSCH physical layer categories for 1.28 Mcps TDD | 10.3.0 |
|  | RP-52 | RP-110672 | 0317 | - |  | Introduction of measurement ID extension | 10.3.0 |
| 09/2011 | RP-53 | RP-111285 | 0321 | 2 |  | Introduction of optional Rel-10 features | 10.4.0 |
|  | RP-53 | RP-111282 | 0329 | - |  | Clarification on DCHSUPA dependence on MAC-i/is | 10.4.0 |
|  | RP-53 | RP-111278 | 0331 | 1 |  | Correction to UE capability parameters for handover to CSG cell | 10.4.0 |
| 12/2011 | RP-54 | RP-111715 | 0332 | - |  | Correction of capability table | 10.5.0 |
|  | RP-54 | RP-111715 | 0333 | 2 |  | Addition of the missing value ranges for 1.28Mbps TDD capabilities | 10.5.0 |
|  | RP-54 | RP-111715 | 0336 | - |  | Introduction of the frequency specific compressed mode | 10.5.0 |
| 12/2011 | RP-54 | - | - | - |  | TS 25.306 v11.0.0 was created based on v10.5.0 | 11.0.0 |
|  | RP-54 | RP-111717 | 0334 | - |  | Introduction of 8C-HSDPA in 25.306 | 11.0.0 |
|  | RP-54 | RP-111718 | 0337 | - |  | Introduction of uplink CLTD in 25.306 | 11.0.0 |
|  | RP-54 | RP-111719 | 0338 | - |  | Introduction of uplink OLTD in 25.306 | 11.0.0 |
| 03/2012 | RP-55 | RP-120327 | 0343 | - |  | Add up several missing optional capabilities | 11.1.0 |
|  | RP-55 | RP-120327 | 0352 | 1 |  | Additional value for Total RLC AM Buffer Size value range | 11.1.0 |
| 06/2012 | RP-56 | RP-120812 | 0357 | - |  | Correction to definition of enhanced inter-frequency measurements without CM | 11.2.0 |
|  | RP-56 | RP-120815 | 0359 | 2 |  | Extend the carrier capability for two-carrier HSDPA for 1.28Mcps TDD | 11.2.0 |
| 09/2012 | RP-57 | RP-121369 | 0371 | 1 |  | Introduction of Multiflow in TS 25.306 | 11.3.0 |
|  | RP-57 | RP-121363 | 0373 | - |  | Correction on the carrier capability for two-carrier HSDPA for 1.28Mcps TDD | 11.3.0 |
|  | RP-57 | RP-121359 | 0378 | - |  | Voice support Capabilities | 11.3.0 |
| 12/2012 | RP-58 | RP-121923 | 0389 | - |  | Adding the capability of supporting MAC-ehs window size extension | 11.4.0 |
|  | RP-58 | RP-121818 | 0390 | 1 |  | CR on rSRVCC capability indicator to 25.306 | 11.4.0 |
|  | RP-58 | RP-121942 | 0391 | 1 |  | Introduction of 4Tx-HSDPA in 25.306 | 11.4.0 |
|  | RP-58 | RP-121941 | 0392 | 1 |  | Introduction of Further Enhancements to CELL\_FACH in 25.306 | 11.4.0 |
|  | RP-58 | RP-121943 | 0393 | 1 |  | Introduction of further Multiflow agreements in TS 25.306. | 11.4.0 |
|  | RP-58 | RP-121945 | 0394 | 1 |  | Introduction of MIMO with 64QAM HSUPA in 25.306 | 11.4.0 |
|  | RP-58 | RP-121937 | 0396 | - |  | Introduction of UM RLC re-establishment via reconfiguration | 11.4.0 |
|  | RP-58 | RP-121942 | 0399 | - |  | L2 buffer sizes for 4Tx-HSDPA and UL MIMO with 64QAM combinations | 11.4.0 |
|  | RP-58 | RP-121938 | 0400 | - |  | Introduction of non-contiguous multi-cell operation | 11.4.0 |
|  | RP-58 | RP-121958 | 0401 | - |  | Introduction of Inter-frequency measurements on configured carriers without compressed mode | 11.4.0 |
|  | RP-58 | RP-121922 | 0403 | - |  | Introduction of Multiple Frequency Band Indicators capability | 11.4.0 |
| 03/2013 | RP-59 | RP-130248 | 0404 | - |  | Introduction of definitions, symbols and abbreviations | 11.5.0 |
|  | RP-59 | RP-130249 | 0405 | - |  | Additional value for Total RLC AM Buffer Size value range | 11.5.0 |
|  | RP-59 | RP-130248 | 0407 | 1 |  | Introduction of Cells excluded from detected set measurements | 11.5.0 |
|  | RP-59 | RP-130239 | 0411 | - |  | Introducing an indication for support of the extended range of HS-DPCCH power offset | 11.5.0 |
|  | RP-59 | RP-130236 | 0413 | - |  | Extend 3G ANR Applicable RRC State | 11.5.0 |
|  | RP-59 | RP-130249 | 0414 | - |  | Introduction of the frequency specific compressed mode for the intra-band non-contiguous operation | 11.5.0 |
|  | RP-59 | RP-130239 | 0415 | 1 |  | Simultaneous operation of Multiflow HSDPA and STTD | 11.5.0 |
| 06/2013 | RP-60 | RP-130806 | 0417 | 1 |  | Cleanups for FE\_FACH related capabilities | 11.6.0 |
|  | RP-60 | RP-130806 | 0418 | - |  | Adding up the capability dependency for non-contiguous multi\_cell | 11.6.0 |
|  | RP-60 | RP-130809 | 0419 | - |  | Addition of abbreviations in 25.306 | 11.6.0 |
|  | RP-60 | RP-130806 | 0425 | 1 |  | Clarification of support for Multiflow with MIMO operation in different bands | 11.6.0 |
| 09/2013 | RP-61 | RP-131311 | 0433 | - |  | Introduction of UE capability signalling for wideband RSRQ measurements | 11.7.0 |
| 12/2013 | RP-62 | RP-131981 | 0439 | - |  | Introduction of capability bit for E-UTRA Multiple Frequency Band Indicators | 11.8.0 |
|  | RP-62 | RP-131995 | 0440 | - |  | Cleanup of wideband RSRQ measurement capability | 11.8.0 |
|  | RP-62 | RP-132004 | 0444 | - |  | Introduction of non-contiguous multi-cell with MIMO | 11.8.0 |
|  | RP-62 | RP-131995 | 0445 | - |  | Editorial correction | 11.8.0 |
|  | RP-62 | RP-131997 | 0441 | 1 |  | Introduction of BDS in UTRAN | 12.0.0 |
|  | RP-62 | RP-131996 | 0442 | 1 |  | Introduction of HSPA signalling enhancements for more efficient resource usage for LCR TDD | 12.0.0 |
| 03/2014 | RP-63 | RP-140347 | 0446 | - |  | Introduction of Cell\_FACH with Second DRX to 3G Logged MDT | 12.1.0 |
| 06/2014 | RP-64 | RP-140880 | 0449 | - |  | Introduction of Hetnet mobility enhancements | 12.2.0 |
|  | RP-64 | RP-140875 | 0450 | - |  | Introduction of cell reselection indication during uplink transmission with common E-DCH | 12.2.0 |
| 09/2014 | RP-65 | RP-141503 | 0464 | - |  | Introduction of DSAC and PPAC update in CELL\_DCH | 12.3.0 |
|  | RP-65 | RP-141501 | 0469 | - |  | Introduction of E-DCH decoupling operation | 12.3.0 |
|  | RP-65 | RP-141511 | 0473 | - |  | Extended measurements ID support mandatory | 12.3.0 |
|  | RP-65 | RP-141500 | 0474 | 1 |  | Introduction of DCH Enhancements | 12.3.0 |
|  | RP-65 | RP-141501 | 0470 | 1 |  | CR to 25.306 on introduction of Radio Links without DPCH/F-DPCH | 12.3.0 |
|  | RP-65 | RP-141501 | 0471 | - |  | CR to 25.306 on introduction of the DPCCH2 | 12.3.0 |
| 12/2014 | RP-66 | RP-142127 | 0477 | - |  | Introduction of the UE capabilities for Further EUL enhancements subfeatures | 12.4.0 |
|  | RP-66 | RP-142113 | 0479 | - |  | Multi-carrier configuration support at inter-RAT handover | 12.4.0 |
|  | RP-66 | RP-142116 | 0480 | - |  | CR to 25.306 on correction of Cell Reselection Indication Reporting | 12.4.0 |
|  | RP-66 | RP-142228 | 0481 | 1 |  | Introduction of the UL CLTD feedback from the Multiflow assisting cell | 12.4.0 |
|  | RP-66 | RP-142128 | 0482 | - |  | Introduction of increased UE carrier monitoring | 12.4.0 |
|  | RP-66 | RP-142140 | 0483 | 1 |  | Introduction of extended RSRQ value range and new RSRQ definition | 12.4.0 |
|  | RP-66 | RP-141984 | 0484 | - |  | UE capability signaling for WLAN/3GPP radio interworking | 12.4.0 |
| 03/2015 | RP-67 | RP-150372 | 0486 | - |  | Clarification for DRX enhancements | 12.5.0 |
|  | RP-67 | RP-150376 | 0485 | - |  | Editorial corrections | 12.5.0 |
| 09/2015 | RP-69 | RP-151440 | 0488 | 1 |  | Increased UE carrier monitoring E-UTRA support mandatory | 12.6.0 |
| 12/2015 | RP-70 | RP-152060 | 0495 | 1 |  | CR to 25.306 on the introduction of Downlink TPC enhancements for UMTS | 13.0.0 |
|  | RP-70 | RP-152065 | 0490 | 1 |  | Introduction of Dual Carrier HSUPA enhancements for UTRAN CS in TS 25.306 | 13.0.0 |
|  | RP-70 | RP-152058 | 0496 | 1 |  | Introduction of DB-DC-HSUPA | 13.0.0 |
|  | RP-70 | RP-152110 | 0497 | - |  | RAT-Independent positioning enhancements | 13.0.0 |
| 03/2016 | RP-71 | RP-160461 | 0498 | 2 |  | Introduction of capability for extended E-UTRA frequency priorities | 13.1.0 |
|  | RP-71 | RP-160466 | 0499 | 2 |  | Correction on signalling transmission control due to access group blocking of DTCH | 13.1.0 |
|  | RP-71 | RP-160470 | 0501 | 2 |  | Missing parameter values for access stratum release indication | 13.1.0 |
|  | RP-71 | RP-160461 | 0503 | 1 |  | Introduction of the UE capabilities for L2 and L3 Downlink enhancements subfeatures | 13.1.0 |
|  | RP-71 | RP-160470 | 0504 | 1 |  | CR to to 25.306 on updating the capability name for supporting power control algorithm 3 | 13.1.0 |
| 09/2016 | RP-73 | RP-161748 | 0508 | 1 |  | Introduction of RRC events for UPH reporting | 14.0.0 |
|  | RP-73 | RP-167148 | 0509 | 1 |  | Introduction of simultaneous setup and release of RABs and RBs | 14.0.0 |
| 12/2016 | RP-74 | RP-162319 | 0511 | - |  | Correction on dual band dual cell E-DCH capability | 14.1.0 |
|  | RP-74 | RP-162330 | 0512 | 3 |  | Introduction of HS-SCCH DRX operation in CELL\_FACH state | 14.1.0 |
|  | RP-74 | RP-162331 | 0513 | 2 |  | Introduction of Dual Cell E-DCH operation enhancements | 14.1.0 |
|  | RP-74 | RP-162327 | 0516 | - |  | Addition of REL-14 parameter value for Access Stratum release indicator | 14.1.0 |
| 03/2017 | RP-75 | RP-170648 | 0520 | 1 | B | Introduction of QoE Measurement Collection for streaming services | 14.2.0 |
| 06/2017 | RP-76 | RP-171242 | 0517 | 6 | A | Unclear naming of feature “Dual cell E-DCH operation” | 14.3.0 |
| 09/2017 | RP-77 | RP-171592 | 0522 | 1 | B | Introduction of Simplified HS-SCCH type 1 operation for UMTS | 15.0.0 |
| 03/2018 | RP-79 | RP-180067 | 0523 | - | C | Introduction of QoE Measurement Collection for MTSI services | 15.1.0 |
| 06/2018 | RP-80 | RP-180820 | 0524 | 2 | F | Addition of REL-15 parameter value for Access Stratum release indicator | 15.2.0 |
| 2020-07 | RP-88e | - | - | - | - | Upgrade to Rel-16 version without technical change | 16.0.0 |
| 2020-09 | RP-89e | RP-202081 | 0525 | 2 | F | Addition of REL-16 parameter value for Access Stratum release indicator | 16.1.0 |