3GPP TS 26.230 V16.0.0 (2020-07)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Services and System Aspects;

Cellular text telephone modem;

Transmitter bit exact C-code

(Release 16)

 

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.   
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.   
This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

Keywords

UMTS, GSM, modem

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

0 Scope [5](#__RefHeading___Toc517284501)

1 Normative references [5](#__RefHeading___Toc517284502)

2 Definitions and Abbreviations [5](#__RefHeading___Toc517284503)

3 C code structure [5](#__RefHeading___Toc517284504)

3.1 Contents of the C source code [6](#__RefHeading___Toc517284505)

3.2 Program execution [6](#__RefHeading___Toc517284506)

3.3 Code hierarchy [10](#__RefHeading___Toc517284507)

3.3.1 Initialization routines [10](#__RefHeading___Toc517284508)

3.3.2 Signal Processing Functions [11](#__RefHeading___Toc517284509)

3.4 Description of global constants used in the C-code [12](#__RefHeading___Toc517284510)

3.5 Type Definitions [13](#__RefHeading___Toc517284511)

3.6 Functions of the C Code [13](#__RefHeading___Toc517284512)

Annex A (informative): Change history [27](#__RefHeading___Toc517284513)

Foreword

This Technical Specification has been produced by T1P1.

The contents of the present document are subject to continuing work within the 3GPP TSG and may change following formal 3GPP approval. Should the 3GPP TSG modify the contents of this TS, it will be re-released by the 3GPP TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to 3GPP for information;

2 presented to 3GPP for approval;

3 Indicates 3GPP approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the specification;

# 0 Scope

This Technical Standard (TS) contains an electronic copy of the ANSI‑C code for the Cellular Text Telephone Modem (CTM) for reliable transmission of text telephone text via the speech channel of cellular networks. While CTM is generally usable with text in UCS coding, the example application linked to CTM in this document is limited to use the signals and character set of the Baudot type.

# 1 Normative references

This TS incorporates by dated and undated reference, provisions from other publications. These normative references are cited at the appropriate places in the text and the publications are listed hereafter. For dated references, subsequent amendments to or revisions of any of these publications apply to this TS only when incorporated in it by amendment or revision. For undated references, the latest edition of the publication referred to applies.

[1] 3GPP TS 26.226: "Cellular text telephone modem; General description".

[2] ISO/IEC 10646-1: "Information technology – Universal Multiple-Octet Coded Character Set (UCS) – Part 1: Architecture and Basic Multilingual Plane".

# 2 Definitions and Abbreviations

For the purposes of this TS, the following abbreviations apply:

CTM Cellular Text Telephone Modem

FEC Forward Error Correction

FSK Frequency Shift Key

HCO Hearing Carry Over, (individual may be able to hear, but cannot speak) Alternating transmission of speech and text.

PCM Pulse Code Modulation

RX Receive

TX Transmit

TTY Text Telephone

UCS Universal Multiple-Octet Coded Character Set

UTF UCS transformation format

VAD Voice Activity Detection

VCO Voice Carry Over, Alternating transmission of speech and text

# 3 C code structure

This clause gives an overview of the structure of the bit‑exact C code and provides an overview of the contents and organization of the C code attached to this document.

The C code has been verified on the following system.

- Sun Microsystems workstations with SUN SolarisTM operating system and the the Gnu C Compiler (gcc version 2.7.2.3) and GNU Make 3.77;

The C code has also been successfully compiled and used in the following environment, with the exception that it cannot be guaranteed that the upper part of the UCS code table in file ucs\_functions.c will be compiled correctly since it depends on the codepage setting of the environment.

- IBM PC/AT compatible computers with WindowsTM NT 4.0 operating system and Microsoft Visual C++ 6.0TM compiler.

## 3.1 Contents of the C source code

The distributed files with suffix "c" contain the source code and the files with suffix "h" are the header files. All these files are in the root level of the ZIP-archive.

Makefiles are provided for the platforms in which the C code has been verified (listed above). They are called "Makefile" for GNU Make and "Makefile.vc" for Microsoft Visual C++TM.

For the Sun Microsystems platform, an example shell script for a transmission via two signal adaptation modules is given in "test\_negotiation". For the Microsoft WindowsTM platform, no shell script or batch program is provided.

The software can be compiled using the commands

make all or gmake all in case of Gnu Make

nmake /f Makefile.vc in case of Microsoft Visual C++.

The executables are compiled into the directory ./solaris (in case of Gnu Make) or into the actual directory in case of Microsoft Visual C++TM.

The directory ./patterns provides the file baudot.pcm that serves as input signal for the test script test\_negotiation. All output data of test\_negotiation will be stored into the directory ./output. If required, this directory will be created by test\_negotiation automatically.

## 3.2 Program execution

The CTM signal adaptation module is implemented in the execuable adaptation\_switch (in case of Sun SolarisTM platform) or adaptation\_switch.exe (in case of the Micorsoft WindowsTM platform).

The program should be called like:

adaptation\_switch -ctmin <file> -ctmout <file>   
 -baudotin <file> -baudotout <file>

using the following parameters:

-ctmin <input\_file> input file with CTM signal

-ctmout <output\_file> output file for CTM signal

-baudotin <input\_file> input file with Baudot Tones

-baudotout <output\_file> output file for Baudot Tones   
 -textout <text\_file> output text file from CTM receiver (optional)  
 -numsamples <number> number of samples to process (optional)  
 -nonegotiation disables the negotiation (optional)

All files contain 16-bit linear encoded PCM audio samples, which are swapped according to the platform's endian type (Sun Microsystems platforms use big endian, Intel platforms use little endian). An example file baudot.pcm containing a Baudot Code modem signal (big endian) is provided in the subdirectory ./patterns.

Due to the fact that the signal adaptation module expects a successful negotiation before Baudot Code signals can be converted to CTM signals, the signal adaptation module has to be executed several times in two instances in order to execute a successful negotiation. For the Sun Microsystems platform, a shell script test\_negotiation is provided for executing the following structure:

----------- ctm\_forward -----------

baudot.pcm --->| | ---------------->| |---> baudot\_out.pcm

| adapt#1 | | adapt#2 |

/dev/null <---| | <----------------| |<--- /dev/zero

----------- ctm\_backward -----------

First, the adaptation module #1 is executed. At this first run, the signal ctm\_backward is not known. Therefore, the negotiation does not get a positive acknowledge, so that the transmission falls back to Baudot Tones.

Then signal adaptation module #2 is executed for the first time.

After that, adaptation module #1 is executed for the second time. With this second run, the signal ctm\_backward is valid. Therefore, the negotiation receives a valid acknowledge, so that CTM signals are transmitted.

At last, adaptation module #2 is executed for the second time. With this run, adaptation module #2 receives a valid CTM signal so that the baudot\_out.pcm signal can be generated.

After executing each of the modules twice, the signal baudot\_out.pcm is analyzed. This analysis is also performed by the program adaptation\_switch. First, the Baudot detector of adaptation\_switch is used for this analysis in order to examine whether the regenerated Baudot signal can be decoded correctly. In a second step it is examined whether the regenerated signal still contains any CTM preambles. This investigation is performed by means of the CTM detector that is integrated in adaptation\_switch. This last test fails if the CTM detector is able to detect any CTM preamble in the regenerated signal.

During the execution of the script test\_negotiation the following text output shall be generated:

=====================================================

Execute adaptation module #1 (first pass)

=====================================================

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

Cellular Text Telephone Modem (CTM) - Example Implementation for

Conversion between CTM and Baudot Code (use option -h for help)

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

number of samples to process: 100000

>>> Enquiry Burst generated! <<<

THE>>> Enquiry Burst generated! <<<

>>> Enquiry Burst generated! <<<

CELL

=====================================================

Execute adaptation module #2 (first pass)

=====================================================

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

Cellular Text Telephone Modem (CTM) - Example Implementation for

Conversion between CTM and Baudot Code (use option -h for help)

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

>>> CTM from far-end detected! <<<

>>> Enquiry From Far End Detected! <<<

THE>>> Enquiry From Far End Detected! <<<

>>> Enquiry From Far End Detected! <<<

CELL

=====================================================

Execute adaptation module #1 (second pass)

=====================================================

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

Cellular Text Telephone Modem (CTM) - Example Implementation for

Conversion between CTM and Baudot Code (use option -h for help)

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

>>> Enquiry Burst generated! <<<

THE>>> CTM from far-end detected! <<<

CELLULAR TEXT TELEPHONE MODEM (CTM) ALLOWS RELIABLE

TRANSMISSION OF A TEXT TELEPHONE CONVERSATION ALTERNATING

WITH A SPEECH CONVERSATION THROUGH THE EXISTING SPEECH

COMMUNICATION PATHS IN CELLULAR MOBILE PHONE SYSTEMS.

THIS RELIABILITY IS ACHIEVED BY AN IMPROVED MODULATION

TECHNIQUE, INCLUDING ERROR PROTECTION, INTERLEAVING AND

SYNCHRONIZATION.

=====================================================

Execute adaptation module #2 (second pass)

=====================================================

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

Cellular Text Telephone Modem (CTM) - Example Implementation for

Conversion between CTM and Baudot Code (use option -h for help)

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

>>> CTM from far-end detected! <<<

>>> Enquiry From Far End Detected! <<<

THE CELLULAR TEXT TELEPHONE MODEM (CTM) ALLOWS RELIABLE

TRANSMISSION OF A TEXT TELEPHONE CONVERSATION ALTERNATING

WITH A SPEECH CONVERSATION THROUGH THE EXISTING SPEECH

COMMUNICATION PATHS IN CELLULAR MOBILE PHONE SYSTEMS.

THIS RELIABILITY IS ACHIEVED BY AN IMPROVED MODULATION

TECHNIQUE, INCLUDING ERROR PROTECTION, INTERLEAVING AND

SYNCHRONIZATION.

====================================================================

Now we try to decode the regenerated Baudot signal. The text message

shall be decoded completely now...

====================================================================

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

Cellular Text Telephone Modem (CTM) - Example Implementation for

Conversion between CTM and Baudot Code (use option -h for help)

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

THE CELLULAR TEXT TELEPHONE MODEM (CTM) ALLOWS RELIABLE

TRANSMISSION OF A TEXT TELEPHONE CONVERSATION ALTERNATING

WITH A SPEECH CONVERSATION THROUGH THE EXISTING SPEECH

COMMUNICATION PATHS IN CELLULAR MOBILE PHONE SYSTEMS.

THIS RELIABILITY IS ACHIEVED BY AN IMPROVED MODULATION

TECHNIQUE, INCLUDING ERROR PROTECTION, INTERLEAVING AND

SYNCHRONIZATION.

=====================================================================

Testing whether the regenerated Baudot signal is free of CTM headers.

No CTM burst shall be detected now...

=====================================================================

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

Cellular Text Telephone Modem (CTM) - Example Implementation for

Conversion between CTM and Baudot Code (use option -h for help)

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

## 3.3 Code hierarchy

This section gives an overview of the hierarchy how the functions are used in the signal adaptation module. All standard C functions: printf(), fwrite(), etc. have been omitted. Also, all functions related to the asynchronous transfer between the signal processing functions by means of FIFO buffers (Shortint\_fifo\_push, Shortint\_fifo\_pop, etc.) are not listed in the charts.

The following functions are not part of the actual CTM bit exact specification but are included to allow demonstration of CTM in a Baudot environment:

- init\_baudot\_tonedemod

- init\_baudot\_tonemod

- baudot\_tonedemod

- convertUCScode2char

- convertChar2TTYcode

- baudot\_tonemod

- convertTTYcode2char

- convertChar2UCScode

### 3.3.1 Initialization routines

The following functions are called for the initialization of the signal adaptation module.

|  |  |  |
| --- | --- | --- |
| init\_baudot\_tonedemod |  |  |
| init\_baudot\_tonemod |  |  |
| init\_ctm\_transmitter | init\_interleaver | generate\_scambling\_sequence |
|  |  | m\_sequence |
|  | init\_tonemod |  |
|  | conv\_encoder\_init |  |
|  | generate\_resync\_sequence | m\_sequence |
|  | calc\_mute\_positions |  |
| init\_ctm\_receiver | init\_tonedemod | sin\_fip |
|  | viterbi\_init |  |
|  | calc\_mute\_positions |  |
|  | init\_deinterleaver | generate\_scambling\_sequence |
|  | init\_wait\_for\_sync | m\_sequence |
|  |  | generate\_scambling\_sequence |

### 3.3.2 Signal Processing Functions

The following functions are called during the main signal processing loop.

|  |  |  |
| --- | --- | --- |
| baudot\_tonedemod | iir\_filt |  |
| ctm\_receiver | tonedemod | rotate\_right |
|  |  | rotate\_left |
|  | wait\_for\_sync |  |
|  | reinit\_deinterleaver |  |
|  | viterbi\_reinit |  |
|  | diag\_deinterleaver |  |
|  | shift\_deinterleaver |  |
|  | mutingRequired |  |
|  | viterbi\_exec |  |
|  | reinit\_wait\_for\_sync |  |
|  | reinit\_deinterleaver |  |
|  | viterbi\_reinit |  |
|  | transformUTF2UCS |  |
| convertUCScode2char |  |  |
| convertChar2TTYcode |  |  |
| baudot\_tonemod |  |  |
| convertTTYcode2char |  |  |
| convertChar2UCScode |  |  |
| ctm\_transmitter | transformUCS2UTF |  |
|  | reinit\_interleaver |  |
|  | conv\_encoder\_exec |  |
|  | mutingRequired |  |
|  | diag\_interleaver |  |
|  | diag\_interleaver\_flush |  |
|  | tonemod |  |

## 3.4 Description of global constants used in the C-code

The following constants are defined in the file ctm\_defines.h

**Constant Value Description**



MAX\_IDLE\_SYMB 5 Number of Idle Symbols at End of Burst  
CHC\_RATE 4 Rate of the Error Protection  
CHC\_K 5 Constraint Length of the Error Protection  
SYMB\_LEN 40 Length of one CTM symbol

LENGTH\_TONE\_VEC 1 frame size  
LENGTH\_TX\_BITS 8 number of bits per 20 ms frame  
BITS\_PER\_SYMB 8 bits per symbol

NCYCLES\_0 2 Number of periods for symbol #0  
NCYCLES\_1 3 Number of periods for symbol #1  
NCYCLES\_2 4 Number of periods for symbol #2  
NCYCLES\_3 5 Number of periods for symbol #3  
  
THRESHOLD\_RELIABILITY\_FOR\_SUPPRESSING\_OUTPUT 100 Characters with lower reliability are suppressed  
THRESHOLD\_RELIABILITY\_FOR\_XCORR 200 Bits with lower reliability don't contribute to xcorr  
THRESHOLD\_RELIABILITY\_FOR\_GOING\_OFFLINE 100 Threshold for regarding a bit as unreliable  
MAX\_NUM\_UNRELIABLE\_GROSS\_BITS 400 Receiver goes offline after 400 unreliable bits  
NUM\_BITS\_GUARD\_INTERVAL 6 Number of muted bits between two bursts  
WAIT\_SYNC\_REL\_THRESHOLD\_0 20316 (=0.62) rel. threshold for preamble  
WAIT\_SYNC\_REL\_THRESHOLD\_1 17039 (=0.52) rel. threshold for preamble  
WAIT\_SYNC\_REL\_THRESHOLD\_2 23065 (=0.71) dto. in case that RX is already online  
RESYNC\_REL\_THRESHOLD 26542 Threshold for Resynchronization (=0.81)  
GUARD\_BIT\_SYMBOL 10 magic number indicating that a bit shall be muted  
intlvB 8 Interleaver block length (number of rows)  
intlvD 2 Interleaver block distance (interlace factor)  
demodSyncLns 1 Number of demodulator sync lines  
deintSyncLns 0 Number of deinterleaver sync lines

IDLE\_SYMB 0x16 UCS code for Idle Symbol

ENQU\_SYMB 0x05 UCS code for Enquiry Symbol

ENQUIRY\_TIMEOUT 3040 number of 20-ms frames for negotiation  
NUM\_ENQUIRY\_BURSTS 3 number of enquiry attempts  
NUM\_MUTE\_ROWS 4 Number of Intl. rows that shall be muted  
RESYNC\_SEQ\_LENGTH 32 length of the resynchronization sequence,   
 must be a multiple of 8  
NUM\_BITS\_BETWEEN\_RESYNC 352 Distance between two resync sequences, the value  
 NUM\_BITS\_BETWEEN\_RESYNC+RESYNC\_SEQ\_LENGTH

must be a multiple of CHC\_RATE, intlvB, and  
 BITS\_PER\_CHAR, and must be greater than  
 intlvB\*((intlvB-1)\*intlvD+NUM\_MUTE\_ROWS  
   
BAUDOT\_NUM\_INFO\_BITS 5 number of information bits per Baudot character  
BAUDOT\_SHIFT\_FIGURES 27 code of shift to figures symbol  
BAUDOT\_SHIFT\_LETTERS 31 code of shift to letters symbol  
BAUDOT\_BIT\_DURATION 176 must be 176 (for 45.45 baud) or 160 (50 baud)  
BAUDOT\_LP\_FILTERORDER 1 Order of the low-pass filters in function  
 baudot\_tonedemod()   
BAUDOT\_BP\_FILTERORDER 2 Order of the according band-pass filters, must  
 be equal to 2\*BAUDOT\_BP\_FILTERORDER

## 3.5 Type Definitions

In order to make the C code platform‑independent, the following type definitions have been used, which are defined in typedefs.h:

defined type meaning corresponding constants

----------------------------------------------------------

Char character (none)

Bool boolean true, false

Shortint 16-bit signed minShortint, maxShortint  
UShortint 16-bit unsigned minUShortint, maxUShortint

Longint 32-bit signed minLongint, maxLongint  
ULongint 32-bit unsigned minULongint, maxULongint

## 3.6 Functions of the C Code

void baudot\_tonedemod(Shortint\* toneVec, Shortint numSamples,

fifo\_state\_t\* ptrOutFifoState,

baudot\_tonedemod\_state\_t\* state);

Purpose: Demodulator for Baudot Tones

Defined in: baudot\_functions.c

Input Variables:

toneVec Vector containing the input audio signal

numSamples Length of toneVec

Input/Output Variables:

ptrOutFifoState Pointer to the state of the output shift register containing the demodulated TTY codes

state Pointer to the state variable of baudot\_tonedemod()

void baudot\_tonemod(Shortint inputTTYcode,

Shortint \*outputToneVec,

Shortint lengthToneVec,

Shortint \*ptrNumBitsStillToModulate,

baudot\_tonemod\_state\_t\* state);

Purpose: Modulator for Baudot Tones

Defined in: baudot\_functions.c

Input Variables:

inputTTYcode TTY code of the character that has to be modulated. inputTTYcode must be in the range 0...63, otherwise it is assumed that there is no character to modulate.

lengthToneVec Indicates how many samples have to be generated.

Output Variables:

outputToneVec Vector where the output samples are written to.

ptrNumBitsStillToModulate Indicates how many bits are still in the fifo buffer.

Input/Output Variables:

state Pointer to the state variable of baudot\_tonedemod()

void calc\_mute\_positions(Shortint \*mute\_positions,

Shortint num\_rows\_to\_mute,

Shortint start\_position,

Shortint B,

Shortint D);

Purpose: Calculation of the indices of the bits that have to be muted within one burst. The indices are returned in the vector mute\_positions.

Defined in: init\_interleaver.c

Shortint convertChar2ttyCode(char inChar);

Purpose: Conversion from character into TTY code

Defined in: baudot\_functions.c

Input Variables:

inChar character that shall be converted

Return Value: baudot code of the input or -1 in case that inChar is not valid (e.g. inChar=='\0')

UShortint convertChar2UCScode(char inChar);

Purpose: Conversion from character into UCS code (Universal Multiple-Octet Coded Character Set, Row 00 of the Multilingual plane according to ISO/IEC 10646-1). This routine only handles characters in the range 0..255 since that is all that is required for demonstration of Baudot support.

Defined in: ucs\_functions.c

Input Variables:

inChar character that shall be converted

Return Value: UCS code of the input or 0x0016 <IDLE> in case that inChar is not valid (e.g. inChar=='\0')

char convertTTYcode2char(Shortint ttyCode);

Purpose: Conversion from TTY code into Character

Defined in: baudot\_functions.c

Input Variables:

ttyCode Baudot code (must be within the range 0...63) or -1 if there is nothing to convert

Return Value:

character (or '\0' if ttyCode is not valid)

char convertUCScode2char(UShortint ucsCode);

Purpose: Conversion from UCS code into character (Universal Multiple-Octet Coded Character Set, Row 00 of the Multilingual plane according to ISO/IEC 10646-1). This routine only handles characters in the range 0..255 since that is all that is required for demonstration of Baudot support.

Defined in: ucs\_functions.c

Input Variables:

ucsCode UCS code index, must be within the range 0...255

Return Value: character (or '\0' if ucsCode is not valid)

void conv\_encoder\_exec(conv\_encoder\_t\* ptr\_state, Shortint\* in,

Shortint inbits, Shortint\* out);

Purpose: Execution of the convolutional encoder for error protection

Defined in: conv\_encoder.c

Input Variables:

in Vector with net bits

inbits Number of valid net bits in vector in

Output variables:

out Vector with the encoded gross bits. The gross bits are either 0 or 1. The vector out must have at least CHC\_RATE\*inbits elements.

Input/output variables:

\*ptr\_state state variable of the encoder

void conv\_encoder\_init(conv\_encoder\_t\* ptr\_state);

Purpose: Initialization of the convolutional encoder

Defined in: conv\_encoder.c

Output Variables:

\*ptr\_state Initialized state variable of the encoder

void ctm\_receiver(fifo\_state\_t\* ptr\_signal\_fifo\_state,

fifo\_state\_t\* ptr\_output\_char\_fifo\_state,  
 Bool\* ptr\_early\_muting\_required,

rx\_state\_t\* rx\_state);

Purpose: Runs the CTM Receiver for a block of (nominally) 160 samples. Due to the internal synchronization, the number of processed samples might vary between 156 and 164 samples. The input of the samples and the output of the decoded characters is handled via fifo buffers, which have to be initialized externally before using this function (see fifo.h for details).

Defined in: ctm\_receiver.c

input/output variables

\*ptr\_signal\_fifo\_state fifo state for the input samples

\*ptr\_output\_char\_fifo\_state fifo state for the output characters

\*ptr\_early\_muting\_required returns whether the original audio signal must not be forwarded. This is to guarantee that the preamble or resync sequence is detected only by the first CTM device, if several CTM devices are cascaded subsequently.

rx\_state pointer to the variable containing the receiver states

void ctm\_transmitter(UShortint ucsCode,

Shortint\* txToneVec,

tx\_state\_t\* tx\_state,

Shortint \*ptrNumBitsStillToModulate,

Bool sineOutput);

Purpose: Runs the CTM Transmitter for a block of 160 output samples, representing 8 gross bits.   
The bits, which are modulated into tones, are taken from an internal fifo buffer. If the fifo buffer is empty, zero-valued samples are generated. The fifo buffer is filled with channel-encoded and interleaved bits, which are generated internally by coding the actual input character. With each call of this function one or less input characters can be coded. If there is no character to for transmission, one of the following codes has be used:   
- 0x0016 <IDLE>: indicates that there is no character to transmit and that the transmitter should stay in idle mode, if it is currently already in idle mode. If the transmitter is NOT in idle mode, it might generate <IDLE> symbols in order to keep an active burst running. The CTM burst is terminated if five <IDLE> symbols have been generated consecutively.  
- 0xFFFF: although there is no character to transmit, a CTM burst is initiated in order to signal to the far-end side that CTM is supported. The burst starts with the <IDLE> symbol and will be continued with <IDLE> symbols if there are no regular characters handed over during the next calls of this function. The CTM burst is terminated if five <IDLE> symbols have been transmitted consecutively.   
In order to avoid an overflow of the internal fifo buffer, the variable \*ptrNumBitsStillToModulate should be checked before calling this function.

Defined in: ctm\_transmitter.c

input variables:

ucsCode UCS code of the character or one of the code 0x0016 or 0xFFFF

sineOutput must be false in regular mode; if true, a pure sine output signal is generated

output variables:

txToneVec output signal (vector of 160 samples)

input/output variables:

tx\_state pointer to the variable containing the transmitter states

void diag\_deinterleaver(Shortint \*out,

Shortint \*in,

Shortint num\_valid\_bits,

interleaver\_state\_t \*intl\_state);

Purpose: Corresponding deinterleaver to diag\_interleaver. An arbitrary number of bits can be interleaved, depending of the length of the vector "in". The vector "out", which must have the same length than "in", contains the interleaved samples. All states (memory etc.) of the interleaver are stored in the variable \*intl\_state. Therefore, a pointer to this variable must be handled to this function. This variable initially has to be initialized by the function init\_interleaver, which offers also the possibility to specify the dimensions of the deinterleaver matrix.

Defined in: diag\_deinterleaver.c

void diag\_interleaver(Shortint \*out,

Shortint \*in,

Shortint num\_bits,

interleaver\_state\_t \*intl\_state);

Purpose: Diagonal (chain) interleaver, based on block-by-block processing. An arbitrary number of bits can be interleaved, depending of the value num\_bits. The vector "out", which must have the same length than "in", contains the interleaved samples.  
All states (memory etc.) of the interleaver are stored in the variable \*intl\_state. Therefore, a pointer to this variable must be handled to this function. This variable initially has to be initialized by the function init\_interleaver(), which offers also the possibility to specify the dimensions of the interleaver matrix.

Defined in: diag\_interleaver.c

void diag\_interleaver\_flush(Shortint \*out,

Shortint \*num\_bits,

interleaver\_state\_t \*intl\_state);

Purpose: Execution of the diagonal (chain) interleaver without writing in new samples. The number of calculated output samples is returned via the value \*num\_bits.

Defined in: diag\_interleaver.c

void generate\_resync\_sequence(Shortint \*sequence);

Purpose: Generation of the sequence for resynchronization. The length of the sequence is defined by the global constant RESYNC\_SEQ\_LENGTH. The vector sequence must be allocated accordingly before calling this function.

Defined in: wait\_for\_sync.c

void generate\_scrambling\_sequence(Shortint \*sequence, Shortint length);

Purpose: Generation of the sequence used for scrambling. The sequence consists of 0 and 1 elements. The sequence is stored into the vector \*sequence and the length of the sequence is specified by the variable length.

Defined in: init\_interleaver.c

void init\_baudot\_tonedemod(baudot\_tonedemod\_state\_t\* state);

Purpose: Initialization of the demodulator for Baudot Tones

Defined in: baudot\_functions.c

Input/Output Variables:

state Pointer to the initialized state variable (must be allocated before calling init\_baudot\_tonedemod()

void init\_baudot\_tonemod(baudot\_tonemod\_state\_t\* state);

Purpose: Initialization of the modulator for Baudot Tones

Defined in: baudot\_functions.c

Input/Output Variables:

state Pointer to the initialized state variable (must be allocated before calling init\_baudot\_tonemod()

void init\_deinterleaver(interleaver\_state\_t \*intl\_state,  
 Shortint B, Shortint D);

Purpose: Initialization of the deinterleaver.

Defined in: init\_interleaver.c

void init\_ctm\_receiver(rx\_state\_t\* rx\_state);

Purpose: Initialization of the CTM Receiver.

Defined in: ctm\_receiver.c

output variables:

rx\_state pointer to a variable of rx\_state\_t containing the initialized states of the receiver

void init\_ctm\_transmitter(tx\_state\_t\* tx\_state);

Purpose: Initialization of the CTM Transmitter

Defined in: ctm\_transmitter.c

input/output variables

tx\_state pointer to a variable of tx\_state\_t containing initialized states of the transmitter

void init\_interleaver(interleaver\_state\_t \*intl\_state,

Shortint B, Shortint D,

Shortint num\_sync\_lines1, Shortint num\_sync\_lines2);

Purpose: Function for initialization of diag\_interleaver and diag\_deinterleaver, respectively. The dimensions of the interleaver must be specified:  
B = (horizontal) blocklength, D = (vertical distance)  
According to this specifications, this function initializes a variable of type interleaver\_state\_t.  
Additionally, this function adds two types of sync information to the bitstream. The first sync info is for the demodulator and consists of a sequence of alternating bits so that the tones produced by the modulator are not the same all the time. This is essential for the demodulator to find the transitions between adjacent bits. The bits for this demodulator synchronization simply precede the bitstream.   
The second sync info is for synchronizing the deinterleaver and of a m-sequence with excellent autocorrelation properties. These bits are positioned at the locations of the dummy bits, which are not used by the interleaver. In addition, even more bits for this can be spent by inserting additional sync bits, which precede the interleaver's bitstream. This is indicated by choosing num\_sync\_lines2>0.

Defined in: init\_interleaver.c

void init\_tonedemod(demod\_state\_t \*demod\_state);

Purpose: Initialization of one instance of the Tone Demodulator. The argument must contain a pointer to a variable of type demod\_state\_t, which contains all the memory of the tone demodulator. Each instance of tonedemod must have its own variable.

Defined In: tonedemod.c

void init\_wait\_for\_sync(wait\_for\_sync\_state\_t \*ptr\_wait\_state,

interleaver\_state\_t intl\_state);

Purpose: Initialization of the synchronization detector. The dimensions of the corresponding interleaver at the TX side must be specified by the variables B, D, and num\_sync\_lines2.

Defined In: wait\_for\_sync.c

Input Variables:

B (horizontal) blocklength

D (vertical) interlace factor

num\_Sync\_line2 number of interleaver lines with additional sync bits (see description of init\_interleaver())

Output Variables:

ptr\_wait\_state pointer to the state variable of the sync detector

int main(int argc, const char\*\* argv)

Purpose: main function of the signal adaptation Module

Defined in: adaptation\_switch.c

Bool mutingRequired(Shortint actualIndex,

Shortint \*mute\_positions,

Shortint length\_mute\_positions);

Purpose: Determines whether the actual bit has to be muted, i.e. whether it is contained in the vector mute\_positions.

Defined in: init\_interleaver.c

void m\_sequence(Shortint \*sequence, Shortint length);

Purpose: Calculates one period of an m-sequence (binary pseudo noise). The sequence is stored in the vector sequence, which must have a of (2^r)-1, where r is an integer number between 2 and 10. Therefore, with this release of m\_sequence, sequences of length 3, 7, 15, 31, 63, 127, 255, 511, or 1023 can be generated. The resulting sequence is bipolar, i.e. it has values -1 and +1.

Defined in: m\_sequence.c

void polynomials(Shortint rate, Shortint k,   
 Shortint\* polya, Shortint\* polyb,   
 Shortint\* polyc, Shortint\* polyd);

Purpose: Returns the polynomials for the convolutional encoder and the Viterbi decoder for various rates and constraint lengths. The following parameters are supported:  
rate = {2, 3, or 4}  
k = {3, 4, 5, 6, 7, 8, 9}

Defined in: conv\_poly.c

Input Variables:

rate Rate of the convolutional encoder (2, 3, or 4)

k Constraint length (length of the impulse response of the encoder)

Output Variables:

poly\_a Vector with polynomials #1

poly\_b Vector with polynomials #2

poly\_c Vector with polynomials #3 (only if rate > 2)

poly\_d Vector with polynomials #4 (only if rate > 3)

void reinit\_deinterleaver(interleaver\_state\_t \*intl\_state);

Purpose: Re-Initialization of the deinterleaver.

Defined in: init\_interleaver.c

void reinit\_interleaver(interleaver\_state\_t \*intl\_state);

Purpose: Re-initialization of the deinterleaver

Defined in: init\_interleaver.c

void reinit\_wait\_for\_sync(wait\_for\_sync\_state\_t \*ptr\_wait\_state);

Purpose: Reinitialization of synchronization detector. This function is used in case that a burst has been finished and the transmitter has switched into idle mode. After calling reinit\_wait\_for\_sync(), the function wait\_for\_sync() inhibits the transmission of the demodulated bits to the deinterleaver, until the next synchronization sequence can be detected.

Defined In: wait\_for\_sync.c

void shift\_deinterleaver(Shortint shift,

Shortint \*insert\_bits,

interleaver\_state\_t \*ptr\_state);

Purpose: Shift of the deinterleaver buffer by <shift> samples.  
shift>0 -> shift to the right  
shift<0 -> shift to the left  
The elements from <insert\_bits> are inserted into the resulting space. The vector <insert\_bits> must have at least abs(shift) elements.

Defined in: diag\_deinterleaver.c

Shortint sin\_fip(Shortint phase\_value);

Purpose: Fixed Point sine function, returns the following value:  
sin\_fip(phase\_value)  
 = round(32767\*sin(2\*pi\*50/8000\*phase\_value))   
phase\_value must be within the range [0...159]. This function can be used for calculating sine waveforms of frequencies that are integer-multiples of 50 Hz

Defined in: sin\_fip.c

void tonedemod(Shortint \*bits\_out,

Shortint \*rx\_tone\_vec,

Shortint num\_in\_samples,

Shortint \*ptr\_sampling\_correction,

demod\_state\_t \*demod\_state);

Purpose: Tone Demodulator for the CTM using one out of four tones for coding two bits in parallel within a frame of 40 samples (5 ms).  
The function has to be called for every frame of 40 samples of the received tone sequence. However, in order to track a non‑ideal of the transmitter's and the receiver's clock frequencies, one frame might be shorter (only 39 samples) or longer (41 samples). The length of the following frame is indicated by the variable \*sampling\_correction, which is calculated and returned by this function.

Defined in: tonedemod.c

input variables:

bits\_out contains the 39, 40 or 41 actual samples of the received tones; the bits are soft bits, i.e. they are in the range between -1.0 and 1.0, where the magnitude serves as reliability information

num\_in\_samples number of valid samples in bits\_out

output variables:

bits\_out contains the two actual decoded soft bits

sampling\_correction is either -1, 0, or 1 and indicates whether the next frame shall contain 39, 40, or 41 samples.

demod\_state contains all the memory of tonedemod. Must be initialized using the function init\_tonedemod()

void tonemod(Shortint \*tones\_out,

Shortint \*bits\_in,

Shortint num\_samples\_tones\_out,

Shortint num\_bits\_in,  
 mod\_state\_t \*mod\_state);

Purpose: Modulator for the CTM. The input vector bits\_in must contain the bits that have to be transmitted. The length of bits\_in must be even because always two bits are coded in parallel. Bits are either unipolar (i.e. {0, 1}) or bipolar (i.e. {-1, +1)}. The length of the output vector tones\_out must be 20 times longer than the length of bits\_in, since each pair of two bits is coded within a frame of 40 audio samples.

Defined In: tonemod.c

void transformUCS2UTF(UShortint ucsCode,

fifo\_state\_t\* ptr\_octet\_fifo\_state);

Purpose: Transformation from UCS code into UTF-8. UTF-8 is a sequence consisting of 1, 2, 3, or 5 octets (bytes). See ISO/IEC 10646‑1 Annex G.  
This routine only handles UCS codes in the range 0...0xFF since that is all that is required for the demonstration of Baudot support.

Defined In: ucs\_functions.c

Input Variables:

ucsCode UCS code index

Output Variables:

ptr\_octet\_fifo\_state pointer to the output fifo state buffer for the UTF-8 octets.

Bool transformUTF2UCS(UShortint \*ptr\_ucsCode,

fifo\_state\_t\* ptr\_octet\_fifo\_state)

Purpose: Transformation from UTF-8 into UCS code.  
  
This routine only handles UTF-8 sequences consisting of one or two octets (corresponding to UCS codes in the range 0...0xFF) since that is all that is required for the demonstration of Baudot support.

Defined In: ucs\_functions.c

Input/Output Variables:

ptr\_octet\_fifo\_state pointer to the input fifo state buffer for the UTF‑8 octets.

Output Variables:

\*ptr\_ucsCode UCS code index

Return Value:

true, if conversion was successful

false, if the input fifo buffer didn't contain enough octets for a conversion into UCS code. The output variable \*ptr\_ucsCode doesn't contain a value in this case.

void viterbi\_exec(Shortint\* inputword, Shortint length\_input,   
 Shortint\* out, Shortint\* num\_valid\_out\_bits,   
 viterbi\_t\* viterbi\_state);

Purpose: Execution of the Viterbi decoder

Defined in: viterbi.c

Input Variables:

inputword Vector with gross bits

length\_input Number of valid gross bits in vector inputword. length\_input must be an integer multiple of CHC\_RATE.

Output variables:

out Vector with the decoded net bits. The net bits are either 0 or 1.

\*num\_valid\_out\_bits Number of valid bits in vector out.

Input/output variables:

\*viterbi state state variable of the decoder

void viterbi\_init(viterbi\_t\* viterbi\_state);

Purpose: Initialization of the Viterbi decoder

Defined in: viterbi.c

Output Variables:

\*viterbi\_state Initialized state variable of the decoder

void viterbi\_reinit(viterbi\_t\* viterbi\_state);

Purpose: Re-Initialization of the Viterbi decoder. This function should be used for re-setting a Viterbi decoder that has already been initialized. In contrast to init\_viterbi(), this reinit function does not calculate the values of all members of viterbi\_state that do not change during the execution of the Viterbi algorithm.

Defined in: viterbi.c

Output Variables:

\*viterbi\_state Initialized state variable of the decoder

Bool wait\_for\_sync(Shortint \*out\_bits,

Shortint \*in\_bits,

Shortint num\_in\_bits,  
 Shortint num\_received\_idle\_symbols,

Shortint \*ptr\_num\_valid\_out\_bits,

Shortint \*ptr\_wait\_interval,

Shortint \*ptr\_resync\_detected,   
 Bool \*ptr\_early\_muting\_required,

wait\_for\_sync\_state\_t \*ptr\_wait\_state);

Purpose: This function shall be inserted between the demodulator and the deinterleaver. The function searches the synchronization bitstream and cuts all received heading bits. As long as no sync is found, this function returns \*ptr\_num\_valid\_out\_bits=0 so that the main program is able to skip the deinterleaver as long as no valid bits are available. If the sync info is found, the complete internal shift register is copied to out\_bits so that wait\_for\_sync can be transparent and causes no delay for future calls. \*ptr\_wait\_interval returns a value of 0 after such a synchronization indicating that this was a regular synchronization.  
  
Regularly, the initial preamble of each burst is used as sync info. In addition, the resynchronization sequences, which occur periodically during a running burst, are used as "back-up" synchronization in order to avoid loosing all characters of a burst, if the preamble was not detected.   
  
If the receiver is already synchronized on a running burst and the resynchronization sequence is detected, \*ptr\_resync\_detected returns a non-negative value in the range 0...num\_in\_bits-1 indicating at which bit the resynchronization sequence has been detected. If no resynchronization has been detected, \*ptr\_resync\_detected is -1. If the receiver is NOT synchronized and the resynchronization sequence is detected, the resynchronization sequence is used as initial synchronization. \*ptr\_wait\_interval returns a value of 32 in this case due to the different alignments of the synchronizations based on the preamble or the resynchronization sequence, respectively.  
  
In order to carry all bits, the minimum length of out\_bits must be  
in\_bits.size()-1 + ptr\_wait\_state->shift\_reg\_length

Defined In: wait\_for\_sync.c

InputVariables:

in\_bits Vector with bits from the demodulator. The vector's length can be arbitrarily chosen, i.e. according to the block length of the signal processing of the main program.

num\_in\_bits length of vector in\_bits

Output Variables:

num\_received\_idle\_symbols Number if idle symbols received coherently

out\_bits Vector with bits for the deinterleaver. The number of the valid bits is indicated by \*ptr\_num\_valid\_out\_bits.

\*ptr\_num\_valid\_out\_bits returns the number of valid output bits

\*ptr\_wait\_interval returns either 0 or 32

\*ptr\_resync\_detected returns a value –1, 0,...num\_in\_bits

\*ptr\_early\_muting\_required returns whether the original audio signal must not be forwarded. This is to guarantee that only the first CTM device will detect the preamble or resync sequence, if several CTM devices are cascaded subsequently.

Input/Output Variables:

ptr\_wait\_state state information. This variable must be initialized with init\_wait\_for\_sync().

Annex A (informative):  
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **TSG SA#** | **TSG Doc.** | **CR** | **Rev** | **Subject/Comment** | **Old** | **New** |
| 12-2000 | 10 | SP-000570 |  |  | Specification approved for Release 4 |  | 4.0.0 |
| 03-2001 | 11 | SP-010108 | 001 |  | Bug fix in source code of the CTM receiver | 4.0.0 | 5.0.0 |
| 05-2001 |  |  |  |  | Correct source code CTM attached | 5.0.0 | 5.0.1 |
| 07-2004 |  |  |  |  | Removed copyright terms and conditions in the source code CTM attached | 5.0.1 | 5.0.2 |
| 12-2004 | 26 |  |  |  | Version for Release 6 | 5.0.2 | 6.0.0 |
| 06-2007 | 36 |  |  |  | Version for Release 7 | 6.0.0 | 7.0.0 |
| 03-2008 | 39 | SP-080006 | 002 | 1 | Bug fix to baudot\_tonemod function in baudot\_functions.c | 7.0.0 | 7.1.0 |
| 12-2008 | 42 |  |  |  | Version for Release 8 | 7.1.0 | 8.0.0 |
| 12-2009 | 46 |  |  |  | Version for Release 9 | 8.0.0 | 9.0.0 |
| 03-2011 | 51 |  |  |  | Version for Release 10 | 9.0.0 | 10.0.0 |
| 09-2012 | 57 |  |  |  | Version for Release 11 | 10.0.0 | 11.0.0 |
| 09-2014 | 65 |  |  |  | Version for Release 12 | 11.0.0 | 12.0.0 |
| 12-2015 | 70 |  |  |  | Version for Release 13 | 12.0.0 | 13.0.0 |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2017-03 | 75 |  |  |  |  | Version for Release 14 | 14.0.0 |
| 2018-06 | 80 |  |  |  |  | Version for Release 15 | 15.0.0 |
| 2020-07 | - | - | - | - | - | Update to Rel-16 version (MCC) | **16.0.0** |