3GPP TS 28.674 V16.0.0 (2020-07)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Services and System Aspects;

Telecommunication management;

Home enhanced Node B (HeNB) Subsystem (HeNS)

Network Resource Model (NRM)

Integration Reference Point (IRP);

Requirements

(Release 16)

* *

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.  
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.   
This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

Keywords

Home enhanced Node B Subsystem, NRM, IRP, Converged Management

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword [5](#__RefHeading___Toc339594423)

Introduction [5](#__RefHeading___Toc339594424)

1 Scope [6](#__RefHeading___Toc339594425)

2 References [6](#__RefHeading___Toc339594426)

3 Definitions, symbols and abbreviations [6](#__RefHeading___Toc339594427)

3.1 Definitions [6](#__RefHeading___Toc339594428)

3.1 Abbreviations [7](#__RefHeading___Toc339594429)

4 Concepts and background [8](#__RefHeading___Toc339594430)

5 Requirements [8](#__RefHeading___Toc339594431)

Annex A (informative): Change history [9](#__RefHeading___Toc339594432)

# Foreword

This Technical Report has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# Introduction

The present document is part of a TS-family covering the 3rd Generation Partnership Project Technical Specification Group Services and System Aspects, Telecommunication Management; as identified below:

**28.674: Telecommunication management; Home enhanced Node B Subsystem (HeNS) Network Resource Model (NRM) Integration Reference Point (IRP); Requirements**

28.675: Telecommunication management; Home enhanced Node B Subsystem (HeNS) Network Resource Model (NRM) Integration Reference Point (IRP); Information Service (IS)

28.676: Telecommunication management; Home enhanced Node B Subsystem (HeNS) Network Resource Model (NRM) Integration Reference Point (IRP); Solution Set (SS) definitions

# 1 Scope

The document describes the requirements for Home eNodeB Subsystem (HeNS), which include Home eNodeB (HeNB) and Home eNodeB gateway (HeNB GW). The HeNS NRM IRP requirements are targeted on both HeNB and HeNB GW NRM.

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TS 25.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 32.101: "Telecommunication management; Principles and high level requirements".

[3] 3GPP TS 32.102: "Telecommunication management; Architecture".

[4] 3GPP TS 32.600: "Telecommunication management; Configuration Management (CM); Concept and high-level requirements".

[5] 3GPP TS 32.150: "Telecommunication management; Integration Reference Point (IRP) Concept and definitions".

[6] 3GPP TS 23.401: “General Packet Radio Service (GPRS) enhancements for Evolved Universal Terrestrial Radio Access Network (E-UTRAN) access”.

[7] 3GPP TS 36.300: "Evolved Universal Terrestrial Radio Access (E-UTRA) and Evolved Universal Terrestrial Radio Access (E-UTRAN); Overall description; Stage 2".

[8] 3GPP TS 32.107: "Telecommunication management; Fixed Mobile Convergence (FMC) Federated Network Information Model (FNIM)".

[9] 3GPP TS 28.620: "Telecommunication management; Fixed Mobile Convergence (FMC) Federated Network Information Model (FNIM) Umbrella Information Model (UIM)".

# 3 Definitions, symbols and abbreviations

## 3.1 Definitions

For the purposes of the present document, the following terms and definitions apply:

**Integration Reference Point (IRP):** See 3GPP TS 32.150 [5].

**Information Service (IS):** See 3GPP TS 32.150 [5].

**Solution Set (SS):** See 3GPP TS 32.150 [5].

**IRP Solution Set:** See 3GPP TS 32.101 [1].

## 3.1 Abbreviations

For the purposes of the present document, the following abbreviations apply:

HeNB Home eNodeB

GW Gateway

HeNB Home enhanced Node B

HeNS Home enhanced Node B Subsystem

IRP Integration Reference Point

IOC Information Object Class

NRM Network Resource Model

# 4 Concepts and background

HeNB Subsystem is defined in TS 23.401[6]. According to the definition, a HeNB Subsystem consists of a HeNB and optionally a HeNB GW. The HeNB Subsystem is connected by means of the standard S1 interface to the EPC (Evolved Packet Core), more specifically to the MME (Mobility Management Entity) by means of the S1-MME interface and to the Serving Gateway (S-GW) by means of the S1-U interface.

Detailed functions of HeNB and HeNB GW are described in TS 36.300 [7]. To be more specific, HeNB is a Customer Premise Equipment that offers the LTE-Uu Interface to the UE. And it could discovery a suitable Serving HeNB GW over S1 interface. A HeNB GW can relay UE-associated S1 application part messages between the MME serving the UE and the HeNB serving the UE. It could terminate non-UE associated S1 application part procedures towards the HeNB and towards the MME and optionally terminate S1-U interface with the HeNB and with the S-GW.

Based on the above characteristics, this specification defines respective HeNS NRM IRP requirements.

# 5 Requirements

The following general and high-level requirements apply for the present IRP:

a) IRP-related requirements in 3GPP TS 32.101 [2].

b) IRP-related requirements in 3GPP TS 32.102 [3].

c) IRP-related requirements in 3GPP TS 32.600 [4].

The NRM defined by this IRP:

d) Shall support communications for telecommunication network management purposes, including management of converged networks.

e) Is a member of the Federated Network Information Model (FNIM) [8] and its information is derived from FNIM Umbrella Information Model (UIM) [9]

In addition to the above, the following more specific requirements apply:

**REQ-HeNS\_GW-CON-001** The Network Resource Model defined by this IRP shall contain HeNB GW specific IOCs and related definitions..

**REQ-HeNS\_GW-CON-002** The Network Resource Model defined by this IRP shall provide support for enabling consistency between HeNB GW, HeNB and related EPC nodes.

Annex A (informative):   
Change history

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Change history | | | | | | | | |
| **Date** | **TSG #** | **TSG Doc.** | **CR** | **Rev** | **Subject/Comment** | **Cat** | **Old** | **New** |
| 2014-06 | SA#64 | SP-140360 | 001 | - | remove the feature support statements | F | 11.0.0 | 11.1.0 |
| 2014-10 | - | - | - | - | Update to Rel-12 version (MCC) |  | 11.1.0 | **12.0.0** |
| 2016-01 | - | - | - | - | Update to Rel-13 version (MCC) |  | 12.0.0 | **13.0.0** |
| 2017-03 | SA#75 | - | - | - | Promotion to Release 14 without technical change |  | 13.0.0 | **14.0.0** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2018-06 |  |  |  |  |  | Update to Rel-15 version (MCC) | 15.0.0 |
| 2020-07 | - | - | - | - | - | Update to Rel-16 version (MCC) | **16.0.0** |