3GPP TS 28.733 V16.0.0 (2020-07)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Services and System Aspects;

Telecommunication management;

Transport Network (TN) interface

Network Resource Model (NRM)

Integration Reference Point (IRP);

Solution Set (SS) definitions

(Release 16)

 

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP..  
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.  
This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

Keywords

NRM, IRP, Converged Management,Transport Network

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword [4](#__RefHeading___Toc398908768)

Introduction [4](#__RefHeading___Toc398908769)

1 Scope [5](#__RefHeading___Toc398908770)

2 References [5](#__RefHeading___Toc398908771)

3 Definitions and abbreviations [6](#__RefHeading___Toc398908772)

3.1 Definitions [6](#__RefHeading___Toc398908773)

3.2 Abbreviations [6](#__RefHeading___Toc398908774)

4 Solution Set Definitions [7](#__RefHeading___Toc398908775)

Annex A (normative): CORBA Solution Set [8](#__RefHeading___Toc398908776)

A.0 General [8](#__RefHeading___Toc398908777)

A.1 Architectural features [8](#__RefHeading___Toc398908778)

A.1.0 Introduction [8](#__RefHeading___Toc398908779)

A.1.1 Syntax for Distinguished Names [8](#__RefHeading___Toc398908780)

A.1.2 Rules for NRM extensions [8](#__RefHeading___Toc398908781)

A.2 Mapping [8](#__RefHeading___Toc398908782)

A.2.1 General mapping [8](#__RefHeading___Toc398908783)

A.2.2 Information Object Class (IOC) mapping [8](#__RefHeading___Toc398908784)

A.2.2.1 IOC TransportNetworkInterface [8](#__RefHeading___Toc398908785)

A.2.2.2 IOC ATMChannelTerminationPoint [9](#__RefHeading___Toc398908786)

A.2.2.3 IOC ATMPathTerminationPoint [9](#__RefHeading___Toc398908787)

A.3 Solution Set definitions [10](#__RefHeading___Toc398908788)

A.3.1 IDL definition structure [10](#__RefHeading___Toc398908789)

A.3.2 IDL specification “TransportNetworkResourcesNRMDefs.idl” [11](#__RefHeading___Toc398908790)

Annex B (normative): XML Definitions [12](#__RefHeading___Toc398908791)

B.0 General [12](#__RefHeading___Toc398908792)

B.1 Architectural features [12](#__RefHeading___Toc398908793)

B.1.0 Introduction [12](#__RefHeading___Toc398908794)

B.1.1 Syntax for Distinguished Names [12](#__RefHeading___Toc398908795)

B.2 Mapping [12](#__RefHeading___Toc398908796)

B.2.1 General mapping [12](#__RefHeading___Toc398908797)

B.2.2 Information Object Class (IOC) mapping [12](#__RefHeading___Toc398908798)

B.3 Solution Set definitions [12](#__RefHeading___Toc398908799)

B.3.1 XML definition structure [12](#__RefHeading___Toc398908800)

B.3.2 Graphical Representation [13](#__RefHeading___Toc398908801)

B.3.3 XML Schema "transportNrm.xsd" [14](#__RefHeading___Toc398908802)

Annex A (informative): Change history [18](#__RefHeading___Toc398908803)

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# Introduction

The present document is part of a TS-family covering the 3rd Generation Partnership Project; Technical Specification Group Services and System Aspects; Telecommunication management; as identified below:

28.731: Transport Network (TN) interface Network Resource Model (NRM) Integration Reference Point (IRP); Requirements.

28.732: Transport Network (TN) interface Network Resource Model (NRM) Integration Reference Point (IRP); Information Service (IS).

**28.733: Transport Network (TN) interface Network Resource Model (NRM) Integration Reference Point (IRP); Solution Set (SS) definitions.**

# 1 Scope

The present document is part of an Integration Reference Point (IRP) named Transport Network (TN) interface Network Resource Model (NRM) IRP, through which an IRPAgent can communicate configuration management information to one or several IRPManagers concerning TN resources. The TN NRM IRP comprises a set of specifications defining Requirements, a protocol neutral Information Service and one or more Solution Set(s).

The present document specifies the Solution Sets for the TN NRM IRP.

This specification is related to 3GPP TS 28.732 [4] V14.0.X.

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TS 32.101: "Telecommunication management; Principles and high level requirements".

[2] 3GPP TS 32.102: "Telecommunication management; Architecture".

[3] 3GPP TS 32.600: "Telecommunication management; Configuration Management (CM); Concept and high-level requirements".

[4] 3GPP TS 28.732: "Telecommunication management; Transport Network (TN) Interface Network Resource Model (NRM) Integration Reference Point (IRP); Information Service (IS)".

[5] 3GPP TS 32.300: "Telecommunication management; Configuration Management (CM); Name convention for Managed Objects".

[6] OMG Notification Service, Version 1.0.

[7] OMG CORBA services: Common Object Services Specification, Update: November 22, 1996.

[8] The Common Object Request Broker: Architecture and Specification (for specification of valid version, see [1]).

[9] 3GPP TS 32.306: "Telecommunication management; Configuration Management (CM); Notification Integration Reference Point (IRP): Solution Set (SS) definitions".

[10] 3GPP TS 32.612: "Telecommunication management; Configuration Management (CM); Bulk CM Integration Reference Point (IRP): Information Service (IS)".

[11] 3GPP TS 32.616: "Telecommunication management; Configuration Management (CM); Bulk CM Integration Reference Point (IRP): Solution Set (SS) definitions ".

[12] W3C REC-xml11-20060816: "Extensible Markup Language (XML) 1.1 (Second Edition)".

[13] Void

[14] W3C XML Schema Definition Language (XSD) 1.1 Part 1: Structures.

[15] W3C XML Schema Definition Language (XSD) 1.1 Part 2: Datatypes.

[16] W3C REC-xml-names-20060816: "Namespaces in XML 1.1 (Second Edition)".

[17] 3GPP TS 28.623: “Generic Network Resource Model (NRM) Integration Reference Point (IRP); Solution Set (SS) definitions”.

# 3 Definitions and abbreviations

## 3.1 Definitions

For terms and definitions please refer to 3GPP TS 32.101 [1], TS 32.102 [2], TS 32.600 [3] and TS 32.712 [4] and the following apply.

**XML file:** See definition of [17].

**XML document:** See definition of [17].

**XML declaration:** See definition of [17].

**XML element:** See definition of [17].

**empty XML element:** See definition of [17].

**XML content (of an XML element):** See definition of [17].

**XML start-tag:** See definition of [17].

**XML end-tag:** See definition of [17].

**XML empty-element tag:** See definition of [17].

**XML attribute specification:** See definition of [17].

**DTD:** See definition of [17].

**XML schema:** See definition of [17].

**XML namespace:** See definition of [17].

**XML complex type:** See definition of [17].

**XML element type:** See definition of [17].

## 3.2 Abbreviations

For the purposes of the present document, the following abbreviations apply:

CM Configuration Management

CORBA Common Object Request Broker Architecture

DN Distinguished Name

DTD Document Type Definition

EDGE Enhanced Data for GSM Evolution

GERAN GSM/EDGE Radio Access Network

GSM Global System for Mobile communication

IS Information Service

IDL Interface Definition Language (OMG)

IOC Information Object Class

IRP Integration Reference Point

MO Managed Object

MOC Managed Object Class

NRM Network Resource Model

OMG Object Management Group

SS Solution Set

TN Transport Network

UMTS Universal Mobile Telecommunications System

UTRAN Universal Terrestrial Radio Access Network

XML eXtensible Markup Language

# 4 Solution Set Definitions

This specification defines the following 3GPP TN NRM IRP Solution Set Definitions:

- 3GPP TN NRM IRP CORBA SS (Annex A)

- 3GPP TN NRM IRP XML Definitions (Annex B)

Annex A (normative):  
CORBA Solution Set

# A.0 General

This annex contains the CORBA Solution Set for the IRP whose semantics is specified in TN NRM IRP: Information Service (TS 32.712 [4]).

# A.1 Architectural features

## A.1.0 Introduction

The overall architectural feature of Transport Network Resources IRP is specified in 3GPP TS 28.712 [4].   
This clause specifies features that are specific to the CORBA SS.

## A.1.1 Syntax for Distinguished Names

See clause A.1.1 of [17].

## A.1.2 Rules for NRM extensions

See clause A.1.2 of [17].

# A.2 Mapping

## A.2.1 General mapping

See clause A.2.1 of [17].

## A.2.2 Information Object Class (IOC) mapping

### A.2.2.1 IOC TransportNetworkInterface

Table A.2.2.1: Mapping from NRM IOC TransportNetworkInterface attributes to SS equivalent MOC TransportNetworkInterface attributes

| NRM Attributes of IOC TransportNetworkInterface in 3GPP TS 28.732 [4] | SS Attributes | SS Type | Support Qualifier | Read | Write |
| --- | --- | --- | --- | --- | --- |
| id | transportNetworkInterfaceId | string | M | M | - |
| userLabel | userLabel | string | M | M | M |
| transportNetworkType | transportNetworkType | string | M | M | - |

### A.2.2.2 IOC ATMChannelTerminationPoint

Table A.2.2.2: Mapping from NRM IOC ATMChannelTerminationPoint attributes and associations to SS equivalent MOC ATMTerminationPoint attributes

| NRM Associations/Attributes of IOC ATMChannelTerminationPoint in 3GPP TS 28.732 [4] | SS Attributes | SS Type | Support Qualifier | Read | Write |
| --- | --- | --- | --- | --- | --- |
| id | aTMChannelTerminationPointId | string | M | M | \_ |
| usageChannel | usageChannel | string | M | M | \_ |
| virtualPathId | virtualPathId | long | M | M | O |
| virtualChannelId | virtualChannelId | long | M | M | O |
| physicalPortId | physicalPortId | string | M | M | O |
| physicalInterfaceType | physicalLinkType | string | M | M | O |
| serviceCategoryIn | serviceCategoryIn | long | M | M | O |
| serviceCategoryEg | serviceCategoryEg | long | M | M | O |
| usedAAL | usedAAL | long | M | M | O |
| peakCellRateIn | peakCellRateIn | long | M | M | O |
| peakCellRateEg | peakCellRateEg | long | M | M | O |
| sustainableCellRateIn | sustainableCellRateIn | long | O | M | O |
| sustainableCellRateEg | sustainableCellRateEg | long | O | M | O |
| maximumBurstSizeIn | maximumBurstSizeIn | long | M | M | O |
| maximumBurstSizeEg | maximumBurstSizeEg | long | M | M | O |
| minimumDesiredCellRateIn | minimumDesiredCellRateIn | long | O | M | O |
| minimumDesiredCellRateEg | minimumDesiredCellRateEg | long | O | M | O |
| minimumCellRateIn | minimumCellRateIn | long | O | M | O |
| minimumCellRateEg | minimumCellRateEg | long | O | M | O |
| aTMChannelTerminationPoint- ATMPathTerminationPoint | aTMChannelTerminationPointATMPathTerminationPoint | GenericNetworkResourcesIRPSystem::AttributeTypes::MOReference | M | M | - |
| aTMChannelTerminationPoint- IubLink | aTMChannelTerminationPointIubLink | GenericNetworkResourcesIRPSystem::AttributeTypes::MOReferenceSet | M | M | - |

### A.2.2.3 IOC ATMPathTerminationPoint

Table A.2.2.3: Mapping from NRM IOC ATMPathTerminationPoint attributes and associations to SS equivalent MOC ATMTerminationPoint attributes

| NRM Associations/Attributes of IOC ATMPathTerminationPoint in 3GPP TS 28.732 [4] | SS Attributes | SS Type | Support Qualifier | Read | Write |
| --- | --- | --- | --- | --- | --- |
| id | aTMPathTerminationPointId | string | M | M | \_ |
| virtualPathId | virtualPathId | long | M | M | O |
| physicalPortIdList | physicalPortIdList | string | M | M | O |
| peakCellRateIn | peakCellRateIn | long | M | M | O |
| peakCellRateEg | peakCellRateEg | long | M | M | O |
| aTMPathTerminationPoint-ATMChannelTerminationPoint | aTMPathTerminationPointATMChannelTerminationPoint | GenericNetworkResourcesIRPSystem::AttributeTypes::MOReferenceSet | M | M | - |

# A.3 Solution Set definitions

## A.3.1 IDL definition structure

Clause A.3.2 defines the MO classes for the TN NRM IRP.

## A.3.2 IDL specification “TransportNetworkResourcesNRMDefs.idl”

//File: TransportNetworkResourcesNRMDefs.idl

#ifndef \_Transport\_Network\_Resources\_NRM\_Defs\_IDL\_

#define \_Transport\_Network\_Resources\_NRM\_Defs\_IDL\_

#include "GenericNetworkResourcesNRMDefs.idl"

#pragma prefix "3gppsa5.org"

/\*\*

\* This module defines constants for each MO class name and

\* the attribute names for each defined MO class.

\*/

module TransportNetworkResourcesNRMDefs

{

/\*\*

\* Definitions for MO class TransportNetworkInterface

\*/

interface TransportNetworkInterface : GenericNetworkResourcesNRMDefs::ManagedFunction

{

const string CLASS = "TransportNetworkInterface";

// Attribute Names

//

const string transportNetworkInterfaceId = "transportNetworkInterfaceId";

const string transportNetworkType= "transportNetworkType";

};

/\*\*

\* Definitions for MO class ATMChannelTerminationPoint

\*/

interface ATMChannelTerminationPoint

{

const string CLASS = "ATMChannelTerminationPoint";

// Attribute Names

//

const string aTMChannelTerminationPointId = "aTMChannelTerminationPointId";

const string usageChannel= "usageChannel";

const string virtualPathId= "virtualPathId";

const string virtualChannelId= "virtualChannelId";

const string physicalPortId= "physicalPortId";

const string physicalLinkType= "physicalLinkType";

const string serviceCategoryIn= "serviceCategoryIn";

const string serviceCategoryEg= "serviceCategoryEg";

const string usedAAL= "usedAAL";

const string peakCellRateIn= "peakCellRateIn";

const string peakCellRateEg= "peakCellRateEg";

const string sustainableCellRateIn= "sustainableCellRateIn";

const string sustainableCellRateEg= "sustainableCellRateEg";

const string maximumBurstSizeIn= "maximumBurstSizeIn";

const string maximumBurstSizeEg= "maximumBurstSizeEg";

const string minimumDesiredCellRateIn= "minimumDesiredCellRateIn";

const string minimumDesiredCellRateEg= "minimumDesiredCellRateEg";

const string minimumCellRateIn= "minimumCellRateIn";

const string minimumCellRateEg= "minimumCellRateEg";

const string aTMChannelTerminationPointATMPathTerminationPoint = "aTMChannelTerminationPointATMPathTerminationPoint";

const string aTMChannelTerminationPointIubLink = "aTMChannelTerminationPointIubLink";

};

/\*\*

\* Definitions for MO class ATMPathTerminationPoint

\*/

interface ATMPathTerminationPoint

{

const string CLASS = "ATMPathTerminationPoint";

// Attribute Names

//

const string aTMPathTerminationPointId = "aTMPathTerminationPoint";

const string virtualPathId= "virtualPathId";

const string physicalPortIdList= "physicalPortIdList";

const string peakCellRateIn= "peakCellRateIn";

const string peakCellRateEg= "peakCellRateEg";

const string aTMPathTerminationPointATMChannelTerminationPoint = "aTMPathTerminationPointATMChannelTerminationPoint";

};

};

#endif // \_Transport\_Network\_Resources\_NRM\_Defs\_IDL\_

Annex B (normative):  
XML Definitions

# B.0 General

This annex contains the XML Definitions for the TN NRM IRP as it applies to Itf-N, in accordance with TN NRM IRP Information Service (TS 32.712 [4]).

The XML file formats are based on XML [12], XML Schema [14] [15] and XML Namespace [16] standards.

# B.1 Architectural features

## B.1.0 Introduction

The overall architectural feature of Transport Network Resources IRP is specified in 3GPP TS 32.712 [4].   
This clause specifies features that are specific to the XML Definitions.

## B.1.1 Syntax for Distinguished Names

The syntax of a Distinguished Name is defined in 3GPP TS 32.300 [5].

# B.2 Mapping

### B.2.1 General mapping

An IOC maps to an XML element of the same name as the IOC's name in the IS. An IOC attribute maps to a sub-element of the corresponding IOC's XML element, and the name of this sub-element is the same as the attribute's name in the IS.

### B.2.2 Information Object Class (IOC) mapping

The mapping is not present in the current version of this specification.

# B.3 Solution Set definitions

## B.3.1 XML definition structure

The overall description of the file format of configuration data XML files is provided by 3GPP TS 32.616 [11].

Annex B.3.3 of the present document defines the NRM-specific XML schema transportNrm.xsd for the Transport interface Network Resources IRP NRM defined in 3GPP TS 32.712 [4].

XML schema transportNrm.xsd explicitly declares NRM-specific XML element types for the related NRM.

The definition of those NRM-specific XML element types complies with the generic mapping rules defined in 3GPP TS 32.616 [11].

## B.3.2 Graphical Representation

The graphical representation is not present in the current version of this specification.

## B.3.3 XML Schema "transportNrm.xsd"

<?xml version="1.1" encoding="UTF-8"?>  
  
<!--  
 3GPP TS 28.733 Transport Network Interface NRM IRP  
 Bulk CM Configuration data file NRM-specific XML schema  
 transportNrm.xsd  
-->  
  
<schema  
 targetNamespace="http://www.3gpp.org/ftp/specs/archive/28\_series/28.733#transportNrm"  
 elementFormDefault="qualified"  
 xmlns="http://www.w3.org/2001/XMLSchema"  
 xmlns:xn="http://www.3gpp.org/ftp/specs/archive/28\_series/28.623#genericNrm"  
 xmlns:tn="http://www.3gpp.org/ftp/specs/archive/28\_series/28.733#transportNrm"  
>  
  
 <import  
 namespace=  
"http://www.3gpp.org/ftp/specs/archive/28\_series/28.623#genericNrm"  
 />  
  
<!--Transport Network Interface Resources IRP NRM attribute related XML types -->

<simpleType name="transportNetworkType">  
 <restriction base="string">  
 <enumeration value="ATM"/>  
 <enumeration value="IP"/>  
 </restriction>  
 </simpleType>  
  
 <simpleType name="serviceCategoryIn">  
 <restriction base="string">  
 <enumeration value="CBR"/>  
 <enumeration value="RT-VBR"/>  
 <enumeration value="NRT-VBR"/>  
 <enumeration value="ABR"/>  
 <enumeration value="UBR"/>  
 <enumeration value="GFR"/>  
 </restriction>  
 </simpleType>  
  
 <simpleType name="serviceCategoryEg">  
 <restriction base="string">  
 <enumeration value="CBR"/>  
 <enumeration value="RT-VBR"/>  
 <enumeration value="NRT-VBR"/>  
 <enumeration value="ABR"/>  
 <enumeration value="UBR"/>  
 <enumeration value="GFR"/>  
 </restriction>  
 </simpleType>  
  
 <simpleType name="usedAAL">  
 <restriction base="string">  
 <enumeration value="Null"/>  
 <enumeration value="AAL1"/>  
 <enumeration value="AAL2"/>  
 <enumeration value="AAL3"/>  
 <enumeration value="AAL4"/>  
 <enumeration value="AAL5"/>  
 </restriction>  
 </simpleType>  
  
 <simpleType name="virtualPathId">  
 <restriction base="integer">  
 <minInclusive value="0"/>  
 </restriction>  
 </simpleType>

<simpleType name="virtualChannelId">  
 <restriction base="integer">  
 <minInclusive value="0"/>  
 </restriction>  
 </simpleType>  
  
 <complexType name="physicalPortIdList">  
 <sequence>  
 <element name="physicalPortId" type="string" minOccurs="1" maxOccurs="unbounded">  
 </element>  
 </sequence>  
 </complexType>  
  
 <simpleType name="peakCellRateIn">  
 <restriction base="integer">  
 <minInclusive value="1"/>  
 </restriction>  
 </simpleType>  
  
 <simpleType name="peakCellRateEg">  
 <restriction base="integer">  
 <minInclusive value="1"/>  
 </restriction>  
 </simpleType>

<simpleType name="sustainableCellRateIn">  
 <restriction base="integer">  
 <minInclusive value="1"/>  
 </restriction>  
 </simpleType>  
  
 <simpleType name="sustainableCellRateEg">  
 <restriction base="integer">  
 <minInclusive value="1"/>  
 </restriction>  
 </simpleType>  
  
 <simpleType name="maximumBurstSizeIn">  
 <restriction base="integer">  
 <minInclusive value="1"/>  
 </restriction>  
 </simpleType>  
  
 <simpleType name="maximumBurstSizeEg">  
 <restriction base="integer">  
 <minInclusive value="1"/>  
 </restriction>  
 </simpleType>  
  
 <simpleType name="minimumCellRateIn">  
 <restriction base="integer">  
 <minInclusive value="1"/>  
 </restriction>  
 </simpleType>  
  
 <simpleType name="minimumCellRateEg">  
 <restriction base="integer">  
 <minInclusive value="1"/>  
 </restriction>  
 </simpleType>  
  
 <simpleType name="minimumDesiredCellRateIn">  
 <restriction base="integer">  
 <minInclusive value="1"/>  
 </restriction>  
 </simpleType>  
  
 <simpleType name="minimumDesiredCellRateEg">  
 <restriction base="integer">  
 <minInclusive value="1"/>  
 </restriction>  
 </simpleType>  
  
 <!-- Transport Network Interface Resources IRP NRM class associated XML elements -->  
  
 <element  
 name="TransportNetworkInterface"  
 substitutionGroup="xn:ManagedElementOptionallyContainedNrmClass"  
 >  
 <complexType>  
 <complexContent>  
 <extension base="xn:NrmClass">  
 <sequence>  
 <element name="attributes" minOccurs="0">  
 <complexType>  
 <all>  
 <element name="userLabel" type="string"/>  
 <element name="vnfParametersList" type="xn:vnfParametersListType" minOccurs="0"/>

<element  
 name="transportNetworkType"  
 type="tn:transportNetworkType"  
 />  
 </all>  
 </complexType>  
 </element>  
 <choice minOccurs="0" maxOccurs="unbounded">  
 <element ref="tn:ATMPathTerminationPoint"/>  
 <element ref="tn:ATMChannelTerminationPoint"/>  
 <element ref="xn:VsDataContainer"/>  
 </choice>  
 </sequence>  
 </extension>  
 </complexContent>  
 </complexType>  
 </element>  
  
 <element name="ATMChannelTerminationPoint">  
 <complexType>  
 <complexContent>  
 <extension base="xn:NrmClass">  
 <sequence>  
 <element name="attributes" minOccurs="0">  
 <complexType>  
 <all>  
 <element name="usageChannel" type="string"/>  
 <element   
 name="virtualPathId"  
 type="tn:virtualPathId"  
 />  
 <element  
 name="virtualChannelId"  
 type="tn:virtualChannelId"  
 />  
 <element  
 name="physicalPortId"  
 type="string"  
 />  
 <element name="physicalInterfaceType" type="string" minOccurs="0"/>  
 <element  
 name="serviceCategoryIn"  
 type="tn:serviceCategoryIn"  
 />  
 <element  
 name="serviceCategoryEg"  
 type="tn:serviceCategoryEg"  
 />  
 <element  
 name="usedAAL"  
 type="tn:usedAAL"  
 />  
 <element  
 name="peakCellRateIn"  
 type="tn:peakCellRateIn"  
 />  
 <element  
 name="peakCellRateEg"  
 type="tn:peakCellRateEg"  
 />  
 <element  
 name="sustainableCellRateIn"  
 type="tn:sustainableCellRateIn"  
 minOccurs="0"  
 />  
 <element  
 name="sustainableCellRateEg"  
 type="tn:sustainableCellRateEg"  
 minOccurs="0"  
 />  
 <element  
 name="maximumBurstSizeIn"  
 type="tn:maximumBurstSizeIn"  
 />  
 <element  
 name="maximumBurstSizeEg"  
 type="tn:maximumBurstSizeEg"  
 />  
 <element  
 name="minimumDesiredCellRateIn"  
 type="tn:minimumDesiredCellRateIn"  
 minOccurs="0"  
 />  
 <element  
 name="minimumDesiredCellRateEg"  
 type="tn:minimumDesiredCellRateEg"  
 minOccurs="0"  
 />  
 <element  
 name="minimumCellRateIn"  
 type="tn:minimumCellRateIn"  
 minOccurs="0"  
 />  
 <element  
 name="minimumCellRateEg"  
 type="tn:minimumCellRateEg"  
 minOccurs="0"  
 />  
 <element name="aTMChannelTerminationPointATMPathTerminationPoint" type="xn:dn"/>  
 <element name="aTMChannelTerminationPointIubLink" type="xn:dnList"/>  
 </all>  
 </complexType>  
 </element>  
 <choice>  
 <element ref="xn:VsDataContainer" minOccurs="0" maxOccurs="unbounded"/>  
 </choice>  
 </sequence>  
 </extension>  
 </complexContent>  
 </complexType>  
 </element>  
  
 <element name="ATMPathTerminationPoint">  
 <complexType>  
 <complexContent>  
 <extension base="xn:NrmClass">  
 <sequence>  
 <element name="attributes" minOccurs="0">  
 <complexType>  
 <all>  
 <element  
 name="virtualPathId"  
 type="tn:virtualPathId"  
 />  
 <element  
 name="physicalPortIdList"  
 type="tn:physicalPortIdList"  
 />  
 <element  
 name="peakCellRateIn"  
 type="tn:peakCellRateIn"  
 />  
 <element  
 name="peakCellRateEg"  
 type="tn:peakCellRateEg"  
 />  
 <element name="aTMPathTerminationPointATMChannelTerminationPoint" type="xn:dnList"/>  
 </all>  
 </complexType>  
 </element>  
 <choice minOccurs="0" maxOccurs="unbounded">  
 <element ref="xn:VsDataContainer"/>  
 </choice>  
 </sequence>  
 </extension>  
 </complexContent>  
 </complexType>  
 </element>  
  
</schema>

Annex A (informative):  
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2014-06 | SA#64 | SP-140358 | 001 | - | F | Upgrade W3C XML Schema version from 1.0 to 1.1 | 11.1.0 |
|  |  | SP-140332 | 002 | - | F | remove the feature support statements | 11.1.0 |
| 2014-09 | SA#65 | SP-140560 | 003 | - | C | Update the link from Solution Set to Information Service due to the end of Release 12 | 12.0.0 |
| 2016-01 |  |  |  |  |  | Update to Rel-13 (MCC) | 13.0.0 |
| 2016-03 | SA#71 | SP-160031 | 006 | - | A | Make the XML schema well formed | 13.1.0 |
| 2016-06 | SA#72 | SP-160407 | 0007 | - | F | Update the link from IRP Solution Set to IRP Information Service | 13.2.0 |
| 2017-03 | SA#75 | - | - | - |  | Promotion to Release 14 without technical change | 14.0.0 |
| 2017-06 | SA#76 | SP-170514 | 0008 | - | F | Update the link from IRP Solution Set to IRP Information Service | 14.1.0 |
| 2017-06 | SA#76 | SP-170510 | 0009 | 1 | B | Update the XML Schema definitions to align with IS to support Configuration Management for mobile networks that include virtualized network functions | 14.1.0 |
| 2018-06 | - | - | - | - | - | Update to Rel-15 version (MCC) | **15.0.0** |
| 2020-07 | - | - | - | - | - | Update to Rel-16 version (MCC) | **16.0.0** |