|  |  |
| --- | --- |
| 3GPP TS 29.168 V16.0.0 (2020-06) | |
| Technical Specification | |
| 3rd Generation Partnership Project;  Technical Specification Group Core Network and Terminals;  Cell Broadcast Centre interfaces with the Evolved Packet Core;  Stage 3  (Release 16) | |
|  | |
|  |  |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  http://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 5

1 Scope 6

2 References 6

3 Definitions and abbreviations 7

3.1 Definitions 7

3.2 Abbreviations 8

4 SBc description 8

4.1 Transport 8

4.1.1 General 8

4.1.2 Network layer 8

4.1.3 Transport layer 8

4.1.4 Services expected from signalling transport 9

4.2. SBc-AP functions 9

4.2.1 Function of SBc-AP 9

4.3 SBc-AP procedure 9

4.3.1 General 9

4.3.2 List of SBc-AP elementary procedure 9

4.3.3 Write Replace Warning Procedure 10

4.3.3.1 General 10

4.3.3.2 Successful Operation 10

4.3.3.3 Unsuccessful Operation 10

4.3.3A Stop Warning Procedure 11

4.3.3A.1 General 11

4.3.3A.2 Successful Operation 11

4.3.3A.3 Unsuccessful Operation 11

4.3.3B Error Indication 12

4.3.3B.1 General 12

4.3.3B.2 Successful Operation 12

4.3.3B.3 Abnormal Conditions 12

4.3.3C Write Replace Warning Indication 12

4.3.3C.1 General 12

4.3.3C.2 Successful Operation 13

4.3.3C.3 Abnormal Conditions 13

4.3.3D Stop Warning Indication 13

4.3.3D.1 General 13

4.3.3D.2 Successful Operation 13

4.3.3D.3 Abnormal Conditions 13

4.3.3E PWS Restart Indication 13

4.3.3E.1 General 13

4.3.3E.2 Successful Operation 14

4.3.3E.3 Abnormal Conditions 14

4.3.3F PWS Failure Indication 14

4.3.3F.1 General 14

4.3.3F.2 Successful Operation 15

4.3.3F.3 Abnormal Conditions 15

4.3.4 Message functional definition and content 15

4.3.4.1 Message contents 15

4.3.4.1.1 Presence 15

4.3.4.1.2 Criticality 15

4.3.4.1.3 Range 16

4.3.4.1.4 Assigned Criticality 16

4.3.4.2 Warning Message Transmission Messages 16

4.3.4.2.1 WRITE-REPLACE WARNING REQUEST 16

4.3.4.2.2 WRITE-REPLACE WARNING RESPONSE 17

4.3.4.2.3 STOP WARNING REQUEST 18

4.3.4.2.4 STOP WARNING RESPONSE 19

4.3.4.2.5 WRITE REPLACE WARNING INDICATION 19

4.3.4.2.6 STOP WARNING INDICATION 19

4.3.4.2.7 PWS RESTART INDICATION 20

4.3.4.2.8 PWS FAILURE INDICATION 21

4.3.4.2A Management Messages 22

4.3.4.2A.1 ERROR INDICATION 22

4.3.4.3 Information element definition 22

4.3.4.3.1 Message Type 22

4.3.4.3.2 Cause 23

4.3.4.3.3 Criticality Diagnostics 23

4.3.4.3.4 OMC ID 24

4.3.4.3.5 Send Write-Replace-Warning-Indication 24

4.3.4.3.6 Unknown Tracking Area List 25

4.3.4.3.7 Send Stop Warning Indication 25

4.3.4.3.8 Stop-All Indicator 25

4.3.4.3.9 Broadcast Empty Area List 25

4.3.4.3.10 RAT Selector 5GS 26

4.3.4.3.11 Unknown 5GS Tracking Area List 26

4.3.4.3.12 Broadcast Scheduled Area List 5GS 26

4.3.4.3.13 Broadcast Cancelled Area List 5GS 26

4.3.4.3.14 Broadcast Empty Area List 5GS 27

4.4 Message and information element abstract syntax 27

4.4.1 General 27

4.4.2 Usage of protocol extension mechanism for non-standard use 27

4.4.3 Elementary procedure definitions 28

4.4.4 PDU definitions 30

4.4.5 Information element definitions 35

4.4.6 Common definitions 44

4.4.7 Constant definitions 44

4.4.8 Container Definitions 46

4.4.9 Message transfer syntax 48

4.5 Handling of unknown, unforeseen or erroneous protocol data 48

4.5.1 General 48

4.5.2 Transfer Syntax Error 48

4.5.3 Abstract Syntax Error 48

4.5.3.1 General 48

4.5.3.2 Criticality information 49

4.5.3.3 Presence information 49

4.5.3.4 Not comprehended IE/IE group 50

4.5.3.4.1 Procedure code 50

4.5.3.4.2 Type of Message 50

4.5.3.4.3 IEs other than the Procedure Code and Type of Message 50

4.5.3.5 Missing IE or IE group 51

4.5.3.6 IEs or IE groups received in wrong order or with too many occurrences or erroneously present 52

4.5.4 Logical Error 53

4.5.5 Exceptions 53

Annex A (informative): Change history: 54

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

* x the first digit:

1. 1 presented to TSG for information;
2. 2 presented to TSG for approval;
3. 3 or greater indicates TSG approved document under change control.

* y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.
* z the third digit is incremented when editorial only changes have been incorporated in the document.

In the present document, modal verbs have the following meanings:

**shall** indicates a mandatory requirement to do something

**shall not** indicates an interdiction (prohibition) to do something

The constructions "shall" and "shall not" are confined to the context of normative provisions, and do not appear in Technical Reports.

The constructions "must" and "must not" are not used as substitutes for "shall" and "shall not". Their use is avoided insofar as possible, and they are not used in a normative context except in a direct citation from an external, referenced, non-3GPP document, or so as to maintain continuity of style when extending or modifying the provisions of such a referenced document.

**should** indicates a recommendation to do something

**should not** indicates a recommendation not to do something

**may** indicates permission to do something

**need not** indicates permission not to do something

The construction "may not" is ambiguous and is not used in normative elements. The unambiguous constructions "might not" or "shall not" are used instead, depending upon the meaning intended.

**can** indicates that something is possible

**cannot** indicates that something is impossible

The constructions "can" and "cannot" are not substitutes for "may" and "need not".

**will** indicates that something is certain or expected to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**will not** indicates that something is certain or expected not to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**might** indicates a likelihood that something will happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

**might not** indicates a likelihood that something will not happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

In addition:

**is** (or any other verb in the indicative mood) indicates a statement of fact

**is not** (or any other negative verb in the indicative mood) indicates a statement of fact

The constructions "is" and "is not" do not indicate requirements.

# 1 Scope

The present document specifies the procedures and the SBc Application Part (SBc-AP) messages used on the SBc-AP interface between the Mobility Management Entity (MME) and the Cell Broadcast Centre (CBC), and between the Public Warning System – Inter Working Function (PWS-IWF) and the CBC.

The present document supports the following functions:

- Warning Message Transmission function in the EPS,

- Warning Message Transmission function in the 5GS via the PWS-IWF (see 3GPP TS 23.041 [14]).

NOTE: The SBc-AP interface is a logical interface between the MME and the CBC and also between the PWS-IWF and the CBC, when connected to 5GC. The PWS-IWF may not be always explicitly mentioned in the remainder of the present document.

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] IETF RFC 2460 (December 1998): "Internet Protocol, Version 6 (IPv6) Specification".

[3] IETF RFC 791 (September 1981): "Internet Protocol".

[4] IETF RFC 4960 (September 2007): "Stream Control Transmission Protocol".

[5] Void

[6] Void

[7] 3GPP TS 36.413: "Evolved Universal Terrestrial Radio Access Network (E-UTRAN); S1 Application Protocol (S1AP)"

[8] ITU-T Recommendation X.680 (07/2002): "Information Technology - Abstract Syntax Notation One (ASN.1): Specification of basic notation".

[9] ITU-T Recommendation X.681 (07/2002): "Information Technology - Abstract Syntax Notation One (ASN.1): Information object specification".

[10] ITU-T Recommendation X.691 (07/2002): "Information Technology - ASN.1 encoding rules - Specification of Packed Encoding Rules (PER)".

[11] 3GPP TS 29.002: "Mobile Application Part (MAP) specification".

[12] Void

[13] 3GPP TS 22.268: "Public Warning System (PWS) requirements".

[14] 3GPP TS 23.041: "Technical realization of Cell Broadcast Service (CBS)".

[15] Void

[16] 3GPP TS 23.007: "Restoration procedures".

[17] 3GPP TS 38.413: "NG-RAN; NG Application Protocol (NGAP)".

[18] 3GPP TS 23.527: "5G System; Restoration procedures".

# 3 Definitions and abbreviations

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in 3GPP TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in 3GPP TR 21.905 [1].

**Elementary Procedure:** SBc-AP consists of Elementary Procedures (EPs). An Elementary Procedure is a unit of interaction between MME and CBC. These Elementary Procedures are defined separately and are intended to be used to build up complete sequences in a flexible manner. If the independence between some EPs is restricted, it is described under the relevant EP description. Unless otherwise stated by the restrictions, the EPs may be invoked independently of each other as stand alone procedures, which can be active in parallel. Examples on using several SBc-APs together with each other and EPs from other interfaces can be found in reference [FFS].

An EP consists of an initiating message and possibly a response message. Two kinds of EPs are used:

- **Class 1:** Elementary Procedures with response (success and/or failure).

- **Class 2:** Elementary Procedures without response.

For Class 1 EPs, the types of responses can be as follows:

Successful:

* - A signalling message explicitly indicates that the elementary procedure successfully completed with the receipt of the response.

Unsuccessful:

* - A signalling message explicitly indicates that the EP failed.
* - On time supervision expiry (i.e. absence of expected response).

Successful and Unsuccessful:

* - One signalling message reports both successful and unsuccessful outcome for the different included requests. The response message used is the one defined for successful outcome.

Class 2 EPs are considered always successful.

## 3.2 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

5GC 5G Core

CMAS Commercial Mobile Alert System

CBC Cell Broadcast Center

CBS Cell Broadcast Service

EPC Evolved Packet Core

EPS Evolved Packet System

ETWS Earthquake and Tsunami Warning System

MME Mobility Management Entity

PWS Public Warning System

PWS-IWF PWS – Inter Working Function

SCTP Stream Control Transmission Protocol

# 4 SBc description

## 4.1 Transport

### 4.1.1 General

This clause specifies the standards for signalling transport to be used across SBc-AP interface. SBc-AP interface is a logical interface between the MME and the CBC. All the SBc-AP messages described in the present document require an SCTP association between the MME and the CBC.

### 4.1.2 Network layer

The MME and the CBC shall support IPv6 (see IETF RFC 2460 [2]) and/or IPv4 (see IETF RFC 791 [3]).

The IP layer of SBc-AP only supports point-to-point transmission for delivering SBc-AP messages.

### 4.1.3 Transport layer

SCTP (see IETF RFC 4960 [4]) shall be supported as the transport layer of SBc-AP messages.

Semi-permanent SCTP associations shall be established between MME and CBC, i.e. the SCTP associations shall remain up under normal circumstances.

Local multi-homing should be supported. Remote multi-homing shall be supported.

Multiple local SCTP endpoints may be supported. Multiple remote SCTP endpoints shall be supported. When multiple local or remote SCTP endpoints are configured, several simultaneous SCTP associations shall be supported between MME and CBC.

Checksum calculation for SCTP shall be supported as specified in RFC 4960 [4].

The CBC shall establish the SCTP association.

The registered port number for SBc-AP is 29168.

The registered payload protocol identifier for SBc-AP is 24.

### 4.1.4 Services expected from signalling transport

The signalling connection shall provide in-sequence delivery of SBc-AP messages. SBc-AP shall be notified if the signalling connection breaks.

### 4.2. SBc-AP functions

### 4.2.1 Function of SBc-AP

SBc-AP has the following function:

- Warning Message Transmission function:  
This functionality provides the means to start, overwrite and stop the broadcasting of warning message in support of the Public Warning System (PWS) messages as defined in 3GPP TS 22.268 [13] which include Commercial Mobile Warning System (CMAS) and Earthquake and Tsunami (ETWS) messages.

### 4.3 SBc-AP procedure

### 4.3.1 General

This clause describes the parameters and detailed behaviors of different procedures.

### 4.3.2 List of SBc-AP elementary procedure

Table 4.3.2-1 lists the SBc-AP Elementary Procedures defined as class 1 procedures.

Table 4.3.2-1: SBc-AP class 1 elementary procedures

|  |  |  |  |
| --- | --- | --- | --- |
| Elementary Procedure | Initiating Message | Successful Outcome | Unsuccessful Outcome |
| Response message | Response message |
| Write-Replace Warning procedure | WRITE-REPLACE WARNING REQUEST | WRITE-REPLACE WARNING RESPONSE |  |
| Stop Warning Procedure | STOP WARNING REQUEST | STOP WARNING RESPONSE |  |

Table 4.3.2-2 lists the SBc-AP Elementary Procedures defined as class 2 procedures.

Table 4.3.2-2: SBc-AP class 2 elementary procedures

|  |  |
| --- | --- |
| Elementary Procedure | Initiating Message |
|
| Error Indication  procedure | ERROR INDICATION |
| Write Replace Warning Indication procedure | WRITE REPLACE WARNING INDICATION |
| Stop Warning Indication procedure | STOP WARNING INDICATION |
| PWS Restart Indication | PWS RESTART INDICATION |
| PWS Failure Indication | PWS FAILURE INDICATION |

#### 4.3.3 Write Replace Warning Procedure

##### 4.3.3.1 General

The purpose of Write-Replace Warning procedure is to start, overwrite the broadcasting of warning message, as defined in 3GPP TS 23.041 [14].

##### 4.3.3.2 Successful Operation



Figure 4.3.3.2-1: Write-Replace Warning procedure. Successful operation.

The CBC initiates the procedure by sending a WRITE-REPLACE WARNING REQUEST message to the MME.

Upon reception of WRITE-REPLACE WARNING REQUEST message, the MME shall forward the message towards the eNBs which belong to the tracking area indicated in List of TAIs IE, if this list is present.

If a Global eNB ID IE is present in the WRITE-REPLACE WARNING REQUEST message, the MME shall forward the message only towards the eNB identified by the Global eNB ID if this IE is supported by the MME. If the Global eNB ID IE is not supported by the MME, the MME shall forward the WRITE-REPLACE WARNING REQUEST message using the List of TAIs IE, if this list is present, otherwise the MME shall send the message towards all connected (H)eNBs. An MME and a CBC which support the PWS Restoration procedures as specified in 3GPP TS 23.007 [16] clause 15A.1 shall support the Global eNB ID IE.

If neither the List of TAIs IE, nor the Global eNB ID IE (if this is supported) are present in WRITE-REPLACE WARNING REQUEST message, the MME shall forward the message towards all connected eNBs.

The MME shall return a WRITE-REPLACE WARNING RESPONSE to the CBC immediately after the reception of the WRITE-REPLACE WARNING REQUEST message without waiting responses from eNBs.

The MME shall set the cause IE to 'Message accepted' in the WRITE-REPLACE WARNING RESPONSE message.

##### 4.3.3.3 Unsuccessful Operation



Figure 4.3.3.3-1: Write-Replace Warning procedure. Unsuccessful operation.

The CBC initiates the procedure by sending a WRITE-REPLACE WARNING REQUEST message to the MME.

If MME cannot process the received WRITE-REPLACE WARNING REQUEST message, the MME shall return a WRITE-REPLACE WARNING RESPONSE message towards the CBC and the MME shall not forward the message towards the eNBs belonged to the tracking area as indicated in List of TAIs IE.

The MME shall indicate a reason of failure in the cause IE.

NOTE: An Unsuccessful Operation is reported as a Successful Outcome in the Response message. See clause 3.1.

### 4.3.3A Stop Warning Procedure

#### 4.3.3A.1 General

The purpose of Stop Warning Procedure is to stop the broadcasting of warning message.

#### 4.3.3A.2 Successful Operation



Figure 4.3.3A.2-1: Stop Warning Procedure, Successful Operation.

The CBC initiates the Stop Warning Procedure by sending a STOP WARNING REQUEST message to the MME.

Upon reception of STOP WARNING REQUEST message, the MME shall forward the message towards the eNBs belonged to the tracking area as indicated in List of TAIs IE.

If none of List of TAIs IE is present in STOP WARNING REQUEST message, the MME shall forward the message towards all connected eNBs.

The MME shall return a STOP WARNING RESPONSE to the CBC immediately after the reception of the STOP WARNING REQUEST message without waiting responses from eNBs.

The MME shall set the cause IE to 'Message accepted' in the STOP WARNING RESPONSE message.

#### 4.3.3A.3 Unsuccessful Operation



Figure 4.3.3A.3-1: Stop Warning procedure, Unsuccessful operation.

The CBC initiates the Stop Warning Procedure by sending a STOP WARNING REQUEST message to the MME.

If MME cannot process the received STOP WARNING REQUEST message, the MME shall return a STOP WARNING RESPONSE message towards the CBC and the MME shall not forward the message towards the eNBs belonged to the tracking area as indicated in List of TAIs IE.

The MME shall indicate a reason of failure in the cause IE.

NOTE: An Unsuccessful Operation is reported as a Successful Outcome in the Response message. See clause 3.1.

### 4.3.3B Error Indication

#### 4.3.3B.1 General

The Error Indication procedure is initiated by a node to report detected errors in one incoming message, provided they cannot be reported by an appropriate failure message.

#### 4.3.3B.2 Successful Operation



Figure 4.3.3B.2-1: Error Indication procedure, CBC originated. Successful operation.



Figure 4.3.3B.2-2: Error Indication procedure, MME originated. Successful operation.

When the conditions defined in clause 4.5 are fulfilled, the Error Indication procedure is initiated by an ERROR INDICATION message sent from the receiving node.

The ERROR INDICATION message shall contain at least either the *Cause* IE or the *Criticality Diagnostics* as indicated in clause 4.5.

#### 4.3.3B.3 Abnormal Conditions

Not applicable.

### 4.3.3C Write Replace Warning Indication

#### 4.3.3C.1 General

If supported by the MME, the Write-Replace-Warning-Indication message(s) shall be sent by the MME to report to the CBC with the Broadcast Scheduled Area List IE if the Send Write-Replace-Warning-Indication parameter was present in the corresponding Write-Replace-Warning-Request. The Broadcast Scheduled Area List IE shall contain the Broadcast Completed Area List the MME has received from the eNodeB(s) (see 3GPP TS 36.413 [7]).

#### 4.3.3C.2 Successful Operation



Figure 4.3.3C.2-1: Write Replace Warning Indication procedure, MME originated. Successful operation.

The MME initiates the Write Replace Warning Indication procedure by sending a WRITE REPLACE WARNING INDICATION message(s) to the CBC after it has previously received a Broadcast Completed Area List from eNodeB(s) in a WRITE-REPLACE WARNING MESSAGE (see 3GPP TS 36.413 [7]). The MME may aggregate Broadcast Completed Area Lists it receives from the eNodeBs.

#### 4.3.3C.3 Abnormal Conditions

Not applicable.

### 4.3.3D Stop Warning Indication

#### 4.3.3D.1 General

If supported by the MME, the Stop Warning Indication message(s) shall be sent by the MME to report to the CBC with the Broadcast Cancelled Area List IE if the Send Stop Warning Indication parameter was present in the corresponding Stop Warning Request. The Broadcast Cancelled Area List IE shall contain the Broadcast Cancelled Area List the MME has received from the eNodeB(s) (see 3GPP TS 36.413 [7]).

#### 4.3.3D.2 Successful Operation



Figure 4.3.3D.2-1: Stop Warning Indication procedure, MME originated. Successful operation.

The MME initiates the Stop Warning Indication procedure by sending a STOP WARNING INDICATION message to the CBC after it has previously received a Broadcast Cancelled Area List from an eNodeB. The MME may aggregate Broadcast Cancelled Area Lists it receives from the eNodeBs.

#### 4.3.3D.3 Abnormal Conditions

Not applicable.

### 4.3.3E PWS Restart Indication

#### 4.3.3E.1 General

The PWS Restart Indication is sent by the MME to the CBC upon receipt of a PWS Restart Indication from an (H)eNB, to indicate that the PWS service is restarted in one or more or all cells served by an (H)eNB, i.e. the service has become operational and no warning message data is available for these cell(s). The CBC shall reload the cells if required.

#### 4.3.3E.2 Successful Operation



Figure 4.3.3E.2-1: PWS Restart Indication, Successful Operation.

The MME initiates the PWS Restart Indication procedure by sending a PWS RESTART INDICATION message to the CBC upon receiving a PWS Restart Indication message from an (H)eNB (see 3GPP TS 36.413 [7]).

The MME shall copy the following parameters from the PWS Restart Indication received from the (H)eNB into the corresponding parameters in the PWS-RESTART-INDICATION towards the CBC:

- Global eNB ID of the (H)eNB;

- E-CGI List for Restart into the Restarted-Cell-List;

- TAI List for Restart into List of TAIs for Restart;

- Emergency Area ID List for Restart (if received from the (H)eNB, i.e. if the restarted cell(s) are configured with Emergency Area ID(s)) into List of EAIs for Restart.

Upon receipt of a PWS Restart Indication message, the CBC shall consider that the PWS service is restarted in the reported cell(s), i.e. the service is operational and no warning messages are being broadcast in these cell(s). The CBC shall then reload the warning message data to the (H)eNB for these cells, if any.

The CBC shall consider a PWS Restart Indication message received shortly after a preceding one for the same cell identity as a duplicate restart indication for that cell which it shall ignore.

NOTE: The CBC can receive the same PWS Restart Indication message via two MMEs of the MME pool for redundancy reasons (see clause 15A.1 of 3GPP TS 23.007 [16]), or via two AMFs of the AMF Region for redundancy reasons (see clause 7.3 of 3GPP TS 23.527 [18]).

The CBC shall reload the warning message data (with the same Message Identifier and Serial Number) to the (H)eNB by initiating Write Replace Warning procedure(s) as specified in clause 4.3.3.2 with the following additions:

- the CBC should set the Warning Area List IE in the Write-Replace Warning Request message to the identities of the cell(s) received in the Restarted-Cell-List which are relevant to the warning message data being reloaded;

- the CBC shall copy the Global eNB ID into the Write-Replace Warning Request message; and

- the CBC may update the Number of Broadcast Requested, if necessary.

#### 4.3.3E.3 Abnormal Conditions

Not applicable.

### 4.3.3F PWS Failure Indication

#### 4.3.3F.1 General

The PWS Failure Indication is sent by the MME to the CBC upon receipt of a PWS Failure Indication from an (H)eNB, to indicate that ongoing PWS operation in one or more or all cells served by an (H)eNB has failed.

#### 4.3.3F.2 Successful Operation



Figure 4.3.3F.2-1: PWS Failure Indication, Successful Operation.

The MME initiates the PWS Failure Indication procedure by sending a PWS FAILURE INDICATION message to the CBC upon receiving a PWS Failure Indication message from an (H)eNB (see 3GPP TS 36.413 [7]).

The MME shall copy the following parameters from the PWS Failure Indication received from the (H)eNB into the corresponding parameters in the PWS-FAILURE-INDICATION towards the CBC:

- Global eNB ID of the (H)eNB;

- E-CGI List Failed for PWS into the Failed-Cell-List;

- PWS Failed E-CGI List into Failed-Cell-List.

#### 4.3.3F.3 Abnormal Conditions

Not applicable.

#### 4.3.4 Message functional definition and content

#### 4.3.4.1 Message contents

##### 4.3.4.1.1 Presence

All information elements in the message descriptions below are marked mandatory, optional or conditional according to table 4.3.4.1.1-1.

Table 4.3.4.1.1-1: Meaning of abbreviations used in SBc-AP messages

|  |  |
| --- | --- |
| Abbreviation | Meaning |
| M | IEs marked as Mandatory (M) shall always be included in the message. |
| O | IEs marked as Optional (O) may or may not be included in the message. |
| C | IEs marked as Conditional (C) shall be included in a message only if the condition is satisfied. Otherwise the IE shall not be included. |

##### 4.3.4.1.2 Criticality

Each Information Element or Group of Information Elements may have criticality information applied to it.  
Following cases are possible:

Table 4.3.4.1.2-1: Meaning of content within "Criticality" column

|  |  |
| --- | --- |
| Abbreviation | **Meaning** |
| – | No criticality information is applied explicitly. |
| YES | Criticality information is applied. This is usable only for non-repeatable IEs |
| GLOBAL | The IE and all its repetitions together have one common criticality information. This is usable only for repeatable IEs. |
| EACH | Each repetition of the IE has its own criticality information. It is not allowed to assign different criticality values to the repetitions. This is usable only for repeatable IEs. |

##### 4.3.4.1.3 Range

The Range column indicates the allowed number of copies of repetitive IEs/IE groups.

##### 4.3.4.1.4 Assigned Criticality

This column provides the actual criticality information as defined in clause 4.5.3.2, if applicable.

#### 4.3.4.2 Warning Message Transmission Messages

##### 4.3.4.2.1 WRITE-REPLACE WARNING REQUEST

This message is sent by the CBC to request start or overwrite of a warning message broadcast.

If the message is sent to the MME, then:

- the List of TAIs IE, the Warning Area List IE and the Global eNB ID IE may be used; and

- the List of 5GS TAIs IE, the Warning Area List 5GS IE, the Global RAN Node ID IE and the RAT Selector 5GS IE shall not be used.

If the message is sent to the PWS-IWF, then:

- the List of 5GS TAIs IE, the Warning Area List 5GS IE, the Global RAN Node ID IE may be used;

- the List of TAIs IE, the Warning Area List IE and the Global eNB ID IE shall not be used; and- the message shall address a Warning Area in E-UTRA or in NR, but not both simultaneously; the RAT Selector 5GS IE shall be used if the message is for the NR RAT.

Direction: CBC → MME, PWS-IWF

Table 4.3.4.2.1-1: WRITE-REPLACE WARNING REQUEST message contents

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 4.3.4.3.1 |  | YES | reject |
| Message Identifier | M |  | [7] |  | YES | reject |
| Serial Number | M |  | [7] |  | YES | reject |
| **List of TAIs** | O |  |  |  | YES | reject |
| **>TAI List Item** |  | 1 to <maxnoofTAI> |  |  |  |  |
| >>TAI | M |  | [7] |  |  |  |
| Warning Area List | O |  | [7] |  | YES | ignore |
| Repetition Period | M |  | [7] |  | YES | reject |
| Extended Repetition Period | O |  | [7] |  | YES | reject |
| Number of Broadcast Requested | M |  | [7] |  | YES | reject |
| Warning Type | O |  | [7] |  | YES | ignore |
| Warning Security Information | O |  | [7] |  | YES | ignore |
| Data Coding Scheme | O |  | [7] |  | YES | ignore |
| Warning Message Contents | O |  | [7] |  | YES | ignore |
| OMC ID | O |  | 4.3.4.3.4 |  | YES | ignore |
| Concurrent Warning Message Indicator | O |  | [7] |  | YES | reject |
| Send Write-Replace-Warning-Indication | O |  | 4.3.4.3.5 |  | YES | ignore |
| Global eNB ID | O |  | [7] |  | YES | ignore |
| List of 5GS TAIs | O |  |  |  | YES | ignore |
| >5GS TAI List Item |  | 1 to <maxnoof5GSTAIs> |  |  |  |  |
| >>5GS TAI | M |  | [17] |  |  |  |
| Warning Area List 5GS | O |  | [17] |  | YES | ignore |
| Global RAN Node ID | O |  | [17] |  | YES | Ignore |
| RAT Selector 5GS | C |  | 4.3.4.3.10 |  | YES | ignore |
| Warning Area Coordinates | O |  | [7] |  | YES | Ignore |

Table 4.3.4.2.1-2: RANGE explanation

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofTAI | Maximum no. of TAI subject for warning message broadcast in E‑UTRAN. Value is 65535. |
| Maxnoof5GSTAIs | Maximum no. of TAI subject for warning message broadcast in 5GS. |

Editor's Note: the Maxnoof5GSTAIs value is FFS in RAN3 (assumption for ASN1 is 65535).

##### 4.3.4.2.2 WRITE-REPLACE WARNING RESPONSE

This message is sent by the MME or PWS-IWF to acknowledge the CBC on the start or overwrite request of a warning message.

If the message is received from an MME then the Unknown Tracking Area IE may be present. If the message is received from a PWS-IWF then the Unknown 5GS Tracking Area List may be present.

Direction: MME, PWS-IWF → CBC

Table 4.3.4.2.2-1: WRITE-REPLACE WARNING RESPONSE message contents

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 4.3.4.3.1 |  | YES | reject |
| Message Identifier | M |  | [7] |  | YES | reject |
| Serial Number | M |  | [7] |  | YES | reject |
| Cause | M |  | 4.3.4.3.2 |  | YES | reject |
| Criticality Diagnostics | O |  | 4.3.4.3.3 |  | YES | ignore |
| Unknown Tracking Area List | O |  | 4.3.4.3.6 |  | YES | ignore |
| Unknown 5GS Tracking Area List | O |  | 4.3.4.3.11 |  | YES | ignore |

##### 4.3.4.2.3 STOP WARNING REQUEST

This message is sent by the CBC to stop a warning message broadcast.

If the message is sent to an MME, then:

- the List of TAIs IE and the Warning Area List IE may be used; and

- the List of 5GS TAIs IE, the Warning Area List 5GS IE and the RAT Selector 5GS IE shall not be used.

If the message is sent to the PWS-IWF, then:

- the List of 5GS TAIs IE, the Warning Area List 5GS IE may be used;

- the List of TAIs IE and the Warning Area List IE shall not be used; and

- the message shall address a Warning Area in E-UTRA or in NR, but not both simultaneously; the RAT Selector 5GS IE shall be used if the message is for the NR RAT.

Direction: CBC → MME, PWS-IWF

Table 4.3.4.2.3-1: STOP WARNING REQUEST message contents

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 4.3.4.3.1 |  | YES | reject |
| Message Identifier | M |  | [7] |  | YES | reject |
| Serial Number | M |  | [7] |  | YES | reject |
| **List of TAIs** | O |  |  |  | YES | reject |
| **>TAI List Item** |  | 1 to <maxnoofTAI> |  |  |  |  |
| >>TAI | M |  | [7] |  |  |  |
| Warning Area List | O |  | [7] |  | YES | Ignore |
| OMC ID | O |  | 4.3.4.3.4 |  | YES | ignore |
| Send Stop Warning Indication | O |  | 4.3.4.3.7 |  | YES | ignore |
| Stop-All Indicator | O |  | 4.3.4.3.8 |  | YES | reject |
| List of 5GS TAIs | O |  |  |  | YES | ignore |
| >5GS TAI List Item |  | 1 to <maxnoof5GSTAIs> |  |  |  |  |
| >>5GS TAI | M |  | [17] |  |  |  |
| Warning Area List 5GS | O |  | [17] |  | YES | ignore |
| RAT Selector 5GS | C |  | 4.3.4.3.10 |  | YES | ignore |

Table 4.3.4.2.3-2: RANGE explanation

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofTAI | Maximum no. of TAI subject for warning message broadcast in E‑UTRAN. Value is 65535. |
| Maxnoof5GSTAIs | Maximum no. of TAI subject for warning message broadcast in 5GS. |

Editor's Note: the Maxnoof5GSTAIs value is FFS in RAN3 (assumption for ASN1 is 65535).

##### 4.3.4.2.4 STOP WARNING RESPONSE

This message is sent by the MME or PWS-IWF to acknowledge the CBC on the stop request of a warning message.

If the message is received from an MME then the Unknown Tracking Area IE may be present, but if the message is received from a PWS-IWF then the Unknown 5GS Tracking Area List may be present.Direction: MME, PWS-IWF → CBC

Table 4.3.4.2.2-1: STOP WARNING RESPONSE message contents

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 4.3.4.3.1 |  | YES | reject |
| Message Identifier | M |  | [7] |  | YES | reject |
| Serial Number | M |  | [7] |  | YES | reject |
| Cause | M |  | 4.3.4.3.2 |  | YES | reject |
| Criticality Diagnostics | O |  | 4.3.4.3.3 |  | YES | ignore |
| Unknown Tracking Area List | O |  | 4.3.4.3.6 |  | YES | ignore |
| Unknown 5GS Tracking Area List | O |  | 4.3.4.3.11 |  | YES | ignore |

##### 4.3.4.2.5 WRITE REPLACE WARNING INDICATION

This message is sent by the MME to report to the CBC the Broadcast Scheduled Area List(s) the MME has received from the eNodeB(s) as Broadcast Completed Area List in a WRITE-REPLACE WARNING RESPONSE [7]. Multiple responses from eNodeBs may be combined in a Broadcast Scheduled Area List.

The Broadcast Scheduled Area List IE is only included in the WRITE-REPLACE WARNING INDICATION when the broadcast is successful in at least one cell within the eNodeBs.

If the message is received from an MME then the Broadscast Scheduled Area List IE may be present, but if the message is received from a PWS-IWF then the Broadscast Scheduled Area List 5GS IE may be present.

Direction: MME, PWS-IWF → CBC

Table 4.3.4.2.5-1: WRITE REPLACE WARNING INDICATION message contents

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 4.3.4.3.1 |  | YES | ignore |
| Message Identifier | M |  | [7] |  | YES | reject |
| Serial Number | M |  | [7] |  | YES | reject |
| Broadcast Scheduled Area List | O |  | [7] |  | YES | reject |
| Broadcast Scheduled Area List 5GS | O |  | 4.3.4.3.12 |  | YES | ignore |

##### 4.3.4.2.6 STOP WARNING INDICATION

This message is sent by the MME to report to the CBC the Broadcast Cancelled Area List the MME has received from the eNodeB in a KILL RESPONSE [7]. If the MME has received a KILL RESPONSE without a Broadcast Cancelled Area List IE, then the eNodeB ID shall be included in the Broadcast Empty Area List instead. Multiple responses from eNodeBs may be aggregated into a combined Broadcast Cancelled Area List.

NOTE: The CBC is able to derive the list of cell IDs that are served by the eNodeB, because the eNodeB ID is contained in the cell ID.The Broadcast Cancelled Area List IE is only included in the STOP WARNING INDICATION when the broadcast is successfully stopped in at least one cell within the eNodeBs.

The Broadcast Empty Area List IE shall be included in the STOP-WARNING-INDICATION when the MME has received at least one KILL RESPONSE without Broadcast Cancelled Area List IE.

If the message is received from an MME then the Broadscast Cancelled Area List IE may be present, but if the message is received from a PWS-IWF then the Broadscast Cancelled Area List 5GS IE may be present.

Direction: MME, PWS-IWF → CBC

Table 4.3.4.2.6-1: STOP WARNING INDICATION message contents

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 4.3.4.3.1 |  | YES | ignore |
| Message Identifier | M |  | [7] |  | YES | reject |
| Serial Number | M |  | [7] |  | YES | reject |
| Broadcast Cancelled Area List | O |  | [7] |  | YES | reject |
| Broadcast Empty Area List | O |  | 4.3.4.3.9 |  | YES | ignore |
| Broadcast Cancelled Area List 5GS | O |  | 4.3.4.3.13 |  | YES | ignore |
| Broadcast Empty Area List 5GS | O |  | 4.3.4.3.14 |  | YES | ignore |

##### 4.3.4.2.7 PWS RESTART INDICATION

This Indication is sent by the MME, or the PWS-IWF to report to the CBC the List of cells that have become available for PWS and have no warning message data.

If the indication is received from a PWS-IWF and the restarted cells are NR cells then:

- the Restarted-Cell-List IE, the Global eNB ID IE and List of TAIs for Restart IE shall be populated with a dummy value (all zeros); and

- the Restarted-Cell-List-NR IE, Global gNB ID IE and List of 5GS TAIs for Restart IE shall be populated.

If the indication is received from a PWS-IWF and the restarted cells are E-UTRA cells then:

- the Restarted-Cell-List-NR IE and the Global gNB ID IE shall not be present;

- the List of TAIs for Restart IE shall be populated with a dummy value (all zeros); and

- the List of 5GS TAI for Restart IE shall be populated.

Direction: MME, PWS-IWF → CBC

Table 4.3.4.2.7-1: PWS RESTART INDICATION message contents

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 4.3.4.3.1 |  | YES | ignore |
| Restarted-Cell-List | M |  | [7] |  | YES | reject |
| >Restarted Cell List  Item |  | 1 to <maxnoofRestartedCells> |  |  |  |  |
| >>E-CGI | M |  | [7] |  |  |  |
| Global eNB ID | M |  | [7] |  | YES | reject |
| List of TAIs for Restart | M |  |  |  | YES | reject |
| >TAI for Restart List Item |  | 1 to <maxnoofTRestartTAIs> |  |  |  |  |
| >>TAI | M |  | [7] |  |  |  |
| List of EAIs for Restart | O |  |  |  | YES | reject |
| >EAI for Restart List Item |  | 1 to <maxnoofRestartEAIs> |  |  |  |  |
| >>Emergency Area ID | M |  | [7] |  |  |  |
| Restarted-Cell-List-NR | O |  |  |  | YES | ignore |
| >Restarted Cell List NR Item |  | 1 to < maxnoofCellsforRestartNR > |  |  |  |  |
| >>NR CGI | O |  | [17] |  |  |  |
| Global gNB ID | O |  | [17] |  | YES | ignore |
| List of 5GS TAI for Restart | O |  |  |  | YES | ignore |
| >5GS TAI for Restart List Item |  | 1 to <maxnoofTRestart5GSTAIs> |  |  |  |  |
| >>5GS TAI | O |  | [17] |  |  |  |

Table 4.3.4.2.7-2: RANGE explanation

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofRestartedCells | Maximum no. of restarted E-UTRA cells. Value is 256. |
| maxnoofRestartTAIs | Maximum no. of Tracking Area IDs configured in the restarted cells. Value is 2048. |
| maxnoofRestartEAIs | Maximum no. of Emergency Area ID configured in the restarted cells. Value is 256. |
| maxnoofCellsforRestartNR | Maximum no. of NR cells subject for reloading warning message broadcast. Value is 16384. |
| maxnoofTRestart5GSTAIs | Maximum no. of 5GS TAIs subject for reloading warning message broadcast. Value is 2048. |

##### 4.3.4.2.8 PWS FAILURE INDICATION

This Indication is sent by the MME or PWS-IWF to report to the CBC the List of cells that are no longer available for PWS.

If the indication is received from a PWS-IWF and the failed cells are NR cells then the Failed-Cell-List IE and the Global eNB ID IE shall be populated with a dummy value (all zeros).

Direction: MME, PWS-IWF → CBC

Table 4.3.4.2.8-1: PWS FAILURE INDICATION message contents

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 4.3.4.3.1 |  | YES | ignore |
| Failed-Cell-List | M |  | [7] |  | YES | reject |
| >Failed Cell List  Item |  | 1 to <maxnoofFailedCells> |  |  |  |  |
| >>E-CGI | M |  | [7] |  |  |  |
| Global eNB ID | M |  | [7] |  | YES | reject |
| Failed Cell List NR | O |  |  |  | YES | ignore |
| >Failed Cell List NR Item |  | 1 to <maxnoofCellsingNB> |  |  |  |  |
| >>NR CGI | O |  | [17] |  |  |  |
| Global gNB ID | O |  | [17] |  | YES | ignore |

Table 4.3.4.2.8-2: RANGE explanation

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofFailedCells | Maximum number of failed cells. Value is 256. |
| maxnoofCellsingNB | Maximum no. of cells that can be served by a gNB. Value is 16384. |

#### 4.3.4.2A Management Messages

#### 4.3.4.2A.1 ERROR INDICATION

This message is sent by both the MME and the CBC and is used to indicate that some error has been detected in the node.

Direction : MME, PWS-IWF → CBC and CBC → MME, PWS-IWF

Table 4.3.4.2A.1-1: ERROR INDICATION message contents

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 4.3.4.3.1 |  | YES | ignore |
| Cause | O |  | 4.3.4.3.2 |  | YES | ignore |
| Criticality Diagnostics | O |  | 4.3.4.3.3 |  | YES | ignore |

#### 4.3.4.3 Information element definition

##### 4.3.4.3.1 Message Type

The Message Type IE uniquely identifies the message being sent. It is mandatory for all messages

Table 4.3.4.3.1-1: Message Type information element

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **Message Type** |  |  |  | Assumed max no of messages is 256. |
| >Procedure Code | M |  | (Write-Replace Warning, Stop Warning, Write-Replace Warning Indication, Stop Warning Indication, PWS Restart Indication, …) |  |
| >Type of Message | M |  | CHOICE (Initiating Message, Successful Outcome, Unsuccessful Outcome,  PWS Failure Indication,  …) |  |

##### 4.3.4.3.2 Cause

The purpose of the Cause IE is to indicate the reason for a particular event for the SBc-AP protocol.

Table 4.3.4.3.2-1: Cause information element

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description |
| Cause | M |  | INTEGER (Message accepted, Parameter not recognised, Parameter value invalid, Valid message not identified, Tracking area not valid, Unrecognised message, Missing mandatory element, MME capacity exceeded, MME memory exceeded, Warning broadcast not supported, Warning broadcast not operational, Message reference already used, Unspecified error, Transfer syntax error, Semantic error, Message not compatible with receiver state, Abstract syntax error reject, Abstract syntax error ignore and notify, Abstract syntax error falsely constructed message, …) |  |

##### 4.3.4.3.3 Criticality Diagnostics

The Criticality Diagnostics IE is sent by the MME when parts of a received message have not been comprehended or were missing, or if the message contained logical errors. When applicable, it contains information about which IEs were not comprehended or were missing.

Table 4.3.4.3.3-1: Criticality Diagnostics information element

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Procedure Code | O |  | INTEGER (0..255) | Procedure Code is to be used if Criticality Diagnostics is part of Error Indication procedure, and not within the response message of the same procedure that caused the error |
| Triggering Message | O |  | ENUMERATED(initiating message, successful outcome, unsuccessful outcome, outcome) | The Triggering Message is used only if the Criticality Diagnostics is part of Error Indication procedure. |
| Procedure Criticality | O |  | ENUMERATED(reject, ignore, notify) | This Procedure Criticality is used for reporting the Criticality of the Triggering message (Procedure). |
| **Information Element Criticality Diagnostics** |  | 0 to <maxnoof errors> |  |  |
| >IE Criticality | M |  | ENUMERATED(reject, ignore, notify) | The IE Criticality is used for reporting the criticality of the triggering IE. The value 'ignore' shall not be used. |
| >IE ID | M |  | INTEGER (0..65535) | The IE ID of the not understood or missing IE |
|  |  |  |  |  |
| >Type of Error | M |  | ENUMERATED(not understood, missing, …) |  |

Table 4.3.4.3.3-2: RANGE explanation

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnooferrors | Maximum no. of IE errors allowed to be reported with a single message. The value for maxnooferrors is 256. |

##### 4.3.4.3.4 OMC ID

The OMC ID IE indicates the identity of an Operation and Maintenance Centre to which Trace records shall be sent.

Table 4.3.4.3.4-1: OMC ID information element

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description |
| OMC ID | O |  | OCTET STRING (SIZE (1..20))  Octets are coded according to 3GPP TS 29.002 [11]. |  |

##### 4.3.4.3.5 Send Write-Replace-Warning-Indication

The Send Write-Replace-Warning-Indication IE indicates to the MME that the MME shall send the WRITE-REPLACE WARNING INDICATION to the CBC for the warning message.

Table 4.3.4.3.5-1: Send Write-Replace-Warning-Indication information element

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description |
| Send Write-Replace-Warning-Indication | O |  | ENUMERATED(true) |  |

##### 4.3.4.3.6 Unknown Tracking Area List

The Unknown Tracking Area List IE identifies the Tracking Areas that are unknown to the MME and where the Request cannot be delivered.

This IE shall only be included if the Cause IE indicates Message accepted, which means the MME will proceed with the request for Tracking Areas that are known to the MME. The Cause IE indicating Tracking area not valid is used when all Tracking Areas in the Request are invalid.

Table 4.3.4.3.5-1: Failure List information element

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description |
| Unknown Tracking Area List | O |  | The Unknown Tracking Area List is of type *List of TAIs*. |  |

##### 4.3.4.3.7 Send Stop Warning Indication

The Send Stop Warning Indication IE indicates to the MME that the MME shall send the STOP WARNING INDICATION to the CBC for the warning message.

Table 4.3.4.3.7-1: Send Stop-Warning-Indication information element

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description |
| Send Stop Warning Indication | O |  | ENUMERATED(true) |  |

##### 4.3.4.3.8 Stop-All Indicator

The Stop-All Indicator IE indicates that the Message Identifier IE and the Serial Number IE do not refer to a specific message that needs to be stopped, but that all messages in the area are referred to and to force the cells in the area into their Warning Message Delivery initial state.

Table 4.3.4.3.8-1: Stop-All Indicator information element

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description |
| Stop-All Indicator | O |  | ENUMERATED(true) |  |

##### 4.3.4.3.9 Broadcast Empty Area List

The Broadcast Empty Area List IE contains the eNodeB IDs of the eNodeBs which have responded with a KILL RESPONSE message which did not contain a Broadcast Cancelled Area List IE [7].

Table 4.3.4.3.9-1: Broadcast Empty Area List information element

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description |
| Broadcast Empty Area List | O |  | The Broadcast Empty Area List is a list of Global eNB IDs [7] |  |

##### 4.3.4.3.10 RAT Selector 5GS

The RAT Selector 5GS IE shall be present in a WRITE-REPLACE WARNING REQUEST and a STOP WARNING REQUEST message sent to a PWS-IWF, to indicate to the AMF that the request shall be distributed to gNodeBs (i.e. NR RAT). If the IE is not present, the AMF shall distribute the request to ng-eNodeBs (i.e. E-UTRA RAT).

Table 4.3.4.3.10-1: RAT Selector 5GS contents

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| RAT Selector 5GS | O |  | Enumerated(true) |  | YES | ignore |

##### 4.3.4.3.11 Unknown 5GS Tracking Area List

The Unknown 5GS Tracking Area List IE identifies the Tracking Areas that are unknown to the AMF and where the Request cannot be delivered.

This IE shall only be included if the Cause IE indicates Message accepted, which means the AMF will proceed with the request for Tracking Areas that are known to the AMF. The Cause IE indicating Tracking area not valid is used when all Tracking Areas in the Request are invalid.

Table 4.3.4.3.11-1: Failure List information element

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description |
| Unknown 5GS Tracking Area List |  |  |  |  |
| >Unknown 5GS TAI List Item |  | 1 to <maxnoof5GSTAIs> |  |  |
| >>5GS TAI | M |  | [17] |  |

Table 4.3.4.3.11-2: RANGE explanation

|  |  |
| --- | --- |
| Range bound | Explanation |
| Maxnoof5GSTAIs | Maximum no. of TAI subject for warning message broadcast in 5GS. |

Editor's Note: the Maxnoof5GSTAIs value is FFS (assumption for ASN1 is 65535).

##### 4.3.4.3.12 Broadcast Scheduled Area List 5GS

This IE is used to identify a Broadcast Scheduled Area List in 5GS.

Table 4.3.4.3.12-1: Broadcast Scheduled Area List 5GS contents

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Broadcast Completed Area List 5GS | M |  | [17] |  | YES | reject |

The Broadcast Scheduled Area List 5GS shall contain the Broadcast Completed Area List IE as specified in clause 9.3.1.43 in 3GPP TS 38.413 [17].

##### 4.3.4.3.13 Broadcast Cancelled Area List 5GS

This IE is used to identify a Broadcast Cancelled Area List in 5GS.

Table 4.3.4.3.13-1: Broadcast Cancelled Area List 5GS contents

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Broadcast Cancelled Area List 5GS | M |  | [17] |  | YES | reject |

The Broadcast Cancelled Area List 5GS shall contain the Broadcast Cancelled Area List IE as specified in clause 9.3.1.44 in 3GPP TS 38.413 [17].

##### 4.3.4.3.14 Broadcast Empty Area List 5GS

The Broadcast Empty Area List 5GS IE contains the RAN Node IDs of the RAN nodes which have responded with a PWS CANCEL RESPONSE message which did not contain a Broadcast Cancelled Area List IE.

Table 4.3.4.3.14-1: Broadcast Empty Area List 5GS information element

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description |
| Broadcast Empty Area List 5GS |  |  |  |  |
| >Broadcast Empty Area List 5GS List Item |  | 1 to <maxnoofRANNodes> |  |  |
| >>RAN Node ID | M |  | [17] |  |

Table 4.3.4.3.14-2: RANGE explanation

|  |  |
| --- | --- |
| Range bound | Explanation |
| MaxnoofRANNodes | Maximum no. of RAN Nodes. |

Editor's Note: the MaxnoofRANNodes value is FFS (assumption for ASN1 is 65535).

## 4.4 Message and information element abstract syntax

### 4.4.1 General

SBC-AP ASN.1 definition conforms with [8] and [9].

The ASN.1 definition specifies the structure and content of SBC-AP messages. SBC-AP messages can contain any IEs specified in the object set definitions for that message without the order or number of occurrence being restricted by ASN.1. However, for this version of the standard, a sending entity shall construct a SBC-AP message according to the PDU definitions module and with the following additional rules (Note that in the following IE means an IE in the object set with an explicit id. If one IE needed to appear more than once in one object set, then the different occurrences have different IE ids):

- IEs shall be ordered (in an IE container) in the order they appear in object set definitions.

- Object set definitions specify how many times IEs may appear. An IE shall appear exactly once if the presence field in an object has value "mandatory". An IE may appear at most once if the presence field in an object has value "optional" or "conditional". If in a tabular format there is multiplicity specified for an IE (i.e. an IE list) then in the corresponding ASN.1 definition the list definition is separated into two parts. The first part defines an IE container list where the list elements reside. The second part defines list elements. The IE container list appears as an IE of its own. For this version of the standard an IE container list may contain only one kind of list elements.

If a SBC-AP message that is not constructed as defined above is received, this shall be considered as Abstract Syntax Error, and the message shall be handled as defined for Abstract Syntax error in clause 4.5.3.6.

### 4.4.2 Usage of protocol extension mechanism for non-standard use

The protocol extension mechanism for non-standard use may be used:

- for special operator- (and/or vendor) specific features considered not to be part of the basic functionality, i.e. the functionality required for a complete and high-quality specification in order to guarantee multivendor interoperability.

- by vendors for research purposes, e.g. to implement and evaluate new algorithms/features before such features are proposed for standardisation.

The extension mechanism shall not be used for basic functionality. Such functionality shall be standardised.

### 4.4.3 Elementary procedure definitions

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Elementary Procedure definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SBC-AP-PDU-Descriptions {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

eps-Access (21) modules (3) sbc-AP (3) version1 (1) sbc-AP-PDU-Descriptions (0)}

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IE parameter types from other modules.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IMPORTS

Criticality,

ProcedureCode

FROM SBC-AP-CommonDataTypes

Write-Replace-Warning-Request,

Write-Replace-Warning-Response,

Stop-Warning-Request,

Stop-Warning-Response,

Error-Indication,

Write-Replace-Warning-Indication,

Stop-Warning-Indication,

PWS-Restart-Indication,

PWS-Failure-Indication

FROM SBC-AP-PDU-Contents

id-Write-Replace-Warning,

id-Stop-Warning,

id-Error-Indication,

id-Write-Replace-Warning-Indication,

id-Stop-Warning-Indication,

id-PWS-Restart-Indication,

id-PWS-Failure-Indication

FROM SBC-AP-Constants;

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Interface Elementary Procedure Class

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SBC-AP-ELEMENTARY-PROCEDURE ::= CLASS {

&InitiatingMessage ,

&SuccessfulOutcome OPTIONAL,

&UnsuccessfulOutcome OPTIONAL,

&procedureCode ProcedureCode UNIQUE,

&criticality Criticality DEFAULT ignore

}

WITH SYNTAX {

INITIATING MESSAGE &InitiatingMessage

[SUCCESSFUL OUTCOME &SuccessfulOutcome]

[UNSUCCESSFUL OUTCOME &UnsuccessfulOutcome]

PROCEDURE CODE &procedureCode

[CRITICALITY &criticality]

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Interface PDU Definition

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SBC-AP-PDU ::= CHOICE {

initiatingMessage InitiatingMessage,

successfulOutcome SuccessfulOutcome,

unsuccessfulOutcome UnsuccessfulOutcome,

...

}

InitiatingMessage ::= SEQUENCE {

procedureCode SBC-AP-ELEMENTARY-PROCEDURE.&procedureCode ({SBC-AP-ELEMENTARY-PROCEDURES}),

criticality SBC-AP-ELEMENTARY-PROCEDURE.&criticality ({SBC-AP-ELEMENTARY-PROCEDURES}{@procedureCode}),

value SBC-AP-ELEMENTARY-PROCEDURE.&InitiatingMessage ({SBC-AP-ELEMENTARY-PROCEDURES}{@procedureCode})

}

SuccessfulOutcome ::= SEQUENCE {

procedureCode SBC-AP-ELEMENTARY-PROCEDURE.&procedureCode ({SBC-AP-ELEMENTARY-PROCEDURES}),

criticality SBC-AP-ELEMENTARY-PROCEDURE.&criticality ({SBC-AP-ELEMENTARY-PROCEDURES}{@procedureCode}),

value SBC-AP-ELEMENTARY-PROCEDURE.&SuccessfulOutcome ({SBC-AP-ELEMENTARY-PROCEDURES}{@procedureCode})

}

UnsuccessfulOutcome ::= SEQUENCE {

procedureCode SBC-AP-ELEMENTARY-PROCEDURE.&procedureCode ({SBC-AP-ELEMENTARY-PROCEDURES}),

criticality SBC-AP-ELEMENTARY-PROCEDURE.&criticality ({SBC-AP-ELEMENTARY-PROCEDURES}{@procedureCode}),

value SBC-AP-ELEMENTARY-PROCEDURE.&UnsuccessfulOutcome ({SBC-AP-ELEMENTARY-PROCEDURES}{@procedureCode})

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Interface Elementary Procedure List

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SBC-AP-ELEMENTARY-PROCEDURES SBC-AP-ELEMENTARY-PROCEDURE ::= {

SBC-AP-ELEMENTARY-PROCEDURES-CLASS-1 |

SBC-AP-ELEMENTARY-PROCEDURES-CLASS-2 ,

...

}

SBC-AP-ELEMENTARY-PROCEDURES-CLASS-1 SBC-AP-ELEMENTARY-PROCEDURE ::= {

write-Replace-Warning |

stop-Warning ,

...

}

SBC-AP-ELEMENTARY-PROCEDURES-CLASS-2 SBC-AP-ELEMENTARY-PROCEDURE ::= {

error-Indication |

write-Replace-Warning-Indication |

stop-Warning-Indication |

pws-Restart-Indication |

pws-Failure-Indication,

...

}

write-Replace-Warning SBC-AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE Write-Replace-Warning-Request

SUCCESSFUL OUTCOME Write-Replace-Warning-Response

PROCEDURE CODE id-Write-Replace-Warning

CRITICALITY reject

}

stop-Warning SBC-AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE Stop-Warning-Request

SUCCESSFUL OUTCOME Stop-Warning-Response

PROCEDURE CODE id-Stop-Warning

CRITICALITY reject

}

error-Indication SBC-AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE Error-Indication

PROCEDURE CODE id-Error-Indication

CRITICALITY ignore

}

write-Replace-Warning-Indication SBC-AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE Write-Replace-Warning-Indication

PROCEDURE CODE id-Write-Replace-Warning-Indication

CRITICALITY ignore

}

stop-Warning-Indication SBC-AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE Stop-Warning-Indication

PROCEDURE CODE id-Stop-Warning-Indication

CRITICALITY ignore

}

pws-Restart-Indication SBC-AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE PWS-Restart-Indication

PROCEDURE CODE id-PWS-Restart-Indication

CRITICALITY ignore

}

pws-Failure-Indication SBC-AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE PWS-Failure-Indication

PROCEDURE CODE id-PWS-Failure-Indication

CRITICALITY ignore

}

END

### 4.4.4 PDU definitions

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU definitions for SBC-AP.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SBC-AP-PDU-Contents {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

eps-Access (21) modules (3) sbc-AP (3) version1 (1) sbc-AP-PDU-Contents (1)}

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IE parameter types from other modules.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IMPORTS

Cause,

Concurrent-Warning-Message-Indicator,

Criticality-Diagnostics,

Data-Coding-Scheme,

Message-Identifier,

Serial-Number,

List-of-TAIs,

Warning-Area-List,

Omc-Id,

Repetition-Period,

Extended-Repetition-Period,

Number-of-Broadcasts-Requested,

Warning-Type,

Warning-Security-Information,

Warning-Message-Content,

Warning-Area-Coordinates,

Send-Write-Replace-Warning-Indication,

Broadcast-Scheduled-Area-List,

Unknown-Tracking-Area-List,

Send-Stop-Warning-Indication,

Broadcast-Cancelled-Area-List,

Stop-All-Indicator,

Broadcast-Empty-Area-List,

Restarted-Cell-List,

Global-ENB-ID,

List-of-TAIs-Restart,

List-of-EAIs-Restart,

Failed-Cell-List,

List-of-5GS-TAIs,

Warning-Area-List-5GS,

Global-RAN-Node-ID,

Global-GNB-ID,

RAT-Selector-5GS,

Unknown-5GS-Tracking-Area-List,

Broadcast-Scheduled-Area-List-5GS,

Broadcast-Cancelled-Area-List-5GS,

Broadcast-Empty-Area-List-5GS,

Restarted-Cell-List-NR,

Failed-Cell-List-NR,

List-of-5GS-TAI-for-Restart

FROM SBC-AP-IEs

ProtocolExtensionContainer{},

ProtocolIE-Container{},

SBC-AP-PROTOCOL-EXTENSION,

SBC-AP-PROTOCOL-IES

FROM SBC-AP-Containers

id-Concurrent-Warning-Message-Indicator,

id-Criticality-Diagnostics,

id-Cause,

id-Data-Coding-Scheme,

id-List-of-TAIs,

id-Message-Identifier,

id-Serial-Number,

id-Number-of-Broadcasts-Requested,

id-Omc-Id,

id-Radio-Resource-Loading-List,

id-Recovery-Indication,

id-Repetition-Period,

id-Extended-Repetition-Period,

id-Warning-Area-List,

id-Warning-Message-Content,

id-Warning-Area-Coordinates,

id-Warning-Security-Information,

id-Warning-Type,

id-Send-Write-Replace-Warning-Indication,

id-Broadcast-Scheduled-Area-List,

id-Unknown-Tracking-Area-List,

id-Send-Stop-Warning-Indication,

id-Broadcast-Cancelled-Area-List,

id-Stop-All-Indicator,

id-Broadcast-Empty-Area-List,

id-Global-ENB-ID,

id-Restarted-Cell-List,

id-List-of-TAIs-Restart,

id-List-of-EAIs-Restart,

id-Failed-Cell-List,

id-List-of-5GS-TAIs,

id-Warning-Area-List-5GS,

id-Global-RAN-Node-ID,

id-Global-GNB-ID,

id-RAT-Selector-5GS,

id-Unknown-5GS-Tracking-Area-List,

id-Broadcast-Scheduled-Area-List-5GS,

id-Broadcast-Cancelled-Area-List-5GS,

id-Broadcast-Empty-Area-List-5GS,

id-Restarted-Cell-List-NR,

id-Failed-Cell-List-NR,

id-List-of-5GS-TAI-for-Restart

FROM SBC-AP-Constants;

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Write-Replace-Warning-Request

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

Write-Replace-Warning-Request ::= SEQUENCE {

protocolIEs ProtocolIE-Container { {Write-Replace-Warning-Request-IEs} },

protocolExtensions ProtocolExtensionContainer { {Write-Replace-Warning-Request-Extensions} } OPTIONAL,

...

}

Write-Replace-Warning-Request-IEs SBC-AP-PROTOCOL-IES ::= {

{ ID id-Message-Identifier CRITICALITY reject TYPE Message-Identifier PRESENCE mandatory } |

{ ID id-Serial-Number CRITICALITY reject TYPE Serial-Number PRESENCE mandatory } |

{ ID id-List-of-TAIs CRITICALITY reject TYPE List-of-TAIs PRESENCE optional } |

{ ID id-Warning-Area-List CRITICALITY ignore TYPE Warning-Area-List PRESENCE optional } |

{ ID id-Repetition-Period CRITICALITY reject TYPE Repetition-Period PRESENCE mandatory } |

{ ID id-Extended-Repetition-Period CRITICALITY reject TYPE Extended-Repetition-Period PRESENCE optional } |

{ ID id-Number-of-Broadcasts-Requested

CRITICALITY reject TYPE Number-of-Broadcasts-Requested PRESENCE mandatory } |

{ ID id-Warning-Type CRITICALITY ignore TYPE Warning-Type PRESENCE optional } |

{ ID id-Warning-Security-Information CRITICALITY ignore TYPE Warning-Security-Information PRESENCE optional } |

{ ID id-Data-Coding-Scheme CRITICALITY ignore TYPE Data-Coding-Scheme PRESENCE optional } |

{ ID id-Warning-Message-Content

CRITICALITY ignore TYPE Warning-Message-Content PRESENCE optional } |

{ ID id-Omc-Id CRITICALITY ignore TYPE Omc-Id PRESENCE optional } |

{ ID id-Concurrent-Warning-Message-Indicator CRITICALITY reject TYPE Concurrent-Warning-Message-Indicator PRESENCE optional } |

{ ID id-Send-Write-Replace-Warning-Indication CRITICALITY ignore TYPE Send-Write-Replace-Warning-Indication PRESENCE optional } |

{ ID id-Global-ENB-ID CRITICALITY ignore TYPE Global-ENB-ID PRESENCE optional },

... ,

{ID id-Warning-Area-Coordinates CRITICALITY ignore TYPE Warning-Area-Coordinates PRESENCE optional}

}

Write-Replace-Warning-Request-Extensions SBC-AP-PROTOCOL-EXTENSION ::= {

{ ID id-List-of-5GS-TAIs CRITICALITY ignore EXTENSION List-of-5GS-TAIs PRESENCE optional }|

{ ID id-Warning-Area-List-5GS CRITICALITY ignore EXTENSION Warning-Area-List-5GS PRESENCE optional }|

{ ID id-Global-RAN-Node-ID CRITICALITY ignore EXTENSION Global-RAN-Node-ID PRESENCE optional }|

{ ID id-RAT-Selector-5GS CRITICALITY ignore EXTENSION RAT-Selector-5GS PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Write-Replace-Warning-Response

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

Write-Replace-Warning-Response ::= SEQUENCE {

protocolIEs ProtocolIE-Container { {Write-Replace-Warning-Response-IEs} },

protocolExtensions ProtocolExtensionContainer { {Write-Replace-Warning-Response-Extensions} } OPTIONAL,

...

}

Write-Replace-Warning-Response-IEs SBC-AP-PROTOCOL-IES ::= {

{ ID id-Message-Identifier CRITICALITY reject TYPE Message-Identifier PRESENCE mandatory } |

{ ID id-Serial-Number CRITICALITY reject TYPE Serial-Number PRESENCE mandatory } |

{ ID id-Cause CRITICALITY reject TYPE Cause PRESENCE mandatory } |

{ ID id-Criticality-Diagnostics CRITICALITY ignore TYPE Criticality-Diagnostics PRESENCE optional } |

{ ID id-Unknown-Tracking-Area-List CRITICALITY ignore TYPE List-of-TAIs PRESENCE optional },

...

}

Write-Replace-Warning-Response-Extensions SBC-AP-PROTOCOL-EXTENSION ::= {

{ ID id-Unknown-5GS-Tracking-Area-List CRITICALITY ignore EXTENSION Unknown-5GS-Tracking-Area-List PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Stop-Warning-Request

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

Stop-Warning-Request ::= SEQUENCE {

protocolIEs ProtocolIE-Container { {Stop-Warning-Request-IEs} },

protocolExtensions ProtocolExtensionContainer { {Stop-Warning-Request-Extensions} } OPTIONAL,

...

}

Stop-Warning-Request-IEs SBC-AP-PROTOCOL-IES ::= {

{ ID id-Message-Identifier CRITICALITY reject TYPE Message-Identifier PRESENCE mandatory } |

{ ID id-Serial-Number CRITICALITY reject TYPE Serial-Number PRESENCE mandatory } |

{ ID id-List-of-TAIs CRITICALITY reject TYPE List-of-TAIs PRESENCE optional } |

{ ID id-Warning-Area-List CRITICALITY ignore TYPE Warning-Area-List PRESENCE optional }|

{ ID id-Omc-Id CRITICALITY ignore TYPE Omc-Id PRESENCE optional } |

{ ID id-Send-Stop-Warning-Indication CRITICALITY ignore TYPE Send-Stop-Warning-Indication PRESENCE optional } |

{ ID id-Stop-All-Indicator CRITICALITY reject TYPE Stop-All-Indicator PRESENCE optional},

...

}

Stop-Warning-Request-Extensions SBC-AP-PROTOCOL-EXTENSION ::= {

{ ID id-List-of-5GS-TAIs CRITICALITY ignore EXTENSION List-of-5GS-TAIs PRESENCE optional }|

{ ID id-Warning-Area-List-5GS CRITICALITY ignore EXTENSION Warning-Area-List-5GS PRESENCE optional } | { ID id-RAT-Selector-5GS CRITICALITY ignore EXTENSION RAT-Selector-5GS PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Stop-Warning-Response

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

Stop-Warning-Response ::= SEQUENCE {

protocolIEs ProtocolIE-Container { {Stop-Warning-Response-IEs} },

protocolExtensions ProtocolExtensionContainer { {Stop-Warning-Response-Extensions} } OPTIONAL,

...

}

Stop-Warning-Response-IEs SBC-AP-PROTOCOL-IES ::= {

{ ID id-Message-Identifier CRITICALITY reject TYPE Message-Identifier PRESENCE mandatory } |

{ ID id-Serial-Number CRITICALITY reject TYPE Serial-Number PRESENCE mandatory } |

{ ID id-Cause CRITICALITY reject TYPE Cause PRESENCE mandatory } |

{ ID id-Criticality-Diagnostics CRITICALITY ignore TYPE Criticality-Diagnostics PRESENCE optional } |

{ ID id-Unknown-Tracking-Area-List CRITICALITY ignore TYPE List-of-TAIs PRESENCE optional },

...

}

Stop-Warning-Response-Extensions SBC-AP-PROTOCOL-EXTENSION ::= {

{ ID id-Unknown-5GS-Tracking-Area-List CRITICALITY ignore EXTENSION Unknown-5GS-Tracking-Area-List PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Write-Replace-Warning-Indication

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

Write-Replace-Warning-Indication ::= SEQUENCE {

protocolIEs ProtocolIE-Container { {Write-Replace-Warning-Indication-IEs} },

protocolExtensions ProtocolExtensionContainer { {Write-Replace-Warning-Indication-Extensions} } OPTIONAL,

...

}

Write-Replace-Warning-Indication-IEs SBC-AP-PROTOCOL-IES ::= {

{ ID id-Message-Identifier CRITICALITY reject TYPE Message-Identifier PRESENCE mandatory } |

{ ID id-Serial-Number CRITICALITY reject TYPE Serial-Number PRESENCE mandatory } |

{ ID id-Broadcast-Scheduled-Area-List CRITICALITY reject TYPE Broadcast-Scheduled-Area-List PRESENCE optional },

...

}

Write-Replace-Warning-Indication-Extensions SBC-AP-PROTOCOL-EXTENSION ::= {

{ ID id-Broadcast-Scheduled-Area-List-5GS CRITICALITY ignore EXTENSION Broadcast-Scheduled-Area-List-5GS PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Stop-Warning-Indication

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

Stop-Warning-Indication ::= SEQUENCE {

protocolIEs ProtocolIE-Container { {Stop-Warning-Indication-IEs} },

protocolExtensions ProtocolExtensionContainer { {Stop-Warning-Indication-Extensions} } OPTIONAL,

...

}

Stop-Warning-Indication-IEs SBC-AP-PROTOCOL-IES ::= {

{ ID id-Message-Identifier CRITICALITY reject TYPE Message-Identifier PRESENCE mandatory } |

{ ID id-Serial-Number CRITICALITY reject TYPE Serial-Number PRESENCE mandatory } |

{ ID id-Broadcast-Cancelled-Area-List CRITICALITY reject TYPE Broadcast-Cancelled-Area-List PRESENCE optional }|

{ ID id-Broadcast-Empty-Area-List CRITICALITY ignore TYPE Broadcast-Empty-Area-List PRESENCE optional },

...

}

Stop-Warning-Indication-Extensions SBC-AP-PROTOCOL-EXTENSION ::= {

{ ID id-Broadcast-Cancelled-Area-List-5GS CRITICALITY ignore EXTENSION Broadcast-Cancelled-Area-List-5GS PRESENCE optional }|

{ ID id-Broadcast-Empty-Area-List-5GS CRITICALITY ignore EXTENSION Broadcast-Empty-Area-List-5GS PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PWS-Restart-Indication

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PWS-Restart-Indication ::= SEQUENCE {

protocolIEs ProtocolIE-Container { {PWS-Restart-Indication-IEs} },

protocolExtensions ProtocolExtensionContainer { {PWS-Restart-Indication-Extensions} } OPTIONAL,

...

}

PWS-Restart-Indication-IEs SBC-AP-PROTOCOL-IES ::= {

{ ID id-Restarted-Cell-List CRITICALITY reject TYPE Restarted-Cell-List PRESENCE mandatory }|

{ ID id-Global-ENB-ID CRITICALITY reject TYPE Global-ENB-ID PRESENCE mandatory } |

{ ID id-List-of-TAIs-Restart CRITICALITY reject TYPE List-of-TAIs-Restart PRESENCE mandatory } |

{ ID id-List-of-EAIs-Restart CRITICALITY reject TYPE List-of-EAIs-Restart PRESENCE optional },

...

}

PWS-Restart-Indication-Extensions SBC-AP-PROTOCOL-EXTENSION ::= {

{ ID id-Restarted-Cell-List-NR CRITICALITY ignore EXTENSION Restarted-Cell-List-NR PRESENCE optional }|

{ ID id-List-of-5GS-TAI-for-Restart CRITICALITY ignore EXTENSION List-of-5GS-TAI-for-Restart PRESENCE optional }|

{ ID id-Global-GNB-ID CRITICALITY ignore EXTENSION Global-GNB-ID PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PWS-Failure-Indication

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PWS-Failure-Indication ::= SEQUENCE {

protocolIEs ProtocolIE-Container { {PWS-Failure-Indication-IEs} },

protocolExtensions ProtocolExtensionContainer { {PWS-Failure-Indication-Extensions} } OPTIONAL,

...

}

PWS-Failure-Indication-IEs SBC-AP-PROTOCOL-IES ::= {

{ ID id-Failed-Cell-List CRITICALITY reject TYPE Failed-Cell-List PRESENCE mandatory }|

{ ID id-Global-ENB-ID CRITICALITY reject TYPE Global-ENB-ID PRESENCE mandatory },

...

}

PWS-Failure-Indication-Extensions SBC-AP-PROTOCOL-EXTENSION ::= {

{ ID id-Failed-Cell-List-NR CRITICALITY ignore EXTENSION Failed-Cell-List-NR PRESENCE optional }|

{ ID id-Global-GNB-ID CRITICALITY ignore EXTENSION Global-GNB-ID PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- ERROR INDICATION ELEMENTARY PROCEDURE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Error Indication

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

Error-Indication ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ErrorIndicationIEs}},

...

}

ErrorIndicationIEs SBC-AP-PROTOCOL-IES ::= {

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE optional } |

{ ID id-Criticality-Diagnostics CRITICALITY ignore TYPE Criticality-Diagnostics PRESENCE optional } ,

...

}

END

### 4.4.5 Information element definitions

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Information Element Definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SBC-AP-IEs {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

eps-Access (21) modules (3) sbc-AP (3) version1 (1) sbc-AP-IEs (2)}

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS

maxNrOfErrors,

maxNrOfTAIs,

maxnoofTAIforWarning,

maxnoofCellID,

maxnoofEmergencyAreaID,

id-TypeOfError,

maxnoofCellinEAI,

maxnoofCellinTAI,

maxnoofeNBIds,

maxnoofRestartTAIs,

maxnoofRestartEAIs,

maxnoofRestartedCells,

maxnoofFailedCells,

maxnoof5GSTAIs,

maxnoofCellsingNB,

maxnoofCellsin5GS,

maxnoofCellsforRestartNR,

maxnoofRANNodes,

maxnoofRestart5GSTAIs,

maxnoofCellsin5GSTAI

FROM SBC-AP-Constants

Criticality,

ProcedureCode,

TriggeringMessage,

ProtocolIE-ID

FROM SBC-AP-CommonDataTypes

ProtocolExtensionContainer{},

SBC-AP-PROTOCOL-EXTENSION

FROM SBC-AP-Containers;

-- A

-- B

Broadcast-Scheduled-Area-List ::= SEQUENCE {

cellId-Broadcast-List CellId-Broadcast-List OPTIONAL,

tAI-Broadcast-List TAI-Broadcast-List OPTIONAL,

emergencyAreaID-Broadcast-List EmergencyAreaID-Broadcast-List OPTIONAL,

iE-Extensions ProtocolExtensionContainer {{Broadcast-Scheduled-Area-List-ExtIEs}} OPTIONAL,

...

}

Broadcast-Scheduled-Area-List-ExtIEs SBC-AP-PROTOCOL-EXTENSION ::= {

...

}

Broadcast-Scheduled-Area-List-5GS ::= SEQUENCE {

cellId-Broadcast-List-5GS CellId-Broadcast-List-5GS OPTIONAL,

tAI-Broadcast-List-5GS TAI-Broadcast-List-5GS OPTIONAL,

emergencyAreaID-Broadcast-List EmergencyAreaID-Broadcast-List OPTIONAL,

iE-Extensions ProtocolExtensionContainer {{Broadcast-Scheduled-Area-List-5GS-ExtIEs}} OPTIONAL,

...

}

Broadcast-Scheduled-Area-List-5GS-ExtIEs SBC-AP-PROTOCOL-EXTENSION ::= {

...

}

Broadcast-Cancelled-Area-List ::= SEQUENCE {

cellID-Cancelled-List CellID-Cancelled-List OPTIONAL,

tAI-Cancelled-List TAI-Cancelled-List OPTIONAL,

emergencyAreaID-Cancelled-List EmergencyAreaID-Cancelled-List OPTIONAL,

iE-Extensions ProtocolExtensionContainer {{Broadcast-Cancelled-Area-List-ExtIEs}} OPTIONAL,

...

}

Broadcast-Cancelled-Area-List-ExtIEs SBC-AP-PROTOCOL-EXTENSION ::= {

...

}

Broadcast-Cancelled-Area-List-5GS ::= SEQUENCE {

cellID-Cancelled-List-5GS CellID-Cancelled-List-5GS OPTIONAL,

tAI-Cancelled-List-5GS TAI-Cancelled-List-5GS OPTIONAL,

emergencyAreaID-Cancelled-List EmergencyAreaID-Cancelled-List OPTIONAL,

iE-Extensions ProtocolExtensionContainer {{Broadcast-Cancelled-Area-List-5GS-ExtIEs}} OPTIONAL,

...

}

Broadcast-Cancelled-Area-List-5GS-ExtIEs SBC-AP-PROTOCOL-EXTENSION ::= {

...

}

Broadcast-Empty-Area-List ::= SEQUENCE (SIZE (1.. maxnoofeNBIds)) OF Global-ENB-ID

Broadcast-Empty-Area-List-5GS ::= SEQUENCE (SIZE (1.. maxnoofRANNodes)) OF Global-RAN-Node-ID

-- C

CancelledCellinEAI ::= SEQUENCE (SIZE(1..maxnoofCellinEAI)) OF CancelledCellinEAI-Item

CancelledCellinEAI-Item ::= SEQUENCE {

eCGI EUTRAN-CGI,

numberOfBroadcasts NumberOfBroadcasts,

iE-Extensions ProtocolExtensionContainer { {CancelledCellinEAI-Item-ExtIEs} } OPTIONAL,

...

}

CancelledCellinEAI-Item-ExtIEs SBC-AP-PROTOCOL-EXTENSION ::= {

...

}

CancelledCellinTAI ::= SEQUENCE (SIZE(1..maxnoofCellinTAI)) OF CancelledCellinTAI-Item

CancelledCellinTAI-Item ::= SEQUENCE{

eCGI EUTRAN-CGI,

numberOfBroadcasts NumberOfBroadcasts,

iE-Extensions ProtocolExtensionContainer { {CancelledCellinTAI-Item-ExtIEs} } OPTIONAL,

...

}

CancelledCellinTAI-Item-ExtIEs SBC-AP-PROTOCOL-EXTENSION ::= {

...

}

CancelledCellinTAI-5GS ::= SEQUENCE (SIZE(1..maxnoofCellsin5GSTAI)) OF

SEQUENCE{

nR-CGI NR-CGI,

numberOfBroadcasts NumberOfBroadcasts,

iE-Extensions ProtocolExtensionContainer { {CancelledCellinTAI-5GS-ExtIEs} } OPTIONAL,

...

}

CancelledCellinTAI-5GS-ExtIEs SBC-AP-PROTOCOL-EXTENSION ::= {

...

}

Cause ::= INTEGER {

message-accepted (0),

parameter-not-recognised (1),

parameter-value-invalid (2),

valid-message-not-identified (3),

tracking-area-not-valid (4),

unrecognised-message (5),

missing-mandatory-element (6),

mME-capacity-exceeded (7),

mME-memory-exceeded (8),

warning-broadcast-not-supported (9),

warning-broadcast-not-operational (10),

message-reference-already-used (11),

unspecifed-error (12),

transfer-syntax-error (13),

semantic-error (14),

message-not-compatible-with-receiver-state (15),

abstract-syntax-error-reject (16),

abstract-syntax-error-ignore-and-notify (17),

abstract-syntax-error-falsely-constructed-message (18)

} (0..255)

CellId-Broadcast-List ::= SEQUENCE (SIZE(1..maxnoofCellID)) OF CellId-Broadcast-List-Item

CellId-Broadcast-List-Item ::= SEQUENCE {

eCGI EUTRAN-CGI,

iE-Extensions ProtocolExtensionContainer { {CellId-Broadcast-List-Item-ExtIEs} } OPTIONAL,

...

}

CellId-Broadcast-List-Item-ExtIEs SBC-AP-PROTOCOL-EXTENSION ::= {

...

}

CellId-Broadcast-List-5GS ::= SEQUENCE (SIZE(1..maxnoofCellsin5GS)) OF

SEQUENCE {

nR-CGI NR-CGI,

iE-Extensions ProtocolExtensionContainer { {CellId-Broadcast-List-5GS-ExtIEs} } OPTIONAL,

...

}

CellId-Broadcast-List-5GS-ExtIEs SBC-AP-PROTOCOL-EXTENSION ::= {

...

}

CellID-Cancelled-List ::= SEQUENCE (SIZE(1..maxnoofCellID)) OF CellID-Cancelled-Item

CellID-Cancelled-Item ::= SEQUENCE {

eCGI EUTRAN-CGI,

numberOfBroadcasts NumberOfBroadcasts,

iE-Extensions ProtocolExtensionContainer { {CellID-Cancelled-Item-ExtIEs} } OPTIONAL,

...

}

CellID-Cancelled-Item-ExtIEs SBC-AP-PROTOCOL-EXTENSION ::= {

...

}

CellID-Cancelled-List-5GS ::= SEQUENCE (SIZE(1..maxnoofCellsin5GS)) OF

SEQUENCE {

nR-CGI NR-CGI,

numberOfBroadcasts NumberOfBroadcasts,

iE-Extensions ProtocolExtensionContainer { {CellID-Cancelled-5GS-ExtIEs} } OPTIONAL,

...

}

CellID-Cancelled-5GS-ExtIEs SBC-AP-PROTOCOL-EXTENSION ::= {

...

}

CellIdentity ::= BIT STRING (SIZE (28))

Concurrent-Warning-Message-Indicator ::= ENUMERATED {true}

Criticality-Diagnostics ::= SEQUENCE {

procedureCode ProcedureCode OPTIONAL,

triggeringMessage TriggeringMessage OPTIONAL,

procedureCriticality Criticality OPTIONAL,

iE-CriticalityDiagnostics CriticalityDiagnostics-IE-List OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {CriticalityDiagnostics-ExtIEs} } OPTIONAL,

...

}

CriticalityDiagnostics-ExtIEs SBC-AP-PROTOCOL-EXTENSION ::= {

...

}

CriticalityDiagnostics-IE-List ::= SEQUENCE (SIZE (1..maxNrOfErrors)) OF

SEQUENCE {

iECriticality Criticality,

iE-ID ProtocolIE-ID,

typeOfError TypeOfError,

iE-Extensions ProtocolExtensionContainer {{CriticalityDiagnostics-IE-Item-ExtIEs}} OPTIONAL,

...

}

CriticalityDiagnostics-IE-Item-ExtIEs SBC-AP-PROTOCOL-EXTENSION ::= {

...

}

-- D

Data-Coding-Scheme ::= BIT STRING (SIZE (8))

-- E

ECGIList ::= SEQUENCE (SIZE(1..maxnoofCellID)) OF EUTRAN-CGI

Emergency-Area-ID-List ::= SEQUENCE (SIZE(1..maxnoofEmergencyAreaID)) OF Emergency-Area-ID

Emergency-Area-ID ::= OCTET STRING (SIZE (3))

EmergencyAreaID-Broadcast-List ::= SEQUENCE (SIZE(1..maxnoofEmergencyAreaID)) OF EmergencyAreaID-Broadcast-List-Item

EmergencyAreaID-Broadcast-List-Item ::= SEQUENCE {

emergencyAreaID Emergency-Area-ID,

scheduledCellinEAI ScheduledCellinEAI,

iE-Extensions ProtocolExtensionContainer { {EmergencyAreaID-Broadcast-List-Item-ExtIEs} } OPTIONAL,

...

}

EmergencyAreaID-Broadcast-List-Item-ExtIEs SBC-AP-PROTOCOL-EXTENSION ::= {

...

}

EmergencyAreaID-Cancelled-List ::= SEQUENCE (SIZE(1..maxnoofEmergencyAreaID)) OF EmergencyAreaID-Cancelled-Item

EmergencyAreaID-Cancelled-Item ::= SEQUENCE {

emergencyAreaID Emergency-Area-ID,

cancelledCellinEAI CancelledCellinEAI,

iE-Extensions ProtocolExtensionContainer { {EmergencyAreaID-Cancelled-Item-ExtIEs} } OPTIONAL,

...

}

EmergencyAreaID-Cancelled-Item-ExtIEs SBC-AP-PROTOCOL-EXTENSION ::= {

...

}

EUTRAN-CGI ::= SEQUENCE {

pLMNidentity PLMNidentity,

cell-ID CellIdentity,

iE-Extensions ProtocolExtensionContainer { {EUTRAN-CGI-ExtIEs} } OPTIONAL,

...

}

EUTRAN-CGI-ExtIEs SBC-AP-PROTOCOL-EXTENSION ::= {

...

}

Extended-Repetition-Period ::= INTEGER (4096..131071)

ENB-ID ::= CHOICE {

macroENB-ID BIT STRING (SIZE(20)),

homeENB-ID BIT STRING (SIZE(28)),

...,

short-macroENB-ID BIT STRING (SIZE(18)),

long-macroENB-ID BIT STRING (SIZE(21))

}

-- F

Failed-Cell-List ::= SEQUENCE (SIZE(1..maxnoofFailedCells)) OF EUTRAN-CGI

Failed-Cell-List-NR ::= SEQUENCE (SIZE(1..maxnoofCellsingNB)) OF NR-CGI

-- G

Global-ENB-ID ::= SEQUENCE {

pLMNidentity PLMNidentity,

eNB-ID ENB-ID,

iE-Extensions ProtocolExtensionContainer { {GlobalENB-ID-ExtIEs} } OPTIONAL,

...

}

GlobalENB-ID-ExtIEs SBC-AP-PROTOCOL-EXTENSION ::= {

...

}

Global-RAN-Node-ID ::= CHOICE {

global-GNB-ID Global-GNB-ID,

global-NgENB-ID Global-NgENB-ID,

...

}

Global-GNB-ID ::= SEQUENCE {

pLMNidentity PLMNidentity,

gNB-ID GNB-ID,

iE-Extensions ProtocolExtensionContainer { {Global-GNB-ID-ExtIEs} } OPTIONAL,

...

}

Global-GNB-ID-ExtIEs SBC-AP-PROTOCOL-EXTENSION ::= {

...

}

GNB-ID ::= CHOICE {

gNB-ID BIT STRING (SIZE(22..32)),

...

}

Global-NgENB-ID ::= SEQUENCE {

pLMNidentity PLMNidentity,

ngENB-ID ENB-ID,

iE-Extensions ProtocolExtensionContainer { {Global-NgENB-ID-ExtIEs} } OPTIONAL,

...

}

Global-NgENB-ID-ExtIEs SBC-AP-PROTOCOL-EXTENSION ::= {

...

}

-- H

-- I

-- J

-- K

-- L

List-of-TAIs ::= SEQUENCE (SIZE (1..maxNrOfTAIs)) OF

SEQUENCE {

tai TAI

}

List-of-TAIs-Restart ::= SEQUENCE (SIZE (1..maxnoofRestartTAIs)) OF

SEQUENCE {

tai TAI

}

List-of-EAIs-Restart ::= SEQUENCE (SIZE(1..maxnoofRestartEAIs)) OF Emergency-Area-ID

List-of-5GS-TAIs ::= SEQUENCE (SIZE (1..maxnoof5GSTAIs)) OF TAI-5GS

List-of-5GS-Cells-for-Failure ::= SEQUENCE ( SIZE(1..maxnoofCellsingNB)) OF NR-CGI

List-of-5GS-TAI-for-Restart ::= SEQUENCE (SIZE (1..maxnoofRestart5GSTAIs)) OF TAI-5GS

-- M

Message-Identifier ::= BIT STRING (SIZE (16))

-- N

Number-of-Broadcasts-Requested ::= INTEGER (0..65535)

-- For Number-of-Broadcasts-Requested = 0 and Repetition-Period = 0, then eNB action is no broadcast

-- for ETWS Secondary and CMAS.

--

-- For Number-of-Broadcasts-Requested = 1 and Repetition-Period = 0, then eNB action is broadcast

-- only once for ETWS and CMAS.

--

-- For Number-of-Broadcasts-Requested = 0 and Repetition-Period > 0, then eNB action is no broadcast

-- for the ETWS Secondary, and broadcast until further notice for the CMAS.

--

-- For Number-of-Broadcasts-Requested > 0 and Repetition-Period > 0, then eNB action is normal

-- broadcast.

-- All other combinations of Number-of-Broadcasts-Requested and Repetition-Period are considered

-- invalid.

NumberOfBroadcasts ::= INTEGER (0..65535)

NR-CGIList ::= SEQUENCE (SIZE(1..maxnoofCellsingNB)) OF NR-CGI

NR-CGI ::= SEQUENCE {

pLMNidentity PLMNidentity,

nRCellIdentity NRCellIdentity,

iE-Extensions ProtocolExtensionContainer { {NR-CGI-ExtIEs} } OPTIONAL,

...

}

NR-CGI-ExtIEs SBC-AP-PROTOCOL-EXTENSION ::= {

...

}

NRCellIdentity ::= BIT STRING (SIZE(36))

NgENB-ID ::= CHOICE {

macroNgENB-ID BIT STRING (SIZE(20)),

shortMacroNgENB-ID BIT STRING (SIZE(18)),

longMacroNgENB-ID BIT STRING (SIZE(21)),

...

}

-- O

Omc-Id ::= OCTET STRING (SIZE (1..20))

-- P

PLMNidentity ::= TBCD-STRING

-- Q

-- R

Repetition-Period ::= INTEGER (0..4096)

-- 1 to 4096: Each unit represents a repetition of one second to a maximum of

-- once per 4096 seconds (~1 hour).

-- 0: no repetition

-- A CBC compliant to this version or later of this specification shall not send a repetition period

-- greater than 4095.

-- For backwards compatibility with a CBC compliant to an earlier version of this specification the

-- maximum value of the repetition period defined in ASN.1 remains at 4096.

-- If the value of the *Repetition Period* IE received in the WRITE-REPLACE WARNING REQUEST message is

-- set to 4096, the MME shall set the *Repetition Period IE* to the maximum value 4095 supported on

-- the S1-MME interface as defined in [7] before forwarding to the selected eNBs.

Restarted-Cell-List ::= SEQUENCE (SIZE(1.. maxnoofRestartedCells)) OF EUTRAN-CGI

RAT-Selector-5GS ::= ENUMERATED {true}

Restarted-Cell-List-NR ::= SEQUENCE (SIZE(1.. maxnoofCellsforRestartNR)) OF NR-CGI

-- S

ScheduledCellinEAI ::= SEQUENCE (SIZE(1..maxnoofCellinEAI)) OF ScheduledCellinEAI-Item

ScheduledCellinEAI-Item ::= SEQUENCE {

eCGI EUTRAN-CGI,

iE-Extensions ProtocolExtensionContainer { {ScheduledCellinEAI-Item-ExtIEs} } OPTIONAL,

...

}

ScheduledCellinEAI-Item-ExtIEs SBC-AP-PROTOCOL-EXTENSION ::= {

...

}

ScheduledCellinTAI ::= SEQUENCE (SIZE(1..maxnoofCellinTAI)) OF ScheduledCellinTAI-Item

ScheduledCellinTAI-Item ::= SEQUENCE{

eCGI EUTRAN-CGI,

iE-Extensions ProtocolExtensionContainer { {ScheduledCellinTAI-Item-ExtIEs} } OPTIONAL,

...

}

ScheduledCellinTAI-Item-ExtIEs SBC-AP-PROTOCOL-EXTENSION ::= {

...

}

ScheduledCellinTAI-5GS ::= SEQUENCE (SIZE(1..maxnoofCellsin5GSTAI)) OF

SEQUENCE{

nR-CGI NR-CGI,

iE-Extensions ProtocolExtensionContainer { {ScheduledCellinTAI-5GS-ExtIEs} } OPTIONAL,

...

}

ScheduledCellinTAI-5GS-ExtIEs SBC-AP-PROTOCOL-EXTENSION ::= {

...

}

Send-Write-Replace-Warning-Indication ::= ENUMERATED {true}

Send-Stop-Warning-Indication ::= ENUMERATED {true}

Serial-Number ::= BIT STRING (SIZE (16))

Stop-All-Indicator ::= ENUMERATED {true}

-- T

TAC ::= OCTET STRING (SIZE (2))

TAC-5GS ::= OCTET STRING (SIZE (3))

TAI-Broadcast-List ::= SEQUENCE (SIZE(1..maxnoofTAIforWarning)) OF TAI-Broadcast-List-Item

TAI-Broadcast-List-Item ::= SEQUENCE {

tAI TAI,

scheduledCellinTAI ScheduledCellinTAI,

iE-Extensions ProtocolExtensionContainer { {TAI-Broadcast-List-Item-ExtIEs} } OPTIONAL,

...

}

TAI-Broadcast-List-Item-ExtIEs SBC-AP-PROTOCOL-EXTENSION ::= {

...

}

TAI-Broadcast-List-5GS ::= SEQUENCE (SIZE(1..maxnoof5GSTAIs)) OF

SEQUENCE {

tAI-5GS TAI-5GS,

scheduledCellinTAI-5GS ScheduledCellinTAI-5GS,

iE-Extensions ProtocolExtensionContainer { {TAI-Broadcast-List-5GS-ExtIEs} } OPTIONAL,

...

}

TAI-Broadcast-List-5GS-ExtIEs SBC-AP-PROTOCOL-EXTENSION ::= {

...

}

TAI-Cancelled-List ::= SEQUENCE (SIZE(1..maxnoofTAIforWarning)) OF TAI-Cancelled-List-Item

TAI-Cancelled-List-Item ::= SEQUENCE {

tAI TAI,

cancelledCellinTAI CancelledCellinTAI,

iE-Extensions ProtocolExtensionContainer { {TAI-Cancelled-List-Item-ExtIEs} } OPTIONAL,

...

}

TAI-Cancelled-List-Item-ExtIEs SBC-AP-PROTOCOL-EXTENSION ::= {

...

}

TAI-Cancelled-List-5GS ::= SEQUENCE (SIZE(1..maxnoof5GSTAIs)) OF

SEQUENCE {

tAI-5GS TAI-5GS,

cancelledCellinTAI-5GS CancelledCellinTAI-5GS,

iE-Extensions ProtocolExtensionContainer { {TAI-Cancelled-List-5GS-ExtIEs} } OPTIONAL,

...

}

TAI-Cancelled-List-5GS-ExtIEs SBC-AP-PROTOCOL-EXTENSION ::= {

...

}

TAI-List-for-Warning ::= SEQUENCE (SIZE(1.. maxnoofTAIforWarning)) OF TAI

TAI ::= SEQUENCE {

pLMNidentity PLMNidentity,

tAC TAC,

iE-Extensions ProtocolExtensionContainer { {TAI-ExtIEs} } OPTIONAL

}

TAI-ExtIEs SBC-AP-PROTOCOL-EXTENSION ::= {

...

}

TBCD-STRING ::= OCTET STRING (SIZE (3))

TypeOfError ::= ENUMERATED {

not-understood,

missing,

...

}

TAI-5GS ::= SEQUENCE {

pLMNidentity PLMNidentity,

tAC-5GS TAC-5GS,

iE-Extensions ProtocolExtensionContainer { {TAI-5GS-ExtIEs} } OPTIONAL

}

TAI-5GS-ExtIEs SBC-AP-PROTOCOL-EXTENSION ::= {

...

}

-- U

Unknown-Tracking-Area-List ::= SEQUENCE (SIZE(1.. maxNrOfTAIs)) OF TAI

Unknown-5GS-Tracking-Area-List ::= SEQUENCE (SIZE(1.. maxnoof5GSTAIs)) OF TAI-5GS

-- V

-- W

Warning-Area-List ::= CHOICE {

cell-ID-List ECGIList,

tracking-Area-List-for-Warning TAI-List-for-Warning,

emergency-Area-ID-List Emergency-Area-ID-List,

...

}

Warning-Message-Content ::= OCTET STRING (SIZE (1..9600))

Warning-Area-Coordinates ::= OCTET STRING (SIZE (1..1024))

Warning-Security-Information ::= OCTET STRING (SIZE (50))

Warning-Type ::= OCTET STRING (SIZE (2))

Warning-Area-List-5GS ::= CHOICE {

cell-ID-List ECGIList,

nR-CGIList NR-CGIList,

tAIList-5GS TAI-5GS,

emergencyAreaIDList Emergency-Area-ID-List,

...

}

-- X

-- Y

END

### 4.4.6 Common definitions

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Common definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SBC-AP-CommonDataTypes {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

eps-Access (21) modules (3) sbc-AP (3) version1 (1) sbc-AP-CommonDataTypes (3)}

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

Criticality ::= ENUMERATED { reject, ignore, notify }

Presence ::= ENUMERATED { optional, conditional, mandatory }

ProcedureCode ::= INTEGER (0..255)

ProtocolExtensionID ::= INTEGER (0..65535)

ProtocolIE-ID ::= INTEGER (0..65535)

TriggeringMessage ::= ENUMERATED {initiating-message, successful-outcome, unsuccessful-outcome, outcome}

END

### 4.4.7 Constant definitions

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Constant definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SBC-AP-Constants {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

eps-Access (21) modules (3) sbc-AP (3) version1 (1) sbc-AP-Constants (4)}

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Elementary Procedures

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

id-Write-Replace-Warning INTEGER ::= 0

id-Stop-Warning INTEGER ::= 1

id-Error-Indication INTEGER ::= 2

id-Write-Replace-Warning-Indication INTEGER ::= 3

id-Stop-Warning-Indication INTEGER ::= 4

id-PWS-Restart-Indication INTEGER ::= 5

id-PWS-Failure-Indication INTEGER ::= 6

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IEs

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

id-Broadcast-Message-Content INTEGER ::= 0

id-Cause INTEGER ::= 1

id-Criticality-Diagnostics INTEGER ::=2

id-Data-Coding-Scheme INTEGER ::= 3

id-Failure-List INTEGER ::= 4

id-Message-Identifier INTEGER ::= 5

id-Number-of-Broadcasts-Completed-List INTEGER ::= 6

id-Number-of-Broadcasts-Requested INTEGER ::= 7

id-Radio-Resource-Loading-List INTEGER ::= 8

id-Recovery-Indication INTEGER ::= 9

id-Repetition-Period INTEGER ::= 10

id-Serial-Number INTEGER ::= 11

id-Service-Areas-List INTEGER ::= 12

id-TypeOfError INTEGER ::= 13

id-List-of-TAIs INTEGER ::= 14

id-Warning-Area-List INTEGER ::= 15

id-Warning-Message-Content INTEGER ::= 16

id-Warning-Security-Information INTEGER ::= 17

id-Warning-Type INTEGER ::= 18

id-Omc-Id INTEGER ::= 19

id-Concurrent-Warning-Message-Indicator INTEGER ::= 20

id-Extended-Repetition-Period INTEGER ::= 21

id-Unknown-Tracking-Area-List INTEGER ::= 22

id-Broadcast-Scheduled-Area-List INTEGER ::= 23

id-Send-Write-Replace-Warning-Indication INTEGER ::= 24

id-Broadcast-Cancelled-Area-List INTEGER ::= 25

id-Send-Stop-Warning-Indication INTEGER ::= 26

id-Stop-All-Indicator INTEGER ::= 27

id-Global-ENB-ID INTEGER ::= 28

id-Broadcast-Empty-Area-List INTEGER ::= 29

id-Restarted-Cell-List INTEGER ::= 30

id-List-of-TAIs-Restart INTEGER ::= 31

id-List-of-EAIs-Restart INTEGER ::= 32

id-Failed-Cell-List INTEGER ::= 33

id-List-of-5GS-TAIs INTEGER ::= 34

id-Warning-Area-List-5GS INTEGER ::= 35

id-Global-RAN-Node-ID INTEGER ::= 36

id-Global-GNB-ID INTEGER ::= 37

id-RAT-Selector-5GS INTEGER ::= 38

id-Unknown-5GS-Tracking-Area-List INTEGER ::= 39

id-Broadcast-Scheduled-Area-List-5GS INTEGER ::= 40

id-Broadcast-Cancelled-Area-List-5GS INTEGER ::= 41

id-Broadcast-Empty-Area-List-5GS INTEGER ::= 42

id-Restarted-Cell-List-NR INTEGER ::= 43

id-Failed-Cell-List-NR INTEGER ::= 44

id-List-of-5GS-TAI-for-Restart INTEGER ::= 45

id-Warning-Area-Coordinates INTEGER ::= 46

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Extension constants

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Lists

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

maxNrOfErrors INTEGER ::= 256

maxnoofCellID INTEGER ::= 65535

maxnoofCellinEAI INTEGER ::= 65535

maxnoofCellinTAI INTEGER ::= 65535

maxNrOfTAIs INTEGER ::= 65535

maxnoofEmergencyAreaID INTEGER ::= 65535

maxnoofTAIforWarning INTEGER ::= 65535

maxProtocolExtensions INTEGER ::= 65535

maxProtocolIEs INTEGER ::= 65535

maxnoofeNBIds INTEGER ::= 256

maxnoofRestartedCells INTEGER ::= 256

maxnoofRestartTAIs INTEGER ::= 2048

maxnoofRestartEAIs INTEGER ::= 256

maxnoofFailedCells INTEGER ::= 256

maxnoof5GSTAIs INTEGER ::= 2048

maxnoofCellsingNB INTEGER ::= 16384

maxnoofCellsin5GS INTEGER ::= 16776960

maxnoofCellsin5GSTAI INTEGER ::= 65535

maxnoofRANNodes INTEGER ::= 65535

maxnoofRestart5GSTAIs INTEGER ::= 2048maxnoofCellsforRestartNR INTEGER ::= 16384

END

### 4.4.8 Container Definitions

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Container definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SBC-AP-Containers {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

eps-Access (21) modules (3) sbc-AP (3) version1 (1) sbc-AP-Containers (5)}

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IE parameter types from other modules.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IMPORTS

Criticality,

Presence,

ProtocolExtensionID,

ProtocolIE-ID

FROM SBC-AP-CommonDataTypes

maxProtocolExtensions,

maxProtocolIEs

FROM SBC-AP-Constants;

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Class Definition for Protocol IEs

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SBC-AP-PROTOCOL-IES ::= CLASS {

&id ProtocolIE-ID UNIQUE,

&criticality Criticality DEFAULT ignore,

&Value,

&presence Presence

}

WITH SYNTAX {

ID &id

CRITICALITY &criticality

TYPE &Value

PRESENCE &presence

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Class Definition for Protocol Extensions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SBC-AP-PROTOCOL-EXTENSION ::= CLASS {

&id ProtocolExtensionID UNIQUE,

&criticality Criticality DEFAULT ignore,

&Extension,

&presence Presence

}

WITH SYNTAX {

ID &id

CRITICALITY &criticality

EXTENSION &Extension

PRESENCE &presence

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Container for Protocol IEs

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ProtocolIE-Container {SBC-AP-PROTOCOL-IES : IEsSetParam} ::=

SEQUENCE (SIZE (0..maxProtocolIEs)) OF

ProtocolIE-Field {{IEsSetParam}}

ProtocolIE-Field {SBC-AP-PROTOCOL-IES : IEsSetParam} ::= SEQUENCE {

id SBC-AP-PROTOCOL-IES.&id ({IEsSetParam}),

criticality SBC-AP-PROTOCOL-IES.&criticality ({IEsSetParam}{@id}),

value SBC-AP-PROTOCOL-IES.&Value ({IEsSetParam}{@id})

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Container Lists for Protocol IE Containers

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ProtocolIE-ContainerList {INTEGER : lowerBound, INTEGER : upperBound, SBC-AP-PROTOCOL-IES : IEsSetParam} ::=

SEQUENCE (SIZE (lowerBound..upperBound)) OF

ProtocolIE-Container {{IEsSetParam}}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Container for Protocol Extensions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ProtocolExtensionContainer {SBC-AP-PROTOCOL-EXTENSION : ExtensionSetParam} ::=

SEQUENCE (SIZE (1..maxProtocolExtensions)) OF

ProtocolExtensionField {{ExtensionSetParam}}

ProtocolExtensionField {SBC-AP-PROTOCOL-EXTENSION : ExtensionSetParam} ::= SEQUENCE {

id SBC-AP-PROTOCOL-EXTENSION.&id ({ExtensionSetParam}),

criticality SBC-AP-PROTOCOL-EXTENSION.&criticality ({ExtensionSetParam}{@id}),

extensionValue SBC-AP-PROTOCOL-EXTENSION.&Extension ({ExtensionSetParam}{@id})

}

END

## 4.4.9 Message transfer syntax

SBC-AP shall use the ASN.1 Basic Packed Encoding Rules (BASIC-PER) Aligned Variant as transfer syntax as specified in ref. [10].

## 4.5 Handling of unknown, unforeseen or erroneous protocol data

## 4.5.1 General

Protocol Error cases can be divided into three classes:

 Transfer Syntax Error;

 Abstract Syntax Error;

 Logical Error.

Protocol errors can occur in the following functions within a receiving node:



Figure 4.5.1-1: Protocol Errors in SBc-AP

The information stated in clauses 4.5.2, 4.5.3 and 4.5.4, to be included in the message used when reporting an error, is what at minimum shall be included. Other optional information elements within the message may also be included, if available. This is also valid for the case when the reporting is done with a response message.

## 4.5.2 Transfer Syntax Error

A Transfer Syntax Error occurs when the receiver is not able to decode the received physical message Transfer syntax errors are always detected in the process of ASN.1 decoding. If a Transfer Syntax Error occurs, the receiver should initiate Error Indication procedure with appropriate cause value for the Transfer Syntax protocol error.

## 4.5.3 Abstract Syntax Error

### 4.5.3.1 General

An Abstract Syntax Error occurs when the receiving functional SBc-AP entity:

1. receives IEs or IE groups that cannot be understood (unknown IE id);

2. receives IEs for which the logical range is violated (e.g.: ASN.1 definition: 0 to 15, the logical range is 0 to 10 (values 11 to 15 are undefined), and 12 will be received; this case will be handled as an abstract syntax error using criticality information sent by the originator of the message);

3. does not receive IEs or IE groups but according to the specified presence of the concerning object, the IEs or IE groups should have been present in the received message;

4. receives IEs or IE groups that are defined to be part of that message in wrong order or with too many occurrences of the same IE or IE group;

5. receives IEs or IE groups but according to the conditional presence of the concerning object and the specified condition, the IEs or IE groups should not have been present in the received message.

Cases 1 and 2 (not comprehended IE/IE group) are handled based on received Criticality information. Case 3 (missing IE/IE group) is handled based on Criticality information and Presence information for the missing IE/IE group specified in the version of the specification used by the receiver. Case 4 (IEs or IE groups in wrong order or with too many occurrences) and Case 5 (erroneously present conditional IEs or IE groups) result in rejecting the procedure.

If an Abstract Syntax Error occurs, the receiver shall read the remaining message and shall then for each detected Abstract Syntax Error act according to the Criticality Information and Presence Information for the IE/IE group due to which Abstract Syntax Error occurred in accordance with clauses 4.5.3.4 and 4.5.3.5. The handling of cases 4 and 5 is specified in clause 4.5.3.6.

### 4.5.3.2 Criticality information

In the SBc-AP messages there is criticality information set for individual IEs and/or IE groups. This criticality information instructs the receiver how to act when receiving an IE or an IE group that is not comprehended i.e. the entire item (IE or IE group) which is not (fully or partially) comprehended shall be treated in accordance with its own criticality information as specified in clause 4.5.3.4.

In addition, the criticality information is used in case of the missing IE/IE group abstract syntax error (see clause 4.5.3.5).

The receiving node shall take different actions depending on the value of the Criticality Information. The three possible values of the Criticality Information for an IE/IE group are:

- Reject IE;

- Ignore IE and Notify Sender;

- Ignore IE.

The following rules restrict when a receiving entity may consider an IE, an IE group or an EP not comprehended (not implemented), and when action based on criticality information is applicable:

1. IE or IE group: When one new or modified IE or IE group is implemented for one EP from a standard version, then other new or modified IEs or IE groups specified for that EP in that standard version shall be considered comprehended by the receiving entity (some may still remain unsupported).

2. EP: The comprehension of different EPs within a standard version or between different standard versions is not mandated. Any EP that is not supported may be considered not comprehended, even if another EP from that standard version is comprehended, and action based on criticality shall be applied.

### 4.5.3.3 Presence information

For many IEs/IE groups which are optional according to the ASN.1 transfer syntax, SBc-AP specifies separately if the presence of these IEs/IE groups is optional or mandatory with respect to MME/CBC application.

The presence field of the indicated classes supports three values:

1. Optional;

2. Conditional;

3. Mandatory.

If an IE/IE group is not included in a received message and the presence of the IE/IE group is mandatory or the presence is conditional and the condition is true according to the version of the specification used by the receiver, an abstract syntax error occurs due to a missing IE/IE group.

### 4.5.3.4 Not comprehended IE/IE group

#### 4.5.3.4.1 Procedure code

The receiving node shall treat the different types of received criticality information of the Procedure Code according to the following:

Reject IE:

- If a message is received with a Procedure Code marked with "Reject IE" which the receiving node does not comprehend, the receiving node shall reject the procedure using the Error Indication procedure.

Ignore IE and Notify Sender:

- If a message is received with a Procedure Code marked with "Ignore IE and Notify Sender" which the receiving node does not comprehend, the receiving node shall ignore the procedure and initiate the Error Indication procedure.

Ignore IE:

- If a message is received with a Procedure Code marked with "Ignore IE" which the receiving node does not comprehend, the receiving node shall ignore the procedure.

When using the Error Indication procedure to reject a procedure or to report an ignored procedure it shall include the Procedure Code IE, the Triggering Message IE, and the Procedure Criticality IE in the Criticality Diagnostics IE.

#### 4.5.3.4.2 Type of Message

When the receiving node cannot decode the Type of Message IE, the Error Indication procedure shall be initiated with an appropriate cause value.

#### 4.5.3.4.3 IEs other than the Procedure Code and Type of Message

The receiving node shall treat the different types of received criticality information of an IE/IE group other than the Procedure Code IE and Type of Message IE according to the following:

**Reject IE:**

- If a message initiating a procedure is received containing one or more IEs/IE groups marked with "Reject IE" which the receiving node does not comprehend; none of the functional requests of the message shall be executed. The receiving node shall reject the procedure and report the rejection of one or more IEs/IE groups using the message normally used to report unsuccessful outcome of the procedure. In case the information received in the initiating message was insufficient to determine a value for all IEs that are required to be present in the message used to report the unsuccessful outcome of the procedure, the receiving node shall instead terminate the procedure and initiate the Error Indication procedure.

- If a message initiating a procedure that does not have a message to report unsuccessful outcome is received containing one or more IEs/IE groups marked with "Reject IE" which the receiving node does not comprehend, the receiving node shall terminate the procedure and initiate the Error Indication procedure.

- If a response message is received containing one or more IEs marked with "Reject IE" which the receiving node does no comprehend, the receiving node shall consider the procedure as unsuccessfully terminated and initiate local error handling.

**Ignore IE and Notify Sender:**

- If a message initiating a procedure is received containing one or more Ies/IE groups marked with "Ignore IE and Notify Sender" which the receiving node does not comprehend, the receiving node shall ignore the content of the not comprehended IEs/IE groups, continue with the procedure as if the not comprehended IEs/IE groups were not received (except for the reporting) using the understood IEs/IE groups, and report in the response message of the procedure that one or more IEs/IE groups have been ignored. In case the information received in the initiating message was insufficient to determine a value for all IEs that are required to be present in the response message, the receiving node shall instead terminate the procedure and initiate the Error Indication procedure.

- if a message initiating a procedure that does not have a message to report the outcome of the procedure is received containing one or more IEs/IE groups marked with "Ignore IE and Notify Sender" which the receiving node does not comprehend, the receiving node shall ignore the content of the not comprehended IEs/IE groups, continue with the procedure as if the not comprehended IEs/IE groups were not received (except for the reporting) using the understood IEs/IE groups, and initiate the Error Indication procedure to report that one or more IEs/IE groups have been ignored.

- If a response message is received containing one or more IEs/IE groups marked with "Ignore IE and Notify Sender" which the receiving node does not comprehend, the receiving node shall ignore the content of the not comprehended IE/IE groups, continue with the procedure as if the not comprehended IEs/IE groups were not received (except for the reporting) using the understood IEs/IE groups and initiate the Error Indication procedure.

**Ignore IE:**

- If a message initiating a procedure is received containing one or more IEs/IE groups marked with "Ignore IE" which the receiving node does not comprehend, the receiving node shall ignore the content of the not comprehended IEs/IE groups and continue with the procedure as if the not comprehended IEs/IE groups were not received using only the understood IEs/IE groups.

- If a response message is received containing one or more IEs/IE groups marked with "Ignore IE" which the receiving node does not comprehend, the receiving node shall ignore the content of the not comprehended IEs/IE groups and continue with the procedure as if the not comprehended IEs/IE groups were not received using the understood IEs/IE groups.

When reporting not comprehended IEs/IE groups marked with "Reject IE" or "Ignore IE and Notify Sender" using a response message defined for the procedure, the Information Element Criticality Diagnostics IE shall be included in the Criticality Diagnostics IE for each reported IE/IE group.

When reporting not comprehended IEs/IE groups marked with "Reject IE" or "Ignore IE and Notify Sender" using the Error Indication procedure, the Procedure Code IE, the Triggering Message IE, Procedure Criticality IE, and the Information Element Criticality Diagnostics IE shall be included in the Criticality Diagnostics IE for each reported IE/IE group.

### 4.5.3.5 Missing IE or IE group

The receiving node shall treat the missing IE/IE group according to the criticality information for the missing IE/IE group in the received message specified in the version of the present document used by the receiver:

**Reject IE:**

- if a received message initiating a procedure is missing one or more IEs/IE groups with specified criticality "Reject IE"; none of the functional requests of the message shall be executed. The receiving node shall reject the procedure and report the missing IEs/IE groups using the message normally used to report unsuccessful outcome of the procedure. In case the information received in the initiating message was insufficient to determine a value for all IEs that are required to be present in the message used to report the unsuccessful outcome of the procedure, the receiving node shall instead terminate the procedure and initiate the Error Indication procedure.

- if a received message initiating a procedure that does not have a message to report unsuccessful outcome is missing one or more IEs/IE groups with specified criticality "Reject IE", the receiving node shall terminate the procedure and initiate the Error Indication procedure.

- if a received response message is missing one or more IEs/IE groups with specified criticality "Reject IE, the receiving node shall consider the procedure as unsuccessfully terminated and initiate local error handling.

**Ignore IE and Notify Sender:**

- if a received message initiating a procedure is missing one or more IEs/IE groups with specified criticality "Ignore IE and Notify Sender", the receiving node shall ignore that those IEs are missing and continue with the procedure based on the other IEs/IE groups present in the message and report in the response message of the procedure that one or more IEs/IE groups were missing. In case the information received in the initiating message was insufficient to determine a value for all IEs that are required to be present in the response message, the receiving node shall instead terminate the procedure and initiate the Error Indication procedure.

- if a received message initiating a procedure that does not have a message to report the outcome of the procedure is missing one or more IEs/IE groups with specified criticality "Ignore IE and Notify Sender", the receiving node shall ignore that those IEs are missing and continue with the procedure based on the other IEs/IE groups present in the message and initiate the Error Indication procedure to report that one or more IEs/IE groups were missing.

- if a received response message is missing one or more IEs/IE groups with specified criticality "Ignore IE and Notify Sender", the receiving node shall ignore that those IEs are missing and continue with the procedure based on the other IEs/IE groups present in the message and initiate the Error Indication procedure to report that one or more IEs/IE groups were missing.

**Ignore IE:**

- if a received message initiating a procedure is missing one or more IEs/IE groups with specified criticality "Ignore IE", the receiving node shall ignore that those IEs are missing and continue with the procedure based on the other IEs/IE groups present in the message.

- if a received response message is missing one or more IEs/IE groups with specified criticality "Ignore IE", the receiving node shall ignore that those IEs/IE groups are missing and continue with the procedure based on the other IEs/IE groups present in the message.

When reporting missing IEs/IE groups with specified criticality "Reject IE" or "Ignore IE and Notify Sender" using a response message defined for the procedure, the Information Element Criticality Diagnostics IE shall be included in the Criticality Diagnostics IE for each reported IE/IE group.

When reporting missing IEs/IE groups with specified criticality "Reject IE" or "Ignore IE and Notify Sender" using the Error Indication procedure, the Procedure Code IE, the Triggering Message IE, Procedure Criticality IE, and the Information Element Criticality Diagnostics IE shall be included in the Criticality Diagnostics IE for each reported IE/IE group.

### 4.5.3.6 IEs or IE groups received in wrong order or with too many occurrences or erroneously present

If a message with IEs or IE groups in wrong order or with too many occurrences is received or if IEs or IE groups with a conditional presence are present when the condition is not met (i.e. erroneously present), the receiving node shall behave according to the following:

- If a message initiating a procedure is received containing IEs or IE groups in wrong order or with too many occurrences or erroneously present, none of the functional requests of the message shall be executed. The receiving node shall reject the procedure and report the cause value "Abstract Syntax Error (Falsely Constructed Message)" using the message normally used to report unsuccessful outcome of the procedure. In case the information received in the initiating message was insufficient to determine a value for all IEs that are required to be present in the message used to report the unsuccessful outcome of the procedure, the receiving node shall instead terminate the procedure and initiate the Error Indication procedure.

- If a message initiating a procedure that does not have a message to report unsuccessful outcome is received containing IEs or IE groups in wrong order or with too many occurrences or erroneously present, the receiving node shall terminate the procedure and initiate the Error Indication procedure, and use cause value "Abstract Syntax Error (Falsely Constructed Message)".

- If a response message is received containing IEs or IE groups in wrong order or with too many occurrences or erroneously present, the receiving node shall consider the procedure as unsuccessfully terminated and initiate local error handling.

When determining the correct order only the IEs specified in the specification version used by the receiver shall be considered.

## 4.5.4 Logical Error

Logical error situations occur when a message is comprehended correctly, but the information contained within the message is not valid (i.e. semantic error), or describes a procedure which is not compatible with the state of the receiver. In these conditions, the following behaviour shall be performed (unless otherwise specified) as defined by the class of the elementary procedure, irrespective of the criticality information of the IE's/IE groups containing the erroneous values.

**Class 1:**

Where the logical error occurs in a request message of a class 1 procedure, and the procedure has a message to report this unsuccessful outcome, this message shall be sent with an appropriate cause value. Typical cause values are:

- Semantic Error;

- Message not compatible with receiver state.

Where the logical error is contained in a request message of a class 1 procedure, and the procedure does not have a message to report this unsuccessful outcome, the procedure shall be terminated and the Error Indication procedure shall be initiated with an appropriate cause value. The Procedure Code IE and the Triggering Message IE within the Criticality Diagnostics IE shall then be included in order to identify the message containing the logical error.

Where the logical error exists in a response message of a class 1 procedure, the procedure shall be considered as unsuccessfully terminated and local error handling shall be initiated.

**Class 2:**

Where the logical error occurs in a message of a class 2 procedure, the procedure shall be terminated and the Error Indication procedure shall be initiated with an appropriate cause value. The Procedure Code IE and the Triggering Message IE within the Criticality Diagnostics IE shall then be included in order to identify the message containing the logical error.

## 4.5.5 Exceptions

The error handling for all the cases described hereafter shall take precedence over any other error handling described in the other clauses of clause 4.5.

- If any type of error (Transfer Syntax Error, Abstract Syntax Error or Logical Error) is detected in the ERROR INDICATION message, it shall not trigger the Error Indication procedure in the receiving Node but local error handling.

- In case a response message or Error Indication message needs to be returned, but the information necessary to determine the receiver of that message is missing, the procedure shall be considered as unsuccessfully terminated and local error handling shall be initiated.

- If an error that terminates a procedure occurs, the returned cause value shall reflect the error that caused the termination of the procedure even if one or more abstract syntax errors with criticality "ignore and notify" have earlier occurred within the same procedure.

Annex A (informative):  
Change history:

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Date** | **TSG #** | **TSG Doc.** | **CR** | **Rev** | **Subject/Comment** | **New** |
| 2008-12 | CT#42 | CP-080972 |  |  | V1.0.2 approved in CT#42 | 8.0.0 |
| 2009-03 | CT#43 | CP-090101 | 0001 | 3 | General clean-up to make an alignment with RAN specifications | 8.1.0 |
|  |  | CP-090022 | 0002 | - | General clean-up to make an alignment with RAN specifications |  |
| 2009-09 | CT#45 | CP-090543 | 0003 | 1 | Correct ASN.1 misalignment between S1AP and SB-AP | 8.2.0 |
|  |  |  | 0004 | 1 | Fix the ASN.1 Object Identifiers (OID) descriptions for SBc-AP |  |
|  |  |  | 0005 | 1 | Update port number and payload protocol identifier for SBc-AP |  |
|  |  |  | 0006 | - | Fix incorrect IETF reference |  |
| 2009-12 | CT#46 | CP-090780 | 0008 | 1 | Missing OMC-ID and other corrections | 8.3.0 |
|  |  |  | 0009 | - | Correction of Warning Message Transmission procedure |  |
| 2009-12 | CT#46 | CP-090799 | 0007 | 4 | Enhancements to Warning Notifications to support PWS/CMAS Requirements | 9.0.0 |
| 2010-06 | CT#48 | CP-100288 | 0011 | 2 | Number of Broadcasts | 9.1.0 |
| 2010-09 | CT#49 | CP-100446 | 0013 | - | Correction of the SCTP Payload Protocol value for the SBc-AP | 9.2.0 |
| 2010-12 | CT#50 | CP-100708 | 0014 | 3 | Correct WRITE-REPLACE-WARNING REQUEST misalignment between S1AP and SBc-AP | 9.3.0 |
| 2011-03 | CT#51 | CP-110080 | 0015 | 2 | SBc-AP Error Indication | 10.0.0 |
| 2011-09 | CT#53 | CP-110579 | 0016 | - | Error Indication procedure | 11.0.0 |
| 2011-12 | CT#54 | CP-110797 | 0018 | - | Error Indication | 11.1.0 |
|  |  | CP-110783 | 0020 | - | Extended Repetition Period |  |
| 2012-03 | CT#55 | CP-120021 | 0024 | - | Correction to Assigned Criticality | 11.2.0 |
| 2012-06 | CT#56 | CP-120246 | 0025 | - | Corrections to ASN.1 code | 11.3.0 |
| 2012-09 | CT#57 | CP-120460 | 0026 | - | Correction to ASN1 syntax | 11.4.0 |
|  |  | CP-120460 | 0027 | - | Editorial updates of references |  |
|  |  | CP-120463 | 0031 | - | ETWS Secondary Notification |  |
| 2012-12 | CT#58 | CP-120886 | 0029 | 4 | Report to CBC on Warning Message Delivery | 12.0.0 |
|  |  | CP-120886 | 0030 | 4 | Failure List in WRITE-REPLACE RESPONSE and STOP WARNING RESONSE |  |
| 2013-03 | CT#59 | CP-130031 | 0034 | - | Corrections to ASN.1 encoding | 12.1.0 |
| 2013-06 | CT#60 | CP-130308 | 0036 | - | Editorial Corrections | 12.2.0 |
| 2013-09 | CT#61 | CP-130455 | 0033 | 1 | Report to CBC on Stop Warning Message Delivery | 12.3.0 |
|  |  |  | 0038 | 1 | Stop-all Warning Messages |  |
| 2013-09 |  |  |  |  | The header 4.3.4.3.8 style corrected | 12.3.1 |
| 2013-12 | CT#62 | CP-130622 | 0044 | 2 | eNodeB ID List | 12.4.0 |
|  |  |  | 0045 | 1 | Correction of references to clauses |  |
|  |  |  | 0048 | 1 | Unsuccessful Outcome |  |
| 2014-03 | CT#63 | CP-140154 | 0042 | 7 | PWS Restart Indication | 12.5.0 |
| 2014-06 | CT#64 | CP-140255 | 0050 | 2 | Routing of PWS messages to HeNBs | 12.6.0 |
| 2014-12 | CT#66 | CP-140782 | 0051 | - | Warning Area List in Write-Replace Warning Request during PWS restoration | 12.7.0 |
|  |  |  | 0052 | 1 | Serial Number in Write-Replace Warning Request during PWS restoration |  |
|  |  |  | 0054 | - | Message Type for PWS Restart Indication |  |
| 2015-03 | CT#67 | CP-150029 | 0055 | 1 | Incorrect reference in STOP WARNING REQUEST | 12.8.0 |
| 2015-06 | CT#68 | CP-150262 | 0056 | 1 | Criticality of the Cause IE in Write-Replace Warning Response and Stop Warning Response | 13.0.0 |
| 2015-09 | CT#69 | CP-150438 | 0057 | 1 | Inconsistent Criticality information | 13.1.0 |
| 2015-12 | CT#70 | CP-150741 | 0065 | - | ASN.1 Corrections | 13.2.0 |
|  |  |  | 0058 | 2 | Failure Indication | 13.2.0 |
|  |  |  | 0059 | 3 | Style fixes and resolution of editor's note | 13.2.0 |
| 2017-03 | CT#75 | - | - | - | Update to Rel-14 version (MCC) | 14.0.0 |
| 2017-09 | CT#77 | CP-172012 | 0068 | 1 | Restarted Cell List in PWS RESTART INDICATION | 14.1.0 |
| 2017-12 | CT#78 | CP-1730 | 0069 | - | Introduction of New types of eNB ID | 14.2.0 |
| 2018-06 | CT#80 | CP-181132 | 0070 | 2 | Modifications needed to address 5GS over SBc | 15.0.0 |
| 2018-09 | CT#81 | CP-182077 | 0071 | 1 | New field Warning Area Coordinates in WRITE-REPLACE WARNING REQUEST | 15.1.0 |
| 2020-06 | CT#88e | CP-201065 | 0074 | 1 | Essential Corrections on PWS Procedures for 5GC | 16.0.0 |