3GPP TS 29.415 V16.0.0 (2020-07)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Core Network and Terminals;

Core Network Nb Interface User Plane Protocols

(Release 16)

* *

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.   
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.   
This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

Keywords

UMTS, network, protocol

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

[http://www.3gpp.org](http://www.3gpp.org/)

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword [5](#__RefHeading___Toc469763397)

Introduction [5](#__RefHeading___Toc469763398)

1 Scope [6](#__RefHeading___Toc469763399)

2 References [6](#__RefHeading___Toc469763400)

3 Definitions, symbols and abbreviations [7](#__RefHeading___Toc469763401)

3.1 Definitions [7](#__RefHeading___Toc469763402)

3.2 Symbols [7](#__RefHeading___Toc469763403)

3.3 Abbreviations [7](#__RefHeading___Toc469763404)

4 User Plane [7](#__RefHeading___Toc469763405)

4.1 General aspects [7](#__RefHeading___Toc469763406)

4.2 Operational and Functional Aspects [8](#__RefHeading___Toc469763407)

5 Transparent Mode [8](#__RefHeading___Toc469763408)

6 Support mode for predefined SDU sizes [8](#__RefHeading___Toc469763409)

6.1 General [8](#__RefHeading___Toc469763410)

6.2 Nb UP protocol layer services in Support Mode [8](#__RefHeading___Toc469763411)

6.3 Services expected from the Transport Network Layer [8](#__RefHeading___Toc469763412)

6.4 Functions of the Nb UP protocol layer in Support Mode [9](#__RefHeading___Toc469763413)

6.4.1 Functional model of the Nb UP protocol layer in Support Mode [9](#__RefHeading___Toc469763414)

6.4.2 Frame handler function [9](#__RefHeading___Toc469763415)

6.4.3 Procedure control functions [9](#__RefHeading___Toc469763416)

6.4.4 Non Access Stratum data streams specific functions [9](#__RefHeading___Toc469763417)

6.4.4.1 Frame quality classification [9](#__RefHeading___Toc469763418)

6.4.4.1.1 General [9](#__RefHeading___Toc469763419)

6.4.4.1.2 Handling of FQC information [10](#__RefHeading___Toc469763420)

6.5 Elementary procedures [10](#__RefHeading___Toc469763421)

6.5.1 Transfer of User Data procedure [10](#__RefHeading___Toc469763422)

6.5.1.1 Successful operation [10](#__RefHeading___Toc469763423)

6.5.1.2 Unsuccessful operation [10](#__RefHeading___Toc469763424)

6.5.2 Initialisation procedure [10](#__RefHeading___Toc469763425)

6.5.2.1 Successful operation [10](#__RefHeading___Toc469763426)

6.5.2.2 Unsuccessful operation [11](#__RefHeading___Toc469763427)

6.5.3 Rate Control [11](#__RefHeading___Toc469763428)

6.5.3.1 Successful operation [11](#__RefHeading___Toc469763429)

6.5.3.1.1 Rate control for codecs other than the EVS codec [11](#__RefHeading___Toc469763430)

6.5.3.1.2 Rate and mode control for the EVS codec [11](#__RefHeading___Toc469763431)

6.5.3.1.3 Interworking of rate control between compatible AMR-WB and EVS codec configurations [12](#__RefHeading___Toc469763432)

6.5.3.2 Unsuccessful operation [12](#__RefHeading___Toc469763433)

6.5.4 Time Alignment [13](#__RefHeading___Toc469763434)

6.5.4.1 Successful operation [13](#__RefHeading___Toc469763435)

6.5.4.2 Unsuccessful operation [13](#__RefHeading___Toc469763436)

6.5.5 Handling of Error Event procedure [13](#__RefHeading___Toc469763437)

6.5.5.1 Successful operation [13](#__RefHeading___Toc469763438)

6.5.5.2 Unsuccessful operation [13](#__RefHeading___Toc469763439)

6.6 Elements for Nb UP communication in Support mode [13](#__RefHeading___Toc469763440)

6.7 Handling of unknown, unforeseen and erroneous protocol data [13](#__RefHeading___Toc469763441)

7 Communication Primitives for the Nb UP protocol layer [13](#__RefHeading___Toc469763442)

7.1 Modelling Principle [13](#__RefHeading___Toc469763443)

7.2 Primitives towards the upper layers at the CNL-SAP [13](#__RefHeading___Toc469763444)

7.3 Primitives towards the transport layers at TNL-SAP [13](#__RefHeading___Toc469763445)

7.3.1 General [13](#__RefHeading___Toc469763446)

7.3.2 ATM/AAL2 based Transport Layer [14](#__RefHeading___Toc469763447)

7.3.2.1 General [14](#__RefHeading___Toc469763448)

7.3.2.2 AAL2 Service Primitives used by the Nb UP protocol [14](#__RefHeading___Toc469763449)

7.3.3 GTP-U based Transport Layer [14](#__RefHeading___Toc469763450)

7.3.4 RTP/UDP/IP based Transport Layer [14](#__RefHeading___Toc469763451)

8 Evolution of Nb UP Protocol [14](#__RefHeading___Toc469763452)

Annex A (informative): Change history [15](#__RefHeading___Toc469763453)

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# Introduction

The present document specifies the user plane protocol used between two Media Gateways in the CS core network. Through out the present document this protocol shall be referred to as the Nb UP protocol. The Nb UP protocol is for a large part identical to the Iu UP protocol (see 3GPP TS 25.415 [2]), and only the differences between the two protocols are specified. This specification defines the applicability of the UP, as defined in 3GPP TS 25.415 [2], for the Nb interface only.

Given that the Nb UP uses the same PDU types as the Iu UP, the term IuFP is used to refer to the common framing.

For the purpose of the present document, any occurrence of the term "Iu UP" in the corresponding sections of 3GPP TS 25.415 [2], shall be interpreted as "Nb UP".

# 1 Scope

The present document specifies the user plane protocol of the bearer used between two MGWs within the BICC-based CS core network, called the Nb UP protocol. The present document assumes the implementation of the split between call control and the bearer transport and control, as specified in 3GPP TS 23.205 [1], see figure 1. Note that the present document does not preclude an implementation of a combined MSC Server and MGW.



Figure 1: CS core network logical architecture

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TS 23.205: "Bearer Independent CS Core Network; Stage 2"

[2] 3GPP TS 25.415: "UTRAN Iu Interface User Plane Protocols"

[3] 3GPP TS 29.232: "Media Gateway Controller; Media Gateway interface; Stage 3"

[4] 3GPP TS 29.414: "Core Network Nb Data Transport and Transport Signalling"

[5] 3GPP TR 41.001: "GSM Release specifications"

[6] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications"

[7] IETF RFC 1889: "RTP A Transport Protocol for Real Time Applications"

[8] ITU-T I.366.1 (06/98): "Segmentation and Reassembly Service Specific Convergence Sublayer for the AAL type 2"

[9] 3GPP TS 26.445:"Codec for Enhanced Voice Services (EVS); Detailed Algorithmic Description".

[10] 3GPP TS 26.453: "Codec for Enhanced Voice Services (EVS); Speech codec frame structure".

[11] 3GPP TS 26.454: "Codec for Enhanced Voice Services (EVS); Interface to Iu, Uu, Nb and Mb".

# 3 Definitions, symbols and abbreviations

## 3.1 Definitions

Definitions used in the present document are listed in 3GPP TR 21.905 [6].

## 3.2 Symbols

For the purposes of the present document, the following symbols apply:

Iu Interface between the RNS and the core network. It is also considered as a reference point.

Nb Interface between media gateways.

IuFP Iu Framing protocol

## 3.3 Abbreviations

For the purposes of the present document, the following abbreviations apply:

AAL ATM Adaptation Layer

AAL2 AAL Type 2

ATM Asynchronous Transfer Mode

CMR Codec Mode Request

CN Core Network

CNL Core Network Layer

CS Circuit Switched

EVS Enhanced Voice Services

EVS-CMR Codec Mode Request for EVS

FFS For Further Study

IPTI Inter PDU Transmission Interval

Iu UP Iu interface User Plane

MGW Media GateWay

PDU Protocol Data Unit

RTP Real-time Transmission Protocol

SAP Service Access Point

SDU Service Data Unit

SRNC Serving Radio Network Controller

# 4 User Plane

## 4.1 General aspects

The Nb UP is located in the user plane of the CS core network over the Nb interface. It is used to convey data between MGWs.

The Nb UP protocol shall be initiated at one MGW and acknowledged by the adjoining MGW.

The Nb UP framing is identical to the Iu UP framing, i.e., the same PDU types are valid for both protocols.

Figure 2 shows the logical location of the Nb UP protocol layer in relation to the Nb interface.



Figure 2: Nb UP protocol layer occurrence in overall architecture.

## 4.2 Operational and Functional Aspects

There are two modes of operation for the Nb UP:

- Transparent mode;

- Support mode for predefined SDU size.

The two modes of operation follow the definition of the corresponding Iu UP modes of operation, as described in 3GPP TS 25.415 [2].

Support mode version 2 is mandatory on the NbUP interface. Support mode version 1 is not required at the Nb but may be used if both MGWs support it, as a result of the version negotiation during the Initialisation procedure.

# 5 Transparent Mode

This mode of operation is identical to that of the Iu UP protocol, see the corresponding section in 3GPP TS 25.415 [2].

# 6 Support mode for predefined SDU sizes

## 6.1 General

See the corresponding section in 3GPP TS 25.415 [2].

## 6.2 Nb UP protocol layer services in Support Mode

See the corresponding section in 3GPP TS 25.415 [2].

## 6.3 Services expected from the Transport Network Layer

See the corresponding section in 3GPP TS 25.415 [2].

## 6.4 Functions of the Nb UP protocol layer in Support Mode

### 6.4.1 Functional model of the Nb UP protocol layer in Support Mode

See the corresponding section in 3GPP TS 25.415 [2].

### 6.4.2 Frame handler function

See the corresponding section in 3GPP TS 25.415 [2].

### 6.4.3 Procedure control functions

See the corresponding section in 3GPP TS 25.415 [2].

### 6.4.4 Non Access Stratum data streams specific functions

See the corresponding section in 3GPP TS 25.415 [2].

#### 6.4.4.1 Frame quality classification

##### 6.4.4.1.1 General

On the Nb UP in Support Mode the frames are classified with the Frame Quality Classifier (FQC). This classifying is based on frame classification on the preceding link and the setting of the attribute "Delivery of erroneous SDUs". The MSC server shall indicate the value of the attribute "Delivery of erroneous SDUs" see 3GPP TS 29.232 [3].

Figure 4 shows the main input and output information for the frame quality classification function on the Nb UP.



Figure 4: Frame quality classification in Nb UP

##### 6.4.4.1.2 Handling of FQC information

The handling of FQC shall be as specified in Table 1.

Table 1. FQC handling in Nb UP protocol, receiving side

|  |  |  |  |
| --- | --- | --- | --- |
| Input | | | Action |
| Delivery of erroneous SDUs | FQC in received PDU | Payload CRC |
| 'yes' or 'no' | 'good' | OK | Leave FQC unchanged. Forward SDU and FQC to upper layer |
| 'yes' | 'bad radio' | OK | Leave FQC unchanged. Forward SDU and FQC to upper layer |
| 'yes' | 'good' or 'bad radio' | Not OK | Set FQC to 'bad'. Forward SDU and FQC to upper layer |
| 'yes' | 'bad' | Any | Leave FQC unchanged. Forward SDU and FQC to upper layer |
| 'no' | 'good' | Not OK | Drop SDU |
| 'no' | 'bad' or 'bad radio' | Any | Not applicable. SDUs are dropped at a previous link. |
| 'no-error-detection-consideration' | Any | Any | Leave FQC unchanged. Forward SDU and FQC to upper layer |

The FQC handling in the Nb UP protocol entity on the sending side is as follows:

- When the upper layer indicates an FQC value in the Nb-UP-DATA-Request message, an FQC shall be set in the PDU as indicated by the upper layer. If the upper layer does not indicate an FQC value, the FQC in the PDU shall be set to 'good'.

- When the upper layer indicates an FQC with the value 'bad' to the Nb UP protocol layer, the Nb UP support functions may generate an erroneous payload CRC.

An MGW may ignore the settings of the "delivery of erroneous SDUs" property of the 3GUP package if the MGW passes frames transparently through the UP entities as described in 3GPP TS 29.232 [3].

## 6.5 Elementary procedures

### 6.5.1 Transfer of User Data procedure

#### 6.5.1.1 Successful operation

See the corresponding section in 3GPP TS 25.415 [2]. For the purpose of the present document, the MGW replaces the function of the SRNC and the CN, and the Nb replaces the function of the Iu.

When the MGW provides the Frame Number IE it shall be based on time according to the handling on Iu (see 3GPP TS 25.415 [2]) for conversational and streaming traffic class.

NOTE: The IuUP Frame Number IE is based on time also and therefore no interworking of this IE is required.

#### 6.5.1.2 Unsuccessful operation

See the corresponding section in 3GPP TS 25.415 [2]. For the purpose of the present document, the MGW replaces the function of the SRNC and the CN, and the Nb replaces the function of the Iu.

### 6.5.2 Initialisation procedure

#### 6.5.2.1 Successful operation

See the corresponding section in 3GPP TS 25.415 [2].

For the EVS codec, Equal Error Protection (EEP) is applied on the radio interface. Only class A bits are defined. Class B and Class C bits are not present. Consequently each RAB sub-flow Combination Indication (RFCI) corresponds to one bit rate of the selected EVS Configuration, as described in 3GPP TS 26.454 [11] subclause 5.

When an Nb UP layer protocol entity receives an initialisation status request from the upper layer, it shall start the initialisation procedure. See 3GPP TS 29.232 [3], concerning the overall initialisation process. When an Nb UP layer protocol entity receives an initialisation message it shall acknowledge this message and indicate to the upper layer that an initialisation message has been received. When an Nb UP layer protocol entity receives a positive initialisation acknowledgement it shall indicate to the upper layer that a positive initialisation acknowledgement has been received.

#### 6.5.2.2 Unsuccessful operation

See the corresponding section in 3GPP TS 25.415 [2]. A negative acknowledgement triggers a repetition of the initialisation message. After N INIT unsuccessful repetitions, the initialisation procedure is terminated.

### 6.5.3 Rate Control

#### 6.5.3.1 Successful operation

##### 6.5.3.1.1 Rate control for codecs other than the EVS codec

See the corresponding section in 3GPP TS 25.415 [2]. When an Nb UP protocol entity receives a rate control message over the Nb interface, it shall provide an indication of the rate control to the upper layer. The rate control indication is acknowledged on request from the upper layer.

##### 6.5.3.1.2 Rate and mode control for the EVS codec

For the EVS codec:

- On the Iu interface, IuFP provides for rate control via the exchange of RATE CONTROL and RATE CONTROL ACK PDUs.

- On the Iu interface, CMR for EVS (EVS-CMR) as specified in 3GPP TS 26.453 [10] subclause 4.5 provides for in-band rate and mode control via the Codec Mode Request (CMR) field of every codec frame (Speech or SID) and CMR-Only frame.

- On the Nb interface of the BICC-based CS CN, EVS-CMR as specified in 3GPP TS 26.453 [10] subclause 4.5 provides for in-band rate and mode control via the Codec Mode Request (CMR) field of every codec frame.

- A MGW receiving an EVS-CMR over an Nb interface may modify its contents based on local policies and include the resulting contents into the EVS-CMR field of the outgoing speech frame on the Nb interface.

- Interworking of rate control procedures at an MGW between an Nb interface and a corresponding Iu interface only applies when the MGW bridges compatible codec configurations between the interfaces without applying a transcoding function.

- A MGW receiving an EVS-CMR from an Nb interface may modify its contents based on local policies and include the resulting contents into the EVS-CMR field of the outgoing speech frame on the corresponding Iu interface.

- An MGW receiving a rate control request and an EVS-CMR on an Iu interface shall determine the lower limit of the maximum bit rates contained in each request and include the resulting limit into the EVS-CMR field of the outgoing speech frame on the corresponding Nb interface, with possible further modifications to the EVS-CMR contents based on configured policies.

- The rules by which the MGW may filter and modify the EVS-CMR contents consist of the following:

1) The MGW shall not modify the EVS-CMR to increase the maximum bit rate;

2) If the MGW observes the incoming stream of speech frames or packets and determines that a lower EVS mode is more appropriate, the MGW may modify the EVS-CMRs sent in the opposite direction of the observed speech flow;

3) If the MGW modifies the EVS-CMR to decrease the maximum bit rate and the resulting maximum bit rate no longer support the originally requested maximum audio bandwidth, then the maximum audio bandwidth may be reduced by the MGW to the next lower one that fits to the reduced maximum bit rate;

4) The MGW shall not modify the EVS-CMR in a way that results in a change of the major operation mode (EVS primary mode or EVS AMR-WB IO mode);

NOTE: The MGW can be forced to change the major operation mode of an incoming EVS-CMR when interworking between EVS and AMR-WB, during handover or after handover.

5) When channel-aware mode is used, if the MGW observes the incoming stream of speech frames or packets and determines that other channel-aware mode parameters are more appropriate, the MGW may modify the EVS-CMRs, flowing in the opposite direction of the observed speech flow to change the received channel-aware offset to a bigger one (e.g. from 2 to 3) and the received channel-aware depth to a lower, more robust one;

6) When channel-aware mode is used, the MGW shall not reduce the received channel-aware offset or modify the received channel-aware depth a less robust one;

7) The MGW should not block the channel-aware mode;

8) The MGW may modify the EVS primary mode in the received EVS-CMR to the EVS Variable Bit Rate mode.

##### 6.5.3.1.3 Interworking of rate control between compatible AMR-WB and EVS codec configurations

The EVS codec includes the EVS AMR-WB IO major operation mode and is therefore TrFO-compatible to the AMR-WB codec, if the configurations are TrFO-compatible. For example, AMR-WB on one MGW termination and EVS on the other MGW termination are TrFO-compatible codecs, if the configurations are TrFO-compatible.

If the MGW bridges compatible EVS codec configurations and AMR-WB codec configurations:

- If the codec of the incoming termination is EVS and the codec of the outgoing termination is AMR-WB, then the rate control procedure for AMR-WB shall apply at the outgoing termination, with the maximum rate equal to or lower than the maximum rate received in the EVS-CMR. The MGW shall map received EVS-CMRs to the selected configuration of the outgoing AMR-WB termination.

- If the codec of the incoming termination is AMR-WB and the codec of the outgoing termination is EVS, then the rate control procedure for AMR-WB shall apply on the incoming termination and shall determine the maximum rate included in the EVS-CMR sent by the MGW. The MWG shall request the EVS AMR-WB IO major operation mode in the outgoing EVS-CMR.

- The MGW may filter and modify the CMR contents according to the following rules:

1) The MGW shall not modify the EVS-CMR to increase the maximum bit rate;

2) If the MGW observes the incoming stream of speech frames or packets and determines that a lower EVS mode is more appropriate, the MGW may modify the EVS-CMRs sent in the opposite direction of the observed speech flow.

If the MGW bridges EVS codec configurations and AMR-WB codec configurations which are not compatible, the MGW shall apply transcoding and shall handle the independent rate and mode control procedures towards the incoming and the outgoing networks.

#### 6.5.3.2 Unsuccessful operation

For codecs other than the EVS codec, see the corresponding section in 3GPP TS 25.415 [2]. Depending on the error cause, a negative acknowledgement is either reported in a status indication to the upper layer, or it triggers a repetition of the control command. After N RC unsuccessful repetitions, the rate control procedure is terminated.

### 6.5.4 Time Alignment

#### 6.5.4.1 Successful operation

See the corresponding section in 3GPP TS 25.415 [2]. When an Nb UP protocol entity receives a time alignment command over the Nb interface, it shall indicate the time alignment to the upper layer. The time alignment is acknowledged on request from the upper layer.

#### 6.5.4.2 Unsuccessful operation

See the corresponding section in 3GPP TS 25.415 [2]. Depending on the error cause, a negative acknowledgement is either reported in a status indication to the upper layer, or it triggers a repetition of the control command. After N TA unsuccessful repetitions, the time alignment procedure is terminated.

### 6.5.5 Handling of Error Event procedure

#### 6.5.5.1 Successful operation

See the corresponding section in 3GPP TS 25.415 [2].

#### 6.5.5.2 Unsuccessful operation

See the corresponding section in 3GPP TS 25.415 [2].

## 6.6 Elements for Nb UP communication in Support mode

See the corresponding section in 3GPP TS 25.415 [2].

## 6.7 Handling of unknown, unforeseen and erroneous protocol data

See the corresponding section in 3GPP TS 25.415 [2].

# 7 Communication Primitives for the Nb UP protocol layer

## 7.1 Modelling Principle

See the corresponding section in 3GPP TS 25.415 [2].

## 7.2 Primitives towards the upper layers at the CNL-SAP

See the corresponding section in 3GPP TS 25.415 [2].

## 7.3 Primitives towards the transport layers at TNL-SAP

### 7.3.1 General

Access to the Transport network Layer is performed through a generic SAP: TNL-SAP.

When the Transport Network upper layer consists of AAL2, the TNL SAP maps to the AAL-SAP which allows communication to be performed using specific AAL primitives.

When the Transport Network upper layer consists of RTP/UDP/IP, the TNL-SAP maps to the services provided by IETF RFC 1889 [7].

The choice of communication, specific or generic, through the TNL-SAP is fixed by the Core Network Layer control plane logic. This choice of communication is based on the requirements placed by, e.g. the RAB characteristics, the core network domain requesting the RAB establishment or other operator's choice.

### 7.3.2 ATM/AAL2 based Transport Layer

#### 7.3.2.1 General

When the Nb UP protocol layer uses the services of an ATM/AAL2 transport, it shall use an established AAL2 connection for transferring frames between the peer TNL-SAPs at both ends of the Nb User plane access points. The Transport Network Control Plane over the Nb interface handles the signalling to establish and release the AAL2 call connections.

#### 7.3.2.2 AAL2 Service Primitives used by the Nb UP protocol

AAL2 services and primitives used at the Service Access Point from the AAL2 layer are shown in table 3.

Table 4: AAL2 primitives and parameters

|  |  |  |  |
| --- | --- | --- | --- |
| Primitive | Type | Parameters | Comments |
| SSSAR-UNITDATA | Request | SSSAR-INFO |  |
| SSSAR-UUI | Not used (note) |
| SSSAR-UNITDATA | Indication | SSSAR-INFO |  |
| SSSAR-UUI | Not used (note) |
| NOTE: The setting of this field is set to not used i.e. decimal value 26 according to ITU-T Q.366.1 [8]. | | | |

These primitives are to be used in the Nb UP.

The Transport Network control plane is as specified in 3GPP TS 29.414 [4].

### 7.3.3 GTP-U based Transport Layer

Not applicable.

### 7.3.4 RTP/UDP/IP based Transport Layer

When the Nb UP protocol layer uses the services of an RTP-based transport, it shall use a dynamic payload type that was negotiated for the connection for transferring Nb UP frames between the two endpoints at both ends of the Nb User plane access points. This dynamic payload type is negotiated using the specified bearer control protocol, 3GPP TS 29.414 [4].

# 8 Evolution of Nb UP Protocol

See the corresponding section in 3GPP TS 25.415 [2].

Annex A (informative):  
Change history

| **Change history** | | | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Date** | **TSG #** | **TSG Doc.** | **CR** | | **Rev** | | **Subject/Comment** | | | **Old** | **New** |
| 03-2001 | TSG#11 | NP-010037 |  | |  | | Approved as Version 4.0.0 to be placed under Change Control | | | 2.0.0 | 4.0.0 |
| 09-2001 | TSG#13 | NP-010438 | 001 | | 1 | | Clarification on FQC handling and alignment with TS 25.415 | | | 4.0.0 | 4.1.0 |
| 12-2001 | TSG#14 | NP-010573 | 002 | | 1 | | Correction to Scope clause | | | 4.1.0 | 4.2.0 |
| 12-2001 | TSG#14 | NP-010573 | 004 | | 1 | | Reference to Iu UP | | | 4.1.0 | 4.2.0 |
| 03-2002 | TSG#15 | NP-020085 | 005 | |  | | Add GERAN Iu mode to scope | | | 4.1.0 | 5.0.0 |
| 03-2003 | TSG#19 | NP-030076 | 007 | | 1 | | No backward compatibility to Nb UP FP support mode version 1 required | | | 5.0.0 | 5.1.0 |
| 12-2004 | CN#26 |  |  | |  | | Upgraded to v6.0.0 | | | 5.1.0 | 6.0.0 |
| 01-2005 |  |  |  | |  | | Correct typo in version number on cover | | | 6.0.0 | 6.0.1 |
| 12-2006 | TSG#34 | CP-060619 | 012 | | 2 | | Time based Nb frame number | | | 6.0.1 | 6.1.0 |
| 06-2007 | TSG#36 |  |  | |  | | Upgraded to v7.0.0 | | | 6.1.0 | 7.0.0 |
| 05-2008 | TSG#40 | CP-080310 | 013 | | 2 | | NbFP not used for SIP-I based CS CN | | | 7.0.0 | 8.0.0 |
| 12-2009 | TSG#46 |  |  | |  | | Automatic upgrade from previous Release | | | 8.0.0 | 9.0.0 |
| 09-2010 | TSG#49 | CP-100555 | 016 | |  | | Correcting unspecific external reference | | | 9.0.0 | 9.1.0 |
| 03-2011 | TSG#51 |  |  | |  | | Automatic upgrade from previous Release version 9.1.0 | | | 9.1.0 | 10.0.0 |
| 03-2011 | TSG#51 |  |  | |  | | Correction of heading and numbering made by MCC | | | 10.0.0 | 10.0.1 |
| 09-2012 | TSG#57 |  |  | |  | | Automatic upgrade from previous Release version 10.0.1 | | | 10.0.1 | 11.0.0 |
| 2014-10 |  |  |  | |  | | Automatic upgrade from previous Release | | | 11.0.0 | 12.0.0 |
| 2015-12 | TSG#70 | CP-150648 | 0017 | | 3 | | Update of TS 29.415 to support EVS over UMTS CS | | | 12.0.0 | 13.0.0 |
| **Change history** | | | | | | | | | | | |
| **Date** | **TSG #** | **TSG Doc.** | | **CR** | | **Rev** | | **Cat** | **Subject/Comment** | | **New** |
| 2016-03 | CT#71 | CP-160112 | | 0018 | | 1 | | B | Resolution of Editor's notes on EVS over UMTS CS | | 13.1.0 |
| 2016-12 | CT#74 | CP-160617 | | 0019 | | 1 | | F | Updates to EVS over CS aspects | | 13.2.0 |
| 2017-03 | CT#75 |  | |  | |  | |  | Automatic upgrade from previous Release | | 14.0.0 |
| 2018-06 | SA#80 | - | | - | | - | | - | Automatic upgrade from previous Release | | 15.0.0 |
| 2020-07 | SA#88e | - | | - | | - | |  | Update to Rel-16 version (MCC) | | 16.0.0 |