|  |  |
| --- | --- |
| 3GPP TS 29.544 V16.3.0 (2020-12) | |
| Technical Specification | |
| 3rd Generation Partnership Project;  Technical Specification Group Core Network and Terminals;  5G System; Secured Packet Application Function (SP-AF) Services;  Stage 3  (Release 16) | |
|  | |
| *5G-logo_175px* | 3GPP-logo_web |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  http://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 5

1 Scope 7

2 References 7

3 Definitions, symbols and abbreviations 8

3.1 Terms 8

3.2 Symbols 8

3.3 Abbreviations 8

4 Overview 8

4.1 Introduction 8

5 Services offered by the SP-AF 9

5.1 Introduction 9

5.2 Nspaf\_SecuredPacket Service 9

5.2.1 Service Description 9

5.2.2 Service Operations 9

5.2.2.1 Introduction 9

5.2.2.2 Provide 9

5.2.2.2.1 General 9

5.2.2.2.2 Secured Packet Retrieval 9

6 API Definitions 10

6.1 Nspaf\_SecuredPacket Service API 10

6.1.1 Introduction 10

6.1.2 Usage of HTTP 10

6.1.2.1 General 10

6.1.2.2 HTTP standard headers 11

6.1.2.2.1 General 11

6.1.2.2.2 Content type 11

6.1.2.3 HTTP custom headers 11

6.1.3 Resources 11

6.1.3.1 Overview 11

6.1.3.2 Resource: SecuredPacket 12

6.1.3.2.1 Description 12

6.1.3.2.2 Resource Definition 12

6.1.3.2.3 Resource Standard Methods 12

6.1.3.2.4 Resource Custom Operations 12

6.1.3.2.4.1 Overview 12

6.1.3.2.4.2 Operation: provide-secured-packet 12

6.1.3.2.4.2.1 Description 12

6.1.3.2.4.2.2 Operation Definition 12

6.1.4 Custom Operations without associated resources 13

6.1.5 Notifications 13

6.1.6 Data Model 13

6.1.6.1 General 13

6.1.6.2 Structured data types 13

6.1.6.2.1 Introduction 13

6.1.6.2.2 Type: UiccConfigurationParameter 14

6.1.6.3 Simple data types and enumerations 14

6.1.6.3.1 Introduction 14

6.1.6.3.2 Simple data types 14

6.1.7 Error Handling 14

6.1.7.1 General 14

6.1.7.2 Protocol Errors 14

6.1.7.3 Application Errors 14

6.1.8 Feature negotiation 14

6.1.9 Security 15

Annex A (normative): OpenAPI specification 16

A.1 General 16

A.2 Nspaf\_SecuredPacket API 16

Annex B (informative): Change history 18

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

In the present document, modal verbs have the following meanings:

**shall** indicates a mandatory requirement to do something

**shall not** indicates an interdiction (prohibition) to do something

The constructions "shall" and "shall not" are confined to the context of normative provisions, and do not appear in Technical Reports.

The constructions "must" and "must not" are not used as substitutes for "shall" and "shall not". Their use is avoided insofar as possible, and they are not used in a normative context except in a direct citation from an external, referenced, non-3GPP document, or so as to maintain continuity of style when extending or modifying the provisions of such a referenced document.

**should** indicates a recommendation to do something

**should not** indicates a recommendation not to do something

**may** indicates permission to do something

**need not** indicates permission not to do something

The construction "may not" is ambiguous and is not used in normative elements. The unambiguous constructions "might not" or "shall not" are used instead, depending upon the meaning intended.

**can** indicates that something is possible

**cannot** indicates that something is impossible

The constructions "can" and "cannot" are not substitutes for "may" and "need not".

**will** indicates that something is certain or expected to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**will not** indicates that something is certain or expected not to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**might** indicates a likelihood that something will happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

**might not** indicates a likelihood that something will not happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

In addition:

**is** (or any other verb in the indicative mood) indicates a statement of fact

**is not** (or any other negative verb in the indicative mood) indicates a statement of fact

The constructions "is" and "is not" do not indicate requirements.

# 1 Scope

The present document specifies the stage 3 protocol and data model for the Nspaf Service Based Interface. It provides stage 3 protocol definitions and message flows, and specifies the API for each service offered by the SP-AF.

The 5G System stage 2 architecture and procedures are specified in 3GPP TS 23.501 [2] and 3GPP TS 23.502 [3].

The Technical Realization of the Service Based Architecture and the Principles and Guidelines for Services Definition are specified in 3GPP TS 29.500 [4] and 3GPP TS 29.501 [5].

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 23.501: "System Architecture for the 5G System; Stage 2".

[3] 3GPP TS 23.502: "Procedures for the 5G System; Stage 2".

[4] 3GPP TS 29.500: "5G System; Technical Realization of Service Based Architecture; Stage 3".

[5] 3GPP TS 29.501: "5G System; Principles and Guidelines for Services Definition; Stage 3".

[6] OpenAPI: "OpenAPI 3.0.0 Specification", <https://github.com/OAI/OpenAPI-Specification/blob/master/versions/3.0.0.md>.

[7] 3GPP TR 21.900: "Technical Specification Group working methods".

[8] 3GPP TS 33.501: "Security architecture and procedures for 5G system".

[9] IETF RFC 6749: "The OAuth 2.0 Authorization Framework".

[10] 3GPP TS 29.510: "5G System; Network Function Repository Services; Stage 3".

[11] IETF RFC 7540: "Hypertext Transfer Protocol Version 2 (HTTP/2)".

[12] IETF RFC 8259: "The JavaScript Object Notation (JSON) Data Interchange Format".

[13] IETF RFC 7807: "Problem Details for HTTP APIs".

[14] 3GPP TS 29.503: "Unified Data Management Services"; Stage 3.

[15] 3GPP TS 29.571: "5G System; Common Data Types for Service Based Interfaces Stage 3".

[16] 3GPP TS 31.115: "Secured packet structure for (Universal) Subscriber Identity Module (U)SIM Toolkit applications".

[17] 3GPP TS 29.509: "Authentication Server Services; Stage 3".

[18] 3GPP TS 23.040: "Technical realization of the Short Message Service (SMS)"

# 3 Definitions, symbols and abbreviations

## 3.1 Terms

Void.

## 3.2 Symbols

Void.

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

OTA Over The Air

SOR-AF Steering Of Roaming Application Function

SP-AF Secured Packet Application Function

UDM Unified Data Management

# 4 Overview

## 4.1 Introduction

Within the 5GC, the SP-AF offers services to the UDM and to the SOR-AF via the Nspaf service based interface.

The UDM or SOR-AF shall make use of the SP-AF services when it needs to protect UE parameters for which the final consumer is the USIM (see 3GPP TS 33.501 [8] clause 6.15.2.1).

Figure 4.1-1 provides the reference model with focus on the SP-AF.

NOTE: The generation of the secured packet and the definition of the storage and handling of OTA keys or other sensitive data are out of scope of this document. For more details, refer to 3GPP TS 23.040 [18] and 3GPP TS 31.115 [16].



Figure 4.1-1: Reference model – SP-AF

# 5 Services offered by the SP-AF

## 5.1 Introduction

The SP-AF offers the following services via the Nspaf interface:

- Nspaf\_SecuredPacket Service

Table 5.1-1 summarizes the corresponding APIs defined for this specification.

Table 5.1-1: API Descriptions

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Service Name** | **Clause** | **Description** | **OpenAPI Specification File** | **apiName** | **Annex** |
| Nspaf\_SecuredPacket | 6.1 | Nspaf Secured Packet Service | TS29544\_Nspaf\_SecuredPacket.yaml | nspaf-secured-packet | A.2 |

## 5.2 Nspaf\_SecuredPacket Service

### 5.2.1 Service Description

The Nspaf\_SecuredPacket Service may be consumed by the NF consumer (e.g. UDM or SOR-AF) when it has detected that a UICC configuration parameter (e.g. Routing ID data or Steering of Roaming information) needs to be updated, and the new value is not available in secured packet format.

For the list of service operations see clause 5.2.2.1

### 5.2.2 Service Operations

#### 5.2.2.1 Introduction

For the Nspaf\_SecuredPacket service the following service operations are defined:

- Provide

The Nspaf\_SecuredPacket Service is used by Consumer NFs (e.g. UDM or SOR-AF) to request the SP-AF to provide a secured packet that contains an UICC configuration parameter as sent in the request by means of the Provide service operation

#### 5.2.2.2 Provide

##### 5.2.2.2.1 General

This service operation is used by the NF Service Consumer (e.g. UDM or SOR-AF) to request construction of a secured packet that contains the provided UICC configuration information (e.g. Routing Indicator or Steering of Roaming information).

The following procedures using the Provide service operation are supported:

- Secured Packet Retrieval

##### 5.2.2.2.2 Secured Packet Retrieval

Figure 5.2.2.2.2-1 shows a scenario where the NF consumer (e.g. UDM or SOR-AF) sends a request to the SP-AF to provide a secured packet.

The request contains the UE's identity (/{supi}) and the UICC configuration parameter.



Figure 5.2.2.2.2-1: NF consumer requests the SP-AF to provide a secured packet

1. The NF consumer sends a POST request (custom method: provide-secured-packet) to the resource representing the SUPI.

2a. On success, the SP-AF responds with "200 OK", containing the requested SecuredPacket.

2b. If the resource does not exist (the supi is unknown in the SP-AF), the SP-AF returns the HTTP status code "404 Not Found", and additional error information should be included in the response body (in "ProblemDetails" element).

On failure, the appropriate HTTP status code indicating the error shall be returned and appropriate additional error information should be returned in the POST response body.

# 6 API Definitions

## 6.1 Nspaf\_SecuredPacket Service API

### 6.1.1 Introduction

The Nspaf\_SecuredPacket service shall use the Nspaf\_SecuredPacket API.

The request URI used in HTTP request from the NF service consumer towards the NF service producer shall have the structure defined in clause 4.4.1 of 3GPP TS 29.501 [5], i.e.:

**{apiRoot}/<apiName>/<apiVersion>/<apiSpecificResourceUriPart>**

with the following components:

- The {apiRoot} shall be set as described in 3GPP TS 29.501 [5].

- The <apiName>shall be "nspaf-secured-packet".

- The <apiVersion> shall be "v1".

- The <apiSpecificResourceUriPart> shall be set as described in clause 6.1.3.

### 6.1.2 Usage of HTTP

#### 6.1.2.1 General

HTTP/2, IETF RFC 7540 [11], shall be used as specified in clause 5 of 3GPP TS 29.500 [4].

HTTP/2 shall be transported as specified in clause 5.3 of 3GPP TS 29.500 [4].

The OpenAPI [6] specification of HTTP messages and content bodies for the Nspaf\_SecuredPacket API is contained in Annex A.

#### 6.1.2.2 HTTP standard headers

##### 6.1.2.2.1 General

See clause 5.2.2 of 3GPP TS 29.500 [4] for the usage of HTTP standard headers.

##### 6.1.2.2.2 Content type

JSON, IETF RFC 8259 [12], shall be used as content type of the HTTP bodies specified in the present specification as specified in clause 5.4 of 3GPP TS 29.500 [4]. The use of the JSON format shall be signalled by the content type "application/json".

"Problem Details" JSON object shall be used to indicate additional details of the error in a HTTP response body and shall be signalled by the content type "application/problem+json", as defined in IETF RFC 7807 [13].

#### 6.1.2.3 HTTP custom headers

The mandatory HTTP custom header fields specified in clause 5.2.3.2 of 3GPP TS 29.500 [4] shall be applicable.

### 6.1.3 Resources

#### 6.1.3.1 Overview



Figure 6.1.3.1-1: Resource URI structure of the nspaf-secured-packet API

Table 6.1.3.1-1 provides an overview of the resources and applicable HTTP methods.

Table 6.1.3.1-1: Resources and methods overview

|  |  |  |  |
| --- | --- | --- | --- |
| Resource name | Resource URI | HTTP method or custom operation | Description |
| SecuredPacket (Custom operation) | /{supi}/provide-secured-packet | Provide-secured-packet (POST) | The SP-AF generates a secured packet containing the presented UICC configuration parameter |

#### 6.1.3.2 Resource: SecuredPacket

##### 6.1.3.2.1 Description

This resource represents the information that is needed to construct secured packets for the SUPI.

##### 6.1.3.2.2 Resource Definition

Resource URI: **{apiRoot}/nspaf-secured-packet/v1/{supi}/provide-secured-packet**

This resource shall support the resource URI variables defined in table 6.1.3.2.2-1.

Table 6.1.3.2.2-1: Resource URI variables for this resource

|  |  |
| --- | --- |
| Name | Definition |
| apiRoot | See clause 6.1.1 |
| supi | Represents the Subscription Permanent Identifier (see 3GPP TS 23.501 [2] clause 5.9.2)  pattern: "^(imsi-[0-9]{5,15}|nai-.+|.+)$" |

##### 6.1.3.2.3 Resource Standard Methods

No Standard Methods are supported for this resource.

##### 6.1.3.2.4 Resource Custom Operations

###### 6.1.3.2.4.1 Overview

Table 6.1.3.2.4.1-1: Custom operations

|  |  |  |
| --- | --- | --- |
| Custom operaration URI | Mapped HTTP method | Description |
| /provide-secured-packet | POST | The SP-AF generates a secured packet for the SUPI that contains the presented UICC configuration parameter. |

###### 6.1.3.2.4.2 Operation: provide-secured-packet

6.1.3.2.4.2.1 Description

This custom operation is used by the NF service consumer (e.g. UDM) to request a secured packet for the SUPI containing the presented UICC configuration parameter. The returned secured packet shall be constructed as an SMS-Deliver as specified in 3GPP TS 23.040 [18] and protected as specified in 3GPP TS 31.115 [16].

6.1.3.2.4.2.2 Operation Definition

This operation shall support the request data structures specified in table 6.1.3.2.4.2.2-1 and the response data structure and response codes specified in table 6.1.3.2.4.2.2-2.

Table 6.1.3.2.4.2.2-1: Data structures supported by the POST Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| UiccConfigurationParameter | M | 1 | Contains the parameter that is to be updated in the UICC |

Table 6.1.3.2.4.2.2-2: Data structures supported by the POST Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  codes | Description |
| SecuredPacket | M | 1 | 200 OK | Upon success, a response body containing the generated secured packet shall be returned. |
| ProblemDetails | O | 0..1 | 404 Not Found | The "cause" attribute may be used to convey the following application error:  - USER\_NOT\_FOUND |
| NOTE: The manadatory HTTP error status code for the POST method listed in Table 5.2.7.1-1 of 3GPP TS 29.500 [4] also apply. | | | | |

### 6.1.4 Custom Operations without associated resources

In this release of this specification, no custom operations without associated resources are defined for the Nspaf\_SecuredPacket Service.

### 6.1.5 Notifications

In this release of this specification, no notifications are defined for the Nspaf\_SecuredPacket Service.

### 6.1.6 Data Model

#### 6.1.6.1 General

This clause specifies the application data model supported by the API.

Table 6.1.6.1-1 specifies the data types defined for the Nspaf service based interface protocol.

Table 6.1.6.1-1: Nspaf specific Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Clause defined | Description | Applicability |
| UiccConfigurationParameter | 6.1.6.2.2 | UICC Configuration Parameters |  |
| RoutingId | 6.1.6.3.2 | Routing ID |  |

Table 6.1.6.1-2 specifies data types re-used by the Nspaf service based interface protocol from other specifications, including a reference to their respective specifications and when needed, a short description of their use within the Nspaf service based interface.

Table 6.1.6.1-2: Nspaf re-used Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Reference | Comments | Applicability |
| SecuredPacket | 3GPP TS 29.503 [14] | Secured Packet |  |
| ProblemDetails | 3GPP TS 29.571 [15] |  |  |
| SteeringInfo | 3GPP TS 29.509 [17] | Steering Information |  |

#### 6.1.6.2 Structured data types

##### 6.1.6.2.1 Introduction

This clause defines the structures to be used in resource representations.

##### 6.1.6.2.2 Type: UiccConfigurationParameter

Table 6.1.6.2.2-1: Definition of type UiccConfigurationParameter

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| routingId | RoutingId | C | 0..1 | The Routing Id that needs to be updated in the USIM. |  |
| steeringContainer | array(SteeringInfo) | C | 1..N | List of PLMN/AccessTechnologies combinations that need to be updated in the USIM. |  |
| Note: Exactly one attribute shall be present | | | | | |

#### 6.1.6.3 Simple data types and enumerations

##### 6.1.6.3.1 Introduction

This clause defines simple data types and enumerations that can be referenced from data structures defined in the previous clauses.

##### 6.1.6.3.2 Simple data types

The simple data types defined in table 6.1.6.3.2-1 shall be supported.

Table 6.1.6.3.2-1: Simple data types

|  |  |  |  |
| --- | --- | --- | --- |
| Type Name | Type Definition | Description | Applicability |
| RoutingId | string | Pattern: "^[0-9]{1,4}$" |  |

### 6.1.7 Error Handling

#### 6.1.7.1 General

For the Nspaf\_SecuredPacket API, HTTP error responses shall be supported as specified in clause 4.8 of 3GPP TS 29.501 [5]. Protocol errors and application errors specified in table 5.2.7.2-1 of 3GPP TS 29.500 [4] shall be supported for an HTTP method if the corresponding HTTP status codes are specified as mandatory for that HTTP method in table 5.2.7.1-1 of 3GPP TS 29.500 [4].

In addition, the requirements in the following clauses are applicable for the Nspaf\_SecuredPacket API.

#### 6.1.7.2 Protocol Errors

No specific procedures for the Nspaf\_SecuredPacket service are specified.

#### 6.1.7.3 Application Errors

The application errors defined for the Nspaf\_SecuredPacket service are listed in Table 6.1.7.3-1.

Table 6.1.7.3-1: Application errors

|  |  |  |
| --- | --- | --- |
| Application Error | HTTP status code | Description |
| USER\_NOT\_FOUND | 404 Not Found | The user does not exist |

## 6.1.8 Feature negotiation

The optional features in table 6.1.8-1 are defined for the Nspaf\_SecuredPacket API. They shall be negotiated using the extensibility mechanism defined in clause 6.6 of 3GPP TS 29.500 [4].

Table 6.1.8-1: Supported Features

|  |  |  |
| --- | --- | --- |
| Feature number | Feature Name | Description |
|  |  |  |

## 6.1.9 Security

As indicated in 3GPP TS 33.501 [8] and 3GPP TS 29.500 [4], the access to the Nspaf\_SecuredPacket API may be authorized by means of the OAuth2 protocol (see IETF RFC 6749 [9]), based on local configuration, using the "Client Credentials" authorization grant, where the NRF (see 3GPP TS 29.510 [10]) plays the role of the authorization server.

If OAuth2 is used, an NF Service Consumer, prior to consuming services offered by the Nspaf\_SecuredPacket API, shall obtain a "token" from the authorization server, by invoking the Access Token Request service, as described in 3GPP TS 29.510 [10], clause 5.4.2.2.

NOTE: When multiple NRFs are deployed in a network, the NRF used as authorization server is the same NRF that the NF Service Consumer used for discovering the Nspaf\_SecuredPacket service.

The Nspaf\_SecuredPacket API defines a single scope "nspaf-secured-packet" for the entire service, and it does not define any additional scopes at resource or operation level.

Annex A (normative):  
OpenAPI specification

## A.1 General

This Annex specifies the formal definition of the API(s) defined in the present specification. It consists of OpenAPI 3.0.0 specifications in YAML format.

This Annex takes precedence when being discrepant to other parts of the specification with respect to the encoding of information elements and methods within the API(s).

NOTE: The semantics and procedures, as well as conditions, e.g. for the applicability and allowed combinations of attributes or values, not expressed in the OpenAPI definitions but defined in other parts of the specification also apply.

Informative copies of the OpenAPI specification files contained in this 3GPP Technical Specification are available on a Git-based repository, that uses the GitLab software version control system (see 3GPP TS 29.501 [5] clause 5.3.1 and 3GPP TR 21.900 [7] clause 5B).

## A.2 Nspaf\_SecuredPacket API

openapi: 3.0.0

info:

title: 'Nspaf\_SecuredPacket'

version: '1.0.1'

description: |

Nspaf Secured Packet Service.

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.544, SP-AF Services, version V16.2.0

url: http://www.3gpp.org/ftp/Specs/archive/29\_series/29.544/

servers:

- url: '{apiRoot}/nspaf-secured-packet/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501

security:

- {}

- oAuth2ClientCredentials:

- nspaf-secured-packet

paths:

/{supi}/provide-secured-packet:

post:

summary: request generation of a secured packet

operationId: ProvideSecuredPacket

tags:

- SecuredPacket Generation (Custom Operation)

parameters:

- name: supi

in: path

description: SUPI of the user

required: true

schema:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/UiccConfigurationParameter'

responses:

'200':

description: Success

content:

application/json:

schema:

$ref: 'TS29503\_Nudm\_SDM.yaml#/components/schemas/SecuredPacket'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{nrfApiRoot}/oauth2/token'

scopes:

nspaf-secured-packet: Access to the nspaf-secured-packet API

schemas:

# COMPLEX TYPES:

UiccConfigurationParameter:

type: object

oneOf:

- required: [routingId ]

- required: [steeringContainer ]

properties:

routingId:

$ref: '#/components/schemas/RoutingId'

steeringContainer:

type: array

items:

$ref: 'TS29509\_Nausf\_SoRProtection.yaml#/components/schemas/SteeringInfo'

minItems: 1

# SIMPLE TYPES:

RoutingId:

type: string

pattern: '^[0-9]{1,4}$'

# ENUMS:

Annex B (informative):  
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2019-10 | CT4#94 | C4-194013 |  |  |  | Initial Draft. | 0.1.0 |
| 2019-10 | CT4#94 | C4-194367 |  |  |  | Notaf Overview | 0.2.0 |
| 2019-10 | CT4#94 | C4-194488 |  |  |  | Notaf\_SecuredPacket-Provide service operation | 0.2.0 |
| 2019-10 | CT4#94 | C4-194492 |  |  |  | Resources | 0.2.0 |
| 2019-10 | CT4#94 | C4-194516 |  |  |  | Data Model | 0.2.0 |
| 2019-10 | CT4#94 | C4-194490 |  |  |  | OpenAPI Specification | 0.2.0 |
| 2019-11 | CT4#95 | C4-195481 |  |  |  | Clean Up | 0.3.0 |
| 2019-12 | CT#86 | CP-193071 |  |  |  | TS presented for information | 1.0.0 |
| 2019-12 | CT#86 | CP-193285 |  |  |  | A title updated | 1.0.1 |
| 2020-03 | CT4#96e | C4-201119 |  |  |  | Pseudo-CR on SOR | 1.1.0 |
| 2020-03 | CT4#96e | C4-201123 |  |  |  | Pseudo-CR on Clean Up | 1.1.0 |
| 2020-03 | CT4#96e | C4-201217 |  |  |  | Pseudo-CR on the necessary modifications to change OTAF NF name to SP-AF | 1.1.0 |
| 2020-03 | CT4#96e | C4-201314 |  |  |  | Pseudo-CR on API descriptions table in clause 5.1 | 1.1.0 |
| 2020-03 | CT#87e | CP-200062 |  |  |  | TS presented for approval | 2.0.0 |
| 2020-03 | CT#87e |  |  |  |  | Approved at CT#87e | 16.0.0 |
| 2020-07 | CT#88e | CP-201040 | 0001 | 1 | C | Clarification on Secured Packet format provided by SP-AF | 16.1.0 |
| 2020-07 | CT#88e | CP-201040 | 0002 |  | F | Storage of YAML files in ETSI Forge | 16.1.0 |
| 2020-07 | CT#88e | CP-201040 | 0003 | 1 | F | Miscellaneous Corrections | 16.1.0 |
| 2020-07 | CT#88e | CP-201073 | 0005 |  | F | 3GPP TS 29.544 API Version and External doc Update | 16.1.0 |
| 2020-09 | CT#89e | CP-202110 | 0006 | 1 | F | Miscelaneous corrections | 16.2.0 |
| 2020-09 | CT#89e | CP-202096 | 0007 |  | F | API version and External doc update | 16.2.0 |
| 2020-12 | CT#90e | CP-203048 | 0008 |  | F | Storage of yaml files | 16.3.0 |