|  |  |
| --- | --- |
| 3GPP TS 29.573 V16.11.0 (2022-09) | |
| Technical Specification | |
| 3rd Generation Partnership Project;  Technical Specification Group Core Network and Terminals;  5G System; Public Land Mobile Network (PLMN)  Interconnection;  Stage 3  (Release 16) | |
|  | |
|  |  |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  http://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 7

1 Scope 8

2 References 8

3 Definitions and abbreviations 9

3.1 Definitions 9

3.2 Abbreviations 9

4 General Description 10

4.1 Introduction 10

4.2 N32 Interface 10

4.2.1 General 10

4.2.2 N32-c Interface 10

4.2.3 N32-f Interface 10

4.3 Protocol Stack 11

4.3.1 General 11

4.3.2 HTTP/2 Protocol 11

4.3.2.1 General 11

4.3.2.2 HTTP standard headers 12

4.3.2.3 HTTP custom headers 12

4.3.2.4 HTTP/2 connection management 12

4.3.3 Transport Protocol 13

4.3.4 Serialization Protocol 13

5 N32 Procedures 13

5.1 Introduction 13

5.2 N32 Handshake Procedures (N32-c) 14

5.2.1 General 14

5.2.2 Security Capability Negotiation Procedure 14

5.2.3 Parameter Exchange Procedure 15

5.2.3.1 General 15

5.2.3.2 Parameter Exchange Procedure for Cipher Suite Negotiation 15

5.2.3.3 Parameter Exchange Procedure for Protection Policy Exchange 16

5.2.3.4 Parameter Exchange Procedure for Security Information list Exchange 19

5.2.4 N32-f Context Termination Procedure 19

5.2.5 N32-f Error Reporting Procedure 20

5.3 JOSE Protected Message Forwarding Procedure on N32 (N32-f) 21

5.3.1 Introduction 21

5.3.2 Use of Application Layer Security 21

5.3.2.1 General 21

5.3.2.2 Protection Policy Lookup 22

5.3.2.3 Message Reformatting 22

5.3.2.4 Message Forwarding to Peer SEPP 24

5.3.3 Message Forwarding to Peer SEPP when TLS is used 25

5.3.4 JOSE Protected Forwarding Options 25

5.4 Nsepp\_Telescopic\_FQDN\_Mapping Service 26

5.4.1 General 26

5.4.2 Foreign FQDN to Telescopic FQDN Mapping Procedure 26

5.4.3 Telescopic FQDN to Foreign FQDN Mapping Procedure 26

6 API Definitions 27

6.1 N32 Handshake API 27

6.1.1 API URI 27

6.1.2 Usage of HTTP 27

6.1.2.1 General 27

6.1.2.2 HTTP standard headers 27

6.1.2.2.1 General 27

6.1.2.2.2 Content type 27

6.1.2.3 HTTP custom headers 28

6.1.2.3.1 General 28

6.1.3 Resources 28

6.1.3.1 Overview 28

6.1.4 Custom Operations without Associated Resources 28

6.1.4.1 Overview 28

6.1.4.2 Operation: Security Capability Negotiation 28

6.1.4.2.1 Description 28

6.1.4.2.2 Operation Definition 28

6.1.4.3 Operation: Parameter Exchange 29

6.1.4.3.1 Description 29

6.1.4.3.2 Operation Definition 29

6.1.4.4 Operation: N32-f Context Terminate 30

6.1.4.4.1 Description 30

6.1.4.4.2 Operation Definition 30

6.1.4.5 Operation: N32-f Error Reporting 31

6.1.4.5.1 Description 31

6.1.4.5.2 Operation Definition 31

6.1.5 Data Model 31

6.1.5.1 General 31

6.1.5.2 Structured data types 32

6.1.5.2.1 Introduction 32

6.1.5.2.2 Type: SecNegotiateReqData 33

6.1.5.2.3 Type: SecNegotiateRspData 33

6.1.5.2.4 Type: SecParamExchReqData 34

6.1.5.2.5 Type: SecParamExchRspData 35

6.1.5.2.6 Type: ProtectionPolicy 36

6.1.5.2.7 Type: ApiIeMapping 36

6.1.5.2.8 Type: IeInfo 37

6.1.5.2.9 Type: ApiSignature 38

6.1.5.2.10 Type: N32fContextInfo 38

6.1.5.2.11 Type: N32fErrorInfo 39

6.1.5.2.12 Type: FailedModificationInfo 39

6.1.5.2.13 Type: N32fErrorDetail 39

6.1.5.2.14 Type: CallbackName 40

6.1.5.2.15 Type: IpxProviderSecInfo 40

6.1.5.3 Simple data types and enumerations 40

6.1.5.3.1 Introduction 40

6.1.5.3.2 Simple data types 40

6.1.5.3.3 Enumeration: SecurityCapability 40

6.1.5.3.4 Enumeration: HttpMethod 41

6.1.5.3.5 Enumeration: IeType 41

6.1.5.3.6 Enumeration: IeLocation 41

6.1.5.3.7 Enumeration: N32fErrorType 42

6.1.5.3.8 Enumeration: FailureReason 42

6.1.5.4 Binary data 42

6.1.6 Error Handling 42

6.1.6.1 General 42

6.1.6.2 Protocol Errors 42

6.1.6.3 Application Errors 43

6.2 JOSE Protected Message Forwarding API on N32 43

6.2.1 API URI 43

6.2.2 Usage of HTTP 43

6.2.2.1 General 43

6.2.2.2 HTTP standard headers 43

6.2.2.2.1 General 43

6.2.2.2.2 Content type 43

6.2.2.2.3 Accept-Encoding 44

6.2.2.3 HTTP custom headers 44

6.2.2.3.1 General 44

6.2.3 Resources 44

6.2.3.1 Overview 44

6.2.4 Custom Operations without associated resources 44

6.2.4.1 Overview 44

6.2.4.2 Operation: JOSE Protected Forwarding 44

6.2.4.2.1 Description 44

6.2.4.2.2 Operation Definition 45

6.2.4.3 Operation: JOSE Protected Forwarding Options 45

6.2.4.3.1 Description 45

6.2.4.3.2 Operation Definition 45

6.2.5 Data Model 46

6.2.5.1 General 46

6.2.5.2 Structured data types 47

6.2.5.2.1 Introduction 47

6.2.5.2.2 Type: N32fReformattedReqMsg 47

6.2.5.2.3 Type: N32fReformattedRspMsg 48

6.2.5.2.4 Type: DataToIntegrityProtectAndCipherBlock 48

6.2.5.2.5 Type: DataToIntegrityProtectBlock 49

6.2.5.2.6 Type: RequestLine 49

6.2.5.2.7 Type: HttpHeader 50

6.2.5.2.8 Type: HttpPayload 51

6.2.5.2.9 Type: MetaData 52

6.2.5.2.10 Type: Modifications 53

6.2.5.2.11 Type: FlatJweJson 53

6.2.5.2.12 Type: FlatJwsJson 54

6.2.5.2.13 Type: IndexToEncryptedValue 54

6.2.5.2.14 Type: EncodedHttpHeaderValue 54

6.2.5.3 Simple data types and enumerations 54

6.2.5.3.1 Introduction 54

6.2.5.3.2 Simple data types 54

6.2.5.3.3 Void 55

6.2.5.3.4 Void 55

6.2.6 Error Handling 55

6.2.6.1 General 55

6.2.6.2 Protocol Errors 55

6.2.6.3 Application Errors 55

6.3 Nsepp\_Telescopic\_FQDN\_Mapping API 55

6.3.1 API URI 55

6.3.2 Usage of HTTP 55

6.3.2.1 General 55

6.3.2.2 HTTP standard headers 55

6.3.2.2.1 General 55

6.3.2.2.2 Content type 56

6.3.2.3 HTTP custom headers 56

6.3.2.3.1 General 56

6.3.3 Resources 56

6.3.3.1 Overview 56

6.3.3.2 Resource: Mapping 56

6.3.3.2.1 Description 56

6.3.3.2.2 Resource Definition 56

6.3.3.2.3 Resource Standard Methods 57

6.3.4 Data Model 57

6.3.4.1 General 57

6.3.4.2 Structured data types 58

6.3.4.2.1 Introduction 58

6.3.4.2.2 Type: TelescopicMapping 58

6.3.4.3 Simple data types and enumerations 58

6.3.4.3.1 Introduction 58

6.3.4.3.2 Simple data types 58

6.3.5 Error Handling 59

6.3.5.1 General 59

6.3.5.2 Protocol Errors 59

6.3.5.3 Application Errors 59

6.3.6 Feature Negotiation 59

6.3.7 Security 59

6.3.7.1 General 59

Annex A (normative): OpenAPI Specification 59

A.1 General 59

A.2 N32 Handshake API 60

A.3 JOSE Protected Message Forwarding API on N32-f 65

A.4 SEPP Telescopic FQDN Mapping API 69

Annex B (informative): Examples of N32-f Encoding 70

B.1 General 70

B.2 Input Message Containing No Binary Part 70

B.3 Input Message Containing Multipart Binary Part 72

Annex C (informative): End to end call flows when SEPP is on path 75

C.1 General 75

C.2 TLS security between SEPPs 75

C.2.1 When http URI scheme is used 75

C.2.1.1 General 75

C.2.1.2 Without TLS protection between NF and SEPP and with TLS security without the 3gpp-Sbi-Target-apiRoot header used over N32f 75

C.2.1.3 Without TLS protection between NF and SEPP and with TLS security with the 3gpp-Sbi-Target-apiRoot header used over N32f 78

C.2.2 When https URI scheme is used 79

C.2.2.1 General 79

C.2.2.2 With TLS protection between NF and SEPP relying on telescopic FQDN, and TLS security without the 3gpp-Sbi-Target-apiRoot header used over N32f 79

C.2.2.3 With TLS protection between NF and SEPP relying on 3gpp-Sbi-Target-apiRoot header, and TLS security without the 3gpp-Sbi-Target-apiRoot header used over N32f 83

C.2.2.4 With TLS protection between NF and SEPP relying on telescopic FQDN, and TLS security with the 3gpp-Sbi-Target-apiRoot header used over N32f 86

C.2.2.5 With TLS protection between NF and SEPP relying on 3gpp-Sbi-Target-apiRoot header, and TLS security with the 3gpp-Sbi-Target-apiRoot header used over N32f 89

C.3 Application Layer Security between SEPPs 91

C.3.1 When http URI scheme is used 91

C.3.2 When https URI scheme is used 93

C.3.2.1 General 93

C.3.2.2 With TLS protection between NF and SEPP relying on telescopic FQDN 94

C.3.2.3 With TLS protection between NF and SEPP relying on 3gpp-Sbi-Target-apiRoot header 97

Annex D (informative): Withdrawn API versions 100

D.1 General 100

D.2 N32 Handshake API 100

Annex E (informative): Change history 102

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

In the present document, modal verbs have the following meanings:

**shall** indicates a mandatory requirement to do something

**shall not** indicates an interdiction (prohibition) to do something

The constructions "shall" and "shall not" are confined to the context of normative provisions, and do not appear in Technical Reports.

The constructions "must" and "must not" are not used as substitutes for "shall" and "shall not". Their use is avoided insofar as possible, and they are not used in a normative context except in a direct citation from an external, referenced, non-3GPP document, or so as to maintain continuity of style when extending or modifying the provisions of such a referenced document.

**should** indicates a recommendation to do something

**should not** indicates a recommendation not to do something

**may** indicates permission to do something

**need not** indicates permission not to do something

The construction "may not" is ambiguous and is not used in normative elements. The unambiguous constructions "might not" or "shall not" are used instead, depending upon the meaning intended.

**can** indicates that something is possible

**cannot** indicates that something is impossible

The constructions "can" and "cannot" are not substitutes for "may" and "need not".

**will** indicates that something is certain or expected to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**will not** indicates that something is certain or expected not to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**might** indicates a likelihood that something will happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

**might not** indicates a likelihood that something will not happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

In addition:

**is** (or any other verb in the indicative mood) indicates a statement of fact

**is not** (or any other negative verb in the indicative mood) indicates a statement of fact

The constructions "is" and "is not" do not indicate requirements.

# 1 Scope

The present document specifies the stage 3 protocol and data model for the PLMN interconnection Interface. It provides stage 3 protocol definitions and message flows, and specifies the APIs for the procedures on the PLMN interconnection interface (i.e N32).

The 5G System stage 2 architecture and procedures are specified in 3GPP TS 23.501 [2] and 3GPP TS 23.502 [3].

The Technical Realization of the Service Based Architecture and the Principles and Guidelines for Services Definition are specified in 3GPP TS 29.500 [4] and 3GPP TS 29.501 [5].

The stage 2 level N32 procedures are specified in 3GPP TS 33.501 [6].

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 23.501: "System Architecture for the 5G System; Stage 2".

[3] 3GPP TS 23.502: "Procedures for the 5G System; Stage 2".

[4] 3GPP TS 29.500: "5G System; Technical Realization of Service Based Architecture; Stage 3".

[5] 3GPP TS 29.501: "5G System; Principles and Guidelines for Services Definition; Stage 3".

[6] 3GPP TS 33.501: "Security architecture and procedures for 5G system".

[7] IETF RFC 7540: "Hypertext Transfer Protocol Version 2 (HTTP/2)".

[8] IETF RFC 8259: "The JavaScript Object Notation (JSON) Data Interchange Format".

[9] IETF RFC 7231: "Hypertext Transfer Protocol (HTTP/1.1): Semantics and Content".

[10] IETF RFC 7230: "Hypertext Transfer Protocol (HTTP/1.1): Message Syntax and Routing".

[11] IETF RFC 793: "Transmission Control Protocol".

[12] 3GPP TS 29.571: "5G System; Common Data Types for Service Based Interfaces Stage 3".

[13] IETF RFC 7518: "JSON Web Algorithms (JWA)".

[14] IETF RFC 7516: "JSON Web Encryption (JWE)".

[15] IETF RFC 4648: "The Base16, Base32, and Base64 Data Encodings".

[16] IETF RFC 7515: "JSON Web Signature (JWS)".

[17] IETF RFC 6901: "JavaScript Object Notation (JSON) Pointer".

[18] 3GPP TS 29.510: "Network Function Repository Services; Stage 3".

[19] 3GPP TS 23.003: "Numbering, addressing and identification".

[20] 3GPP TR 21.900: "Technical Specification Group working methods".

[21] IETF RFC 7468: "Textual Encodings of PKIX, PKCS, and CMS Structures".

[22] IETF RFC 7807: "Problem Details for HTTP APIs".

[23] IETF RFC 1952: "GZIP file format specification version 4.3".

[24] IETF RFC 7694: "Hypertext Transfer Protocol (HTTP) Client-Initiated Content-Encoding".

[25] 3GPP TS 29.518: "5G System; Access and Mobility Management Service; Stage 3".

[26] 3GPP TS 29.503: "5G System; Unified Data Management Services; Stage 3".

# 3 Definitions and abbreviations

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in 3GPP TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in 3GPP TR 21.905 [1].

**c-SEPP:** The SEPP that is present on the NF service consumer side is called the c-SEPP.

**p-SEPP:** The SEPP that is present on the NF service producer side is called the p-SEPP.

NOTE: For the purpose of N32-c procedures, the two interacting SEPPs are called "initiating" SEPP and "responding" SEPP. The c-SEPP and p-SEPP terminology is not used in this specification though it is used in 3GPP TS 33.501 [6].

**c-IPX**: The IPX on the NF service consumer side.

**p-IPX**: The IPX of the NF service producer side.

## 3.2 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

GZIP GNU ZIP

IPX IP Exchange Service

JOSE Javascript Object Signing and Encryption

JWE JSON Web Encryption

JWS JSON Web Signature

PRINS PRotocol for N32 INterconnect Security

SEPP Security and Edge Protection Proxy

TLS Transport Layer Security

UPU UE Parameters Update

# 4 General Description

## 4.1 Introduction

This clause provides a general description of the interconnect interfaces used between the PLMNs for transporting the service based interface message exchanges.

## 4.2 N32 Interface

### 4.2.1 General

The N32 interface is used between the SEPPs in different PLMNs for both roaming and PLMN interconnect scenarios. The SEPP that is on the NF service consumer side is called the c-SEPP and the SEPP that is on the NF service producer is called the p-SEPP. The N32 interface can be logically considered as 2 separate interfaces as given below.

- N32-c, a control plane interface between the SEPPs for performing initial handshake and negotiating the parameters to be applied for the actual N32 message forwarding.

- N32-f, a forwarding interface between the SEPPs which is used for forwarding the communication between the NF service consumer and the NF service producer after applying application level security protection.

### 4.2.2 N32-c Interface

The following figure shows the scope of the N32-c interface.



Figure 4.2.2-1: N32-c Interface

The N32-c interface provides the following functionalities:

- Initial handshake procedure between the SEPP in PLMN A (called the initiating SEPP) and the SEPP in PLMN B (called the responding SEPP), that involves capability negotiation and parameter exchange as specified in 3GPP TS 33.501 [6].

### 4.2.3 N32-f Interface

The following figure shows the scope of the N32-f interface.



Figure 4.2.3-1: N32-f Interface

The N32-f interface shall be used to forward the HTTP/2 messages of the NF service producers and the NF service consumers in different PLMN, through the SEPPs of the respective PLMN. The application layer security protection functionality of the N32-f is used only if the PRotocol for N32 INterconnect Security (PRINS) is negotiated between the SEPPs using N32-c.

The N32-f interface provides the following application layer security protection functionalities:

- Message protection of the information exchanged between the NF service consumer and the NF service producer across PLMNs by applying application layer security mechanisms as specified in 3GPP TS 33.501 [6].

- Forwarding of the application layer protected message from a SEPP in one PLMN to a SEPP in another PLMN. Such forwarding may involve IPX providers on path.

- If IPX providers are on the path from SEPP in PLMN A to SEPP in PLMN B, the forwarding on the N32-f interface may involve the insertion of content modification instructions which the receiving SEPP applies after verifying the integrity of such modification instructions.

If TLS is the negotiated security policy between the SEPP, then the N32-f shall involve only the forwarding of the HTTP/2 messages of the NF service producers and the NF service consumers without any reformatting at the SEPPs and/or the IPXs.

## 4.3 Protocol Stack

### 4.3.1 General

The protocol stack for the N32 interface is shown below in Figure 4.2.1-1



Figure 4.3.1-1: N32 Protocol Stack

The N32 interfaces (N32-c and N32-f) use HTTP/2 protocol (see clause 4.2.2) with JSON (see clause 4.2.4) as the application layer serialization protocol. For the security protection at the transport layer, the SEPPs shall support TLS as specified in 3GPP TS 33.501 [6].

For the N32-f interface, the application layer (i.e the JSON payload) encapsulates the complete HTTP/2 message between the NF service consumer and the NF service producer, by transforming the HTTP/2 headers and the body into specific JSON attributes as specified in clause 6.2.

### 4.3.2 HTTP/2 Protocol

#### 4.3.2.1 General

HTTP/2 as described in IETF RFC 7540 [7] shall be used for N32 interface.

#### 4.3.2.2 HTTP standard headers

The HTTP request standard headers and the HTTP response standard headers that shall be supported on the N32 interface are defined in Table 4.2.2.2-1 and in Table 4.2.2.2-2 respectively.

Table 4.3.2.2-1: Mandatory to support HTTP request standard headers

|  |  |  |
| --- | --- | --- |
| Name | Reference | Description |
| Accept | IETF RFC 7231 [9] | This header is used to specify response media types that are acceptable. |
| Accept-Encoding | IETF RFC 7231 [9] | This header may be used to indicate what response content-encodings (e.g gzip) are acceptable in the response. |
| Content-Length | IETF RFC 7230 [10] | This header is used to provide the anticipated size, as a decimal number of octets, for a potential payload body. |
| Content-Type | IETF RFC 7231 [9] | This header is used to indicate the media type of the associated representation. |
| Via | IETF RFC 7230 [10] | This header is used to indicate the intermediate proxies in the service request path. Please refer to clause 6.10.8 of 3GPP TS 29.500 [4] for encoding of the via header |

Table 4.3.2.2-2: Mandatory to support HTTP response standard headers

|  |  |  |
| --- | --- | --- |
| Name | Reference | Description |
| Content-Length | IETF RFC 7230 [10] | This header may be used to provide the anticipated size, as a decimal number of octets, for a potential payload body. |
| Content-Type | IETF RFC 7231 [9] | This header shall be used to indicate the media type of the associated representation. |
| Content-Encoding | IETF RFC 7231 [9] | This header may be used in some responses to indicate to the HTTP/2 client the content encodings (e.g gzip) applied to the response body beyond those inherent in the media type. |
| Via | IETF RFC 7230 [10] | This header is used to indicate the intermediate proxies in the service response path. Please refer to clause 6.10.8 of 3GPP TS 29.500 [4] for encoding of the via header. |
| Server | IETF RFC 7231 [9] | This header is used to indicate the originator of an HTTP error response. |

#### 4.3.2.3 HTTP custom headers

The HTTP custom headers specified in clause 5.2.3 of 3GPP TS 29.500 [4] shall be supported on the N32 interface.

#### 4.3.2.4 HTTP/2 connection management

Each SEPP initiates HTTP/2 connections towards its peer SEPP for the following purposes

- N32-c interface

- N32-f interface

The scope of the HTTP/2 connection used for the N32-c interface is short-lived. Once the initial handshake is completed the connection is torn down as specified in 3GPP TS 33.501 [6]. The HTTP/2 connection used for N32-c is end to end between the SEPPs and does not involve an IPX to intercept the HTTP/2 connection, though an IPX may be involved for IP level routing.

The scope of the HTTP/2 connection used for the N32-f interface is long-lived. The N32-f HTTP/2 connection at a SEPP can be:

- Case A: Towards a SEPP of another PLMN without involving any IPX intermediaries or involving IPX intermediaries where IPX does not require modification or observation of the information; or

- Case B: Towards a SEPP of another PLMN via IPX where IPX requires modification or observation of the information. In this case, the HTTP/2 connection from a SEPP terminates at the next hop IPX with the IPX acting as a HTTP proxy.

For the N32-f interface the HTTP/2 connection management requirements specified in clause 5.2.6 of 3GPP TS 29.500 [4] shall be applicable. The URI scheme used for the N32-f JOSE protected message forwarding API shall be "http". If confidentiality protection of all IEs for the N32-f JOSE protected message forwarding procedure is required, then:

- For case A, the security between the SEPPs shall be ensured by means of an IPSec or TLS connection;

- For case B, hop-by-hop security between the SEPP and the IPXs should be established on N32-f. This hop-by-hop security shall be established using an IPSec or TLS connection.

### 4.3.3 Transport Protocol

The Transmission Control Protocol as described in IETF RFC 793 [11] shall be used as transport protocol as required by HTTP/2 (see IETF RFC 7540 [7]).

When there is no IPX between the SEPPs or IPX(s) are offering only IP routing service without modification or observation of the content, TLS shall be used for security protection (see clause 13.1.2 of 3GPP TS 33.501 [6]). When there is IPX between the SEPPs and IPX requires modification or observation of the content, TLS or NDS/IP should be used for security protection as specified in clause 13.1.2 of 3GPP TS 33.501 [6].

NOTE: When using TCP as the transport protocol, an HTTP/2 connection is mapped to a TCP connection.

### 4.3.4 Serialization Protocol

The JavaScript Object Notation (JSON) format as described in IETF RFC 8259 [8] shall be used as the serialization protocol.

# 5 N32 Procedures

## 5.1 Introduction

The procedures on the N32 interface are split into two categories:

- Procedures that happen end to end between the SEPPs on the N32-c interface;

- Procedures that are used for the forwarding of messages on the service based interface between the NF service consumer and the NF service producer via the SEPP across the N32-f interface.

Table 5.1-1 summarizes the corresponding APIs defined for this specification.

Table 5.1-1: API Descriptions

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Service Name | Clause | Description | OpenAPI Specification File | apiName | Annex |
| N32 Handshake | 6.1 | N32-c Handshake Service | TS29573\_N32\_Handshake.yaml | n32c-handshake | A.2 |
| JOSE Protected Message Forwarding | 6.2 | N32-f Message Forwarding Service | TS29573\_JOSEProtectedMessageForwarding.yaml | n32f-forward | A.3 |
| Nsepp\_Telescopic\_FQDN\_Mapping | 6.3 | SEPP Telescopic FQDN Mapping | TS29573\_SeppTelescopicFqdnMapping.yaml | nsepp-telescopic | A.4 |

## 5.2 N32 Handshake Procedures (N32-c)

### 5.2.1 General

The N32 handshake procedure is used between the SEPPs in two PLMNs to mutually authenticate each other and negotiate the security mechanism to use over N32-f along with associated security configuration parameters.

A HTTP/2 connection shall be established between the initiating SEPP and the responding SEPP end to end over TLS. The following N32 handshake procedures are specified in the clauses below.

- Security Capability Negotiation Procedure

- Parameter Exchange Procedure

- N32-f Context Termination Procedure

- N32-f Error Reporting Procedure

### 5.2.2 Security Capability Negotiation Procedure

The initiating SEPP shall initiate a Security Capability Negotiation procedure towards the responding SEPP to agree on a security mechanism to use for protecting NF service related signalling over N32-f. An end to end TLS connection shall be setup between the SEPPs before the initiation of this procedure. The procedure is described in Figure 5.2.2-1 below.



Figure 5.2.2-1: Security Capability Negotiation Procedure

1. The initiating SEPP issues a HTTP POST request towards the responding SEPP with the request body containing the "SecNegotiateReqData" IE carrying the following information:

- Supported security capabilities (i.e PRINS and/or TLS);

- Whether the 3gpp-Sbi-Target-apiRoot HTTP header is supported, if TLS security is supported;

- Sender PLMN ID(s).

- Target PLMN ID.

If different PLMNs are represented by different PLMN IDs supported by a SEPP, then the SEPP shall use separate N32-connections for each pair of home and visited PLMN. Both SEPPs shall store the mapping between the N32 connections and their pair of PLMN IDs.

NOTE 1: If SEPPs support separate fqdn per PLMN, then Target PLMN Id is not required as target PLMN can be selected by the fqdn.

2a. On successful processing of the request, the responding SEPP shall respond to the initiating SEPP with a "200 OK" status code and a POST response body that contains "SecNegotiateRspData" IE carrying the following information:

- Selected security capability (i.e PRINS or TLS);

- Whether the 3gpp-Sbi-Target-apiRoot HTTP header is supported, if TLS security is selected;

- Sender PLMN ID(s).

The responding SEPP compares the initiating SEPP's supported security capabilities to its own supported security capabilities and selects, based on its local policy, a security mechanism, which is supported by both the SEPPs. If the selected security capability indicates any other capability other than PRINS, then the HTTP/2 connection initiated between the two SEPPs for the N32 handshake procedures shall be terminated. The negotiated security capability shall be applicable on both the directions. If the selected security capability is PRINS, then the two SEPPs may decide to create (if not available) / maintain HTTP/2 connection(s) where each SEPP acts as a client towards the other (which acts as a server). This may be used for later signalling of N32-f error reporting procedure (see clause 5.2.5) and N32-f context termination procedure (see clause 5.2.4).

If different PLMNs are represented by different PLMN IDs supported by a SEPP, then the SEPP shall use separate N32-connections for each pair of home and visited PLMN. Both SEPPs shall store the mapping between the N32 connections and their pair of PLMN IDs.

The SEPP shall select the PLMN from the list of supported PLMN(s) based on the received Target PLMN ID or PLMN specific fqdn used in the request and provide the selected PLMN's PLMN Id(s) in the plmnIdList.

2b. On failure, the responding SEPP shall respond to the initiating SEPP with an appropriate 4xx/5xx status code as specified in clause 6.1.4.2.

### 5.2.3 Parameter Exchange Procedure

#### 5.2.3.1 General

The parameter exchange procedure shall be executed if the security capability negotiation procedure selected the security capability as PRINS. The parameter exchange procedure is performed to:

- Agree on a cipher suite to use for protecting NF service related signalling over N32-f; and

- Optionally, exchange the protection policies to use for protecting NF service related signalling over N32.

#### 5.2.3.2 Parameter Exchange Procedure for Cipher Suite Negotiation

The parameter exchange procedure for cipher suite negotiation shall be performed after the security capability negotiation procedure if the selected security policy is PRINS. If there is a change in the cipher suite and the SEPP wants to renegotiate it, then the SEPP may reuse the parameter exchange procedure to override what was exchanged before.

The procedure is described in Figure 5.2.3.2-1 below.



Figure 5.2.3.2-1: Parameter Exchange Procedure for Cipher Suite Negotiation

1. The initiating SEPP issues a HTTP POST request towards the responding SEPP with the request body containing the "SecParamExchReqData" IE carrying the following information

- Supported cipher suites;

The supported cipher suites shall be an ordered list with the cipher suites mandated by 3GPP TS 33.501 [6] appearing at the top of the list.

The initiating SEPP also provides a N32-f context identifier for the responding SEPP to use towards the initiating SEPP for subsequent JOSE Protected Message Forwarding procedures over N32-f (see clause 5.3.3) when the responding SEPP acts as the forwarding SEPP.

2a. On successful processing of the request, the responding SEPP shall respond to the initiating SEPP with a "200 OK" status code and a POST response body that contains the following information

- Selected cipher suite

The responding SEPP compares the initiating SEPP's supported cipher suites to its own supported cipher suites and selects, based on its local policy, a cipher suite, which is supported by both the SEPPs. The responding SEPP's supported cipher suites shall be an ordered list with the cipher suites mandated by 3GPP TS 33.501 [6] appearing at the top of the list. The selected cipher suite is applicable for both the directions of communication between the SEPPs.

The responding SEPP also provides a N32-f context identifier for the initiating SEPP to use towards the responding SEPP for subsequent JOSE Protected Message Forwarding procedures over N32-f (see clause 5.3.3) when the initiating SEPP acts as the forwarding SEPP.

If the receiving SEPP already has a previously negotiated cipher suite, the SEPP shall overwrite it with the new one.

2b. On failure, the responding p-SEPP shall respond to the initiating SEPP with an appropriate 4xx/5xx status code as specified in clause 6.1.4.3. If the SEPP already has a previously negotiated cipher suite, the SEPP shall continue to use the same.

NOTE : If a SEPP already has a previously negotiated cipher suite and a new cipher suite is also received, the SEPP starts applying the new cipher suite immediately and also continues with the old cipher suite for a limited time period. This allows messages with old policies to be completed gracefully.

#### 5.2.3.3 Parameter Exchange Procedure for Protection Policy Exchange

The parameter exchange procedure for protection policy exchange may be performed after the Parameter Exchange Procedure for Cipher Suite Negotiation (see clause 5.2.3.2). If a HTTP/2 connection does not exist towards the peer SEPP at the time of initiating this procedure, the HTTP/2 connection shall be established. If there is a change in the protection policy exchange and the SEPP wants to renegotiate it, then the SEPP may reuse the parameter exchange procedure for the protection policy exchange to override what was exchanged before. If the parameter exchange procedure for the protection policy exchange is not performed then the protection policies between the SEPP shall be exchanged out of bands.

The procedure is described in Figure 5.2.3.3-1 below.



Figure 5.2.3.3-1: Parameter Exchange Procedure for Protection Policy Exchange

1. The initiating SEPP issues a HTTP POST request towards the responding SEPP with the request body containing the "SecParamExchReqData" IE carrying the following information

- Protection policy information

The protection policy information contains:

- API to IE mapping containing the mapping information of list of leaf IEs for each:

- Request/response and Subscribe / Unsubscribe service operation, identified by the API URI and method; and/or

- Callbacks (e.g Notification service operation), identified by the value of the 3GPP custom HTTP header "3gpp-Sbi-Callback" (see clause 5.2.3 of 3GPP TS 29.500 [4]).

- List of IE types that are to be protected across N32-f (i.e the data type encryption policy as specified in clause 13.2.3.2 of 3GPP TS 33.501 [6]); and

- Modification policy: Against each leaf IE in the API to IE mapping information, a boolean flag indicating whether that IE is allowed to be modified by an IPX on the side of the SEPP sending the protection policy information.

If the initiating SEPP connects to several IPXs, an isModifiable IE may be included to indicate an IE is allowed to be modified by all IPX(s) or an map type of isModifiableByIpx IE may be included to indicate an IE is allowed to be modified by an IPX identified by the key of ipxProviderId IE if this IE is allowed to be modified by some of (but not all) the IPX(s), as specified in clause 13.2.3.4 of 3GPP TS 33.501 [6].

2a. On successful processing of the request, the responding SEPP shall respond to the initiating SEPP with a "200 OK" status code and a POST response body that contains the following information

- Selected protection policy information

The Selected protection policy information contains the IEs allowed to be modified by an IPX on the side of the responding SEPP. If the responding SEPP connects to several IPXs, an isModifiable IE may be included to indicate an IE is allowed to be modified by all IPX(s) or an map type of isModifiableByIpx IE may be included to indicate an IE is allowed to be modified by an IPX identified by the key of ipxProviderId IE if this IE is allowed to be modified by some of (but not all) the IPX(s), as specified in clause 13.2.3.4 of 3GPP TS 33.501 [6].

The initiating SEPP shall store the modification policy which are sent from responding SEPP in selected protection policy information and the responding SEPP shall store the modification policy which are sent from the initiating SEPP in the protection policy information. The SEPP receving the subsequent message transfers over N32-f shall check whether the modifications performed by the IPXs were permitted by the respective modification policy.

The SEPPs shall store the encryption policy in selected protection policy information and shall apply this policy for subsequent message transfers over N32-f. The encryption policy in selected protection policy is applicable for both the directions of communication between the SEPPs.

If the receiving SEPP already has a previously negotiated protection policy information, the SEPP shall overwrite it with the new one.

The HTTP/2 connection used for the N32 handshake procedures may be terminated after the completion of this procedure.

2b. On failure, the responding SEPP shall respond to the initiating SEPP with an appropriate 4xx/5xx status code as specified in clause 6.1.4.3. If the SEPP already has previously negotiated protection policy information, the SEPP shall continue to use the same.

NOTE : If a SEPP already has a previously negotiated cipher suite and a new cipher suite is also received, the SEPP starts applying the new cipher suite immediately and also continues with the old cipher suite for a limited time period. This allows messages with old policies to be completed gracefully.

An illustration of how the protection policy is stored and looked up in the SEPP is provided in figure 5.2.3.3-2



Figure 5.2.3.3-2: Protection Policy Storage and Lookup in SEPP

During the N32-f message forwarding, the SEPP looks at a HTTP request or response it receives from an NF service consumer or NF service producer and then uses the above tables to decide which IEs and headers in the message it shall cipher and integrity protect and which IEs it shall allow the IPXes to modify.

#### 5.2.3.4 Parameter Exchange Procedure for Security Information list Exchange

The initiating SEPP shall initiate a Security Information list exchange procedure towards the responding SEPP to exchange the Security Information lists that contain information on IPX public keys or certificates that are needed to verify IPX modifications at the receiving SEPP as specified in clause 13.2.2.2 of 3GPP TS 33.501 [6]. If there is a change in the security information list and the SEPP wants to renegotiate it, then the SEPP may reuse the parameter exchange procedure for the security information list exchange to override what was exchanged before.

The procedure is described in Figure 5.2.3.4-1 below.



Figure 5.2.3.4-1: Parameter Exchange Procedure for Security Information List exchange

1. The initiating SEPP issues a HTTP POST request towards the responding SEPP with the request body containing the "SecParamExchReqData" IE carrying the following information:

- IPX provider identifier connected to the initiating SEPP;

- List of raw public keys or certificates for that IPX.

2a. On successful processing of the request, the responding SEPP shall respond to the initiating SEPP with a "200 OK" status code and a POST response body that contains the "SecParamExchRspData" IE carrying the following information:

- IPX provider identifier connected to the responding SEPP;

- List of raw public keys or certificates for that IPX.

If the receiving SEPP already has a previously negotiated security information list, the SEPP shall overwrite it with the new one.

2b. On failure, the responding SEPP shall respond to the initiating SEPP with an appropriate 4xx/5xx status code as specified in clause 6.1.4.3. If the SEPP already has previously negotiated security information list, the SEPP shall continue to use the same.

NOTE : If a SEPP already has a previously negotiated cipher suite and a new cipher suite is also received, the SEPP starts applying the new cipher suite immediately and also continues with the old cipher suite for a limited time period. This allows messages with old policies to be completed gracefully.

### 5.2.4 N32-f Context Termination Procedure

After the completion of the security capability negotiation procedure and/or the parameter exchange procedures, an N32-f context is established between the two SEPPs. The "n32fContextId" of each SEPP is provided to the other SEPP. This context identifier shall be stored in each SEPP until the context is explicitly terminated by the N32-f context termination procedure. The SEPP that is initiating the N32-f context termination procedure shall use the HTTP method POST on the URI: {apiRoot}/n32c-handshake/v1/n32f-terminate. If a HTTP/2 connection does not exist towards the receiving SEPP, a HTTP/2 connection shall be created before initiating this procedure. The procedure is shown below in Figure 5.2.4-1.



Figure 5.2.4-1: N32f Context Termination Procedure

1. The initiating SEPP issues a HTTP POST request towards the responding SEPP with the request body containing the N32-f context id information that is to be terminated.

2a. On success, the responding SEPP, shall:

- stop sending any further messages over the N32-f towards the initiating SEPP;

- once all the ongoing N32-f message exchanges with the initiating SEPP are completed or timed out, delete the N32-f context identified by the "n32fContextId" provided in the request.

The N32-f HTTP/2 connections from the responding SEPP shall not be deleted if they terminate at an IPX, since that HTTP/2 connection may carry traffic towards other PLMN SEPPs as well. The responding SEPP shall return the status code "200 OK" together with an N32ContextInfo payload body that carries the "n32fContextId" of the initiating SEPP that the responding SEPP has stored.

The initiating SEPP shall:

- stop sending any further messages over the N32-f towards the responding SEPP;

- once all the ongoing N32-f message exchanges with the responding SEPP are completed or timed out, delete the local N32-f context identified by this "n32fContextId".

2b. On failure, the responding SEPP shall return an appropriate 4xx/5xx status code together with the "ProblemDetails" JSON body.

### 5.2.5 N32-f Error Reporting Procedure

When a SEPP is not able to process a message it received over the N32-f interface due to errors, the error information is conveyed to the sending SEPP by using the N32-f error reporting procedure over the N32-c interface. The SEPP that is initiating the N32-f error reporting procedure shall use the HTTP method POST on the URI: {apiRoot}/n32c-handshake/v1/n32f-error. If a HTTP/2 connection does not exist towards the receiving SEPP, a HTTP/2 connection shall be created before initiating this procedure. The procedure is shown below in Figure 5.2.5-1.



Figure 5.2.5-1: N32f Error Reporting Procedure

1. The initiating SEPP issues a HTTP POST request towards the responding SEPP with the request body containing the N32-f error information that is to be reported.

2a. On success, the responding SEPP, shall:

- log that the N32-f request / response message identified by the "messageId" is not processed by the receiving SEPP;

The responding SEPP shall return the status code "204 No Content".

2b. On failure, the responding SEPP shall return an appropriate 4xx/5xx status code together with the "ProblemDetails" JSON body.

## 5.3 JOSE Protected Message Forwarding Procedure on N32 (N32-f)

### 5.3.1 Introduction

The N32-f interface is used between two SEPPs for:

- The forwarding of JOSE protected HTTP/2 messages between the NF service consumer and the NF service producer across two PLMNs, when PRINS is the negotiated security policy. The message forwarding on N32-f shall be based on the negotiated security capability and the exchanged security parameters between the two SEPPs (see clause 5.2).

- Forwarding of the HTTP/2 messages between the NF service consumer and the NF service producer without any reformatting and application layer protection, when TLS is the negotiated security policy.

### 5.3.2 Use of Application Layer Security

#### 5.3.2.1 General

If the negotiated security capability between the two SEPPs is PRINS, one or more HTTP/2 connections between the two SEPPs for the forwarding of JOSE protected message shall be established, which may involve IPX providers on path. The forwarding of messages over the N32-f interface involves the following steps at the sending SEPP:

1. Identification of the protection policy applicable for the API being invoked (i.e either a request/response NF service API or a subscribe/unsubscribe service API or a notification API).

2. Message reformatting as per the identified protection policy.

3. Forwarding of the reformatted message over the N32 interface.

The processing of a message received over the N32-f interface at the receiving IPX provider involves the following steps:

1. Apply the modifications in the "modificationsBlock" appended by the sending IPX provider as JSON patches in the DataToIntegrityProtectBlock (from the decoded "aad" part), if the "modificationsBlock" is received in the message.

2. Determine further modifications required based on modification policy and insert the modification entries in "modificationsBlock".

3. Forwarding the received message with the above inserted modification entries in "modificationsBlock" over the N32 interface.

The processing of a message received over the N32-f interface at the receiving SEPP involves the following steps.

1. Identify the N32-f context using the N32-f context Id received in the message.

2. Verify the integrity protection of the message using the keying material obtained from the TLS layer during the parameter exchange procedure for that N32-f context (see 3GPP TS 33.501 [6]). The TLS connection from which the keying material is obtained is the N32-c TLS connection used for the parameter exchange procedure.

3. Decrypt the ciphertext part of the received JWE message. Decode the "aad" part of the JWE message using BASE64URL decoding.

4. For each entry in the "modificationsBlock" of the received message:

- First verify the integity protection of that entry using the keying material applicable for the IPX that inserted that block (using the "identity" IE in the "modificationsBlock");

- Identify the modifications policy exchanged during the parameter exchange procedure with the sending SEPP if the IPX that inserted the modificationsBlock is from the sending SEPP side; else identify the modifications policy applicable for the IPX based on local configuration;

- Check if the inserted modifications are as per the identified modifications policy;

- Apply the modifications as a JSON patch in the DataToIntegrityProtectBlock (from the decoded "aad" part).

5. Form the original JSON request / response body from the decrypted ciphertext and the decoded integrity verified "aad" block possibly modified as described in step 4.

6. If the reconstructed HTTP message has a "Authorization" header, then the SEPP shall check whether the service consumer's PLMN ID is present in the Bearer token contained in the Authorization header (see 3GPP TS 29.510 [18], clause 6.3.5.2.4) and if it matches with the "Remote PLMN ID" of the N32-f context. If they do not match, the SEPP shall respond to the sending SEPP with "403 Forbidden" status code with the application specific cause set as "PLMNID\_MISMATCH".

NOTE 1: In this case, the N32-f Error Reporting procedure specified in clause 5.2.5 is not used since the processing of the complete N32-f message fails at the receiving SEPP.

NOTE 2: If the service consumer's PLMN ID is present in the reconstructed HTTP message, then the receiving SEPP compares this with the sending SEPP's PLMN ID, which is retrieved from N32f Context (see clause 5.9.3 in 3GPP TS 33.501 [6]). See the above step 6 for the receiving SEPP behaviour. If the service consumer's PLMN ID is not present, the comparison is not done.

SEPPs and IPX should support gzip coding (see IETF RFC 1952 [23]) in HTTP requests and responses and indicate so in the Accept-Encoding header, as described in clause 6.9 of 3GPP TS 29.500 [4] and clause 6.2.2.2.3.

#### 5.3.2.2 Protection Policy Lookup

When a SEPP receives a HTTP/2 request or response message intended to be routed towards another PLMN, the sending SEPP shall identify the protection policy as given below

1. Identify the target PLMN from the ":aurthority" part of the message using the format specified in clause 6.1.4.3 of 3GPP TS 29.500 [4].

2. Check if the incoming HTTP/2 message has the "3gpp-Sbi-Callback" header. When present, the SEPP shall select the data encryption and modification policy applicable for the specific notification type, identified by the value of the "3gpp-Sbi-Callback" header and the target PLMN, using the notification type list stored as specified in subclase 5.2.3.3.

3. Else, if it is a HTTP/2 request message, then from the ":authority" and ":path" part of the received HTTP/2 request message, form the API URI. For the identified PLMN, check if a protection policy exists for the API URI using the table stored as specified in clause 5.2.3.3.

4. Else, if it is a HTTP/2 response message, then based on the HTTP/2 stream ID on which the response is received, identify the corresponding request that was sent by the SEPP and the protection policy applicable for that request, as specified in step 3.

5. If an entry is not found, then it means that either the particular API has no protection policy exchanged.

Once a protection policy is identified, the SEPP shall apply the application layer security as per the identified protection policy.

#### 5.3.2.3 Message Reformatting

A SEPP on the sending side PLMN applies message reformatting in the following cases:

- When it receives a HTTP/2 request message from an NF service consumer to a an NF service producer in another PLMN;

- When it receives a response HTTP/2 response message from an NF service producer to an NF service consumer in another PLMN.

- When it receives a HTTP/2 notification request message from an NF service producer to an NF service consumer in another PLMN;

- When it receives a HTTP/2 notification response message from an NF service consumer to an NF service producer in another PLMN

The SEPP shall reformat the HTTP/2 message by encapsulating the whole message into the body of a new HTTP POST message. The body of the HTTP POST request / response message shall contain the reformatted original HTTP/2 request/response message respectively. The HTTP POST request/response body shall be encoded as the "N32fReformattedReqMsg"/"N32fReformattedRspMsg" JSON bodies respectively, as specified in clause 6.2.5.

The "N32fReformattedReqMsg"/"N32fReformattedRspMsg" are structured as given below:



Figure 5.3.2.3-1 JSON representation of a reformatted HTTP message

The "cipherText" part of the reformatted message in FlatJweJson shall be prepared as given below



Figure 5.3.2.3-2 Transformation of HTTP Header and Payload to Encrypt into CipherText

1. Based on the protection policy exchanged between the SEPPs, the sending SEPP prepares an input for the JWE ciphering and integrity protection as an array of arbitrary types in the "DataToIntegrityProtectAndCipher" block with each entry containing either a HTTP header value or the value of a JSON payload IE of the API message being reformatted. The index value "encBlockIdx" in the payload part of DataToIntegrityProtectBlock shall point to the index of a header value or IE value in this input array.

2. The input block is fed into an encryption function along with the other required inputs for JWE as specified in IETF RFC 7516 [14].

3. The encryption function outputs the cipher text information. This cipher text is then subjected to BASE64URL transformation as specified in IETF RFC 4648 [15] clause 5.

4. The output of the BASE64URL transform is them encoded as the ciphertext part of FlatJweJson IE specified in clause 6.2.5.2.11.

#### 5.3.2.4 Message Forwarding to Peer SEPP

Once a SEPP reformats the HTTP/2 message into the "N32ReformattedReqMsg"/"N32ReformattedRspMsg" JSON object as specified in clause 5.3.2, the SEPP forwards the message to the receiving SEPP by invoking a HTTP POST method as shown in figure 5.3.2.4-1 below.



Figure 5.3.2.4-1 Message Forwarding between SEPP on N32-f

1. The initiating SEPP issues a HTTP POST request towards the responding SEPP with the request body containing the "N32ReformattedReqMsg" IE carrying the reformatted HTTP/2 message. The request message shall contain the "n32fContextId" information provided by the responding SEPP to the initiating SEPP earlier during the parameter exchange procedure (see clause 5.2.3). The responding SEPP shall use the "n32fContextId" information to:

- Locate the agreed cipher suite and protection policy;

- Locate the n32ContextId to be used in the response.

The HTTP request payload may be compressed hop by hop over N32-f, if the initiating SEPP or IPX and its next hop (IPX or SEPP) support gzip coding (see IETF RFC 1952 [23]).

2a. On successful processing of the request, the responding SEPP shall:

- decompress the N32-f HTTP request payload, if it is compressed;

- reconstruct the HTTP/2 message towards the NF service producer;

- compress the reconstructed HTTP request if the reconstructed HTTP payload contains a Content-Encoding header indicating gzip compression;

- forward the reconstructed HTTP/2 message to the NF service producer;

- wait for the response from the NF service producer; and then

- once the response from the NF service producer is received, respond to the initiating SEPP with a "200 OK" status code and a POST response body that contains the "N32ReformattedRspMsg". The "N32ReformattedRspMsg" shall contain the reformatted HTTP response message from the responding PLMN. The response message shall contain the "n32fContextId" information provided by the initiating SEPP to the responding SEPP earlier during the parameter exchange procedure (see clause 5.2.3).

NOTE 1: For unsuccessful processing of the request see clause 5.3.2.1.

The responding SEPP shall be able to map the response received from the NF service producer to the HTTP/2 stream ID for the corresponding response it needs to generate towards the initiating SEPP. The HTTP/2 stream ID and the HTTP/2 connection information on either side shall be used to derive this mapping.

The HTTP response payload may be compressed hop by hop over N32-f, if the responding SEPP or IPX and its next hop (IPX or SEPP) support gzip coding (see IETF RFC 1952 [23]).

2b. On failure, the responding SEPP shall respond to the initiating SEPP with an appropriate 4xx/5xx status code as specified in clause 6.2.4.2.

### 5.3.3 Message Forwarding to Peer SEPP when TLS is used

When the negotiated security policy between the SEPPs is TLS, then the procedures described in clause 5.3.2 shall not be applied. Messages shall be forwarded to the peer SEPP as specified in clause 6.1.4.3.4 of 3GPP TS 29.500 [4].

### 5.3.4 JOSE Protected Forwarding Options

The JOSE Protected Forwarding Options is used by the sending SEPP or IPX to discover the communication options supported by its next hop (IPX or SEPP) for N32-f message processing.



Figure 5.3.4-1: Procedure for the discovery of communication options supported by the next hop

1. The sending SEPP or IPX shall send an OPTIONS request to discover the communication options supported by its next hop (IPX or SEPP) for N32-f message processing.

2. If the request is accepted, the next hop (IPX or SEPP) shall respond with the status code 204 No Content and include an Accept-Encoding header (as described in IETF RFC 7694 [24]).

On failure, the next hop shall return one of the HTTP status code listed in Table 6.2.4.3.2.1-3.

## 5.4 Nsepp\_Telescopic\_FQDN\_Mapping Service

### 5.4.1 General

The Nsepp\_Telescopic\_FQDN\_Mapping service is used between any Network Function and the SEPPs in the same PLMN, if TLS protection between the Network Function and the SEPP relies on using telescopic FQDN. See clause 28.5.2 of 3GPP TS 23.003 [19] and clause 6.1.4.3 of 3GPP TS 29.500 [4]) for the definition and use of Telescopic FQDN.

### 5.4.2 Foreign FQDN to Telescopic FQDN Mapping Procedure

This procedure is initiated by an NF Service Consumer (typically an NRF or an NSSF) that needs to interact with a NF in a foreign PLMN (typically the corresponding NRF or NSSF), and to do so, it needs to build a telescopic FQDN of said NF (i.e. concatenation of the FQDN of the foreign FQDN, and the FQDN of the local SEPP), and then the resulting telescopic FQDN needs to be "flattened" (i.e. the FQDN of the NF in the foreign PLMN needs to be converted to a singel label). The procedure is described in Figure 5.4.2-1 below.



Figure 5.4.2-1: Foreign FQDN to Telescopic FQDN Mapping Procedure

1. The NF Service Consumer issues an HTTP GET request towards the local SEPP with a query parameter "foreign-fqdn" containing the FQDN of the NF in the foreign PLMN, that needs to be transformed into a flattened telescopic FQDN.

2a. On successful processing of the request, the responding SEPP shall respond to the NF Service Consumer with a "200 OK" status code and a response body that contains a JSON object of type "TelescopicMapping", containing as attributes the label to be used as first label in the telescopic FQDN, and the domain of the local SEPP to be appended after such first label. The resulting FQDN shall be used by the NF Consumer to setup a TLS session terminated in the local SEPP, where the SEPP shall present a server certificate with a wildcard domain matching the returned telescopic FQDN.

### 5.4.3 Telescopic FQDN to Foreign FQDN Mapping Procedure

This procedure is initiated by an NF Service Consumer (typically another SEPP) that has received a service request with an unknown first label of a telescopic FQDN. Typically, this SEPP may interact with other SEPPs in the same PLMN in order to determine if there is an existing mapping for a given label to an FQDN of a foreign FQDN; this procedure is only expected to be used when multiple SEPPs are deployed in a PLMN. The procedure is described in Figure 5.4.3-1 below.



Figure 5.4.3-1: Foreign FQDN to Telescopic FQDN Mapping Procedure

1. The NF Service Consumer issues an HTTP GET request towards another SEPP with a query parameter "telescopic-label" containing the first label of a given telescopic FQDN, whose mapping towards an FQDN of an NF in a foreign PLMN needs to be verified.

2a. On successful processing of the request, the responding SEPP shall respond to the NF Service Consumer with a "200 OK" status code and a response body that contains a JSON object of type "TelescopicMapping", containing as attribute "foreignFqdn", containing the FQDN of the NF in the foreign PLMN.

# 6 API Definitions

## 6.1 N32 Handshake API

### 6.1.1 API URI

URIs of this API shall have the following root:

{apiRoot}/{apiName}/{apiVersion}/

where "apiRoot" is defined in clause 4.4.1 of 3GPP TS 29.501 [5], the "apiName" shall be set to "n32c -handshake" and the "apiVersion" shall be set to "v1" for the current version of this specification.

### 6.1.2 Usage of HTTP

#### 6.1.2.1 General

HTTP/2, as defined in IETF RFC 7540 [7], shall be used as specified in clause 4.3.2.1.

HTTP/2 shall be transported as specified in clause 4.3.3.

HTTP messages and bodies for the N32 handshake API shall comply with the OpenAPI [15] specification contained in Annex A.

#### 6.1.2.2 HTTP standard headers

##### 6.1.2.2.1 General

The HTTP standard headers as specified in clause 4.3.2.2 shall be supported for this API.

##### 6.1.2.2.2 Content type

The following content types shall be supported:

- the JSON format (see IETF RFC 8259 [8]). The use of the JSON format shall be signalled by the content type "application/json". See also clause 5.3.4.

- the Problem Details JSON Object (see IETF RFC 7807 [22]). The use of the Problem Details JSON object in a HTTP response body shall be signalled by the content type "application/problem+json".

#### 6.1.2.3 HTTP custom headers

##### 6.1.2.3.1 General

In this release of the specification, no specific custom headers are defined for the N32 handshake API.

For 3GPP specific HTTP custom headers used across all service based interfaces, see clause 4.3.2.3.

### 6.1.3 Resources

#### 6.1.3.1 Overview

There are no resources in this version of the N32 handshake API. All the operations are realized as custom operations without resources.

### 6.1.4 Custom Operations without Associated Resources

#### 6.1.4.1 Overview

Table 6.1.4.1-1: Custom operations without associated resources

|  |  |  |  |
| --- | --- | --- | --- |
| Operation Name | Custom operation URI | Mapped HTTP method | Description |
| Security Capability Negotiation | /exchange-capability | POST | This is the N32 capability exchange API used to negotiate the security capabilities between SEPPs. |
| Parameter Exchange | /exchange-params | POST | This is the N32 parameter exchange API used to exchange the cipher suites and protection policies. |
| N32-f Context Terminate | /n32f-terminate | POST | This is the N32-f context termination procedure API. |
| N32-f Error Reporting | /n32f-error | POST | This is the N32-f error reporting procedure API. |

#### 6.1.4.2 Operation: Security Capability Negotiation

##### 6.1.4.2.1 Description

This custom operation is used between the SEPPs to negotiate their security capabilities. The HTTP method POST shall be used on the following URI:

URI: {apiRoot}/n32c-handshake/v1/exchange-capability

This operation shall support the resource URI variables defined in table 6.1.4.2.1-1.

Table 6.1.4.2.1-1: Resource URI variables for this Operation

|  |  |  |
| --- | --- | --- |
| Name | Data type | Definition |
| apiRoot | string | See clause 6.1.1. |

##### 6.1.4.2.2 Operation Definition

This operation shall support the request data structures and response codes specified in tables 6.2.4.2.2-1 and 6.2.4.2.2-2.

Table 6.1.4.2.2-1: Data structures supported by the POST Request Body

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| SecNegotiateReqData | M | 1 | The IE shall contain the security capabilities of the initiating SEPP. |

Table 6.1.4.2.2-2: Data structures supported by the POST Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  codes | Description |
| SecNegotiateRspData | M | 1 | 200 OK | This represents the successful processing of the requested security capabilities. The responding SEPP shall provide the security capabilities that it has selected, in the response. |
| NOTE: The mandatory HTTP error status codes for the POST method listed in Table 5.2.7.1-1 of 3GPP TS 29.500 [4] other than those specified in the table above also apply, with a ProblemDetails data type (see clause 5.2.7 of 3GPP TS 29.500 [4]). | | | | |

#### 6.1.4.3 Operation: Parameter Exchange

##### 6.1.4.3.1 Description

This custom operation is used between the SEPPs to exchange the parameters for the N32-f connection. The HTTP method POST shall be used on the following URI:

URI: {apiRoot}/n32c-handshake/v1/exchange-params

This operation shall support the resource URI variables defined in table 6.1.4.3.1-1.

Table 6.1.4.3.1-1: Resource URI variables for this Operation

|  |  |  |
| --- | --- | --- |
| Name | Data type | Definition |
| apiRoot | string | See clause 6.1.1. |

##### 6.1.4.3.2 Operation Definition

This operation shall support the request data structures and response codes specified in tables 6.1.4.3.2-1 and 6.1.4.3.2-2.

Table 6.1.4.3.2-1: Data structures supported by the POST Request Body

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| SecParamExchReqData | M | 1 | The IE shall contain the parameters requested by the requesting SEPP. |

Table 6.1.4.3.2-2: Data structures supported by the POST Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  codes | Description |
| SecParamExchRspData | M | 1 | 200 OK | This represents the successful processing of the requested parameters. The SEPP shall provide the selected parameters (i.e selected cipher suite and/or selected data type encryption policy) depending on what was requested by the requesting SEPP and what is supported by the responding SEPP, or the SEPP shall provide the modification policy and/or security information lists of the connected IPXs. |
| ProblemDetails | O | 0..1 | 409 Conflict | The "cause" attribute may be used to indicate one of the following application errors:  - REQUESTED\_PARAM\_MISMATCH |
| NOTE: The mandatory HTTP error status codes for the POST method listed in Table 5.2.7.1-1 of 3GPP TS 29.500 [4] other than those specified in the table above also apply, with a ProblemDetails data type (see clause 5.2.7 of 3GPP TS 29.500 [4]). | | | | |

#### 6.1.4.4 Operation: N32-f Context Terminate

##### 6.1.4.4.1 Description

This custom operation is used between the SEPPs to terminate an N32-f context. The HTTP method POST shall be used on the following URI:

URI: {apiRoot}/n32c-handshake/v1/n32f-terminate

This operation shall support the resource URI variables defined in table 6.1.4.3.1-1.

Table 6.1.4.4.1-1: Resource URI variables for this Operation

|  |  |  |
| --- | --- | --- |
| Name | Data type | Definition |
| apiRoot | string | See clause 6.1.1. |

##### 6.1.4.4.2 Operation Definition

This operation shall support the request data structures and response codes specified in tables 6.1.4.4.2-1 and 6.1.4.4.2-2.

Table 6.1.4.4.2-1: Data structures supported by the POST Request Body

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| N32fContextInfo | M | 1 | The IE shall contain the information about the N32-f context requested to be terminated by the requesting SEPP. |

Table 6.1.4.4.2-2: Data structures supported by the POST Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  codes | Description |
| N32fContextInfo | M | 1 | 200 OK | This represents the successful deletion of the request N32-f context. The responding SEPP shall return the "n32fContextId" it had towards the initiating SEPP, in this IE. |
| NOTE: The mandatory HTTP error status codes for the POST method listed in Table 5.2.7.1-1 of 3GPP TS 29.500 [4] other than those specified in the table above also apply, with a ProblemDetails data type (see clause 5.2.7 of 3GPP TS 29.500 [4]). | | | | |

#### 6.1.4.5 Operation: N32-f Error Reporting

##### 6.1.4.5.1 Description

This custom operation is used between the SEPPs to report errors identified while processing the messages received on N32-f. The HTTP method POST shall be used on the following URI:

URI: **{apiRoot}/n32c-handshake/v1/n32f-error**

This operation shall support the resource URI variables defined in table 6.1.4.5.1-1.

Table 6.1.4.5.1-1: Resource URI variables for this Operation

|  |  |  |
| --- | --- | --- |
| Name | Data type | Definition |
| apiRoot | string | See clause 6.1.1. |

##### 6.1.4.5.2 Operation Definition

This operation shall support the request data structures and response codes specified in tables 6.1.4.5.2-1 and 6.1.4.5.2-2.

Table 6.1.4.5.2-1: Data structures supported by the POST Request Body

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| N32fErrorInfo | M | 1 | The IE shall contain the information about the N32-f message that failed to process at the SEPP initiating the N32-f error reporting procedure, together with information related to the nature of the error. |

Table 6.1.4.5.2-2: Data structures supported by the POST Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  codes | Description |
|  |  |  | 204 No Content | This represents the successful processing of the N32-f error report at the receiving SEPP. |
| NOTE: The mandatory HTTP error status codes for the POST method listed in Table 5.2.7.1-1 of 3GPP TS 29.500 [4] other than those specified in the table above also apply, with a ProblemDetails data type (see clause 5.2.7 of 3GPP TS 29.500 [4]). | | | | |

### 6.1.5 Data Model

#### 6.1.5.1 General

This clause specifies the application data model supported by the API.

Table 6.1.5.1-1 specifies the data types defined for the N32 interface.

Table 6.1.5.1-1: N32 specific Data Types

|  |  |  |
| --- | --- | --- |
| Data type | Clause defined | Description |
| SecNegotiateReqData | 6.1.5.2.2 | Defines the security capabilities of a SEPP sent to a receiving SEPP. |
| SecNegotiateRspData | 6.1.5.2.3 | Defines the selected security capabilities by a SEPP. |
| SecurityCapability | 6.1.5.3.3 | Enumeration of security capabilities. |
| SecParamExchReqData | 6.1.5.2.4 | Request data structure for parameter exchange |
| SecParamExchRspData | 6.1.5.2.5 | Response data structure for parameter exchange |
| ProtectionPolicy | 6.1.5.2.6 | The protection policy to be negotiated between the SEPPs. |
| ApiIeMapping | 6.1.5.2.7 | API URI to IE mapping on which the protection policy needs to be applied. |
| IeInfo | 6.1.5.2.8 |  |
| ApiSignature | 6.1.5.2.9 |  |
| N32fContextInfo | 6.1.5.2.10 | N32-f context information |
| N32fErrorInfo | 6.1.5.2.11 | N32-f error information. |
| FailedModificationInfo | 6.1.5.2.12 | Information on N32-f modifications block that failed to process. |
| N32fErrorDetail | 6.1.5.2.13 | Details about the N32f error. |
| CallbackName | 6.1.5.2.14 | Callback Name. |
| IpxProviderSecInfo | 6.1.5.2.15 | Defines the security information list of an IPX. |
| HttpMethod | 6.1.5.3.4 | Enumeration of HTTP methods. |
| IeType | 6.1.5.3.5 | Enumeration of types of IEs (i.e kind of IE) to specify the protection policy. |
| IeLocation | 6.1.5.3.6 | Location of the IE in a HTTP message. |
| N32fErrorType | 6.1.5.3.7 | Type of error while processing N32-f message. |
| FailureReason | 6.1.5.3.8 | Reason for failure to reconstruct a HTTP/2 message from N32-f message. |

Table 6.1.5.1-2 specifies data types re-used by the N32 interface protocol from other specifications, including a reference to their respective specifications and when needed, a short description of their use within the Namf service based interface.

Table 6.1.5.1-2: N32 re-used Data Types

|  |  |  |
| --- | --- | --- |
| Data type | Reference | Comments |
| Fqdn | 3GPP TS 29.510 [18] |  |

#### 6.1.5.2 Structured data types

##### 6.1.5.2.1 Introduction

This clause defines the structures to be used in the N32 Handshake API.

##### 6.1.5.2.2 Type: SecNegotiateReqData

Table 6.1.5.2.2-1: Definition of type SecNegotiateReqData

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| sender | Fqdn | M | 1 | This IE shall uniquely identify the SEPP that is sending the request. This IE is used to store the negotiated security capability against the right SEPP. |
| supportedSecCapabilityList | array(SecurityCapability) | M | 1..N | This IE shall contain the list of security capabilities that the requesting SEPP supports. |
| 3GppSbiTargetApiRootSupported | boolean | C | 0..1 | This IE should be present and indicate that the 3gpp-Sbi-Target-apiRoot HTTP header is supported, if TLS security is supported for N32f message forwarding.  When present, it shall indicate if TLS security using the 3gpp-Sbi-Target-apiRoot HTTP header is supported:  - true: supported  - false (default): not supported |
| plmnIdList | array(PlmnId) | O | 1..N | A list of PLMN IDs associated with the SEPP, which is sending the request. The list to be stored by the receiving SEPP in a N32-f Context (see clause 5.9.3 in 3GPP TS 33.501 [6]) |
| targetPlmnId | PlmnId | O | 1 | When present, this IE shall contain a PLMN ID of the target SEPP.  See clause 5.2.2 step 1. |

##### 6.1.5.2.3 Type: SecNegotiateRspData

Table 6.1.5.2.3-1: Definition of type SecNegotiateRspData

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| sender | Fqdn | M | 1 | This IE shall uniquely identify the SEPP that is sending the response. This IE is used to store the negotiated security capability against the right SEPP. |
| selectedSecCapability | SecurityCapability | M | 1 | This IE shall contain the security capability selected by the responding SEPP. |
| 3GppSbiTargetApiRootSupported | boolean | C | 0..1 | This IE should be present and indicate that the 3gpp-Sbi-Target-apiRoot HTTP header is supported, if TLS security is negotiated for N32f message forwarding and the initiating SEPP indicated support of this header.  When present, it shall indicate if TLS security using the 3gpp-Sbi-Target-apiRoot HTTP header is supported:  - true: supported  - false (default): not supported |
| plmnIdList | array(PlmnId) | O | 1..N | A list of PLMN IDs of a single PLMN associated with the SEPP, which is sending the response. The list to be stored by the receiving SEPP in a N32-f Context (see clause 5.9.3 in 3GPP TS 33.501 [6]).  If different PLMNs are represented by different PLMN IDs supported by a SEPP, then the SEPP shall select the PLMN as specified in clause 5.2.2 step 2a. |

##### 6.1.5.2.4 Type: SecParamExchReqData

Table 6.1.5.2.4-1: Definition of type SecParamExchReqData

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| n32fContextId | string | M | 1 | This IE shall contain the context identifier to be used by the responding SEPP for subsequent JOSE protected message forwarding procedure over N32-f towards the initiating SEPP. The initiating SEPP shall use this context identifier to locate the cipher suite and protection policy exchanged and agreed to be used with the responding SEPP, for the message forwarding procedure over N32-f.  The n32fContextId shall encode a 64-bit integer in hexadecimal representation. Each character in the string shall take a value of "0" to "9" or "A" to "F" and shall represent 4 bits. The most significant character representing the 4 most significant bits of the N32-f context Id shall appear first in the string, and the character representing the 4 least significant bit of the N32-f context Id shall appear last in the string.  Pattern: '^[A-Fa-f0-9]{16}$'  Example: "0600AD1855BD6007". |
| jweCipherSuiteList | array(string) | C | 1..N | This IE shall be present during the parameter exchange procedure for cipher suite negotiation (see clause 5.2.3.2). When present, this IE shall contain the ordered list of JWE cipher suites supported by the requesting SEPP. Valid values for the string are as specified in clause 5.1 of IETF RFC 7518 [13]. |
| jwsCipherSuiteList | array(string) | C | 1..N | This IE shall be present during the parameter exchange procedure for cipher suite negotiation (see clause 5.2.3.2). When present, this IE shall contain the ordered list of JWS cipher suites supported by the requesting SEPP. Valid values for the string are as specified in clause 3.1 of IETF RFC 7518 [13]. |
| protectionPolicyInfo | ProtectionPolicy | C | 0..1 | This IE shall be present during the parameter exchange procedure for protection policy exchange (see clause 5.2.3.3). When present, this IE shall contain the data type encryption policy requested by the requesting SEPP and/or the modification policy supported by the IPX(s) on the side of the requesting SEPP. |
| ipxProviderSecInfoList | array(IpxProviderSecInfo) | C | 1..N | This IE includes the list of IPX security information. |
| sender | Fqdn | C | 0..1 | This IE shall be present if the Parameter Exchange request is sent on a different N32-c HTTP connection than the one used to perform the Security Capability Negotiation procedure. It may be present otherwise.  When present, it shall uniquely identify the SEPP that is sending the request. This IE is used to store the exchanged parameters against the right SEPP. |

##### 6.1.5.2.5 Type: SecParamExchRspData

Table 6.1.5.2.5-1: Definition of type SecParamExchRspData

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| n32fContextId | string | M | 1 | This IE shall contain the context identifier to be used by the initiating SEPP for subsequent JOSE protected message forwarding procedure over N32-f towards the responding SEPP. The responding SEPP shall use this context identifier to locate the cipher suite and protection policy exchanged and agreed to be used with the initiating SEPP, for the message forwarding procedure over N32-f.  The n32fContextId shall encode a 64-bit integer in hexadecimal representation. Each character in the string shall take a value of "0" to "9" or "A" to "F" and shall represent 4 bits. The most significant character representing the 4 most significant bits of the N32-f context Id shall appear first in the string, and the character representing the 4 least significant bit of the N32-f context Id shall appear last in the string.  Pattern: '^[A-Fa-f0-9]{16}$'  Example: "0600AD1855BD6007". |
| selectedJweCipherSuite | string | C | 1 | This IE shall be present during the parameter exchange procedure for cipher suite negotiation (see clause 5.2.3.2). When present, this IE shall contain the JWE cipher suite selected by the responding SEPP. |
| selectedJwsCipherSuite | string | C | 1 | This IE shall be present during the parameter exchange procedure for cipher suite negotiation (see clause 5.2.3.2). When present, this IE shall contain the JWS cipher suite selected by the responding SEPP. |
| selProtectionPolicyInfo | ProtectionPolicy | C | 0..1 | This IE shall be present during the parameter exchange procedure for protection policy exchange (see clause 5.2.3.3). When present, this IE shall contain the data type encryption policy selected by the responding SEPP and/or the modification policy supported by the IPX(s) on the side of the responding SEPP. |
| ipxProviderSecInfoList | array(IpxProviderSecInfo) | C | 1..N | This IE includes the list of IPX security information. |
| sender | Fqdn | C | 0..1 | This IE shall be present if the Parameter Exchange response is sent on a different N32-c HTTP connection than the one used to perform the Security Capability Negotiation procedure. It may be present otherwise.  When present, it shall uniquely identify the SEPP that is sending the response. This IE is used to store the exchanged parameters against the right SEPP. |

##### 6.1.5.2.6 Type: ProtectionPolicy

Table 6.1.5.2.6-1: Definition of type ProtectionPolicy

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| apiIeMappingList | array(ApiIeMapping) | M | 1..N | Contains an array of API URI to IE type - IE name mapping. The mapping includes an indication against each IE if that IE is allowed to be modified by the IPX on the side of the SEPP or not. |
| dataTypeEncPolicy | array(IeType) | C | 1..N | This IE shall be present when the SEPPs need to exchange the IE protection policies. When present, this IE shall contain the list of IE types that the SEPP intends to protect by ciphering. |

##### 6.1.5.2.7 Type: ApiIeMapping

Table 6.1.5.2.7-1: Definition of type ApiIeMapping

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| apiSignature | ApiSignature | M | 1 | This IE shall contain:  - The API URI of the NF service operations following request/response semantic; or  - The API URI of the subscribe / unsubscribe service operation |
| apiMethod | HttpMethod | M | 1 | This IE shall contain the HTTP method used by the API. |
| IeList | array(IeInfo) | M | 1..N | This IE shall contain the array of Ies in the API. |

##### 6.1.5.2.8 Type: IeInfo

Table 6.1.5.2.8-1: Definition of type IeInfo

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| ieLoc | IeLocation | M | 1 | This IE shall contain the location of the IE mentioned in "reqBodyIePath" or "rspBodyIePath" (i.e URI parameter or JSON body or multipart message) |
| ieType | IeType | M | 1 | This IE shall contain the type of the IE, representing the nature of the information the IE is carrying. |
| reqIe | string | C | 0..1 | This IE shall be included when the Ies in HTTP/2 request messages of an API need to be protected when forwarded over N32-f. When present, this IE shall contain:  - The JSON pointer representation of the IE to be protected, if the "ieLoc" indicates "BODY". Only the JSON pointer of the leaf IEs are included;  - The name of the URI query attribute to be protected, if the "ieLoc" indicates "URI\_PARAM";  - The name of the HTTP header, if the "ieLoc" indicates "HEADER";  - The JSON pointer representation of the attribute defined with the RefToBinaryData type if the "ieLoc" indicates "MULTIPART\_BINARY". It shall be encoded as: <JSON Pointer of the attribute defined with the RefToBinaryData type>/data. |
| rspIe | string | C | 0..1 | This IE shall be included when the IEs in HTTP/2 response messages of an API need to be protected when forwarded over N32-f. When present, this IE shall contain:  - The JSON pointer representation of the IE to be protected, if the "ieLoc" indicates "BODY". Only the JSON pointer of the leaf IEs are included;  - The name of the URI query attribute to be protected, if the "ieLoc" indicates "URI\_PARAM";  - The name of the HTTP header, if the "ieLoc" indicates "HEADER";  - The JSON pointer representation of the attribute defined with the RefToBinaryData type if the "ieLoc" indicates "MULTIPART\_BINARY". It shall be encoded as: <JSON Pointer of the attribute defined with the RefToBinaryData type>/data. |
| isModifiable | boolean | C | 0..1 | This IE shall be included if the IE is allowed to be modified by all IPX(s) on the side of the SEPP sending the API IE mapping. When present,  - true, indicates that the IE is allowed to be modified by all IPX(s) on the side of the SEPP;  - false, indicates that the IE is not allowed to be modified by any IPX on the side of the SEPP;  - default is false.  When the IE is not included, the default value shall be applied.  (NOTE) |
| isModifiableByIpx | map(boolean) | C | 0..1 | This IE shall be included if the IE is allowed to be modified by some of (but not all) the IPX(s) on the side of the SEPP sending the API IE mapping. The key of the map is the *ipxProviderId* for which the boolean applies.  When present, each element carries the isModifiable indication for the IPX indicated by the key.  (NOTE) |
| NOTE: Either isModifiable or isModifiableByIpx may be present, but not both. | | | | |

##### 6.1.5.2.9 Type: ApiSignature

Table 6.1.5.2.9-1: Definition of type ApiSignature as a list of "mutually exclusive alternatives"

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Cardinality | Description | Applicability |
| Uri | 1 | API URI of a request/response or subscribe/unsubscribe NF service operation as specified in the respective API specification with the variable parts other than {apiVersion} unresolved.  Examples:  "{apiRoot}/nsmf-pdusession/v1/sm-contexts", for the SMF PDUSession Create SM Context service operation.  "{apiRoot}/nsmf-pdusession/v1/sm-contexts/{smContextRef}/modify", for the SMF PDUSession Update SM Context service operation.  . |  |
| CallbackName | 1 | A value identifying the type of callback. |  |

##### 6.1.5.2.10 Type: N32fContextInfo

Table 6.1.5.2.10-1: Definition of type N32fContextInfo

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| n32fContextId | string | M | 1 | This IE shall contain the N32-f context identifier of the receiving SEPP.  The n32fContextId shall encode a 64-bit integer in hexadecimal representation. Each character in the string shall take a value of "0" to "9" or "A" to "F" and shall represent 4 bits. The most significant character representing the 4 most significant bits of the N32-f context Id shall appear first in the string, and the character representing the 4 least significant bit of the N32-f context Id shall appear last in the string.  Pattern: '^[A-Fa-f0-9]{16}$'  Example: "0600AD1855BD6007". |

##### 6.1.5.2.11 Type: N32fErrorInfo

Table 6.1.5.2.11-1: Definition of type N32fErrorInfo

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| n32fMessageId | string | M | 1 | This IE shall contain the N32-f message identifier received over N32-f (see clause 6.2.5.2.9). |
| n32fErrorType | N32fErrorType | M | 1 | This IE shall contain the type of processing error encountered by the SEPP initiating the N32-f error reporting procedure. |
| failedModificationList | array(FailedModificationInfo) | C | 1..N | This IE shall be present if the n32ErrorType is "INTEGRITY\_CHECK\_ON\_MODIFICATIONS\_FAILED" or "MODIFICATIONS\_INSTRUCTIONS\_FAILED". When present this IE shall contain a list of FQDNs of the IPX-es whose inserted modifications failed to process at the SEPP initiating the N32-f error reporting procedure, together with the reason for the failure to process. |
| errorDetailsList | array(N32fErrorDetail) | O | 1..N | This IE may be included when the n32ErrorType IE indicates "MESSAGE\_RECONSTRUCTION\_FAILED ". When present, this IE shall contain a list of JSON pointers to the IEs that failed to process together with the reason for the failure to process that IE. |

##### 6.1.5.2.12 Type: FailedModificationInfo

Table 6.1.5.2.12-1: Definition of type FailedModificationInfo

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| ipxId | Fqdn | M | 1 | This IE shall identify the IPX. |
| n32fErrorType | N32fErrorType | M | 1 | This IE shall contain the type of processing error on the modifications block, encountered by the SEPP initiating the N32-f error reporting procedure. The value shall be one of the following:  INTEGRITY\_CHECK\_ON\_MODIFICATIONS\_FAILED;  MODIFICATIONS\_INSTRUCTIONS\_FAILED |

##### 6.1.5.2.13 Type: N32fErrorDetail

Table 6.1.5.2.13-1: Definition of type N32fErrorDetail

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| attribute | string | M | 1 | Contains either a HTTP header name or the JSON pointer of an attribute within the N32-f message that failed to reconstruct. The value shall be one of the values of the iePath attribtue (see clause 6.2.5.2.8) in the received N32-f message. |
| msgReconstructFailReason | FailureReason | M | 1 | Indicates the reason for the failure to reconstruct the attribute. |

##### 6.1.5.2.14 Type: CallbackName

Table 6.1.5.2.14-1: Definition of type CallbackName

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| callbackType | string | M | 1 | This IE shall contain a string identifying the type of callback. The value shall be one of the values specified in 3GPP 29.500 [4], Annex B. |

##### 6.1.5.2.15 Type: IpxProviderSecInfo

Table 6.1.5.2.15-1: Definition of type IpxProviderSecInfo

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| ipxProviderId | Fqdn | M | 1 | This IE shall uniquely identify the IPX. |
| rawPublicKeyList | array(string) | C | 1..N | This IE includes the list of raw public keys for the IPX.  When present, each array item shall contain a raw public key for the IPX, with textual encoding as specified in clause 13 of IETF RFC 7468 [21]. |
| certificateList | array(string) | C | 1..N | This IE includes the list of certificates for the IPX.  When present, each array item shall contain a certificate for the IPX, with textual encoding as specified in IETF RFC 7468 [21]. |
| NOTE: Either the rawPublicKeyList attribute, or the certificateList attribute, shall be present. | | | | |

#### 6.1.5.3 Simple data types and enumerations

##### 6.1.5.3.1 Introduction

This clause defines simple data types and enumerations that can be referenced from data structures defined in the previous clauses.

##### 6.1.5.3.2 Simple data types

The simple data types defined in table 6.1.5.3.2-1 shall be supported.

Table 6.1.5.3.2-1: Simple data types

|  |  |  |
| --- | --- | --- |
| Type Name | Type Definition | Description |
|  |  |  |

##### 6.1.5.3.3 Enumeration: SecurityCapability

Table 6.1.5.3.3-1: Enumeration SecurityCapability

|  |  |
| --- | --- |
| Enumeration value | Description |
| "TLS" | TLS security. |
| "PRINS" | PRotocol for N32 INterconnect Security. |

##### 6.1.5.3.4 Enumeration: HttpMethod

Table 6.1.5.3.4-1: Enumeration HttpMethod

|  |  |
| --- | --- |
| Enumeration value | Description |
| "GET" | HTTP GET Method. |
| "PUT" | HTTP PUT Method. |
| "POST" | HTTP POST Method. |
| "DELETE" | HTTP DELETE Method. |
| "PATCH" | HTTP PATCH Method. |
| "HEAD" | HTTP HEAD Method. |
| "OPTIONS" | HTTP OPTIONS Method. |
| "CONNECT" | HTTP CONNECT Method. |
| "TRACE" | HTTP TRACE Method. |

##### 6.1.5.3.5 Enumeration: IeType

Table 6.1.5.3.5-1: Enumeration IeType

|  |  |
| --- | --- |
| Enumeration value | Description |
| "UEID" | These are IEs which carry the UE identity (i.e. SUPI and GPSI). This also includes the long-lasting identity Charging ID.  An example of a UEID IE is gpsi IE defined in 3GPP TS 29.518 [25]. |
| "LOCATION" | These are IEs which carry location information (i.e. cell-id and TAI).  An example of a LOCATION IE is ncgi IE defined in 3GPP TS 29.571 [12]. |
| "KEY\_MATERIAL" | These are IEs which carry keying material as KSEAF and UPU related information.  An example of a KEY\_MATERIAL IE is upuInfo IE defined in 3GPP TS 29.503 [26]. |
| "AUTHENTICATION\_MATERIAL" | These are IEs which carry authentication material like authentication vectors and EAP payload.  An example of an AUTHENTICATION\_MATERIAL IE is authenticationVector IE defined in 3GPP TS 29.503 [26]. |
| "AUTHORIZATION\_TOKEN" | These are IEs which carry authorization Token. The oauth2 access\_token would be of this type.  An example of an AUTHORIZATION\_TOKEN IE is access\_token IE defined in 3GPP TS 29.510 [18]. |
| "OTHER" | These are IEs which do not fall into one of the above types, but they would be considered sensitive, and which protection policies may wish to apply confidentiality protection. |
| "NONSENSITIVE" | These are IEs which carry information that are not sensitive. A protection policy would not normally encrypt (confidentiality protect) these. |

##### 6.1.5.3.6 Enumeration: IeLocation

Table 6.1.5.3.6-1: Enumeration IeLocation

|  |  |
| --- | --- |
| Enumeration value | Description |
| "URI\_PARAM" | IE is located in the URI parameters. |
| "HEADER" | IE is located in the HTTP header. |
| "BODY" | IE is located in the body. |
| "MULTIPART\_BINARY" | IE is located in the message body but encoded as a multipart message information in binary format. |

##### 6.1.5.3.7 Enumeration: N32fErrorType

Table 6.1.5.3.7-1: Enumeration N32fErrorType

|  |  |
| --- | --- |
| Enumeration value | Description |
| "INTEGRITY\_CHECK\_FAILED" | The integrity check verification on the received N32-f message failed. |
| "INTEGRITY\_CHECK\_ON\_MODIFICATIONS\_FAILED" | The integrity check verification on the modifications block of the received N32-f message failed. |
| "MODIFICATIONS\_INSTRUCTIONS\_FAILED" | Failed to apply the JSON patch instructions in the modifications block of the received N32-f message, e.g. the references to encBlockIndex is inserted or relocated by IPX (see clause 5.9.3.2 of 3GPP TS 33.501 [6]). |
| "DECIPHERING\_FAILED" | The deciphering of the encrypted block of the received N32-f message failed. |
| "MESSAGE\_RECONSTRUCTION\_FAILED" | The reconstruction of the original HTTP/2 message from the received N32-f message failed. |
| "CONTEXT\_NOT\_FOUND" | The n32fContextId is unknown in the receiving SEPP. |
| "INTEGRITY\_KEY\_EXPIRED" | The integrity keys in the receiving SEPP have expired. |
| "ENCRYPTION\_KEY\_EXPIRED" | The encryption keys in the receiving SEPP have expired. |
| "POLICY\_MISMATCH" | The encryption policy verification on the received N32-f message has failed, e.g. protected IEs are not ciphered, or unprotected IEs are ciphered. |

##### 6.1.5.3.8 Enumeration: FailureReason

Table 6.1.5.3.8-1: Enumeration FailureReason

|  |  |
| --- | --- |
| Enumeration value | Description |
| "INVALID\_JSON\_POINTER" | The JSON pointer value in iePath attribute (see clause 6.2.5.2.8) is invalid. |
| "INVALID\_INDEX\_TO\_ENCRYPTED\_BLOCK" | The value part of the HttpPayload attribute (see clause 6.2.5.2.8) or HttpHeader attribute (see clause 6.2.5.2.7) is pointing to an invalid index to the encrypted block. |
| "INVALID\_HTTP\_HEADER" | The name of the header in the received HttpHeader attribute is invalid. |

#### 6.1.5.4 Binary data

There are no multipart/binary part used on the N32-c API(s) in this release of this specification.

### 6.1.6 Error Handling

#### 6.1.6.1 General

HTTP error handling shall be supported as specified in clause 5.2.4 of 3GPP TS 29.500 [4].

#### 6.1.6.2 Protocol Errors

Protocol Error Handling shall be supported as specified in clause 5.2.7.2 of 3GPP TS 29.500 [4].

#### 6.1.6.3 Application Errors

The common application errors defined in the Table 5.2.7.2-1 in 3GPP TS 29.500 [4] may also be used for the N32-c Handshake service. The following application errors listed in Table 6.1.6.3-1 are specific for the N32-c Handshake service.

Table 6.1.6.3-1: Application errors

|  |  |  |
| --- | --- | --- |
| **Application Error** | **HTTP status code** | **Description** |
| REQUESTED\_PARAM\_MISMATCH | 409 Conflict | This represents a parameter mismatch has been detected by the receiving SEPP, i.e. received data-type encryption or modification policy conflict with the one manually configured for the specific roaming partner, interconnect partner and IPX provider |

## 6.2 JOSE Protected Message Forwarding API on N32

### 6.2.1 API URI

URIs of this API shall have the following root:

{apiRoot}/{apiName}/{apiVersion}/

where "apiRoot" is defined in clause 4.4.1 of 3GPP TS 29.501 [5]. The apiRoot to use towards a SEPP of the target PLMN shall be configured at the SEPP. The URI scheme of the API shall be "http". The "apiName" shall be set to "n32f-forward" and the "apiVersion" shall be set to "v1" for the current version of this specification. The apiName part of the URI shall be as specified here for homogeneity of the API across PLMNs.

### 6.2.2 Usage of HTTP

#### 6.2.2.1 General

HTTP/2, as defined in IETF RFC 7540 [7], shall be used as specified in clause 4.3.2.1.

HTTP/2 shall be transported as specified in clause 4.3.3.

HTTP messages and bodies for the JOSE protected message forwarding API on N32-f shall comply with the OpenAPI [15] specification contained in Annex A.

#### 6.2.2.2 HTTP standard headers

##### 6.2.2.2.1 General

The HTTP standard headers as specified in clause 4.3.2.2 shall be supported for this API.

##### 6.2.2.2.2 Content type

The following content types shall be supported:

- the JSON format (see IETF RFC 8259 [8]). The use of the JSON format shall be signalled by the content type "application/json". See also clause 5.3.4.

- the Problem Details JSON Object (see IETF RFC 7807 [22]). The use of the Problem Details JSON object in a HTTP response body shall be signalled by the content type "application/problem+json".

##### 6.2.2.2.3 Accept-Encoding

SEPPs and IPX should support gzip coding (see IETF RFC 1952 [23]) in HTTP requests and responses and indicate so in the Accept-Encoding header, as described in clause 5.3.2.1.

#### 6.2.2.3 HTTP custom headers

##### 6.2.2.3.1 General

In this release of the specification, no specific custom headers are defined for the JOSE protected message forwarding API on N32.

For 3GPP specific HTTP custom headers used across all service based interfaces, see clause 4.3.2.3.

### 6.2.3 Resources

#### 6.2.3.1 Overview

There are no resources in this version of this API. All the operations are realized as custom operations without resources.

### 6.2.4 Custom Operations without associated resources

#### 6.2.4.1 Overview

Table 6.2.4.1-1: Custom operations without associated resources

|  |  |  |  |
| --- | --- | --- | --- |
| Operation Name | Custom operation URI | Mapped HTTP method | Description |
| JOSE Protected Forwarding | /n32f-process | POST | This is the N32f forwarding API used to forward a reformatted and JOSE protected message to a receiving SEPP. |
| JOSE Protected Forwarding Options | /n32f-process | OPTIONS | Discover the communication options supported by the next hop (IPX or SEPP) for N32-f message processing. |

#### 6.2.4.2 Operation: JOSE Protected Forwarding

##### 6.2.4.2.1 Description

This custom operation is used between the SEPPs to forward the reformatted and JOSE protected HTTP/2 message on N32-f. The HTTP method POST shall be used on the following URI:

URI: **{apiRoot}/n32f-forward/v1/n32f-process**

This operation shall support the resource URI variables defined in table 6.1.4.2.1-1.

Table 6.2.4.2.1-1: Resource URI variables for this Operation

|  |  |  |
| --- | --- | --- |
| Name | Data type | Definition |
| apiRoot | string | See clause 6.1.1. |

##### 6.2.4.2.2 Operation Definition

This operation shall support the request data structures and response codes specified in tables 6.2.4.2.2-1 and 6.2.4.2.2-2.

Table 6.2.4.2.2-1: Data structures supported by the POST Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| N32fReformattedReqMsg | M | 1 | This IE shall contain the reformatted HTTP/2 message comprising the plain text part, encrypted information, meta data and modification chain information. See clause 6.2.5.2.2. |

Table 6.2.4.2.2-2: Data structures supported by the POST Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  codes | Description |
| N32fReformattedRspMsg | M | 1 | 200 OK | This represents the successful processing of the reformatted JOSE protected message at the responding SEPP. The responding SEPP shall provide the reformatted and JOSE protected content of the corresponding HTTP/2 response message. |
| ProblemDetails | O | 0..1 | 403 Forbidden | When the receiving SEPP fails to process the reconstructed message due to PLMN ID verification failure, the "cause" attribute shall be set to "PLMNID\_MISMATCH". |
| NOTE: The mandatory HTTP error status codes for the POST method listed in Table 5.2.7.1-1 of 3GPP TS 29.500 [4] other than those specified in the table above also apply, with a ProblemDetails data type (see clause 5.2.7 of 3GPP TS 29.500 [4]). | | | | |

#### 6.2.4.3 Operation: JOSE Protected Forwarding Options

##### 6.2.4.3.1 Description

This service operation queries the communication options supported by the next hop (IPX or SEPP) for N32-f message processing (see clauses 5.3.2.4 and 5.3.4).

The HTTP method OPTIONS shall be used on the following URI:

URI: **{apiRoot}/n32f-forward/v1/n32f-process**

This operation shall support the resource URI variables defined in table 6.2.4.3.1-1.

Table 6.2.4.3.1-1: Resource URI variables for this Operation

|  |  |  |
| --- | --- | --- |
| Name | Data type | Definition |
| apiRoot | string | See clause 6.1.1. |

##### 6.2.4.3.2 Operation Definition

6.2.4.3.2.1 OPTIONS

This method shall support the URI query parameters specified in table 6.2.4.3.2.1-1.

Table 6.2.4.3.2.1-1: URI query parameters supported by the OPTIONS method

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| n/a |  |  |  |  |

This method shall support the request data structures specified in table 6.2.4.3.2.1-2 and the response data structures and response codes specified in table 6.2.4.3.2.1-3.

Table 6.2.4.3.2.1-2: Data structures supported by the OPTIONS Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| n/a |  |  |  |

Table 6.2.4.3.2.1-3: Data structures supported by the OPTIONS Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  codes | Description |
| n/a |  |  | 204 No Content |  |
| ProblemDetails | O | 0..1 | 405 Method Not Allowed |  |
| ProblemDetails | O | 0..1 | 501 Not Implemented |  |
| NOTE: The mandatory HTTP error status codes for the OPTIONS method listed in Table 5.2.7.1-1 of 3GPP TS 29.500 [4] other than those specified in the table above also apply, with a ProblemDetails data type (see clause 5.2.7 of 3GPP TS 29.500 [4]). | | | | |

Table 6.2.4.3.2.1-4: Headers supported by the 204 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Accept-Encoding | string | O | 0..1 | Accept-Encoding, described in IETF RFC 7694 [24] |

### 6.2.5 Data Model

#### 6.2.5.1 General

This clause specifies the application data model supported by the API.

Table 6.2.5.1-1 specifies the data types defined for the N32 interface.

Table 6.2.5.1-1: N32 specific Data Types

|  |  |  |
| --- | --- | --- |
| Data type | Clause defined | Description |
| N32fReformattedReqMsg | 6.2.5.2.2 |  |
| N32fReformattedRspMsg | 6.2.5.2.3 |  |
| DataToIntegrityProtectAndCipherBlock | 6.2.5.2.4 |  |
| DataToIntegrityProtectBlock | 6.2.5.2.5 |  |
| RequestLine | 6.2.5.2.6 |  |
| HttpHeader | 6.2.5.2.7 |  |
| HttpPayload | 6.2.5.2.8 |  |
| MetaData | 6.2.5.2.9 |  |
| Modifications | 6.2.5.2.10 |  |
| FlatJweJson | 6.2.5.2.11 |  |
| FlatJwsJson | 6.2.5.2.12 |  |
| IndexToEncryptedValue | 6.2.5.2.13 |  |
| EncodedHttpHeaderValue | 6.2.5.2.14 |  |

Table 6.2.5.1-2 specifies data types re-used by the N32 interface protocol from other specifications, including a reference to their respective specifications and when needed, a short description of their use within the Namf service based interface.

Table 6.2.5.1-2: N32 re-used Data Types

|  |  |  |
| --- | --- | --- |
| Data type | Reference | Comments |
| HttpMethod | 6.1.5.3.5 |  |
| IeLocation | 6.1.5.3.6 |  |
| PatchItem | 3GPP TS 29.571 [12] |  |
| UriScheme | 3GPP TS 29.571 [12] |  |
| Fqdn | 3GPP TS 29.510 [18] |  |

#### 6.2.5.2 Structured data types

##### 6.2.5.2.1 Introduction

This clause defines the structures to be used in the JOSE Protected Message Forwarding API on N32.

##### 6.2.5.2.2 Type: N32fReformattedReqMsg

Table 6.2.5.2.2-1: Definition of type N32fReformattedReqMsg

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| reformattedData | FlatJweJson | M | 1 | This IE shall contain the integrity protected reformatted block as well as the ciphered part of the reformatted block of the HTTP/2 request message sent between NF service producer and consumer.  The SEPP shall reformat the HTTP/2 request message as:  - The part of original HTTP/2 request message headers and the payload that needs to be only integrity protected is first reformatted into "DataToIntegrityProtectBlock" and then fed as input for the "aad" parameter of the FlatJweJson after subjecting to BASE64URL encoding.  The part of the original HTTP/2 request message headers and payload that require integrity protection and ciphering is first reformatted into "DataToIntegrityProtectAndCipherBlock" and then fed as input for JWE ciphering and the JWE ciphered block is then BASE64URL encoded and set into the "ciphertext" parameter of the FlatJweJson. |
| modificationsBlock | array(FlatJwsJson) | C | 1..N | This IE shall be included if the IPXes on path are allowed to apply modification policies and if they have any specific modification to be applied on the message contained in the DataToIntegrityProtectBlock. |

##### 6.2.5.2.3 Type: N32fReformattedRspMsg

Table 6.2.5.2.3-1: Definition of type N32fReformattedRspMsg

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| reformattedData | FlatJweJson | M | 1 | This IE shall contain the integrity protected reformatted block as well as the ciphered part of the reformatted block of the HTTP/2 response message sent between NF service producer and consumer.  The SEPP shall reformat the HTTP/2 response message as:  - The part of original HTTP/2 response message headers and the payload that needs to be only integrity protected is first reformatted into "DataToIntegrityProtectBlock" and then fed as input for the "aad" parameter of the FlatJweJson after subjecting to BASE64URL encoding.  - The part of the original HTTP/2 response message headers and payload that require integrity protection and ciphering is first reformatted into "DataToIntegrityProtectAndCipherBlock" and then fed as input for JWE ciphering and the JWE ciphered block is then BASE64URL encoded and set into the "ciphertext" parameter of the FlatJweJson. |
| modificationsBlock | array(FlatJwsJson) | C | 1..N | This IE shall be included if the IPXes on path are allowed to apply modification policies and if they have any specific modification to be applied on the message contained in the DataToIntegrityProtectBlock. |

##### 6.2.5.2.4 Type: DataToIntegrityProtectAndCipherBlock

Table 6.2.5.2.4-1: Definition of type DataToIntegrityProtectAndCipherBlock

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| dataToEncrypt | array(Any Type) | M | 1..N | This IE shall contain the input for ciphering as a JSON object block containing an array of values with arbitrary types. Each entry of the array shall contain the value of a HTTP header to be encrypted or the value of a JSON attribute to be encrypted. |

##### 6.2.5.2.5 Type: DataToIntegrityProtectBlock

Table 6.2.5.2.5-1: Definition of type DataToIntegrityProtectBlock

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| metaData | MetaData | C | 0..1 | This IE shall be included if the SEPP encodes additional information for replay protection. When present this IE shall contain the meta data information needed for replay protection. |
| requestLine | RequestLine | C | 1 | This IE shall be included when a JOSE protected API "request" is forwarded over N32-f. When present, this IE shall contain the request line of the HTTP API request being reformatted and forwarded over N32-f. |
| statusLine | string | C | 0..1 | This IE shall be included when a JOSE protected API "response" is forwarded over N32-f. When present, this IE shall contain the status line of the HTTP API response being reformatted and forwarded over N32-f. |
| headers | array(HttpHeader) | C | 1..N | This IE shall be included when a JOSE protected API request / response contains HTTP headers. When present this IE shall contain the encoding of HTTP headers in the API request / response. |
| payload | array(HttpPayload) | C | 1..N | This IE shall be included when a JOSE protected API request / response contains JSON payload that needs to be sent in clear text. When present this IE shall contain the encoding of JSON payload in the API request / response. |

##### 6.2.5.2.6 Type: RequestLine

Table 6.2.5.2.6-1: Definition of type RequestLine

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| method | HttpMethod | M | 1 | This IE shall contain the HTTP method of the API invoked by the NF service consumer / producer behind the SEPP towards its peer NF service in the other PLMN. |
| scheme | UriScheme | M | 1 | This IE shall contain the HTTP scheme of the API. |
| authority | string | M | 1 | This IE shall contain the authority part of the URI of the API being invoked. |
| path | string | M | 1 | This IE shall contain the path part of the URI of the API being invoked. |
| protocolVersion | string | M | 1 | This IE shall contain the HTTP protocol version. The version shall be 2 in this release of this specification. |
| queryFragment | string | C | 0..1 | This IE shall contain the query fragment part of the API, if available. |

##### 6.2.5.2.7 Type: HttpHeader

Table 6.2.5.2.7-1: Definition of type HttpHeader

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| header | string | M | 1 | This IE shall contain the name of the HTTP header to encoded. |
| value | EncodedHttpHeaderValue | M | 1 | This IE shall contain the value of the HTTP header. The value of the HTTP header shall be encoded as:  - value field of the EncodedHttpHeaderValue structure specified in clause 6.2.5.2.14 if the HTTP header is not to be encrypted.  - IndexToEncryptedValue structure specified in clause 6.2.5.2.13 if the value of the HTTP header is to be encrypted. |

##### 6.2.5.2.8 Type: HttpPayload

Table 6.2.5.2.8-1: Definition of type HttpPayload

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| iePath | string | M | 1 | This IE identifies the JSON pointer representation (see IETF RFC 6901 [17]) of full JSON path of the IE to be encoded. IEs that are of type object shall be flattened into each individual attribute's full JSON path and the HttpPayload IE shall only contain the final leaf attribute IE path and its corresponding value. |
| ieValueLocation | IeLocation | M | 1 | This IE shall identify where the IE value is located - i,e in the JSON body or in the multipart message part. |
| value | object | M | 1 | This IE shall contain the value of the IE corresponding to "iePath", encoded as a free form object.  If the value of this IE is encrypted, then the value part shall be encoded as  {  "encBlockIndex": <array index in DataToIntegrityProtectAndCipherBlock>  }  (see clause 6.2.5.2.4).  If the value of this IE is a RefToBinary data type (see 3GPP TS 29.571 [12], then value shall contain the value of the Content-ID header field of the referenced binary body part.  The referenced binary body part of the multipart/related message shall be either encrypted or not encrypted depending on the protection policy exchanged between the SEPPs.  If the referenced binary body part is required to be encrypted, then the binary part is first base64 encoded into a byte array and then inserted into the "DataToIntegrityProtectAndCipherBlock". Then two HttpPayload instances with the following values shall be added immediately after this HttpPayload instance in the "DataToIntegrityProtectBlock"  {  "iePath": <JSON Pointer of the attribute defined with the RefToBinaryData type>/contenttype  "ieValueLocation": "MULTIPART\_BINARY"  "value": <value of the content type of multipart binary>  },  {  "iePath": <JSON Pointer of the attribute defined with the RefToBinaryData type>/data,  "ieValueLocation": "MULTIPART\_BINARY"  "value": {"encBlockIndex": <array index in DataToIntegrityProtectAndCipherBlock that contains the byte array>}  }  If the referenced binary body part is not required to be encrypted, then the binary part is first base64 encoded into a byte array and then inserted as new instance of HttpPayload IE in " DataToIntegrityProtectBlock" as  {  "iePath": <JSON Pointer of the attribute defined with the RefToBinaryData type>/contenttype  "ieValueLocation": "MULTIPART\_BINARY"  "value": <value of the content type of multipart binary>  },  {  "iePath": <JSON path of the attribute defined with the RefToBinaryData type>/data,  "ieValueLocation": "MULTIPART\_BINARY"  "value": <base64 encoded byte array>  }  See NOTE 1. |
| NOTE 1: In this release of this specification only N16 interface has binary content and there is no sensitive information carried over N16 interface. Consequently ciphering of binary part is not required in this release of this specification. The encoding specified here is to provide a N32-f framework in a future proof manner so that if a binary part need to be encrypted in future this structure can be used. | | | | |

##### 6.2.5.2.9 Type: MetaData

Table 6.2.5.2.9-1: Definition of type MetaData

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| n32fContextId | string | M | 1 | This IE shall contain the n32fContextId provided by the initiating SEPP to the responding SEPP during the parameter exchange procedure (see clause 5.2.3).  The n32fContextId shall encode a 64-bit integer in hexadecimal representation. Each character in the string shall take a value of "0" to "9" or "A" to "F" and shall represent 4 bits. The most significant character representing the 4 most significant bits of the N32-f context Id shall appear first in the string, and the character representing the 4 least significant bit of the N32-f context Id shall appear last in the string.  Pattern: '^[A-Fa-f0-9]{16}$'  Example: "0600AD1855BD6007". |
| messageId | string | M | 1 | This IE identifies a particular request that is transformed by the SEPP. The value of this IE shall be encoded in hexadecimal representation of a 64 bit integer. This identifier is used in the N32-f error reporting procedure as specified in clause 6.1.4.5.  Pattern: ^[a-fA-F0-9]{1, 16}$ |
| authorizedIpxId | string | M | 1 | This IE identifies the first hop IPX that is authorized to insert modifications block. The identifier of the IPX shall be an FQDN. When there is no IPX that's authorized to update, the value of this IE is set to the string "NULL". |

##### 6.2.5.2.10 Type: Modifications

Table 6.2.5.2.10-1: Definition of type Modifications

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| operations | array(PatchItem) | C | 1..N | This IE shall be included if an intermediary IPX inserts modification instructions on the JSON data carried in the "DataToIntegrityProtectBlock" part of the N32-f forwarded message. For the first modifications entry, this IE shall not be included, since the first entry is inserted by the SEPP. |
| identity | Fqdn | M | 1 | This IE shall contain the identity of the entity inserting the modifications entry. The identity shall be encoded in the form of an URI. |
| tag | string | C | 0..1 | This IE shall be present when the JWE Authentication Tag value is non-empty as specified in IETF RFC 7515 [16]. When present, this IE shall contain the BASE64URL(JWE Authentication Tag). |

##### 6.2.5.2.11 Type: FlatJweJson

Table 6.2.5.2.11-1: Definition of type FlatJweJson

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| protected | string | C | 0..1 | This IE shall be present if there is a JWE Protected Header part of the JOSE header to encode as specified in IETF RFC 7516 [14]. When present, this IE shall contain the BASE64URL(UTF8(JWE Protected Header)) encoding of the JWE protected header. |
| unprotected | object | C | 0..1 | This IE shall be present if there is a JWE unprotected header part of the JOSE header that is shared across recipients, to encode as specified in IETF RFC 7515 [16]. This value is represented as  an unencoded free form JSON object, rather than as a string. These Header Parameter values are not integrity protected. |
| header | object | C | 0..1 | This IE shall be present if there is a JWE unprotected header part of the JOSE header that is specific for the recipient, to encode as specified in IETF RFC 7515 [16]. This value is represented as  an unencoded free form JSON object, rather than as a string. These Header Parameter values are not integrity protected. |
| encrypted\_key | string | C | 0..1 | This IE shall be present when the JWE Encrypted Key for the recipient is non empty. When present this IE shall contain BASE64URL(JWE Encrypted Key). |
| aad | string | C | 0..1 | This IE shall be present when the JWE AAD value is non-empty as specified in IETF RFC 7515 [16]. When present, this IE shall contain BASE64URL encoding of the DataToIntegrityProtectBlock JSON object (see clause 6.2.5.2.5). |
| iv | string | C | 0..1 | This IE shall be present when the JWE Initialization Vector is non-empty as specified in IETF RFC 7515 [16]. When present, this IE shall contain the BASE64URL(JWE Initialization Vector). |
| ciphertext | string | M | 1 | This IE shall contain BASE64URL(JWE Ciphertext). The input for JWE ciphering is the DataToIntegrityProtecAndCiphertBlock (see clause 6.2.5.2.5). |
| tag | string | C | 0..1 | This IE shall be present when the JWE Authentication Tag value is non-empty as specified in IETF RFC 7515 [16]. When present, this IE shall contain the BASE64URL(JWE Authentication Tag). |

##### 6.2.5.2.12 Type: FlatJwsJson

Table 6.2.5.2.12-1: Definition of type FlatJwsJson

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| payload | string | M | 1 | This IE shall contain the BASE64URL encoding of the Modifications JSON object (see clause 6.2.5.2.10). |
| protected | string | C | 0..1 | This IE shall be present if there is a JWS Protected Header part of the JOSE header to encode as specified in IETF RFC 7515 [16]. When present, this IE shall contain the BASE64URL(UTF8(JWS Protected Header)) encoding of the JWS protected header. |
| header | object | C | 0..1 | This IE shall be present if there is a JWS unprotected header part of the JOSE header to encode as specified in IETF RFC 7515 [16]. This value is represented as  an unencoded free form JSON object, rather than as a string. These Header Parameter values are not integrity protected. |
| signature | string | M | 1 | This IE shall contain the BASE64URL encoded value of the calculated JWS signature. |

##### 6.2.5.2.13 Type: IndexToEncryptedValue

Table 6.2.5.2.13-1: Definition of type IndexToEncryptedHttpHeader

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| encBlockIndex | Uinteger | M | 1 | Index to the value in DataToIntegrityProtectAndCipherBlock |

##### 6.2.5.2.14 Type: EncodedHttpHeaderValue

Table 6.2.5.2.14-1: Definition of type EncodedHttpHeaderValue as a list of "mutually exclusive alternatives"

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Cardinality | Description | Applicability |
| string | 1 | HTTP header value. |  |
| IndexToEncryptedValue | 1 | Index to encrypted HTTP header in the DataToIntegrityProtectAndCipherBlock |  |

#### 6.2.5.3 Simple data types and enumerations

##### 6.2.5.3.1 Introduction

This clause defines simple data types and enumerations that can be referenced from data structures defined in the previous clauses.

##### 6.2.5.3.2 Simple data types

The simple data types defined in table 6.1.5.3.2-1 shall be supported.

Table 6.2.5.3.2-1: Simple data types

|  |  |  |
| --- | --- | --- |
| Type Name | Type Definition | Description |
|  |  |  |

##### 6.2.5.3.3 Void

##### 6.2.5.3.4 Void

### 6.2.6 Error Handling

#### 6.2.6.1 General

HTTP error handling shall be supported as specified in clause 5.2.4 of 3GPP TS 29.500 [4].

#### 6.2.6.2 Protocol Errors

Protocol Error Handling shall be supported as specified in clause 5.2.7.2 of 3GPP TS 29.500 [4].

#### 6.2.6.3 Application Errors

The application errors defined for the JOSE protected message forwarding API on N32-f are listed in Table 6.2.6.3-1.

Table 6.2.6.3-1: Application errors

|  |  |  |
| --- | --- | --- |
| Application Error | HTTP status code | Description |
| PLMNID\_MISMATCH | 403 Forbidden | The PLMN ID in the Bearer token carried in the "Authorization" header of the reconstructed message does not match the PLMN ID of the N32-f context. |

## 6.3 Nsepp\_Telescopic\_FQDN\_Mapping API

### 6.3.1 API URI

URIs of this API shall have the following root:

{apiRoot}/{apiName}/{apiVersion}/

where "apiRoot" is defined in clause 4.4.1 of 3GPP TS 29.501 [5], the "apiName" shall be set to "nsepp-telescopic" and the "apiVersion" shall be set to "v1" for the current version of this specification.

### 6.3.2 Usage of HTTP

#### 6.3.2.1 General

HTTP/2, as defined in IETF RFC 7540 [7], shall be used as specified in clause 5 of 3GPP TS 29.500 [4].

HTTP/2 shall be transported as specified in clause 5.3 of 3GPP TS 29.500 [4].

HTTP messages and bodies for the Nsepp\_Telescopic\_FQDN\_Mapping service shall comply with the OpenAPI [8] specification contained in Annex A.

#### 6.3.2.2 HTTP standard headers

##### 6.3.2.2.1 General

The HTTP standard headers as specified in clause 4.3.2.2 shall be supported for this API.

##### 6.3.2.2.2 Content type

The following content types shall be supported:

- JSON, as defined in IETF RFC 8259 [9]. The use of the JSON format shall be signalled by the content type "application/json". See also clause 5.4 of 3GPP TS 29.500 [4].

- The Problem Details JSON Object (IETF RFC 7807 [10]. The use of the Problem Details JSON object in a HTTP response body shall be signalled by the content type "application/problem+json".

#### 6.3.2.3 HTTP custom headers

##### 6.3.2.3.1 General

In this release of this specification, no custom headers specific to the Nsepp\_Telescopic\_FQDN\_Mapping service are defined. For 3GPP specific HTTP custom headers used across all service-based interfaces, see clause 5.2.3 of 3GPP TS 29.500 [4].

### 6.3.3 Resources

#### 6.3.3.1 Overview



Figure 6.3.3.1-1: Resource URI structure of the nsepp-telescopic API

Table 6.3.3.1-1 provides an overview of the resources and applicable HTTP methods.

Table 6.3.3.1-1: Resources and methods overview

|  |  |  |  |
| --- | --- | --- | --- |
| Resource name | Resource URI | HTTP method or custom operation | Description |
| Mapping | /mapping | GET | Retrieve the mapping between the FQDN in a foreign PLMN and a telescopic FQDN, or viceversa. |

#### 6.3.3.2 Resource: Mapping

##### 6.3.3.2.1 Description

This resource represents the mapping between the FQDN of an NF in a foreign PLMN and a telescopic FQDN.

##### 6.3.3.2.2 Resource Definition

Resource URI: {apiRoot}/nsepp-telescopic/v1/mapping

This resource shall support the resource URI variables defined in table 6.3.3.2.2-1.

Table 6.3.3.2.2-1: Resource URI variables for this resource

|  |  |  |
| --- | --- | --- |
| Name | Data type | Definition |
| apiRoot | string | See clause 6.3.1 |

##### 6.3.3.2.3 Resource Standard Methods

6.3.3.2.3.1 GET

This method shall support the URI query parameters specified in table 6.3.3.2.3.1-1.

Table 6.3.3.2.3.1-1: URI query parameters supported by the GET method on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| foreign-fqdn | Fqdn | O | 0..1 | This parameter shall contain the FQDN of the NF in the foreign network, that needs to be flattened to a telescopic FQDN in the local network (i.e. an FQDN that points to the local SEPP). |
| telescopic-label | string | O | 0..1 | This parameter shall contain the first label used in a telescopic FQDN (i.e. an FQDN that points to the local SEPP) that needs to be mapped to an NF in the foreign network. |
| NOTE: The parameters "foreign-fqdn" and "telescopic-label" shall not be present simultaneously. | | | | |

This method shall support the request data structures specified in table 6.3.3.2.3.1-2 and the response data structures and response codes specified in table 6.3.3.2.3.1-3.

Table 6.3.3.2.3.1-2: Data structures supported by the GET Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| n/a |  |  |  |

Table 6.3.3.2.3.1-3: Data structures supported by the GET Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  codes | Description |
| TelescopicMapping | M | 1 | 200 OK | Upon success, a response body containing a TelescopicMapping object shall be returned |
| ProblemDetails | O | 0..1 | 404 Not Found | The mapping between a foreign FQDN and a telescopic FQDN could not be found. |

### 6.3.4 Data Model

#### 6.3.4.1 General

This clause specifies the application data model supported by the API.

Table 6.3.4.1-1 specifies the data types defined for the Nsepp\_Telescopic\_FQDN\_Mapping service-based interface protocol.

Table 6.3.4.1-1: Nsepp\_Telescopic\_FQDN\_Mapping specific Data Types

|  |  |  |
| --- | --- | --- |
| Data type | Clause defined | Description |
| TelescopicMapping | 6.3.4.2.2 |  |

Table 6.3.4.1-2 specifies data types re-used by the Nsepp\_Telescopic\_Mapping service-based interface protocol from other specifications.

Table 6.3.4.1-2: Nsepp\_Telescopic\_FQDN\_Mapping re-used Data Types

|  |  |  |
| --- | --- | --- |
| Data type | Reference | Comments |
| Fqdn | 3GPP TS 29.510 [18] |  |
| ProblemDetails | 3GPP TS 29.571 [12] | Common data type for error responses |

#### 6.3.4.2 Structured data types

##### 6.3.4.2.1 Introduction

This clause defines the structures to be used in resource representations.

##### 6.3.4.2.2 Type: TelescopicMapping

Table 6.3.4.2.2-1: Definition of type TelescopicMapping

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description |
| telescopicLabel | string | C | 0..1 | This parameter shall contain the first label to be used in a telescopic FQDN (i.e. an FQDN that points to the local SEPP) that corresponds to a given NF in the foreign network.  In a successful response, this parameter shall be included when the query parameter "foreign-fqdn" is present in the request. |
| seppDomain | Fqdn | C | 0..1 | This parameter shall contain the FQDN of the domain of the local SEPP that needs to be appended after the "telescopicLabel" to compose the complete flattened telescopic FQDN.  In a successful response, this parameter shall be included when the query parameter "foreign-fqdn" is present in the request. |
| foreignFqdn | Fqdn | C | 0..1 | This parameter shall contain the FQDN of the NF in the foreign network.  In a successful response, this parameter shall be included when the query parameter "telescopic-label" is present in the request. |

#### 6.3.4.3 Simple data types and enumerations

##### 6.3.4.3.1 Introduction

This clause defines simple data types and enumerations that can be referenced from data structures defined in the previous clauses.

##### 6.3.4.3.2 Simple data types

The simple data types defined in table 6.3.4.3.2-1 shall be supported.

Table 6.3.4.3.2-1: Simple data types

|  |  |  |
| --- | --- | --- |
| Type Name | Type Definition | Description |
|  |  |  |

### 6.3.5 Error Handling

#### 6.3.5.1 General

HTTP error handling shall be supported as specified in clause 5.2.4 of 3GPP TS 29.500 [4].

#### 6.3.5.2 Protocol Errors

Protocol Error Handling shall be supported as specified in clause 5.2.7 of 3GPP TS 29.500 [4].

#### 6.3.5.3 Application Errors

The common application errors defined in the Table 5.2.7.2-1 in 3GPP TS 29.500 [4] may also be used for the Nsepp\_Telescopic\_Mapping service, and the following application errors listed in Table 6.3.5.3-1 are specific for the Nsepp\_Telescopic\_Mapping service.

Table 6.3.5.3-1: Application errors

|  |  |  |
| --- | --- | --- |
| Application Error | HTTP status code | Description |
|  |  |  |

### 6.3.6 Feature Negotiation

This API does not currently specify any features.

### 6.3.7 Security

#### 6.3.7.1 General

This API shall be accessed only from NFs in the same PLMN as the SEPP; it shall not be exposed externally to NFs from another PLMN.

Annex A (normative):  
OpenAPI Specification

# A.1 General

This Annex specifies the formal definition of the N32 Handshake API(s) on the N32-c interface. It consists of OpenAPI 3.0.0 specifications, in YAML format.

This Annex takes precedence when being discrepant to other parts of the specification with respect to the encoding of information elements and methods within the API(s).

NOTE: The semantics and procedures, as well as conditions, e.g. for the applicability and allowed combinations of attributes or values, not expressed in the OpenAPI definitions but defined in other parts of the specification also apply.

Informative copies of the OpenAPI specification files contained in this 3GPP Technical Specification are available on a Git-based repository that uses the GitLab software version control system (see 3GPP TS 29.501 [5] clause 5.3.1 and 3GPP TR 21.900 [7] clause 5B).

# A.2 N32 Handshake API

openapi: 3.0.0

info:

version: '1.1.3'

title: 'N32 Handshake API'

description: |

N32-c Handshake Service.

© 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

servers:

- url: '{apiRoot}/n32c-handshake/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501.

externalDocs:

description: 3GPP TS 29.573 V16.9.0; 5G System; Public Land Mobile Network (PLMN) Interconnection; Stage 3

url: https://www.3gpp.org/ftp/Specs/archive/29\_series/29.573/

paths:

/exchange-capability:

post:

summary: Security Capability Negotiation

tags:

- Security Capability Negotiation

operationId: PostExchangeCapability

requestBody:

description: Custom operation for security capability negotiation

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/SecNegotiateReqData'

responses:

'200':

description: OK (Successful negitiation of security capabilities)

content:

application/json:

schema:

$ref: '#/components/schemas/SecNegotiateRspData'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

description: Unexpected error

/exchange-params:

post:

summary: Parameter Exchange

tags:

- Parameter Exchange

operationId: PostExchangeParams

requestBody:

description: Custom operation for parameter exchange

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/SecParamExchReqData'

responses:

'200':

description: OK (Successful exchange of parameters)

content:

application/json:

schema:

$ref: '#/components/schemas/SecParamExchRspData'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'409':

$ref: 'TS29571\_CommonData.yaml#/components/responses/409'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

description: Unexpected error

/n32f-terminate:

post:

summary: N32-f Context Terminate

tags:

- N32-f Context Terminate

operationId: PostN32fTerminate

requestBody:

description: Custom operation for n32-f context termination

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/N32fContextInfo'

responses:

'200':

description: OK (Successful exchange of parameters)

content:

application/json:

schema:

$ref: '#/components/schemas/N32fContextInfo'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

description: Unexpected error

/n32f-error:

post:

summary: N32-f Error Reporting Procedure

tags:

- N32-f Error Report

operationId: PostN32fError

requestBody:

description: Custom operation for n32-f error reporting procedure

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/N32fErrorInfo'

responses:

'204':

description: successful error reporting

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

description: Unexpected error

components:

schemas:

SecurityCapability:

anyOf:

- type: string

enum:

- TLS

- PRINS

- type: string

ApiSignature:

oneOf:

- $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

- $ref: '#/components/schemas/CallbackName'

HttpMethod:

anyOf:

- type: string

enum:

- GET

- PUT

- POST

- DELETE

- PATCH

- HEAD

- OPTIONS

- CONNECT

- TRACE

- type: string

IeType:

anyOf:

- type: string

enum:

- UEID

- LOCATION

- KEY\_MATERIAL

- AUTHENTICATION\_MATERIAL

- AUTHORIZATION\_TOKEN

- OTHER

- NONSENSITIVE

- type: string

IeLocation:

anyOf:

- type: string

enum:

- URI\_PARAM

- HEADER

- BODY

- MULTIPART\_BINARY

- type: string

IeInfo:

type: object

required:

- ieLoc

- ieType

properties:

ieLoc:

$ref: '#/components/schemas/IeLocation'

ieType:

$ref: '#/components/schemas/IeType'

reqIe:

type: string

rspIe:

type: string

isModifiable:

type: boolean

isModifiableByIpx:

type: object

additionalProperties:

type: boolean

minProperties: 1

ApiIeMapping:

type: object

required:

- apiSignature

- apiMethod

- IeList

properties:

apiSignature:

$ref: '#/components/schemas/ApiSignature'

apiMethod:

$ref: '#/components/schemas/HttpMethod'

IeList:

type: array

items:

$ref: '#/components/schemas/IeInfo'

minItems: 1

ProtectionPolicy:

type: object

required:

- apiIeMappingList

properties:

apiIeMappingList:

type: array

items:

$ref: '#/components/schemas/ApiIeMapping'

minItems: 1

dataTypeEncPolicy:

type: array

items:

$ref: '#/components/schemas/IeType'

minItems: 1

SecNegotiateReqData:

type: object

required:

- sender

- supportedSecCapabilityList

properties:

sender:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/Fqdn'

supportedSecCapabilityList:

type: array

items:

$ref: '#/components/schemas/SecurityCapability'

minItems: 1

3GppSbiTargetApiRootSupported:

type: boolean

default: false

plmnIdList:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

minItems: 1

targetPlmnId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

SecNegotiateRspData:

type: object

required:

- sender

- selectedSecCapability

properties:

sender:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/Fqdn'

selectedSecCapability:

$ref: '#/components/schemas/SecurityCapability'

3GppSbiTargetApiRootSupported:

type: boolean

default: false

plmnIdList:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

minItems: 1

SecParamExchReqData:

type: object

required:

- n32fContextId

properties:

n32fContextId:

type: string

pattern: '^[A-Fa-f0-9]{16}$'

jweCipherSuiteList:

type: array

items:

type: string

minItems: 1

jwsCipherSuiteList:

type: array

items:

type: string

minItems: 1

protectionPolicyInfo:

$ref: '#/components/schemas/ProtectionPolicy'

ipxProviderSecInfoList:

type: array

items:

$ref: '#/components/schemas/IpxProviderSecInfo'

minItems: 1

sender:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/Fqdn'

SecParamExchRspData:

type: object

required:

- n32fContextId

properties:

n32fContextId:

type: string

pattern: '^[A-Fa-f0-9]{16}$'

selectedJweCipherSuite:

type: string

selectedJwsCipherSuite:

type: string

selProtectionPolicyInfo:

$ref: '#/components/schemas/ProtectionPolicy'

ipxProviderSecInfoList:

type: array

items:

$ref: '#/components/schemas/IpxProviderSecInfo'

minItems: 1

sender:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/Fqdn'

N32fContextInfo:

type: object

required:

- n32fContextId

properties:

n32fContextId:

type: string

pattern: '^[A-Fa-f0-9]{16}$'

CallbackName:

type: object

required:

- callbackType

properties:

callbackType:

type: string

N32fErrorInfo:

type: object

required:

- n32fMessageId

- n32fErrorType

properties:

n32fMessageId:

type: string

n32fErrorType:

$ref: '#/components/schemas/N32fErrorType'

failedModificationList:

type: array

items:

$ref: '#/components/schemas/FailedModificationInfo'

minItems: 1

errorDetailsList:

type: array

items:

$ref: '#/components/schemas/N32fErrorDetail'

minItems: 1

FailedModificationInfo:

type: object

required:

- ipxId

- n32fErrorType

properties:

ipxId:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/Fqdn'

n32fErrorType:

$ref: '#/components/schemas/N32fErrorType'

N32fErrorDetail:

type: object

required:

- attribute

- msgReconstructFailReason

properties:

attribute:

type: string

msgReconstructFailReason:

$ref: '#/components/schemas/FailureReason'

IpxProviderSecInfo:

type: object

required:

- ipxProviderId

properties:

ipxProviderId:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/Fqdn'

rawPublicKeyList:

type: array

items:

type: string

minItems: 1

certificateList:

type: array

items:

type: string

minItems: 1

N32fErrorType:

anyOf:

- type: string

enum:

- INTEGRITY\_CHECK\_FAILED

- INTEGRITY\_CHECK\_ON\_MODIFICATIONS\_FAILED

- MODIFICATIONS\_INSTRUCTIONS\_FAILED

- DECIPHERING\_FAILED

- MESSAGE\_RECONSTRUCTION\_FAILED

- CONTEXT\_NOT\_FOUND

- INTEGRITY\_KEY\_EXPIRED

- ENCRYPTION\_KEY\_EXPIRED

- POLICY\_MISMATCH

- type: string

FailureReason:

anyOf:

- type: string

enum:

- INVALID\_JSON\_POINTER

- INVALID\_INDEX\_TO\_ENCRYPTED\_BLOCK

- INVALID\_HTTP\_HEADER

- type: string

# A.3 JOSE Protected Message Forwarding API on N32-f

openapi: 3.0.0

info:

version: '1.1.3'

title: 'JOSE Protected Message Forwarding API'

description: |

N32-f Message Forwarding Service.

© 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

servers:

- url: '{apiRoot}/n32f-forward/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501.

externalDocs:

description: 3GPP TS 29.573 V16.10.0; 5G System; Public Land Mobile Network (PLMN) Interconnection; Stage 3

url: https://www.3gpp.org/ftp/Specs/archive/29\_series/29.573/

paths:

/n32f-process:

post:

summary: N32-f Message Forwarding

tags:

- N32-f Forward

operationId: PostN32fProcess

parameters:

- name: Content-Encoding

in: header

description: Content-Encoding, described in IETF RFC 7231

schema:

type: string

- name: Accept-Encoding

in: header

description: Accept-Encoding, described in IETF RFC 7231

schema:

type: string

requestBody:

description: Custom operation N32-f Message Forwarding

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/N32fReformattedReqMsg'

responses:

'200':

description: OK (Successful forwarding of reformatted message over N32-f)

content:

application/json:

schema:

$ref: '#/components/schemas/N32fReformattedRspMsg'

headers:

Accept-Encoding:

description: Accept-Encoding, described in IETF RFC 7694

schema:

type: string

Content-Encoding:

description: Content-Encoding, described in IETF RFC 7231

schema:

type: string

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

description: Unexpected error

options:

summary: Discover communication options supported by next hop (IPX or SEPP)

operationId: N32fProcessOptions

tags:

- N32-f Forward

responses:

'204':

description: No Content

headers:

Accept-Encoding:

description: Accept-Encoding, described in IETF RFC 7694

schema:

type: string

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'405':

$ref: 'TS29571\_CommonData.yaml#/components/responses/405'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'501':

$ref: 'TS29571\_CommonData.yaml#/components/responses/501'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

schemas:

FlatJweJson:

type: object

required:

- ciphertext

properties:

protected:

type: string

unprotected:

type: object

header:

type: object

encrypted\_key:

type: string

aad:

type: string

iv:

type: string

ciphertext:

type: string

tag:

type: string

FlatJwsJson:

type: object

required:

- payload

- signature

properties:

payload:

type: string

protected:

type: string

header:

type: object

signature:

type: string

N32fReformattedReqMsg:

type: object

required:

- reformattedData

properties:

reformattedData:

$ref: '#/components/schemas/FlatJweJson'

modificationsBlock:

type: array

items:

$ref: '#/components/schemas/FlatJwsJson'

minItems: 1

N32fReformattedRspMsg:

type: object

required:

- reformattedData

properties:

reformattedData:

$ref: '#/components/schemas/FlatJweJson'

modificationsBlock:

type: array

items:

$ref: '#/components/schemas/FlatJwsJson'

minItems: 1

DataToIntegrityProtectAndCipherBlock:

type: object

required:

- dataToEncrypt

properties:

dataToEncrypt:

type: array

items: {}

minItems: 1

DataToIntegrityProtectBlock:

type: object

properties:

metaData:

$ref: '#/components/schemas/MetaData'

requestLine:

$ref: '#/components/schemas/RequestLine'

statusLine:

type: string

headers:

type: array

items:

$ref: '#/components/schemas/HttpHeader'

minItems: 1

payload:

type: array

items:

$ref: '#/components/schemas/HttpPayload'

minItems: 1

RequestLine:

type: object

required:

- method

- scheme

- authority

- path

- protocolVersion

properties:

method:

$ref: 'TS29573\_N32\_Handshake.yaml#/components/schemas/HttpMethod'

scheme:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/UriScheme'

authority:

type: string

path:

type: string

protocolVersion:

type: string

queryFragment:

type: string

HttpHeader:

type: object

required:

- header

- value

properties:

header:

type: string

value:

$ref: '#/components/schemas/EncodedHttpHeaderValue'

HttpPayload:

type: object

required:

- iePath

- ieValueLocation

- value

properties:

iePath:

type: string

ieValueLocation:

$ref: 'TS29573\_N32\_Handshake.yaml#/components/schemas/IeLocation'

value:

type: object

MetaData:

type: object

required:

- n32fContextId

- messageId

- authorizedIpxId

properties:

n32fContextId:

type: string

pattern: '^[A-Fa-f0-9]{16}$'

messageId:

type: string

authorizedIpxId:

type: string

Modifications:

type: object

required:

- identity

properties:

identity:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/Fqdn'

operations:

type: array

items:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PatchItem'

minItems: 1

tag:

type: string

IndexToEncryptedValue:

type: object

required:

- encBlockIndex

properties:

encBlockIndex:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

EncodedHttpHeaderValue:

oneOf:

- type: string

- $ref: '#/components/schemas/IndexToEncryptedValue'

# A.4 SEPP Telescopic FQDN Mapping API

openapi: 3.0.0

info:

version: '1.0.0'

title: 'SEPP Telescopic FQDN Mapping API'

description: |

SEPP Telescopic FQDN Mapping Service.

© 2019, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

servers:

- url: '{apiRoot}/nsepp-telescopic/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501.

externalDocs:

description: 3GPP TS 29.573 V16.3.0; 5G System; Public Land Mobile Network (PLMN) Interconnection; Stage 3

url: http://www.3gpp.org/ftp/Specs/archive/29\_series/29.573/

paths:

/mapping:

get:

summary: Maps an FQDN to/from a telescopic FQDN

operationId: GetTelescopicMapping

tags:

- Telescopic Mapping (Document)

parameters:

- name: foreign-fqdn

in: query

description: FQDN of the NF in the foreign PLMN

schema:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/Fqdn'

- name: telescopic-label

in: query

description: Telescopic Label

schema:

type: string

responses:

'200':

description: Expected response to a valid request

content:

application/json:

schema:

$ref: '#/components/schemas/TelescopicMapping'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

schemas:

TelescopicMapping:

type: object

properties:

telescopicLabel:

type: string

seppDomain:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/Fqdn'

foreignFqdn:

$ref: 'TS29510\_Nnrf\_NFManagement.yaml#/components/schemas/Fqdn'

Annex B (informative):  
Examples of N32-f Encoding

# B.1 General

This Annex provides some example encodings of HTTP/2 request and response messages initiated by NF service consumer / producer when they are reformatted and sent over N32-f

# B.2 Input Message Containing No Binary Part

Consider the following example:

- Some headers of the input HTTP/2 message need to be integrity protected and ciphered.

- Some payload part of the input HTTP/2 message need to be integrity protected and ciphered.

- The input HTTP/2 message has no multipart/related binary content.

- The headers and payload that are not required to be integrity protected and ciphered in the input HTTP/2 message need to be only integrity protected.

The N32fReformattedReqMessage for this example looks like

"reformattedData": {

"protected": BASE64URL(UTF8(JWE Protected Header),

"unprotected": <non integrity protected shared JOSE headers>,

"header": <non integrity protected recipient specific JOSE headers>,

"encrypted\_key": BASE64URL(JWE Encrypted Key),

"aad": BASE64URL(DataToIntegrityProtectBlock),

"iv": BASE64URL(JWE Initialization Vector),

"ciphertext": BASE64URL(JWE CipherText(DataToIntegrityProtectAndCipherBlock),

"tag": BASE64URL(JWE Authentication Tag)

}

The DataToIntegrityProtectBlock for this example looks like

{

"metaData":

{

"n32fContextId": <the n32fcontext Id of receiving SEPP>,

"messageId": <Id of the message>,

"authorizedIpxId": <FQDN of the IPX>

},

"requestLine":

{

"method": <http method of the NF service API>,

"scheme": <http scheme of the NF service API>,

"authority": <authority part of the NF service API URI>,

"path": <path part of the NF service API URI>,

"protocolVersion": <HTTP protocol version>,

"queryFragment": <query fragment of the NF service API, if available>

},

"headers":

[

{

"header": <name of HTTP header 1>,

"value": {"headerval": <string carrying value of the header>}

},

{

"header": <name of HTTP header 2>,

"value": {"encBlockIndex": 1}

}

],

"payload":

[

{

"iePath": <JSON Pointer of IE 1>,

"ieValueLocation": "BODY",

"value": <value of IE>

},

{

"iePath": <JSON Pointer of IE 2>,

"ieValueLocation": "BODY",

"value": {"encBlockIndex": 2}

}

]

}

The DataToIntegrityProtectAndCipherBlock for this example looks like

{

"dataToEncrypt":

[

<value of HTTP header 2>,

<value of payload 2>

]

}

# B.3 Input Message Containing Multipart Binary Part

Consider the following example:

- Some headers of the input HTTP/2 message need to be integrity protected and ciphered.

- Some payload part of the input HTTP/2 message need to be integrity protected and ciphered.

- The input HTTP/2 message has two multipart/related binary content out of which one binary content needs to be integrity protected and ciphered while the other is only required to be integrity protected.

- The headers and payload that are not required to be integrity protected and ciphered in the input HTTP/2 message need to be only integrity protected.

The N32fReformattedReqMessage for this example looks like

"reformattedData": {

"protected": BASE64URL(UTF8(JWE Protected Header),

"unprotected": <non integrity protected shared JOSE headers>,

"header": <non integrity protected recipient specific JOSE headers>,

"encrypted\_key": BASE64URL(JWE Encrypted Key),

"aad": BASE64URL(DataToIntegrityProtectBlock),

"iv": BASE64URL(JWE Initialization Vector),

"ciphertext": BASE64URL(JWE CipherText(DataToIntegrityProtectAndCipherBlock),

"tag": BASE64URL(JWE Authentication Tag)

}

The DataToIntegrityProtectBlock for this example looks like

{

"metaData":

{

"n32fContextId": <the n32fcontext Id of receiving SEPP>,

"messageId": <Id of the message>,

"authorizedIpxId": <FQDN of the IPX>

},

"requestLine":

{

"method": <http method of the NF service API>,

"scheme": <http scheme of the NF service API>,

"authority": <authority part of the NF service API URI>,

"path": <path part of the NF service API URI>,

"protocolVersion": <HTTP protocol version>,

"queryFragment": <query fragment of the NF service API, if available>

},

"headers":

[

{

"header": <name of HTTP header 1>,

"value": {"headerval": <string carrying value of the header>}

},

{

"header": <name of HTTP header 2>,

"value": {"encBlockIndex": 1}

}

],

"payload":

[

{

"iePath": <JSON Pointer of IE 1>,

"ieValueLocation": "BODY",

"value": <value of IE>

},

{

"iePath": <JSON Pointer of IE 2 - which is an attribute defined with the RefToBinaryData type>/contentId,

"ieValueLocation": "BODY",

"value": <value of the Content ID>

},

{

"iePath": <JSON Pointer of IE 2 - which is an attribute defined with the RefToBinaryData type>/contenttype,

"ieValueLocation": "MULTIPART\_BINARY",

"value": <value of the Content Type>

},

{

"iePath": <JSON Pointer of IE 2 - which is an attribute defined with the RefToBinaryData type>/data,

"ieValueLocation": "MULTIPART\_BINARY",

"value": <BASE 64 encoded byte array of the binary part>

}

{

"iePath": <JSON Pointer of IE 3 - which is an attribute defined with the RefToBinaryData type>/contentId,

"ieValueLocation": "BODY",

"value": <value of the Content ID>

},

{

"iePath": <JSON Pointer of IE 3 - which is an attribute defined with the RefToBinaryData type>/contenttype,

"ieValueLocation": "MULTIPART\_BINARY",

"value": <value of the Content Type>

},

{

"iePath": <JSON Pointer of IE 3 - which is an attribute defined with the RefToBinaryData type>/data,

"ieValueLocation": "MULTIPART\_BINARY",

"value": {"encBlockIndex": 2}

}

]

}

NOTE: The "iePath" for Content Type or data is a virtual path, which actually refers to the "Content-Type" and "data" in multipart body.

EXAMPLE: If the input HTTP message contains multipart binary part, as:  
  
POST /example.com/namf-comm/v1/ue-contexts/{ueContextId}/n1-n2-messages HTTP/2  
Content-Type: multipart/related; boundary=----Boundary  
Content-Length: xyz  
  
------Boundary  
Content-Type: application/json  
  
{  
 "n2InfoContainer": {  
 "n2InformationClass": "SM",  
 "smInfo": {  
 "pduSessionId": 5,  
 "n2InfoContent": {  
 "ngapIeType": "PDU\_RES\_SETUP\_REQ",  
 "ngapData": {  
 "contentId": "n2msg"  
 }  
 }  
 }  
 },  
 "pduSessionId": 5  
}  
------Boundary  
Content-Type: application/vnd.3gpp.ngap  
Content-Id: n2msg  
  
{ … N2 Information binary data …}  
------Boundary  
  
the binary content only required to be integrity protected will be formatted, as:  
  
"payload":  
 [  
 {  
 "iePath": "/n2InfoContainer/smInfo/n2InfoContent/ngapData/contentId",  
 "ieValueLocation": "BODY",  
 "value": "n2msg"  
 },  
 {  
 "iePath": "/n2InfoContainer/smInfo/n2InfoContent/ngapData/contenttype",  
 "ieValueLocation": "MULTIPART\_BINARY",  
 "value": "application/vnd.3gpp.ngap"  
 },  
 {  
 "iePath": "/n2InfoContainer/smInfo/n2InfoContent/ngapData/data",  
 "ieValueLocation": "MULTIPART\_BINARY",  
 "value": <BASE 64 encoded byte array of N2 Information binary data >  
 }  
 ]

The DataToIntegrityProtectAndCipherBlock for this example looks like

{

"dataToEncrypt":

[

<value of HTTP header 2>,

<byte array containing BASE 64 encoding of the binary part>

]

}

Annex C (informative):  
End to end call flows when SEPP is on path

# C.1 General

This Annex provides an informative reference for how the end to end call flow works when the NF service consumer and the NF service producer are in different PLMNs and SEPP is involved on path.

The following clauses explain how the HTTP messages are forwarded between NF services in two PLMNs via the SEPP. In these clauses, the following aspects are not shown to avoid cluttering of the figures and procedure:

- Resolution of FQDN into an IP address using DNS. TCP / TLS connection for sending the HTTP/2 messages is initiated towards the IP address obtained from DNS resolution.

When https URI scheme is used, TLS protection between the Network Function and the SEPP may rely on using telescopic FQDN or 3gpp-Sbi-Target-apiRoot header. See clause 6.1.4.3 of 3GPP TS 29.500 [4].

# C.2 TLS security between SEPPs

## C.2.1 When http URI scheme is used

### C.2.1.1 General

The following figure shows the end to end call flow between an NF service consumer and a NF service producer in different PLMNs when:

- the SEPP in each PLMN acts as a security proxy;

- the negotiated security policy between the SEPPs is TLS;

- "http" scheme URI is used between the NF service consumer and NF service producer; and

- "http" scheme URI is used for accessing NRF's NF discovery service.

NOTE: There may be one or more IPX(s), offering only IP routing serving without content modification or observation of the information, in between the SEPPs.

### C.2.1.2 Without TLS protection between NF and SEPP and with TLS security without the 3gpp-Sbi-Target-apiRoot header used over N32f



Figure C.2.1.2-1: End to end call flow when http scheme URI is used and TLS security without the 3gpp-Sbi-Target-apiRoot header used is used between SEPPs

1. The SEPP on the NF service consumer side (c-SEPP) and the SEPP on the NF service producer side (p-SEPP) negotiate the security capabilities using the procedure specified in clause 5.2.2. The SEPPs mutually negotiate to use TLS as the security policy.

2. A TLS connection is setup between the c-SEPP and the p-SEPP for N32-f forwarding.

3. Before the NF service consumer starts using the API of the NF service producer it needs to discover the NF service profile of the producer by querying the NRF. The NF service consumer uses "http" scheme URI to access the Nnrf\_NFDiscovery service.

4. The NRF on the NF service consumer side (c-NRF) needs to further initiate a discovery request to the NRF on the NF service producer side (p-NRF). The c-NRF is configured to route all HTTP messages with inter PLMN FQDN as the "authority" part of the URI via the c-SEPP. The c-SEPP acts as a HTTP proxy.

5. The c-SEPP forwards the NF discovery request within the N32-f TLS tunnel established in step 2.

6. The p-SEPP forwards the NF discovery request to the p-NRF.

7. The p-NRF sends the NF discovery response. The NF service profile contains service URI with "http" scheme. The FQDN of the NF service is an inter PLMN FQDN.

8. The p-SEPP forwards the NF discovery response within TLS tunnel to the c-SEPP.

9. The c-SEPP forwards the NF discovery response to c-NRF.

10. The c-NRF sends the NF discovery response to NF service consumer.

11. The NF service profile received at the NF service consumer contains service URI with "http" scheme. The NF service consumer initiates a HTTP message (as supported by the NF service producer API) using "http" scheme URI. The NF service consumer is configured to route all HTTP messages with inter PLMN FQDN as the "authority" part of the URI via the c-SEPP. The c-SEPP acts as a HTTP proxy.

12. The c-SEPP forwards the HTTP service request within the N32-f TLS tunnel established in step 2.

13. The p-SEPP forwards the HTTP service request to the NF service producer.

14. The NF service producer sends the HTTP service response.

15. The p-SEPP forwards the HTTP service response within TLS tunnel to the c-SEPP.

16. The c-SEPP forwards the HTTP service response to the NF service consumer.

### C.2.1.3 Without TLS protection between NF and SEPP and with TLS security with the 3gpp-Sbi-Target-apiRoot header used over N32f



Figure C.2.1.3-1: End to end call flow when http scheme URI is used and TLS security with the 3gpp-Sbi-Target-apiRoot header used is used between SEPPs

1. Same as step 1 of Figure C.2.1.2-1.

2. Same as step 3 of Figure C.2.1.2-1

3. Same as step 4 of Figure C.2.1.2-1

4. The c-SEPP setups a TLS connection with the authoritative server for the p-SEPP FQDN (in the apiRoot of the Request URI) and verifies that the certificate presented by the endpoint of the TLS connection belongs to the authoritative server of the p-SEPP. The c-SEPP is configured with the p-SEPP FQDN.

5. The c-SEPP sets the apiRoot in the request URI with the apiRoot of the p-SEPP, inserts the 3gpp-Sbi-Target-apiRoot header set to the apiRoot of the p-NRF, and sends the request towards p-SEPP.

6. The p-SEPP extracts the HTTP message received on the TLS connection, replaces the apiRoot of the p-SEPP FQDN in the request URI with the apiRoot of the p-NRF received in the 3gpp-Sbi-Target-apiRoot header, and then seeing that the URI scheme of the NF discovery service of the p-NRF is "http", the p-SEPP forwards the NF discovery request to the p-NRF.

7 to 11. Same as steps 7 to 11 of Figure C.2.1.2-1.

12. The c-SEPP sets the apiRoot of the p-SEPP FQDN in the request URI, inserts the 3gpp-Sbi-Target-apiRoot header set to the apiRoot of the p-NF, and sends the request towards p-SEPP.

13. The p-SEPP extracts the HTTP message received on the TLS connection, replaces the apiRoot of the p-SEPP FQDN in the request URI with the apiRoot of the p-NF received in the 3gpp-Sbi-Target-apiRoot header and then seeing that the URI scheme of the NF service producer is "http", the p-SEPP forwards the request to the p-NF.

13 to 16. Same as steps 13 to 16 of Figure C.2.1.2-1.

## C.2.2 When https URI scheme is used

### C.2.2.1 General

The following figures show the end to end call flow between an NF service consumer and a NF service producer in different PLMNs when:

- the SEPP in each PLMN acts as a security proxy;

- the negotiated security policy between the SEPPs is TLS;

- "https" scheme URI is used between the NF service consumer and NF service producer;

- "https" scheme URI is used for accessing NRF's NF discovery service; and

- TLS protection between NF and SEPP relies on using telescopic FQDN or 3gpp-Sbi-Target-apiRoot header.

### C.2.2.2 With TLS protection between NF and SEPP relying on telescopic FQDN, and TLS security without the 3gpp-Sbi-Target-apiRoot header used over N32f



Figure C.2.2.2-1: End to end call flow when https scheme URI is used, telescopic FQDNs are used between NF and SEPP and TLS security without the 3gpp-Sbi-Target-apiRoot header is used between SEPPs

1. The SEPP on the NF service consumer side (c-SEPP) and the SEPP on the NF service producer side (p-SEPP) negotiate the security capabilities using the procedure specified in clause 5.2.2. The SEPPs mutually negotiate to use TLS as the security policy.

2. A TLS connection is setup between the c-SEPP and the p-SEPP for N32-f forwarding.

3. Before the NF service consumer starts using the API of the NF service producer it needs to discover the NF service profile of the producer by querying the NRF. The NF service consumer uses "https" scheme URI to access the Nnrf\_NFDiscovery service. This implies that the NF service consumer sets up a TLS connection to the c-NRF and then sends the HTTP request over the TLS connection to the c-NRF.

4. The NRF on the NF service consumer side (c-NRF) needs to further initiate a discovery request to the NRF on the NF service producer side (p-NRF). The c-NRF uses "https" scheme URI to access the NF discovery service of the p-NRF. Since "https" requires setup of TLS connection with the p-NRF and it requires that c-NRF has to verify that the certificate presented by the endpoint of the TLS connection belongs to the authoritative server of the p-NRF, a telescopic FQDN with wildcarded certificate scheme mechanism is specified in 3GPP TS 33.501 [6]. The c-NRF is configured with the telescopic FQDN of the p-NRF with the telescopic FQDN having the FQDN of the c-SEPP as the trailing part. The c-NRF sets up a TLS connection with the authoritative server for the telescopic FQDN (i.e. the c-SEPP).

5. The c-NRF forwards the NF discovery request in this TLS connection.

6. The c-SEPP extracts the NF discovery request from the TLS connection, replaces the telescopic FQDN in the request URI with the FQDN of the p-NRF and sends the request towards p-SEPP in the TLS tunnel setup in step 2. The c-SEPP and the p-SEPP act as a man in the middle proxy in this case.

7. The p-SEPP extracts the HTTP message received on the TLS connection, and then seeing that the URI scheme of the NF discovery service of the p-NRF in the request URI is "https", the p-SEPP sets up a TLS connection with the p-NRF.

8. The p-SEPP forwards the NF discovery request to the p-NRF.

9. The p-NRF sends the NF discovery response within the TLS connection. The NF service profile contains service URI with "https" scheme. The FQDN of the NF service is an inter PLMN FQDN.

10. The p-SEPP forwards the NF discovery response within TLS tunnel setup in step 2 to the c-SEPP. The p-SEPP may replace the inter PLMN FQDN of the NF service producer's API endpoint with a label representing that FQDN. The p-SEPP re-maps the label with the NF service producer's API endpoint in step 17.

11. The c-SEPP upon receiving the HTTP response message for NF discovery response, within the TLS tunnel in step 2, replaces the trailing part of the inter PLMN FQDN of the NF service producer's API endpoint in the NF service profile with the FQDN of the c-SEPP, to form a telescopic FQDN as specified in clause 28.5.2 of 3GPP TS 23.003 [19]. The c-SEPP may replace the label part of the telescopic FQDN with a label of it's own significance. The p-SEPP re-maps the label in step 16.

12. The c-SEPP then forwards the NF discovery response to c-NRF, with the NF service profile containing the telescopic FQDN.

13. The c-NRF sends the NF discovery response to NF service consumer.

14. The NF service profile received at the NF service consumer contains service URI with "https" scheme. The NF service consumer sets up a TLS connection with the authoritative server for the telescopic FQDN (i.e. c-SEPP) received in step 13.

15. The NF service consumer sends the HTTP service request within the TLS connection to the c-SEPP.

16. The c-SEPP extracts the HTTP request from the TLS connection, replaces telescopic FQDN in the request URI with the FQDN of the NF service producer and sends the request towards p-SEPP in the TLS tunnel setup in step 2. The c-SEPP and the p-SEPP act as a man in the middle proxy in this case.

17. The p-SEPP extracts the HTTP message received on the TLS connection, and then seeing that the URI scheme of the NF service producer in the request URI is "https", the p-SEPP sets up a TLS connection with the NF service producer. The p-SEPP also replaces callback URI and link relations within the extracted HTTP message with a telescopic FQDN containing the FQDN of the p-SEPP as the trailing part, as specified in clause 6.1.4.3 of 3GPP TS 29.500 [4].

18. The p-SEPP forwards the HTTP request to the NF service producer.

19. The NF service producer sends the HTTP response within the TLS connection.

20. The p-SEPP forwards the HTTP response within TLS tunnel setup in step 2 to the c-SEPP.

21. The c-SEPP upon receiving the HTTP response message within the TLS tunnel setup in step 2, forwards the response to the NF service consumer. The c-SEPP replaces callback URI and link relations within the extracted HTTP response message with a telescopic FQDN containing the FQDN of the c-SEPP as the trailing part, as specified in clause 6.1.4.3 of 3GPP TS 29.500 [4].

### C.2.2.3 With TLS protection between NF and SEPP relying on 3gpp-Sbi-Target-apiRoot header, and TLS security without the 3gpp-Sbi-Target-apiRoot header used over N32f



Figure C.2.2.3-1 End to end call flow when https scheme URI is used, 3gpp-Sbi-Target-apiRoot header is used between NF and SEPP and TLS security without the 3gpp-Sbi-Target-apiRoot header is used between SEPPs

1. Same as step 1 of Figure C.2.2.2-1.

2. Same as step 2 of Figure C.2.2.2-1.

3. Same as step 3 of Figure C.2.2.2-1

4. The NRF on the NF service consumer side (c-NRF) needs to further initiate a discovery request to the NRF on the NF service producer side (p-NRF). The c-NRF uses "https" scheme URI to access the NF discovery service of the p-NRF. The c-NRF setups a TLS connection with the authoritative server for the SEPP FQDN (in the apiRoot of the Request URI) and verifies that the certificate presented by the endpoint of the TLS connection belongs to the authoritative server of the c-SEPP. The c-NRF is configured with the c-SEPP FQDN.

5. The c-NRF forwards the NF discovery request in this TLS connection, including an 3gpp-Sbi-Target-apiRoot header set to the apiRoot of the p-NRF.

6. The c-SEPP extracts the NF discovery request from the TLS connection, replaces the apiRoot of the SEPP FQDN in the request URI with the apiRoot of the p-NRF received in the 3gpp-Sbi-Target-apiRoot header and sends the request towards p-SEPP in the TLS tunnel setup in step 2. The c-SEPP and the p-SEPP act as a man in the middle proxy in this case.

7. The p-SEPP extracts the HTTP message received on the TLS connection, and then seeing that the URI scheme of the NF discovery service of the p-NRF is "https", the p-SEPP sets up a TLS connection with the p-NRF.

8. Same as step 8 of Figure C.2.2.2-1

9. Same as step 9 of Figure C.2.2.2-1

10. Same as step 10 of Figure C.2.2.2-1

11, 12. The c-SEPP forwards the NF discovery response to c-NRF.

13. Same as step 13 of Figure C.2.2.2-1

14. The NF service profile received at the NF service consumer contains service URI with "https" scheme. Since the URI of the p-NF contains an authority of a remote PLMN, the NF service consumer sets up a TLS connection with the authoritative server for the SEPP FQDN (i.e. c-SEPP). The c-NF is configured with the c-SEPP FQDN.

15. The NF service consumer sends the HTTP service request within the TLS connection to the c-SEPP, including a 3pp-Sbi-Target-apiRoot header set to the apiRoot of the p-NF.

16. The c-SEPP extracts the HTTP request from the TLS connection, replaces the apiRoot of the SEPP FQDN in the request URI with the apiRoot of the p-NRF received in the 3gpp-Sbi-Target-apiRoot header and sends the request towards p-SEPP in the TLS tunnel setup in step 2. The c-SEPP and the p-SEPP act as a man in the middle proxy in this case.

17. The p-SEPP extracts the HTTP message received on the TLS connection and then seeing that the URI scheme of the NF service producer is "https", the p-SEPP sets up a TLS connection with the NF service producer.

18. Same as step 18 of Figure C.2.2.2-1

19. Same as step 19 of Figure C.2.2.2-1

20. Same as step 20 of Figure C.2.2.2-1

21. The c-SEPP upon receiving the HTTP response message within the TLS tunnel setup in step 2, forwards the response to the NF service consumer.

### C.2.2.4 With TLS protection between NF and SEPP relying on telescopic FQDN, and TLS security with the 3gpp-Sbi-Target-apiRoot header used over N32f



Figure C.2.2.4-1: End to end call flow when https scheme URI is used, telescopic FQDNs are used between NF and SEPP and TLS security with the 3gpp-Sbi-Target-apiRoot header is used between SEPPs

1. Same as step 1 of Figure C.2.2.2-1.

2. Same as step 3 of Figure C.2.2.2-1.

3. Same as step 4 of Figure C.2.2.2-1.

4. Same as step 5 of Figure C.2.2.2-1

5. The c-SEPP setups a TLS connection with the authoritative server for the p-SEPP FQDN (in the apiRoot of the Request URI) and verifies that the certificate presented by the endpoint of the TLS connection belongs to the authoritative server of the p-SEPP. The c-SEPP is configured with the p-SEPP FQDN.

6. The c-SEPP sets the apiRoot in the request URI with the apiRoot of the p-SEPP, inserts the 3gpp-Sbi-Target-apiRoot header set to the apiRoot of the p-NRF derived from the telescopic FQDN received in step 4, and sends the request towards p-SEPP.

7. The p-SEPP extracts the HTTP message received on the TLS connection, replaces the apiRoot of the p-SEPP FQDN in the request URI with the apiRoot of the p-NRF received in the 3gpp-Sbi-Target-apiRoot header, and then seeing that the URI scheme of the NF discovery service of the p-NRF is "https", the p-SEPP sets up a TLS connection with the p-NRF.

8 to 15. Same as steps 8 to 15 of Figure C.2.2.3-1.

16. The c-SEPP extracts the HTTP request from the TLS connection, sets the apiRoot of the p-SEPP FQDN in the request URI, inserts the 3gpp-Sbi-Target-apiRoot header set to the apiRoot of the p-NF derived from the telescopic FQDN received in step 15, and sends the request towards p-SEPP.

17. The p-SEPP extracts the HTTP message received on the TLS connection, replaces the apiRoot of the p-SEPP FQDN in the request URI with the apiRoot of the p-NF received in the 3gpp-Sbi-Target-apiRoot header and then seeing that the URI scheme of the NF service producer is "https", the p-SEPP sets up a TLS connection with the NF service producer.

18 to 21. Same as steps 18 to 21 of Figure C.2.2.2-1

### C.2.2.5 With TLS protection between NF and SEPP relying on 3gpp-Sbi-Target-apiRoot header, and TLS security with the 3gpp-Sbi-Target-apiRoot header used over N32f



Figure C.2.2.5-1: End to end call flow when https scheme URI is used, 3gpp-Sbi-Target-apiRoot header is used between NF and SEPP and TLS security with the 3gpp-Sbi-Target-apiRoot header is used between SEPPs

1. Same as step 1 of Figure C.2.2.3-1.

2. Same as step 3 of Figure C.2.2.3-1

3. Same as step 4 of Figure C.2.2.3-1

4. Same as step 5 of Figure C.2.2.3-1.

5. The c-SEPP setups a TLS connection with the authoritative server for the p-SEPP FQDN (in the apiRoot of the Request URI) and verifies that the certificate presented by the endpoint of the TLS connection belongs to the authoritative server of the p-SEPP. The c-SEPP is configured with the p-SEPP FQDN.

6. The c-SEPP sets the apiRoot in the request URI with the apiRoot of the p-SEPP and sends the request towards p-SEPP including the 3gpp-Sbi-Target-apiRoot header received in step 4.

7. The p-SEPP extracts the HTTP message received on the TLS connection, replaces the apiRoot of the p-SEPP FQDN in the request URI with the apiRoot of the p-NRF received in the 3gpp-Sbi-Target-apiRoot header, and then seeing that the URI scheme of the NF discovery service of the p-NRF is "https", the p-SEPP sets up a TLS connection with the p-NRF.

8 to 15. Same as steps 8 to 15 of Figure C.2.2.3-1.

16. The c-SEPP extracts the HTTP request from the TLS connection, replaces the apiRoot of the c-SEPP FQDN in the request URI with the apiRoot of the p-SEPP, and sends the request towards p-SEPP including the 3gpp-Sbi-Target-apiRoot header received in step 15.

17. The p-SEPP extracts the HTTP message received on the TLS connection, replaces the apiRoot of the p-SEPP FQDN in the request URI with the apiRoot of the p-NF received in the 3gpp-Sbi-Target-apiRoot header and then seeing that the URI scheme of the NF service producer is "https", the p-SEPP sets up a TLS connection with the NF service producer.

18 to 21. Same as steps 18 to 21 of Figure C.2.2.2-1

# C.3 Application Layer Security between SEPPs

## C.3.1 When http URI scheme is used

The following figure shows the end to end call flow between an NF service consumer and a NF service producer in different PLMNs when:

- the SEPP in each PLMN acts as a security proxy;

- the negotiated security policy between the SEPPs is "PRINS";

- "http" scheme URI is used between the NF service consumer and NF service producer; and

- "http" scheme URI is used for accessing NRF's NF discovery service.



Figure C.3.1-1 End to end call flow when http scheme URI is used and "PRINS" security is used between SEPPs

1. The SEPP on the NF service consumer side (c-SEPP) and the SEPP on the NF service producer side (p-SEPP) negotiate the security capabilities using the procedure specified in clause 5.2.2. The SEPPs mutually negotiate to use "PRINS" as the security policy.

2. A TLS connection is setup between the c-SEPP and the p-SEPP for N32-f forwarding. If IPX-es are deployed between the c-SEPP and p-SEPP, the TLS connection is set up hop by hop with the authoritative server of the next hop.

3. Before the NF service consumer starts using the API of the NF service producer it needs to discover the NF service profile of the producer by querying the NRF. The NF service consumer uses "http" scheme URI to access the Nnrf\_NFDiscovery service.

4. The NRF on the NF service consumer side (c-NRF) needs to further initiate a discovery request to the NRF on the NF service producer side (p-NRF). The c-NRF is configured to route all HTTP messages with inter PLMN FQDN as the "authority" part of the URI via the c-SEPP. The c-SEPP acts as a HTTP proxy.

5. The c-SEPP forwards the NF discovery request within the N32-f TLS tunnel established in step 2 and using the JOSE protected message forwarding procedure and API specified in clauses 5.3 and 6.2 respectively. The apiRoot of the Request URI of the HTTP request shall contain the apiRoot of p-SEPP. The HTTP request shall not contain any 3gpp-Sbi-Target-apiRoot header.

6. The p-SEPP forwards the NF discovery request to the p-NRF.

7. The p-NRF sends the NF discovery response. The NF service profile contains service URI with "http" scheme. The FQDN of the NF service is an inter PLMN FQDN.

8. The p-SEPP forwards the NF discovery response within TLS tunnel to the c-SEPP using the JOSE protected message forwarding procedure and API specified in clauses 5.3 and 6.2 respectively.

9. The c-SEPP forwards the NF discovery response to c-NRF.

10. The c-NRF sends the NF discovery response to NF service consumer.

11. The NF service profile received at the NF service consumer contains service URI with "http" scheme. The NF service consumer initiates a HTTP message (as supported by the NF service producer API) using "http" scheme URI. The NF service consumer is configured to route all HTTP messages with inter PLMN FQDN as the "authority" part of the URI via the c-SEPP. The c-SEPP acts as a HTTP proxy.

12. The c-SEPP forwards the HTTP service request within the N32-f TLS tunnel established in step 2 and using the JOSE protected message forwarding procedure and API specified in clauses 5.3 and 6.2 respectively. The apiRoot of the Request URI of the HTTP request shall contain the apiRoot of p-SEPP. The HTTP request shall not contain any 3gpp-Sbi-Target-apiRoot header.

13. The p-SEPP forwards the HTTP service request to the NF service producer.

14. The NF service producer sends the HTTP service response.

15. The p-SEPP forwards the HTTP service response within TLS tunnel to the c-SEPP using the JOSE protected message forwarding procedure and API specified in clauses 5.3 and 6.2 respectively.

16. The c-SEPP forwards the HTTP service response to the NF service consumer.

## C.3.2 When https URI scheme is used

### C.3.2.1 General

The following figure shows the end to end call flow between an NF service consumer and a NF service producer in different PLMNs when:

- the SEPP in each PLMN acts as a security proxy;

- the negotiated security policy between the SEPPs is "PRINS";

- "https" scheme URI is used between the NF service consumer and NF service producer; and

- "https" scheme URI is used for accessing NRF's NF discovery service; and

- TLS protection between NF and SEPP relies on using telescopic FQDN or 3gpp-Sbi-Target-apiRoot header.

When https URI scheme is used, TLS protection between the Network Function and the SEPP may rely on using telescopic FQDN or 3gpp-Sbi-Target-apiRoot header. See clause 6.1.4.3 of 3GPP TS 29.500 [4].

### C.3.2.2 With TLS protection between NF and SEPP relying on telescopic FQDN



Figure C.3.2.2-1 End to end call flow when https scheme URI is used, telescopic FQDNs are used between NF and SEPP and "PRINS" security is used between SEPPs

1. The SEPP on the NF service consumer side (c-SEPP) and the SEPP on the NF service producer side (p-SEPP) negotiate the security capabilities using the procedure specified in clause 5.2.2. The SEPPs mutually negotiate to use "PRINS" as the security policy.

2. A TLS connection is setup between the c-SEPP and the p-SEPP for N32-f forwarding. If IPX-es are deployed between the c-SEPP and p-SEPP, the TLS connection is set up hop by hop with the authoritative server of the next hop.

3. Before the NF service consumer starts using the API of the NF service producer it needs to discover the NF service profile of the producer by querying the NRF. The NF service consumer uses "https" scheme URI to access the Nnrf\_NFDiscovery service. This implies that the NF service consumer sets up a TLS connection to the c-NRF and then sends the HTTP request over the TLS connection to the c-NRF.

4. The NRF on the NF service consumer side (c-NRF) needs to further initiate a discovery request to the NRF on the NF service producer side (p-NRF). The c-NRF uses "https" scheme URI to access the NF discovery service of the p-NRF. Since "https" requires setup of TLS connection with the p-NRF and it requires that c-NRF has to verify that the certificate presented by the endpoint of the TLS connection belngs to the authoritative server of the p-NRF, a telescopic FQDN with wildcarded certificate scheme mechanism is specified in 3GPP TS 33.501 [6]. The c-NRF is configured with the telescopic FQDN of the p-NRF with the telescopic FQDN having the FQDN of the c-SEPP as the trailing part. The c-NRF sets up a TLS connection with the authoritative server for the telescopic FQDN (i.e. the c-SEPP).

5. The c-NRF forwards the NF discovery request in this TLS connection.

6. The c-SEPP extracts the NF discovery request from the TLS connection, replaces the telescopic FQDN in the request URI with the FQDN of the p-NRF and sends the request towards p-SEPP in the TLS tunnel setup in step 2 and using the JOSE protected message forwarding procedure and API specified in clauses 5.3 and 6.2 respectively. The apiRoot of the Request URI of the HTTP request shall contain the apiRoot of p-SEPP. The HTTP request shall not contain any 3gpp-Sbi-Target-apiRoot header. The c-SEPP and the p-SEPP act as a man in the middle proxy in this case.

7. The p-SEPP extracts the HTTP message received on the TLS connection, and then seeing that the URI scheme of the NF discovery service of the p-NRF in the request URI is "https", the p-SEPP sets up a TLS connection with the p-NRF.

8. The p-SEPP forwards the NF discovery request to the p-NRF.

9. The p-NRF sends the NF discovery response within the TLS connection. The NF service profile contains service URI with "https" scheme. The FQDN of the NF service is an inter PLMN FQDN.

10. The p-SEPP forwards the NF discovery response within TLS tunnel setup in step 2 using the JOSE protected message forwarding procedure and API specified in clauses 5.3 and 6.2 respectively, to the c-SEPP. The p-SEPP may replace the inter PLMN FQDN of the NF service producer's API endpoint with a label representing that FQDN. The p-SEPP re-maps the label with the NF service producer's API endpoint in step 17.

11. The c-SEPP upon receiving the HTTP response message for NF discovery response, within the TLS tunnel in step 2, replaces the trailing part of the inter PLMN FQDN of the NF service producer's API endpoint in the NF service profile with the FQDN of the c-SEPP, to form a telescopic FQDN as specified in clause 28.5.2 of 3GPP TS 23.003 [19]. The c-SEPP may replace the label part of the telescopic FQDN with a label of it's own significance. The p-SEPP re-maps the label in step 16.

12. The c-SEPP then forwards the NF discovery response to c-NRF, with the NF service profile containing the telescopic FQDN.

13. The c-NRF sends the NF discovery response to NF service consumer.

14. The NF service profile received at the NF service consumer contains service URI with "https" scheme. The NF service consumer sets up a TLS connection with the authoritative server for the telescopic FQDN (i.e. the c-SEPP).

15. The NF service consumer sends the HTTP service request within the TLS connection to the c-SEPP.

16. The c-SEPP extracts the HTTP request from the TLS connection, replaces the telescopic FQDN in the request URI with the FQDN of the NF service producer and sends the request towards p-SEPP in the TLS tunnel setup in step 2 using the JOSE protected message forwarding procedure and API specified in clauses 5.3 and 6.2 respectively. The apiRoot of the Request URI of the HTTP request shall contain the apiRoot of p-SEPP. The HTTP request shall not contain any 3gpp-Sbi-Target-apiRoot header. The c-SEPP and the p-SEPP act as a man in the middle proxy in this case.

17. The p-SEPP extracts the HTTP message received on the TLS connection, then seeing that the URI scheme of the NF service producer in the request URI is "https", the p-SEPP sets up a TLS connection with the NF service producer. The p-SEPP also replaces callback URI and link relations within the extracted HTTP message with a telescopic FQDN containing the FQDN of the p-SEPP as the trailing part, as specified in clause 6.1.4.3 of 3GPP TS 29.500 [4].

18. The p-SEPP forwards the HTTP request to the NF service producer.

19. The NF service producer sends the HTTP response within the TLS connection.

20. The p-SEPP forwards the HTTP response within TLS tunnel setup in step 2 to the c-SEPP using the JOSE protected message forwarding procedure and API specified in clauses 5.3 and 6.2 respectively.

21. The c-SEPP upon receiving the HTTP response message within the TLS tunnel setup in step 2, forwards the response to the NF service consumer. The c-SEPP replaces callback URI and link relations within the extracted HTTP response message with a telescopic FQDN containing the FQDN of the c-SEPP as the trailing part, as specified in clause 6.1.4.3 of 3GPP TS 29.500 [4].

### C.3.2.3 With TLS protection between NF and SEPP relying on 3gpp-Sbi-Target-apiRoot header



Figure C.3.2.3-1 End to end call flow when https scheme URI is used, 3gpp-Sbi-Target-apiRoot header is used between NF and SEPP and "PRINS" security is used between SEPPs

1. Same as step 1 of Figure C.3.2.2-1.

2. Same as step 2 of Figure C.3.2.2-1.

3. Same as step 3 of Figure C.3.2.2-1.

4. The NRF on the NF service consumer side (c-NRF) needs to further initiate a discovery request to the NRF on the NF service producer side (p-NRF). The c-NRF uses "https" scheme URI to access the NF discovery service of the p-NRF. The c-NRF uses "https" scheme URI to access the NF discovery service of the p-NRF. The c-NRF setups a TLS connection with the authoritative server for the SEPP FQDN (in the apiRoot of the Request URI) and verifies that the certificate presented by the endpoint of the TLS connection belongs to the authoritative server of the c-SEPP. The c-NRF is configured with the c-SEPP FQDN.

5. The c-NRF forwards the NF discovery request in this TLS connection, including an 3gpp-Sbi-Target-apiRoot header set to the apiRoot of the p-NRF.

6. The c-SEPP extracts the NF discovery request from the TLS connection, replaces the apiRoot of the SEPP FQDN in the request URI with the apiRoot of the p-NRF received in the 3gpp-Sbi-Target-apiRoot header and sends the request towards p-SEPP in the TLS tunnel setup in step 2 and using the JOSE protected message forwarding procedure and API specified in clauses 5.3 and 6.2 respectively. The apiRoot of the Request URI of the HTTP request shall contain the apiRoot of p-SEPP. The HTTP request shall not contain any 3gpp-Sbi-Target-apiRoot header. The c-SEPP and the p-SEPP act as a man in the middle proxy in this case.

7. The p-SEPP extracts the HTTP message received on the TLS connection, and then seeing that the URI scheme of the NF discovery service of the p-NRF is "https", the p-SEPP sets up a TLS connection with the p-NRF.

8. Same as step 8 of Figure C.3.2.2-1.

9. Same as step 9 of Figure C.3.2.2-1.

10. Same as step 10 of Figure C.3.2.2-1.

11, 12. The c-SEPP forwards the NF discovery response to c-NRF.

13. Same as step 13 of Figure C.3.2.2-1.

14. The NF service profile received at the NF service consumer contains service URI with "https" scheme. Since the URI of the p-NF contains an authority of a remote PLMN, the NF service consumer sets up a TLS connection with the authoritative server for the SEPP FQDN (i.e. c-SEPP). The c-NF is configured with the c-SEPP FQDN.

15. The NF service consumer sends the HTTP service request within the TLS connection to the c-SEPP, including a 3pp-Sbi-Target-apiRoot header set to the apiRoot of the p-NF.

16. The c-SEPP extracts the HTTP request from the TLS connection, replaces the apiRoot of the SEPP FQDN in the request URI with the apiRoot of the p-NF received in the 3gpp-Sbi-Target-apiRoot header and sends the request towards p-SEPP in the TLS tunnel setup in step 2 using the JOSE protected message forwarding procedure and API specified in clauses 5.3 and 6.2 respectively. The c-SEPP and the p-SEPP act as a man in the middle proxy in this case. The apiRoot of the Request URI of the HTTP request shall contain the apiRoot of p-SEPP. The HTTP request shall not contain any 3gpp-Sbi-Target-apiRoot header.

17. The p-SEPP extracts the HTTP message received on the TLS connection, and then seeing that the URI scheme of the NF service producer is "https", the p-SEPP sets up a TLS connection with the NF service producer.

18. Same as step 18 of Figure C.3.2.2-1.

19. Same as step 19 of Figure C.3.2.2-1.

20. Same as step 20 of Figure C.3.2.2-1.

21. The c-SEPP upon receiving the HTTP response message within the TLS tunnel setup in step 2, forwards the response to the NF service consumer.

Annex D (informative):  
Withdrawn API versions

# D.1 General

This Annex lists withdrawn API versions of the APIs defined in the present specification. 3GPP TS 29.501 [5] clause 4.3.1.6 describes the withdrawal of API versions.

# D.2 N32 Handshake API

The API versions listed in table D.2-1 are withdrawn for the N32 Handshake API.

Table D.2-1: Withdrawn API versions of the N32 Handshake API service

|  |  |
| --- | --- |
| API version number | Reason for withdrawal |
| 1.0.0 | A backward incompatible change has been introduced in v1.0.1 to align with related stage 2 specifications. Indeed, the term "ALS" has been replaced by "PRINS" during the handshake procedure. As a consequence, the v1.0.0 must not be used in the field in order to avoid interoperability problem between roaming partners. |

Annex E (informative):  
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2018-07 | CT4#85bis | C4-185523 |  |  |  | TS Skeleton, Scope, General Description and N32 Procedures. Implementation of C4-185531, C4-185353, C4-185352, C4-185469 | 0.1.0 |
| 2018-08 | CT4#86 | C4-186630 |  |  |  | Implementations of PCRs agreed in CT4#86 - C4-186157, C4-186421, C4-186422, C4-186423, C4-186425 and C4-186599 | 0.2.0 |
| 2018-09 | CT#81 | CP-182082 |  |  |  | Presented for information and approval | 1.0.0 |
| 2018-09 | CT#81 | CP-182233 |  |  |  | Approved in CT#81 | 15.0.0 |
| 2018-12 | CT#82 | CP-183026 | 0001 | 1 | F | Resolve the editor's note on HTTP/2 connection management | 15.1.0 |
| 2018-12 | CT#82 | CP-183026 | 0002 | 1 | F | Clarification to N32-f Forwarding Procedure | 15.1.0 |
| 2018-12 | CT#82 | CP-183026 | 0003 | 2 | F | N32-f Error Reporting | 15.1.0 |
| 2018-12 | CT#82 | CP-183026 | 0004 | 2 | F | Resolve editor's notes on identification of notifications | 15.1.0 |
| 2018-12 | CT#82 | CP-183026 | 0005 | 2 | F | Resolve Editor's Notes on RequestId and NextHopId | 15.1.0 |
| 2018-12 | CT#82 | CP-183026 | 0006 | 2 | F | General Cleanup | 15.1.0 |
| 2018-12 | CT#82 | CP-183026 | 0007 | 1 | F | OpenAPI for N32 Handshake API | 15.1.0 |
| 2018-12 | CT#82 | CP-183196 | 0008 | 2 | F | OpenAPI for JOSE Protected Message Forwarding API on N32-f | 15.1.0 |
| 2018-12 | CT#82 | CP-183026 | 0009 | 1 | F | Cardinality | 15.1.0 |
| 2018-12 | CT#82 | CP-183026 | 0010 | - | F | Error Handling Clauses | 15.1.0 |
| 2019-06 | CT#84 | CP-191043 | 0011 | 4 | F | PLMN ID verification at receiving SEPP | 15.2.0 |
| 2019-06 | CT#84 | CP-191043 | 0012 | 1 | F | Informative Annex on End to End Call Flow via SEPP | 15.2.0 |
| 2019-06 | CT#84 | CP-191043 | 0013 | 2 | F | Storage of OpenAPI specification files | 15.2.0 |
| 2019-06 | CT#84 | CP-191043 | 0014 |  | F | New name for Application Layer Security protocol | 15.2.0 |
| 2019-06 | CT#84 | CP-191043 | 0015 | 1 | F | Copyright Note in YAML file | 15.2.0 |
| 2019-06 | CT#84 | CP-191043 | 0016 |  | F | 3GPP TS 29.573 API version update | 15.2.0 |
| 2019-09 | CT#85 | CP-192114 | 0017 |  | F | ALS renaming to PRINS | 15.3.0 |
| 2019-09 | CT#85 | CP-192114 | 0019 | 1 | F | Add an Annex to Withdrawn N32 Handshake API v1.0.0 | 15.3.0 |
| 2019-09 | CT#85 | CP-192123 | 0018 | 1 | B | Telescopic FQDN Mapping Service | 16.0.0 |
| 2019-09 | CT#85 | CP-192080 | 0020 | 2 | B | Exchange IPX security information lists | 16.0.0 |
| 2019-09 | CT#85 | CP-192123 | 0021 |  | F | SecurityNegotiateReqData in the Security Capability Negotiation | 16.0.0 |
| 2019-09 | CT#85 | CP-192120 | 0023 |  | F | 3GPP TS 29.573 API Version Update | 16.0.0 |
| 2019-10 |  |  |  |  |  | Corrupted references fixed | 16.0.1 |
| 2019-12 | CT#86 | CP-193063 | 0024 |  | F | Certificate and Public key Encoding | 16.1.0 |
| 2019-12 | CT#86 | CP-193044 | 0026 |  | F | 3GPP TS 29.573 API version update | 16.1.0 |
| 2020-03 | CT#87 | CP-200039 | 0027 | 2 | F | Add Corresponding API descriptions in clause 5.1 | 16.2.0 |
| 2020-03 | CT#87 | CP-200016 | 0028 | 3 | F | Inter-PLMN communication using 3gpp-Sbi-Target-apiRoot | 16.2.0 |
| 2020-03 | CT#87 | CP-200047 | 0030 | 2 | F | Corrections to N32 procedures for PRINS (PRotocol for N32 INterconnect Security) | 16.2.0 |
| 2020-03 | CT#87 | CP-200039 | 0031 | 2 | D | Editorial corrections | 16.2.0 |
| 2020-03 | CT#87 | CP-200039 | 0032 | 1 | F | Correction - formatting consistency | 16.2.0 |
| 2020-03 | CT#87 | CP-200140 | 0033 | 3 | B | 29573 CR optionality of ProblemDetails | 16.2.0 |
| 2020-03 | CT#87 | CP-200052 | 0035 |  | F | 3GPP TS 29.573 Rel16 API External doc update | 16.2.0 |
| 2020-07 | CT#88 | CP-201061 | 0036 |  | F | Storage of YAML files in ETSI Forge | 16.3.0 |
| 2020-07 | CT#88 | CP-201061 | 0037 | 1 | F | Data type column in Resource URI variables Table | 16.3.0 |
| 2020-07 | CT#88 | CP-201061 | 0038 | 1 | F | Add custom operation Name | 16.3.0 |
| 2020-07 | CT#88 | CP-201327 | 0039 | 1 | F | 29.573 Rel-16 API version and External doc update | 16.3.0 |
| 2020-09 | CT#89 | CP-202110 | 0040 | 1 | F | N32f Error Type | 16.4.0 |
| 2020-09 | CT#89 | CP-202119 | 0041 | 1 | F | TLS security with the 3gpp-Sbi-Target-apiRoot header on N32f | 16.4.0 |
| 2020-09 | CT#89 | CP-202119 | 0042 |  | F | Corrections to PRINS call flows | 16.4.0 |
| 2020-09 | CT#89 | CP-202023 | 0044 | 3 | F | Error handling of mismatch of polices at SEPP | 16.4.0 |
| 2020-09 | CT#89 | CP-202043 | 0046 | 2 | F | Correction of flow description | 16.4.0 |
| 2020-09 | CT#89 | CP-202096 | 0047 |  | F | 29.573 Rel-16 API version and External doc update | 16.4.0 |
| 2020-12 | CT#90 | CP-203048 | 0049 | 3 | F | PLMN ID handling over N32 | 16.5.0 |
| 2020-12 | CT#90 | CP-203048 | 0050 | 2 | F | N32-f payload compression | 16.5.0 |
| 2020-12 | CT#90 | CP-203037 | 0051 |  | F | Update of the metaData | 16.5.0 |
| 2020-12 | CT#90 | CP-203037 | 0052 | 2 | F | Exchange of the modification policy | 16.5.0 |
| 2020-12 | CT#90 | CP-203035 | 0053 |  | F | Storage of YAML files in 3GPP Forge | 16.5.0 |
| 2020-12 | CT#90 | CP-203037 | 0054 | 2 | F | Update the description of IeType | 16.5.0 |
| 2020-12 | CT#90 | CP-203036 | 0055 |  | F | Rel-16 API version and External doc update | 16.5.0 |
| 2021-03 | CT#91-e | CP-210062 | 0058 |  | F | dataToEncrypt encoding in DataToIntegrityProtectAndCipherBlock | 16.6.0 |
| 2021-03 | CT#91-e | CP-210058 | 0059 | 1 | F | Error handling for encBlockIndex | 16.6.0 |
| 2021-03 | CT#91-e | CP-210054 | 0062 |  | F | 29.573 Rel-16 API version and External doc update | 16.6.0 |
| 2021-06 | CT#92-e | CP-211081 | 0067 | 1 | F | Annex C.2.2.2 & C.3.2.2 correction of Telescopic FQDN handling in call flow over N32 | 16.7.0 |
| 2021-09 | CT#93-e | CP-212076 | 0070 | 4 | F | Correction on Parameter Exchange procedure | 16.8.0 |
| 2021-09 | CT#93-e | CP-212076 | 0072 | 1 | F | Via and server header | 16.8.0 |
| 2021-09 | CT#93-e | CP-212082 | 0077 | 1 | A | Essential Correction in TLS for N32-f | 16.8.0 |
| 2022-03 | CT#95-e | CP-220080 | 0087 | 1 | F | SEPP for interconnect scenarios | 16.9.0 |
| 2022-03 | CT#95-e | CP-220080 | 0074 | 2 | F | PLMN Specific N32-C connection | 16.9.0 |
| 2022-03 | CT#95-e | CP-220067 | 0091 |  | F | 29.573 Rel-16 API version and External doc update | 16.9.0 |
| 2022-06 | CT#96 | CP-221069 | 0102 | 1 | F | Message Containing Multipart Binary | 16.10.0 |
| 2022-06 | CT#96 | CP-221069 | 0106 |  | F | JWE Authentication tag | 16.10.0 |
| 2022-06 | CT#96 | CP-221070 | 0110 |  | F | 29.573 Rel-16 API version and External doc update | 16.10.0 |
| 2022-09 | CT#97-e | CP-222051 | 0118 |  | F | Correction on applying modification policies | 16.11.0 |
| 2022-09 | CT#97-e | CP-222071 | 0114 | 1 | F | Modification policy in IPX | 16.11.0 |