3GPP TS 32.591 V16.0.0 (2020-07)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Services and System Aspects;

Telecommunication management;   
Home enhanced Node B (HeNB)   
Operations, Administration, Maintenance and Provisioning (OAM&P);   
Concepts and requirements for Type 1 interface HeNB to HeNB Management System (HeMS)

(Release 16)

* *

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.   
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.   
This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

Keywords

3GPP, management

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword [4](#__RefHeading___Toc295905888)

Introduction [4](#__RefHeading___Toc295905889)

1 Scope [5](#__RefHeading___Toc295905890)

2 References [5](#__RefHeading___Toc295905891)

3 Definitions and abbreviations [5](#__RefHeading___Toc295905892)

3.1 Definitions [5](#__RefHeading___Toc295905893)

3.2 Abbreviations [5](#__RefHeading___Toc295905894)

4 Concepts and background [6](#__RefHeading___Toc295905895)

5 Business level requirements [6](#__RefHeading___Toc295905896)

5.1 Requirements [6](#__RefHeading___Toc295905897)

5.1.1 Configuration Management [6](#__RefHeading___Toc295905898)

5.1.2 Performance Management [6](#__RefHeading___Toc295905899)

5.1.3 Fault Management [7](#__RefHeading___Toc295905900)

5.1.4 Security Management [7](#__RefHeading___Toc295905901)

5.2 Actor roles [7](#__RefHeading___Toc295905902)

5.3 Telecommunications resources [7](#__RefHeading___Toc295905903)

5.4 High level use cases [7](#__RefHeading___Toc295905904)

6 Specification level requirements [7](#__RefHeading___Toc295905905)

6.1 Requirements [7](#__RefHeading___Toc295905906)

6.1.1 Configuration Management [7](#__RefHeading___Toc295905907)

6.1.2 Performance Management [8](#__RefHeading___Toc295905908)

6.1.3 Fault Management [8](#__RefHeading___Toc295905909)

6.1.4 Security Management [9](#__RefHeading___Toc295905910)

6.2 Actor roles [10](#__RefHeading___Toc295905911)

6.3 Telecommunications resources [10](#__RefHeading___Toc295905912)

6.4 Use cases [10](#__RefHeading___Toc295905913)

Annex A (informative): Change history [11](#__RefHeading___Toc295905914)

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# Introduction

The present document is part of a TS-family covering the 3rd Generation Partnership Project Technical Specification Group Services and System Aspects, Telecommunication Management; as identified below:

3GPP TS 32.591: "Telecommunications management; Home eNode B (HeNB) Operations, Administration, Maintenance and Provisioning (OAM&P); Concepts and requirements for Type 1 interface HeNB to HeNB Management System (HeMS)".

3GPP TS 32.592: "Telecommunications management; Home eNode B (HeNB) Operations, Administration, Maintenance and Provisioning (OAM&P); Information model for Type 1 interface HeNB to HeNB Management System (HeMS) ".

3GPP TS 32.593: "Telecommunications management; Home eNode B (HeNB) Operations, Administration, Maintenance and Provisioning (OAM&P); Procedure flows for Type 1 interface HeNB to HeNB Management System (HeMS)".

3GPP TS 32.594: "Telecommunications management; Home eNode B (HeNB) Operations, Administration, Maintenance and Provisioning (OAM&P); Data definitions for Type 1 interface HeNB to HeNB Management System (HeMS)".

# 1 Scope

The present document describes the concepts and requirements of OAM for Home eNodeB (HeNB). The requirements captured in this document shall be met via Type 1 interface between HeNB and HeMS.

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 32.101: "Telecommunication management; Principles and high level requirements".

[3] 3GPP TS 32.102: "Telecommunication management; Architecture".

[4] TR-069 Amendment 2, CPE WAN Management Protocol v1.1, Broadband Forum.

[5] 3GPP TS 32.435: "Performance Measurement, eXtensible Markup Language (XML) file format definition".

[6] 3GPP TS 32.111-2: "Telecommunication management; Fault Management; Alarm Integration Reference Point (IRP): Information Service (IS) ".

[7] 3GPP TS 22.220: " Service requirements for Home Node B (HNB) and Home eNode B (HeNB)".

[8] 3GPP TS 33.320: "Security of Home Node B (HNB) / Home evolved Node B (HeNB)".

[9] 3GPP TS 32.551: " Energy Saving Management (ESM); Concepts and requirements ".

[10] 3GPP TR 32.826: " Study on Energy Savings Management (ESM) ".

# 3 Definitions and abbreviations

For the purposes of the present document, the terms and definitions given in TS 32.101 [2], TS 32.102 [3] and TS 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in TS 32.101 [2], TS 32.102 [3] and TS 21.905 [1], in that order.

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in TR 21.905 [1].

## 3.2 Abbreviations

For the purposes of the present document, the following abbreviations apply:

HeMS Home eNodeB Management System

HeNB Home eNodeB

# 4 Concepts and background

Home eNodeB has the following characteristics:

- The quantity of Home eNodeBs is likely to be large

- There may be many Home eNodeB vendors

- The location of Home eNodeB could be in a private residence which may not be accessible for frequent on-site maintenance

Based on the above characteristics, this specification defines the functionalities needed for the management of Home eNodeB over a Type 1 interface.

# 5 Business level requirements

## 5.1 Requirements

### 5.1.1 Configuration Management

**REQ-OAMP\_CM-CON-001** The HeNB shall be able to automatically, i.e. without human operator on-line interaction or attention, configure itself to be ready for service when powered up and connected to HeMS.

**REQ-OAMP\_CM-CON-002** The HeNB shall be able to automatically, i.e. without human operator on-line interaction or attention, configure itself to be in service when powered up and connected to HeMS.

**REQ-OAMP\_CM-CON-003** The HeNB shall be able to automatically, i.e. without human operator on-line interaction or attention, upgrade its software/firmware and configuration.

**REQ-OAMP\_CM-CON-004** The HeNB auto-configuration shall be done in such way that the performance of the surrounding macro cells is not adversely affected.

**REQ-OAMP\_CM-CON-005** The HeNB auto-configuration function should be adaptive to react to change in the network and changes in the radio environment.

**REQ-OAMP\_CM-CON-006** The operator shall be able to remotely reboot the HeNB.

**REQ-OAMP\_CM-CON-007** The operator shall be able to remotely start/stop the radio transmission of the HeNB.

**REQ-OAMP\_CM-CON-008** In case IPsec is used, the system should be engineered to ensure that the HeNB IP address changes as minimally as possible.

**REQ-OAMP\_CM-CON-009** The operator shall be able to remotely reconfigure the frequency and radio bandwidth of HeNB to adapt to changes in the radio environment and required bandwidth.

**REQ-OAMP\_CM-CON-010** The HeNB should allow configuration of the IPsec or non-IPsec usage option based on the operator’s policy [8].

**REQ-OAMP\_CM-CON-011** The operator shall be able to activate/deactivate energy savings on one or multiple HeNBs in the network [9][10].

**REQ-OAMP\_CM-CON-012** The operator shall be able to configure energy saving policy for the one or more HeNBs in the network [9][10].

### 5.1.2 Performance Management

**REQ-OAMP\_PM-CON-001** The HeNB may have the capability to collect its performance related data.

**REQ-OAMP\_PM-CON-002** The HeNB shall send performance data based on operator configured policy.

**REQ-OAMP\_PM-CON-003** Operator shall be able to retrieve performance data file from the HeNB.

### 5.1.3 Fault Management

**REQ-OAMP\_FM-CON-001** The HeNB shall support Fault Management to enable the operator to monitor and manage the HeNB.

**REQ-OAMP\_FM-CON-002** The HeNB shall provide alarm related information only on demand by the operator or based on operator configured policy.

### 5.1.4 Security Management

**REQ-OAMP\_SM-CON-001** The HeNB shall have the capability to protect itself against Denial of Service attack over the Type 1 interface.

## 5.2 Actor roles

Not defined in this version.

## 5.3 Telecommunications resources

Not defined in this version.

## 5.4 High level use cases

### 5.4.1 HeNB Energy Saving use cases

UC1a: Capacity-Limited Networks

Capacity-limited networks are normally dimensioned to cope with peak time traffic demand and can hence be under-utilized in off-peak times peak time traffic demand e.g. at certain hours of the night, when the overall load as well as the load distribution onto the different cells may differ significantly from peak times.

For energy saving management in such networks, the objective is therefore to adapt the network to these changing conditions by activating energy saving on selected cells. One approach is to concentrate the load into a few selected cells that remain active during low traffic demand periods with increased coverage area and to deactivate the remaining less loaded cells.

UC1b: Hybrid E-UTRAN Macro Cell and HeNB Cell Coverage

A variation of the above use case is to have all cells in the building can be shut down. The overlay macro cell can provide coverage for all the HeNBs in that area.

Depending on the architecture, energy saving decisions and corresponding state transfers are made by network elements (or element / domain managers) or by network management systems.

# 6 Specification level requirements

## 6.1 Requirements

### 6.1.1 Configuration Management

The requirements for configuration management are as follows:

**REQ-OAMP\_CM-FUN-001** The HeNB configuration shall be administered by the HeMS utilising the TR-069 CWMP Protocol, reference [4].

**REQ-OAMP\_CM-FUN-002** HeMS shall be able to reboot the HeNB.

**REQ-OAMP\_CM-FUN-003** HeMS shall have remote access to the HeNB to start/stop the radio transmission.

**REQ-OAMP\_CM-FUN-004** HeMS shall have remote access to the HeNB to start/stop the radio transmission on the frequencies specified by HeMS.

**REQ-OAMP\_CM-FUN-005** HeMS shall maintain the configuration data of the HeNB.

**REQ-OAMP\_CM-FUN-006** When the HeNB is initially powered up and connected to the HeMS, HeMS shall send the initially needed configuration data to the HeNB.

**REQ-OAMP\_CM-FUN-007** If the inner IPsec tunnel IP address of the HeNB changes and HeNB is connected to HeMS via IPsec Tunnel then the HeNB shall notify the HeMS using TR-069.

**REQ-OAMP\_CM-FUN-008** The HeMS shall specify which parameters it needs to be notified of when the HeNB changes their values through auto-configuration. The HeNB shall notify the HeMS of changes in the values of any such auto-configured parameters.

**REQ-OAMP\_CM-FUN-009** The HeNB shall inform the HeMS of its ability to auto-configure parameters or groups of parameters that are relevant to the HeMS.

**REQ-OAMP\_CM-FUN-010** HeMS shall be able to specify a value, or a valid range of values, for any parameter that is auto-configurable by the HeNB.

**REQ-OAMP\_CM-FUN-011** Configuration management capability for the HeNB shall be supported by means of TR-069 RPCs SetParameterValues, AddObject and DeleteObject . Optionally a bulk configuration management file may be supported. In this case the TR-069 manager uses the RPC download method to trigger a CM file download from a file server.

**REQ-OAMP\_CM-FUN-012** The HeNB shall provide a capability allowing the HeMS to manage downloading of HeNB software/firmware image files and provide mechanisms for version identification and notification to the HeMS of the success or failure of a file download.

**REQ-OAMP\_CM-FUN-013** In normal operation, the HeNB shall maintain its configuration data following a HeNB reboot.

**REQ-OAMP\_CM-FUN-014** The HeNB shall support capabilities to inform the HeMS about the results of specific actions triggered by the HeMS.

**REQ-OAMP\_CM-FUN-015** It shall be possible to initiate a management connection at the request of either the HeNB or the HeMS.

**REQ-OAMP\_CM-FUN-016** The HeNB shall be able to inform the HeMS of the changes in radio environment and required radio bandwidth.

**REQ-OAMP\_CM-FUN-017** The operator shall be able to remotely reconfigure the frequency and radio bandwidth of HeNB.

**REQ-OAMP\_CM-FUN-018** If the HeNB is unable to offer service for an operator configured time period it will deactivate the air interface.

**REQ-OAMP\_CM-FUN-019** The HeNB shall support a capability to allow the HeMS to activate Local IP Access.

**REQ-OAMP\_CM-FUN-020** The HeNB shall support a capability to allow the HeMS to deactivate Local IP Access.

**REQ-OAMP\_CM-FUN-021** The HeMS should be able to securely configure the HeNB according to the operator's policy, whether or not to use IPsec for subsequent connections.

**REQ-OAMP\_CM-FUN-022** The HeNB should support a capability allowing the HeMS to initiate energy saving activation.

**REQ-OAMP\_CM-FUN-023** The HeNB should support a capability allowing the HeMS to initiate energy saving deactivation.

**REQ-OAMP\_CM-FUN-024** When a HeNB is in energySaving state the HeMS shall not consider the NE as a fault, and no alarms shall be raised.

**REQ-OAMP\_CM-FUN-025** The HeNB should support a capability allowing the HeMS to configure the time period during which energy saving is allowed or not allowed.

**REQ-OAMP\_CM-FUN-026** The HeNB should support a capability to notify the HeMS when it goes into or out of energySaving state.

**REQ-OAMP\_CM-FUN-027** The HeNB should support a capability allowing the HeMS to configure a cell traffic load threshold and time duration to be used for the decision if a network element goes into energySaving state.

**REQ-OAMP\_CM-FUN-028** The HeNB should support a capability allowing the HeMS to configure a cell traffic load threshold to be used for the decision if a network element goes out of energySaving state.

### 6.1.2 Performance Management

The HeNB may support Performance Management to enable the operator to monitor the HeNB network based on the business level requirements.

The requirements for performance management are as follows.

**REQ-OAMP\_PM-FUN-001** The HeNB may have the Performance Management capabilities administered by the HeMS.

**REQ-OAMP\_PM-FUN-002** The HeNB shall support the retrieval of the Performance Information from the HeNB utilising the file transfer option of TR-069 CWMP Protocol, reference [4].

**REQ-OAMP\_PM-FUN-003** The HeNB shall be configurable by the HeMS to produce an XML File at regular intervals which contains the HeNB performance Information and then upload the XML File.

**REQ-OAMP\_PM-FUN-004** The XML File Formats produced by the HeNB shall adhere to the 3GPP XML Performance Management File Formats, reference [5].

**REQ-OAMP\_PM-FUN-005** The HeNB shall upload PM files using TR-069 compliant file transfer protocols.

**REQ-OAMP\_PM-FUN-006** HeMS shall have the ability to configure policies for the HeNB performance data file upload.

### 6.1.3 Fault Management

**REQ-OAMP\_FM-FUN-001** The HeNB shall have the Fault Management capabilities administered through the HeMS.

**REQ-OAMP\_FM-FUN-002** The HeNB shall have the ability to send alarm related information to HeMS according to operator configured policy.

**REQ-OAMP\_FM-FUN-003** The alarm related information to be sent to the HeMS by the HeNB shall support the inclusion of the appropriate Information attributes, as defined in 3GPP TS.32.111-2, reference [6].

**REQ-OAMP\_FM-FUN-004** The HeNB shall maintain the following information:

a. Alarm Management Information – which contains the alarm management and reporting parameters configurable by the HeMS

b. Alarms List – Alarms currently active on the HeNB

c. Alarm History – contains the alarms previously created by the HeNB.

d. Pending Delivery Queue – contains the alarms queued to be sent to the HeMS on the next management connection

**REQ-OAMP\_FM-FUN-005** The HeNB shall support the following ways of alarm handling:

a. Expedited handling– the HeNB connects to the HeMS immediately to raise the alarm and logs the alarm in the Alarm History.

b. Queued handling – the HeNB queues the alarm internally pending connection to the HeMS, logs the alarm in the Alarm History, and delivers the alarm on the next connection to the HeMS

c. Logged handling – the HeNB does not send the alarm to the HeMS and logs the alarm in the Alarm History.

d. Disabled handling– the HeNB does not send the alarm to the HeMS and will not log the alarm in the Alarm History

**REQ-OAMP\_FM-FUN-006** The HeMS may configure the alarm handling for each type of HeNB alarm according to the HeNB alarm handling capabilities and the default handling if not specified by the HeMS shall be “Logged handling”.

**REQ-OAMP\_FM-FUN-007** The HeMS shall have the ability to throttle the sending of alarms from the HeNB to the HeMS

**REQ-OAMP\_FM-FUN-008** The HeMS shall have the capability to retrieve alarm related information from the HeNB using TR-069 RPC Method Calls.

**REQ-OAMP\_FM-FUN-009** The HeMS shall have the capability to completely purge on the HeNB the Alarms List and the Pending Delivery Queue and may have the capability to completely purge on the HeNB the history of Alarms.

**REQ-OAMP\_FM-FUN-010** The HeMS shall have the capability to activate and deactivate the alarm reporting by the HeNB.

**REQ-OAMP\_FM-FUN-011** The HeMS shall be able to define the frequency of passive reporting.

**REQ-OAMP\_FM-FUN-012** The HeMS shall be informed immediately of alarms (raised, changed, cleared) classified as expedited notifications only.

**REQ-OAMP\_FM-FUN-013** The HeNB shall provide a capability allowing the HeMS to access information that it may use to diagnose and resolve connectivity or service issues.

### 6.1.4 Security Management

**REQ-OAMP\_SM-FUN-001**.The HeNB shall have the capability to communicate with the HeMS via TR-069 CWMP, reference [4], through the support of one of the two security mechanisms determined by the Network Operator’s Security Policies:

- utilising SSL/TLS outside the IPsec Tunnel

- within the IPsec Tunnel with the option to utilise SSL/TLS within the IPsec Tunnel for additional end-to-end security

TR-069 CPE devices are currently factory programmed with a Bootstrap HeMS URL only and therefore the HeNB capable CPEs requiring to utilise IPsec for connection to the HeMS either require to be factory programmed with Bootstrap Security Gateway/IPsec Information or this information is supplied outside of the IPsec tunnel before tunnel establishment utilising SSL/TLS.

**REQ-OAMP\_SM-FUN-002** The HeNB shall provide a capability to prevent tampering with the interactions that take place between the HeNB and the HeMS as well as management functions of a HeNB.

**REQ-OAMP\_SM-FUN-003** The HeNB shall provide a capability allowing the HeMS to authenticate the HeNBs.

**REQ-OAMP\_SM-FUN-004** The HeNB shall be able to authenticate the HeMS prior to responding to interactionstriggered by the HeMS.

**REQ-OAMP\_SM-FUN-005** The HeNB shall provide a capability supporting confidentiality for interactionstaking place between the HeNB and the HeMS.

## 6.2 Actor roles

Not defined in this version.

## 6.3 Telecommunications resources

Not defined in this version.

## 6.4 Use cases

### 6.4.1 Energy saving activation on selected network elements (Centralized ES)

| Use Case Stage | Evolution / Specification | <<Uses>>  Related use |
| --- | --- | --- |
| Goal | Activating energy saving for a selected network elements in a part of the network |  |
| Actors and Roles | HeMS as the user |  |
| Telecom resources | Network elements (NEs) and their OSS. |  |
| Assumptions | Centralized ES is performed.  The network operator has decided to activate energy saving on selected network elements in a part of the network (network elements, e.g. base stations) based on time period and network load. This requires to activate energy saving on some network elements and to activate compensatingForEnergySaving on others.  HeMS is monitoring the load on the NE. |  |
| Pre conditions | The network topology should allow transferring some network elements into energySavingState while maintaining coverage by transferring some other into ES-Compensate state.  Network elements (e.g. base stations) are not in a faulty state. |  |
| Begins when | The HeMS decides to activate energy saving on selected network elements in a part of the network based on monitored decreased network load and time period. |  |
| Step 1 (M) | The HeMS makes a decision on which NEs should enter energySaving state, compensatingForEnergySaving state, or notEnergySaving state based on network load, geographic positions and time of day. |  |
| Step 2 (M) | Based on the output of step1, the HeMS initiates energy saving activation and energy saving compensation activation on the NEs selected for the respective state transition. |  |
| Step 3 (M) | After the completion of the energy saving activation process, theNE informs the HeMS on the result of the process. |  |
| Ends when | The selected network elements are in energySaving state, and other selected network elements are in compensatingForEnergySaving state. |  |
| Exceptions | FFS |  |
| Post Conditions | Energy saving activation has been performed on some selected NEs. Other selected NEs are in compensatingForEnergySaving state. The network coverage is maintained. The network capacity is adapted to the reduced load. |  |
| Traceability | REQ-OAMP\_CM-FUN –023, REQ-OAMP,\_CM-FUN –025, REQ-OAMP\_CM-FUN –027 |  |

### 6.4.2 Deactivation of energy saving on selected network elements (Centralized ES )

| Use Case Stage | Evolution / Specification | <<Uses>>  Related use |
| --- | --- | --- |
| Goal | Deactivating energy saving for a selected part of the network |  |
| Actors and Roles | HeMS as user |  |
| Telecom resources | Network elements (NEs) and their OSS. |  |
| Assumptions | Centralized ES is performed.  The network operator has decided to deactivate energy saving on selected network elements in a part of the network (network elements, e.g. base stations) based on time period and network load.  HeMS is monitoring the load on the NE. |  |
| Pre conditions | The affected network elements are in energySavingstate or in ES-Compensate state.  Network elements (base stations) are not in a faulty state. |  |
| Begins when | The HeMS decides to deactivate energySaving for selected network elements in a part of the network based on network load. |  |
| Step 1 (M) | The HeMS makes a decision on which NEs should remain in energySaving state or compensatingforEnergySaving state, or enter notEnergySaving state based on network load, geographic positions and maximum coverage of base stations. |  |
| Step 2 (M) | Based on the output of step1, the HeMS initiates energy saving deactivation and energy saving compensation deactivation on the NEs selected for the respective state transition. |  |
| Step 3 (M) | After the completion of the energy saving deactivation process, the NE informs the HeMS on the result of the process. |  |
| Ends when | The selected network elements come out of energy saving state. |  |
| Exceptions | FFS. |  |
| Post Conditions | Energy saving deactivation has been performed on the selected NEs. The selected NEs are in notEnergySaving state. The network coverage is maintained. The network capacity accommodates the increased load. |  |
| Traceability | REQ-OAMP\_CM-FUN –024, REQ-OAMP\_CM-FUN –025, REQ-OAMP\_CM-FUN –027 |  |

### 6.4.3 Energy saving activation on selected network elements (Distributed ES)

| Use Case Stage | Evolution / Specification | <<Uses>>  Related use |
| --- | --- | --- |
| Goal | Activating energy saving for a selected network elements in a part of the network |  |
| Actors and Roles | HeMS as user |  |
| Telecom resources | Network elements (NEs) and their OSS. |  |
| Assumptions | The network operator has enabled the distributed energy saving function on selected network elements in a part of the network (network elements, e.g. base stations). This allows to activate energy saving on some network elements and to activate energy saving compensation on others.  HeMS configures the policy for load threshold. |  |
| Pre conditions | The network topology should allow transferring some network elements into energySavingstate while maintaining coverage by transferring some others into ES-Compensate state.  Network elements (e.g. base stations) are not in a faulty state. |  |
| Begins when | The distributed algorithm decides to activate energy saving on selected network elements in a part of the network based on monitored decreased network load and time period provisioned policy. |  |
| Step 1 (M) | The NE executes the energy saving algorithm to determine which neighboring NEs should enter energySaving, compensatingForEnergySaving, or notEnergySaving state. |  |
| Step 2 (M) | Based on the output of step 1, those NEs that have been selected to be transferred to compensatingForEnergySaving state, initiate energy saving compensation and inform the HeMS. |  |
| Step 3 (M) | Based on the output of step 1, those NEs that have been selected to be transferred to energySaving state, perform energy saving activation and inform the HeMS. |  |
| Ends when | The selected base stations are in energySaving state, and other selected base stations are in compensatingForEnergySaving state. |  |
| Exceptions | FFS. |  |
| Post Conditions | Energy saving activation has been performed on some selected NEs. Other selected NEs are in compensatingForEnergySaving state. The network coverage is maintained. The network capacity is adapted to the reduced load. |  |
| Traceability | REQ-OAMP\_CM-FUN–25, REQ-OAMP\_CM-FUN –026, REQ-OAMP,\_CM-FUN –028, REQ-OAMP\_CM- REQ-OAMP\_CM-FUN –030 |  |

### 6.4.4 Energy saving deactivation on selected network elements (Distributed ES)

| Use Case Stage | Evolution / Specification | <<Uses>>  Related use |
| --- | --- | --- |
| Goal | Deactivating energy saving for a selected part of the network |  |
| Actors and Roles | HeMS as user |  |
| Telecom resources | Network elements (NEs) and their OSS. |  |
| Assumptions | The network operator has enabled the energy saving distributed function on selected network elements in a part of the network, so that the NEs can deactivate energy saving state depending on load conditions. |  |
| Pre conditions | The affected network elements are in energySaving state or in compensatingForEnergySaving state.    Network elements (e.g. base stations) are not in a faulty state. |  |
| Begins when | The distributed algorithm decides to deactivate energy saving for a selected part of the network based on energy saving policy. |  |
| Step 1 (M) | The NE executes the energy saving algorithm that decides which NEs remain in energySaving state or compensatingforEnergySaving state or enter notEnergySaving state. |  |
| Step 2 (M) | Based on the output of step 1, those NEs that in energySaving state or compensatingforEnergySaving state which have been selected to be transferred to notEnergySaving state, initiate energy saving deactivation or energy saving compensation deactivation and inform the HeMS. |  |
| Ends when | The selected network elements are in nonEnergySaving state. |  |
| Exceptions | FFS. |  |
| Post Conditions | Energy saving deactivation has been performed on the selected NEs. The selected NEs are in notEnergySaving state. The network coverage is maintained. The network capacity accommodates the increased load. |  |
| Traceability | REQ-OAMP\_CM-FUN–25, REQ-OAMP\_CM-FUN –026, REQ-OAMP,\_CM-FUN –029, REQ-OAMP\_CM- REQ-OAMP\_CM-FUN –030 |  |

Annex A (informative):  
Energy Saving use cases for HeNB

# A.1 UC1a: Capacity-Limited Networks

Capacity-limited networks are normally dimensioned to cope with peak time traffic demand and can hence be under-utilized in off-peak times peak time traffic demand e.g. at certain hours of the night, when the overall load as well as the load distribution onto the different cells may differ significantly from peak times.

For energy saving management in such networks, the objective is therefore to adapt the network to these changing conditions by activating energy saving on selected cells. One approach is to concentrate the load into a few selected cells that remain active during low traffic demand periods with increased coverage area and to deactivate the remaining less loaded cells.

HeNBs are ideal candidates for policy based energy saving. For this use case let us consider an office building where there are several HeNBs deployed.



Figure A.1-1

Offices are generally closed between 9:00 PM to 6:00 AM. A policy based energy saving can be used to shut down cells that would not have any traffic during these times. Depending on the need one of cells can provide minimum coverage for the building.



Figure A.1-2: Different network arrangements corresponding to capacity demand variation for energy saving purposes

# A.2 UC 1b: Hybrid E-UTRAN Macro Cell and HeNB Cell Coverage

Alternately, if the building is completely closed for holidays or weekends all cells in the building can be shut down. The overlay macro cell can provide coverage for all the HeNBs in that area.




Figure A.2-1



Figure A.2-2: Hybrid E-UTRAN Macro Cell and HeNB Cell Coverage

In this scenario, two E-UTRAN Cells with different cell types cover the same geographical area. Cell B (HeNB Cell) is covered totally by Cell A (Macro Cell). Generally, Cell A is deployed by eNB to provide continuous coverage of the area, while Cell B is deployed by Home eNB to increase the capacity of the special sub-areas, such as home or business mall or office. The energy saving procedure in the coverage of Cell B (ES area) may be triggered in case that light traffic or no traffic in Cell B is detected. Cell B deactivation of energy saving may also be triggered when the traffic of ES area resumes to a high level. Home eNB which deploys the HeNB cell can be totally switched off during the ES procedure.

Activating energy saving on certain NEs and modifying radio parameters for increasing coverage for other cells can lead to different neighbor relations as well as different cell and frequency layouts, which should be addressed by automatic neighbor relation, interference control, e.g. through OAM-driven configuration or SON function. Depending on the specific scenarios, activating energy saving on NEs could ultimately lead to switching off all radio-transmission-related functions at a site, which would lead to reduced energy consumption and could implicitly lead to even further energy saving, e.g. when air condition systems at a site adapt to the reduced cooling requirements – which is not considered here in detail.

Depending on the architecture, energy saving decisions and corresponding state transfers are made by network elements (or element / domain managers) or by network management systems.

Annex B (informative):  
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **TSG #** | **TSG Doc.** | **CR** | **Rev** | **Subject/Comment** | **Old** | **New** |
| Jun 2009 | SA#44 | SP-090304 | -- | -- | Presentation to SA for information | -- | 1.0.0 |
| Mar 2010 | SA#47 | SP-100057 | -- | -- | Presentation to SA for approval | 1.0.0 | 2.0.0 |
| Mar 2010 | -- | -- | -- | -- | Publication of SA approved version | 2.0.0 | 9.0.0 |
| Jun 2010 | SA#48 | SP-100264 | 001 | -- | Missing Requirement for an operator’s defined time period at the HeNB | 9.0.0 | 10.0.0 |
| Mar 2011 | SA#51 | SP-110099 | 002 | 1 | Add LIPA management requirements | 10.0.0 | 10.1.0 |
| May 2011 | SA#52 | SP-110288 | 004 | 2 | Correction of requirements for HeNB non-IPsec usage - alignment with 33.320 | 10.1.0 | 10.2.0 |
| 2012-09 | - | - | - | - | Update to Rel-11 version (MCC) | 10.2.0 | **11.0.0** |
| 2014-10 | - | - | - | - | Update to Rel-12 version (MCC) | 11.0.0 | **12.0.0** |
| 2014-12 | SA#66 | SP-140799 | 006 | 1 | Use case description for energy saving management for HeNBs | 12.0.0 | **13.0.0** |
| 007 | 1 | Use case for energy saving management for HeNBs |
| 008 | 1 | Requirements for energy saving management for HeNBs |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **Tdoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2016-12 |  |  |  |  |  | Correction of LTE logo (MCC) | 13.0.1 |
| 2017-04 | SA#75 | - | - | - |  | Promotion to Release 14 without technical change | **14.0.0** |
| 2018-06 | - | - | - | - | - | Update to Rel-15 version (MCC) | **15.0.0** |
| 2020-07 | - | - | - | - | - | Update to Rel-16 version (MCC) | **16.0.0** |