3GPP TS 34.121-1 V16.2.0 (2019-09)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Radio Access Network;

User Equipment (UE) conformance specification;

Radio transmission and reception (FDD);

Part 1: Conformance specification

(Release 16)

** 

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.   
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.   
This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

Keywords

Testing, UMTS

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

[http://www.3gpp.org](http://www.3gpp.org/)

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2019, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TTA, TTC).

All rights reserved.

Change the copyright date above as necessary.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI currently being registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword 60

Introduction 60

1 Scope 61

2 References 61

3 Definitions, symbols, abbreviations and equations 63

3.1 Definitions 63

3.2 Symbols 64

3.3 Abbreviations 64

3.4 Equations 65

4 Frequency bands and channel arrangement 67

4.1 General 67

4.2 Frequency bands 68

4.3 TX-RX frequency separation 69

4.4 Channel arrangement 69

4.4.1 Channel spacing 69

4.4.2 Channel raster 70

4.4.3 Channel number 70

4.4.4 UARFCN 72

4A Reference Conditions 73

4A.1 Generic setup procedures 73

4A.2 System information 73

4A.3 Message contents 73

4A.4 Measurement configurations 74

5 Transmitter Characteristics 74

5.1 General 74

5.2 Maximum Output Power 75

5.2.1 Definition and applicability 75

5.2.2 Minimum Requirements 76

5.2.3 Test purpose 77

5.2.4 Method of test 77

5.2.4.1 Initial conditions 77

5.2.4.2 Procedure 78

5.2.5 Test requirements 78

5.2A Maximum Output Power with HS-DPCCH (Release 5 only) 79

5.2A.1 Definition and applicability 79

5.2A.2 Minimum Requirements 79

5.2A.3 Test purpose 79

5.2A.4 Method of test 79

5.2A.4.1 Initial conditions 79

5.2A.4.2 Procedure 80

5.2A.5 Test requirements 80

5.2AA Maximum Output Power with HS-DPCCH (Release 6 and later) 81

5.2AA.1 Definition and applicability 81

5.2AA.2 Minimum Requirements 81

5.2AA.3 Test purpose 81

5.2AA.4 Method of test 81

5.2AA.4.1 Initial conditions 81

5.2AA.4.2 Procedure 82

5.2AA.5 Test requirements 82

5.2AB Maximum Output Power for OLTD 83

5.2AB.1 Definition and applicability 83

5.2AB.2 Minimum Requirements 84

5.2AB.3 Test purpose 84

5.2AB.4 Method of test 84

5.2AB.4.1 Initial conditions 84

5.2AB.4.2 Procedure 85

5.2AB.5 Test requirements 85

5.2AC Maximum Output Power for UL CLTD activation state 1 87

5.2AC.1 Definition and applicability 87

5.2AC.2 Minimum Requirements 87

5.2AC.3 Test purpose 88

5.2AC.4 Method of test 88

5.2AC.4.1 Initial conditions 88

5.2AC.4.2 Procedure 88

5.2AC.5 Test requirements 89

5.2AD Maximum Output Power for UL CLTD activation state 2 and 3 90

5.2AD.1 Definition and applicability 90

5.2AD.2 Minimum Requirements 90

5.2AD.3 Test purpose 91

5.2AD.4 Method of test 91

5.2AD.4.1 Initial conditions 91

5.2AD.4.2 Procedure 92

5.2AD.5 Test requirements 92

5.2B Maximum Output Power with HS-DPCCH and E-DCH 93

5.2B.1 Definition and applicability 93

5.2B.2 Minimum Requirements 93

5.2B.3 Test purpose 94

5.2B.4 Method of test 94

5.2B.4.1 Initial conditions 94

5.2B.4.2 Procedure 96

5.2B.5 Test requirements 96

5.2BA UE Maximum Output Power for DC-HSUPA (QPSK) 98

5.2BA.1 Definition and applicability 98

5.2BA.2 Minimum Requirements 98

5.2BA.3 Test purpose 99

5.2BA.4 Method of test 99

5.2BA.4.1 Initial conditions 99

5.2BA.4.2 Procedure 100

5.2BA.5 Test requirements 100

5.2BB UE Maximum Output Power for DC-HSUPA (16QAM) 101

5.2BB.1 Definition and applicability 101

5.2BB.2 Minimum Requirements 102

5.2BB.3 Test purpose 103

5.2BB.4 Method of test 103

5.2BB.4.1 Initial conditions 103

5.2BB.4.2 Procedure 103

5.2BB.5 Test requirements 104

5.2BC Maximum Output Power with HS-DPCCH and E-DCH for OLTD 105

5.2BC.1 Definition and applicability 105

5.2BC.2 Minimum Requirements 105

5.2BC.3 Test purpose 105

5.2BC.4 Method of test 105

5.2BC.4.1 Initial conditions 105

5.2BC.4.2 Procedure 107

5.2BC.4.2.1 Procedure for sub-test 1 to 4 107

5.2BC.5 Test requirements 108

5.2BD Maximum Output Power with HS-DPCCH and E-DCH for UL CLTD activation state 1 109

5.2BD.1 Definition and applicability 109

5.2BD.2 Minimum Requirements 109

5.2BD.3 Test purpose 110

5.2BD.4 Method of test 110

5.2BD.4.1 Initial conditions 110

5.2BD.4.2 Procedure 112

5.2BD.4.2.1 Procedure for sub-test 1 to 4 112

5.2BD.5 Test requirements 112

5.2BE Maximum Output Power with HS-DPCCH and E-DCH for UL CLTD activation state 2 and 3. 114

5.2BE.1 Definition and applicability 114

5.2BE.2 Minimum Requirements 114

5.2BE.3 Test purpose 114

5.2BE.4 Method of test 115

5.2BE.4.1 Initial conditions 115

5.2BE.4.2 Procedure 117

5.2BE.4.2.1 Procedure for sub-test 1 to 4 117

5.2BE.5 Test requirements 117

5.2C UE relative code domain power accuracy 118

5.2C.1 Definition and applicability 118

5.2C.2 Minimum Requirements 119

5.2C.3 Test purpose 119

5.2C.4 Method of test 119

5.2C.4.1 Initial conditions 119

5.2C.4.2 Procedure 120

5.2C.5 Test requirements 120

5.2CA UE relative code domain power accuracy for OLTD 121

5.2CA.1 Definition and applicability 121

5.2CA.2 Minimum Requirements 122

5.2CA.3 Test purpose 122

5.2CA.4 Method of test 122

5.2CA.4.1 Initial conditions 122

5.2CA.4.2 Procedure 122

5.2CA.5 Test requirements 123

5.2CB UE relative code domain power accuracy for UL CLTD activation state 1 124

5.2CB.1 Definition and applicability 124

5.2CB.2 Minimum Requirements 125

5.2CB.3 Test purpose 125

5.2CB.4 Method of test 125

5.2CB.4.1 Initial conditions 125

5.2CB.4.2 Procedure 126

5.2CB.5 Test requirements 126

5.2CC UE relative code domain power accuracy for UL CLTD activation state 2 and 3 127

5.2CC.1 Definition and applicability 127

5.2CC.2 Minimum Requirements 128

5.2CC.3 Test purpose 128

5.2CC.4 Method of test 128

5.2CC.4.1 Initial conditions 128

5.2CC.4.2 Procedure 129

5.2CC.5 Test requirements 130

5.2D UE Relative Code Domain Power Accuracy for HS-DPCCH and E-DCH 130

5.2D.1 Definition and applicability 130

5.2D.2 Minimum Requirements 131

5.2D.3 Test purpose 131

5.2D.4 Method of test 131

5.2D.4.1 Initial conditions 131

5.2D.4.2 Procedure 133

5.2D.5 Test requirements 133

5.2DA UE Relative Code Domain Power Accuracy for DC-HSUPA with QPSK 134

5.2DA.1 Definition and applicability 134

5.2DA.2 Minimum Requirements 135

5.2DA.3 Test purpose 135

5.2DA.4 Method of test 135

5.2DA.4.1 Initial conditions 135

5.2DA.4.2 Procedure 136

5.2DA.5 Test requirements 136

5.2DB UE Relative Code Domain Power Accuracy for HS-DPCCH and E-DCH for OLTD 137

5.2DB.1 Definition and applicability 137

5.2DB.2 Minimum Requirements 137

5.2DB.3 Test purpose 137

5.2DB.4 Method of test 137

5.2DB.4.1 Initial conditions 137

5.2DB.4.2 Procedure 139

5.2DB.5 Test requirements 140

5.2DC UE Relative Code Domain Power Accuracy for HS-DPCCH and E-DCH for UL CLTD activation state 1 141

5.2DC.1 Definition and applicability 141

5.2DC.2 Minimum Requirements 141

5.2DC.3 Test purpose 141

5.2DC.4 Method of test 141

5.2DC.4.1 Initial conditions 141

5.2DC.4.2 Procedure 143

5.2DC.5 Test requirements 144

5.2DD UE Relative Code Domain Power Accuracy for HS-DPCCH and E-DCH for UL CLTD activation state 2 and 3 145

5.2DD.1 Definition and applicability 145

5.2DD.2 Minimum Requirements 145

5.2DD.3 Test purpose 145

5.2DD.4 Method of test 145

5.2DD.4.1 Initial conditions 145

5.2DD.4.2 Procedure 147

5.2DD.5 Test requirements 148

5.2E UE Relative Code Domain Power Accuracy for HS-DPCCH and E-DCH with 16QAM 149

5.2E.1 Definition and applicability 149

5.2E.2 Minimum Requirements 149

5.2E.3 Test purpose 149

5.2E.4 Method of test 150

5.2E.4.1 Initial conditions 150

5.2E.4.2 Procedure 151

5.2E.5 Test requirements 151

5.2EA UE Relative Code Domain Power Accuracy for DC-HSUPA with 16QAM 152

5.2EA.1 Definition and applicability 152

5.2EA.2 Minimum Requirements 153

5.2EA.3 Test purpose 153

5.2EA.4 Method of test 153

5.2EA.4.1 Initial conditions 153

5.2EA.4.2 Procedure 154

5.2EA.5 Test requirements 154

5.2EB UE Relative Code Domain Power Accuracy for HS-DPCCH and E-DCH with 16QAM for OLTD 154

5.2EB.1 Definition and applicability 154

5.2EB.2 Minimum Requirements 155

5.2EB.3 Test purpose 155

5.2EB.4 Method of test 156

5.2EB.4.1 Initial conditions 156

5.2EB.4.2 Procedure 157

5.2EB.5 Test requirements 158

5.2EC UE Relative Code Domain Power Accuracy for HS-DPCCH and E-DCH with 16QAM for UL CLTD activation state 1 158

5.2EC.1 Definition and applicability 158

5.2EC.2 Minimum Requirements 159

5.2EC.3 Test purpose 159

5.2EC.4 Method of test 159

5.2EC.4.1 Initial conditions 159

5.2EC.4.2 Procedure 160

5.2EC.5 Test requirements 161

5.2ED UE Relative Code Domain Power Accuracy for HS-DPCCH and E-DCH with 16QAM for UL CLTD activation state 2 and 3 162

5.2ED.1 Definition and applicability 162

5.2ED.2 Minimum Requirements 162

5.2ED.3 Test purpose 163

5.2ED.4 Method of test 163

5.2ED.4.1 Initial conditions 163

5.2ED.4.2 Procedure 164

5.2ED.5 Test requirements 165

5.3 Frequency Error 166

5.3.1 Definition and applicability 166

5.3.2 Minimum Requirements 166

5.3.3 Test purpose 166

5.3.4 Method of test 166

5.3.4.1 Initial conditions 166

5.3.4.2 Procedure 167

5.3.5 Test Requirements 167

5.3A Frequency Error for DC-HSUPA 167

5.3A.1 Definition and applicability 167

5.3A.2 Minimum Requirements 167

5.3A.3 Test purpose 167

5.3A.4 Method of test 167

5.3A.4.1 Initial conditions 167

5.3A.4.2 Procedure 168

5.3A.5 Test Requirements 168

5.3B Frequency Error for OLTD 168

5.3B.1 Definition and applicability 168

5.3B.2 Minimum Requirements 168

5.3B.3 Test purpose 168

5.3B.4 Method of test 169

5.3B.4.1 Initial conditions 169

5.3B.4.2 Procedure 169

5.3B.5 Test Requirements 170

5.3C Frequency Error for UL CLTD Activation state 1 170

5.3C.1 Definition and applicability 170

5.3C.2 Minimum Requirements 170

5.3C.3 Test purpose 170

5.3C.4 Method of test 170

5.3C.4.1 Initial conditions 170

5.3C.4.2 Procedure 171

5.3C.5 Test Requirements 171

5.3D Frequency Error for UL CLTD Activation state 2 and 3 171

5.3D.1 Definition and applicability 171

5.3D.2 Minimum Requirements 171

5.3D.3 Test purpose 171

5.3D.4 Method of test 172

5.3D.4.1 Initial conditions 172

5.3D.4.2 Procedure 172

5.3D.5 Test Requirements 173

5.4 Output Power Dynamics in the Uplink 173

5.4.1 Open Loop Power Control in the Uplink 173

5.4.1.1 Definition and applicability 173

5.4.1.2 Minimum requirements 173

5.4.1.3 Test purpose 173

5.4.1.4 Method of test 173

5.4.1.5 Test requirements 175

5.4.1A Open Loop Power Control in the Uplink for DC-HSUPA 175

5.4.1A.1 Definition and applicability 175

5.4.1A.2 Minimum requirements 175

5.4.1A.3 Test purpose 175

5.4.1A.4 Method of test 176

5.4.1A.5 Test requirements 177

5.4.2 Inner Loop Power Control in the Uplink 177

5.4.2.1 Definition and applicability 177

5.4.2.2 Minimum requirements 177

5.4.2.3 Test purpose 178

5.4.2.4 Method of test 179

5.4.2.5 Test requirements 182

5.4.2A Inner Loop Power Control in the Uplink for DC-HSUPA 184

5.4.2A.1 Definition and applicability 184

5.4.2A.2 Minimum requirements 184

5.4.2A.3 Test purpose 185

5.4.2A.4 Method of test 186

5.4.2A.5 Test requirements 188

5.4.2B Inner Loop Power Control in the Uplink for OLTD 190

5.4.2B.1 Definition and applicability 190

5.4.2B.2 Minimum requirements 190

5.4.2B.3 Test purpose 191

5.4.2B.4 Method of test 192

5.4.2B.4.1 Initial conditions 192

5.4.2B.4.2 Procedure 192

5.4.2B.5 Test requirements 195

5.4.2C Inner Loop Power Control in the Uplink for UL CLTD activation state 1 197

5.4.2C.1 Definition and applicability 197

5.4.2C.2 Minimum requirements 197

5.4.2C.3 Test purpose 199

5.4.2C.4 Method of test 199

5.4.2C.4.1 Initial conditions 199

5.4.2C.4.2 Procedure 200

5.4.2C.5 Test requirements 203

5.4.2D Inner Loop Power Control in the Uplink for UL CLTD activation state 2 and 3 205

5.4.2D.1 Definition and applicability 205

5.4.2D.2 Minimum requirements 205

5.4.2D.3 Test purpose 207

5.4.2D.4 Method of test 207

5.4.2D.4.1 Initial conditions 207

5.4.2D.4.2 Procedure 208

5.4.2D.5 Test requirements 211

5.4.3 Minimum Output Power 213

5.4.3.1 Definition and applicability 213

5.4.3.2 Minimum Requirements 213

5.4.3.3 Test purpose 213

5.4.3.4 Method of test 213

5.4.3.5 Test requirements 214

5.4.3A Minimum Output Power for DC-HSUPA 214

5.4.3A.1 Definition and applicability 214

5.4.3A.2 Minimum Requirements 214

5.4.3A.3 Test purpose 214

5.4.3A.4 Method of test 214

5.4.3A.4.1 Initial conditions 214

5.4.3A.4.2 Procedure 215

5.4.3A.5 Test requirements 215

5.4.3B Minimum Output Power for OLTD 215

5.4.3B.1 Definition and applicability 215

5.4.3B.2 Minimum Requirements 215

5.4.3B.3 Test purpose 215

5.4.3B.4 Method of test 216

5.4.3B.4.1 Initial conditions 216

5.4.3B.4.2 Procedure 216

5.4.3B.5 Test requirements 216

5.4.3C Minimum Output Power for UL CLTD Activation state 1 216

5.4.3C.1 Definition and applicability 216

5.4.3C.2 Minimum Requirements 216

5.4.3C.3 Test purpose 217

5.4.3C.4 Method of test 217

5.4.3C.4.1 Initial conditions 217

5.4.3C.4.2 Procedure 217

5.4.3C.5 Test requirements 217

5.4.3D Minimum Output Power for UL CLTD Activation state 2 and 3 217

5.4.3D.1 Definition and applicability 217

5.4.3D.2 Minimum Requirements 218

5.4.3D.3 Test purpose 218

5.4.3D.4 Method of test 218

5.4.3D.4.1 Initial conditions 218

5.4.3D.4.2 Procedure 218

5.4.3D.5 Test requirements 219

5.4.4 Out-of-synchronisation handling of output power 219

5.4.4.1 Definition and applicability 219

5.4.4.2 Minimum Requirements 219

5.4.4.3 Test purpose 221

5.4.4.4 Method of test 221

5.4.4.5 Test requirements 222

5.4.4A Out-of-synchronization handling of output power for a UE which supports type1 for DCH 222

5.4.4A.1 Definition and applicability 222

5.4.4A.2 Minimum requirement 222

5.4.4A.3 Test purpose 224

5.4.4A.4 Method of test 224

5.4.4A.5 Test requirements 225

5.4.4B Out-of-synchronisation handling of output power for OLTD 225

5.4.4B.1 Definition and applicability 226

5.4.4B.2 Minimum Requirements 226

5.4.4B.3 Test purpose 227

5.4.4B.4 Method of test 228

5.4.4B.4.1 Initial conditions 228

5.4.4B.4.2 Procedure 228

5.4.4B.5 Test requirements 228

5.4.4C Out-of-synchronisation handling of output power for UL CLTD activation state 1 228

5.4.4C.1 Definition and applicability 229

5.4.4C.2 Minimum Requirements 229

5.4.4C.3 Test purpose 231

5.4.4C.4 Method of test 231

5.4.4C.5 Test requirements 232

5.4.4D Out-of-synchronisation handling of output power for UL CLTD activation state 2 and 3 232

5.4.4D.1 Definition and applicability 232

5.4.4D.2 Minimum Requirements 232

5.4.4D.3 Test purpose 234

5.4.4D.4 Method of test 234

5.4.4D.5 Test requirements 235

5.4.5 Out of quality handling of TPI for UL CLTD activation state 1 235

5.4.5.1 Definition and applicability 235

5.4.5.2 Minimum Requirements 236

5.4.5.3 Test purpose 237

5.4.5.4 Method of test 237

5.4.5.5 Test requirements 238

5.5 Transmit ON/OFF Power 238

5.5.1 Transmit OFF Power 238

5.5.1.1 Definition and applicability 238

5.5.1.2 Minimum Requirements 238

5.5.1.3 Test purpose 238

5.5.1.4 Method of test 238

5.5.1.5 Test requirements 238

5.5.2 Transmit ON/OFF Time mask 239

5.5.2.1 Definition and applicability 239

5.5.2.2 Minimum requirements 239

5.5.2.3 Test purpose 241

5.5.2.4 Method of test 241

5.5.2.5 Test requirements 243

5.6 Change of TFC 244

5.6.1 Definition and applicability 244

5.6.2 Minimum requirements 244

5.6.3 Test purpose 246

5.6.4 Method of test 246

5.6.5 Test requirements 246

5.6AA Change of TFC for OLTD 247

5.6AA.1 Definition and applicability 247

5.6AA.2 Minimum requirements 247

5.6AA.3 Test purpose 249

5.6AA.4 Method of test 249

5.6AA.4.1 Initial conditions 249

5.6AA.4.2 Procedure 249

5.6AA.5 Test requirements 249

5.6AB Void 249

5.6AC Void 249

5.7 Power setting in uplink compressed mode 249

5.7.1 Definition and applicability 249

5.7.2 Minimum requirements 250

5.7.3 Test purpose 252

5.7.4 Method of test 252

5.7.5 Test requirements 259

5.7A HS-DPCCH power control 261

5.7A.1 Definition and applicability 261

5.7A.2 Minimum requirement 261

5.7A.3 Test purpose 263

5.7A.4 Method of test 263

5.7A.5 Test requirements 264

5.7BA HS-DPCCH power control for UL OLTD 265

5.7BA.1 Definition and applicability 266

5.7BA.2 Minimum requirement 266

5.7BA.3 Test purpose 266

5.7BA.4 Method of test 267

5.7BA.4.1 Initial conditions 267

5.7BA.4.2 Procedure 267

5.7BA.5 Test requirements 268

5.7BB HS-DPCCH power control for UL CLTD activation state 1 269

5.7BB.1 Definition and applicability 270

5.7BB.2 Minimum requirement 270

5.7BB.3 Test purpose 270

5.7BB.4 Method of test 271

5.7BB.4.1 Initial conditions 271

5.7BB.4.2 Procedure 271

5.7BB.5 Test requirements 272

5.7BC HS-DPCCH power control for UL CLTD activation state 2 and 3 274

5.7BC.1 Definition and applicability 274

5.7BC.2 Minimum requirement 274

5.7BC.3 Test purpose 275

5.7BC.4 Method of test 275

5.7BC.4.1 Initial conditions 275

5.7BC.4.2 Procedure 275

5.7BC.5 Test requirements 276

5.8 Occupied Bandwidth (OBW) 278

5.8.1 Definition and applicability 278

5.8.2 Minimum Requirements 278

5.8.3 Test purpose 278

5.8.4 Method of test 279

5.8.5 Test Requirements 279

5.8A Occupied Bandwidth (OBW) for DC-HSUPA 279

5.8A.1 Definition and applicability 279

5.8A.2 Minimum Requirements 279

5.8A.3 Test purpose 279

5.8A.4 Method of test 280

5.8A.4.1 Initial conditions 280

5.8A.4.2 Procedure 280

5.8A.5 Test Requirements 281

5.8B Occupied Bandwidth (OBW) for OLTD 281

5.8B.1 Definition and applicability 281

5.8B.2 Minimum Requirements 281

5.8B.3 Test purpose 281

5.8B.4 Method of test 281

5.8B.4.1 Initial conditions 281

5.8B.4.2 Procedure 281

5.8B.5 Test Requirements 282

5.8C Occupied Bandwidth (OBW) for UL CLTD Activation state 1 282

5.8C.1 Definition and applicability 282

5.8C.2 Minimum Requirements 282

5.8C.3 Test purpose 282

5.8C.4 Method of test 282

5.8C.4.1 Initial conditions 282

5.8C.4.2 Procedure 283

5.8C.5 Test Requirements 283

5.9 Spectrum emission mask 283

5.9.1 Definition and applicability 283

5.9.2 Minimum Requirements 283

5.9.3 Test purpose 285

5.9.4 Method of test 285

5.9.4.1 Initial conditions 285

5.9.4.2 Procedure 285

5.9.5 Test requirements 285

5.9A Spectrum Emission Mask with HS-DPCCH 287

5.9A.1 Definition and applicability 287

5.9A.2 Minimum Requirements 287

5.9A.3 Test purpose 288

5.9A.4 Method of test 288

5.9A.4.1 Initial conditions 288

5.9A.4.2 Procedure 289

5.9A.5 Test requirements 289

5.9AA Spectrum Emission Mask with HS-DPCCH for UL OLTD 291

5.9AA.1 Definition and applicability 291

5.9AA.2 Minimum Requirements 291

5.9AA.3 Test purpose 292

5.9AA.4 Method of test 292

5.9AA.4.1 Initial conditions 292

5.9AA.4.2 Procedure 293

5.9AA.5 Test requirements 293

5.9AB Spectrum Emission Mask with HS-DPCCH for UL CLTD activation state 1 295

5.9AB.1 Definition and applicability 295

5.9AB.2 Minimum Requirements 295

5.9AB.3 Test purpose 296

5.9AB.4 Method of test 296

5.9AB.4.1 Initial conditions 296

5.9AB.4.2 Procedure 297

5.9AB.5 Test requirements 297

5.9AC Spectrum Emission Mask with HS-DPCCH for UL CLTD activation state 2 and 3 299

5.9AC.1 Definition and applicability 299

5.9AC.2 Minimum Requirements 299

5.9AC.3 Test purpose 300

5.9AC.4 Method of test 300

5.9AC.4.1 Initial conditions 300

5.9AC.4.2 Procedure 301

5.9AC.5 Test requirements 301

5.9B Spectrum Emission Mask with E-DCH 302

5.9B.1 Definition and applicability 302

5.9B.2 Minimum Requirements 303

5.9B.3 Test purpose 304

5.9B.4 Method of test 304

5.9B.4.1 Initial conditions 304

5.9B.4.2 Procedure 305

5.9B.5 Test requirements 305

5.9BA Spectrum Emission Mask with E-DCH for UL OLTD 307

5.9BA.1 Definition and applicability 307

5.9BA.2 Minimum Requirements 307

5.9BA.3 Test purpose 308

5.9BA.4 Method of test 308

5.9BA.4.1 Initial conditions 308

5.9BA.4.2 Procedure 309

5.9BA.5 Test requirements 309

5.9BB Spectrum Emission Mask with E-DCH for UL CLTD activation state 1 311

5.9BB.1 Definition and applicability 311

5.9BB.2 Minimum Requirements 311

5.9BB.3 Test purpose 312

5.9BB.4 Method of test 312

5.9BB.4.1 Initial conditions 312

5.9BB.4.2 Procedure 313

5.9BB.5 Test requirements 313

5.9BC Spectrum Emission Mask with E-DCH for UL CLTD activation state 2 and 3 315

5.9BC.1 Definition and applicability 315

5.9BC.2 Minimum Requirements 315

5.9BC.3 Test purpose 316

5.9BC.4 Method of test 316

5.9BC.4.1 Initial conditions 316

5.9BC.4.2 Procedure 317

5.9BC.5 Test requirements 317

5.9C Additional Spectrum Emission Mask for DC-HSUPA (QPSK) 319

5.9C.1 Definition and applicability 319

5.9C.2 Minimum Requirements 319

5.9C.3 Test purpose 319

5.9C.4 Method of test 320

5.9C.4.1 Initial conditions 320

5.9C.4.2 Procedure 320

5.9C.5 Test requirements 320

5.9D Additional Spectrum Emission Mask for DC-HSUPA (16QAM) 321

5.9D.1 Definition and applicability 321

5.9D.2 Minimum Requirements 321

5.9D.3 Test purpose 322

5.9D.4 Method of test 322

5.9D.4.1 Initial conditions 322

5.9D.4.2 Procedure 323

5.9D.5 Test requirements 323

5.10 Adjacent Channel Leakage Power Ratio (ACLR) 323

5.10.1 Definition and applicability 323

5.10.2 Minimum Requirements 324

5.10.3 Test purpose 324

5.10.4 Method of test 324

5.10.5 Test requirements 325

5.10A Adjacent Channel Leakage Power Ratio (ACLR) with HS-DPCCH 325

5.10A.1 Definition and applicability 325

5.10A.2 Minimum Requirements 325

5.10A.3 Test purpose 325

5.10A.4 Method of test 326

5.10A.5 Test requirements 327

5.10AA Adjacent Channel Leakage Power Ratio (ACLR) with HS-DPCCH for OLTD 327

5.10AA.1 Definition and applicability 327

5.10AA.2 Minimum Requirements 327

5.10AA.3 Test purpose 327

5.10AA.4 Method of test 328

5.10AA.5 Test requirements 329

5.10AB Adjacent Channel Leakage Power Ratio (ACLR) with HS-DPCCH for UL CLTD Activation state 1 329

5.10AB.1 Definition and applicability 329

5.10AB.2 Minimum Requirements 329

5.10AB.3 Test purpose 329

5.10AB.4 Method of test 330

5.10AB.4.1 Initial conditions 330

5.10AB.4.2 Procedure 330

5.10AB.5 Test requirements 330

5.10AC Adjacent Channel Leakage Power Ratio (ACLR) with HS-DPCCH for UL CLTD Activation state 2 and 3 331

5.10AC.1 Definition and applicability 331

5.10AC.2 Minimum Requirements 331

5.10AC.3 Test purpose 331

5.10AC.4 Method of test 331

5.10AC.4.1 Initial conditions 331

5.10AC.4.2 Procedure 332

5.10AC.5 Test requirements 333

5.10B Adjacent Channel Leakage Power Ratio (ACLR) with E-DCH 333

5.10B.1 Definition and applicability 333

5.10B.2 Minimum Requirements 333

5.10B.3 Test purpose 333

5.10B.4 Method of test 334

5.10B.5 Test requirements 335

5.10BA Adjacent Channel Leakage Power Ratio (ACLR) with E-DCH for OLTD 335

5.10BA.1 Definition and applicability 335

5.10BA.2 Minimum Requirements 335

5.10BA.3 Test purpose 335

5.10BA.4 Method of test 336

5.10BA.5 Test requirements 336

5.10BB Adjacent Channel Leakage Power Ratio (ACLR) with E-DCH for UL CLTD Activation state 1 337

5.10BB.1 Definition and applicability 337

5.10BB.2 Minimum Requirements 337

5.10BB.3 Test purpose 337

5.10BB.4 Method of test 337

5.10BB.5 Test requirements 338

5.10BC Adjacent Channel Leakage Power Ratio (ACLR) with E-DCH for UL CLTD Activation state 2 and 3 338

5.10BC.1 Definition and applicability 338

5.10BC.2 Minimum Requirements 339

5.10BC.3 Test purpose 339

5.10BC.4 Method of test 339

5.10BC.5 Test requirements 340

5.10C Adjacent Channel Leakage Power Ratio (ACLR) with E-DCH for DC-HSUPA (QPSK) 341

5.10C.1 Definition and applicability 341

5.10C.2 Minimum Requirements 341

5.10C.3 Test purpose 341

5.10C.4 Method of test 341

5.10C.5 Test requirements 342

5.10D Adjacent Channel Leakage Power Ratio (ACLR) with E-DCH for DC-HSUPA (16QAM) 342

5.10D.1 Definition and applicability 342

5.10D.2 Minimum Requirements 343

5.10D.3 Test purpose 343

5.10D.4 Method of test 343

5.10D.5 Test requirements 344

5.11 Spurious Emissions 344

5.11.1 Definition and applicability 344

5.11.2 Minimum Requirements 344

5.11.3 Test purpose 352

5.11.4 Method of test 353

5.11.5 Test requirements 353

5.11A Spurious Emissions for DC-HSUPA 360

5.11A.1 Definition and applicability 360

5.11A.2 Minimum Requirements 361

5.11A.3 Test purpose 365

5.11A.4 Method of test 365

5.11A.5 Test requirements 366

5.11B Spurious Emissions for UL OLTD 371

5.11B.1 Definition and applicability 371

5.11B.2 Minimum Requirements 372

5.11B.3 Test purpose 372

5.11B.4 Method of test 372

5.11B.5 Test requirements 372

5.11C Spurious Emissions for UL CLTD Activation state 1 379

5.11C.1 Definition and applicability 380

5.11C.2 Minimum Requirements 380

5.11C.3 Test purpose 380

5.11C.4 Method of test 380

5.11C.5 Test requirements 380

5.11D Spurious Emissions for UL CLTD Activation state 2 and 3 388

5.11D.1 Definition and applicability 389

5.11D.2 Minimum Requirements 389

5.11D.3 Test purpose 389

5.11D.4 Method of test 389

5.11D.5 Test requirements 390

5.12 Transmit Intermodulation 397

5.12.1 Definition and applicability 397

5.12.2 Minimum Requirements 398

5.12.3 Test purpose 398

5.12.4 Method of test 398

5.12.5 Test requirements 398

5.12A Transmit Intermodulation for DC-HSUPA 399

5.12A.1 Definition and applicability 399

5.12A.2 Minimum Requirements for DC-HSUPA 399

5.12A.3 Test purpose 399

5.12A.4 Method of test 399

5.12A.5 Test requirements 400

5.13 Transmit Modulation 400

5.13.1 Error Vector Magnitude (EVM) 400

5.13.1.1 Definition and applicability 400

5.13.1.2 Minimum Requirements 400

5.13.1.3 Test purpose 401

5.13.1.4 Method of test 401

5.13.1.5 Test requirements 401

5.13.1A Error Vector Magnitude (EVM) with HS-DPCCH 401

5.13.1A.1 Definition and applicability 401

5.13.1A.2 Minimum Requirements 402

5.13.1A.3 Test purpose 402

5.13.1A.4 Method of test 402

5.13.1A.5 Test requirements 404

5.13.1AA Error Vector Magnitude (EVM) and phase discontinuity with HS-DPCCH 404

5.13.1AA.1 Definition and applicability 404

5.13.1AA.2 Minimum Requirements 404

5.13.1AA.3 Test purpose 405

5.13.1AA.4 Method of test 405

5.13.1AA.5 Test requirements 407

5.13.1AB Error Vector Magnitude (EVM) and phase discontinuity with HS-DPCCH for OLTD 407

5.13.1AB.1 Definition and applicability 407

5.13.1AB.2 Minimum Requirements 408

5.13.1AB.3 Test purpose 408

5.13.1AB.4 Method of test 409

5.13.1AB.5 Test requirements 410

5.13.1AB Error Vector Magnitude (EVM) and phase discontinuity with HS-DPCCH for OLTD 410

5.13.1AC Error Vector Magnitude (EVM) and phase discontinuity with HS-DPCCH for UL CLTD Activation state 1 410

5.13.1AC.1 Definition and applicability 410

5.13.1AC.2 Minimum Requirements 411

5.13.1AC.3 Test purpose 412

5.13.1AC.4 Method of test 412

5.13.1AC.5 Test requirements 413

5.13.1AD Error Vector Magnitude (EVM) and phase discontinuity with HS-DPCCH for UL CLTD Activation state 2 and 3 414

5.13.1AD.1 Definition and applicability 414

5.13.1AD.2 Minimum Requirements 414

5.13.1AD.3 Test purpose 415

5.13.1AD.4 Method of test 415

5.13.1AD.5 Test requirements 417

5.13.1AAA EVM and IQ origin offset for HS-DPCCH and E-DCH with 16 QAM 417

5.13.1AAA.1 Definition and applicability 417

5.13.1AAA.2 Minimum requirement 417

5.13.1AAA.3 Test purpose 418

5.13.1AAA.4 Method of test 418

5.13.1AAA.5 Test requirements 419

5.13.2 Peak code domain error 420

5.13.2.1 Definition and applicability 420

5.13.2.2 Minimum Requirements 420

5.13.2.3 Test purpose 420

5.13.2.4 Method of test 420

5.13.2.5 Test requirements 421

5.13.2A Relative Code Domain Error with HS-DPCCH 421

5.13.2A.1 Definition and applicability 421

5.13.2A.2 Minimum Requirements 421

5.13.2A.3 Test purpose 422

5.13.2A.4 Method of test 422

5.13.2B Relative Code Domain Error with HS-DPCCH and E-DCH 424

5.13.2B.1 Definition and applicability 424

5.13.2B.2 Minimum Requirements 424

5.13.2B.3 Test purpose 425

5.13.2B.4 Method of test 425

5.13.2B.5 Test requirements 427

5.13.2BA Relative Code Domain Error with HS-DPCCH and E-DCH for DC-HSUPA 428

5.13.2BA.1 Definition and applicability 428

5.13.2BA.2 Minimum Requirements 428

5.13.2BA.3 Test purpose 429

5.13.2BA.4 Method of test 429

5.13.2BA.5 Test requirements 430

5.13.2C Relative Code Domain Error for HS-DPCCH and E-DCH with 16QAM 430

5.13.2C.1 Definition and applicability 430

5.13.2C.2 Minimum Requirements 431

5.13.2C.3 Test purpose 432

5.13.2C.4 Method of test 432

5.13.2CA Relative Code Domain Error for HS-DPCCH and E-DCH with 16QAM for DC-HSUPA 434

5.13.2CA.1 Definition and applicability 434

5.13.2CA.2 Minimum Requirements 435

5.13.2CA.3 Test purpose 436

5.13.2CA.4 Method of test 436

5.13.2CA.5 Test requirements 437

5.13.3 UE phase discontinuity 438

5.13.3.1 Definition and applicability 438

5.13.3.2 Minimum requirements 438

5.13.3.3 Test purpose 439

5.13.3.4 Method of test 439

5.13.3.5 Test requirements 440

5.13.4 PRACH preamble quality 441

5.13.4.1 Definition and applicability 441

5.13.4.2 Minimum requirements 441

5.13.4.3 Test purpose 441

5.13.4.4 Method of test 441

5.13.4.5 Test requirements 442

5.13.5 In-band emission for DC-HSUPA 443

5.13.5.1 Definition and applicability 443

5.13.5.2 Minimum Requirements 443

5.13.5.3 Test purpose 443

5.13.5.4 Method of test 443

5.13.5.5 Test requirements 444

6 Receiver Characteristics 445

6.1 General 445

6.1A Reference input power adjustment for a dual band device 446

6.2 Reference Sensitivity Level 447

6.2.1 Definition and applicability 447

6.2.2 Minimum Requirements 447

6.2.3 Test purpose 448

6.2.4 Method of test 448

6.2.5 Test requirements 449

6.2A Reference Sensitivity Level for DC-HSDPA 449

6.2A.1 Definition and applicability 449

6.2A.2 Minimum Requirements 450

6.2A.3 Test purpose 451

6.2A.4 Method of test 451

6.2A.5 Test requirements 452

6.2B Reference Sensitivity Level for DB-DC-HSDPA 453

6.2B.1 Definition and applicability 453

6.2B.2 Minimum Requirements 453

6.2B.3 Test purpose 454

6.2B.4 Method of test 454

6.2B.5 Test requirements 455

6.2C Reference Sensitivity Level for Single band 4C-HSDPA 455

6.2C.1 Definition and applicability 455

6.2C.2 Minimum Requirements 456

6.2C.3 Test purpose 457

6.2C.4 Method of test 457

6.2C.4.2 Procedure 457

6.2C.5 Test requirements 457

6.2D Reference Sensitivity Level for Dual band 4C-HSDPA 458

6.2D.1 Definition and applicability 458

6.2D.2 Minimum Requirements 458

6.2D.3 Test purpose 459

6.2D.4 Method of test 459

6.2D.5 Test requirements 460

6.2DA Reference Sensitivity Level for Dual band 4C-HSDPA (3 carrier) 460

6.2DA.1 Definition and applicability 460

6.2DA.2 Minimum Requirements 460

6.2DA.3 Test purpose 461

6.2DA.4 Method of test 461

6.2DA.5 Test requirements 462

6.3 Maximum Input Level 462

6.3.1 Definition and applicability 462

6.3.2 Minimum requirements 462

6.3.3 Test purpose 462

6.3.4 Method of test 463

6.3.5 Test requirements 463

6.3A Maximum Input Level for HS-PDSCH Reception (16QAM) 464

6.3A.1 Definition and applicability 464

6.3A.2 Minimum requirements 464

6.3A.3 Test purpose 464

6.3A.4 Method of test 464

6.3A.5 Test requirements 465

6.3B Maximum Input Level for HS-PDSCH Reception (64QAM) 465

6.3B.1 Definition and applicability 465

6.3B.2 Minimum requirements 465

6.3B.3 Test purpose 466

6.3B.4 Method of test 466

6.3B.5 Test requirements 468

6.3C Maximum Input Level for DC-HSDPA Reception (16QAM) 468

6.3C.1 Definition and applicability 468

6.3C.2 Minimum requirements 468

6.3C.3 Test purpose 469

6.3C.4 Method of test 469

6.3C.5 Test requirements 470

6.3D Maximum Input Level for DC-HSDPA Reception (64QAM) 470

6.3D.1 Definition and applicability 470

6.3D.2 Minimum requirements 470

6.3D.3 Test purpose 471

6.3D.4 Method of test 471

6.3D.5 Test requirements 472

6.3E Maximum Input Level for DB-DC-HSDPA Reception (16QAM) 472

6.3E.1 Definition and applicability 472

6.3E.2 Minimum requirements 472

6.3E.3 Test purpose 473

6.3E.4 Method of test 473

6.3E.5 Test requirements 474

6.3F Maximum Input Level for DB-DC-HSDPA Reception (64QAM) 474

6.3F.1 Definition and applicability 474

6.3F.2 Minimum requirements 474

6.3F.3 Test purpose 475

6.3F.4 Method of test 475

6.3F.5 Test requirements 476

6.3G Maximum Input Level for 4C-HSDPA Reception (16QAM) 477

6.3G.1 Definition and applicability 477

6.3G.2 Minimum requirements 477

6.3G.3 Test purpose 477

6.3G.4 Method of test 477

6.3G.5 Test requirements 478

6.3GA Maximum Input Level for 4C-HSDPA Reception (16QAM) (3 carrier) 479

6.3GA.1 Definition and applicability 479

6.3GA.2 Minimum requirements 479

6.3GA.3 Test purpose 479

6.3GA.4 Method of test 479

6.3GA.5 Test requirements 480

6.3H Maximum Input Level for 4C-HSDPA Reception (64QAM) 481

6.3H.1 Definition and applicability 481

6.3H.2 Minimum requirements 481

6.3H.3 Test purpose 481

6.3H.4 Method of test 481

6.3H.5 Test requirements 483

6.3HA Maximum Input Level for 4C-HSDPA Reception (64QAM) (3 carrier) 483

6.3HA.1 Definition and applicability 483

6.3HA.2 Minimum requirements 483

6.3HA.3 Test purpose 484

6.3HA.4 Method of test 484

6.3HA.5 Test requirements 485

6.4 Adjacent Channel Selectivity (ACS) (Rel-99 and Rel-4) 486

6.4.1 Definition and applicability 486

6.4.2 Minimum Requirements 486

6.4.3 Test purpose 486

6.4.4 Method of test 487

6.4.5 Test requirements 487

6.4A Adjacent Channel Selectivity (ACS) (Rel-5 and later releases) 488

6.4A.1 Definition and applicability 488

6.4A.2 Minimum Requirements 488

6.4A.3 Test purpose 488

6.4A.4 Method of test 488

6.4A.5 Test requirements 489

6.4B Adjacent Channel Selectivity (ACS) for DC-HSDPA 489

6.4B.1 Definition and applicability 489

6.4B.2 Minimum Requirements 490

6.4B.3 Test purpose 490

6.4B.4 Method of test 490

6.4B.5 Test requirements 491

6.4C Adjacent Channel Selectivity (ACS) for DB-DC-HSDPA 492

6.4C.1 Definition and applicability 492

6.4C.2 Minimum Requirements 492

6.4C.3 Test purpose 493

6.4C.4 Method of test 493

6.4C.5 Test requirements 494

6.5 Blocking Characteristics 494

6.5.1 Definition and applicability 494

6.5.2 Minimum Requirements 494

6.5.2.1 Minimum Requirements (In-band blocking) 494

6.5.2.2 Minimum requirements (Out of-band blocking) 496

6.5.2.3 Minimum requirements (Narrow band blocking) 498

6.5.3 Test purpose 498

6.5.4 Method of test 498

6.5.5 Test requirements 499

6.5A Blocking Characteristics for DC-HSDPA 502

6.5A.1 Definition and applicability 502

6.5A.2 Minimum Requirements 503

6.5A.2.1 Minimum Requirements (In-band blocking) 503

6.5A.2.2 Minimum requirements (Out of-band blocking) 504

6.5A.2.3 Minimum requirements (Narrow band blocking) 506

6.5A.3 Test purpose 506

6.5A.4 Method of test 506

6.5A.5 Test requirements 508

6.5B Blocking Characteristics for DB-DC-HSDPA 511

6.5B.1 Definition and applicability 511

6.5B.2 Minimum Requirements 511

6.5B.2.1 Minimum Requirements (In-band blocking) 511

6.5B.2.2 Minimum requirements (Out of-band blocking) 513

6.5B.2.3 Minimum requirements (Narrow band blocking) 514

6.5B.3 Test purpose 514

6.5B.4 Method of test 514

6.5B.5 Test requirements 515

6.5C Blocking Characteristics for DC-HSUPA 518

6.5C.1 Definition and applicability 518

6.5C.2 Minimum Requirements 518

6.5C.2.1 Minimum Requirements (In-band blocking) 518

6.5C.2.2 Minimum requirements (Narrow band blocking) 520

6.5C.3 Test purpose 521

6.5C.4 Method of test 521

6.5C.5 Test requirements 522

6.5D Blocking Characteristics for single Uplink Single band 4C-HSDPA 525

6.5D.1 Definition and applicability 525

6.5D.2 Minimum Requirements 525

6.5D.2.1 Minimum Requirements (In-band blocking) 525

6.5D.2.2 Minimum requirements (Out of-band blocking) 526

6.5D.3 Test purpose 526

6.5D.4 Method of test 527

6.5D.4.1 Initial conditions 527

6.5D.4.2 Procedure 527

6.5D.5 Test requirements 527

6.5E Blocking Characteristics for dual uplink single band 4C-HSDPA 529

6.5E.1 Definition and applicability 529

6.5E.2 Minimum Requirements 529

6.5E.2.1 Minimum Requirements (In-band blocking) 529

6.5E.3 Test purpose 529

6.5E.4 Method of test 530

6.5E.4.1 Initial conditions 530

6.5E.4.2 Procedure 530

6.5E.5 Test requirements 530

6.5F Blocking Characteristics for single Uplink dual band 4C-HSDPA 531

6.5F.1 Definition and applicability 531

6.5F.2 Minimum Requirements 531

6.5F.2.1 Minimum Requirements (In-band blocking) 531

6.5F.2.2 Minimum requirements (Out of-band blocking) 532

6.5F.2.3 Minimum requirements (Narrow band blocking) 534

6.5F.3 Test purpose 535

6.5F.4 Method of test 535

6.5F.4.1 Initial conditions 535

6.5F.4.2 Procedure 536

6.5F.5 Test requirements 536

6.5FA Blocking Characteristics for single Uplink dual band 4C-HSDPA (3 carrier) 539

6.5FA.1 Definition and applicability 539

6.5FA.2 Minimum Requirements 539

6.5FA.2.1 Minimum Requirements (In-band blocking) 539

6.5FA.2.2 Minimum requirements (Out of-band blocking) 540

6.5FA.2.3 Minimum requirements (Narrow band blocking) 542

6.5FA.3 Test purpose 543

6.5FA.4 Method of test 543

6.5FA.4.1 Initial conditions 543

6.5FA.4.2 Procedure 544

6.5FA.5 Test requirements 544

6.5G Blocking Characteristics for dual uplink dual band 4C-HSDPA 547

6.5G.1 Definition and applicability 547

6.5G.2 Minimum Requirements 547

6.5G.2.1 Minimum Requirements (In-band blocking) 547

6.5G.2.2 Minimum requirements (Narrow band blocking) 549

6.5G.3 Test purpose 550

6.5G.4 Method of test 550

6.5G.5 Test requirements 551

6.5GA Blocking Characteristics for dual uplink dual band 4C-HSDPA (3 carrier) 553

6.5GA.1 Definition and applicability 553

6.5GA.2 Minimum Requirements 554

6.5GA.2.1 Minimum Requirements (In-band blocking) 554

6.5GA.2.2 Minimum requirements (Narrow band blocking) 555

6.5GA.3 Test purpose 556

6.5GA.4 Method of test 556

6.5GA.5 Test requirements 557

6.6 Spurious Response 559

6.6.1 Definition and applicability 559

6.6.2 Minimum Requirements 559

6.6.3 Test purpose 560

6.6.4 Method of test 560

6.6.5 Test requirements 560

6.6A Spurious Response for DC-HSDPA 561

6.6A.1 Definition and applicability 561

6.6A.2 Minimum Requirements 561

6.6A.3 Test purpose 561

6.6A.4 Method of test 561

6.6A.5 Test requirements 562

6.6B Spurious Response for DB-DC-HSDPA 563

6.6B.1 Definition and applicability 563

6.6B.2 Minimum Requirements 563

6.6B.3 Test purpose 563

6.6B.4 Method of test 563

6.6B.5 Test requirements 564

6.6C Spurious Response for single band 4C-HSDPA 565

6.6C.1 Definition and applicability 565

6.6C.2 Minimum Requirements 565

6.6C.3 Test purpose 565

6.6C.4 Method of test 565

6.6C.5 Test requirements 566

6.6D Spurious Response for dual band 4C-HSDPA 566

6.6D.1 Definition and applicability 566

6.6D.2 Minimum Requirements 567

6.6D.3 Test purpose 567

6.6D.4 Method of test 567

6.6D.5 Test requirements 568

6.6DA Spurious Response for dual band 4C-HSDPA (3 carrier) 568

6.6DA.1 Definition and applicability 568

6.6DA.2 Minimum Requirements 568

6.6DA.3 Test purpose 569

6.6DA.4 Method of test 569

6.6DA.5 Test requirements 569

6.7 Intermodulation Characteristics 570

6.7.1 Definition and applicability 570

6.7.2 Minimum Requirements 570

6.7.3 Test purpose 571

6.7.4 Method of test 571

6.7.5 Test requirements 572

6.7A Intermodulation Characteristics for DC-HSDPA 572

6.7A.1 Definition and applicability 572

6.7A.2 Minimum Requirements 573

6.7A.3 Test purpose 573

6.7A.4 Method of test 574

6.7A.5 Test requirements 574

6.7B Intermodulation Characteristics for DB-DC-HSDPA 575

6.7B.1 Definition and applicability 575

6.7B.2 Minimum Requirements 576

6.7B.3 Test purpose 576

6.7B.4 Method of test 577

6.7B.5 Test requirements 577

6.7C Intermodulation Characteristics for DC-HSUPA 578

6.7C.1 Definition and applicability 578

6.7C.2 Minimum Requirements 579

6.7C.3 Test purpose 580

6.7C.4 Method of test 580

6.7C.5 Test requirements 581

6.7D Intermodulation Characteristics for single uplink single band 4C-HSDPA 583

6.7D.1 Definition and applicability 583

6.7D.2 Minimum Requirements 583

6.7D.3 Test purpose 584

6.7D.4 Method of test 584

6.7D.5 Test requirements 585

6.7E Intermodulation Characteristics for single uplink dual band 4C-HSDPA 585

6.7E.1 Definition and applicability 585

6.7E.2 Minimum Requirements 585

6.7E.3 Test purpose 587

6.7E.4 Method of test 587

6.7E.5 Test requirements 588

6.7EA Intermodulation Characteristics for single uplink dual band 4C-HSDPA (3 carrier) 590

6.7EA.1 Definition and applicability 590

6.7EA.2 Minimum Requirements 590

6.7EA.3 Test purpose 591

6.7EA.4 Method of test 592

6.7EA.5 Test requirements 592

6.8 Spurious Emissions 594

6.8.1 Definition and applicability 594

6.8.2 Minimum Requirements 594

6.8.3 Test purpose 595

6.8.4 Method of test 596

6.8.5 Test requirements 596

6.8A Spurious Emissions for DB-DC-HSDPA 599

6.8A.1 Definition and applicability 599

6.8A.2 Minimum Requirements 599

6.8A.3 Test purpose 599

6.8A.4 Method of test 599

6.8A.5 Test requirements 599

7 Performance requirements 601

7.1 General 601

7.1.1 Measurement Configurations 601

7.1.2 Definition of Additive White Gaussian Noise (AWGN) Interferer 601

7.2 Demodulation in Static Propagation conditions 602

7.2.1 Demodulation of Dedicated Channel (DCH) 602

7.2.1.1 Definition and applicability 602

7.2.1.2 Minimum requirements 602

7.2.1.3 Test purpose 602

7.2.1.4 Method of test 602

7.2.1.5 Test requirements 603

7.2.2 Demodulation of Dedicated Channel (DCH) when (DL\_DCH\_FET\_Config) is configured by higher layers 603

7.2.2.1 Definition and applicability 603

7.2.2.2 Minimum requirements 604

7.2.2.3 Test purpose 604

7.2.2.4 Method of test 604

7.2.2.4.1 Initial conditions 604

7.2.2.4.2 Procedures 605

7.2.2.5 Test requirements 605

7.3 Demodulation of DCH in Multi-path Fading Propagation conditions 606

7.3.1 Single Link Performance 606

7.3.1.1 Definition and applicability 606

7.3.1.2 Minimum requirements 606

7.3.1.3 Test purpose 608

7.3.1.4 Method of test 608

7.3.1.5 Test requirements 609

7.3.2 Single Link Performance when (DL\_DCH\_FET\_Config) is configured by higher layers 611

7.3.2.1 Definition and applicability 611

7.3.2.2 Minimum requirements 612

7.3.2.3 Test purpose 613

7.3.2.4 Method of test 613

7.3.2.4.1 Initial conditions 613

7.3.2.5 Test requirements 614

7.4 Demodulation of DCH in Moving Propagation conditions 616

7.4.1 Single Link Performance 616

7.4.1.1 Definition and applicability 616

7.4.1.2 Minimum requirements 616

7.4.1.3 Test purpose 617

7.4.1.4 Method of test 617

7.4.1.5 Test requirements 617

7.5 Demodulation of DCH in Birth-Death Propagation conditions 618

7.5.1 Single Link Performance 618

7.5.1.1 Definition and applicability 618

7.5.1.2 Minimum requirements 618

7.5.1.3 Test purpose 618

7.5.1.4 Method of test 618

7.5.1.5 Test requirements 619

7.5A Demodulation of DCH in high speed train condition 619

7.5A.1 Single Link Performance 619

7.5A.1.1 Definition and applicability 619

7.5A.1.2 Minimum requirement 619

7.5A.1.3 Test purpose 620

7.5A.1.4 Method of test 620

7.5A.1.5 Test requirements 620

7.6 Demodulation of DCH in downlink Transmit diversity modes 621

7.6.1 Demodulation of DCH in open-loop transmit diversity mode 621

7.6.1.1 Definition and applicability 621

7.6.1.2 Minimum requirements 621

7.6.1.3 Test purpose 621

7.6.1.4 Method of test 621

7.6.1.5 Test Requirements 622

7.6.2 Demodulation of DCH in closed loop transmit diversity mode 623

7.6.2.1 Definition and applicability 623

7.6.2.2 Minimum requirements 623

7.6.2.3 Test purpose 624

7.6.2.4 Method of test 624

7.6.2.5 Test Requirements 625

7.6.3 Demodulation of DCH in Site Selection Diversity Transmission Power Control mode 626

7.6.3.1 Definition and applicability 626

7.6.3.2 Minimum requirements 626

7.6.3.3 Test purpose 627

7.6.3.4 Method of test 627

7.6.3.5 Test Requirements 630

7.7 Demodulation in Handover conditions 631

7.7.1 Demodulation of DCH in Inter-Cell Soft Handover (Release 5 and earlier) 631

7.7.1.1 Definition and applicability 631

7.7.1.2 Minimum requirements 631

7.7.1.3 Test purpose 632

7.7.1.4 Method of test 632

7.7.1.5 Test requirements 632

7.7.1A Demodulation of DCH in Inter-Cell Soft Handover (Release 6 and later) 633

7.7.1A.1 Definition and applicability 633

7.7.1A.2 Minimum requirements 633

7.7.1A.3 Test purpose 634

7.7.1A.4 Method of test 634

7.7.1A.5 Test requirements 634

7.7.1B Demodulation of DCH in Inter-Cell Soft Handover when (DL\_DCH\_FET\_Config) is configured by higher layers 635

7.7.1B.1 Definition and applicability 635

7.7.1B.2 Minimum requirements 635

7.7.1B.3 Test purpose 636

7.7.1B.4 Method of test 636

7.7.1B.4.1 Initial conditions 636

7.7.1B.4.2 Procedures 636

7.7.1B.5 Test requirements 636

7.7.2 Combining of TPC commands from radio links of different radio link sets 637

7.7.2.1 Definition and applicability 637

7.7.2.2 Minimum requirements 637

7.7.2.3 Test purpose 638

7.7.2.4 Method of test 638

7.7.2.5 Test requirements 639

7.7.2A Combining of TPC commands from radio links of different radio link sets when (DL\_DCH\_FET\_Config) is configured by higher layers 640

7.7.2A.1 Definition and applicability 640

The requirements and this test apply to release 12 and later releases for all types of UTRA for the FDD UE that support DCH Enhancement for UMTS.7.7.2A.2 Minimum requirements 640

7.7.2A.3 Test purpose 641

7.7.2A.4 Method of test 641

7.7.2A.4.1 Initial conditions 641

7.7.2A.4.2 Procedures 642

7.7.2A.5 Test requirements 643

7.7.3 Combining of reliable TPC commands from radio links of different radio link sets 644

7.7.3.1 Definition and applicability 644

7.7.3.2 Minimum requirements 644

7.7.3.3 Test purpose 644

7.7.3.4 Method of test 645

7.7.3.4.1 Test 1 Initial conditions 645

7.7.3.4.2 Test 1 Procedures 645

7.7.3.4.3 Test 2 Initial conditions 645

7.7.3.4.4 Test 2 Procedures 645

7.7.3.5 Test requirements 646

7.7.3A Combining of reliable TPC commands from radio links of different radio link sets when DL\_DCH\_FET\_Config [10] is configured by higher layers 647

7.7.3A.1 Definition and applicability 647

7.7.3A.2 Minimum requirements 647

7.7.3A.3 Test purpose 647

7.7.3A.4 Method of test 648

7.7.3A.4.1 Test 1 Initial conditions 648

7.7.3A.4.2 Test 1 Procedures 648

7.7.3A.4.3 Test 2 Initial conditions 648

7.7.3A.4.4 Test 2 Procedures 648

7.7.3A.5 Test requirements 649

7.8 Power control in downlink 650

7.8.1 Power control in the downlink, constant BLER target (Release 5 and earlier) 651

7.8.1.1 Definition and applicability 651

7.8.1.2 Minimum requirements 651

7.8.1.3 Test purpose 651

7.8.1.4 Method of test 651

7.8.1.5 Test Requirements 652

7.8.1A Power control in the downlink, constant BLER target (Release 6 and later) 653

7.8.1A.1 Definition and applicability 653

7.8.1A.2 Minimum requirements 653

7.8.1A.3 Test purpose 653

7.8.1A.4 Method of test 653

7.8.1A.5 Test Requirements 654

7.8.1B Power control in the downlink, constant BLER target when DL\_DCH\_FET\_Config is configured by higher layers 655

7.8.1B.1 Definition and applicability 655

7.8.1B.2 Minimum requirements 655

7.8.1B.3 Test purpose 656

7.8.1B.4 Method of test 656

7.8.1B.5 Test Requirements 658

7.8.2 Power control in the downlink, initial convergence 660

7.8.2.1 Definition and applicability 660

7.8.2.2 Minimum requirements 660

7.8.2.3 Test purpose 661

7.8.2.4 Method of test 661

7.8.2.5 Test Requirements 661

7.8.2A Power control in the downlink, initial convergence when DL\_DCH\_FET\_Config is configured by higher layers 663

7.8.2A.1 Definition and applicability 663

7.8.2A.2 Minimum requirements 663

7.8.2A.3 Test purpose 664

7.8.2A.4 Method of test 664

7.8.2A.5 Test Requirements 665

7.8.3 Power control in the downlink, wind up effects (Release 5 and earlier) 667

7.8.3.1 Definition and applicability 667

7.8.3.2 Minimum requirements 667

7.8.3.3 Test purpose 667

7.8.3.4 Method of test 667

7.8.3.5 Test Requirements 668

7.8.3A Power control in the downlink, wind up effects (Release 6 and later) 669

7.8.3A.1 Definition and applicability 669

7.8.3A.2 Minimum requirements 669

7.8.3A.3 Test purpose 670

7.8.3A.4 Method of test 670

7.8.3B Power control in the downlink, wind up effects (Release 6 and later) when DL\_DCH\_FET\_Config is configured by higher layers 671

7.8.3B.1 Definition and applicability 671

7.8.3B.2 Minimum requirements 671

7.8.3B.3 Test purpose 673

7.8.3B.4 Method of test 674

7.8.3B.4.1 Initial conditions 674

7.8.3B.4.2 Procedure 674

7.8.3B.5 Test Requirements 676

7.8.4 Power control in the downlink, different transport formats 678

7.8.4.1 Definition and applicability 678

7.8.4.2 Minimum requirements 678

7.8.4.3 Test purpose 679

7.8.4.4 Method of test 679

7.8.4.5 Test Requirements 680

7.8.4A Power control in the downlink, different transport formats when DL\_DCH\_FET\_Config is configured by higher layers 681

7.8.4A.1 Definition and applicability 681

7.8.4A.2 Minimum requirements 681

7.8.4A.3 Test purpose 682

7.8.4A.4 Method of test 682

7.8.4A.4.1 Initial conditions 682

7.8.4A.4.2 Procedure 683

7.8.4.5 Test Requirements 684

7.8.5 Power control in the downlink for F-DPCH 686

7.8.5.1 Definition and applicability 686

7.8.5.2 Minimum requirements 686

7.8.5.3 Test purpose 687

7.8.5.4 Method of test 687

7.8.5.5 Test Requirements 690

7.9 Downlink compressed mode 690

7.9.1 Single link performance (Release 5 and earlier) 691

7.9.1.1 Definition and applicability 691

7.9.1.2 Minimum requirements 691

7.9.1.3 Test purpose 692

7.9.1.4 Method of test 692

7.9.1.5 Test requirements 692

7.9.1A Single link performance (Release 6 and later) 694

7.9.1A.1 Definition and applicability 694

7.9.1A.2 Minimum requirements 694

7.9.1A.3 Test purpose 694

7.9.1A.4 Method of test 695

7.9.1A.5 Test requirements 695

7.10 Blind transport format detection 696

7.10.1 Definition and applicability 696

7.10.2 Minimum requirements 696

7.10.3 Test purpose 697

7.10.4 Method of test 697

7.10.5 Test requirements 698

7.11 Demodulation of Paging Channel (PCH) 698

7.11.1 Definition and applicability 698

7.11.2 Minimum requirements 698

7.11.3 Test purpose 699

7.11.4 Method of test 699

7.11.5 Test requirements 702

7.12 Detection of Acquisition Indicator (AI) 702

7.12.1 Definition and applicability 702

7.12.2 Minimum requirements 703

7.12.3 Test purpose 703

7.12.4 Method of test 703

7.12.5 Test requirements 705

7.12A Detection of E-DCH Acquisition Indicator (E-AI) 705

7.12A.1 Definition and applicability 705

7.12A.2 Minimum requirements 705

7.12A.3 Test purpose 706

7.12A.4 Method of test 706

7.12A.5 Test requirements 707

7.13 UE UL power control operation with discontinuous UL DPCCH transmission operation 708

7.13.1 Definition and applicability 708

7.13.2 Minimum requirement 708

7.13.3 Test purpose 708

7.13.4 Method of test 709

7.13.4.1 Initial conditions 709

7.13.4.2 Procedure 709

7.13.5. Test Requirements 711

8 Requirements for support of RRM 712

8.1 General 712

8.1.1 Definition of Additive White Gaussian Noise (AWGN) Interferer 712

8.1.2 Groups of E-UTRA bands 712

8.2 Idle Mode Tasks 713

8.2.1 Cell Selection 713

8.2.2 Cell Re-Selection 713

8.2.2.1 Scenario 1: Single carrier case 713

8.2.2.1.1 Definition and applicability 713

8.2.2.1.2 Minimum requirement 713

8.2.2.1.3 Test purpose 714

8.2.2.1.4 Method of test 714

8.2.2.1.5 Test requirements 717

8.2.2.2 Scenario 2: Multi carrier case 717

8.2.2.2.1 Definition and applicability 717

8.2.2.2.2 Minimum requirement 717

8.2.2.2.3 Test purpose 717

8.2.2.2.4 Method of test 718

8.2.2.2.5 Test requirements 720

8.2.3 UTRAN to GSM Cell Re-Selection 722

8.2.3.1 Scenario 1: Both UTRA and GSM level changed 722

8.2.3.1.1 Definition and applicability 722

8.2.3.1.2 Minimum requirement 722

8.2.3.1.3 Test purpose 722

8.2.3.1.4 Method of test 722

8.2.3.1.5 Test requirements 724

8.2.3.2 Scenario 2: Only UTRA level changed 725

8.2.3.2.1 Definition and applicability 725

8.2.3.2.2 Minimum requirement 725

8.2.3.2.3 Test purpose 725

8.2.3.2.4 Method of test 725

8.2.3.2.5 Test requirements 727

8.2.3.3 Scenario 3: HCS with only UTRA level changed 728

8.2.3.3.1 Definition and applicability 728

8.2.3.3.2 Minimum requirement 728

8.2.3.3.3 Test purpose 728

8.2.3.3.4 Method of test 728

8.2.3.3.5 Test requirements 730

8.2.4 FDD/TDD Cell Re-selection 731

8.2.4.1 Definition and applicability 731

8.2.4.1.1 3.84 Mcps TDD Option 731

8.2.4.1.2 1.28 Mcps TDD Option 731

8.2.4.2 Minimum requirement 732

8.2.4.3 Test purpose 732

8.2.4.4 Method of test 732

8.2.4.4.1 Initial conditions 732

8.2.4.4.1.1 3.84 Mcps TDD Option 732

8.2.4.4.1.2 1.28Mcps TDD Option 733

8.2.4.4.2 Procedures 734

8.2.4.5 Test requirements 734

8.2.5 UTRAN to E-UTRA Cell Re-Selection 735

8.2.5.1 E-UTRA is of higher priority 735

8.2.5.1.1 Definition and applicability 735

8.2.5.1.2 Minimum requirement 735

8.2.5.1.3 Test purpose 735

8.2.5.1.4 Method of test 735

8.2.5.1.5 Test requirements 738

8.2.5.2 E-UTRA is of lower priority 739

8.2.5.2.1 Definition and applicability 739

8.2.5.2.2 Minimum requirement 740

8.2.5.2.3 Test purpose 740

8.2.5.2.4 Method of test 740

8.2.5.2.5 Test requirements 743

8.2.5.3 RSRQ based reselection when E-UTRA FDD is of higher priority 744

8.2.5.3.1 Definition and applicability 744

8.2.5.3.2 Minimum requirement 744

8.2.5.3.3 Test purpose 744

8.2.5.3.4 Method of test 744

8.2.5.3.5 Test requirements 749

8.3 UTRAN Connected Mode Mobility 750

8.3.1 FDD/FDD Soft Handover 750

8.3.1.1 Definition and applicability 750

8.3.1.2 Minimum requirement 751

8.3.1.3 Test purpose 751

8.3.1.4 Method of test 751

8.3.1.5 Test requirements 756

8.3.2 FDD/FDD Hard Handover 757

8.3.2.1 FDD/FDD Hard Handover to intra-frequency cell 757

8.3.2.1.1 Definition and applicability 757

8.3.2.1.2 Minimum requirement 757

8.3.2.1.3 Test purpose 758

8.3.2.1.4 Method of test 758

8.3.2.1.5 Test requirements 764

8.3.2.2 FDD/FDD Hard Handover to inter-frequency cell 764

8.3.2.2.1 Definition and applicability 764

8.3.2.2.2 Minimum requirement 764

8.3.2.2.3 Test purpose 765

8.3.2.2.4 Method of test 765

8.3.2.2.5 Test requirements 770

8.3.3 FDD/TDD Handover 771

8.3.3.1 Definition and applicability 771

8.3.3.2 Minimum requirement 771

8.3.3.3 Test purpose 771

8.3.3.4 Method of test 771

8.3.3.5 Test requirements 776

8.3.4 Inter-system Handover from UTRAN FDD to GSM 777

8.3.4.1 Definition and applicability 777

8.3.4.2 Minimum requirement 777

8.3.4.3 Test purpose 777

8.3.4.4 Method of test 777

8.3.4.5 Test requirements 784

8.3.4a Inter-system Handover from UTRAN FDD to E-UTRAN FDD 784

8.3.4a.1 Definition and applicability 784

8.3.4a.2 Minimum requirement 785

8.3.4a.3 Test purpose 785

8.3.4a.4 Method of test 785

8.3.4a.5 Test requirements 793

8.3.4b Inter-system Handover from UTRAN FDD to E-UTRAN TDD 794

8.3.4b.1 Definition and applicability 794

8.3.4b.2 Minimum requirement 795

8.3.4b.3 Test purpose 795

8.3.4b.4 Method of test 795

8.3.4b.4.1 Initial conditions 795

8.3.4b.4.2 Procedure 797

8.3.4b.5 Test requirements 803

8.3.4c Inter-system Handover from UTRAN FDD to E-UTRAN FDD: Unknown Target Cell 805

8.3.4c.1 Definition and applicability 805

8.3.4c.2 Minimum requirement 805

8.3.4c.3 Test purpose 805

8.3.4c.4 Method of test 805

8.3.4c.5 Test requirements 811

8.3.4d Inter-system Handover from UTRAN FDD to E-UTRAN TDD; Unknown Target Cell 812

8.3.4d.1 Definition and applicability 812

8.3.4d.2 Minimum requirement 812

8.3.4d.3 Test purpose 812

8.3.4d.4 Method of test 812

8.3.4d.4.1 Initial conditions 812

8.3.4d.4.2 Procedure 814

8.3.4d.5 Test requirements 818

8.3.5 Cell Re-selection in CELL\_FACH 818

8.3.5.1 One frequency present in neighbour lis and FACH measurement occasions configured 818

8.3.5.1.1 Definition and applicability 818

8.3.5.1.2 Minimum requirements 819

8.3.5.1.3 Test purpose 819

8.3.5.1.4 Method of test 819

8.3.5.1.5 Test requirements 821

8.3.5.1a One frequency present in neighbour list and HS-DSCH DRX configured 822

8.3.5.1a.1 Definition and applicability 822

8.3.5.1a.2 Minimum requirements 822

8.3.5.1a.3 Test purpose 822

8.3.5.1a.4 Method of test 823

8.3.5.1a.5 Test requirements 825

8.3.5.2 Two frequencies present in the neighbour list and FACH measurement occasions configured 826

8.3.5.2.1 Definition and applicability 826

8.3.5.2.2 Minimum requirements 826

8.3.5.2.3 Test purpose 826

8.3.5.2.4 Method of test 827

8.3.5.2.5 Test requirements 830

8.3.5.2a Two frequencies present in the neighbour list and HS-DSCH DRX configured (Absolute priority levels not configured) 830

8.3.5.2a.1 Definition and applicability 830

8.3.5.2a.2 Minimum requirements 830

8.3.5.2a.3 Test purpose 831

8.3.5.2a.4 Method of test 831

8.3.5.2a.5 Test requirements 833

8.3.5.2b Two frequencies present in the neighbour list and HS-DSCH DRX configured (Absolute priority levels configured) 834

8.3.5.2b.1 Definition and applicability 834

8.3.5.2b.2 Minimum requirements 834

8.3.5.2b.3 Test purpose 834

8.3.5.2b.4 Method of test 835

8.3.5.2b.5 Test requirements 837

8.3.5.2c Two frequencies present in the neighbour list and HS-DSCH 2nd DRX configured (Absolute priority levels not configured) 838

8.3.5.2c.1 Definition and applicability 838

8.3.5.2c.2 Minimum requirements 838

8.3.5.2c.3 Test purpose 838

8.3.5.2c.4 Method of test 839

8.3.5.2c.5 Test requirements 841

8.3.5.2d Two frequencies present in the neighbour list and HS-DSCH 2nd DRX configured (Absolute priority levels configured) 842

8.3.5.2d.1 Definition and applicability 842

8.3.5.2d.2 Minimum requirements 842

8.3.5.2d.3 Test purpose 843

8.3.5.2d.4 Method of test 843

8.3.5.2d.5 Test requirements 846

8.3.5.3 Cell Reselection to GSM 847

8.3.5.3.1 Definition and applicability 847

8.3.5.3.2 Minimum requirements 847

8.3.5.3.3 Test purpose 848

8.3.5.3.4 Method of test 848

8.3.5.3.5 Test requirements 850

8.3.5.4 Cell Reselection during an MBMS session, two frequencies present in neighbour list 851

8.3.5.4.1 Definition and applicability 851

8.3.5.4.2 Minimum requirements 851

8.3.5.4.3 Test purpose 851

8.3.5.4.4 Method of test 852

8.3.5.4.5 Test requirements 856

8.3.5.5 UTRAN to E-UTRA Cell Reselection 857

8.3.5.5.1 Reselection to E-UTRA FDD when HS-DSCH DRX is configured (E-UTRA has higher priority) 857

8.3.5.5.1.1 Definition and applicability 857

8.3.5.5.1.1 Minimum requirements 857

8.3.5.5.1.3 Test purpose 857

8.3.5.5.1.4 Method of test 857

8.3.5.5.1.4.1 Initial conditions 857

8.3.5.5.1.4.2 Procedure 860

8.3.5.5.1.5 Test requirements 861

8.3.5.5.2 Reselection to E-UTRA FDD when HS-DSCH DRX is configured (E-UTRA has lower priority) 863

8.3.5.5.2.1 Definition and applicability 863

8.3.5.5.2.1 Minimum requirements 863

8.3.5.5.2.3 Test purpose 863

8.3.5.5.2.4 Method of test 863

8.3.5.5.2.4.1 Initial conditions 863

8.3.5.5.2.4.2 Procedure 866

8.3.5.5.2.5 Test requirements 867

8.3.5.5.3 Reselection to E-UTRA FDD when HS-DSCH 2nd DRX is configured (E-UTRA has higher priority) 869

8.3.5.5.3.1 Definition and applicability 869

8.3.5.5.3.1 Minimum requirements 869

8.3.5.5.3.3 Test purpose 870

8.3.5.5.3.4 Method of test 870

8.3.5.5.3.4.1 Initial conditions 870

8.3.5.5.3.4.2 Procedure 873

8.3.5.5.1.5 Test requirements 874

8.3.5.5.4 Reselection to E-UTRA TDD when HS-DSCH DRX is configured (E-UTRA has higher priority) 876

8.3.5.5.4.1 Definition and applicability 876

8.3.5.5.4.1 Minimum requirements 876

8.3.5.5.4.3 Test purpose 877

8.3.5.5.4.4 Method of test 877

8.3.5.5.4.4.1 Initial conditions 877

8.3.5.5.4.4.2 Procedure 880

8.3.5.5.4.5 Test requirements 880

8.3.5.5.5 Reselection to E-UTRA TDD when HS-DSCH DRX is configured (E-UTRA has lower priority) 881

8.3.5.5.5.1 Definition and applicability 881

8.3.5.5.5.1 Minimum requirements 881

8.3.5.5.5.3 Test purpose 882

8.3.5.5.5.4 Method of test 882

8.3.5.5.5.4.1 Initial conditions 882

8.3.5.5.5.4.2 Procedure 885

8.3.5.5.5.5 Test requirements 885

8.3.5.5.6 Reselection to E-UTRA TDD when HS-DSCH 2nd DRX is configured (E-UTRA has higher priority) 886

8.3.5.5.6.1 Definition and applicability 886

8.3.5.5.6.2 Minimum requirements 886

8.3.5.5.6.3 Test purpose 887

8.3.5.5.6.4 Method of test 887

8.3.5.5.6.4.1 Initial conditions 887

8.3.5.5.6.4.2 Procedure 890

8.3.5.5.6.5 Test requirements 890

8.3.6 Cell Re-selection in CELL\_PCH 892

8.3.6.1 One frequency present in the neighbour list 892

8.3.6.1.1 Definition and applicability 892

8.3.6.1.2 Minimum requirements 892

8.3.6.1.3 Test purpose 892

8.3.6.1.4 Method of test 892

8.3.6.1.5 Test requirements 896

8.3.6.2 Two frequencies present in the neighbour list 896

8.3.6.2.1 Definition and applicability 896

8.3.6.2.2 Minimum requirement 896

8.3.6.2.3 Test purpose 897

8.3.6.2.4 Method of test 897

8.3.6.2.5 Test requirements 901

8.3.6.3 Cell re-selection during an MBMS session, one UTRAN inter-frequency and 2 GSM cells present in the neighbour list 902

8.3.6.3.1 Definition and applicability 902

8.3.6.3.2 Minimum requirement 902

8.3.6.3.3 Test purpose 902

8.3.6.3.4 Method of test 902

8.3.6.3.5 Test requirements 906

8.3.7 Cell Re-selection in URA\_PCH 907

8.3.7.1 One frequency present in the neighbour list 907

8.3.7.1.1 Definition and applicability 907

8.3.7.1.2 Minimum requirement 907

8.3.7.1.3 Test purpose 908

8.3.7.1.4 Method of test 908

8.3.7.1.5 Test requirements 911

8.3.7.2 Two frequencies present in the neighbour list 911

8.3.7.2.1 Definition and applicability 911

8.3.7.2.2 Minimum requirement 911

8.3.7.2.3 Test purpose 912

8.3.7.2.4 Method of test 912

8.3.7.2.5 Test requirements 915

8.3.8 Serving HS-DSCH cell change 916

8.3.8.1 Definition and applicability 916

8.3.8.2 Minimum requirement 916

8.3.8.3 Test purpose 916

8.3.8.4 Method of test 916

8.3.8.4.1 Initial conditions 920

8.3.8.4.2 Procedure 920

8.3.8.5 Test requirements 929

8.3.9 Enhanced Serving HS-DSCH cell change 931

8.3.9.1 Definition and applicability 931

8.3.9.2 Minimum requirement 931

8.3.9.3 Test purpose 931

8.3.9.4 Method of test 932

8.3.9.4.1 Initial conditions 933

8.3.9.4.2 Procedure 933

8.3.9.5 Test requirements 941

8.3.10 System information acquisition for CSG cell 941

8.3.10.1 Intrafrequency System information acquisition for CSG cell 941

8.3.10.1.1 Definition and applicability 941

8.3.10.1.2 Minimum requirement 942

8.3.10.1.3 Test purpose 942

8.3.10.1.4 Method of test 942

8.3.10.1.5 Test requirements 946

8.3.10.2 Inter frequency System information acquisition for CSG cell 946

8.3.10.2.1 Definition and applicability 946

8.3.10.2.2 Minimum requirement 946

8.3.10.2.3 Test purpose 947

8.3.10.2.4 Method of test 947

8.3.10.2.5 Test requirements 953

8.4 RRC Connection Control 954

8.4.1 RRC Re-establishment delay 954

8.4.1.1 Test 1 954

8.4.1.1.1 Definition and applicability 954

8.4.1.1.2 Minimum requirement 954

8.4.1.1.3 Test purpose 954

8.4.1.1.4 Method of test 955

8.4.1.1.5 Test requirements 957

8.4.1.2 Test 2 957

8.4.1.2.1 Definition and applicability 957

8.4.1.2.2 Minimum requirement 957

8.4.1.2.3 Test purpose 958

8.4.1.2.4 Method of test 958

8.4.1.2.5 Test requirements 959

8.4.2 Random Access 960

8.4.2.1 Correct behaviour when receiving an ACK (Release 5 and earlier) 960

8.4.2.1.1 Definition and applicability 960

8.4.2.1.2 Minimum Requirements 960

8.4.2.1.3 Test purpose 960

8.4.2.1.4 Method of test 960

8.4.2.1.5 Test requirements 962

8.4.2.1A Correct behaviour when receiving an ACK (Release 6 and later) 963

8.4.2.1A.1 Definition and applicability 963

8.4.2.1A.2 Minimum Requirements 963

8.4.2.1A.3 Test purpose 963

8.4.2.1A.4 Method of test 963

8.4.2.1A.5 Test requirements 965

8.4.2.2 Correct behaviour when receiving an NACK 966

8.4.2.2.1 Definition and applicability 966

8.4.2.2.2 Minimum Requirements 966

8.4.2.2.3 Test purpose 966

8.4.2.2.4 Method of test 966

8.4.2.2.5 Test requirements 966

8.4.2.3 Correct behaviour at Time-out 967

8.4.2.3.1 Definition and applicability 967

8.4.2.3.2 Minimum Requirements 967

8.4.2.3.3 Test purpose 967

8.4.2.3.4 Method of test 967

8.4.2.3.5 Test requirements 967

8.4.2.4 Correct behaviour when reaching maximum transmit power 967

8.4.2.4.1 Definition and applicability 967

8.4.2.4.2 Minimum Requirements 968

8.4.2.4.3 Test purpose 968

8.4.2.4.4 Method of test 968

8.4.2.4.5 Test requirements 969

8.4.3 Transport format combination selection in UE 969

8.4.3.1 Interactive or Background, PS, UL: 64 kbps 969

8.4.3.1.1 Definition and applicability 969

8.4.3.1.2 Minimum requirements 969

8.4.3.1.3 Test purpose 970

8.4.3.1.4 Method of test 970

8.4.3.1.5 Test requirements 973

8.4.3.1A Interactive or Background, PS, UL: 64 kbps + Conversational / speech, CS, UL: 12.2kbps 973

8.4.3.1A.1 Definition and applicability 973

8.4.3.1A.2 Minimum requirements 973

8.4.3.1A.3 Test purpose 975

8.4.3.1A.4 Method of test 975

8.4.3.1A.5 Test requirements 978

8.4.4 E-TFC restriction in UE 979

8.4.4.1 10ms TTI E-DCH E-TFC restriction 979

8.4.4.1.1 Definition and applicability 979

8.4.4.1.2 Minimum requirements 979

8.4.4.1.3 Test Purpose 981

8.4.4.1.4 Method of test 981

8.4.4.1.5 Test Requirements 985

8.4.4.2 2ms TTI E-DCH E-TFC restriction 985

8.4.4.2.1 Definition and applicability 985

8.4.4.2.2 Minimum requirements 985

8.4.4.2.3 Test Purpose 988

8.4.4.2.4 Method of test 988

8.4.4.2.5 Test Requirements 992

8.5 Timing and Signalling Characteristics 992

8.5.1 UE Transmit Timing 992

8.5.1.1 Definition and applicability 992

8.5.1.2 Minimum requirements 993

8.5.1.3 Test purpose 994

8.5.1.4 Method of test 994

8.5.1.5 Test requirements 998

8.6 UE Measurements Procedures 999

8.6.1 FDD intra frequency measurements 999

8.6.1.1 Event triggered reporting in AWGN propagation conditions (R99) 999

8.6.1.1.1 Definition and applicability 999

8.6.1.1.2 Minimum requirements 999

8.6.1.1.3 Test purpose 1000

8.6.1.1.4 Method of test 1001

8.6.1.1.5 Test requirements 1004

8.6.1.1A Event triggered reporting in AWGN propagation conditions (Rel-4 and later) 1004

8.6.1.1A.1 Definition and applicability 1004

8.6.1.1A.2 Minimum requirements 1005

8.6.1.1A.3 Test purpose 1006

8.6.1.1A.4 Method of test 1006

8.6.1.1A.5 Test requirements 1009

8.6.1.2 Event triggered reporting of multiple neighbours in AWGN propagation condition (R99) 1010

8.6.1.2.1 Definition and applicability 1010

8.6.1.2.2 Minimum requirements 1010

8.6.1.2.3 Test purpose 1010

8.6.1.2.4 Method of test 1010

8.6.1.2.5 Test requirements 1017

8.6.1.2A Event triggered reporting of multiple neighbours in AWGN propagation condition (Rel-4 and later) 1019

8.6.1.2A.1 Definition and applicability 1019

8.6.1.2A.2 Minimum requirements 1019

8.6.1.2A.3 Test purpose 1019

8.6.1.2A.4 Method of test 1019

8.6.1.2A.5 Test requirements 1025

8.6.1.3 Event triggered reporting of two detectable neighbours in AWGN propagation condition (R99) 1026

8.6.1.3.1 Definition and applicability 1026

8.6.1.3.2 Minimum requirements 1026

8.6.1.3.3 Test purpose 1026

8.6.1.3.4 Method of test 1026

8.6.1.3.5 Test requirements 1032

8.6.1.3A Event triggered reporting of two detectable neighbours in AWGN propagation condition (Rel-4 and later) 1034

8.6.1.3A.1 Definition and applicability 1034

8.6.1.3A.2 Minimum requirements 1034

8.6.1.3A.3 Test purpose 1034

8.6.1.3A.4 Method of test 1034

8.6.1.3A.5 Test requirements 1037

8.6.1.4 Void 1038

8.6.1.4A Correct reporting of neighbours in fading propagation condition (Rel-4 and later) 1038

8.6.1.4A.1 Definition and applicability 1038

8.6.1.4A.2 Minimum requirements 1039

8.6.1.4A.3 Test purpose 1039

8.6.1.4A.4 Method of test 1039

8.6.1.4A.5 Test requirements 1042

8.6.1.5 Event triggered reporting of multiple neighbour cells in Case 1 fading condition 1043

8.6.1.5.1 Definition and applicability 1043

8.6.1.5.2 Minimum requirements 1043

8.6.1.5.3 Test purpose 1043

8.6.1.5.4 Method of test 1043

8.6.1.5.5 Test requirements 1046

8.6.1.6 Event triggered reporting of multiple neighbour cells in Case 3 fading condition 1047

8.6.1.6.1 Definition and applicability 1047

8.6.1.6.2 Minimum requirements 1047

8.6.1.6.3 Test purpose 1047

8.6.1.6.4 Method of test 1047

8.6.1.6.5 Test requirements 1051

8.6.2 FDD inter frequency measurements 1052

8.6.2.1 Correct reporting of neighbours in AWGN propagation condition (Release 5 and earlier) 1052

8.6.2.1.1 Definition and applicability 1052

8.6.2.1.2 Minimum requirements 1052

8.6.2.1.3 Test purpose 1053

8.6.2.1.4 Method of test 1053

8.6.2.1.5 Test requirements 1059

8.6.2.1A Correct reporting of neighbours in AWGN propagation condition (Release 6 and later) 1060

8.6.2.1A.1 Definition and applicability 1060

8.6.2.1A.2 Minimum requirements 1061

8.6.2.1A.3 Test purpose 1061

8.6.2.1A.4 Method of test 1062

8.6.2.1A.5 Test requirements 1068

8.6.2.2 Correct reporting of neighbours in fading propagation condition (Release 5 only) 1069

8.6.2.2.1 Definition and applicability 1069

8.6.2.2.2 Minimum requirements 1069

8.6.2.2.3 Test purpose 1069

8.6.2.2.4 Method of test 1069

8.6.2.2.4.1 Initial conditions 1069

8.6.2.2.4.2 Procedure 1070

8.6.2.2.5 Test requirements 1074

8.6.2.2A Correct reporting of neighbours in fading propagation condition (Release 6 and later) 1074

8.6.2.2A.1 Definition and applicability 1074

8.6.2.2A.2 Minimum requirements 1074

8.6.2.2A.3 Test purpose 1074

8.6.2.2A.4 Method of test 1075

8.6.2.2A.4.1 Initial conditions 1075

8.6.2.2A.4.2 Procedure 1075

8.6.2.2A.5 Test requirements 1079

8.6.2.3 Correct reporting of neighbours in fading propagation condition using TGL1=14 1079

8.6.2.3.1 Definition and applicability 1079

8.6.2.3.2 Minimum requirements 1080

8.6.2.3.3 Test purpose 1080

8.6.2.3.4 Method of test 1080

8.6.2.3.4.1 Initial conditions 1080

8.6.2.3.4.2 Procedure 1081

8.6.2.3.5 Test requirements 1084

8.6.3 TDD measurements 1085

8.6.3.1 Correct reporting of TDD neighbours in AWGN propagation condition 1085

8.6.3.1.1 Definition and applicability 1085

8.6.3.1.2 Minimum requirement 1085

8.6.3.1.2.1 3.84Mcps TDD option 1085

8.6.3.1.2.2 1.28Mcps TDD option 1086

8.6.3.1.3 Test purpose 1087

8.6.3.1.4 Method of test 1087

8.6.3.1.4.1 Initial conditions 1087

8.6.3.1.4.1.1 3.84Mcps TDD option 1087

8.6.3.1.4.1.2 1.28Mcps TDD option 1089

8.6.3.1.5 Test requirements 1094

8.6.4 GSM measurements 1094

8.6.4.1 Correct reporting of GSM neighbours in AWGN propagation condition 1094

8.6.4.1.1 Definition and applicability 1094

8.6.4.1.2 Minimum requirements 1095

8.6.4.1.3 Test purpose 1095

8.6.4.1.4 Method of test 1095

8.6.4.1.4.1 Test 1 initial conditions 1095

8.6.4.1.4.2 Test 1 Procedure 1096

8.6.4.1.4.3 Test 2 initial conditions 1100

8.6.4.1.4.4 Test 2 Procedure 1101

8.6.4.1.5 Test requirements 1104

8.6.4.1.5.1 TEST 1 With BSIC verification required 1104

8.6.4.1.5.2 TEST 2 Without BSIC verification required 1104

8.6.5 Combined inter frequency and GSM measurements 1105

8.6.5.1 Correct reporting of neighbours in AWGN propagation condition 1105

8.6.5.1.1 Definition and applicability 1105

8.6.5.1.2 Minimum requirement 1105

8.6.5.1.3 Test purpose 1106

8.6.5.1.4 Method of test 1106

8.6.5.1.5 Test requirements 1118

8.6.6 E-UTRAN Measurement 1118

8.6.6.1 Correct reporting of E-UTRAN FDD neighbour in fading propagation condition in CELL\_DCH 1118

8.6.6.1.1 Definition and applicability 1118

8.6.6.1.2 Minimum requirement 1119

8.6.6.1.3 Test purpose 1119

8.6.6.1.4 Method of test 1119

8.6.6.1.5 Test requirements 1124

8.6.6.2 Correct reporting of E-UTRAN TDD neighbour in fading propagation condition in CELL\_DCH 1126

8.6.6.2.1 Definition and applicability 1126

8.6.6.2.2 Minimum requirement 1127

8.6.6.2.3 Test purpose 1127

8.6.6.2.4 Method of test 1127

8.6.6.2.5 Test requirements 1132

8.6.7 Combined Inter-frequency and E-UTRAN measurements 1133

8.6.7.1 Correct reporting of E-UTRA FDD neighbours in fading propagation condition 1133

8.6.7.1.1 Definition and applicability 1133

8.6.7.1.2 Minimum requirement 1134

8.6.7.1.3 Test purpose 1135

8.6.7.1.4 Method of test 1135

8.6.7.1.5 Test requirements 1141

8.6.7.2 Correct reporting of E-UTRA TDD neighbours in Fading propagation condition 1143

8.6.7.2.1 Definition and applicability 1143

8.6.7.2.2 Minimum requirement 1143

8.6.7.2.3 Test purpose 1144

8.6.7.2.4 Method of test 1144

8.6.7.2.5 Test requirements 1151

8.7 Measurements Performance Requirements 1153

8.7.1 CPICH RSCP 1153

8.7.1.1 Intra frequency measurements accuracy 1153

8.7.1.1.1 Absolute accuracy requirement 1153

8.7.1.1.2 Relative accuracy requirement 1158

8.7.1.2 Inter frequency measurement accuracy 1161

8.7.1.2.1 Relative accuracy requirement 1161

8.7.2 CPICH Ec/Io 1168

8.7.2.1 Intra frequency measurements accuracy 1168

8.7.2.1.1 Absolute accuracy requirement 1168

8.7.2.1.2 Relative accuracy requirement 1173

8.7.2.2 Inter frequency measurement accuracy 1176

8.7.2.2.1 Absolute accuracy requirement 1176

8.7.2.2.2 Relative accuracy requirement 1176

8.7.3 UTRA Carrier RSSI 1182

8.7.3.1 Absolute measurement accuracy requirement 1183

8.7.3.1.1 Definition and applicability 1183

8.7.3.1.2 Minimum Requirements 1183

8.7.3.1.3 Test purpose 1183

8.7.3.1.4 Method of test 1183

8.7.3.1.5 Test requirements 1187

8.7.3.2 Relative measurement accuracy requirement 1188

8.7.3.2.1 Definition and applicability 1188

8.7.3.2.2 Minimum Requirements 1188

8.7.3.2.3 Test purpose 1189

8.7.3.2.4 Method of test 1189

8.7.3.2.5 Test requirements 1193

8.7.3A GSM Carrier RSSI 1194

8.7.3A.1 Definition and applicability 1194

8.7.3A.2 Minimum Requirements 1194

8.7.3A.3 Test purpose 1196

8.7.3A.4 Method of test 1196

8.7.3A.4.1 Initial conditions 1196

8.7.3A.4.2 Procedure 1198

8.7.3A.5 Test requirements 1201

8.7.3B Transport channel BLER 1203

8.7.3C UE transmitted power (R99 and Rel-4 only) 1203

8.7.3C.1 Definition and applicability 1203

8.7.3C.2 Minimum requirements 1204

8.7.3C.3 Test purpose 1204

8.7.3C.4 Method of test 1204

8.7.3C.4.1 Initial conditions 1204

8.7.3C.4.2 Procedure 1205

8.7.3C.5 Test requirements 1207

8.7.3D UE transmitted power (Rel-5 and later) 1207

8.7.3D.1 Definition and applicability 1207

8.7.3D.2 Minimum requirements 1207

8.7.3D.3 Test purpose 1208

8.7.3D.4 Method of test 1208

8.7.3D.4.1 Initial conditions 1208

8.7.3D.4.2 Procedure 1209

8.7.3D.5 Test requirements 1212

8.7.4 SFN-CFN observed time difference 1212

8.7.4.1 Intra frequency measurement requirement 1212

8.7.4.1.1 Definition and applicability 1212

8.7.4.1.2 Minimum requirements 1213

8.7.4.1.3 Test Purpose 1213

8.7.4.1.4 Method of test 1213

8.7.4.1.5 Test requirements 1215

8.7.4.2 Inter frequency measurement requirement 1217

8.7.4.2.1 Definition and applicability 1217

8.7.4.2.2 Minimum requirements 1217

8.7.4.2.3 Test purpose 1217

8.7.4.2.4 Method of test 1217

8.7.4.2.5 Test requirements 1221

8.7.5 SFN-SFN observed time difference 1223

8.7.5.1 SFN-SFN observed time difference type 1 1223

8.7.5.1.1 Definition and applicability 1223

8.7.5.1.2 Minimum requirements 1223

8.7.5.1.3 Test purpose 1223

8.7.5.1.4 Method of test 1224

8.7.5.1.5 Test requirements 1226

8.7.5.2 SFN-SFN observed time difference type 2 without IPDL period active 1228

8.7.5.2.1 Definition and applicability 1228

8.7.5.2.2 Minimum requirements 1228

8.7.5.2.3 Test purpose and Environment 1228

8.7.5.3 SFN-SFN observed time difference type 2 with IPDL period active 1229

8.7.5.3.1 Definition and applicability 1229

8.7.5.3.2 Minimum requirements 1229

8.7.5.3.3 Test purpose and Environment 1230

8.7.6 UE Rx-Tx time difference 1231

8.7.6.1 UE Rx-Tx time difference type 1 (Release 5 and earlier) 1231

8.7.6.1.1 Definition and applicability 1231

8.7.6.1.2 Minimum requirements 1231

8.7.6.1.3 Test purpose 1231

8.7.6.1.4 Method of test 1231

8.7.6.1.5 Test requirements 1233

8.7.6.1A UE Rx-Tx time difference type 1 (Release 6 and later) 1235

8.7.6.1A.1 Definition and applicability 1235

8.7.6.1A.2 Minimum requirements 1235

8.7.6.1A.3 Test purpose 1235

8.7.6.1A.4 Method of test 1235

8.7.6.1A.5 Test requirements 1237

8.7.6.2 UE Rx-Tx time difference type 2 1239

8.7.6.2.1 Definition and applicability 1239

8.7.6.2.2 Minimum requirements 1239

8.7.6.2.3 Test purpose 1239

8.7.7 Observed time difference to GSM cell (R99 and Rel-4 only) 1240

8.7.8 P-CCPCH RSCP 1240

8.7.8.1 Absolute measurement accuracy 1240

8.7.8.1.1 Definition and applicability 1240

8.7.8.1.2 Minimum Requirements 1240

8.7.8.1.3 Test purpose 1241

8.7.8.1.4 Method of test 1241

8.7.8.1.5 Test requirements 1245

8.7.9 UE Transmission Power Headroom 1245

8.7.9.1 Definition and applicability 1245

8.7.9.2 Minimum Requirements 1245

8.7.9.3 Test purpose 1246

8.7.9.4 Method of test 1246

8.7.9.4.1 Initial conditions 1246

8.7.9.4.2 Test procedure 1248

8.7.9.5 Test requirements 1249

8.7.10 E-UTRAN FDD RSRP absolute accuracy (CELL\_DCH) 1249

8.7.10.1 Definition and applicability 1249

8.7.10.2 Minimum Requirements 1249

8.7.10.3 Test purpose 1250

8.7.10.4 Method of test 1250

8.7.10.5 Test requirements 1254

8.7.11 E-UTRAN TDD RSRP absolute accuracy (CELL\_DCH) 1256

8.7.11.1 Definition and applicability 1256

8.7.11.2 Minimum Requirements 1257

8.7.11.3 Test purpose 1257

8.7.11.4 Method of test 1257

8.7.11.5 Test requirements 1261

8.7.12 E-UTRAN FDD RSRQ absolute accuracy (CELL\_DCH) 1263

8.7.12.1 Definition and applicability 1263

8.7.12.2 Minimum Requirements 1263

8.7.12.3 Test purpose 1264

8.7.12.4 Method of test 1264

8.7.12.5 Test requirements 1268

8.7.13 E-UTRAN TDD RSRQ absolute accuracy (CELL\_DCH) 1270

8.7.13.1 Definition and applicability 1270

8.7.13.2 Minimum Requirements 1270

8.7.13.3 Test purpose 1271

8.7.13.4 Method of test 1271

8.7.13.5 Test requirements 1275

9 Performance requirements for HSDPA 1278

9.1 General 1278

9.2 Demodulation of HS-DSCH (Fixed Reference Channel) 1278

9.2.1 Single Link Performance 1288

9.2.1A Single Link Performance - QPSK/16QAM, Fixed Reference Channel (FRC) H-Set 1/2/3 1288

9.2.1A.1 Definition and applicability 1288

9.2.1A.2 Minimum requirements 1288

9.2.1A.3 Test purpose 1289

9.2.1A.4 Method of test 1289

9.2.1A.4.1 Initial conditions 1289

9.2.1A.4.2 Procedure 1290

9.2.1A.5 Test Requirements 1290

9.2.1B Single Link Performance - QPSK, Fixed Reference Channel (FRC) H-Set 4/5 1291

9.2.1B.1 Definition and applicability 1291

9.2.1B.2 Minimum requirements 1291

9.2.1B.3 Test purpose 1292

9.2.1B.4 Method of test 1292

9.2.1B.4.1 Initial conditions 1292

9.2.1B.4.2 Procedure 1293

9.2.1B.5 Test Requirements 1293

9.2.1C Single Link Performance - QPSK/16QAM, Fixed Reference Channel (FRC) H-Set 6/3 1294

9.2.1C.1 Definition and applicability 1294

9.2.1C.2 Minimum requirements 1294

9.2.1C.3 Test purpose 1297

9.2.1C.4 Method of test 1297

9.2.1C.4.1 Initial conditions 1297

9.2.1C.4.2 Procedure 1297

9.2.1C.5 Test Requirements 1297

9.2.1D Single Link Performance - Enhanced Performance Requirements Type 1 - QPSK/16QAM, Fixed Reference Channel (FRC) H-Set 1/2/3 1299

9.2.1D.1 Definition and applicability 1299

9.2.1D.2 Minimum requirements 1299

9.2.1D.3 Test purpose 1301

9.2.1D.4 Method of test 1301

9.2.1D.4.1 Initial conditions 1301

9.2.1D.4.2 Procedure 1301

9.2.1D.5 Test Requirements 1301

9.2.1E Single Link Performance - Enhanced Performance Requirements Type 1- QPSK/16QAM, Fixed Reference Channel (FRC) H-Set 6/3 1303

9.2.1E.1 Definition and applicability 1303

9.2.1E.2 Minimum requirements 1303

9.2.1E.3 Test purpose 1305

9.2.1E.4 Method of test 1305

9.2.1E.4.1 Initial conditions 1305

9.2.1E.4.2 Procedure 1305

9.2.1E.5 Test Requirements 1306

9.2.1F Single Link Performance - Enhanced Performance Requirements Type 2 - QPSK/16QAM, Fixed Reference Channel (FRC) H-Set 6/3 1307

9.2.1F.1 Definition and applicability 1307

9.2.1F.2 Minimum requirements 1308

9.2.1F.3 Test purpose 1309

9.2.1F.4 Method of test 1310

9.2.1F.4.1 Initial conditions 1310

9.2.1F.4.2 Procedure 1310

9.2.1F.5 Test Requirements 1310

9.2.1FA Single Link Performance - Enhanced Performance Requirements Type 2 - QPSK/16QAM, Fixed Reference Channel (FRC) H-Set 6A/3A 1312

9.2.1FA.1 Definition and applicability 1312

9.2.1FA.2 Minimum requirements 1312

9.2.1FA.3 Test purpose 1314

9.2.1FA.4 Method of test 1314

9.2.1FA.4.1 Initial conditions 1314

9.2.1FA.4.2 Procedure 1315

9.2.1FA.5 Test Requirements 1315

9.2.1FB Single Link Performance - Enhanced Performance Requirements Type 2 - QPSK/16QAM, Fixed Reference Channel (FRC) H-Set 6A/3A for DB-DC-HSDPA 1317

9.2.1FB.1 Definition and applicability 1317

9.2.1FB.2 Minimum requirements 1317

9.2.1FB.3 Test purpose 1319

9.2.1FB.4 Method of test 1319

9.2.1FB.4.1 Initial conditions 1319

9.2.1FB.4.2 Procedure 1320

9.2.1FB.5 Test Requirements 1320

9.2.1FC Single Link Performance - Enhanced Performance Requirements Type 2 - QPSK/16QAM, Fixed Reference Channel (FRC) H-Set 6B/3B 1321

9.2.1FC.1 Definition and applicability 1321

9.2.1FC.2 Minimum requirements 1322

9.2.1FC.3 Test purpose 1323

9.2.1FC.4 Method of test 1324

9.2.1FC.4.1 Initial conditions 1324

9.2.1FC.4.2 Procedure 1324

9.2.1FC.5 Test Requirements 1324

9.2.1FD Single Link Performance - Enhanced Performance Requirements Type 2 - QPSK/16QAM, Fixed Reference Channel (FRC) H-Set 6C/3C 1326

9.2.1FD.1 Definition and applicability 1326

9.2.1FD.2 Minimum requirements 1326

9.2.1FD.3 Test purpose 1328

9.2.1FD.4 Method of test 1328

9.2.1FD.4.1 Initial conditions 1328

9.2.1FD.4.2 Procedure 1329

9.2.1FD.5 Test Requirements 1329

9.2.1G Single Link Performance - Enhanced Performance Requirements Type 3 - QPSK/16QAM, Fixed Reference Channel (FRC) H-Set 6/3 1331

9.2.1G.1 Definition and applicability 1331

9.2.1G.2 Minimum requirements 1331

9.2.1G.3 Test purpose 1333

9.2.1G.4 Method of test 1333

9.2.1G.4.1 Initial conditions 1333

9.2.1G.4.2 Procedure 1334

9.2.1G.5 Test Requirements 1334

9.2.1GA Single Link Performance - Enhanced Performance Requirements Type 3 - QPSK/16QAM, Fixed Reference Channel (FRC) H-Set 6A/3A 1336

9.2.1GA.1 Definition and applicability 1336

9.2.1GA.2 Minimum requirements 1336

9.2.1GA.3 Test purpose 1339

9.2.1GA.4 Method of test 1339

9.2.1GA.4.1 Initial conditions 1339

9.2.1GA.4.2 Procedure 1340

9.2.1GA.5 Test Requirements 1340

9.2.1GB Single Link Performance - Enhanced Performance Requirements Type 3 - QPSK/16QAM, Fixed Reference Channel (FRC) H-Set 6A/3A for DB-DC-HSDPA 1342

9.2.1GB.1 Definition and applicability 1342

9.2.1GB.2 Minimum requirements 1342

9.2.1GB.3 Test purpose 1345

9.2.1GB.4 Method of test 1345

9.2.1GB.4.1 Initial conditions 1345

9.2.1GB.4.2 Procedure 1346

9.2.1GB.5 Test Requirements 1346

9.2.1GC Single Link Performance - Enhanced Performance Requirements Type 3 - QPSK/16QAM, Fixed Reference Channel (FRC) H-Set 6B/3B 1348

9.2.1GC.1 Definition and applicability 1348

9.2.1GC.2 Minimum requirements 1348

9.2.1GC.3 Test purpose 1351

9.2.1GC.4 Method of test 1351

9.2.1GC.4.1 Initial conditions 1351

9.2.1GC.4.2 Procedure 1352

9.2.1GC.5 Test Requirements 1352

9.2.1GD Single Link Performance - Enhanced Performance Requirements Type 3 - QPSK/16QAM, Fixed Reference Channel (FRC) H-Set 6C/3C 1354

9.2.1GD.1 Definition and applicability 1354

9.2.1GD.2 Minimum requirements 1354

9.2.1GD.3 Test purpose 1357

9.2.1GD.4 Method of test 1357

9.2.1GD.4.1 Initial conditions 1357

9.2.1GD.4.2 Procedure 1358

9.2.1GD.5 Test Requirements 1358

9.2.1H Single Link Performance - Enhanced Performance Requirements Type 2 - 64QAM, Fixed Reference Channel (FRC) H-Set 8 1360

9.2.1H.1 Definition and applicability 1360

9.2.1H.2 Minimum requirements 1360

9.2.1H.3 Test purpose 1361

9.2.1H.4 Method of test 1361

9.2.1H.4.1 Initial conditions 1361

9.2.1H.4.2 Procedure 1363

9.2.1H.5 Test Requirements 1363

9.2.1HA Single Link Performance - Enhanced Performance Requirements Type 2 - 64QAM, Fixed Reference Channel (FRC) H-Set 8 A 1363

9.2.1HA.1 Definition and applicability 1363

9.2.1HA.2 Minimum requirements 1363

9.2.1HA.3 Test purpose 1364

9.2.1HA.4 Method of test 1364

9.2.1HA.4.1 Initial conditions 1364

9.2.1HA.4.2 Procedure 1365

9.2.1HA.5 Test Requirements 1365

9.2.1HB Single Link Performance - Enhanced Performance Requirements Type 2 - 64QAM, Fixed Reference Channel (FRC) H-Set 8 A for DB-DC-HSDPA 1366

9.2.1HB.1 Definition and applicability 1366

9.2.1HB.2 Minimum requirements 1366

9.2.1HB.3 Test purpose 1367

9.2.1HB.4 Method of test 1367

9.2.1HB.4.1 Initial conditions 1367

9.2.1HB.4.2 Procedure 1368

9.2.1HB.5 Test Requirements 1368

9.2.1HC Single Link Performance - Enhanced Performance Requirements Type 2 - 64QAM, Fixed Reference Channel (FRC) H-Set 8B 1369

9.2.1HC.1 Definition and applicability 1369

9.2.1HC.2 Minimum requirements 1369

9.2.1HC.3 Test purpose 1370

9.2.1HC.4 Method of test 1370

9.2.1HC.4.1 Initial conditions 1370

9.2.1HC.4.2 Procedure 1371

9.2.1HC.5 Test Requirements 1371

9.2.1HD Single Link Performance - Enhanced Performance Requirements Type 2 - 64QAM, Fixed Reference Channel (FRC) H-Set 8C 1372

9.2.1HD.1 Definition and applicability 1372

9.2.1HD.2 Minimum requirements 1372

9.2.1HD.3 Test purpose 1373

9.2.1HD.4 Method of test 1373

9.2.1HD.4.1 Initial conditions 1373

9.2.1HD.4.2 Procedure 1374

9.2.1HD.5 Test Requirements 1374

9.2.1I Single Link Performance - Enhanced Performance Requirements Type 3 - 64QAM, Fixed Reference Channel (FRC) H-Set 8 1375

9.2.1I.1 Definition and applicability 1375

9.2.1I.2 Minimum requirements 1375

9.2.1I.3 Test purpose 1376

9.2.1I.4 Method of test 1376

9.2.1I.4.1 Initial conditions 1376

9.2.1I.4.2 Procedure 1377

9.2.1I.5 Test Requirements 1378

9.2.1IA Single Link Performance - Enhanced Performance Requirements Type 3 - 64QAM, Fixed Reference Channel (FRC) H-Set 8A 1378

9.2.1IA.1 Definition and applicability 1378

9.2.1IA.2 Minimum requirements 1378

9.2.1IA.3 Test purpose 1379

9.2.1IA.4 Method of test 1379

9.2.1IA.4.1 Initial conditions 1379

9.2.1IA.4.2 Procedure 1380

9.2.1IA.5 Test Requirements 1380

9.2.1IB Single Link Performance - Enhanced Performance Requirements Type 3 - 64QAM, Fixed Reference Channel (FRC) H-Set 8A for DB-DC-HSDPA 1381

9.2.1IB.1 Definition and applicability 1381

9.2.1IB.2 Minimum requirements 1381

9.2.1IB.3 Test purpose 1382

9.2.1IB.4 Method of test 1382

9.2.1IB.4.1 Initial conditions 1382

9.2.1IB.4.2 Procedure 1383

9.2.1IB.5 Test Requirements 1383

9.2.1IC Single Link Performance - Enhanced Performance Requirements Type 3 - 64QAM, Fixed Reference Channel (FRC) H-Set 8B 1384

9.2.1IC.1 Definition and applicability 1384

9.2.1IC.2 Minimum requirements 1384

9.2.1IC.3 Test purpose 1385

9.2.1IC.4 Method of test 1385

9.2.1IC.4.1 Initial conditions 1385

9.2.1IC.4.2 Procedure 1386

9.2.1IC.5 Test Requirements 1386

9.2.1ID Single Link Performance - Enhanced Performance Requirements Type 3 - 64QAM, Fixed Reference Channel (FRC) H-Set 8C 1387

9.2.1ID.1 Definition and applicability 1387

9.2.1ID.2 Minimum requirements 1387

9.2.1ID.3 Test purpose 1388

9.2.1ID.4 Method of test 1388

9.2.1ID.4.1 Initial conditions 1388

9.2.1ID.4.2 Procedure 1389

9.2.1ID.5 Test Requirements 1389

9.2.1J Single Link Performance - Enhanced Performance Requirements Type 2 - QPSK/16QAM, Fixed Reference Channel (FRC) H-Set 10 1390

9.2.1J.1 Definition and applicability 1390

9.2.1J.2 Minimum requirements 1390

9.2.1J.3 Test purpose 1391

9.2.1J.4 Method of test 1391

9.2.1J.4.1 Initial conditions 1391

9.2.1J.4.2 Procedure 1392

9.2.1J.5 Test Requirements 1393

9.2.1JA Single Link Performance - Enhanced Performance Requirements Type 2 - QPSK/16QAM, Fixed Reference Channel (FRC) H-Set 10A 1393

9.2.1JA.1 Definition and applicability 1393

9.2.1JA.2 Minimum requirements 1393

9.2.1JA.3 Test purpose 1395

9.2.1JA.4 Method of test 1395

9.2.1JA.4.1 Initial conditions 1395

9.2.1JA.4.2 Procedure 1396

9.2.1JA.5 Test Requirements 1396

9.2.1JB Single Link Performance - Enhanced Performance Requirements Type 2 - QPSK/16QAM, Fixed Reference Channel (FRC) H-Set 10A DB-DC-HSDPA 1397

9.2.1JB.1 Definition and applicability 1397

9.2.1JB.2 Minimum requirements 1397

9.2.1JB.3 Test purpose 1398

9.2.1JB.4 Method of test 1398

9.2.1JB.4.1 Initial conditions 1398

9.2.1JB.4.2 Procedure 1399

9.2.1JB.5 Test Requirements 1399

9.2.1JC Single Link Performance - Enhanced Performance Requirements Type 2 - QPSK/16QAM, Fixed Reference Channel (FRC) H-Set 10B 1400

9.2.1JC.1 Definition and applicability 1400

9.2.1JC.2 Minimum requirements 1400

9.2.1JC.3 Test purpose 1402

9.2.1JC.4 Method of test 1402

9.2.1JC.4.1 Initial conditions 1402

9.2.1JC.4.2 Procedure 1403

9.2.1JC.5 Test Requirements 1403

9.2.1JD Single Link Performance - Enhanced Performance Requirements Type 2 - QPSK/16QAM, Fixed Reference Channel (FRC) H-Set 10C 1404

9.2.1JD.1 Definition and applicability 1404

9.2.1JD.2 Minimum requirements 1404

9.2.1JD.3 Test purpose 1405

9.2.1JD.4 Method of test 1405

9.2.1JD.4.1 Initial conditions 1405

9.2.1JD.4.2 Procedure 1406

9.2.1JD.5 Test Requirements 1406

9.2.1K Single Link Performance - Enhanced Performance Requirements Type 3 - QPSK/16QAM, Fixed Reference Channel (FRC) H-Set 10 1407

9.2.1K.1 Definition and applicability 1407

9.2.1K.2 Minimum requirements 1407

9.2.1K.3 Test purpose 1409

9.2.1K.4 Method of test 1409

9.2.1K.4.1 Initial conditions 1409

9.2.1K.4.2 Procedure 1410

9.2.1K.5 Test Requirements 1410

9.2.1KA Single Link Performance - Enhanced Performance Requirements Type 3 - QPSK/16QAM, Fixed Reference Channel (FRC) H-Set 10A 1411

9.2.1KA.1 Definition and applicability 1411

9.2.1KA.2 Minimum requirements 1411

9.2.1KA.3 Test purpose 1412

9.2.1KA.4 Method of test 1412

9.2.1KA.4.1 Initial conditions 1412

9.2.1KA.4.2 Procedure 1413

9.2.1KA.5 Test Requirements 1413

9.2.1KB Single Link Performance - Enhanced Performance Requirements Type 3 - QPSK/16QAM, Fixed Reference Channel (FRC) H-Set 10A for DB-DC-HSDPA 1414

9.2.1KB.1 Definition and applicability 1414

9.2.1KB.2 Minimum requirements 1414

9.2.1KB.3 Test purpose 1415

9.2.1KB.4 Method of test 1416

9.2.1KB.4.1 Initial conditions 1416

9.2.1KB.4.2 Procedure 1417

9.2.1KB.5 Test Requirements 1417

9.2.1KC Single Link Performance - Enhanced Performance Requirements Type 3 - QPSK/16QAM, Fixed Reference Channel (FRC) H-Set 10B 1418

9.2.1KC.1 Definition and applicability 1418

9.2.1KC.2 Minimum requirements 1418

9.2.1KC.3 Test purpose 1419

9.2.1KC.4 Method of test 1419

9.2.1KC.4.1 Initial conditions 1419

9.2.1KC.4.2 Procedure 1420

9.2.1KC.5 Test Requirements 1420

9.2.1KD Single Link Performance - Enhanced Performance Requirements Type 3 - QPSK/16QAM, Fixed Reference Channel (FRC) H-Set 10C 1421

9.2.1KD.1 Definition and applicability 1421

9.2.1KD.2 Minimum requirements 1421

9.2.1KD.3 Test purpose 1422

9.2.1KD.4 Method of test 1423

9.2.1KD.4.1 Initial conditions 1423

9.2.1KD.4.2 Procedure 1423

9.2.1KD.5 Test Requirements 1424

9.2.1L Single Link Performance - Enhanced Performance Requirements Type 3i - QPSK, Fixed Reference Channel (FRC) H-Set 6 1424

9.2.1L.1 Definition and applicability 1424

9.2.1L.2 Minimum requirements 1425

9.2.1L.3 Test purpose 1425

9.2.1L.4 Method of test 1425

9.2.1L.5 Test Requirements 1427

9.2.1LA Enhanced Performance Requirements Type 3i - QPSK, Fixed Reference Channel (FRC) H-Set 6A 1428

9.2.1LA.1 Definition and applicability 1428

9.2.1LA.2 Minimum requirements 1428

9.2.1LA.3 Test purpose 1429

9.2.1LA.4 Method of test 1429

9.2.1LA.5 Test Requirements 1430

9.2.1LB Enhanced Performance Requirements Type 3i - QPSK, Fixed Reference Channel (FRC) H-Set 6A for DB-DC-HSDPA 1431

9.2.1LB.1 Definition and applicability 1431

9.2.1LB.2 Minimum requirements 1431

9.2.1LB.3 Test purpose 1432

9.2.1LB.4 Method of test 1432

9.2.1LB.5 Test Requirements 1433

9.2.1LC Enhanced Performance Requirements Type 3i - QPSK, Fixed Reference Channel (FRC) H-Set 6B 1434

9.2.1LC.1 Definition and applicability 1434

9.2.1LC.2 Minimum requirements 1434

9.2.1LC.3 Test purpose 1435

9.2.1LC.4 Method of test 1435

9.2.1LC.5 Test Requirements 1436

9.2.1LD Enhanced Performance Requirements Type 3i - QPSK, Fixed Reference Channel (FRC) H-Set 6C 1437

9.2.1LD.1 Definition and applicability 1437

9.2.1LD.2 Minimum requirements 1437

9.2.1LD.3 Test purpose 1438

9.2.1LD.4 Method of test 1438

9.2.1LD.5 Test Requirements 1439

9.2.1M Single Link Performance - Enhanced Performance Requirements Type 3i – 16QAM/QPSK, Fixed Reference Channel (FRC) H-Set 6 for Multiflow HSDPA (2 cells) 1440

9.2.1M.1 Definition and applicability 1440

9.2.1M.2 Minimum requirements 1440

9.2.1M.3 Test purpose 1441

9.2.1M.4 Method of test 1441

9.2.1M.4.1 Initial conditions 1441

9.2.1M.4.2 Procedure 1442

9.2.1M.5 Test Requirements 1442

9.2.1MA Single Link Performance - Enhanced Performance Requirements Type 3i – 16QAM/QPSK, Fixed Reference Channel (FRC) H-Set 6 for Multiflow HSDPA (3 cells) 1443

9.2.1MA.1 Definition and applicability 1443

9.2.1MA.2 Minimum requirements 1443

9.2.1MA.3 Test purpose 1444

9.2.1MA.4 Method of test 1444

9.2.1MA.4.1 Initial conditions 1444

9.2.1MA.4.2 Procedure 1445

9.2.1MA.5 Test Requirements 1445

9.2.2 Open Loop Diversity Performance 1446

9.2.2A Open Loop Diversity Performance - QPSK/16QAM, Fixed Reference Channel (FRC) H-Set 1/2/3 1446

9.2.2A.1 Definition and applicability 1446

9.2.2A.2 Minimum requirements 1446

9.2.2A.3 Test purpose 1448

9.2.2A.4 Method of test 1448

9.2.2B Open Loop Diversity Performance - QPSK, Fixed Reference Channel (FRC) H-Set 4/5 1451

9.2.2B.1 Definition and applicability 1451

9.2.2B.2 Minimum requirements 1451

9.2.2B.3 Test purpose 1452

9.2.2B.4 Method of test 1452

9.2.2C Open Loop Diversity Performance - Enhanced Performance Requirements Type 1 - QPSK/16QAM, Fixed Reference Channel (FRC) H-Set 1/2/3 1454

9.2.2C.1 Definition and applicability 1454

9.2.2C.2 Minimum requirements 1455

9.2.2C.3 Test purpose 1456

9.2.2C.4 Method of test 1456

9.2.2D Open Loop Diversity Performance - Enhanced Performance Requirements Type 2 - QPSK/16QAM, Fixed Reference Channel (FRC) H-Set 3 1459

9.2.2D.1 Definition and applicability 1459

9.2.2D.2 Minimum requirements 1459

9.2.2D.3 Test purpose 1461

9.2.2D.4 Method of test 1461

9.2.2D.4.1 Initial conditions 1461

9.2.2D.4.2 Procedure 1462

9.2.2D.5 Test Requirements 1463

9.2.2E Open Loop Diversity Performance - Enhanced Performance Requirements Type 3 - QPSK/16QAM, Fixed Reference Channel (FRC) H-Set 3 1464

9.2.2E.1 Definition and applicability 1464

9.2.2E.2 Minimum requirements 1464

9.2.2E.3 Test purpose 1466

9.2.2E.4 Method of test 1466

9.2.2E.4.1 Initial conditions 1466

9.2.2E.4.2 Procedure 1467

9.2.2E.5 Test Requirements 1467

9.2.3 Closed Loop Diversity Performance 1468

9.2.3A Closed Loop Diversity Performance - QPSK/16QAM, Fixed Reference Channel (FRC) H-Set 1/2/3 1468

9.2.3A.1 Definition and applicability 1468

9.2.3A.2 Minimum requirements 1469

9.2.3A.3 Test purpose 1470

9.2.3A.4 Method of test 1470

9.2.3A.4.1 Initial conditions 1470

9.2.3A.4.2 Procedure 1471

9.2.3A.5 Test Requirements 1472

9.2.3B Closed Loop Diversity Performance - QPSK, Fixed Reference Channel (FRC) H-Set 4/5 1473

9.2.3B.1 Definition and applicability 1473

9.2.3B.2 Minimum requirements 1473

9.2.3B.3 Test purpose 1474

9.2.3B.4 Method of test 1474

9.2.3B.4.1 Initial conditions 1474

9.2.3B.4.2 Procedure 1476

9.2.3B.5 Test Requirements 1476

9.2.3C Closed Loop Diversity Performance Enhanced Performance Requirements Type 1, QPSK/16QAM, Fixed Reference Channel (FRC) H-Set 1/2/3 1477

9.2.3C.1 Definition and applicability 1477

9.2.3C.2 Minimum requirements 1477

9.2.3C.3 Test purpose 1479

9.2.3C.4 Method of test 1479

9.2.3C.4.1 Initial conditions 1479

9.2.3C.4.2 Procedure 1480

9.2.3C.5 Test Requirements 1480

9.2.3D Closed Loop Diversity Performance - Enhanced Performance Requirements Type 2 - QPSK/16QAM, Fixed Reference Channel (FRC) H-Set 6/3 1482

9.2.3D.1 Definition and applicability 1482

9.2.3D.2 Minimum requirements 1482

9.2.3D.3 Test purpose 1485

9.2.3D.4 Method of test 1485

9.2.3D.4.1 Initial conditions 1485

9.2.3D.4.2 Procedure 1486

9.2.3D.5 Test Requirements 1486

9.2.3E Closed Loop Diversity Performance Enhanced Performance Requirements Type 3, QPSK/16QAM, Fixed Reference Channel (FRC) H-Set 3 1488

9.2.3E.1 Definition and applicability 1488

9.2.3E.2 Minimum requirements 1488

9.2.3E.3 Test purpose 1490

9.2.3E.4 Method of test 1490

9.2.3E.4.1 Initial conditions 1490

9.2.3E.4.2 Procedure 1491

9.2.3E.5 Test Requirements 1492

9.2.4 MIMO Performance 1493

9.2.4A MIMO Performance - Fixed Reference Channel (FRC) H-Set 9 1493

9.2.4A.1 Definition and applicability 1493

9.2.4A.2 Minimum requirements 1493

9.2.4A.3 Test purpose 1494

9.2.4A.4 Method of test 1494

9.2.4A.4.1 Initial conditions 1494

9.2.4A.4.2 Procedure 1495

9.2.4A.5 Test Requirements 1496

9.2.4B MIMO Performance - Fixed Reference Channel (FRC) H-Set 11 1496

9.2.4B.1 Definition and applicability 1496

9.2.4B.2 Minimum requirements 1496

9.2.4B.3 Test purpose 1497

9.2.4B.4 Method of test 1497

9.2.4B.4.1 Initial conditions 1497

9.2.4B.4.2 Procedure 1498

9.2.4B.5 Test Requirements 1498

9.2.4C MIMO Performance - Fixed Reference Channel (FRC) H-Set 9A 1499

9.2.4C.1 Definition and applicability 1499

9.2.4C.2 Minimum requirements 1499

9.2.4C.3 Test purpose 1500

9.2.4C.4 Method of test 1500

9.2.4C.4.1 Initial conditions 1500

9.2.4C.4.2 Procedure 1502

9.2.4C.5 Test Requirements 1502

9.2.4CA MIMO Performance - Fixed Reference Channel (FRC) H-Set 9A for DB DC-HSDPA 1503

9.2.4CA.1 Definition and applicability 1503

9.2.4CA.2 Minimum requirements 1503

9.2.4CA.3 Test purpose 1504

9.2.4CA.4 Method of test 1504

9.2.4CA.4.1 Initial conditions 1504

9.2.4CA.4.2 Procedure 1505

9.2.4CA.5 Test Requirements 1505

9.2.4D MIMO Performance - Fixed Reference Channel (FRC) H-Set 11A 1506

9.2.4D.1 Definition and applicability 1506

9.2.4D.2 Minimum requirements 1506

9.2.4D.3 Test purpose 1507

9.2.4D.4 Method of test 1507

9.2.4D.4.1 Initial conditions 1507

9.2.4D.4.2 Procedure 1508

9.2.4D.5 Test Requirements 1508

9.2.4DA MIMO Performance - Fixed Reference Channel (FRC) H-Set 11A for DB DC-HSDPA 1509

9.2.4DA.1 Definition and applicability 1509

9.2.4DA.2 Minimum requirements 1509

9.2.4DA.3 Test purpose 1510

9.2.4DA.4 Method of test 1510

9.2.4DA.4.1 Initial conditions 1510

9.2.4DA.4.2 Procedure 1511

9.2.4DA.5 Test Requirements 1511

9.2.4E MIMO Performance - Fixed Reference Channel (FRC) H-Set 9 Asymmetric CPICHs 1512

9.2.4E.1 Definition and applicability 1512

9.2.4E.2 Minimum requirements 1512

9.2.4E.3 Test purpose 1513

9.2.4E.4 Method of test 1513

9.2.4E.4.1 Initial conditions 1513

9.2.4E.4.2 Procedure 1514

9.2.4E.5 Test Requirements 1515

9.2.4F MIMO Performance - Fixed Reference Channel (FRC) H-Set 11 Asymmetric CPICHs 1515

9.2.4F.1 Definition and applicability 1515

9.2.4F.2 Minimum requirements 1515

9.2.4F.3 Test purpose 1516

9.2.4F.4 Method of test 1516

9.2.4F.4.1 Initial conditions 1516

9.2.4F.4.2 Procedure 1517

9.2.4F.5 Test Requirements 1517

9.2.4G MIMO Performance - Fixed Reference Channel (FRC) H-Set 9A Asymmetric CPICHs 1518

9.2.4G.1 Definition and applicability 1518

9.2.4G.2 Minimum requirements 1518

9.2.4G.3 Test purpose 1519

9.2.4G.4 Method of test 1519

9.2.4G.4.1 Initial conditions 1519

9.2.4G.4.2 Procedure 1521

9.2.4G.5 Test Requirements 1521

9.2.4H MIMO Performance - Fixed Reference Channel (FRC) H-Set 11A Asymmetric CPICHs 1522

9.2.4H.1 Definition and applicability 1522

9.2.4H.2 Minimum requirements 1522

9.2.4H.3 Test purpose 1523

9.2.4H.4 Method of test 1523

9.2.4H.4.1 Initial conditions 1523

9.2.4H.4.2 Procedure 1524

9.2.4H.5 Test Requirements 1524

9.3 Reporting of Channel Quality Indicator 1525

9.3.1 Single Link Performance - AWGN Propagation Conditions 1525

9.3.1.1 Definition and applicability 1525

9.3.1.2 Minimum requirements 1526

9.3.1.3 Test purpose 1526

9.3.1.4 Method of test 1527

9.3.1.4.1 Initial conditions 1527

9.3.1.4.2 Procedure 1527

9.3.1.5 Test Requirements 1528

9.3.1A Single Link Performance - AWGN Propagation Conditions, 64QAM 1528

9.3.1A.1 Definition and applicability 1528

9.3.1A.2 Minimum requirements 1528

9.3.1A.3 Test purpose 1529

9.3.1A.4 Method of test 1529

9.3.1A.4.1 Initial conditions 1529

9.3.1A.4.2 Procedure 1530

9.3.1A.5 Test Requirements 1532

9.3.1B Single Link Performance - AWGN Propagation Conditions, DC-HSDPA requirements 1532

9.3.1B.1 Definition and applicability 1532

9.3.1B.2 Minimum requirements 1533

9.3.1B.3 Test purpose 1533

9.3.1B.4 Method of test 1534

9.3.1B.4.1 Initial conditions 1534

9.3.1B.4.2 Procedure 1534

9.3.1B.5 Test Requirements 1536

9.3.1BA Single Link Performance - AWGN Propagation Conditions, DB-DC-HSDPA requirements 1536

9.3.1BA.1 Definition and applicability 1536

9.3.1BA.2 Minimum requirements 1536

9.3.1BA.4 Method of test 1537

9.3.1BA.4.1 Initial conditions 1537

9.3.1BA.4.2 Procedure 1538

9.3.1BA.5 Test Requirements 1539

9.3.1BB Single Link Performance - AWGN Propagation Conditions, 4C-HSDPA requirements (3 Carriers) 1540

9.3.1BB.1 Definition and applicability 1540

9.3.1BB.2 Minimum requirements 1540

9.3.1BB.4 Method of test 1541

9.3.1BB.4.1 Initial conditions 1541

9.3.1BB.4.2 Procedure 1541

9.3.1BB.5 Test Requirements 1542

9.3.1BC Single Link Performance - AWGN Propagation Conditions, 4C-HSDPA requirements 1542

9.3.1BC.1 Definition and applicability 1542

9.3.1BC.2 Minimum requirements 1543

9.3.1BC.4 Method of test 1543

9.3.1BC.4.1 Initial conditions 1543

9.3.1BC.4.2 Procedure 1544

9.3.1BC.5 Test Requirements 1545

9.3.2AB Single Link Performance - Fading Propagation Conditions, 4C-HSDPA requirements(3 Carriers) 1545

9.3.2AB.1 Definition and applicability 1545

9.3.2AB.2 Minimum requirements 1545

9.3.2AB.3 Test purpose 1546

9.3.2AB.4 Method of test 1546

9.3.2AB.4.1 Initial conditions 1546

9.3.2AB.4.2 Procedure 1547

9.3.2AB.5 Test Requirements 1548

9.3.2AC Single Link Performance - Fading Propagation Conditions, 4C-HSDPA requirements 1548

9.3.2AC.1 Definition and applicability 1548

9.3.2AC.2 Minimum requirements 1548

9.3.2AC.3 Test purpose 1549

9.3.2AC.4 Method of test 1549

9.3.2AC.4.1 Initial conditions 1549

9.3.2AC.4.2 Procedure 1550

9.3.2AC.5 Test Requirements 1551

9.3.1C Single Link Performance - AWGN Propagation Conditions, Periodically Varying Radio Conditions 1551

9.3.1C.1 Definition and applicability 1551

9.3.1C.2 Minimum requirements 1551

9.3.1C.3 Test purpose 1553

9.3.1C.4 Method of test 1554

9.3.1C.4.1 Initial conditions 1554

9.3.1C.4.2 Procedure 1554

9.3.1C.5 Test Requirements 1555

9.3.2 Single Link Performance - Fading Propagation Conditions 1555

9.3.2.1 Definition and applicability 1555

9.3.2.2 Minimum requirements 1555

9.3.2.3 Test purpose 1556

9.3.2.4 Method of test 1556

9.3.2.4.1 Initial conditions 1556

9.3.2.4.2 Procedure 1557

9.3.2.5 Test Requirements 1558

9.3.2A Single Link Performance - Fading Propagation Conditions, DC-HSDPA requirements 1558

9.3.2A.1 Definition and applicability 1558

9.3.2A.2 Minimum requirements 1558

9.3.2A.3 Test purpose 1559

9.3.2A.4 Method of test 1559

9.3.2A.4.1 Initial conditions 1559

9.3.2A.4.2 Procedure 1560

9.3.2A.5 Test Requirements 1562

9.3.2AA Single Link Performance - Fading Propagation Conditions, DB-DC-HSDPA requirements 1562

9.3.2AA.1 Definition and applicability 1562

9.3.2AA.2 Minimum requirements 1562

9.3.2AA.3 Test purpose 1563

9.3.2AA.4 Method of test 1563

9.3.2AA.4.1 Initial conditions 1563

9.3.2AA.4.2 Procedure 1564

9.3.2AA.5 Test Requirements 1566

9.3.2B Single Link Performance - Fading Propagation Conditions, 64QAM 1566

9.3.2B.1 Definition and applicability 1566

9.3.2B.2 Minimum requirements 1566

9.3.2B.3 Test purpose 1567

9.3.2B.4 Method of test 1567

9.3.2B.4.1 Initial conditions 1567

9.3.2B.4.2 Procedure 1568

9.3.2B.5 Test Requirements 1570

9.3.2C Single Link Performance - Fading Propagation Conditions, Multiflow HSDPA requirements (2 Cells) 1570

9.3.2C.1 Definition and applicability 1571

9.3.2C.2 Minimum requirements 1571

9.3.2C.3 Test purpose 1572

9.3.2C.4 Method of test 1572

9.3.2C.4.1 Initial conditions 1572

9.3.2C.4.2 Procedure 1572

9.3.2C.5 Test Requirements 1574

9.3.2CA Single Link Performance - Fading Propagation Conditions, Multiflow HSDPA requirements (3 Cells) 1574

9.3.2CA.1 Definition and applicability 1574

9.3.2CA.2 Minimum requirements 1574

9.3.2CA.3 Test purpose 1576

9.3.2CA.4 Method of test 1576

9.3.2CA.4.1 Initial conditions 1576

9.3.2CA.4.2 Procedure 1576

9.3.2CA.5 Test Requirements 1578

9.3.3 Open Loop Diversity Performance - AWGN Propagation Conditions 1578

9.3.3.1 Definition and applicability 1578

9.3.3.2 Minimum requirements 1578

9.3.3.3 Test purpose 1579

9.3.3.4 Method of test 1579

9.3.3.4.1 Initial conditions 1579

9.3.3.4.2 Procedure 1579

9.3.3.5 Test Requirements 1582

9.3.4 Open Loop Diversity Performance - Fading Propagation Conditions 1582

9.3.4.1 Definition and applicability 1582

9.3.4.2 Minimum requirements 1582

9.3.4.3 Test purpose 1583

9.3.4.4 Method of test 1583

9.3.4.4.1 Initial conditions 1583

9.3.4.4.2 Procedure 1584

9.3.4.5 Test Requirements 1586

9.3.5 Closed Loop Diversity Performance - AWGN Propagation Conditions 1586

9.3.5.1 Definition and applicability 1586

9.3.5.2 Minimum requirements 1586

9.3.5.3 Test purpose 1587

9.3.5.4 Method of test 1587

9.3.5.4.1 Initial conditions 1587

9.3.5.4.2 Procedure 1588

9.3.5.5 Test Requirements 1590

9.3.6 Closed Loop Diversity Performance - Fading Propagation Conditions 1590

9.3.6.1 Definition and applicability 1590

9.3.6.2 Minimum requirements 1590

9.3.6.3 Test purpose 1591

9.3.6.4 Method of test 1591

9.3.6.4.1 Initial conditions 1591

9.3.6.4.2 Procedure 1592

9.3.6.5 Test Requirements 1594

9.3.7 MIMO Performance - Reporting of Channel Quality Indicator 1594

9.3.7A MIMO Single Stream Fading Conditions 1594

9.3.7A.1 Definition and applicability 1594

9.3.7A.2 Minimum requirements 1595

9.3.7A.3 Test purpose 1596

9.3.7A.4 Method of test 1596

9.3.7A.4.1 Initial conditions 1596

9.3.7A.4.2 Procedure 1596

9.3.7A.5 Test Requirements 1597

9.3.7B MIMO Dual Stream Fading Conditions 1597

9.3.7B.1 Definition and applicability 1597

9.3.7B.2 Minimum requirements 1598

9.3.7B.3 Test purpose 1599

9.3.7B.4 Method of test 1599

9.3.7B.4.1 Initial conditions 1599

9.3.7B.4.2 Procedure 1600

9.3.7B.5 Test Requirements 1601

9.3.7C MIMO Dual Stream Fading Conditions - UE categories 19-20 1601

9.3.7C.1 Definition and applicability 1601

9.3.7C.2 Minimum requirements 1602

9.3.7C.3 Test purpose 1603

9.3.7C.4 Method of test 1604

9.3.7C.4.1 Initial conditions 1604

9.3.7C.4.2 Procedure 1604

9.3.7C.5 Test Requirements 1605

9.3.7D MIMO Dual Stream Static Orthogonal Conditions - UE categories 15-20 1605

9.3.7D.1 Definition and applicability 1605

9.3.7D.2 Minimum requirements 1606

9.3.7D.3 Test purpose 1606

9.3.7D.4 Method of test 1606

9.3.7D.4.1 Initial conditions 1606

9.3.7D.4.2 Procedure 1607

9.3.7D.5 Test Requirements 1608

9.3.7E MIMO Dual Stream Static Orthogonal Conditions - UE categories 19-20 1608

9.3.7E.1 Definition and applicability 1608

9.3.7E.2 Minimum requirements 1608

9.3.7E.3 Test purpose 1609

9.3.7E.4 Method of test 1609

9.3.7E.4.1 Initial conditions 1609

9.3.7E.4.2 Procedure 1610

9.3.7E.5 Test Requirements 1611

9.3.7F MIMO Single Stream Fading Conditions - Asymmetric CPICHs 1611

9.3.7F.1 Definition and applicability 1611

9.3.7F.2 Minimum requirements 1611

9.3.7F.3 Test purpose 1612

9.3.7F.4 Method of test 1612

9.3.7F.4.1 Initial conditions 1612

9.3.7F.4.2 Procedure 1613

9.3.7F.5 Test Requirements 1614

9.3.7G MIMO Dual Stream Fading Conditions- Asymmetric CPICHs 1614

9.3.7G.1 Definition and applicability 1614

9.3.7G.2 Minimum requirements 1615

9.3.7G.3 Test purpose 1616

9.3.7G.4 Method of test 1616

9.3.7G.4.1 Initial conditions 1616

9.3.7G.4.2 Procedure 1617

9.3.7G.5 Test Requirements 1618

9.3.7H MIMO Dual Stream Fading Conditions - UE categories 19-20 - Asymmetric CPICHs 1618

9.3.7H.1 Definition and applicability 1618

9.3.7H.2 Minimum requirements 1619

9.3.7H.3 Test purpose 1620

9.3.7H.4 Method of test 1621

9.3.7H.4.1 Initial conditions 1621

9.3.7H.4.2 Procedure 1621

9.3.7H.5 Test Requirements 1622

9.3.7I MIMO Dual Stream Static Orthogonal Conditions - UE categories 15-20 - Asymmetric CPICHs 1622

9.3.7I.1 Definition and applicability 1622

9.3.7I.2 Minimum requirements 1623

9.3.7I.3 Test purpose 1623

9.3.7I.4 Method of test 1623

9.3.7I.4.1 Initial conditions 1623

9.3.7I.4.2 Procedure 1624

9.3.7I.5 Test Requirements 1625

9.3.7J MIMO Dual Stream Static Orthogonal Conditions - UE categories 19-20- Asymmetric CPICHs 1625

9.3.7J.1 Definition and applicability 1625

9.3.7J.2 Minimum requirements 1625

9.3.7J.3 Test purpose 1626

9.3.7J.4 Method of test 1626

9.3.7J.4.1 Initial conditions 1626

9.3.7J.4.2 Procedure 1627

9.3.7J.5 Test Requirements 1628

9.4 HS-SCCH Detection Performance 1628

9.4.1 Single Link Performance 1628

9.4.1.1 Definition and applicability 1628

9.4.1.2 Minimum requirements 1628

9.4.1.3 Test purpose 1629

9.4.1.4 Method of test 1629

9.4.1.4.1 Initial conditions 1629

9.4.1.4.2 Procedure 1629

9.4.1.5 Test Requirements 1629

9.4.1A Single Link Performance - Enhanced Performance Requirements Type 1 1630

9.4.1A.1 Definition and applicability 1630

9.4.1A.2 Minimum requirements 1631

9.4.1A.3 Test purpose 1631

9.4.1A.4 Method of test 1631

9.4.1A.4.1 Initial conditions 1631

9.4.1A.4.2 Procedure 1632

9.4.1A.5 Test Requirements 1632

9.4.2 Open Loop Diversity Performance 1633

9.4.2.1 Definition and applicability 1633

9.4.2.2 Minimum requirements 1633

9.4.2.3 Test purpose 1633

9.4.2.4 Method of test 1633

9.4.2.4.1 Initial conditions 1633

9.4.2.4.2 Procedure 1634

9.4.2.5 Test Requirements 1635

9.4.2A Open Loop Diversity Performance - Enhanced Performance Requirements Type 1 1635

9.4.2A.1 Definition and applicability 1635

9.4.2A.2 Minimum requirements 1636

9.4.2A.3 Test purpose 1636

9.4.2A.4 Method of test 1636

9.4.2A.4.1 Initial conditions 1636

9.4.2A.4.2 Procedure 1636

9.4.2A.5 Test Requirements 1637

9.4.3 HS-SCCH Type 3 Performance 1638

9.4.3.1 Definition and applicability 1638

9.4.3.2 Minimum requirements 1638

9.4.3.3 Test purpose 1639

9.4.3.4 Method of test 1639

9.4.3.4.1 Initial conditions 1639

9.4.3.4.2 Procedure 1640

9.4.3.5 Test Requirements 1640

9.4.3A HS-SCCH Type 3 Performance -STTD disabled- Asymmetric CPICHs 1641

9.4.3A.1 Definition and applicability 1641

9.4.3A.2 Minimum requirements 1642

9.4.3A.3 Test purpose 1643

9.4.3A.4 Method of test 1643

9.4.3A.4.1 Initial conditions 1643

9.4.3A.5 Test Requirements 1644

9.4.3B HS-SCCH Type 3 Performance -STTD enabled- Asymmetric CPICHs 1645

9.4.3B.1 Definition and applicability 1645

9.4.3B.2 Minimum requirements 1645

9.4.3B.3 Test purpose 1646

9.4.3B.4 Method of test 1646

9.4.3B.4.1 Initial conditions 1646

9.4.3B.4.2 Procedure 1647

9.4.3B.5 Test Requirements 1647

9.4.4 HS-SCCH Type 3 Performance for MIMO only with single-stream restriction 1649

9.4.4.1 Definition and applicability 1649

9.4.4.2 Minimum requirements 1649

9.4.4.3 Test purpose 1650

9.4.4.4 Method of test 1650

9.4.4.4.1 Initial conditions 1650

9.4.4.4.2 Procedure 1650

9.4.4.5 Test Requirements 1650

9.4.4A HS-SCCH Type 3 Performance for MIMO only with single-stream restriction- Enhanced Performance Requirements Type 1 1651

9.4.4A.1 Definition and applicability 1651

9.4.4A.2 Minimum requirements 1651

9.4.4A.3 Test purpose 1652

9.4.4A.4 Method of test 1652

9.4.4A.4.1 Initial conditions 1652

9.4.4A.4.2 Procedure 1652

9.4.4A.5 Test Requirements 1653

9.4.4B HS-SCCH Type 3 Performance for MIMO only with single-stream restriction-STTD disabled-asymmetric CPICHs 1654

9.4.4B.1 Definition and applicability 1654

9.4.4B.2 Minimum requirements 1654

9.4.4B.3 Test purpose 1655

9.4.4B.4 Method of test 1655

9.4.4B.4.1 Initial conditions 1655

9.4.4B.4.2 Procedure 1655

9.4.4B.5 Test Requirements 1656

9.4.4C HS-SCCH Type 3 Performance for MIMO only with single-stream restriction-STTD disabled-asymmetric CPICHs- Enhanced Performance Requirements Type 1 1656

9.4.4C.1 Definition and applicability 1656

9.4.4C.2 Minimum requirements 1657

9.4.4C.3 Test purpose 1657

9.4.4C.4 Method of test 1657

9.4.4C.4.1 Initial conditions 1657

9.4.4C.4.2 Procedure 1658

9.4.4C.5 Test Requirements 1658

9.4.4D HS-SCCH Type 3 Performance for MIMO only with single-stream restriction-STTD enabled-asymmetric CPICHs 1659

9.4.4D.1 Definition and applicability 1659

9.4.4D.2 Minimum requirements 1659

9.4.4D.3 Test purpose 1660

9.4.4D.4 Method of test 1660

9.4.4D.4.1 Initial conditions 1660

9.4.4D.4.2 Procedure 1660

9.4.4D.5 Test Requirements 1661

9.4.4E HS-SCCH Type 3 Performance for MIMO only with single-stream restriction-STTD enabled-asymmetric CPICHs- Enhanced Performance Requirements Type 1 1661

9.4.4E.1 Definition and applicability 1661

9.4.4E.2 Minimum requirements 1662

9.4.4E.3 Test purpose 1662

9.4.4E.4 Method of test 1662

9.4.4E.4.1 Initial conditions 1662

9.4.4E.4.2 Procedure 1663

9.4.4E.5 Test Requirements 1663

9.5 HS-SCCH-less demodulation of HS-DSCH (Fixed Reference Channel) 1664

9.5.1 Requirement QPSK, Fixed Reference Channel (FRC) H-Set 7 1664

9.5.1.1 Definition and applicability 1664

9.5.1.2 Minimum requirements 1664

9.5.1.3 Test purpose 1665

9.5.1.4 Method of test 1665

9.5.1.5 Test Requirements 1666

9.5.1A Requirement QPSK, Fixed Reference Channel (FRC) H-Set 7 - Enhanced Performance Requirements Type 1 1666

9.5.1A.1 Definition and applicability 1666

9.5.1A.2 Minimum requirements 1667

9.5.1A.3 Test purpose 1667

9.5.1A.4 Method of test 1667

9.5.1A.5 Test Requirements 1668

9.6 HS-DSCH and HS-SCCH reception in CELL-FACH state 1669

9.6.1 Single link HS-DSCH Demodulation performance in CELL\_FACH state 1669

9.6.1.1 Definition and applicability 1669

9.6.1.2 Minimum requirement QPSK, Fixed Reference Channel (FRC) H-Set 3 1669

9.6.1.3 Test purpose 1670

9.6.1.4 Method of test 1670

9.6.1.5 Test Requirements 1671

9.6.2 Single link HS-SCCH Detection performance in CELL\_FACH state 1671

9.6.2.1 Definition and applicability 1671

9.6.2.2 Minimum requirement 1671

9.6.2.3 Test purpose 1672

9.6.2.4 Method of test 1672

9.6.2.5 Test Requirements 1672

10 Performance requirement (E-DCH) 1674

10.1 General 1674

10.2 Detection of E-DCH HARQ ACK Indicator Channel (E-HICH) 1674

10.2.1 Single link performance 1674

10.2.1.1 Single link performance (10ms TTI) 1674

10.2.1.1.1 Definition and applicability 1674

10.2.1.1.2 Minimum requirement 1674

10.2.1.1.3 Test purpose 1675

10.2.1.1.4 Method of test 1675

10.2.1.1.4.1 Initial conditions 1675

10.2.1.1.4.2 Procedure 1676

10.2.1.1.5. Test requirements 1677

10.2.1.1A Single link performance (10ms TTI, Type 1) 1677

10.2.1.1A.1 Definition and applicability 1677

10.2.1.1A.2 Minimum requirement 1677

10.2.1.1A.3 Test purpose 1678

10.2.1.1A.4 Method of test 1678

10.2.1.1A.4.1 Initial conditions 1678

10.2.1.1A.4.2 Procedure 1678

10.2.1.1A.5. Test requirements 1679

10.2.1.2 Single link performance (2ms TTI) 1679

10.2.1.2.1 Definition and applicability 1679

10.2.1.2.2 Minimum requirement 1679

10.2.1.2.3 Test purpose 1680

10.2.1.2.4 Method of test 1680

10.2.1.2.4.1 Initial conditions 1680

10.2.1.2.4.2 Procedure 1681

10.2.1.2.5. Test requirements 1682

10.2.1.2A Single link performance (2ms TTI, Type 1) 1682

10.2.1.2A.1 Definition and applicability 1682

10.2.1.2A.2 Minimum requirement 1682

10.2.1.2A.3 Test purpose 1683

10.2.1.2A.4 Method of test 1683

10.2.1.2A.4.1 Initial conditions 1683

10.2.1.2A.4.2 Procedure 1683

10.2.1.2A.5. Test requirements 1684

10.2.2 Detection in Inter-Cell Handover conditions 1684

10.2.2.1 RLS not containing the Serving E-DCH cell 1684

10.2.2.1.1 RLS not containing the Serving E-DCH cell (10ms TTI) 1684

10.2.2.1.1.1 Definition and applicability 1684

10.2.2.1.1.2 Minimum requirement 1685

10.2.2.1.1.3 Test Purpose 1685

10.2.2.1.1.4 Method of test 1686

10.2.2.1.1.5 Test Requirements 1688

10.2.2.1.1A RLS not containing the Serving E-DCH cell (10ms TTI, Type 1) 1689

10.2.2.1.1A.1 Definition and applicability 1689

10.2.2.1.1A.2 Minimum requirement 1689

10.2.2.1.1A.3 Test Purpose 1690

10.2.2.1.1A.4 Method of test 1690

10.2.2.1.1A.5 Test Requirements 1692

10.2.2.1.2 RLS not containing the Serving E-DCH cell (2ms TTI) 1693

10.2.2.1.2.1 Definition and applicability 1693

10.2.2.1.2.2 Minimum requirement 1693

10.2.2.1.2.3 Test Purpose 1694

10.2.2.1.2.4 Method of test 1694

10.2.2.1.2.4.1 Initial conditions 1694

10.2.2.1.2.4.2 Procedure 1695

10.2.2.1.2.5 Test Requirements 1697

10.2.2.1.2A RLS not containing the Serving E-DCH cell (2ms TTI, Type 1) 1698

10.2.2.1.2A.1 Definition and applicability 1698

10.2.2.1.2A.2 Minimum requirement 1698

10.2.2.1.2A.3 Test Purpose 1699

10.2.2.1.2A.4 Method of test 1699

10.2.2.1.2A.4.1 Initial conditions 1699

10.2.2.1.2A.4.2 Procedure 1700

10.2.2.1.2A.5 Test Requirements 1701

10.2.2.2 RLS containing the Serving E-DCH cell 1702

10.2.2.2.1 RLS containing the Serving E-DCH cell (10ms TTI) 1702

10.2.2.2.1.1 Definition and applicability 1702

10.2.2.2.1.2 Minimum requirement 1702

10.2.2.2.1.3 Test purpose 1703

10.2.2.2.1.4 Method of test 1703

10.2.2.2.1.4.1 Initial conditions 1703

10.2.2.2.1.4.2 Procedure 1704

10.2.2.2.1.5 Test requirements 1706

10.2.2.2.1A RLS containing the Serving E-DCH cell (10ms TTI, Type 1) 1707

10.2.2.2.1A.1 Definition and applicability 1707

10.2.2.2.1A.2 Minimum requirement 1708

10.2.2.2.1A.3 Test purpose 1708

10.2.2.2.1A.4 Method of test 1708

10.2.2.2.1A.4.1 Initial conditions 1708

10.2.2.2.1A.4.2 Procedure 1709

10.2.2.2.1A.5 Test requirements 1710

10.2.2.2.2 RLS containing the Serving E-DCH cell (2ms TTI) 1711

10.2.2.2.2.1 Definition and applicability 1711

10.2.2.2.2.2 Minimum requirement 1711

10.2.2.2.2.3 Test purpose 1712

10.2.2.2.2.4 Method of test 1712

10.2.2.2.2.4.1 Initial conditions 1712

10.2.2.2.2.4.2 Procedure 1713

10.2.2.2.2.5 Test requirements 1715

10.2.2.2.2A RLS containing the Serving E-DCH cell (2ms TTI, Type 1) 1716

10.2.2.2.2A.1 Definition and applicability 1716

10.2.2.2.2A.2 Minimum requirement 1716

10.2.2.2.2A.3 Test purpose 1717

10.2.2.2.2A.4 Method of test 1717

10.2.2.2.2A.4.1 Initial conditions 1717

10.2.2.2.2A.4.2 Procedure 1718

10.2.2.2.2A.5 Test requirements 1719

10.3 Detection of E-DCH Relative Grant Channel (E-RGCH) 1720

10.3.1 Single link performance 1720

10.3.1.1 Single link performance (10ms TTI) 1720

10.3.1.1.1 Definition and applicability 1720

10.3.1.1.2 Minimum requirement 1720

10.3.1.1.3 Test purpose 1721

10.3.1.1.4 Method of test 1721

10.3.1.1.4.1 Initial conditions 1721

10.3.1.1.4.2 Procedure 1722

10.3.1.1.5 Test requirements 1723

10.3.1.1A Single link performance (10ms TTI, Type 1) 1724

10.3.1.1A.1 Definition and applicability 1724

10.3.1.1A.2 Minimum requirement 1724

10.3.1.1A.3 Test purpose 1724

10.3.1.1A.4 Method of test 1725

10.3.1.1A.4.1 Initial conditions 1725

10.3.1.1A.4.2 Procedure 1725

10.3.1.1A.5 Test requirements 1726

10.3.1.2 Single link performance (2ms TTI) 1727

10.3.1.2.1 Definition and applicability 1727

10.3.1.2.2 Minimum requirement 1727

10.3.1.2.3 Test purpose 1728

10.3.1.2.4 Method of test 1728

10.3.1.2.4.1 Initial conditions 1728

10.3.1.2.4.2 Procedure 1728

10.3.1.2.5 Test requirements 1730

10.3.1.2A Single link performance (2ms TTI, Type 1) 1731

10.3.1.2A.1 Definition and applicability 1731

10.3.1.2A.2 Minimum requirement 1731

10.3.1.2A.3 Test purpose 1731

10.3.1.2A.4 Method of test 1731

10.3.1.2A.4.1 Initial conditions 1731

10.3.1.2A.4.2 Procedure 1732

10.3.1.2A.5 Test requirements 1733

10.3.2 Detection in Inter-Cell Handover conditions 1734

10.3.2.1 Definition and applicability 1734

10.3.2.2 Minimum requirement for Non-serving E-DCH RL 1734

10.3.2.3 Test Purpose 1734

10.3.2.4 Method of test 1735

10.3.2.4.1 Initial conditions 1735

10.3.2.4.2 Procedure 1735

10.3.2.5 Test Requirements 1738

10.3.2A Detection in Inter-Cell Handover conditions (Type 1) 1739

10.3.2A.1 Definition and applicability 1739

10.3.2A.2 Minimum requirement for Non-serving E-DCH RL 1740

10.3.2A.3 Test Purpose 1740

10.3.2A.4 Method of test 1740

10.3.2A.4.1 Initial conditions 1740

10.3.2A.4.2 Procedure 1741

10.3.2A.5 Test Requirements 1743

10.4 Demodulation of E-DCH Absolute Grant Channel (E-AGCH) 1744

10.4.1 Single link performance 1744

10.4.1.1 Definition and applicability 1744

10.4.1.2 Minimum requirement 1744

10.4.1.3 Test Purpose 1745

10.4.1.4 Method of test 1745

10.4.1.4.1 Initial conditions 1745

10.4.1.4.2 Procedure 1745

10.4.1.5 Test Requirements 1746

10.4.1A Single link performance (Type 1) 1747

10.4.1A.1 Definition and applicability 1747

10.4.1A.2 Minimum requirement 1747

10.4.1A.3 Test Purpose 1747

10.4.1A.4 Method of test 1747

10.4.1A.4.1 Initial conditions 1747

10.4.1A.4.2 Procedure 1748

10.4.1A.5 Test Requirements 1748

11 Performance requirement (MBMS) 1749

11.1 General 1749

11.2 Demodulation of MTCH 1749

11.2.1 Definition and applicability 1749

11.2.2 Minimum requirement 1749

11.2.3 Test Purpose 1750

11.2.4 Method of test 1750

11.2.4.1 Initial conditions 1750

11.2.4.2 Procedure 1751

11.2.5 Test Requirements 1752

11.2A Demodulation of MTCH - Enhanced Performance Requirements Type 1 1753

11.2A.1 Definition and applicability 1753

11.2A.2 Minimum requirement 1753

11.2A.3 Test Purpose 1753

11.2A.4 Method of test 1753

11.2A.4.1 Initial conditions 1753

11.2A.4.2 Procedure 1754

11.2A.5 Test Requirements 1755

11.3 Demodulation of MTCH and cell identification 1756

11.3.1 Definition and applicability 1756

11.3.2 Minimum requirements 1756

11.3.3 Test purpose 1757

11.3.4 Method of test 1757

11.3.5 Test requirements 1759

Annex A (informative): Connection Diagrams 1760

Annex B (normative): Global In-Channel TX-Test 1799

B.1 General 1799

B.2 Definition of the process 1799

B.2.1 Basic principle 1799

B.2.2 Output signal of the TX under test 1799

B.2.3 Reference signal 1799

B.2.4 void 1800

B.2.5 Classification of measurement results 1800

B.2.6 Process definition to achieve results f, t, , g1, g2, and O 1800

B.2.6.1 Decision Point Power 1801

B.2.6.2 Measured total power of all active codes 1801

B.2.6.3 Code-Domain Power 1801

B.2.6.4 Code-Domain Power of the varied reference signal 1802

B.2.7 Process definition to achieve results EVM, PCDE, RCDE 1802

B.2.7.1 Error Vector Magnitude (EVM) 1802

B.2.7.2 Code Domain Error Power 1803

B.2.7.3 Relative Code Domain Error (RCDE) 1803

B.3 Notes 1804

Annex C (normative): Measurement channels 1807

C.1 General 1807

C.2 UL reference measurement channel 1807

C.2.1 UL reference measurement channel (12,2 kbps) 1807

C.2.2 UL reference measurement channel (64 kbps) 1808

C.2.3 UL reference measurement channel (144 kbps) 1810

C.2.4 UL reference measurement channel (384 kbps) 1812

C.2.5 UL reference measurement channel (768 kbps) 1814

C.2.6 UL E-DCH reference measurement channel for DC-HSUPA using BPSK modulation 1816

C.2.7 UL E-DCH reference measurement channel for DC-HSUPA using 16QAM modulation 1817

C.2.8 Combinations of UL E-DCH reference measurement channel for DC-HSUPA tests 1818

C.3 DL reference measurement channel 1818

C.3.1 DL reference measurement channel (12.2 kbps) 1818

C.3.1A DL reference measurement channel (0 kbps and 12.2 kbps) 1820

C.3.2 DL reference measurement channel (64 kbps) 1822

C.3.3 DL reference measurement channel (144 kbps) 1824

C.3.4 DL reference measurement channel (384 kbps) 1826

C.3.5 DL reference measurement channel 2 (64 kbps) 1828

C.4 Reference measurement channel for BTFD performance requirements 1829

C.4.1 UL reference measurement channel for BTFD performance requirements 1829

C.4.2 DL reference measurement channel for BTFD performance requirements 1832

C.4.3 Reference parameters for discontinuous UL DPCCH transmission 1835

C.5 DL reference compressed mode parameters 1835

C.6 Auxiliary measurement channels 1838

C.6.1 Introduction 1838

C.6.2 Channel combinations for BLER measurements 1839

C.6.3 UL auxiliary reference measurement channel (TM, 12.2 kbps, no CRC) 1840

C.6.3A UL auxiliary reference measurement channel (TM, 0 kbps and 12.2 kbps, no CRC) 1840

C.6.4 Void 1841

C.6.5 Void 1841

C.6.6 Void 1841

C.6.7 UL AUXMC AM 12.2 kbps 1842

C.6.8 UL AUXMC AM 12.2 kbps(DCCH with TB size of 148bit) 1842

C.7 DL reference parameters for PCH tests 1843

C.8 DL reference channel parameters for HSDPA tests 1843

C.8.1 Fixed Reference Channel (FRC) 1843

C.8.1.1 Fixed Reference Channel Definition H-Set 1/1A/1B/1C 1843

C.8.1.2 Fixed Reference Channel Definition H-Set 2 1844

C.8.1.3 Fixed Reference Channel Definition H-Set 3/3A/3B/3C 1845

C.8.1.4 Fixed Reference Channel Definition H-Set 4 1846

C.8.1.5 Fixed Reference Channel Definition H-Set 5 1847

C.8.1.6 Fixed Reference Channel Definition H-Set 6/6A/6B/6C 1848

C.8.1.7 Fixed Reference Channel Definition H-Set 7 1849

C.8.1.8 Fixed Reference Channel Definition H-Set 8/8A/8B/8C 1850

C.8.1.9 Fixed Reference Channel Definition H-Set 9/9A/9B/9C 1851

C.8.1.10 Fixed Reference Channel Definition H-Set 10/10A/10B/10C 1852

C.8.1.11 Fixed Reference Channel Definition H-Set 11/11A/11B/11C 1854

C.8.1.12 Fixed Reference Channel Definition H-Set 12 1855

C.9 Downlink reference channel dummy DCCH transmission on DCH 1856

C.9A MAC header transmission on HS-DSCH 1856

C.10 UL reference channel parameters for HSDPA tests 1856

C.10.1 UL reference measurement channel for HSDPA tests 1856

C.10.2 UL reference measurement channel for HSDPA tests with UL OLTD/CLTD 1857

C.11 Reference channel parameters for E-DCH tests 1859

C.11.1 UL reference measurement channel for E-DCH tests 1859

C.11.1A UL reference measurement channel for E-DCH tests with UL OLTD/CLTD 1860

C.11.2 DL reference measurement channel for E-DCH tests 1862

C.11.3 RLC SDU size for E-DCH tests 1862

C.11A Reference channel parameters for DC-HSUPA tests 1864

C.11A.1 UL reference measurement channel for DC-HSUPA tests 1864

C.11A.2 DL reference measurement channel for DC-HSUPA tests 1865

C.11A.3 RLC SDU size for DC-HSUPA tests 1865

C.12 DL reference parameters for MBMS tests 1866

C.12.1 MTCH 1866

C.12.2 Combined MTCH demodulation and cell identification 1866

Annex D (normative): Propagation Conditions 1867

D.1 General 1867

D.1.1 Definition of Additive White Gaussian Noise (AWGN) Interferer 1867

D.2 Propagation Conditions 1867

D.2.1 Static propagation condition 1867

D.2.2 Multi-path fading propagation conditions 1867

D.2.3 Moving propagation conditions 1869

D.2.4 Birth-Death propagation conditions 1869

D.2.4A High speed train conditions 1870

D.2.5 Conditions for HSDPA enhanced performance requirements type 1 with UE receiver diversity 1871

D.2.6 Conditions for HSDPA enhanced performance requirements type 3 with UE receiver diversity 1871

D.2.7 Conditions for open and closed loop diversity performance 1871

D.2.8 Conditions for MBMS enhanced performance requirements type 1 with UE receiver diversity 1871

D.2.9 MIMO propagation conditions 1872

D.2.9.1 MIMO Single Stream Fading Conditions 1872

D.2.9.2 MIMO Dual Stream Fading Conditions 1873

D.2.9.3 MIMO Dual Stream Static Orthogonal Conditions 1874

Annex E (normative): Downlink Physical Channels 1875

E.1 General 1875

E.2 Connection Set-up for non-HSDPA test cases 1875

E.2.1 Measurement without dedicated connection 1875

E.3 During connection for non-HSDPA test cases 1875

E.3.1 Measurement of Tx Characteristics 1876

E.3.2 Measurement of Rx Characteristics 1876

E.3.3 Measurement of Performance requirements 1876

E.3.4 Connection with open-loop transmit diversity mode 1878

E.3.5 Connection with closed loop transmit diversity mode 1879

E.3.6 OCNS Definition 1879

E.4 W-CDMA Modulated Interferer for non-HSDPA test cases 1880

E.5 HSDPA DL Physical channels 1880

E.5.0 Downlink Physical Channels for connection set-up 1880

E.5.1 Downlink Physical Channels for measurement 1880

E.5.2 HSDPA OCNS Definition 1889

E.5.3 Downlink Physical Channels for measurement including test tolerances 1890

E.5.4 Downlink Physical Channels for Transmitter Characteristics with HS-DPCCH 1892

E.5A E-DCH with HSDPA DL Physical channels 1893

E.5A.0 Downlink Physical Channels for connection set-up 1893

E.5A.1 Downlink Physical Channels for measurement 1893

E.5A.2 E-DCH OCNS Definition 1895

E.5B MBMS DL Physical channels 1896

E.5B.1 Downlink Physical Channels for connection set-up 1896

E.5C F-DPCH with HSDPA DL Physical channels 1896

E.5C.0 Downlink Physical Channels for connection set-up 1896

E.5C.1 Downlink Physical Channels for measurement 1896

E.5D HSDPA and E-DCH DL Physical channels with discontinuous UL DPCCH transmission 1898

E.5D.0 Downlink Physical Channels for connection set-up 1898

E.5D.1 Downlink Physical Channels for measurement 1898

E.5E Test Definition for Enhanced Performance Type 3i 1899

E.5E.1 Transmitted code and power characteristics for serving cell 1900

E.5E.2 Transmitted code and power characteristics for interfering cells 1902

E.5E.3 Model for power control sequence generation 1902

E.5F Test Definition for MultiFlow HSDPA 1903

E.5F.1 Test configuration when 2 cells are configured in Multiflow mode 1903

E.5F.2 Test configuration when 3 cells are configured in Multiflow mode 1905

E.5F.3 Test configuration when 4 cells are configured in Multiflow mode 1905

E.6 Downlink Physical Channels Code Allocation (This clause is informative) 1905

E.6.1 Downlink Physical Channels Code Allocation for non-HSDPA test cases 1905

E.6.2 Downlink Physical Channels Code Allocation for HSDPA test cases 1908

E.6.3 Downlink Physical Channels Code Allocation for E-DCH test cases 1912

E.6.4 Downlink Physical Channels Code Allocation for MBMS test cases 1914

Annex F (normative): General test conditions and declarations 1916

F.1 Acceptable uncertainty of Test System 1916

F.1.1 Measurement of test environments 1916

F.1.2 Measurement of transmitter 1917

F.1.3 Measurement of receiver 1924

F.1.4 Performance requirement 1929

F.1.5 Requirements for support of RRM 1937

F.1.6 Performance requirement (HSDPA) 1963

F.1.7 Performance requirement (E-DCH) 1969

F.1.8 Performance requirement (MBMS) 1972

F.2 Test Tolerances (This clause is informative) 1973

F.2.1 Transmitter 1973

F.2.2 Receiver 1978

F.2.3 Performance requirements 1980

F.2.4 Requirements for support of RRM 1984

F.2.5 Performance requirements (HSDPA) 1993

F.2.6 Performance requirements (E-DCH) 1996

F.2.7 Performance requirements (MBMS) 1997

F.3 Interpretation of measurement results 1997

F.4 Derivation of Test Requirements (This clause is informative) 1997

F.4.1 Transmitter 1998

F.4.2 Receiver 2022

F.4.3 Performance requirements 2028

F.4.4 Requirements for support of RRM 2042

F.4.5 Performance requirements (HSDPA) 2077

F.4.6 Performance requirements (E-DCH) 2085

F.4.7 Performance requirements (MBMS) 2088

F.5 Acceptable uncertainty of Test Equipment (This clause is informative) 2088

F.5.1 Transmitter measurements 2089

F.5.2 Receiver measurements 2091

F.5.3 Performance measurements 2092

F.5.4 Requirements for support of RRM 2092

F.5.5 Performance measurements (HSDPA) 2093

F.5.6 Performance measurements (E-DCH) 2095

F.5.7 Performance measurements (MBMS) 2096

F.6 General rules for statistical testing 2096

F.6.1 Statistical testing of receiver BER/BLER performance 2096

F.6.1.1 Error Definition 2096

F.6.1.2 Test Method 2096

F.6.1.3 Test Criteria 2096

F.6.1.4 Calculation assumptions 2097

F.6.1.4.1 Statistical independence 2097

F.6.1.4.2 Applied formulas 2097

F.6.1.4.3 Approximation of the distribution 2097

F.6.1.5 Definition of good pass fail decision. 2097

F.6.1.6 Good balance between test time and statistical significance 2098

F.6.1.7 Pass fail decision rules 2099

F.6.1.8 Test conditions for BER, BLER, RLC SDU Error Rate tests 2100

F.6.1.9 Practical Use (informative) 2103

F.6.1.10 Dual limit BLER tests 2105

F.6.1.10.1 Description of the parameters for dual limit BLER tests 2106

F.6.1.10.2 Pass fail decision rules 2108

F.6.1.10.3 Test conditions for dual limit BLER tests 2109

F.6.1.10.4 Test conditions for dual limit TPC Command Error Rate tests 2110

F.6.2 Statistical testing of RRM delay performance 2110

F.6.2.1 Test Method 2110

F.6.2.2 Bad Delay Ratio (ER) 2110

F.6.2.3 Test Criteria 2110

F.6.2.4 Calculation assumptions 2110

F.6.2.4.1 Statistical independence 2110

F.6.2.4.2 Applied formulas 2111

F.6.2.4.3 Approximation of the distribution 2111

F.6.2.5 Definition of good pass fail decision 2111

F.6.2.6 Good balance between test-time and statistical significance 2112

F.6.2.7 Pass fail decision rules 2112

F.6.2.8 Test conditions for RRM delay tests, Combining of TPC commands test 1, Demodulation of Paging channel and Detection of acquisition indicator tests and UE measurement performance tests. 2112

F.6.2.9 Practical Use (informative) 2116

F.6.3 Statistical Testing of HSDPA Receiver Performance 2117

F.6.3.1 Definition 2117

F.6.3.2 Mapping throughput to block error ratio 2118

F.6.3.3 Bad DUT factor 2118

F.6.3.3.1 Bad DUT factor, range of applicability 2119

F.6.3.4 Minimum Test time 2120

F.6.3.5 Test conditions for HSDPA Receiver Performance 2122

F.6.4 Statistical testing of performance requirement (E-DCH and MBMS) 2143

F.6.4.1 Test Method 2143

F.6.4.2 Bad Result Ratio (ER) 2143

F.6.4.3 Mapping of E-DCH and MBMS tests to RRM tests (F.6.2) and HSDPA tests (F.6.3) 2143

F.6.4.4 Test conditions for E-DCH tests and MBMS 2144

Annex G (normative): Environmental conditions 2145

G.1 General 2145

G.2 Environmental requirements 2145

G.2.1 Temperature 2145

G.2.2 Voltage 2145

G.2.3 Vibration 2146

G.2.4 Specified frequency range 2146

Annex H (normative): UE Capabilities (FDD) 2147

H.1 Void 2147

H.2 Void 2147

Annex I (normative): Default Message Contents 2148

Contents of MEASUREMENT REPORT message for Intra frequency test cases 2148

Contents of MEASUREMENT REPORT message for Inter frequency test cases 2149

Contents of MEASUREMENT REPORT message for inter – RAT test cases 2150

Contents of RRC CONNECTION SETUP message: UM (Transition to CELL\_DCH) 2150

Contents of RADIO BEARER SETUP message: AM or UM (HSDPA) 2150

Contents of Master Information Block PLMN type is the case of GSM-MAP 2151

Contents of Scheduling Block 1 (FDD) 2151

Contents of Scheduling Block 1 (FDD) 2152

Contents of Scheduling Block 1 (FDD) 2152

Contents of System Information Block type 11 (FDD) 2153

Contents of System Information Block type 11 (FDD) 2154

Contents of System Information Block type 11 (FDD) 2154

Contents of System Information Block type 11 (FDD) 2155

Contents of Scheduling Block 1 (FDD) 2155

Contents of System Information Block type 11 (FDD) 2156

Contents of System Information Block type 11 (FDD) 2157

Contents of Scheduling Block 1 (FDD) 2158

Contents of System Information Block type 11 (FDD) 2158

Contents of System Information Block type 11 (FDD) 2159

Contents of ACTIVE SET UPDATE message for test cases with SHO in clauses 7.7.1, 7.7.1A, 7.7.2, and 7.7.3. 2163

Annex J (informative): Information about special regional application of test cases and requirements 2166

J.1 Japan 2166

Annex K (normative): Cell configuration mapping 2167

Annex L (normative): Conditions for RRM requirements applicability for operating bands 2172

L.1 Conditions for Idle mode tasks 2172

L.1.1 Conditions for measurements of inter-RAT E-UTRA cells 2172

L.2 Conditions for UE Measurements Procedures 2172

L.2.1 Conditions for E-UTRAN measurements 2172

L.3 Conditions for Measurement Performance for UE 2173

L.3.1 Conditions for intra frequency CPICH RSCP measurements accuracy 2173

L.3.2 Conditions for intra frequency CPICH RSCP relative measurements accuracy 2173

L.3.3 Conditions for inter frequency CPICH RSCP relative measurements accuracy 2174

L.3.4 Conditions for intra frequency CPICH Ec/Io measurements accuracy 2174

L.3.5 Conditions for intra frequency CPICH Ec/Io relative measurements accuracy 2174

L.3.6 Conditions for inter frequency CPICH Ec/Io measurements accuracy 2174

L.3.7 Conditions for inter frequency CPICH Ec/Io relative measurements accuracy 2174

L.3.8 Conditions for intra frequency SFN-SFN observed time difference 2174

L.3.9 Conditions for inter frequency SFN-SFN observed time difference 2175

L.3.10 Conditions for SFN-SFN observed time difference type 1 2175

L.3.11 Conditions for intra frequency SFN-SFN observed time difference type 2 without or with IPDL period active 2175

L.3.12 Conditions for inter frequency SFN-SFN observed time difference type 2 2175

L.4 Conditions for UTRAN Connected mode mobility 2175

L.4.1 Conditions for identification of a new CGI of inter-RAT E-UTRA cell with autonomous gaps 2175

Annex M (informative): Change history 2177