3GPP TS 34.123-3 V16.3.0 (2022-06)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Radio Access Network;

User Equipment (UE) conformance specification;

Part 3: Abstract Test Suite (ATS)

(Release 16)

** 

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.   
The present document has not been subject to any approval process by the 3GPPOrganisational Partners and shall not be implemented.   
This Specification is provided for future development work within 3GPPonly. The Organisational Partners accept no liability for any use of this Specification.  
Specifications and reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organisational Partners' Publications Offices.

Keywords

UMTS, ATS, terminal, radio, mobile

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

[http://www.3gpp.org](http://www.3gpp.org/)

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword 15

Introduction 15

1 Scope 16

2 References 16

3 Definitions and abbreviations 19

3.1 Definitions 19

3.2 Abbreviations 19

4 Requirements on the TTCN development 19

5 TTCN-2 ATS structure 20

5.1 Modularity 21

5.1.1 Module structure 21

5.1.2 Contents of the modules 23

5.1.3 Example of a working platform 23

6 Test method and testing architecture 24

6.1 Test method 24

6.2 TTCN-2 Testing architecture 25

6.2.1 Lower Tester (LT) 25

6.2.2 Configuration and initialization 25

6.2.3 Upper Tester (UT) 26

6.2.4 TTCN-2 26

6.2.5 Model extension 26

6.2.6 Multiplexing of RLC services 26

6.3 NAS test method and architecture 26

6.3.1 Test configuration 26

6.3.2 Routing UL NAS massages in SS 27

6.4 RRC and RAB test method and architecture 28

6.4.1 Test configuration 28

6.4.2 RAB test method 29

6.4.2.1 Sending data on the same TTI 29

6.4.2.2 Sending continuous data on consecutive TTIs 29

6.5 RLC test method and architecture 30

6.5.1 Testing architecture 30

6.5.2 Test method 31

6.5.2.1 Handling SUFIs in TTCN 34

6.5.2.2 Void 35

6.6 SMS test method and architecture 35

6.6.1 SMS CS test method and architecture 35

6.6.2 SMS PS test method and architecture 35

6.6.3 SMS Cell broadcasting test method and architecture 35

6.7 MAC test method and architecture 35

6.7.1 Testing architecture 35

6.7.2 Test method 36

6.7.2.1 Abnormal decoding situations 36

6.7.2.2 MAC\_es/e test method (Rel-6 or later) 36

6.7.2.3 MAC\_is/i test method (Rel-8 or later) 37

6.8 BMC test method and architecture 39

6.8.1 BMC test architecture 39

6.8.2 BMC test method 39

6.9 PDCP test 41

6.9.1 PDCP test architecture 41

6.9.2 PDCP test method 42

6.9.2.1 CS voice over HSPA 42

6.9.2.2 Network initiated secondary PDP context 43

6.10 Multi-RAT Handover Test Model 43

6.10.1 Overview 43

6.10.2 ASP function description 44

6.10.2.1 Identities 44

6.10.2.2 Cell configuration and control 44

6.10.2.3 L1 (GERAN) configuration and control 44

6.10.2.3.1 Basic physical channel configuration 45

6.10.2.3.2 Multislot configuration for circuit or packet switched channels 45

6.10.2.3.3 Frame in the near future 46

6.10.2.3.4 L1 header 46

6.10.2.4 L2 configuration and control 46

6.10.2.4.1 Don't response to some handover access bursts 46

6.10.2.4.2 No UA reply to SABM 46

6.10.2.5 System Information sending 46

6.10.2.6 Paging 47

6.10.2.7 Generic procedures for GPRS signalling 47

6.10.2.7.1 GPRS generic attach procedures and ciphering mode control 47

6.10.2.7.2 Cell change order within a TBF 49

6.10.2.8 Generic configuration procedure for GSM ciphering mode control 51

6.10.2.9 L|H bits convention and bit padding in DL 51

6.10.2.9.1 GERAN DL RLC/MAC message bit padding 51

6.10.2.9.2 GSM DL message spare padding 52

6.10.2.9.3 L | H convention in rest octets of GSM DL messages 52

6.10.2.9.4 Spare Bits 52

6.10.2.9.5 GSM System Information messages on SACCH 52

6.10.2.9.6 GSM Measurement Information messages on SACCH 52

6.11 DCH-DSCH model (R99 or Rel-4) 54

6.12 DCH with HS-DSCH (MAC-hs) model (FDD, Rel-5 or later) 55

6.12a DCH with HS-DSCH model for 1.28 Mcps TDD (Rel-5 or later) 56

6.12b DCH with HS-DSCH (MAC-ehs) model (FDD, Rel-7 or later) 57

6.12c HS-DSCH (MAC-hs/ehs) model (FDD, Rel-7 or later)(No DCH Associated) 58

6.12d HS-DSCH (MAC-ehs) model for DC/4C -HSDPA (FDD, Rel-8 or later) 59

6.12e HS-DSCH (MAC-ehs) model for Multiflow Operation (FDD, Rel-11 or later) 60

6.13 E-DCH model (Rel-6 or later) 62

6.13.1 MAC-e/MAC-es test model 62

6.13.2 MAC-i/MAC-is test model (Rel-8 or later) 64

6.13.2.1 MAC-i/MAC-is test model for Enhanced UL in Cell\_FACH (Rel-8 or later) 65

6.13.2.2 MAC-i/MAC-is test model for DC-HSUPA (Rel-9 or later) 65

6.14 MBMS model (Rel-6 or later) 66

6.14.1 MBMS RLC test model 69

6.14.1.1 RLC test model for MTCH test 69

6.14.1.2 RLC test model for MCCH test 69

6.15 IP signalling 69

6.16 Supplementary Service test method and architecture 69

6.16.1 Test configuration 69

6.17 UTRAN-WLAN Inter working Test Model 69

6A TTCN-3 Test method and testing architecture 70

6A.1 Test system architecture 70

6A.1.1 General system architecture 70

6A.1.2 Component architecture 70

6A.2 Test model 70

6A.3 ASP specifications 72

6A.3.1 ASPs for Control Primitive Transmission 72

6A.3.1.1 FDD Control ASP extension types 75

6A.3.1.1.1 CPHY\_RL\_Setup extension 76

6A.3.1.1.1a CPHY\_RL\_Modify extension 80

6A.3.1.1.2 CMAC\_MACehs\_HARQAssign\_MultiFlows extension 80

6A.3.1.1.3 CMAC\_MAChs\_MACehs\_TFRCconfigure extension 81

6A.3.1.1.4 CRLC\_BindTestDataInMultipleMACehs\_PDU\_MultiFlows extension 83

6A.3.1.1.5 CMAC\_Config 83

6A.3.1.1.6 CRLC\_Config 85

6A.3.1.2 TDD Control ASP extension types 85

6A.3.1.3 FDD and TDD Control ASP types 85

6A.3.1.3.1 CPHY\_HS\_DPCCH\_CQI\_MultiCell (Rel-10 or later) 85

6A.3.1.3.2 CPHY\_MeasurementConfig 86

6A.3.1.3.3 CMAC\_ConfigMACehs\_NodeB (Rel-11 or later) 87

6A.3.1.3.4 CMAC\_MACehs\_NodeB\_CellMapping (Rel-11 or later) 87

6A.3.1.3.5 CMAC\_MACehs\_HARQAssign\_NodeB (Rel-11 or later) 88

6A.3.1.3.6 CRLC\_BindTestDataInMultipleMACehs\_PDU\_NodeB (Rel-11 or later) 89

6A.3.1.3.7 CPHY\_AICH\_NegAckModeSet (Rel-11 or later) 90

6A.3.2 ASPs for Data Transmission and Reception 90

6A.4 Upper Tester Interface 91

6A.5 IXIT Proforma 91

7 PCO and ASP definitions 91

7.1 NAS PCO and ASP definitions 91

7.1.1 NAS PCO Definitions 91

7.1.2 Primitives used at Dc PCO 91

7.2 Ut PCO and ASP definitions 93

7.2.1 Ut PCO Declarations 93

7.2.2 Primitives used at Ut PCO 93

7.3 RRC PCO and ASP definitions 94

7.3.1 AM/UM/TM PCO and ASP definitions 94

7.3.1.1 SAP and PCO for data transmission and reception 94

7.3.2 Control PCO and ASP 94

7.3.2.1 SAP and PCO for control primitives transmission and reception 94

7.3.2.2 Control ASP Type Definition 96

7.3.2.2.1 CPHY\_AICH\_AckModeSet 96

7.3.2.2.2 CPHY\_Cell\_Config 96

7.3.2.2.3 CPHY\_Cell\_Release 97

7.3.2.2.3a CPHY\_Cell\_TimingAdjust 98

7.3.2.2.3b CPHY\_Detect\_TFCI 99

7.3.2.2.4 CPHY\_Ini 99

7.3.2.2.5 CPHY\_Cell\_TxPower\_Modify 100

7.3.2.2.6 CPHY\_Frame\_Number 100

7.3.2.2.6a CPHY\_SFN (Rel-6 or later) 101

7.3.2.2.6b CPHY\_MBMS\_MICH\_q (Rel-6 or later) 101

7.3.2.2.6c CPHY\_MBMS\_NI (Rel-6 or later) 105

7.3.2.2.7 CPHY\_Out\_of\_Sync 106

7.3.2.2.8 CPHY\_PRACH\_Measurement 106

7.3.2.2.9 CPHY\_RL\_Modify 107

7.3.2.2.10 CPHY\_RL\_Release 108

7.3.2.2.11 CPHY\_RL\_Setup 109

7.3.2.2.12 CPHY\_Sync 124

7.3.2.2.12a CPHY\_HS\_DPCCH\_AckNack (Rel-5 or later) 124

7.3.2.2.12b CPHY\_HS\_DPCCH\_CQI (Rel-5 or later) 125

7.3.2.2.12b1 CPHY\_HS\_DPCCH\_CQI\_DC (Rel-8 or later) 126

7.3.2.2.12c CPHY\_HS\_DSCH\_CRC\_Mode (Rel-5 or later) 127

7.3.2.2.13 CPHY\_TrCH\_Config 128

7.3.2.2.14a CPHY\_UL\_PowerModify 134

7.3.2.2.14 CPHY\_TrCH\_Release 135

7.3.2.2.15 CMAC\_BMC\_Scheduling 135

7.3.2.2.16 CMAC\_Ciphering\_Activate 136

7.3.2.2.16a CMAC\_FACH\_MeasOccas 137

7.3.2.2.17 CMAC\_Config 137

7.3.2.2.17a CMAC\_MAChs\_MACehs\_TFRCconfigure (Rel-5 or later) 142

7.3.2.2.17a0 CMAC\_MAChs\_MACehs\_HARQprocAssign 145

7.3.2.2.17a1 CMAC\_MACehs\_HARQAssign\_MultiFlows (Rel-7 or later) 146

7.3.2.2.17aa CMAC \_MACehs\_HS\_SCCH\_Orders (Rel-7 or later) 146

7.3.2.2.17b CMAC\_MACe\_Config (Rel-6 or later) 147

7.3.2.2.17c CMAC\_MACe\_NodeB\_CellMapping (Rel-6 or later) 148

7.3.2.2.17d CMAC\_MACes\_Config (Rel-6 or later) 149

7.3.2.2.17e CMAC\_MACe\_AG (Rel-6 or later) 150

7.3.2.2.17f CMAC\_MACe\_AckNack (Rel-6 or later) 151

7.3.2.2.17g CMAC\_MACe\_E\_TFC\_Restriction (Rel-6 or later) 151

7.3.2.2.17h CMAC\_MACe\_RG (Rel-6 or later) 152

7.3.2.2.17ha Void 153

7.3.2.2.17i CMAC\_MACes\_SI\_IND (Rel-6 or later) 153

7.3.2.2.17j CMAC\_MACes\_SI\_Config (Rel-6 or later) 153

7.3.2.2.17k CMAC\_MACi\_Config (Rel-8 or later) 153

7.3.2.2.17l CMAC\_MACi\_NodeB\_CellMapping (Rel-8 or later) 156

7.3.2.2.17m CMAC\_MACis\_Config (Rel-8 or later) 156

7.3.2.2.17n CMAC\_MACi\_AG (Rel-8 or later) 158

7.3.2.2.17o CMAC\_MACi\_AckNack (Rel-8 or later) 158

7.3.2.2.17p CMAC\_MACi\_E\_TFC\_Restriction (Rel-8 or later) 159

7.3.2.2.17q CMAC\_MACi\_RG (Rel-8 or later) 159

7.3.2.2.17r Void 160

7.3.2.2.17s CMAC\_MACis\_SI\_IND 160

7.3.2.2.17t CMAC\_MACis\_SI\_Config (Rel-8 or later) 160

7.3.2.2.17u CMAC\_MBMS\_ConfigInfo (Rel-6 or later) 160

7.3.2.2.18 CMAC\_PAGING\_Config 161

7.3.2.2.19 CMAC\_Restriction 162

7.3.2.2.20 CMAC\_SecurityMode\_Config 163

7.3.2.2.21 CMAC\_SequenceNumber 163

7.3.2.2.22 CMAC\_SYSINFO\_Config 163

7.3.2.2.22a CRLC\_Bind\_TestData\_TTI 164

7.3.2.2.22b CRLC\_BindTestDataInOneMAChs\_MACehs\_PDU (Rel-5 or later) 165

7.3.2.2.22c CRLC\_BindTestDataInMultipleMACehs\_PDU\_MultiFlows (Rel-7 or later) 165

7.3.2.2.23 CRLC\_Ciphering\_Activate 166

7.3.2.2.24 CRLC\_Config 167

7.3.2.2.25 CRLC\_Integrity\_Activate 170

7.3.2.2.26 CRLC\_Integrity\_Failure 171

7.3.2.2.26a CRLC\_MAC\_I\_Mode 171

7.3.2.2.26b CRLC\_NotAckNxtRxSDU 172

7.3.2.2.26c CRLC\_ProhibitRLC\_Ack 172

7.3.2.2.26d CRLC\_ReportDataReceivedCellId (Rel-9 or later) 173

7.3.2.2.27 CRLC\_Resume 173

7.3.2.2.27a CRLC\_RRC\_MessageSN 174

7.3.2.2.28 CRLC\_SecurityMode\_Config 174

7.3.2.2.28a CRLC\_SetRRC\_MessageSN 175

7.3.2.2.28b CRLC\_Set\_Count\_I 176

7.3.2.2.29 CRLC\_SequenceNumber 176

7.3.2.2.29a CRLC\_SendContinuousData\_TTI 177

7.3.2.2.30 CRLC\_Status 178

7.3.2.2.31 CRLC\_Suspend 178

7.3.2.2.31a CRLC\_MTCH\_Scheduling (Rel-6 or later) 179

7.3.2.2.32 CBMC\_Config 180

7.3.2.2.32b DEC\_PERbitstring 180

7.3.2.2.32c ENC\_PERbitstring 181

7.3.2.2.33 RLC\_TR\_DATA 181

7.3.2.2.34 RLC\_AM\_DATA 182

7.3.2.2.34a RLC\_UM\_ACCESSinfo (Rel-6 or later) 183

7.3.2.2.34b RLC\_UM\_CriticalMCCHMsg (Rel-6 or later) 184

7.3.2.2.34c RLC\_TR\_SeqOfRlcPdus 184

7.3.2.2.35 RLC\_UM\_DATA 185

7.3.2.2.35a RLC\_UM\_MSCH\_Msg (Rel-6 or later) 185

7.3.2.2.36 RLC\_TR\_MACesDATA\_IND (Rel-6 or later) 187

7.3.2.2.36a RLC\_TR\_MACisDATA\_IND (Rel-8 or later) 187

7.3.2.2.36b RLC\_TR\_MACisDATA\_ExtTSN\_IND (Rel-9 or later) 188

7.3.2.3 Specific ASP and IE definitions for 1.28 Mcps TDD (Rel-4 or later) 188

7.3.2.3.1 Specific ASP definitions 189

7.3.2.3.2 Specific IE definitions 199

7.3.3 TTCN primitives 215

7.3.3.1 UTRAN TTCN primitives 216

7.3.4 GERAN PCO and ASP definitions 218

7.3.4.1 PCO Type definitions 218

7.3.4.1.1 PCO type for data transmission and reception in GERAN 218

7.3.4.1.2 PCO type for configuration and control in GERAN 218

7.3.4.2 PCO definitions 218

7.3.4.2.1 PCOs for data transmission and reception in GERAN 218

7.3.4.2.2 PCOs for control primitives transmission and reception in GERAN 219

7.3.4.3 GERAN ASP Definitions 220

7.3.4.3.1 ASPs for data transmission and reception in GERAN 220

7.3.4.3.2 ASPs for control primitive transmission and reception in GERAN 231

7.3.5 A-GPS Upper tester, PCO and ASP definitions 244

7.3.5.1 Upper tester 244

7.3.5.2 SV PCO 244

7.3.5.3 A-GPS Primitives 244

7.3.5.3.1 Control ASP Type Definition 245

7.3.5.3.2 Data ASP Type Definition 245

7.3.6 ROHC test model and ASP 246

7.3.6.1 ROHC test method 246

7.3.6.2 ASP and PCO for control primitives transmission and reception 247

7.3.6.2.1 PCO definition 247

7.3.6.2.2 CPDCP\_Config 248

7.3.6.2.3 CPDCP\_ComProtocolControl 249

7.3.6.3 ASP and PCO for data transmission and reception 250

7.3.6.3.1 PCO definition 250

7.3.6.3.2 PDCP\_DATA 250

7.3.6.3.3 PDCP\_DL\_FeedBack 250

7.3.7 Handling RLP for CS non-transparent data 252

7.3.7.1 UTRAN cell 252

7.3.7.2 GERAN cell 254

7.3.7.3 ASP and PCO for control primitives 254

7.3.7.4 ASP and PCO for data transmission and reception 255

8 Design Considerations 257

8.1 Channel mapping 257

8.2 Channel and RB identity 257

8.2.1 Physical channels 262

8.2.2 Transport channels 263

8.2.2.1 Support of Default Configurations 263

8.2.3 Logical Channels 264

8.2.4 Radio bearers 264

8.2.5 Scrambling and channelization codes 267

8.2.6 MAC-d 271

8.2.6.1 MAC-d configuration examples 271

8.2.7 Configuration of compressed mode 272

8.2.7.1 UE Side 272

8.2.7.2 SS Side 272

8.2.8 Use of U-RNTI and C-RNTI 273

8.3 Channels configurations 273

8.3.1 Configuration of Cell\_FACH 273

8.3.1a Configuration of Cell\_FACH\_NoDedicated 274

8.3.2 Configuration of Cell\_DCH\_StandAloneSRB 275

8.3.3 Configuration of Cell\_DCH\_Speech 275

8.3.4 Configuration of Cell\_DCH\_64kCS\_RAB\_SRB 276

8.3.5 Configuration of Cell\_DCH\_57\_6kCS\_RAB\_SRB 277

8.3.6 Configuration of Cell\_RLC\_DCH\_RAB 278

8.3.7 Configuration of Cell\_FACH\_BMC 279

8.3.8 Configuration of PS Cell\_DCH\_64kPS\_RAB\_SRB and Cell\_PDCP\_AM\_RAB 280

8.3.9 Configuration of Cell\_Two\_DTCH 281

8.3.10 Configuration of Cell\_Single\_DTCH (CS) 281

8.3.11 Configuration of PS Cell\_PDCP\_UM\_RAB 282

8.3.12 Configuration of PS Cell\_PDCP\_AM\_UM\_RAB 283

8.3.13 Configuration of Cell\_2SCCPCH\_BMC 283

8.3.14 Configuration of Cell\_Four\_DTCH\_CS\_PS, Cell\_Four\_DTCH\_PS\_CS 285

8.3.14a Configuration of Cell\_Five\_DTCH\_CS\_PS 286

8.3.15 Configuration of Cell\_Two\_DTCH\_CS\_PS, Cell\_Two\_DTCH\_PS\_CS 287

8.3.16 Configuration of Cell\_Four\_DTCH\_CS 288

8.3.17 Configuration of Cell\_DCH\_MAC\_SRB 289

8.3.18 Configuration of Cell\_FACH\_MAC\_SRB 290

8.3.19 Configuration of Cell\_FACH\_MAC\_SRB0 291

8.3.20 Configuration of Cell\_FACH\_2SCCPCH\_StandAlonePCH 292

8.3.21 Configuration of PS Cell\_DCH\_2AM\_PS 292

8.3.21a Configuration of Cell\_DCH\_3AM\_PS 293

8.3.22 Configuration of PS Cell\_DCH\_2\_PS\_Call 294

8.3.23 Configuration of Cell\_FACH\_3\_SCCPCH\_4\_FACH\_Cnfg1 295

8.3.24 Configuration of Cell\_FACH\_3\_SCCPCH\_4\_FACH\_Cnfg2 296

8.3.25 Configuration of Cell\_FACH\_3\_SCCPCH\_3\_FACH\_CTCH 297

8.3.26 Configuration of PS Cell\_DCH\_DSCH\_PS\_RAB 298

8.3.27 Configuration of Cell\_DCH\_DSCH\_CS\_PS 298

8.3.28 Configuration of Cell\_FACH\_2SCCPCH\_StandAlonePCH\_2a 299

8.3.29 Configuration of Cell\_FACH\_3\_SCCPCH\_4\_FACH\_2a\_Cnfg1 300

8.3.30 Configuration of Cell\_FACH\_3\_SCCPCH\_4\_FACH\_2a\_Cnfg2 301

8.3.31 Configuration of Cell\_FACH\_3\_SCCPCH\_3\_FACH\_CTCH\_2a 302

8.3.32 Configuration of Cell\_DCH\_HS\_DSCH (Rel-5 or later) 303

8.3.32a Configuration of Cell\_DCH\_E\_DPCH\_PS 303

8.3.33 Configuration of cell\_One\_DTCH\_HS\_DSCH\_MAC (Rel-5 or later) 304

8.3.33a Configuration of cell\_Three\_DTCH\_1Q\_HS\_DSCH\_MAC (Rel-7 or later) 305

8.3.33b Configuration of cell\_Three\_DTCH\_3Q\_HS\_DSCH\_MAC (Rel-7 or later) 306

8.3.33c Configuration of Cell\_E\_HS\_SRB\_MAC\_TM\_RAB (Rel-7 or later) 307

8.3.34 Configuration of Cell\_2UM\_3AM\_DCH\_HS\_DSCH (Rel-5 or later) 308

8.3.35 Configuration of Cell\_DCH\_Speech\_WAMR (Rel-5 or later) 309

8.3.36 Configuration of PS Cell\_Four\_DTCH\_HS\_CS and Cell\_Four\_DTCH\_CS\_HS (Rel-5 or later) 310

8.3.37 Configuration of PS Cell\_Two\_DTCH\_HS\_CS (Rel-5 or later) 310

8.3.38 Configuration of PS Cell\_DCH\_64kPS\_RAB\_SRB\_HS (Rel-5 or later) 311

8.3.39 Configuration of PS Cell\_DCH\_2AM\_HS\_DSCH (Rel-5 or later) 312

8.3.39a Configuration of Cell\_DCH\_2AM\_E\_DPCH 312

8.3.40 Configuration of Cell\_Three\_DTCH\_5SRB (Rel-5 or later) 315

8.3.41 Configuration of Cell\_Five\_DTCH\_CS\_HS (Rel-5 or later) 316

8.3.41a Configuration of Cell\_FiveDTCH\_E\_DPCH 317

8.3.42 Configuration of Cell\_DCH\_E\_HS (Rel-6 or later) 318

8.3.43 Configuration of Cell\_DCH\_dlSRB\_E\_HS (Rel-6 or later) 318

8.3.44 Configuration of Cell\_E\_HS (Rel-6 or later) 319

8.3.45 Configuration of PS Cell\_Four\_DTCH\_E\_HS\_CS and Cell\_Four\_DTCH\_CS\_E\_HS (Rel-6 or later) 319

8.3.45a Configuration of Cell\_FourDTCH\_E\_DPCH 320

8.3.46 Configuration of Cell\_2DCH\_2AM\_dlSRB\_E\_HS (Rel-6 or later) 321

8.3.47 Configuration of Cell\_E\_HS\_MAC\_TM\_RAB (Rel-6 or later) 322

8.3.48 Configuration of Cell\_2DCH\_MAC\_2TM\_dlSRB\_E\_HS (Rel-6 or later) 322

8.3.49 Configuration of Cell\_2DCH\_1AM\_1UM\_E\_HS (Rel-6 or later) 323

8.3.50 Configuration of Cell\_3DCH\_2AM\_1UM\_E\_HS (Rel-6 or later) 324

8.3.51 Configuration of Cell\_Four\_DTCH\_CS\_E\_HS\_5SRB (Rel-6 or later) 325

8.3.52 Configuration of Cell\_Four\_DTCH\_HS\_5SRB (Rel-5 or later) 325

8.3.53 Configuration of Cell\_E\_HS\_StandAloneSRB/ Cell\_E\_HS\_StandAloneSRB\_NoConn (Rel-6 or later) 327

8.3.54 MBMS channel configuration (Rel-6 or later) 328

8.3.54.1 Configuration cell\_MBMS\_MCCH (Rel-6 or later) 328

8.3.54.2 Configuration cell\_MBMS\_MCCH\_One\_MTCH (Rel-6 or later) 328

8.3.55 Configuration of PS Cell\_DCH\_64kPS\_AM\_RAB 329

8.3.56 Configuration of PS Cell\_MBMS\_PTPRB 330

8.3.57 Configuration of PS Cell\_MBMS\_PTPRB\_AM 330

8.3.58 Configuration of Cell\_FACH\_MCCH\_SRB / Cell\_FACH\_MCCH\_NoDedicated 331

8.3.59 Configuration of Cell\_DCH\_MCCH\_PS 332

8.3.60 Configuration of PS Cell\_DCH\_1AM\_2AM\_HS\_DSCH (Rel-6 or later) 352

8.3.61 Configuration of Cell\_FACH\_enhDL\_PCH (Rel-7 or later) 352

8.3.62 Configuration of Cell\_FACH\_enhDL\_PS (Rel-7 or later) 353

8.3.63 Configuration of Cell\_E\_HS\_UM (Rel-7 or later) 354

8.3.64 Configuration of Cell\_FACH\_enhDL\_SRB (Rel-7 or later) 355

8.3.65 Configuration of Cell\_DCH\_3TM\_dlSRB\_E\_HS (Rel-8 or later) 356

8.3.66 Configuration of Cell\_E\_HS\_TM (Rel-8 or later) 357

8.3.67 Dual cell configurations (Rel-8 or later) 357

8.3.67.1 Configuration of cell\_SecondaryDualCell\_SRB (Rel-8 or later) 357

8.3.67.2 Configuration of cell\_SecondaryDualCell\_RAB (Rel-8 or later) 358

8.3.67.3 Configuration of cell\_SecondaryDualCell\_2RAB (Rel-8 or later) 358

8.3.67.4 Void 359

8.3.67.5 Configuration of cell\_SecondaryDCU\_SRB\_2TM (Rel-9 or later) 359

8.3.67.6 Configuration of cell\_SecondaryDCU\_SRB\_RAB (Rel-9 or later) 360

8.3.67.7 Configuration of cell\_SecondaryDCU\_SRB\_TM (Rel-9 or later) 360

8.3.68 Enhanced FACH Uplink configurations (Rel-8 or later) 361

8.3.68.1 Configuration of Cell\_FACH\_UL\_SRB (Rel-8 or later) 361

8.3.68.2 Configuration of Cell\_FACH\_UL\_PS (Rel-8 or later) 361

8.3.68.3 Configuration of Cell\_FACH\_UL\_TM\_PS (Rel-8 or later) 362

8.3.68.4 Configuration of Cell\_FACH\_UL\_NoDedicated (Rel-8 or later) 363

8.3.68.5 Configuration of Cell\_FACH\_UL\_FallBack (Rel-11 or later) 363

8.3.68.6 Configuration of Cell\_FACH\_UL\_SRB\_NoConn (Rel-8 or later) 363

8.3.69 Configuration of Cell\_FACH\_2\_SCCPCH\_CTCHenhDL\_PS (Rel-8 or later) 365

8.3.70 Configuration of Cell\_FACH\_2\_SCCPCH\_CTCHenhDL\_PCH (Rel-8 or later) 366

8.3.71 Configuration of Cell\_FACH\_HS (rel-7 or later) 366

8.3.72 Configuration of Cell\_E\_HS\_MAC\_TM\_dlSRB (Rel-9 or later) 367

8.3.73 Configuration of Cell\_E\_HS\_2TM (Rel-9 or later) 368

8.3.74 Configuration of Cell\_DCH\_E\_HS\_TM\_RAB (Rel-11 or later) 369

8.4 System information blocks scheduling 370

8.4.1 Grouping SIBs for testing 370

8.4.2 SIB configurations 370

8.4.3 Test SIB default schedule 370

8.4.3.1 Test SIB schedule for idle mode, measurement and Inter-RAT UTRAN to GERAN test cases 370

8.4.4 Test SIB special schedule 370

8.4.4.1 Test SIB schedule for two S-CCPCH or two PRACH 370

8.4.4.2 Test SIB schedule for Inter-Rat Handover from GERAN to UTRAN Test 370

8.4.5 Handling the transmission of SIB 370

8.4.5.1 Delivery of System Information content 371

8.4.5.2 Scheduling of system Information blocks 371

8.4.5.3 Example of usage 371

8.5 Security in testing 354

8.5.1 Authentication 354

8.5.2 Ciphering 354

8.5.3 Integrity 356

8.5.4 Test security scenarios 356

8.5.4.1 Start security function 357

8.5.4.1.1 Start integrity protection without start of ciphering 357

8.5.4.1.2 Start both integrity protection and ciphering 357

8.5.4.1.3 Void 358

8.5.4.2 RB setup 358

8.5.4.2.1 AM / UM RB 358

8.5.4.2.2 TM RB 359

8.5.4.3 RB Reconfiguration for AM RAB modification of RLC size 360

8.5.4.3.1 "RB mapping info" in CELL UPDATE CONFIRM 360

8.5.4.3.2 "RB mapping info" in RB RECONFIGURATION / RELEASE 360

8.5.4.4 Security modification 360

8.5.4.4.1 Integrity started, ciphering not started 361

8.5.4.4.2 Integrity and ciphering started 361

8.5.4.5 SRNS relocation 362

8.5.4.5.1 Void 362

8.5.4.5.2 Presence of "Integrity protection mode info" but absence of "Ciphering mode info" 362

8.5.4.5**.**3 Presence of "Integrity protection mode info" and "Ciphering mode info" IE 365

8.5.4.6 CELL/URA update 368

8.5.4.6.1 RLC re-establish (RB2, RB3, RB4) 368

8.5.4.6.2 RLC re-establish (RAB) 369

8.5.4.7 Inter RAT handover to UTRAN 369

8.5.4.7.1 ciphering has not been activated 369

8.5.4.7.2 ciphering has been activated 370

8.5.4.8 Hard handover 370

8.5.5 Test USIM configurations 371

8.5.5.1 Test USIM for Idle mode tests 371

8.6 Downlink power setting in SS 375

8.7 TTCN-2 Test suite operation definitions 375

8.7.1 Test suite operation definitions in the common modules 375

8.7.1.1 Specific test suite operation for RLC defined in BasicM 388

8.7.1.1.1 Pseudocode in a C like notation 388

8.7.2 Specific test suite operation definitions for Multi RAT Handover testing 390

8.7.3 Specific test suite operation for Multi RAB testing 394

8.7.4 Specific test suite operation for InterSystem Handover testing 395

8.7.5 Specific test suite operation for RAB\_HS testing 395

8.7.6 Specific test suite operation for Intersystem HS Testing 397

8.7.7 Specific test suite operation for A-GPS testing 398

8.7.8 Specific test suite operation for E-DCH Testing 401

8.7.9 Specific test suite operation for E-DCH/HS-ENH and MBMS testing 402

8.7.10 Specific test suite operation for CMAS testing 408

8.8 AT commands 409

8.8.1 AT command lists in TTCN-2 ATSs 410

8.8.1.1 AT commands in IR\_U ATS: 410

8.8.1.2 AT commands in MAC and RLC ATS: 410

8.8.1.3 AT commands in NAS ATS: 411

8.8.1.4 AT commands in RAB ATS: 412

8.8.1.5 AT commands in RRC ATS: 413

8.8.1.6 AT commands SMS ATS: 414

8.8.1.7 AT commands in HSDPA ATS (Rel-5 or later): 415

8.8.1.8 AT commands for E-DCH testing (Rel-6 or later) and HS-ENH testing (Rel-7 or later) 416

8.8.2 TTCN-2 AT Command Handling in TTCN 416

8.8.2.1 AT Command Interface 416

8.8.2.2 AT Command Dialogues 417

8.8.2.3 AT Response Types 417

8.8.2.3.1 'OK' Response 417

8.8.2.3.2 Name String 417

8.8.2.3.3 Error strings 417

8.8.2.4 AT Command Parameters And Options 417

8.9 Bit padding 418

8.9.1 Requirements for implementation 418

8.10 Test PDP contexts 418

8.10.1 Mapping of Quality of service and AT command for HSPA DL testing 420

8.10.1a Mapping of Quality of service and AT command for LCR TDD HSPA DL testing 422

8.10.2 Mapping of Quality of service and AT command for HSPA UL testing 423

8.10.2a Mapping of Quality of service and AT command for LCR TDD HSPA UL testing 424

8.10.3 Peak Throughput Class for HSPA testing 424

8.11 DCH-DSCH Configurations 425

8.11a DCH with HS-DSCH Configurations (Rel-5 or later) 426

8.11aa HS-DSCH Configurations without DCH associated (Rel-6 or later) 428

8.11b HS-DSCH Configuration Verification 431

8.11c HS-DSCH Configurations for enhanced Cell FACH (Rel-7 or later) [Mapping CCCH/BCCH/PCCH on HS-DSCH] 431

8.12 Pre- and postambles for GERAN to UTRAN tests 432

8.12.1 Preamble for GERAN to UTRAN tests 432

8.12.2 Postamble for GERAN to UTRAN tests 432

8.12.2.1 GERAN to UTRAN handover in CS 432

8.12.2.2 GERAN to UTRAN cell change in PS (in PMM-CONNECTED) 433

8.12.2.3 GERAN to UTRAN DTM test cases 434

8.13 E-DCH configurations (Rel-6 or later) 435

8.13.1 DPCH (SRB) and E-DCH (RAB) configuration 435

8.13.1.1 Serving E-DCH cell 435

8.13.1.2 SHO - addition of E-DCH RL in a serving RL cell (intra node B) 437

8.13.1.3 SHO – addition of E-DCH RL in a non-serving RL cell (inter node B) 438

8.13.2 DPCH/HS-DSCH/E-DCH setup and release order 439

8.13.3 Serving E-DCH cell with UL DTX Configured [Rel-7] 439

8.13.4 E-DCH configuration for enhanced Cell\_FACH uplink (Rel-8 or later) 440

8.13.4.1 E-DCH configuration at cell creation 440

8.13.4.2 E-DCH reconfiguration during signalling connection establishment 442

8.13.4.3 E-DCH reconfiguration during radio bearer establishment 443

8.14 Guidelines of MBMS implementations 443

8.14.1 MCCH scheduling implementation 443

8.14.2 MSCH scheduling and service data on MTCH 445

8.14.2.1 Scheduled service data on MTCH without MSCH configured 446

8.15 Cell mapping 447

8.16 Guidelines for CS voice over HSPA implementation 448

8.17 Cell Timing 449

Annex A (normative): Abstract Test Suites (ATS) 450

A.1 Version of specifications 450

A.2 NAS TTCN-2 ATS 450

A.2.1 Void 453

A.2.2 The TTCN Machine Processable form (TTCN.MP) 453

A.3 SMS TTCN-2 ATS 453

A.3.1 Void 454

A.3.2 The TTCN Machine Processable form (TTCN.MP) 454

A.4 RRC TTCN-2 ATS 454

A.4.1 Void 459

A.4.2 The TTCN Machine Processable form (TTCN.MP) 459

A.5 RLC TTCN-2 ATS 459

A.5.1 Void 460

A.5.2 The TTCN Machine Processable form (TTCN.MP) 460

A.6 MAC TTCN-2 ATS 460

A.6.1 Void 460

A.6.2 The TTCN Machine Processable form (TTCN.MP) 460

A.7 BMC TTCN-2 ATS 460

A.7.1 Void 460

A.7.2 The TTCN Machine Processable form (TTCN.MP) 460

A.8 PDCP TTCN-2 ATS 461

A.8.1 Void 461

A.8.2 The TTCN Machine Processable form (TTCN.MP) 461

A.9 RAB TTCN-2 ATS 461

A.9.1 Void 463

A.9.2 The TTCN Machine Processable form (TTCN.MP) 463

A.10 IR\_U TTCN-2 ATS 463

A.10.1 Void 464

A.10.2 The TTCN Machine Processable form (TTCN.MP) 464

A.11 AGPS TTCN-2 ATS 465

A.11.1 Void 465

A.11.2 The TTCN Machine Processable form (TTCN.MP) 465

A.12 HSD\_ENH TTCN-2 ATS 465

A.12.1 Void 468

A.12.2 The TTCN Machine Processable form (TTCN.MP) 468

A.13 HSU\_ENH TTCN-2 ATS 468

A.13.1 Void 470

A.13.2 The TTCN Machine Processable form (TTCN.MP) 470

A.14 MBMS TTCN-2 ATS 471

A.14.1 Void 472

A.14.2 The TTCN Machine Processable form (TTCN.MP) 472

A.15 HSPA7\_ENH TTCN-2 ATS 472

A.15.1 Void 475

A.15.2 The TTCN Machine Processable form (TTCN.MP) 475

A.16 HSPA8\_ENH TTCN-2 ATS 476

A.16.1 Void 478

A.16.2 The TTCN Machine Processable form (TTCN.MP) 478

A.17 HSPA9\_ENH TTCN-2 ATS 478

A.17.1 Void 479

A.17.2 The TTCN Machine Processable form (TTCN.MP) 479

A.18 UTRAN TTCN-3 TS 479

Annex B (normative): Partial IXIT proforma 483

B.0 Introduction 483

B.1 Parameter values 483

B.1.1 BasicM test suite parameter declarations 483

B.1.2 L3M test suite parameters declarations 486

B.1.3 NAS test suite parameters declarations 488

B.1.4 SMS test suite parameters declarations 488

B.1.5 RRC\_M test suite parameters declarations 489

B.1.6 PDCP test suite parameters declarations 490

B.1.7 BMC test suite parameters declarations 491

B.1.8 RRC test suite parameters declarations 491

B.1.9 RAB test suite parameters declarations 492

B.1.10 RLC and MAC test suite parameters declarations 492

B.1.11 Multi RAT test suite parameters declarations 493

B.1.12 MMI questions 494

B.1.13 A-GPS test suite parameters declarations 496

B.1.14 HSD\_ENH test suite parameters declarations 496

B.1.15 HSU\_ENH test suite parameters declarations 497

B.1.16 HS\_ENH test suite parameters declarations 497

B.1.17 Audit capabilities test suite parameters declarations 498

B.1.18 eCall and HSPA8 test suite parameters declarations 502

B.1.19 IR\_U test suite parameters declarations 503

B.1.20 TTCN-3 test suite parameters declarations 503

Annex C (informative): Additional information to IXIT 504

C.1 Identification Summary 504

C.2 Abstract Test Suite Summary 504

C.3 Test Laboratory 505

C.3.1 Test Laboratory Identification 505

C.3.2 Accreditation status of the test service 505

C.3.3 Manager of Test Laboratory 505

C.3.4 Contact person of Test Laboratory 505

C.3.5 Means of Testing 506

C.3.6 Instructions for Completion 506

C.4 Client 507

C.4.1 Client Identification 507

C.4.2 Client Test Manager 507

C.4.3 Client Contact person 508

C.4.4 Test Facilities Required 508

C.5 System Under Test 509

C.5.1 SUT Information 509

C.5.2 Limitations of the SUT 509

C.5.3 Environmental Conditions 510

C.6 Ancillary Protocols 510

C.6.1 Ancillary Protocols 1 510

C.6.2 Ancillary Protocols 2 511

Annex D (informative): PCTR Proforma 512

Annex E (informative): TTCN style guide for 3GPP ATS 513

E.1 Introduction 513

E.2 ETR 141 rules and applicability 513

E.2.1 Multiple words are separated by upper case letters at the start of each word 514

E.2.2 Identifiers shall be protocol standard aligned 515

E.2.3 Identifiers shall be distinguishing (use of prefixes) 516

E.2.4 Identifiers should not be too long (use standard abbreviations) 518

E.2.5 Test suite operations must not use global data 521

E.3 3GPP ATS implementation guidelines 525

E.3.1 Test case groups shall reflect the TSS&TP document 525

E.3.2 Test case names correspond to the clause number in the prose 525

E.3.3 Use standard template for test case and test step header 526

E.3.4 Do not use identical tags in nested CHOICE constructions 527

E.3.5 Incorrect usage of enumerations 528

E.3.6 Structured type as OCTETSTRING should not be used 528

E.3.7 Wildcards in PDU constraints for structured types should not be used 528

E.3.8 TSOs should be passed as many parameters as meaningful to facilitate their implementation 529

E.3.9 Specification of Encoding rules and variation should be indicated 530

E.3.10 Use of global data should be limited 530

E.3.11 Limit ATS scope to a single layer / sub-layer 530

E.3.12 Place system information in specially designed data structures 530

E.3.13 Place channel configuration in specially designed data structures 530

E.3.14 PICS / PIXIT parameters 530

E.3.15 Dynamic vs. static choices 531

E.3.16 Definition of Pre-Ambles and Post Ambles 531

E.3.17 Use test steps to encapsulate AT and MMI commands 532

E.3.18 Use system failure guard timers 532

E.3.19 Mapping between prose specification and individual test cases 532

E.3.20 Verdict assignment 532

E.3.20.1 General 532

E.3.20.2 Test cases 533

E.3.20.3 Test steps 534

E.3.20.4 Defaults 535

E.3.21 Test suite and test case variables 535

E.3.22 Use of macros is forbidden 536

E.3.23 Support for future Radio Access Technologies 536

E.3.24 Managing multiple representations of the same information 536

E.3.24.1 Predefined types 536

E.3.24.2 Simple types 537

E.3.24.3 Structured types 538

E.3.24.4 Conversion responsibility 538

E.3.24.5 Option 1: Calling party conversions 539

E.3.24.5.1 Advantages 539

E.3.24.5.2 Disadvantages 539

E.3.24.6 Option 2: Called party conversions 539

E.3.24.6.1 Advantages 539

E.3.24.6.2 Disadvantages 539

E.3.25 Assignment using constraint 539

E.3.26 Guidelines for use of timers when tolerances are applicable 539

E.3.26.1 Specific situations 539

E.3.26.2 Example situations 540

E.3.26.2.1 Example of situation 1 540

E.3.26.2.2 Example of situation 2 541

E.3.26.2.3 Example of situation 3 541

Annex F (informative): Void 542

Annex G (informative): Recommendation of an unique ICS/IXIT electronic exchange format 543

G.1 Syntax 543

G.2 Examples 544

Annex H (informative): A-GPS and Supplementary Services ASN.1 modules 545

H.1 A-GPS ASN.1 modules 545

H.2 SS and A-GNSS ASN.1 modules 556

H.2.1 Encoding information 556

H.2.2 TCAP-Definitions ASN.1 module 556

H.2.3 TCAP-Definitions-Para ASN.1 module 558

H.2.4 LCS-Definitions-Arguments ASN.1 module 561

H.2.5 SS-Definitions-Arguments ASN.1 module 569

H.2.6 Common-Definitions ASN.1 module 576

Annex I (Informative): Guidance on test execution 577

I.1 Void 577

I.2 FDD test execution on different frequency bands 577

I.2.1 FDD Band VI, XIII, IX, XIV 577

I.2.2 FDD Band XII, XIX, XX, XXI 577

I.2.3 FDD Band XXXII 578

I.3 Void 578

I.4 Void 578

Annex J (informative): Change history 579