3GPP TS 36.117 V16.0.0 (2020-06)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Radio Access Network;

Evolved Universal Terrestrial Radio Access (E-UTRA);

Relay conformance testing

(Release 16)

** 

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.  
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.  
This Report is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword [7](#__RefHeading___Toc528249851)

1 Scope [8](#__RefHeading___Toc528249852)

2 References [8](#__RefHeading___Toc528249853)

3 Definitions, symbols and abbreviations [8](#__RefHeading___Toc528249854)

3.1 Definitions [8](#__RefHeading___Toc528249855)

3.2 Symbols [9](#__RefHeading___Toc528249856)

3.3 Abbreviations [9](#__RefHeading___Toc528249857)

4. General test conditions and declarations [10](#__RefHeading___Toc528249858)

4.1 Measurement uncertainties and Test Requirements [11](#__RefHeading___Toc528249859)

4.1.1 General [11](#__RefHeading___Toc528249860)

4.1.2 Acceptable uncertainty of Test System [11](#__RefHeading___Toc528249861)

4.1.2.1 Measurement of relay access transmitter [11](#__RefHeading___Toc528249862)

4.1.2.2 Measurement of relay access receiver [11](#__RefHeading___Toc528249863)

4.1.2.3 Measurement of performance requirement [11](#__RefHeading___Toc528249864)

4.2 Relay classes [11](#__RefHeading___Toc528249865)

4.3 Regional requirements [11](#__RefHeading___Toc528249866)

4.4 Selection of configurations for testing [12](#__RefHeading___Toc528249867)

4.5 Manufacturer's declarations of regional and optional requirements [12](#__RefHeading___Toc528249868)

4.6 Specified frequency range and supported channel bandwidth [12](#__RefHeading___Toc528249869)

4.7 Format and interpretation of tests [12](#__RefHeading___Toc528249870)

5 Operating bands and Channel arrangement [13](#__RefHeading___Toc528249871)

5.1 General [13](#__RefHeading___Toc528249872)

5.2 Operating bands [13](#__RefHeading___Toc528249873)

5.3 Channel bandwidth [13](#__RefHeading___Toc528249874)

5.4 Channel arrangement [13](#__RefHeading___Toc528249875)

6. Transmitter characteristics [13](#__RefHeading___Toc528249876)

6.1 General [13](#__RefHeading___Toc528249877)

6.1.1 E-UTRA Test Models [13](#__RefHeading___Toc528249878)

6.2 Output power [14](#__RefHeading___Toc528249879)

6.2.1 Definition and applicability [14](#__RefHeading___Toc528249880)

6.2.2 Minimum Requirement [14](#__RefHeading___Toc528249881)

6.2.3 Test purpose [15](#__RefHeading___Toc528249882)

6.2.4 Method of test [15](#__RefHeading___Toc528249883)

6.2.5 Test Requirements [15](#__RefHeading___Toc528249884)

6.2.6 Configured transmitted Power for backhaul link [16](#__RefHeading___Toc528249885)

6.3 Output power dynamics [16](#__RefHeading___Toc528249886)

6.3.1 Access Link Test Requirements. [16](#__RefHeading___Toc528249887)

6.3.1.1 RE Power control dynamic range [16](#__RefHeading___Toc528249888)

6.3.1.2 Total power dynamic range [16](#__RefHeading___Toc528249889)

6.3.1.3 Transmitter OFF power [16](#__RefHeading___Toc528249890)

6.3.1.4 Transmitter transient period [16](#__RefHeading___Toc528249891)

6.3.2 Backhaul Link Test Requirements [16](#__RefHeading___Toc528249892)

6.3.2.1 Minimum Output Power [16](#__RefHeading___Toc528249893)

6.3.2.1.1 Test purpose [16](#__RefHeading___Toc528249894)

6.3.2.1.2 Test applicability [16](#__RefHeading___Toc528249895)

6.3.2.1.3 Minimum conformance requirements [17](#__RefHeading___Toc528249896)

6.3.2.1.4 Test description [17](#__RefHeading___Toc528249897)

6.3.2.1.5 Test Requirement [17](#__RefHeading___Toc528249898)

6.3.2.2 Power Control Absolute power tolerance [17](#__RefHeading___Toc528249899)

6.3.2.3 Power Control Relative power tolerance [17](#__RefHeading___Toc528249900)

6.3.2.4 Aggregate power control tolerance [18](#__RefHeading___Toc528249901)

6.3.2.5 Power Control for UL-MIMO [18](#__RefHeading___Toc528249902)

6.3.2.6 Transmit ON/OFF Time Mask [18](#__RefHeading___Toc528249903)

6.3.2.7 Transmit OFF Power [18](#__RefHeading___Toc528249904)

6.3.2.7.1 Minimum requirement [18](#__RefHeading___Toc528249905)

6.3.2.7.2 Test requirement [18](#__RefHeading___Toc528249906)

6.4 Transmitted signal quality [19](#__RefHeading___Toc528249907)

6.4.1 Frequency error [19](#__RefHeading___Toc528249908)

6.4.1.1 Definition and applicability [19](#__RefHeading___Toc528249909)

6.4.1.2 Minimum Requirement [19](#__RefHeading___Toc528249910)

6.4.1.3 Test purpose [19](#__RefHeading___Toc528249911)

6.4.1.4 Method of test [19](#__RefHeading___Toc528249912)

6.4.1.5 Test requirement [19](#__RefHeading___Toc528249913)

6.4.2 EVM [19](#__RefHeading___Toc528249914)

6.4.3 Time alignment error [19](#__RefHeading___Toc528249915)

6.4.4 DL RS power [20](#__RefHeading___Toc528249916)

6.5 Unwanted emissions [20](#__RefHeading___Toc528249917)

6.5.1 Transmitter spurious emissions [20](#__RefHeading___Toc528249918)

6.5.2 Adjacent Channel Leakage power Ratio (ACLR) [20](#__RefHeading___Toc528249919)

6.5.3 Operating Bands Unwanted Emissions [20](#__RefHeading___Toc528249920)

6.5.3.1 Definition and applicability [20](#__RefHeading___Toc528249921)

6.5.3.2 Minimum Requirement [21](#__RefHeading___Toc528249922)

6.5.3.3 Test purpose [21](#__RefHeading___Toc528249923)

6.5.3.4 Method of test [21](#__RefHeading___Toc528249924)

6.5.3.5 Test Requirement [21](#__RefHeading___Toc528249925)

6.6 Transmitter intermodulation [24](#__RefHeading___Toc528249926)

7. Receiver characteristics [24](#__RefHeading___Toc528249927)

7.1 General [24](#__RefHeading___Toc528249928)

7.2 Reference sensitivity level [24](#__RefHeading___Toc528249929)

7.2.1 Backhaul link reference sensitivity [24](#__RefHeading___Toc528249930)

7.2.1.1 Test requirement [24](#__RefHeading___Toc528249931)

7.2.2 Access link reference sensitivity [25](#__RefHeading___Toc528249932)

7.3 Dynamic range [25](#__RefHeading___Toc528249933)

7.3.1 Backhaul link Maximum Input Level [25](#__RefHeading___Toc528249934)

7.3.2 Access link Receiver Dynamic Range [25](#__RefHeading___Toc528249935)

7.4 In-channel selectivity [25](#__RefHeading___Toc528249936)

7.5 Adjacent Channel Selectivity (ACS) [25](#__RefHeading___Toc528249937)

7.5.1 Backhaul Adjacent Channel Selectivity (ACS) [25](#__RefHeading___Toc528249938)

7.5.2 Access Link Adjacent Channel Selectivity (ACS) [26](#__RefHeading___Toc528249939)

7.6 Blocking characteristics [26](#__RefHeading___Toc528249940)

7.6.1 Backhaul Blocking Characteristics [26](#__RefHeading___Toc528249941)

7.6.2 Access Link Blocking Characteristics [26](#__RefHeading___Toc528249942)

7.6.3 Blocking requirements for co-location [26](#__RefHeading___Toc528249943)

7.7 Receiver spurious emissions [26](#__RefHeading___Toc528249944)

7.7.1 Backhaul Link Receiver Spurious Emissions [26](#__RefHeading___Toc528249945)

7.7.2 Access Link Receiver Spurious Emissions [26](#__RefHeading___Toc528249946)

7.8 Receiver intermodulation [26](#__RefHeading___Toc528249947)

7.8.1 Backhaul Link Receiver Intermodulation [26](#__RefHeading___Toc528249948)

7.8.2 Access Link Receiver Intermodulation [27](#__RefHeading___Toc528249949)

8. Access Performance requirement [27](#__RefHeading___Toc528249950)

8.1 General [27](#__RefHeading___Toc528249951)

8.2 Performance requirements for PUSCH [27](#__RefHeading___Toc528249952)

8.2.1 Requirements in multipath fading propagation conditions [27](#__RefHeading___Toc528249953)

8.2.2 Requirements for UL timing adjustment [27](#__RefHeading___Toc528249954)

8.2.3 Requirements for HARQ-ACK multiplexed on PUSCH [28](#__RefHeading___Toc528249955)

8.3 Performance requirements for PUCCH [28](#__RefHeading___Toc528249956)

8.3.1 ACK missed detection requirements for single user PUCCH format 1a [28](#__RefHeading___Toc528249957)

8.3.2 CQI missed detection requirements for PUCCH format2 [28](#__RefHeading___Toc528249958)

8.3.3 ACK missed detection requirements for multi user PUCCH format 1a [28](#__RefHeading___Toc528249959)

8.4 Performance requirements for PRACH [28](#__RefHeading___Toc528249960)

8.4.1 PRACH false alarm probability and missed detection [28](#__RefHeading___Toc528249961)

9. Backhaul Performance requirement [29](#__RefHeading___Toc528249962)

9.1 General [29](#__RefHeading___Toc528249963)

9.2 Demodulation of PDSCH (Cell-Specific Reference Symbols) [29](#__RefHeading___Toc528249964)

9.3 Demodulation of PDSCH (User-Specific Reference Symbols) [29](#__RefHeading___Toc528249965)

9.4 Demodulation of PDCCH/PCFICH [29](#__RefHeading___Toc528249966)

9.5 Demodulation of PHICH [29](#__RefHeading___Toc528249967)

9.6 Demodulation of PBCH [29](#__RefHeading___Toc528249968)

9.7 Sustained downlink data rate provided by lower layers [29](#__RefHeading___Toc528249969)

9.8 Demodulation of R-PDCCH [30](#__RefHeading___Toc528249970)

9.8.1 FDD [30](#__RefHeading___Toc528249971)

9.8.1.1 FDD R-PDCCH performance based on UE-specific reference signals transmitted on antenna port 7 with 1x2 antenna configuration [30](#__RefHeading___Toc528249972)

9.8.1.1.1 Test purpose [30](#__RefHeading___Toc528249973)

9.8.1.1.2 Test applicability [30](#__RefHeading___Toc528249974)

9.8.1.1.3 Minimum conformance requirements [30](#__RefHeading___Toc528249975)

9.8.1.1.4 Test description [31](#__RefHeading___Toc528249976)

9.8.1.1.4.1 Initial conditions [31](#__RefHeading___Toc528249977)

9.8.1.1.4.2 Test procedure [32](#__RefHeading___Toc528249978)

9.8.1.1.4.3 Message contents [32](#__RefHeading___Toc528249979)

9.8.1.1.5 Test requirement [34](#__RefHeading___Toc528249980)

9.8.1.2 FDD R-PDCCH performance based on UE-specific reference signals transmitted on antenna port 7 with 4x2 antenna configuration [35](#__RefHeading___Toc528249981)

9.8.1.2.1 Test purpose [35](#__RefHeading___Toc528249982)

9.8.1.2.2 Test applicability [35](#__RefHeading___Toc528249983)

9.8.1.2.3 Minimum conformance requirements [35](#__RefHeading___Toc528249984)

9.8.1.2.4 Test description [37](#__RefHeading___Toc528249985)

9.8.1.2.4.1 Initial conditions [37](#__RefHeading___Toc528249986)

9.8.1.2.4.2 Test procedure [37](#__RefHeading___Toc528249987)

9.8.1.2.4.3 Message contents [38](#__RefHeading___Toc528249988)

9.8.1.2.5 Test requirement [40](#__RefHeading___Toc528249989)

9.8.2 TDD [40](#__RefHeading___Toc528249990)

9.8.2.1 TDD R-PDCCH performance based on UE-specific reference signals transmitted on antenna port 7 with 1x2 antenna configuration [40](#__RefHeading___Toc528249991)

9.8.2.1.1 Test purpose [40](#__RefHeading___Toc528249992)

9.8.2.1.2 Test applicability [40](#__RefHeading___Toc528249993)

9.8.2.1.3 Minimum conformance requirements [40](#__RefHeading___Toc528249994)

9.8.2.1.4 Test description [41](#__RefHeading___Toc528249995)

9.8.2.1.4.1 Initial conditions [41](#__RefHeading___Toc528249996)

9.8.2.1.4.2 Test procedure [42](#__RefHeading___Toc528249997)

9.8.2.1.4.3 Message contents [42](#__RefHeading___Toc528249998)

9.8.2.1.5 Test requirement [44](#__RefHeading___Toc528249999)

9.8.2.2 TDD R-PDCCH performance based on UE-specific reference signals transmitted on antenna port 7 with 4x2 antenna configuration [45](#__RefHeading___Toc528250000)

9.8.2.2.1 Test purpose [45](#__RefHeading___Toc528250001)

9.8.2.2.2 Test applicability [45](#__RefHeading___Toc528250002)

9.8.2.2.3 Minimum conformance requirements [45](#__RefHeading___Toc528250003)

9.8.2.2.4 Test description [46](#__RefHeading___Toc528250004)

9.8.2.2.4.1 Initial conditions [46](#__RefHeading___Toc528250005)

9.8.2.2.4.2 Test procedure [47](#__RefHeading___Toc528250006)

9.8.2.2.4.3 Message contents [47](#__RefHeading___Toc528250007)

9.8.2.2.5 Test requirement [50](#__RefHeading___Toc528250008)

Annex A (normative): Propagation models for relay demodulation requirements [51](#__RefHeading___Toc528250009)

A.1 Propagation models for backhaul link [51](#__RefHeading___Toc528250010)

A.1.1 Delay Profiles [51](#__RefHeading___Toc528250011)

A.1.1.1 LOS between eNB and relay [51](#__RefHeading___Toc528250012)

A.1.1.2 NLOS between eNB and relay [51](#__RefHeading___Toc528250013)

A.1.2 Doppler Frequency [52](#__RefHeading___Toc528250014)

A.1.3 MIMO Correlation Matrices [52](#__RefHeading___Toc528250015)

A.2 multipath propagation fading conditions for access link [53](#__RefHeading___Toc528250016)

Annex B (normative): Reference Measurement Channel [55](#__RefHeading___Toc528250017)

B.1 Reference measurement channels for R-PDCCH performance requirements [55](#__RefHeading___Toc528250018)

B.1.1 R-PDCCH format without cross-interleaving [55](#__RefHeading___Toc528250019)

B.1.1.1 FDD [55](#__RefHeading___Toc528250020)

B.1.1.2 TDD [55](#__RefHeading___Toc528250021)

B.2 OCNG patterns for R-PDCCH performance requirements [55](#__RefHeading___Toc528250022)

B.2.1 FDD [56](#__RefHeading___Toc528250023)

B.2.1.1 OCNG FDD pattern 1for R-PDCCH [56](#__RefHeading___Toc528250024)

B.2.2 TDD [56](#__RefHeading___Toc528250025)

B.2.2.1 OCNG TDD pattern 1for R-PDCCH [56](#__RefHeading___Toc528250026)

Annex C (normative): Physical Channel Set-up for conformance tests [58](#__RefHeading___Toc528250027)

C.1 Set-up for R-PDCCH [58](#__RefHeading___Toc528250028)

C.2 Set-up for PDSCH [58](#__RefHeading___Toc528250029)

Annex D (informative): Change history [60](#__RefHeading___Toc528250030)

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# 1 Scope

The present document specifies the Radio Frequency (RF) test methods and conformance requirements for E-UTRA Relay. These have been derived from, and are consistent with the E-UTRA Relay specifications defined in [2].

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 36.116: "Evolved Universal Terrestrial Radio Access (E-UTRA); Relay radio transmission and reception".

[3] 3GPP TS 36.141: "Evolved Universal Terrestrial Radio Access (E-UTRA); Base Station (BS) Conformance Testing (Release 11)".

[4] 3GPP TS 36.104: "Evolved Universal Terrestrial Radio Access (E-UTRA); Base Station (BS) Radio Transmission and Reception (Release 11)".

[5] 3GPP TR 36.826: "Evolved Universal Terrestrial Radio Access (E-UTRA); Base Station (BS) Relay Radio Transmission and Reception".

[6] 3GPP TS 36.101: "User Equipment (UE) radio transmission and reception".

[7] 3GPP TS 36.521-1 "Evolved Universal Terrestrial Radio Access (E-UTRA) and Evolved Packet Core (EPC); User Equipment (UE) conformance specification; Part 1: Protocol conformance specification".

[8] 3GPP TS 36.508 "Evolved Universal Terrestrial Radio Access (E-UTRA) and Evolved Packet Core (EPC); Common test environments for User Equipment (UE) conformance testing".

[9] 3GPP TS 36.211: "Evolved Universal Terrestrial Radio Access (E-UTRA); Physical channels and modulation".

[10] 3GPP TS 36.213: "Evolved Universal Terrestrial Radio Access (E-UTRA); Physical layer procedures".

[11] 3GPP TS 36.331: "Evolved Universal Terrestrial Radio Access (E-UTRA); Radio Resource Control (RRC); Protocol specification".

# 3 Definitions, symbols and abbreviations

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in TR 21.905 [1].

**access link:** Link for communication between Relay and UE.

**backhaul link:** Link for communication between Relay and BS.

**carrier:** The modulated waveform conveying the E-UTRA or UTRA physical channels

**channel bandwidth:** The RF bandwidth supporting a single E-UTRA RF carrier with the transmission bandwidth configured in the uplink or downlink of a cell. The channel bandwidth is measured in MHz and is used as a reference for transmitter and receiver RF requirements.

**channel edge:** The lowest and highest frequency of the E-UTRA carrier, separated by the channel bandwidth.

**in-band relay:** A Relay where the access link and backhaul link operates in the same operating band.

**measurement bandwidth**: The bandwidth in which an emission level is specified.

**occupied bandwidth:** The width of a frequency band such that, below the lower and above the upper frequency limits, the mean powers emitted are each equal to a specified percentage β/2 of the total mean power of a given emission.

**RRC filtered mean power:** The mean power of a UTRA carrier as measured through a root raised cosine filter with roll-off factor  and a bandwidth equal to the chip rate of the radio access mode.

NOTE: The RRC filtered mean power of a perfectly modulated UTRA signal is 0.246 dB lower than the mean power of the same signal.

**transmission bandwidth:** Bandwidth of an instantaneous transmission from a UE or BS, measured in Resource Block units.

**transmission bandwidth configuration:** The highest transmission bandwidth allowed for uplink or downlink in a given channel bandwidth, measured in Resource Block units.

## 3.2 Symbols

For the purposes of the present document, the following symbols apply:

Pout Output Power

Pmax Maximum total output power

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in TR 21.905 [1].

ACLR Adjacent Channel Leakage Ratio

ACK Acknowledgement (in HARQ protocols)

ACS Adjacent Channel Selectivity

AWGN Additive White Gaussian Noise

BS Base Station

CP Cyclic prefix

CRC Cyclic Redundancy Check

CW Continuous Wave

DC Direct Current

DFT Discrete Fourier Transformation

DTX Discontinuous Transmission

DUT Device Under Test

DwPTS Downlink part of the special subframe (for TDD operation)

EARFCN E-UTRA Absolute Radio Frequency Channel Number

EPA Extended Pedestrian A model

ETU Extended Typical Urban model

E-UTRA Evolved UTRA

EVA Extended Vehicular A model

EVM Error Vector Magnitude

FDD Frequency Division Duplex

FFT Fast Fourier Transformation

FRC Fixed Reference Channel

GP Guard Period (for TDD operation)

HARQ Hybrid Automatic Repeat Request

HD-FDD Half- Duplex FDD

ICS In-Channel Selectivity

ITU‑R Radiocommunication Sector of the ITU

LA Local Area

MCS Modulation and Coding Scheme

MCL Minimum Coupling Loss

OFDM Orthogonal Frequency Division Multiplex

OOB Out-of-band

PA Power Amplifier

PBCH Physical Broadcast Channel

PDCCH Physical Downlink Control Channel

PDSCH Physical Downlink Shared Channel

PUSCH Physical Uplink Shared Channel

PUCCH Physical Uplink Control Channel

PRACH Physical Random Access Channel

PRAT Rated output power

PSS Primary Synchronization Signal

QAM Quadrature Amplitude Modulation

QPSK Quadrature Phase-Shift Keying

RAT Radio Access Technology

RB Resource Block

RE Resource Element

REFSENS Reference Sensitivity power level

RF Radio Frequency

RMS Root Mean Square (value)

R-PDCCH Relay Physical Downlink Control Channel

RS Reference Symbol

RX Receiver

RRC Root Raised Cosine

SNR Signal-to-Noise Ratio

SSS Secondary Synchronization Signal

TA Timing Advance

TDD Time Division Duplex

TX Transmitter

UE User Equipment

UMTS Universal Mobile Telecommunications System

UTRA UMTS Terrestrial Radio Access

UTRAN UMTS Terrestrial Radio Access Network

WA Wide Area

# 4. General test conditions and declarations

Many of the tests in this specification measure a parameter relative to a value that is not fully specified in the E-UTRA specifications. For these tests, the Minimum Requirement is determined relative to a nominal value specified by the manufacturer.

Certain functions of a relay are optional in the E-UTRA specifications. Furthermore some requirements for the relay may be regional as listed in clause 4.3.

When specified in a test, the manufacturer shall declare the nominal value of a parameter, or whether an option is supported.

## 4.1 Measurement uncertainties and Test Requirements

### 4.1.1 General

The requirements of this clause apply to all applicable tests in the present document.

The Minimum Requirements are given in 36.116 [2] except that they apply to a relay node and test requirements are given in this specification. Test Tolerances are defined in Annex G of TS 36.141 [3] and in Annex F of TS36.521-1 [7]. Test Tolerances are individually calculated for each test. The Test Tolerances are used to relax the Minimum Requirements in TS 36.116 [2] to create Test Requirements.

### 4.1.2 Acceptable uncertainty of Test System

The maximum acceptable uncertainty of the Test System is specified below for each test, where appropriate. The Test System shall enable the stimulus signals in the test case to be adjusted to within the specified tolerance and the equipment under test to be measured with an uncertainty not exceeding the specified values. All tolerances and uncertainties are absolute values, and are valid for a confidence level of 95%, unless otherwise stated.

A confidence level of 95% is the measurement uncertainty tolerance interval for a specific measurement that contains 95% of the performance of a population of test equipment.

For RF tests, it should be noted that the uncertainties in clause 4.1.2 apply to the Test System operating into a nominal 50 ohm load and do not include system effects due to mismatch between the DUT and the Test System.

#### 4.1.2.1 Measurement of relay access transmitter

The maximum test system uncertainty for relay access transmitter test shall be as defined in Table 4.1.2.1 of TS 36.141 [3] except that the requirements apply to relay nodes.

#### 4.1.2.2 Measurement of relay access receiver

The maximum test system uncertainty for relay access receiver tests shall be as defined in Table 4.1.2.2 of TS 36.141 [3] except that the requirements apply to relay nodes.

#### 4.1.2.3 Measurement of performance requirement

The maximum test system uncertainty for relay access performance requirementsshallbe as defined in Table 4.1.2.3 of TS 36.141 [3] except that the requirements apply to relay nodes.

## 4.2 Relay classes

The Relay classes are defined based on the RF scenarios expected for the Relay access deployment, defined in terms of the Minimum Coupling Loss (MCL) between Relay and UE. The following definitions are used:

- High-CL Relay are characterised by requirements derived from outdoor Relay scenarios with a Relay to UE minimum coupling loss equals to 59 dB

- Low-CL Relay are characterised by requirements derived from indoor Relay scenarios with a Relay to UE minimum coupling loss equals to 45 dB

## 4.3 Regional requirements

Some requirements in the present document may only apply in certain regions either as optional requirements or set by local and regional regulation as mandatory requirements. It is normally not stated in the 3GPP specifications under what exact circumstances that the requirements apply, since this is defined by local or regional regulation.

Table 4.3-1 of 36.141 [3] lists all the requirements that may be applied differently to relay nodes in different regions.

## 4.4 Selection of configurations for testing

The requirements for selection of configurations for testing shall be the same as in clauses 4.4 and 4.5 of TS 36.141 [3] except that the requirements shall apply to relay nodes.

## 4.5 Manufacturer's declarations of regional and optional requirements

The requirements for manufacturer's declarations of regional and optional requirements shall be the same as in clause 4.6 of TS 36.141 [3] except that the requirements shall apply to relay nodes.

## 4.6 Specified frequency range and supported channel bandwidth

The requirements for specified frequency range and supported channel bandwidth requirements shall be the same as in clause 4.6 of TS 36.141 [3] except that the requirements shall apply to relay nodes.

## 4.7 Format and interpretation of tests

Each test in the following clauses has a standard format:

**X Title**

All tests are applicable to all equipment within the scope of the present document, unless otherwise stated.

**X.1 Definition and applicability**

This subclause gives the general definition of the parameter under consideration and specifies whether the test is applicable to all equipment or only to a certain subset. Required manufacturer declarations may be included here.

**X.2 Minimum Requirement**

This subclause contains the reference to the subclause to the 3GPP reference (or core) specification which defines the Minimum Requirement.

**X.3 Test Purpose**

This subclause defines the purpose of the test.

**X.4 Method of test**

**X.4.1 Initial conditions**

This subclause defines the initial conditions for each test, including the test environment, the RF channels to be tested and the basic measurement set-up.

**X.4.2 Procedure**

This subclause describes the steps necessary to perform the test and provides further details of the test definition like point of access (e.g. test port), domain (e.g. frequency-span), range, weighting (e.g. bandwidth), and algorithms (e.g. averaging).

**X.5 Test Requirement**

This subclause defines the pass/fail criteria for the equipment under test. See subclause 4.1.2.5 Interpretation of measurement results.

# 5 Operating bands and Channel arrangement

## 5.1 General

The channel arrangements presented in this clause are based on the operating bands and channel bandwidths defined in the present release of specifications.

NOTE: Other operating bands and channel bandwidths may be considered in future releases.

## 5.2 Operating bands

E-UTRA is designed to operate in the operating bands defined in Table 5.5-1 of TS 36.104 [4].

## 5.3 Channel bandwidth

Requirements in the present document are specified for the channel bandwidths listed in Table 5.6-1 of TS 36.104 [4].

For the access link the manufacturer shall declare the channel bandwidths supported by the Relay.

For the backhaul link the Relay shall support the channel bandwidths denoted by "Yes" in Table 5.6.1-1 of TS 36.101 [6] for the supported operating band. Note 1 in Table 5.6.1-1 does not apply.

## 5.4 Channel arrangement

The channel spacing is specified in clause 5.7.1 of TS 36.104 [4].

The channel raster is specified in clause 5.7.2 of TS 36.104 [4].

Carrier frequency and EARFCN is specified in clause 5.7.3 of TS 36.104 [4].

# 6. Transmitter characteristics

## 6.1 General

General test conditions for transmitter tests are given in clause 4, including interpretation of measurement results and configurations for testing. Test configurations are defined in clause 4.5 of TS 36.141 [3] except that they apply to relays, while Annex H of TS 36.141 [3] provides an informative description of E-UTRAN test cases.

### 6.1.1 E-UTRA Test Models

The set-up of physical channels for the access transmitter tests shall be according to one of the E-UTRA test models (E-TM) defined in clause 6.1.1 of TS 36.141 [3] except that they apply to relay nodes.

The set-up of physical channels for the backhaul transmitter tests shall be according to one of the E-UTRA test models (E-TM) defined in clause 4.1 of TS 36.508 [8] except that they apply to relay nodes. The following reference test conditions shall apply

Test Environment: Normal, as defined in TS 36.508 [8] clause 4.1.

Frequencies to be tested: Mid Range, as defined in TS 36.508 [8] clause 4.3.1.1.

Channel Bandwidths to be tested: 10MHz, as defined in TS 36.508 [8] clause 4.3.1.1.

## 6.2 Output power

### 6.2.1 Definition and applicability

Output power, Pout, of the relay is the mean power of one carrier delivered to a load with resistance equal to the nominal load impedance of the transmitter.

The maximum total output power (Pmax), of the relay is the mean power level measured at the antenna connector during the transmitter ON period in a specified reference condition.

Rated total output power of the relay is the mean power for relay operating in single carrier or multiple carrier configurations that the manufacturer has declared to be available at the antenna connector during the transmitter ON period.

Relay maximum output power (Pmax, c), of the relay is the mean power level per carrier measured at the antenna connector during the transmitter ON period in a specified reference condition.

The rated output power, PRAT, is the mean power level that the manufacturer has declared to be available at the antenna connector during the transmitter ON period.

NOTE: Different PRATs may be declared for different configurations

In certain regions, the minimum requirement for normal conditions may apply also for some conditions outside the ranges defined for the Normal test environment in Annex D of TS 36.141 [3].

Two power classes are defined for relay access link and single power class is defined for relay backhaul link, where the rated output power, PRAT, shall be as specified in Table 6.2.1-2 and Table 6.2.1-3.

Table 6.2.1-1: Void

Table 6.2.1-2: Relay access link rated output power

|  |  |
| --- | --- |
| Access link Power class | PRAT [dBm] |
| Power class 1 | ≤ +24 (for one transmit antenna port)  ≤ +21 (for two transmit antenna ports)  ≤ +18 (for four transmit antenna ports)  ≤ +15 (for eight transmit antenna ports) |
| Power class 2 | ≤ +30 (for one transmit antenna port)  ≤ +27 (for two transmit antenna ports)  ≤ +24 (for four transmit antenna ports)  ≤ +21 (for eight transmit antenna ports) |

Table 6.2.1-3: Relay backhaul link rated output power

|  |  |
| --- | --- |
| Backhaul link Power class | PRAT [dBm] |
| Power class 1 | ≤ +24 (for one transmit antenna port)  ≤ +21 (for two transmit antenna ports)  ≤ +18 (for four transmit antenna ports) |

NOTE: For coexistence with a victim base station a minimum MCL should be met in all scenarios. This is particularly relevant for use cases where relays are placed wall mounted or in rooftops. The value for this MCL is 45 dB.

### 6.2.2 Minimum Requirement

The minimum requirement is defined in TS 36.116 [2] clause 6.2.1.1.

### 6.2.3 Test purpose

The test purpose is to verify the accuracy of the maximum output power across the frequency range and under normal and extreme conditions for all transmitters in the relay node.

### 6.2.4 Method of test

The requirements for method of test for the relay access link maximum output power shall be the same as in clause 6.2.4 of TS 36.141 [3] except that the requirements shall apply to relay nodes.

The requirements for method of test for the relay backhaul link maximum output power shall be the same as in clause 6.2.2.4 of TS 36.521 [7] except that the requirements shall apply to relay nodes.

### 6.2.5 Test Requirements

Test Requirements for the relay access link shall be the same as defined in Table 6.2.5-1

Table 6.2.5-1: Relay Rated output power

|  |  |  |  |
| --- | --- | --- | --- |
| Relay power class | PRAT | Minimum requirement Tolerance in TS 36.116 [dB] for  normal conditions | Test requirements in  TS 36.117 [dB]  Tolerance [dB] for  extreme conditions |
| Power class 1 | ≤+ 24 dBm (for one transmit antenna port)  ≤+ 21 dBm (for two transmit antenna ports)  ≤+ 18 dBm (for four transmit antenna ports)  ≤+ 15 dBm (for eight transmit antenna ports) | In normal conditions: within ±2 dB of manufacturer's rated output power  In extreme conditions:  within ±2.5 dB of manufacturer's rated output power | In normal conditions: within +2.7 dB and -2.7 dB of the manufacturer's rated output power, f ≤ 3.0GHz;  within +3.0 dB and -3.0 dB of the manufacturer's rated output power, 3.0 GHz < f ≤ 4.2 GHz  In extreme conditions:  within +3.2 dB and -3.2 dB of the manufacturer's rated output power, f ≤ 3.0 GHz  within +3.5 dB and -3.5 dB of the manufacturer's rated output power, 3.0 GHz < f ≤ 4.2 GHz |
| Power class 2 | ≤+ 30 dBm (for one transmit antenna port)  ≤+27 dBm (for two transmit antenna ports)  ≤+ 24dBm (for four transmit antenna ports) \*  ≤+ 21dBm (for eight transmit antenna ports)\* | In normal conditions: within ±2 dB of manufacturer's rated output power  In extreme conditions:  within ±2.5 dB of manufacturer's rated output power | In normal conditions: within +2.7 dB and -2.7 dB of the manufacturer's rated output power, f ≤ 3.0 GHz  within +3.0 dB and -3.0 dB of the manufacturer's rated output power, 3.0 GHz < f ≤ 4.2 GHz  In extreme conditions:  within +3.2 dB and -3.2 dB of the manufacturer's rated output power, f ≤ 3.0 GHz  within +3.5 dB and -3.5 dB of the manufacturer's rated output power, 3.0 GHz < f ≤ 4.2 GHz |

In certain regions, the minimum requirement for normal conditions may apply also for some conditions outside the range of conditions defined as normal.

For the backhaul link the minimum test requirements of Power Class 1 in Table 6.2.5-1 shall apply.

### 6.2.6 Configured transmitted Power for backhaul link

The Relay backhaul link is allowed to set its configured maximum output power PCMAX. The configured maximum output power PCMAX is set within the following bounds:

- PCMAX = MIN { PEMAX, PRAT }.

- PEMAX is the value given to IE *P-Max*, defined in TS 36.331.

- PRAT is the Relay rated output power specified in Table 6.2.1-2 and Table 6.2.1-3 without taking into account the tolerance specified in the Table 6.2.2.1-1 of TS 36.116 [2].

. The minimum requirement is defined in TS 36.116 [2], clause 6.2.2.1.

The requirements for method of test for the relay backhaul link maximum output power shall be the same as in clause 6.2.5 of TS 36.521 [7] except that the requirements shall apply to relay nodes and the reference measurement channel for R-PDCCH defined in Annex B of TS 36.116 [2] shall apply for R-PDCCH .

## 6.3 Output power dynamics

### 6.3.1 Access Link Test Requirements.

#### 6.3.1.1 RE Power control dynamic range

The RE Power control dynamic range test requirements for the relay access link shall be the same as in clause 6.3.1 of TS 36.141[3] except that the requirements apply to relay nodes.

#### 6.3.1.2 Total power dynamic range

The total power dynamic range test requirements for the relay access link shall be the same as in clause 6.3.2 of TS 36.141 [3] except that the requirements apply to relay nodes.

#### 6.3.1.3 Transmitter OFF power

The transmitter off power for Relay access link should be applied the same requirement defined in clause 6.4.1 of TS 36.141 [3].

#### 6.3.1.4 Transmitter transient period

The transmitter transient period for Relay access link should be applied the same requirement defined in clause 6.4.2 of TS 36.141 [3].

### 6.3.2 Backhaul Link Test Requirements

For backhaul link test the configuration of OFDM symbols for eNB-to-RN transmission in the first slot shall be as specified in Table 5.4-1 in TS 36.216. Furthermore the reference measurement channel for R-PDCCH defined in Annex B of TS 36.116 [2] shall apply.

#### 6.3.2.1 Minimum Output Power

##### 6.3.2.1.1 Test purpose

To verify the relay nodes ability to transmit with a broadband output power below the value specified in the test requirement when the power is set to a minimum value.

##### 6.3.2.1.2 Test applicability

This test applies to all types of E-UTRA relay nodes.

##### 6.3.2.1.3 Minimum conformance requirements

For a Relay backhaul link with one antenna connector the minimum output power shall not exceed -50 dBm.

For a relay backhaul link with multiple transmit antenna connectors, the minimum output power level is defined with respect to the sum of the mean power at each relay node backhaul antenna connector in one sub-frame (1 ms). The sum of these mean powers will be subject to the -50 dBm minimum output power requirement.

The minimum output power is defined as the mean power in one sub-frame (1ms). The minimum output power shall not exceed the values specified in Table 6.3.2.3-1.

Table 6.3.2.3-1: Minimum output power

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | Channel bandwidth / minimum output power / measurement bandwidth | | | | | |
| 1.4 MHz | 3.0 MHz | 5 MHz | 10 MHz | 15 MHz | 20 MHz |
| Minimum output power | -50 dBm | | | | | |
| Measurement bandwidth | 1.08 MHz | 2.7 MHz | 4.5 MHz | 9.0 MHz | 13.5 MHz | 18 MHz |

The minimum output power test verifies the relay node's ability to transmit with a broadband output power below the specified limit when the power is set to a minimum value. The broadband output power is defined as the power in the channel bandwidth, for all transmit bandwidth configurations (resource blocks).

##### 6.3.2.1.4 Test description

The requirements for method of test shall be the same as in clause 6.3.2.4 of TS 36.521 [7] except that the requirements shall apply to relay nodes.

##### 6.3.2.1.5 Test Requirement

The minimum output power measured shall not exceed the values specified in Table 6.3.2.5-1.

Table 6.3.2.1.5-1: Minimum output power

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | Channel bandwidth / minimum output power/ measurement bandwidth | | | | | |
| 1.4 MHz | 3.0 MHz | 5 MHz | 10 MHz | 15 MHz | 20 MHz |
| Minimum output power | For carrier frequency f ≤ 3.0 GHz: ≤ -49 dBm  For carrier frequency 3.0 GHz < f ≤ 4.2 GHz: ≤ -48.7 dBm | | | | | |
| Measurement bandwidth (see note) | 1.08 MHz | 2.7 MHz | 4.5 MHz | 9.0 MHz | 13.5 MHz | 18 MHz |
| Note: Different implementations such as FFT or spectrum analyzer approach are allowed. For spectrum analyzer approach the measurement bandwidth is defined as an equivalent noise bandwidth. | | | | | | |

The requirements in clause 6.3.2.1 apply during the transmitter ON period. Transmit signal quality (as specified in clause 6.4 of TS 36.116 [2] specific to the relay backhaul link signal quality) shall be maintained for the output power dynamics requirements of this clause.

#### 6.3.2.2 Power Control Absolute power tolerance

The relay backhaul link test requirements for power control absolute power tolerance shall be the same as in clause 6.3.5.1 of TS 36.521 [7] except that the requirements shall apply to relay nodes.

#### 6.3.2.3 Power Control Relative power tolerance

The relay backhaul link test requirements for power control relative power tolerance shall be the same as in clause 6.3.5.2 of TS 36.521 [7] except that the requirements shall apply to relay nodes.

#### 6.3.2.4 Aggregate power control tolerance

The relay backhaul link test requirements for aggregate power control tolerance shall be the same as in clause 6.3.5.3 of TS 36.521 [7] except that the requirements shall apply to relay nodes.

#### 6.3.2.5 Power Control for UL-MIMO

The relay backhaul link test requirements for power control for UL-MIMO shall be the same as in clause 6.3.5B of TS 36.521 [7] except that the requirements shall apply to relay nodes.

#### 6.3.2.6 Transmit ON/OFF Time Mask

With the exception of requirements for PRACH all the other requirements defined in clause 6.3.4 of TS 36.101 shall be applied for Relay backhaul link as transmitter ON/OFF time mask. The off power for Relay backhaul link is defined in clause 8.1.3.2.

For a relay backhaul link with multiple transmit antenna connectors, the requirement defined in clause 6.3.4B of TS 36.101 shall be applied, besides the requirements for PRACH.

For the relay backhaul link the transmit ON/OFF time mask test requirements shall be the same as in clause 6.3.4 of TS 36.521 [7] except that the requirements shall apply to relay nodes.

#### 6.3.2.7 Transmit OFF Power

Transmit OFF power is defined as the mean power when the transmitter is OFF. The transmitter is considered to be OFF when the Relay backhaul is not allowed to transmit or during periods when the Relay is not transmitting a sub-frame. During DTX and measurements gaps, the Relay backhaul is not considered to be OFF.

##### 6.3.2.7.1 Minimum requirement

The transmit OFF power is defined as the mean power in a duration of at least one sub-frame (1ms) excluding any transient periods. The transmit OFF power shall not exceed the values specified in Table 6.3.2-1 of TS 36.116 [2].

Table 6.3.2.7.1-1: Void

The relay backhaul link transmit OFF power mothod of test shall be the same as in clause 6.3.3 of TS 36.521 [7] except that the requirements shall apply to relay nodes.

##### 6.3.2.7.2 Test requirement

The requirement for the transmit OFF power shall not exceed the values specified in Table 6.3.2.7.2-1.

Table 6.3.2.7.2-1: Transmit OFF power

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | Channel bandwidth / Transmit OFF power / measurement bandwidth | | | | | |
| 1.4  MHz | 3.0  MHz | 5  MHz | 10  MHz | 15  MHz | 20  MHz |
| Transmit OFF power | For carrier frequency f ≤ 3.0GHz: ≤ -64.5 dBm  For carrier frequency 3.0GHz < f ≤ 4.2GHz: ≤ -64.2 dBm | | | | | |
| Measurement bandwidth | 1.08 MHz | 2.7 MHz | 4.5 MHz | 9.0 MHz | 13.5 MHz | 18 MHz |

## 6.4 Transmitted signal quality

### 6.4.1 Frequency error

#### 6.4.1.1 Definition and applicability

Frequency error is the measure of the difference between the actual relay transmit frequency and the assigned frequency. The same source shall be used for RF frequency and data clock generation.

It is not possible to verify by testing that the data clock is derived from the same frequency source as used for RF generation. This may be confirmed by the manufacturer's declaration.

#### 6.4.1.2 Minimum Requirement

The minimum requirement is in TS 36.116 [2], clause 6.4.1.1.

#### 6.4.1.3 Test purpose

To verify that the Frequency Error is within the limits of the minimum requirement.

#### 6.4.1.4 Method of test

For the relay access link, the frequency error requirement is tested together with the Error Vector Magnitude test, as described in clause 6.5.2 of TS 36.141 [3] except that the requirements apply to relay nodes.

For the relay backhaul link, the frequency error test method shall be the same as in clause 6.5.1.4 of TS 36.521 [7] except that the requirements shall apply to relay nodes.

#### 6.4.1.5 Test requirement

For the relay access link, the modulated carrier frequency of each E-UTRA carrier configured by the relay shall be accurate to within an accuracy of ± (0.1 ppm + 12 Hz) observed over a period of one subframe (1ms).

For the relay backhaul link the frequency error Δf results must fulfill the test requirement: |Δf| ≤ (0.1 PPM + 15 Hz)

NOTE: If the above Test Requirement differs from the Minimum Requirement then the Test Tolerance applied for this test is non-zero. The Test Tolerance for this test and the explanation of how the Minimum Requirement has been relaxed by the Test Tolerance are given in Annex G of TS 36.141 [3] and in Annex F of TS36.521-1 [7].

### 6.4.2 EVM

The EVM test requirements for the relay access link shall be the same as in clause 6.5.2 of TS 36.141 [3] except that the requirements apply to relay nodes.

The EVM test requirements for the relay backhaul link shall be the same as in clause 6.5.2 of TS 36.521 [7] except that the requirements apply to relay nodes

### 6.4.3 Time alignment error

The test requirements for time alignment error for the relay access link shall be the same as in clause 6.5.3 of TS 36.141 [3] except that the requirements apply to relay nodes.

The test requirements time alignment error for the relay backhaul link shall be the same as in clause 6.8 of TS 36.521 [7] except that the requirements apply to relay nodes

### 6.4.4 DL RS power

The DL RS power test requirements for the relay access link shall be the same as in clause 6.5.4 of TS 36.141 [3] except that the requirements apply to relay nodes.

## 6.5 Unwanted emissions

Unwanted emissions consist of out-of-band emissions and spurious emissions [4]. Out of band emissions are unwanted emissions immediately outside the channel bandwidth resulting from the modulation process and non-linearity in the transmitter but excluding spurious emissions. Spurious emissions are emissions which are caused by unwanted transmitter effects such as harmonics emission, parasitic emission, intermodulation products and frequency conversion products, but exclude out of band emissions.

The out-of-band emissions requirement for the BS transmitter is specified in terms of an Operating band unwanted emissions requirement that defines limits for emissions in the downlink operating band plus the frequency ranges 10 MHz above and 10 MHz below the band. Emissions outside of this frequency range are limited by a spurious emissions requirement.

### 6.5.1 Transmitter spurious emissions

The access link and backhaul link minimum requirement for transmitter spurious emissions is defined in TS 36.116 [2] clause 6.5.1.

The method of test for transmitter spurious emissions for the relay access link shall be the same as in clause 6.6.4 of TS 36.141 [3] except that the requirements apply to relay nodes.

The method of test for transmitter spurious emissions for the relay backhaul link shall be the same as in clause 6.6.3.1 of TS 36.521 [7] except that the requirements apply to relay nodes.

For the test requirements, the local area requirements of clause 6.6.4.5 of TS 36.141 [3] shall apply for both access link and backhaul link.

### 6.5.2 Adjacent Channel Leakage power Ratio (ACLR)

The access link and backhaul link minimum requirement ACLR is defined in TS 36.116 [2] clause 6.5.2.

The adjacent channel leakage power ratio (ACLR) method of test for the relay access link shall be the same as in clause 6.6.2 of TS 36.141 [3] except that the requirements apply to relay nodes.

The adjacent channel leakage power ratio (ACLR) method of test for the relay backhaul link shall be the same as in clause 6.6.2.3 of TS 36.521 [7] except that the requirements apply to relay nodes.

The test requirements for ACLR for both access link and backhaul link is defined in clause 6.6.2.5 of TS 36.141[3].

### 6.5.3 Operating Bands Unwanted Emissions

#### 6.5.3.1 Definition and applicability

Unless otherwise stated, the Operating band unwanted emission limits are defined from 10 MHz below the lowest frequency of the downlink operating band up to 10 MHz above the highest frequency of the downlink operating band (see Table 5.5-1 of TS 36.141 [3]).

The unwanted emission limits in the part of the downlink operating band that falls in the spurious domain are consistent with ITU-R Recommendation SM.329 [9].

For the access link and backhaul link of relay nodes, the requirements of clause 6.5.3.5 shall apply (Category A and B).

The application of either Category A or Category B limits shall be the same as for Transmitter spurious emissions (Mandatory Requirements) in clause 6.6.4.5 of TS 36.141 [3].

#### 6.5.3.2 Minimum Requirement

The minimum requirement shall be as defined in TS 36.116 [2] clause 6.5.3.

#### 6.5.3.3 Test purpose

This test measures the emissions of the relay access link and backhaul link, close to the assigned channel bandwidth of the wanted signal, while the corresponding transmitter is in operation.

#### 6.5.3.4 Method of test

The Operating bands unwanted emissions method of test for the relay access link shall be the same as in clause 6.6.3.4 of TS 36.141 [3] except that the requirements apply to relay nodes

The Operating bands unwanted emissions method of test for the relay backhaul link shall be the same as in clause 6.6.2.1.4 of TS 36.521 [7] except that the requirements apply to relay nodes.

#### 6.5.3.5 Test Requirement

The measurement results shall not exceed the maximum levels specified in the tables below, where:

- f is the separation between the channel edge frequency and the nominal -3dB point of the measuring filter closest to the carrier frequency.

- f\_offset is the separation between the channel edge frequency and the centre of the measuring filter.

- f\_offsetmax is the offset to the frequency 10 MHz outside the downlink operating band.

- fmax is equal to f\_offsetmax minus half of the bandwidth of the measuring filter.

Table 6.5.3.5-1: Relay operating band unwanted emission limits for 1.4 MHz channel bandwidth (E-UTRA bands ≤ 3 GHz)

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Value | | |
| Frequency offset of measurement filter -3dB point, f | 0 MHz  f < 1.4 MHz | 1.4 MHz  f < 2.8 MHz | 2.8 MHz  f < fmax |
| Frequency offset of measurement filter centre frequency, f\_offset | 0.05 MHz   f\_offset  < 1.45 MHz | 1.45 MHz   f\_offset  < 2.85 MHz | 2.85 MHz   f\_offset  < f\_offsetmax |
| Measurement bandwidth (Note 1) | 100 kHz | 100 kHz | 100 kHz |
| Minimum requirement  Power class 1 |  | -29.5 dBm | -31 dBm |
| Minimum requirement  Power class 2 |  | -23.5 dBm | -25 dBm |

Table 6.5.3.5-2: Relay operating band unwanted emission limits  
 for 1.4 MHz channel bandwidth (E-UTRA bands > 3 GHz)

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Value | | |
| Frequency offset of measurement filter -3dB point, f | 0 MHz  f < 1.4 MHz | 1.4 MHz  f < 2.8 MHz | 2.8 MHz  f < fmax |
| Frequency offset of measurement filter centre frequency, f\_offset | 0.05 MHz   f\_offset  < 1.45 MHz | 1.45 MHz   f\_offset  < 2.85 MHz | 2.85 MHz   f\_offset  < f\_offsetmax |
| Measurement bandwidth (Note 1) | 100 kHz | 100 kHz | 100 kHz |
| Minimum requirement  Power class 1 |  | -29.2 dBm | -31 dBm |
| Minimum requirement  Power class 2 |  | -23.2 dBm | -25 dBm |

Table 6.5.3.5-3: Relay operating band unwanted emission limits for 3 MHz channel bandwidth (E-UTRA bands ≤ 3 GHz)

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Value | | |
| Frequency offset of measurement filter -3dB point, f | 0 MHz  f < 3 MHz | 3 MHz  f < 6 MHz | 6 MHz  f < fmax |
| Frequency offset of measurement filter centre frequency, f\_offset | 0.05 MHz   f\_offset  < 3.05 MHz | 3.05 MHz   f\_offset  < 6.05 MHz | 6.05 MHz   f\_offset  < f\_offsetmax |
| Measurement bandwidth (Note 1) | 100 kHz | 100 kHz | 100 kHz |
| Minimum requirement  Power class 1 |  | -33.5 dBm | -35 dBm |
| Minimum requirement  Power class 2 |  | -27.5 dBm | -29 dBm |

Table 6.5.3.5-4: Relay operating band unwanted emission limits for 3 MHz channel bandwidth (E-UTRA bands > 3 GHz)

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Value | | |
| Frequency offset of measurement filter -3dB point, f | 0 MHz  f < 3 MHz | 3 MHz  f < 6 MHz | 6 MHz  f < fmax |
| Frequency offset of measurement filter centre frequency, f\_offset | 0.05 MHz   f\_offset  < 3.05 MHz | 3.05 MHz   f\_offset  < 6.05 MHz | 6.05 MHz   f\_offset  < f\_offsetmax |
| Measurement bandwidth (Note 1) | 100 kHz | 100 kHz | 100 kHz |
| Minimum requirement  Power class 1 |  | -33.2 dBm | -35 dBm |
| Minimum requirement  Power class 2 |  | -27.2 dBm | -29 dBm |

Table 6.5.3.5-5: Relay operating band unwanted emission limits for 5, 10, 15 and 20 MHz channel bandwidth (E-UTRA bands ≤ 3 GHz)

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Value | | |
| Frequency offset of measurement filter -3dB point, f | 0 MHz  f < 5 MHz | 5 MHz  f < min(10 MHz, fmax) | 10 MHz  f < fmax |
| Frequency offset of measurement filter centre frequency, f\_offset | 0.05 MHz   f\_offset  < 5.05 MHz | 5.05 MHz   f\_offset  < min(10.05 MHz,f\_offsetmax) | 10.05 MHz   f\_offset  < f\_offsetmax |
| Measurement bandwidth (Note 1) | 100 kHz | 100 kHz | 100 kHz |
| Minimum requirement  Power class 1 |  | -35.5 dBm | -37 dBm (Note 2) |
| Minimum requirement  Power class 2 |  | -29.5 dBm | -31 dBm |

Table 6.5.3.5-6: Relay operating band unwanted emission limits for 5, 10, 15 and 20 MHz channel bandwidth (E-UTRA bands > 3 GHz)

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Value | | |
| Frequency offset of measurement filter -3dB point, f | 0 MHz  f < 5 MHz | 5 MHz  f < min(10 MHz, fmax) | 10 MHz  f < fmax |
| Frequency offset of measurement filter centre frequency, f\_offset | 0.05 MHz   f\_offset  < 5.05 MHz | 5.05 MHz   f\_offset  < min(10.05 MHz,f\_offsetmax) | 10.05 MHz   f\_offset  < f\_offsetmax |
| Measurement bandwidth (Note 1) | 100 kHz | 100 kHz | 100 kHz |
| Minimum requirement  Power class 1 |  | -35.2 dBm | -37 dBm (Note 2) |
| Minimum requirement  Power class 2 |  | -29.2 dBm | -31 dBm |

NOTE 1: As a general rule for the requirements in clause 6.5.3, the resolution bandwidth of the measuring equipment should be equal to the measurement bandwidth. However, to improve measurement accuracy, sensitivity and efficiency, the resolution bandwidth may be smaller than the measurement bandwidth. When the resolution bandwidth is smaller than the measurement bandwidth, the result should be integrated over the measurement bandwidth in order to obtain the equivalent noise bandwidth of the measurement bandwidth.

NOTE 2: The requirement is not applicable when fmax < 10 MHz.

## 6.6 Transmitter intermodulation

The minimum requirement for transmitter intermodulation for both the relay access and backhaul links shall be as defined in TS 36.116 [2] clause 6.6.

The method of test for the transmitter intermodulation of the relay access link shall be the same as in clause 6.7 of TS 36.141 [3] except that the requirements apply to relay nodes.

The method of test for the transmitter intermodulation of the relay backhaul link shall be the same as in clause 6.7 of TS 36.521 [7] except that the requirements apply to relay nodes.

The test requirements for transmitter intermodulation for both access link and backhaul link is defined in clause 6.7.5 of TS 36.141[3].

# 7. Receiver characteristics

## 7.1 General

## 7.2 Reference sensitivity level

The reference sensitivity power level REFSENS is the minimum mean power applied to both the backhaul antenna ports at which the throughput shall meet or exceed the requirements for the specified reference measurement channel.

## 7.2.1 Backhaul link reference sensitivity

The method of test for the relay backhaul link reference sensitivity shall be the same as in clause 7.3 of TS 36.521 [7] except that the requirements apply to relay nodes.

The minimum requirement shall be as defined in clause 7.2.1 of TS 36.116 [2].

#### 7.2.1.1 Test requirement

The throughput shall be ≥ 95% of the maximum throughput of the reference measurement channels as specified in Annexes A.2.2, A.2.3 and A.3.2 of TS 36.101[6] (with one sided dynamic OCNG Pattern OP.1 FDD/TDD for the DL-signal as described in Annex A.5.1.1/A.5.2.1 of TS 36.101[6]) with parameters specified in Table 7.1.1.1-1.

NOTE: Whether the transmitter should be turned on or not during tests is FFS.

Table 7.2.1.1-1 Backhaul antenna connector reference sensitivity

|  |  |  |
| --- | --- | --- |
| E-UTRA channel bandwidth [MHz] | Reference sensitivity power level, PREFSENS [dBm] | |
| f ≤ 3.0GHz | 3.0GHz < f ≤ 4.2GHz |
| 1.4 | -105 | -104.7 |
| 3 | -102 | -101.7 |
| 5 | -100.3 | -100 |
| 10 | -97.3 | -97 |
| 15 | -95.5 | -95.2 |
| 20 | -94.3 | -94 |

### 7.2.2 Access link reference sensitivity

The test requirements for the relay access link reference sensitivity shall be the same as in clause 7.2 of TS 36.141 [3] except that the requirements apply to relay nodes and the minimum requirement shall be as defined in clause 7.2.2 of TS 36.116 [2].

## 7.3 Dynamic range

### 7.3.1 Backhaul link Maximum Input Level

The test requirements for the relay backhaul link maximum input level are specified in clause 7.4 of TS 36.521 [7], except that the requirements apply to relay nodes and the minimum requirement shall be as defined in clause 7.3.1 of TS 36.116 [2].

### 7.3.2 Access link Receiver Dynamic Range

The test requirements for the relay access link receiver dynamic range shall be the same as in clause 7.3 of TS 36.141 [3] except that the requirements apply to relay nodes and the minimum requirement shall be as defined in clause 7.3.2 of TS 36.116 [2]. For the test requirements, only those of Table 7.3.2 for local area of TS 36.141 [3] shall apply.

## 7.4 In-channel selectivity

The test requirements for the relay access link In-channel selectivity shall be the same as in clause 7.4 of TS 36.141 [3] except that the requirements apply to relay nodes and the minimum requirement shall be as defined in clause 7.4 of TS 36.116 [2]. For the test requirements, only those of Table 7.4-2 for local area of TS 36.141 [3] shall apply.

## 7.5 Adjacent Channel Selectivity (ACS)

### 7.5.1 Backhaul Adjacent Channel Selectivity (ACS)

The method of test for the relay backhaul link ACS is specified in clause 7.5 of TS 36.521 [7], except that the requirements apply to relay nodes.

The minimum requirement shall be as defined in clause 7.5.1 of TS 36.116 [2].

The test requirement for the relay backhaul link ACS shall be the same as the minimum requirement as defined in clause 7.5.1 of TS 36.116 [2].

### 7.5.2 Access Link Adjacent Channel Selectivity (ACS)

The test requirements for the relay access link ACS shall be the same as in clause 7.5 of TS 36.141 [3] except that the requirements apply to relay nodes and the minimum requirement shall be as defined in clause 7.5.2 of TS 36.116 [2]. For the test requirements, only those for local area of clause 7.5 of TS 36.141 [3] shall apply.

## 7.6 Blocking characteristics

### 7.6.1 Backhaul Blocking Characteristics

The method of test for the relay backhaul link blocking characteristics is specified in clause 7.6 of TS 36.521 [7], except that the requirements apply to relay nodes.

The minimum requirement shall be as defined in clause 7.6.1 of TS 36.116 [2].

The test requirement for the relay backhaul link blocking characteristics shall be the same as the minimum requirement as defined in clause 7.6.1 of TS 36.116 [2].

### 7.6.2 Access Link Blocking Characteristics

The test requirements for the relay access link blocking characteristics shall be the same as in clause 7.6 of TS 36.141 [3] except that the requirements apply to relay nodes and the minimum requirement shall be as defined in clause 7.6.2 of TS 36.116 [2].

For the test requirements, only those for local area of clause 7.6 of TS 36.141 [3] shall apply.

### 7.6.3 Blocking requirements for co-location

The test requirements for the relay backhaul link blocking requirements for co-location shall be the same as in clause 7.6.5.2 of TS 36.141 [3] except that the requirements apply to relay nodes. For the test requirements, only those for local area of clause 7.6.5.2 of TS 36.141 [3] shall apply.

The Local Area BS requirements shall apply for the access link for relay power class 1. For relay power class 2 the interfering signal power in table 7.6-4 of TS 36.141[3] shall be changed to 0 dBm. The test requirements for the relay access link blocking requirements for co-location shall be the same as in clause 7.6.5.2 of TS 36.141 [3] except that the requirements apply to relay nodes. For the test requirements, only those for local area of clause 7.6.5.2 of TS 36.141 [3] shall apply.

## 7.7 Receiver spurious emissions

### 7.7.1 Backhaul Link Receiver Spurious Emissions

The test requirements for the relay backhaul link receiver spurious emissions are specified in clause 7.9 of TS 36.521 [7], except that the requirements apply to relay nodes.

### 7.7.2 Access Link Receiver Spurious Emissions

The test requirements for the relay access link receiver spurious emissions shall be the same as in clause 7.7 of TS 36.141 [3], except that the requirements apply to relay nodes.

## 7.8 Receiver intermodulation

### 7.8.1 Backhaul Link Receiver Intermodulation

The method of test for the relay backhaul link receiver intermodulation is specified in clause 7.8 of TS 36.521 [7], except that the requirements apply to relay nodes.

The minimum requirement shall be as defined in clause 7.8.1 of TS 36.116 [2].

The test requirement for the relay backhaul link receiver intermodulation shall be the same as the minimum requirement as defined in clause 7.8.1 of TS 36.116 [2].

### 7.8.2 Access Link Receiver Intermodulation

*The test requirements for the relay access link receiver intermodulation shall be the same as in clause 7.8 of TS 36.141 [3] except that the requirements apply to relay nodes. For the test requirements, only those for local area of clause 7.8 of TS 36.141 [3] shall apply.*

# 8. Access Performance requirement

## 8.1 General

Access performance requirements are specified for a number of test environments and multipath channel classes and unless specified otherwise shall meet the performance requirements defined in clause 8 of TS 36.104 [4].

Unless stated otherwise, access performance requirements apply for a single carrier only. Performance requirements for a relay supporting carrier aggregation are defined in terms of single carrier requirements. The requirements only apply to those measurement channels that are supported by the base station.

The performance requirements for High Speed Train conditions defined in Annex B.3 of [3] are optional.

The performance requirements for UL timing adjustment scenario 2 defined in Annex B.4 of [3] are optional.

For BS with receiver antenna diversity the required SNR shall be applied separately at each antenna port.

In tests performed with signal generators a synchronization signal may be provided, from the base station to the signal generator, to enable correct timing of the wanted signal.

For tests in clause 8 the transmitter may be off.

## 8.2 Performance requirements for PUSCH

### 8.2.1 Requirements in multipath fading propagation conditions

The definition and applicability is the same as defined in TS 36.141 [3] except that the conformance test is applied for a relay. The requirements associated with ETU 70Hz or ETU 300Hz are optional.

The PUSCH performance requirements in multipath fading propagation conditions are the same as defined in TS 36.104 [4].

The test purpose, test method and test requirement in multipath fading propagation conditions are the same as defined in TS 36.141 [3].

### 8.2.2 Requirements for UL timing adjustment

The definition and applicability is the same as defined in TS 36.141 [3] except that the conformance test is applied for a relay.

The minimum requirements for UL timing adjustment are the same as defined in TS 36.104 [4]

The test purpose, test method and test requirement for UL timing adjustment are the same as defined in TS 36.141 [3].

### 8.2.3 Requirements for HARQ-ACK multiplexed on PUSCH

The definition and applicability is the same as defined in TS 36.141 [3] except that the conformance test is applied for a relay. The requirements associated with ETU 70Hz are optional.

The minimum performance requirements for HARQ-ACK multiplexed on PUSCH are the same as defined in TS 36.104 [3].

The test purpose, test method and test requirement for HARQ-ACK multiplexed on PUSCH are the same as defined in TS 36.141 [3].

## 8.3 Performance requirements for PUCCH

### 8.3.1 ACK missed detection requirements for single user PUCCH format 1a

The definition and applicability is the same as defined in TS 36.141 [3] except that the conformance test is applied for a relay. The requirements associated with ETU 70Hz or ETU 300Hz are optional.

The minimum requirements for DTX to ACK performance and for ACK missed detection are as defined in TS36.104 [4].

The test purpose, test method and test requirement for PUCCH format 1a are the same as defined in TS 36.141 [3].

### 8.3.2 CQI missed detection requirements for PUCCH format2

The definition and applicability is the same as defined in TS 36.141 [3] except that the conformance test is applied for a relay. The requirements associated with ETU 70Hz are optional.

The CQI missed detection requirements for PUCCH format 2 are the same as defined in TS 36.104 [4].

The test purpose, test method and test requirement for PUCCH format 2 are the same as defined in TS 36.141 [3].

### 8.3.3 ACK missed detection requirements for multi user PUCCH format 1a

The requirements for multi user PUCCH format 1a are optional. The definition and applicability is the same as defined in TS 36.141 [3] except that the conformance test is applied for a relay.

The ACK missed detection requirements for multi user PUCCH format 1a are optional and are the same as defined in TS 36.104 [4].

The test purpose, test method and test requirement for multi user PUCCH format 1a are the same as defined in TS 36.141 [3].

## 8.4 Performance requirements for PRACH

### 8.4.1 PRACH false alarm probability and missed detection

The definition and applicability is the same as defined in TS 36.141 [3] except that the conformance test is applied for a relay. The requirements associated with ETU 70Hz are optional.

The minimum requirements for PRACH False alarm probability are the same as defined in TS 36.104 [4].

The test purpose, test method and test requirement for PRACH are the same as defined in TS 36.141 [3].

# 9. Backhaul Performance requirement

## 9.1 General

The performance requirements for the backhaul are based on relays that utilize a dual-antenna receiver.

For all test cases, the SNR is defined as:

where the superscript indicates the receiver antenna connector. The SNR is defined assuming resource elements (RE's) are not precoded, and the relative power of physical channels transmitted is defined in TS 36.101[2], Table C.3.2-1.

## 9.2 Demodulation of PDSCH (Cell-Specific Reference Symbols)

For the demodulation of PDSCH (cell-specific reference symbols), the test requirements are specified in clause 8.2 of TS 36.521 [7], except that the requirements apply to relay nodes.

## 9.3 Demodulation of PDSCH (User-Specific Reference Symbols)

For the demodulation of PDSCH (user-specific reference symbols), the test requirements are specified in clause 8.3 of TS 36.521 [7], except that the requirements apply to relay nodes.

## 9.4 Demodulation of PDCCH/PCFICH

For the demodulation of PDCCH/PCFICH, the test requirements are specified in clause 8.4 of TS 36.521 [7], except that the requirements apply to relay nodes.

## 9.5 Demodulation of PHICH

For the demodulation of PHFICH, the test requirements are specified in clause 8.5 of TS 36.521 [7], except that the requirements apply to relay nodes.

## 9.6 Demodulation of PBCH

For the demodulation of PBCH, the test requirements are specified in clause 8.6 of TS 36.521 [7], except that the requirements apply to relay nodes.

## 9.7 Sustained downlink data rate provided by lower layers

For sustained downlink data rate provided by lower layers, the test requirements are specified in clause 8.7 of TS 36.521 [7], except that the requirements apply to relay nodes.

## 9.8 Demodulation of R-PDCCH

### 9.8.1 FDD

#### 9.8.1.1 FDD R-PDCCH performance based on UE-specific reference signals transmitted on antenna port 7 with 1x2 antenna configuration

##### 9.8.1.1.1 Test purpose

This test verifies the demodulation performance of R-PDCCH when R-PDCCH is based on UE-specific reference signals transmitted on antenna port 7 with 1x2 antenna configuration. With a given SNR, the average probability of miss-detection of the Downlink Scheduling Grant for RN, tested on R-PDCCH of the specified reference measurement channels in B.1.1.1 of TR 36.826 [5] remains below a given reference value.

##### 9.8.1.1.2 Test applicability

This test applies to all types of E-UTRA FDD relay node release 11 and forward.

##### 9.8.1.1.3 Minimum conformance requirements

The receiver characteristics of the R-PDCCH are determined by the probability of miss-detection of the relay Downlink Scheduling Grant (Pm-dsg).

Table 9.8.1.1.3-1: Test Parameters for single-layer transmission on port 7 of R-PDCCH

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | | Unit | Test 1 |
| Cyclic prefix | |  | Normal |
| Cell ID | |  | 0 |
| Un subframe type in DeNB | |  | Normal subframe |
| SubframeConfigurationFDD | |  | 10110101 |
| Number of OFDM symbols for PDCCH | | OFDM symbols | 2 |
| Configuration of OFDM symbols for eNB-to-RN transmission in the first slot | |  | 2 (Note 1) |
| Downlink power allocation | R-PDCCH\_RA | dB | 0 |
| R-PDCCH\_RB | dB | 0 |
| Cell-specific reference symbols | |  | Antenna port 0 |
| CSI reference signal configuration | |  | 1 |
| Number of CSI reference signals configured | |  | 1 |
| CSI reference signal subframe configuration | |  | *I*CSI-RS = 37 |
| at antenna port | | dBm/15kHz | -98 |
| Number of allocated resource blocks | | PRB | 2 |
| Symbols for unused PRBs | |  | OCNG (Note 2) |
| Simultaneous transmission (Note 3) | |  | No |
| Beamforming Model | |  | No precoding |
| Precoder update granularity | |  | Frequency domain: 1 PRG  Time domain: 1 ms |
| Note 1: as specified in Table 5.4-1 in TS 36.216.  Note 2: These physical resource blocks are assigned to an arbitrary number of virtual UEs with one PDSCH per virtual UE; the data transmitted over the OCNG PDSCHs shall be uncorrelated pseudo random data, which is QPSK modulated.  Note 3: The modulation symbols of the signal under test are mapped onto antenna port 7 while antenna port 8 is unused.  Note 4: | | | |

For the parameters specified in Table 9.8.1.1.3-1 the average probability of a missed relay downlink scheduling grant (Pm-dsg) shall be below the specified value in Table 9.8.1.1.3-2.

Table 9.8.1.1.3-2: Minimum performance for R-PDCCH without cross-interleaving (FRC)

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Test number | Bandwidth | Reference channel | OCNG Pattern | Aggregation level | DCI format | Propagation Condition | Antenna configuration and correlation Matrix | Reference value | |
| Pm-dsg (%) | SNR (dB) |
| 1 | 10 MHz | R.1 FDD | Table B.2.1-1 of [5] | 2 PRB | Format 2C | LOS with strong dominant component | 1x2 | 1 | 2.1 |

##### 9.8.1.1.4 Test description

###### 9.8.1.1.4.1 Initial conditions

Initial conditions are a set of test configurations the RN needs to be tested in and the steps for the SS to take with the RN to reach the correct measurement state.

Configurations of PDSCH and PDCCH before measurement are specified in TS 36.521-1 [7], Annex C.2.

Test Environment: Normal, as defined in TS 36.508 [8] clause 4.1.

Frequencies to be tested: Mid Range, as defined in TS 36.508 [8] clause 4.3.1.1.

Channel Bandwidths to be tested: 10MHz, as defined in TS 36.508 [8] clause 4.3.1.1:

1. Connect the SS, the faders and AWGN noise source to the RN antenna connector (s) as shown in TS 36.508 [8] Annex A, Figure A.9.

2. The parameter settings for the cell are set up according to Table 9.8.1.1.3-1.

3. The backhaul signals except for R-PDCCH are initially set up according to Annex C.1 and Annex C.3.2 defined in TS 36.521-1[7] and uplink signals according to Annex H.1 and H.3.2 defined in TS 36.521-1[7]. R-PDCCH is mapped to physical resources according to Table 9.8.1.1.3-1, Table 9.8.1.1.3-2 and Table B.1.1.1-1 of TR 36.826 [5]. The signals of R-PDCCH are initially set up according to Annex C.1 of TR 36.826 [5].

4. Propagation conditions are set according to Annex A clause A.1 of TR 36.826 [5].

5. Ensure the RN is in State 3A-RF according to TS 36.508 [8] clause 5.2A.2 with the following exceptions. Message contents are defined in clause 9.8.1.1.4.3.

Table 9.8.1.1.4.1-1: RN registration with test mode activation procedure (state 1 to state 2A)

|  |  |  |  |
| --- | --- | --- | --- |
| Step | Procedure | Message Sequence | |
| R - S | Message |
| 1 to 17 | Same procedure for steps 1 to 17 as specified in the procedure in Table 4.5.2A.3-1 [TS 36.508] |  |  |
| 18 | The SS transmits an *RNReconfiguration message to configurate the backhaul link* | <-- | RRC: *RNReconfiguration* |
| 19 | The RN transmits an *RNReconfigurationComplete message to comfirm the configuration of backhal link* | --> | RRC: *RNReconfigurationComplete* |
| 20 | This message includes the ATTACH COMPLETE message. The ACTIVATE DEFAULT EPS BEARER CONTEXT ACCEPT message is piggybacked in ATTACH COMPLETE. | --> | RRC: *ULInformationTransfer*  NAS: ATTACH COMPLETE  NAS: ACTIVATE DEFAULT EPS BEARER CONTEXT ACCEPT |
| 21 | The SS transmits an *RRCConnectionRelease* message to release RRC connection and move to RRC\_IDLE (State 2A). | <-- | RRC: *RRCConnectionRelease* |

###### 9.8.1.1.4.2 Test procedure

1. SS transmits PDSCH via R-PDCCH DCI format 2C for C\_RNTI to transmit the DL RMC according to Table 9.8.1.1.3-1 and Table 9.8.1.1.3-2.The details of R-PDCCH and PDSCH are specified in Table B.1.1.1-1 and R.3 FDD in Table C.2-1 respectively of TR 36.826 [5]. The SS sends downlink MAC padding bits on the DL RMC.

2. Set the parameters of the propagation condition, antenna configuration, the correlation matrix and the SNR according to Table 9.8.1.1.5-1 as appropriate.

3. Measure the Pm-dsg for a duration sufficient to achieve statistical significance according to Annex G clause G.4 defined in TS 36.521-1 [7]. Count the number of NACKs, ACKs and statDTXs on the UL PUCCH during each subtest interval. Pm-dsg is the ratio (statDTX)/(NACK+ACK+statDTX). If Pm-dsg is less than the value specified in table 9.8.1.1.5-1, pass the RN. Otherwise fail the RN.

###### 9.8.1.1.4.3 Message contents

Message contents are according to TS 36.508 [8] clause 4.6 with the following exceptions

Table 9.8.1.1.4.3-1: RRCConnectionSetupComplete

|  |  |  |  |
| --- | --- | --- | --- |
| Derivation Path: 36.331 clause 6.2.2 |  |  |  |
| Information Element | Value/remark | Comment | Condition |
| RRCConnectionSetupComplete ::= SEQUENCE { |  |  |  |
| rrc-TransactionIdentifier | RRC-TransactionIdentifier-UL |  |  |
| criticalExtensions CHOICE { |  |  |  |
| c1 CHOICE { |  |  |  |
| rrcConnectionSetupComplete-r8 SEQUENCE { |  |  |  |
| selectedPLMN-Identity | 1 |  |  |
| registeredMME | Not checked |  |  |
| dedicatedInfoNAS | Present but contents not checked |  |  |
| nonCriticalExtension SEQUENCE { |  |  |  |
| lateNonCriticalExtension | Not checked |  |  |
| nonCriticalExtension SEQUENCE { |  |  |  |
| gummei-Type-r10 | native |  |  |
| rlf-InfoAvailable-r10 | true |  |  |
| logMeasAvailable-r10 | true |  |  |
| rn-SubframeConfigReq-r10 | required |  |  |
| nonCriticalExtension SEQUENCE{} | Not checked |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |

Table 9.8.1.1.4.3-2: RNReconfiguration

|  |  |  |  |
| --- | --- | --- | --- |
| Derivation Path: 36.331 clause 6.2.2 | | | |
| Information Element | Value/remark | Comment | Condition |
| RNReconfiguration ::= SEQUENCE { |  |  |  |
| rrc-TransactionIdentifier | RRC-TransactionIdentifier-DL |  |  |
| criticalExtensions CHOICE { |  |  |  |
| c1 CHOISE { |  |  |  |
| RnReconfiguration-r10 SEQUENCE{ |  |  |  |
| rn-SystemInfo-r10{} | Not Checked |  |  |
| rn-SubframeConfig-r10 | RN-SubframeConfig-r10 |  |  |
| lateNonCriticalExtension | Not checked |  |  |
| nonCriticalExtension SEQUENCE{} | Not checked |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |
|  |  |  |  |

Table 9.8.1.1.4.3-3: RN-SubframeConfig

|  |  |  |  |
| --- | --- | --- | --- |
| Derivation Path: 36.331 clause 6.3.2 | | | |
| Information Element | Value/remark | Comment | Condition |
| RN-SubframeConfig-r10::= SEQUENCE { |  |  |  |
| subframeConfigPattern-r10 CHOICE{ |  |  |  |
| subframeConfigPatternFDD-r10 | 10110101 |  |  |
| } |  |  |  |
| rpdcch-Config-r10 SEQUENCE{ |  |  |  |
| resourceAllocationType-r10 | type0 |  |  |
| resourceBlockAssignment-r10 CHOICE{ |  |  |  |
| type01-r10 SEQUENCE{ |  |  |  |
| nrb50-r10 | 0000 0000 1000 0000 0 |  |  |
| } |  |  |  |
| } |  |  |  |
| demodulationRS-r10 CHOICE{ |  |  |  |
| noInterleaving-r10 | dmrs |  |  |
| } |  |  |  |
| pdsch-Start-r10 | 3 |  |  |
| pucch-Config-r10 CHOICE{ |  |  |  |
| fdd SEQUENCE{ |  |  |  |
| n1PUCCH-AN-P0-r10 | 0 |  |  |
| n1PUCCH-AN-P1-r10 | Not Checked |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |
|  |  |  |  |

Table 9.8.1.1.4.3-4: RNReconfigurationComplete

|  |  |  |  |
| --- | --- | --- | --- |
| Derivation Path: 36.331 clause 6.2.2 | | | |
| Information Element | Value/remark | Comment | Condition |
| *RNReconfigurationComplete*::= SEQUENCE { |  |  |  |
| rrc-TransactionIdentifier | RRC-TransactionIdentifier-UL |  |  |
| criticalExtensions CHOICE { |  |  |  |
| c1 CHOICE{ |  |  |  |
| rnReconfigurationComplete-r10 SEQUENCE{ |  |  |  |
| lateNonCriticalExtension | Not checked |  |  |
| nonCriticalExtension | Not checked |  |  |
| } |  |  |  |
| } |  |  |  |
| criticalExtensionsFuture SEQUENCE{} | Not checked |  |  |
| } |  |  |  |
| } |  |  |  |
|  |  |  |  |

##### 9.8.1.1.5 Test requirement

For the parameters specified in Table 9.8.1.1.3-1 the average probability of a missed downlink scheduling grant (Pm-dsg) shall be below the specified value in Table 9.8.1.1.5-1.

Table 9.8.1.1.5-1: Test requirement R-PDCCH without cross-interleaving (FRC)

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Test number | Bandwidth | Reference channel | OCNG Pattern | Aggregation level | DCI format | Propagation Condition | Antenna configuration and correlation Matrix | Reference value | |
| Pm-dsg (%) | SNR (dB) |
| 1 | 10MHz | R.1 FDD | Table B.2.1-1 of [5] | 2 PRB | Format 2C | LOS with strong dominant component | 1x2 | 1 | 3.1 |

#### 9.8.1.2 FDD R-PDCCH performance based on UE-specific reference signals transmitted on antenna port 7 with 4x2 antenna configuration

##### 9.8.1.2.1 Test purpose

This test verifies the demodulation performance of R-PDCCH when R-PDCCH is based on UE-specific reference signals transmitted on antenna port 7 with 4x2 antenna configuration. With a given SNR, the average probability of miss-detection of the Downlink Scheduling Grant for RN, tested on R-PDCCH of the specified reference measurement channels in B.1.1.1 of [5] remains below a given reference value.

##### 9.8.1.2.2 Test applicability

This test applies to all types of E-UTRA FDD relay node release 11 and forward.

##### 9.8.1.2.3 Minimum conformance requirements

The receiver characteristics of the R-PDCCH are determined by the probability of miss-detection of the relay Downlink Scheduling Grant (Pm-dsg).

Table 9.8.1.2.3-1: Test Parameters for single-layer transmission on port 7 of R-PDCCH

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | | Unit | Test 2 |
| Cyclic prefix | |  | Normal |
| Cell ID | |  | 0 |
| Un subframe type in DeNB | |  | Normal subframe |
| SubframeConfigurationFDD | |  | 10110101 |
| Number of OFDM symbols for PDCCH | | OFDM symbols | 2 |
| Configuration of OFDM symbols for eNB-to-RN transmission in the first slot | |  | 2 (Note 1) |
| Downlink power allocation | R-PDCCH\_RA | dB | 0 |
| R-PDCCH\_RB | dB | 0 |
| Cell-specific reference symbols | |  | Antenna port 0,1 |
| CSI reference signal configuration | |  | 1 |
| Number of CSI reference signals configured | |  | 4 |
| CSI reference signal subframe configuration | |  | *I*CSI-RS = 37 |
| at antenna port | | dBm/15 kHz | -98 |
| Number of allocated resource blocks | | PRB | 4 |
| Symbols for unused PRBs | |  | OCNG (Note 2) |
| Simultaneous transmission (Note 3) | |  | No |
| Beamforming Model | |  | a precoder vector of size is randomly selected with the number of layers from Table 6.3.4.2.3-2 in TS 36.211 as beamforming weights |
| Precoder update granularity | |  | Frequency domain: 1 PRG  Time domain: 1 ms |
| Note 1: As specified in Table 5.4-1 in TS 36.216.  Note 2: These physical resource blocks are assigned to an arbitrary number of virtual UEs with one PDSCH per virtual UE; the data transmitted over the OCNG PDSCHs shall be uncorrelated pseudo random data, which is QPSK modulated.  Note 3: The modulation symbols of the signal under test are mapped onto antenna port 7 while antenna port 8 is unused.  Note 4: | | | |

For the parameters specified in Table 9.8.1.2.3-1 the average probability of a missed relay downlink scheduling grant (Pm-dsg) shall be below the specified value in Table 9.8.1.2.3-2.

Table 9.8.1.2.3-2: Minimum performance for R-PDCCH without cross-interleaving (FRC)

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Test number | Bandwidth | Reference channel | OCNG Pattern | Aggregation level | DCI format | Propagation Condition | Antenna configuration and correlation Matrix | Reference value | |
| Pm-dsg (%) | SNR (dB) |
| 2 | 10 MHz | R.2 FDD | Table B.2.1-1 of [5] | 4 PRB | Format 2C | NLOS with medium correlation | 4x2 | 1 | 11.5 |

##### 9.8.1.2.4 Test description

###### 9.8.1.2.4.1 Initial conditions

Initial conditions are a set of test configurations the RN needs to be tested in and the steps for the SS to take with the RN to reach the correct measurement state.

Configurations of PDSCH and PDCCH before measurement are specified in TS 36.521-1 [7] Annex C.2.

Test Environment: Normal, as defined in TS 36.508 [8] clause 4.1.

Frequencies to be tested: Mid Range, as defined in TS 36.508 [8] clause 4.3.1.1.

Channel Bandwidths to be tested: 10MHz, as defined in TS 36.508 [8] clause 4.3.1.1:

1. Connect the SS, the faders and AWGN noise source to the RN antenna connector (s) as shown in TS 36.508 [8] Annex A, Figure A.11.

2. The parameter settings for the cell are set up according to Table 9.8.1.2.3-1.

3. The downlink signals are initially set up according to Annex C.1 and Annex C.3.2 of TR 36.826 [5] and uplink signals according to Annex H.1 and H.3.2 defined in TS 36.521-1[7].

4. Propagation conditions are set according to Annex A clause A.1 of TR 36.826 [5].

5. Ensure the RN is in State 3A-RF according to TS 36.508 [8] clause 5.2A.2 with the following exceptions. Message contents are defined in clause 9.8.1.2.4.3.

Table 9.8.1.2.4.1-1: RN registration with test mode activation procedure (state 1 to state 2A)

|  |  |  |  |
| --- | --- | --- | --- |
| Step | Procedure | Message Sequence | |
| R - S | Message |
| 1 to 17 | Same procedure for steps 1 to 17 as specified in the procedure in Table 4.5.2A.3-1  [TS 36.508] |  |  |
| 18 | The SS transmits an *RNReconfiguration message to configurate the backhaul link* | <-- | RRC: *RNReconfiguration* |
| 19 | The RN transmits an *RNReconfigurationComplete message to comfirm the configuration of backhal link* | --> | RRC: *RNReconfigurationComplete* |
| 20 | This message includes the ATTACH COMPLETE message. The ACTIVATE DEFAULT EPS BEARER CONTEXT ACCEPT message is piggybacked in ATTACH COMPLETE. | --> | RRC: *ULInformationTransfer*  NAS: ATTACH COMPLETE  NAS: ACTIVATE DEFAULT EPS BEARER CONTEXT ACCEPT |
| 21 | The SS transmits an *RRCConnectionRelease* message to release RRC connection and move to RRC\_IDLE (State 2A). | <-- | RRC: *RRCConnectionRelease* |

###### 9.8.1.2.4.2 Test procedure

1. SS transmits PDSCH via R-PDCCH DCI format 2C for C\_RNTI to transmit the DL RMC according to Table 9.8.1.2.3-2.The details of R-PDCCH and PDSCH are specified in Table B1.1.1-1 of TR 36.826 [5] and R.4 FDD in Table C.2-1respectively. The SS sends downlink MAC padding bits on the DL RMC.

2. Set the parameters of the propagation condition, antenna configuration, the correlation matrix and the SNR according to Table 9.8.1.2.5-1 as appropriate.

3. Measure the Pm-dsg for a duration sufficient to achieve statistical significance according to Annex G clause G.4 defined in TS 36.521-1[7]. Count the number of NACKs, ACKs and statDTXs on the UL PUCCH during each subtest interval. Pm-dsg is the ratio (statDTX)/(NACK+ACK+statDTX). If Pm-dsg is less than the value specified in table 9.8.1.2.5-1, pass the UE. Otherwise fail the UE. If Pm-dsg is less than the value specified in table 9.8.1.2.5-1, pass the UE. Otherwise fail the UE.

###### 9.8.1.2.4.3 Message contents

Message contents are according to TS 36.508 [8] clause 4.6 with the following exceptions.

Table 9.8.1.2.4.3-1: PhysicalConfigDedicated-DEFAULT

|  |  |  |  |
| --- | --- | --- | --- |
| Derivation Path: 36.331 clause 6.3.2 | | | |
| Information Element | Value/remark | Comment | Condition |
| PhysicalConfigDedicated-DEFAULT ::= SEQUENCE { |  |  |  |
| antennaInfo-r10 CHOICE { |  |  |  |
| AntennaInfoDedicated-r10::= SEQUENCE { |  |  |  |
| transmissionMode | tm9-v1020 |  |  |
| codebookSubsetRestriction-r10 |  |  |  |
| ue-TransmitAntennaSelection CHOICE { |  |  |  |
| release | NULL |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |

Table 9.8.1.2.4.3-2: RRCConnectionSetupComplete

|  |  |  |  |
| --- | --- | --- | --- |
| Derivation Path: 36.331 clause 6.2.2 | | | |
| Information Element | Value/remark | Comment | Condition |
| RRCConnectionSetupComplete ::= SEQUENCE { |  |  |  |
| rrc-TransactionIdentifier | RRC-TransactionIdentifier-UL |  |  |
| criticalExtensions CHOICE { |  |  |  |
| c1 CHOICE { |  |  |  |
| rrcConnectionSetupComplete-r8 SEQUENCE { |  |  |  |
| selectedPLMN-Identity | 1 |  |  |
| registeredMME | Not checked |  |  |
| dedicatedInfoNAS | Present but contents not checked |  |  |
| nonCriticalExtension SEQUENCE { |  |  |  |
| lateNonCriticalExtension | Not checked |  |  |
| nonCriticalExtension SEQUENCE { |  |  |  |
| gummei-Type-r10 | native |  |  |
| rlf-InfoAvailable-r10 | true |  |  |
| logMeasAvailable-r10 | true |  |  |
| rn-SubframeConfigReq-r10 | required |  |  |
| nonCriticalExtension SEQUENCE{} | No checked |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |

Table 9.8.1.2.4.3-3: RNReconfiguration

|  |  |  |  |
| --- | --- | --- | --- |
| Derivation Path: 36.331 clause 6.2.2 | | | |
| Information Element | Value/remark | Comment | Condition |
| RNReconfiguration ::= SEQUENCE { |  |  |  |
| rrc-TransactionIdentifier | RRC-TransactionIdentifier-DL |  |  |
| criticalExtensions CHOICE { |  |  |  |
| c1 CHOISE { |  |  |  |
| RnReconfiguration-r10 SEQUENCE{ |  |  |  |
| rn-SystemInfo-r10{} | Not checked |  |  |
| rn-SubframeConfig-r10 | RN-SubframeConfig-r10 |  |  |
| lateNonCriticalExtension | Not checked |  |  |
| nonCriticalExtension SEQUENCE{} | Not checked |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |
|  |  |  |  |

Table 9.8.1.2.4.3-4: *RN-SubframeConfig*

|  |  |  |  |
| --- | --- | --- | --- |
| Derivation Path: 36.331 clause 6.3.2 | | | |
| Information Element | Value/remark | Comment | Condition |
| RN-SubframeConfig-r10::= SEQUENCE { |  |  |  |
| subframeConfigPattern-r10 CHOICE{ |  |  |  |
| subframeConfigPatternFDD-r10 | 10110101 |  |  |
| } |  |  |  |
| rpdcch-Config-r10 SEQUENCE{ |  |  |  |
| resourceAllocationType-r10 | Type0 |  |  |
| resourceBlockAssignment-r10 CHOICE{ |  |  |  |
| type01-r10 SEQUENCE{ |  |  |  |
| nrb50-r10 | 0000 0001 1000 0000 0 |  |  |
| } |  |  |  |
| } |  |  |  |
| demodulationRS-r10 CHOICE{ |  |  |  |
| noInterleaving-r10 | dmrs |  |  |
| } |  |  |  |
| pdsch-Start-r10 | 3 |  |  |
| pucch-Config-r10 CHOICE{ |  |  |  |
| fdd SEQUENCE{ |  |  |  |
| n1PUCCH-AN-P0-r10 | 0 |  |  |
| n1PUCCH-AN-P1-r10 | Not Checked |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |
|  |  |  |  |

Table 9.8.1.2.4.3-5: RNReconfigurationComplete

|  |  |  |  |
| --- | --- | --- | --- |
| Derivation Path: 36.331 clause 6.2.2 | | | |
| Information Element | Value/remark | Comment | Condition |
| *RNReconfigurationComplete*::= SEQUENCE { |  |  |  |
| rrc-TransactionIdentifier | RRC-TransactionIdentifier-UL |  |  |
| criticalExtensions CHOICE { |  |  |  |
| c1 CHOICE{ |  |  |  |
| rnReconfigurationComplete-r10 SEQUENCE{ |  |  |  |
| lateNonCriticalExtension | Not checked |  |  |
| nonCriticalExtension | Not checked |  |  |
| } |  |  |  |
| } |  |  |  |
| criticalExtensionsFuture SEQUENCE{} | Not checked |  |  |
| } |  |  |  |
| } |  |  |  |
|  |  |  |  |

##### 9.8.1.2.5 Test requirement

For the parameters specified in Table 9.8.1.2.3-1 the average probability of a missed downlink scheduling grant (Pm-dsg) shall be below the specified value in Table 9.8.1.2.5-1.

Table 9.8.1.2.4-1: Test requirement R-PDCCH without cross-interleaving (FRC)

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Test number | Bandwidth | Reference channel | OCNG Pattern | Aggregation level | DCI format | Propagation Condition | Antenna configuration and correlation Matrix | Reference value | |
| Pm-dsg (%) | SNR (dB) |
| 2 | 10 MHz | R.2 FDD | Table B.2.1-1 of [5] | 4 PRB | Format 2C | NLOS with medium correlation | 4x2 | 1 | 12.5 |

### 9.8.2 TDD

#### 9.8.2.1 TDD R-PDCCH performance based on UE-specific reference signals transmitted on antenna port 7 with 1x2 antenna configuration

##### 9.8.2.1.1 Test purpose

This test verifies the demodulation performance of R-PDCCH when R-PDCCH is based on UE-specific reference signals transmitted on antenna port 7 with 1x2 antenna configuration. With a given SNR, the average probability of miss-detection of the Downlink Scheduling Grant for RN, tested on R-PDCCH of the specified reference measurement channels in B.1.1.2 of TR 36.826 [5] remains below a given reference value.

##### 9.8.2.1.2 Test applicability

This test applies to all types of E-UTRA TDD relay node release 11 and forward.

##### 9.8.2.1.3 Minimum conformance requirements

The receiver characteristics of the R-PDCCH are determined by the probability of miss-detection of the relay Downlink Scheduling Grant (Pm-dsg).

Table 9.8.2.1.3-1: Test Parameters for single-layer transmission on port 7 of R-PDCCH

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | | Unit | Test 1 |
| Cyclic prefix | |  | Normal |
| Cell ID | |  | 0 |
| Un subframe type in DeNB | |  | Normal subframe |
| SubframeConfigurationTDD | |  | 4 |
| Number of OFDM symbols for PDCCH | | OFDM symbols | 2 |
| Configuration of OFDM symbols for eNB-to-RN transmission in the first slot | |  | 2 (Note 1) |
| Downlink power allocation | R-PDCCH\_RA | dB | 0 |
| R-PDCCH\_RB | dB | 0 |
| Cell-specific reference symbols | |  | Antenna port 0 |
| CSI reference signal configuration | |  | 1 |
| Number of CSI reference signals configured | |  | 1 |
| CSI reference signal subframe configuration | |  | *I*CSI-RS = 35 |
| at antenna port | | dBm/15 kHz | -98 |
| Number of allocated resource blocks | | PRB | 2 |
| Symbols for unused PRBs | |  | OCNG (Note 2) |
| Simultaneous transmission (Note 3) | |  | No |
| Beamforming Model | |  | No precoding |
| Precoder update granularity | |  | Frequency domain: 1 PRG  Time domain: 1 ms |
| Note 1: As specified in Table 5.4-1 in TS 36.216.  Note 2: These physical resource blocks are assigned to an arbitrary number of virtual UEs with one PDSCH per virtual UE; the data transmitted over the OCNG PDSCHs shall be uncorrelated pseudo random data, which is QPSK modulated.  Note 3: The modulation symbols of the signal under test are mapped onto antenna port 7 while antenna port 8 is unused.  Note 4: | | | |

For the parameters specified in Table 9.8.2.1.3-1 the average probability of a missed relay downlink scheduling grant (Pm-dsg) shall be below the specified value in Table 9.8.2.1.3-2.

Table 9.8.2.1.3-2: Minimum performance for R-PDCCH without cross-interleaving (FRC)

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Test number | Bandwidth | Reference channel | OCNG Pattern | Aggregation level | DCI format | Propagation Condition | Antenna configuration and correlation Matrix | Reference value | |
| Pm-dsg (%) | SNR (dB) |
| 1 | 10 MHz | R.1 TDD | Table B.2.1-1 of [5] | 2 PRB | Format 2C | LOS with strong dominant component | 1x2 | 1 | 2.1 |

##### 9.8.2.1.4 Test description

###### 9.8.2.1.4.1 Initial conditions

Initial conditions are a set of test configurations the RN needs to be tested in and the steps for the SS to take with the RN to reach the correct measurement state.

Configurations of PDSCH and PDCCH before measurement are specified in TS 36.521-1 [7] Annex C.2.

Test Environment: Normal, as defined in TS 36.508 [8] clause 4.1.

Frequencies to be tested: Mid Range, as defined in TS 36.508 [8] clause 4.3.1.1.

Channel Bandwidths to be tested: 10MHz, as defined in TS 36.508 [8] clause 4.3.1.1:

1. Connect the SS, the faders and AWGN noise source to the RN antenna connector (s) as shown in TS 36.508 [8] Annex A, Figure A.9.

2. The parameter settings for the cell are set up according to Table 9.8.2.1.3-1.

3. The backhaul link downlink signals except for R-PDCCH are initially set up according to Annex C.1 and Annex C.3.2 of TR 36.826 [5] and uplink signals according to Annex H.1 and H.3.2 defined in TS 36.521-1[8]. R-PDCCH is mapped to physical resources according to Table 10.2.2.1.3-1, Table 10.2.2.1.3-2 and Table B.1.1.2-1. The signals of R-PDCCH are initially set up according to AnnexC.1 of TR 36.826 [5].

4. Propagation conditions are set according to Annex A clause A.1 of TR 36.826 [5].

5. Ensure the RN is in State 3A-RF according to TS 36.508 [8] clause 5.2A.2 with the following exception. Message contents are defined in clause 9.8.2.1.4.3.

Table 9.8.2.1.4.1-1: RN registration with test mode activation procedure (state 1 to state 2A)

|  |  |  |  |
| --- | --- | --- | --- |
| Step | Procedure | Message Sequence | |
| R - S | Message |
| 1 to 17 | Same procedure for steps 1 to 17 as specified in the procedure in Table 4.5.2A.3-1 [36.508] |  |  |
| 18 | The SS transmits an *RNReconfiguration message to configurate the backhaul link* | <-- | RRC: *RNReconfiguration* |
| 19 | The RN transmits an *RNReconfigurationComplete message to comfirm the configuration of backhal link* | --> | RRC: *RNReconfigurationComplete* |
| 20 | This message includes the ATTACH COMPLETE message. The ACTIVATE DEFAULT EPS BEARER CONTEXT ACCEPT message is piggybacked in ATTACH COMPLETE. | --> | RRC: *ULInformationTransfer*  NAS: ATTACH COMPLETE  NAS: ACTIVATE DEFAULT EPS BEARER CONTEXT ACCEPT |
| 21 | The SS transmits an *RRCConnectionRelease* message to release RRC connection and move to RRC\_IDLE (State 2A). | <-- | RRC: *RRCConnectionRelease* |

###### 9.8.2.1.4.2 Test procedure

1. SS transmits PDSCH via R-PDCCH DCI format 2C for C\_RNTI to transmit the DL RMC according to Table 9.8.2.1.3-1 and 9.8.2.1.3-2.The details of R-PDCCH and PDSCH are specified in Table B1.1.2-1 of TR 36.826 [5] and R.3 TDD in Table C.2-2 of TR 36.826 [5] respectively. The SS sends downlink MAC padding bits on the DL RMC.

2. Set the parameters of the propagation condition, antenna configuration, the correlation matrix and the SNR according to Table 9.8.2.1.5-1 as appropriate.

3. Measure the Pm-dsg for a duration sufficient to achieve statistical significance according to Annex G clause G.4 defined in TS 36.521-1[7]. Count the number of NACKs, ACKs and statDTXs on the UL PUCCH during each subtest interval. Pm-dsg is the ratio (statDTX)/(NACK+ACK+statDTX). If Pm-dsg is less than the value specified in table 9.8.2.1.5-1, pass the RN. Otherwise fail the RN.

###### 9.8.2.1.4.3 Message contents

Message contents are according to TS 36.508 [8] clause 4.6 with the following exceptions.

*Table 9.8.2.1.4.3-1:* RRCConnectionSetupComplete

|  |  |  |  |
| --- | --- | --- | --- |
| Derivation Path: 36.331 clause 6.2.2 | | | |
| Information Element | Value/remark | Comment | Condition |
| RRCConnectionSetupComplete ::= SEQUENCE { |  |  |  |
| rrc-TransactionIdentifier | RRC-TransactionIdentifier-UL |  |  |
| criticalExtensions CHOICE { |  |  |  |
| c1 CHOICE { |  |  |  |
| rrcConnectionSetupComplete-r8 SEQUENCE { |  |  |  |
| selectedPLMN-Identity | 1 |  |  |
| registeredMME | Not checked |  |  |
| dedicatedInfoNAS | Present but contents not checked |  |  |
| nonCriticalExtension SEQUENCE { |  |  |  |
| lateNonCriticalExtension | Not checked |  |  |
| nonCriticalExtension SEQUENCE { |  |  |  |
| gummei-Type-r10 | native |  |  |
| rlf-InfoAvailable-r10 | true |  |  |
| logMeasAvailable-r10 | true |  |  |
| rn-SubframeConfigReq-r10 | required |  |  |
| nonCriticalExtension SEQUENCE{} | No checked |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |

Table 9.8.2.1.4.3-2: *RNReconfiguration*

|  |  |  |  |
| --- | --- | --- | --- |
| Derivation Path: 36.331 clause 6.2.2 | | | |
| Information Element | Value/remark | Comment | Condition |
| RNReconfiguration ::= SEQUENCE { |  |  |  |
| rrc-TransactionIdentifier | RRC-TransactionIdentifier-DL |  |  |
| criticalExtensions CHOICE { |  |  |  |
| c1 CHOISE { |  |  |  |
| RnReconfiguration-r10 SEQUENCE{ |  |  |  |
| rn-SystemInfo-r10{} | Not checked |  |  |
| rn-SubframeConfig-r10 | RN-SubframeConfig-r10 |  |  |
| lateNonCriticalExtension | Not checked |  |  |
| nonCriticalExtension SEQUENCE{} | Not checked |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |
|  |  |  |  |

Table 9.8.2.1.4.3-3: *RN-SubframeConfig*

|  |  |  |  |
| --- | --- | --- | --- |
| Derivation Path: 36.331 clause 6.3.2 | | | |
| Information Element | Value/remark | Comment | Condition |
| RN-SubframeConfig-r10::= SEQUENCE { |  |  |  |
| subframeConfigPattern-r10 CHOICE{ |  |  |  |
| subframeConfigPatternTDD-r10 | 4 |  |  |
| } |  |  |  |
| rpdcch-Config-r10 SEQUENCE{ |  |  |  |
| resourceAllocationType-r10 |  |  |  |
| resourceBlockAssignment-r10 CHOICE{ |  |  |  |
| type01-r10 SEQUENCE{ |  |  |  |
| nrb50-r10 | 0000 0000 1000 0000 0 |  |  |
| } |  |  |  |
| } |  |  |  |
| demodulationRS-r10 CHOICE{ |  |  |  |
| noInterleaving-r10 | dmrs |  |  |
| } |  |  |  |
| pdsch-Start-r10 | 3 |  |  |
| pucch-Config-r10 CHOICE{ |  |  |  |
| tdd choice{ |  |  |  |
| fallbackForFormat3 SEQUENCE{ |  |  |  |
| n1PUCCH-AN-P0-r10 | 0 |  |  |
| n1PUCCH-AN-P1-r10 | Not checked |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |
|  |  |  |  |

Table 9.8.2.1.4.3-4: *RNReconfigurationComplete*

|  |  |  |  |
| --- | --- | --- | --- |
| Derivation Path: 36.331 clause 6.2.2 | | | |
| Information Element | Value/remark | Comment | Condition |
| *RNReconfigurationComplete*::= SEQUENCE { |  |  |  |
| rrc-TransactionIdentifier | RRC-TransactionIdentifier-UL |  |  |
| criticalExtensions CHOICE { |  |  |  |
| c1 CHOICE{ |  |  |  |
| rnReconfigurationComplete-r10 SEQUENCE{ |  |  |  |
| lateNonCriticalExtension | Not checked |  |  |
| nonCriticalExtension | Not checked |  |  |
| } |  |  |  |
| } |  |  |  |
| criticalExtensionsFuture SEQUENCE{} | Not checked |  |  |
| } |  |  |  |
| } |  |  |  |
|  |  |  |  |

###### 9.8.2.1.5 Test requirement

For the parameters specified in Table 9.8.2.1.3-1 the average probability of a missed downlink scheduling grant (Pm-dsg) shall be below the specified value in Table 9.8.2.1.5-1.

Table 9.8.2.1.5-1: Test requirement R-PDCCH without cross-interleaving (FRC)

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Test number | Bandwidth | Reference channel | OCNG Pattern | Aggregation level | DCI format | Propagation Condition | Antenna configuration and correlation Matrix | Reference value | |
| Pm-dsg (%) | SNR (dB) |
| 1 | 10 MHz | R.1 TDD | Table B.2.1-1 of [5] | 2 PRB | Format 2C | LOS with strong dominant component | 1x2 | 1 | 3.1 |

#### 9.8.2.2 TDD R-PDCCH performance based on UE-specific reference signals transmitted on antenna port 7 with 4x2 antenna configuration

##### 9.8.2.2.1 Test purpose

This test verifies the demodulation performance of R-PDCCH when R-PDCCH is based on UE-specific reference signals transmitted on antenna port 7 with 4x2 antenna configuration. With a given SNR, the average probability of miss-detection of the Downlink Scheduling Grant for RN, tested on R-PDCCH of the specified reference measurement channels in B.1.1.2 remains below a given reference value.

##### 9.8.2.2.2 Test applicability

This test applies to all types of E-UTRA TDD relay node release 11 and forward.

##### 9.8.2.2.3 Minimum conformance requirements

The receiver characteristics of the R-PDCCH are determined by the probability of miss-detection of the relay Downlink Scheduling Grant (Pm-dsg).

Table 9.8.2.2.3-1: Test Parameters for single-layer transmission on port 7 of R-PDCCH

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | | Unit | Test 2 |
| Cyclic prefix | |  | Normal |
| Cell ID | |  | 0 |
| Un subframe type in DeNB | |  | Normal subframe |
| SubframeConfigurationTDD | |  | 4 |
| Number of OFDM symbols for PDCCH | | OFDM symbols | 2 |
| Configuration of OFDM symbols for eNB-to-RN transmission in the first slot | |  | 2 (Note 1) |
| Downlink power allocation | R-PDCCH\_RA | dB | 0 |
| R-PDCCH\_RB | dB | 0 |
| Cell-specific reference symbols | |  | Antenna port 0 |
| CSI reference signal configuration | |  | 1 |
| Number of CSI reference signals configured | |  | 4 |
| CSI reference signal subframe configuration | |  | *I*CSI-RS = 35 |
| at antenna port | | dBm/15 kHz | -98 |
| Number of allocated resource blocks | | PRB | 4 |
| Symbols for unused PRBs | |  | OCNG (Note 2) |
| Simultaneous transmission (Note 3) | |  | No |
| Beamforming Model | |  | a precoder vector of size is randomly selected with the number of layers from Table 6.3.4.2.3-2 in TS 36.211 as beamforming weights |
| Precoder update granularity | |  | Frequency domain: 1 PRG  Time domain: 1 ms |
| Note 1: As specified in Table 5.4-1 in TS 36.216.  Note 2: These physical resource blocks are assigned to an arbitrary number of virtual UEs with one PDSCH per virtual UE; the data transmitted over the OCNG PDSCHs shall be uncorrelated pseudo random data, which is QPSK modulated.  Note 3: The modulation symbols of the signal under test are mapped onto antenna port 7 while antenna port 8 is unused.  Note 4: | | | |

For the parameters specified in Table 9.8.2.2.3-1 the average probability of a missed relay downlink scheduling grant (Pm-dsg) shall be below the specified value in Table 9.8.2.2.3-2.

Table 9.8.2.2.3-2: Minimum performance for R-PDCCH without cross-interleaving (FRC)

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Test number | Bandwidth | Reference channel | OCNG Pattern | Aggregation level | DCI format | Propagation Condition | Antenna configuration and correlation Matrix | Reference value | |
| Pm-dsg (%) | SNR (dB) |
| 2 | 10MHz | R.2 TDD | B.2.2-1 of [5] | 4 PRB | Format 2C | NLOS with medium correlation | 4x2 | 1 | 11.5 |

##### 9.8.2.2.4 Test description

###### 9.8.2.2.4.1 Initial conditions

Initial conditions are a set of test configurations the RN needs to be tested in and the steps for the SS to take with the RN to reach the correct measurement state.

Configurations of PDSCH and PDCCH before measurement are specified in TS 36.521-1 [7] Annex C.2.

Test Environment: Normal, as defined in TS 36.508 [8] clause 4.1.

Frequencies to be tested: Mid Range, as defined in TS 36.508 [8] clause 4.3.1.1.

Channel Bandwidths to be tested: 10MHz, as defined in TS 36.508 [8] clause 4.3.1.1:

1. Connect the SS, the faders and AWGN noise source to the RN antenna connector (s) as shown in TS 36.508 [8] Annex A, Figure A.11.

2. The parameter settings for the cell are set up according to Table 9.8.2.2.3-1.

3. The backhaul link downlink signals except for R-PDCCH are initially set up according to Annex C.1 and Annex C.3.2 of TR 36.826 [5] and uplink signals according to Annex H.1 and H.3.2 defined in TS36.521-1[7]. R-PDCCH is mapped to physical resources according to Table 10.2.2.2.3-1, Table 10.2.2.2.3-2 and Table B.1.1.2-1. The signals of R-PDCCH are initially set up according to AnnexC.1.

4. Propagation conditions are set according to Annex A clause A.1 of TR 36.826 [5].

5. Ensure the RN is in State 3A-RF according to TS 36.508 [8] clause 5.2A.2 with the following exceptions. Message contents are defined in clause 9.8.2.2.4.3.

Table 9.8.2.2.4.1-1: RN registration with test mode activation procedure (state 1 to state 2A)

|  |  |  |  |
| --- | --- | --- | --- |
| Step | Procedure | Message Sequence | |
| R - S | Message |
| 1 to 17 | Same procedure for steps 1 to 17 as specified in the procedure in Table 4.5.2A.3-1 [36.508] |  |  |
| 18 | The SS transmits an *RNReconfiguration message to configurate the backhaul link* | <-- | RRC: *RNReconfiguration* |
| 19 | The RN transmits an *RNReconfigurationComplete message to comfirm the configuration of backhal link* | --> | RRC: *RNReconfigurationComplete* |
| 20 | This message includes the ATTACH COMPLETE message. The ACTIVATE DEFAULT EPS BEARER CONTEXT ACCEPT message is piggybacked in ATTACH COMPLETE. | --> | RRC: *ULInformationTransfer*  NAS: ATTACH COMPLETE  NAS: ACTIVATE DEFAULT EPS BEARER CONTEXT ACCEPT |
| 21 | The SS transmits an *RRCConnectionRelease* message to release RRC connection and move to RRC\_IDLE (State 2A). | <-- | RRC: *RRCConnectionRelease* |

###### 9.8.2.2.4.2 Test procedure

1. SS transmits PDSCH via R-PDCCH DCI format 2C for C\_RNTI to transmit the DL RMC according to Table 9.8.2.2.2.3-1 and 9.8.2.2.3-2.The details of R-PDCCH and PDSCH are specified in Table B1.1.2-1 of TR 36.826 [5] and R.4 TDD in Table C.2-2 of TR 36.826 [5] respectively. The SS sends downlink MAC padding bits on the DL RMC.

2. Set the parameters of the propagation condition, antenna configuration, the correlation matrix and the SNR according to Table 9.8.2.2.5-1 as appropriate.

3. Measure the Pm-dsg for a duration sufficient to achieve statistical significance according to Annex G clause G.4 defined in TS 36.521-1[7]. Count the number of NACKs, ACKs and statDTXs on the UL PUCCH during each subtest interval. Pm-dsg is the ratio (statDTX)/(NACK+ACK+statDTX). If Pm-dsg is less than the value specified in table 9.8.2.2.5-1, pass the RN. Otherwise fail the RN

###### 9.8.2.2.4.3 Message contents

Message contents are according to TS 36.508 [8] clause 4.6 with the following exceptions.

Table 9.8.2.2.4.3-1: PhysicalConfigDedicated-DEFAULT

|  |  |  |  |
| --- | --- | --- | --- |
| Derivation Path: 36.331 clause 6.3.2 | | | |
| Information Element | Value/remark | Comment | Condition |
| PhysicalConfigDedicated-DEFAULT ::= SEQUENCE { |  |  |  |
| antennaInfo-r10 CHOICE { |  |  |  |
| AntennaInfoDedicated-r10::= SEQUENCE { |  |  |  |
| transmissionMode | tm9-v1020 |  |  |
| codebookSubsetRestriction-r10 |  |  |  |
| ue-TransmitAntennaSelection CHOICE { |  |  |  |
| release | NULL |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |

Table 9.8.2.2.4.3-2: RRCConnectionSetupComplete

|  |  |  |  |
| --- | --- | --- | --- |
| Derivation Path: 36.331 clause 6.2.2 | | | |
| Information Element | Value/remark | Comment | Condition |
| RRCConnectionSetupComplete ::= SEQUENCE { |  |  |  |
| rrc-TransactionIdentifier | RRC-TransactionIdentifier-UL |  |  |
| criticalExtensions CHOICE { |  |  |  |
| c1 CHOICE { |  |  |  |
| rrcConnectionSetupComplete-r8 SEQUENCE { |  |  |  |
| selectedPLMN-Identity | 1 |  |  |
| registeredMME | Not checked |  |  |
| dedicatedInfoNAS | Present but contents not checked |  |  |
| nonCriticalExtension SEQUENCE { |  |  |  |
| lateNonCriticalExtension | Not checked |  |  |
| nonCriticalExtension SEQUENCE { |  |  |  |
| gummei-Type-r10 | native |  |  |
| rlf-InfoAvailable-r10 | true |  |  |
| logMeasAvailable-r10 | true |  |  |
| rn-SubframeConfigReq-r10 | required |  |  |
| nonCriticalExtension SEQUENCE{} | No checked |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |

Table 9.8.2.2.4.3-3: RNReconfiguration

|  |  |  |  |
| --- | --- | --- | --- |
| Derivation Path: 36.331 clause 6.2.2 | | | |
| Information Element | Value/remark | Comment | Condition |
| RNReconfiguration ::= SEQUENCE { |  |  |  |
| rrc-TransactionIdentifier | RRC-TransactionIdentifier-DL |  |  |
| criticalExtensions CHOICE { |  |  |  |
| c1 CHOISE { |  |  |  |
| RnReconfiguration-r10 SEQUENCE{ |  |  |  |
| rn-SystemInfo-r10{} | Not checked |  |  |
| rn-SubframeConfig-r10 | RN-SubframeConfig-r10 |  |  |
| lateNonCriticalExtension | Not checked |  |  |
| nonCriticalExtension SEQUENCE{} | Not checked |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |
|  |  |  |  |

Table 9.8.2.2.4.3-4: RN-SubframeConfig

|  |  |  |  |
| --- | --- | --- | --- |
| Derivation Path: 36.331 clause 6.3.2 | | | |
| Information Element | Value/remark | Comment | Condition |
| RN-SubframeConfig-r10::= SEQUENCE { |  |  |  |
| subframeConfigPattern-r10 CHOICE{ |  |  |  |
| subframeConfigPatternTDD-r10 | 4 |  |  |
| } |  |  |  |
| rpdcch-Config-r10 SEQUENCE{ |  |  |  |
| resourceAllocationType-r10 | type0 |  |  |
| resourceBlockAssignment-r10 CHOICE{ |  |  |  |
| type01-r10 SEQUENCE{ |  |  |  |
| nrb50-r10 | 0000 0001 1000 0000 0 |  |  |
| } |  |  |  |
| } |  |  |  |
| demodulationRS-r10 CHOICE{ |  |  |  |
| noInterleaving-r10 | dmrs |  |  |
| } |  |  |  |
| pdsch-Start-r10 | 3 |  |  |
| pucch-Config-r10 CHOICE{ |  |  |  |
| tdd choice{ |  |  |  |
| fallbackForFormat3 SEQUENCE{ |  |  |  |
| n1PUCCH-AN-P0-r10 | 0 |  |  |
| n1PUCCH-AN-P1-r10 | Not Checked |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |
| } |  |  |  |
|  |  |  |  |

Table 9.8.2.2.4.3-5: RNReconfigurationComplete

|  |  |  |  |
| --- | --- | --- | --- |
| Derivation Path: 36.331 clause 6.2.2 | | | |
| Information Element | Value/remark | Comment | Condition |
| *RNReconfigurationComplete*::= SEQUENCE { |  |  |  |
| rrc-TransactionIdentifier | RRC-TransactionIdentifier-UL |  |  |
| criticalExtensions CHOICE { |  |  |  |
| c1 CHOICE{ |  |  |  |
| rnReconfigurationComplete-r10 SEQUENCE{ |  |  |  |
| lateNonCriticalExtension | Not checked |  |  |
| nonCriticalExtension | Not checked |  |  |
| } |  |  |  |
| } |  |  |  |
| criticalExtensionsFuture SEQUENCE{} | Not checked |  |  |
| } |  |  |  |
| } |  |  |  |
|  |  |  |  |

##### 9.8.2.2.5 Test requirement

For the parameters specified in Table 9.8.2.2.3-1 the average probability of a missed downlink scheduling grant (Pm-dsg) shall be below the specified value in Table 9.8.2.2.5-1.

Table 9.8.2.2.5-1: Test requirement R-PDCCH without cross-interleaving (FRC)

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Test number | Bandwidth | Reference channel | OCNG Pattern | Aggregation level | DCI format | Propagation Condition | Antenna configuration and correlation Matrix | Reference value | |
| Pm-dsg (%) | SNR (dB) |
| 2 | 10 MHz | R.2 TDD | B.2.2-1 of [5] | 4 PRB | Format 2C | NLOS with medium correlation | 4x2 | 1 | 12.5 |

Annex A (normative): Propagation models for relay demodulation requirements

# A.1 Propagation models for backhaul link

## A.1.1 Delay Profiles

Three representative delay profiles are selected corresponding to the LOS and NLOS scenarios.

### A.1.1.1 LOS between eNB and relay

Table A.1.1-1 and Table A.1.1-2 show the delay profiles for the LOS scenarios: one with strong dominant component and the other with medium dominant component. Note that the first tap in both Table A.1.1-1 and Table A.1.1-2 corresponds to the LOS component, it is therefore a non-fading tap and the corresponding Doppler frequency is 0.

Table A.1.1-1: Delay Profile for LOS Scenario (strong dominant component)

|  |  |
| --- | --- |
| Excess tap delay [ns] | Relative power  [dB] |
| 0 | 0.0 |
| 30 | -21.0 |
| 70 | -22.0 |
| 90 | -23.0 |

Note that as the first tap is at least 21dB stronger than the rest taps, this channel may be considered as an AWGN channel. The exact one-tap static AWGN channel model is FFS.

Table A.1.1-2: Delay Profile for LOS Scenario (medium dominant component)

|  |  |
| --- | --- |
| Excess tap delay [ns] | Relative power  [dB] |
| 0 | 0.0 |
| 30 | -11.0 |
| 70 | -12.0 |
| 90 | -13.0 |
| 110 | -18.0 |
| 190 | -27.2 |
| [410] | [-30.8] |

Note that as the first tap is at least 11dB stronger than the rest taps, this channel may be characterized by one dominant path combined with significant scattering paths.

### A.1.1.2 NLOS between eNB and relay

For NLOS scenario, the delay profile is given in Table A.1.1-3.

Table A.1.1-3: Delay Profile for NLOS Scenario

|  |  |
| --- | --- |
| Excess tap delay [ns] | Relative power  [dB] |
| 0 | 0.0 |
| 30 | -1.0 |
| 70 | -2.0 |
| 90 | -3.0 |
| 110 | -8.0 |
| 190 | -17.2 |
| 410 | -20.8 |

## A.1.2 Doppler Frequency

For NLOS between the eNB and the relay, as the relay nodes are often fixed, hence a low Doppler frequency of 2Hz is used. Note that this 2 Hz Doppler frequency is only used for the new channels (such as R-PDCCH).

## A.1.3 MIMO Correlation Matrices

For LOS component between the eNB and the relay, the spatial channel correlation matrix is modeled as an all one matrix unless cross-polarized antennas are deployed. This is because the correlation matrix for the channel with single LOS component is of rank 1.

For NLOS scenario, the correlation matrices are given in the following tables.

Table A.1.3-1 defines the correlation matrices for the eNB:

Table A.1.3-1: eNB correlation matrix

|  |  |  |  |
| --- | --- | --- | --- |
|  | One antenna | Two antennas | Four antennas |
| eNB Correlation |  |  |  |

Table A.1.3-2 defines the correlation matrices for the relay:

Table A.1.3-2: Relay correlation matrix

|  |  |  |  |
| --- | --- | --- | --- |
|  | One antenna | Two antennas | Four antennas |
| Relay Correlation |  |  |  |

The values of ** and ** for different correlation types are given in Table A.1.3-3.

Table A.1.3-3: Low, Medium and High Correlation Values

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Low correlation | | Medium Correlation | | High Correlation | |
|  |  |  |  |  |  |
| 0 | 0 | 0.3 | 0.9 | 0.9 | 0.9 |

For the channel from the eNB to the relay, the channel spatial correlation matrix  is then given as the Kronecker product of the eNB correlation matrix and the relay correlation matrix, i.e. .

# A.2 multipath propagation fading conditions for access link

Tables A.2-1 to Table A.2-3 show multi-path delay profiles that are used for the performance measurements in multi-path fading environment. All taps have classical Doppler spectrum, defined as:

(CLASS)  for *f*  -*fD*, *fD*.

Table A.2-1: Extended Pedestrian A model (EPA)

|  |  |
| --- | --- |
| Excess tap delay [ns] | Relative power  [dB] |
| 0 | 0.0 |
| 30 | -1.0 |
| 70 | -2.0 |
| 90 | -3.0 |
| 110 | -8.0 |
| 190 | -17.2 |
| 410 | -20.8 |

Table A.2-2: Extended Vehicular A model (EVA)

|  |  |
| --- | --- |
| Excess tap delay [ns] | Relative power [dB] |
| 0 | 0.0 |
| 30 | -1.5 |
| 150 | -1.4 |
| 310 | -3.6 |
| 370 | -0.6 |
| 710 | -9.1 |
| 1090 | -7.0 |
| 1730 | -12.0 |
| 2510 | -16.9 |

Table A.2-3: Extended Typical Urban model (ETU)

|  |  |
| --- | --- |
| Excess tap delay [ns] | Relative power [dB] |
| 0 | -1.0 |
| 50 | -1.0 |
| 120 | -1.0 |
| 200 | 0.0 |
| 230 | 0.0 |
| 500 | 0.0 |
| 1600 | -3.0 |
| 2300 | -5.0 |
| 5000 | -7.0 |

A multipath fading propagation condition is defined by a combination of a multi-path delay profile and a maximum Doppler frequency *fD* which is either 5, 70 or 300 Hz.

Note that the ETU model shown in Table A.2-3 and Doppler frequency of 300Hz are optional for relay access link demodulation requirments.

The relay access link demodulation requirements are the same or subset of the eNB requirements as described in TS 36.104.

Annex B (normative):  
Reference Measurement Channel

# B.1 Reference measurement channels for R-PDCCH performance requirements

## B.1.1 R-PDCCH format without cross-interleaving

### B.1.1.1 FDD

Table B.1.1.1-1: Fixed Reference Channel for R-PDCCH transmitted on single-layer antenna port 7

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Unit | Value | |
| Reference channel |  | R.1 FDD | R.2 FDD |
| Number of transmitter antennas |  | 1 | 4 |
| Channel bandwidth | MHz | 10 | 10 |
| Allocated RB for R-PDCCH | RB | 24, 25 | 23, 24, 25, 26 |
| Aggregation level | PRB | 2 | 4 |
| DCI Format |  | Format 2C | Format 2C |
| Cell ID |  | 0 | 0 |
| Payload (without CRC) | Bits | 42 | 42 |

### B.1.1.2 TDD

Table B.1.1.2-1: Fixed Reference Channel for R-PDCCH transmitted on single-layer antenna port 7

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Unit | Value | |
| Reference channel |  | R.1 TDD | R.2 TDD |
| Number of transmitter antennas |  | 1 | 4 |
| Channel bandwidth | MHz | 10 | 10 |
| Allocated RB for R-PDCCH | RB | 24, 25 | 23, 24, 25, 26 |
| Aggregation level | PRB | 2 | 4 |
| DCI Format |  | Format 2C | Format 2C |
| Cell ID |  | 0 | 0 |
| Payload (without CRC) | Bits | 45 | 45 |

# B.2 OCNG patterns for R-PDCCH performance requirements

The following OCNG patterns are used for modelling allocations to virtual UEs (which are not under test) and/or allocations used for MBSFN. The OCNG pattern for each sub frame specifies the allocations that shall be filled with OCNG, and furthermore, the relative power level of each such allocation.

In each test case the OCNG is expressed by parameters OCNG\_RA and OCNG\_RB which together with a relative power level () specifies the PDSCH EPRE-to-RS EPRE ratios in OFDM symbols with and without reference symbols, respectively. The relative power, which is used for modelling boosting per virtual UE allocation, is expressed by:



where  denotes the relative power level of the i:th virtual UE. The parameter settings of OCNG\_RA, OCNG\_RB, and the set of relative power levels are chosen such that when also taking allocations to the UE under test into account, as given by a PDSCH reference channel, a constant transmitted power spectral density that is constant on an OFDM symbol basis is targeted.

Moreover the OCNG pattern is accompanied by a PCFICH/PDCCH/PHICH reference channel which specifies the control region. For any aggregation and PHICH allocation, the PDCCH and any unused PHICH groups are padded with resource element groups with a power level given respectively by PDCCH\_RA/RB and PHICH\_RA/RB as specified in the test case such that a total power spectral density in the control region that is constant on an OFDM symbol basis is targeted.

## B.2.1 FDD

### B.2.1.1 OCNG FDD pattern 1for R-PDCCH

This OCNG Pattern fills with OCNG all empty PRB-s (PRB-s with no allocation of data or system information) of the DL sub-frames, when the unallocated area is discontinuous (divided in two parts by the allocated area – two sided) or continuous (one sided) in the frequency domain, starts with PRB 0 and ends with PRB *NRB*-1.

Table B.2.1-1: OCNG for FDD R-PDCCH

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Relative power level *γPRB* [dB] | | | | | PDSCH Data |
| Subframe | | | | |
| Allocated subframes for R-PDCCH | | Subframes unallocated for R-PDCCH | | |
| The 1st slot | The 2nd slot | 0 | 5 | Other subframes |
| Allocation | | | | |
| 0 – (First allocated PRB-1)  and  (Last allocated PRB+1) – (*NRB*-1) | First unallocated PRB  –  Last unallocated PRB | First unallocated PRB  –  Last unallocated PRB | First unallocated PRB  –  Last unallocated PRB | First unallocated PRB  –  Last unallocated PRB |
| 0 | 0 | 0 | 0 | 0 | Note 1 |
| Note 1: These physical resource blocks are assigned to an arbitrary number of virtual UEs with one PDSCH per virtual UE; the data transmitted over the OCNG PDSCHs shall be uncorrelated pseudo random data, which is QPSK modulated. The parameter *γPRB* is used to scale the power of PDSCH.  Note 2: If two or more transmit antennas with CRS are used in the test, the OCNG shall be transmitted to the virtual users by all the transmit antennas with CRS according to transmission mode 2. The parameter *γPRB* applies to each antenna port separately, so the transmit power is equal between all the transmit antennas with CRS used in the test. The antenna transmission modes are specified in clause 7.1 in 3GPP TS 36.213. | | | | | |

## B.2.2 TDD

### B.2.2.1 OCNG TDD pattern 1for R-PDCCH

This OCNG Pattern fills with OCNG all empty PRB-s (PRB-s with no allocation of data or system information) of the subframes available for DL transmission (depending on TDD UL/DL configuration), when the unallocated area is discontinuous (divided in two parts by the allocated area – two sided) or continuous (one sided) in the frequency domain, starts with PRB 0 and ends with PRB *NRB* -1.

Table B.2.2-1: OCNG for TDD R-PDCCH

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Relative power level *γPRB* [dB] | | | | | | PDSCH Data |
| Subframe (only if available for DL Note 2) | | | | | |
| Allocated subframes for R-PDCCH | | Subframes unallocated for R-PDCCH | | | |
| The 1st slot | The 2nd slot | 0 | 5 | **1 and 6 (as special subframes)** | **Other normal subframes** |
| Allocation | | | | | |
| 0 – (First allocated PRB-1)  and  (Last allocated PRB+1) – (*NRB*-1) | First unallocated PRB  –  Last unallocated PRB | First unallocated PRB  –  Last unallocated PRB | First unallocated PRB  –  Last unallocated PRB | First unallocated PRB  –  Last unallocated PRB | First unallocated PRB  –  Last unallocated PRB |
| 0 | 0 | 0 | 0 | 0 | 0 | Note 1 |
| Note 1: These physical resource blocks are assigned to an arbitrary number of virtual UEs with one PDSCH per virtual UE; the data transmitted over the OCNG PDSCHs shall be uncorrelated pseudo random data, which is QPSK modulated. The parameter *γPRB* is used to scale the power of PDSCH.  Note 2: Subframes available for DL transmission depends on the Uplink-Downlink configuration in Table 4.2-2 in 3GPP TS 36.211.  Note 3: If two or more transmit antennas with CRS are used in the test, the OCNG shall be transmitted to the virtual users by all the transmit antennas with CRS according to transmission mode 2. The parameter *γPRB* applies to each antenna port separately, so the transmit power is equal between all the transmit antennas with CRS used in the test. The antenna transmission modes are specified in clause 7.1 in 3GPP TS 36.213. | | | | | | |

Annex C (normative):  
Physical Channel Set-up for conformance tests

# C.1 Set-up for R-PDCCH

Table C.1-1 is applicable for demodulation performance requirements in which uniform RS-to-EPRE boosting for R-PDCCH.

Table C.1-1: Downlink Physical Channels transmitted during a connection (FDD and TDD)

|  |  |  |
| --- | --- | --- |
| Physical Channel | EPRE Ratio | Note |
| R-PDCCH | R-PDCCH\_RA = A |  |
| R-PDCCH\_RB = B |
| PDSCH | PDSCH\_RA = A |  |
| PDSCH\_RB = B |

NOTE 1: A= B = 0 dB means no RS boosting.

NOTE 2: A denotes the ratio of PDSCH EPRE to cell-specific RS EPRE among PDSCH REs in all the OFDM symbols not containing cell-specific RS. B denotes the ratio of PDSCH EPRE to cell-specific RS EPRE among PDSCH REs in all the OFDM symbols containing cell-specific RS.

The power allocation for OFDM symbols and reference signals is the same as defined in Annex C.3.2 in TS 36.521-1 [7].

The PDCCH aggregation level for R-PDCCH demodulation tests is 8 CCE-s.

# C.2 Set-up for PDSCH

Table C.2-1: PDSCH Reference Channel FDD for R-PDCCH test

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Unit | Value | |
| Reference channel |  | R.3 FDD | R.4 FDD |
| Number of transmitter antennas |  | 1 | 4 |
| Channel bandwidth | MHz | 10 | 10 |
| Allocated Resource Blocks |  | 24 (Note 2) | 21 (Note 3) |
| Modulation |  | QPSK | QPSK |
| Target Coding Rate |  | 1/3 | 1/3 |
| Information Bit Payload |  | 2088 |  |
| For Sub-Frames 1,2,3,4,6,7,8,9 | Bits | 2088 | 1480 |
| For Sub-Frame 5 |  | n/a | n/a |
| For Sub-Frame0 | Bits | n/a | n/a |
| Number of Code Blocks per Sub-Frame |  |  |  |
| For Sub-Frames 1,2,3,4,6,7,8,9 |  | 1 | 1 |
| For Sub-Frame 5 |  | n/a | n/a |
| For Sub-Frame 0 |  | n/a | n/a |
| Binary Channel Bits Per Sub-Frame |  |  |  |
| For Sub-Frames 1,2,3,4,6,7,8,9 | Bits | 6048 | 5040 |
| For Sub-Frame 5 | Bits | n/a | n/a |
| For Sub-Frame 0 |  | n/a | n/a |
| Note 1: 2 symbols allocated to PDCCH for all BW, and DMRS port 7 is used.  Note 2: PRB #0 to RPB #23 is allocated for PDSCH transmission.  Note 3:  PRB #0 to RPB #20 is allocated for PDSCH transmission. | | | |

Table C.2-2: PDSCH Reference Channel TDD for R-PDCCH test

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | Unit | Value | | |
| Reference channel |  | R.3 TDD | R.4 TDD |  |
| Number of transmitter antennas |  | 1 | 4 |  |
| Channel bandwidth | MHz | 10 | 10 |  |
| Uplink-Downlink Configuration (Note 2) |  | 1 | 1 |  |
| Special subframe configuration(Note 3) |  | 4 | 4 |  |
| Allocated Resource Blocks |  | 24 (Note 4) | 21 (Note 5) |  |
| Modulation |  | QPSK | QPSK |  |
| Target Coding Rate |  | 1/3 | 1/3 |  |
| Information Bit Payload |  |  |  |  |
| For Sub-Frame 4,9 |  | 2088 | 1480 |  |
| For Sub-Frame 1,6 | Bits | n/a | n/a |  |
| For Sub-Frame 5 | Bits | n/a | n/a |  |
| For Sub-Frame 0 | Bits | n/a | n/a |  |
| Number of Code Blocks per Sub-Frame |  |  |  |  |
| For  Sub-Frame 4,9 | Bits | 1 | 1 |  |
| For Sub-Frame 1,6 | Bits | n/a | n/a |  |
| For Sub-Frame 5 | Bits | n/a | n/a |  |
| For Sub-Frame 0 | Bits | n/a | n/a |  |
| Binary Channel Bits Per Sub-Frame |  |  |  |  |
| For Sub-Frame 4,9 | Bits | 6048 | 5040 |  |
| For Sub-Frame 1,6 | Bits | n/a | n/a |  |
| For Sub-Frame 5 | Bits | n/a | n/a |  |
| For Sub-Frame 0 | Bits | n/a | n/a |  |
| Note 1: 2 symbols allocated to PDCCH for all BW, and DMRS port 7 is used.  Note 2: As per Table 4.2-2 in TS 36.211.  Note 3: As specified in Table 4.2-1 in TS 36.211.  Note 4: PRB #0 to RPB #23 is allocated for PDSCH transmission.  Note 5: PRB #0 to RPB #20 is allocated for PDSCH transmission. | | | | |

Annex D (informative):  
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Change history | | | | | | | |
| Date | TSG # | TSG Doc. | CR | Rev | Subject/Comment | Old | New |
| 2012-10 | RAN4#64bis | R4-125715 |  |  | Skeleton TS for Relay Conformance Testing |  | 0.0.1 |
| 2012-11 | RAN4#65 | R4-126627 |  |  | Added sections 8.0 Access Performance Requirements; and 9.8 Demodulation of R-PDCCH | 0.0.1 | 0.1.0 |
| 2012-11 | RAN4#66 | R4-126634 |  |  | Updated Sections 2 on References; section 3 on Definitions, symbols, and abbreviations; section 4 on General test conditions and declarations; and section 5 on Operating bands and channel arrangement; | 0.1.0 | 0.2.0 |
| 2013-04 | RAN4#66bis | R4-130540 |  |  | Updated section 4.7 on interpretation of tests | 0.2.0 | 0.3.0 |
| 2013-04 | RAN4#66bis | R4-130540 |  |  | Updated section 6 on transmitter characteristics | 0.2.0 | 0.3.0 |
| 2013-04 | RAN4#66bis | R4-130544 |  |  | Updated section 7 on receiver characteristics | 0.2.0 | 0.3.0 |
| 2013-04 | RAN4#66bis | R4-130552 |  |  | Updated section 9 on backhaul performance requirements | 0.2.0 | 0.3.0 |
| 2013-04 | RAN4#66bis | R4-125893, R4-126297, R4-126806, R4-130233 |  |  | Updated section 9.8.2 on TDD backhaul link test requirements | 0.2.0 | 0.3.0 |
| 2013-05 | RAN4#67 | R4-131184 |  |  | Updated backhaul link conformance tests to be consistent with changes in CR 007 for TR 36.826 | 0.3.0 | 0.4.0 |
| 2013-05 | RAN4#67 | R4-131569 |  |  | Updates MCL in section 6.2 and minimum output power in section 6.3.2 for the backhaul link test requirements | 0.3.0 | 0.4.0 |
| 2013-05 | RAN4#67 |  |  |  | Editorial corrections and reference corrections and additions | 0.3.0 | 0.4.0 |
| 2013-05 | RAN4#67 |  |  |  | Updated TOC | 0.3.0 | 0.4.0 |
| 2013-05 | RAN4#67 | R4132368 |  |  | Corrections to unwanted emissions tests in section 6.5.3 | 0.4.0 | 1.0.0 |
| 2013-05 | RAN4#67 | R4-132363 |  |  | Corrections to output power tests in section 6.2.5 | 0.4.0 | 1.0.0 |
| 2013-05 | RAN4#67 | R4-132979 |  |  | Corrections to blocking for co-location requirements in section 7.6.3 | 0.4.0 | 1.0.0 |
| 2013-05 | RAN4#67 | R4132945 |  |  | Correction to backhaul configuration tests in section 9.8 | 0.4.0 | 1.0.0 |
| 2013-05 | RP-60 | RP-130648 |  |  | TR Approved by RAN | 1.0.0 | 11.0.0 |
| 2013-09 |  |  |  |  | Editorial Correction of the version in the change history table | 11.0.0 | 11.0.1 |
| 2013-09 | RP-61 | RP-131285 | 0001 |  | CR on TS 36.117 Section 7.7.1: Backhaul Link Receiver Spurious Emissions | 11.0.1 | 11.1.0 |
| 2014-09 | SP-65 | - | - | - | Update to Rel-12 version (MCC) | 11.1.0 | 12.0.0 |
| 2015-07 | RP-68 | RP-150955 | 0005 |  | Corrections on power class for relay backhaul link | 12.0.0 | 12.1.0 |
| 2015-07 | RP-68 | RP-150955 | 0009 |  | Corrections for transmitter requirements in TS 36.117 | 12.0.0 | 12.1.0 |
| 2015-09 | RP-69 | RP-151476 | 0013 | - | Correction on the transmitter requirements in TS36.117 | 12.1.0 | 12.2.0 |
| 2015-09 | RP-69 | RP-151476 | 0015 | - | Correction on test requirement for Relay nodes | 12.1.0 | 12.2.0 |
| 2015-12 | RP-70 | RP-152132 | 0017 |  | Some corrections for TS36.117 | 12.2.0 | 12.3.0 |
| 2016-01 | SP-70 | - | - | - | Update to Rel-13 version (MCC) | 12.3.0 | 13.0.0 |
| 2016-01 |  | - | - | - | Editorial correction in the cover page | 13.0.0 | 13.0.1 |
| 2017-03 | RP-75 | - | - | - | Update to Rel-14 version (MCC) | 13.0.1 | 14.0.0 |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2018-09 | RAN#81 |  |  |  |  | Update to Rel-15 version (MCC) | 15.0.0 |
| 2020-06 | SA#88 | - | - | - | - | Update to Rel-16 version (MCC) | **16.0.0** |