3GPP TR 36.762 V16.0.0 (2019-06)

Technical Report

3rd Generation Partnership Project;

Technical Specification Group Radio Access Network;

410 – 430 MHz Evolved Universal Terrestrial Radio Access (E-UTRA) Frequency Division Duplex (FDD) Band(s) for LTE Public Protection and Disaster Relief (PPDR) and Professional Mobile Radio (PMR) / Public Access Mobile Radio (PAMR) in Europe;

(Release 16)

** 

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.  
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.  
This Report is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2019, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword [4](#__RefHeading___Toc13089345)

1 Scope [5](#__RefHeading___Toc13089346)

2 References [5](#__RefHeading___Toc13089347)

3 Abbreviations [5](#__RefHeading___Toc13089348)

3.1 Abbreviations [5](#__RefHeading___Toc13089349)

4 Frequency band arrangements and regulatory background [6](#__RefHeading___Toc13089350)

4.1 Frequency allocations and compatibility studies [6](#__RefHeading___Toc13089351)

4.2 Relevant ECC Decisions [6](#__RefHeading___Toc13089352)

5 Operating band, channel bandwidths, channel numbering [8](#__RefHeading___Toc13089353)

6 Study of UE and BS requirements [10](#__RefHeading___Toc13089354)

6.1 UE requirements [10](#__RefHeading___Toc13089355)

6.2 BS requirements [17](#__RefHeading___Toc13089356)

Annex A: Change history [22](#__RefHeading___Toc13089357)

# Foreword

This Technical Report has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# 1 Scope

The present document is a technical report for the work item of 410 – 430 MHz E-UTRA FDD Band(s) for LTE PPDR and PMR/PAMR in Europe.

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications"

[2] RP-182898, “New WID on 410 – 430 MHz E-UTRA FDD Band(s) for LTE PPDR and PMR/PAMR in Europe”

[3] ECC Report 283, Compatibility and sharing studies related to the introduction of broadband and narrowband systems in the bands 410-430 MHz and 450-470 MHz

[4] ECC Decision (04)06, The availability of frequency bands for the introduction of Wide Band Digital Land Mobile PMR/PAMR in the 400 MHz and 800/900 MHz bands

[5] ECC Decision (16)02, Harmonised technical conditions and frequency bands for the implementation of Broadband Public Protection and Disaster Relief (BB-PPDR) systems, [amended xx yy 2019]

[6] ECC Decision (19)02, Land mobile systems in the frequency ranges 68-87.5 MHz, 146-174 MHz, 406.1-410 MHz, 410-430 MHz, 440-450 MHz, and 450-470 MHz

[7] 3GPP TR 36.101: "Evolved Universal Terrestrial Radio Access (E-UTRA); User Equipment (UE) radio transmission and reception"

[8] 3GPP TR 36.104: "Evolved Universal Terrestrial Radio Access (E-UTRA); Base Station (BS) radio transmission and reception"

# 3 Abbreviations

## 3.1 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply.   
An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

PAMR Public Access Mobile Radio

PMR Private Mobile Radio

PMSE Programme Making and Special Events

# 4 Frequency band arrangements and regulatory background

## 4.1 Frequency allocations and compatibility studies

The ECC Report 283 [3] considers the compatibility and sharing studies related to the introduction of broadband and narrowband systems in the band 410-430 MHz and in adjacent bands. It is stated that the 400 MHz band is very complex – both in terms of which services already use the bands and on the density of usage by country.

ECC Decision (04)06 [4] decides that Wide Band Digital Land Mobile PMR/PAMR systems in this band shall be with 10 MHz duplex spacing between the transmit frequencies of mobile stations (410-420 MHz) and the transmit frequencies of base stations (420-430 MHz). The same duplex spacing applies to 450 MHz bands.



Figure 4.1-1: Illustrative mobile service allocations in the 400 MHz range: Simplex (SI) and paired Mobile station (MS) Base station (BS) use (from [3])

The band 406.1-410 MHz is allocated to fixed, mobile (except aeronautical) and radio astronomy services on a primary basis. Many countries in Europe have this band registered for radio astronomy service, and administrations are urged to take all practical steps to protect the service from harmful interference. The service involves only passive systems, which are very sensitive. To meet the needs of radio astronomy, there may be a need to limit the unwanted emission levels of the radio transmitters and their use in the vicinity of the radio astronomy observatories. The band is also used for many simplex PMR/PAMR services.

In the band 420-430 MHz there is a secondary allocation to radiolocation service in the majority of European countries, except for the UK where it is allocated on a primary basis. On 430-440 MHz, radiolocation has a primary allocation. 420-450 MHz is the tuning range of airborne and ground radars. This frequency range is harmonised for NATO ground, air and naval military radar systems.

The ECC Report 283 includes sharing studies with new LTE-based systems as aggressors and various other systems as victims, and concludes on required protection distances and unwanted emission masks. The compatibility is considered with narrowband PMR, digital television above 470 MHz, radars (radiolocation), radio astronomy, fixed links, PMSE, paging devices, and short range devices. The study results are used for basis of the regulatory decisions, which are outlined in section 4.2.

## 4.2 Relevant ECC Decisions

The technical conditions for operating broadband PPDR systems in the frequency range 410-430 MHz in Europe are listed in ECC Decision (16)02, which has been amended on [5]. The same Decision covers PPDR also for 700 MHz range and 450 MHz range. Regarding 410 MHz operation, the document lists the following new frequency bands:

CEPT administrations wishing to introduce additional spectrum for BB-PPDR in parts of the 400 MHz range **shall apply** LRTC with channelling arrangements 1.4 MHz, 3 MHz or 5 MHz within the following paired frequency ranges:

a) 450.5-456.0 MHz (uplink) / 460.5-466.0 MHz (downlink) those specified in Annex 2;

b) 452.0-457.5 MHz (uplink) / 462.0-467.5 MHz (downlink) those specified in Annex 2;

c) 410.0-415.0 MHz (uplink) / 420.0-425.0 MHz (downlink) those specified in Annex 3;

d) 411.0-416.0 MHz (uplink) / 421.0-426.0 MHz (downlink) those specified in Annex 3;

e) 412.0-417.0 MHz (uplink) / 422.0-427.0 MHz (downlink) those specified in Annex 3.

Annex 3 of the Decision include the least restrictive technical conditions derived from ECC Report 283 [3] for both user equipment and base stations. Channel bandwidths of 1.4, 3, and 5 MHz are allowed.

The maximum mean in-block power for UE uplink transmissions is 23 dBm. Some administrations may allow up to 31 dBm for special deployment scenarios e.g. for fixed rural installations. Also the uplink maximum power may be limited to protect other services on a cell-by-cell basis. The UE maximum unwanted emission levels are the same as E-UTRA general spectrum emission mask (as in TS 36.101 [7]).

The base station conditions only specify unwanted emission levels to protect the UL band at 410-420 MHz with   
-43 dBm/100 kHz EIRP, and also the same level is required to be met at 1 MHz offset from the DL transmit band edge. Based on national requirements, additional 40 dB of unwanted emissions suppression may be needed to protect radiolocation services.

The technical conditions for operating land mobile systems in the 410-430 MHz range in Europe are covered in ECC Decision (19)02 [6]. The same frequency ranges are identified as for PPDR systems:

CEPT administrations wishing to introduce spectrum for land mobile systems with channel bandwidth of 1.25 MHz, 1.4 MHz, 3 MHz and 5 MHz in parts of the 400 MHz range shall apply technical conditions within the following paired frequency arrangements:

a) 410-415 MHz (uplink) / 420-425 MHz (downlink) those specified in Annex 2;

b) 411-416 MHz (uplink) / 421-426 MHz (downlink) those specified in Annex 2;

c) 412-417 MHz (uplink) / 422-427 MHz (downlink) those specified in Annex 2;

d) 451-456 MHz (uplink) / 461-466 MHz (downlink) those specified in Annex 3;

e) 452.5-457.5 MHz (uplink) / 462.5-467.5 MHz (downlink) those specified in Annex 3;

For land mobile, the least restrictive technical conditions in Annex 2 of the Decision allow the same 1.4, 3, and 5 MHz channels as the PPDR for E-UTRA, but additionally 1.25 MHz channels for CDMA systems.

The UE conditions for transmit power and unwanted emission mask are the same as for PPDR, including the provision for 31 dBm output power in special deployments. While the PPDR conditions do not include limits for spurious emissions, the land mobile conditions include limits that are the same as for E-UTRA in TS 36.101 [7] and TS 36.104 [8].

The base station conditions likewise are the same as for PPDR, except that additional unwanted emission requirements apply within 0 to 1 MHz offset from the band edge.

The following tables collect the regulatory requirements regarding in-block and out-of-block emission requirements for E-UTRA UE and BS.

Table 4.2-1: UE transmitter characteristics (from [5] and [6])

|  |  |
| --- | --- |
| Parameter | Value |
| Channel bandwidth | 1.25 MHz (CDMA) 1.4, 3, or 5 MHz (LTE) |
| Maximum mean in-block power | 23 dBm (Note) |
| Note: administrations may use higher UE maximum mean in-block power for special deployment scenarios, e.g. fixed terminal stations in rural areas provided that protection of other services, networks and applications is not compromised. Vice-versa, the maximum mean in-block power of UEs for the protection of other services may be limited on a cell-by-cell basis. | |

Table 4.2-2: UE maximum unwanted emission levels (from [5] and [6])

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Frequency offset from channel edge (MHz) | Channel width | | | Measurement bandwidth |
| **1.4 MHz** | **3 MHz** | **5 MHz** |
| ± 0-1 | -10 dBm | -13 dBm | -15 dBm | 30 kHz |
| ± 1-2.5 | -10 dBm | -10 dBm | -10 dBm | 1 MHz |
| ± 2.5-2.8 | -25 dBm | -10 dBm | -10 dBm | 1 MHz |
| ± 2.8-5 |  | -10 dBm | -10 dBm | 1 MHz |
| ± 5-6 |  | -25 dBm | -13 dBm | 1 MHz |
| ± 6-10 |  |  | -25 dBm | 1 MHz |

Table 4.2-3: BS in-block e.i.r.p (dBm/cell) (from [5] and [6])

|  |  |
| --- | --- |
| Parameter | Value (dBm/cell) |
| Maximum in-block e.i.r.p. | 56 (optionally: no limit for macro cells) |

Table 4.2-4: BS frequency range of out-of-block emissions (OOBE) (from [5] and [6])

|  |  |  |
| --- | --- | --- |
| Frequency range | Maximum mean out-of-block e.i.r.p. (dBm/cell) | Measurement bandwidth |
| UL band 410-420 MHz | -43 | 100 kHz |
| 0 MHz ≤ ∆ f < 0.2 MHz offset from BS transmit band edge | -11 dBm (see note) | 100 kHz |
| 0.2 MHz ≤ ∆ f < 1 MHz offset from BS transmit band edge | -26 dBm (see note) | 100 kHz |
| 1 MHz ≤ ∆ f < 10 MHz offset from BS transmit band edge | -43 dBm (see note) | 100 kHz |
| Note: additional 40 dB of out-of-block emission reduction may be needed on national level for the protection of radiolocation services. | | |

Requirements regarding transmitter unwanted emissions in the spurious domain follow the same limits that apply for E-UTRA UE and BS in Europe. For receivers, the requirements likewise follow 3GPP definitions.

# 5 Operating band, channel bandwidths, channel numbering

The core objectives of the WI stated the new operating bands to be standardized:

- Standardization of two new FDD E-UTRA bands within 410-415 MHz UL / 420-425 MHz DL range and 412-417 MHz UL / 422-427 MHz DL range

*====== Start of text extracted from TS 36.101 ======*

**5.5 Operating bands**

New FDD E-UTRA bands will get operating band numbers from 65 – 256 range. NR has used numbers up to n86 thus 87 is the first available.

Table 5.5-1 E-UTRA operating bands

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| E‑UTRA Operating Band | Uplink (UL) operating band BS receive UE transmit | | | Downlink (DL) operating band BS transmit  UE receive | | | Duplex Mode |
| FUL\_low – FUL\_high | | | FDL\_low – FDL\_high | | |
| 76 |  | N/A |  | 1427 MHz | – | 1432 MHz | FDD2 |
| 85 | 698 MHz | – | 716 MHz | 728 MHz | – | 746 MHz | FDD |
| 87 | 410 MHz | – | 415 MHz | 420 MHz | – | 425 MHz | FDD |
| 88 | 412 MHz | – | 417 MHz | 422 MHz | – | 427 MHz | FDD |
| NOTE 1: Band 6, 23 is not applicable  .... | | | | | | | |

**5.5E Operating bands for UE category 0, UE category M1 and M2 and UE category 1bis**

UE category M1 and M2 are in the scope of the WI this those are added into the list of applicable M1/M2 bands.

UE category M1 and M2 is designed to operate in the E-UTRA operating bands 1, 2, 3, 4, 5, 7, 8, 11, 12, 13, 14, 18, 19, 20, 21, 25, 26, 27, 28, 31, 66, 71, 72, 73, 74, 85, 87 and 88 in both half duplex FDD mode and full-duplex FDD mode, and in bands 39, 40 and 41 in TDD mode. The E-UTRA bands are defined in Table 5.5-1.

**5.5F Operating bands for category NB1 and NB2**

UE category NB1 and NB2 are in the scope of the WI this those are added into the list of applicable NB1/NB2 bands.

Category NB1 and NB2 are designed to operate in the E-UTRA operating bands 1, 2, 3, 4, 5, 8, 11, 12, 13, 14, 17, 18, 19, 20, 21, 25, 26, 28, 31, 41, 66, 70, 71, 72, 73, 74, 85, 87 and 88 which are defined in Table 5.5-1. Category NB1 and NB2 systems operate in HD-FDD duplex mode or in TDD mode.

**5.6 UE channel bandwidth**

From the WID objectives we can determine the applicable channel bandwidths.

Table 5.6.1-1: E-UTRA channel bandwidth

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| E-UTRA band / Channel bandwidth | | | | | | |
| E-UTRA Band | 1.4 MHz | 3 MHz | 5 MHz | 10 MHz | 15 MHz | 20 MHz |
| 74 | Yes | Yes | Yes | Yes1 | Yes1 | Yes1 |
| 85 |  |  | Yes1 | Yes1 |  |  |
| 87 | Yes | Yes1 | Yes1 |  |  |  |
| 88 | Yes | Yes1 | Yes1 |  |  |  |
| NOTE 1: 1 refers to the bandwidth for which a relaxation of the specified UE receiver sensitivity requirement (subclause 7.3) is allowed.  ... | | | | | | |

5.7.3 Carrier frequency and EARFCN

EARFCN is specified as follows.

Table 5.7.3-1: E-UTRA channel numbers

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| E-UTRA Operating  Band | Downlink | | | Uplink | | |
| FDL\_low (MHz) | NOffs-DL | Range of NDL | FUL\_low (MHz) | NOffs-UL | Range of NUL |
| 85 | 728 | 70366 | 70366 - 70545 | 698 | 134002 | 134002 - 134181 |
| 87 | 420 | 70546 | 70546 - 70595 | 410 | 134182 | 134182 - 134231 |
| 88 | 422 | 70596 | 70596 - 70645 | 422 | 134231 | 134231 - 134280 |
| NOTE 1: The channel numbers that designate carrier frequencies so close to the operating band edges that the carrier extends beyond the operating band edge shall not be used. This implies that the first 7, 15, 25, 50, 75 and 100 channel numbers at the lower operating band edge and the last 6, 14, 24, 49, 74 and 99 channel numbers at the upper operating band edge shall not be used for channel bandwidths of 1.4, 3, 5, 10, 15 and 20 MHz respectively.  ... | | | | | | |

**5.7.4 TX–RX frequency separation**

TX-RX separation is 10 MHz.

Table 5.7.4-1: Default UE TX-RX frequency separation

| E-UTRA Operating Band | TX – RX  carrier centre frequency separation |
| --- | --- |
| 85 | 30 MHz |
| 87 | 10 MHz |
| 88 | 10 MHz |
| NOTE 1: Default TX-RX carrier centre frequency separation. | |

*====== End of text extracted from TS 36.101 ======*

# 6 Study of UE and BS requirements

## 6.1 UE requirements

Due to exactly same operating band arrangement with bands 31 and 72 i.e. uplink and downlink bandwidth of 5 MHz with a duplex-gap of 5 MHz and the fact that these new bands are also very close to bands 31 and 72 in terms of center frequency it is proposed to define the requirements based on the work done for bands 31 and 72 [2].

*====== Start of text extracted from TS 36.101 ======*

**6.2.2 UE maximum output power**

This work-item is for PC1 and PC3. Tolerances are adopted from E-UTRA bands 31 and 72.

Table 6.2.2-1: UE Power Class

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| EUTRA band | Class 1 (dBm) | Tolerance (dB) | Class 2 (dBm) | Tolerance (dB) | Class 3 (dBm) | Tolerance (dB) | Class 4 (dBm) | Tolerance (dB) |
| 85 |  |  |  |  | 23 | ±22 |  |  |
| 87 | 31 | +2/-3 |  |  | 23 | ±2 |  |  |
| 88 | 31 | +2/-3 |  |  | 23 | ±2 |  |  |
| NOTE 1: Void  ...  NOTE 8: Generally, PC1 UE is not targeted for smartphone form factor. | | | | | | | | |

**6.2.2E UE maximum output power for Category M1 and M2 UE**

Bands 87 and 88 are added to M1 and M2 power class table.

Table 6.2.2E-1: UE Power Class

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| EUTRA band | Class 3 (dBm) | Tolerance (dB) | Class 5 (dBm) | Tolerance (dB) | Class 6 (dBm) | Tolerance (dB) |
| 31 | 23 | ±2 | 20 | ±2 | 14 | ±2.5 |
| 72 | 23 | ±2 | 20 | ±2 | 14 | ±2.5 |
| 87 | 23 | ±2 | 20 | ±2 | 14 | ±2.5 |
| 88 | 23 | ±2 | 20 | ±2 | 14 | ±2.5 |
| NOTE 1: Void  ... | | | | | | |

**6.2.2F UE maximum output power for category NB1 and NB2**

Bands 87 and 88 are added to NB1 and NB2 power class table.

Table 6.2.2F-1: UE Power Class

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| EUTRA band | Class 3 (dBm) | Tolerance (dB) | Class 5 (dBm) | Tolerance (dB) | Class 6 (dBm) | Tolerance (dB) |
| 31 | 23 | ±2 | 20 | ±2 | 14 | ±2.5 |
| 72 | 23 | ±2 | 20 | ±2 | 14 | ±2.5 |
| 87 | 23 | ±2 | 20 | ±2 | 14 | ±2.5 |
| 88 | 23 | ±2 | 20 | ±2 | 14 | ±2.5 |

**6.2.4 UE maximum output power with additional requirements**

No A-MPR is necessary.

**6.6.3.2 Spurious emission band UE co-existence**

UE to UE co-existence is specified as for band 72 with an exception that there is no harmonic impact to bands 3, 8 or 40. Band 87 has second harmonic for band 20.

Table 6.6.3.2-1: Requirements

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| E-UTRA Band | Spurious emission | | | | | | |
| Protected band | Frequency range (MHz) | | | Maximum Level (dBm) | MBW (MHz) | NOTE |
| 72 | E-UTRA Band 1, 7, 20, 22, 28, 31, 32, 33, 34, 38, 42, 43, 47, 52, 65, 68, [72] | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3, 8, 40 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 470 | - | 694 | -42 | 8 |  |
| 87 | E-UTRA Band 1, 3, 7, 8, 20, 22, 28, 31, 32, 33, 34, 38, 40, 42, 43, 47, 52, 65, 68, 72 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band, 20 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 470 | - | 694 | -42 | 8 |  |
| 88 | E-UTRA Band 1, 3, 7, 8, 20, 22, 28, 31, 32, 33, 34, 38, 40, 42, 43, 47, 52, 65, 68, 72 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 470 | - | 694 | -42 | 8 |  |
| NOTE 1: FDL\_low and FDL\_high refer to each E-UTRA frequency band specified in Table 5.5-1  ... | | | | | | | |

**6.6.3G Spurious emission for V2X Communication**

Bands 87 and 88 are added as protected bands for applicable V2X con-current band Configurations.

Table 6.6.3G-0: Requirements for inter-band con-current V2X operation

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| V2X con-current band Configuration | Spurious emission | | | | | | |
| Protected band | Frequency range (MHz) | | | Maximum Level (dBm) | MBW (MHz) | NOTE |
| V2X\_3A-47A | E-UTRA Band 1, 5, 7, 8, 26, 28, 34, 39, 40, 44, 45, 65, 87, 88 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3 | FDL\_low | - | FDL\_high | -50 | 1 | 3 |
| E-UTRA Band 22, 41, 42, 52 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 5925 | - | 5950 | -30 | 1 | 7,8 |
| Frequency range | 5815 | - | 5855 | -30 | 1 | 7 |
| V2X\_7A-47A | E-UTRA Band 1, 3, 5, 7, 8, 22, 26, 28, 34, 39, 40, 41, 42, 44, 45, 52, 65, 87, 88 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 2570 | - | 2575 | +1.6 | 5 | 3, 6, 4 |
| Frequency range | 2575 | - | 2595 | -15.5 | 5 | 3, 6, 4 |
| Frequency range | 2595 | - | 2620 | -40 | 1 | 3, 6 |
| Frequency range | 5925 | - | 5950 | -30 | 1 | 7, 8 |
| Frequency range | 5815 | - | 5855 | -30 | 1 | 7 |
| V2X\_8A-47A | E-UTRA Band 1, 5, 26, 28, 34, 39, 40, 44, 45, 65, 87, 88 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 7, 22, 41, 42, 52 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 3, 8 | FDL\_low | - | FDL\_high | -50 | 1 | 2, 3 |
| Frequency range | 5925 | - | 5950 | -30 | 1 | 7, 8 |
| Frequency range | 5815 | - | 5855 | -30 | 1 | 7 |
| V2X\_20A-47A | E-UTRA Band 1, 3, 7, 8, 22, 31, 32, 33, 34, 40, 43, 65, 67, 87, 88 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 20 | FDL\_low | - | FDL\_high | -50 | 1 | 3 |
| E-UTRA Band 38, 42, 52, 69 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 758 | - | 788 | -50 | 1 |  |
| Frequency range | 5925 | - | 5950 | -30 | 1 | 7, 8 |
| Frequency range | 5815 | - | 5855 | -30 | 1 | 7 |
| V2X\_28A-47A | E-UTRA Band 1, 22, 42, 43, 65, 87, 88 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 1 | FDL\_low | - | FDL\_high | -50 | 1 | 10, 11 |
| E-UTRA Band 3, 7, 8, 20, 31, 38, 40 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 470 | - | 694 | -42 | 8 | 3, 12 |
| Frequency range | 470 | - | 710 | -26.2 | 6 | 13 |
| Frequency range | 662 | - | 694 | -26.2 | 6 | 3 |
| Frequency range | 758 | - | 773 | -32 | 1 | 3 |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range | 5925 | - | 5950 | -30 | 1 | 7, 8 |
| Frequency range | 5815 | - | 5855 | -30 | 1 | 7 |
| V2X\_34A-47A | E-UTRA Band 1, 3, 5, 7, 8, 11, 18, 19, 20, 21, 22, 26, 28, 31, 32, 33, 34, 38,39, 40, 41, 42, 43, 44, 45, 52, 65, 67, 69, 87, 88 | FDL\_low | - | FDL\_high | -50 | 1 | 9 |
| Frequency range | 5925 | - | 5950 | -30 | 1 | 7, 8 |
| Frequency range | 5815 | - | 5855 | -30 | 1 | 7 |

**7.3 Reference sensitivity power level**

Band 31 and 72 REFSENS is adopted.

Table 7.3.1-1: Reference sensitivity QPSK PREFSENS

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Channel bandwidth | | | | | | | |
| E-UTRA Band | 1.4 MHz (dBm) | 3 MHz (dBm) | 5 MHz (dBm) | 10 MHz (dBm) | 15 MHz (dBm) | 20 MHz (dBm) | Duplex Mode |
| 31 | -99.0 | -95.7 | -93.5 |  |  |  | FDD |
| 72 | -99.0 | -95.7 | -93.5 |  |  |  | FDD |
| 87 | -99.0 | -95.7 | -93.5 |  |  |  | FDD |
| 88 | -99.0 | -95.7 | -93.5 |  |  |  | FDD |
| NOTE 1: The transmitter shall be set to PUMAX as defined in subclause 6.2.5  ... | | | | | | | |

Table 7.3.1-2: Uplink configuration for reference sensitivity

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| E-UTRA Band / Channel bandwidth / NRB / Duplex mode | | | | | | | |
| E-UTRA Band | 1.4 MHz | 3 MHz | 5 MHz | 10 MHz | 15 MHz | 20 MHz | Duplex Mode |
| 31 | 6 | 54 | 54 |  |  |  | FDD |
| 72 | 6 | 54 | 54 |  |  |  | FDD |
| 31 | 6 | 54 | 54 |  |  |  | FDD |
| 72 | 6 | 54 | 54 |  |  |  | FDD |
| NOTE 1: 1 refers to the UL resource blocks shall be located as close as possible to the downlink operating band but confined within the transmission bandwidth configuration for the channel bandwidth (Table 5.6-1).  NOTE 2: For the UE which supports both Band 11 and Band 21 the uplink configuration for reference sensitivity is FFS.  NOTE 3: 3 refers to Band 20; in the case of 15MHz channel bandwidth, the UL resource blocks shall be located at RBstart 11 and in the case of 20MHz channel bandwidth, the UL resource blocks shall be located at RBstart 16  NOTE 4: 4 refers to Bands 31, 72, 73, 87 and 88; in the case of 3 MHz channel bandwidth, the UL resource blocks shall be located at RBstart 9 and in the case of 5 MHz channel bandwidth, the UL resource blocks shall be located at RBstart 10. | | | | | | | |

**7.3.1E Minimum requirements (QPSK) for UE category 0, M1, M2 and 1bis**

Bands 87 and 88 are added to M1 and M2 REFSENS tables.

Table 7.3.1E-3: Reference sensitivity for FDD and TDD UE category M1 QPSK PREFSENS

|  |  |  |
| --- | --- | --- |
| E-UTRA Band | REFSENS (dBm) | Duplex Mode |
| 31 | -96.5 | FDD |
| 72 | -96.5 | FDD |
| 87 | -96.5 | FDD |
| 88 | -96.5 | FDD |
| NOTE 1: The transmitter shall be set to PUMAX as defined in subclause 6.2.5  ... | | |

Table 7.3.1E-4: Reference sensitivity for HD-FDD UE category M1 QPSK PREFSENS

|  |  |  |
| --- | --- | --- |
| E-UTRA Band | REFSENS (dBm) | Duplex Mode |
| 31 | -97.3 | HD-FDD |
| 72 | -97.3 | HD-FDD |
| 87 | -97.3 | HD-FDD |
| 88 | -97.3 | HD-FDD |
| NOTE 1: The transmitter shall be set to PUMAX as defined in subclause 6.2.5  ... | | |

Table 7.3.1E-5: FDD and TDD UE category M1 Uplink configuration for reference sensitivity

|  |  |  |
| --- | --- | --- |
| E-UTRA Band | NRB | Duplex Mode |
| 31 | 61 | FDD and HD-FDD |
| 72 | 61 | FDD and HD-FDD |
| 87 | 61 | FDD and HD-FDD |
| 88 | 61 | FDD and HD-FDD |
| NOTE 1: 1 refers to the UL resource blocks shall be located as close as possible to the downlink operating band but confined within the transmission bandwidth configuration for the channel bandwidth (Table 5.6-1). | | |

**7.3.1F.1 Reference sensitivity for UE category NB1 and NB2**

Bands 87 and 88 are added to NB1 and NB2 REFSENS table.

Table 7.3.1F.1-1: Reference sensitivity for UE category NB1 and NB2

|  |  |
| --- | --- |
| Operating band | REFSENS [dBm] |
| 1, 2, 3, 5, 8, 11, 12, 13, 14, 17, 18, 19, 20, 21, 25, 26, 28, 31, 41, 66, 70, 71, 72, 73, 74, 85, 87, 88 | - 108.2 |

**7.6.1 In-band blocking**

Bands 87 and 88 are added to in-band blocking table.

Table 7.6.1.1-2: In-band blocking

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| E-UTRA band | Parameter | Unit | Case 1 | Case 2 | Case 3 | Case 4 | Case 5 | Case 6 |
| PInterferer | dBm | -56 | -44 | Void | Void | -38 | -15 |
| FInterferer (offset) | MHz | =-BW/2 – FIoffset,case 1  &  =+BW/2 + FIoffset,case 1 | ≤-BW/2 – FIoffset,case 2  &  ≥+BW/2 + FIoffset,case 2 | -BW/2 - 11 |  |
| 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 17, 18, 19, 20, 21, 22, 23,  25, 26, 27, 28, 31, 33, 34, 35, 36, 37, 38, 39, 40, 41, 42, 43, 44, 45, 48, 50, 51, 52, 65, 66, 68, 70, 72, 73, 74, 85, 87, 88 | FInterferer | MHz | (NOTE 2) | FDL\_low – 15  to  FDL\_high + 15 |  |  |
| 30 | FInterferer | MHz | (NOTE 2) | FDL\_low – 15  to  FDL\_high + 15 | FDL\_low – 11 |  |
| 71 | FInterferer | MHz | (NOTE 2) | FDL\_low – 12 to FDL\_high + 15 |  |  |  | FDL-low - 12 |
| NOTE 1: For certain bands, the unwanted modulated interfering signal may not fall inside the UE receive band, but within the first 15 MHz below or above the UE receive band  ... | | | | | | | | |

**7.6.2 Out-of-band blocking**

Bands 87 and 88 are added to Out-of-band blocking table.

Table 7.6.2.1-2: Out of band blocking

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| E-UTRA band | Parameter | Units | Frequency | | | |
| Range 1 | Range 2 | Range 3 | Range 4 |
| PInterferer | dBm | -44 | -30 | -15 | -15 |
| 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 17, 18, 19, 20, 21, 22, 23, 24, 25, 26, 27, 28, 30, 31, 33, 34, 35, 36, 37, 38, 39, 40, 41, 42 (NOTE 2), 43 (NOTE 2), 44, 45, 48 (NOTE 2), 50, 51, 52 (NOTE 6), 65, 66, 68, 70, 71, 72, 73, 74, 85, 87, 88 | FInterferer (CW) | MHz | FDL\_low -15 to  FDL\_low -60 | FDL\_low -60 to  FDL\_low -85 | FDL\_low -85 to  1 MHz | - |
| FDL\_high +15 to  FDL\_high + 60 | FDL\_high +60 to  FDL\_high +85 | FDL\_high +85 to  +12750 MHz | - |
| 2, 5, 12, 17, 85 | FInterferer | MHz | - | - | - | FUL\_low**-** FUL\_high  (NOTE 5) |
| NOTE 1: For the UE which supports both Band 11 and Band 21 the out of blocking is FFS.  ... | | | | | | |

*====== End of text extracted from TS 36.101 ======*

## 6.2 BS requirements

The following BS specific TS 36.104 [8] changes are expected due to introduction of Band 87 and 88:

*====== Start of text extracted from TS 36.104 ======*

**6.6.3.1 Minimum requirements for Wide Area BS (Category A)**

For E-UTRA BS operating in Bands 5, 6, 8, 12, 13, 14, 17, 18, 19, 26, 27, 28, 29, 31, 44, 68, 71, 72, 73, 85, 87, 88 emissions shall not exceed the maximum levels specified in Tables 6.6.3.1‑1 to 6.6.3.1-3.

**6.6.3.2.1 Category B requirements (Option 1)**

For E-UTRA BS operating in Bands 5, 8, 12, 13, 14, 17, 20, 26, 27, 28, 29, 31, 44, 68, 67, 71, 72, 73, 85, 87, 88 emissions shall not exceed the maximum levels specified in Tables 6.6.3.2.1-1 to 6.6.3.2.1-3:

**6.6.4.3 Additional spurious emissions requirements**

Table 6.6.4.3.1-1: BS Spurious emissions limits for E-UTRA BS for co-existence with systems operating in other frequency bands

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| System type for E-UTRA to co-exist with | Frequency range for co-existence requirement | Maximum Level | Measurement Bandwidth | Note |
| E-UTRA Band 87 | 420 - 425 MHz | -52 dBm | 1 MHz | This requirement does not apply to E-UTRA BS operating in band 87 or 88. |
| 410 – 415 MHz | -49 dBm | 1 MHz | This requirement does not apply to E-UTRA BS operating in band 87, since it is already covered by the requirement in sub-clause 6.6.4.2 |
| E-UTRA Band 88 | 422 - 427 MHz | -52 dBm | 1 MHz | This requirement does not apply to E-UTRA BS operating in band 87 or 88. |
| 412 - 417 MHz | -49 dBm | 1 MHz | This requirement does not apply to E-UTRA BS operating in band 88, since it is already covered by the requirement in sub-clause 6.6.4.2. This requirement does not apply to E-UTRA BS operating in band 87. |

**6.6.4.4 Co-location with other base stations**

Table 6.6.4.4.1-1: BS Spurious emissions limits for Wide Area BS co-located with another BS

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Type of co-located BS | Frequency range for co-location requirement | Maximum Level | Measurement Bandwidth | Note |
| WA E-UTRA Band 87 | 410 - 415 MHz | -96 dBm | 100 kHz |  |
| WA E-UTRA Band 88 | 412 - 417 MHz | -96 dBm | 100 kHz |  |

Table 6.6.4.4.1-2: BS Spurious emissions limits for Local Area BS co-located with another BS

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Type of co-located BS | Frequency range for co-location requirement | Maximum Level | Measurement Bandwidth | Note |
| LA E-UTRA Band 87 | 410 - 415 MHz | -88 dBm | 100 kHz |  |
| LA E-UTRA Band 88 | 412 - 417 MHz | -88 dBm | 100 kHz |  |

Table 6.6.4.4.1-3: BS Spurious emissions limits for Medium range BS co-located with another BS

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Type of co-located BS | Frequency range for co-location requirement | Maximum Level | Measurement Bandwidth | Note |
| MR E-UTRA Band 87 | 410 - 415 MHz | -91 dBm | 100 kHz |  |
| MR E-UTRA Band 88 | 412 - 417 MHz | -91 dBm | 100 kHz |  |

**7.6.1.1 Minimum requirement**

Table 7.6.1.1-1: Blocking performance requirement for Wide Area BS for E-UTRA

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Operating Band | Centre Frequency of Interfering Signal [MHz] | | | Interfering Signal mean power [dBm] | Wanted Signal mean power [dBm] | Interfering signal centre frequency minimum frequency offset from the lower/upper Base Station RF Bandwidth edge or sub-block edge inside a sub-block gap [MHz] | Type of Interfering Signal |
| 31, 72, 73, 74, 87, 88 | (FUL\_low -20) | to | (FUL\_high +5) | -43 | PREFSENS +6dB (Note 1) | See table 7.6.1.1-2 | See table 7.6.1.1-2 |
| 1  (FUL\_high +5) | to  to | (FUL\_low -20)  12750 | -15 | PREFSENS +6dB (Note 1) |  | CW carrier |

Table 7.6.1.1-1a: Blocking performance requirement for Local Area BS for E-UTRA

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Operating Band | Centre Frequency of Interfering Signal [MHz] | | | Interfering Signal mean power [dBm] | Wanted Signal mean power [dBm] | Interfering signal centre frequency minimum frequency offset from the lower/upper Base Station RF Bandwidth edge or sub-block edge inside a sub-block gap [MHz] | Type of Interfering Signal |
| 31, 72, 73, 74, 87, 88 | (FUL\_low -20) | to | (FUL\_high +5) | -35 | PREFSENS +6dB (Note 1) | See table 7.6.1.1-2 | See table 7.6.1.1-2 |
| 1  (FUL\_high +5) | to  to | (FUL\_low -20)  12750 | -15 | PREFSENS +6dB (Note 1) |  | CW carrier |

Table 7.6.1.1-1c: Blocking performance requirement for Medium Range BS for E-UTRA

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Operating Band | Centre Frequency of Interfering Signal [MHz] | | | Interfering Signal mean power [dBm] | Wanted Signal mean power [dBm] | Interfering signal centre frequency minimum frequency offset to the lower/higher Base Station RF Bandwidth edge or sub-block edge inside a sub-block gap [MHz] | Type of Interfering Signal |
| 31, 72, 73, 74, 87, 88 | (FUL\_low -20) | to | (FUL\_high +5) | -38 | PREFSENS +6dB (Note 1) | See table 7.6.1.1-2 | See table 7.6.1.1-2 |
| 1  (FUL\_high +5) | to  to | (FUL\_low -20)  12750 | -15 | PREFSENS +6dB (Note 1) |  | CW carrier |

Table 7.6.1.1-3: Blocking performance requirement for Wide Area BS for NB-IoT standalone operation

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Operating Band | Centre Frequency of Interfering Signal [MHz] | | | Interfering Signal mean power [dBm] | Wanted Signal mean power [dBm] | Interfering signal centre frequency minimum frequency offset from the lower/upper Base Station RF Bandwidth edge or sub-block edge inside a sub-block gap [MHz] | Type of Interfering Signal |
| 31, 72, 73, 74, 87, 88 | (FUL\_low -20) | to | (FUL\_high +5) | -43 | PREFSENS +6dB (Note 1) | See table 7.6.1.1-4 | See table 7.6.1.1-4 |
| 1  (FUL\_high +5) | to  to | (FUL\_low -20)  12750 | -15 (Note 2) | PREFSENS +6dB (Note 1) |  | CW carrier |

Table 7.6.1.1-3a: Blocking performance requirement for Local Area BS for NB-IoT standalone operation

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Operating Band | Centre Frequency of Interfering Signal [MHz] | | | Interfering Signal mean power [dBm] | Wanted Signal mean power [dBm] | Interfering signal centre frequency minimum frequency offset from the lower/upper Base Station RF Bandwidth edge or sub-block edge inside a sub-block gap [MHz] | Type of Interfering Signal |
| 31, 72, 74, 87, 88 | (FUL\_low -20) | to | (FUL\_high +5) | -35 | PREFSENS +6dB (Note 2) | See table 7.6.1.1-4 | See table 7.6.1.1-4 |
| 1  (FUL\_high +5) | to  to | (FUL\_low -20)  12750 | -15 (Note 2) | PREFSENS +6dB (Note 2) |  | CW carrier |

Table 7.6.1.1-3c: Blocking performance requirement for Medium Range BS for NB-IoT standalone operation

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Operating Band | Centre Frequency of Interfering Signal [MHz] | | | Interfering Signal mean power [dBm] | Wanted Signal mean power [dBm] | Interfering signal centre frequency minimum frequency offset from the lower/upper Base Station RF Bandwidth edge or sub-block edge inside a sub-block gap [MHz] | Type of Interfering Signal |
| 31, 72, 74, 87, 88 | (FUL\_low -20) | to | (FUL\_high +5) | -38 | PREFSENS +6dB (Note 1) | See table 7.6.1.1-4 | See table 7.6.1.1-4 |
| 1  (FUL\_high +5) | to  to | (FUL\_low -20)  12750 | -15 (Note 2) | PREFSENS +6dB (Note 1) |  | CW carrier |

Table 7.6.1.1-5: Blocking performance requirement for Wide Area BS for E-UTRA with NB-IoT in-band/guard band operation

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Operating Band | Centre Frequency of Interfering Signal [MHz] | | | Interfering Signal mean power [dBm] | Wanted Signal mean power [dBm] | Interfering signal centre frequency minimum frequency offset from the lower/upper Base Station RF Bandwidth edge or sub-block edge inside a sub-block gap [MHz] | Type of Interfering Signal |
| 31, 72, 73, 74, 87, 88 | (FUL\_low -20) | to | (FUL\_high +5) | -43 | PREFSENS +6dB (Note 1) | See table 7.6.1.1-6 | See table 7.6.1.1-6 |
| 1  (FUL\_high +5) | to  to | (FUL\_low -20)  12750 | -15 (Note 3) | PREFSENS +6dB (Note 1) |  | CW carrier |

Table 7.6.1.1-5a: Blocking performance requirement for Local Area BS for E-UTRA with NB-IoT in-band/guard band operation

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Operating Band | Centre Frequency of Interfering Signal [MHz] | | | Interfering Signal mean power [dBm] | Wanted Signal mean power [dBm] | Interfering signal centre frequency minimum frequency offset from the lower/upper Base Station RF Bandwidth edge or sub-block edge inside a sub-block gap [MHz] | Type of Interfering Signal |
| 31, 72, 74, 87, 88 | (FUL\_low -20) | to | (FUL\_high +5) | -35 | PREFSENS +6dB (Note 1) | See table 7.6.1.1-6 | See table 7.6.1.1-6 |
| 1  (FUL\_high +5) | to  to | (FUL\_low -20)  12750 | -15 (Note 3) | PREFSENS +6dB (Note 1) |  | CW carrier |

Table 7.6.1.1-5c: Blocking performance requirement for Medium Range BS for E-UTRA with NB-IoT in-band/guard band operation

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Operating Band | Centre Frequency of Interfering Signal [MHz] | | | Interfering Signal mean power [dBm] | Wanted Signal mean power [dBm] | Interfering signal centre frequency minimum frequency offset from the lower/upper Base Station RF Bandwidth edge or sub-block edge inside a sub-block gap [MHz] | Type of Interfering Signal |
| 31, 72, 74, 87, 88 | (FUL\_low -20) | to | (FUL\_high +5) | -38 | PREFSENS +6dB (Note 1) | See table 7.6.1.1-6 | See table 7.6.1.1-6 |
| 1  (FUL\_high +5) | to  to | (FUL\_low -20)  12750 | -15 (Note 3) | PREFSENS +6dB (Note 1) |  | CW carrier |

**7.6.2 Co-location with other base stations**

Table 7.6.2.1-1: Blocking performance requirement for E-UTRA and NB-IoT Wide Area BS when co-located with BS in other frequency bands.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Co-located BS type | Centre Frequency of Interfering Signal (MHz) | Interfering Signal mean power (dBm) | Wanted Signal mean power (dBm) | Type of Interfering Signal |
| WA E-UTRA Band 87 | 420 – 425 | +16\*\* | PREFSENS + 6dB\* | CW carrier |
| WA E-UTRA Band 88 | 422 – 427 | +16\*\* | PREFSENS + 6dB\* | CW carrier |

Table 7.6.2.1-2: Blocking performance requirement for E-UTRA and NB-IoT Local Area BS when co-located with BS in other frequency bands.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Co-located BS type | Centre Frequency of Interfering Signal (MHz) | Interfering Signal mean power (dBm) | Wanted Signal mean power (dBm) | Type of Interfering Signal |
| LA E-UTRA Band 87 | 420 – 425 | -6\*\* | PREFSENS + 6dB\* | CW carrier |
| LA E-UTRA Band 88 | 422 – 427 | -6\*\* | PREFSENS + 6dB\* | CW carrier |

Table 7.6.2.1-3: Blocking performance requirement for E-UTRA and NB-IoT Medium Range BS when co-located with BS in other frequency bands.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Co-located BS type | Centre Frequency of Interfering Signal (MHz) | Interfering Signal mean power (dBm) | Wanted Signal mean power (dBm) | Type of Interfering Signal |
| MR E-UTRA Band 87 | 420 – 425 | +8\*\* | PREFSENS + 6dB\* | CW carrier |
| MR E-UTRA Band 88 | 422 – 427 | +8\*\* | PREFSENS + 6dB\* | CW carrier |

*====== End of text extracted from TS 36.104 ======*

Annex A:  
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2019-02 | RAN4#90 | R4-1900058 |  |  |  | TR skeleton for TR 36.762 | 0.0.1 |
| 2019-04 | RAN4#90-Bis | R4-1903531 |  |  |  | Approved TPs from RAN4#90 captured  R4-1900060 TP to TR 36.762: Regulatory background for LTE 410 - 430 MHz WI  R4-1900059 TP to TR 36.762: Analysis on UE requirements for LTE 410 – 430 MHz  R4-1900403 TP to TR 36.762: BS requirements | 0.1.0 |
| 2019-06 | RAN#84 |  |  |  |  | 3GPP TR 36.762 V1.0.0 is submitted for 1 step approval | 1.0.0 |
| 2019-06 | RAN#84 | RP-191288 |  |  |  | Approved by plenary – Rel-16 spec under change control | 16.0.0 |