|  |  |
| --- | --- |
| 3GPP TS 38.101-1 V16.17.0 (2023-09) | |
| Technical Specification | |
| 3rd Generation Partnership Project;  Technical Specification Group Radio Access Network;  NR;  User Equipment (UE) radio transmission and reception;  Part 1: Range 1 Standalone  (Release 16) | |
|  | |
| *5G-logo_175px* | 3GPP-logo_web |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  http://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2023, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 16

1 Scope 18

2 References 18

3 Definitions, symbols and abbreviations 18

3.1 Definitions 18

3.2 Symbols 19

3.3 Abbreviations 21

4 General 23

4.1 Relationship between minimum requirements and test requirements 23

4.2 Applicability of minimum requirements 23

4.3 Specification suffix information 23

5 Operating bands and channel arrangement 24

5.1 General 24

5.2 Operating bands 24

5.2A Operating bands for CA 26

5.2A.0 General 26

5.2A.1 Intra-band CA 26

5.2A.2 Inter-band CA 27

5.2A.2.1 Inter-band CA (two bands) 27

5.2A.2.2 Inter-band CA (three bands) 31

5.2A.2.3 Inter-band CA (four bands) 32

5.2B Operating bands for DC 32

5.2C Operating band combination for SUL 32

5.2D Operating bands for UL MIMO 33

5.2E Operating band for V2X 33

5.2E.1 V2X operating bands 33

5.2E.2 V2X operating bands for con-current operation 34

5.3 UE channel bandwidth 34

5.3.1 General 34

5.3.2 Maximum transmission bandwidth configuration 35

5.3.3 Minimum guardband and transmission bandwidth configuration 35

5.3.4 RB alignment 37

5.3.5 UE channel bandwidth per operating band 37

5.3.6 Asymmetric channel bandwidths 40

5.3A UE channel bandwidth for CA 41

5.3A.1 General 41

5.3A.2 Maximum transmission bandwidth configuration for CA 41

5.3A.3 Minimum guardband and transmission bandwidth configuration for CA 41

5.3A.4 Void 43

5.3A.5 UE channel bandwidth per operating band for CA 43

5.3E Channel bandwidth for V2X 44

5.3E.1 General 44

5.3E.2 Channel bandwidth for V2X concurrent operation 45

5.4 Channel arrangement 45

5.4.1 Channel spacing 45

5.4.1.1 Channel spacing for adjacent NR carriers 45

5.4.2 Channel raster 45

5.4.2.1 NR-ARFCN and channel raster 45

5.4.2.2 Channel raster to resource element mapping 46

5.4.2.3 Channel raster entries for each operating band 46

5.4.3 Synchronization raster 49

5.4.3.1 Synchronization raster and numbering 49

5.4.3.3 Synchronization raster entries for each operating band 50

5.4.4 TX–RX frequency separation 53

5.4A Channel arrangement for CA 53

5.4A.1 Channel spacing for CA 53

5.4A.2 Channel raster for CA 54

5.4A.3 Synchronization raster for CA 54

5.4A.4 Tx-Rx frequency separation for CA 54

5.4B Reserved 54

5.4C Reserved 54

5.4D Reserved 54

5.4E Channel arrangement for V2X 54

5.4E.1 Channel spacing 54

5.4E.2 Channel raster 55

5.4E.2.1 NR-ARFCN and channel raster 55

5.4E.2.2 Channel raster to resource element mapping 55

5.4E.2.3 Channel raster entries for each operating band 55

5.4E.3 Synchronization raster for V2X 55

5.5 Void 55

5.5A Configurations for CA 55

5.5A.0 General 55

5.5A.1 Configurations for intra-band contiguous CA 57

5.5A.2 Configurations for intra-band non-contiguous CA 60

5.5A.3 Configurations for inter-band CA 60

5.5A.3.1 Configurations for inter-band CA (two bands) 60

5.5A.3.2 Configurations for inter-band CA (three bands) 72

5.5A.3.3 Configurations for inter-band CA (four bands) 80

5.5B Configurations for DC 83

5.5C Configurations for SUL 84

6 Transmitter characteristics 84

6.1 General 84

6.1A General 84

6.1F General 84

6.2 Transmitter power 84

6.2.1 UE maximum output power 84

6.2.2 UE maximum output power reduction 86

6.2.3 UE additional maximum output power reduction 89

6.2.3.1 General 89

6.2.3.2 A-MPR for NS\_04 94

6.2.3.3 A-MPR for NS\_10 95

6.2.3.4 A-MPR for NS\_05 and NS\_05U 95

6.2.3.5 A-MPR for NS\_40 98

6.2.3.6 A-MPR for NS\_43 and NS\_43U 98

6.2.3.7 A-MPR for NS\_03 and NS\_03U 99

6.2.3.8 A-MPR for NS\_37 100

6.2.3.9 A-MPR for NS\_38 101

6.2.3.10 A-MPR for NS\_39 101

6.2.3.11 A-MPR for NS\_41 101

6.2.3.12 A-MPR for NS\_42 102

6.2.3.13 A-MPR for NS\_18 102

6.2.3.14 A-MPR for NS\_21 103

6.2.3.15 A-MPR for NS\_24 103

6.2.3.16 A-MPR for NS\_27 104

6.2.3.17 A-MPR for NS\_46 105

6.2.3.18 A-MPR for NS\_47 106

6.2.3.19 A-MPR for NS\_50 107

6.2.3.20 A-MPR for NS\_44 107

6.2.3.21 A-MPR for NS\_12 108

6.2.3.22 A-MPR for NS\_13 108

6.2.3.23 A-MPR for NS\_14 109

6.2.3.24 A-MPR for NS\_15 110

6.2.3.25 A-MPR for NS\_45 110

6.2.3.26 A-MPR for NS\_48 111

6.2.3.27 A-MPR for NS\_49 111

6.2.3.28 A-MPR for NS\_51 112

6.2.4 Configured transmitted power 113

6.2A Transmitter power for CA 115

6.2A.1 UE maximum output power for CA 115

6.2A.1.1 UE maximum output power for Intra-band contiguous CA 115

6.2A.1.2 UE maximum output power for Intra-band non-contiguous CA 115

6.2A.1.3 UE maximum output power for Inter-band CA 116

6.2A.1.4 Void 119

6.2A.1.5 Void 119

6.2A.2 UE maximum output power reduction for CA 119

6.2A.2.1 UE maximum output power reduction for Intra-band contiguous CA 119

6.2A.2.2 UE maximum output power reduction for Intra-band non-contiguous CA 121

6.2A.2.2.0 General 121

6.2A.2.2.1 MPR to meet -30dBm/MHz 121

6.2A.2.2.2 MPR to meet -13dBm/MHz 122

6.2A.2.3 UE maximum output power reduction for Inter-band CA 122

6.2A.2.4 Void 122

6.2A.3 UE additional maximum output power reduction for CA 122

6.2A.3.1.1 UE additional maximum output power reduction for Intra-band contiguous CA 122

6.2A.3.1.1.1 A-MPR for CA\_NS\_04 123

6.2A.3.1.2 UE additional maximum output power reduction for Intra-band non-contiguous CA 129

6.2A.3.1.3 UE additional maximum output power reduction for Inter-band CA 131

6.2A.4 Configured output power for CA 133

6.2A.4.1 Configured transmitted power level 133

6.2A.4.1.1 Configured transmitted power for Intra-band contiguous CA 133

6.2A.4.1.2 Configured transmitted power for Intra-band non-contiguous CA 135

6.2A.4.1.3 Configured transmitted power for Inter-band CA 137

6.2A.4.1.4 Void 139

6.2A.4.2 ΔTIB,c for CA 139

6.2A.4.2.1 Void 139

6.2A.4.2.2 Void 139

6.2A.4.2.3 ΔTIB,c for Inter-band CA (two bands) 139

6.2A.4.2.4 ΔTIB,c for Inter-band CA (three bands) 144

6.2A.4.2.5 ΔTIB,c for Inter-band CA (four bands) 147

6.2B Transmitter power for NR-DC 147

6.2B.0 General 147

6.2B.1 UE maximum output power for NR-DC 147

6.2B.2 UE maximum output power reduction for NR-DC 148

6.2B.3 UE additional maximum output power reduction for NR-DC 148

6.2B.4 Configured output power for NR-DC 148

6.2B.4.1 Configured transmitted power level for NR-DC 148

6.2B.4.2 ΔTIB,c for NR-DC 151

6.2C Transmitter power for SUL 151

6.2C.1 Configured transmitted power for SUL 151

6.2C.2 ΔTIB,c 151

6.2D Transmitter power for UL MIMO 152

6.2D.1 UE maximum output power for UL MIMO 152

6.2D.2 UE maximum output power reduction for UL MIMO 153

6.2D.3 UE additional maximum output power reduction for UL MIMO 154

6.2D.4 Configured transmitted power for UL MIMO 154

6.2E Transmitter power for V2X 155

6.2E.1 UE maximum output power for V2X 155

6.2E.1.1 General 155

6.2E.1.2 UE maximum output power for V2X con-current operation 156

6.2E.2 UE maximum output power reduction for V2X 156

6.2E.2.1 General 156

6.2E.2.2 MPR for Power class 3 V2X UE 156

6.2E.2.3 MPR for Power class 3 V2X con-current operation 157

6.2E.3 UE additional maximum output power reduction for V2X 157

6.2E.3.1 General 157

6.2E.3.2 A-MPR for Power class 3 V2X UE by NS\_33 158

6.2E.3.3 A-MPR for Power class 3 V2X UE by NS\_52 160

6.2E.3.4 A-MPR for power class 3 V2X con-current operation 161

6.2E.4 Configured transmitted power for V2X 161

6.2E.4.1 General 161

6.2E.4.2 Configured transmitted power for V2X con-current operation 162

6.2F Transmitter power for shared spectrum channel access 163

6.2F.1 UE maximum output power 163

6.2F.1A UE maximum output power for CA 164

6.2F.1A.1 UE maximum output power for inter-band CA 164

6.2F.2 UE maximum output power reduction 164

6.2F.2A UE maximum output power reduction for CA 165

6.2F.2A.1 UE maximum output power reduction for inter-band CA 165

6.2F.3 UE additional maximum output power reduction 165

6.2F.3.1 General 165

6.2F.3.2 A-MPR for NS\_28 166

6.2F.3.3 A-MPR for NS\_29 167

6.2F.3.4 A-MPR for NS\_30 167

6.2F.3.5 A-MPR for NS\_31 168

6.2F.3.6 A-MPR for NS\_53 168

6.2F.3.7 A-MPR for NS\_54 169

6.2F.3A UE additional maximum output power reduction for CA 169

6.2F.3A.1 UE additional maximum output power reduction for inter-band CA 169

6.2F.4 Configured transmitted power 170

6.3 Output power dynamics 170

6.3.1 Minimum output power 170

6.3.2 Transmit OFF power 170

6.3.3 Transmit ON/OFF time mask 171

6.3.3.1 General 171

6.3.3.2 General ON/OFF time mask 171

6.3.3.3 Transmit power time mask for slot and short or long subslot boundaries 171

6.3.3.4 PRACH time mask 172

6.3.3.5 Void 173

6.3.3.6 SRS time mask 173

6.3.3.7 PUSCH-PUCCH and PUSCH-SRS time masks 174

6.3.3.8 Transmit power time mask for consecutive slot or long subslot transmission and short subslot transmission boundaries 176

6.3.3.9 Transmit power time mask for consecutive short subslot transmissions boundaries 176

6.3.4 Power control 177

6.3.4.1 General 177

6.3.4.2 Absolute power tolerance 177

6.3.4.3 Relative power tolerance 178

6.3.4.4 Aggregate power tolerance 178

6.3A Output power dynamics for CA 178

6.3A.1 Minimum output power for CA 178

6.3A.1.1 Minimum output power for intra-band contiguous CA 178

6.3A.1.2 Minimum output power for intra-band non-contiguous CA 179

6.3A.1.3 Minimum output power for inter-band CA 179

6.3A.1.4 Void 179

6.3A.2 Transmit OFF power for CA 179

6.3A.2.1 Transmit OFF power for intra-band contiguous CA 179

6.3A.2.2 Transmit OFF power for intra-band non-contiguous CA 179

6.3A.2.3 Transmit OFF power for inter-band CA 179

6.3A.2.4 Void 179

6.3A.3 Transmit ON/OFF time mask for CA 179

6.3A.3.1 Transmit ON/OFF time mask for intra-band contiguous CA 179

6.3A.3.2 Transmit ON/OFF time mask for intra-band non-contiguous CA 180

6.3A.3.3 Transmit ON/OFF time mask for inter-band CA 180

6.3A.3.3.1 General 180

6.3A.3.3.2 Time mask for switching between two uplink carriers 180

6.3A.3.4 Void 181

6.3A.4 Power control for CA 181

6.3A.4.1 Power control for intra-band contiguous CA 181

6.3A.4.1.1 Absolute power tolerance 181

6.3A.4.1.2 Relative power tolerance 181

6.3A.4.1.3 Aggregate power control tolerance 182

6.3A.4.2 Power control for intra-band non-contiguous CA 182

6.3A.4.2.1 Absolute power tolerance 182

6.3A.4.2.1.1 Minimum requirements 182

6.3A.4.2.2 Relative power tolerance 182

6.3A.4.2.2.1 Minimum requirements 182

6.3A.4.2.3 Aggregate power control tolerance 183

6.3A.4.3 Power control for inter-band CA 183

6.3A.4.4 Void 183

6.3B Output power dynamics for NR-DC 183

6.3C Output power dynamics for SUL 183

6.3C.1 Void 183

6.3C.2 Void 183

6.3C.3 Transmit ON/OFF time mask for SUL 183

6.3C.3.1 Time mask for switching between two uplink carriers 183

6.3D Output power dynamics for UL MIMO 184

6.3D.1 Minimum output power for UL MIMO 184

6.3D.2 Transmit OFF power for UL MIMO 184

6.3D.3 Transmit ON/OFF time mask for UL MIMO 184

6.3D.4 Power control for UL MIMO 185

6.3E Output power dynamics for V2X 185

6.3E.1 Minimum output power for V2X 185

6.3E.1.1 General 185

6.3E.1.2 Minimum output power for V2X con-current operation 185

6.3E.2 Transmit OFF power for V2X 185

6.3E.2.1 General 185

6.3E.2.2 Transmit OFF power for V2X con-current operation 186

6.3E.3 Transmit ON/OFF time mask for V2X 186

6.3E.3.1 General 186

6.3E.3.2 General time mask 186

6.3E.3.3 S-SSB time mask 187

6.3E.3.4 Transmit ON/OFF time mask for V2X con-current operation 187

6.3E.4 Power control for V2X 187

6.3E.4.1 General 187

6.3E.4.2 Absolute power tolerance 187

6.3E.4.3 Power control for V2X con-current operation 187

6.3F Output power dynamics for shared spectrum channel access 188

6.3F.1 Minimum output power 188

6.3F.2 Transmit OFF power 188

6.3F.3 Transmit ON/OFF time mask 188

6.3F.3.1 General 188

6.3F.3.2 General ON/OFF time mask 188

6.3F.3A General ON/OFF mask for CA 188

6.3F.3A.1 General ON/OFF mask for inter-band CA 188

6.3F.4 Power control 189

6.3F.4.1 General 189

6.3F.4.2 Absolute power tolerance 189

6.3F.4.3 Relative power tolerance 189

6.3F.4.4 Aggregate power tolerance 189

6.4 Transmit signal quality 189

6.4.1 Frequency error 189

6.4.2 Transmit modulation quality 189

6.4.2.0 General 189

6.4.2.1 Error Vector Magnitude 189

6.4.2.1a Error Vector Magnitude including symbols with transient period 190

6.4.2.2 Carrier leakage 191

6.4.2.3 In-band emissions 191

6.4.2.4 EVM equalizer spectrum flatness 192

6.4.2.4.1 Requirements for Pi/2 BPSK modulation 193

6.4A Transmit signal quality for CA 194

6.4A.1 Frequency error for CA 194

6.4A.1.1 Frequency error for intra-band contiguous CA 194

6.4A.1.2 Frequency error for intra-band non-contiguous CA 194

6.4A.1.3 Frequency error for inter-band CA 194

6.4A.1.4 Void 195

6.4A.2 Transmit modulation quality for CA 195

6.4A.2.1 Transmit modulation quality for intra-band contiguous CA 195

6.4A.2.1.0 General 195

6.4A.2.1.1 Error Vector Magnitude 195

6.4A.2.1.2 In-band emissions 195

6.4A.2.1.3 Carrier leakage 198

6.4A.2.2 Transmit modulation quality for intra-band non-contiguous CA 198

6.4A.2.2.0 General 198

6.4A.2.2.1 Error Vector Magnitude 198

6.4A.2.2.2 In-band emissions 199

6.4A.2.2.3 Carrier leakage 199

6.4A.2.3 Transmit modulation quality for inter-band CA 199

6.4A.2.4 Void 199

6.4B Transmit signal quality for NR-DC 199

6.4D Transmit signal quality for UL MIMO 199

6.4D.0 General 199

6.4D.1 Frequency error for UL MIMO 200

6.4D.2 Transmit modulation quality for UL MIMO 200

6.4D.2.0 General 200

6.4D.2.1 Error Vector Magnitude 200

6.4D.2.2 Carrier leakage 200

6.4D.2.3 In-band emissions 200

6.4D.2.4 EVM equalizer spectrum flatness for UL MIMO 200

6.4D.3 Time alignment error for UL MIMO 201

6.4D.4 Requirements for coherent UL MIMO 201

6.4E Transmit signal quality for V2X 201

6.4E.1 Frequency error for V2X 201

6.4E.1.1 General 201

6.4E.1.2 Frequency error for V2X con-current operation 202

6.4E.2 Transmit modulation quality for V2X 202

6.4E.2.1 General 202

6.4E.2.2 Error Vector Magnitude for V2X 202

6.4E.2.3 Carrier leakage for V2X 202

6.4E.2.4 In-band emissions for V2X 202

6.4E.2.5 EVM equalizer spectrum flatness for V2X 202

6.4E.2.6 Transmit modulation quality for V2X con-current operation 202

6.4F Transmit signal quality for shared spectrum channel access 203

6.4F.1 Frequency error 203

6.4F.2 Transmit modulation quality 203

6.4F.2.0 General 203

6.4F.2.1 Error Vector Magnitude 203

6.4F.2.2 Carrier leakage 203

6.4F.2.3 In-band emissions 203

6.4F.2.4 EVM equalizer spectrum flatness 204

6.4F.2A Transmit modulation quality for CA 204

6.4F.2A.1 Transmit modulation quality for inter-band CA 204

6.5 Output RF spectrum emissions 205

6.5.1 Occupied bandwidth 205

6.5.2 Out of band emission 205

6.5.2.1 General 205

6.5.2.2 Spectrum emission mask 205

6.5.2.3 Additional spectrum emission mask 206

6.5.2.3.1 Requirements for network signalling value "NS\_35" 206

6.5.2.3.2 Requirements for network signalling value "NS\_04" 207

6.5.2.3.3 Requirements for network signalling values "NS\_03", “NS\_03U”, and "NS\_21" 207

6.5.2.3.4 Requirements for network signalling value "NS\_06" 208

6.5.2.3.5 Void 209

6.5.2.3.6 Void 209

6.5.2.3.7 Void 209

6.5.2.3.8 Requirements for network signalling value "NS\_27" 209

6.5.2.4 Adjacent channel leakage ratio 209

6.5.2.4.1 NR ACLR 209

6.5.2.4.2 UTRA ACLR 210

6.5.3 Spurious emissions 210

6.5.3.0 General 210

6.5.3.1 General spurious emissions 211

6.5.3.2 Spurious emissions for UE co-existence 211

6.5.3.3 Additional spurious emissions 219

6.5.3.3.1 Requirement for network signalling value "NS\_04" 219

6.5.3.3.2 Requirement for network signalling value "NS\_17" 220

6.5.3.3.3 Requirement for network signalling value "NS\_18" 220

6.5.3.3.4 Requirement for network signalling values "NS\_05" and “NS\_05U” 220

6.5.3.3.5 Requirement for network signalling values "NS\_43" and “NS\_43U” 220

6.5.3.3.6 Requirement for network signalling value "NS\_37" 221

6.5.3.3.7 Requirement for network signalling value "NS\_38" 221

6.5.3.3.8 Requirement for network signalling value "NS\_39" 221

6.5.3.3.9 Requirement for network signalling value "NS\_40" 221

6.5.3.3.10 Requirement for network signalling value "NS\_41" 222

6.5.3.3.11 Requirement for network signalling value "NS\_42" 222

6.5.3.3.12 Requirement for network signalling value "NS\_21" 222

6.5.3.3.13 Requirement for network signalling value "NS\_24" 223

6.5.3.3.14 Requirement for network signalling value "NS\_27" 223

6.5.3.3.15 Requirement for network signalling value "NS\_47" 223

6.5.3.3.16 Requirement for network signalling value "NS\_50" 224

6.5.3.3.17 Requirement for network signalling value "NS\_12" 224

6.5.3.3.18 Requirement for network signalling value "NS\_13" 224

6.5.3.3.19 Requirement for network signalling value "NS\_14" 225

6.5.3.3.20 Requirement for network signalling value "NS\_15" 225

6.5.3.3.21 Requirement for network signalling value "NS\_45" 225

6.5.3.3.22 Requirement for network signalling values "NS\_48" and "NS\_51" 226

6.5.3.3.23 Requirement for network signalling value "NS\_49" 226

6.5.3.3.24 Requirement for network signalling value "NS\_44" 226

6.5.3.3.25 Requirement for network signalling value "NS\_46" 227

6.5.4 Transmit intermodulation 227

6.5A Output RF spectrum emissions for CA 228

6.5A.0 General 228

6.5A.1 Occupied bandwidth for CA 228

6.5A.1.1 Void 228

6.5A.1.1a Occupied bandwidth for Intra-band contiguous CA 228

6.5A.1.2 Occupied bandwidth for Intra-band non-contiguous CA 228

6.5A.1.3 Occupied bandwidth for Inter-band CA 228

6.5A.2 Out of band emission for CA 228

6.5A.2.1 General 228

6.5A.2.2 Spectrum emission mask 228

6.5A.2.2.1 Spectrum emission mask for intra-band contiguous CA 228

6.5A.2.2.2 Spectrum emission mask for intra-band non-contiguous CA 229

6.5A.2.2.3 Spectrum emission mask for Inter-band CA 229

6.5.A.2.2.4 Void 229

6.5A.2.3 Additional spectrum emission mask for CA 229

6.5A.2.3.1 Additional spectrum emission mask for intra-band contiguous CA 229

6.5A.2.3.1 Void 230

6.5A.2.3.2 Additional spectrum emission mask for Intra-band non-contiguous CA 230

6.5A.2.3.2.1 Minimum requirement (network signalling value “CA\_NC\_NS\_04”) 230

6.5A.2.3.3 Additional spectrum emission mask for Inter-band CA 230

6.5A.2.4 Adjacent channel leakage ratio 230

6.5A.2.4.1 NR ACLR 230

6.5A.2.4.2 UTRA ACLR 231

6.5A.3 Spurious emission for CA 231

6.5A.3.1 General spurious emissions 231

6.5A.3.2 Spurious emissions for UE co-existence 232

6.5A.3.2.1 Spurious emissions for UE co-existence for intra-band contiguous CA 232

6.5A.3.2.2 Spurious emissions for UE co-existence for intra-band non-contiguous CA 233

6.5A.3.2.3 Spurious emissions for UE co-existence for Inter-band CA 234

6.5A.3.2.4 Void 237

6.5A.3.2.5 Void 237

6.5A.3.2.6 Void 237

6.5A.3.3 Additional spurious emissions for CA 237

6.5A.3.3.1 Additional spurious emissions for intra-band contiguous CA 237

6.5A.3.3.2 Additional spurious emissions for intra-band non-contiguous CA 238

6.5A.4 Transmit intermodulation for CA 238

6.5A.4.2.1 Transmit intermodulation for intra-band contiguous CA 238

6.5A.4.2.2 Void 239

6.5B Output RF spectrum emissions for NR-DC 239

6.5D Output RF spectrum emissions for UL MIMO 239

6.5D.1 Occupied bandwidth for UL MIMO 239

6.5D.2 Out of band emission for UL MIMO 239

6.5D.3 Spurious emission for UL MIMO 240

6.5D.4 Transmit intermodulation for UL MIMO 240

6.5E Output RF spectrum emissions for V2X 240

6.5E.1 Occupied bandwidth for V2X 240

6.5E.1.1 General 240

6.5E.1.2 Occupied bandwidth for V2X con-current operation 240

6.5E.2 Out of band emission for V2X 241

6.5E.2.1 General 241

6.5E.2.2 Spectrum emission mask 241

6.5E.2.2.1 General 241

6.5E.2.2.2 Spectrum emission mask for V2X con-current operation 241

6.5E.2.3 Additional Spectrum emission mask 241

6.5E.2.3.1 Requirements for network signalling value "NS\_33" 241

6.5E.2.3.2 Requirements for network signalling value "NS\_52" 242

6.5E.2.4 Adjacent channel leakage ratio 242

6.5E.2.4.1 General 242

6.5E.2.4.2 ACLR for V2X con-current operation 242

6.5E.3 Spurious emissions for V2X 242

6.5E.3.1 General spurious emissions 242

6.5E.3.2 Spurious emissions for UE co-existence 243

6.5E.3.3 Spurious emissions for UE co-existence for V2X con-current operation 243

6.5E.3.4 Additional spurious emissions requirements for V2X 243

6.5E.3.4.1 General 243

6.5E.3.4.2 Requirements for network signalling value "NS\_33" 244

6.5E.3.4.3 Void 244

6.5E.4 Transmit intermodulation 244

6.5E.4.1 General 244

6.5E.4.2 Transmit intermodulation for V2X con-current operation 244

6.5F Output RF spectrum emissions 244

6.5F.1 Occupied bandwidth 244

6.5F.2 Out of band emission 245

6.5F.2.1 General 245

6.5F.2.2 Spectrum emission mask for operation with shared spectrum channel access 245

6.5F.2.2.0 General 245

6.5F.2.2.1 Spectrum emission mask for non-transmitted channels 246

6.5F.2.3 Additional spectrum emission mask 246

6.5F.2.4 Adjacent channel leakage ratio 246

6.5F.2.4.0 General 246

6.5F.2.4.1 Shared spectrum channel access ACLR 246

6.5F.2.4.2 Additional requirement for network signaled value "NS\_29" 246

6.5F.3 Spurious emissions 247

6.5F.3.0 General 247

6.5F.3.1 General spurious emissions 247

6.5F.3.2 Spurious emissions for UE co-existence 247

6.5F.3.3 Additional spurious emissions 247

6.5F.3.3.0 General 247

6.5F.3.3.1 Requirement for network signalling value "NS\_28" 247

6.5F.3.3.2 Requirement for network signalling value "NS\_29" 248

6.5F.3.3.3 Requirement for network signalling value "NS\_30" 249

6.5F.3.3.4 Requirement for network signalling value "NS\_31" 250

6.5F.3.3.5 Requirements for network signalling value "NS\_53" or "NS\_54" 251

6.5F.4 Transmit intermodulation 251

6.6 Void 251

6.6E Time alignment error 251

7 Receiver characteristics 252

7.1 General 252

7.1A General 252

7.1F General 253

7.2 Diversity characteristics 253

7.3 Reference sensitivity 253

7.3.1 General 253

7.3.2 Reference sensitivity power level 253

7.3.3 ΔRIB,c 261

7.3A Reference sensitivity for CA 262

7.3A.1 General 262

7.3A.2 Reference sensitivity power level for CA 262

7.3A.2.1 Reference sensitivity power level for Intra-band contiguous CA 262

7.3A.2.2 Reference sensitivity power level for Intra-band non-contiguous CA 262

7.3A.2.3 Reference sensitivity power level for Inter-band CA 263

7.3A.2.4 Void 263

7.3A.3 ΔRIB,c for CA 263

7.3A.3.1 General 263

7.3A.3.2 ΔRIB,c for Inter-band CA 263

7.3A.3.2.1 ΔRIB,c for two bands 265

7.3A.3.2.2 Void 268

7.3A.3.2.3 ΔRIB,c for three bands 268

7.3A.3.2.4 ΔRIB,c for four bands 270

7.3A.4 Reference sensitivity exceptions due to UL harmonic interference for CA 270

7.3A.5 Reference sensitivity exceptions due to intermodulation interference due to 2UL CA 275

7.3A.6 Reference sensitivity exceptions due to cross band isolation for CA 281

7.3B Reference sensitivity for NR-DC 282

7.3C Reference sensitivity for SUL 282

7.3C.1 General 282

7.3C.2 Reference sensitivity power level for SUL 282

7.3C.3 ΔRIB,c for SUL 285

7.3C.3.1 General 285

7.3C.3.2 SUL band combination 285

7.3C.3.2.1 ΔRIB,c for two bands 286

7.3D Reference sensitivity for UL MIMO 286

7.3E Reference sensitivity for V2X 286

7.3E.1 General 286

7.3E.2 Minimum requirements 286

7.3F Reference sensitivity for shared spectrum channel access 288

7.3F.1 General 288

7.3F.2 Reference sensitivity power level 288

7.3F.3 ΔRIB,c 289

7.3F.4 Intra-band contiguous shared spectrum channel access CA 290

7.3F.5 Inter-band CA with shared spectrum channel access 290

7.3F.5.1 Reference sensitivity exceptions due to UL harmonic interference 290

7.3F.5.2 Reference sensitivity exceptions due to receiver harmonic mixing 290

7.3F.5.3 Reference sensitivity exceptions due to cross band isolation 291

7.4 Maximum input level 291

7.4A Maximum input level for CA 292

7.4A.1 Maximum input level for Intra-band contiguous CA 292

7.4A.2 Maximum input level for Intra-band non-contiguous CA 292

7.4A.3 Maximum input level for Inter-band CA 292

7.4B Maximum input level for NR-DC 293

7.4D Maximum input level for UL MIMO 293

7.4E Maximum input level for V2X 293

7.4E.1 General 293

7.4E.2 Maximum input level for V2X con-current operation 293

7.5 Adjacent channel selectivity 293

7.5A Adjacent channel selectivity for CA 298

7.5A.1 Adjacent channel selectivity for Intra-band contiguous CA 298

7.5A.2 Adjacent channel selectivity Intra-band non-contiguous CA 300

7.5A.3 Adjacent channel selectivity Inter-band CA 301

7.5B Adjacent channel selectivity for NR-DC 301

7.5D Adjacent channel selectivity for UL MIMO 301

7.5E Adjacent channel selectivity for V2X 301

7.5E.1 General 301

7.5E.2 Adjacent channel selectivity for V2X con-current operation 302

7.5F Adjacent channel selectivity 302

7.5F.1 General 302

7.5F.2 Intra-band contiguous shared spectrum channel access CA 303

7.6 Blocking characteristics 304

7.6.1 General 304

7.6.2 In-band blocking 304

7.6.3 Out-of-band blocking 308

7.6.4 Narrow band blocking 311

7.6A Blocking characteristics for CA 312

7.6A.1 General 312

7.6A.2 In-band blocking for CA 312

7.6A.2.1 In-band blocking for Intra-band contiguous CA 312

7.6A.2.2 In-band blocking for Intra-band non-contiguous CA 314

7.6A.2.3 In-band blocking for Inter-band CA 314

7.6A.3 Out-of-band blocking for CA 315

7.6A.3.1 Out-of-band blocking for Intra-band contiguous CA 315

7.6A.3.2 Out-of-band blocking for Intra-band non-contiguous CA 316

7.6A.3.3 Out-of-band blocking for Inter-band CA 316

7.6A.4 Narrow band blocking for CA 317

7.6A.4.1 Narrow band blocking for Intra-band contiguous CA 317

7.6A.4.2 Narrow band blocking for Intra-band non-contiguous CA 318

7.6A.4.3 Narrow band blocking for Inter-band CA 318

7.6B Blocking characteristics for NR-DC 318

7.6C Blocking characteristics for SUL 319

7.6C.1 General 319

7.6C.2 In-band blocking for SUL 319

7.6C.3 Out-of-band blocking for SUL 319

7.6C.4 Narrow band blocking for SUL 319

7.6D Blocking characteristics for UL MIMO 319

7.6E Blocking characteristics for V2X 320

7.6E.1 General 320

7.6E.2 In-band blocking 320

7.6E.2.1 General 320

7.6E.2.2 In-band blocking for V2X con-current operation 320

7.6E.3 Out-of-band blocking 321

7.6E.3.1 General 321

7.6E.3.2 Out-of-band blocking for V2X con-current operation 321

7.6F Blocking characteristics 321

7.6F.1 General 321

7.6F.2 In-band blocking 321

7.6F.2.1 General 321

7.6F.2.2 Intra-band contiguous shared spectrum channel access CA 322

7.6F.3 Out-of-band blocking 323

7.6F.3.1 General 323

7.6F.3.2 Intra-band contiguous shared spectrum channel access CA 324

7.7 Spurious response 325

7.7A Spurious response for CA 326

7.7A.1 Spurious response for Intra-band contiguous CA 326

7.7A.2 Spurious response for Intra-band non-contiguous CA 327

7.7A.3 Spurious response for Inter-band CA 327

7.7B Spurious response for NR-DC 327

7.7D Spurious response for UL MIMO 327

7.7E Spurious response for V2X 327

7.7E.1 General 327

7.7E.2 Spurious response for V2X con-current operation 328

7.7F Spurious response for shared spectrum channel access 328

7.7F.1 General 328

7.7F.2 Intra-band contiguous shared spectrum channel access CA 328

7.8 Intermodulation characteristics 329

7.8.1 General 329

7.8.2 Wide band Intermodulation 329

7.8A Intermodulation characteristics for CA 331

7.8A.1 General 331

7.8A.2 Wide band intermodulation for CA 331

7.8A.2.1 Wide band intermodulation for Intra-band contiguous CA 331

7.8A.2.2 Wide band intermodulation for Intra-band non-contiguous CA 332

7.8A.2.3 Wide band intermodulation for Inter-band CA 332

7.8B Intermodulation characteristics for NR-DC 332

7.8D Intermodulation characteristics for UL MIMO 333

7.8E Intermodulation characteristics for V2X 333

7.8E.1 General 333

7.8E.2 Wide band Intermodulation 333

7.8E.2.1 General 333

7.8E.2.2 Wide band Intermodulation for V2X con-current operation 333

7.8F Intermodulation characteristics for shared spectrum channel access 333

7.8F.1 General 333

7.8F.2 Wide band Intermodulation 334

7.9 Spurious emissions 334

7.9A Spurious emissions for CA 335

7.9A.1 Void 335

7.9A.2 Void 335

7.9A.3 Spurious emissions for Inter-band CA 335

7.9B Spurious emissions for NR-DC 335

Annex A (normative): Measurement channels 336

A.1 General 336

A.2 UL reference measurement channels 336

A.2.1 General 336

A.2.2 Reference measurement channels 338

A.2.2.1 DFT-s-OFDM Pi/2-BPSK 338

A.2.2.2 DFT-s-OFDM QPSK 339

A.2.2.3 DFT-s-OFDM 16QAM 340

A.2.2.4 DFT-s-OFDM 64QAM 341

A.2.2.5 DFT-s-OFDM 256QAM 342

A.2.2.6 CP-OFDM QPSK 343

A.2.2.7 CP-OFDM 16QAM 345

A.2.2.8 CP-OFDM 64QAM 347

A.2.2.9 CP-OFDM 256QAM 349

A.2.3 Reference measurement channels for TDD 351

A.2.3.1 DFT-s-OFDM Pi/2-BPSK 351

A.2.3.2 DFT-s-OFDM QPSK 351

A.2.3.3 DFT-s-OFDM 16QAM 351

A.2.3.4 DFT-s-OFDM 64QAM 351

A.2.3.5 DFT-s-OFDM 256QAM 352

A.2.3.6 CP-OFDM QPSK 352

A.2.3.7 CP-OFDM 16QAM 352

A.2.3.8 CP-OFDM 64QAM 352

A.2.3.9 CP-OFDM 256QAM 353

A.3 DL reference measurement channels 354

A.3.1 General 354

A.3.2 DL reference measurement channels for FDD 356

A.3.2.1 General 356

A.3.2.2 FRC for receiver requirements for QPSK 357

A.3.2.3 FRC for maximum input level for 64QAM 359

A.3.2.4 FRC for maximum input level for 256 QAM 362

A.3.3 DL reference measurement channels for TDD 365

A.3.3.1 General 365

A.3.3.2 FRC for receiver requirements for QPSK 366

A.3.3.3 FRC for maximum input level for 64QAM 369

A.3.3.4 FRC for maximum input level for 256 QAM 372

A.4 CSI reference measurement channels 375

A.5 OFDMA Channel Noise Generator (OCNG) 375

A.5.1 OCNG Patterns for FDD 375

A.5.1.1 OCNG FDD pattern 1: Generic OCNG FDD Pattern for all unused REs 375

A.5.2 OCNG Patterns for TDD 375

A.5.2.1 OCNG TDD pattern 1: Generic OCNG TDD Pattern for all unused REs 375

A.6 Void 376

A.7 V2X reference measurement channels 376

A.7.1 General 376

A.7.2 FRC for V2X receiver requirements for QPSK 376

A.7.3 FRC for maximum input level for 64QAM 378

A.7.4 FRC for maximum input level for 256QAM 379

Annex B (informative): Void 381

Annex C (informative): Downlink physical channels 382

C.1 General 382

C.2 Setup 382

C.3 Connection 382

C.3.1 Measurement of Receiver Characteristics 382

Annex D (normative): Characteristics of the interfering signal 383

D.1 General 383

D.2 Interference signals 383

Annex E (normative): Environmental conditions 384

E.1 General 384

E.2 Environmental 384

E.2.1 Temperature 384

E.2.2 Voltage 385

E.2.3 Vibration 385

Annex F (normative): Transmit modulation 386

F.0 General 386

F.1 Measurement Point 386

F.2 Basic Error Vector Magnitude measurement 386

F.3 Basic in-band emissions measurement 387

F.4 Modified signal under test 388

F.5 Window length 390

F.5.1 Timing offset 390

F.5.2 Window length 390

F.5.3 Window length for normal CP 390

F.5.4 Window length for Extended CP 391

F.5.5 Window length for PRACH 392

F.6 Averaged EVM 393

F.7 Spectrum Flatness 394

F.8 394

F.9 394

F.10 EVM for UL MIMO 394

F10.1 General 394

F10.2 MIMO Equalization 395

F10.3 Layer processing 395

Annex G (normative): 397

G.0 General 397

G.1 Measurement Point 397

G.2 Relative Phase Error Measurement 398

G.2.1 Symbols and subcarriers used 398

G.2.2 CFO (carrier frequency offset) correction 398

G.2.3 Steps of the measurement method 398

Annex H (informative): Void 399

Annex I (informative): Void 399

Annex J (informative): Void 399

Annex K (informative): Void 399

Annex L (normative): ModifiedMPR-Behavior 399

L.1 Indication of modified MPR behavior 399

Annex M (informative): Change history 401