|  |  |
| --- | --- |
| 3GPP TS 38.101-3 V16.17.0 (2023-09) | |
| Technical Specification | |
| 3rd Generation Partnership Project;  Technical Specification Group Radio Access Network;  NR;  User Equipment (UE) radio transmission and reception;  Part 3: Range 1 and Range 2 Interworking operation with other radios  (Release 16) | |
|  | |
| *5G-logo_175px* | 3GPP-logo_web |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  http://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2023, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 12

1 Scope 14

2 References 14

3 Definitions, symbols and abbreviations 15

3.1 Definitions 15

3.2 Symbols 15

3.3 Abbreviations 15

4 General 16

4.1 Relationship between minimum requirements and test requirements 16

4.2 Applicability of minimum requirements 17

4.3 Specification suffix information 17

5 Operating bands and channel arrangement 18

5.1 General 18

5.2 Operating bands 18

5.2A Operating bands for CA 18

5.2A.1 Inter-band CA between FR1 and FR2 18

5.2B Operating bands for DC 20

5.2B.1 General 20

5.2B.2 Void 20

5.2B.3 Void 20

5.2B.4 Void 20

5.2B.5 Void 20

5.2B.6 Void 20

5.2B.7 Void 20

5.2E Operating bands for V2X 20

5.2E.1 Intra-band V2X bands 20

5.2E.2 Inter-band V2X bands 20

5.3 UE Channel bandwidth 21

5.3A UE Channel bandwidth for CA 21

5.3A.1 Inter-band CA between FR1 and FR2 21

5.3B UE Channel bandwidth for DC 21

5.3B.0 General 21

5.3B.1 Intra-band EN-DC in FR1 21

5.3B.1.1 General 21

5.3B.1.2 BCS for Intra-band contiguous EN-DC 22

5.3B.1.3 BCS for Intra-band non-contiguous EN-DC 26

5.3C Void 30

5.3D Void 30

5.3E UE Channel bandwidth for V2X 30

5.3E.0 General 30

5.3E.1 Intra-band contiguous V2X in FR1 30

5.3E.2 Intra-band non-contiguous V2X in FR1 30

5.3E.3 Inter-band V2X in FR1 30

5.4 Void 31

5.4A Channel arrangement for CA 31

5.4B Channel arrangement for DC 31

5.4B.0 General 31

5.4B.1 Channel spacing for intra-band EN-DC carriers 31

5.5 Configuration 32

5.5A Configuration for CA 32

5.5A.1 Inter-band CA configurations between FR1 and FR2 32

5.5B Configuration for DC 71

5.5B.1 General 71

5.5B.2 Intra-band contiguous EN-DC 72

5.5B.3 Intra-band non-contiguous EN-DC 72

5.5B.4 Inter-band EN-DC within FR1 74

5.5B.4.1 Inter-band EN-DC configurations within FR1 (two bands) 74

5.5B.4.2 Inter-band EN-DC configurations within FR1 (three bands) 82

5.5B.4.3 Inter-band EN-DC configurations within FR1 (four bands) 103

5.5B.4.4 Inter-band EN-DC configurations within FR1 (five bands) 123

5.5B.4.5 Inter-band EN-DC configurations within FR1 (six bands) 131

5.5B.4a Inter-band NE-DC within FR1 132

5.5B.4a.1 Inter-band NE-DC configurations within FR1 (two bands) 132

5.5B.5 Inter-band EN-DC including FR2 133

5.5B.5.1 Inter-band EN-DC configurations including FR2 (two bands) 133

5.5B.5.2 Inter-band EN-DC configurations including FR2 (three bands) 153

5.5B.5.3 Inter-band EN-DC configurations including FR2 (four bands) 176

5.5B.5.4 Inter-band EN-DC configurations including FR2 (five bands) 194

5.5B.5.5 Void 201

5.5B.6 Inter-band EN-DC including FR1 and FR2 201

5.5B.6.1 Void 201

5.5B.6.2 Inter-band EN-DC configurations including FR1 and FR2 (three bands) 201

5.5B.6.3 Inter-band EN-DC configurations including FR1 and FR2 (four bands) 210

5.5B.6.4 Inter-band EN-DC configurations including FR1 and FR2 (five bands) 228

5.5B.6.5 Inter-band EN-DC configurations including FR1 and FR2 (six bands) 242

5.5B.7 Inter-band NR-DC between FR1 and FR2 245

5.5B.7.0 General 245

5.5B.7.1 Inter-band NR-DC configurations between FR1 and FR2 (two bands) 247

5.5B.7.2 Inter-band NR-DC configurations between FR1 and FR2 (three bands) 250

5.5C Void 251

5.5D Void 251

5.5E Configuration for V2X operation 251

5.5E.1 General 251

5.5E.2 Intra-band contiguous V2X operation in FR1 251

5.5E.3 Intra-band non-contiguous V2X operation in FR1 251

5.5E.4 Inter-band V2X operation in FR1 251

5.5E.4.1 Inter-band V2X configurations within FR1 (two bands) 251

6 Transmitter characteristics 252

6.1 General 252

6.2 Void 252

6.2A Transmitter power for CA 252

6.2A.1 UE maximum output power for CA 252

6.2A.1.1 Inter-band CA between FR1 and FR2 252

6.2A.2 UE maximum output power reduction for CA 252

6.2A.2.1 Inter-band CA between FR1 and FR2 252

6.2A.3 UE additional maximum output power reduction for CA 252

6.2A.4 Configured output power for CA 252

6.2A.4.1 Configured output power level 252

6.2A.4.2 ΔTIB,c for CA 253

6.2A.4.2.1 ΔTIB,c for Inter-band CA between FR1 and FR2 253

6.2B Transmitter power for DC 253

6.2B.1 UE maximum output power for DC 253

6.2B.1.1 Intra-band contiguous EN-DC 253

6.2B.1.2 Intra-band non-contiguous EN-DC 255

6.2B.1.3 Inter-band EN-DC within FR1 256

6.2B.1.3a Inter-band NE-DC within FR1 262

6.2B.1.4 Inter-band EN-DC including FR2 263

6.2B.1.5 Inter-band EN-DC including both FR1 and FR2 263

6.2B.2 UE maximum output power reduction for DC 263

6.2B.2.0 General 263

6.2B.2.1 Intra-band contiguous EN-DC 263

6.2B.2.1.1 General 263

6.2B.2.1.2 MPR for power class 3 and power class 2 264

6.2B.2.2 Intra-band non-contiguous EN-DC 264

6.2B.2.2.1 General 264

6.2B.2.2.2 MPR for power class 3 and power class 2 265

6.2B.2.3 Inter-band EN-DC within FR1 266

6.2B.2.3a Inter-band NE-DC within FR1 266

6.2B.2.4 Inter-band EN-DC including FR2 266

6.2B.2.5 Inter-band EN-DC including both FR1 and FR2 266

6.2B.3 UE additional maximum output power reduction for EN-DC 266

6.2B.3.1 Intra-band contiguous EN-DC 266

6.2B.3.1.0 General 266

6.2B.3.1.1 A-MPR for DC\_(n)71AA 266

6.2B.3.1.2 A-MPR for NS\_04 268

6.2B.3.2 Intra-band non-contiguous EN-DC 270

6.2B.3.2.0 General 270

6.2B.3.2.1 A-MPR for NS\_04 271

6.2B.3.3 Inter-band EN-DC within FR1 272

6.2B.3.3A Inter-band NE-DC within FR1 275

6.2B.3.4 Inter-band EN-DC including FR2 276

6.2B.3.5 Inter-band EN-DC including both FR1 and FR2 276

6.2B.4 Configured output power for DC 276

6.2B.4.1 Configured output power level 276

6.2B.4.1.1 Intra-band contiguous EN-DC 276

6.2B.4.1.2 Intra-band non-contiguous EN-DC 280

6.2B.4.1.3a Inter-band NE-DC within FR1 285

6.2B.4.1.4 Inter-band EN-DC including FR2 288

6.2B.4.1.5 Inter-band EN-DC including both FR1 and FR2 289

6.2B.4.2 ΔTIB,c for DC 289

6.2B.4.2.0 General 289

6.2B.4.2.1 Intra-band contiguous EN-DC 289

6.2B.4.2.2 Intra-band non-contiguous EN-DC 289

6.2B.4.2.3 Inter-band EN-DC within FR1 290

6.2B.4.2.3.1 ΔTIB,c for EN-DC two bands 290

6.2B.4.2.3.2 ΔTIB,c for EN-DC three bands 297

6.2B.4.2.3.3 ΔTIB,c for EN-DC four bands 316

6.2B.4.2.3.4 ΔTIB,c for EN-DC five bands 334

6.2B.4.2.3.5 ΔTIB,c for EN-DC six bands 340

6.2B.4.2.3a Inter-band NE-DC within FR1 341

6.2B.4.2.4 Inter-band EN-DC including FR2 341

6.2B.4.2.4.1 ΔTIB,c for EN-DC two bands 341

6.2B.4.2.4.2 ΔTIB,c for EN-DC three bands 341

6.2B.4.2.4.3 ΔTIB,c for EN-DC four bands 341

6.2B.4.2.4.4 ΔTIB,c for EN-DC five bands 341

6.2B.4.2.4.5 Void 341

6.2B.4.2.5 Inter-band EN-DC including both FR1 and FR2 341

6.2B.4.2.5.1 ΔTIB,c for EN-DC three bands 341

6.2B.4.2.5.2 ΔTIB,c for EN-DC four bands 341

6.2B.4.2.5.3 ΔTIB,c for EN-DC five bands 342

6.2B.4.2.5.4 ΔTIB,c for EN-DC six bands 342

6.2B.5 Configured output power for NR-DC 342

6.2B.5.1 Configured output power level 342

6.2B.5.1.1 Inter-band NR-DC between FR1 and FR2 342

6.2E Transmitter power for V2X in FR1 342

6.2E.1 UE maximum output power for V2X 342

6.2E.1.1 UE maximum output power for Intra-band contiguous V2X 342

6.2E.1.2 UE maximum output power for Intra-band non-contiguous V2X 342

6.2E.1.3 UE maximum output power for Inter-band V2X 343

6.2E.2 UE maximum output power reduction for V2X 343

6.2E.2.1 UE maximum output power reduction for Intra-band V2X 343

6.2E.2.2 UE maximum output power reduction for Inter-band V2X 343

6.2E.3 UE additional maximum output power reduction for V2X 343

6.2E.3.1 UE additional maximum output power reduction for Intra-band V2X 343

6.2E.3.2 UE additional maximum output power reduction for Inter-band V2X 343

6.2E.4 Configured output power for V2X 343

6.2E.4.1 UE configured output power for Intra-band V2X 343

6.2E.4.2 UE configured output power for Inter-band V2X 344

6.3 Output power dynamics 344

6.3A Output power dynamics for CA 345

6.3B Output power dynamics for DC 345

6.3B.0 General 345

6.3B.1 Output power dynamics for EN-DC with UL sharing from UE perspective 345

6.3B.1.1 E-UTRA and NR switching time mask for TDM based UL sharing from UE perspective 345

6.3B.1a Output power dynamics for NE-DC with UL sharing from UE perspective 346

6.3B.2 Output power dynamics for intra-band EN-DC without dual PA capability 346

6.3B.3 Output power dynamics for intra-band EN-DC with dual PA capability 347

6.3B.4 Output power dynamics for switching between two uplink carriers 348

6.3B.4.1 E-UTRA and NR switching time mask between two uplink carriers 348

6.3B.5 Output power dynamics for inter-band EN-DC 349

6.3E Output power dynamics for V2X 349

6.3E.1 General 349

6.3E.2 Output power dynamics for intra-band V2X operation 350

6.3E.3 Output power dynamics for inter-band V2X con-current operation 350

6.4 Void 350

6.4A Transmit signal quality for CA 350

6.4A.1 Frequency error for CA 350

6.4A.2 Transmit modulation quality for CA 350

6.4B Transmit signal quality for DC 350

6.4B.2 Transmit modulation quality for DC 351

6.4B.2.1 Transmit modulation quality for Intra-band contiguous EN-DC 351

6.4B.2.1.1 Error Vector Magnitude 351

6.4B.2.1.2 Carrier leakage 351

6.4B.2.1.3 In-band emissions 351

6.4B.2.2 Transmit modulation quality for Intra-band non-contiguous EN-DC 352

6.4B.2.2.1 Error Vector Magnitude 352

6.4B.2.2.2 Carrier leakage 352

6.4B.2.2.3 In-band emissions 352

6.4B.2.3a Transmit modulation quality for Inter-band NE-DC within FR1 352

6.4B.2.4 Transmit modulation quality for Inter-band EN-DC including FR2 352

6.4B.2.5 Transmit modulation quality for inter-band EN-DC including both FR1 and FR2 352

6.4E Transmit signal quality for V2X operation in FR1 353

6.4E.1 Frequency error for V2X 353

6.4E.2 Transmit modulation quality for V2X 353

6.4E.2.1 Transmit modulation quality for Intra-band V2X 353

6.4E.2.2.1 Error Vector Magnitude 353

6.4E.2.2.2 Carrier leakage 353

6.4E.2.2.3 In-band emissions 353

6.4E.2.2 Transmit modulation quality for Inter-band V2X 353

6.5 Void 353

6.5A Output RF spectrum emissions for CA 353

6.5A.1 Occupied bandwidth for CA 353

6.5A.2 Out-of-band emissions for CA 354

6.5A.3 Spurious emissions for CA 354

6.5A.3.1 Inter-band CA between FR1 and FR2 354

6.5A.4 Transmit intermodulation for CA 354

6.5B Output RF spectrum emissions for DC 354

6.5B.1 Occupied bandwidth for EN-DC 354

6.5B.1.4 Inter-band EN-DC including FR2 354

6.5B.1.5 Inter-band EN-DC including both FR1 and FR2 354

6.5B.2 Out-of-band emissions for DC 355

6.5B.2.1 Intra-band contiguous EN-DC 355

6.5B.2.1.1 Spectrum emissions mask 355

6.5B.2.1.2 Additional spectrum emissions mask 355

6.5B.2.1.2.1 Requirements for network signalled value "NS\_35" 355

6.5B.2.1.2.2 Requirements for network signalled value "NS\_04" 355

6.5B.2.1.3 Adjacent channel leakage ratio 356

6.5B.2.2 Intra-band non-contiguous EN-DC 356

6.5B.2.2.1 Spectrum emissions mask 356

6.5B.2.2.2 Additional spectrum emissions mask 357

6.5B.2.2.3 Adjacent channel leakage ratio 357

6.5B.2.3 Inter-band EN-DC within FR1 357

6.5B.2.3a Inter-band NE-DC within FR1 357

6.5B.2.4 Inter-band EN-DC including FR2 357

6.5B.2.5 Inter-band EN-DC including both FR1 and FR2 357

6.5B.3 Spurious emissions for DC 357

6.5B.3.1 Intra-band contiguous EN-DC 357

6.5B.3.1.1 General spurious emissions 357

6.5B.3.1.2 Spurious emission band UE co-existence 357

6.5B.3.2 Intra-band non-contiguous EN-DC 358

6.5B.3.2.1 General spurious emissions 358

6.5B.3.2.2 Spurious emission band UE co-existence 358

6.5B.3.3 Inter-band EN-DC within FR1 359

6.5B.3.3.2 Spurious emission band UE co-existence 360

6.5B.3.3a Inter-band NE-DC within FR1 372

6.5B.3.3a.1 General spurious emissions 372

6.5B.3.3a.2 Spurious emission band UE co-existence 372

6.5B.3.4 Inter-band EN-DC including FR2 372

6.5B.3.4.0 General spurious emission 372

6.5B.3.4.1 Spurious emission band UE co-existence 372

6.5B.3.5 Inter-band EN-DC including both FR1 and FR2 372

6.5B.3.5.0 General spurious emission 372

6.5B.3.5.1 Spurious emission band UE co-existence 372

6.5B.4 Additional spurious emissions 373

6.5B.4.1 General 373

6.5B.4.1.1 Void 373

6.5B.4.2 Intra-band contiguous EN-DC 373

6.5B.4.2.1 Minimum requirement (network signalled value "NS\_04") 373

6.5B.4.3 Intra-band non-contiguous EN-DC 373

6.5B.4.3.1 Minimum requirement (network signalled value "NS\_04") 373

6.5B.4.4 Inter-band EN-DC within FR1 374

6.5B.4.4a Inter-band NE-DC within FR1 374

6.5B.4.5 Inter-band EN-DC including FR2 374

6.5B.4.6 Inter-band EN-DC including both FR1 and FR2 374

6.5B.5 Transmit intermodulation for DC 374

6.5B.5.1 Intra-band contiguous EN-DC 374

6.5B.5.2 Intra-band non-contiguous EN-DC 374

6.5B.5.3 Inter-band EN-DC within FR1 374

6.5B.5.3a Inter-band NE-DC within FR1 374

6.5B.5.4 Inter-band EN-DC including FR2 374

6.5B.5.5 Inter-band EN-DC including both FR1 and FR2 374

6.5E Output RF spectrum emissions for V2X operation in FR1 375

6.5E.1 Occupied bandwidth 375

6.5E.1.1 Intra-band V2X 375

6.5E.1.2 inter-band V2X con-current operation 375

6.5E.2 Out-of-band emissions 375

6.5E.2.1 Intra-band V2X 375

6.5E.2.2 Inter-band V2X con-current operation 375

6.5E.3 Spurious emissions 375

6.5E.3.1 Intra-band V2X 375

6.5E.3.1.1 General spurious emissions 375

6.5E.3.1.2 Spurious emission band UE co-existence 375

6.5E.3.2 Inter-band V2X con-current operation 375

6.5E.3.2.1 General spurious emissions 375

6.5E.3.2.2 Spurious emission band UE co-existence 376

6.5E.4 Transmit intermodulation 376

6.5E.4.1 Intra-band V2X 376

6.5E.4.2 Inter-band V2X con-current operation 376

6.6B Beam correspondence for DC 377

6.6B.1 Void 377

6.6B.2 Void 377

6.6B.3 Void 377

6.6B.4 Inter-band EN-DC including FR2 377

6.6B.5 Inter-band EN-DC including both FR1 and FR2 377

7 Receiver characteristics 377

7.1 General 377

7.2 Void 378

7.3 Void 378

7.3A Reference sensitivity for CA 378

7.3A.1 General 378

7.3A.2 Reference sensitivity power level for CA 378

7.3A.3 ΔRIB,c for CA 378

7.3A.3.1 ΔRIB,c for Inter-band CA between FR1 and FR2 379

7.3A.4 Void 379

7.3B Reference sensitivity level for DC 379

7.3B.1 General 379

7.3B.2 Reference sensitivity for DC 380

7.3B.2.1 Intra-band contiguous EN-DC 380

7.3B.2.2 Intra-band non-contiguous EN-DC 381

7.3B.2.3 Inter-band EN-DC within FR1 382

7.3B.2.3.0 General 382

7.3B.2.3.1 Reference sensitivity exceptions due to UL harmonic interference for EN-DC in NR FR1 382

7.3B.2.3.2 Reference sensitivity exceptions due to receiver harmonic mixing for EN-DC in NR FR1 389

7.3B.2.3.3 Void 391

7.3B.2.3.4 Reference sensitivity exceptions due to cross band isolation for EN-DC in NR FR1 391

7.3B.2.3.5 MSD for intermodulation interference due to dual uplink operation for EN-DC in NR FR1 399

7.3B.2.3.5.1 MSD test points for intermodulation interference due to dual uplink operation for PC3 EN-DC in NR FR1 involving two bands 400

7.3B.2.3.5.2 MSD test points for intermodulation interference due to dual uplink operation for EN-DC in NR FR1 involving three bands 405

7.3B.2.3.5.3 Void 429

7.3B.2.3.5.4 MSD test points for intermodulation interference due to dual uplink operation for EN-DC in NR FR1 involving four bands 429

7.3B.2.3.6 Reference sensitivity exceptions due to Tx non-linearity interference in 1st or 2nd adjacent channel of UL band for EN-DC in NR FR1 429

7.3B.2.3a Inter-band NE-DC within FR1 430

7.3B.2.3a.0 General 430

7.3B.2.3a.1 Reference sensitivity exceptions due to UL harmonic interference for NE-DC in NR FR1 430

7.3B.2.4 Inter-band EN-DC including FR2 430

7.3B.2.4.1 Void 430

7.3B.2.5 Inter-band EN-DC including both FR1 and FR2 430

7.3B.2.5.1 Reference sensitivity exceptions due to UL harmonic interference for EN-DC including both FR1 and FR2 430

7.3B.3 ΔRIB,c, ΔRIBNC for DC 430

7.3B.3.0 General 430

7.3B.3.1 Intra-band contiguous EN-DC 432

7.3B.3.2 Intra-band non-contiguous EN-DC 432

7.3B.3.3 Inter-band EN-DC within FR1 437

7.3B.3.3.1 ΔRIB,c for EN-DC in two bands 437

7.3B.3.3.2 ΔRIB,c for EN-DC three bands 441

7.3B.3.3.3 ΔRIB,c for EN-DC four bands 452

7.3B.3.3.4 ΔRIB,c for EN-DC five bands 465

7.3B.3.3.5 ΔRIB,c for EN-DC six bands 470

7.3B.3.3a Inter-band NE-DC within FR1 470

7.3B.3.4 Inter-band EN-DC including FR2 470

7.3B.3.4.1 ΔRIB,c for EN-DC in two bands 470

7.3B.3.4.2 ΔRIB,c for EN-DC three bands 471

7.3B.3.4.3 ΔRIB,c for EN-DC four bands 471

7.3B.3.4.4 ΔRIB,c for EN-DC five bands 471

7.3B.3.4.5 Void 471

7.3B.3.5 Inter-band EN-DC including both FR1 and FR2 471

7.3B.3.5.2 ΔRIB,c for EN-DC three bands 471

7.3B.3.5.3 ΔRIB,c for EN-DC four bands 471

7.3B.3.5.4 ΔRIB,c for EN-DC five bands 471

7.3B.3.5.5 ΔRIB,c for EN-DC six bands 471

7.3E Reference sensitivity for V2X operation in FR1 472

7.3E.1 General 472

7.3E.2 Reference sensitivity for V2X 472

7.3E.2.1 Intra-band contiguous V2X 472

7.3E.2.2 Intra-band non-contiguous V2X 472

7.3E.2.3 Inter-band V2X con-current operation 472

7.3E.2.3.0 General 472

7.3E.2.3.1 Reference sensitivity exception due to UL harmonic problem 473

7.4 Void 474

7.4A Maximum input level for CA 474

7.4B Maximum input level for DC in FR1 474

7.4B.1 Intra-band contiguous EN-DC in FR1 474

7.4B.2 Intra-band non-contiguous EN-DC in FR1 474

7.4B.3 Inter-band EN-DC within FR1 474

7.4E Maximum input level for V2X operation in FR1 475

7.5 Void 475

7.5A Adjacent channel selectivity for CA 475

7.5B Adjacent channel selectivity for DC in FR1 475

7.5B.1 Intra-band contiguous EN-DC in FR1 475

7.5B.2 Intra-band non-contiguous EN-DC in FR1 476

7.5B.3 Inter-band EN-DC within FR1 476

7.5E Adjacent channel selectivity for V2X operation in FR1 477

7.6 Void 477

7.6A Blocking characteristics for CA 477

7.6B Blocking characteristics for DC in FR1 477

7.6B.1 General 477

7.6B.2 In-band blocking for DC in FR1 477

7.6B.2.1 Intra-band contiguous EN-DC in FR1 477

7.6B.2.2 Intra-band non-contiguous EN-DC in FR1 477

7.6B.2.3 Inter-band EN-DC within FR1 478

7.6B.2.3a Inter-band NE-DC within FR1 478

7.6B.2.4 Inter-band EN-DC including FR2 478

7.6B.2.5 Inter-band EN-DC including both FR1 and FR2 478

7.6B.2.6 Void 478

7.6B.3 Out-of-band blocking for DC in FR1 478

7.6B.3.1 Intra-band contiguous EN-DC in FR1 478

7.6B.3.2 Intra-band non-contiguous EN-DC in FR1 479

7.6B.3.3 Inter-band EN-DC within FR1 479

7.6B.4 Narrow band blocking for DC in FR1 480

7.6B.4.1 Intra-band contiguous EN-DC in FR1 480

7.6B.4.2 Intra-band non-contiguous EN-DC in FR1 480

7.6B.4.3 Inter-band EN-DC within FR1 481

7.6E Blocking characteristics for V2X in FR1 481

7.7 Void 481

7.7A Spurious response for CA 481

7.7B Spurious response for DC in FR1 481

7.7B.1 Intra-band contiguous EN-DC in FR1 481

7.7B.2 Intra-band non-contiguous EN-DC in FR1 482

7.7B.3 Inter-band EN-DC within FR1 482

7.7E Spurious response for V2X in FR1 482

7.8 Void 483

7.8A Intermodulation characteristics for CA 483

7.8B Intermodulation characteristics for DC in FR1 483

7.8B.1 General 483

7.8B.2 Wide band Intermodulation 483

7.8B.2.1 Intra-band contiguous EN-DC in FR1 483

7.8B.2.2 Intra-band non-contiguous EN-DC in FR1 483

7.8B.2.3 Inter-band EN-DC within FR1 483

7.8E Intermodulation characteristics for V2X operation in FR1 484

7.9 Void 484

7.9A Spurious emissions for CA 484

7.9B Spurious emissions for DC in FR1 484

7.9B.1 Intra-band contiguous EN-DC in FR1 484

7.9B.2 Intra-band non-contiguous EN-DC in FR1 484

7.9B.3 Inter-band EN-DC within FR1 484

7.10 Void 485

7.10A Void 485

7.10B power imbalance for DC 485

7.10B.1 Void 485

7.10B.2 Void 485

7.10B.3 Inter-band EN-DC within FR1 485

Annex A (normative): Measurement channels 487

A.1 General 487

A.2 UL reference measurement channels for E-UTRA TDD Config 2 487

A.2.1 General 487

A.2.2 Reference measurement channels for E-UTRA 488

A.2.2.1 Full RB allocation 488

A.2.2.1.1 QPSK 488

A.2.2.1.2 16-QAM 489

A.2.2.1.3 64-QAM 490

A.2.2.1.4 256 QAM 491

A.2.2.2 Partial RB allocation 492

A.2.2.2.1 QPSK 492

A.2.2.2.2 16-QAM 495

A.2.2.2.3 64-QAM 498

A.2.2.2.4 256 QAM 501

A.3 DL reference measurement channels for E-UTRA 504

A.3.1 General 504

A.3.1.1 QPSK 505

A.3.1.2 64-QAM 506

A.3.1.3 256-QAM 507

Annex B: Void 507

Annex C: Void 507

Annex D: Void 507

Annex E: Void 508

Annex F: Void 508

Annex G: Void 508

Annex H (normative): Modified MPR behavior 508

Annex I (normative): Dual uplink interferer 509

Annex J: Void 509

Annex K: Void 509

Annex L (informative): Change history 510