|  |  |
| --- | --- |
| 3GPP TS 38.133 V16.17.0 (2023-09) | |
| Technical Specification | |
| 3rd Generation Partnership Project;  Technical Specification Group Radio Access Network;  NR;  Requirements for support of radio resource management  (Release 16) | |
|  | |
|  |  |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  http://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2023, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 42

1 Scope 44

2 References 44

3 Definitions, symbols and abbreviations 45

3.1 Definitions 45

3.2 Symbols 46

3.3 Abbreviations 47

3.4 Test tolerances 50

3.5 Frequency bands grouping 50

3.5.1 Introduction 50

3.5.2 NR operating bands in FR1 50

3.5.3 NR operating bands in FR2 51

3.6 Applicability of requirements in this specification version 51

3.6.1 RRC connected state requirements in DRX 52

3.6.2 Number of serving carriers 52

3.6.2.1 Number of serving carriers for SA 52

3.6.2.2 Number of serving carriers for EN-DC 52

3.6.2.3 Number of serving carriers for NE-DC 52

3.6.2.4 Number of serving carriers for NR-DC 53

3.6.3 Applicability for intra-band FR2 53

3.6.4 Applicability for FR2 UE power classes 53

3.6.5 Applicability for SDL bands 53

3.6.6 Applicability of requirements for NGEN-DC operation 53

3.6.7 Applicability of QCL 53

3.6.9 Applicability of requirements for scheduling availability 54

3.6.10 Applicability of requirements for measurement restrictions 54

4 SA: RRC\_IDLE state mobility 54

4.1 Cell Selection 54

4.2 Cell Re-selection 54

4.2.1 Introduction 54

4.2.2 Requirements 55

4.2.2.1 UE measurement capability 55

4.2.2.2 Measurement and evaluation of serving cell 55

4.2.2.3 Measurements of intra-frequency NR cells 56

4.2.2.4 Measurements of inter-frequency NR cells 57

4.2.2.5 Measurements of inter-RAT E-UTRAN cells 59

4.2.2.6 Maximum interruption in paging reception 61

4.2.2.7 General requirements 61

4.2.2.8 Minimum requirement at transitions 61

4.2.2.9 Measurements of intra-frequency NR cells for UE configured with relaxed measurement criterion 62

4.2.2.9.1 Introduction 62

4.2.2.9.2 Measurements for UE fulfilling low mobility criterion 62

4.2.2.9.3 Measurements for UE fulfilling not-at-cell edge criterion 63

4.2.2.9.4 Measurements for UE fulfilling low mobility and not-at-cell edge criteria 64

4.2.2.10 Measurements of inter-frequency NR cells for UE configured with relaxed measurement criterion 64

4.2.2.10.1 Introduction 64

4.2.2.10.2 Measurements for UE fulfilling low mobility criterion 64

4.2.2.10.3 Measurements for UE fulfilling not-at-cell edge criterion 65

4.2.2.10.4 Measurements for UE fulfilling low mobility and not-at-cell edge criterion 66

4.2.2.11 Measurements of inter-RAT E-UTRAN cells for UE configured with relaxed measurement criterion 67

4.2.2.11.1 Introduction 67

4.2.2.11.2 Measurements for UE fulfilling low mobility criterion 67

4.2.2.11.3 Measurements for UE fulfilling with not-at-cell edge criterion 68

4.2.2.11.4 Measurements for UE fulfilling low mobility and not-at-cell edge criterion 69

4.2A Cell Re-selection when subject to CCA 69

4.2A.1 Introduction 69

4.2A.2 Requirements 70

4.2A.2.1 UE measurement capability 70

4.2A.2.2 Measurement and evaluation when subject to CCA on the serving cell 70

4.2A.2.3 Measurements of intra-frequency NR cells when subject to CCA on the serving cell and target cell 71

4.2A.2.4 Measurements of inter-frequency NR cells when subject to CCA on the target cell 72

4.2A.2.5 Measurements of inter-RAT E-UTRAN cells when subject to CCA on the serving cell 74

4.2A.2.6 Maximum interruption in paging reception when subject to CCA on the target cell 74

4.2A.2.7 General requirements 74

4.3 Minimization of Drive Tests (MDT) 75

4.3.1 Introduction 75

4.3.2 Measurement Requirements 75

4.3.3 Requirements for Relative Time Stamp Accuracy 75

4.3.4 Requirements for Relative Time Stamp Accuracy for RRC Connection Establishment Failure Log Reporting 76

4.3.5 Requirements for Relative Time Stamp Accuracy for Radio Link Failure and Handover Failure Log Reporting 76

4.4 Idle Mode CA/DC Measurements 76

4.4.1 Introduction 76

4.4.2 Measurement Requirements 76

4.4.2.1 Detected cell requirement during state transition and Idle mode 76

4.4.2.2 Measurements of inter-frequency CA/DC candidate cells 77

4.4.2.3 Measurements on serving cell 78

4.4.2.4 Measurements of E-UTRAN inter-RAT DC candidate cells 78

5 SA: RRC\_INACTIVE state mobility 80

5.1 Cell Re-selection 80

5.1.1 Introduction 80

5.1.2 Requirements 80

5.1.2.1 UE measurement capability 80

5.1.2.2 Measurement and evaluation of serving cell 80

5.1.2.3 Measurements of intra-frequency NR cells 80

5.1.2.4 Measurements of inter-frequency NR cells 80

5.1.2.5 Measurements of inter-RAT E-UTRAN cells 80

5.1.2.6 Maximum interruption in paging reception 80

5.1.2.7 General requirements 80

5.1A Cell Re-selection with CCA 80

5.1A.1 Introduction 80

5.1A.2 Requirements 81

5.1A.2.1 UE measurement capability 81

5.1A.2.2 Measurement and evaluation when CCA is used on the serving cell 81

5.1A.2.3 Measurements of intra-frequency NR cells when CCA is used on the serving cell and target cell 81

5.1A.2.4 Measurements of inter-frequency NR cells when CCA is used on the target cell 81

5.1A.2.5 Measurements of inter-RAT E-UTRAN cells when CCA is used on the serving cell 81

5.1A.2.6 Maximum interruption in paging reception when CCA is used on the target cell 81

5.1A.2.7 General requirements 81

5.2 Void 81

5.3 Minimization of Drive Tests (MDT) 81

5.3.1 Introduction 81

5.3.2 Measurement Requirements 82

5.3.3 Requirements for Relative Time Stamp Accuracy 82

5.3.4 Requirements for Relative Time Stamp Accuracy for RRC Connection Establishment Failure Log Reporting 82

5.3.5 Requirements for Relative Time Stamp Accuracy for Radio Link Failure and Handover Failure Log Reporting 82

5.3.6 Requirements for Relative Time Stamp Accuracy for RRC Resume Failure Log Reporting 82

5.4 Idle Mode CA/DC Measurements 82

5.4.1 Introduction 82

5.4.2 Measurement Requirements 82

5.4.2.1 Detected cell requirement during state transition and Idle mode 83

5.4.2.2 Measurements of inter-frequency CA/DC candidate cells 83

5.4.2.3 Measurements on serving cell 83

5.4.2.4 Measurements on E-UTRAN inter-RAT DC candidate cells 83

6 RRC\_CONNECTED state mobility 83

6.1 Handover 83

6.1.1 NR Handover 83

6.1.1.1 Introduction 83

6.1.1.2 NR FR1 - NR FR1 Handover 83

6.1.1.2.1 Handover delay 83

6.1.1.2.2 Interruption time 83

6.1.1.3 NR FR2- NR FR1 Handover 84

6.1.1.3.1 Handover delay 84

6.1.1.3.2 Interruption time 84

6.1.1.4 NR FR2- NR FR2 Handover 85

6.1.1.4.1 Handover delay 85

6.1.1.4.2 Interruption time 85

6.1.1.5 NR FR1- NR FR2 Handover 86

6.1.1.5.1 Handover delay 86

6.1.1.5.2 Interruption time 86

6.1.2 NR Handover to other RATs 87

6.1.2.1 NR – E-UTRAN Handover 87

6.1.2.1.1 Introduction 87

6.1.2.1.2 Handover delay 87

6.1.2.1.3 Interruption time 87

6.1.2.2 NR – UTRAN Handover 88

6.1.2.2.1 Introduction 88

6.1.2.2.2 Handover delay 88

6.1.2.2.3 Interruption time 88

6.1.3 NR DAPS Handover 89

6.1.3.1 Introduction 89

6.1.3.2 NR FR1 - NR FR1 DAPS Handover 89

6.1.3.2.1 DAPS handover delay 89

6.1.3.2.2 Interruption time 90

6.1.3.3 NR FR2- NR FR1 DAPS Handover 92

6.1.3.3.1 DAPS handover delay 92

6.1.3.3.2 Interruption time 92

6.1.3.4 NR FR1- NR FR2 DAPS Handover 93

6.1.3.4.1 DAPS handover delay 93

6.1.3.4.2 Interruption time 94

6.1.4 NR Conditional Handover 94

6.1.4.1 Introduction 94

6.1.4.2 NR FR1 – NR FR1 conditional handover 94

6.1.4.3 NR FR2 – NR FR1 conditional handover 95

6.1.4.4 NR FR2 – NR FR2 conditional handover 96

6.1.4.4.1 Handover delay 96

6.1.4.4.2 Measurement time 96

6.1.4.4.3 Preparation time 96

6.1.4.4.4 Interruption time 97

6.1.4.5 NR FR1 – NR FR2 conditional handover 97

6.1A Void 97

6.1A.1 Void 97

6.1A.1.1 Void 97

6.1A.1.2 Void 97

6.1A.1.2.1 Void 97

6.1A.1.2.2 Void 97

6.1B Handover to target cell using CCA 98

6.1B.1 NR Handover 98

6.1B.1.1 Introduction 98

6.1B.1.2 NR FR1 - NR FR1 Handover 98

6.1B.1.2.1 Handover delay 98

6.1B.1.2.2 Interruption time 98

6.2 RRC Connection Mobility Control 99

6.2.1 SA: RRC Re-establishment 99

6.2.1.1 Introduction 99

6.2.1.2 Requirements 99

6.2.1.2.1 UE Re-establishment delay requirement 99

6.2.1A RRC Re-establishment with CCA 101

6.2.1A.1 Introduction 101

6.2.1A.2 Requirements 101

6.2.1A.2.1 UE Re-establishment with CCA delay requirement 101

6.2.2 Random access 103

6.2.2.1 Introduction 103

6.2.2.2 Requirements for 4-step RA type 103

6.2.2.2.1 Contention based random access 104

6.2.2.2.2 Non-Contention based random access 104

6.2.2.2.3 UE behaviour when configured with supplementary UL 105

6.2.2.3 Requirements for 2-step RA type 105

6.2.2.3.1 Contention based random access 106

6.2.2.3.2 Non-Contention based random access 107

6.2.2.3.3 UE behaviour when configured with supplementary UL 107

6.2.2A Random access when CCA is used on target frequency 107

6.2.2A.1 Introduction 107

6.2.2A.2 Requirements for 4-step RA type 108

6.2.2A.2.1 Contention based random access 108

6.2.2A.2.2 Non-Contention based random access 109

6.2.2A.3 Requirements for 2-step RA type 110

6.2.2A.3.1 Contention based random access 110

6.2.2A.3.2 Non-Contention based random access 111

6.2.3 SA: RRC Connection Release with Redirection 112

6.2.3.1 Introduction 112

6.2.3.2 Requirements 112

6.2.3.2.1 RRC connection release with redirection to NR 112

6.2.3.2.2 RRC connection release with redirection to E-UTRAN 113

6.2.3.2.3 RRC connection release with redirection to NR carrier subject to CCA 114

7 Timing 115

7.1 UE transmit timing 115

7.1.1 Introduction 115

7.1.2 Requirements 115

7.1.2.1 Gradual timing adjustment 116

7.1.2.2 Void 117

7.2 UE timer accuracy 117

7.2.1 Introduction 117

7.2.2 Requirements 117

7.3 Timing advance 118

7.3.1 Introduction 118

7.3.2 Requirements 118

7.3.2.1 Timing Advance adjustment delay 118

7.3.2.2 Timing Advance adjustment accuracy 118

7.4 Cell phase synchronization accuracy 118

7.4.1 Definition 118

7.4.2 Minimum requirements 118

7.5 Maximum Transmission Timing Difference 118

7.5.1 Introduction 118

7.5.2 Minimum Requirements for inter-band EN-DC 119

7.5.2.1 Minimum Requirements for inter-band synchronous EN-DC 119

7.5.3 Minimum Requirements for intra-band EN-DC 119

7.5.4 Minimum Requirements for NR Carrier Aggregation 120

7.5.5 Minimum Requirements for inter-band NE-DC 120

7.5.5.1 Minimum Requirements for inter-band synchronous NE-DC 121

7.5.6 Minimum Requirements for inter-band NR DC 121

7.6 Maximum Receive Timing Difference 122

7.6.1 Introduction 122

7.6.2 Minimum Requirements for inter-band EN-DC 122

7.6.2.1 Minimum Requirements for inter-band synchronous EN-DC 122

7.6.3 Minimum Requirements for intra-band EN-DC 123

7.6.4 Minimum Requirements for NR Carrier Aggregation 123

7.6.5 Minimum Requirements for inter-band NE-DC 124

7.6.5.1 Minimum Requirements for inter-band synchronous NE-DC 124

7.6.6 Minimum Requirements for inter-band NR DC 124

7.7 *deriveSSB-IndexFromCell* tolerance 125

7.7.1 Minimum requirements 125

7.8 Void 125

8 Signalling characteristics 125

8.1 Radio Link Monitoring 125

8.1.1 Introduction 125

8.1.2 Requirements for SSB based radio link monitoring 126

8.1.2.1 Introduction 126

8.1.2.2 Minimum requirement 127

8.1.2.3 Measurement restrictions for SSB based RLM 129

8.1.3 Requirements for CSI-RS based radio link monitoring 129

8.1.3.1 Introduction 129

8.1.3.2 Minimum requirement 130

8.1.3.3 Measurement restrictions for CSI-RS based RLM 132

8.1.4 Minimum requirement at transitions 133

8.1.5 Minimum requirement for UE turning off the transmitter 133

8.1.6 Minimum requirement for L1 indication 133

8.1.7 Scheduling availability of UE during radio link monitoring 134

8.1.7.1 Scheduling availability of UE performing radio link monitoring with a same subcarrier spacing as PDSCH/PDCCH on FR1 134

8.1.7.2 Scheduling availability of UE performing radio link monitoring with a different subcarrier spacing than PDSCH/PDCCH on FR1 134

8.1.7.3 Scheduling availability of UE performing radio link monitoring on FR2 134

8.1.7.4 Scheduling availability of UE performing radio link monitoring on FR1 or FR2 in case of FR1-FR2 inter-band CA and NR-DC 135

8.1A Radio Link Monitoring with CCA on Target Frequency 135

8.1A.1 Introduction 135

8.1A.2 Requirements for SSB Based Radio Link Monitoring 136

8.1A.2.1 Introduction 136

8.1A.2.2 Minimum Requirement 137

8.1A.3 Minimum requirement at transitions 138

8.1A.4 Minimum requirement for UE turning off the transmitter 139

8.1A.5 Minimum requirement for L1 indication 139

8.1A.6 Scheduling availability of UE during radio link monitoring 139

8.1A.6.1 Scheduling availability of UE performing radio link monitoring with the same subcarrier spacing as PDSCH/PDCCH 139

8.1A.6.2 Scheduling availability of UE performing radio link monitoring with a different subcarrier spacing than PDSCH/PDCCH 139

8.2 Interruption 140

8.2.1 EN-DC Interruption 140

8.2.1.1 Introduction 140

8.2.1.2 Requirements 140

8.2.1.2.1 Interruptions at transitions between active and non-active during DRX 140

8.2.1.2.2 Interruptions at transitions from non-DRX to DRX 141

8.2.1.2.3 Interruptions at SCell addition/release 141

8.2.1.2.4 Interruptions at SCell activation/deactivation 142

8.2.1.2.5 Interruptions during measurements on SCC 143

8.2.1.2.6 Interruptions at UL carrier RRC reconfiguration 145

8.2.1.2.7 Interruptions due to Active BWP switching Requirement 145

8.2.1.2.8 Interruptions at direct SCell activation and hibernation 146

8.2.1.2.9 Interruptions at SCell hibernation 147

8.2.1.2.10 Interruptions at SCell activation/deactivation with multiple downlink SCells 147

8.2.1.2.11 Interruptions due to UE-specific CBW change 147

8.2.1.2.12 Interruptions at NR SRS carrier based switching 148

8.2.1.2.13 Interruptions at E-UTRA SRS carrier based switching 149

8.2.1.2.14 DL Interruptions at switching between two uplink carriers 150

8.2.1.2.15 Interruptions due to SCell dormancy 150

8.2.1.2.16 Interruptions when identifying CGI of an NR cell with autonomous gaps 151

8.2.1.2.17 Interruptions when identifying CGI of an E-UTRA cell with autonomous gaps 151

8.2.2 SA: Interruptions with Standalone NR Carrier Aggregation 152

8.2.2.1 Introduction 152

8.2.2.2 Requirements 153

8.2.2.2.1 Interruptions at SCell addition/release 153

8.2.2.2.2 Interruptions at SCell activation/deactivation 154

8.2.2.2.3 Interruptions during measurements on deactivated SCC 155

8.2.2.2.4 Interruptions at UL carrier RRC reconfiguration 156

8.2.2.2.5 Interruptions due to Active BWP switching Requirement 156

8.2.2.2.6 Interruptions at inter-frequency SFTD measurement 157

8.2.2.2.7 Interruptions at SCell activation/deactivation with multiple downlink SCells 158

8.2.2.2.8 Interruptions due to UE-specific CBW change 158

8.2.2.2.9 Interruptions at NR SRS carrier based switching 159

8.2.2.2.10 DL Interruptions at UE switching between two uplink carriers 160

8.2.2.2.11 Interruptions at direct SCell activation 161

8.2.2.2.12 Interruptions due to SCell dormancy 161

8.2.2.2.13 Interruptions at transitions between active and non-active during DRX 161

8.2.2.2.14 Interruptions when identifying CGI of an NR cell with autonomous gaps 162

8.2.2.2.15 Interruptions when identifying CGI of an E-UTRA cell with autonomous gaps 162

8.2.3 NE-DC Interruptions 163

8.2.3.1 Introduction 163

8.2.3.2 Requirements 163

8.2.3.2.1 Interruptions at transitions between active and non-active during DRX 163

8.2.3.2.2 Interruptions at transitions from non-DRX to DRX 164

8.2.3.2.3 Interruptions at PSCell/SCell addition/release 164

8.2.3.2.4 Interruptions at SCell activation/deactivation 165

8.2.3.2.5 Interruptions during measurements on SCC 166

8.2.3.2.6 Interruptions at UL carrier RRC reconfiguration 167

8.2.3.2.7 Interruptions due to Active BWP switching Requirement 168

8.2.3.2.8 Interruptions at direct SCell activation and hibernation 168

8.2.3.2.9 Interruptions at SCell hibernation 168

8.2.3.2.10 Interruptions at SCell activation/deactivation with multiple downlink SCells 169

8.2.3.2.11 Interruptions at NR SRS carrier based switching 169

8.2.3.2.12 Interruptions at E-UTRA SRS carrier based switching 170

8.2.3.2.13 Interruptions due to SCell dormancy 171

8.2.3.2.14 Interruptions when identifying CGI of an NR cell with autonomous gaps 172

8.2.3.2.15 Interruptions when identifying CGI of an E-UTRA cell with autonomous gaps 172

8.2.3.2.16 Interruptions due to UE-specific CBW change 173

8.2.4 NR-DC: Interruptions 173

8.2.4.1 Introduction 173

8.2.4.2 Requirements 174

8.2.4.2.1 Interruptions at PSCell/SCell addition/release 174

8.2.4.2.3 Interruptions during measurements on SCC 175

8.2.4.2.4 Interruptions at UL carrier RRC reconfiguration 175

8.2.4.2.5 Interruptions due to Active BWP switching Requirement 176

8.2.4.2.6 Interruptions at transitions between active and non-active during DRX 176

8.2.4.2.7 Interruptions at transitions from non-DRX to DRX 176

8.2.4.2.8 Interruptions at SCell activation/deactivation with multiple downlink SCells 177

8.2.4.2.9 Interruptions at NR SRS carrier based switching 177

8.2.4.2.10 Interruptions at direct SCell activation 178

8.2.4.2.11 Interruptions when identifying CGI of an NR cell with autonomous gaps 179

8.2.4.2.12 Interruptions when identifying CGI of an E-UTRA cell with autonomous gaps 179

8.2.4.2.13 Interruptions due to SCell dormancy 180

8.2.4.2.14 Interruptions due to UE-specific CBW change 180

8.2.4.2A Void 181

8.2.4.2A.1 Void 181

8.2.4.2A.2 Void 181

8.2.4.2A.3 Void 181

8.3 SCell Activation and Deactivation Delay 181

8.3.1 Introduction 181

8.3.2 SCell Activation Delay Requirement for Deactivated SCell 181

8.3.3 SCell Deactivation Delay Requirement for Activated SCell 185

8.3.4 Direct SCell Activation at SCell addition 185

8.3.5 Direct SCell Activation at Handover 187

8.3.7 SCell Activation Delay Requirement for Deactivated SCell with Multiple Downlink SCells 189

8.3.8 SCell Deactivation Delay Requirement for Activated SCell with Multiple Downlink SCells 193

8.3.9 Direct SCell Activation of Multiple Downlink SCells at SCell addition 193

8.3.10 Direct SCell Activation of Multiple Downlink SCells at Handover 194

8.3A SCell Activation and Deactivation Delay in Carriers with CCA 196

8.3A.1 Introduction 196

8.3A.2 SCell Activation Delay Requirement for Deactivated SCell 196

8.3A.3 SCell Deactivation Delay Requirement for Activated SCell 199

8.4 UE UL carrier RRC reconfiguration delay 199

8.4.1 Introduction 199

8.4.2 UE UL carrier configuration delay requirement 199

8.4.3 UE UL carrier deconfiguration delay requirement 199

8.5 Link Recovery Procedures 200

8.5.1 Introduction 200

8.5.2 Requirements for SSB based beam failure detection 201

8.5.2.1 Introduction 201

8.5.2.2 Minimum requirement 201

8.5.2.3 Measurement restriction for SSB based beam failure detection 203

8.5.3 Requirements for CSI-RS based beam failure detection 203

8.5.3.1 Introduction 203

8.5.3.2 Minimum requirement 204

8.5.3.3 Measurement restrictions for CSI-RS beam failure detection 206

8.5.4 Minimum requirement for L1 indication 207

8.5.5 Requirements for SSB based candidate beam detection 207

8.5.5.1 Introduction 207

8.5.5.2 Minimum requirement 207

8.5.5.3 Measurement restriction for SSB based candidate beam detection 209

8.5.6 Requirements for CSI-RS based candidate beam detection 210

8.5.6.1 Introduction 210

8.5.6.2 Minimum requirement 210

8.5.6.3 Measurement restriction for CSI-RS based candidate beam detection 212

8.5.7 Scheduling availability of UE during beam failure detection 213

8.5.7.1 Scheduling availability of UE performing beam failure detection with a same subcarrier spacing as PDSCH/PDCCH on FR1 213

8.5.7.2 Scheduling availability of UE performing beam failure detection with a different subcarrier spacing than PDSCH/PDCCH on FR1 213

8.5.7.3 Scheduling availability of UE performing beam failure detection on FR2 213

8.5.7.4 Scheduling availability of UE performing beam failure detection on FR1 or FR2 in case of FR1-FR2 inter-band CA and NR DC 214

8.5.8 Scheduling availability of UE during candidate beam detection 214

8.5.8.1 Scheduling availability of UE performing L1-RSRP measurement with a same subcarrier spacing as PDSCH/PDCCH on FR1 214

8.5.8.2 Scheduling availability of UE performing L1-RSRP measurement with a different subcarrier spacing than PDSCH/PDCCH on FR1 214

8.5.8.3 Scheduling availability of UE performing L1-RSRP measurement on FR2 214

8.5.8.4 Scheduling availability of UE performing L1-RSRP measurement on FR1 or FR2 in case of FR1-FR2 inter-band CA and NR-DC 215

8.5.9 Requirements for Beam Failure Recovery in SCell 215

8.5.9.1 Introduction 215

8.5.9.2 Requirement 215

8.5.10 Minimum requirement at transitions for beam failure detection 215

8.5A Link Recovery Procedures when CCA is used on target frequency 216

8.5A.1 Introduction 216

8.5A.2 Requirements for SSB based beam failure detection 216

8.5A.2.1 Introduction 216

8.5A.2.2 Minimum requirement 217

8.5A.2.3 Measurement restriction for SSB based beam failure detection 217

8.5A.4 Minimum requirement for L1 indication 218

8.5A.5 Requirements for SSB based candidate beam detection 218

8.5A.5.1 Introduction 218

8.5A.5.2 Minimum requirement 218

8.5A.5.3 Measurement restriction for SSB based candidate beam detection 219

8.5A.7 Scheduling availability of UE during beam failure detection 219

8.5A.7.1 Scheduling availability of UE performing beam failure detection with a same subcarrier spacing as PDSCH/PDCCH 219

8.5A.7.2 Scheduling availability of UE performing beam failure detection with a different subcarrier spacing than PDSCH/PDCCH 219

8.5A.8 Scheduling availability of UE during candidate beam detection 219

8.5A.8.1 Scheduling availability of UE performing L1-RSRP measurement with a same subcarrier spacing as PDSCH/PDCCH 220

8.5A.8.2 Scheduling availability of UE performing L1-RSRP measurement with a different subcarrier spacing than PDSCH/PDCCH 220

8.6 Active BWP switch delay 220

8.6.1 Introduction 220

8.6.2 DCI and timer based BWP switch delay on a single CC 220

8.6.2A DCI based BWP switch delay on multiple CCs 221

8.6.2A.1 Simultaneous DCI based BWP switch delay on multiple CCs 221

8.6.2A.2 Non-simultaneous DCI based BWP switch delay on multiple CCs 223

8.6.2B Timer based BWP switch delay on multiple CCs 223

8.6.2B.1 Simultaneous timer based BWP switch delay on multiple CCs 223

8.6.2B.2 Non-simultaneous timer based BWP switch delay on multiple CCs 224

8.6.3 RRC based BWP switch delay on a single CC 224

8.6.3A RRC based BWP switch delay on multiple CCs 225

8.6.3A.1 Simultaneous RRC based BWP switch delay on multiple CCs 225

8.6.3A.2 Non-simultaneous RRC based BWP switch delay on multiple CCs 225

8.6.4 BWP switch delay on Consistent UL CCA recovery 226

8.7 Void 226

8.8 NE-DC: E-UTRAN PSCell Addition and Release Delay 226

8.8.1 Introduction 226

8.8.2 E-UTRAN PSCell Addition Delay Requirement 226

8.8.3 E-UTRAN PSCell Release Delay Requirement 227

8.9 NR-DC: PSCell Addition and Release Delay 227

8.9.1 Introduction 227

8.9.2 PSCell Addition Delay Requirement 227

8.9.3 PSCell Release Delay Requirement 228

8.10 Active TCI state switching delay 228

8.10.4 DCI based TCI state switch delay 230

8.10.5 RRC based TCI state switch delay 230

8.10.6 Active TCI state list update delay 230

8.10A Active TCI state switching delay with CCA 231

8.10A.1 Introduction 231

8.10A.2 Known conditions for TCI state 231

8.10A.3 MAC-CE based TCI state switch delay 231

8.10A.4 DCI based TCI state switch delay 232

8.10A.5 RRC based TCI state switch delay 232

8.10A.6 Active TCI state list update delay 233

8.11 PSCell Change 233

8.11A void 234

8.11B Conditional PSCell Change 234

8.11B.1 Introduction 234

8.11B.2 Conditoinal PSCell Change delay 234

8.11B.2.1 Measurement time 234

8.12 Uplink spatial relation switch delay 235

8.12.1 Introduction 235

8.12.2 Known conditions for spatial relation when associated with DL-RS 235

8.12.3 MAC-CE based spatial relation switch delay 235

8.12.4 DCI based spatial relation switch delay 236

8.12.5 RRC based spatial relation switch delay 236

8.13 UE-specific CBW change 237

8.13.1 Introduction 237

8.13.2 UE-specific CBW change delay 237

8.14 Pathloss reference signal switching delay 237

8.14.1 Introduction 237

8.14.2 Known conditions for pathloss reference signal 237

8.14.3 MAC-CE based pathloss reference signal switch delay 238

9 Measurement Procedure 239

9.1 General measurement requirement 239

9.1.1 Introduction 239

9.1.2 Measurement gap 239

9.1.2.1 EN-DC: Measurement Gap Sharing 250

9.1.2.1a SA: Measurement Gap Sharing 250

9.1.2.1b NE-DC: Measurement Gap Sharing 251

9.1.2.1c NR-DC: Measurement Gap Sharing 252

9.1.3 UE Measurement capability 253

9.1.3.1 EN-DC: Monitoring of multiple layers using gaps 253

9.1.3.1a SA: Monitoring of multiple layers using gaps 253

9.1.3.1b NE-DC: Monitoring of multiple layers using gaps 254

9.1.3.1c NR-DC: Monitoring of multiple layers using gaps 254

9.1.3.2 EN-DC: Maximum allowed layers for multiple monitoring 255

9.1.3.2a SA: Maximum allowed layers for multiple monitoring 256

9.1.3.2b NE-DC: Maximum allowed layers for multiple monitoring 256

9.1.3.2c NR-DC: Maximum allowed layers for multiple monitoring 257

9.1A.3.2 Void 258

9.1.3A UE Measurement capability under operation mode with CCA 258

9.1.3A.1 EN-DC: Monitoring of multiple layers using gaps under CCA 258

9.1.3A.1A SA: Monitoring of multiple layers using gaps under CCA 258

9.1.3A.2 EN-DC: Maximum allowed layers for multiple monitoring under CCA 258

9.1A.3.2a Void 259

9.1.3A.2A SA: Maximum allowed layers for multiple monitoring under CCA 259

9.1.4 Capabilities for Support of Event Triggering and Reporting Criteria 259

9.1.4.1 Introduction 259

9.1.4.2 Requirements 259

9.1.5 Carrier-specific scaling factor 263

9.1.5.1 Monitoring of multiple layers outside gaps 263

9.1.5.1.1 EN-DC mode: carrier-specific scaling factor for SSB-based, CSI-RS based L3 measurements and RSSI and channel occupancy measurements performed outside gaps 265

9.1.5.1.2 SA mode: carrier-specific scaling factor for SSB-based, CSI-RS based L3 measurements and RSSI and channel occupancy measurements performed outside gaps 266

9.1.5.1.3 NR-DC mode: carrier-specific scaling factor for SSB-based and CSI-RS based L3 measurements performed outside gaps 267

9.1.5.1.4 NE-DC mode: carrier-specific scaling factor for SSB-based and CSI-RS based measurements performed outside gaps 268

9.1.5.2 Monitoring of multiple layers within gaps 269

9.1.5.2.1 EN-DC mode: carrier-specific scaling factor for SSB, CSI-RS-based L3 measurements and RSSI and channel occupancy measurements performed within gaps 270

9.1.5.2.2 SA mode: carrier-specific scaling factor for SSB, CSI-RS-based L3 measurements and RSSI and channel occupancy measurements performed within gaps 272

9.1.5.2.3 NE-DC: carrier-specific scaling factor for SSB-based and CSI-RS based L3 measurements performed within gaps 274

9.1.5.2.4 NR-DC: carrier-specific scaling factor for SSB-based and CSI-RS-based L3 measurements performed within gaps 276

9.1.5.2.5 SA mode: carrier-specific scaling factor for PRS-based measurements performed within gaps 277

9.1.5.2.6 NE-DC: carrier-specific scaling factor for PRS-based measurements performed within gaps 278

9.1.5.2.7 NR-DC: carrier-specific scaling factor for PRS-based measurements performed within gaps 278

9.1.6 Minimum requirement at transitions 278

9.2 NR intra-frequency measurements 278

9.2.1 Introduction 278

9.2.2 Requirements applicability 279

9.2.3 Number of cells and number of SSB 279

9.2.3.1 Requirements for FR1 279

9.2.3.2 Requirements for FR2 279

9.2.4 Measurement Reporting Requirements 280

9.2.4.1 Periodic Reporting 280

9.2.4.2 Event-triggered Periodic Reporting 280

9.2.4.3 Event Triggered Reporting 280

9.2.5 Intrafrequency measurements without measurement gaps 281

9.2.5.1 Intrafrequency cell identification 281

9.2.5.2 Measurement period 283

9.2.5.3 Scheduling availability of UE during intra-frequency measurements 285

9.2.5.3.1 Scheduling availability of UE performing measurements in TDD bands on FR1 285

9.2.5.3.2 Scheduling availability of UE performing measurements with a different subcarrier spacing than PDSCH/PDCCH on FR1 285

9.2.5.3.3 Scheduling availability of UE performing measurements on FR2 286

9.2.5.3.4 Scheduling availability of UE performing measurements on FR1 or FR2 in case of FR1-FR2 inter-band CA 287

9.2.5.4 SFTD Measurements between PCell and PSCell 287

9.2.5.4.1 Introduction 287

9.2.5.4.2 SFTD Measurement delay 287

9.2.5.4.3 SFTD Measurement Reporting Delay 288

9.2.6 Intra-frequency measurements with measurement gaps 288

9.2.6.1 Void 288

9.2.6.2 Intra-frequency cell identification 288

9.2.6.3 Intrafrequency Measurement Period 290

9.2A NR intra-frequency measurements with CCA 291

9.2A.1 Introduction 291

9.2A.2 Requirements applicability 291

9.2A.3 Number of cells and number of SSB 292

9.2A.4 Measurement Reporting Requirements 292

9.2A.5 Intra-frequency measurements without measurement gaps 292

9.2A.5.2 Measurement period 295

9.2A.5.3 Scheduling availability of UE during intra-frequency measurements 296

9.2A.5.3.1 Scheduling availability of UE performing measurements in TDD bands 296

9.2A.5.3.2 Scheduling availability of UE performing measurements with a different subcarrier spacing than PDSCH/PDCCH 297

9.2A.6 Intra-frequency measurements with measurement gaps 297

9.2A.6.1 Intra-frequency cell identification 297

9.2A.6.2 Intra-frequency Measurement Period 298

9.2A.7 Intra-frequency RSSI and Channel occupancy measurements 299

9.2A.7.1 Intra-frequency RSSI measurements 299

9.2A.7.2 Intra-frequency Channel occupancy measurements 300

9.2A.7.3 Scheduling restriction during RSSI and Channel Occupancy measurements 301

9.3 NR inter-frequency measurements 301

9.3.1 Introduction 301

9.3.2 Requirements applicability 302

9.3.2.1 Void 302

9.3.2.2 Void 302

9.3.3 Number of cells and number of SSB 302

9.3.3.1 Requirements for FR1 302

9.3.3.2 Requirements for FR2 302

9.3.4 Inter-frequency measurement with measurement gaps 302

9.3.4.1 Void 304

9.3.4.2 Void 304

9.3.5 Inter-frequency measurements 304

9.3.5.1 Void 304

9.3.5.2 Void 304

9.3.5.3 Void 304

9.3.6 Inter-frequency measurements reporting requirements 304

9.3.6.1 Periodic Reporting 304

9.3.6.2 Event-triggered Periodic Reporting 305

9.3.6.3 Event-triggered Reporting 305

9.3.7 Void 305

9.3.8 Inter-frequency SFTD measurement requirements 305

9.3.8.1 Introduction 305

9.3.8.2 SFTD Measurement delay 305

9.3.8.3 SFTD Measurement reporting delay 306

9.3.9 Inter frequency measurements without measurement gaps 307

9.3.9.1 Inter frequency Cell identification 307

9.3.9.2 Measurement period 308

9.3.9.3 Scheduling availability of UE during inter-frequency measurements 309

9.3.9.3.1 Scheduling availability of UE performing measurements in TDD bands on FR1 309

9.3.9.3.2 Scheduling availability of UE performing measurements with a different subcarrier spacing than PDSCH/PDCCH on FR1 310

9.3.9.3.3 Scheduling availability of UE performing measurements on FR2 310

9.3.9.3.4 Scheduling availability of UE performing measurements on FR1 or FR2 in case of FR1-FR2 inter-band CA 310

9.3A NR inter-frequency measurements in carrier frequencies with CCA 311

9.3A.1 Introduction 311

9.3A.2 Requirements applicability 311

9.3A.3 Number of cells and number of SSB 311

9.3A.3.1 Requirements 311

9.3A.4 Inter-frequency cell identification 312

9.3A.5 Inter-frequency measurements 313

9.3A.6 NR Inter-frequency measurements reporting requirements 314

9.3A.6.1 Periodic Reporting 314

9.3A.6.2 Event-triggered Periodic Reporting 314

9.3A.6.3 Event-triggered Reporting 314

9.3A.8 Inter-frequency RSSI measurements 314

9.3A.9 Inter-frequency channel occupancy measurements 315

9.4 Inter-RAT measurements 315

9.4.1 Introduction 315

9.4.2 NR − E-UTRAN FDD measurements 317

9.4.2.1 Introduction 317

9.4.2.2 Requirements when no DRX is used 317

9.4.2.3 Requirements when DRX is used 318

9.4.2.4 Measurement reporting requirements 319

9.4.2.4.1 Periodic Reporting 319

9.4.2.4.2 Event-Triggered Periodic Reporting 319

9.4.2.4.3 Event-Triggered Reporting 319

9.4.3 NR − E-UTRAN TDD measurements 319

9.4.3.1 Introduction 319

9.4.3.2 Requirements when no DRX is used 319

9.4.3.3 Requirements when DRX is used 320

9.4.3.4 Measurement reporting requirements 322

9.4.3.4.1 Periodic Reporting 322

9.4.3.4.2 Event-Triggered Periodic Reporting 322

9.4.3.4.3 Event-Triggered Reporting 322

9.4.4 Inter-RAT RSTD measurements 322

9.4.4.1 NR − E-UTRAN FDD RSTD measurements 322

9.4.4.1.1 Introduction 322

9.4.4.1.2 Requirements 323

9.4.4.2 NR − E-UTRAN TDD RSTD measurements 326

9.4.4.2.1 Introduction 326

9.4.4.2.2 Requirements 327

9.4.5 Inter-RAT E-CID measurements 330

9.4.5.1 NR−E-UTRAN FDD E-CID RSRP and RSRQ measurements 330

9.4.5.1.1 Introduction 330

9.4.5.1.2 Requirements 330

9.4.5.1.3 Measurement Reporting Delay 330

9.4.5.2 NR−E-UTRAN TDD E-CID RSRP and RSRQ measurements 330

9.4.5.2.1 Introduction 330

9.4.5.2.2 Requirements 330

9.4.5.2.3 Measurement Reporting Delay 331

9.4.6 NR − UTRAN FDD measurements 331

9.4.6.1 Introduction 331

9.4.6.2 Requirements when no DRX is used 331

9.4.6.3 Requirements when DRX is used 332

9.4.7 NR – E-UTRAN measurements with autonomous gaps 334

9.4.7.1 CGI identification of an E-UTRA cell with autonomous gaps 334

9.4.7.2 CGI reporting delay 334

9.5 L1-RSRP measurements for Reporting 335

9.5.1 Introduction 335

9.5.2 Requirements applicability 335

9.5.3 Measurement Reporting Requirements 335

9.5.3.1 Periodic Reporting 336

9.5.3.2 Semi-Persistent Reporting 336

9.5.3.3 Aperiodic Reporting 336

9.5.4 L1-RSRP measurement requirements 336

9.5.4.1 SSB based L1-RSRP Reporting 336

9.5.4.2 CSI-RS based L1-RSRP Reporting 338

9.5.4A Void 341

9.5.4A.1 Void 341

9.5.5 Measurement restriction for CSI-RS and SSB for L1-RSRP measurement 341

9.5.5.1 Measurement restriction for SSB based L1-RSRP 341

9.5.5.2 Measurement restriction for CSI-RS based L1-RSRP 341

9.5.6 Scheduling availability of UE during L1-RSRP measurement 342

9.5.6.1 Scheduling availability of UE performing L1-RSRP measurement with a same subcarrier spacing as PDSCH/PDCCH on FR1 342

9.5.6.2 Scheduling availability of UE performing L1-RSRP measurement with a different subcarrier spacing than PDSCH/PDCCH on FR1 342

9.5.6.3 Scheduling availability of UE performing L1-RSRP measurement on FR2 343

9.5.6.4 Scheduling availability of UE performing L1-RSRP measurement on FR1 or FR2 in case of FR1-FR2 inter-band CA 343

9.5A L1-RSRP measurements for Reporting under CCA 344

9.5A.1 Introduction 344

9.5A.2 Requirements applicability 344

9.5A.3 Measurement Reporting Requirements 344

9.5A.3.1 Periodic Reporting 344

9.5A.3.2 Semi-Persistent Reporting 345

9.5A.3.3 Aperiodic Reporting 345

9.5A.4 L1-RSRP measurement requirements 345

9.5A.4.1 SSB based L1-RSRP Reporting 345

9.5A.5 Measurement restriction for L1-RSRP measurement 346

9.5A.5.1 Measurement restriction for SSB based L1-RSRP 346

9.5A.6 Scheduling availability of UE during L1-RSRP measurement 346

9.5A.6.1 Scheduling availability of UE performing L1-RSRP measurement with a same subcarrier spacing as PDSCH/PDCCH 346

9.5A.6.2 Scheduling availability of UE performing L1-RSRP measurement with a different subcarrier spacing than PDSCH/PDCCH 347

9.5A.6.3 Scheduling availability of UE performing L1-RSRP measurement in case of FR1-FR2 inter-band CA 347

9.6 NE-DC: Measurements 347

9.6.1 Introduction 347

9.6.2 SFTD Measurements 347

9.6.2.1 Introduction 347

9.6.2.2 SFTD Measurement requirements 347

9.7 Cross Link Interference measurements 348

9.7.1 Introduction 348

9.7.2 SRS-RSRP measurements 348

9.7.2.1 Introduction 348

9.7.2.2 Requirements applicability 348

9.7.2.3 Measurement Reporting Requirements 349

9.7.2.3.1 Periodic Reporting 349

9.7.2.3.2 Event-triggered Periodic Reporting 349

9.7.2.3.3 Event Triggered Reporting 349

9.7.2.4 Measurement capability 349

9.7.2.5 SRS-RSRP measurement period 349

9.7.3 CLI-RSSI measurements 350

9.7.3.1 Introduction 350

9.7.3.2 Requirements applicability 350

9.7.3.3 Measurement Reporting Requirements 350

9.7.3.3.1 Periodic Reporting 350

9.7.3.3.2 Event-triggered Periodic Reporting 350

9.7.3.3.3 Event Triggered Reporting 350

9.7.3.4 Measurement capability 351

9.7.3.5 CLI-RSSI measurement period 351

9.7.4 Scheduling availability of UE during CLI measurements 351

9.7.4.1 Scheduling availability of UE performing measurement on FR1 351

9.7.4.2 Scheduling availability of UE performing measurement on FR2 351

9.8 L1-SINR measurements for Reporting 352

9.8.1 Introduction 352

9.8.2 Requirements applicability 352

9.8.3 Measurement Reporting Requirements 353

9.8.3.1 Periodic Reporting 353

9.8.3.2 Semi-Persistent Reporting 353

9.8.3.3 Aperiodic Reporting 354

9.8.4 L1-SINR measurement requirements 354

9.8.4.1 L1-SINR reporting with CSI-RS based CMR and no dedicated IMR configured 354

9.8.4.3 L1-SINR reporting with CSI-RS based CMR and dedicated IMR configured 357

9.8.5 Measurement restriction for L1-SINR measurement 359

9.8.5.1 Measurement restriction if SSB configured for L1-SINR Measurement 359

9.8.5.2 Measurement restriction if CSI-RS configured for L1-SINR measurement 360

9.8.5.3 Measurement restriction if CSI-IM configured for L1-SINR measurement 360

9.8.6 Scheduling availability of UE during L1-SINR measurement 361

9.8.6.1 Scheduling availability of UE performing L1-SINR measurement with a same subcarrier spacing as PDSCH/PDCCH on FR1 361

9.8.6.2 Scheduling availability of UE performing L1-SINR measurement with a different subcarrier spacing than PDSCH/PDCCH on FR1 361

9.8.6.4 Scheduling availability of UE performing L1-SINR measurement on FR1 or FR2 in case of FR1-FR2 inter-band CA 362

9.9 NR measurements for positioning 362

9.9.1 Introduction 362

9.9.2 RSTD measurements 363

9.9.2.1 Introduction 363

9.9.2.2 Requirements Applicability 363

9.9.2.3 Measurement Capability 363

9.9.2.4 Measurement Reporting Requirements 363

9.9.2.4.1 Void 363

9.9.2.4.2 Void 363

9.9.2.4.3 Void 363

9.9.2.5 Measurements Period Requirements 363

9.9.2.6 Void 365

9.9.3 PRS-RSRP measurements 365

9.9.3.1 Introduction 365

9.9.3.2 Requirements applicability 365

9.9.3.3 Measurement Capability 366

9.9.3.4 Measurement Reporting Requirements 366

9.9.3.5 Measurement Period Requirements 366

9.9.4 UE Rx-Tx time difference measurements 368

9.9.4.1 Introduction 368

9.9.4.2 Requirements Applicability 368

9.9.4.3 Measurement Capability 368

9.9.4.4 Measurement Reporting Requirements 368

9.9.4.5 Measurement Period Requirements 368

9.9.5 NR E-CID measurements 371

9.9.5.1 Introduction 371

9.9.5.2 Measurement Requirements 371

9.9.5.2.1 Intra-frequency Measurement Requirements 371

9.9.5.2.2 Inter-frequency Measurement Requirements 371

9.9.5.2.3 Measurement Reporting Delay 372

9.10 CSI-RS based L3 measurements 372

9.10.1 Introduction 372

9.10.2 CSI-RS based intra-frequency measurements 372

9.10.2.1 Introduction 372

9.10.2.2 Requirements applicability 373

9.10.2.3 Number of cells and number of CSI-RS 374

9.10.2.3.1 Requirements for FR1 374

9.10.2.3.2 Requirements for FR2 374

9.10.2.4 Measurement Reporting Requirements 374

9.10.2.4.1 Periodic Reporting 375

9.10.2.4.2 Event-triggered Periodic Reporting 375

9.10.2.4.3 Event Triggered Reporting 375

9.10.2.5 Intra-frequency measurements without measurement gaps 375

9.10.2.6 Scheduling availability of UE during CSI-RS based intra-frequency measurements 376

9.10.2.6.1 Scheduling availability of UE performing CSI-RS based measurements in TDD bands 376

9.10.2.6.2 Scheduling availability of UE performing CSI-RS based measurements in FR2 377

9.10.3 CSI-RS based Inter-frequency measurements 377

9.10.3.1 Introduction 377

9.10.3.2 Requirements applicability 377

9.10.3.3 Number of cells and number of CSI-RS resources 378

9.10.3.3.1 Requirements for FR1 378

9.10.3.3.2 Requirements for FR2 378

9.10.3.4 Measurements reporting requirements 378

9.10.3.4.1 Periodic Reporting 378

9.10.3.4.2 Event-triggered Periodic Reporting 378

9.10.3.4.3 Event-triggered Reporting 379

9.10.3.5 Inter frequency measurements with measurement gaps 379

9.11 NR measurements with autonomous gaps 380

9.11.1 Introduction 380

9.11.2 CGI identification of an NR cell with autonomous gaps 380

9.11.3 CGI reporting delay 381

10 Measurement Performance requirements 381

10.1 NR measurements 381

10.1.1 Introduction 381

10.1.2 Intra-frequency RSRP accuracy requirements for FR1 382

10.1.2.1 Intra-frequency SS-RSRP accuracy requirements 382

10.1.2.1.1 Absolute SS-RSRP Accuracy 382

10.1.2.1.2 Relative SS-RSRP Accuracy 383

10.1.2.2 Void 384

10.1.2.3 Intra-frequency CSI-RSRP accuracy requirements 384

10.1.2.3.1 Absolute CSI-RSRP Accuracy 384

10.1.2.3.2 Relative CSI-RSRP Accuracy 385

10.1.2B Intra-frequency RSRP accuracy requirements for FR1 for CA/DC Idle Mode Measurements 386

10.1.2B.1 Intra-frequency SS-RSRP accuracy requirements 386

10.1.2B.1.1 Absolute SS-RSRP Accuracy 386

10.1.3 Intra-frequency RSRP accuracy requirements for FR2 387

10.1.3.1 Intra-frequency SS-RSRP accuracy requirements 387

10.1.3.1.1 Absolute SS-RSRP Accuracy 387

10.1.3.1.2 Relative SS-RSRP Accuracy 388

10.1.3.2 Void 389

10.1.3.3 Intra-frequency CSI-RSRP accuracy requirements 389

10.1.3.3.1 Absolute CSI-RSRP Accuracy 389

10.1.3.3.2 Relative CSI-RSRP Accuracy 389

10.1.3B Intra-frequency RSRP accuracy requirements for FR2 for CA/DC Idle Mode Measurements 390

10.1.3B.1 Intra-frequency SS-RSRP accuracy requirements 390

10.1.3B.1.1 Absolute SS-RSRP Accuracy 391

10.1.4 Inter-frequency RSRP accuracy requirements for FR1 391

10.1.4.1 Inter-frequency SS-RSRP accuracy requirements 391

10.1.4.1.1 Absolute Accuracy of SS-RSRP in FR1 391

10.1.4.1.2 Relative Accuracy of SS-RSRP in FR1 392

10.1.4.2 Void 393

10.1.4.3 Inter-frequency CSI-RSRP accuracy requirements 393

10.1.4.3.1 Absolute Accuracy of CSI-RSRP in FR1 393

10.1.4.3.2 Relative Accuracy of CS-RSRP in FR1 394

10.1.4B Inter-frequency RSRP accuracy requirements for FR1 for CA/DC Idle Mode Measurements 395

10.1.4B.1 Inter-frequency SS-RSRP accuracy requirements 395

10.1.4B.1.1 Absolute Accuracy of SS-RSRP in FR1 395

10.1.5 Inter-frequency RSRP accuracy requirements for FR2 396

10.1.5.1 Inter-frequency SS-RSRP accuracy requirements 396

10.1.5.1.1 Absolute SS-RSRP Accuracy 396

10.1.5.1.2 Relative SS-RSRP Accuracy 397

10.1.5.2 Void 398

10.1.5.3 Inter-frequency CSI-RSRP accuracy requirements 398

10.1.5.3.1 Absolute CSI-RSRP Accuracy 398

10.1.5.3.2 Relative CSI-RSRP Accuracy 398

10.1.5B Inter-frequency RSRP accuracy requirements for FR2 for CA/DC Idle Mode Measurements 399

10.1.6 RSRP Measurement Report Mapping 400

10.1.7 Intra-frequency RSRQ accuracy requirements for FR1 402

10.1.7.1 Intra-frequency SS-RSRQ accuracy requirements in FR1 402

10.1.7.1.1 Absolute SS-RSRQ Accuracy in FR1 402

10.1.7.2 Intra-frequency CSI-RSRQ accuracy requirements 403

10.1.7.2.1 Absolute CSI-RSRQ Accuracy 403

10.1.7B Intra-frequency RSRQ accuracy requirements for FR1 for CA/DC Idle Mode Measurements 404

10.1.7B.1 Intra-frequency SS-RSRQ accuracy requirements in FR1 404

10.1.7B.1.1 Absolute SS-RSRQ Accuracy in FR1 404

10.1.8 Intra-frequency RSRQ accuracy requirements for FR2 405

10.1.8.1 Intra-frequency SS-RSRQ accuracy requirements in FR2 405

10.1.8.1.1 Absolute SS-RSRQ Accuracy in FR2 405

10.1.8.2 Intra-frequency CSI-RSRQ accuracy requirements 406

10.1.8.2.1 Absolute CSI-RSRQ Accuracy 406

10.1.8B Intra-frequency RSRQ accuracy requirements for FR2 for CA/DC Idle Mode Measurements 407

10.1.8B.1 Intra-frequency SS-RSRQ accuracy requirements in FR2 407

10.1.8B.1.1 Absolute SS-RSRQ Accuracy in FR2 407

10.1.9 Inter-frequency RSRQ accuracy requirements for FR1 408

10.1.9.1 Inter-frequency SS-RSRQ accuracy requirements in FR1 408

10.1.9.1.1 Absolute Accuracy of SS-RSRQ in FR1 408

10.1.9.1.2 Relative Accuracy of SS-RSRQ in FR1 409

10.1.9.2 Inter-frequency CSI-RSRQ accuracy requirements 410

10.1.9.2.1 Absolute CSI-RSRQ Accuracy 410

10.1.9.2.2 Relative CSI-RSRQ Accuracy 411

10.1.9B Inter-frequency RSRQ accuracy requirements for FR1 for CA/DC Idle Mode Measurements 412

10.1.9B.1 Inter-frequency SS-RSRQ accuracy requirements in FR1 412

10.1.9B.1.1 Absolute Accuracy of SS-RSRQ in FR1 412

10.1.10 Inter-frequency RSRQ accuracy requirements for FR2 413

10.1.10.2 Inter-frequency CSI-RSRQ accuracy requirements 415

10.1.10.2.1 Absolute CSI-RSRQ Accuracy 415

10.1.10.2.2 Relative CSI-RSRQ Accuracy 415

10.1.10B Inter-frequency RSRQ accuracy requirements for FR2 for CA/DC Idle Mode Measurements 416

10.1.10B.1 Inter-frequency SS-RSRQ accuracy requirements in FR2 416

10.1.10B.1.1 Absolute Accuracy of SS-RSRQ in FR2 416

10.1.11 RSRQ report mapping 417

10.1.12 Intra-frequency SINR accuracy requirements for FR1 418

10.1.12.2 Intra-frequency CSI-SINR accuracy requirements in FR1 418

10.1.12.2.1 Absolute CSI-SINR Accuracy in FR1 418

10.1.13 Intra-frequency SINR accuracy requirements for FR2 419

10.1.13.2 Intra-frequency CSI-SINR accuracy requirements in FR2 420

10.1.13.2.1 Absolute CSI-SINR Accuracy in FR2 420

10.1.14 Inter-frequency SINR accuracy requirements for FR1 421

10.1.14.2 Inter-frequency CSI-SINR accuracy requirements in FR1 423

10.1.14.2.1 Aboslute Accuracy of CSI-SINR in FR1 423

10.1.15 Inter-frequency SINR accuracy requirements for FR2 425

10.1.15.2 Inter-frequency CSI-SINR accuracy requirements in FR2 427

10.1.15.2.1 Aboslute Accuracy of CSI-SINR in FR2 427

10.1.15.2.2 Relative Accuracy of CSI-SINR in FR2 427

10.1.16 SINR report mapping 428

10.1.17 Power Headroom 429

10.1.18 PCMAX,c,f 430

10.1.19 L1-RSRP accuracy requirements for FR1 430

10.1.20 L1-RSRP accuracy requirements for FR2 434

10.1.21 SFTD accuracy requirements 437

10.1.22 CLI measurement accuracy requirements 441

10.1.24.3.1 Absolute PRS-RSRP Measurement Report Mapping 445

10.1.24.3.2 Differential Report Mapping for PRS-RSRP Measurement 445

10.1.23 RSTD Measurements 447

10.1.23.1 Introduction 447

10.1.23.2 Measurement Accuracy Requirements 448

10.1.23.3 Report mapping 454

10.1.23.3.1 Absolute DL RSTD Measurement Reporting 454

10.1.23.3.2 Differential Reporting for DL RSTD Measurement 456

10.1.23.3.3 Additional Path Report Mapping for DL RSTD 458

10.1.24 PRS-RSRP Measurements 460

10.1.24.1 Introduction 460

10.1.24.2 Measurement Accuracy Requirements 460

10.1.24.2.1 Absolute PRS RSRP accuracy 460

10.1.24.3 Report mapping 464

10.1.24.3.1 Absolute PRS-RSRP Measurement Report Mapping 464

10.1.24.3.2 Differential Report Mapping for PRS-RSRP Measurement 465

10.1.25 UE Rx-Tx Time Difference Measurements 467

10.1.25.1 Introduction 467

10.1.25.2 Measurement Accuracy Requirements 468

10.1.25.3 Report mapping 474

10.1.25.3.1 Absolute UE Rx-Tx Measurement Report Mapping 474

10.1.25.3.2 Differential UE Rx-Tx Measurement Report Mapping 476

10.1.25.3.3 Additional Path Report Mapping for UE Rx-Tx Time Difference 477

10.1.26 FR2 P-MPR report 479

10.1.26.1 Report mapping 479

10.1.27 L1-SINR accuracy requirements for FR1 479

10.1.27.1 L1-SINR accuracy requirements with CSI-RS based CMR and no dedicated IMR configured 479

10.1.27.1.1 Absolute Accuracy 479

10.1.27.1.2 Relative Accuracy 480

10.1.27.2 L1-SINR accuracy requirements with SSB based CMR and dedicated IMR configured 481

10.1.27.2.1 Absolute Accuracy 481

10.1.27.2.2 Relative Accuracy 482

10.1.27.3 L1-SINR accuracy requirements with CSI-RS based CMR and dedicated IMR configured 484

10.1.27.3.1 Absolute Accuracy 484

10.1.27.3.2 Relative Accuracy 486

10.1.28 L1-SINR accuracy requirements for FR2 487

10.1.28.1 L1-SINR accuracy requirements with CSI-RS based CMR and no dedicated IMR configured 487

10.1.28.1.1 Absolute Accuracy 487

10.1.28.1.2 Relative Accuracy 488

10.1.28.2 L1-SINR accuracy requirements with SSB based CMR and dedicated IMR configured 489

10.1.28.2.1 Absolute Accuracy 489

10.1.28.2.2 Relative Accuracy 490

10.1.28.3 L1-SINR accuracy requirements with CSI-RS based CMR and dedicated IMR configured 491

10.1.28.3.1 Absolute Accuracy 491

10.1.28.3.2 Relative Accuracy 492

10.1.29 Intra-frequency RSRQ accuracy requirements under CCA 494

10.1.29.1 Intra-frequency SS-RSRQ accuracy requirements in FR1 494

10.1.29.1.1 Absolute SS-RSRQ Accuracy 494

10.1.30 Inter-frequency RSRQ accuracy requirements under CCA 495

10.1.30.1 Inter-frequency SS-RSRQ accuracy requirements in FR1 495

10.1.30.1.1 Aboslute Accuracy of SS-RSRQ 495

10.1.30.1.2 Relative Accuracy of SS-RSRQ 495

10.1.31 Intra-frequency SINR accuracy requirements under CCA 496

10.1.32 Inter-frequency SINR accuracy requirements under CCA 497

10.1.33 L1-RSRP accuracy requirements under CCA 498

10.1.34 RSSI measurements under CCA 499

10.1.34.1 Intra-frequency absolute RSSI measurement accuracy requirements in FR1 499

10.1.34.2 Inter-frequency absolute RSSI measurement accuracy requirements in FR1 500

10.1.34.3 RSSI measurement report mapping 500

10.1.35 Channel occupancy measurements under CCA 500

10.1.35.1 Intra-frequency channel occupancy measurement accuracy requirements in FR1 500

10.1.35.2 Inter-frequency channel occupancy measurement accuracy requirements in FR1 501

10.1.36 Intra-frequency RSRP accuracy requirements under CCA 501

10.1.36.1 Intra-frequency SS-RSRP accuracy requirements in FR1 501

10.1.36.1.1 Absolute SS-RSRP Accuracy 501

10.1.36.1.2 Relative SS-RSRP Accuracy 502

10.1.37 Inter-frequency RSRP accuracy requirements under CCA 502

10.1.37.1 Inter-frequency SS-RSRP accuracy requirements in FR1 502

10.1.37.1.1 Absolute Accuracy of SS-RSRP 502

10.1.37.1.2 Relative Accuracy of SS-RSRP 503

10.2 E-UTRAN measurements 503

10.2.1 Introduction 503

10.2.2 E-UTRAN RSRP measurements 504

10.2.3 E-UTRAN RSRQ measurements 504

10.2.4 E-UTRAN RSTD measurements 504

10.2.5 E-UTRAN RS-SINR measurements 505

10.2.6 E-UTRAN RSRP measurements for CA/DC Idle Mode Measurements 505

10.2.7 E-UTRAN RSRQ measurements for CA/DC Idle Mode Measurements 505

10.3 UTRAN FDD Measurements 505

10.3.1 UTRAN FDD CPICH RSCP 506

10.3.2 UTRAN FDD CPICH Ec/No 506

10.4 V2X measurements 507

10.4.1 Introduction 507

10.4.2 Intra-frequency PSBCH-RSRP accuracy requirements for FR1 507

10.4.2.1 PSBCH-RSRP Absolute Accuracy 507

10.4.2.2 PSBCH-RSRP Relative Accuracy 507

10.4.3 Intra-Frequency SL-RSSI Measurement Accuracy Requirements for FR1 508

10.4.3.1 Absolute SL-RSSI Accuracy 508

10.4.4 Intra-Frequency L1 SL-RSRP Measurement Accuracy Requirements for FR1 509

10.4.4.1 Absolute L1 SL-RSRP Accuracy 509

11 Void 510

12 V2X Requirements 510

12.1 Introduction 510

12.2 UE Transmit Timing 510

12.2.1 Introduction 510

12.2.2 GNSS as synchronization reference source 510

12.2.3 NR Cell as synchronization reference source 511

12.2.4 E-URTAN Cell as synchronization reference source 511

12.2.5 SyncRef UE as synchronization reference source 511

12.3 Initiation/Cease of SLSS Transmissions 512

12.3.1 Introduction 512

12.3.1.1 Initiation/Cease of SLSS transmissions with NR cell as synchronization reference source 512

12.3.1.2 Initiation/Cease of SLSS transmissions with EUTRAN cell as synchronization reference source 513

12.3.1.3 Initiation/Cease of SLSS transmissions with GNSS as synchronization reference source 514

12.3.1.4 Initiation/Cease of SLSS transmissions with SyncRef UE as synchronization reference source 514

12.4 Selection / Reselection of V2X Synchronization Reference Source 514

12.5 L1 SL-RSRP measurements 515

12.5.1 Introduction 515

12.5.2 SL-RSRP measurements 515

12.6 Congestion Control measurements 516

12.7 Interruption 516

12.7.1 Interruptions to WAN due to V2X Sidelink Communication 516

12.7.2 V2X Sidelink Communication Dropping due to synchronization source change 516

12.7.3 Interruptions to WAN due to switching between E-UTRA V2X Sidelink and NR V2X Sidelink 518

12.8 Reliability of GNSS signal 518

12.9 Scheduling availability 519

12.9.1 Scheduling availability of UE switching between E-UTRA sidelink and NR sidelink 519

13 Measurement Performance Requirements for NR gNB 519

13.1 UL-RTOA 519

13.1.1 Report mapping 519

13.2 gNB Rx-Tx time difference 521

13.2.1 Report mapping 521

13.2.2 Measurement Accuracy Requirements 523

13.2.2.1 Introduction 523

13.2.2.2 Requirements 524

13.3 UL SRS RSRP measurement 525

13.3.1 Report mapping 525

13.3.2 Measurement accuracy requirements 525

13.3.2.1 Introduction 525

13.3.2.2 Requirements 526

13.4 AoA/ZoA 527

13.4.1 Report mapping 527

Annex A (normative): Test Cases 423

A.1 Purpose of annex 423

A.2 Requirement classification for statistical testing 423

A.2.1 Types of requirements in TS 38.133 423

A.2.1.1 Time and delay requirements on UE higher layer actions 423

A.2.1.2 Measurements of power levels, relative powers and time 423

A.2.1.3 Implementation requirements 424

A.2.1.4 Physical layer timing requirements 424

A.2.1.5 Requirements under CCA 424

A.3 RRM test configurations 425

A.3.1 Reference measurement channels 425

A.3.1.1 PDSCH 425

A.3.1.1.1 FDD 425

A.3.1.1.2 TDD 426

A.3.1A Reference measurement channels under CCA 429

A.3.1A.1 PDSCH 429

A.3.1A.1.1 TDD 429

A.3.1A.2 CORESET for RMSI scheduling 430

A.3.1A.2.1 TDD 430

A.3.1A.3 CORESET for RMC scheduling 431

A.3.1A.3.1 TDD 431

A.3.1A.4 TDD UL/DL configuration 432

A.3.1A.5 RMC burst transmission model 432

A.3.1.2 CORESET for RMSI scheduling 433

A.3.1.2.1 FDD 433

A.3.1.2.2 TDD 434

A.3.1.3 CORESET for RMC scheduling 437

A.3.1.3.1 FDD 437

A.3.1.3.2 TDD 438

A.3.1.4 TDD UL/DL configuration 441

A.3.2 OFDMA channel noise generator (OCNG) 442

A.3.2.1 Generic OFDMA Channel Noise Generator (OCNG) 442

A.3.2.1.1 OCNG pattern 1: Generic OCNG pattern for all unused REs 442

A.3.2.1.2 OCNG pattern 2: Generic OCNG pattern for all unused REs for 2AoA setup 443

A.3.2.1.3 OCNG pattern 3: Generic OCNG pattern for unused REs in the same bandwidth as CORESET 443

A.3.2.1.4 OCNG pattern 4: Generic OCNG pattern for all unused REs outside SSB slot(s) 444

A.3.2.2 Void 445

A.3.3 Reference DRX configurations 445

A.3.3.1 DRX Configuration 1: DRX cycle = 40 ms and TAT = 500 ms 445

A.3.3.2 DRX Configuration 2: DRX cycle = 640 ms and TAT = 500 ms 445

A.3.3.3 DRX Configuration 3: DRX cycle = 40 ms and TAT = Infinity 445

A.3.3.4 DRX Configuration 4: DRX cycle = 160 ms and TAT = Infinity 446

A.3.3.5 DRX Configuration 5: DRX cycle = 320 ms and TAT = Infinity 446

A.3.3.6 DRX Configuration 6: DRX cycle = 320 ms and TAT = 500 ms 446

A.3.3.7 DRX Configuration 7: DRX cycle = 640 ms and TAT = Infinity 447

A.3.3.8 DRX Configuration 8: DRX cycle = 320 ms and TAT = Infinity 447

A.3.3.9 DRX Configuration 9: DRX cycle = 40 ms and TAT = 500 ms 447

A.3.3.10 DRX Configuration 10: DRX cycle = 640 ms and TAT = 500 ms 448

A.3.3.11 DRX Configuration 11: DRX cycle = 20 ms and TAT = Infinity 448

A.3.3.12 DRX Configuration 12: DRX cycle = 640 ms and TAT = Infinity 448

A.3.4 Test Cases with Different Channel Bandwidths 448

A.3.4.1 Test Cases with Different E-UTRA Channel Bandwidths 448

A.3.4.1.1 Introduction 448

A.3.4.1.2 Principle of testing 449

A.3.5 Test Cases for Synchronous and Asynchronous DC Operations 449

A.3.5.1 EN-DC Test Cases for Synchronous and Asynchronous EN-DC Operations 449

A.3.5.1.1 Introduction 449

A.3.5.1.2 Principle of Testing 449

A.3.6 Antenna configurations 449

A.3.6.1 Antenna configurations for FR1 449

A.3.6.1.1 Antenna connection for 4 Rx capable UEs 449

A.3.6.1.1.1 Introduction 449

A.3.6.1.1.2 Principle of testing 449

A.3.6.2 Antenna configurations for FR2 452

A.3.6A Antenna configurations with unlicensed bands 452

A.3.6A.1 Antenna configurations for FR1 452

A.3.6A.1.1 Antenna connection for 4 Rx capable UEs 452

A.3.6A.1.1.1 Introduction 452

A.3.6A.1.1.2 Principle of testing 452

A.3.7 EN-DC test setup 454

A.3.7.1 Introduction 454

A.3.7.2 E-UTRAN Serving Cell Parameters 454

A.3.7.2.1 E-UTRAN Serving Cell Parameters for Tests with NR Cell(s) in FR1 454

A.3.7.2.2 E-UTRAN Serving Cell Parameters for Tests with NR Cell(s) in FR2 455

A.3.7A NR FR1-FR2 test setup 456

A.3.7B EN-DC test setup with unlicensed bands 457

A.3.7B.1 Introduction 457

A.3.7B.2 E-UTRAN Serving Cell Parameters 457

A.3.7B.2.1 E-UTRAN Serving Cell Parameters for Tests with NR Cell(s) under CCA in FR1 457

A.3.7C LTE-FR1/FR2 test setup 458

A.3.7D NE-DC test setup 458

A.3.7D.1 Introduction 458

A.3.7D.2 E-UTRAN Serving Cell Parameters 458

A.3.7D.2.1 E-UTRAN Serving Cell Parameters for Tests with NR Cell(s) in FR1 458

A.3.7D.2.2 E-UTRAN Serving Cell Parameters for Tests with NR Cell(s) in FR2 458

A.3.8 PRACH configurations 458

A.3.8.1 Introduction 458

A.3.8.2 PRACH configurations in FR1 459

A.3.8.2.1 FR1 PRACH configuration 1 459

A.3.8.2.2 FR1 PRACH configuration 2 459

A.3.8.2.3 FR1 PRACH configuration 3 460

A.3.8.2.4 FR1 PRACH configuration 4 461

A.3.8.3 PRACH configurations in FR2 462

A.3.8.3.1 FR2 PRACH configuration 1 462

A.3.8.3.2 FR2 PRACH configuration 2 463

A.3.8.3.3 FR2 PRACH configuration 3 464

A.3.8.3.4 FR2 PRACH configuration 4 465

A.3.8A PRACH configurations under CCA 466

A.3.8A.1 Introduction 466

A.3.8A.2 PRACH configurations in FR1 466

A.3.8A.2.1 FR1 PRACH configuration 1 under CCA 466

A.3.8A.2.2 FR1 PRACH configuration 2 under CCA 467

A.3.9 BWP configurations 468

A.3.9.1 Introduction 468

A.3.9.2 Downlink BWP configurations 469

A.3.9.2.1 Initial BWP 469

A.3.9.2.2 Dedicated BWP 469

A.3.9.3 Uplink BWP configurations 469

A.3.9.3.1 Initial BWP 469

A.3.9.3.2 Dedicated BWP 470

A.3.10 SSB Configurations 470

A.3.10.1 SSB Configurations for FR1 470

A.3.10.1.1 SSB pattern 1 in FR1: SSB allocation for SSB SCS=15 kHz in 10 MHz 470

A.3.10.1.5 SSB pattern 5 in FR1: SSB allocation for SSB SCS=15 kHz starting from odd SFN in 10 MHz 472

A.3.10A SSB Configurations under CCA 477

A.3.10A.1 SSB Configurations under CCA for FR1 477

A.3.10A.1.1 SSB pattern 1 under CCA for semi-static channel access: SSB allocation for SSB SCS=30kHz in 40MHz 477

A.3.10A.1.2 SSB pattern 2 under CCA for dynamic channel access: SSB allocation for SSB SCS=30kHz in 40MHz 478

A.3.10A.1.3 SSB pattern 3 under CCA for semi-static channel access: SSB allocation for SSB SCS=30 kHz in 40 MHz 478

A.3.10A.1.4 SSB pattern 4 under CCA for dynamic channel access: SSB allocation for SSB SCS=30 kHz in 40 MHz 479

A.3.11 SMTC Configurations 479

A.3.11.1 SMTC pattern 1: SMTC period = 20 ms with SMTC duration = 1 ms 479

A.3.11.2 SMTC pattern 2: SMTC period = 20 ms with SMTC duration = 5 ms 479

A.3.11.3 SMTC pattern 3: SMTC period = 160 ms with SMTC duration = 1 ms 480

A.3.11.4 SMTC pattern 4: SMTC period = 20 ms with SMTC duration = 1 ms 480

A.3.11.5 SMTC pattern 5: SMTC period = 20 ms with SMTC duration = 5 ms 480

A.3.11.6 SMTC pattern 6: SMTC period = 20 ms with SMTC duration = 5 ms 480

A.3.12 Test Cases with Different CC Configurations 480

A.3.12.1 EN-DC Test Cases with Different EN-DC Configurations 480

A.3.12.1.1 Introduction 480

A.3.12.1.2 Principle of testing 481

A.3.12.2 Carrier Aggregation Test Cases with Different CA Configurations 481

A.3.12.2.1 Introduction 481

A.3.12.2.2 Principle of testing 481

A.3.13 Test Cases in SA and EN-DC Operations 481

A.3.13.1 Introduction 481

A.3.13.2 Principle of Testing 481

A.3.13A Test Cases involving E-UTRA/FR1 and FR2 carriers 482

A.3.13A.1 Introduction 482

A.3.13A.2 Principle of Testing in EN-DC 482

A.3.13A.3 Principle of Testing in SA 482

A.3.13B Test Cases for EN-DC and NE-DC Operations 483

A.3.13B.1 Active BWP switch Test Cases for EN-DC and NE-DC Operations 483

A.3.13B.1.1 Introduction 483

A.3.13B.1.2 Principle of Testing 483

A.3.13B.2 SFTD accuracy Test Cases for EN-DC and NE-DC Operations 483

A.3.13B.2.1 Introduction 483

A.3.13B.2.2 Principle of Testing 483

A.3.14 CSI-RS configurations 484

A.3.14.1 FDD 484

A.3.14.2 TDD 486

A.3.15 Angle of Arrival (AoA) for FR2 RRM test cases 491

A.3.15.1 Setup 1: Single AoA in Rx beam peak direction 491

A.3.15.2 Setup 2: Single AoA in non Rx beam peak direction 491

A.3.15.2.1 Setup 2a: Single AoA in non Rx beam peak direction without change in direction 491

A.3.15.2.2 Setup 2b: Single AoA in non Rx beam peak direction with change in direction 492

A.3.15.3 Setup 3: 2 AoAs 492

A.3.15.4 Setup 4: 2 AoAs, 1 AoA in Rx beam peak direction, 1 in non Rx beam peak 492

A.3.15.4.1 Setup 4a: 2 AoAs, 1 AoA in Rx beam peak direction, 1 in non Rx beam peak without change in direction 492

A.3.15.4.2 Setup 4b: 2 AoAs, 1 AoA in Rx beam peak direction, 1 in non Rx beam peak with change in direction 492

A.3.16 TCI State Configuration 493

A.3.16.1 Introduction 493

A.3.16.2 TCI states 493

A.3.17 Configurations of CSI-RS for tracking 493

A.3.17.1 Configuration of CSI-RS for tracking for FR1 493

A.3.17.1.1 FDD 493

A.3.17.1.2 TDD 494

A.3.17.2 Configuration of CSI-RS for tracking for FR2 495

A.3.17.2.1 TDD 495

A.3.18 Additional definitions related to OTA testing for FR2 RRM test cases 496

A.3.18.1 Introduction 496

A.3.18.2 PRACH Power Measurement 496

A.3.19 Test applicability for DAPS handover 496

A.3.19.1 Introduction 496

A.3.19.2 Principle of testing 496

A.3.20 MsgA configurations 497

A.3.20.1 Introduction 497

A.3.20.2 MsgA configurations in FR1 497

A.3.20.2.1 FR1 MsgA configuration 1 497

A.3.20.2.2 FR1 MsgA configuration 2 498

A.3.20.3 MsgA configurations in FR2 500

A.3.20.3.1 FR2 MsgA configuration 1 500

A.3.20.3.2 FR2 MsgA configuration 2 501

A.3.20A MsgA configurations under CCA 503

A.3.20A.1 Introduction 503

A.3.20A.2 MsgA configurations in FR1 503

A.3.20A.2.1 FR1 MsgA configuration 1 under CCA 503

A.3.20A.2.2 FR1 MsgA configuration 2 under CCA 504

A.3.21 V2X sidelink communication 507

A.3.21.1 Introduction 507

A.3.21.2 Reference resource pool configurations for V2X Sidelink Communication 507

A.3.21.3 Reference measurement channels for V2X Sidelink Communication 511

A.3.22 CSI-IM configurations 511

A.3.22.1 FDD 511

A.3.22.2 TDD 512

A.3.23 Spatial Relation Configuration 514

A.3.23.1 Introduction 514

A.3.23.2 Spatial Relation 514

A.3.24 SRS configuration 515

A.3.25 Channel bandwidth (CBW) configurations 517

A.3.25.1 DL UE specific CBW 518

A.3.26 CCA model 518

A.3.26.1 Introduction 518

A.3.26.2 CCA model for operation on a carrier frequency with CCA in FR1 518

A.3.26.2.1 DL CCA model 518

A.3.26.2.2 UL CCA model 520

A.3.27 Test Cases with at Least One Cell on a Carrier Frequency with CCA 520

A.3.27.1 Introduction 521

A.3.27.2 NR Standalone Tests with NR SCell under CCA and All Other NR Cells in FR1 521

A.3.27.3 EN-DC Tests with NR PSCell under CCA and Other NR Cells in FR1 521

A.3.27.4 NR Standalone Tests with NR PCell under CCA and Other NR Cells in FR1 521

A.3.27.5 E-UTRA Standalone Tests with at Least One NR Cell under CCA 521

A.3.28 Discovery Burst Transmission Window configuration under CCA 521

A.3.28.1 DBT Window pattern 1: DBT Window period = 20 ms with DBT Window duration = 1 ms 521

A.3.29 Testing principles for UE capable of only NR bands with shared spectrum access 521

A.3.29.1 Introduction 521

A.3.29.2 Principle of testing for UE capable of EN-DC with only NR bands with shared spectrum access 522

A.3.29.3 Principle of testing for UE capable of SA operation with only NR bands with shared spectrum access 522

A.3.30 CSI-RS configurations for RRM 523

A.3.30.1 FDD 523

A.3.30.2 TDD 524

A.3.31 PRS Configurations 526

A.3.31.1. PRS Configurations for FR1 526

A.3.31.1.1. PRS pattern 1 in FR1: SCS=15 KHz 526

A.3.31.1.2. PRS pattern 2 in FR1: SCS=30 KHz 527

A.3.31.2. PRS Configurations for FR2 527

A.3.31.2.1. PRS pattern 1 in FR2: SCS=120 KHz 527

A.4 EN-DC tests with all NR cells in FR1 528

A.4.1 Void 528

A.4.2 Void 528

A.4.3 RRC\_CONNECTED state mobility 528

A.4.3.1 Void 528

A.4.3.2 RRC Connection Mobility Control 528

A.4.3.2.1 Void 528

A.4.3.2.2 Random Access 528

A.4.3.2.2.1 4-step RA type contention based random access test in FR1 for PSCell in EN-DC 528

A.4.3.2.2.2 4-step RA type non-contention based random access test in FR1 for PSCell in EN-DC 532

A.4.3.2.2.3 2-step RA type contention based random access test in FR1 for PSCell in EN-DC 536

A.4.3.2.2.4 2-step RA type non-contention based random access test in FR1 for PSCell in EN-DC 540

A.4.3.2.3 Void 544

A.4.4 Timing 544

A.4.4.1 UE transmit timing 544

A.4.4.1.1 NR UE Transmit Timing Test for FR1 544

A.4.4.1.1.1 Test Purpose and environment 544

A.4.4.1.1.2 Test requirements 548

A.4.4.2 UE timer accuracy 548

A.4.4.3 Timing advance 548

A.4.4.3.1 EN-DC FR1 timing advance adjustment accuracy 548

A.4.4.3.1.1 Test Purpose and Environment 548

A.4.4.3.1.2 Test Parameters 548

A.4.4.3.1.3 Test Requirements 552

A.4.5 Signaling characteristics 552

A.4.5.1 Radio link Monitoring 552

A.4.5.1.1 Radio Link Monitoring Out-of-sync Test for FR1 PSCell configured with SSB-based RLM RS in non-DRX mode 553

A.4.5.1.1.1 Test Purpose and Environment 553

A.4.5.1.1.2 Test Requirements 557

A.4.5.1.2 Radio Link Monitoring In-sync Test for FR1 PSCell configured with SSB-based RLM RS in non-DRX mode 557

A.4.5.1.2.1 Test Purpose and Environment 557

A.4.5.1.2.2 Test Requirements 563

A.4.5.1.3 Radio Link Monitoring Out-of-sync Test for FR1 PSCell configured with SSB-based RLM RS in DRX mode 563

A.4.5.1.3.1 Test Purpose and Environment 563

A.4.5.1.3.2 Test Requirements 569

A.4.5.1.4 Radio Link Monitoring In-sync Test for FR1 PSCell configured with SSB-based RLM RS in DRX mode 569

A.4.5.1.4.1 Test Purpose and Environment 569

A.4.5.1.4.2 Test Requirements 574

A.4.5.1.5 EN-DC Radio Link Monitoring Out-of-sync Test for FR1 PSCell configured with CSI-RS-based RLM in non-DRX mode 574

A.4.5.1.5.1 Test Purpose and Environment 574

A.4.5.1.5.2 Test Requirements 580

A.4.5.1.6 EN-DC Radio Link Monitoring In-sync Test for FR1 PSCell configured with CSI-RS-based RLM in non-DRX mode 580

A.4.5.1.6.1 Test Purpose and Environment 580

A.4.5.1.6.2 Test Requirements 586

A.4.5.1.7 EN-DC Radio Link Monitoring Out-of-sync Test for FR1 PSCell configured with CSI-RS-based RLM in DRX mode 586

A.4.5.1.7.1 Test Purpose and Environment 586

A.4.5.1.7.2 Test Requirements 591

A.4.5.1.8 EN-DC Radio Link Monitoring In-sync Test for FR1 PSCell configured with CSI-RS-based RLM in DRX mode 592

A.4.5.1.8.1 Test Purpose and Environment 592

A.4.5.1.8.2 Test Requirements 597

A.4.5.2 Interruption 597

A.4.5.2.1 E-UTRAN – NR FR1 interruptions at transitions between active and non-active during DRX in synchronous EN-DC 597

A.4.5.2.1.1 Test Purpose and Environment 597

A.4.5.2.1.2 Test Requirements 601

A.4.5.2.2 E-UTRAN – NR FR1 interruptions at transitions between active and non-active during DRX in asynchronous EN-DC 601

A.4.5.2.2.1 Test Purpose and Environment 601

A.4.5.2.2.2 Test Requirements 605

A.4.5.2.3 E-UTRAN – NR FR1 interruptions during measurements on deactivated NR SCC in synchronous EN-DC 605

A.4.5.2.3.1 Test Purpose and Environment 605

A.4.5.2.3.2 Test Requirements 610

A.4.5.2.4 E-UTRAN – NR FR1 interruptions during measurements on deactivated NR SCC in asynchronous EN-DC 611

A.4.5.2.4.1 Test Purpose and Environment 611

A.4.5.2.4.2 Test Requirements 615

A.4.5.2.5 E-UTRAN – NR FR1 interruptions during measurements on deactivated E-UTRAN SCC in synchronous EN-DC 616

A.4.5.2.5.1 Test Purpose and Environment 616

A.4.5.2.5.2 Test Requirements 620

A.4.5.2.6 E-UTRAN – NR FR1 interruptions during measurements on deactivated E-UTRAN SCC in asynchronous EN-DC 620

A.4.5.2.6.1 Test Purpose and Environment 620

A.4.5.2.6.2 Test Requirements 624

A.4.5.2.7 Void 624

A.4.5.2.8 E-UTRAN - NR FR1 interruptions at NR SRS carrier based switching in asynchronous EN-DC 624

A.4.5.2.8.1 Test Purpose and Environment 624

A.4.5.2.8.2 Test Requirements 627

A.4.5.2.9 E-UTRAN – NR interruptions at E-UTRA SRS carrier based switching 628

A.4.5.2.9.1 Test Purpose and Environment 628

A.4.5.2.9.2 Test Requirements 632

A.4.5.3 SCell Activation and Deactivation Delay 633

A.4.5.3.1 SCell Activation and deactivation of known SCell in FR1 for 160ms SCell measurement cycle 633

A.4.5.3.1.1 Test Purpose and Environment 633

A.4.5.3.1.2 Test Requirements 639

A.4.5.3.2 SCell Activation and deactivation of known SCell in FR1 for 640ms SCell measurement cycle 640

A.4.5.3.2.1 Test Purpose and Environment 640

A.4.5.3.2.2 Test Requirements 640

A.4.5.3.3 SCell Activation and deactivation of unknown SCell in FR1 640

A.4.5.3.3.1 Test Purpose and Environment 640

A.4.5.3.3.2 Test Requirements 641

A.4.5.3.4 SCell Activation and deactivation of multiple unknown SCells in FR1 with single activation/deactivation command 642

A.4.5.3.4.1 Test Purpose and Environment 642

A.4.5.3.4.2 Test Requirements 646

A.4.5.3.5 Direct SCell activation at SCell addition of known SCell in FR1 646

A.4.5.3.5.1 Test Purpose and Environment 646

A.4.5.3.5.2 Test Requirements 654

A.4.5.4 UE UL carrier RRC reconfiguration Delay 655

A.4.5.4.1 UE UL carrier RRC reconfiguration Delay 655

A.4.5.4.1.1 Test Purpose and Environment 655

A.4.5.4.1.2 Test Requirements 663

A.4.5.5 Beam Failure Detection and Link recovery procedures 664

A.4.5.5.1 EN-DC Beam Failure Detection and Link Recovery Test for FR1 PSCell configured with SSB-based BFD and LR in non-DRX mode 664

A.4.5.5.1.1 Test Purpose and Environment 664

A.4.5.5.1.2 Test Requirements 669

A.4.5.5.2 EN-DC Beam Failure Detection and Link Recovery Test for FR1 PSCell configured with SSB-based BFD and LR in DRX mode 670

A.4.5.5.2.1 Test Purpose and Environment 670

A.4.5.5.2.2 Test Requirements 675

A.4.5.5.3 EN-DC Beam Failure Detection and Link Recovery Test for FR1 PSCell configured with CSI-RS-based BFD and LR in non-DRX mode 676

A.4.5.5.3.1 Test Purpose and Environment 676

A.4.5.5.3.2 Test Requirements 681

A.4.5.5.4 EN-DC Beam Failure Detection and Link Recovery Test for FR1 PSCell configured with CSI-RS-based BFD and LR in DRX mode 682

A.4.5.5.4.1 Test Purpose and Environment 682

A.4.5.5.4.2 Test Requirements 687

A.4.5.5.5 EN-DC Beam Failure Detection and Link Recovery Test for FR1 SCell configured with CSI-RS-based BFD and SSB-based LR in non-DRX mode 688

A.4.5.5.5.1 Test Purpose and Environment 688

A.4.5.5.5.2 Test Requirements 693

A.4.5.5.6 EN-DC Beam Failure Detection and Link Recovery Test for FR1 SCell configured with CSI-RS-based BFD and SSB-based LR in DRX mode 694

A.4.5.5.6.1 Test Purpose and Environment 694

A.4.5.5.6.2 Test Requirements 700

A.4.5.6 Active BWP switch 701

A.4.5.6.1 DCI-based and Timer-based Active BWP Switch 701

A.4.5.6.1.1 E-UTRAN – NR PSCell FR1 DL active BWP switch in non-DRX in synchronous EN-DC 701

A.4.5.6.1.2 E-UTRAN – NR PSCell FR1 DL active BWP switch with FR1 SCell in non-DRX in synchronous EN-DC 706

A.4.5.6.2 RRC-based Active BWP Switch 712

A.4.5.6.3 Simultaneous DCI-based and Timer-based Active BWP Switch on multiple CCs 716

A.4.5.6.3.1 Simultaneous E-UTRAN – NR PSCell FR1 DL active BWP switch in non-DRX in EN-DC on multiple CCs 716

A.4.5.6.3.1.2 Test Requirements 722

A.4.5.6.4 SCell dormancy switch 722

A.4.5.6.4.1 E-UTRAN – NR FR1 PSCell SCell dormancy switch of single FR1 SCell outside active time 722

A.4.5.6.4.1.1 Test Purpose and Environment 722

A.4.5.6.4.1.2 Test Requirements 730

A.4.5.6.4.2 E-UTRAN – NR FR1 PSCell SCell dormancy switch of two FR1 SCells inside active time 730

A.4.5.6.4.2.1 Test Purpose and Environment 730

A.4.5.6.4.2.2 Test Requirements 742

A.4.5.6.5 Simultaneous RRC-based Active BWP Switch on multiple CCs 743

A.4.5.6.5.1 E-UTRAN – NR PSCell FR1 DL active BWP switch in non-DRX in synchronous EN-DC on multiple CCs 743

A.4.5.7 PSCell addition and release delay 747

A.4.5.7.1 Addition and Release Delay of known NR PSCell 747

A.4.5.7.1.1 Test purpose and environment 747

A.4.5.7.1.2 Test Requirements 751

A.4.5.8 DL Interruptions at switching between two uplink carriers 752

A.4.5.8.1 Test Purpose and Environment 752

A.4.5.8.2 Test Requirements 755

A.4.5.9 UE specific CBW change 756

A.4.5.9.1 UE specific CBW change on FR1 NR PSCell with non-DRX in synchronous EN- DC 756

A.4.5.9.1.1 Test Purpose and Environment 756

A.4.5.9.1.2 Test Requirements 760

A.4.6 Measurement procedure 760

A.4.6.1 Intra-frequency Measurements 760

A.4.6.1.1 EN-DC event triggered reporting tests without gap under non-DRX 760

A.4.6.1.1.1 Test purpose and Environment 760

A.4.6.1.1.2 Test parameters 760

A.4.6.1.1.3 Test Requirements 764

A.4.6.1.2 EN-DC event triggered reporting tests without gap under DRX 764

A.4.6.1.2.1 Test purpose and Environment 764

A.4.6.1.2.2 Test parameters 764

A.4.6.1.2.2 Test Requirements 768

A.4.6.1.3 EN-DC event triggered reporting tests with per-UE gaps under non-DRX 768

A.4.6.1.3.1 Test purpose and Environment 768

A.4.6.1.3.2 Test parameters 768

A.4.6.1.3.3 Test Requirements 772

A.4.6.1.4 EN-DC event triggered reporting tests with per-UE gaps under DRX 772

A.4.6.1.4.1 Test purpose and Environment 772

A.4.6.1.4.2 Test parameters 772

A.4.6.1.4.3 Test Requirements 776

A.4.6.1.5 EN-DC event triggered reporting tests without gap under non-DRX with SSB index reading 776

A.4.6.1.5.1 Test purpose and Environment 776

A.4.6.1.5.2 Test parameters 776

A.4.6.1.5.3 Test Requirements 778

A.4.6.1.6 EN-DC event triggered reporting tests with SSB index reading with per-UE gaps 779

A.4.6.1.6.1 Test purpose and Environment 779

A.4.6.1.6.2 Test parameters 779

A.4.6.1.6.3 Test Requirements 781

A.4.6.1.7 EN-DC event triggered reporting tests under DRX for UE configured with highSpeedMeasFlag-r16 782

A.4.6.1.7.1 Test purpose and Environment 782

A.4.6.1.7.2 Test parameters 782

A.4.6.1.7.3 Test Requirements 786

A.4.6.2 Inter-frequency Measurements 786

A.4.6.2.1 EN-DC event triggered reporting tests for FR1 cell without SSB time index detection when DRX is not used 786

A.4.6.2.1.1 Test Purpose and Environment 786

A.4.6.2.1.2 Test Requirements 790

A.4.6.2.2 EN-DC event triggered reporting tests for FR1 cell without SSB time index detection when DRX is used 790

A.4.6.2.2.1 Test Purpose and Environment 790

A.4.6.2.2.2 Test Requirements 794

A.4.6.2.3 Void 794

A.4.6.2.4 Void 794

A.4.6.2.5 EN-DC event triggered reporting tests for FR1 cell with SSB time index detection when DRX is not used 794

A.4.6.2.5.1 Test Purpose and Environment 794

A.4.6.2.5.2 Test Requirements 799

A.4.6.2.6 EN-DC event triggered reporting tests for FR1 cell with SSB time index detection when DRX is used 799

A.4.6.2.6.1 Test Purpose and Environment 799

A.4.6.2.6.2 Test Requirements 804

A.4.6.2.7 Void 805

A.4.6.2.8 Void 805

A.4.6.3 Void 805

A.4.6.4 L1-RSRP measurement for beam reporting 805

A.4.6.4.1 SSB based L1-RSRP measurement when DRX is not used 805

A.4.6.4.1.1 Test Purpose and Environment 805

A.4.6.4.1.2 Test parameters 805

A.4.6.4.1.3 Test Requirements 808

A.4.6.4.2 SSB based L1-RSRP measurement when DRX is used 808

A.4.6.4.2.1 Test Purpose and Environment 808

A.4.6.4.2.2 Test parameters 809

A.4.6.4.2.3 Test Requirements 812

A.4.6.4.3 CSI-RS based L1-RSRP measurement when DRX is not used 812

A.4.6.4.3.1 Test Purpose and Environment 812

A.4.6.4.3.2 Test parameters 813

A.4.6.4.3.3 Test Requirements 816

A.4.6.4.4 CSI-RS based L1-RSRP measurement when DRX is used 816

A.4.6.4.4.1 Test Purpose and Environment 816

A.4.6.4.4.2 Test parameters 817

A.4.6.4.4.3 Test Requirements 819

A.4.6.4.5 SSB based L1-RSRP measurement when DRX is used for UE configured with *highSpeedMeasFlag-r16* 819

A.4.6.4.5.1 Test Purpose and Environment 819

A.4.6.4.5.2 Test parameters 820

A.4.6.4.5.3 Test Requirements 823

A.4.6.5 CLI measurements 823

A.4.6.5.1 SRS-RSRP measurement with non-DRX 823

A.4.6.5.1.1 Test Purpose and Environment 823

A.4.6.5.1.2 Test Parameters 824

A.4.6.5.1.3 Test Requirements 827

A.4.6.5.2 CLI-RSSI measurement with non-DRX 827

A.4.6.5.2.1 Test Purpose and Environment 827

A.4.6.5.2.2 Test Parameters 828

A.4.6.5.2.3 Test Requirements 829

A.4.6.6 Measurements with autonomous gaps 830

A.4.6.6.1 EN-DCintra-frequency CGI identification of NR FR1 cell with autonomous gaps in synchronous EN-DC 830

A.4.6.6.1.1 Test Purpose and Environment 830

A.4.6.6.1.2 Test Requirements 834

A.4.6.7 L1-SINR measurement for beam reporting 834

A.4.6.7.1 L1-SINR measurement with CSI-RS based CMR and no dedicated IMR when DRX is not used 834

A.4.6.7.1.1 Test Purpose and Environment 834

A.4.6.7.1.2 Test parameters 835

A.4.6.7.1.3 Test Requirements 838

A.4.6.7.2 L1-SINR measurement with SSB based CMR and dedicated IMR when DRX is used 838

A.4.6.7.2.1 Test Purpose and Environment 838

A.4.6.7.2.2 Test parameters 839

A.4.6.7.2.3 Test Requirements 842

A.4.6.7.3 L1-SINR measurement with CSI-RS based CMR and dedicated IMR configured when DRX is used 842

A.4.6.7.3.1 Test Purpose and Environment 842

A.4.6.7.3.2 Test parameters 843

A.4.6.7.3.3 Test Requirements 846

A.4.6.8 CSI-RS based intra-frequency Measurement 846

A.4.6.8.1 EN-DC event triggered reporting tests without gap under DRX 846

A.4.6.8.1.1 Test purpose and Environment 846

A.4.6.8.1.2 Test Requirements 849

A.4.6.9 CSI-RS based inter-frequency Measurement 850

A.4.6.9.1 EN-DC event triggered reporting tests for FR1 cell when non-DRX is used 850

A.4.6.9.1.1 Test Purpose and Environment 850

A.4.6.9.1.2 Test Requirements 853

A.4.7 Measurement Performance requirements 854

A.4.7.1 SS-RSRP 854

A.4.7.1.1 EN-DC Intra-frequency measurement accuracy with FR1 serving cell and FR1 target cell 854

A.4.7.1.1.1 Test Purpose and Environment 854

A.4.7.1.1.2 Test parameters 854

A.4.7.1.1.3 Test Requirements 858

A.4.7.1.2 EN-DC inter-frequency measurement accuracy with FR1 serving cell and FR1 target cell 858

A.4.7.1.2.1 Test Purpose and Environment 858

A.4.7.1.2.2 Test parameters 859

A.4.7.1.2.3 Test Requirements 863

A.4.7.1.3 Void 863

A.4.7.2 SS-RSRQ 863

A.4.7.2.1 EN-DC Intra-frequency measurement accuracy with FR1 serving cell and FR1 target cell 863

A.4.7.2.1.1 Test Purpose and Environment 863

A.4.7.2.1.2 Test Parameters 864

A.4.7.2.1.3 Test Requirements 869

A.4.7.2.2 EN-DC Inter-frequency measurement accuracy with FR1 serving cell and FR1 target cell 869

A.4.7.2.2.1 Test Purpose and Environment 869

A.4.7.2.2.2 Test Parameters 869

A.4.7.2.2.3 Test Requirements 874

A.4.7.3 SS-SINR 874

A.4.7.3.1 EN-DC Intra-frequency measurement accuracy with FR1 serving cell and FR1 target cell 874

A.4.7.3.1.1 Test Purpose and Environment 874

A.4.7.3.1.2 Test Parameters 874

A.4.7.3.1.3 Test Requirements 878

A.4.7.3.2 EN-DC Inter-frequency measurement accuracy with FR1 serving cell and FR1 target cell 878

A.4.7.3.2.1 Test Purpose and Environment 878

A.4.7.3.2.2 Test Parameters 878

A.4.7.3.2.3 Test Requirements 883

A.4.7.4 L1-RSRP measurement for beam reporting 883

A.4.7.4.1 SSB based L1-RSRP measurement 883

A.4.7.4.1.1 Test Purpose and Environment 883

A.4.7.4.1.2 Test parameters 884

A.4.7.4.1.3 Test Requirements 887

A.4.7.4.2 CSI-RS based L1-RSRP measurement on resource set with repetition off 887

A.4.7.4.2.1 Test Purpose and Environment 887

A.4.7.4.2.2 Test parameters 888

A.4.7.4.2.3 Test Requirements 891

A.4.7.5 SFTD accuracy 891

A.4.7.5.1 SFTD accuracy 891

A.4.7.5.1.1 Test Purpose and Environment 891

A.4.7.5.1.2 Test Parameters 891

A.4.7.5.1.3 Test Requirements 896

A.4.7.5.2 Void 896

A.4.7.5.3 Void 896

A.4.7.6 CLI measurements 896

A.4.7.6.1 EN-DC SRS-RSRP measurement accuracy with FR1 serving cell 896

A.4.7.6.1.1 Test Purpose and Environment 896

A.4.7.6.1.2 Test parameters 897

A.4.7.6.1.3 Test Requirements 902

A.4.7.6.2 EN-DC CLI-RSSI measurement accuracy with FR1 serving cell 902

A.4.7.6.2.1 Test Purpose and Environment 902

A.4.7.6.2.2 Test parameters 903

A.4.7.6.2.3 Test Requirements 906

A.4.7.7 L1-SINR measurement for beam reporting 906

A.4.7.7.1 L1-SINR measurement with CSI-RS based CMR and no dedicated IMR configured and CSI-RS resource set with repetition off 906

A.4.7.7.1.1 Test Purpose and Environment 906

A.4.7.7.1.2 Test parameters 907

A.4.7.7.1.3 Test Requirements 911

A.4.7.7.2 L1-SINR measurement with SSB based CMR and dedicated IMR 911

A.4.7.7.2.1 Test Purpose and Environment 911

A.4.7.7.2.2 Test parameters 912

A.4.7.7.2.3 Test Requirements 916

A.4.7.7.3 L1-SINR measurement with CSI-RS based CMR and dedicated IMR 916

A.4.7.7.3.1 Test Purpose and Environment 916

A.4.7.7.3.2 Test parameters 917

A.4.7.7.3.3 Test Requirements 920

A.4.7.8 CSI-RSRP 920

A.4.7.8.1 EN-DC Intra-frequency measurement accuracy with FR1 serving cell and FR1 target cell 920

A.4.7.8.1.1 Test Purpose and Environment 920

A.4.7.8.1.2 Test parameters 921

A.4.7.8.1.3 Test Requirements 924

A.4.7.8.2 EN-DC inter-frequency measurement accuracy with FR1 serving cell and FR1 target cell 924

A.4.7.8.2.1 Test Purpose and Environment 924

A.4.7.8.2.2 Test parameters 925

A.4.7.8.2.3 Test Requirements 928

A.4.7.9 CSI-RSRQ 929

A.4.7.9.1 EN-DC Intra-frequency measurement accuracy with FR1 serving cell and FR1 target cell 929

A.4.7.9.1.1 Test Purpose and Environment 929

A.4.7.9.1.2 Test Parameters 929

A.4.7.9.1.3 Test Requirements 934

A.4.7.9.2 EN-DC Inter-frequency measurement accuracy with FR1 serving cell and FR1 target cell 934

A.4.7.9.2.1 Test Purpose and Environment 934

A.4.7.9.2.2 Test Parameters 934

A.4.7.2.2.3 Test Requirements 939

A.4.7.10 CSI-SINR 939

A.4.7.10.1 EN-DC Intra-frequency measurement accuracy with FR1 serving cell and FR1 target cell 939

A.4.7.10.1.1 Test Purpose and Environment 939

A.4.7.10.1.2 Test Parameters 940

A.4.7.10.1.3 Test Requirements 943

A.4.7.10.2 EN-DC Inter-frequency measurement accuracy with FR1 serving cell and FR1 target cell 943

A.4.7.10.2.1 Test Purpose and Environment 943

A.4.7.10.2.2 Test Parameters 943

A.4.7.10.2.3 Test Requirements 946

A.4.8 Void 947

A.4A NE-DC test with all NR cells in FR1 947

A.4A.1 Signaling characteristics 947

A.4A.1.1 E-UTRAN PSCell addition 947

A.4A.1.1.1 Test purpose and environment 947

A.4A.1.1.2 Test Requirements 951

A.4A.1.2 Active BWP switch 952

A.4A.1.2.1 E-UTRAN PSCell – NR PCell FR1 DCI-based and Timer-based DL active BWP switch in non-DRX in synchronous NE-DC 952

A.4A.1.2.1.1 Test Purpose and Environment 952

A.4A.1.2.1.2 Test Requirements 956

A.4A.2 Measurement performance 957

A.4A.2.1 SFTD accuracy 957

A.4A.2.1.1 SFTD accuracy 957

A.4A.2.1.1.1 Test Purpose 957

A.4A.2.1.1.2 Test Environment 957

A.4A.2.1.1.3 Test Requirements 960

A.5 EN-DC tests with one or more NR cells in FR2 961

A.5.1 Void 961

A.5.2 Void 961

A.5.3 RRC\_CONNECTED state mobility 961

A.5.3.1 Void 961

A.5.3.2 RRC Connection Mobility Control 961

A.5.3.2.1 Void 961

A.5.3.2.2 Random Access 961

A.5.3.2.2.1 4-step RA type contention based random access test in FR2 for PSCell/SCell in EN-DC 961

A.5.3.2.2.2 4-step RA type non-contention based random access test in FR2 for PSCell/SCell in EN-DC 964

A.5.3.2.2.3 2-step RA type contention based random access test in FR2 for PSCell/SCell in EN-DC 970

A.5.3.2.2.4 2-step RA type non-contention based random access test in FR2 for PSCell/SCell in EN-DC 973

A.5.3.2.3 Void 977

A.5.4 Timing 977

A.5.4.1 UE transmit timing 977

A.5.4.1.1 NR UE Transmit Timing Test for FR2 977

A.5.4.1.1.1 Test Purpose and environment 977

A.5.4.1.1.2 Test requirements 980

A.5.4.2 UE timer accuracy 981

A.5.4.3 Timing advance 981

A.5.4.3.1 EN-DC FR2 timing advance adjustment accuracy 981

A.5.4.3.1.1 Test Purpose and Environment 981

A.5.4.3.1.2 Test Parameters 981

A.5.4.3.1.3 Test Requirements 985

A.5.5 Signaling characteristics 985

A.5.5.1 Radio link Monitoring 985

A.5.5.1.1 Radio Link Monitoring Out-of-sync Test for FR2 PSCell configured with SSB-based RLM RS in non-DRX mode 985

A.5.5.1.1.1 Test Purpose and Environment 985

A.5.5.1.1.2 Test Requirements 989

A.5.5.1.2 Radio Link Monitoring In-sync Test for FR2 PSCell configured with SSB-based RLM RS in non-DRX mode 990

A.5.5.1.2.1 Test Purpose and Environment 990

A.5.5.1.2.2 Test Requirements 993

A.5.5.1.3 Radio Link Monitoring Out-of-sync Test for FR2 PSCell configured with SSB-based RLM RS in DRX mode 994

A.5.5.1.3.1 Test Purpose and Environment 994

A.5.5.1.3.2 Test Requirements 998

A.5.5.1.4 Radio Link Monitoring In-sync Test for FR2 PSCell configured with SSB-based RLM RS in DRX mode 998

A.5.5.1.4.1 Test Purpose and Environment 998

A.5.5.1.4.2 Test Requirements 1002

A.5.5.1.5 EN-DC Radio Link Monitoring Out-of-sync Test for FR2 PSCell configured with CSI-RS-based RLM in non-DRX mode 1002

A.5.5.1.6 EN-DC Radio Link Monitoring In-sync Test for FR2 PSCell configured with CSI-RS-based RLM in non-DRX mode 1006

A.5.5.1.7 EN-DC Radio Link Monitoring Out-of-sync Test for FR2 PSCell configured with CSI-RS-based RLM in DRX mode 1010

A.5.5.1.8 EN-DC Radio Link Monitoring In-sync Test for FR2 PSCell configured with CSI-RS-based RLM in DRX mode 1015

A.5.5.1.8.2 Test Requirements 1019

A.5.5.1.9 EN-DC Radio Link Monitoring UE Scheduling Restrictions on FR2 1020

A.5.5.1.9.1 Test Purpose and Environment 1020

A.5.5.1.9.2 Test Requirements 1022

A.5.5.2 Interruption 1022

A.5.5.2.1 E-UTRAN – NR FR2 interruptions at transitions between active and non-active during DRX in synchronous EN-DC 1022

A.5.5.2.1.1 Test Purpose and Environment 1022

A.5.5.2.1.2 Test Requirements 1025

A.5.5.2.2 E-UTRAN – NR FR2 interruptions at transitions between active and non-active during DRX in asynchronous EN-DC 1025

A.5.5.2.2.1 Test Purpose and Environment 1025

A.5.5.2.2.2 Test Requirements 1028

A.5.5.2.3 E-UTRAN – NR FR2 interruptions during measurements on deactivated NR SCC in synchronous EN-DC 1028

A.5.5.2.3.1 Test Purpose and Environment 1028

A.5.5.2.3.2 Test Requirements 1032

A.5.5.2.4 E-UTRAN – NR FR2 interruptions during measurements on deactivated NR SCC in asynchronous EN-DC 1032

A.5.5.2.4.1 Test Purpose and Environment 1032

A.5.5.2.4.2 Test Requirements 1035

A.5.5.2.5 E-UTRAN – NR FR2 interruptions during measurements on deactivated E-UTRAN SCC in synchronous EN-DC 1036

A.5.5.2.5.1 Test Purpose and Environment 1036

A.5.5.2.5.2 Test Requirements 1039

A.5.5.2.6 E-UTRAN – NR FR2 interruptions during measurements on deactivated E-UTRAN SCC in asynchronous EN-DC 1040

A.5.5.2.6.1 Test Purpose and Environment 1040

A.5.5.2.6.2 Test Requirements 1042

A.5.5.2.7 E-UTRAN – NR FR2 interruptions at E-UTRA SRS carrier based switching 1043

A.5.5.2.7.1 Test Purpose and Environment 1043

A.5.5.2.7.2 Test Requirements 1046

A.5.5.2.8 E-UTRAN – NR FR2 interruptions at NR SRS carrier based switching 1046

A.5.5.2.8.1 Test Purpose and Environment 1046

A.5.5.2.8.3 Test Requirements 1049

A.5.5.3 SCell Activation and Deactivation Delay 1049

A.5.5.3.1 SCell Activation and deactivation of SCell in FR2 intra-band 1049

A.5.5.3.1.1 Test Purpose and Environment 1049

A.5.5.3.1.2 Test Requirements 1052

A.5.5.3.2 SCell Activation and deactivation of known SCell in FR1 for 160ms SCell measurement cycle 1052

A.5.5.3.2.1 Test Purpose and Environment 1052

A.5.5.3.2.2 Test Requirements 1056

A.5.5.3.3 Void 1056

A.5.5.3.4 Void 1056

A.5.5.3.5 SCell Activation and deactivation of SCell in FR2 1056

A.5.5.3.5.1 Test Purpose and Environment 1056

A.5.5.3.5.2 Test Requirements 1060

A.5.5.3.6 Multiple SCell Activation and deactivation of one unknown SCell and one known SCell in FR2 1061

A.5.5.3.6.1 Test Purpose and Environment 1061

A.5.5.3.6.2 Test Requirements 1064

A.5.5.3.7 Direct SCell activation at SCell addition of known SCell in FR2 1065

A.5.5.3.7.1 Test Purpose and Environment 1065

A.5.5.3.7.2 Test Requirements 1068

A.5.5.4 Void 1068

A.5.5.5 Beam Failure Detection and Link recovery procedures 1068

A.5.5.5.1 EN-DC Beam Failure Detection and Link Recovery Test for FR2 PSCell configured with SSB-based BFD and LR in non-DRX mode 1068

A.5.5.5.1.1 Test Purpose and Environment 1068

A.5.5.5.1.2 Test Requirements 1072

A.5.5.5.2 EN-DC Beam Failure Detection and Link Recovery Test for FR2 PSCell configured with SSB-based BFD and LR in DRX mode 1073

A.5.5.5.2.1 Test Purpose and Environment 1073

A.5.5.5.2.2 Test Requirements 1077

A.5.5.5.3 EN-DC Beam Failure Detection and Link Recovery Test for FR2 PSCell configured with CSI-RS-based BFD and LR in non-DRX mode 1078

A.5.5.5.3.1 Test Purpose and Environment 1078

A.5.5.5.3.2 Test Requirements 1082

A.5.5.5.4 EN-DC Beam Failure Detection and Link Recovery Test for FR2 PSCell configured with CSI-RS-based BFD and LR in DRX mode 1083

A.5.5.5.4.1 Test Purpose and Environment 1083

A.5.5.5.4.2 Test Requirements 1087

A.5.5.5.5 EN-DC scheduling availability restriction during Beam Failure Detection and Link Recovery for FR2 PSCell configured with SSB-based BFD and LR in non-DRX mode 1088

A.5.5.5.5.1 Test Purpose and Environment 1088

A.5.5.5.5.2 Test Requirements 1092

A.5.5.5.6 EN-DC Beam Failure Detection and Link Recovery Test for FR2 SCell configured with CSI-RS-based BFD and LR in non-DRX mode 1093

A.5.5.5.6.1 Test Purpose and Environment 1093

A.5.5.5.6.2 Test Requirements 1097

A.5.5.5.7 EN-DC Beam Failure Detection and Link Recovery Test for FR2 SCell configured with CSI-RS-based BFD and LR in DRX mode 1098

A.5.5.5.7.1 Test Purpose and Environment 1098

A.5.5.5.7.2 Test Requirements 1102

A.5.5.6 Active BWP switch 1103

A.5.5.6.1 DCI-based and Timer-based Active BWP Switch 1103

A.5.5.6.1.1 E-UTRAN – NR PSCell FR2 DL active BWP switch with non-DRX in synchronous EN-DC 1103

A.5.5.6.1.1.1 Test Purpose and Environment 1103

A.5.5.6.1.1.2 Test Requirements 1106

A.5.5.6.1.2 E-UTRAN – NR PSCell FR2 with FR2 SCell DL active BWP switch in non-DRX in synchronous EN-DC 1106

A.5.5.6.2 RRC-based Active BWP Switch 1111

A.5.5.6.3 Simultaneous DCI-based and Timer-based Active BWP Switch on multiple CCs 1115

A.5.5.6.3.1 E-UTRAN – NR PSCell FR2 and NR SCell FR2 DL active BWP switch on multiple CCs in synchronous EN-DC 1115

A.5.5.6.3.1.1 Test Purpose and Environment 1115

A.5.5.6.4 SCell dormancy switch 1119

A.5.5.6.4.1 E-UTRAN – NR FR2 PSCell SCell dormancy switch of single FR2 SCell inside active time 1119

A.5.5.6.4.1.1 Test Purpose and Environment 1119

A.5.5.6.4.1.2 Test Requirements 1123

A.5.5.6.4.2 E-UTRAN – NR FR1 PSCell SCell dormancy switch of two FR2 SCells outside active time 1123

A.5.5.6.4.2.1 Test Purpose and Environment 1123

A.5.5.6.4.2.2 Test Requirements 1130

A.5.5.6.5 Simultaneous RRC-based Active BWP Switch on multiple CCs 1130

A.5.5.7 PSCell addition and release delay 1133

A.5.5.7.1 Addition and Release Delay of NR PSCell 1133

A.5.5.7.1.1 Test purpose and environment 1133

A.5.5.7.1.2 Test Requirements 1137

A.5.5.8 Active TCI state switch delay 1138

A.5.5.8.1 MAC-CE based active TCI state switch 1138

A.5.5.8.1.1 E-UTRAN – NR PSCell FR2 active TCI state switch for a known TCI state 1138

A.5.5.8.1.1.1 Test Purpose and Environment 1138

A.5.5.8.1.1.2 Test Requirements 1141

A.5.5.8.2 RRC based active TCI state switch 1141

A.5.5.8.2.1 E-UTRAN – NR PSCell FR2 active TCI state switch for a known TCI state 1141

A.5.5.8.2.1.1 Test Purpose and Environment 1141

A.5.5.8.2.1.2 Test Requirements 1145

A.5.5.9 Uplink spatial relation switch delay 1145

A.5.5.9.1 MAC-CE based uplink spatial relation switch 1145

A.5.5.9.1.1 E-UTRAN – NR PSCell FR2 uplink spatial relation switch for a known spatial relation 1145

A.5.5.9.1.1.1 Test Purpose and Environment 1145

A.5.5.9.1.1.2 Test Requirements 1148

A.5.5.9.2 RRC based spatial relation switch 1148

A.5.5.9.2.1 E-UTRAN – NR PSCell FR2 spatial relation switch associated with a known DL-RS 1148

A.5.5.9.2.1.1 Test Purpose and Environment 1148

A.5.5.9.2.1.2 Test Requirements 1151

A.5.5.10 UE specific CBW change 1151

A.5.5.10.1 UE specific CBW change on FR2 NR PSCell 1151

A.5.5.10.1.1 Test Purpose and Environment 1151

A.5.5.10.1.2 Test Requirements 1154

A.5.6 Measurement procedure 1155

A.5.6.1 Intra-frequency Measurements 1155

A.5.6.1.1 EN-DC event triggered reporting test without gap under non-DRX 1155

A.5.6.1.1.1 Test purpose and Environment 1155

A.5.6.1.1.2 Test Requirements 1158

A.5.6.1.2 EN-DC event triggered reporting test without gap under DRX 1158

A.5.6.1.2.1 Test purpose and Environment 1158

A.5.6.1.2.2 Test Requirements 1160

A.5.6.1.3 EN-DC event triggered reporting test with per-UE gaps under non-DRX 1161

A.5.6.1.3.1 Test purpose and Environment 1161

A.5.6.1.3.2 Test Requirements 1165

A.5.6.1.4 EN-DC event triggered reporting test with per-UE gaps under DRX 1165

A.5.6.1.4.1 Test purpose and Environment 1165

A.5.6.1.4.2 Test Requirements 1168

A.5.6.2 Inter-frequency Measurements 1169

A.5.6.2.1 EN-DC event triggered reporting tests for FR2 cell without SSB time index detection when DRX is not used 1169

A.5.6.2.1.1 Test Purpose and Environment 1169

A.5.6.2.1.2 Test Requirements 1172

A.5.6.2.2 EN-DC event triggered reporting tests for FR2 cell without SSB time index detection when DRX is used 1172

A.5.6.2.2.1 Test Purpose and Environment 1172

A.5.6.2.2.2 Test Requirements 1176

A.5.6.2.3 EN-DC event triggered reporting tests for FR2 cell with SSB time index detection when DRX is not used 1176

A.5.6.2.3.1 Test Purpose and Environment 1176

A.5.6.2.3.2 Test Requirements 1180

A.5.6.2.4 EN-DC event triggered reporting tests for FR2 cell with SSB time index detection when DRX is used 1180

A.5.6.2.4.1 Test Purpose and Environment 1180

A.5.6.2.4.2 Test Requirements 1184

A.5.6.2.5 EN-DC event triggered reporting tests for FR2 cell without SSB time index detection when DRX is not used 1184

A.5.6.2.5.1 Test Purpose and Environment 1184

A.5.6.2.5.2 Test Requirements 1189

A.5.6.2.6 EN-DC event triggered reporting tests for FR2 cell without SSB time index detection when DRX is used 1189

A.5.6.2.6.1 Test Purpose and Environment 1189

A.5.6.2.6.2 Test Requirements 1193

A.5.6.2.7 EN-DC event triggered reporting tests for FR2 cell with SSB time index detection when DRX is not used 1193

A.5.6.2.7.1 Test Purpose and Environment 1193

A.5.6.2.7.2 Test Requirements 1198

A.5.6.2.8 EN-DC event triggered reporting tests for FR2 cell with SSB time index detection when DRX is used 1198

A.5.6.2.8.1 Test Purpose and Environment 1198

A.5.6.2.8.2 Test Requirements 1203

A.5.6.3 L1-RSRP measurement for beam reporting 1203

A.5.6.3.1 SSB based L1-RSRP measurement when DRX is not used 1203

A.5.6.3.1.1 Test Purpose and Environment 1203

A.5.6.3.1.2 Test parameters 1203

A.5.6.3.1.3 Test Requirements 1205

A.5.6.3.2 SSB based L1-RSRP measurement when DRX is used 1205

A.5.6.3.2.1 Test Purpose and Environment 1205

A.5.6.3.2.2 Test parameters 1206

A.5.6.3.2.3 Test Requirements 1208

A.5.6.3.3 CSI-RS based L1-RSRP measurement when DRX is not used 1208

A.5.6.3.3.1 Test Purpose and Environment 1208

A.5.6.3.3.2 Test parameters 1209

A.5.6.3.3.3 Test Requirements 1211

A.5.6.3.4 CSI-RS based L1-RSRP measurement when DRX is used 1212

A.5.6.3.4.1 Test Purpose and Environment 1212

A.5.6.3.4.2 Test parameters 1212

A.5.6.3.4.3 Test Requirements 1214

A.5.6.4 CLI measurements 1215

A.5.6.4.1 SRS-RSRP measurement with DRX 1215

A.5.6.4.1.1 Test Purpose and Environment 1215

A.5.6.4.1.2 Test Parameters 1215

A.5.6.4.1.3 Test Requirements 1217

A.5.6.4.2 CLI-RSSI measurement with DRX 1217

A.5.6.4.2.1 Test Purpose and Environment 1217

A.5.6.4.2.2 Test Parameters 1218

A.5.6.4.2.3 Test Requirements 1220

A.5.6.5 Measurements with autonomous gaps 1220

A.5.6.5.1 EN-DC inter-frequency CGI identification of NR neighbor cell in FR2 1220

A.5.6.5.1.1 Test Purpose and Environment 1220

A.5.6.5.1.2 Test Requirements 1223

A.5.6.6 L1-SINR measurement for beam reporting 1224

A.5.6.6.1 L1-SINR measurement with CSI-RS based CMR and no dedicated IMR configured when DRX is used 1224

A.5.6.6.1.1 Test Purpose and Environment 1224

A.5.6.6.1.2 Test parameters 1224

A.5.6.6.1.3 Test Requirements 1226

A.5.6.6.2 L1-SINR measurement with SSB based CMR and dedicated IMR when DRX is not used 1226

A.5.6.6.2.1 Test Purpose and Environment 1226

A.5.6.6.2.2 Test parameters 1227

A.5.6.6.2.3 Test Requirements 1230

A.5.6.6.3 L1-SINR measurement with CSI-RS based CMR and dedicated IMR configured when DRX is not used 1230

A.5.6.6.3.1 Test Purpose and Environment 1230

A.5.6.6.3.2 Test parameters 1231

A.5.6.6.3.3 Test Requirements 1233

A.5.6.7 CSI-RS based Intra-frequency Measurements 1233

A.5.6.7.1 EN-DC event triggered reporting test without gap under non-DRX 1233

A.5.6.7.1.1 Test purpose and Environment 1233

A.5.6.7.1.2 Test Requirements 1236

A.5.6.8 CSI-RS based Inter-frequency Measurements 1236

A.5.6.8.1 EN-DC event triggered reporting tests for NR FR2 cell when DRX is used 1236

A.5.6.8.1.1 Test Purpose and Environment 1236

A.5.6.8.1.2 Test Requirements 1240

A.5.7 Measurement Performance requirements 1240

A.5.7.1 SS-RSRP 1241

A.5.7.1.1 EN-DC intra-frequency case measurement accuracy with FR2 serving cell and FR2 target cell 1241

A.5.7.1.1.1 Test Purpose and Environment 1241

A.5.7.1.1.2 Test parameters 1241

A.5.7.1.1.3 Test Requirements 1243

A.5.7.1.2 EN-DC inter-frequency case measurement accuracy with FR2 serving cell and FR2 target cell 1244

A.5.7.1.2.1 Test Purpose and Environment 1244

A.5.7.1.2.2 Test parameters 1244

A.5.7.1.2.3 Test Requirements 1249

A.5.7.1.3 EN-DC inter-frequency measurement accuracy with FR1 serving cell and FR2 target cell 1250

A.5.7.1.3.1 Test Purpose and Environment 1250

A.5.7.1.3.2 Test parameters 1250

A.5.7.1.3.3 Test Requirements 1253

A.5.7.2 SS-RSRQ 1254

A.5.7.2.1 EN-DC Intra-frequency measurement accuracy with FR2 serving cell and FR2 TDD target cell 1254

A.5.7.2.1.1 Test Purpose and Environment 1254

A.5.7.2.1.2 Test Parameters 1254

A.5.7.2.1.3 Test Requirements 1256

A.5.7.2.2 EN-DC Inter-frequency measurement accuracy with FR2 serving cell and FR2 TDD target cell 1257

A.5.7.2.2.1 Test Purpose and Environment 1257

A.5.7.2.2.2 Test Parameters 1257

A.5.7.2.2.3 Test Requirements 1259

A.5.7.3 SS-SINR 1259

A.5.7.3.1 EN-DC Intra-frequency measurement accuracy with FR2 serving cell and FR2 TDD target cell 1259

A.5.7.3.1.1 Test Purpose and Environment 1259

A.5.7.3.1.2 Test Parameters 1259

A.5.7.3.1.3 Test Requirements 1261

A.5.7.3.2 EN-DC Inter-frequency measurement accuracy with FR2 serving cell and FR2 TDD target cell 1261

A.5.7.3.2.1 Test Purpose and Environment 1261

A.5.7.3.2.2 Test Parameters 1261

A.5.7.3.2.3 Test Requirements 1263

A.5.7.4 L1-RSRP measurement for beam reporting 1263

A.5.7.4.1 SSB based L1-RSRP measurement 1263

A.5.7.4.1.1 Test Purpose and Environment 1263

A.5.7.4.1.2 Test parameters 1264

A.5.7.4.1.3 Test Requirements 1266

A.5.7.4.2 CSI-RS based L1-RSRP measurement on resource set with repetition off 1267

A.5.7.4.2.1 Test Purpose and Environment 1267

A.5.7.4.2.2 Test parameters 1267

A.5.7.4.2.3 Test Requirements 1269

A.5.7.5 CLI measurements 1270

A.5.7.5.1 EN-DC SRS-RSRP measurement accuracy with FR2 serving cell 1270

A.5.7.5.1.1 Test Purpose and Environment 1270

A.5.7.5.1.2 Test parameters 1270

A.5.7.5.1.3 Test Requirements 1273

A.5.7.5.2 EN-DC CLI-RSSI measurement accuracy with FR2 serving cell 1274

A.5.7.5.2.1 Test Purpose and Environment 1274

A.5.7.5.2.2 Test parameters 1274

A.5.7.5.2.3 Test Requirements 1276

A.5.7.6 L1-SINR measurement for beam reporting 1277

A.5.7.6.1 L1-SINR measurement with CSI-RS based CMR and no dedicated IMR configured and CSI-RS resource set with repetition off 1277

A.5.7.6.1.1 Test Purpose and Environment 1277

A.5.7.6.1.2 Test parameters 1277

A.5.7.6.1.3 Test Requirements 1279

A.5.7.6.2 L1-SINR measurement with SSB based CMR and dedicated IMR 1280

A.5.7.6.2.1 Test Purpose and Environment 1280

A.5.7.6.2.2 Test parameters 1280

A.5.7.6.2.3 Test Requirements 1282

A.5.7.6.3 L1-SINR measurement with CSI-RS based CMR and dedicated IMR 1283

A.5.7.6.3.1 Test Purpose and Environment 1283

A.5.7.6.3.2 Test parameters 1283

A.5.7.6.3.3 Test Requirements 1285

A.5.7.7 CSI-RSRP 1286

A.5.7.7.1 EN-DC intra-frequency case measurement accuracy with FR2 serving cell and FR2 target cell 1286

A.5.7.7.1.2 Test parameters 1286

A.5.7.7.1.3 Test Requirements 1288

A.5.7.7.2 EN-DC inter-frequency case measurement accuracy with FR2 serving cell and FR2 target cell 1289

A.5.7.7.2.1 Test Purpose and Environment 1289

A.5.7.7.2.2 Test parameters 1289

A.5.7.7.2.3 Test Requirements 1293

A.5.7.8 CSI-RSRQ 1294

A.5.7.8.1 EN-DC Intra-frequency measurement accuracy with FR2 serving cell and FR2 target cell 1294

A.5.7.8.1.1 Test Purpose and Environment 1294

A.5.7.8.1.2 Test Parameters 1294

A.5.7.8.1.3 Test Requirements 1296

A.5.7.8.2 EN-DC Inter-frequency measurement accuracy with FR2 serving cell and FR2 TDD target cell 1296

A.5.7.8.2.1 Test Purpose and Environment 1296

A.5.7.8.2.2 Test Parameters 1296

A.5.7.9 CSI-SINR 1298

A.5.7.9.1 EN-DC Intra-frequency measurement accuracy with FR2 serving cell and FR2 TDD target cell 1298

A.5.7.9.1.1 Test Purpose and Environment 1298

A.5.7.9.1.2 Test Parameters 1298

Table A.5.7.9.1.2-1: CSI-SINR Intra frequency CSI-SINR supported test configurations 1299

A.5.7.9.1.3 Test Requirements 1301

A.5.7.9.2 EN-DC Inter-frequency measurement accuracy with FR2 serving cell and FR2 TDD target cell 1301

A.5.7.9.2.1 Test Purpose and Environment 1301

A.5.7.9.2.2 Test Parameters 1301

A.5.7.9.2.3 Test Requirements 1304

A.5.8 Void 1304

A.6 NR standalone tests with all NR cells in FR1 1011

A.6.1 SA: RRC\_IDLE state mobility 1011

A.6.1.1 Cell re-selection to NR 1011

A.6.1.1.1 Cell reselection to FR1 intra-frequency NR case 1011

A.6.1.1.1.1 Test Purpose and Environment 1011

A.6.1.1.1.2 Test Parameters 1011

A.6.1.1.1.3 Test Requirements 1015

A.6.1.1.2 Cell reselection to FR1 inter-frequency NR case 1015

A.6.1.1.2.1 Test Purpose and Environment 1015

A.6.1.1.2.2 Test Parameters 1015

A.6.1.1.2.3 Test Requirements 1019

A.6.1.1.3 Cell reselection to FR1 intra-frequency NR case for UE fulfilling low mobility relaxed measurement criterion 1019

A.6.1.1.3.1 Test Purpose and Environment 1019

A.6.1.1.3.2 Test Parameters 1019

A.6.1.1.3.3 Test Requirements 1024

A.6.1.1.4 Cell reselection to FR1 intra-frequency NR case for UE fulfilling not-at-cell edge relaxed measurement criterion 1024

A.6.1.1.4.1 Test Purpose and Environment 1024

A.6.1.1.4.2 Test Parameters 1024

A.6.1.1.4.3 Test Requirements 1028

A.6.1.1.5 Cell reselection to FR1 inter-frequency NR case for UE fulfilling low mobility relaxed measurement criterion 1028

A.6.1.1.5.1 Test Purpose and Environment 1028

A.6.1.1.5.2 Test Parameters 1028

A.6.1.1.5.3 Test Requirements 1032

A.6.1.1.6 Cell reselection to FR1 inter-frequency NR case for UE fulfilling not-at-cell edge relaxed measurement criterion 1033

A.6.1.1.6.1 Test Purpose and Environment 1033

A.6.1.1.6.2 Test Parameters 1033

A.6.1.1.6.3 Test Requirements 1037

A.6.1.1.7 Cell reselection to FR1 intra-frequency NR case for UE configured with *highSpeedMeasFlag-r16* 1038

A.6.1.1.7.1 Test Purpose and Environment 1038

A.6.1.1.7.2 Test Parameters 1038

A.6.1.1.7.3 Test Requirements 1042

A.6.1.2 Inter-RAT E-UTRAN cell re-selection 1042

A.6.1.2.1 Cell reselection to higher priority E-UTRAN 1042

A.6.1.2.1.1 Test Purpose and Environment 1042

A.6.1.2.1.2 Test Parameters 1042

A.6.1.2.1.3 Test Requirements 1045

A.6.1.2.2 Cell reselection to lower priority E-UTRAN 1046

A.6.1.2.2.1 Test Purpose and Environment 1046

A.6.1.2.2.2 Test Parameters 1046

A.6.1.2.2.3 Test Requirements 1049

A.6.1.2.3 Cell reselection to lower priority E-UTRAN for UE fulfilling low mobility relaxed measurement criterion 1050

A.6.1.2.3.1 Test Purpose and Environment 1050

A.6.1.2.3.2 Test Parameters 1050

A.6.1.2.3.3 Test Requirements 1053

A.6.1.2.4 Cell reselection to lower priority E-UTRAN for UE fulfilling not-at-cell edge relaxed measurement criterion 1054

A.6.1.2.4.1 Test Purpose and Environment 1054

A.6.1.2.4.2 Test Parameters 1054

A.6.1.2.4.3 Test Requirements 1057

A.6.1.2.5.3 Test Requirements 1061

A.6.2 SA: RRC\_INACTIVE state mobility 1062

A.6.3 RRC\_CONNECTED state mobility 1062

A.6.3.1 Handover 1062

A.6.3.1.1 Intra-frequency handover from FR1 to FR1; known target cell 1062

A.6.3.1.1.1 Test Purpose and Environment 1062

A.6.3.1.1.2 Test Parameters 1062

A.6.3.1.1.3 Test Requirements 1066

A.6.3.1.2 Intra-frequency handover from FR1 to FR1; unknown target cell 1066

A.6.3.1.2.1 Test Purpose and Environment 1066

A.6.3.1.2.2 Test Parameters 1066

A.6.3.1.2.3 Test Requirements 1070

A.6.3.1.3 Inter-frequency handover from FR1 to FR1; unknown target cell 1070

A.6.3.1.3.1 Test Purpose and Environment 1070

A.6.3.1.3.2 Test Parameters 1070

A.6.3.1.3.3 Test Requirements 1074

A.6.3.1.4 SA NR - E-UTRAN handover 1074

A.6.3.1.4.1 Test Purpose and Environment 1074

A.6.3.1.4.2 Test Requirements 1080

A.6.3.1.5 SA NR - E-UTRAN handover with unknown target cell 1080

A.6.3.1.5.1 Test Purpose and Environment 1080

A.6.3.1.5.2 Test Requirements 1086

A.6.3.1.6 SA NR - UTRAN FDD handover 1086

A.6.3.1.6.1 Test Purpose and Environment 1086

A.6.3.1.6.2 Test Requirements 1090

A.6.3.1.7 Intra-frequency synchronous DAPS handover in FR1 1090

A.6.3.1.7.1 Test Purpose and Environment 1090

A.6.3.1.7.2 Test Parameters 1090

A.6.3.1.7.3 Test Requirements 1094

A.6.3.1.8 Intra-frequency asynchronous DAPS handover in FR1 1095

A.6.3.1.8.1 Test Purpose and Environment 1095

A.6.3.1.8.2 Test Parameters 1095

A.6.3.1.8.3 Test Requirements 1099

A.6.3.1.9 Intra-band inter-frequency synchronous DAPS handover test in SA for FR1 1100

A.6.3.1.9.1 Test Purpose and Environment 1100

A.6.3.1.9.2 Test Parameters 1100

A.6.3.1.9.3 Test Requirements 1104

A.6.3.1.10 Intra-band inter-frequency asynchronous DAPS handover test in SA for FR1 1104

A.6.3.1.10.1 Test Purpose and Environment 1104

A.6.3.1.10.2 Test Parameters 1104

A.6.3.1.10.3 Test Requirements 1107

A.6.3.1.11 Inter-band inter-frequency synchronous DAPS handover from FR1 to FR1 1107

A.6.3.1.11.1 Test Purpose and Environment 1107

A.6.3.1.11.2 Test Parameters 1107

A.6.3.1.11.3 Test Requirements 1114

A.6.3.1.12 Inter-band inter-frequency asynchronous DAPS handover from FR1 to FR1 1114

A.6.3.1.12.1 Test Purpose and Environment 1114

A.6.3.1.12.2 Test Parameters 1114

A.6.3.1.12.3 Test Requirements 1122

A.6.3.2 RRC Connection Mobility Control 1122

A.6.3.2.1 SA: RRC Re-establishment 1122

A.6.3.2.1.1 Intra-frequency RRC Re-establishment in FR1 1122

A.6.3.2.1.2 Inter-frequency RRC Re-establishment in FR1 1126

A.6.3.2.1.3 Intra-frequency RRC Re-establishment in FR1 without serving cell timing 1130

A.6.3.2.2 Random Access 1134

A.6.3.2.2.1 4-step RA type contention based random access test in FR1 for NR standalone 1134

A.6.3.2.2.2 4-step RA type non-contention based random access test in FR1 for NR standalone 1139

A.6.3.2.2.3 2-step RA type contention based random access test in FR1 for NR standalone 1143

A.6.3.2.2.4 2-step RA type non-contention based test in FR1 for NR standalone 1148

A.6.3.2.3 SA: RRC Connection Release with Redirection 1152

A.6.3.2.3.1 Redirection from NR in FR1 to NR in FR1 1152

A.6.3.2.3.2 Redirection from NR in FR1 to E-UTRAN 1156

A.6.3.3 Conditional handover 1163

A.6.3.3.1 Intra-frequency conditional handover from FR1 to FR1 1163

A.6.3.3.1.1 Test Purpose and Environment 1163

A.6.3.3.1.2 Test Parameters 1163

A.6.3.3.1.3 Test Requirements 1167

A.6.3.3.2 Inter-frequency conditional handover from FR1 to FR1 1167

A.6.3.3.2.1 Test Purpose and Environment 1167

A.6.3.3.2.2 Test Parameters 1167

A.6.3.3.2.3 Test Requirements 1171

A.6.4 Timing 1171

A.6.4.1 UE transmit timing 1171

A.6.4.1.1 NR UE Transmit Timing Test for FR1 1171

A.6.4.1.1.1 Test Purpose and environment 1171

A.6.4.1.1.2 Test requirements 1175

A.6.4.2 UE timer accuracy 1175

A.6.4.3 Timing advance 1175

A.6.4.3.1 SA FR1 timing advance adjustment accuracy 1175

A.6.4.3.1.1 Test Purpose and Environment 1175

A.6.4.3.1.2 Test Parameters 1175

A.6.4.3.1.3 Test Requirements 1179

A.6.5 Signalling characteristics 1179

A.6.5.1 Radio link Monitoring 1179

A.6.5.1.1 Radio Link Monitoring Out-of-sync Test for FR1 PCell configured with SSB-based RLM RS in non-DRX mode 1180

A.6.5.1.1.1 Test Purpose and Environment 1180

A.6.5.1.1.2 Test Requirements 1185

A.6.5.1.2 Radio Link Monitoring In-sync Test for FR1 PCell configured with SSB-based RLM RS in non-DRX mode 1185

A.6.5.1.2.1 Test Purpose and Environment 1185

A.6.5.1.2.2 Test Requirements 1191

A.6.5.1.3 Radio Link Monitoring Out-of-sync Test for FR1 PCell configured with SSB-based RLM RS in DRX mode 1191

A.6.5.1.3.1 Test Purpose and Environment 1191

A.6.5.1.3.2 Test Requirements 1197

A.6.5.1.4 Radio Link Monitoring In-sync Test for FR1 PCell configured with SSB-based RLM RS in DRX mode 1197

A.6.5.1.4.1 Test Purpose and Environment 1197

A.6.5.1.4.2 Test Requirements 1203

A.6.5.1.5 Radio Link Monitoring Out-of-sync Test for FR1 PCell configured with CSI-RS-based RLM in non-DRX mode 1203

A.6.5.1.5.1 Test Purpose and Environment 1203

A.6.5.1.5.2 Test Requirements 1209

A.6.5.1.6 Radio Link Monitoring In-sync Test for FR1 PCell configured with CSI-RS-based RLM in non-DRX mode 1209

A.6.5.1.6.1 Test Purpose and Environment 1209

A.6.5.1.6.2 Test Requirements 1214

A.6.5.1.7 Radio Link Monitoring Out-of-sync Test for FR1 PCell configured with CSI-RS-based RLM in DRX mode 1214

A.6.5.1.7.1 Test Purpose and Environment 1214

A.6.5.1.7.2 Test Requirements 1218

A.6.5.1.8 Radio Link Monitoring In-sync Test for FR1 PCell configured with CSI-RS-based RLM in DRX mode 1218

A.6.5.1.8.1 Test Purpose and Environment 1218

A.6.5.1.8.2 Test Requirements 1224

A.6.5.2 Interruption 1224

A.6.5.2.1 Interruptions during measurements on deactivated NR SCC in FR1 1224

A.6.5.2.1.2 Test Requirements 1228

A.6.5.2.2 SA interruptions at NR SRS carrier based switching 1229

A.6.5.2.2.1 Test Purpose and Environment 1229

A.6.5.2.2.2 Test Parameters 1229

A.6.5.2.2.3 Test Requirements 1231

A.6.5.3 SCell Activation and Deactivation Delay 1232

A.6.5.3.1 SCell Activation and deactivation of known SCell in FR1 in non-DRX for 160ms SCell measurement cycle 1232

A.6.5.3.1.1 Test Purpose and Environment 1232

A.6.5.3.1.2 Test Requirements 1237

A.6.5.3.2 SCell Activation and deactivation of known SCell in FR1 in non-DRX for 640 ms SCell measurement cycle 1238

A.6.5.3.2.1 Test Purpose and Environment 1238

A.6.5.3.2.2 Test Requirements 1238

A.6.5.3.3 SCell Activation and deactivation of unknown SCell in FR1 in non-DRX 1238

A.6.5.3.3.1 Test Purpose and Environment 1238

A.6.5.3.3.2 Test Requirements 1239

A.6.5.3.4 Direct SCell activation at SCell addition of known SCell in FR1 1239

A.6.5.3.4.1 Test Purpose and Environment 1239

A.6.5.3.4.2 Test Requirements 1244

A.6.5.3.5 Direct SCell activation at handover with known SCell in FR1 1244

A.6.5.3.5.1 Test Purpose and Environment 1244

A.6.5.3.5.2 Test Requirements 1249

A.6.5.4 UE UL carrier RRC reconfiguration Delay 1250

A.6.5.4.1 UE UL carrier RRC reconfiguration Delay 1250

A.6.5.4.1.1 Test Purpose and Environment 1250

A.6.5.4.1.2 Test Requirements 1260

A.6.5.4.2 Void 1261

A.6.5.5 Beam Failure Detection and Link recovery procedures 1261

A.6.5.5.1 Beam Failure Detection and Link Recovery Test for FR1 PCell configured with SSB-based BFD and LR in non-DRX mode 1261

A.6.5.5.1.1 Test Purpose and Environment 1261

A.6.5.5.1.2 Test Requirements 1266

A.6.5.5.2 Beam Failure Detection and Link Recovery Test for FR1 PCell configured with SSB-based BFD and LR in DRX mode 1267

A.6.5.5.2.1 Test Purpose and Environment 1267

A.6.5.5.2.2 Test Requirements 1273

A.6.5.5.3 Beam Failure Detection and Link Recovery Test for FR1 PCell configured with CSI-RS-based BFD and LR in non-DRX mode 1274

A.6.5.5.3.1 Test Purpose and Environment 1274

A.6.5.5.3.2 Test Requirements 1279

A.6.5.5.4 Beam Failure Detection and Link Recovery Test for FR1 PCell configured with CSI-RS-based BFD and LR in DRX mode 1280

A.6.5.5.4.1 Test Purpose and Environment 1280

A.6.5.5.4.2 Test Requirements 1285

A.6.5.5.5 Beam Failure Detection and Link Recovery Test for FR1 SCell configured with CSI-RS-based BFD and SSB-based LR in non-DRX mode 1286

A.6.5.5.5.1 Test Purpose and Environment 1286

A.6.5.5.5.2 Test Requirements 1290

A.6.5.5.6 Beam Failure Detection and Link Recovery Test for FR1 SCell configured with CSI-RS-based BFD and SSB-based LR in DRX mode 1290

A.6.5.5.6.1 Test Purpose and Environment 1290

A.6.5.5.6.2 Test Requirements 1294

A.6.5.6 Active BWP switch 1295

A.6.5.6.1 DCI-based and Timer-based Active BWP Switch 1295

A.6.5.6.1.1 NR FR1- NR FR1 DL active BWP switch of SCell with non-DRX in SA 1295

A.6.5.6.1.2 NR FR1 DL active BWP switch with non-DRX in SA 1302

A.6.5.6.2 RRC-based Active BWP Switch 1306

A.6.5.6.2.1 NR FR1 DL active BWP switch of Cell with non-DRX in SA 1306

A.6.5.6.3 Simultaneous DCI-based and Timer-based Active BWP Switch on multiple CCs 1310

A.6.5.6.3.1 NR FR1- NR FR1 DL active BWP switch on multiple CCs with non-DRX in SA 1310

A.6.5.6.4 SCell dormancy switch 1317

A.6.5.6.4.1 NR FR1 PCell SCell dormancy switch of single FR1 SCell outside active time 1317

A.6.5.6.4.2 NR FR1 PCell SCell dormancy switch of two FR1 SCells inside active time 1323

A.6.5.6.5 Simultaneous RRC-based Active BWP Switch on multiple CCs 1330

A.6.5.6.5.1 NR FR1- NR FR1 DL active BWP switch on multiple CCs with non-DRX in SA 1330

A.6.5.7 DL interruptions at switching between two uplink carriers 1335

A.6.5.7.1 DL interruptions at switching between two uplink carriers in FDD-TDD CA 1335

A.6.5.7.1.1 Test Purpose and Environment 1335

A.6.5.7.1.2 Test Requirements 1339

A.6.5.7.2 DL interruptions at switching between two uplink carriers in TDD-TDD CA 1339

A.6.5.7.2.1 Test Purpose and Environment 1339

A.6.5.7.2.2 Test Requirements 1343

A.6.5.8 UE specific CBW change 1343

A.6.5.8.1 UE specific CBW change on PCell in FR1 in non-DRX 1343

A.6.5.8.1.1 Test Purpose and Environment 1343

A.6.5.8.1.2 Test Requirements 1347

A.6.5.9 Pathloss reference signal switching delay 1347

A.6.5.9.1 MAC-CE based pathloss reference signal switch delay 1347

A.6.5.9.1.1 Test Purpose and Environment 1347

A.6.5.9.1.2 Test Requirements 1350

A.6.6 Measurement procedure 1351

A.6.6.1 Intra-frequency Measurements 1351

A.6.6.1.1 SA event triggered reporting tests without gap under non-DRX 1351

A.6.6.1.1.1 Test purpose and Environment 1351

A.6.6.1.1.2 Test parameters 1351

A.6.6.1.1.3 Test Requirements 1355

A.6.6.1.2 SA event triggered reporting tests without gap under DRX 1355

A.6.6.1.2.1 Test purpose and Environment 1355

A.6.6.1.2.2 Test parameters 1355

A.6.6.1.2.3 Test Requirements 1359

A.6.6.1.3 SA event triggered reporting tests with per-UE gaps under non-DRX 1359

A.6.6.1.3.1 Test purpose and Environment 1359

A.6.6.1.3.2 Test parameters 1359

A.6.6.1.3.3 Test Requirements 1363

A.6.6.1.4 SA event triggered reporting tests with per-UE gaps under DRX 1363

A.6.6.1.4.1 Test purpose and Environment 1363

A.6.6.1.4.2 Test parameters 1363

A.6.6.1.4.3 Test Requirements 1367

A.6.6.1.5 SA event triggered reporting tests without gap under non-DRX with SSB index reading 1367

A.6.6.1.5.1 Test purpose and Environment 1367

A.6.6.1.5.2 Test parameters 1367

A.6.6.1.5.3 Test Requirements 1369

A.6.6.1.6 SA event triggered reporting tests with per-UE gaps under non-DRX with SSB index reading 1370

A.6.6.1.6.1 Test purpose and Environment 1370

A.6.6.1.6.2 Test parameters 1370

A.6.6.1.6.3 Test Requirements 1371

A.6.6.1.7 SA event triggered reporting tests under DRX for UE configured with highSpeedMeasFlag-r16 1372

A.6.6.1.7.1 Test purpose and Environment 1372

A.6.6.1.7.2 Test parameters 1372

A.6.6.1.7.3 Test Requirements 1376

A.6.6.2 Inter-frequency Measurements 1376

A.6.6.2.1 SA event triggered reporting tests for FR1 without SSB time index detection when DRX is not used 1376

A.6.6.2.1.1 Test Purpose and Environment 1376

A.6.6.2.1.2 Test Requirements 1380

A.6.6.2.2 SA event triggered reporting tests for FR1 without SSB time index detection when DRX is used 1380

A.6.6.2.2.1 Test Purpose and Environment 1380

A.6.6.2.2.2 Test Requirements 1384

A.6.6.2.3 Void 1385

A.6.6.2.4 Void 1385

A.6.6.2.5 SA event triggered reporting tests for FR1 with SSB time index detection when DRX is not used 1385

A.6.6.2.5.1 Test Purpose and Environment 1385

A.6.6.2.5.2 Test Requirements 1389

A.6.6.2.6 SA event triggered reporting tests for FR1 with SSB time index detection when DRX is used 1389

A.6.6.2.6.1 Test Purpose and Environment 1389

A.6.6.2.6.2 Test Requirements 1393

A.6.6.2.7 Void 1394

A.6.6.2.8 Void 1394

A.6.6.2.9 SA event triggered reporting tests with additional mandatory gap pattern 1394

A.6.6.2.9.1 Test Purpose and Environment 1394

A.6.6.2.9.2 Test Requirements 1397

A.6.6.2.10 SA event triggered reporting tests for FR1 when DRX is used 1397

A.6.6.2.10.1 Test Purpose and Environment 1397

A.6.6.2.10.2 Test Requirements 1401

A.6.6.2.11 SA event triggered reporting tests for FR1 without gap when DRX is not used 1402

A.6.6.2.11.1 Test Purpose and Environment 1402

A.6.6.2.11.2 Test Requirements 1405

A.6.6.3 Inter-RAT Measurements 1405

A.6.6.3.1 SA NR - E-UTRAN event-triggered reporting in non-DRX in FR1 1405

A.6.6.3.1.1 Test Purpose and Environment 1405

A.6.6.3.1.2 Test Requirements 1411

A.6.6.3.2 SA NR - E-UTRAN event-triggered reporting in DRX in FR1 1411

A.6.6.3.2.1 Test Purpose and Environment 1411

A.6.6.3.2.2 Test Requirements 1418

A.6.6.3.3 SA NR - E-UTRAN event-triggered reporting in DRX in FR1 for UE configured with highSpeedMeasFlag-r16 1418

A.6.6.3.3.1 Test Purpose and Environment 1418

A.6.6.3.3.2 Test Requirements 1425

A.6.6.4 L1-RSRP measurement for beam reporting 1425

A.6.6.4.1 SSB based L1-RSRP measurement when DRX is not used 1425

A.6.6.4.1.1 Test Purpose and Environment 1425

A.6.6.4.1.2 Test parameters 1425

A.6.6.4.1.3 Test Requirements 1428

A.6.6.4.2 SSB based L1-RSRP measurement when DRX is used 1428

A.6.6.4.2.1 Test Purpose and Environment 1428

A.6.6.4.2.2 Test parameters 1429

A.6.6.4.2.3 Test Requirements 1432

A.6.6.4.3 CSI-RS based L1-RSRP measurement when DRX is not used 1432

A.6.6.4.3.1 Test Purpose and Environment 1432

A.6.6.4.3.2 Test parameters 1433

A.6.6.4.3.3 Test Requirements 1436

A.6.6.4.4 CSI-RS based L1-RSRP measurement when DRX is used 1436

A.6.6.4.4.1 Test Purpose and Environment 1436

A.6.6.4.4.2 Test parameters 1437

A.6.6.4.4.3 Test Requirements 1440

A.6.6.4.5 SSB based L1-RSRP measurement when DRX is used for UE configured with *highSpeedMeasFlag-r16* 1440

A.6.6.4.5.1 Test Purpose and Environment 1440

A.6.6.4.5.2 Test parameters 1441

A.6.6.4.5.3 Test Requirements 1444

A.6.6.5 1444

A.6.6.5.1 SA NR - UTRAN FDD event-triggered reporting in non-DRX in FR1 1444

A.6.6.5.1.1 Test Purpose and Environment 1444

A.6.6.5.1.2 Test Requirements 1448

A.6.6.6 CLI measurements 1448

A.6.6.6.1 SRS-RSRP measurement with DRX 1448

A.6.6.6.1.1 Test Purpose and Environment 1448

A.6.6.6.1.2 Test Parameters 1449

A.6.6.6.1.3 Test Requirements 1452

A.6.6.6.2 CLI-RSSI measurement with DRX 1452

A.6.6.6.2.1 Test Purpose and Environment 1452

A.6.6.6.2.2 Test Parameters 1453

A.6.6.6.2.3 Test Requirements 1455

A.6.6.7 NR measurements with autonomous gaps 1455

A.6.6.7.1 SA intra-frequency CGI identification of NR neighbor cell in FR1 1455

A.6.6.7.1.1 Test Purpose and Environment 1455

A.6.6.7.1.2 Test Parameters 1455

A.6.6.7.1.3 Test Requirements 1458

A.6.6.7.2 Identification of a new CGI of inter-RAT E-UTRA cell using autonomous gaps in NR SA 1458

A.6.6.7.2.1 Test Purpose and Environment 1458

A.6.6.7.2.2 Test Requirements 1461

A.6.6.8 L1-SINR measurement for beam reporting 1462

A.6.6.8.1 L1-SINR measurement with CSI-RS based CMR and no dedicated IMR configured when DRX is used 1462

A.6.6.8.1.1 Test Purpose and Environment 1462

A.6.6.8.2 L1-SINR measurement with SSB based CMR and dedicated IMR when DRX is not used 1465

A.6.6.8.2.1 Test Purpose and Environment 1465

A.6.6.8.2.2 Test parameters 1466

A.6.6.8.2.3 Test Requirements 1470

A.6.6.8.3 L1-SINR measurement with CSI-RS based CMR and dedicated IMR configured when DRX is not used 1470

A.6.6.8.3.1 Test Purpose and Environment 1470

A.6.6.8.3.2 Test parameters 1471

A.6.6.8.3.3 Test Requirements 1474

A.6.6.9 Idle Mode CA/DC Measurements 1474

A.6.6.9.1 SA Idle mode CA/DC measurement for FR1 1474

A.6.6.9.1.1 Test Purpose and Environment 1474

A.6.6.9.1.2 Test Requirements 1481

A.6.6.10 CSI-RS based intra-frequency Measurements 1481

A.6.6.10.1 SA event triggered reporting tests without gap under non-DRX 1481

A.6.6.10.1.1 Test purpose and Environment 1481

A.6.6.10.1.2 Test Requirements 1484

A.6.6.11 CSI-RS based inter-frequency Measurements 1484

A.6.6.11.1 SA event triggered reporting tests with gap under DRX 1484

A.6.6.11.1.1 Test Purpose and Environment 1484

A.6.6.11.1.2 Test Requirements 1488

A.6.6.12 RSTD measurements 1488

A. 6.6.12.1 NR RSTD measurement reporting delay test case for single positioning frequency layer in FR1 SA 1488

A. 6.6.12.1.1 Test Purpose and Environment 1488

A.6.6.12.1.2 Test Requirements 1496

A. 6.6.12.2 NR RSTD measurement reporting delay test case for dual positioning frequency layers in FR1 SA 1496

A. 6.6.12.2.1 Test Purpose and Environment 1496

A.6.6.12.2.2 Test Requirements 1503

A.6.6.13 PRS-RSRP measurements 1503

A.6.6.13.1 PRS-RSRP reporting delay test case for single positioning frequency layer 1503

A.6.6.13.1.1 Test purpose and Environment 1503

A.6.6.13.1.2 Test Requirements 1507

A.6.6.13.2 PRS-RSRP reporting delay test case for dual positioning frequency layer 1507

A.6.6.13.2.1 Test purpose and Environment 1507

A.6.6.13.2.2 Test Requirements 1511

A.6.6.14 UE Rx-Tx time difference measurements 1511

A.6.6.14.1 UE Rx-Tx time difference measurement for single positioning frequency layer in FR1 SA 1511

A.6.6.14.1.1 Test purpose and environment 1511

A.6.6.14.1.2 Test requirements 1515

A.6.6.14.2 UE Rx-Tx time difference measurement for dual positioning frequency layers in FR1 SA 1515

A.6.6.14.2.1 Test purpose and environment 1515

A.6.6.14.2.2 Test requirements 1519

A.6.6.15 Idle Mode measurements of inter-RAT DC candidate cells for early reporting 1519

A.6.6.15.1 Test Purpose and Environment 1519

A.6.6.15.2 Test Requirements 1526

A.6.7 Measurement Performance requirements 1527

A.6.7.1 SS-RSRP 1527

A.6.7.1.1 SA: intra-frequency case measurement accuracy with FR1 serving cell and FR1 target cell 1527

A.6.7.1.1.1 Test Purpose and Environment 1527

A.6.7.1.1.2 Test parameters 1527

A.6.7.1.1.3 Test Requirements 1532

A.6.7.1.2 SA inter-frequency case measurement accuracy with FR1 serving cell and FR1 target cell 1532

A.6.7.1.2.1 Test Purpose and Environment 1532

A.6.7.1.2.2 Test parameters 1532

A.6.7.1.2.3 Test Requirements 1536

A.6.7.1.3 Void 1536

A.6.7.2 SS-RSRQ 1536

A.6.7.2.1 SA: Intra-frequency measurement accuracy with FR1 serving cell and FR1 target cell 1536

A.6.7.2.1.1 Test Purpose and Environment 1536

A.6.7.2.1.2 Test Parameters 1537

A.6.7.2.1.3 Test Requirements 1542

A.6.7.2.2 SA Inter-frequency measurement accuracy with FR1 serving cell and FR1 target cell 1542

A.6.7.2.2.1 Test Purpose and Environment 1542

A.6.7.2.2.2 Test Parameters 1542

A.6.7.2.2.3 Test Requirements 1547

A.6.7.3 SS-SINR 1547

A.6.7.3.1 SA intra-frequency measurement accuracy with FR1 serving cell and FR1 target cell 1547

A.6.7.3.1.1 Test Purpose and Environment 1547

A.6.7.3.1.2 Test Parameters 1548

A.6.7.3.1.3 Test Requirements 1552

A.6.7.3.2 SA Inter-frequency measurement accuracy with FR1 serving cell and FR1 target cell 1552

A.6.7.3.2.1 Test Purpose and Environment 1552

A.6.7.3.2.2 Test Parameters 1553

A.6.7.3.2.3 Test Requirements 1558

A.6.7.4 L1-RSRP measurement for beam reporting 1559

A.6.7.4.1 SSB based L1-RSRP measurement 1559

A.6.7.4.1.1 Test Purpose and Environment 1559

A.6.7.4.1.2 Test parameters 1559

A.6.7.4.1.3 Test Requirements 1563

A.6.7.4.2 CSI-RS based L1-RSRP measurement on resource set with repetition off 1563

A.6.7.4.2.1 Test Purpose and Environment 1563

A.6.7.4.2.2 Test parameters 1564

A.6.7.4.2.3 Test Requirements 1568

A.6.7.5 E-UTRAN RSRP 1568

A.6.7.5.1 SA: inter-RAT measurement accuracy with FR1 serving cell 1568

A.6.7.5.1.1 Test Purpose and Environment 1568

A.6.7.5.1.2 Test parameters 1569

A.6.7.5.1.3 Test Requirements 1575

A.6.7.6 E-UTRAN RSRQ 1576

A.6.7.6.1 SA: inter-RAT measurement accuracy with FR1 serving cell 1576

A.6.7.6.1.1 Test Purpose and Environment 1576

A.6.7.6.1.2 Test parameters 1576

A.6.7.6.1.3 Test Requirements 1581

A.6.7.7 E-UTRAN RS-SINR 1582

A.6.7.7.1 SA: inter-RAT measurement accuracy with FR1 serving cell 1582

A.6.7.7.1.1 Test Purpose and Environment 1582

A.6.7.7.1.2 Test parameters 1582

A.6.7.7.1.3 Test Requirements 1588

A.6.7.8 CLI measurements 1589

A.6.7.8.1 SA SRS-RSRP measurement accuracy with FR1 serving cell 1589

A.6.7.8.1.1 Test Purpose and Environment 1589

A.6.7.8.1.2 Test parameters 1589

A.6.7.8.1.3 Test Requirements 1595

A.6.7.8.2 SA CLI-RSSI measurement accuracy with FR1 serving cell 1595

A.6.7.8.2.1 Test Purpose and Environment 1595

A.6.7.8.2.2 Test parameters 1596

A.6.7.8.2.3 Test Requirements 1599

A.6.7.9 L1-SINR measurement for beam reporting 1600

A.6.7.9.1 L1-SINR measurement with CSI-RS based CMR and no dedicated IMR configured and CSI-RS resource set with repetition off 1600

A.6.7.9.1.1 Test Purpose and Environment 1600

A.6.7.9.1.2 Test parameters 1600

A.6.7.9.1.3 Test Requirements 1604

A.6.7.9.2 L1-SINR measurement with SSB based CMR and dedicated IMR 1604

A.6.7.9.2.1 Test Purpose and Environment 1604

A.6.7.9.2.2 Test parameters 1605

A.6.7.9.2.3 Test Requirements 1610

A.6.7.9.3 L1-SINR measurement with CSI-RS based CMR and dedicated IMR 1610

A.6.7.9.3.1 Test Purpose and Environment 1610

A.6.7.9.3.2 Test parameters 1610

A.6.7.9.3.3 Test Requirements 1615

A.6.7.10 CSI-RSRP 1615

A.6.7.10.1 SA: intra-frequency case measurement accuracy with FR1 serving cell and FR1 target cell 1615

A.6.7.10.1.1 Test Purpose and Environment 1615

A.6.7.10.1.2 Test parameters 1616

A.6.7.10.1.3 Test Requirements 1621

A.6.7.10.2 SA inter-frequency case measurement accuracy with FR1 serving cell and FR1 target cell 1621

A.6.7.10.2.1 Test Purpose and Environment 1621

A.6.7.10.2.2 Test parameters 1621

A.6.7.10.2.3 Test Requirements 1626

A.6.7.11 CSI-RSRQ 1626

A.6.7.11.1 SA: Intra-frequency measurement accuracy with FR1 serving cell and FR1 target cell 1626

A.6.7.11.1.1 Test Purpose and Environment 1626

A.6.7.11.1.2 Test Parameters 1626

A.6.7.11.1.3 Test Requirements 1631

A.6.7.11.2 SA Inter-frequency measurement accuracy with FR1 serving cell and FR1 target cell 1631

A.6.7.11.2.1 Test Purpose and Environment 1631

A.6.7.11.2.2 Test Parameters 1631

A.6.7.11.2.3 Test Requirements 1636

A.6.7.12 CSI-SINR 1637

A.6.7.12.1 SA intra-frequency measurement accuracy with FR1 serving cell and FR1 target cell 1637

A.6.7.12.1.1 Test Purpose and Environment 1637

A.6.7.12.1.2 Test Parameters 1637

A.6.7.12.1.3 Test Requirements 1641

A.6.7.12.2 SA Inter-frequency measurement accuracy with FR1 serving cell and FR1 target cell 1642

A.6.7.12.2.1 Test Purpose and Environment 1642

A.6.7.12.2.2 Test Parameters 1642

A.6.7.12.2.3 Test Requirements 1648

A.6.7.13 RSTD measurements 1648

A.6.7.13.1 RSTD measurement accuracy test case for single positioning frequency layer 1648

A.6.7.13.1.1 Test purpose and Environment 1648

A.6.7.13.1.2 Test Requirements 1651

A.6.7.13.2 RSTD measurement accuracy test case for dual positioning frequency layer 1651

A.6.7.13.2.1 Test purpose and Environment 1651

A.6.7.13.2.2 Test Requirements 1655

A.6.7.14 PRS-RSRP measurements 1655

A.6.7.14.1 SA: measurement accuracy with PRS in FR1 1655

A.6.7.14.1.1 Test Purpose and Environment 1655

A.6.7.14.1.2 Test parameters 1656

A.6.7.14.1.3 Test Requirements 1660

A.6.7.15 UE Rx-Tx time difference measurements 1660

A.6.7.15.1 UE Rx-Tx time difference measurement accuracy for single positioning frequency layer in FR1 SA 1660

A.6.7.15.1.1 Test purpose and environment 1660

A.6.7.15.1.2 Test parameters 1661

A.6.7.15.1.3 Test requirements 1664

A.7.1 SA: RRC\_IDLE state mobility 1665

A.7.1.1 Cell re-selection to NR 1665

A.7.1.1.1 Cell reselection to FR2 intra-frequency NR case 1665

A.7.1.1.1.1 Test Purpose and Environment 1665

A.7.1.1.1.2 Test Parameters 1665

A.7.1.1.1.3 Test Requirements 1668

A.7.1.1.2 Cell reselection to FR2 inter-frequency NR case 1668

A.7.1.1.2.1 Test Purpose and Environment 1668

A.7.1.1.2.2 Test Parameters 1669

A.7.1.1.2.3 Test Requirements 1671

A.7.1.1.3 Cell reselection to FR2 intra-frequency NR case for UE fulfilling low mobility relaxed measurement criterion 1671

A.7.1.1.3.1 Test Purpose and Environment 1671

A.7.1.1.3.2 Test Parameters 1671

A.7.1.1.3.3 Test Requirements 1674

A.7.1.1.4 Cell reselection to FR2 intra-frequency NR case for UE fulfilling not-at-cell edge relaxed measurement criterion 1674

A.7.1.1.4.1 Test Purpose and Environment 1674

A.7.1.1.4.2 Test Parameters 1674

A.7.1.1.4.3 Test Requirements 1677

A.7.1.1.5 Cell reselection to FR2 inter-frequency NR case for UE fulfilling low mobility relaxed measurement criterion 1677

A.7.1.1.5.1 Test Purpose and Environment 1677

A.7.1.1.5.2 Test Parameters 1677

A.7.1.1.5.3 Test Requirements 1680

A.7.1.1.6 Cell reselection to FR2 inter-frequency NR case for UE fulfilling not-at-cell edge relaxed measurement criterion 1680

A.7.1.1.6.1 Test Purpose and Environment 1680

A.7.1.1.6.2 Test Parameters 1680

A.7.1.1.6.3 Test Requirements 1683

A.7.2 SA: RRC\_INACTIVE state mobility 1683

A.7.3 RRC\_CONNECTED state mobility 1683

A.7.3.1 Handover 1683

A.7.3.1.1 Inter-frequency handover from FR1 to FR2; unknown target cell 1683

A.7.3.1.1.1 Test Purpose and Environment 1683

A.7.3.1.1.2 Test Parameters 1683

A.7.3.1.1.3 Test Requirements 1687

A.7.3.1.2 Intra-frequency handover from FR2 to FR2; unknown target cell 1687

A.7.3.1.2.1 Test Purpose and Environment 1687

A.7.3.1.2.2 Test Parameters 1687

A.7.3.1.2.3 Test Requirements 1690

A.7.3.1.3 Inter-frequency handover from FR2 to FR2; unknown target cell 1690

A.7.3.1.3.1 Test Purpose and Environment 1690

A.7.3.1.3.2 Test Parameters 1690

A.7.3.1.3.3 Test Requirements 1691

A.7.3.1.4 Inter-band inter-frequency synchronous DAPS handover from FR1 to FR2 1692

A.7.3.1.4.1 Test Purpose and Environment 1692

A.7.3.1.4.2 Test Parameters 1692

A.7.3.1.4.3 Test Requirements 1699

A.7.3.1.5 Inter-band inter-frequency asynchronous DAPS handover from FR1 to FR2 1699

A.7.3.1.5.1 Test Purpose and Environment 1699

A.7.3.1.5.2 Test Parameters 1699

A.7.3.1.5.3 Test Requirements 1706

A.7.3.2 RRC Connection Mobility Control 1706

A.7.3.2.1 SA: RRC Re-establishment 1706

A.7.3.2.1.1 Intra-frequency RRC Re-establishment in FR2 1706

A.7.3.2.1.2 Inter-frequency RRC Re-establishment in FR2 1709

A.7.3.2.1.3 Intra-frequency RRC Re-establishment in FR2 without serving cell timing 1712

A.7.3.2.1.3.1 Test Purpose and Environment 1712

A.7.3.2.1.3.2 Test Requirements 1714

A.7.3.2.2 Random Access 1715

A.7.3.2.2.1 4-step RA type contention based random access test in FR2 for NR Standalone 1715

A.7.3.2.2.2 4-step RA type non-contention based random access test in FR2 for NR Standalone 1719

A.7.3.2.2.3 2-step RA type contention based random access test in FR2 for NR Standalone 1724

A.7.3.2.2.4 2-step RA type non-contention based random access test in FR2 for NR Standalone 1727

A.7.3.2.3 SA: RRC Connection Release with Redirection 1730

A.7.3.2.3.1 Redirection from NR in FR2 to NR in FR2 1730

A.7.3.3 Conditional Handover 1734

A.7.3.3.1 Intra-frequency conditional handover from FR2 to FR2 1734

A.7.3.3.1.1 Test Purpose and Environment 1734

A.7.3.3.1.2 Test Parameters 1734

A.7.3.3.1.2.3 Test Requirements 1737

A.7.3.3.2 Inter-frequency conditional handover from FR2 to FR2; unknown target cell 1737

A.7.3.3.2.1 Test Purpose and Environment 1737

A.7.3.3.2.2 Test Parameters 1737

A.7.3.3.2.3 Test Requirements 1740

A.7.4 Timing 1740

A.7.4.1 UE transmit timing 1740

A.7.4.1.1 NR UE Transmit Timing Test for FR2 1740

A.7.4.1.1.1 Test Purpose and environment 1740

A.7.4.1.1.2 Test requirements 1743

A.7.4.2 UE timer accuracy 1744

A.7.4.3 Timing advance 1744

A.7.4.3.1 SA FR2 timing advance adjustment accuracy 1744

A.7.4.3.1.1 Test Purpose and Environment 1744

A.7.4.3.1.2 Test Parameters 1744

A.7.4.3.1.3 Test Requirements 1747

A.7.5 Signaling characteristics 1748

A.7.5.1 Radio link Monitoring 1748

A.7.5.1.1 Radio Link Monitoring Out-of-sync Test for FR2 PCell configured with SSB-based RLM RS in non-DRX mode 1748

A.7.5.1.1.1 Test Purpose and Environment 1748

A.7.5.1.1.2 Test Requirements 1751

A.7.5.1.2 Radio Link Monitoring In-sync Test for FR2 PCell configured with SSB-based RLM RS in non-DRX mode 1752

A.7.5.1.2.1 Test Purpose and Environment 1752

A.7.5.1.2.2 Test Requirements 1756

A.7.5.1.3 Radio Link Monitoring Out-of-sync Test for FR2 PCell configured with SSB-based RLM RS in DRX mode 1757

A.7.5.1.3.1 Test Purpose and Environment 1757

A.7.5.1.3.2 Test Requirements 1761

A.7.5.1.4 Radio Link Monitoring In-sync Test for FR2 PCell configured with SSB-based RLM RS in DRX mode 1761

A.7.5.1.4.1 Test Purpose and Environment 1761

A.7.5.1.4.2 Test Requirements 1766

A.7.5.1.5 Radio Link Monitoring Out-of-sync Test for FR2 PCell configured with CSI-RS-based RLM in non-DRX mode 1766

A.7.5.1.5.1 Test Purpose and Environment 1766

A.7.5.1.5.2 Test Requirements 1771

A.7.5.1.6 Radio Link Monitoring In-sync Test for FR2 PCell configured with CSI-RS-based RLM in non-DRX mode 1771

A.7.5.1.6.1 Test Purpose and Environment 1771

A.7.5.1.6.2 Test Requirements 1775

A.7.5.1.7 Radio Link Monitoring Out-of-sync Test for FR2 PCell configured with CSI-RS-based RLM in DRX mode 1775

A.7.5.1.7.1 Test Purpose and Environment 1775

A.7.5.1.7.2 Test Requirements 1779

A.7.5.1.8 Radio Link Monitoring In-sync Test for FR2 PCell configured with CSI-RS-based RLM in DRX mode 1779

A.7.5.1.8.1 Test Purpose and Environment 1779

A.7.5.1.8.2 Test Requirements 1784

A.7.5.1.9 UE Radio Link Monitoring Scheduling Restrictions on FR2 1784

A.7.5.1.9.1 Test Purpose and Environment 1784

A.7.5.1.9.2 Test Requirements 1787

A.7.5.2 Interruption 1787

A.7.5.2.1 Interruptions during measurements on deactivated NR SCC in FR2 1787

A.7.5.2.2 SA interruptions at NR SRS carrier-based switching 1791

A.7.5.2.2.1 Test Purpose and Environment 1791

A.7.5.2.2.2 Test Parameters 1791

A.7.5.2.2.3 Test Requirements 1793

A.7.5.3 SCell Activation and Deactivation Delay 1793

A.7.5.3.1 SCell Activation and deactivation for SCell in FR2 intra-band in non-DRX 1793

A.7.5.3.1.1 Test Purpose and Environment 1793

A.7.5.3.1.2 Test Requirements 1795

A.7.5.3.2 SCell Activation and deactivation for FR1+FR2 inter-band with target SCell in FR2 1795

A.7.5.3.2.1 Test Purpose and Environment 1795

A.7.5.3.2.2 Test Requirements 1799

A.7.5.3.3 SCell Activation and deactivation for SCell in FR2 inter-band in non-DRX 1800

A.7.5.3.3.1 Test Purpose and Environment 1800

A.7.5.3.3.2 Test Requirements 1803

A.7.5.3.4 Direct SCell activation at SCell addition of known SCell in FR2 1804

A.7.5.3.4.1 Test Purpose and Environment 1804

A.7.5.3.4.2 Test Requirements 1807

A.7.5.3.5 Direct SCell activation at handover with known SCell in FR2 1808

A.7.5.3.5.1 Test Purpose and Environment 1808

A.7.5.3.5.2 Test Requirements 1811

A.7.5.4 Void 1812

A.7.5.5 Beam Failure Detection and Link recovery procedures 1812

A.7.5.5.1 Beam Failure Detection and Link Recovery Test for FR2 PCell configured with SSB-based BFD and LR in non-DRX mode 1812

A.7.5.5.1.1 Test Purpose and Environment 1812

A.7.5.5.1.2 Test Requirements 1816

A.7.5.5.2 Beam Failure Detection and Link Recovery Test for FR2 PCell configured with SSB-based BFD and LR in DRX mode 1817

A.7.5.5.2.1 Test Purpose and Environment 1817

A.7.5.5.2.2 Test Requirements 1820

A.7.5.5.3 Beam Failure Detection and Link Recovery Test for FR2 PCell configured with CSI-RS-based BFD and LR in non-DRX mode 1821

A.7.5.5.3.1 Test Purpose and Environment 1821

A.7.5.5.3.2 Test Requirements 1825

A.7.5.5.4 Beam Failure Detection and Link Recovery Test for FR2 PCell configured with CSI-RS-based BFD and LR in DRX mode 1826

A.7.5.5.4.1 Test Purpose and Environment 1826

A.7.5.5.4.2 Test Requirements 1830

A.7.5.5.5 Scheduling availability restriction during Beam Failure Detection and Link Recovery for FR2 PCell configured with SSB-based BFD and LR in non-DRX mode 1831

A.7.5.5.5.1 Test Purpose and Environment 1831

A.7.5.5.5.2 Test Requirements 1834

A.7.5.5.6 Beam Failure Detection and Link Recovery Test for FR2 SCell configured with CSI-RS-based BFD and LR in non-DRX mode 1835

A.7.5.5.6.1 Test Purpose and Environment 1835

A.7.5.5.6.2 Test Requirements 1839

A.7.5.5.7 Beam Failure Detection and Link Recovery Test for FR2 SCell configured with CSI-RS-based BFD and LR in DRX mode 1840

A.7.5.5.7.1 Test Purpose and Environment 1840

A.7.5.5.7.2 Test Requirements 1844

A.7.5.6 Active BWP switch 1845

A.7.5.6.1 DCI-based and Timer-based Active BWP Switch 1845

A.7.5.6.1.1 NR FR2- NR FR2 DL active BWP switch of SCell with non-DRX in SA 1845

A.7.5.6.1.2 NR FR1- NR FR2 DL active BWP switch of SCell with non-DRX in SA A.7.5.6.1.2.1 Test Purpose and Environment 1849

A.7.5.6.1.3 NR FR2 DL active BWP switch with non-DRX in SA 1854

A.7.5.6.1.3.1 Test Purpose and Environment 1854

A.7.5.6.1.3.2 Test Requirements 1857

A.7.5.6.2 RRC-based Active BWP Switch 1857

A.7.5.6.3 Simultaneous DCI-based and Timer-based Active BWP Switch on multiple CCs 1861

A.7.5.6.3.1 Active BWP switch on multiple SCells with non-DRX in SA 1861

A.7.5.6.4 SCell dormancy switch 1864

A.7.5.6.4.1 NR FR2 PCell SCell dormancy switch of single FR2 SCell inside active time 1864

A.7.5.6.4.2 NR FR1 PCell SCell dormancy switch of two FR2 SCells outside active time 1869

A.7.5.6.4.2.2 Test Requirements 1874

A.7.5.6.5 Simultaneous RRC-based Active BWP Switch on multiple CCs 1874

A.7.5.6.5.1 Active BWP switch on multiple SCells with non-DRX in SA 1874

A.7.5.7 PSCell addition and release delay 1877

A.7.5.7.1 Addition and Release Delay of known NR PSCell 1877

A.7.5.7.1.1 Test Purpose and Environment 1877

A.7.5.7.2 Addition and Release Delay of unknown NR PSCell 1881

A.7.5.7.2.1 Test Purpose and Environment 1881

A.7.5.7.2.2 Test Requirements 1884

A.7.5.8 Active TCI state switch delay 1884

A.7.5.8.1 MAC-CE based active TCI state switch 1884

A.7.5.8.2 RRC based active TCI state switch 1888

A.7.5.9 Uplink spatial relation switch delay 1892

A.7.5.9.1 MAC-CE based Spatial Relation switch 1892

A.7.5.9.1.1 NR PCell FR2 spatial relation associated with known DL-RS 1892

A.7.5.9.1.1.2 Test Requirements 1895

A.7.5.9.2 RRC based spatial relation switch 1895

A.7.5.9.2.1 NR PCell FR2 spatial relation switch associated with a known DL-RS 1895

A.7.5.9.2.1.1 Test Purpose and Environment 1895

A.7.5.9.2.1.2 Test Requirements 1898

A.7.5.10 UE specific CBW change 1898

A.7.5.10.1 NR FR2 UE specific CBW change of PCell with non-DRX in SA 1898

A.7.5.10.1.1 Test Purpose and Environment 1898

A.7.5.10.1.2 Test Requirements 1901

A.7.6 Measurement procedure 1902

A.7.6.1 Intra-frequency Measurements 1902

A.7.6.1.1 SA event triggered reporting test without gap under non-DRX 1902

A.7.6.1.1.1 Test purpose and Environment 1902

A.7.6.1.1.2 Test Requirements 1904

A.7.6.1.2 SA event triggered reporting test without gap under DRX 1905

A.7.6.1.2.1 Test purpose and Environment 1905

A.7.6.1.2.2 Test Requirements 1907

A.7.6.1.3 SA event triggered reporting test with per-UE gaps under non-DRX 1908

A.7.6.1.3.1 Test purpose and Environment 1908

A.7.6.1.3.2 Test Requirements 1910

A.7.6.1.4 SA event triggered reporting test with per-UE gaps under DRX 1911

A.7.6.1.4.1 Test purpose and Environment 1911

A.7.6.1.4.2 Test Requirements 1914

A.7.6.2 Inter-frequency Measurements 1915

A.7.6.2.1 SA event triggered reporting tests For FR2 without SSB time index detection when DRX is not used (PCell in FR2) 1915

A.7.6.2.1.1 Test Purpose and Environment 1915

A.7.6.2.1.2 Test Requirements 1918

A.7.6.2.2 SA event triggered reporting tests For FR2 without SSB time index detection when DRX is used (PCell in FR2) 1918

A.7.6.2.2.1 Test Purpose and Environment 1918

A.7.6.2.2.2 Test Requirements 1922

A.7.6.2.3 SA event triggered reporting tests For FR2 with SSB time index detection when DRX is not used (PCell in FR2) 1922

A.7.6.2.3.1 Test Purpose and Environment 1922

A.7.6.2.3.2 Test Requirements 1926

A.7.6.2.4 SA event triggered reporting tests For FR2 with SSB time index detection when DRX is used (PCell in FR2) 1926

A.7.6.2.4.1 Test Purpose and Environment 1926

A.7.6.2.4.2 Test Requirements 1930

A.7.6.2.5 SA event triggered reporting tests for FR2 without SSB time index detection when DRX is not used (PCell in FR1) 1930

A.7.6.2.5.1 Test Purpose and Environment 1930

A.7.6.2.5.2 Test Requirements 1934

A.7.6.2.6 SA event triggered reporting tests for FR2 without SSB time index detection when DRX is used (PCell in FR1) 1935

A.7.6.2.6.1 Test Purpose and Environment 1935

A.7.6.2.6.2 Test Requirements 1939

A.7.6.2.7 SA event triggered reporting tests for FR2 with SSB time index detection when DRX is not used (PCell in FR1) 1940

A.7.6.2.7.1 Test Purpose and Environment 1940

A.7.6.2.7.2 Test Requirements 1944

A.7.6.2.8 SA event triggered reporting tests for FR2 with SSB time index detection when DRX is used (PCell in FR1) 1945

A.7.6.2.8.1 Test Purpose and Environment 1945

A.7.6.2.8.2 Test Requirements 1949

A.7.6.2.9 SA event triggered reporting tests For FR2 without SSB time index detection when DRX is not used (PCell in FR2) (rel16 additional mandatory gap pattern 17) 1950

A.7.6.2.9.1 Test Purpose and Environment 1950

A.7.6.2.9.2 Test Requirements 1953

A.7.6.2.10 SA event triggered reporting test without gap under non-DRX 1953

A.7.6.2.10.1 Test Purpose and Environment 1953

A.7.6.2.10.2 Test Requirements 1955

A.7.6.2.11 SA event triggered reporting test without gap under DRX 1955

A.7.6.2.11.1 Test Purpose and Environment 1955

A.7.6.2.11.2 Test Requirements 1958

A.7.6.3 L1-RSRP measurement for beam reporting 1959

A.7.6.3.1 SSB based L1-RSRP measurement when DRX is not used 1959

A.7.6.3.1 SSB based L1-RSRP measurement when DRX is not used 1959

A.7.6.3.1.1 Test Purpose and Environment 1959

A.7.6.3.1.2 Test parameters 1959

A.7.6.3.1.3 Test Requirements 1961

A.7.6.3.2 SSB based L1-RSRP measurement when DRX is used 1961

A.7.6.3.2.1 Test Purpose and Environment 1961

A.7.6.3.2.2 Test parameters 1962

A.7.6.3.2.3 Test Requirements 1964

A.7.6.3.3 CSI-RS based L1-RSRP measurement when DRX is not used 1964

A.7.6.3.3.1 Test Purpose and Environment 1964

A.7.6.3.3.2 Test parameters 1965

A.7.6.3.3.3 Test Requirements 1967

A.7.6.3.4 CSI-RS based L1-RSRP measurement when DRX is used 1968

A.7.6.3.4.1 Test Purpose and Environment 1968

A.7.6.3.4.2 Test parameters 1968

A.7.6.3.3.3 Test Requirements 1970

A.7.6.4 CLI measurements 1971

A.7.6.4.1 SRS-RSRP measurement with non-DRX 1971

A.7.6.4.1.1 Test Purpose and Environment 1971

A.7.6.4.1.2 Test Parameters 1971

A.7.6.4.1.3 Test Requirements 1973

A.7.6.4.2 CLI-RSSI measurement with non-DRX 1973

A.7.6.4.2.1 Test Purpose and Environment 1973

A.7.6.4.2.2 Test Parameters 1974

A.7.6.4.2.3 Test Requirements 1975

A.7.6.5 NR Measurements with autonomous gaps 1976

A.7.6.5.1 SA interfrequency CGI reporting in autonomous gaps test (PCell in FR2) 1976

A.7.6.5.1.1 Test Purpose and Environment 1976

A.7.6.5.1.2 Test Requirements 1979

A.7.6.6 L1-SINR measurement for beam reporting 1979

A.7.6.6.1 L1-SINR measurement with CSI-RS based CMR and no dedicated IMR configured when DRX is not used 1979

A.7.6.6.1.1 Test Purpose and Environment 1979

A.7.6.6.1.2 Test parameters 1979

A.7.6.6.1.3 Test Requirements 1981

A.7.6.6.2 L1-SINR measurement with SSB based CMR and dedicated IMR when DRX is used 1981

A.7.6.6.2.1 Test Purpose and Environment 1981

A.7.6.6.2.2 Test parameters 1982

A.7.6.6.2.3 Test Requirements 1984

A.7.6.6.3 L1-SINR measurement with CSI-RS based CMR and dedicated IMR configured when DRX is used 1984

A.7.6.6.3.1 Test Purpose and Environment 1984

A.7.6.6.3.2 Test parameters 1985

A.7.6.6.3.3 Test Requirements 1987

A.7.6.7 CSI-RS based intra-frequency Measurements 1987

A.7.6.7.1 SA event triggered reporting test without gap under DRX for CSI-RS based intra-frequency measurement 1987

A.7.6.7.1.1 Test purpose and Environment 1987

A.7.6.7.1.2 Test Requirements 1990

A.7.6.8 CSI-RS based inter-frequency Measurements 1990

A.7.6.8.1 SA event triggered reporting tests for FR2 CSI-RS based measurement when non-DRX is used (PCell in FR2) 1990

A.7.6.8.1.1 Test Purpose and Environment 1990

A.7.6.2.2.2 Test Requirements 1994

A.7.6.9 RSTD measurements 1994

A.7.6.9.1 NR RSTD measurement reporting delay test case for single positioning frequency layer in FR2 SA 1994

A.7.6.9.1.1 Test Purpose and Environment 1994

A.7.6.9.1.2 Test Requirements 2000

A.7.6.9.2 NR RSTD measurement reporting delay test case for dual positioning frequency layers in FR2 SA 2000

A.7.6.9.2.1 Test Purpose and Environment 2000

A.7.6.9.2.2 Test Requirements 2007

A.7.6.10 PRS-RSRP measurements 2007

A.7.6.10.1 PRS-RSRP reporting delay test case for single positioning frequency layer 2007

A.7.6.10.1.1 Test Purpose and Environment 2007

A.7.6.10.1.2 Test Requirements 2011

A.7.6.10.2 PRS-RSRP reporting delay test case for dual positioning frequency layer 2011

A.7.6.10.2.1 Test Purpose and Environment 2011

A.7.6.10.2.2 Test Requirements 2014

A.7.6.11 UE Rx-Tx time difference measurements 2014

A.7.6.11.1 UE Rx-Tx time difference measurements for single positioning frequency layer in FR2 SA 2014

A.7.6.11.1.1 Test purpose and environment 2014

A.7.6.11.1.2 Test requirements 2018

A.7.6.11.2 UE Rx-Tx time difference measurement period for dual positioning frequency layers in FR2 SA 2018

A.7.6.11.2.1 Test purpose and environment 2018

A.7.6.11.2.2 Test requirements 2022

A.7.7 Measurement Performance requirements 2022

A.7.7.1 SS-RSRP 2022

A.7.7.1.1 SA intra-frequency case measurement accuracy with FR2 serving cell and FR2 target cell 2022

A.7.7.1.1.1 Test Purpose and Environment 2022

A.7.7.1.1.2 Test parameters 2023

A.7.7.1.1.3 Test Requirements 2027

A.7.7.1.2 SA inter-frequency case measurement accuracy with FR2 serving cell and FR2 target cell 2027

A.7.7.1.2.1 Test Purpose and Environment 2027

A.7.7.1.2.2 Test parameters 2028

A.7.7.1.2.3 Test Requirements 2032

A.7.7.1.3 SA inter-frequency measurement accuracy with FR1 serving cell and FR2 target cell 2033

A.7.7.1.3.1 Test Purpose and Environment 2033

A.7.7.1.3.2 Test parameters 2033

A.7.7.1.3.3 Test Requirements 2037

A.7.7.2 SS-RSRQ 2037

A.7.7.2.1 SA intra-frequency measurement accuracy with FR2 serving cell and FR2 target cell 2037

A.7.7.2.1.1 Test Purpose and Environment 2037

A.7.7.2.1.2 Test Parameters 2037

A.7.7.2.1.3 Test Requirements 2039

A.7.7.2.2 SA Inter-frequency measurement accuracy with FR2 serving cell and FR2 TDD target cell 2039

A.7.7.2.2.1 Test Purpose and Environment 2039

A.7.7.2.2.2 Test Parameters 2039

A.7.7.2.2.3 Test Requirements 2041

A.7.7.3 SS-SINR 2041

A.7.7.3.1 SA intra-frequency case measurement accuracy with FR2 serving cell and FR2 target cell 2041

A.7.7.3.1.1 Test Purpose and Environment 2041

A.7.7.3.1.2 Test Parameters 2041

A.7.7.3.1.3 Test Requirements 2044

A.7.7.3.2 SA Inter-frequency measurement accuracy with FR2 serving cell and FR2 TDD target cell 2044

A.7.7.3.2.1 Test Purpose and Environment 2044

A.7.7.3.2.2 Test Parameters 2044

A.7.7.3.2.3 Test Requirements 2046

A.7.7.4 L1-RSRP measurement for beam reporting 2046

A.7.7.4.1 SSB based L1-RSRP measurement 2046

A.7.7.4.1.1 Test Purpose and Environment 2046

A.7.7.4.1.2 Test parameters 2047

A.7.7.4.1.3 Test Requirements 2049

A.7.7.4.2 CSI-RS based L1-RSRP measurement on resource set with repetition off 2050

A.7.7.4.2.1 Test Purpose and Environment 2050

A.7.7.4.2.2 Test parameters 2050

A.7.7.4.2.3 Test Requirements 2052

A.7.7.5 CLI measurements 2053

A.7.7.5.1 SA SRS-RSRP measurement accuracy with FR2 serving cell 2053

A.7.7.5.1.1 Test Purpose and Environment 2053

A.7.7.5.1.2 Test parameters 2053

A.7.7.5.1.3 Test Requirements 2056

A.7.7.5.2 SA CLI-RSSI measurement accuracy with FR2 serving cell 2057

A.7.7.5.2.1 Test Purpose and Environment 2057

A.7.7.5.2.2 Test parameters 2057

A.7.7.5.2.3 Test Requirements 2059

A.7.7.6 L1-SINR measurement for beam reporting 2060

A.7.7.6.1 L1-SINR measurement with CSI-RS based CMR and no dedicated IMR configured and CSI-RS resource set with repetition off 2060

A.7.7.6.1.1 Test Purpose and Environment 2060

A.7.7.6.1.2 Test parameters 2060

A.7.7.6.1.3 Test Requirements 2062

A.7.7.6.2 L1-SINR measurement with SSB based CMR and dedicated IMR 2063

A.7.7.6.2.1 Test Purpose and Environment 2063

A.7.7.6.2.2 Test parameters 2063

A.7.7.6.2.3 Test Requirements 2065

A.7.7.6.3 L1-SINR measurement with CSI-RS based CMR and dedicated IMR 2066

A.7.7.6.3.1 Test Purpose and Environment 2066

A.7.7.6.3.2 Test parameters 2066

A.7.7.6.3.3 Test Requirements 2068

A.7.7.7 CSI-RSRP 2069

A.7.7.7.1 SA intra-frequency case measurement accuracy with FR2 serving cell and FR2 target cell 2069

A.7.7.7.1.1 Test Purpose and Environment 2069

A.7.7.7.1.2 Test parameters 2069

A.7.7.7.1.3 Test Requirements 2072

A.7.7.7.2 SA inter-frequency case measurement accuracy with FR2 serving cell and FR2 target cell 2073

A.7.7.7.2.1 Test Purpose and Environment 2073

A.7.7.7.2.2 Test parameters 2073

A.7.7.7.2.3 Test Requirements 2076

A.7.7.8 CSI-RSRQ 2077

A.7.7.8.1 SA intra-frequency measurement accuracy with FR2 serving cell and FR2 target cell 2077

A.7.7.8.1.1 Test Purpose and Environment 2077

A.7.7.8.1.2 Test Parameters 2077

A.7.7.8.1.3 Test Requirements 2079

A.7.7.8.2 SA Inter-frequency measurement accuracy with FR2 serving cell and FR2 TDD target cell 2079

A.7.7.8.2.1 Test Purpose and Environment 2079

A.7.7.8.2.2 Test Parameters 2079

A.7.7.8.2.3 Test Requirements 2081

A.7.7.9 CSI-SINR 2081

A.7.7.9.1 SA intra-frequency case measurement accuracy with FR2 serving cell and FR2 target cell 2081

A.7.7.9.1.1 Test Purpose and Environment 2081

A.7.7.9.1.2 Test Parameters 2081

A.7.7.9.1.3 Test Requirements 2084

A.7.7.9.2 SA Inter-frequency measurement accuracy with FR2 serving cell and FR2 TDD target cell 2084

A.7.7.9.2.2 Test Parameters 2084

A.7.7.9.2.3 Test Requirements 2086

A.7.7.10 RSTD measurements 2086

A.7.7.10.1 RSTD measurement accuracy test case for single positioning frequency layer 2086

A.7.7.10.1.1 Test purpose and Environment 2086

A.7.7.10.1.2 Test Requirements 2089

A.7.7.10.2 RSTD measurement accuracy test case for dual positioning frequency layer 2089

A.7.7.10.2.1 Test purpose and Environment 2089

A.7.7.10.2.2 Test Requirements 2092

A.7.7.11 PRS-RSRP measurements 2092

A.7.7.11.1 SA measurement accuracy with PRS in FR2 2092

A.7.7.11.1.1 Test Purpose and Environment 2092

A.7.7.11.1.2 Test parameters 2092

A.7.7.11.1.3 Test Requirements 2096

A.7.7.12 UE Rx-Tx time difference measurements 2097

A.7.7.12.1 UE Rx-Tx time difference measurement accuracy for single positioning frequency layer in FR2 SA 2097

A.7.7.12.1.1 Test purpose and environment 2097

A.7.7.12.1.2 Test parameters 2097

A.7.7.12.1.3 Test requirements 2100

A.8 E-UTRA standalone tests for NR RRM 2100

A.8.1 Void 2101

A.8.2 RRC\_IDLE state mobility 2101

A.8.2.1 Inter-RAT NR Cell re-selection 2101

A.8.2.1.1 E-UTRA Cell reselection to higher priority NR target Cell in FR1 2101

A.8.2.1.1.1 Test Purpose and Environment 2101

A.8.2.1.1.2 Test Requirements 2106

A.8.2.1.2 E-UTRA Cell reselection to lower priority NR target Cell in FR1 for UE configured with highSpeedInterRAT-NR-r16 2107

A.8.2.1.2.1 Test Purpose and Environment 2107

A.8.2.1.2.2 Test Requirements 2112

A.8.2.2 E-UTRA – NR Inter-RAT Early Measruement Reporting 2113

A.8.2.2.1 E-UTRA – NR Early Measurement Reporting for NR in FR1 2113

A.8.2.2.1.1 Test Purpose and Environment 2113

A.8.2.2.1.2 Test Requirements 2118

A.8.2.2.2 E-UTRA – NR Early Measurement Reporting for NR in FR2 2118

A.8.2.2.2.1 Test Purpose and Environment 2118

A.8.2.2.2.2 Test Requirements 2121

A.8.3 RRC\_CONNECTED state mobility 2122

A.8.3.1 Handover 2122

A.8.3.1.1 E-UTRAN - NR handover in FR1 2122

A.8.3.1.1.1 Test Purpose and Environment 2122

A.8.3.1.1.2 Test Requirements 2127

A.8.4 Measurement procedure 2127

A.8.4.1 E-UTRA – NR Inter-RAT SFTD Measurement Delay 2127

A.8.4.1.1 E-UTRA – NR Inter-RAT SFTD Measurement Delay in non-DRX 2127

A.8.4.1.1.1 Test Purpose and Environment 2127

A.8.4.1.1.2 Test Requirements 2129

A.8.4.1.2 E-UTRA – NR Inter-RAT SFTD Measurement Delay in DRX 2130

A.8.4.1.2.1 Test Purpose and Environment 2130

A.8.4.1.2.2 Test Requirements 2131

A.8.4.2 E-UTRA – NR Inter-RAT Measurements 2131

A.8.4.2.1 NR Inter-RAT event triggered reporting tests for FR1 without SSB time index detection when DRX is not used 2131

A.8.4.2.1.1 Test Purpose and Environment 2131

A.8.4.2.1.2 Test Requirements 2136

A.8.4.2.2 NR Inter-RAT event triggered reporting tests for FR1 without SSB time index detection when DRX is used 2136

A.8.4.2.2.1 Test Purpose and Environment 2136

A.8.4.2.2.2 Test Requirements 2140

A.8.4.2.3 NR Inter-RAT event triggered reporting tests for FR1 with SSB time index detection when DRX is not used 2140

A.8.4.2.3.1 Test Purpose and Environment 2140

A.8.4.2.3.2 Test Requirements 2145

A.8.4.2.4 NR Inter-RAT event triggered reporting tests for FR1 with SSB time index detection when DRX is used 2145

A.8.4.2.4.1 Test Purpose and Environment 2145

A.8.4.2.4.2 Test Requirements 2149

A.8.4.2.5 NR Inter-RAT event triggered reporting tests for FR2 without SSB time index detection when DRX is not used 2149

A.8.4.2.5.1 Test Purpose and Environment 2149

A.8.4.2.5.2 Test Requirements 2151

A.8.4.2.6 NR Inter-RAT event triggered reporting tests for FR2 without SSB time index detection when DRX is used 2152

A.8.4.2.6.1 Test Purpose and Environment 2152

A.8.4.2.6.2 Test Requirements 2154

A.8.4.2.7 NR Inter-RAT event triggered reporting tests for FR2 with SSB time index detection when DRX is not used 2155

A.8.4.2.7.1 Test Purpose and Environment 2155

A.8.4.2.7.2 Test Requirements 2157

A.8.4.2.8 NR Inter-RAT event triggered reporting tests for FR2 with SSB time index detection when DRX is used 2158

A.8.4.2.8.1 Test Purpose and Environment 2158

A.8.4.2.8.2 Test Requirements 2160

A.8.4.2.9 NR Inter-RAT event triggered reporting tests for FR1 with SSB time index detection in DRX for UE configured with highSpeedInterRAT-NR-r16 2161

A.8.4.2.9.1 Test Purpose and Environment 2161

A.8.4.2.9.2 Test Requirements 2167

A.8.5 Measurement performance 2167

A.8.5.1 SFTD accuracy 2167

A.8.5.1.1 SFTD accuracy 2167

A.8.5.1.1.1 Test Purpose 2167

A.8.5.1.1.2 Test Environment 2167

A.8.5.1.1.3 Test Requirements 2173

A.8.5.2 E-UTRA – NR Inter-RAT Measurement Performance requirements 2173

A.8.5.2.1.1 E-UTRAN – NR inter-RAT measurements with FR1 target cell 2173

A.8.5.2.1.2 E-UTRAN – NR inter-RAT measurements with FR2 target cell 2178

A.8.5.2.1.2.1 Test Purpose and Environment 2178

A.8.5.2.1.2.2 Test Parameters 2178

A.8.5.2.1.2.3 Test Requirements 2180

A.8.5.2.2 SS-RSRQ 2180

A.8.5.2.2.1 E-UTRAN – NR inter-RAT measurements with FR1 target cell 2180

A.8.5.2.2.2 E-UTRAN – NR inter-RAT measurements with FR2 target cell 2185

A.8.5.2.2.2.1 Test Purpose and Environment 2185

A.8.5.2.2.2.2 Test Parameters 2185

A.8.5.2.2.2.3 Test Requirements 2187

A.8.5.2.3 SS-SINR 2187

A.8.5.2.3.1 E-UTRAN – NR inter-RAT measurements with FR1 target cell 2187

A.8.5.2.3.2 E-UTRAN – NR inter-RAT measurements with FR2 target cell 2191

A.8.5.2.3.2.1 Test Purpose and Environment 2191

A.8.5.2.3.2.2 Test Parameters 2191

A.8.5.2.3.2.3 Test Requirements 2193

A.9 V2X Tests 2194

A.9.1 V2X Tests in FR1 2194

A.9.1.1 Test for V2X UE Transmit Timing 2194

A.9.1.1.1 Test for GNSS as Synchronization Reference Source 2194

A.9.1.1.1.1 Test Purpose and Environment 2194

A.9.1.1.1.2 Test requirements 2194

A.9.1.1.2 Test for SyncRef UE as Synchronization Reference Source 2194

A.9.1.1.2.1 Test Purpose and Environment 2194

A.9.1.1.2.2 Test requirements 2195

A.9.1.1.3 Test for FR1 NR Cell as Synchronization Reference Source 2195

A.9.1.1.3.1 Test Purpose and Environment 2195

A.9.1.1.3.2 Test requirements 2198

A.9.1.2 Test for Initiation/Cease of S-SSB Transmission with V2X Sidelink Communication 2198

A.9.1.2.1 Test for FR1 NR Cell as synchronization reference source without gap under non-DRX 2198

A.9.1.2.1.1 Test Purpose and Environment 2198

A.9.1.2.1.2 Test Requirements 2202

A.9.1.2.2 Test for SyncRef UE as synchronization reference source 2202

A.9.1.2.2.1 Test Purpose and Environment 2202

A.9.1.2.2.2 Test Requirements 2203

A.9.1.3 Test for V2X Synchronization Reference Selection/Reselection 2204

A.9.1.3.1 Test for GNSS configured as the highest priority 2204

A.9.1.3.1.1 Test Purpose and Environment 2204

A.9.1.3.1.2 Test Requirements 2206

A.9.1.3.2 Test for FR1 NR Cell configured as the highest priority 2208

A.9.1.3.2.1 Test Purpose and Environment 2208

A.9.1.3.2.2 Test Requirements 2210

A.9.1.4 Test for L1 SL-RSRP Measurement 2211

A.9.1.4.1 Test for V2X UE Autonomous Resource Selection/Reselection 2211

A.9.1.4.1.1 Test Purpose and Environment 2211

A.9.1.4.1.2 Test Requirements 2214

A.9.1.4.2 Test for V2X UE Resource Pre-emption 2215

A.9.1.4.2.1 Test Purpose and Environment 2215

A.9.1.4.2.2 Test Requirements 2218

A.9.1.4.3 Test for V2X UE Resource Re-evaluation 2218

A.9.1.4.3.1 Test Purpose and Environment 2218

A.9.1.4.3.2 Test Requirements 2225

A.9.1.5 Test for Congestion Control Measurement 2225

A.9.1.5.1 Test Purpose and Environment 2225

A.9.1.5.2 Test Requirements 2231

A.9.1.6 Test for Interruption 2231

A.9.1.6.1 Test for Interruption to WAN due to V2X Sidelink Communication 2231

A.9.1.6.1.1 Test Purpose and Environment 2231

A.9.1.6.1.2 Test Requirements 2234

A.10 EN-DC Tests with NR PSCell under CCA and Other NR Cells in FR1 2234

A.10.1 RRC\_CONNECTED state mobility 2234

A.10.1.1 RRC connection mobility control 2234

A.10.1.1.1 Random Access 2234

A.10.1.1.1.1 4-step RA type contention-based random access for NR PSCell with CCA 2234

A.10.1.1.1.1.1 Test Purpose and Environment 2234

A.10.1.1.1.1.2 Test Requirements 2237

A.10.1.1.1.1.2.1 Random Access Preamble Transmission 2237

A.10.1.1.1.1.2.2 Random Access Response Reception 2237

A.10.1.1.1.1.2.3 No Random Access Response Reception 2238

A.10.1.1.1.1.2.4 Receiving an UL grant for msg3 retransmission 2238

A.10.1.1.1.1.2.5 Contention Resolution Timer expiry 2238

A.10.1.1.1.2 4-step RA type non-contention based random access for NR PSCell with CCA 2239

A.10.1.1.1.2.1 Test Purpose and Environment 2239

A.10.1.1.1.2.2 Test Requirements 2242

A.10.1.1.1.2.2.1 SSB-based Random Access Preamble Transmission 2242

A.10.1.1.1.2.2.2 Random Access Response Reception 2243

A.10.1.1.1.2.2.3 No Random Access Response Reception 2243

A.10.1.1.1.3 2-step RA type contention-based random access for NR PSCell with CCA 2243

A.10.1.1.1.3.1 Test Purpose and Environment 2243

A.10.1.1.1.3.2 Test Requirements 2247

A.10.1.1.1.3.2.1 MsgA Transmission 2247

A.10.1.1.1.3.2.2 MsgB Reception 2247

A.10.1.1.1.3.2.3 No MsgB Reception 2248

A.10.1.1.1.4 2-step RA type non-contention based random access for NR PSCell with CCA 2248

A.10.1.1.1.4.1 Test Purpose and Environment 2248

A.10.1.1.1.4.2 Test Requirements 2252

A.10.1.1.1.4.2.1 MsgA Transmission 2252

A.10.1.1.1.4.2.2 MsgB Reception 2253

A.10.1.1.1.4.2.3 No MsgB Reception 2253

A.10.2 Timing 2254

A.10.2.1 UE transmit timing 2254

A.10.2.2 UE timing advance 2258

A.10.3 Signalling characteristics 2261

A.10.3.1 Radio link monitoring 2261

A.10.3.1.1 Introduction 2261

A.10.3.1.2 Radio link monitoring out-of-sync test for PSCell configured with SSB-based RLM RS in non-DRX mode 2262

A.10.3.1.2.1 Test purpose and environment 2262

A.10.3.1.2.2 Test requirements 2267

A.10.3.1.3 Radio link monitoring in-sync test for PSCell configured with SSB-based RLM RS in non-DRX mode 2267

A.10.3.1.3.1 Test purpose and environment 2267

A.10.3.1.3.2 Test requirements 2273

A.10.3.1.4 Void 2273

A.10.3.1.4.1 Void 2273

A.10.3.1.4.2 Void 2273

A.10.3.1.5 Void 2273

A.10.3.1.5.1 Void 2273

A.10.3.1.5.2 Void 2273

A.10.3.2 Interruption 2273

A.10.3.2.1 E-UTRAN – NR interruptions during SCell operations with CCA 2273

A.10.3.2.1.1 Test Purpose and Environment 2273

A.10.3.2.1.2 Test Requirements 2278

A.10.3.3 SCell activation and deactivation delay 2278

A.10.3.3.2 SCell Activation and Deactivation of known NR SCell with NR PSCell and NR SCell under CCA, 640 ms SCell measurement cycle 2283

A.10.3.3.2.1 Test Purpose and Environment 2283

A.10.3.3.2.2 Test Requirements 2284

A.10.3.3.3 SCell Activation and Deactivation of unknown NR SCell with NR PSCell and NR SCell under CCA 2284

A.10.3.3.3.1 Test Purpose and Environment 2284

A.10.3.3.3.2 Test Requirements 2285

A.10.3.4 Beam failure detection and link recovery procedures 2285

A.10.3.4.1 EN-DC Beam Failure Detection and Link Recovery Test for FR1 PSCell configured with SSB-based BFD and LR in non-DRX mode 2285

A.10.3.4.1.1 Test Purpose and Environment 2285

A.10.3.4.1.2 Test Requirements 2290

A.10.3.4.2 EN-DC Beam Failure Detection and Link Recovery Test for FR1 PSCell configured with SSB-based BFD and LR in DRX mode 2290

A.10.3.4.2.1 Test Purpose and Environment 2290

A.10.3.4.2.2 Test Requirements 2296

A.10.3.5 Active BWP switching 2296

A.10.3.5.1 UL active BWP switch delay with consistent UL LBT failure on PSCell subject to UL CCA in EN-DC 2296

A.10.3.5.1.1 Test Purpose and Environment 2296

A.10.3.5.1.2 Test Requirements 2301

A.10.3.5.2 DCI-based and Timer-based Active BWP Switch 2302

A.10.3.5.2.1 E-UTRAN – NR PSCell FR1 DL active BWP switch in non-DRX in synchronous EN-DC 2302

A.10.3.5.2.2 E-UTRAN – NR PSCell FR1 DL active BWP switch with FR1 SCell in non-DRX in synchronous EN-DC 2305

A.10.3.5.3 RRC-based Active BWP Switch 2309

A.10.3.6 PSCell addition and release delay 2313

A.10.3.6.1 Addition and Release Delay of known NR PSCell on the carrier under CCA 2313

A.10.3.6.1.1 Test purpose and environment 2313

A.10.3.6.1.2 Test Requirements 2318

A.10.3.7 Void 2319

A.10.4 Measurement procedure 2319

A.10.4.1 Intra-frequency measurements 2319

A.10.4.1.1 Event-triggered reporting tests on PSCC without gaps under non-DRX 2319

A.10.4.1.1.1 Test purpose and environment 2319

A.10.4.1.1.2 Test parameters 2319

A.10.4.1.1.3 Test Requirements 2319

A.10.4.1.2 Event-triggered reporting tests on PSCC without gaps under DRX 2320

A.10.4.1.2.1 Test purpose and environment 2320

A.10.4.1.2.2 Test parameters 2320

A.10.4.1.2.3 Test Requirements 2320

A.10.4.1.3 Event-triggered reporting tests on PSCC with per-UE gaps under non-DRX 2320

A.10.4.1.3.1 Test purpose and environment 2320

A.10.4.1.3.2 Test parameters 2320

A.10.4.1.3.3 Test Requirements 2320

A.10.4.1.4 Event-triggered reporting tests on PSCC with per-UE gaps under DRX 2321

A.10.4.1.4.1 Test purpose and environment 2321

A.10.4.1.4.2 Test parameters 2321

A.10.4.1.4.3 Test Requirements 2321

A.10.4.1.5 Event-triggered reporting tests on SCC without gaps under non-DRX 2321

A.10.4.1.5.1 Test purpose and environment 2321

A.10.4.1.5.2 Test parameters 2321

A.10.4.1.5.3 Test Requirements 2321

A.10.4.1.6 Event-triggered reporting tests on SCC without gaps under DRX 2322

A.10.4.1.6.1 Test purpose and environment 2322

A.10.4.1.6.2 Test parameters 2322

A.10.4.1.6.3 Test Requirements 2322

A.10.4.1.7 Event-triggered reporting tests on SCC with per-UE gaps under non-DRX 2322

A.10.4.1.7.1 Test purpose and environment 2322

A.10.4.1.7.2 Test parameters 2322

A.10.4.1.7.3 Test Requirements 2322

A.10.4.1.8 Event-triggered reporting tests on SCC with per-UE gaps under DRX 2323

A.10.4.1.8.1 Test purpose and environment 2323

A.10.4.1.8.2 Test parameters 2323

A.10.4.1.8.3 Test Requirements 2323

A.10.4.1.9 RSSI measurement reporting on PSCC 2323

A.10.4.1.9.1 Test purpose and environment 2323

A.10.4.1.9.2 Test parameters 2323

A.10.4.1.10 Channel occupancy measurement reporting on PSCC 2324

A.10.4.1.10.1 Test purpose and environment 2324

A.10.4.1.10.2 Test parameters 2324

A.10.4.1.11 RSSI measurement reporting on SCC 2324

A.10.4.1.11.1 Test purpose and environment 2324

A.10.4.1.11.2 Test parameters 2324

A.10.4.1.12 Channel occupancy measurement reporting on SCC 2325

A.10.4.1.12.1 Test purpose and environment 2325

A.10.4.1.12.2 Test parameters 2325

A.10.4.2 Inter-frequency measurements 2325

A.10.4.2.1 RSSI measurement reporting 2325

A.10.4.2.1.1 Test purpose and environment 2325

A.10.4.2.1.2 Test parameters 2325

A.10.4.2.2 Channel occupancy measurement reporting 2326

A.10.4.2.2.1 Test purpose and environment 2326

A.10.4.2.2.2 Test parameters 2326

A.10.4.2.3 EN-DC event triggered reporting tests for FR1 with CCA cell without SSB time index detection when DRX is not used 2326

A.10.4.2.3.1 Test Purpose and Environment 2326

A.10.4.2.3.2 Test Requirements 2331

A.10.4.2.4 EN-DC event triggered reporting tests for FR1 cell with CCA without SSB time index detection when DRX is used 2332

A.10.4.2.4.1 Test Purpose and Environment 2332

A.10.4.2.4.2 Test Requirements 2336

A.10.4.2.5 EN-DC event triggered reporting tests for FR1 cell with CCA with SSB time index detection when DRX is not used 2337

A.10.4.2.5.1 Test Purpose and Environment 2337

A.10.4.2.5.2 Test Requirements 2341

A.10.4.2.6 EN-DC event triggered reporting tests for FR1 cell with CCA with SSB time index detection when DRX is used 2342

A.10.4.2.6.1 Test Purpose and Environment 2342

A.10.4.2.6.2 Test Requirements 2346

A.10.4.2.7 EN-DC event triggered reporting tests for FR1 cell without SSB time index detection when DRX is not used 2347

A.10.4.2.7.1 Test Purpose and Environment 2347

A.10.4.2.7.2 Test Requirements 2353

A.10.4.2.8 EN-DC event triggered reporting tests for FR1 cell without SSB time index detection when DRX is used 2353

A.10.4.2.8.1 Test Purpose and Environment 2353

A.10.4.2.8.2 Test Requirements 2359

A.10.4.2.9 EN-DC event triggered reporting tests for FR1 cell with SSB time index detection when DRX is not used 2360

A.10.4.2.9.1 Test Purpose and Environment 2360

A.10.4.2.9.2 Test Requirements 2365

A.10.4.2.10 EN-DC event triggered reporting tests for FR1 cell with SSB time index detection when DRX is used 2365

A.10.4.2.10.1 Test Purpose and Environment 2365

A.10.4.2.10.2 Test Requirements 2371

A.10.4.3 L1-RSRP measurements for beam reporting 2372

A.10.4.3.1 SSB based L1-RSRP measurement on PSCC when DRX is not used 2372

A.10.4.3.1.1 Test Purpose and Environment 2372

A.10.4.3.1.2 Test parameters 2372

A.10.4.3.1.3 Test Requirements 2374

A.10.4.3.2 SSB based L1-RSRP measurement on PSCC when DRX is used 2375

A.10.4.3.2.1 Test Purpose and Environment 2375

A.10.4.3.2.2 Test parameters 2375

A.10.4.3.2.3 Test Requirements 2377

A.10.4.3.3 SSB based L1-RSRP measurement on SCC when DRX is not used 2378

A.10.4.3.3.1 Test Purpose and Environment 2378

A.10.4.3.3.2 Test parameters 2378

A.10.4.3.3.3 Test Requirements 2381

A.10.4.3.4 SSB based L1-RSRP measurement on SCC when DRX is used 2382

A.10.4.3.4.1 Test Purpose and Environment 2382

A.10.4.3.4.2 Test parameters 2382

A.10.4.3.4.3 Test Requirements 2385

A.10.4.4 E-UTRAN−NR inter-RAT measurements on NR carrier frequency under CCA 2386

A.10.4.4.1 E-UTRA-NR inter-RAT event triggered reporting tests for FR1 without SSB time index detection when DRX is not used 2386

A.10.4.4.1.1 Test Purpose and Environment 2386

A.10.4.4.1.2 Test Requirements 2390

A.10.4.4.2 E-UTRA-NR inter-RAT event triggered reporting tests for FR1 without SSB time index detection when DRX is used 2391

A.10.4.4.2.1 Test Purpose and Environment 2391

A.10.4.4.2.2 Test Requirements 2396

A.10.4.4.3 NR Inter-RAT event triggered reporting tests for FR1 with SSB time index detection when DRX is not used 2397

A.10.4.4.3.1 Test Purpose and Environment 2397

A.10.4.4.3.2 Test Requirements 2401

A.10.4.4.4 NR Inter-RAT event triggered reporting tests for FR1 with SSB time index detection when DRX is used 2402

A.10.4.4.4.1 Test Purpose and Environment 2402

A.10.4.4.4.2 Test Requirements 2407

A.10.5 Measurement performance 2408

A.10.5.1 SS-RSRP 2408

A.10.5.1.1 Intra-frequency measurement accuracy on a CCA serving cell 2408

A.10.5.1.1.1 Test Purpose and Environment 2408

A.10.5.1.1.2 Test parameters 2408

A.10.5.1.1.3 Test Requirements 2411

A.10.5.1.2 Inter-frequency measurement accuracy with FR1 CCA serving cell and FR1 CCA target cell 2411

A.10.5.1.2.1 Test Purpose and Environment 2411

A.10.5.1.2.2 Test parameters 2411

A.10.5.1.2.3 Test Requirements 2415

A.10.5.2 SS-RSRQ 2415

A.10.5.2.1 Intra-frequency measurement accuracy with FR1 CCA serving cell and FR1 CCA target cell 2415

A.10.5.2.1.1 Test Purpose and Environment 2415

A.10.5.2.1.2 Test Parameters 2415

A.10.5.2.1.3 Test Requirements 2418

A.10.5.2.2 Inter-frequency measurement accuracy with FR1 CCA serving cell and FR1 CCA target cell 2418

A.10.5.2.2.1 Test Purpose and Environment 2418

A.10.5.2.2.2 Test Parameters 2418

A.10.5.2.2.3 Test Requirements 2421

A.10.5.3 SS-SINR 2421

A.10.5.3.1 Intra-frequency measurement accuracy on PSCC 2421

A.10.5.3.1.1 Test Purpose and Environment 2421

A.10.5.3.1.2 Test Parameters 2421

A.10.5.3.1.3 Test Requirements 2424

A.10.5.3.2 Inter-frequency measurement accuracy on PSCC 2424

A.10.5.3.2.1 Test Purpose and Environment 2424

A.10.5.3.2.2 Test Parameters 2424

A.10.5.3.2.3 Test Requirements 2428

A.10.5.3.3 Intra-frequency measurement accuracy on SCC 2428

A.10.5.3.3.1 Test Purpose and Environment 2428

A.10.5.3.3.2 Test Parameters 2428

A.10.5.3.3.3 Test Requirements 2431

A.10.5.4 L1-RSRP measurement for beam reporting with CCA serving cell 2431

A.10.5.4.1 SSB based L1-RSRP measurement 2431

A.10.5.4.1.1 Test Purpose and Environment 2431

A.10.5.4.1.2 Test parameters 2432

A.10.5.4.1.3 Test Requirements 2434

A.10.5.5 RSSI 2434

A.10.5.5.1 RSSI measurement accuracy on PSCC with CCA 2434

A.10.5.5.1.1 Test Purpose and Environment 2434

A.10.5.5.1.2 Test parameters 2434

A.10.5.5.1.3 Test Requirements 2437

A.10.5.5.2 RSSI measurement accuracy on SCC with CCA 2437

A.10.5.5.2.1 Test Purpose and Environment 2437

A.10.5.5.2.2 Test parameters 2437

A.10.5.5.2.3 Test Requirements 2440

A.10.5.5.3 Inter-frequency RSSI measurement accuracy on a carrier with CCA 2440

A.10.5.5.3.1 Test Purpose and Environment 2440

A.10.5.5.3.2 Test parameters 2440

A.10.5.5.3.3 Test Requirements 2444

A.10.5.6 Channel occupancy 2444

A.10.5.6.1 Channel occupancy measurement accuracy on PSCC with CCA 2444

A.10.5.6.1.1 Test Purpose and Environment 2444

A.10.5.6.1.2 Test parameters 2444

A.10.5.6.1.3 Test Requirements 2448

A.10.5.6.2 Channel occupancy measurement accuracy on SCC with CCA 2448

A.10.5.6.2.1 Test Purpose and Environment 2448

A.10.5.6.2.2 Test parameters 2448

A.10.5.6.2.3 Test Requirements 2451

A.10.5.6.3 Inter-frequency channel occupancy measurement accuracy on a carrier with CCA 2451

A.10.5.6.3.1 Test Purpose and Environment 2451

A.10.5.6.3.2 Test parameters 2451

A.10.5.6.3.3 Test Requirements 2455

A.11 NR Standalone Tests with NR PCell under CCA and Other NR Cells in FR1 2455

A.11.1 RRC\_IDLE state mobility 2455

A.11.1.1 Cell re-selection with both source and target NR carrier frequencies under CCA 2455

A.11.1.1.1 Cell reselection to FR1 intra-frequency NR cells when subject to CCA on the serving and target cell 2455

A.11.1.1.1.1 Test Purpose and Environment 2455

A.11.1.1.1.2 Test Parameters 2456

A.11.1.1.1.3 Test Requirements 2459

A.11.1.1.2 Cell reselection to FR1 inter-frequency NR case when subject to CCA on the serving and target cell 2459

A.11.1.1.2.1 Test Purpose and Environment 2459

A.11.1.1.2.2 Test Parameters 2459

A.11.1.1.2.3 Test Requirements 2463

A.11.1.2 Cell re-selection to NR with source NR carrier frequency under CCA 2463

A.11.1.2.1 Cell reselection to FR1 inter-frequency NR case when serving cell is subject to CCA 2463

A.11.1.2.1.1 Test Purpose and Environment 2463

A.11.1.2.1.2 Test Parameters 2464

A.11.1.2.1.3 Test Requirements 2470

A.11.1.3 Cell re-selection from NR carrier with target NR carrier frequency under CCA 2471

A.11.1.3.1 Cell reselection to FR1 inter-frequency NR case when target cell is subject to CCA 2471

A.11.1.3.1.1 Test Purpose and Environment 2471

A.11.1.3.1.2 Test Parameters 2471

A.11.1.3.1.3 Test Requirements 2476

A.11.1.4 Inter-RAT cell re-selection to E-UTRAN with source NR carrier frequency under CCA 2477

A.11.1.4.1 Cell reselection to higher priority E-UTRAN when serving cell is subject to CCA 2477

A.11.1.4.1.1 Test Purpose and Environment 2477

A.11.1.4.1.2 Test Parameters 2477

A.11.1.4.1.3 Test Requirements 2480

A.11.1.4.2 Cell reselection to lower priority E-UTRAN when serving cell is subject to CCA 2481

A.11.1.4.2.1 Test Purpose and Environment 2481

A.11.1.4.2.2 Test Requirements 2483

A.11.2 RRC\_CONNECTED state mobility 2484

A.11.2.1 Handover 2484

A.11.2.1.1 Intra-frequency handover from FR1 carrier under CCA to FR1 carrier under CCA; known target cell 2484

A.11.2.1.1.1 Test Purpose and Environment 2484

A.11.2.1.1.2 Test Parameters 2484

A.11.2.1.1.3 Test Requirements 2487

A.11.2.1.2 Intra-frequency handover from FR1 carrier under CCA to FR1 carrier under CCA; unknown target cell 2487

A.11.2.1.2.1 Test Purpose and Environment 2487

A.11.2.1.2.2 Test Parameters 2487

A.11.2.1.2.3 Test Requirements 2490

A.11.2.1.3 Inter-frequency handover from FR1 carrier under CCA to FR1 carrier under CCA; unknown target cell 2490

A.11.2.1.3.1 Test Purpose and Environment 2490

A.11.2.1.3.2 Test Parameters 2490

A.11.2.1.3.3 Test Requirements 2493

A.11.2.1.4 Inter-frequency handover from FR1 carrier under CCA to FR1; known target cell 2493

A.11.2.1.4.1 Test Purpose and Environment 2493

A.11.2.1.4.2 Test Parameters 2493

A.11.2.1.4.3 Test Requirements 2497

A.11.2.1.5 Inter-frequency handover from FR1 carrier under CCA to FR1; unknown target cell 2498

A.11.2.1.5.1 Test Purpose and Environment 2498

A.11.2.1.5.2 Test Parameters 2498

A.11.2.1.5.3 Test Requirements 2501

A.11.2.1.6 Inter-frequency handover from FR1 to FR1 carrier under CCA; unknown target cell 2502

A.11.2.1.6.1 Test Purpose and Environment 2502

A.11.2.1.6.2 Test Parameters 2502

A.11.2.1.6.3 Test Requirements 2505

A.11.2.1.7 SA NR FR1 carrier under CCA - E-UTRAN handover with known target cell 2506

A.11.2.1.7.1 Test Purpose and Environment 2506

A.11.2.1.7.2 Test Requirements 2512

A.11.2.1.8 SA NR FR1 carrier under CCA - E-UTRAN handover with unknown target cell 2512

A.11.2.1.8.1 Test Purpose and Environment 2512

A.11.2.1.8.2 Test Requirements 2517

A.11.2.2 RRC connection mobility control 2517

A.11.2.2.1 RRC re-establishment 2517

A.11.2.2.1.1 Intra-frequency RRC Re-establishment with CCA in FR1 2517

A.11.2.2.1.2 Inter-frequency RRC Re-establishment with CCA in FR1 2520

A.11.2.2.1.3 Intra-frequency RRC Re-establishment with CCA in FR1 without serving cell timing 2524

A.11.2.2.1.4 Inter-frequency RRC Re-establishment from NR FR1 carrier without CCA to NR FR1 carrier under CCA 2527

A.11.2.2.2 Random Access 2532

A.11.2.2.2.1 4-step RA type contention-based random access for NR PCell with CCA 2532

A.11.2.2.2.1.1 Test Purpose and Environment 2532

A.11.2.2.2.1.2 Test Requirements 2535

A.11.2.2.2.1.2.1 Random Access Preamble Transmission 2535

A.11.2.2.2.1.2.2 Random Access Response Reception 2535

A.11.2.2.2.1.2.3 No Random Access Response Reception 2536

A.11.2.2.2.1.2.4 Receiving an UL grant for msg3 retransmission 2536

A.11.2.2.2.1.2.5 Reception of an Incorrect Message over Temporary C-RNTI 2536

A.11.2.2.2.1.2.6 Reception of a Correct Message over Temporary C-RNTI 2537

A.11.2.2.2.1.2.7 Contention Resolution Timer expiry 2537

A.11.2.2.2.2 4-step RA type non-contention based random access for NR PSCell with CCA 2537

A.11.2.2.2.2.1 Test Purpose and Environment 2537

A.11.2.2.2.2.2 Test Requirements 2540

A.11.2.2.2.2.2.1 SSB-based Random Access Preamble Transmission 2540

A.11.2.2.2.2.2.2 Random Access Response Reception 2541

A.11.2.2.2.2.2.3 No Random Access Response Reception 2541

A.11.2.2.2.3 2-step RA type contention-based random access for NR PCell with CCA 2541

A.11.2.2.2.3.1 Test Purpose and Environment 2541

A.11.2.2.2.3.2 Test Requirements 2545

A.11.2.2.2.3.2.1 MsgA Transmission 2545

A.11.2.2.2.3.2.2 MsgB Reception 2545

A.11.2.2.2.3.2.3 No MsgB Reception 2546

A.11.2.2.2.4 2-step RA type non-contention-based random access for NR PCell with CCA 2546

A.11.2.2.2.4.1 Test Purpose and Environment 2546

A.11.2.2.2.4.2 Test Requirements 2550

A.11.2.2.2.4.2.1 MsgA Transmission 2550

A.11.2.2.2.4.2.2 MsgB Reception 2551

A.11.2.2.2.4.2.3 No MsgB Reception 2551

A.11.2.2.3 RRC connection release with redirection 2552

A.11.2.2.3.1 Redirection from NR FR1 carrier under CCA to NR FR1 carrier under CCA 2552

A.11.3 Timing 2560

A.11.3.1 UE transmit timing 2560

A.11.3.2 UE timing advance 2564

A.11.3.2.1 UE Timing Advance Adjustment Accuracy with PCell under DL CCA 2564

A.11.3.2.1.1 Test Purpose and Environment 2564

A.11.3.2.1.2 Test Parameters 2564

A.11.3.2.1.3 Test Requirements 2568

A.11.4 Signalling characteristics 2568

A.11.4.1 Radio link monitoring 2568

A.11.4.1.1 Introduction 2568

A.11.4.1.2 Radio link monitoring out-of-sync test for PCell configured with SSB-based RLM RS in non-DRX mode 2569

A.11.4.1.2.1 Test purpose and environment 2569

A.11.4.1.2.2 Test requirements 2573

A.11.4.1.3 Radio link monitoring in-sync test for PCell configured with SSB-based RLM RS in non-DRX mode 2573

A.11.4.1.3.1 Test purpose and environment 2573

A.11.4.1.3.2 Test requirements 2579

A.11.4.1.4 Void 2579

A.11.4.1.4.1 Void 2579

A.11.4.1.4.2 Void 2579

A.11.4.1.5 Void 2579

A.11.4.1.5.1 Void 2579

A.11.4.1.5.2 Void 2579

A.11.4.2 Interruption 2579

A.11.4.2.1 NR interruptions during Scell operations with CCA on PCell and SCell 2579

A.11.4.2.1.1 Test Purpose and Environment 2579

A.11.4.2.1.2 Test Requirements 2583

A.11.4.3 SCell activation and deactivation delay 2583

A.11.4.3.2 SCell Activation and Deactivation of known SCell with PCell and SCell under CCA, 640 ms SCell measurement cycle 2588

A.11.4.3.2.1 Test Purpose and Environment 2588

A.11.4.3.2.2 Test Requirements 2589

A.11.4.4 Beam failure detection and link recovery procedures 2590

A.11.4.4.1 Beam Failure Detection and Link Recovery Test for FR1 PCell configured with SSB-based BFD and LR in non-DRX mode 2590

A.11.4.4.1.1 Test Purpose and Environment 2590

A.11.4.4.1.2 Test Requirements 2596

A.11.4.4.2 Beam Failure Detection and Link Recovery Test for FR1 PCell configured with SSB-based BFD and LR in DRX mode 2596

A.11.4.4.2.1 Test Purpose and Environment 2596

A.11.4.4.2.2 Test Requirements 2602

A.11.4.5 Active BWP switching 2602

A.11.4.5.1 UL active BWP switch delay with consistent UL LBT failure on PCell subject to UL CCA 2602

A.11.4.5.1.1 Test Purpose and Environment 2602

A.11.4.5.1.2 Test Requirements 2606

A.11.4.6 Void 2616

A.11.5 Measurement procedure 2616

A.11.5.1 Intra-frequency measurements 2616

A.11.5.1.1 Event-triggered reporting tests on PCC without gaps under non-DRX 2616

A.11.5.1.1.1 Test purpose and environment 2616

A.11.5.1.1.2 Test parameters 2616

A.11.5.1.1.3 Test Requirements 2620

A.11.5.1.2 Event-triggered reporting tests on PCC without gaps under DRX 2620

A.11.5.1.2.1 Test purpose and environment 2620

A.11.5.1.2.2 Test parameters 2620

A.11.5.1.2.3 Test Requirements 2624

A.11.5.1.3 Event-triggered reporting tests on PCC with per-UE gaps under non-DRX 2624

A.11.5.1.3.1 Test purpose and environment 2624

A.11.5.1.3.2 Test parameters 2624

A.11.5.1.3.3 Test Requirements 2624

A.11.5.1.4 Event-triggered reporting tests on PCC with per-UE gaps under DRX 2624

A.11.5.1.4.1 Test purpose and environment 2624

A.11.5.1.4.2 Test parameters 2625

A.11.5.1.4.3 Test Requirements 2625

A.11.5.1.5 Event-triggered reporting tests on SCC without gaps under non-DRX 2625

A.11.5.1.5.1 Test purpose and environment 2625

A.11.5.1.5.2 Test parameters 2625

A.11.5.1.6 Event-triggered reporting tests on SCC without gaps under DRX 2625

A.11.5.1.6.1 Test purpose and environment 2625

A.11.5.1.6.2 Test parameters 2625

A.11.5.1.6.3 Test Requirements 2625

A.11.5.1.7 Event-triggered reporting tests on SCC with per-UE gaps under non-DRX 2626

A.11.5.1.7.1 Test purpose and environment 2626

A.11.5.1.7.2 Test parameters 2626

A.11.5.1.7.3 Test Requirements 2626

A.11.5.1.8 Event-triggered reporting tests on SCC with per-UE gaps under DRX 2626

A.11.5.1.8.1 Test purpose and environment 2626

A.11.5.1.8.2 Test parameters 2626

A.11.5.1.8.3 Test Requirements 2626

A.11.5.1.9 RSSI measurement reporting on PCC 2627

A.11.5.1.9.1 Test purpose and environment 2627

A.11.5.1.9.2 Test parameters 2627

A.11.5.1.10 Channel occupancy measurement reporting on PCC 2627

A.11.5.1.10.1 Test purpose and environment 2627

A.11.5.1.10.2 Test parameters 2627

A.11.5.1.11 RSSI measurement reporting on SCC 2628

A.11.5.1.11.1 Test purpose and environment 2628

A.11.5.1.11.2 Test parameters 2628

A.11.5.1.12 Channel occupancy measurement reporting on SCC 2628

A.11.5.1.12.1 Test purpose and environment 2628

A.11.5.1.12.2 Test parameters 2628

A.11.5.2 Inter-frequency measurements 2629

A.11.5.2.1 RSSI measurement reporting 2629

A.11.5.2.1.1 Test purpose and environment 2629

A.11.5.2.1.2 Test parameters 2629

A.11.5.2.2 Channel occupancy measurement reporting 2629

A.11.5.2.2.1 Test purpose and environment 2629

A.11.5.2.2.2 Test parameters 2629

A.11.5.2.3 Event triggered reporting tests for FR1 with CCA without SSB time index detection when DRX is not used 2630

A.11.5.2.3.1 Test Purpose and Environment 2630

A.11.5.2.3.2 Test Requirements 2634

A.11.5.2.4 Event triggered reporting tests for FR1 with CCA without SSB time index detection when DRX is used 2635

A.11.5.2.4.1 Test Purpose and Environment 2635

A.11.5.2.4.2 Test Requirements 2640

A.11.5.2.5 Event triggered reporting tests for FR1 with CCA with SSB time index detection when DRX is not used 2640

A.11.5.2.5.1 Test Purpose and Environment 2640

A.11.5.2.5.2 Test Requirements 2644

A.11.5.2.6 Event triggered reporting tests for FR1 with CCA with SSB time index detection when DRX is used 2645

A.11.5.2.6.1 Test Purpose and Environment 2645

A.11.5.2.6.2 Test Requirements 2650

A.11.5.2.7 Event triggered reporting tests for FR1 without SSB time index detection when DRX is not used 2650

A.11.5.2.7.1 Test Purpose and Environment 2650

A.11.5.2.7.2 Test Requirements 2654

A.11.5.2.8 Event triggered reporting tests for FR1 without SSB time index detection when DRX is used 2655

A.11.5.2.8.1 Test Purpose and Environment 2655

A.11.5.2.8.2 Test Requirements 2660

A.11.5.2.9 Event triggered reporting tests for FR1 with SSB time index detection when DRX is not used 2660

A.11.5.2.9.1 Test Purpose and Environment 2660

A.11.5.2.9.2 Test Requirements 2665

A.11.5.2.10 Event triggered reporting tests for FR1 with SSB time index detection when DRX is used 2666

A.11.5.2.10.1 Test Purpose and Environment 2666

A.11.5.2.10.2 Test Requirements 2671

A.11.5.3 Inter-RAT E-UTRAN measurements 2672

A.11.5.3.1 SA NR - E-UTRAN event-triggered reporting in non-DRX in FR1 2672

A.11.5.3.1.1 Test Purpose and Environment 2672

A.11.5.3.1.2 Test Requirements 2676

A.11.5.3.2 SA NR - E-UTRAN event-triggered reporting in DRX in FR1 2676

A.11.5.3.2.1 Test Purpose and Environment 2676

A.11.5.3.2.2 Test Requirements 2681

A.11.5.4 L1-RSRP measurements for beam reporting 2681

A.11.5.4.1 SSB based L1-RSRP measurement when DRX is not used 2681

A.11.5.4.1.1 Test Purpose and Environment 2681

A.11.5.4.1.2 Test parameters 2681

A.11.5.4.1.3 Test Requirements 2683

A.11.5.4.2 SSB based L1-RSRP measurement when DRX is used 2683

A.11.5.4.2.1 Test Purpose and Environment 2683

A.11.5.4.2.2 Test parameters 2684

A.11.5.4.2.3 Test Requirements 2686

A.11.5.4.3 SSB based L1-RSRP measurement on SCC when DRX is not used 2686

A.11.5.4.3.1 Test Purpose and Environment 2686

A.11.5.4.3.2 Test parameters 2687

A.11.5.4.3.3 Test Requirements 2690

A.11.5.4.4 SSB based L1-RSRP measurement on SCC when DRX is used 2691

A.11.5.4.4.1 Test Purpose and Environment 2691

A.11.5.4.4.2 Test parameters 2691

A.11.5.4.4.3 Test Requirements 2694

A.11.6 Measurement performance 2695

A.11.6.1 SS-RSRP 2695

A.11.6.1.1 Intra-frequency measurement accuracy on a carrier frequency with CCA 2695

A.11.6.1.1.1 Test Purpose and Environment 2695

A.11.6.1.1.2 Test parameters 2695

A.11.6.1.1.3 Test Requirements 2697

A.11.6.1.2 Intra-frequency measurement accuracy on SCC on a carrier frequency with CCA 2697

A.11.6.1.2.1 Test Purpose and Environment 2697

A.11.6.1.2.2 Test parameters 2697

A.11.6.1.2.3 Test Requirements 2699

A.11.6.2 SS-RSRQ 2699

A.11.6.2.1 Intra-frequency measurement accuracy 2699

A.11.6.2.1.1 Test Purpose and Environment 2699

A.11.6.2.1.2 Test Parameters 2699

A.11.6.2.1.3 Test Requirements 2702

A.11.6.2.2 Inter-frequency measurement accuracy 2702

A.11.6.2.2.1 Test Purpose and Environment 2702

A.11.6.2.2.2 Test Parameters 2702

A.11.6.2.2.3 Test Requirements 2705

A.11.6.2.3 Intra-frequency measurement accuracy on SCC 2705

A.11.6.2.3.1 Test Purpose and Environment 2705

A.11.6.2.3.2 Test Parameters 2705

A.11.6.2.3.3 Test Requirements 2708

A.11.6.2.4 Inter-frequency measurement accuracy 2708

A.11.6.2.4.1 Test Purpose and Environment 2708

A.11.6.2.4.2 Test Parameters 2708

A.11.6.2.4.3 Test Requirements 2717

A.11.6.3 SS-SINR 2717

A.11.6.3.1 Intra-frequency measurement accuracy 2717

A.11.6.3.1.1 Test Purpose and Environment 2717

A.11.6.3.1.2 Test Parameters 2717

A.11.6.3.1.3 Test Requirements 2720

A.11.6.3.2 Inter-frequency measurement accuracy 2720

A.11.6.3.2.1 Test Purpose and Environment 2720

A.11.6.3.2.2 Test Parameters 2720

A.11.6.3.2.3 Test Requirements 2723

A.11.6.3.3 Intra-frequency measurement accuracy on SCC 2723

A.11.6.3.3.1 Test Purpose and Environment 2723

A.11.6.3.3.2 Test Parameters 2723

A.11.6.3.3.3 Test Requirements 2726

A.11.6.3.4 Inter-frequency measurement accuracy 2726

A.11.6.3.4.1 Test Purpose and Environment 2726

A.11.6.3.4.2 Test Parameters 2726

A.11.6.3.4.3 Test Requirements 2734

A.11.6.4 L1-RSRP measurement for beam reporting with CCA serving cell 2734

A.11.6.4.1 SSB based L1-RSRP measurement 2734

A.11.6.4.1.1 Test Purpose and Environment 2734

A.11.6.4.1.2 Test parameters 2735

A.11.6.4.1.3 Test Requirements 2738

A.11.6.5 RSSI 2738

A.11.6.5.1 Intra-frequency RSSI measurement accuracy on PCC with CCA 2738

A.11.6.5.1.1 Test Purpose and Environment 2738

A.11.6.5.1.2 Test parameters 2738

A.11.6.5.1.3 Test Requirements 2741

A.11.6.5.2 Intra-frequency RSSI measurement accuracy on SCC with CCA 2741

A.11.6.5.2.1 Test Purpose and Environment 2741

A.11.6.5.2.2 Test parameters 2741

A.11.6.5.2.3 Test Requirements 2744

A.11.6.5.3 Inter-frequency RSSI measurement accuracy on a carrier with CCA 2744

A.11.6.5.3.1 Test Purpose and Environment 2744

A.11.6.5.3.2 Test parameters 2744

A.11.6.5.3.3 Test Requirements 2747

A.11.6.6 Channel occupancy 2747

A.11.6.6.1 Intra-frequency channel occupancy measurement accuracy on PCC with CCA 2747

A.11.6.6.1.1 Test Purpose and Environment 2747

A.11.6.6.1.2 Test parameters 2747

A.11.6.6.1.3 Test Requirements 2751

A.11.6.6.2 Intra-frequency channel occupancy measurement accuracy on SCC with CCA 2751

A.11.6.6.2.1 Test Purpose and Environment 2751

A.11.6.6.2.2 Test parameters 2751

A.11.6.6.2.3 Test Requirements 2754

A.11.6.6.3 Inter-frequency channel occupancy measurement accuracy on a carrier with CCA 2754

A.11.6.6.3.1 Test Purpose and Environment 2754

A.11.6.6.3.2 Test parameters 2754

A.11.6.6.3.3 Test Requirements 2757

A.11.6.7 E-UTRAN RSRP 2757

A.11.6.8 E-UTRAN RSRQ 2757

A.11.6.9 E-UTRAN SINR 2757

A.12 E-UTRA Standalone Tests with at Least One NR Cell under CCA 2757

A.12.1 RRC\_IDLE state mobility 2757

A.12.1.1 Inter-RAT cell re-selection to NR on a carrier frequency with CCA 2757

A.12.1.1.1 E-UTRA Cell reselection to higher priority NR target Cell in FR1 when target cell is subject to CCA 2757

A.12.1.1.1.1 Test Purpose and Environment 2757

A.12.1.1.1.2 Test Requirements 2763

A.12.2 RRC\_CONNECTED state mobility 2764

A.12.2.1 Handover 2764

A.12.2.1.1 E-UTRAN - NR with CCA handover 2764

A.12.2.1.1.1 Test Purpose and Environment 2764

A.12.2.1.1.2 Test Requirements 2769

A.12.3 Signalling characteristics 2770

A.12.3.1 Interruptions 2770

A.12.4 Measurement procedure 2770

A.12.4.1 E-UTRAN−NR inter-RAT SFTD measurements 2770

A.12.4.1.1 E-UTRA – NR Inter-RAT SFTD Measurement Delay with NR under CCA in non-DRX 2770

A.12.4.1.1.1 Test Purpose and Environment 2770

A.12.4.1.1.2 Test Requirements 2774

A.12.4.2 E-UTRAN−NR inter-RAT measurements on NR carrier frequency under CCA 2774

A.12.4.2.1 E-UTRA-NR inter-RAT event triggered reporting tests for FR1 without SSB time index detection when DRX is not used 2774

A.12.4.2.1.1 Test Purpose and Environment 2774

A.12.4.2.1.2 Test Requirements 2778

A.12.4.2.2 E-UTRA-NR inter-RAT event triggered reporting tests for FR1 without SSB time index detection when DRX is used 2779

A.12.4.2.2.1 Test Purpose and Environment 2779

A.12.4.2.2.2 Test Requirements 2783

A.12.4.2.3 NR Inter-RAT event triggered reporting tests for FR1 with SSB time index detection when DRX is not used 2784

A.12.4.2.3.1 Test Purpose and Environment 2784

A.12.4.2.3.2 Test Requirements 2788

A.12.4.2.4 NR Inter-RAT event triggered reporting tests for FR1 with SSB time index detection when DRX is used 2789

A.12.4.2.4.1 Test Purpose and Environment 2789

A.12.4.2.4.2 Test Requirements 2793

A.12.4.2.5 RSSI measurement reporting 2794

A.12.4.2.5.1 Test purpose and environment 2794

A.12.4.2.5.2 Test parameters 2794

A.12.4.2.5.3 Test Requirements 2797

A.12.4.2.6 Channel occupancy measurement reporting 2797

A.12.4.2.6.1 Test purpose and environment 2797

A.12.4.2.6.2 Test parameters 2797

A.12.4.2.6.3 Test Requirements 2801

A.12.5 Measurement performance 2801

A.12.5.1 E-UTRAN−NR SFTD 2801

A.12.5.2 E-UTRAN−NR SS-RSRP 2807

A.12.5.3 E-UTRAN−NR SS-RSRQ 2807

A.12.5.4 E-UTRAN−NR SS-SINR 2807

A.12.5.5 E-UTRAN−NR RSSI 2807

A.12.5.6 E-UTRAN−NR channel occupancy 2807

A.13 NR Standalone Tests with NR SCell under CCA and All Other NR Cells in FR1 2807

A.13.1 Timing 2807

A.13.1.1 UE transmit timing 2807

A.13.1.2 Timing advance 2807

A.13.2 Signalling characteristics 2807

A.13.2.1 Interruption 2807

A.13.2.1.1 NR interruptions during SCell operations with CCA on SCell 2807

A.13.2.1.1.1 Test Purpose and Environment 2807

A.13.2.1.1.2 Test Requirements 2811

A.13.2.2 SCell activation and deactivation delay 2811

A.13.2.2.2 SCell Activation and Deactivation of known SCell under CCA, 640 ms SCell measurement cycle 2816

A.13.2.2.2.1 Test Purpose and Environment 2816

A.13.2.2.2.2 Test Requirements 2817

A.13.2.2.3 SCell Activation and Deactivation of unknown SCell under CCA 2817

A.13.2.2.3.1 Test Purpose and Environment 2817

A.13.2.2.3.2 Test Requirements 2818

A.13.2.3 Void 2818

A.13.3 Measurement procedure 2818

A.13.3.1 Intra-frequency measurements 2818

A.13.3.1.1 Event-triggered reporting tests on SCC without gaps under non-DRX 2818

A.13.3.1.1.1 Test purpose and environment 2818

A.13.3.1.1.2 Test parameters 2818

A.13.3.1.1.3 Test Requirements 2823

A.13.3.1.2 Event-triggered reporting tests on SCC without gaps under DRX 2823

A.13.3.1.2.1 Test purpose and environment 2823

A.13.3.1.2.2 Test parameters 2823

A.13.3.1.2.3 Test Requirements 2828

A.13.3.1.3 Event-triggered reporting tests on SCC with per-UE gaps under non-DRX 2828

A.13.3.1.3.1 Test purpose and environment 2828

A.13.3.1.3.2 Test parameters 2828

A.13.3.1.3.3 Test Requirements 2833

A.13.3.1.4 Event-triggered reporting tests on SCC with per-UE gaps under DRX 2833

A.13.3.1.4.1 Test purpose and environment 2833

A.13.3.1.4.2 Test parameters 2833

A.13.3.1.4.3 Test Requirements 2838

A.13.3.1.5 RSSI measurement reporting on SCC 2838

A.13.3.1.5.1 Test purpose and environment 2838

A.13.3.1.5.2 Test parameters 2838

A.13.3.1.6 Channel occupancy measurement reporting on SCC 2840

A.13.3.1.6.1 Test purpose and environment 2840

A.13.3.1.6.2 Test parameters 2841

A.13.3.2 Inter-frequency measurements 2841

A.13.3.2.1 RSSI measurement reporting 2841

A.13.3.2.1.1 Test purpose and environment 2841

A.13.3.2.1.2 Test parameters 2841

A.13.3.2.2 Channel occupancy measurement reporting 2842

A.13.3.2.2.1 Test purpose and environment 2842

A.13.3.2.2.2 Test parameters 2842

A.13.3.2.3 Event triggered reporting tests for FR1 with CCA without SSB time index detection when DRX is not used 2842

A.13.3.2.3.1 Test Purpose and Environment 2842

A.13.3.2.3.2 Test Requirements 2848

A.13.3.2.4 Event triggered reporting tests for FR1 with CCA without SSB time index detection when DRX is used 2848

A.13.3.2.4.1 Test Purpose and Environment 2848

A.13.3.2.4.2 Test Requirements 2853

A.13.3.2.5 Event triggered reporting tests for FR1 with CCA with SSB time index detection when DRX is not used 2854

A.13.3.2.5.1 Test Purpose and Environment 2854

A.13.3.2.5.2 Test Requirements 2859

A.13.3.2.6 Event triggered reporting tests for FR1 with CCA with SSB time index detection when DRX is used 2859

A.13.3.2.6.1 Test Purpose and Environment 2859

A.13.3.2.6.2 Test Requirements 2865

A.13.3.3 L1-RSRP measurements for beam reporting 2866

A.13.3.3.1 SSB based L1-RSRP measurement when DRX is not used 2866

A.13.3.3.1.1 Test Purpose and Environment 2866

A.13.3.3.1.2 Test parameters 2866

A.13.3.3.1.3 Test Requirements 2871

A.13.3.3.2 SSB based L1-RSRP measurement when DRX is used 2871

A.13.3.3.2.1 Test Purpose and Environment 2871

A.13.3.3.2.2 Test parameters 2871

A.13.3.3.2.3 Test Requirements 2875

A.13.4 Measurement performance 2875

A.13.4.1 SS-RSRP 2875

A.13.4.1.1 Intra-frequency measurement accuracy on a carrier frequency with CCA 2875

A.13.4.1.1.1 Test Purpose and Environment 2875

A.13.4.1.1.2 Test parameters 2875

A.13.4.1.1.3 Test Requirements 2877

A.13.4.2 SS-RSRQ 2877

A.13.4.2.1 Intra-frequency measurement accuracy on SCC 2877

A.13.4.2.1.1 Test Purpose and Environment 2877

A.13.4.2.1.2 Test Parameters 2877

A.13.4.2.1.3 Test Requirements 2885

A.13.4.3 SS-SINR 2885

A.13.4.3.1 Intra-frequency measurement accuracy on SCC 2885

A.13.4.3.1.1 Test Purpose and Environment 2885

A.13.4.3.1.2 Test Parameters 2885

A.13.4.3.1.3 Test Requirements 2891

A.13.4.4 L1-RSRP measurement for beam reporting with CCA serving cell 2892

A.13.4.4.1 SSB based L1-RSRP measurement 2892

A.13.4.4.1.1 Test Purpose and Environment 2892

A.13.4.4.1.2 Test parameters 2892

A.13.4.4.1.3 Test Requirements 2896

A.13.4.5 RSSI 2896

A.13.4.5.1 Intra-frequency RSSI measurement accuracy on a carrier with CCA 2896

A.13.4.5.1.1 Test Purpose and Environment 2896

A.13.4.5.1.2 Test parameters 2896

A.13.4.5.1.3 Test Requirements 2900

A.13.4.5.2 Inter-frequency RSSI measurement accuracy on a carrier with CCA 2900

A.13.4.5.2.1 Test Purpose and Environment 2900

A.13.4.5.2.2 Test parameters 2900

A.13.4.5.2.3 Test Requirements 2904

A.13.4.6 Channel occupancy 2904

A.13.4.6.1 Intra-frequency channel occupancy measurement accuracy on SCC with CCA 2904

A.13.4.6.1.1 Test Purpose and Environment 2904

A.13.4.6.1.2 Test parameters 2904

A.13.4.6.1.3 Test Requirements 2908

A.13.4.6.2 Inter-frequency channel occupancy measurement accuracy on a carrier with CCA 2908

A.13.4.6.2.1 Test Purpose and Environment 2908

A.13.4.6.2.2 Test parameters 2908

A.13.4.6.2.3 Test Requirements 2912

Annex B (normative): Conditions for RRM requirements applicability for operating bands 2914

B.1 Conditions for NR RRC\_IDLE state mobility 2914

B.1.1 Introduction 2914

B.1.2 Conditions for measurements on NR intra-frequency cells for cell re-selection 2914

B.1.3 Conditions for measurements on NR inter-frequency cells for cell re-selection 2915

B.2 Conditions for UE measurements procedures and performance requirements in RRC\_CONNECTED state 2916

B.2.1 Introduction 2916

B.2.1.1 General 2916

B.2.1.2 Derivation of Minimum SSB\_RP values for FR1 2916

B.2.1.3 Derivation of Minimum SSB\_RP values for FR2 2916

B.2.1.3.1 Minimum SSB\_RP values for Rx Beam Peak angle of arrival 2916

B.2.1.3.2 Minimum SSB\_RP values for angle of arrival within Spherical coverage 2917

B.2.1.4 Gain to SS-RSRP and CSI-RSRP measurement point for FR1 2917

B.2.1.5 Gain to SS-RSRP and CSI-RSRP measurement point for FR2 2918

B.2.1.5.1 Gain to SS-RSRP and CSI-RSRP measurement point for Rx Beam Peak angle of arrival 2918

B.2.1.5.2 Gain to SS-RSRP measurement point for different frequency 2918

B.2.1.5.3 Alignment of Rough beam to Rx beam Peak 2918

B.2.1.6 Gain to PRS-RSRP measurement point for FR2 2919

B.2.1.6.1 Gain to PRS-RSRP measurement point for Rx Beam Peak angle of arrival 2919

B.2.2 Conditions for NR intra-frequency measurements 2920

B.2.3 Conditions for NR inter-frequency measurements 2921

B.2.4 Conditions for NR L1-RSRP reporting 2922

B.2.4.1 Conditions for SSB based L1-RSRP reporting 2922

B.2.4.2 Conditions for CSI-RS based L1-RSRP reporting 2923

B.2.5 Conditions for RRC connection release with redirection to NR 2925

B.2.6 Void 2926

B.2.6.1 Void 2926

B.2.6.2 Void 2926

B.2.7 Conditions for SRS-RSRP measurements 2926

B.2.8 Conditions for NR L1-SINR reporting 2927

B.2.8.1 Conditions for L1-SINR reporting with CSI-RS based CMR and no dedicated IMR configured 2927

B.2.8.2 Conditions for L1-SINR reporting with SSB based CMR and dedicated IMR configured 2928

B.2.8.2.1 L1-SINR reporting with SSB based CMR and dedicated ZP-IMR configured 2928

B.2.8.2.2 L1-SINR reporting with SSB based CMR and dedicated NZP-IMR configured 2928

B.2.8.3 Conditions for L1-SINR reporting with CSI-RS based CMR and dedicated IMR configured 2930

B.2.8.3.1 L1-SINR reporting with CSI-RS based CMR and dedicated ZP-IMR configured 2930

B.2.8.3.2 L1-SINR reporting with CSI-RS based CMR and dedicated NZP-IMR configured 2931

B.2.9 Conditions for NR intra-frequency measurements under CCA 2932

B.2.10 Conditions for NR inter-frequency measurements under CCA 2932

B.2.11 Conditions for NR L1-RSRP reporting under CCA 2932

B.2.11.1 Conditions for SSB based L1-RSRP reporting 2932

B.2.12 Conditions for NR CSI-RS based intra-frequency measurements 2933

B.2.13 Conditions for NR CSI-RS based inter-frequency measurements 2934

B.2.14 Conditions for NR PRS-based measurements 2936

B.3 RRM Requirements Exceptions 2937

B.3.1 Introduction 2937

B.3.2 Receiver sensitivity relaxation for CA 2937

B.3.2.1 Receiver sensitivity relaxation for UE supporting CA in FR1 2937

B.3.2.2 Receiver sensitivity relaxation for UE configured with CA in FR1 2938

B.3.2.2.1 Inter-band carrier aggregation 2938

B.3.2.2.2 Reference sensitivity exceptions due to UL harmonic interference for CA 2938

B.3.2.2.3 Reference sensitivity exceptions due to intermodulation interference due to 2UL CA 2938

B.3.2.3 Receiver sensitivity relaxation for UE supporting CA in FR2 2938

B.3.2.4 Receiver sensitivity relaxation for UE configured with CA in FR2 2938

B.3.2.4.1 Intra-band contiguous carrier aggregation 2938

B.3.2.4.2 Intra-band non-contiguous carrier aggregation 2939

B.3.3 Receiver sensitivity relaxation for DC 2939

B.3.3.1 Receiver sensitivity relaxation for EN-DC 2939

B.3.3.2 Receiver sensitivity relaxation for NE-DC 2939

B.3.4 Receiver sensitivity relaxation for SUL 2939

B.3.4.1 Receiver sensitivity relaxation for UE supporting SUL in FR1 2939

B.3.4.2 Receiver sensitivity relaxation for UE configured with SUL in FR1 2939

B.3.4.2.1 Reference sensitivity exceptions due to UL harmonic interference for SUL 2939

B.4 Conditions for V2X 2939

B.4.1 Test parameters for GNSS signals 2939

B.4.2 Conditions for PSBCH-RSRP Accuracy Requirements 2940

B.4.3 Conditions for Selection/Reselection to Intra-frequency SyncRef UE 2940

B.4.4 Conditions for L1 SL-RSRP Accuracy Requirements 2940

Annex C (informative): Change history 2942