3GPP TS 38.414 V16.0.0 (2020-07)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Radio Access Network;

NG-RAN;

NG data transport

(Release 16)

** 

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP..  
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.  
This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword [4](#__RefHeading___Toc45887869)

1 Scope [5](#__RefHeading___Toc45887870)

2 References [5](#__RefHeading___Toc45887871)

3 Definitions and abbreviations [5](#__RefHeading___Toc45887872)

3.1 Definitions [5](#__RefHeading___Toc45887873)

3.2 Abbreviations [6](#__RefHeading___Toc45887874)

4 Data Link Layer [6](#__RefHeading___Toc45887875)

5 NG Interface user plane protocol [6](#__RefHeading___Toc45887876)

5.1 General [6](#__RefHeading___Toc45887877)

5.2 GTP-U [6](#__RefHeading___Toc45887878)

5.3 UDP/IP [6](#__RefHeading___Toc45887879)

5.4 Diffserv code point marking [7](#__RefHeading___Toc45887880)

Annex A (informative): Change history [8](#__RefHeading___Toc45887881)

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# 1 Scope

The present document specifies the standards for user data transport protocols and related signalling protocols to establish user plane transport bearers over the NG interface.

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 23.501: "System Architecture for the 5G System; Stage 2".

[3] 3GPP TS 29.281: "General Packet Radio System (GPRS) Tunnelling Protocol User Plane (GTPv1-U)".

[4] IETF RFC 768 (1980-08): "User Datagram Protocol".

[5] IETF RFC 8200 (2017-07): "Internet Protocol, Version 6 (IPv6) Specification".

[6] IETF RFC 791 (1981-09): "Internet Protocol".

[7] IETF RFC 2474 (1998-12): "Definition of the Differentiated Services Field (DS Field) in the Ipv4 and Ipv6 Headers".

[8] 3GPP TS 38.300: "NR and NG-RAN Overall Description Stage 2"

# 3 Definitions and abbreviations

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in 3GPP TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in 3GPP TR 21.905 [1].

**gNB**: as defined in TS 38.300 [8].

**ng-eNB**: as defined in TS 38.300 [8].

**NG-RAN node**: as defined in TS 38.300 [8].

**NG-U**: as defined in TS 38.300 [8].

**PDU Session:** as defined in TS 23.501[2].

## 3.2 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

5GC 5G Core

5QI 5G QoS Identifier

AMF Access and Mobility Management Function

GTP GPRS Tunnelling Protocol

IP Internet Protocol

NGAP NG Application Protocol

TEID Tunnel Endpoint Identifier

UDP User Datagram Protocol

UPF User Plane Function

# 4 Data Link Layer

Any data link protocol that fulfills the requirements toward the upper layer may be used.

# 5 NG Interface user plane protocol

## 5.1 General

Both gNB and ng-eNB can be connected to the 5GC over the NG interface.

The transport layer for data streams over NG is an IP based Transport. The following figure shows the transport protocol stacks over NG.



Figure 5.1: Transport network layer for data streams over NG

The GTP-U (TS 29.281 [3]) protocol over UDP over IP shall be supported as the transport for data streams on the NG interface. The data link layer is as specified in clause 4.

The transport bearer is identified by the GTP-U TEID (TS 29.281 [3]) and the IP address (source TEID, destination TEID, source IP address, destination IP address).

## 5.2 GTP-U

The GTP-U (TS 29.281 [3]) protocol shall be used over the NG-U interface toward the 5GC.

## 5.3 UDP/IP

The path protocol used shall be UDP (IETF RFC 768 [4]).

The UDP port number for GTP-U shall be as defined in TS 29.281 [3].

The NG-RAN node and the 5GC shall support fragmentation and assembly of GTP packets at the IP layer.

The NG-RAN node and the 5GC shall support IPv6 (IETF RFC 8200 [5]) and/or IPv4 (IETF RFC 791 [6]).

There may be one or several IP addresses in the NG-RAN node and in the 5GC. The packet processing function in the 5GC shall send downstream packets of a given PDU Session to the NG-RAN node IP address (received in NGAP) associated to that particular PDU Session. The packet processing function in the NG-RAN node shall send upstream packets of a given PDU Session to the 5GC IP address (received in NGAP) associated to that particular PDU Session.

The Transport Layer Address signalled in NGAP messages is a bit string of

a) 32 bits in case of IPv4 address according to IETF RFC 791 [6]; or

b) 128 bits in case of IPv6 address according to IETF RFC 8200 [5]; or

c) 160 bits if both IPv4 and IPv6 addresses are signalled, in which case the IPv4 address is contained in the first 32 bits.

## 5.4 Diffserv code point marking

IP Differentiated Services code point marking (IETF RFC 2474 [7]) shall be supported. The mapping between traffic categories and Diffserv code points shall be configurable by O&M based on 5QI, the Priority Level (if explicitly signalled), and other NG-RAN traffic parameters (e.g. ARP). Traffic categories are implementation-specific and may be determined from the application parameters.

Annex A (informative):  
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| May 2017 | RAN3#96 | R3-171514 |  |  |  | Initial DraftTS endorsed | 0.0.2 |
| October 2017 | RAN3#97bis | R3-174240 |  |  |  | Update some texts due to new 5G terminologies  Add up "Diffserv code point marking" | 0.3.0 |
| January 2018 | RAN3-adhoc1801 |  |  |  |  | Incorporate agreed TPs from RAN3-adhoc1801 | 0.4.0 |
| May 2018 | RAN3#100 | R3-182642 |  |  |  | Covering agreements of RAN3#100 | 0.5.0 |
| 06-2018 | RP-80 | RP-180787 | - | - | - | Presentation to RAN for approval | 1.0.0 |
| 06-2018 | RP-80 |  | - | - | - | Specification approved at TSG-RAN and placed under change control | 15.0.0 |
| 09-2018 | RP-81 | RP-181920 | 0001 | - | F | Updated reference to IPv6 | 15.1.0 |
| 2019-07 | RP-84 | RP-191396 | 0005 | 1 | F | Use of Priority Level and ARP for the DSCP Derivation at the gNB | 15.2.0 |
| 2020-07 | RP-88-e | RP-201093 | 0006 | 1 | D | Rapporteur Clean-ups of TS38.414 | 15.3.0 |
| 2020-07 | SA-88-e | - | - | - | - | Update to Rel-16 version (MCC) | 16.0.0 |