3GPP TS 46.011 V16.0.0 (2020-07)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Services and System Aspects;

Full rate speech;

Substitution and muting of lost frames for

full rate speech channels

(Release 16)

 

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.   
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.   
This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

Keywords

GSM, speech, codec

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword [4](#__RefHeading___Toc477456138)

1 Scope [5](#__RefHeading___Toc477456139)

2 References [5](#__RefHeading___Toc477456140)

3 Definitions and abbreviations [5](#__RefHeading___Toc477456141)

4 General [5](#__RefHeading___Toc477456142)

5 Requirements [5](#__RefHeading___Toc477456143)

5.1 First lost speech frame [5](#__RefHeading___Toc477456144)

5.2 Subsequent lost speech frames [6](#__RefHeading___Toc477456145)

5.3 First lost SID frame [6](#__RefHeading___Toc477456146)

5.4 Subsequent lost SID frame [6](#__RefHeading___Toc477456147)

6 Example solution [6](#__RefHeading___Toc477456148)

Annex A (informative): Change history [8](#__RefHeading___Toc477456149)

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# 1 Scope

The present document defines a frame substitution and muting procedure which shall be used by the RX DTX handler when one or more lost speech or SID frames are received from the radio subsystem.

The requirements of the present document are mandatory for implementation in all GSM Base Station Systems (BSS) and Mobile Stations (MS).

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

* References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.
* For a specific reference, subsequent revisions do not apply.
* For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] GSM 01.04: "Digital cellular telecommunications system (Phase 2+); Abbreviations and acronyms".

[2] GSM 06.10: "Digital cellular telecommunications system (Phase 2+); Full rate speech; Transcoding".

[3] GSM 06.31: "Digital cellular telecommunications system (Phase 2+); Full rate speech; Discontinuous Transmission (DTX) for full rate speech traffic channel".

# 3 Definitions and abbreviations

Abbreviations used in the present document are listed in GSM 01.04 [1].

The definitions of terms used in the present document can be found in GSM 06.31 [3].

# 4 General

The purpose of the frame substitution is to conceal the effect of lost frames.

The purpose of muting the output in the case of several lost frames is to indicate the breakdown of the channel to the user.

# 5 Requirements

## 5.1 First lost speech frame

Normal decoding of lost speech frames would result in very unpleasant noise effects. In order to improve the subjective quality, the first lost speech frame shall be substituted with either a repetition or an extrapolation of the previous good speech frame(s). Lost speech frames shall not be delivered to the speech decoder, nor shall the output be muted directly.

## 5.2 Subsequent lost speech frames

For subsequent lost speech frames, a muting technique shall be used that will gradually decrease the output level, resulting in silencing of the output after a maximum of 320 ms. Clause 6 gives an example solution.

## 5.3 First lost SID frame

A single lost SID frame shall be substituted by the last valid SID frame and the procedure for valid SID frames be applied as described in GSM 06.31 [3].

## 5.4 Subsequent lost SID frame

For the second lost SID frame, a muting technique shall be used on the comfort noise that will gradually decrease the output level, resulting in silencing of the output after a maximum of 320 ms. Clause 6 gives an example solution.

For subsequent lost SID frames, the muting of the output shall be maintained.

# 6 Example solution

For guidance, an example solution is given.

The first lost speech frame is replaced at the speech decoder input by the previous good speech frame. Normal decoding is then performed.

The muting procedure to be used in the case of subsequent lost speech frames or for comfort noise frames following the second lost SID frame is as follows:

The pseudo‑logarithmic encoded block amplitude Xmaxcr (GSM 06.10 [2]), coded on the interval from 0 to 63, is decreased with a constant value d=4 in each frame, down to the lowest possible value. Consequently, Xmaxcr will be reduced gradually, and the output muted after a maximum of 320 ms. The grid position parameters are chosen randomly between 0 and 3 during this time.

For subsequent unusable frames, after the frame where Xmaxcr reached the lowest possible value, "silence frames" are passed from the RX DTX handler to the speech decoder to guarantee a low output level under all conditions. The silence frame is defined in table 1.

Table 1: Encoded parameters (GSM 06.10) of the silence frame

|  |  |
| --- | --- |
| Log area ratio 1 = 42 |  |
| Log area ratio 2 = 39 |  |
| Log area ratio 3 = 21 |  |
| Log area ratio 4 = 10 |  |
| Log area ratio 5 = 9 |  |
| Log area ratio 6 = 4 |  |
| Log area ratio 7 = 3 |  |
| Log area ratio 8 = 2 |  |
| \_ |  |
| LTP gain = 0 |  |
| LTP lag = 40 |  |
|  |  |
| Grid position = 1 |  |
| Block amplitude = 0 |  |
|  |  |
| RPE pulse no. 1 = 3 |  |
| RPE pulse no. 2 = 4 |  |
| RPE pulse no. 3 = 3 |  |
| RPE pulse no. 4 = 4 |  |
| RPE pulse no. 5 = 4 |  |
|  | ‑ repeated for each subsegment |
| RPE pulse no. 6 = 3 |  |
| RPE pulse no. 7 = 3 |  |
| RPE pulse no. 8 = 3 |  |
| RPE pulse no. 9 = 3 |  |
| RPE pulse no. 10 = 4 |  |
| RPE pulse no. 11 = 4 |  |
| RPE pulse no. 12 = 3 |  |
| RPE pulse no. 13 = 3 \_ |  |

Annex A (informative):  
Change history

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Change history | | | | | |
| SMG No. | TDoc. No. | CR. No. | Section affected | New version | Subject/Comments |
| SMG#07 |  |  |  | 4.0.4 | ETSI Publication |
| SMG#20 |  |  |  | 5.0.1 | Release 1996 version |
| SMG#27 |  |  |  | 6.0.0 | Release 1997 version |
| SMG#28 |  |  |  | 6.0.1 | ETSI Publication |
| SMG#29 |  |  |  | 7.0.0 | Specification version 6.0.0 upgrade to Release 1998 version 7.0.0 |
|  |  |  |  | 7.0.1 | Version update for Publication |
| SMG#31 |  |  |  | 8.0.0 | Release 1999 version |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **TSG #** | **TSG Doc.** | **CR** | **Rev** | **Subject/Comment** | **Old** | **New** |
| 03-2001 | 11 |  |  |  | Version for Release 4 |  | 4.0.0 |
| 06-2002 | 16 |  |  |  | Version for Release 5 | 4.0.0 | 5.0.0 |
| 12-2004 | 26 |  |  |  | Version for Release 6 | 5.0.0 | 6.0.0 |
| 06-2007 | 36 |  |  |  | Version for Release 7 | 6.0.0 | 7.0.0 |
| 12-2008 | 42 |  |  |  | Version for Release 8 | 7.0.0 | 8.0.0 |
| 12-2009 | 46 |  |  |  | Version for Release 9 | 8.0.0 | 9.0.0 |
| 03-2011 | 51 |  |  |  | Version for Release 10 | 9.0.0 | 10.0.0 |
| 09-2012 | 57 |  |  |  | Version for Release 11 | 10.0.0 | 11.0.0 |
| 09-2014 | 65 |  |  |  | Version for Release 12 | 11.0.0 | 12.0.0 |
| 12-2015 | 70 |  |  |  | Version for Release 13 | 12.0.0 | 13.0.0 |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 03-2017 | SA#75 |  |  |  |  | Version for Release 14 | 14.0.0 |
| 06-2018 | SA#80 | - | - | - | - | Version for Release 15 | 15.0.0 |
| 2020-07 | - | - | - | - | - | Update to Rel-16 version (MCC) | **16.0.0** |