3GPP TS 46.053 V16.0.0 (2020-07)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Services and System Aspects;

ANSI-C code for the GSM Enhanced Full Rate (EFR)

speech codec

(Release 16)

 

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.   
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.   
This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

Keywords

GSM, speech, codec

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword [4](#__RefHeading___Toc477458321)

1 Scope [5](#__RefHeading___Toc477458322)

2 References [5](#__RefHeading___Toc477458323)

3 Definitions and abbreviations [5](#__RefHeading___Toc477458324)

3.1 Definitions [5](#__RefHeading___Toc477458325)

3.2 Abbreviations [6](#__RefHeading___Toc477458326)

4 C code structure [6](#__RefHeading___Toc477458327)

4.1 Contents of the C source code disk [6](#__RefHeading___Toc477458328)

4.2 Program execution [7](#__RefHeading___Toc477458329)

4.3 Code hierarchy [7](#__RefHeading___Toc477458330)

Annex A (informative): Change History [13](#__RefHeading___Toc477458331)

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The present document provides the bit exact definition of the Enhanced Full Rate (EFR) speech traffic codec for the digital cellular telecommunications system.

An electronic attachment accompanies the present document, containing clause 5, the bit‑exact ANSI‑C code for the Enhanced Full Rate speech transcoder.

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# 1 Scope

The present document contains an electronic copy of the ANSI‑C code for the GSM Enhanced Full Rate codec. The ANSI‑C code is necessary for a bit exact implementation of the Enhanced Full Rate speech transcoder (GSM 06.60 [3]), Voice Activity Detection (GSM 06.82 [7]), comfort noise (GSM 06.62 [5]), Discontinuous Transmission (GSM 06.81 [6]) and example solutions for substituting and muting of lost frames (GSM 06.61 [4]).

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

* References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.
* For a specific reference, subsequent revisions do not apply.
* For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] GSM 01.04: "Digital cellular telecommunications system (Phase 2+); Abbreviations and acronyms".

[2] GSM 06.54: "Digital cellular telecommunications system (Phase 2+); Test sequences for the GSM Enhanced Full Rate (EFR) speech codec".

[3] GSM 06.60: "Digital cellular telecommunications system (Phase 2+); Enhanced Full Rate (EFR) speech transcoding".

[4] GSM 06.61: "Digital cellular telecommunications system (Phase 2+); Substitution and muting of lost frame for Enhanced Full Rate (EFR) speech traffic channels".

[5] GSM 06.62: "Digital cellular telecommunications system (Phase 2+); Comfort noise aspects for Enhanced Full Rate (EFR) speech traffic channels".

[6] GSM 06.81: "Digital cellular telecommunications system (Phase 2+); Discontinuous transmission (DTX) for Enhanced Full Rate (EFR) speech traffic channels".

[7] GSM 06.82: "Digital cellular telecommunications system (Phase 2+); Voice Activity Detector (VAD) for Enhanced Full Rate (EFR) speech traffic channels".

# 3 Definitions and abbreviations

## 3.1 Definitions

Definition of terms used in the present document can be found in GSM 06.60 [3], GSM 06.61 [4], GSM 06.62 [5], GSM 06.81 [6] and GSM 06.82 [7].

## 3.2 Abbreviations

For the purposes of the present document, the following abbreviations apply:

ANSI American National Standards Institute

DS‑HD Double Sided High Density

ETS European Telecommunication Standard

GSM Global System for Mobile communications

I/O Input/Output

ROM Read Only Memory

For abbreviations not given in this clause see GSM 01.04 [1].

# 4 C code structure

This clause gives an overview of the structure of the bit‑exact C code and provides an overview of the contents and organization of the archive en\_300724v080000o0.ZIP which accompanies the present document.

The C code has been verified on the following systems:

‑ Sun Microsystems [[1]](#footnote-2)1) workstations and Sun Microsystems cc compiler and gcc compiler;

‑ IBM [[2]](#footnote-3)2) PC/AT compatible computers and Borland Turbo‑C++ [[3]](#footnote-4)3) compiler;

‑ Hewlett Packard's [[4]](#footnote-5)4) workstations and HP cc compiler;

ANSI‑C 9899 was selected as the programming language because portability was desirable.

## 4.1 Contents of the C source code disk

The C code disk has all of the files in the root level.

In this disk, the files with suffix "c" contain the source code and the files with suffix "h" are the header files. The ROM data is contained mostly in files with suffix "tab". All text files are formatted such that they are correct for an IBM PC/AT compatible.

The archive en\_300724v080000o0.ZIP which accompanies the present document contains one speech coder installation verification data file, "spch\_dos.inp". The reference encoder output file is named "spch\_dos.cod", the reference decoder input file is named "spch\_dos.dec" and the reference decoder output file is named "spch\_dos.out". These four files are formatted such that they are correct for an IBM PC/AT compatible. The same files with reversed byte order of the 16 bit words are named "spch\_unx.inp", "spch\_unx.cod", "spch\_unx."dec" and "spch\_unx.out", respectively.

In an IBM PC/AT compatible platform, the installation verification can be performed by running the batch file "ts\_dos.bat". In most UNIX platforms, the installation verification can be performed by running the batch file "ts\_unx.bat". Final verification is to be performed using the GSM Enhanced Full Rate test sequences described in GSM 06.54 [2].

Makefiles are provided for the three platforms in which the C code has been verified (listed above). Once the software is installed, this directory will have compiled versions of *coder* and *decoder* (the bit‑exact C executables of the speech codec), *ed\_iface* (interface program between coder and decoder) and all the object files.

The programs *coder* and *decoder* are the GSM Enhanced Full Rate encoder and decoder executable files, respectively. A third program, *ed\_iface*, is also contained in this directory. This is the program which provides the format conversion between the encoder output file format and the decoder input file format.

## 4.2 Program execution

The GSM enhanced full rate speech codec is implemented as three separate programs:

‑ (*coder*) speech encoder;

‑ *(ed\_iface)* encoder/decoder interface;

‑ (*decoder*) speech decoder.

For encoding using the *coder* program, the input is a binary speech file (\*.inp) and the output is a binary encoded parameter file (\*.cod). For decoding using the *decoder* program, the input is a binary parameter file (\*.dec) and the output is a binary synthesized speech file (\*.out).

NOTE: The format for the parameter input file required for decoding (\*.dec) is not the same as the format of the parameter output file generated by encoding (\*.cod). The *ed\_iface* program will translate an \*.cod file into a \*.dec file.

See the file readme.txt for more information on how to run the coder, *ed\_iface* and *decoder* programs.

## 4.3 Code hierarchy

Figures 1 to 5 are call graphs that show the functions used in the speech codec, including the functions of VAD, DTX, and comfort noise generation.

The encode call graph is broken down into three separate call graphs, and the decode call graph is broken down into two separate call graphs. Those clauses which are large are separated from the primary call tree and given their own call tree. Each vertical column represents a call level. For example, main() is at level 0, Coder\_12k2() at level 1, Int\_lpc2() at level 2, Lsp\_Az() at level 3, Get\_lsp\_pol() at level 4, etc. The basic operations are not counted as extending the depth, therefore the deepest level in this software is level 4.

Some items have been omitted from this call graph. All standard C functions: printf(), fwrite(), etc. have been omitted. Also, no basic operations (add(), L\_add(), mac(), etc.) or double precision extended operations (e.g. L\_Extract()) appear in the graphs. The reset functions of the encoder and decoder are only visible as the functions reset\_enc and reset\_dec, respectively. There are several subroutine calls from inside these functions.

The time order in the call graphs is from the bottom upwards as the processing of a frame advances.



Figure 1: Speech encoder call graph (see figures 2 and 3)



Figure 2: Speech encoder subframe processing call graph



Figure 3: Voice Activity Detector (VAD) call graph



Figure 4: Speech decoder call graph (see figure 5)



Figure 5: Speech decoder postfilter call graph

Annex A (informative):  
Change History

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Change history | | | | | |
| SMG No. | TDoc. No. | CR. No. | Clause affected | New version | Subject/Comments |
| SMG#23 |  |  |  | 4.0.1 | ETSI Publication |
| SMG#20 |  |  |  | 5.1.2 | Release 1996 version |
| SMG#27 |  |  |  | 6.0.0 | Release 1997 version |
| SMG#29 |  |  |  | 7.0.0 | Release 1998 version |
|  |  |  |  | 7.0.1 | Version update to 7.0.1 for Publication |
| SMG#31 |  |  |  | 8.0.0 | Release 1999 version |
|  |  |  |  | 8.0.1 | Update to Version 8.0.1 for Publication |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **TSG #** | **TSG Doc.** | **CR** | **Rev** | **Subject/Comment** | **Old** | **New** |
| 03-2001 | 11 |  |  |  | Version for Release 4 |  | 4.0.0 |
| 06-2002 | 16 |  |  |  | Version for Release 5 | 4.0.0 | 5.0.0 |
| 12-2004 | 26 |  |  |  | Version for Release 6 | 5.0.0 | 6.0.0 |
| 06-2007 | 36 |  |  |  | Version for Release 7 | 6.0.0 | 7.0.0 |
| 12-2008 | 42 |  |  |  | Version for Release 8 | 7.0.0 | 8.0.0 |
| 12-2009 | 46 |  |  |  | Version for Release 9 | 8.0.0 | 9.0.0 |
| 03-2011 | 51 |  |  |  | Version for Release 10 | 9.0.0 | 10.0.0 |
| 09-2012 | 57 |  |  |  | Version for Release 11 | 10.0.0 | 11.0.0 |
| 09-2014 | 65 |  |  |  | Version for Release 12 | 11.0.0 | 12.0.0 |
| 12-2015 | 70 |  |  |  | Version for Release 13 | 12.0.0 | 13.0.0 |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 03-2017 | SA#75 |  |  |  |  | Version for Release 14 | 14.0.0 |
| 06-2018 | SA#80 | - | - | - | - | Version for Release 15 | 15.0.0 |
| 2020-07 | - | - | - | - | - | Update to Rel-16 version (MCC) | **16.0.0** |

1. 1 )Registered trade mark of Sun Microsystems [↑](#footnote-ref-2)
2. 2 )Registered trade mark of International Business Machines [↑](#footnote-ref-3)
3. 3 )Registered trade mark of Borland [↑](#footnote-ref-4)
4. 4 ) Registered trade mark of Hewlett Packard [↑](#footnote-ref-5)