3GPP TS 55.242 V16.0.0(2020-07)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Services and System Aspects;

Specification of the GIA4 integrity algorithm for General Packet Radio Service (GPRS);

Implementers' test data

(Release 16)

 

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP..  
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.  
This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

Keywords

GPRS, GIA4,test,algorithm,security

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword [4](#__RefHeading___Toc476044321)

Introduction [4](#__RefHeading___Toc476044322)

1 Scope [5](#__RefHeading___Toc476044323)

2 References [5](#__RefHeading___Toc476044324)

3 Definitions and abbreviations [5](#__RefHeading___Toc476044325)

3.1 Definitions [5](#__RefHeading___Toc476044326)

3.2 Abbreviations [5](#__RefHeading___Toc476044327)

4 Introductory information [5](#__RefHeading___Toc476044328)

4.1 Introduction [5](#__RefHeading___Toc476044329)

4.2 Notation [5](#__RefHeading___Toc476044330)

4.2.1 Radix [5](#__RefHeading___Toc476044331)

4.2.2 Conventions [6](#__RefHeading___Toc476044332)

4.2.3 Bit/Byte ordering [6](#__RefHeading___Toc476044333)

4.3 List of variables [6](#__RefHeading___Toc476044334)

5 Test data [7](#__RefHeading___Toc476044335)

Annex A (informative): Change history [8](#__RefHeading___Toc476044336)

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# Introduction

The present documenthas been prepared by the 3GPP Task Force, and gives a detailed specification of the 3GPP integrity algorithm GIA4.

The present document is the second of three, which between them form the entire specification of the 3GPP Integrity Algorithm GIA4:

- 3GPP TS 55.241: "3rd Generation Partnership Project; Technical Specification Group Services and System Aspects; Specification of the GIA4 integrity algorithms for GPRS; GIA4 specification".

**- 3GPP TS 55.242: "3rd Generation Partnership Project; Technical Specification Group Services and System Aspects; Specification of the GIA4 integrity** **algorithms for GPRS; Implementers' test data".**

- 3GPP TS 55.243: "3rd Generation Partnership Project; Technical Specification Group Services and System Aspects; Specification of the GIA4 integrity algorithms for GPRS; Design conformance test data".

# 1 Scope

The present document defines the implementers test data of the 3GPP integrity algorithm GIA4.

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 55.241: "Specification of the GIA4 encryption algorithms for GPRS; GIA4 specification".

# 3 Definitions and abbreviations

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in 3GPP TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in 3GPP TR 21.905 [1].

## 3.2 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

# 4 Introductory information

## 4.1 Introduction

The integrity algorithm GIA4computes a 32-bit MAC (Message Authentication Code) of a given input message using integrity key KI128. The approach adopted uses KASUMI [2] in a form of CBC-MAC mode.

## 4.2 Notation

### 4.2.1 Radix

"0x" is used to indicate hexadecimal numbers.

### 4.2.2 Conventions

The assignment operator "=", is used as in several programming languages. The following:

<variable> = <expression>

means that <*variable*> assumes the value that <*expression*> had before the assignment took place. For instance,

*x* = *x* + *y* + 3

means

(new value of *x*) becomes (old value of *x*) + (old value of *y*) + 3.

### 4.2.3 Bit/Byte ordering

All data variables in this specification are presented with the most significant bit (or byte) on the left hand side and the least significant bit (or byte) on the right hand side. Where a variable is broken down into a number of sub-strings, the left most (most significant) sub-string is numbered 0, the next most significant is numbered 1 and so on through to the least significant.

For example an n-bit MESSAGE is subdivided into 64-bit substrings MB0,MB1…MBi so for a message:

0x0123456789ABCDEFFEDCBA987654321086545381AB594FC28786404C50A37…

The resulting notation is:

MB0 = 0x0123456789ABCDEF  
MB1 **=** 0xFEDCBA9876543210  
MB2 = 0x86545381AB594FC2  
MB3 = 0x8786404C50A37…

In binary this would be:

000000010010001101000101011001111000100110101011110011011110111111111110…

with

**MB0** = 0000000100100011010001010110011110001001101010111100110111101111  
**MB1 =** 1111111011011100101110101001100001110110010101000011001000010000  
**MB2** = 1000011001010100010100111000000110101011010110010100111111000010  
**MB3** = 1000011110000110010000000100110001010000101000110111…

## 4.3 List of variables

A, B are 64-bit registers that are used within the function to hold intermediate values.

BLOCKS an integer variable indicating the number of successive applications of KASUMI that need to be performed.

CONSTANT-F a 32-bit parameter which is constant for any given FRAMETYPE input.

DIRECTION a 1-bit input indicating the direction of transmission (uplink or downlink).

FRAMETYPE an 8-bit input to the function indicating the type of frame to be protected.

INPUT-I a 32-bit time variant input to the function.

KI128 the 128-bit integrity key.

KM a 128-bit constant that is used to modify a key.

M an input to the function which specifies the number of octets of message to be MAC’d (1-65536).

MAC the 32-bit message authentication code (MAC) produced by the function.

MESSAGE the input octet stream of length M octets that is to be processed by the function.

PS is the input padded string processed by the function.

# 5 Test data

This clause only available under licence.   
See <http://www.etsi.org/about/what-we-do/security-algorithms-and-codes/cellular-algorithm-licences>.

Annex A (informative):  
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2017-03 | SA#75 | SP-170088 |  |  |  | Presented for approval | 2.0.0 |
| 2017-03 | SA#75 |  |  |  |  | Upgrade to change control version | 13.0.0 |
| 2017-03 | SA#75 | - | - | - |  | Promotion to Release 14 without technical change | **14.0.0** |
| 2018-06 | - | - | - | - | - | Update to Rel-15 version (MCC) | **15.0.0** |
| 2020-07 | - | - | - | - | - | Update to Rel-16 version (MCC) | **16.0.0** |